<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="BROADCOM_HDSP-B09G_0">
                    <description>18:88 and 88:88 0.56" Four Digit GaP Green Seven Segment Display</description>
                </package>
            </packages>
            <symbols>
                <symbol name="BROADCOM_HDSP-B09G_0_0">
                    <description>18:88 and 88:88 0.56" Four Digit GaP Green Seven Segment Display</description>
                    <pin name="ANODE_E"/>
                    <pin name="ANODE_D"/>
                    <pin name="ANODE_DP"/>
                    <pin name="ANODE_C"/>
                    <pin name="ANODE_G"/>
                    <pin name="DIGIT_4_COMMON_CATHODE"/>
                    <pin name="ANODE_B"/>
                    <pin name="DIGIT_3_COMMON_CATHODE"/>
                    <pin name="DIGIT_2_COMMON_CATHODE"/>
                    <pin name="ANODE_F"/>
                    <pin name="ANODE_A"/>
                    <pin name="DIGIT_1_COMMON_CATHODE"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="DS" name="BROADCOM_HDSP-B09G">
                    <description>18:88 and 88:88 0.56" Four Digit GaP Green Seven Segment Display</description>
                    <gates>
                        <gate name="G$0" symbol="BROADCOM_HDSP-B09G_0_0"/>
                    </gates>
                    <devices>
                        <device name="BROADCOM_HDSP-B09G_0_0" package="BROADCOM_HDSP-B09G_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="ANODE_E"/>
                                <connect gate="G$0" pad="2" pin="ANODE_D"/>
                                <connect gate="G$0" pad="3" pin="ANODE_DP"/>
                                <connect gate="G$0" pad="4" pin="ANODE_C"/>
                                <connect gate="G$0" pad="5" pin="ANODE_G"/>
                                <connect gate="G$0" pad="6" pin="DIGIT_4_COMMON_CATHODE"/>
                                <connect gate="G$0" pad="7" pin="ANODE_B"/>
                                <connect gate="G$0" pad="8" pin="DIGIT_3_COMMON_CATHODE"/>
                                <connect gate="G$0" pad="9" pin="DIGIT_2_COMMON_CATHODE"/>
                                <connect gate="G$0" pad="10" pin="ANODE_F"/>
                                <connect gate="G$0" pad="11" pin="ANODE_A"/>
                                <connect gate="G$0" pad="12" pin="DIGIT_1_COMMON_CATHODE"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="630-HDSP-B09G"/>
                                    <attribute name="Test_Current_(mA)" value="10.0"/>
                                    <attribute name="temperature_range_high" value="+105°C"/>
                                    <attribute name="MPN" value="HDSP-B09G"/>
                                    <attribute name="digikey_description" value='DISPLAY 7SEG 4DIG GREEN CC 0.56"'/>
                                    <attribute name="Manufacturer_Product_Page" value="https://www.broadcom.com/products/leds-and-displays/7-segment/through-hole/hdsp-b09g"/>
                                    <attribute name="digikey_part_number" value="HDSP-B09G-ND"/>
                                    <attribute name="prefix" value="DS"/>
                                    <attribute name="datasheet" value="https://docs.broadcom.com/docs/AV01-0698EN"/>
                                    <attribute name="Configuration" value="Common Cathode"/>
                                    <attribute name="Typical_Dominant_Wavelength_(nm)" value="573"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="Digit/Alpha_Size" value='0.56" (14.22mm)'/>
                                    <attribute name="Typical_Luminous_Intensity_(mcd)" value="5.05"/>
                                    <attribute name="Size_/_Dimension" value='0.752" H x 2.016" W x 0.315" D (19.10mm x 51.20mm x 8.00mm)'/>
                                    <attribute name="Number_of_Characters" value="4"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="MF" value="Broadcom"/>
                                    <attribute name="package" value="DISP_PTH_15MM2_19MM1"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
