<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;H1&gt;FNE Library - Digital Potencimeters&lt;/h1&gt;

&lt;p&gt;Knihovna obsahuje digitální potenciometry a reostaty od firmy Microchip&lt;/p&gt;

&lt;p&gt;This library contain digital potenciometrs and rheostats from Microchip company&lt;/p&gt;</description>
<packages>
<package name="SOT65P210X110-6N">
</package>
<package name="SOP65P490X110-8N">
</package>
<package name="SOP65P640X120-14N">
</package>
<package name="SOP50P490X110-10N">
</package>
</packages>
<symbols>
<symbol name="MCP4017T-103E/LT">
<pin name="B"/>
<pin name="W"/>
<pin name="VDD" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MCP4531-103E/MS">
<pin name="VDD" direction="pwr"/>
<pin name="HVC/A0" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="VSS" direction="pwr"/>
<pin name="P0A" direction="pas"/>
<pin name="P0B" direction="pas"/>
<pin name="P0W" direction="pas"/>
</symbol>
<symbol name="MCP4631-502E/ST">
<pin name="NC" direction="nc"/>
<pin name="VDD" direction="pwr"/>
<pin name="HVC/A0" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P0A" direction="pas"/>
<pin name="P0B" direction="pas"/>
<pin name="P0W" direction="pas"/>
<pin name="P1A" direction="pas"/>
<pin name="P1B" direction="pas"/>
<pin name="P1W" direction="pas"/>
<pin name="SDA"/>
</symbol>
<symbol name="MCP4631-503E/ST">
<pin name="NC" direction="nc"/>
<pin name="VDD" direction="pwr"/>
<pin name="HVC/A0" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P0A" direction="pas"/>
<pin name="P0B" direction="pas"/>
<pin name="P0W" direction="pas"/>
<pin name="P1A" direction="pas"/>
<pin name="P1B" direction="pas"/>
<pin name="P1W" direction="pas"/>
<pin name="SDA"/>
</symbol>
<symbol name="MCP4652-502E/UN">
<pin name="VDD" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="HVC/A0" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P0B" direction="pas"/>
<pin name="P0W" direction="pas"/>
<pin name="P1B" direction="pas"/>
<pin name="P1W" direction="pas"/>
<pin name="SDA"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MCP4017T" prefix="U">
<description>&lt;h1&gt;MCP4017&lt;/h1&gt;&lt;br&gt;

&lt;b&gt;IC, 7-Bit Single I2C  Digital Rheostat with Volatile Memory in SC-70-6&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;b&gt;Features&lt;/b&gt;&lt;br&gt;
• Potentiometer or Rheostat configuration options&lt;br&gt;
• 7-bit: Resistor Network Resolution&lt;br&gt;
- 127 Resistors (128 Steps)&lt;br&gt;
• Zero Scale to Full Scale Wiper operation&lt;br&gt;
• RAB Resistances: 5 kΩ, 10 kΩ, 50 kΩ, or 100 kΩ&lt;br&gt;
• Low Wiper Resistance: 100Ω (typical)&lt;br&gt;
• Low Tempco:&lt;br&gt;
- Absolute (Rheostat): 50 ppm typical
(0°C to 70°C)&lt;br&gt;
- Ratiometric (Potentiometer): 10 ppm typical&lt;br&gt;
• Simple I2C Protocol with read &amp; write commands&lt;br&gt;
• Brown-out reset protection (1.5V typical)&lt;br&gt;
• Power-on Default Wiper Setting (Mid-scale)&lt;br&gt;
• Low-Power Operation:&lt;br&gt;
- 2.5 μA Static Current (typical)&lt;br&gt;
• Wide Operating Voltage Range:&lt;br&gt;
- 2.7V to 5.5V - Device Characteristics&lt;br&gt;&lt;br&gt;

&lt;b&gt;Specified&lt;/b&gt;&lt;br&gt;
- 1.8V to 5.5V - Device Operation&lt;br&gt;
• Wide Bandwidth (-3 dB) Operation:&lt;br&gt;
- 2 MHz (typical) for 5.0 kΩ device&lt;br&gt;
• Extended temperature range (-40°C to +125°C)&lt;br&gt;
• Very small package (SC70)&lt;br&gt;
• Lead free (Pb-free) package&lt;br&gt;</description>
<gates>
<gate name="A" symbol="MCP4017T-103E/LT"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-6N">
<connects>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="SCL" pad="3"/>
<connect gate="A" pin="SDA" pad="4"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="2"/>
<connect gate="A" pin="W" pad="6"/>
</connects>
<technologies>
<technology name="-103E/LT">
<attribute name="MPN" value="MCP4017T-103E/LT"/>
<attribute name="OC_FARNELL" value="1715846"/>
<attribute name="OC_NEWARK" value="25R4724"/>
<attribute name="PACKAGE" value="SC-70-6"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4531">
<description>&lt;H1&gt;MCP453X/455X/463X/465X&lt;/h1&gt;&lt;br&gt;

&lt;b&gt;7/8-Bit Single/Dual I2C Digital POT with
Volatile Memory&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;b&gt;Features:&lt;/b&gt;&lt;br&gt;
• Single or Dual Resistor Network Options&lt;br&gt;
• Potentiometer or Rheostat Configuration Options&lt;br&gt;
• Resistor Network Resolution&lt;br&gt;
- 7-bit: 128 Resistors (129 Steps)&lt;br&gt;
- 8-bit: 256 Resistors (257 Steps)&lt;br&gt;
• RAB Resistances Options of:&lt;br&gt;
- 5kOhm&lt;br&gt;
- 10kOhm&lt;br&gt;
- 50kOhm&lt;br&gt;
- 100kOhm&lt;br&gt;
• Zero-Scale to Full-Scale Wiper Operation&lt;br&gt;
• Low Wiper Resistance: 75Ohm (typical)&lt;br&gt;
• Low Tempco:&lt;br&gt;
- Absolute (Rheostat): 50 ppm typical&lt;br&gt;
(0°C to 70°C)
- Ratiometric (Potentiometer): 15 ppm typical&lt;br&gt;
• I2C Serial Interface&lt;br&gt;
- 100 kHz, 400 kHz and 3.4 MHz Support&lt;br&gt;
• Serial Protocol Allows:&lt;br&gt;
- High-Speed Read/Write to Wiper&lt;br&gt;
- Increment/Decrement of Wiper&lt;br&gt;
• Resistor Network Terminal Disconnect Feature&lt;br&gt;
via the Terminal Control (TCON) Register&lt;br&gt;
• Brown-Out Reset Protection (1.5V typical)&lt;br&gt;
• Serial Interface Inactive Current (2.5 uA typical)&lt;br&gt;
• High-Voltage Tolerant Digital Inputs: up to 12.5V&lt;br&gt;
• Wide Operating Voltage:&lt;br&gt;
- 2.7V to 5.5V - Device Characteristics Specified&lt;br&gt;
- 1.8V to 5.5V - Device Operation&lt;br&gt;
• Wide Bandwidth (-3dB) Operation:&lt;br&gt;
- 2 MHz (typical) for 5.0 k Device&lt;br&gt;
• Extended Temperature Range (-40°C to +125°C)&lt;br&gt;&lt;br&gt;
&lt;b&gt;Description:&lt;/b&gt;&lt;br&gt;
The MCP45XX and MCP46XX devices offer a wide
range of product offerings using an I2C interface. This
family of devices support 7-bit and 8-bit resistor
networks, volatile memory configurations, and
Potentiometer and Rheostat pinouts.</description>
<gates>
<gate name="A" symbol="MCP4531-103E/MS"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="HVC/A0" pad="1"/>
<connect gate="A" pin="P0A" pad="5"/>
<connect gate="A" pin="P0B" pad="7"/>
<connect gate="A" pin="P0W" pad="6"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="-103E/MS">
<attribute name="MPN" value="MCP4531-103E/MS"/>
<attribute name="OC_FARNELL" value="1698946"/>
<attribute name="OC_NEWARK" value="77M2840"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4631-502E/ST" prefix="U">
<description>&lt;H1&gt;MCP453X/455X/463X/465X&lt;/h1&gt;&lt;br&gt;

&lt;b&gt;7/8-Bit Single/Dual I2C Digital POT with
Volatile Memory&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;b&gt;Features:&lt;/b&gt;&lt;br&gt;
• Single or Dual Resistor Network Options&lt;br&gt;
• Potentiometer or Rheostat Configuration Options&lt;br&gt;
• Resistor Network Resolution&lt;br&gt;
- 7-bit: 128 Resistors (129 Steps)&lt;br&gt;
- 8-bit: 256 Resistors (257 Steps)&lt;br&gt;
• RAB Resistances Options of:&lt;br&gt;
- 5kOhm&lt;br&gt;
- 10kOhm&lt;br&gt;
- 50kOhm&lt;br&gt;
- 100kOhm&lt;br&gt;
• Zero-Scale to Full-Scale Wiper Operation&lt;br&gt;
• Low Wiper Resistance: 75Ohm (typical)&lt;br&gt;
• Low Tempco:&lt;br&gt;
- Absolute (Rheostat): 50 ppm typical&lt;br&gt;
(0°C to 70°C)
- Ratiometric (Potentiometer): 15 ppm typical&lt;br&gt;
• I2C Serial Interface&lt;br&gt;
- 100 kHz, 400 kHz and 3.4 MHz Support&lt;br&gt;
• Serial Protocol Allows:&lt;br&gt;
- High-Speed Read/Write to Wiper&lt;br&gt;
- Increment/Decrement of Wiper&lt;br&gt;
• Resistor Network Terminal Disconnect Feature&lt;br&gt;
via the Terminal Control (TCON) Register&lt;br&gt;
• Brown-Out Reset Protection (1.5V typical)&lt;br&gt;
• Serial Interface Inactive Current (2.5 uA typical)&lt;br&gt;
• High-Voltage Tolerant Digital Inputs: up to 12.5V&lt;br&gt;
• Wide Operating Voltage:&lt;br&gt;
- 2.7V to 5.5V - Device Characteristics Specified&lt;br&gt;
- 1.8V to 5.5V - Device Operation&lt;br&gt;
• Wide Bandwidth (-3dB) Operation:&lt;br&gt;
- 2 MHz (typical) for 5.0 k Device&lt;br&gt;
• Extended Temperature Range (-40°C to +125°C)&lt;br&gt;&lt;br&gt;
&lt;b&gt;Description:&lt;/b&gt;&lt;br&gt;
The MCP45XX and MCP46XX devices offer a wide
range of product offerings using an I2C interface. This
family of devices support 7-bit and 8-bit resistor
networks, volatile memory configurations, and
Potentiometer and Rheostat pinouts.</description>
<gates>
<gate name="A" symbol="MCP4631-502E/ST"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="13"/>
<connect gate="A" pin="A2" pad="12"/>
<connect gate="A" pin="HVC/A0" pad="1"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="P0A" pad="8"/>
<connect gate="A" pin="P0B" pad="10"/>
<connect gate="A" pin="P0W" pad="9"/>
<connect gate="A" pin="P1A" pad="7"/>
<connect gate="A" pin="P1B" pad="5"/>
<connect gate="A" pin="P1W" pad="6"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MCP4631-502E/ST"/>
<attribute name="OC_FARNELL" value="1840737"/>
<attribute name="OC_NEWARK" value="77M2938"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4631" prefix="U">
<description>&lt;H1&gt;MCP453X/455X/463X/465X&lt;/h1&gt;&lt;br&gt;

&lt;b&gt;7/8-Bit Single/Dual I2C Digital POT with
Volatile Memory&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;b&gt;Features:&lt;/b&gt;&lt;br&gt;
• Single or Dual Resistor Network Options&lt;br&gt;
• Potentiometer or Rheostat Configuration Options&lt;br&gt;
• Resistor Network Resolution&lt;br&gt;
- 7-bit: 128 Resistors (129 Steps)&lt;br&gt;
- 8-bit: 256 Resistors (257 Steps)&lt;br&gt;
• RAB Resistances Options of:&lt;br&gt;
- 5kOhm&lt;br&gt;
- 10kOhm&lt;br&gt;
- 50kOhm&lt;br&gt;
- 100kOhm&lt;br&gt;
• Zero-Scale to Full-Scale Wiper Operation&lt;br&gt;
• Low Wiper Resistance: 75Ohm (typical)&lt;br&gt;
• Low Tempco:&lt;br&gt;
- Absolute (Rheostat): 50 ppm typical&lt;br&gt;
(0°C to 70°C)
- Ratiometric (Potentiometer): 15 ppm typical&lt;br&gt;
• I2C Serial Interface&lt;br&gt;
- 100 kHz, 400 kHz and 3.4 MHz Support&lt;br&gt;
• Serial Protocol Allows:&lt;br&gt;
- High-Speed Read/Write to Wiper&lt;br&gt;
- Increment/Decrement of Wiper&lt;br&gt;
• Resistor Network Terminal Disconnect Feature&lt;br&gt;
via the Terminal Control (TCON) Register&lt;br&gt;
• Brown-Out Reset Protection (1.5V typical)&lt;br&gt;
• Serial Interface Inactive Current (2.5 uA typical)&lt;br&gt;
• High-Voltage Tolerant Digital Inputs: up to 12.5V&lt;br&gt;
• Wide Operating Voltage:&lt;br&gt;
- 2.7V to 5.5V - Device Characteristics Specified&lt;br&gt;
- 1.8V to 5.5V - Device Operation&lt;br&gt;
• Wide Bandwidth (-3dB) Operation:&lt;br&gt;
- 2 MHz (typical) for 5.0 k Device&lt;br&gt;
• Extended Temperature Range (-40°C to +125°C)&lt;br&gt;&lt;br&gt;
&lt;b&gt;Description:&lt;/b&gt;&lt;br&gt;
The MCP45XX and MCP46XX devices offer a wide
range of product offerings using an I2C interface. This
family of devices support 7-bit and 8-bit resistor
networks, volatile memory configurations, and
Potentiometer and Rheostat pinouts.</description>
<gates>
<gate name="A" symbol="MCP4631-503E/ST"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="13"/>
<connect gate="A" pin="A2" pad="12"/>
<connect gate="A" pin="HVC/A0" pad="1"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="P0A" pad="8"/>
<connect gate="A" pin="P0B" pad="10"/>
<connect gate="A" pin="P0W" pad="9"/>
<connect gate="A" pin="P1A" pad="7"/>
<connect gate="A" pin="P1B" pad="5"/>
<connect gate="A" pin="P1W" pad="6"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="-503E/ST">
<attribute name="MPN" value="MCP4631-503E/ST"/>
<attribute name="OC_FARNELL" value="1840711"/>
<attribute name="OC_NEWARK" value="77M2939"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4652">
<description>&lt;H1&gt;MCP453X/455X/463X/465X&lt;/h1&gt;&lt;br&gt;

&lt;b&gt;7/8-Bit Single/Dual I2C Digital POT with
Volatile Memory&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;b&gt;Features:&lt;/b&gt;&lt;br&gt;
• Single or Dual Resistor Network Options&lt;br&gt;
• Potentiometer or Rheostat Configuration Options&lt;br&gt;
• Resistor Network Resolution&lt;br&gt;
- 7-bit: 128 Resistors (129 Steps)&lt;br&gt;
- 8-bit: 256 Resistors (257 Steps)&lt;br&gt;
• RAB Resistances Options of:&lt;br&gt;
- 5kOhm&lt;br&gt;
- 10kOhm&lt;br&gt;
- 50kOhm&lt;br&gt;
- 100kOhm&lt;br&gt;
• Zero-Scale to Full-Scale Wiper Operation&lt;br&gt;
• Low Wiper Resistance: 75Ohm (typical)&lt;br&gt;
• Low Tempco:&lt;br&gt;
- Absolute (Rheostat): 50 ppm typical&lt;br&gt;
(0°C to 70°C)
- Ratiometric (Potentiometer): 15 ppm typical&lt;br&gt;
• I2C Serial Interface&lt;br&gt;
- 100 kHz, 400 kHz and 3.4 MHz Support&lt;br&gt;
• Serial Protocol Allows:&lt;br&gt;
- High-Speed Read/Write to Wiper&lt;br&gt;
- Increment/Decrement of Wiper&lt;br&gt;
• Resistor Network Terminal Disconnect Feature&lt;br&gt;
via the Terminal Control (TCON) Register&lt;br&gt;
• Brown-Out Reset Protection (1.5V typical)&lt;br&gt;
• Serial Interface Inactive Current (2.5 uA typical)&lt;br&gt;
• High-Voltage Tolerant Digital Inputs: up to 12.5V&lt;br&gt;
• Wide Operating Voltage:&lt;br&gt;
- 2.7V to 5.5V - Device Characteristics Specified&lt;br&gt;
- 1.8V to 5.5V - Device Operation&lt;br&gt;
• Wide Bandwidth (-3dB) Operation:&lt;br&gt;
- 2 MHz (typical) for 5.0 k Device&lt;br&gt;
• Extended Temperature Range (-40°C to +125°C)&lt;br&gt;&lt;br&gt;
&lt;b&gt;Description:&lt;/b&gt;&lt;br&gt;
The MCP45XX and MCP46XX devices offer a wide
range of product offerings using an I2C interface. This
family of devices support 7-bit and 8-bit resistor
networks, volatile memory configurations, and
Potentiometer and Rheostat pinouts.</description>
<gates>
<gate name="A" symbol="MCP4652-502E/UN"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="HVC/A0" pad="1"/>
<connect gate="A" pin="P0B" pad="8"/>
<connect gate="A" pin="P0W" pad="7"/>
<connect gate="A" pin="P1B" pad="5"/>
<connect gate="A" pin="P1W" pad="6"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VDD" pad="10"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="-502E/UN">
<attribute name="MPN" value="MCP4652-502E/UN"/>
<attribute name="OC_FARNELL" value="1840747"/>
<attribute name="OC_NEWARK" value="77M2998"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>