<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:29:04</description>
<packages>
<package name="BGA256C100P16X16_1700X1700X220">
</package>
<package name="BGA324C100P18X18_1900X1900X220">
</package>
<package name="QFP50P3460X3460X410-240N">
</package>
<package name="BGA324C18X18X100P_1900X1900X22">
</package>
<package name="BGA400C20X20X100P_2100X2100X22">
</package>
<package name="QFP50P1600X1600X120-100N">
</package>
<package name="QFP50P2200X2200X160-144N">
</package>
<package name="BGA256C100P16X16X_1700X1700X22">
</package>
<package name="BGA484N100P22X22_2300X2300X350">
</package>
<package name="QFP50P3060X3060X410-208N">
</package>
<package name="BGA484C22X22X100P_2300X2300X35">
</package>
<package name="BGA780C100P28X28_2900X2900X350">
</package>
<package name="BGA672C100P26X26_2700X2700X350">
</package>
<package name="BGA780C28X28X100P_2900X2900X35">
</package>
<package name="BGA672C26X26X100P_2700X2700X35">
</package>
<package name="BGA1020C100P32X32_3300X3300X35">
</package>
<package name="BGA256C16X16X100C_1700X1700X22">
</package>
<package name="BGA484C100P22X22_2300X2300X350">
</package>
<package name="BGA484C80P22X22_1900X1900X220">
</package>
<package name="BGA484C22X22X80P_1900X1900X220">
</package>
<package name="BGA484C100P22X22-2300X2300X350">
</package>
<package name="BGA1020C32X32X100C_3300X3300X3">
</package>
<package name="BGA1508C100P39X39_4000X4000X35">
</package>
<package name="BGA1152C100P34X34_3500X3500X35">
</package>
<package name="QFP50P2200X2200X160-145N">
</package>
<package name="DIP254P762X431-8">
</package>
<package name="PLCC127P1000X1000X457-20N">
</package>
<package name="QFP80P900X900X120-32N">
</package>
<package name="QFP65P1720X2320X340-100N">
</package>
<package name="BGA88C12X8X80P_800X1100X140">
</package>
<package name="PLCC127P990X990X457-20N">
</package>
<package name="SOIC127P600X175-8N">
</package>
<package name="SOIC127P1030X265-16N">
</package>
<package name="BGA256C16X16X100P_1700X1700X22">
</package>
<package name="BGA256C50P20X20_1100X1100X120">
</package>
<package name="BGA324N100P18X18_1900X1900X220">
</package>
<package name="BGA256C16X16X100C_1700X1700X15">
</package>
<package name="BGA100C50P11X11_600X600X120">
</package>
<package name="PLCC127P1752X1752X457-44N">
</package>
<package name="QFP80P1200X1200X120-44N">
</package>
<package name="PLCC127P1765X1765X457-44N">
</package>
<package name="BGA100N100P10X10_1100X1100X170">
</package>
<package name="BGA100C100P10X10_1100X1100X170">
</package>
<package name="PLCC127P3022X3022X457-84N">
</package>
<package name="PLCC127P3035X3035X475-84N">
</package>
<package name="QFP65P3100X3100X410-160N">
</package>
<package name="QFP65P3120X3120X410-160N">
</package>
</packages>
<symbols>
<symbol name="EP1C12F256C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="pas"/>
<pin name="CLK0" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP1C12F256C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO_60" direction="pas"/>
<pin name="IO_61" direction="pas"/>
<pin name="IO_62" direction="pas"/>
<pin name="IO_63" direction="pas"/>
<pin name="IO_64" direction="pas"/>
<pin name="IO_65" direction="pas"/>
<pin name="IO_66" direction="pas"/>
<pin name="IO_67" direction="pas"/>
<pin name="IO_68" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP1C12F256C8N_C">
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EP1C12F256I7N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="pas"/>
<pin name="CLK0" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP1C12F256I7N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO_60" direction="pas"/>
<pin name="IO_61" direction="pas"/>
<pin name="IO_62" direction="pas"/>
<pin name="IO_63" direction="pas"/>
<pin name="IO_64" direction="pas"/>
<pin name="IO_65" direction="pas"/>
<pin name="IO_66" direction="pas"/>
<pin name="IO_67" direction="pas"/>
<pin name="IO_68" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP1C12F256I7N_C">
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EP1C12F324C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C12F324C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="NCEO" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C12F324C8N_C">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C12F324C8N_D">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C12Q240C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C12Q240C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C12Q240C8N_C">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F324C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F324C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="NCEO" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F324C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F324C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F400C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="MSEL0" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="CLK0/LVDSCLK1P" direction="in"/>
<pin name="CLK1/LVDSCLK1N" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO/ASDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F400C8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F400C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C20F400C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TDO" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T100C7N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T100C8N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T100I7N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T144C7_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T144C7_B">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T144C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T144C8N_B">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T144I7N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C3T144I7N_B">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F324C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F324C8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F324C8N_C">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F324C8N_D">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TDO" direction="pas"/>
<pin name="TMS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
<pin name="IO/LVDS107N"/>
<pin name="IO/LVDS104P"/>
<pin name="IO/LVDS105N/DQ0B4"/>
<pin name="IO/LVDS105P/DQ0B5"/>
<pin name="IO/LVDS106N/DQ0B6"/>
<pin name="IO/LVDS106P/DQ0B7"/>
</symbol>
<symbol name="EP1C4F400C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F400C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F400C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C4F400C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TDO" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6F256C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="VCCA_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6F256C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6F256C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pas"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EP1C6F256I7N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="VCCA_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6F256I7N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6F256I7N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pas"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EP1C6Q240C6N_A">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="DATA0" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6Q240C6N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6Q240C6N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6Q240C8N_A">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="DATA0" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6Q240C8N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6Q240C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6T144C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="DATA0" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1C6T144C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FI256-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="NCONFIG" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/CS"/>
<pin name="TDO" direction="out"/>
<pin name="NCEO" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FI256-2N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FI256-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_NCLR"/>
<pin name="IO/DEV_OE"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT_9" direction="pas"/>
<pin name="GNDINT_10" direction="pas"/>
<pin name="GNDINT_11" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FC484-1_A">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="DATA0" direction="in"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA5"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="*CE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA7"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="IO_26"/>
<pin name="TDI" direction="in"/>
<pin name="IO/DATA3"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO/DATA6"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FC484-1_B">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="NC_2" direction="nc"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO_7" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="MSEL0" direction="in"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="MSEL1" direction="in"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FC484-1_C">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="CLOCK" direction="in"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO/CS"/>
<pin name="IO/*CS"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="INPUT_2" direction="in"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO/*WS"/>
<pin name="TCK" direction="in"/>
<pin name="*CEO" direction="out"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO/*RS"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO/*DEV_CLR"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO/CLKUSR"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
<pin name="INPUT" direction="in"/>
</symbol>
<symbol name="EP1K100FC484-1_D">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO/RDY/*BSY"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_13"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO_7" direction="pwr"/>
<pin name="VCCIO_8" direction="pwr"/>
<pin name="VCCIO_9" direction="pwr"/>
<pin name="VCCIO_10" direction="pwr"/>
<pin name="VCCIO_11" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="INPUT" direction="in"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100FC484-1_E">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="*CONFIG" direction="in"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO/LOCK"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="TMS" direction="in"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="INPUT" direction="in"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="TRST" direction="in"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="*STATUS" direction="in"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="NC_10" direction="nc"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="NC" direction="nc"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100QC208-3N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100QC208-3N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100QC208-3N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100QI208-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100QI208-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K100QI208-2N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K10QC208-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K10QC208-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K10QC208-2N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K10TC100-1N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLKUSR" direction="pas"/>
<pin name="GCLK1" direction="in"/>
<pin name="DCLK" direction="pas"/>
<pin name="CLOCK" direction="in"/>
<pin name="VCC_CKLK" direction="in"/>
<pin name="TCK" direction="pas"/>
<pin name="GND_CKLK" direction="in"/>
<pin name="NRS" direction="pas"/>
<pin name="NWS" direction="pas"/>
<pin name="NCS" direction="pas"/>
<pin name="CS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="RDYNBUSY" direction="pas"/>
<pin name="IO/DEV_CLRN" direction="pas"/>
<pin name="DEV_OE" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="LOCK" direction="pas"/>
<pin name="INIT_DONE" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
</symbol>
<symbol name="EP1K10TC100-3N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLKUSR" direction="pas"/>
<pin name="GCLK1" direction="in"/>
<pin name="DCLK" direction="pas"/>
<pin name="CLOCK" direction="in"/>
<pin name="VCC_CKLK" direction="in"/>
<pin name="TCK" direction="pas"/>
<pin name="GND_CKLK" direction="in"/>
<pin name="NRS" direction="pas"/>
<pin name="NWS" direction="pas"/>
<pin name="NCS" direction="pas"/>
<pin name="CS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="RDYNBUSY" direction="pas"/>
<pin name="IO/DEV_CLRN" direction="pas"/>
<pin name="DEV_OE" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="LOCK" direction="pas"/>
<pin name="INIT_DONE" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
</symbol>
<symbol name="EP1K10TC144-3N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="TDO" direction="out"/>
<pin name="IO/LOCK"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K10TC144-3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
</symbol>
<symbol name="EP1K30FC256-1N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="NCONFIG" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/CS"/>
<pin name="TDO" direction="out"/>
<pin name="NCEO" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30FC256-1N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30FC256-1N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_NCLR"/>
<pin name="IO/DEV_OE"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT_9" direction="pas"/>
<pin name="GNDINT_10" direction="pas"/>
<pin name="GNDINT_11" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30FI256-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="NCONFIG" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/CS"/>
<pin name="TDO" direction="out"/>
<pin name="NCEO" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30FI256-2N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30FI256-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_NCLR"/>
<pin name="IO/DEV_OE"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT_9" direction="pas"/>
<pin name="GNDINT_10" direction="pas"/>
<pin name="GNDINT_11" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30QC208-3N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30QC208-3N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30QC208-3N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30TC144-3N_A">
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="*CEO" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="INPUT_2" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="TMS" direction="in"/>
<pin name="*STATUS" direction="in"/>
<pin name="IO_15"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO/RDY/*BUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/LOCK"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30TC144-3N_B">
<pin name="IO_2"/>
<pin name="*CONFIG" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="TDI" direction="in"/>
<pin name="*CE" direction="in"/>
<pin name="DCLK" direction="pas"/>
<pin name="DATA0" direction="in"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO/*DEV_CLR"/>
<pin name="CLOCK" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
<pin name="IO/*RS"/>
<pin name="IO/*WS"/>
<pin name="IO/CS"/>
<pin name="IO/*CS"/>
</symbol>
<symbol name="EP1K30TI144-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/CLKUSR"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K30TI144-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="DATA0" direction="in"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/RS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO/NDEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50FC256-1N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="NCONFIG" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/CS"/>
<pin name="TDO" direction="out"/>
<pin name="NCEO" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50FC256-1N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50FC256-1N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_NCLR"/>
<pin name="IO/DEV_OE"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT_9" direction="pas"/>
<pin name="GNDINT_10" direction="pas"/>
<pin name="GNDINT_11" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50FI256-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="NCONFIG" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/CS"/>
<pin name="TDO" direction="out"/>
<pin name="NCEO" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50FI256-2N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50FI256-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_NCLR"/>
<pin name="IO/DEV_OE"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT_9" direction="pas"/>
<pin name="GNDINT_10" direction="pas"/>
<pin name="GNDINT_11" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50QC208-1N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/LOCK"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50QC208-1N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50QC208-1N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50QC208-2N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT_8" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/LOCK"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50QC208-2N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50QC208-2N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50TC144-1N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_CKLK" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CLOCK/GCLK1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT_7" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/LOCK"/>
<pin name="IO/RDY/NBUSY"/>
<pin name="IO/CLKUSR"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1K50TC144-1N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NCS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S10F484C7N_A">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCG_PLL4" direction="pwr"/>
<pin name="VREF0B4" direction="in"/>
<pin name="VREF1B4" direction="in"/>
<pin name="VREF0B5" direction="in"/>
<pin name="VREF1B5" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CLK10P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GNDG_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S10F484C7N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCG_PLL3" direction="pwr"/>
<pin name="CLK8P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK12P" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="VREF1B6" direction="in"/>
<pin name="VREF1B7" direction="in"/>
<pin name="VREF0B6" direction="in"/>
<pin name="VREF0B7" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDG_PLL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S10F484C7N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="CLK13P" direction="in"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S10F484C7N_D">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREF0B1" direction="in"/>
<pin name="VREF1B1" direction="in"/>
<pin name="VREF0B2" direction="in"/>
<pin name="VREF0B3" direction="in"/>
<pin name="VREF1B2" direction="in"/>
<pin name="VREF1B3" direction="in"/>
<pin name="VREF1B8" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S10F484C7N_E">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREF0B8" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="CLK4P" direction="in"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK6P" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S20F780C7N_A">
<pin name="VCCIO5" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="NC_3" direction="nc"/>
<pin name="VREF1B4" direction="pas"/>
<pin name="VREF1B5" direction="pas"/>
<pin name="VREF0B4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO_83"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S20F780C7N_B">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCG_PLL4" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCG_PLL3" direction="pwr"/>
<pin name="VREF1B6" direction="pas"/>
<pin name="CLK11N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK10P" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK8P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDG_PLL3" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S20F780C7N_C">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VREF2B7" direction="pas"/>
<pin name="VREF0B6" direction="pas"/>
<pin name="VREF1B7" direction="pas"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S20F780C7N_D">
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VREF1B3" direction="pas"/>
<pin name="VREF2B3" direction="pas"/>
<pin name="VREF0B2" direction="pas"/>
<pin name="VREF2B4" direction="pas"/>
<pin name="VREF0B3" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="VCC_PLL5_OUTB" direction="pwr"/>
</symbol>
<symbol name="EP1S20F780C7N_E">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK12P" direction="in"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="VREF1B2" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="TRST" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S20F780C7N_F">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VREF0B5" direction="pas"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S20F780C7N_G">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pas"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="VCCSEL" direction="pas"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="CLK4P" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="VREF1B1" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="VCC_PLL6_OUTB" direction="pwr"/>
</symbol>
<symbol name="EP1S20F780C7N_H">
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCIO8_2" direction="pas"/>
<pin name="VCCIO8" direction="pas"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VREF1B8" direction="pas"/>
<pin name="VREF0B7" direction="pas"/>
<pin name="VREF2B8" direction="pas"/>
<pin name="VREF0B8" direction="pas"/>
<pin name="CLK6P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VREF2B3" direction="pas"/>
<pin name="VREF1B3" direction="pas"/>
<pin name="VREF0B2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO_83"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_B">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREF0B1" direction="pas"/>
<pin name="VREF2B1" direction="pas"/>
<pin name="VREF1B2" direction="pas"/>
<pin name="VREF1B1" direction="pas"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_C">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VREF0B8" direction="pas"/>
<pin name="VREF1B8" direction="pas"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK12P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="TRST" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_D">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="pas"/>
<pin name="VREF1B5" direction="pas"/>
<pin name="VREF0B3" direction="pas"/>
<pin name="VREF2B4" direction="pas"/>
<pin name="VREF0B4" direction="pas"/>
<pin name="VREF1B4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_E">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCINT_20" direction="pwr"/>
<pin name="VCCINT_21" direction="pwr"/>
<pin name="VCCINT_22" direction="pwr"/>
<pin name="VCCINT_23" direction="pwr"/>
<pin name="VCCINT_24" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCG_PLL4" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCG_PLL3" direction="pwr"/>
<pin name="VREF0B5" direction="pas"/>
<pin name="VREF2B6" direction="pas"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="CLK8P" direction="in"/>
<pin name="CLK10P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_F">
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="MSEL2" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="VREF1B6" direction="pas"/>
<pin name="VREF2B8" direction="pas"/>
<pin name="VREF0B6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDG_PLL3" direction="pas"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F672C7N_G">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK4P" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="CLK6P" direction="in"/>
<pin name="VREF2B7" direction="pas"/>
<pin name="VREF0B7" direction="pas"/>
<pin name="VREF1B7" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VREF0B4" direction="pas"/>
<pin name="VREF1B4" direction="pas"/>
<pin name="VREF1B5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO_83"/>
<pin name="IO_84"/>
<pin name="IO_85"/>
<pin name="IO_86"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_B">
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCG_PLL3" direction="pwr"/>
<pin name="VCCG_PLL4" direction="pwr"/>
<pin name="VREF1B6" direction="pas"/>
<pin name="CLK11N" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK8P" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK10P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL3" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GNDG_PLL4" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_C">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="VREF2B7" direction="pas"/>
<pin name="VREF1B7" direction="pas"/>
<pin name="VREF0B6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_D">
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VREF2B3" direction="pas"/>
<pin name="VREF0B2" direction="pas"/>
<pin name="VREF1B3" direction="pas"/>
<pin name="VREF2B4" direction="pas"/>
<pin name="VREF0B3" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="VCC_PLL5_OUTB" direction="pwr"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_E">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREF1B2" direction="pas"/>
<pin name="TRST" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK12P" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_F">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREF0B1" direction="pas"/>
<pin name="VREF0B5" direction="pas"/>
<pin name="VREF2B6" direction="pas"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_G">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK4P" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="VREF1B1" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="VCC_PLL6_OUTB" direction="pwr"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S25F780C6N_H">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="CLK6P" direction="in"/>
<pin name="VREF1B8" direction="pas"/>
<pin name="VREF0B8" direction="pas"/>
<pin name="VREF2B1" direction="pas"/>
<pin name="VREF2B8" direction="pas"/>
<pin name="VREF0B7" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VREF0B4" direction="in"/>
<pin name="VREF1B4" direction="in"/>
<pin name="VREF1B5" direction="in"/>
<pin name="VREF2B5" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO_83"/>
<pin name="IO_84"/>
<pin name="IO_85"/>
<pin name="IO_86"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_B">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCG_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCG_PLL4" direction="pwr"/>
<pin name="CLK8P" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK10P" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="VREF1B6" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDG_PLL3" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GNDG_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_C">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VREF2B7" direction="in"/>
<pin name="VREF1B7" direction="in"/>
<pin name="VREF0B6" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO_79"/>
<pin name="IO_80"/>
<pin name="IO_81"/>
<pin name="IO_82"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_D">
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="VCC_PLL5_OUTB" direction="pwr"/>
<pin name="VREF0B2" direction="in"/>
<pin name="VREF0B3" direction="in"/>
<pin name="VREF1B3" direction="in"/>
<pin name="VREF2B3" direction="in"/>
<pin name="VREF2B4" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_E">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CLK12P" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="VREF1B2" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_F">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREF0B1" direction="in"/>
<pin name="VREF2B2" direction="in"/>
<pin name="VREF0B5" direction="in"/>
<pin name="VREF2B6" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_G">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="VCC_PLL6_OUTB" direction="pwr"/>
<pin name="PORSEL" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="VREF1B1" direction="in"/>
<pin name="NO_PULLUP" direction="in"/>
<pin name="CLK4P" direction="in"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1S30F780C7N_H">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="CLK6P" direction="in"/>
<pin name="VREF0B7" direction="in"/>
<pin name="VREF0B8" direction="in"/>
<pin name="VREF1B8" direction="in"/>
<pin name="VREF2B8" direction="in"/>
<pin name="VREF2B1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCR_B15" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="RREFB15A" direction="in"/>
<pin name="VREF0B4" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC_7" direction="pas"/>
<pin name="GND/NC_8" direction="pas"/>
<pin name="GND/NC_9" direction="pas"/>
<pin name="GND/NC_10" direction="pas"/>
<pin name="GND/NC_11" direction="pas"/>
<pin name="GND/NC_12" direction="pas"/>
<pin name="GND/NC_13" direction="pas"/>
<pin name="GND/NC_14" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_4_DQ0T4"/>
<pin name="IO_4_DQ0T5"/>
<pin name="IO_4_DQ0T0"/>
<pin name="IO_4_DQ0T2"/>
<pin name="IO_4_DQ0T1"/>
<pin name="IO_4_DQ0T3"/>
<pin name="IO_4_DQ0T6"/>
<pin name="IO_4_DQ0T7"/>
<pin name="IO_4_DQ1T5"/>
<pin name="IO_4_DQ1T2"/>
<pin name="IO_4_DQ1T4"/>
<pin name="IO_4_DQ2T3"/>
<pin name="IO_4_DQ2T0"/>
<pin name="IO_4_DQ2T7"/>
<pin name="IO_4_DQ2T4"/>
<pin name="IO_4_DQ3T1"/>
<pin name="IO_4_DQ3T5"/>
<pin name="IO_4_DQ3T6"/>
<pin name="IO_4_DQ1T1"/>
<pin name="IO_4_DQ1T3"/>
<pin name="IO_4_DQ1T7"/>
<pin name="IO_4_DQ2T5"/>
<pin name="IO_4_DQ2T6"/>
<pin name="IO_4_DQ2T1"/>
<pin name="IO_4_DQ2T2"/>
<pin name="IO_4_DQ3T3"/>
<pin name="IO_4_DQ3T2"/>
<pin name="IO_4_DQ3T0"/>
<pin name="IO_4_DQ3T7"/>
<pin name="IO_4_DQ1T0"/>
<pin name="IO_4_DQ1T6"/>
<pin name="IO_4_DQS0T"/>
<pin name="IO_4_DQS1T"/>
<pin name="IO_4_DQS2T"/>
<pin name="IO_4_DQS3T"/>
<pin name="IO_4_DEV_OE"/>
<pin name="IO_4_FCLK7"/>
<pin name="IO_4_RDN4"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4_5"/>
<pin name="IO_4_6"/>
<pin name="IO_4"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_B">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCG_B15_2" direction="pwr"/>
<pin name="VCCA_B15_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCT_B15_2" direction="pwr"/>
<pin name="VCCP_B15_2" direction="pwr"/>
<pin name="VCCR_B15_2" direction="pwr"/>
<pin name="VCCP_B15_3" direction="pwr"/>
<pin name="VCCA_B15" direction="pwr"/>
<pin name="VCCG_B15" direction="pwr"/>
<pin name="VCCT_B15_3" direction="pwr"/>
<pin name="VCCR_B15_3" direction="pwr"/>
<pin name="VCCP_B15_4" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCR_B15" direction="pwr"/>
<pin name="VCCP_B15" direction="pwr"/>
<pin name="NCE" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="GXB_RX9P" direction="in"/>
<pin name="GXB_RX8P" direction="in"/>
<pin name="GXB_RX9N" direction="in"/>
<pin name="GXB_RX8N" direction="in"/>
<pin name="RREFB15" direction="in"/>
<pin name="REFCLKB15P" direction="in"/>
<pin name="REFCLKB15N" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND_22" direction="pas"/>
<pin name="GXB_GND_23" direction="pas"/>
<pin name="GXB_GND_24" direction="pas"/>
<pin name="GXB_GND_25" direction="pas"/>
<pin name="GXB_GND_26" direction="pas"/>
<pin name="GXB_GND_27" direction="pas"/>
<pin name="GXB_GND_28" direction="pas"/>
<pin name="GXB_GND_29" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_7_FCLK5"/>
<pin name="IO_7_DQ2B6"/>
<pin name="IO_7_DQ2B2"/>
<pin name="IO_4_DQ3T4"/>
<pin name="IO_7_FCLK4"/>
<pin name="IO_7_RDN7"/>
<pin name="IO_3_CLK14N"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7"/>
<pin name="IO_3_DQ8T2"/>
<pin name="IO_3_DQ8T5"/>
<pin name="IO_3_DQ7T2"/>
<pin name="IO_3_DQ8T4"/>
<pin name="IO_3_DQ9T0"/>
<pin name="IO_3_DQ9T4"/>
<pin name="IO_10_PLL5_OUT3N"/>
<pin name="GXB_TX8P" direction="out"/>
<pin name="GXB_TX8N" direction="out"/>
<pin name="GXB_TX9P" direction="out"/>
<pin name="GXB_TX9N" direction="out"/>
<pin name="GXB_TX10P" direction="out"/>
<pin name="GXB_TX10N" direction="out"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="GXB_RX10P" direction="in"/>
<pin name="GXB_RX10N" direction="in"/>
<pin name="GXB_RX11P" direction="in"/>
<pin name="GXB_RX11N" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="GXB_TX11P" direction="out"/>
<pin name="GXB_TX11N" direction="out"/>
<pin name="IO_7_DQ2B5"/>
<pin name="IO_7_DQ2B1"/>
<pin name="IO_7_DQS2B"/>
<pin name="IO_7_DQ2B0"/>
<pin name="IO_7_DQ2B3"/>
<pin name="IO_7_DQ0B5"/>
<pin name="IO_7_DQ0B0"/>
<pin name="IO_7_DQ1B0"/>
<pin name="IO_7_DQ1B1"/>
<pin name="IO_7_DQ2B4"/>
<pin name="IO_7_DQ2B7"/>
<pin name="IO_7_DQ0B4"/>
<pin name="IO_7_DQ0B3"/>
<pin name="IO_7_DQ1B3"/>
<pin name="IO_7_DQ1B6"/>
<pin name="IO_7_DQ3B0"/>
<pin name="IO_7_DQ3B1"/>
<pin name="IO_7_DQ0B2"/>
<pin name="IO_7_DQ0B1"/>
<pin name="IO_7_DQS0B"/>
<pin name="IO_7_DQ0B6"/>
<pin name="IO_7_DQS1B"/>
<pin name="IO_7_DQ1B4"/>
<pin name="IO_7_DQ3B3"/>
<pin name="IO_7_DQS3B"/>
<pin name="IO_7_DQ0B7"/>
<pin name="IO_7_DQ1B7"/>
<pin name="IO_7_DQ1B2"/>
<pin name="IO_7_DQ1B5"/>
<pin name="IO_7_DQ3B7"/>
<pin name="IO_7_DQ3B2"/>
<pin name="IO_3_DQ6T1"/>
<pin name="IO_3_DQ6T7"/>
<pin name="IO_3_DQ7T1"/>
<pin name="IO_3_DQ7T5"/>
<pin name="IO_3_DQS8T"/>
<pin name="IO_3_DQ8T3"/>
<pin name="IO_3_DQ9T1"/>
<pin name="IO_3_DQS9T"/>
<pin name="IO_3_DQ9T5"/>
<pin name="IO_3_DQ9T7"/>
<pin name="IO_3_DQ9T6"/>
<pin name="IO_3_DQS6T"/>
<pin name="IO_3_DQ6T6"/>
<pin name="IO_3_DQ6T3"/>
<pin name="IO_3_DQS7T"/>
<pin name="IO_3_DQ7T4"/>
<pin name="IO_3_DQ8T0"/>
<pin name="IO_3_DQ8T6"/>
<pin name="IO_3_DQ9T2"/>
<pin name="IO_3_DQ9T3"/>
<pin name="IO_3_CLK15N"/>
<pin name="IO_4_CLK12N"/>
<pin name="IO_9_PLL5_OUT1P"/>
<pin name="IO_9_PLL5_OUT0P"/>
<pin name="IO_9_PLL5_OUT1N"/>
<pin name="IO_9_PLL5_OUT0N"/>
<pin name="IO_10_PLL5_OUT3P"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_D">
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="CLK12P" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="VREF0B3" direction="in"/>
<pin name="VREF1B3" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT_5" direction="in"/>
<pin name="INPUT_6" direction="in"/>
<pin name="INPUT_7" direction="in"/>
<pin name="INPUT_8" direction="in"/>
<pin name="INPUT_9" direction="in"/>
<pin name="INPUT_10" direction="in"/>
<pin name="INPUT_11" direction="in"/>
<pin name="INPUT_12" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="IO_3_DQ8T1"/>
<pin name="IO_3_DQ7T3"/>
<pin name="IO_3_DQ6T4"/>
<pin name="IO_3_DQ7T6"/>
<pin name="IO_3_DQ8T7"/>
<pin name="IO_3_DQ6T5"/>
<pin name="IO_3_FCLK0"/>
<pin name="IO_3_FCLK1"/>
<pin name="IO_3_DQ6T2"/>
<pin name="IO_3_DQ6T0"/>
<pin name="IO_3_DQ7T0"/>
<pin name="IO_3_DQ7T7"/>
<pin name="IO_4_FCLK6"/>
<pin name="IO_4_RUP4"/>
<pin name="IO_4_CLK13N"/>
<pin name="IO_9_PLL5_FBN"/>
<pin name="IO_9_PLL5_FBP"/>
<pin name="IO_10_PLL5_OUT2P"/>
<pin name="IO_10_PLL5_OUT2N"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_3_4"/>
<pin name="IO_3_5"/>
<pin name="IO_3"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4"/>
<pin name="IO_2_DIFFIO_TX21P"/>
<pin name="IO_2_DIFFIO_TX21N"/>
<pin name="IO_2_DIFFIO_TX18P"/>
<pin name="IO_2_DIFFIO_TX18N"/>
<pin name="IO_2_DIFFIO_TX20P"/>
<pin name="IO_2_DIFFIO_TX20N"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_E">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_PLL5_OUTB" direction="pwr"/>
<pin name="VCC_PLL6_OUTB" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREF0B2" direction="in"/>
<pin name="VREF1B2" direction="in"/>
<pin name="VREF0B1" direction="in"/>
<pin name="VREF1B4" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT_5" direction="in"/>
<pin name="INPUT_6" direction="in"/>
<pin name="INPUT_7" direction="in"/>
<pin name="INPUT_8" direction="in"/>
<pin name="INPUT_9" direction="in"/>
<pin name="INPUT_10" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_1_DIFFIO_TX9P"/>
<pin name="IO_1_DIFFIO_TX9N"/>
<pin name="IO_1_DIFFIO_TX10P"/>
<pin name="IO_1_DIFFIO_TX10N"/>
<pin name="IO_2_DIFFIO_TX11P"/>
<pin name="IO_2_DIFFIO_TX11N"/>
<pin name="IO_2_DIFFIO_TX12P"/>
<pin name="IO_2_DIFFIO_TX12N"/>
<pin name="IO_2_DIFFIO_TX13P"/>
<pin name="IO_2_DIFFIO_TX13N"/>
<pin name="IO_2_DIFFIO_TX14P"/>
<pin name="IO_2_DIFFIO_TX14N"/>
<pin name="IO_2_DIFFIO_TX15P"/>
<pin name="IO_2_DIFFIO_TX15N"/>
<pin name="IO_2_DIFFIO_TX16P"/>
<pin name="IO_2_DIFFIO_TX16N"/>
<pin name="IO_2_DIFFIO_TX17P"/>
<pin name="IO_2_DIFFIO_TX17N"/>
<pin name="IO_2_DIFFIO_TX19P"/>
<pin name="IO_2_DIFFIO_TX19N"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_3"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_1_CLK3N"/>
<pin name="IO_2_CLK1N"/>
<pin name="IO_3_RUP3"/>
<pin name="IO_3_RDN3"/>
<pin name="IO_8_RDN8"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_F">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREF1B1" direction="in"/>
<pin name="VREF1B7" direction="in"/>
<pin name="VREF0B7" direction="in"/>
<pin name="VREF1B8" direction="in"/>
<pin name="VREF0B8" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT_5" direction="in"/>
<pin name="INPUT_6" direction="in"/>
<pin name="INPUT_7" direction="in"/>
<pin name="INPUT_8" direction="in"/>
<pin name="INPUT_9" direction="in"/>
<pin name="INPUT_10" direction="in"/>
<pin name="INPUT_11" direction="in"/>
<pin name="INPUT_12" direction="in"/>
<pin name="INPUT_13" direction="in"/>
<pin name="INPUT_14" direction="in"/>
<pin name="INPUT_15" direction="in"/>
<pin name="INPUT_16" direction="in"/>
<pin name="INPUT_17" direction="in"/>
<pin name="INPUT_18" direction="in"/>
<pin name="INPUT_19" direction="in"/>
<pin name="INPUT_20" direction="in"/>
<pin name="INPUT_21" direction="in"/>
<pin name="INPUT_22" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_1_DIFFIO_TX0P"/>
<pin name="IO_1_DIFFIO_TX0N"/>
<pin name="IO_1_DIFFIO_TX1P"/>
<pin name="IO_1_DIFFIO_TX1N"/>
<pin name="IO_1_DIFFIO_TX2P"/>
<pin name="IO_1_DIFFIO_TX2N"/>
<pin name="IO_1_DIFFIO_TX3P"/>
<pin name="IO_1_DIFFIO_TX3N"/>
<pin name="IO_1_DIFFIO_TX4P"/>
<pin name="IO_1_DIFFIO_TX4N"/>
<pin name="IO_1_DIFFIO_TX5P"/>
<pin name="IO_1_DIFFIO_TX5N"/>
<pin name="IO_1_DIFFIO_TX6P"/>
<pin name="IO_1_DIFFIO_TX6N"/>
<pin name="IO_1_DIFFIO_TX7P"/>
<pin name="IO_1_DIFFIO_TX7N"/>
<pin name="IO_1_DIFFIO_TX8P"/>
<pin name="IO_1_DIFFIO_TX8N"/>
<pin name="IO_7_CLK7N"/>
<pin name="IO_7_DEV_CLRN"/>
<pin name="IO_7_RUP7"/>
<pin name="IO_8_RUP8"/>
<pin name="IO_8_DQ7B0"/>
<pin name="IO_8_DQ7B1"/>
<pin name="IO_8_DQ7B4"/>
<pin name="IO_8_DQ7B7"/>
<pin name="IO_8_FCLK2"/>
<pin name="IO_8_FCLK3"/>
<pin name="IO_11_PLL6_OUT1P"/>
<pin name="IO_12_PLL6_OUT2P"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_8_6"/>
<pin name="IO_8"/>
</symbol>
<symbol name="EP1SGX10CF672C6N_G">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="CLK4P" direction="in"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK6P" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_11_PLL6_OUT1N"/>
<pin name="IO_11_PLL6_FBP"/>
<pin name="IO_11_PLL6_OUT0N"/>
<pin name="IO_11_PLL6_OUT0P"/>
<pin name="IO_11_PLL6_FBN"/>
<pin name="IO_12_PLL6_OUT2N"/>
<pin name="IO_12_PLL6_OUT3P"/>
<pin name="IO_12_PLL6_OUT3N"/>
<pin name="IO_8"/>
<pin name="IO_8_DQS7B"/>
<pin name="IO_8_DQ7B6"/>
<pin name="IO_8_DQ7B3"/>
<pin name="IO_8_DQ7B2"/>
<pin name="IO_8_DQ7B5"/>
<pin name="IO_8_DQ6B2"/>
<pin name="IO_8_DQ6B1"/>
<pin name="IO_8_DQ6B3"/>
<pin name="IO_8_DQ8B1"/>
<pin name="IO_8_CLK5N"/>
<pin name="IO_8_DQ6B5"/>
<pin name="IO_8_DQS6B"/>
<pin name="IO_8_DQ6B6"/>
<pin name="IO_8_DQ8B5"/>
<pin name="IO_8_DQ8B4"/>
<pin name="IO_8_DQ9B1"/>
<pin name="IO_8_DQ9B2"/>
<pin name="IO_8_DQ9B5"/>
<pin name="IO_8_DQ6B0"/>
<pin name="IO_8_DQ6B4"/>
<pin name="IO_8_DQ6B7"/>
<pin name="IO_8_DQS8B"/>
<pin name="IO_8_DQ8B6"/>
<pin name="IO_8_DQ9B0"/>
<pin name="IO_8_DQS9B"/>
<pin name="IO_8_DQ9B6"/>
<pin name="IO_8_CLK4N"/>
<pin name="IO_8_DQ8B2"/>
<pin name="IO_8_DQ8B0"/>
<pin name="IO_8_DQ8B3"/>
<pin name="IO_8_DQ8B7"/>
<pin name="IO_8_DQ9B3"/>
<pin name="IO_8_DQ9B4"/>
<pin name="IO_8_DQ9B7"/>
<pin name="IO_7_DQ3B5"/>
<pin name="IO_7_DQ3B4"/>
<pin name="IO_7_CLK6N"/>
<pin name="IO_7_DQ3B6"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCR_B15" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="RREFB15A" direction="in"/>
<pin name="VREF0B4" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC_7" direction="pas"/>
<pin name="GND/NC_8" direction="pas"/>
<pin name="GND/NC_9" direction="pas"/>
<pin name="GND/NC_10" direction="pas"/>
<pin name="GND/NC_11" direction="pas"/>
<pin name="GND/NC_12" direction="pas"/>
<pin name="GND/NC_13" direction="pas"/>
<pin name="GND/NC_14" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_4_DQ0T4"/>
<pin name="IO_4_DQ0T5"/>
<pin name="IO_4_DQ0T0"/>
<pin name="IO_4_DQ0T2"/>
<pin name="IO_4_DQ0T1"/>
<pin name="IO_4_DQ0T3"/>
<pin name="IO_4_DQ0T6"/>
<pin name="IO_4_DQ0T7"/>
<pin name="IO_4_DQ1T5"/>
<pin name="IO_4_DQ1T2"/>
<pin name="IO_4_DQ1T4"/>
<pin name="IO_4_DQ2T3"/>
<pin name="IO_4_DQ2T0"/>
<pin name="IO_4_DQ2T7"/>
<pin name="IO_4_DQ2T4"/>
<pin name="IO_4_DQ3T1"/>
<pin name="IO_4_DQ3T5"/>
<pin name="IO_4_DQ3T6"/>
<pin name="IO_4_DQ1T1"/>
<pin name="IO_4_DQ1T3"/>
<pin name="IO_4_DQ1T7"/>
<pin name="IO_4_DQ2T5"/>
<pin name="IO_4_DQ2T6"/>
<pin name="IO_4_DQ2T1"/>
<pin name="IO_4_DQ2T2"/>
<pin name="IO_4_DQ3T3"/>
<pin name="IO_4_DQ3T2"/>
<pin name="IO_4_DQ3T0"/>
<pin name="IO_4_DQ3T7"/>
<pin name="IO_4_DQ1T0"/>
<pin name="IO_4_DQ1T6"/>
<pin name="IO_4_DQS0T"/>
<pin name="IO_4_DQS1T"/>
<pin name="IO_4_DQS2T"/>
<pin name="IO_4_DQS3T"/>
<pin name="IO_4_DEV_OE"/>
<pin name="IO_4_FCLK7"/>
<pin name="IO_4_RDN4"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4_5"/>
<pin name="IO_4_6"/>
<pin name="IO_4"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_B">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCG_B15_2" direction="pwr"/>
<pin name="VCCA_B15_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCT_B15_2" direction="pwr"/>
<pin name="VCCP_B15_2" direction="pwr"/>
<pin name="VCCR_B15_2" direction="pwr"/>
<pin name="VCCP_B15_3" direction="pwr"/>
<pin name="VCCA_B15" direction="pwr"/>
<pin name="VCCG_B15" direction="pwr"/>
<pin name="VCCT_B15_3" direction="pwr"/>
<pin name="VCCR_B15_3" direction="pwr"/>
<pin name="VCCP_B15_4" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCR_B15" direction="pwr"/>
<pin name="VCCP_B15" direction="pwr"/>
<pin name="NCE" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="GXB_RX9P" direction="in"/>
<pin name="GXB_RX8P" direction="in"/>
<pin name="GXB_RX9N" direction="in"/>
<pin name="GXB_RX8N" direction="in"/>
<pin name="RREFB15" direction="in"/>
<pin name="REFCLKB15P" direction="in"/>
<pin name="REFCLKB15N" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND_22" direction="pas"/>
<pin name="GXB_GND_23" direction="pas"/>
<pin name="GXB_GND_24" direction="pas"/>
<pin name="GXB_GND_25" direction="pas"/>
<pin name="GXB_GND_26" direction="pas"/>
<pin name="GXB_GND_27" direction="pas"/>
<pin name="GXB_GND_28" direction="pas"/>
<pin name="GXB_GND_29" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_7_FCLK5"/>
<pin name="IO_7_DQ2B6"/>
<pin name="IO_7_DQ2B2"/>
<pin name="IO_4_DQ3T4"/>
<pin name="IO_7_FCLK4"/>
<pin name="IO_7_RDN7"/>
<pin name="IO_3_CLK14N"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7"/>
<pin name="IO_3_DQ8T2"/>
<pin name="IO_3_DQ8T5"/>
<pin name="IO_3_DQ7T2"/>
<pin name="IO_3_DQ8T4"/>
<pin name="IO_3_DQ9T0"/>
<pin name="IO_3_DQ9T4"/>
<pin name="IO_10_PLL5_OUT3N"/>
<pin name="GXB_TX8P" direction="out"/>
<pin name="GXB_TX8N" direction="out"/>
<pin name="GXB_TX9P" direction="out"/>
<pin name="GXB_TX9N" direction="out"/>
<pin name="GXB_TX10P" direction="out"/>
<pin name="GXB_TX10N" direction="out"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="GXB_RX10P" direction="in"/>
<pin name="GXB_RX10N" direction="in"/>
<pin name="GXB_RX11P" direction="in"/>
<pin name="GXB_RX11N" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="GXB_TX11P" direction="out"/>
<pin name="GXB_TX11N" direction="out"/>
<pin name="IO_7_DQ2B5"/>
<pin name="IO_7_DQ2B1"/>
<pin name="IO_7_DQS2B"/>
<pin name="IO_7_DQ2B0"/>
<pin name="IO_7_DQ2B3"/>
<pin name="IO_7_DQ0B5"/>
<pin name="IO_7_DQ0B0"/>
<pin name="IO_7_DQ1B0"/>
<pin name="IO_7_DQ1B1"/>
<pin name="IO_7_DQ2B4"/>
<pin name="IO_7_DQ2B7"/>
<pin name="IO_7_DQ0B4"/>
<pin name="IO_7_DQ0B3"/>
<pin name="IO_7_DQ1B3"/>
<pin name="IO_7_DQ1B6"/>
<pin name="IO_7_DQ3B0"/>
<pin name="IO_7_DQ3B1"/>
<pin name="IO_7_DQ0B2"/>
<pin name="IO_7_DQ0B1"/>
<pin name="IO_7_DQS0B"/>
<pin name="IO_7_DQ0B6"/>
<pin name="IO_7_DQS1B"/>
<pin name="IO_7_DQ1B4"/>
<pin name="IO_7_DQ3B3"/>
<pin name="IO_7_DQS3B"/>
<pin name="IO_7_DQ0B7"/>
<pin name="IO_7_DQ1B7"/>
<pin name="IO_7_DQ1B2"/>
<pin name="IO_7_DQ1B5"/>
<pin name="IO_7_DQ3B7"/>
<pin name="IO_7_DQ3B2"/>
<pin name="IO_3_DQ6T1"/>
<pin name="IO_3_DQ6T7"/>
<pin name="IO_3_DQ7T1"/>
<pin name="IO_3_DQ7T5"/>
<pin name="IO_3_DQS8T"/>
<pin name="IO_3_DQ8T3"/>
<pin name="IO_3_DQ9T1"/>
<pin name="IO_3_DQS9T"/>
<pin name="IO_3_DQ9T5"/>
<pin name="IO_3_DQ9T7"/>
<pin name="IO_3_DQ9T6"/>
<pin name="IO_3_DQS6T"/>
<pin name="IO_3_DQ6T6"/>
<pin name="IO_3_DQ6T3"/>
<pin name="IO_3_DQS7T"/>
<pin name="IO_3_DQ7T4"/>
<pin name="IO_3_DQ8T0"/>
<pin name="IO_3_DQ8T6"/>
<pin name="IO_3_DQ9T2"/>
<pin name="IO_3_DQ9T3"/>
<pin name="IO_3_CLK15N"/>
<pin name="IO_4_CLK12N"/>
<pin name="IO_9_PLL5_OUT1P"/>
<pin name="IO_9_PLL5_OUT0P"/>
<pin name="IO_9_PLL5_OUT1N"/>
<pin name="IO_9_PLL5_OUT0N"/>
<pin name="IO_10_PLL5_OUT3P"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_D">
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="CLK12P" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="VREF0B3" direction="in"/>
<pin name="VREF1B3" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT_5" direction="in"/>
<pin name="INPUT_6" direction="in"/>
<pin name="INPUT_7" direction="in"/>
<pin name="INPUT_8" direction="in"/>
<pin name="INPUT_9" direction="in"/>
<pin name="INPUT_10" direction="in"/>
<pin name="INPUT_11" direction="in"/>
<pin name="INPUT_12" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="IO_3_DQ8T1"/>
<pin name="IO_3_DQ7T3"/>
<pin name="IO_3_DQ6T4"/>
<pin name="IO_3_DQ7T6"/>
<pin name="IO_3_DQ8T7"/>
<pin name="IO_3_DQ6T5"/>
<pin name="IO_3_FCLK0"/>
<pin name="IO_3_FCLK1"/>
<pin name="IO_3_DQ6T2"/>
<pin name="IO_3_DQ6T0"/>
<pin name="IO_3_DQ7T0"/>
<pin name="IO_3_DQ7T7"/>
<pin name="IO_4_FCLK6"/>
<pin name="IO_4_RUP4"/>
<pin name="IO_4_CLK13N"/>
<pin name="IO_9_PLL5_FBN"/>
<pin name="IO_9_PLL5_FBP"/>
<pin name="IO_10_PLL5_OUT2P"/>
<pin name="IO_10_PLL5_OUT2N"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_3_4"/>
<pin name="IO_3_5"/>
<pin name="IO_3"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4"/>
<pin name="IO_2_DIFFIO_TX21P"/>
<pin name="IO_2_DIFFIO_TX21N"/>
<pin name="IO_2_DIFFIO_TX18P"/>
<pin name="IO_2_DIFFIO_TX18N"/>
<pin name="IO_2_DIFFIO_TX20P"/>
<pin name="IO_2_DIFFIO_TX20N"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_E">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCC_PLL5_OUTB" direction="pwr"/>
<pin name="VCC_PLL6_OUTB" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREF0B2" direction="in"/>
<pin name="VREF1B2" direction="in"/>
<pin name="VREF0B1" direction="in"/>
<pin name="VREF1B4" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT_5" direction="in"/>
<pin name="INPUT_6" direction="in"/>
<pin name="INPUT_7" direction="in"/>
<pin name="INPUT_8" direction="in"/>
<pin name="INPUT_9" direction="in"/>
<pin name="INPUT_10" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_1_DIFFIO_TX9P"/>
<pin name="IO_1_DIFFIO_TX9N"/>
<pin name="IO_1_DIFFIO_TX10P"/>
<pin name="IO_1_DIFFIO_TX10N"/>
<pin name="IO_2_DIFFIO_TX11P"/>
<pin name="IO_2_DIFFIO_TX11N"/>
<pin name="IO_2_DIFFIO_TX12P"/>
<pin name="IO_2_DIFFIO_TX12N"/>
<pin name="IO_2_DIFFIO_TX13P"/>
<pin name="IO_2_DIFFIO_TX13N"/>
<pin name="IO_2_DIFFIO_TX14P"/>
<pin name="IO_2_DIFFIO_TX14N"/>
<pin name="IO_2_DIFFIO_TX15P"/>
<pin name="IO_2_DIFFIO_TX15N"/>
<pin name="IO_2_DIFFIO_TX16P"/>
<pin name="IO_2_DIFFIO_TX16N"/>
<pin name="IO_2_DIFFIO_TX17P"/>
<pin name="IO_2_DIFFIO_TX17N"/>
<pin name="IO_2_DIFFIO_TX19P"/>
<pin name="IO_2_DIFFIO_TX19N"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_3"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_1_CLK3N"/>
<pin name="IO_2_CLK1N"/>
<pin name="IO_3_RUP3"/>
<pin name="IO_3_RDN3"/>
<pin name="IO_8_RDN8"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_F">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="CLK7P" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREF1B1" direction="in"/>
<pin name="VREF1B7" direction="in"/>
<pin name="VREF0B7" direction="in"/>
<pin name="VREF1B8" direction="in"/>
<pin name="VREF0B8" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT_3" direction="in"/>
<pin name="INPUT_4" direction="in"/>
<pin name="INPUT_5" direction="in"/>
<pin name="INPUT_6" direction="in"/>
<pin name="INPUT_7" direction="in"/>
<pin name="INPUT_8" direction="in"/>
<pin name="INPUT_9" direction="in"/>
<pin name="INPUT_10" direction="in"/>
<pin name="INPUT_11" direction="in"/>
<pin name="INPUT_12" direction="in"/>
<pin name="INPUT_13" direction="in"/>
<pin name="INPUT_14" direction="in"/>
<pin name="INPUT_15" direction="in"/>
<pin name="INPUT_16" direction="in"/>
<pin name="INPUT_17" direction="in"/>
<pin name="INPUT_18" direction="in"/>
<pin name="INPUT_19" direction="in"/>
<pin name="INPUT_20" direction="in"/>
<pin name="INPUT_21" direction="in"/>
<pin name="INPUT_22" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_1_DIFFIO_TX0P"/>
<pin name="IO_1_DIFFIO_TX0N"/>
<pin name="IO_1_DIFFIO_TX1P"/>
<pin name="IO_1_DIFFIO_TX1N"/>
<pin name="IO_1_DIFFIO_TX2P"/>
<pin name="IO_1_DIFFIO_TX2N"/>
<pin name="IO_1_DIFFIO_TX3P"/>
<pin name="IO_1_DIFFIO_TX3N"/>
<pin name="IO_1_DIFFIO_TX4P"/>
<pin name="IO_1_DIFFIO_TX4N"/>
<pin name="IO_1_DIFFIO_TX5P"/>
<pin name="IO_1_DIFFIO_TX5N"/>
<pin name="IO_1_DIFFIO_TX6P"/>
<pin name="IO_1_DIFFIO_TX6N"/>
<pin name="IO_1_DIFFIO_TX7P"/>
<pin name="IO_1_DIFFIO_TX7N"/>
<pin name="IO_1_DIFFIO_TX8P"/>
<pin name="IO_1_DIFFIO_TX8N"/>
<pin name="IO_7_CLK7N"/>
<pin name="IO_7_DEV_CLRN"/>
<pin name="IO_7_RUP7"/>
<pin name="IO_8_RUP8"/>
<pin name="IO_8_DQ7B0"/>
<pin name="IO_8_DQ7B1"/>
<pin name="IO_8_DQ7B4"/>
<pin name="IO_8_DQ7B7"/>
<pin name="IO_8_FCLK2"/>
<pin name="IO_8_FCLK3"/>
<pin name="IO_11_PLL6_OUT1P"/>
<pin name="IO_12_PLL6_OUT2P"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_8_6"/>
<pin name="IO_8"/>
</symbol>
<symbol name="EP1SGX25CF672C7N_G">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="CLK4P" direction="in"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK6P" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_11_PLL6_OUT1N"/>
<pin name="IO_11_PLL6_FBP"/>
<pin name="IO_11_PLL6_OUT0N"/>
<pin name="IO_11_PLL6_OUT0P"/>
<pin name="IO_11_PLL6_FBN"/>
<pin name="IO_12_PLL6_OUT2N"/>
<pin name="IO_12_PLL6_OUT3P"/>
<pin name="IO_12_PLL6_OUT3N"/>
<pin name="IO_8"/>
<pin name="IO_8_DQS7B"/>
<pin name="IO_8_DQ7B6"/>
<pin name="IO_8_DQ7B3"/>
<pin name="IO_8_DQ7B2"/>
<pin name="IO_8_DQ7B5"/>
<pin name="IO_8_DQ6B2"/>
<pin name="IO_8_DQ6B1"/>
<pin name="IO_8_DQ6B3"/>
<pin name="IO_8_DQ8B1"/>
<pin name="IO_8_CLK5N"/>
<pin name="IO_8_DQ6B5"/>
<pin name="IO_8_DQS6B"/>
<pin name="IO_8_DQ6B6"/>
<pin name="IO_8_DQ8B5"/>
<pin name="IO_8_DQ8B4"/>
<pin name="IO_8_DQ9B1"/>
<pin name="IO_8_DQ9B2"/>
<pin name="IO_8_DQ9B5"/>
<pin name="IO_8_DQ6B0"/>
<pin name="IO_8_DQ6B4"/>
<pin name="IO_8_DQ6B7"/>
<pin name="IO_8_DQS8B"/>
<pin name="IO_8_DQ8B6"/>
<pin name="IO_8_DQ9B0"/>
<pin name="IO_8_DQS9B"/>
<pin name="IO_8_DQ9B6"/>
<pin name="IO_8_CLK4N"/>
<pin name="IO_8_DQ8B2"/>
<pin name="IO_8_DQ8B0"/>
<pin name="IO_8_DQ8B3"/>
<pin name="IO_8_DQ8B7"/>
<pin name="IO_8_DQ9B3"/>
<pin name="IO_8_DQ9B4"/>
<pin name="IO_8_DQ9B7"/>
<pin name="IO_7_DQ3B5"/>
<pin name="IO_7_DQ3B4"/>
<pin name="IO_7_CLK6N"/>
<pin name="IO_7_DQ3B6"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_A">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCG_B13" direction="pwr"/>
<pin name="GXB_RX5P" direction="in"/>
<pin name="GXB_RX5N" direction="in"/>
<pin name="GXB_RX4P" direction="in"/>
<pin name="GXB_RX4N" direction="in"/>
<pin name="GXB_RX6P" direction="in"/>
<pin name="GXB_RX6N" direction="in"/>
<pin name="GXB_RX7N" direction="in"/>
<pin name="GXB_RX7P" direction="in"/>
<pin name="REFCLKB13N" direction="in"/>
<pin name="REFCLKB14P" direction="in"/>
<pin name="REFCLKB14N" direction="in"/>
<pin name="RREFB13" direction="in"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC_7" direction="pas"/>
<pin name="GND/NC_8" direction="pas"/>
<pin name="GND/NC_9" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND_22" direction="pas"/>
<pin name="GXB_GND_23" direction="pas"/>
<pin name="GXB_GND_24" direction="pas"/>
<pin name="GXB_GND_25" direction="pas"/>
<pin name="GXB_GND_26" direction="pas"/>
<pin name="GXB_GND_27" direction="pas"/>
<pin name="GXB_GND_28" direction="pas"/>
<pin name="GXB_GND_29" direction="pas"/>
<pin name="GXB_GND_30" direction="pas"/>
<pin name="GXB_GND_31" direction="pas"/>
<pin name="GXB_GND_32" direction="pas"/>
<pin name="GXB_GND_33" direction="pas"/>
<pin name="GXB_GND_34" direction="pas"/>
<pin name="GXB_GND_35" direction="pas"/>
<pin name="GXB_GND_36" direction="pas"/>
<pin name="GXB_GND_37" direction="pas"/>
<pin name="GXB_GND_38" direction="pas"/>
<pin name="GXB_GND_39" direction="pas"/>
<pin name="GXB_GND_40" direction="pas"/>
<pin name="GXB_GND_41" direction="pas"/>
<pin name="GXB_GND_42" direction="pas"/>
<pin name="GXB_GND_43" direction="pas"/>
<pin name="GXB_GND_44" direction="pas"/>
<pin name="GXB_GND_45" direction="pas"/>
<pin name="GXB_GND_46" direction="pas"/>
<pin name="GXB_GND_47" direction="pas"/>
<pin name="GXB_GND_48" direction="pas"/>
<pin name="GXB_GND_49" direction="pas"/>
<pin name="GXB_GND_50" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="GXB_TX5P" direction="out"/>
<pin name="GXB_TX5N" direction="out"/>
<pin name="GXB_TX4P" direction="out"/>
<pin name="GXB_TX4N" direction="out"/>
<pin name="IO_4_DQS0T"/>
<pin name="IO_4_DQ0T5"/>
<pin name="IO_4_2"/>
<pin name="IO_4_DQ0T6"/>
<pin name="IO_4_DQ0T0"/>
<pin name="GXB_TX6P" direction="out"/>
<pin name="GXB_TX6N" direction="out"/>
<pin name="IO_4_DQ0T1"/>
<pin name="IO_4_DQ0T3"/>
<pin name="IO_4"/>
<pin name="IO_4_DQ0T2"/>
<pin name="IO_4_DQ0T4"/>
<pin name="GXB_TX7P" direction="out"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_B">
<pin name="VCCA_B14_2" direction="pwr"/>
<pin name="VCCT_B14_2" direction="pwr"/>
<pin name="VCCR_B14_2" direction="pwr"/>
<pin name="VCCP_B14_2" direction="pwr"/>
<pin name="VCCG_B14" direction="pwr"/>
<pin name="VCCT_B14_3" direction="pwr"/>
<pin name="VCCR_B14_3" direction="pwr"/>
<pin name="VCCP_B14_3" direction="pwr"/>
<pin name="VCCT_B14_4" direction="pwr"/>
<pin name="VCCR_B14_4" direction="pwr"/>
<pin name="VCCP_B14_4" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCA_B14" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="VCCA_B15" direction="pwr"/>
<pin name="VCCR_B14" direction="pwr"/>
<pin name="VCCT_B15_2" direction="pwr"/>
<pin name="VCCP_B14" direction="pwr"/>
<pin name="VCCR_B15_2" direction="pwr"/>
<pin name="VCCT_B15_3" direction="pwr"/>
<pin name="VCCP_B15_2" direction="pwr"/>
<pin name="VCCG_B15_2" direction="pwr"/>
<pin name="VCCG_B15" direction="pwr"/>
<pin name="VCCR_B15_3" direction="pwr"/>
<pin name="VCCT_B15_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCR_B15_4" direction="pwr"/>
<pin name="VCCP_B15_3" direction="pwr"/>
<pin name="VCCP_B15_4" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCR_B15" direction="pwr"/>
<pin name="VCCP_B15" direction="pwr"/>
<pin name="REFCLKB17P" direction="in"/>
<pin name="REFCLKB17N" direction="in"/>
<pin name="RREFB17" direction="in"/>
<pin name="RREFB14" direction="in"/>
<pin name="RREFB15" direction="in"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC_7" direction="pas"/>
<pin name="GND/NC_8" direction="pas"/>
<pin name="GND/NC_9" direction="pas"/>
<pin name="GND/NC_10" direction="pas"/>
<pin name="GND/NC_11" direction="pas"/>
<pin name="GND/NC_12" direction="pas"/>
<pin name="GND/NC_13" direction="pas"/>
<pin name="GND/NC_14" direction="pas"/>
<pin name="GND/NC_15" direction="pas"/>
<pin name="GND/NC_16" direction="pas"/>
<pin name="GND/NC_17" direction="pas"/>
<pin name="GND/NC_18" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND_22" direction="pas"/>
<pin name="GXB_GND_23" direction="pas"/>
<pin name="GXB_GND_24" direction="pas"/>
<pin name="GXB_GND_25" direction="pas"/>
<pin name="GXB_GND_26" direction="pas"/>
<pin name="GXB_GND_27" direction="pas"/>
<pin name="GXB_GND_28" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="GXB_TX7N" direction="out"/>
<pin name="IO_4"/>
<pin name="IO_4_DQ0T7"/>
<pin name="IO_4_DQ4T2"/>
<pin name="IO_4_DQ4T1"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_C">
<pin name="VCCA_B15_2" direction="pwr"/>
<pin name="VCCT_B15_2" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCR_B15_2" direction="pwr"/>
<pin name="VCCR_B15" direction="pwr"/>
<pin name="VCCP_B15_2" direction="pwr"/>
<pin name="VCCP_B15" direction="pwr"/>
<pin name="VCCG_B15" direction="pwr"/>
<pin name="VCCA_B15" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="REFCLKB15P" direction="in"/>
<pin name="REFCLKB15N" direction="in"/>
<pin name="RREFB16" direction="in"/>
<pin name="GXB_RX10P" direction="in"/>
<pin name="GXB_RX10N" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_RX9P" direction="in"/>
<pin name="GXB_RX9N" direction="in"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_RX8P" direction="in"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_RX8N" direction="in"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND_22" direction="pas"/>
<pin name="GXB_GND_23" direction="pas"/>
<pin name="GXB_GND_24" direction="pas"/>
<pin name="GXB_GND_25" direction="pas"/>
<pin name="GXB_GND_26" direction="pas"/>
<pin name="GXB_GND_27" direction="pas"/>
<pin name="GXB_GND_28" direction="pas"/>
<pin name="GXB_GND_29" direction="pas"/>
<pin name="GXB_GND_30" direction="pas"/>
<pin name="GXB_GND_31" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="IO_10_PLL5_OUT2N"/>
<pin name="IO_3_CLK14N"/>
<pin name="IO_3_DQ6T2"/>
<pin name="IO_3_DQ6T3"/>
<pin name="IO_3_DQ7T0"/>
<pin name="IO_3_DQ7T4"/>
<pin name="IO_3_DQ8T0"/>
<pin name="IO_3_DQ8T3"/>
<pin name="IO_3_DQ9T0"/>
<pin name="IO_3_DQS9T"/>
<pin name="IO_3_DQ9T5"/>
<pin name="GXB_TX9P" direction="out"/>
<pin name="GXB_TX9N" direction="out"/>
<pin name="GXB_TX8P" direction="out"/>
<pin name="GXB_TX8N" direction="out"/>
<pin name="IO_7_DQ0B4"/>
<pin name="IO_7_DQ0B7"/>
<pin name="IO_7"/>
<pin name="IO_7_DQ0B2"/>
<pin name="IO_7_DQ0B1"/>
<pin name="GXB_TX10P" direction="out"/>
<pin name="GXB_TX10N" direction="out"/>
<pin name="IO_7_DQ0B3"/>
<pin name="IO_7_DQ0B0"/>
<pin name="IO_7_DQ0B6"/>
<pin name="IO_7_DQS0B"/>
<pin name="GXB_TX11P" direction="out"/>
<pin name="GXB_TX11N" direction="out"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="CLK14P" direction="in"/>
<pin name="CLK15P" direction="in"/>
<pin name="CLK12P" direction="in"/>
<pin name="REFCLKB16P" direction="in"/>
<pin name="REFCLKB16N" direction="in"/>
<pin name="GXB_RX11P" direction="in"/>
<pin name="GXB_RX11N" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC_7" direction="pas"/>
<pin name="GND/NC_8" direction="pas"/>
<pin name="GND/NC_9" direction="pas"/>
<pin name="GND/NC_10" direction="pas"/>
<pin name="GND/NC_11" direction="pas"/>
<pin name="GND/NC_12" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND_5" direction="pas"/>
<pin name="GXB_GND_6" direction="pas"/>
<pin name="GXB_GND_7" direction="pas"/>
<pin name="GXB_GND_8" direction="pas"/>
<pin name="GXB_GND_9" direction="pas"/>
<pin name="GXB_GND_10" direction="pas"/>
<pin name="GXB_GND_11" direction="pas"/>
<pin name="GXB_GND_12" direction="pas"/>
<pin name="GXB_GND_13" direction="pas"/>
<pin name="GXB_GND_14" direction="pas"/>
<pin name="GXB_GND_15" direction="pas"/>
<pin name="GXB_GND_16" direction="pas"/>
<pin name="GXB_GND_17" direction="pas"/>
<pin name="GXB_GND_18" direction="pas"/>
<pin name="GXB_GND_19" direction="pas"/>
<pin name="GXB_GND_20" direction="pas"/>
<pin name="GXB_GND_21" direction="pas"/>
<pin name="GXB_GND_22" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_4_DQS4T"/>
<pin name="IO_4_DQ4T3"/>
<pin name="IO_10_PLL5_OUT2P"/>
<pin name="IO_3_CLK15N"/>
<pin name="IO_3_DQ5T4"/>
<pin name="IO_3_DQS6T"/>
<pin name="IO_3_DQ6T6"/>
<pin name="IO_3_DQ7T1"/>
<pin name="IO_3_DQ7T5"/>
<pin name="IO_3_DQ8T1"/>
<pin name="IO_3_DQ8T5"/>
<pin name="IO_3_DQ9T1"/>
<pin name="IO_3_DQ9T3"/>
<pin name="IO_3_DQ9T6"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_4_DQ4T0"/>
<pin name="IO_4_DQ4T4"/>
<pin name="IO_4_CLK12N"/>
<pin name="IO_9_PLL5_OUT1N"/>
<pin name="IO_10_PLL5_OUT3N"/>
<pin name="IO_3_DQ5T5"/>
<pin name="IO_3_DQ6T0"/>
<pin name="IO_3_DQ6T4"/>
<pin name="IO_3_DQ7T2"/>
<pin name="IO_3_DQ7T6"/>
<pin name="IO_3_DQ8T2"/>
<pin name="IO_3_DQ8T6"/>
<pin name="IO_3_DQ9T2"/>
<pin name="IO_3_DQ9T4"/>
<pin name="IO_3_DQ9T7"/>
<pin name="IO_3_4"/>
<pin name="IO_3_5"/>
<pin name="IO_4_DQ3T1"/>
<pin name="IO_4_DQ4T6"/>
<pin name="IO_9_PLL5_OUT1P"/>
<pin name="IO_10_PLL5_OUT3P"/>
<pin name="IO_3_DQ5T3"/>
<pin name="IO_3_DQ5T6"/>
<pin name="IO_3_DQ6T1"/>
<pin name="IO_3_DQ6T5"/>
<pin name="IO_3_DQS7T"/>
<pin name="IO_3_DQ7T7"/>
<pin name="IO_3_DQS8T"/>
<pin name="IO_3_DQ8T7"/>
<pin name="IO_3"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_E">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="CLK13P" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO_3_2"/>
<pin name="IN_2_DIFFIO_RX44P"/>
<pin name="IN_2_DIFFIO_RX44N"/>
<pin name="IN_2_DIFFIO_RX43P"/>
<pin name="IN_2_DIFFIO_RX43N"/>
<pin name="IO_4_DQ3T3"/>
<pin name="IO_4_DQ4T7"/>
<pin name="IO_4_CLK13N/PLL11_OUT"/>
<pin name="IO_9_PLL5_FBN"/>
<pin name="IO_9_PLL5_OUT0N"/>
<pin name="IO_3_DQ5T0"/>
<pin name="IO_3_DQ5T2"/>
<pin name="IO_3_DQ5T7"/>
<pin name="IO_3_DQ6T7"/>
<pin name="IO_3_DQ7T3"/>
<pin name="IO_3_3"/>
<pin name="IO_3_DQ8T4"/>
<pin name="IO_3_4"/>
<pin name="IO_3_5"/>
<pin name="IO_3_6"/>
<pin name="IN_2_DIFFIO_RX41P"/>
<pin name="IN_2_DIFFIO_RX41N"/>
<pin name="IO_4_DQ3T2"/>
<pin name="IO_4_DQ4T5"/>
<pin name="IO_9_PLL5_FBP"/>
<pin name="IO_9_PLL5_OUT0P"/>
<pin name="IO_3_DQ5T1"/>
<pin name="IO_3_DQS5T"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_3_7"/>
<pin name="IO_3_8"/>
<pin name="IO_3_9"/>
<pin name="IO_3_10"/>
<pin name="IO_3_11"/>
<pin name="IO_3_12"/>
<pin name="IO_2_DIFFIO_TX44P"/>
<pin name="IO_2_DIFFIO_TX44N"/>
<pin name="IN_2_DIFFIO_RX42P"/>
<pin name="IN_2_DIFFIO_RX42N"/>
<pin name="IN_2_DIFFIO_RX40P"/>
<pin name="IN_2_DIFFIO_RX40N"/>
<pin name="IO_4_DQ1T2"/>
<pin name="IO_4_DQ1T7"/>
<pin name="IO_4_DQ2T2"/>
<pin name="IO_4_DQ3T0"/>
<pin name="IO_4_DQS3T"/>
<pin name="IO_4_DQ3T6"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_3_13"/>
<pin name="IO_3_RDN3"/>
<pin name="IO_3_FCLK0"/>
<pin name="IO_3_14"/>
<pin name="IO_3_15"/>
<pin name="IO_2_DIFFIO_TX42P"/>
<pin name="IO_2_DIFFIO_TX42N"/>
<pin name="IO_2_DIFFIO_TX43P"/>
<pin name="IO_2_DIFFIO_TX43N"/>
<pin name="IN_2_DIFFIO_RX39P"/>
<pin name="IN_2_DIFFIO_RX39N"/>
<pin name="IN_2_DIFFIO_RX38P"/>
<pin name="IN_2_DIFFIO_RX38N"/>
<pin name="IO_4_DQS1T"/>
<pin name="IO_4_DQ1T4"/>
<pin name="IO_4_DQS2T"/>
<pin name="IO_4_DQ2T4"/>
<pin name="IO_4_DQ3T4"/>
<pin name="IO_4_DQ3T7"/>
<pin name="IO_4_5"/>
<pin name="IO_4"/>
<pin name="IO_4_RUP4"/>
<pin name="IO_3_16"/>
<pin name="IO_3_RUP3"/>
<pin name="IO_3_FCLK1"/>
<pin name="IO_3"/>
<pin name="IO_2_DIFFIO_TX39P"/>
<pin name="IO_2_DIFFIO_TX39N"/>
<pin name="IO_2_DIFFIO_TX40P"/>
<pin name="IO_2_DIFFIO_TX40N"/>
<pin name="IO_2_DIFFIO_TX41N"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_F">
<pin name="VCCG_PLL7" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="VCCG_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUTA" direction="pwr"/>
<pin name="VCCG_PLL11" direction="pwr"/>
<pin name="VCC_PLL5_OUTB" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="VREF0B3" direction="in"/>
<pin name="VREF1B3" direction="in"/>
<pin name="VREF2B3" direction="in"/>
<pin name="VREF3B3" direction="in"/>
<pin name="VREF0B2" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL7" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="GNDG_PLL11" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="GNDG_PLL5" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="IN_2_DIFFIO_RX37P"/>
<pin name="IN_2_DIFFIO_RX37N"/>
<pin name="IN_2_DIFFIO_RX35P"/>
<pin name="IN_2_DIFFIO_RX35N"/>
<pin name="IO_4_DQ1T0"/>
<pin name="IO_4_DQ1T5"/>
<pin name="IO_4_DQ2T0"/>
<pin name="IO_4_DQ2T5"/>
<pin name="IO_4_DQ3T5"/>
<pin name="TDO" direction="out"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_3_2"/>
<pin name="IO_3"/>
<pin name="IO_2_DIFFIO_TX24N"/>
<pin name="IO_2_DIFFIO_TX37P"/>
<pin name="IO_2_DIFFIO_TX37N"/>
<pin name="IO_2_DIFFIO_TX41P"/>
<pin name="IN_2_DIFFIO_RX33P"/>
<pin name="IN_2_DIFFIO_RX33N"/>
<pin name="IN_2_DIFFIO_RX34P"/>
<pin name="IN_2_DIFFIO_RX34N"/>
<pin name="IO_4_DQ1T1"/>
<pin name="IO_4_DQ1T3"/>
<pin name="IO_4_DQ2T1"/>
<pin name="IO_4_DQ2T7"/>
<pin name="IO_4_RDN4"/>
<pin name="IO_4_4"/>
<pin name="CONF_DONE"/>
<pin name="IO_2_DIFFIO_TX24P"/>
<pin name="IO_2_DIFFIO_TX36P"/>
<pin name="IO_2_DIFFIO_TX36N"/>
<pin name="IO_2_DIFFIO_TX38N"/>
<pin name="IN_2_DIFFIO_RX36P"/>
<pin name="IN_2_DIFFIO_RX36N"/>
<pin name="IN_2_DIFFIO_RX28P"/>
<pin name="IN_2_DIFFIO_RX28N"/>
<pin name="IO_4_5"/>
<pin name="IO_4_DQ1T6"/>
<pin name="IO_4_DQ2T3"/>
<pin name="IO_4_DQ2T6"/>
<pin name="IO_4_6"/>
<pin name="IO_4_7"/>
<pin name="IO_4_8"/>
<pin name="NSTATUS"/>
<pin name="IO_2_DIFFIO_TX23N"/>
<pin name="IO_2_DIFFIO_TX35P"/>
<pin name="IO_2_DIFFIO_TX35N"/>
<pin name="IO_2_DIFFIO_TX34P"/>
<pin name="IO_2_DIFFIO_TX34N"/>
<pin name="IO_2_DIFFIO_TX38P"/>
<pin name="IN_2_DIFFIO_RX32P/RUP2"/>
<pin name="IN_2_DIFFIO_RX32N/RDN2"/>
<pin name="IN_2_DIFFIO_RX31P"/>
<pin name="IN_2_DIFFIO_RX31N"/>
<pin name="IO_4_9"/>
<pin name="IO_4_10"/>
<pin name="IO_4_11"/>
<pin name="IO_4_FCLK6"/>
<pin name="IO_4_DEV_OE"/>
<pin name="IO_4"/>
<pin name="IO_2_DIFFIO_TX23P"/>
<pin name="IO_2_DIFFIO_TX33P"/>
<pin name="IO_2_DIFFIO_TX33N"/>
<pin name="IO_2_DIFFIO_TX32P"/>
<pin name="IO_2_DIFFIO_TX32N"/>
<pin name="IN_2_DIFFIO_RX30P"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_G">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCG_PLL1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREF0B4" direction="in"/>
<pin name="VREF1B2" direction="in"/>
<pin name="VREF2B2" direction="in"/>
<pin name="VREF1B4" direction="in"/>
<pin name="VREF2B4" direction="in"/>
<pin name="VREF3B4" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IN_2_DIFFIO_RX30N"/>
<pin name="IN_2_DIFFIO_RX27P"/>
<pin name="IN_2_DIFFIO_RX27N"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4_5"/>
<pin name="IO_4_6"/>
<pin name="IO_2_DIFFIO_TX31P"/>
<pin name="IO_2_DIFFIO_TX31N"/>
<pin name="IO_2_DIFFIO_TX30P"/>
<pin name="IO_2_DIFFIO_TX30N"/>
<pin name="IN_2_DIFFIO_RX29P"/>
<pin name="IN_2_DIFFIO_RX29N"/>
<pin name="IN_2_DIFFIO_RX25P"/>
<pin name="IN_2_DIFFIO_RX25N"/>
<pin name="IO_4_7"/>
<pin name="IO_4_8"/>
<pin name="IO_4_9"/>
<pin name="IO_4_10"/>
<pin name="IO_4_11"/>
<pin name="IO_2_DIFFIO_TX28P"/>
<pin name="IO_2_DIFFIO_TX29P"/>
<pin name="IO_2_DIFFIO_TX29N"/>
<pin name="IO_2_DIFFIO_TX27P"/>
<pin name="IO_2_DIFFIO_TX27N"/>
<pin name="IN_2_DIFFIO_RX26P"/>
<pin name="IN_2_DIFFIO_RX26N"/>
<pin name="IN_2_DIFFIO_RX24P"/>
<pin name="IO_4_12"/>
<pin name="IO_4_13"/>
<pin name="IO_4_14"/>
<pin name="IO_4_15"/>
<pin name="IO_4_16"/>
<pin name="IO_2_DIFFIO_TX28N"/>
<pin name="IO_2_DIFFIO_TX25P"/>
<pin name="IO_2_DIFFIO_TX25N"/>
<pin name="IO_2_DIFFIO_TX26P"/>
<pin name="IO_2_DIFFIO_TX26N"/>
<pin name="IN_2_DIFFIO_RX23P"/>
<pin name="IN_2_DIFFIO_RX23N"/>
<pin name="IN_2_DIFFIO_RX24N"/>
<pin name="IO_4_17"/>
<pin name="IO_4"/>
<pin name="IO_4_FCLK7"/>
<pin name="IO_1_DIFFIO_TX22P"/>
<pin name="IO_2_CLK1N"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_H">
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCG_PLL2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK0P" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="CLK0N" direction="in"/>
<pin name="CLK2P" direction="in"/>
<pin name="CLK2N" direction="in"/>
<pin name="VREF3B7" direction="in"/>
<pin name="VREF2B7" direction="in"/>
<pin name="VREF1B7" direction="in"/>
<pin name="VREF0B7" direction="in"/>
<pin name="VREF1B1" direction="in"/>
<pin name="VREF0B1" direction="in"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDG_PLL2" direction="pas"/>
<pin name="IO_4"/>
<pin name="IO_7_2"/>
<pin name="IO_7_FCLK4"/>
<pin name="IO_1_DIFFIO_TX22N"/>
<pin name="IO_1_CLK3N"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_7_7"/>
<pin name="IO_1_DIFFIO_TX17P"/>
<pin name="IO_1_DIFFIO_TX18P"/>
<pin name="IO_1_DIFFIO_TX18N"/>
<pin name="IO_1_DIFFIO_TX19P"/>
<pin name="IO_1_DIFFIO_TX19N"/>
<pin name="IN_1_DIFFIO_RX22P"/>
<pin name="IN_1_DIFFIO_RX22N"/>
<pin name="IN_1_DIFFIO_RX21P"/>
<pin name="IO_7_8"/>
<pin name="IO_7_9"/>
<pin name="IO_7_10"/>
<pin name="IO_7_11"/>
<pin name="IO_7_12"/>
<pin name="IO_1_DIFFIO_TX17N"/>
<pin name="IO_1_DIFFIO_TX15P"/>
<pin name="IO_1_DIFFIO_TX15N"/>
<pin name="IO_1_DIFFIO_TX16P"/>
<pin name="IO_1_DIFFIO_TX16N"/>
<pin name="IN_1_DIFFIO_RX19P"/>
<pin name="IN_1_DIFFIO_RX19N"/>
<pin name="IN_1_DIFFIO_RX21N"/>
<pin name="IO_7_13"/>
<pin name="IO_7_14"/>
<pin name="IO_7_15"/>
<pin name="IO_7_16"/>
<pin name="IO_7"/>
<pin name="IO_1_DIFFIO_TX14P"/>
<pin name="IO_1_DIFFIO_TX14N"/>
<pin name="IO_1_DIFFIO_TX13P"/>
<pin name="IO_1_DIFFIO_TX13N"/>
<pin name="IN_1_DIFFIO_RX16P"/>
<pin name="IN_1_DIFFIO_RX16N"/>
<pin name="IN_1_DIFFIO_RX20P"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_I">
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCCG_PLL6" direction="pwr"/>
<pin name="VCCG_PLL8" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCG_PLL12" direction="pwr"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="VREF3B8" direction="in"/>
<pin name="VREF2B8" direction="in"/>
<pin name="VREF1B8" direction="in"/>
<pin name="VREF0B8" direction="in"/>
<pin name="VREF2B1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="IN_1_DIFFIO_RX20N"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_1_DIFFIO_TX21P"/>
<pin name="IO_1_DIFFIO_TX12P"/>
<pin name="IO_1_DIFFIO_TX12N"/>
<pin name="IO_1_DIFFIO_TX11P"/>
<pin name="IO_1_DIFFIO_TX11N"/>
<pin name="IN_1_DIFFIO_RX14P"/>
<pin name="IN_1_DIFFIO_RX14N"/>
<pin name="IN_1_DIFFIO_RX18P"/>
<pin name="IN_1_DIFFIO_RX18N"/>
<pin name="IO_7_7"/>
<pin name="GNDG_PLL12" direction="pas"/>
<pin name="GNDG_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDG_PLL8" direction="pas"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="VCC_PLL6_OUTB" direction="pwr"/>
<pin name="VCC_PLL6_OUTA" direction="pwr"/>
<pin name="IO_7_DQ1B6"/>
<pin name="IO_7_DQ1B5"/>
<pin name="IO_7_DQ2B3"/>
<pin name="IO_7_8"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_1_DIFFIO_TX21N"/>
<pin name="IO_1_DIFFIO_TX9P"/>
<pin name="IO_1_DIFFIO_TX9N"/>
<pin name="IO_1_DIFFIO_TX10P"/>
<pin name="IO_1_DIFFIO_TX10N"/>
<pin name="IO_1_DIFFIO_TX6P"/>
<pin name="IN_1_DIFFIO_RX13P/RUP1"/>
<pin name="IN_1_DIFFIO_RX13N/RDN1"/>
<pin name="IN_1_DIFFIO_RX15P"/>
<pin name="IN_1_DIFFIO_RX15N"/>
<pin name="IO_7_DQ1B1"/>
<pin name="IO_7_DQ1B3"/>
<pin name="IO_7_DQ2B1"/>
<pin name="IO_7_DQ2B6"/>
<pin name="IO_7_RDN7"/>
<pin name="IO_7_9"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_1_DIFFIO_TX20P"/>
<pin name="IO_1_DIFFIO_TX8P"/>
<pin name="IO_1_DIFFIO_TX8N"/>
<pin name="IO_1_DIFFIO_TX6N"/>
<pin name="IN_1_DIFFIO_RX12P"/>
<pin name="IN_1_DIFFIO_RX12N"/>
<pin name="IN_1_DIFFIO_RX17P"/>
<pin name="IN_1_DIFFIO_RX17N"/>
<pin name="IO_7_DQ1B0"/>
<pin name="IO_7_DQS1B"/>
<pin name="IO_7_DQ2B0"/>
<pin name="IO_7_DQ2B7"/>
<pin name="IO_7_DEV_CLRN"/>
<pin name="IO_7_10"/>
<pin name="IO_7_11"/>
<pin name="IO_7"/>
<pin name="IO_8_RDN8"/>
<pin name="IO_8"/>
<pin name="IO_1_DIFFIO_TX20N"/>
<pin name="IO_1_DIFFIO_TX7P"/>
<pin name="IO_1_DIFFIO_TX7N"/>
<pin name="IO_1_DIFFIO_TX3P"/>
<pin name="IN_1_DIFFIO_RX8P"/>
<pin name="IN_1_DIFFIO_RX8N"/>
<pin name="IN_1_DIFFIO_RX11P"/>
<pin name="IN_1_DIFFIO_RX11N"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_J">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK7P" direction="in"/>
<pin name="FPLL8CLKP" direction="in"/>
<pin name="FPLL8CLKN" direction="in"/>
<pin name="IO_7_DQ1B2"/>
<pin name="IO_7_DQ1B4"/>
<pin name="IO_7_DQS2B"/>
<pin name="IO_7_DQ2B5"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="NCEO" direction="out"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_FCLK3"/>
<pin name="IO_8_4"/>
<pin name="IO_1_DIFFIO_TX5P"/>
<pin name="IO_1_DIFFIO_TX5N"/>
<pin name="IO_1_DIFFIO_TX4P"/>
<pin name="IO_1_DIFFIO_TX4N"/>
<pin name="IO_1_DIFFIO_TX3N"/>
<pin name="IN_1_DIFFIO_RX9P"/>
<pin name="IN_1_DIFFIO_RX9N"/>
<pin name="IN_1_DIFFIO_RX10P"/>
<pin name="IN_1_DIFFIO_RX10N"/>
<pin name="IO_7_DQ0B5"/>
<pin name="IO_7_DQ1B7"/>
<pin name="IO_7_DQ2B2"/>
<pin name="IO_7_DQ2B4"/>
<pin name="IO_7_7"/>
<pin name="IO_7_FCLK5"/>
<pin name="IO_7_8"/>
<pin name="IO_7_9"/>
<pin name="IO_7"/>
<pin name="IO_7_RUP7"/>
<pin name="IO_8_RUP8"/>
<pin name="IO_8_5"/>
<pin name="IO_8_FCLK2"/>
<pin name="IO_8_6"/>
<pin name="IO_8_7"/>
<pin name="IO_1_DIFFIO_TX2P"/>
<pin name="IO_1_DIFFIO_TX2N"/>
<pin name="IO_1_DIFFIO_TX1P"/>
<pin name="IO_1_DIFFIO_TX1N"/>
<pin name="IN_1_DIFFIO_RX7P"/>
<pin name="IN_1_DIFFIO_RX7N"/>
<pin name="IN_1_DIFFIO_RX6P"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IN_1_DIFFIO_RX6N"/>
<pin name="IO_7_DQ3B0"/>
<pin name="IO_7_DQ3B7"/>
<pin name="IO_7_DQ4B7"/>
<pin name="IO_11_PLL6_FBP"/>
<pin name="IO_12_PLL6_OUT3P"/>
<pin name="IO_8_DQ5B1"/>
<pin name="IO_8_DQS5B"/>
<pin name="IO_8_8"/>
<pin name="IO_8_9"/>
<pin name="IO_8_10"/>
<pin name="IO_8_11"/>
<pin name="IO_1_2"/>
<pin name="IO_1"/>
<pin name="IO_1_DIFFIO_TX0P"/>
<pin name="IO_1_DIFFIO_TX0N"/>
<pin name="IN_1_DIFFIO_RX4P"/>
<pin name="IN_1_DIFFIO_RX4N"/>
<pin name="IN_1_DIFFIO_RX5P"/>
<pin name="IN_1_DIFFIO_RX5N"/>
<pin name="IO_7_DQS3B"/>
<pin name="IO_7_DQ3B6"/>
<pin name="IO_7_DQ4B5"/>
<pin name="IO_7_CLK7N"/>
<pin name="IO_11_PLL6_FBN"/>
<pin name="IO_12_PLL6_OUT3N"/>
<pin name="IO_8_DQ5B0"/>
<pin name="IO_8_DQ5B2"/>
<pin name="IO_8_DQ5B7"/>
<pin name="IO_8_DQ6B7"/>
<pin name="IO_8_DQ7B3"/>
<pin name="IO_8_12"/>
<pin name="IO_8_DQ8B4"/>
<pin name="IO_8"/>
<pin name="IN_1_DIFFIO_RX0P"/>
<pin name="IN_1_DIFFIO_RX0N"/>
<pin name="IN_1_DIFFIO_RX3P"/>
<pin name="IN_1_DIFFIO_RX3N"/>
</symbol>
<symbol name="EP1SGX40GF1020C6N_K">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="CLK6P" direction="in"/>
<pin name="CLK5P" direction="in"/>
<pin name="CLK4P" direction="in"/>
<pin name="IO_7_DQ3B2"/>
<pin name="IO_7_DQ3B3"/>
<pin name="IO_7_DQ4B6"/>
<pin name="IO_11_PLL6_OUT1P"/>
<pin name="IO_12_PLL6_OUT2P"/>
<pin name="IO_8_DQ5B3"/>
<pin name="IO_8_DQ5B6"/>
<pin name="IO_8_DQ6B1"/>
<pin name="IO_8_DQ6B5"/>
<pin name="IO_8_DQS7B"/>
<pin name="IO_8_DQ7B7"/>
<pin name="IO_8_DQS8B"/>
<pin name="IO_8_DQ8B7"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IN_1_DIFFIO_RX1P"/>
<pin name="IN_1_DIFFIO_RX1N"/>
<pin name="IN_1_DIFFIO_RX2P"/>
<pin name="IN_1_DIFFIO_RX2N"/>
<pin name="IO_7_DQ3B1"/>
<pin name="IO_7_DQ4B0"/>
<pin name="IO_7_DQ4B4"/>
<pin name="IO_7_CLK6N/PLL12_OUT"/>
<pin name="IO_11_PLL6_OUT1N"/>
<pin name="IO_12_PLL6_OUT2N"/>
<pin name="IO_8_DQ5B5"/>
<pin name="IO_8_DQ6B0"/>
<pin name="IO_8_DQ6B4"/>
<pin name="IO_8_DQ7B2"/>
<pin name="IO_8_DQ7B6"/>
<pin name="IO_8_DQ8B2"/>
<pin name="IO_8_DQ8B6"/>
<pin name="IO_8_DQ9B2"/>
<pin name="IO_8_DQ9B4"/>
<pin name="IO_8_DQ9B7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="GXB_GND_2" direction="pas"/>
<pin name="GXB_GND_3" direction="pas"/>
<pin name="GXB_GND_4" direction="pas"/>
<pin name="GXB_GND" direction="pas"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_7_DQ3B5"/>
<pin name="IO_7_DQS4B"/>
<pin name="IO_7_DQ4B3"/>
<pin name="IO_11_PLL6_OUT0P"/>
<pin name="IO_8_CLK5N"/>
<pin name="IO_8_DQ5B4"/>
<pin name="IO_8_DQS6B"/>
<pin name="IO_8_DQ6B6"/>
<pin name="IO_8_DQ7B1"/>
<pin name="IO_8_DQ7B5"/>
<pin name="IO_8_DQ8B1"/>
<pin name="IO_8_DQ8B5"/>
<pin name="IO_8_DQ9B1"/>
<pin name="IO_8_DQ9B3"/>
<pin name="IO_8_DQ9B6"/>
<pin name="IO_7_DQ3B4"/>
<pin name="IO_7_DQ4B2"/>
<pin name="IO_7_DQ4B1"/>
<pin name="IO_11_PLL6_OUT0N"/>
<pin name="IO_8_CLK4N"/>
<pin name="IO_8_DQ6B2"/>
<pin name="IO_8_DQ6B3"/>
<pin name="IO_8_DQ7B0"/>
<pin name="IO_8_DQ7B4"/>
<pin name="IO_8_DQ8B0"/>
<pin name="IO_8_DQ8B3"/>
<pin name="IO_8_DQ9B0"/>
<pin name="IO_8_DQS9B"/>
<pin name="IO_8_DQ9B5"/>
<pin name="IO_8_6"/>
<pin name="IO_8"/>
</symbol>
<symbol name="EP2C15AF256I8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C15AF256I8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C15AF256I8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F256C8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pas"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="DCLK" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F256C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pas"/>
<pin name="VCCA_PLL1" direction="pas"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F256C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pas"/>
<pin name="VCCD_PLL2" direction="pas"/>
<pin name="VCCD_PLL4" direction="pas"/>
<pin name="VCCA_PLL4" direction="pas"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F256I8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pas"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="DCLK" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F256I8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pas"/>
<pin name="VCCA_PLL1" direction="pas"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F256I8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pas"/>
<pin name="VCCD_PLL2" direction="pas"/>
<pin name="VCCD_PLL4" direction="pas"/>
<pin name="VCCA_PLL4" direction="pas"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484C8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C20F484C8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK9" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484C8N_C">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK11" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484C8N_E">
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484I8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C20F484I8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK9" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484I8N_C">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK11" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484I8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C20F484I8N_E">
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484C8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C35F484C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484C8N_C">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484C8N_E">
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484I8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C35F484I8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484I8N_C">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484I8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F484I8N_E">
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3_4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO_78"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="pas"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_C">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_D">
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4_5" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_E">
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO5_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCINT_20" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_F">
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35F672I8N_G">
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="NC" direction="nc"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484C8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C35U484C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484C8N_C">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484C8N_E">
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484I8N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="DCLK" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C35U484I8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484I8N_C">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484I8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C35U484I8N_E">
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50F484C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C50F484C8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO_60" direction="pas"/>
<pin name="IO_61" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP2C50F484C8N_C">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO_60" direction="pas"/>
<pin name="IO_61" direction="pas"/>
<pin name="IO_62" direction="pas"/>
<pin name="IO_63" direction="pas"/>
<pin name="IO_64" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP2C50F484C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_20" direction="pwr"/>
<pin name="VCCINT_21" direction="pwr"/>
<pin name="VCCINT_22" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_23" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50F484C8N_E">
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50F484I8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2C50F484I8N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO_60" direction="pas"/>
<pin name="IO_61" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP2C50F484I8N_C">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO_59" direction="pas"/>
<pin name="IO_60" direction="pas"/>
<pin name="IO_61" direction="pas"/>
<pin name="IO_62" direction="pas"/>
<pin name="IO_63" direction="pas"/>
<pin name="IO_64" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EP2C50F484I8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_20" direction="pwr"/>
<pin name="VCCINT_21" direction="pwr"/>
<pin name="VCCINT_22" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_23" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50F484I8N_E">
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="CLK15" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50U484C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL3_2" direction="pas"/>
<pin name="GND_PLL3" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50U484C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50U484C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50U484C8N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCINT_20" direction="pwr"/>
<pin name="VCCINT_21" direction="pwr"/>
<pin name="VCCINT_22" direction="pwr"/>
<pin name="VCCINT_23" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C50U484C8N_E">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCIO7_5" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL4_2" direction="pas"/>
<pin name="GND_PLL4" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5F256C8_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EP2C5F256C8_B">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5F256C8_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5Q208C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5Q208C8N_B">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5Q208C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCIO2_5" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5Q208I8_A">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="GND_2" direction="in"/>
<pin name="GND_3" direction="in"/>
<pin name="GND_4" direction="in"/>
<pin name="GND_5" direction="in"/>
<pin name="GND_6" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="GNDA_PLL1" direction="in"/>
<pin name="GND_PLL1_2" direction="in"/>
<pin name="GND_PLL1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5Q208I8_B">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="GND_2" direction="in"/>
<pin name="GND_3" direction="in"/>
<pin name="GND_4" direction="in"/>
<pin name="GND_5" direction="in"/>
<pin name="GND_6" direction="in"/>
<pin name="GND_7" direction="in"/>
<pin name="GND_8" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5Q208I8_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCIO2_5" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="GND_2" direction="in"/>
<pin name="GND_3" direction="in"/>
<pin name="GND_4" direction="in"/>
<pin name="GND_5" direction="in"/>
<pin name="GND_6" direction="in"/>
<pin name="GND_7" direction="in"/>
<pin name="GND_8" direction="in"/>
<pin name="GND_9" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="GNDA_PLL2" direction="in"/>
<pin name="GND_PLL2_2" direction="in"/>
<pin name="GND_PLL2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5T144C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C5T144C8N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C8Q208C8N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C8Q208C8N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="NSTATUS"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C8Q208C8N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCIO2_5" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C8T144C8N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="DATA0" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GND_PLL1_2" direction="pas"/>
<pin name="GND_PLL1" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2C8T144C8N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND_PLL2_2" direction="pas"/>
<pin name="GND_PLL2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C3N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VREFB5N0" direction="pas"/>
<pin name="VREFB4N0" direction="pas"/>
<pin name="VREFB4N1" direction="pas"/>
<pin name="VREFB5N1" direction="pas"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="MSEL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C3N_B">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VREFB6N1" direction="pas"/>
<pin name="VREFB6N0" direction="pas"/>
<pin name="VREFB7N1" direction="pas"/>
<pin name="VREFB7N0" direction="pas"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C3N_C">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VREFB2N0" direction="pas"/>
<pin name="VREFB3N0" direction="pas"/>
<pin name="VREFB3N1" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
</symbol>
<symbol name="EP2S15F484C3N_D">
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
</symbol>
<symbol name="EP2S15F484C3N_E">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TRST" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="VREFB1N1" direction="pas"/>
<pin name="VREFB1N0" direction="pas"/>
<pin name="VREFB8N0" direction="pas"/>
<pin name="VREFB8N1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C5N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C5N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C5N_C">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="NCEO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C5N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F484C5N_E">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F672C3N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F672C3N_B">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F672C3N_C">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F672C3N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC_39" direction="nc"/>
<pin name="NC_40" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F672C3N_E">
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EP2S15F672C3N_F">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S15F672C3N_G">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCD_PLL10" direction="pwr"/>
<pin name="VCCA_PLL10" direction="pwr"/>
<pin name="FPLL10CLKP" direction="in"/>
<pin name="FPLL10CLKN" direction="in"/>
<pin name="VREFB4N0" direction="pas"/>
<pin name="VREFB5N2" direction="pas"/>
<pin name="VREFB4N2" direction="pas"/>
<pin name="VREFB4N1" direction="pas"/>
<pin name="VREFB5N4" direction="pas"/>
<pin name="VREFB5N3" direction="pas"/>
<pin name="VREFB5N1" direction="pas"/>
<pin name="TEMPDIODEN" direction="pas"/>
<pin name="TEMPDIODEP" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL10_2" direction="pas"/>
<pin name="GNDA_PLL10" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_B">
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VREFB5N0" direction="pas"/>
<pin name="VREFB6N4" direction="pas"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_C">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL9" direction="pwr"/>
<pin name="VCCD_PLL9" direction="pwr"/>
<pin name="VREFB7N3" direction="pas"/>
<pin name="VREFB6N2" direction="pas"/>
<pin name="VREFB6N1" direction="pas"/>
<pin name="VREFB6N3" direction="pas"/>
<pin name="VREFB6N0" direction="pas"/>
<pin name="FPLL9CLKP" direction="in"/>
<pin name="FPLL9CLKN" direction="in"/>
<pin name="PLL_ENA" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL9_2" direction="pas"/>
<pin name="GNDA_PLL9" direction="pas"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_D">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VREFB4N4" direction="pas"/>
<pin name="VREFB3N0" direction="pas"/>
<pin name="VREFB7N2" direction="pas"/>
<pin name="VREFB3N4" direction="pas"/>
<pin name="VREFB7N4" direction="pas"/>
<pin name="VREFB3N2" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_E">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCD_PLL7" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VREFB3N3" direction="pas"/>
<pin name="VREFB3N1" direction="pas"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="VREFB4N3" direction="pas"/>
<pin name="MSEL3" direction="pas"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL7_2" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL11_2" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_F">
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCC_PLL11_OUT" direction="pwr"/>
<pin name="VCCD_PLL11" direction="pwr"/>
<pin name="VCCPD4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="VREFB2N2" direction="pas"/>
<pin name="VREFB2N3" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_G">
<pin name="VCCPD5_2" direction="pwr"/>
<pin name="VCCPD2_2" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB2N4" direction="pas"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_H">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD6_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCPD1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB1N0" direction="pas"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_I">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD7_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8_2" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB1N1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_J">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL12" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCC_PLL12_OUT" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCCD_PLL8" direction="pwr"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="VREFB7N1" direction="pas"/>
<pin name="VREFB1N3" direction="pas"/>
<pin name="VREFB1N2" direction="pas"/>
<pin name="VREFB8N2" direction="pas"/>
<pin name="VREFB8N1" direction="pas"/>
<pin name="VREFB1N4" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="GNDA_PLL8_2" direction="pas"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S180F1020C3N_K">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VREFB8N3" direction="pas"/>
<pin name="VREFB8N0" direction="pas"/>
<pin name="VREFB7N0" direction="pas"/>
<pin name="VREFB8N4" direction="pas"/>
<pin name="FPLL8CLKN" direction="in"/>
<pin name="FPLL8CLKP" direction="in"/>
<pin name="TRST" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C3N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C3N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C3N_C">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="NCEO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C3N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C3N_E">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C5N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C5N_B">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCIO6_2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C5N_C">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="NCEO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C5N_D">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F484C5N_E">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C3N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C3N_B">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C3N_C">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C3N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC_39" direction="nc"/>
<pin name="NC_40" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C3N_E">
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EP2S30F672C3N_F">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C3N_G">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C5N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C5N_B">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C5N_C">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C5N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC_39" direction="nc"/>
<pin name="NC_40" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C5N_E">
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EP2S30F672C5N_F">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S30F672C5N_G">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCD_PLL10" direction="pwr"/>
<pin name="VCCA_PLL10" direction="pwr"/>
<pin name="VREFB4N0" direction="pas"/>
<pin name="VREFB4N1" direction="pas"/>
<pin name="VREFB5N2" direction="pas"/>
<pin name="VREFB5N1" direction="pas"/>
<pin name="TEMPDIODEN" direction="pas"/>
<pin name="TEMPDIODEP" direction="pas"/>
<pin name="FPLL10CLKP" direction="in"/>
<pin name="FPLL10CLKN" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL10_2" direction="pas"/>
<pin name="GNDA_PLL10" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_B">
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="VREFB5N0" direction="pas"/>
<pin name="VREFB6N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_C">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL9" direction="pwr"/>
<pin name="VCCD_PLL9" direction="pwr"/>
<pin name="PLL_ENA" direction="pas"/>
<pin name="FPLL9CLKP" direction="in"/>
<pin name="FPLL9CLKN" direction="in"/>
<pin name="VREFB6N1" direction="pas"/>
<pin name="VREFB6N0" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL9_2" direction="pas"/>
<pin name="GNDA_PLL9" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="VREFB7N1" direction="pas"/>
<pin name="VREFB7N2" direction="pas"/>
<pin name="VREFB3N1" direction="pas"/>
<pin name="VREFB3N2" direction="pas"/>
<pin name="VREFB4N2" direction="pas"/>
<pin name="VREFB3N0" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_E">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL7" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VREFB2N0" direction="pas"/>
<pin name="MSEL3" direction="pas"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="NC_2" direction="nc"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL7_2" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL11_2" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_F">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCPD4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCPD3_2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCC_PLL11_OUT" direction="pwr"/>
<pin name="VCCD_PLL11" direction="pwr"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_G">
<pin name="VCCPD2_2" direction="pwr"/>
<pin name="VCCPD5_2" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VREFB2N2" direction="pas"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_H">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD1_2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD6_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB1N0" direction="pas"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_I">
<pin name="VCCPD7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VREFB1N1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_J">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCC_PLL12_OUT" direction="pwr"/>
<pin name="VCCD_PLL8" direction="pwr"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCD_PLL12" direction="pwr"/>
<pin name="VREFB1N2" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GNDA_PLL8_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C3N_K">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VREFB7N0" direction="pas"/>
<pin name="VREFB8N0" direction="pas"/>
<pin name="VREFB8N2" direction="pas"/>
<pin name="VREFB8N1" direction="pas"/>
<pin name="FPLL8CLKN" direction="in"/>
<pin name="FPLL8CLKP" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TRST" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCD_PLL10" direction="pwr"/>
<pin name="VCCA_PLL10" direction="pwr"/>
<pin name="VREFB4N0" direction="pas"/>
<pin name="VREFB4N1" direction="pas"/>
<pin name="VREFB5N2" direction="pas"/>
<pin name="VREFB5N1" direction="pas"/>
<pin name="TEMPDIODEN" direction="pas"/>
<pin name="TEMPDIODEP" direction="pas"/>
<pin name="FPLL10CLKP" direction="in"/>
<pin name="FPLL10CLKN" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL10_2" direction="pas"/>
<pin name="GNDA_PLL10" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_B">
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="VREFB5N0" direction="pas"/>
<pin name="VREFB6N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_C">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCA_PLL9" direction="pwr"/>
<pin name="VCCD_PLL9" direction="pwr"/>
<pin name="PLL_ENA" direction="pas"/>
<pin name="FPLL9CLKP" direction="in"/>
<pin name="FPLL9CLKN" direction="in"/>
<pin name="VREFB6N1" direction="pas"/>
<pin name="VREFB6N0" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL9_2" direction="pas"/>
<pin name="GNDA_PLL9" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="VREFB7N1" direction="pas"/>
<pin name="VREFB7N2" direction="pas"/>
<pin name="VREFB3N1" direction="pas"/>
<pin name="VREFB3N2" direction="pas"/>
<pin name="VREFB4N2" direction="pas"/>
<pin name="VREFB3N0" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_E">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL7" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VREFB2N0" direction="pas"/>
<pin name="MSEL3" direction="pas"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="NC_2" direction="nc"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL7_2" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL11_2" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_F">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCPD4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCPD3_2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCC_PLL11_OUT" direction="pwr"/>
<pin name="VCCD_PLL11" direction="pwr"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_G">
<pin name="VCCPD2_2" direction="pwr"/>
<pin name="VCCPD5_2" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VREFB2N2" direction="pas"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_H">
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD1_2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD6_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB1N0" direction="pas"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_I">
<pin name="VCCPD7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VREFB1N1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_J">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCC_PLL12_OUT" direction="pwr"/>
<pin name="VCCD_PLL8" direction="pwr"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCD_PLL12" direction="pwr"/>
<pin name="VREFB1N2" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GNDA_PLL8_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S60F1020C5N_K">
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VREFB7N0" direction="pas"/>
<pin name="VREFB8N0" direction="pas"/>
<pin name="VREFB8N2" direction="pas"/>
<pin name="VREFB8N1" direction="pas"/>
<pin name="FPLL8CLKN" direction="in"/>
<pin name="FPLL8CLKP" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TRST" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_A">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCD_PLL10" direction="pwr"/>
<pin name="VCCA_PLL10" direction="pwr"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TDO" direction="pas"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB5N1" direction="in"/>
<pin name="VREFB5N2" direction="in"/>
<pin name="FPLL10CLKP" direction="in"/>
<pin name="FPLL10CLKN" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL10_2" direction="pas"/>
<pin name="GNDA_PLL10" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_B">
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO5_2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pwr"/>
<pin name="VCCA_PLL3" direction="pwr"/>
<pin name="VCCA_PLL4" direction="pwr"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="VREFB5N0" direction="in"/>
<pin name="VREFB6N2" direction="in"/>
<pin name="CLK9P" direction="in"/>
<pin name="CLK9N" direction="in"/>
<pin name="CLK11P" direction="in"/>
<pin name="CLK11N" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL3_2" direction="pas"/>
<pin name="GNDA_PLL3" direction="pas"/>
<pin name="GNDA_PLL4_2" direction="pas"/>
<pin name="GNDA_PLL4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_C">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCA_PLL9" direction="pwr"/>
<pin name="VCCD_PLL9" direction="pwr"/>
<pin name="VREFB6N0" direction="in"/>
<pin name="VREFB6N1" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="FPLL9CLKP" direction="in"/>
<pin name="FPLL9CLKN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL9_2" direction="pas"/>
<pin name="GNDA_PLL9" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_D">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="VREFB7N2" direction="in"/>
<pin name="VREFB4N2" direction="in"/>
<pin name="VREFB3N2" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_E">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCD_PLL7" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDA_PLL7_2" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="GNDA_PLL11_2" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_F">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD3_2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4_2" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCD_PLL11" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCC_PLL11_OUT" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_G">
<pin name="VCCPD2_2" direction="pwr"/>
<pin name="VCCPD5_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCPD5" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VREFB2N2" direction="in"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_H">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCPD1_2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCPD6_2" direction="pwr"/>
<pin name="VCCPD6" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_I">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCPD7_2" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8_2" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_J">
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCD_PLL8" direction="pwr"/>
<pin name="VCCD_PLL12" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCC_PLL12_OUT" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="VREFB1N2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL8_2" direction="pas"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2S90F1020C5N_K">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="VREFB8N2" direction="in"/>
<pin name="FPLL8CLKN" direction="in"/>
<pin name="FPLL8CLKP" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_A">
<pin name="VCCA" direction="pwr"/>
<pin name="REFCLK1_B13P" direction="in"/>
<pin name="REFCLK1_B13N" direction="in"/>
<pin name="REFCLK0_B13P" direction="in"/>
<pin name="REFCLK0_B13N" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO"/>
<pin name="RREFB13" direction="pas"/>
<pin name="GXB_TX0P" direction="pas"/>
<pin name="GXB_TX0N" direction="pas"/>
<pin name="GXB_TX1P" direction="pas"/>
<pin name="GXB_TX1N" direction="pas"/>
<pin name="GXB_TX2N" direction="pas"/>
<pin name="GXB_TX2P" direction="pas"/>
<pin name="GXB_TX3P" direction="pas"/>
<pin name="GXB_TX3N" direction="pas"/>
<pin name="GXB_TX4N" direction="pas"/>
<pin name="GXB_TX4P" direction="pas"/>
<pin name="GXB_TX5P" direction="pas"/>
<pin name="GXB_TX5N" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND_55" direction="pas"/>
<pin name="GND_56" direction="pas"/>
<pin name="GND_57" direction="pas"/>
<pin name="GND_58" direction="pas"/>
<pin name="GND_59" direction="pas"/>
<pin name="GND_60" direction="pas"/>
<pin name="GND_61" direction="pas"/>
<pin name="GND_62" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GXB_RX0P" direction="pas"/>
<pin name="GXB_RX0N" direction="pas"/>
<pin name="GXB_RX1P" direction="pas"/>
<pin name="GXB_RX1N" direction="pas"/>
<pin name="GXB_RX2P" direction="pas"/>
<pin name="GXB_RX2N" direction="pas"/>
<pin name="GXB_RX3P" direction="pas"/>
<pin name="GXB_RX3N" direction="pas"/>
<pin name="GXB_RX4P" direction="pas"/>
<pin name="GXB_RX4N" direction="pas"/>
<pin name="GXB_RX5P" direction="pas"/>
<pin name="GXB_RX5N" direction="pas"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_B">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA_5" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCL_B13" direction="pwr"/>
<pin name="VCCL_B14" direction="pwr"/>
<pin name="REFCLK1_B15P" direction="in"/>
<pin name="REFCLK1_B15N" direction="in"/>
<pin name="REFCLK0_B14P" direction="in"/>
<pin name="REFCLK0_B14N" direction="in"/>
<pin name="REFCLK1_B14P" direction="in"/>
<pin name="REFCLK1_B14N" direction="in"/>
<pin name="RREFB14" direction="pas"/>
<pin name="RREFB15" direction="pas"/>
<pin name="GXB_TX6P" direction="pas"/>
<pin name="GXB_TX6N" direction="pas"/>
<pin name="GXB_TX7P" direction="pas"/>
<pin name="GXB_TX7N" direction="pas"/>
<pin name="GXB_TX8P" direction="pas"/>
<pin name="GXB_TX8N" direction="pas"/>
<pin name="GXB_TX9P" direction="pas"/>
<pin name="GXB_TX9N" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO"/>
<pin name="GXB_RX6P" direction="pas"/>
<pin name="GXB_RX6N" direction="pas"/>
<pin name="GXB_RX7P" direction="pas"/>
<pin name="GXB_RX7N" direction="pas"/>
<pin name="GXB_RX8P" direction="pas"/>
<pin name="GXB_RX9P" direction="pas"/>
<pin name="GXB_RX8N" direction="pas"/>
<pin name="GXB_RX9N" direction="pas"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_C">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCL_B15" direction="pwr"/>
<pin name="VCCL_B16" direction="pwr"/>
<pin name="RREFB16" direction="pas"/>
<pin name="REFCLK0_B15P" direction="in"/>
<pin name="REFCLK0_B16P" direction="in"/>
<pin name="REFCLK0_B15N" direction="in"/>
<pin name="REFCLK0_B16N" direction="in"/>
<pin name="REFCLK1_B16P" direction="in"/>
<pin name="REFCLK1_B16N" direction="in"/>
<pin name="GXB_TX10P" direction="pas"/>
<pin name="GXB_TX10N" direction="pas"/>
<pin name="GXB_TX11P" direction="pas"/>
<pin name="GXB_TX11N" direction="pas"/>
<pin name="GXB_TX12P" direction="pas"/>
<pin name="GXB_TX12N" direction="pas"/>
<pin name="GXB_TX13P" direction="pas"/>
<pin name="GXB_TX13N" direction="pas"/>
<pin name="GXB_TX14P" direction="pas"/>
<pin name="GXB_TX14N" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO"/>
<pin name="GXB_RX10P" direction="pas"/>
<pin name="GXB_RX10N" direction="pas"/>
<pin name="GXB_RX11P" direction="pas"/>
<pin name="GXB_RX11N" direction="pas"/>
<pin name="GXB_RX12N" direction="pas"/>
<pin name="GXB_RX12P" direction="pas"/>
<pin name="GXB_RX13P" direction="pas"/>
<pin name="GXB_RX13N" direction="pas"/>
<pin name="GXB_RX14P" direction="pas"/>
<pin name="GXB_RX14N" direction="pas"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_D">
<pin name="VCCL_B17" direction="pwr"/>
<pin name="RREFB17" direction="pas"/>
<pin name="REFCLK0_B17P" direction="in"/>
<pin name="REFCLK1_B17P" direction="in"/>
<pin name="REFCLK0_B17N" direction="in"/>
<pin name="REFCLK1_B17N" direction="in"/>
<pin name="GXB_TX15P" direction="pas"/>
<pin name="GXB_TX15N" direction="pas"/>
<pin name="GXB_TX16P" direction="pas"/>
<pin name="GXB_TX16N" direction="pas"/>
<pin name="GXB_TX17P" direction="pas"/>
<pin name="GXB_TX17N" direction="pas"/>
<pin name="GXB_TX19P" direction="pas"/>
<pin name="GXB_TX19N" direction="pas"/>
<pin name="GXB_TX18P" direction="pas"/>
<pin name="GXB_TX18N" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND_55" direction="pas"/>
<pin name="GND_56" direction="pas"/>
<pin name="GND_57" direction="pas"/>
<pin name="GND_58" direction="pas"/>
<pin name="GND_59" direction="pas"/>
<pin name="GND_60" direction="pas"/>
<pin name="GND_61" direction="pas"/>
<pin name="GND_62" direction="pas"/>
<pin name="GND_63" direction="pas"/>
<pin name="GND_64" direction="pas"/>
<pin name="GND_65" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO"/>
<pin name="GXB_RX15P" direction="pas"/>
<pin name="GXB_RX15N" direction="pas"/>
<pin name="GXB_RX16P" direction="pas"/>
<pin name="GXB_RX16N" direction="pas"/>
<pin name="GXB_RX17P" direction="pas"/>
<pin name="GXB_RX17N" direction="pas"/>
<pin name="GXB_RX18P" direction="pas"/>
<pin name="GXB_RX18N" direction="pas"/>
<pin name="GXB_RX19P" direction="pas"/>
<pin name="GXB_RX19N" direction="pas"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_E">
<pin name="VREFB4N0" direction="pas"/>
<pin name="VREFB4N2" direction="pas"/>
<pin name="VREFB4N3" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="NCE" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_F">
<pin name="VREFB4N4" direction="pas"/>
<pin name="VREFB3N1" direction="pas"/>
<pin name="VREFB3N0" direction="pas"/>
<pin name="VREFB3N2" direction="pas"/>
<pin name="VREFB3N3" direction="pas"/>
<pin name="VREFB3N4" direction="pas"/>
<pin name="VREFB4N1" direction="pas"/>
<pin name="VREFB2N4" direction="pas"/>
<pin name="TEMPDIODEP" direction="pas"/>
<pin name="MSEL3" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_G">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4_5" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCIO3_4" direction="pwr"/>
<pin name="VCCIO3_5" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCT_B13_2" direction="pwr"/>
<pin name="VCCH_B13_2" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCD_PLL11" direction="pwr"/>
<pin name="VCC_PLL11_OUT" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VREFB2N3" direction="pas"/>
<pin name="TEMPDIODEN" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL11_2" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="GNDA_PLL7_2" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_H">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCPD3_2" direction="pwr"/>
<pin name="VCCPD3_3" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCPD4_2" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="VCCPD4_3" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCD_PLL7" direction="pwr"/>
<pin name="VREFB2N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_I">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD2_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCPD2_3" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_J">
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCT_B15_2" direction="pwr"/>
<pin name="VCCH_B15_2" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCH_B15" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VREFB2N0" direction="pas"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_K">
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCPD1_2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCINT_20" direction="pwr"/>
<pin name="VCCINT_21" direction="pwr"/>
<pin name="VCCINT_22" direction="pwr"/>
<pin name="VCCINT_23" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCT_B16_2" direction="pwr"/>
<pin name="VCCH_B16_2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCT_B16" direction="pwr"/>
<pin name="VCCH_B16" direction="pwr"/>
<pin name="VREFB1N4" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_L">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VREFB1N3" direction="pas"/>
<pin name="VCCT_B17" direction="pwr"/>
<pin name="VCCH_B17" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_M">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCT_B17" direction="pwr"/>
<pin name="VCCH_B17" direction="pwr"/>
<pin name="VCCPD8_2" direction="pwr"/>
<pin name="VCCPD8_3" direction="pwr"/>
<pin name="VCCPD7_2" direction="pwr"/>
<pin name="VCCPD7_3" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL12" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCD_PLL8" direction="pwr"/>
<pin name="VCC_PLL12_OUT" direction="pwr"/>
<pin name="VREFB1N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL12_2" direction="pas"/>
<pin name="GNDA_PLL8_2" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_N">
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NIO_PULLUP" direction="pas"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="VREFB1N1" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_O">
<pin name="VCCSEL" direction="pwr"/>
<pin name="VREFB1N0" direction="pas"/>
<pin name="VREFB8N2" direction="pas"/>
<pin name="VREFB8N1" direction="pas"/>
<pin name="VREFB8N3" direction="pas"/>
<pin name="VREFB8N0" direction="pas"/>
<pin name="VREFB8N4" direction="pas"/>
<pin name="VREFB7N1" direction="pas"/>
<pin name="VREFB7N4" direction="pas"/>
<pin name="VREFB7N2" direction="pas"/>
<pin name="VREFB7N0" direction="pas"/>
<pin name="VREFB7N3" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="TRST" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX130GF1508C4N_P">
<pin name="FPLL8CLKN" direction="pas"/>
<pin name="FPLL8CLKP" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_F">
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_D">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_A">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="GXB_RX0P" direction="in"/>
<pin name="GXB_RX0N" direction="in"/>
<pin name="GXB_RX1P" direction="in"/>
<pin name="GXB_RX1N" direction="in"/>
<pin name="GXB_RX2P" direction="in"/>
<pin name="GXB_RX2N" direction="in"/>
<pin name="GXB_TX0P" direction="in"/>
<pin name="GXB_TX0N" direction="in"/>
<pin name="GXB_TX1P" direction="in"/>
<pin name="GXB_TX1N" direction="in"/>
<pin name="GXB_TX2P" direction="in"/>
<pin name="GXB_TX2N" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="REFCLK0_B13P" direction="in"/>
<pin name="REFCLK0_B13N" direction="in"/>
<pin name="REFCLK1_B13P" direction="in"/>
<pin name="REFCLK1_B13N" direction="in"/>
<pin name="RREFB13" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_B">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA_5" direction="pwr"/>
<pin name="VCCA_6" direction="pwr"/>
<pin name="VCCA_7" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCH_B14_2" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCL_B13" direction="pwr"/>
<pin name="VCCL_B14" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCR_3" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="VCCT_B14_2" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="GXB_RX3P" direction="in"/>
<pin name="GXB_RX3N" direction="in"/>
<pin name="GXB_TX3P" direction="in"/>
<pin name="GXB_TX3N" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_C">
<pin name="PLL_ENA" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NCEO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_E">
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_G">
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30CF780C5N_H">
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_F">
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_D">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_A">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="GXB_RX0P" direction="in"/>
<pin name="GXB_RX0N" direction="in"/>
<pin name="GXB_RX1P" direction="in"/>
<pin name="GXB_RX1N" direction="in"/>
<pin name="GXB_RX2P" direction="in"/>
<pin name="GXB_RX2N" direction="in"/>
<pin name="GXB_TX0P" direction="in"/>
<pin name="GXB_TX0N" direction="in"/>
<pin name="GXB_TX1P" direction="in"/>
<pin name="GXB_TX1N" direction="in"/>
<pin name="GXB_TX2P" direction="in"/>
<pin name="GXB_TX2N" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="REFCLK0_B13P" direction="in"/>
<pin name="REFCLK0_B13N" direction="in"/>
<pin name="REFCLK1_B13P" direction="in"/>
<pin name="REFCLK1_B13N" direction="in"/>
<pin name="RREFB13" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_B">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA_5" direction="pwr"/>
<pin name="VCCA_6" direction="pwr"/>
<pin name="VCCA_7" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCH_B14_2" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCL_B13" direction="pwr"/>
<pin name="VCCL_B14" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCR_3" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="VCCT_B14_2" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="GXB_RX3P" direction="in"/>
<pin name="GXB_RX3N" direction="in"/>
<pin name="GXB_TX3P" direction="in"/>
<pin name="GXB_TX3N" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_C">
<pin name="PLL_ENA" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NCEO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_E">
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_G">
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX30DF780C3N_H">
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_F">
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_D">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="VREFB3N2" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB2N2" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB4N2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_A">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="GXB_RX0P" direction="in"/>
<pin name="GXB_RX0N" direction="in"/>
<pin name="GXB_RX1P" direction="in"/>
<pin name="GXB_RX1N" direction="in"/>
<pin name="GXB_RX2P" direction="in"/>
<pin name="GXB_RX2N" direction="in"/>
<pin name="GXB_TX0P" direction="in"/>
<pin name="GXB_TX0N" direction="in"/>
<pin name="GXB_TX1P" direction="in"/>
<pin name="GXB_TX1N" direction="in"/>
<pin name="GXB_TX2P" direction="in"/>
<pin name="GXB_TX2N" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="REFCLK0_B13P" direction="in"/>
<pin name="REFCLK0_B13N" direction="in"/>
<pin name="REFCLK1_B13P" direction="in"/>
<pin name="REFCLK1_B13N" direction="in"/>
<pin name="RREFB13" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_B">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA_5" direction="pwr"/>
<pin name="VCCA_6" direction="pwr"/>
<pin name="VCCA_7" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCH_B14_2" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCL_B13" direction="pwr"/>
<pin name="VCCL_B14" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCR_3" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="VCCT_B14_2" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="GXB_RX3P" direction="in"/>
<pin name="GXB_RX3N" direction="in"/>
<pin name="GXB_TX3P" direction="in"/>
<pin name="GXB_TX3N" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_C">
<pin name="VREFB7N2" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NCEO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_E">
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_G">
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="VREFB1N2" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60CF780C5N_H">
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB8N2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_F">
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VREFB2N0" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1_2" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2_2" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_D">
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="VREFB3N2" direction="in"/>
<pin name="VREFB3N0" direction="in"/>
<pin name="VREFB2N2" direction="in"/>
<pin name="VREFB3N1" direction="in"/>
<pin name="VREFB4N1" direction="in"/>
<pin name="VREFB4N2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NSTATUS" direction="out"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_A">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="GXB_RX0P" direction="in"/>
<pin name="GXB_RX0N" direction="in"/>
<pin name="GXB_RX1P" direction="in"/>
<pin name="GXB_RX1N" direction="in"/>
<pin name="GXB_RX2P" direction="in"/>
<pin name="GXB_RX2N" direction="in"/>
<pin name="GXB_TX0P" direction="in"/>
<pin name="GXB_TX0N" direction="in"/>
<pin name="GXB_TX1P" direction="in"/>
<pin name="GXB_TX1N" direction="in"/>
<pin name="GXB_TX2P" direction="in"/>
<pin name="GXB_TX2N" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="MSEL3" direction="in"/>
<pin name="VREFB4N0" direction="in"/>
<pin name="REFCLK0_B13P" direction="in"/>
<pin name="REFCLK0_B13N" direction="in"/>
<pin name="REFCLK1_B13P" direction="in"/>
<pin name="REFCLK1_B13N" direction="in"/>
<pin name="RREFB13" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_B">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA_5" direction="pwr"/>
<pin name="VCCA_6" direction="pwr"/>
<pin name="VCCA_7" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCH_B14_2" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCL_B13" direction="pwr"/>
<pin name="VCCL_B14" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCR_3" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="VCCT_B14_2" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="GXB_RX3P" direction="in"/>
<pin name="GXB_RX3N" direction="in"/>
<pin name="GXB_TX3P" direction="in"/>
<pin name="GXB_TX3N" direction="in"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_C">
<pin name="VREFB7N2" direction="in"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NCEO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_E">
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VREFB2N1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_G">
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="VREFB1N1" direction="in"/>
<pin name="VREFB1N2" direction="in"/>
<pin name="VREFB7N0" direction="in"/>
<pin name="VREFB7N1" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60DF780C5N_H">
<pin name="VREFB8N0" direction="in"/>
<pin name="VREFB8N1" direction="in"/>
<pin name="VREFB1N0" direction="in"/>
<pin name="VREFB8N2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_A">
<pin name="REFCLK1_B13P" direction="pas"/>
<pin name="REFCLK1_B13N" direction="pas"/>
<pin name="REFCLK0_B13P" direction="pas"/>
<pin name="REFCLK0_B13N" direction="pas"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="RREFB13" direction="pas"/>
<pin name="GXB_RX0P" direction="pas"/>
<pin name="GXB_RX0N" direction="pas"/>
<pin name="GXB_RX1P" direction="pas"/>
<pin name="GXB_RX1N" direction="pas"/>
<pin name="GXB_RX2P" direction="pas"/>
<pin name="GXB_RX2N" direction="pas"/>
<pin name="GXB_RX3P" direction="pas"/>
<pin name="GXB_RX3N" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO"/>
<pin name="GXB_TX0P" direction="pas"/>
<pin name="GXB_TX0N" direction="pas"/>
<pin name="GXB_TX1P" direction="pas"/>
<pin name="GXB_TX1N" direction="pas"/>
<pin name="GXB_TX2P" direction="pas"/>
<pin name="GXB_TX2N" direction="pas"/>
<pin name="GXB_TX3P" direction="pas"/>
<pin name="GXB_TX3N" direction="pas"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_B">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCA_3" direction="pwr"/>
<pin name="VCCA_4" direction="pwr"/>
<pin name="VCCA_5" direction="pwr"/>
<pin name="VCCA_6" direction="pwr"/>
<pin name="VCCR_2" direction="pwr"/>
<pin name="VCCA_7" direction="pwr"/>
<pin name="VCCR_3" direction="pwr"/>
<pin name="VCCA_8" direction="pwr"/>
<pin name="VCCR_4" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCR_5" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCL_B14" direction="pwr"/>
<pin name="VCCL_B13" direction="pwr"/>
<pin name="REFCLK1_B14P" direction="pas"/>
<pin name="REFCLK1_B14N" direction="pas"/>
<pin name="REFCLK0_B14P" direction="pas"/>
<pin name="REFCLK0_B14N" direction="pas"/>
<pin name="GXB_RX4P" direction="pas"/>
<pin name="GXB_RX4N" direction="pas"/>
<pin name="GXB_RX5P" direction="pas"/>
<pin name="GXB_RX5N" direction="pas"/>
<pin name="GXB_RX6P" direction="pas"/>
<pin name="GXB_RX6N" direction="pas"/>
<pin name="RREFB14" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO"/>
<pin name="GXB_TX4P" direction="pas"/>
<pin name="GXB_TX4N" direction="pas"/>
<pin name="GXB_TX5P" direction="pas"/>
<pin name="GXB_TX5N" direction="pas"/>
<pin name="GXB_TX6P" direction="pas"/>
<pin name="GXB_TX6N" direction="pas"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_C">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCL_B15" direction="pwr"/>
<pin name="REFCLK1_B15P" direction="pas"/>
<pin name="REFCLK1_B15N" direction="pas"/>
<pin name="REFCLK0_B15P" direction="pas"/>
<pin name="PLL_ENA" direction="in"/>
<pin name="NO_PULLUP" direction="pas"/>
<pin name="PORSEL" direction="pas"/>
<pin name="NCEO" direction="pas"/>
<pin name="RREFB15" direction="pas"/>
<pin name="GXB_RX7P" direction="pas"/>
<pin name="GXB_RX7N" direction="pas"/>
<pin name="GXB_RX8P" direction="pas"/>
<pin name="GXB_RX8N" direction="pas"/>
<pin name="GXB_RX9P" direction="pas"/>
<pin name="GXB_RX9N" direction="pas"/>
<pin name="GXB_RX10P" direction="pas"/>
<pin name="GXB_RX10N" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO"/>
<pin name="GXB_TX7P" direction="pas"/>
<pin name="GXB_TX7N" direction="pas"/>
<pin name="GXB_TX9P" direction="pas"/>
<pin name="GXB_TX9N" direction="pas"/>
<pin name="GXB_TX8P" direction="pas"/>
<pin name="GXB_TX8N" direction="pas"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_D">
<pin name="DCLK" direction="in"/>
<pin name="FPLL7CLKN" direction="in"/>
<pin name="FPLL7CLKP" direction="in"/>
<pin name="REFCLK0_B15N" direction="pas"/>
<pin name="GXB_RX11P" direction="pas"/>
<pin name="GXB_RX11N" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
<pin name="GXB_TX10P" direction="pas"/>
<pin name="GXB_TX10N" direction="pas"/>
<pin name="GXB_TX11P" direction="pas"/>
<pin name="GXB_TX11N" direction="pas"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_E">
<pin name="VREFB4N0" direction="pas"/>
<pin name="VREFB3N0" direction="pas"/>
<pin name="VREFB3N2" direction="pas"/>
<pin name="VREFB3N1" direction="pas"/>
<pin name="VREFB4N2" direction="pas"/>
<pin name="VREFB4N1" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="MSEL3" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_F">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCPD4_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCPD4" direction="pwr"/>
<pin name="VCCPD3_2" direction="pwr"/>
<pin name="VCCPD3" direction="pwr"/>
<pin name="VCCA_PLL5" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3_4" direction="pwr"/>
<pin name="VCCD_PLL7" direction="pwr"/>
<pin name="VCCD_PLL5" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCD_PLL11" direction="pwr"/>
<pin name="VCCA_PLL7" direction="pwr"/>
<pin name="VCCA_PLL11" direction="pwr"/>
<pin name="MSEL0" direction="pas"/>
<pin name="MSEL2" direction="pas"/>
<pin name="VREFB2N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL5_2" direction="pas"/>
<pin name="GNDA_PLL5" direction="pas"/>
<pin name="GNDA_PLL11_2" direction="pas"/>
<pin name="GNDA_PLL7_2" direction="pas"/>
<pin name="GNDA_PLL11" direction="pas"/>
<pin name="GNDA_PLL7" direction="pas"/>
<pin name="VCC_PLL11_OUT" direction="pwr"/>
<pin name="VCC_PLL5_OUT" direction="pwr"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_G">
<pin name="VCCT_B13_2" direction="pwr"/>
<pin name="VCCT_B13" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCH_B13_2" direction="pwr"/>
<pin name="VCCPD2_2" direction="pwr"/>
<pin name="VCCH_B13" direction="pwr"/>
<pin name="VCCPD2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="VREFB2N1" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_H">
<pin name="VCCA_2" direction="pwr"/>
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCT_B14_2" direction="pwr"/>
<pin name="VCCH_B14_2" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCT_B14" direction="pwr"/>
<pin name="VCCH_B14" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT_11" direction="pwr"/>
<pin name="VCCINT_12" direction="pwr"/>
<pin name="VCCINT_13" direction="pwr"/>
<pin name="VCCINT_14" direction="pwr"/>
<pin name="VCCINT_15" direction="pwr"/>
<pin name="VCCINT_16" direction="pwr"/>
<pin name="VCCINT_17" direction="pwr"/>
<pin name="VCCINT_18" direction="pwr"/>
<pin name="VCCINT_19" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB2N0" direction="pas"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL1" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_I">
<pin name="VCCP_2" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VCCPD1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCT_B15_2" direction="pwr"/>
<pin name="VCCH_B15_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCT_B15" direction="pwr"/>
<pin name="VCCH_B15" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT_8" direction="pwr"/>
<pin name="VCCINT_9" direction="pwr"/>
<pin name="VCCINT_10" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VREFB1N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL2" direction="pas"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_J">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7_3" direction="pwr"/>
<pin name="VCCPD7_2" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCPD7" direction="pwr"/>
<pin name="VCCIO8_3" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCPD8_2" direction="pwr"/>
<pin name="VCCIO7_4" direction="pwr"/>
<pin name="VCCPD8" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCD_PLL8" direction="pwr"/>
<pin name="VCCD_PLL6" direction="pwr"/>
<pin name="VCCA_PLL12" direction="pwr"/>
<pin name="VCCA_PLL6" direction="pwr"/>
<pin name="VCCD_PLL12" direction="pwr"/>
<pin name="VCCA_PLL8" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="VREFB1N1" direction="pas"/>
<pin name="VREFB1N0" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_PLL6_2" direction="pas"/>
<pin name="GNDA_PLL12_2" direction="pas"/>
<pin name="GNDA_PLL8_2" direction="pas"/>
<pin name="GNDA_PLL6" direction="pas"/>
<pin name="GNDA_PLL12" direction="pas"/>
<pin name="GNDA_PLL8" direction="pas"/>
<pin name="VCC_PLL12_OUT" direction="pwr"/>
<pin name="VCC_PLL6_OUT" direction="pwr"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_K">
<pin name="VCCIO8" direction="pwr"/>
<pin name="VREFB7N0" direction="pas"/>
<pin name="VREFB7N1" direction="pas"/>
<pin name="VREFB7N2" direction="pas"/>
<pin name="VREFB8N0" direction="pas"/>
<pin name="VREFB8N1" direction="pas"/>
<pin name="VREFB8N2" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO"/>
</symbol>
<symbol name="EP2SGX60EF1152C5N_L">
<pin name="TRST" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TCK" direction="in"/>
<pin name="FPLL8CLKN" direction="in"/>
<pin name="FPLL8CLKP" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO"/>
</symbol>
<symbol name="EP3C25E144C8NES_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCA1" direction="pwr"/>
<pin name="VCCA3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL3" direction="pas"/>
<pin name="VCCD_PLL4" direction="pwr"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK12" direction="in"/>
<pin name="CLK13" direction="in"/>
<pin name="CLK14" direction="in"/>
<pin name="CLK15" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA3" direction="pas"/>
<pin name="GNDA1" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO"/>
</symbol>
<symbol name="EP3C25E144C8NES_B">
<pin name="VCCA2" direction="pwr"/>
<pin name="VCCA4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT_7" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO5" direction="pwr"/>
<pin name="VCCIO6" direction="pwr"/>
<pin name="VCCIO7_2" direction="pwr"/>
<pin name="VCCIO7" direction="pwr"/>
<pin name="VCCIO8_2" direction="pwr"/>
<pin name="VCCIO8" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="CLK4" direction="in"/>
<pin name="CLK5" direction="in"/>
<pin name="CLK6" direction="in"/>
<pin name="CLK7" direction="in"/>
<pin name="CLK8" direction="in"/>
<pin name="CLK9" direction="in"/>
<pin name="CLK10" direction="in"/>
<pin name="CLK11" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="GNDA2" direction="pas"/>
<pin name="GNDA4" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO"/>
</symbol>
<symbol name="EP3SL150F1152C4N_A">
<pin name="VCCIO7A_2" direction="pwr"/>
<pin name="VCCIO6A_2" direction="pwr"/>
<pin name="VCCPT" direction="pwr"/>
<pin name="VCCIO6A_3" direction="pwr"/>
<pin name="VCCIO7A" direction="pwr"/>
<pin name="VCCBAT" direction="pwr"/>
<pin name="VCCIO6C" direction="pwr"/>
<pin name="VCCIO6A" direction="pwr"/>
<pin name="TEMPDIODEP" direction="in"/>
<pin name="TEMPDIODEN" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_7_7"/>
<pin name="IO_7_8"/>
<pin name="IO_7_9"/>
<pin name="IO_7_10"/>
<pin name="IO_7_11"/>
<pin name="IO_7_12"/>
<pin name="IO_7_13"/>
<pin name="IO_7_14"/>
<pin name="IO_6_2"/>
<pin name="IO_7_15"/>
<pin name="IO_7_16"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_7_17"/>
<pin name="IO_7_18"/>
<pin name="IO_7_19"/>
<pin name="IO_7_20"/>
<pin name="IO_6_3"/>
<pin name="IO_6_4"/>
<pin name="IO_6_5"/>
<pin name="IO_7_21"/>
<pin name="IO_7_22"/>
<pin name="IO_7_23"/>
<pin name="IO_7_24"/>
<pin name="IO_6_6"/>
<pin name="IO_6_7"/>
<pin name="IO_6_RDN6A"/>
<pin name="IO_6_RUP6A"/>
<pin name="IO_7_RDN7A"/>
<pin name="IO_7_25"/>
<pin name="IO_6_8"/>
<pin name="IO_6_9"/>
<pin name="IO_6_10"/>
<pin name="IO_7_26"/>
<pin name="IO_7_RUP7A"/>
<pin name="IO_7_27"/>
<pin name="IO_7_28"/>
<pin name="IO_6_11"/>
<pin name="IO_6_12"/>
<pin name="IO_6_13"/>
<pin name="IO_6_14"/>
<pin name="IO_7_29"/>
<pin name="IO_7"/>
<pin name="IO_6_15"/>
<pin name="IO_6_16"/>
<pin name="IO_6_17"/>
<pin name="IO_6_18"/>
<pin name="IO_6_19"/>
<pin name="IO_6_20"/>
<pin name="IO_6_21"/>
<pin name="IO_6_22"/>
<pin name="IO_6_23"/>
<pin name="IO_6_24"/>
<pin name="IO_6_25"/>
<pin name="IO_6_26"/>
<pin name="IO_6_27"/>
<pin name="IO_6_28"/>
<pin name="IO_6_29"/>
<pin name="IO_6_30"/>
<pin name="IO_6_31"/>
<pin name="IO_6_32"/>
<pin name="IO_6_33"/>
<pin name="IO_6_34"/>
<pin name="IO_6_35"/>
<pin name="IO_6_36"/>
<pin name="IO_6_37"/>
<pin name="IO_6_38"/>
<pin name="IO_6"/>
</symbol>
<symbol name="EP3SL150F1152C4N_B">
<pin name="VCCPT" direction="pwr"/>
<pin name="VCCIO5C_2" direction="pwr"/>
<pin name="VCCIO6A" direction="pwr"/>
<pin name="VCCIO6C_2" direction="pwr"/>
<pin name="VCCIO5C_3" direction="pwr"/>
<pin name="VCCIO5C" direction="pwr"/>
<pin name="VCCIO8C" direction="pwr"/>
<pin name="VCCIO6C" direction="pwr"/>
<pin name="VCCA_PLL_R2" direction="pwr"/>
<pin name="VCCD_PLL_R2" direction="pwr"/>
<pin name="VCCD_PLL_R3" direction="pwr"/>
<pin name="VCCA_PLL_R3" direction="pwr"/>
<pin name="VREF6C" direction="pwr"/>
<pin name="VREF6A" direction="pwr"/>
<pin name="CLK10N" direction="in"/>
<pin name="CLK10P" direction="in"/>
<pin name="CLK8N" direction="in"/>
<pin name="CLK8P" direction="in"/>
<pin name="IO_6_CLK11N"/>
<pin name="IO_6_CLK11P"/>
<pin name="IO_5_CLK9N"/>
<pin name="IO_5_CLK9P"/>
<pin name="IO_7_CLK13N"/>
<pin name="IO_7_CLK12N"/>
<pin name="IO_8_CLK14N"/>
<pin name="IO_8_CLK15N"/>
<pin name="IO_6_2"/>
<pin name="IO_6_3"/>
<pin name="IO_6_4"/>
<pin name="IO_6_5"/>
<pin name="IO_6_6"/>
<pin name="IO_5_2"/>
<pin name="IO_6_7"/>
<pin name="IO_5_3"/>
<pin name="IO_5_4"/>
<pin name="IO_5_5"/>
<pin name="IO_5_6"/>
<pin name="IO_5_7"/>
<pin name="IO_5_8"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_5_PLL_R3_CLKOUT0N"/>
<pin name="IO_6_8"/>
<pin name="IO_6_9"/>
<pin name="IO_6_10"/>
<pin name="IO_6_11"/>
<pin name="IO_6_12"/>
<pin name="IO_6_13"/>
<pin name="IO_6_14"/>
<pin name="IO_6_15"/>
<pin name="IO_6_16"/>
<pin name="IO_6_17"/>
<pin name="IO_6_18"/>
<pin name="IO_6_19"/>
<pin name="IO_6_20"/>
<pin name="IO_6_21"/>
<pin name="IO_6_22"/>
<pin name="IO_6_23"/>
<pin name="IO_6_24"/>
<pin name="IO_6_25"/>
<pin name="IO_6_26"/>
<pin name="IO_6_27"/>
<pin name="IO_6_28"/>
<pin name="IO_6_29"/>
<pin name="IO_6_30"/>
<pin name="IO_6_31"/>
<pin name="IO_6_32"/>
<pin name="IO_6_33"/>
<pin name="IO_6_34"/>
<pin name="IO_6_35"/>
<pin name="IO_6_36"/>
<pin name="IO_6"/>
<pin name="IO_5_9"/>
<pin name="IO_5_10"/>
<pin name="IO_5_11"/>
<pin name="IO_5_12"/>
<pin name="IO_5_13"/>
<pin name="IO_5_14"/>
<pin name="IO_5_15"/>
<pin name="IO_5_16"/>
<pin name="IO_5"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_7"/>
<pin name="IO_8_2"/>
<pin name="IO_8"/>
</symbol>
<symbol name="EP3SL150F1152C4N_C">
<pin name="VCCIO5A_2" direction="pwr"/>
<pin name="VCCIO5A_3" direction="pwr"/>
<pin name="VCCIO5A_4" direction="pwr"/>
<pin name="VCCIO5A" direction="pwr"/>
<pin name="VCCPT" direction="pwr"/>
<pin name="VCCIO5C" direction="pwr"/>
<pin name="VREF5C" direction="pwr"/>
<pin name="VREF5A" direction="pwr"/>
<pin name="NIO_PULLUP" direction="in"/>
<pin name="IO_5_2"/>
<pin name="IO_4_2"/>
<pin name="IO_5_3"/>
<pin name="IO_4_3"/>
<pin name="IO_5_4"/>
<pin name="IO_4_4"/>
<pin name="IO_5_5"/>
<pin name="IO_4_5"/>
<pin name="IO_5_6"/>
<pin name="IO_5_7"/>
<pin name="IO_5_8"/>
<pin name="IO_5_9"/>
<pin name="IO_4"/>
<pin name="IO_5_10"/>
<pin name="IO_5_11"/>
<pin name="IO_5_12"/>
<pin name="IO_5_13"/>
<pin name="IO_5_14"/>
<pin name="IO_5_15"/>
<pin name="IO_5_16"/>
<pin name="IO_5_17"/>
<pin name="IO_5_18"/>
<pin name="IO_5_19"/>
<pin name="IO_5_20"/>
<pin name="IO_5_21"/>
<pin name="IO_5_22"/>
<pin name="IO_5_23"/>
<pin name="IO_5_24"/>
<pin name="IO_5_25"/>
<pin name="IO_5_26"/>
<pin name="IO_5_27"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_8_6"/>
<pin name="IO_8_7"/>
<pin name="IO_8_8"/>
<pin name="IO_8_9"/>
<pin name="IO_8_10"/>
<pin name="IO_8_11"/>
<pin name="IO_8"/>
<pin name="IO_5_28"/>
<pin name="IO_5_29"/>
<pin name="IO_5_30"/>
<pin name="IO_5_31"/>
<pin name="IO_5_32"/>
<pin name="IO_5_33"/>
<pin name="IO_5_34"/>
<pin name="IO_5_35"/>
<pin name="IO_5_36"/>
<pin name="IO_5_37"/>
<pin name="IO_5_38"/>
<pin name="IO_5_39"/>
<pin name="IO_5_40"/>
<pin name="IO_5_41"/>
<pin name="IO_5_42"/>
<pin name="IO_5_43"/>
<pin name="IO_5_44"/>
<pin name="IO_5_45"/>
<pin name="IO_5_46"/>
<pin name="IO_5_47"/>
<pin name="IO_5_48"/>
<pin name="IO_5_49"/>
<pin name="IO_5_50"/>
<pin name="IO_5_51"/>
<pin name="IO_5_52"/>
<pin name="IO_5"/>
<pin name="IO_4_RUP4A"/>
<pin name="IO_5_RDN5A"/>
<pin name="IO_4_RDN4A"/>
<pin name="IO_5_RUP5A"/>
<pin name="ASDO"/>
<pin name="NCEO" direction="out"/>
<pin name="NCSO"/>
</symbol>
<symbol name="EP3SL150F1152C4N_D">
<pin name="VCCIO1A" direction="pwr"/>
<pin name="VCCIO4A_2" direction="pwr"/>
<pin name="VCCIO7B" direction="pwr"/>
<pin name="VCCIO4A" direction="pwr"/>
<pin name="VCCIO8A" direction="pwr"/>
<pin name="VCCIO5A" direction="pwr"/>
<pin name="VCCIO7C" direction="pwr"/>
<pin name="VCCIO8C" direction="pwr"/>
<pin name="VCCIO8B" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="IO_7_CLK13P"/>
<pin name="IO_7_CLK12P"/>
<pin name="IO_8_CLK14P"/>
<pin name="IO_8_CLK15P"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_4"/>
<pin name="IO_7_2"/>
<pin name="IO_8_5"/>
<pin name="IO_8_6"/>
<pin name="IO_8_7"/>
<pin name="IO_8_8"/>
<pin name="IO_8_9"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_7_7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_5_2"/>
<pin name="IO_5_3"/>
<pin name="IO_4_5"/>
<pin name="IO_4_6"/>
<pin name="IO_4_7"/>
<pin name="IO_4_8"/>
<pin name="IO_4_9"/>
<pin name="IO_5_4"/>
<pin name="IO_5"/>
<pin name="IO_4_10"/>
<pin name="IO_4_11"/>
<pin name="IO_4_12"/>
<pin name="IO_4_13"/>
<pin name="IO_4_14"/>
<pin name="IO_4_15"/>
<pin name="IO_4_16"/>
<pin name="IO_4_17"/>
<pin name="IO_4_18"/>
<pin name="IO_4_19"/>
<pin name="IO_4_20"/>
<pin name="IO_4_21"/>
<pin name="IO_4_22"/>
<pin name="IO_4_23"/>
<pin name="IO_4_24"/>
<pin name="IO_4_25"/>
<pin name="IO_4_26"/>
<pin name="IO_4_27"/>
<pin name="IO_4"/>
<pin name="IO_7_8"/>
<pin name="IO_7_9"/>
<pin name="IO_7_10"/>
<pin name="IO_7_11"/>
<pin name="IO_8_10"/>
<pin name="IO_8_11"/>
<pin name="IO_8_12"/>
<pin name="IO_8_13"/>
<pin name="IO_8_14"/>
<pin name="IO_8_15"/>
<pin name="IO_8_16"/>
<pin name="IO_8_17"/>
<pin name="IO_8_18"/>
<pin name="IO_8_19"/>
<pin name="IO_8"/>
<pin name="IO_1_2"/>
<pin name="IO_1"/>
<pin name="IO_7_12"/>
<pin name="IO_7_13"/>
<pin name="IO_7_14"/>
<pin name="IO_7_15"/>
<pin name="IO_7_16"/>
<pin name="IO_7"/>
<pin name="IO_8_PLL_T1_FBN/CLKOUT2"/>
</symbol>
<symbol name="EP3SL150F1152C4N_E">
<pin name="VCCIO7A" direction="pwr"/>
<pin name="VCCIO8B" direction="pwr"/>
<pin name="VCCIO7C_2" direction="pwr"/>
<pin name="VCCIO8A_2" direction="pwr"/>
<pin name="VCCIO7C" direction="pwr"/>
<pin name="VCCIO1A" direction="pwr"/>
<pin name="VCCIO8A" direction="pwr"/>
<pin name="VCCA_PLL_T2" direction="pwr"/>
<pin name="VCCPT" direction="pwr"/>
<pin name="VCCA_PLL_T1" direction="pwr"/>
<pin name="VREF7C" direction="pwr"/>
<pin name="VREF8C" direction="pwr"/>
<pin name="VREF7A" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_8_6"/>
<pin name="IO_8_7"/>
<pin name="IO_8_8"/>
<pin name="IO_8_9"/>
<pin name="IO_8_10"/>
<pin name="IO_8_11"/>
<pin name="IO_8_12"/>
<pin name="IO_1_2"/>
<pin name="IO_1_3"/>
<pin name="IO_1_4"/>
<pin name="IO_1_5"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_8_13"/>
<pin name="IO_8_14"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_7_7"/>
<pin name="IO_7_8"/>
<pin name="IO_8_PLL_T1_FBP/CLKOUT1"/>
<pin name="IO_8_15"/>
<pin name="IO_8_16"/>
<pin name="IO_8_17"/>
<pin name="IO_8_18"/>
<pin name="IO_8_19"/>
<pin name="IO_8_20"/>
<pin name="IO_8_21"/>
<pin name="IO_8_22"/>
<pin name="IO_8_23"/>
<pin name="IO_8_24"/>
<pin name="IO_8_25"/>
<pin name="IO_8_26"/>
<pin name="IO_1_6"/>
<pin name="IO_1_7"/>
<pin name="IO_7_9"/>
<pin name="IO_7_10"/>
<pin name="IO_7_11"/>
<pin name="IO_7_12"/>
<pin name="IO_7_PLL_T2_FBN/CLKOUT2"/>
<pin name="IO_7_13"/>
<pin name="IO_8_27"/>
<pin name="IO_8_28"/>
<pin name="IO_8_29"/>
<pin name="IO_8_30"/>
<pin name="IO_8_31"/>
<pin name="IO_8_32"/>
<pin name="IO_8_33"/>
<pin name="IO_8_34"/>
<pin name="IO_1_RUP1A"/>
<pin name="IO_1_RDN1A"/>
<pin name="IO_1_8"/>
<pin name="IO_7_14"/>
<pin name="IO_7_15"/>
<pin name="IO_7_16"/>
<pin name="IO_7_17"/>
<pin name="IO_7_18"/>
<pin name="IO_7_PLL_T2_FBP/CLKOUT1"/>
<pin name="IO_8_35"/>
<pin name="IO_8_36"/>
<pin name="IO_8_RDN8A"/>
<pin name="IO_8"/>
<pin name="IO_1_9"/>
<pin name="IO_1_10"/>
<pin name="IO_1_11"/>
<pin name="IO_1"/>
<pin name="IO_7"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EP3SL150F1152C4N_F">
<pin name="VCCIO8C" direction="pwr"/>
<pin name="VCCIO7A" direction="pwr"/>
<pin name="VCCIO1A_2" direction="pwr"/>
<pin name="VCCD_PLL_T2" direction="pwr"/>
<pin name="VCCIO7B" direction="pwr"/>
<pin name="VCCD_PLL_T1" direction="pwr"/>
<pin name="VCCPT" direction="pwr"/>
<pin name="VCCIO6A" direction="pwr"/>
<pin name="VCCIO8A" direction="pwr"/>
<pin name="VCCIO1A" direction="pwr"/>
<pin name="VCC_CLKIN7C" direction="pwr"/>
<pin name="VCC_CLKIN8C" direction="pwr"/>
<pin name="VREF7B" direction="pwr"/>
<pin name="VREF8A" direction="pwr"/>
<pin name="VREF8B" direction="pwr"/>
<pin name="VREF1A" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_7_2"/>
<pin name="IO_7_3"/>
<pin name="IO_8_2"/>
<pin name="IO_8_3"/>
<pin name="IO_8_RUP8A"/>
<pin name="IO_1_2"/>
<pin name="IO_1_3"/>
<pin name="IO_1_4"/>
<pin name="IO_7_4"/>
<pin name="IO_7_5"/>
<pin name="IO_7_6"/>
<pin name="IO_7_7"/>
<pin name="IO_7_8"/>
<pin name="IO_8_PLL_T1_CLKOUT0N"/>
<pin name="IO_8_4"/>
<pin name="IO_8_5"/>
<pin name="IO_8_6"/>
<pin name="IO_8_7"/>
<pin name="IO_8_8"/>
<pin name="IO_1_5"/>
<pin name="IO_1_6"/>
<pin name="IO_1_7"/>
<pin name="IO_1_8"/>
<pin name="IO_1_9"/>
<pin name="IO_1_10"/>
<pin name="IO_7_9"/>
<pin name="IO_7_10"/>
<pin name="IO_7_11"/>
<pin name="IO_7_12"/>
<pin name="IO_7_13"/>
<pin name="IO_7_PLL_T2_CLKOUT3"/>
<pin name="IO_7_PLL_T2_CLKOUT0N"/>
<pin name="IO_8_PLL_T1_CLKOUT0P"/>
<pin name="IO_8_9"/>
<pin name="IO_8_10"/>
<pin name="IO_8_11"/>
<pin name="IO_8_12"/>
<pin name="IO_8_13"/>
<pin name="IO_8_14"/>
<pin name="IO_1_11"/>
<pin name="IO_1_12"/>
<pin name="IO_1_13"/>
<pin name="IO_1_14"/>
<pin name="IO_1_15"/>
<pin name="IO_1_16"/>
<pin name="IO_1_17"/>
<pin name="IO_1_18"/>
<pin name="IO_7_14"/>
<pin name="IO_7"/>
<pin name="IO_7_PLL_T2_CLKOUT4"/>
<pin name="IO_7_PLL_T2_CLKOUT0P"/>
<pin name="IO_8_PLL_T1_CLKOUT3"/>
<pin name="IO_8_PLL_T1_CLKOUT4"/>
<pin name="IO_8_15"/>
<pin name="IO_8"/>
<pin name="IO_1_19"/>
<pin name="IO_1_20"/>
<pin name="IO_1_21"/>
<pin name="IO_1"/>
</symbol>
<symbol name="EP3SL150F1152C4N_G">
<pin name="VCCPD7A" direction="pwr"/>
<pin name="VCCPD1A" direction="pwr"/>
<pin name="VCCPD7B" direction="pwr"/>
<pin name="VCCIO1A" direction="pwr"/>
<pin name="VCCPD7C" direction="pwr"/>
<pin name="VCCPD8C" direction="pwr"/>
<pin name="VCCPD8B" direction="pwr"/>
<pin name="VCC_2" direction="pwr"/>
<pin name="VCCPD8A" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCCL_2" direction="pwr"/>
<pin name="VCCL_3" direction="pwr"/>
<pin name="VCCIO1C" direction="pwr"/>
<pin name="VCCPD6A" direction="pwr"/>
<pin name="VCCL_4" direction="pwr"/>
<pin name="VCCL_5" direction="pwr"/>
<pin name="VCCL_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCL_7" direction="pwr"/>
<pin name="VCCL_8" direction="pwr"/>
<pin name="VCCPD1C" direction="pwr"/>
<pin name="VCCL_9" direction="pwr"/>
<pin name="VCCL_10" direction="pwr"/>
<pin name="VCCL_11" direction="pwr"/>
<pin name="VCCL" direction="pwr"/>
<pin name="VREF1C" direction="pwr"/>
<pin name="IO_1_2"/>
<pin name="IO_1_3"/>
<pin name="IO_1_4"/>
<pin name="IO_6_2"/>
<pin name="IO_6_3"/>
<pin name="IO_1_5"/>
<pin name="IO_1_6"/>
<pin name="IO_1_7"/>
<pin name="IO_1_8"/>
<pin name="IO_1_9"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_1_10"/>
<pin name="IO_6_4"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_1_11"/>
<pin name="IO_1_12"/>
<pin name="IO_1_13"/>
<pin name="IO_1_14"/>
<pin name="IO_1_15"/>
<pin name="IO_1_16"/>
<pin name="IO_1_17"/>
<pin name="IO_1_18"/>
<pin name="IO_1_19"/>
<pin name="IO_6_5"/>
<pin name="IO_6_6"/>
<pin name="IO_1_20"/>
<pin name="IO_1_21"/>
<pin name="IO_1_22"/>
<pin name="IO_1_23"/>
<pin name="IO_1_24"/>
<pin name="IO_1_25"/>
<pin name="IO_1_26"/>
<pin name="IO_1_27"/>
<pin name="IO_1_28"/>
<pin name="IO_1_29"/>
<pin name="IO_6_7"/>
<pin name="IO_6"/>
<pin name="IO_1_30"/>
<pin name="IO_1_31"/>
<pin name="IO_1_32"/>
<pin name="IO_1"/>
</symbol>
<symbol name="EP3SL150F1152C4N_H">
<pin name="VCCIO6C" direction="pwr"/>
<pin name="VCCPD6C" direction="pwr"/>
<pin name="VCCIO1C_2" direction="pwr"/>
<pin name="VCCL_2" direction="pwr"/>
<pin name="VCC_2" direction="pwr"/>
<pin name="VCCL_3" direction="pwr"/>
<pin name="VCCL_4" direction="pwr"/>
<pin name="VCCL_5" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCCL_6" direction="pwr"/>
<pin name="VCCL_7" direction="pwr"/>
<pin name="VCCL_8" direction="pwr"/>
<pin name="VCCL_9" direction="pwr"/>
<pin name="VCCL_10" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCCL_11" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCL_12" direction="pwr"/>
<pin name="VCCL_13" direction="pwr"/>
<pin name="VCCPT" direction="pwr"/>
<pin name="VCCL_14" direction="pwr"/>
<pin name="VCCD_PLL_L2" direction="pwr"/>
<pin name="VCCL_15" direction="pwr"/>
<pin name="VCCIO1C_3" direction="pwr"/>
<pin name="VCCL_16" direction="pwr"/>
<pin name="VCCL" direction="pwr"/>
<pin name="VCCPD2C" direction="pwr"/>
<pin name="VCCD_PLL_L3" direction="pwr"/>
<pin name="VCCIO1C" direction="pwr"/>
<pin name="VCCA_PLL_L2" direction="pwr"/>
<pin name="VCCA_PLL_L3" direction="pwr"/>
<pin name="CLK1P" direction="in"/>
<pin name="CLK1N" direction="in"/>
<pin name="CLK3N" direction="in"/>
<pin name="CLK3P" direction="in"/>
<pin name="VREF2C" direction="pwr"/>
<pin name="DNU" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_1_2"/>
<pin name="IO_1_3"/>
<pin name="IO_1_4"/>
<pin name="IO_1_5"/>
<pin name="IO_1_6"/>
<pin name="IO_1_7"/>
<pin name="IO_6"/>
<pin name="IO_1_8"/>
<pin name="IO_1_9"/>
<pin name="IO_1_10"/>
<pin name="IO_1_11"/>
<pin name="IO_1_12"/>
<pin name="IO_1_13"/>
<pin name="IO_1_PLL_L2_FB_CLKOUT0P"/>
<pin name="IO_1_PLL_L2_CLKOUT0N"/>
<pin name="IO_1_14"/>
<pin name="IO_6_PLL_R2_CLKOUT0N"/>
<pin name="IO_6_PLL_R2_FB_CLKOUT0P"/>
<pin name="IO_1_15"/>
<pin name="IO_1_16"/>
<pin name="IO_1"/>
<pin name="IO_5_PLL_R3_FB_CLKOUT0P"/>
<pin name="IO_2_2"/>
<pin name="IO_2_3"/>
<pin name="IO_2_PLL_L3_CLKOUT0N"/>
<pin name="IO_1_CLK0P"/>
<pin name="IO_1_CLK0N"/>
<pin name="IO_5_2"/>
<pin name="IO_5_3"/>
<pin name="IO_5"/>
<pin name="IO_2"/>
</symbol>
<symbol name="EP3SL150F1152C4N_I">
<pin name="VCCL_2" direction="pwr"/>
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCCL_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCCL_4" direction="pwr"/>
<pin name="VCCL_5" direction="pwr"/>
<pin name="VCCL_6" direction="pwr"/>
<pin name="VCCL_7" direction="pwr"/>
<pin name="VCCL_8" direction="pwr"/>
<pin name="VCCL_9" direction="pwr"/>
<pin name="VCCL_10" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCL_11" direction="pwr"/>
<pin name="VCCL" direction="pwr"/>
<pin name="VCCPD4A" direction="pwr"/>
<pin name="VCCIO2C_2" direction="pwr"/>
<pin name="VCCPD5A" direction="pwr"/>
<pin name="VCCIO2C_3" direction="pwr"/>
<pin name="VCCPD4B" direction="pwr"/>
<pin name="VCCIO2C" direction="pwr"/>
<pin name="VCCPD2A" direction="pwr"/>
<pin name="VCCPD5C" direction="pwr"/>
<pin name="VCCPD3C" direction="pwr"/>
<pin name="VCCIO2A" direction="pwr"/>
<pin name="VCCPD4C" direction="pwr"/>
<pin name="VREF2A" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2_PLL_L3_FB_CLKOUT0P"/>
<pin name="IO_2_2"/>
<pin name="IO_2_3"/>
<pin name="IO_2_4"/>
<pin name="IO_2_5"/>
<pin name="IO_2_CLK2P"/>
<pin name="IO_2_CLK2N"/>
<pin name="IO_5_2"/>
<pin name="IO_5_3"/>
<pin name="IO_2_6"/>
<pin name="IO_2_7"/>
<pin name="IO_2_8"/>
<pin name="IO_2_9"/>
<pin name="IO_2_10"/>
<pin name="IO_2_11"/>
<pin name="IO_2_12"/>
<pin name="IO_2_13"/>
<pin name="IO_5_4"/>
<pin name="IO_5_5"/>
<pin name="IO_2_14"/>
<pin name="IO_2_15"/>
<pin name="IO_2_16"/>
<pin name="IO_2_17"/>
<pin name="IO_2_18"/>
<pin name="IO_2_19"/>
<pin name="IO_2_20"/>
<pin name="IO_2_21"/>
<pin name="IO_2_22"/>
<pin name="IO_2_23"/>
<pin name="IO_5_6"/>
<pin name="IO_5_7"/>
<pin name="IO_2_24"/>
<pin name="IO_2_25"/>
<pin name="IO_2_26"/>
<pin name="IO_2_27"/>
<pin name="IO_2_28"/>
<pin name="IO_2_29"/>
<pin name="IO_2_30"/>
<pin name="IO_2_31"/>
<pin name="IO_2_32"/>
<pin name="IO_2"/>
<pin name="IO_5"/>
<pin name="IO_4"/>
</symbol>
<symbol name="EP3SL150F1152C4N_J">
<pin name="VCCPD3B" direction="pwr"/>
<pin name="VCCPD3A" direction="pwr"/>
<pin name="VCCPGM_2" direction="pwr"/>
<pin name="VCCIO2A" direction="pwr"/>
<pin name="VCCIO3A" direction="pwr"/>
<pin name="VCCIO2C" direction="pwr"/>
<pin name="VCCIO4C" direction="pwr"/>
<pin name="VCCIO3B" direction="pwr"/>
<pin name="VCCIO4A" direction="pwr"/>
<pin name="VCCPGM" direction="pwr"/>
<pin name="VCCD_PLL_B2" direction="pwr"/>
<pin name="VCCD_PLL_B1" direction="pwr"/>
<pin name="VCC_CLKIN4C" direction="pwr"/>
<pin name="NCONFIG" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="VREF4A" direction="pwr"/>
<pin name="VREF4B" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_3_2"/>
<pin name="IO_2_2"/>
<pin name="IO_2_3"/>
<pin name="IO_2_4"/>
<pin name="IO_2_5"/>
<pin name="IO_2_6"/>
<pin name="IO_2_7"/>
<pin name="IO_2_8"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_PLL_B2_CLKOUT3"/>
<pin name="IO_4_PLL_B2_CLKOUT4"/>
<pin name="IO_3_PLL_B1_CLKOUT0P"/>
<pin name="IO_3_PLL_B1_CLKOUT3"/>
<pin name="IO_3_3"/>
<pin name="IO_3_4"/>
<pin name="IO_2_9"/>
<pin name="IO_2_10"/>
<pin name="IO_2_11"/>
<pin name="IO_2_12"/>
<pin name="IO_2_13"/>
<pin name="IO_2_14"/>
<pin name="IO_2_15"/>
<pin name="IO_2_16"/>
<pin name="IO_4_4"/>
<pin name="IO_4_5"/>
<pin name="IO_4_6"/>
<pin name="IO_4_7"/>
<pin name="IO_4_8"/>
<pin name="IO_4_9"/>
<pin name="IO_4_PLL_B2_CLKOUT0P"/>
<pin name="IO_3_PLL_B1_CLKOUT0N"/>
<pin name="IO_3_PLL_B1_CLKOUT4"/>
<pin name="IO_3_5"/>
<pin name="IO_3_6"/>
<pin name="IO_3_7"/>
<pin name="IO_3_8"/>
<pin name="IO_3_9"/>
<pin name="IO_2_17"/>
<pin name="IO_2_18"/>
<pin name="IO_2_19"/>
<pin name="IO_2_20"/>
<pin name="IO_2_21"/>
<pin name="IO_2_22"/>
<pin name="IO_2_23"/>
<pin name="IO_2_24"/>
<pin name="IO_4_10"/>
<pin name="IO_4_11"/>
<pin name="IO_4_12"/>
<pin name="IO_4_13"/>
<pin name="IO_4_14"/>
<pin name="IO_4_PLL_B2_CLKOUT0N"/>
<pin name="IO_3_10"/>
<pin name="IO_3_11"/>
<pin name="IO_3_12"/>
<pin name="IO_3_13"/>
<pin name="IO_3"/>
<pin name="IO_2_25"/>
<pin name="IO_2_26"/>
<pin name="IO_2_27"/>
<pin name="IO_2_28"/>
<pin name="IO_2"/>
<pin name="IO_4_15"/>
<pin name="IO_4"/>
</symbol>
<symbol name="EP3SL150F1152C4N_K">
<pin name="VCCPT_2" direction="pwr"/>
<pin name="VCC_CLKIN3C" direction="pwr"/>
<pin name="VCCA_PLL_B2" direction="pwr"/>
<pin name="VCCIO2A_2" direction="pwr"/>
<pin name="VCCA_PLL_B1" direction="pwr"/>
<pin name="VCCIO4A" direction="pwr"/>
<pin name="VCCIO3C_2" direction="pwr"/>
<pin name="VCCIO4B" direction="pwr"/>
<pin name="VCCIO3C" direction="pwr"/>
<pin name="VCCIO2A" direction="pwr"/>
<pin name="VCCIO3A" direction="pwr"/>
<pin name="VCCPT" direction="pwr"/>
<pin name="VREF3B" direction="pwr"/>
<pin name="VREF3C" direction="pwr"/>
<pin name="VREF4C" direction="pwr"/>
<pin name="VREF3A" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_3_4"/>
<pin name="IO_2_2"/>
<pin name="IO_2_3"/>
<pin name="IO_2_4"/>
<pin name="IO_2_5"/>
<pin name="IO_2_6"/>
<pin name="IO_2_7"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4_5"/>
<pin name="IO_3_5"/>
<pin name="IO_3_6"/>
<pin name="IO_3_7"/>
<pin name="IO_3_8"/>
<pin name="IO_3_9"/>
<pin name="IO_3_10"/>
<pin name="IO_3_11"/>
<pin name="NSTATUS"/>
<pin name="CONF_DONE"/>
<pin name="IO_2_8"/>
<pin name="IO_2_9"/>
<pin name="IO_2_10"/>
<pin name="IO_2_11"/>
<pin name="IO_4_6"/>
<pin name="IO_4_7"/>
<pin name="IO_4_8"/>
<pin name="IO_4_9"/>
<pin name="IO_4_10"/>
<pin name="IO_4_11"/>
<pin name="IO_4_12"/>
<pin name="IO_3_12"/>
<pin name="IO_3_13"/>
<pin name="IO_3_14"/>
<pin name="IO_3_15"/>
<pin name="IO_3_16"/>
<pin name="IO_3_17"/>
<pin name="IO_3_18"/>
<pin name="IO_3_RUP3A"/>
<pin name="IO_3_19"/>
<pin name="IO_2_12"/>
<pin name="IO_2_13"/>
<pin name="IO_2_14"/>
<pin name="IO_4_13"/>
<pin name="IO_4_14"/>
<pin name="IO_4_15"/>
<pin name="IO_4_16"/>
<pin name="IO_4_17"/>
<pin name="IO_3_20"/>
<pin name="IO_3_PLL_B1_FBN/CLKOUT2"/>
<pin name="IO_3_PLL_B1_FBP/CLKOUT1"/>
<pin name="IO_3_21"/>
<pin name="IO_3_22"/>
<pin name="IO_3_23"/>
<pin name="IO_3_24"/>
<pin name="IO_3"/>
<pin name="IO_3_RDN3A"/>
<pin name="IO_2_RUP2A"/>
<pin name="IO_2_RDN2A"/>
<pin name="IO_2_15"/>
<pin name="IO_2"/>
<pin name="IO_4_18"/>
<pin name="IO_4_19"/>
<pin name="IO_4"/>
</symbol>
<symbol name="EP3SL150F1152C4N_L">
<pin name="VCCIO2A" direction="pwr"/>
<pin name="VCCIO4C_2" direction="pwr"/>
<pin name="VCCIO3A_2" direction="pwr"/>
<pin name="VCCIO4B" direction="pwr"/>
<pin name="VCCIO4C" direction="pwr"/>
<pin name="VCCIO3C" direction="pwr"/>
<pin name="VCCIO3B" direction="pwr"/>
<pin name="VCCIO3A" direction="pwr"/>
<pin name="IO_3_2"/>
<pin name="IO_3_3"/>
<pin name="IO_3_4"/>
<pin name="IO_3_5"/>
<pin name="IO_3_6"/>
<pin name="IO_3_7"/>
<pin name="IO_3_8"/>
<pin name="IO_3_9"/>
<pin name="IO_3_10"/>
<pin name="IO_3_11"/>
<pin name="IO_3_12"/>
<pin name="IO_3_13"/>
<pin name="IO_2_2"/>
<pin name="IO_2_3"/>
<pin name="IO_2_4"/>
<pin name="IO_4_2"/>
<pin name="IO_4_3"/>
<pin name="IO_4_4"/>
<pin name="IO_4_5"/>
<pin name="IO_4_6"/>
<pin name="IO_3_14"/>
<pin name="IO_3_15"/>
<pin name="IO_3_16"/>
<pin name="IO_3_17"/>
<pin name="IO_3_18"/>
<pin name="IO_3_19"/>
<pin name="IO_3_20"/>
<pin name="IO_3_21"/>
<pin name="IO_3_22"/>
<pin name="IO_3_23"/>
<pin name="IO_3_24"/>
<pin name="IO_3_25"/>
<pin name="IO_2"/>
<pin name="IO_4_7"/>
<pin name="IO_4_8"/>
<pin name="IO_4_9"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_4_10"/>
<pin name="IO_4_11"/>
<pin name="IO_4_12"/>
<pin name="IO_4_13"/>
<pin name="IO_4_PLL_B2_FBP/CLKOUT1"/>
<pin name="IO_4_PLL_B2_FBN/CLKOUT2"/>
<pin name="IO_4_CLK7P"/>
<pin name="IO_4_CLK6P"/>
<pin name="IO_3_CLK4P"/>
<pin name="IO_3_CLK5P"/>
<pin name="IO_3_26"/>
<pin name="IO_3_27"/>
<pin name="IO_3_28"/>
<pin name="IO_3_29"/>
<pin name="IO_3_30"/>
<pin name="IO_3_31"/>
<pin name="IO_3_32"/>
<pin name="IO_3_33"/>
<pin name="IO_3_34"/>
<pin name="IO_4_14"/>
<pin name="IO_4_15"/>
<pin name="IO_4_16"/>
<pin name="IO_4_17"/>
<pin name="IO_4"/>
<pin name="IO_4_CLK7N"/>
<pin name="IO_4_CLK6N"/>
<pin name="IO_3_CLK4N"/>
<pin name="IO_3_CLK5N"/>
<pin name="IO_3_35"/>
<pin name="IO_3_36"/>
<pin name="IO_3_37"/>
<pin name="IO_3_38"/>
<pin name="IO_3_39"/>
<pin name="IO_3_40"/>
<pin name="IO_3_41"/>
<pin name="IO_3_42"/>
<pin name="IO_3_43"/>
<pin name="IO_3_44"/>
<pin name="IO_3_45"/>
<pin name="IO_3_46"/>
<pin name="IO_3_47"/>
<pin name="IO_3"/>
</symbol>
<symbol name="EPC1064PC8">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
<pin name="NCASC" direction="out"/>
</symbol>
<symbol name="EPC1441LC20N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="NCASC" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPC1441TC32N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OE" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C_3" direction="nc"/>
<pin name="N.C_4" direction="nc"/>
<pin name="N.C_5" direction="nc"/>
<pin name="N.C_6" direction="nc"/>
<pin name="N.C_7" direction="nc"/>
<pin name="N.C_8" direction="nc"/>
<pin name="N.C_9" direction="nc"/>
<pin name="N.C_10" direction="nc"/>
<pin name="N.C_11" direction="nc"/>
<pin name="N.C_12" direction="nc"/>
<pin name="N.C_13" direction="nc"/>
<pin name="N.C_14" direction="nc"/>
<pin name="N.C_15" direction="nc"/>
<pin name="N.C_16" direction="nc"/>
<pin name="N.C_17" direction="nc"/>
<pin name="N.C_18" direction="nc"/>
<pin name="N.C_19" direction="nc"/>
<pin name="N.C_20" direction="nc"/>
<pin name="N.C_21" direction="nc"/>
<pin name="N.C_22" direction="nc"/>
<pin name="N.C_23" direction="nc"/>
<pin name="N.C_24" direction="nc"/>
<pin name="N.C_25" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPC16QC100N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~BYTE/VCC" direction="pwr"/>
<pin name="VCCW" direction="pwr"/>
<pin name="FLOATING_2" direction="in"/>
<pin name="FLOATING_3" direction="in"/>
<pin name="FLOATING_4" direction="in"/>
<pin name="FLOATING_5" direction="in"/>
<pin name="FLOATING" direction="in"/>
<pin name="RY/~BY~/FLOATING" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="~F_-WE~" direction="in"/>
<pin name="EXCLK" direction="in"/>
<pin name="~F-RP~" direction="in"/>
<pin name="~OE~" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="~CE~" direction="in"/>
<pin name="TM1" direction="in"/>
<pin name="TM0" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="F-A0" direction="in"/>
<pin name="F-A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="F-A15" direction="in"/>
<pin name="F-A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="C-A0" direction="out"/>
<pin name="C-A1" direction="out"/>
<pin name="C-A15" direction="out"/>
<pin name="C-A16" direction="out"/>
<pin name="~INIT_CONF~" direction="out"/>
<pin name="~C-WE~" direction="out"/>
<pin name="~C-RP~" direction="out"/>
<pin name="OE"/>
<pin name="TDO" direction="out"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="DATA0" direction="out"/>
<pin name="DATA1" direction="out"/>
<pin name="DATA2" direction="out"/>
<pin name="DATA3" direction="out"/>
<pin name="DATA4" direction="out"/>
<pin name="DATA5" direction="out"/>
<pin name="DATA6" direction="out"/>
<pin name="DATA7" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EPC16QI100N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~BYTE/VCC" direction="pwr"/>
<pin name="VCCW" direction="pwr"/>
<pin name="FLOATING_2" direction="in"/>
<pin name="FLOATING_3" direction="in"/>
<pin name="FLOATING_4" direction="in"/>
<pin name="FLOATING_5" direction="in"/>
<pin name="FLOATING" direction="in"/>
<pin name="RY/~BY~/FLOATING" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="~F_-WE~" direction="in"/>
<pin name="EXCLK" direction="in"/>
<pin name="~F-RP~" direction="in"/>
<pin name="~OE~" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="~CE~" direction="in"/>
<pin name="TM1" direction="in"/>
<pin name="TM0" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="F-A0" direction="in"/>
<pin name="F-A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="F-A15" direction="in"/>
<pin name="F-A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="C-A0" direction="out"/>
<pin name="C-A1" direction="out"/>
<pin name="C-A15" direction="out"/>
<pin name="C-A16" direction="out"/>
<pin name="~INIT_CONF~" direction="out"/>
<pin name="~C-WE~" direction="out"/>
<pin name="~C-RP~" direction="out"/>
<pin name="OE"/>
<pin name="TDO" direction="out"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="DATA0" direction="out"/>
<pin name="DATA1" direction="out"/>
<pin name="DATA2" direction="out"/>
<pin name="DATA3" direction="out"/>
<pin name="DATA4" direction="out"/>
<pin name="DATA5" direction="out"/>
<pin name="DATA6" direction="out"/>
<pin name="DATA7" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EPC16UC88N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCW" direction="pwr"/>
<pin name="N_INIT___CONF" direction="in"/>
<pin name="F_-WE" direction="in"/>
<pin name="RY/BY" direction="in"/>
<pin name="C_-WE" direction="in"/>
<pin name="F_-_RP" direction="in"/>
<pin name="C_-_RP" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="TM1" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="OE_2" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TM0" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="EXCLK" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="A20" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="DQ1_2"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="DATA0" direction="out"/>
<pin name="DATA1" direction="out"/>
<pin name="DATA2" direction="out"/>
<pin name="DATA3" direction="out"/>
<pin name="DATA4" direction="out"/>
<pin name="DATA5" direction="out"/>
<pin name="DATA6" direction="out"/>
<pin name="DATA7" direction="out"/>
</symbol>
<symbol name="EPC1LC20N">
<pin name="VCC" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VPPSEL" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="NINIT_CONF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VPP" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="DATA" direction="out"/>
<pin name="NCASC" direction="out"/>
</symbol>
<symbol name="EPC1PI8">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
<pin name="NCASC" direction="out"/>
</symbol>
<symbol name="EPC2LC20">
<pin name="VCC" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VPP" direction="pwr"/>
<pin name="VPPSEL" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="~INIT_CONF" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~CASC" direction="out"/>
<pin name="DATA" direction="out"/>
<pin name="OE"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="EPC2LI20N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="NCASC" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPC2TC32N">
<pin name="VCC" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VPP" direction="pwr"/>
<pin name="VPPSEL" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCS_2" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="NCASC" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="NINIT_CONF" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPC2TI32N">
<pin name="VCC" direction="pwr"/>
<pin name="VCCSEL" direction="pwr"/>
<pin name="VPP" direction="pwr"/>
<pin name="VPPSEL" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="NCS_2" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="NCASC" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="NINIT_CONF" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPC4QC100N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~BYTE/VCC" direction="pwr"/>
<pin name="VCCW" direction="pwr"/>
<pin name="FLOATING_2" direction="in"/>
<pin name="FLOATING_3" direction="in"/>
<pin name="FLOATING_4" direction="in"/>
<pin name="FLOATING_5" direction="in"/>
<pin name="FLOATING" direction="in"/>
<pin name="RY/~BY~/FLOATING" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="~F_-WE~" direction="in"/>
<pin name="EXCLK" direction="in"/>
<pin name="~F-RP~" direction="in"/>
<pin name="~OE~" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="~CE~" direction="in"/>
<pin name="TM1" direction="in"/>
<pin name="TM0" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="F-A0" direction="in"/>
<pin name="F-A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="F-A15" direction="in"/>
<pin name="F-A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="C-A0" direction="out"/>
<pin name="C-A1" direction="out"/>
<pin name="C-A15" direction="out"/>
<pin name="C-A16" direction="out"/>
<pin name="~INIT_CONF~" direction="out"/>
<pin name="~C-WE~" direction="out"/>
<pin name="~C-RP~" direction="out"/>
<pin name="OE"/>
<pin name="TDO" direction="out"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="DATA0" direction="out"/>
<pin name="DATA1" direction="out"/>
<pin name="DATA2" direction="out"/>
<pin name="DATA3" direction="out"/>
<pin name="DATA4" direction="out"/>
<pin name="DATA5" direction="out"/>
<pin name="DATA6" direction="out"/>
<pin name="DATA7" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EPC8QC100N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~BYTE/VCC" direction="pwr"/>
<pin name="VCCW" direction="pwr"/>
<pin name="FLOATING_2" direction="in"/>
<pin name="FLOATING_3" direction="in"/>
<pin name="FLOATING_4" direction="in"/>
<pin name="FLOATING_5" direction="in"/>
<pin name="FLOATING" direction="in"/>
<pin name="RY/~BY~/FLOATING" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="~F_-WE~" direction="in"/>
<pin name="EXCLK" direction="in"/>
<pin name="~F-RP~" direction="in"/>
<pin name="~OE~" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="~CE~" direction="in"/>
<pin name="TM1" direction="in"/>
<pin name="TM0" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="F-A0" direction="in"/>
<pin name="F-A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="F-A15" direction="in"/>
<pin name="F-A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="C-A0" direction="out"/>
<pin name="C-A1" direction="out"/>
<pin name="C-A15" direction="out"/>
<pin name="C-A16" direction="out"/>
<pin name="~INIT_CONF~" direction="out"/>
<pin name="~C-WE~" direction="out"/>
<pin name="~C-RP~" direction="out"/>
<pin name="OE"/>
<pin name="TDO" direction="out"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="DATA0" direction="out"/>
<pin name="DATA1" direction="out"/>
<pin name="DATA2" direction="out"/>
<pin name="DATA3" direction="out"/>
<pin name="DATA4" direction="out"/>
<pin name="DATA5" direction="out"/>
<pin name="DATA6" direction="out"/>
<pin name="DATA7" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EPC8QI100N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~BYTE/VCC" direction="pwr"/>
<pin name="VCCW" direction="pwr"/>
<pin name="FLOATING_2" direction="in"/>
<pin name="FLOATING_3" direction="in"/>
<pin name="FLOATING_4" direction="in"/>
<pin name="FLOATING_5" direction="in"/>
<pin name="FLOATING" direction="in"/>
<pin name="RY/~BY~/FLOATING" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="~F_-WE~" direction="in"/>
<pin name="EXCLK" direction="in"/>
<pin name="~F-RP~" direction="in"/>
<pin name="~OE~" direction="in"/>
<pin name="PORSEL" direction="in"/>
<pin name="~CE~" direction="in"/>
<pin name="TM1" direction="in"/>
<pin name="TM0" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="F-A0" direction="in"/>
<pin name="F-A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="F-A15" direction="in"/>
<pin name="F-A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="GND/NC_2" direction="pas"/>
<pin name="GND/NC_3" direction="pas"/>
<pin name="GND/NC_4" direction="pas"/>
<pin name="GND/NC_5" direction="pas"/>
<pin name="GND/NC_6" direction="pas"/>
<pin name="GND/NC" direction="pas"/>
<pin name="C-A0" direction="out"/>
<pin name="C-A1" direction="out"/>
<pin name="C-A15" direction="out"/>
<pin name="C-A16" direction="out"/>
<pin name="~INIT_CONF~" direction="out"/>
<pin name="~C-WE~" direction="out"/>
<pin name="~C-RP~" direction="out"/>
<pin name="OE"/>
<pin name="TDO" direction="out"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="DATA0" direction="out"/>
<pin name="DATA1" direction="out"/>
<pin name="DATA2" direction="out"/>
<pin name="DATA3" direction="out"/>
<pin name="DATA4" direction="out"/>
<pin name="DATA5" direction="out"/>
<pin name="DATA6" direction="out"/>
<pin name="DATA7" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="EPCS1SI8N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="ASDI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPCS64SI16N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="DCLK" direction="in"/>
<pin name="ASDI" direction="in"/>
<pin name="NCS" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C_5" direction="nc"/>
<pin name="N/C_6" direction="nc"/>
<pin name="N/C_7" direction="nc"/>
<pin name="N/C_8" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DATA" direction="out"/>
</symbol>
<symbol name="EPF10K10QC208-4N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="NSTATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO"/>
<pin name="IO/RDY/NBSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/CLKUSR"/>
</symbol>
<symbol name="EPF10K10QC208-4N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K10QC208-4N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/NWS"/>
<pin name="IO/CS"/>
<pin name="IO/NRS"/>
<pin name="IO/NCS"/>
<pin name="IO/DEV_NCLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K10TC144-3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/RDY/NBSY"/>
<pin name="NSTATUS" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K10TC144-3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/CS"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K10TI144-4N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/RDY/NBSY"/>
<pin name="NSTATUS" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K10TI144-4N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/CS"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K20TC144-3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/RDY/NBSY"/>
<pin name="NSTATUS" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K20TC144-3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/CS"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K20TI144-4N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/RDY/NBSY"/>
<pin name="NSTATUS" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K20TI144-4N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/CS"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K30ATC144-3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="NCEO" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="IO/CLKUSR"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/RDY/NBSY"/>
<pin name="NSTATUS" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF10K30ATC144-3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="NCE" direction="in"/>
<pin name="NCONFIG" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="DATA0"/>
<pin name="IO/DATA1"/>
<pin name="IO/DATA2"/>
<pin name="IO/DATA3"/>
<pin name="IO/DATA4"/>
<pin name="IO/DATA5"/>
<pin name="IO/DATA6"/>
<pin name="IO/DATA7"/>
<pin name="IO/CS"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/NCS"/>
<pin name="IO/NRS"/>
<pin name="IO/NWS"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF6016ATC144-3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="IO/TCK"/>
<pin name="MSEL" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO/NCEO" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IN_2" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF6016ATC144-3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="IN_2" direction="pas"/>
<pin name="DATA" direction="pas"/>
<pin name="DCLK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IN" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/INIT_DONE" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO/CLKUSR" direction="pas"/>
<pin name="IO/RDYNBUSY" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
<pin name="IO/NCS" direction="pas"/>
<pin name="IO/CS" direction="pas"/>
<pin name="IO/NRS" direction="pas"/>
<pin name="IO/NWS" direction="pas"/>
<pin name="IO/DEV_CLRN" direction="pas"/>
<pin name="IO/DEV_OE" direction="pas"/>
</symbol>
<symbol name="EPF6016QC208-2N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="NCE" direction="in"/>
<pin name="INPUT_2" direction="pas"/>
<pin name="INPUT" direction="pas"/>
<pin name="MSEL" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF6016QC208-2N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="INPUT_2" direction="pas"/>
<pin name="INPUT" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO/NCEO"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/TDO"/>
</symbol>
<symbol name="EPF6016QC208-2N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="IO/NRS"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="CLKUSR" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO/NCS"/>
<pin name="IO/CS"/>
<pin name="IO/NWS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPF6016TC144-2N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="IO/TCK"/>
<pin name="MSEL" direction="pas"/>
<pin name="NCE" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO/NCEO" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IN_2" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF6016TC144-2N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="IN_2" direction="pas"/>
<pin name="DATA" direction="pas"/>
<pin name="DCLK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IN" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/INIT_DONE" direction="pas"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO/CLKUSR" direction="pas"/>
<pin name="IO/RDYNBUSY" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
<pin name="IO/NCS" direction="pas"/>
<pin name="IO/CS" direction="pas"/>
<pin name="IO/NRS" direction="pas"/>
<pin name="IO/NWS" direction="pas"/>
<pin name="IO/DEV_CLRN" direction="pas"/>
<pin name="IO/DEV_OE" direction="pas"/>
</symbol>
<symbol name="EPF6016TC144-3N_A">
<pin name="*CE" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="MSEL" direction="in"/>
<pin name="*STATUS" direction="in"/>
<pin name="IO/TDI"/>
<pin name="*CONFIG" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/*CEO"/>
<pin name="IO/TMS"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF6016TC144-3N_B">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="DATA" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="IO/RDY/*BUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/CLKUSR"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="IO/TDO"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO/*CS"/>
<pin name="IO/CS"/>
<pin name="IO/*WS"/>
<pin name="IO/*RS"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="DCLK" direction="in"/>
<pin name="IO/DEV_*CLR"/>
</symbol>
<symbol name="EPF6024AQC208-3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="NCE" direction="in"/>
<pin name="INPUT_2" direction="pas"/>
<pin name="INPUT" direction="pas"/>
<pin name="MSEL" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPF6024AQC208-3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="INPUT_2" direction="pas"/>
<pin name="INPUT" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO/NCEO"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
<pin name="IO/RDYNBUSY"/>
<pin name="IO/INIT_DONE"/>
<pin name="IO/TDO"/>
</symbol>
<symbol name="EPF6024AQC208-3N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="IO/NRS"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="CLKUSR" direction="pas"/>
<pin name="DCLK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO/NCS"/>
<pin name="IO/CS"/>
<pin name="IO/NWS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPF8282ATC100-4N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT_5" direction="pwr"/>
<pin name="VCCINT_6" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT_2" direction="pas"/>
<pin name="INPUT_3" direction="pas"/>
<pin name="DCLK" direction="pas"/>
<pin name="DATA1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DATA2" direction="in"/>
<pin name="DATA3" direction="in"/>
<pin name="DATA4" direction="in"/>
<pin name="DATA5" direction="in"/>
<pin name="DATA6" direction="in"/>
<pin name="DATA7" direction="in"/>
<pin name="CONF_DONE" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/CS"/>
<pin name="IO/*CS"/>
<pin name="IO/TMS"/>
<pin name="IO/NWS"/>
<pin name="INPUT_4" direction="pas"/>
<pin name="RDCLK" direction="pas"/>
<pin name="NSTATUS" direction="pas"/>
<pin name="CLKUSR" direction="pas"/>
<pin name="NCONFIG" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="TRST" direction="pas"/>
<pin name="MSEL1" direction="pas"/>
<pin name="MSEL0" direction="pas"/>
<pin name="NRS" direction="pas"/>
<pin name="NSP" direction="pas"/>
<pin name="RDYNBUSY" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/ADD2"/>
<pin name="IO/ADD3"/>
<pin name="IO/ADD4"/>
<pin name="IO/ADD5"/>
<pin name="IO/ADD6"/>
<pin name="IO/ADD7"/>
<pin name="IO/ADD8"/>
<pin name="IO/ADD9"/>
<pin name="IO/ADD10"/>
<pin name="IO/ADD11"/>
<pin name="IO/ADD12"/>
<pin name="IO/ADD13"/>
<pin name="IO/ADD14"/>
<pin name="IO/ADD15"/>
<pin name="IO/ADD16"/>
<pin name="IO/ADD17"/>
<pin name="IO/TDI"/>
<pin name="IO/TCK"/>
<pin name="INPUT" direction="pas"/>
<pin name="IO/ADD1"/>
<pin name="IO/ADD0"/>
<pin name="IO/SDOUT"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256C3N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM1270F256C3N_B">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM1270F256C3N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
</symbol>
<symbol name="EPM1270F256C4N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256C4N_B">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256C4N_C">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256C5N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM1270F256C5N_B">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256C5N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256I5N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM1270F256I5N_B">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270F256I5N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270GM256C5N_A">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="R4" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270GM256C5N_B">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270GM256C5N_C">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3_4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270GT144C4N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM1270GT144C4N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM1270GT144C5N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM1270GT144C5N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM1270M256C5N_A">
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="R4" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270M256C5N_B">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270M256C5N_C">
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3_4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4_4" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM1270T144C3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM1270T144C3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM1270T144C5N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM1270T144C5N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM1270T144I5N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM1270T144I5N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM2210F256C4N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM2210F256C4N_B">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F256C4N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F256C5N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM2210F256C5N_B">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F256C5N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F256I5N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM2210F256I5N_B">
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F256I5N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C3N_A">
<pin name="GNDIO_2" direction="pas"/>
<pin name="IO_2"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="GNDINT" direction="pas"/>
<pin name="VCCINT" direction="pwr"/>
</symbol>
<symbol name="EPM2210F324C3N_B">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO/GCLK1"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="TDI" direction="in"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="TDO" direction="in"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="TMS" direction="in"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="TCK" direction="in"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_58"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C3N_C">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="IO_8"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="GNDINT" direction="pas"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C3N_D">
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="IO/GCLK2"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO/*DEV_CLR"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO"/>
<pin name="GNDIO" direction="pas"/>
</symbol>
<symbol name="EPM2210F324C4N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C4N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK1"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C4N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C4N_D">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK2"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C5N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C5N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK1"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C5N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210F324C5N_D">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO/GCLK2"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210GF256C3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT_5" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210GF256C3N_B">
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="VCCIO4_3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210GF256C3N_C">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="VCCIO3_3" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210GF324C5N_A">
<pin name="GNDIO_2" direction="pas"/>
<pin name="IO_2"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="GNDINT" direction="pas"/>
<pin name="VCCINT" direction="pwr"/>
</symbol>
<symbol name="EPM2210GF324C5N_B">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO/GCLK1"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="TDI" direction="in"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="TDO" direction="in"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO/DEV_OE"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="TMS" direction="in"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="TCK" direction="in"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_58"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210GF324C5N_C">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="IO_8"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="GNDINT" direction="pas"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM2210GF324C5N_D">
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="VCCIO3_2" direction="pwr"/>
<pin name="IO/GCLK2"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="VCCIO4_2" direction="pwr"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO/*DEV_CLR"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="VCCIO4" direction="pwr"/>
<pin name="IO"/>
<pin name="GNDIO" direction="pas"/>
</symbol>
<symbol name="EPM240GM100C5N">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="IO/GCLK1" direction="in"/>
<pin name="IO/GCLK0" direction="in"/>
<pin name="IO/GCLK2" direction="in"/>
<pin name="IO/GCLK3" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
<pin name="IO/NDEV_CLR"/>
<pin name="IO/DEV_OE"/>
</symbol>
<symbol name="EPM240GT100C3N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM240M100C4N">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="IO/GCLK1" direction="in"/>
<pin name="IO/GCLK0" direction="in"/>
<pin name="IO/GCLK2" direction="in"/>
<pin name="IO/GCLK3" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
<pin name="IO/NDEV_CLR"/>
<pin name="IO/DEV_OE"/>
</symbol>
<symbol name="EPM240T100C3N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM240T100C5N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM240T100I5N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM3032ALC44-10N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3032ATC44-4N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3032ATC44-7N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3032ATI44-10N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ALC44-10N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
<pin name="I/O/TDI"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
</symbol>
<symbol name="EPM3064ATC100-10N">
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/*GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATC100-4N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATC100-7N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATC44-10N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATC44-4N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATC44-7N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATI100-10N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3064ATI44-10N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC100-10N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC100-5N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC100-7N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C._14" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO_8" direction="pas"/>
<pin name="GNDIO_9" direction="pas"/>
<pin name="GNDIO_10" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC144-10N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC144-10N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC144-5N_A">
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO/TMS"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC144-5N_B">
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/*GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO/TDO"/>
<pin name="IO/TCK"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC144-7N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3128ATC144-7N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256AQC208-10N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256AQC208-10N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256AQC208-10N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256AQC208-7N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256AQC208-7N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256AQC208-7N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256ATC144-10N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256ATC144-10N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3256ATC144-7N_A">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
<pin name="IO/TMS"/>
<pin name="IO/TDI"/>
</symbol>
<symbol name="EPM3256ATC144-7N_B">
<pin name="IO/TCK"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/*GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO/TDO"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3512AQC208-10N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3512AQC208-10N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TMS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM3512AQC208-10N_C">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570F100C4N">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK0"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO/GCLK2"/>
<pin name="IO/*DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/GCLK3"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570F256C4N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM570F256C4N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570F256C4N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570F256C5N_A">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
</symbol>
<symbol name="EPM570F256C5N_B">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO_7" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570F256C5N_C">
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570GF100C5N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK0"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO/DEV_CLRN"/>
</symbol>
<symbol name="EPM570GM100C5N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EPM570GT100C5N">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570GT144C3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570GT144C3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570M100C4N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EPM570M100C5N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
<pin name="TDO" direction="pas"/>
</symbol>
<symbol name="EPM570M100I5N">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO/*DEV_CLR"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK0"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="TDO" direction="out"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570M256C5N_A">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK0"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C_3" direction="nc"/>
<pin name="N.C_4" direction="nc"/>
<pin name="N.C_5" direction="nc"/>
<pin name="N.C_6" direction="nc"/>
<pin name="N.C_7" direction="nc"/>
<pin name="N.C_8" direction="nc"/>
<pin name="N.C_9" direction="nc"/>
<pin name="N.C_10" direction="nc"/>
<pin name="N.C_11" direction="nc"/>
<pin name="N.C_12" direction="nc"/>
<pin name="N.C_13" direction="nc"/>
<pin name="N.C_14" direction="nc"/>
<pin name="N.C_15" direction="nc"/>
<pin name="N.C_16" direction="nc"/>
<pin name="N.C_17" direction="nc"/>
<pin name="N.C_18" direction="nc"/>
<pin name="N.C_19" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570M256C5N_B">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C_3" direction="nc"/>
<pin name="N.C_4" direction="nc"/>
<pin name="N.C_5" direction="nc"/>
<pin name="N.C_6" direction="nc"/>
<pin name="N.C_7" direction="nc"/>
<pin name="N.C_8" direction="nc"/>
<pin name="N.C_9" direction="nc"/>
<pin name="N.C_10" direction="nc"/>
<pin name="N.C_11" direction="nc"/>
<pin name="N.C_12" direction="nc"/>
<pin name="N.C_13" direction="nc"/>
<pin name="N.C_14" direction="nc"/>
<pin name="N.C_15" direction="nc"/>
<pin name="N.C_16" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570M256C5N_C">
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK3"/>
<pin name="IO/GCLK2"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C_3" direction="nc"/>
<pin name="N.C_4" direction="nc"/>
<pin name="N.C_5" direction="nc"/>
<pin name="N.C_6" direction="nc"/>
<pin name="N.C_7" direction="nc"/>
<pin name="N.C_8" direction="nc"/>
<pin name="N.C_9" direction="nc"/>
<pin name="N.C_10" direction="nc"/>
<pin name="N.C_11" direction="nc"/>
<pin name="N.C_12" direction="nc"/>
<pin name="N.C_13" direction="nc"/>
<pin name="N.C_14" direction="nc"/>
<pin name="N.C_15" direction="nc"/>
<pin name="N.C_16" direction="nc"/>
<pin name="N.C_17" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570T100C3N">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570T100C4N">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570T100C5N">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570T100I5N">
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="TMS" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDINT_3" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDINT_4" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM570T144C3N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570T144C3N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570T144C5N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570T144C5N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570T144I5N_A">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO1_2" direction="pwr"/>
<pin name="VCCIO1_3" direction="pwr"/>
<pin name="VCCIO1_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="IO/GCLK0"/>
<pin name="IO/GCLK1"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO/DEV_OE"/>
<pin name="IO/DEV_CLRN"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM570T144I5N_B">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO2_2" direction="pwr"/>
<pin name="VCCIO2_3" direction="pwr"/>
<pin name="VCCIO2_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="IO_2" direction="pas"/>
<pin name="IO_3" direction="pas"/>
<pin name="IO_4" direction="pas"/>
<pin name="IO_5" direction="pas"/>
<pin name="IO_6" direction="pas"/>
<pin name="IO_7" direction="pas"/>
<pin name="IO_8" direction="pas"/>
<pin name="IO_9" direction="pas"/>
<pin name="IO_10" direction="pas"/>
<pin name="IO_11" direction="pas"/>
<pin name="IO_12" direction="pas"/>
<pin name="IO_13" direction="pas"/>
<pin name="IO_14" direction="pas"/>
<pin name="IO_15" direction="pas"/>
<pin name="IO_16" direction="pas"/>
<pin name="IO_17" direction="pas"/>
<pin name="IO_18" direction="pas"/>
<pin name="IO_19" direction="pas"/>
<pin name="IO_20" direction="pas"/>
<pin name="IO_21" direction="pas"/>
<pin name="IO_22" direction="pas"/>
<pin name="IO_23" direction="pas"/>
<pin name="IO_24" direction="pas"/>
<pin name="IO_25" direction="pas"/>
<pin name="IO_26" direction="pas"/>
<pin name="IO_27" direction="pas"/>
<pin name="IO_28" direction="pas"/>
<pin name="IO_29" direction="pas"/>
<pin name="IO/GCLK2"/>
<pin name="IO/GCLK3"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_30" direction="pas"/>
<pin name="IO_31" direction="pas"/>
<pin name="IO_32" direction="pas"/>
<pin name="IO_33" direction="pas"/>
<pin name="IO_34" direction="pas"/>
<pin name="IO_35" direction="pas"/>
<pin name="IO_36" direction="pas"/>
<pin name="IO_37" direction="pas"/>
<pin name="IO_38" direction="pas"/>
<pin name="IO_39" direction="pas"/>
<pin name="IO_40" direction="pas"/>
<pin name="IO_41" direction="pas"/>
<pin name="IO_42" direction="pas"/>
<pin name="IO_43" direction="pas"/>
<pin name="IO_44" direction="pas"/>
<pin name="IO_45" direction="pas"/>
<pin name="IO_46" direction="pas"/>
<pin name="IO_47" direction="pas"/>
<pin name="IO_48" direction="pas"/>
<pin name="IO_49" direction="pas"/>
<pin name="IO_50" direction="pas"/>
<pin name="IO_51" direction="pas"/>
<pin name="IO_52" direction="pas"/>
<pin name="IO_53" direction="pas"/>
<pin name="IO_54" direction="pas"/>
<pin name="IO_55" direction="pas"/>
<pin name="IO_56" direction="pas"/>
<pin name="IO_57" direction="pas"/>
<pin name="IO_58" direction="pas"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="EPM7032AETC44-10N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1N" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7032AETC44-4N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1N" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7032AETI44-7N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1N" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064AETI44-7N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064LC44-15">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064LI44-15">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064SLC44-10">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064SLC44-10N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064SLI44-7N">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064STC44-10N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064STC44-7N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7064STI44-7N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT_3" direction="pwr"/>
<pin name="VCCINT_4" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/~GCLR" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128AETC100-10N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128AETC100-5N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128AETC144-10N_A">
<pin name="IO/TDI"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO/TMS"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C._8" direction="nc"/>
<pin name="N.C._9" direction="nc"/>
<pin name="N.C._10" direction="nc"/>
<pin name="N.C._11" direction="nc"/>
<pin name="N.C._12" direction="nc"/>
<pin name="N.C._13" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128AETC144-10N_B">
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/*GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C._7" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="IO/TDO"/>
<pin name="IO/TCK"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128AETI100-7N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128SLC84-15N">
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO/TCK"/>
<pin name="IO/TDI"/>
<pin name="IO/TDO"/>
<pin name="IO/TMS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128SLC84-10">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GLCRN" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE2/(GCLK2)" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO/TCK"/>
<pin name="IO/TMS"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128SQC100-10N">
<pin name="VCCIO_(3.3_V_OR_5.0_V)" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_2" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_3" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_4" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_5" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_6" direction="pwr"/>
<pin name="VCCINT_(5.0_V_ONLY)" direction="pwr"/>
<pin name="VCCINT_(5.0_V_ONLY)_2" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128SQC160-15N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128SQC160-15N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128SQI100-10N">
<pin name="VCCIO_(3.3_V_OR_5.0_V)" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_2" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_3" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_4" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_5" direction="pwr"/>
<pin name="VCCIO_(3.3_V_OR_5.0_V)_6" direction="pwr"/>
<pin name="VCCINT_(5.0_V_ONLY)" direction="pwr"/>
<pin name="VCCINT_(5.0_V_ONLY)_2" direction="pwr"/>
<pin name="TMS/IO" direction="in"/>
<pin name="TCK/IO" direction="in"/>
<pin name="TDO/IO"/>
<pin name="TDI/IO" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO_77"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128STC100-15N">
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/*GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO/TDI"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7128STI100-10N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7160STI100-10N">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO_6" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLR" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO_61"/>
<pin name="IO_62"/>
<pin name="IO_63"/>
<pin name="IO_64"/>
<pin name="IO_65"/>
<pin name="IO_66"/>
<pin name="IO_67"/>
<pin name="IO_68"/>
<pin name="IO_69"/>
<pin name="IO_70"/>
<pin name="IO_71"/>
<pin name="IO_72"/>
<pin name="IO_73"/>
<pin name="IO_74"/>
<pin name="IO_75"/>
<pin name="IO_76"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7192SQI160-10N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO_59"/>
<pin name="IO_60"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7192SQI160-10N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7256AETC144-7N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7256AETC144-7N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7256AETI144-7N_A">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO_4" direction="pas"/>
<pin name="GNDIO_5" direction="pas"/>
<pin name="GNDIO_6" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TDI"/>
<pin name="IO/TMS"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO_55"/>
<pin name="IO_56"/>
<pin name="IO_57"/>
<pin name="IO_58"/>
<pin name="IO"/>
</symbol>
<symbol name="EPM7256AETI144-7N_B">
<pin name="VCCIO_2" direction="pwr"/>
<pin name="VCCIO_3" direction="pwr"/>
<pin name="VCCIO_4" direction="pwr"/>
<pin name="VCCIO_5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCINT_2" direction="pwr"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="INPUT/GCLK1" direction="in"/>
<pin name="INPUT/OE1" direction="in"/>
<pin name="INPUT/GCLRN" direction="in"/>
<pin name="INPUT/OE2/GCLK2" direction="in"/>
<pin name="IO_2"/>
<pin name="IO_3"/>
<pin name="IO_4"/>
<pin name="IO_5"/>
<pin name="IO_6"/>
<pin name="IO_7"/>
<pin name="IO_8"/>
<pin name="IO_9"/>
<pin name="IO_10"/>
<pin name="IO_11"/>
<pin name="IO_12"/>
<pin name="IO_13"/>
<pin name="IO_14"/>
<pin name="IO_15"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
<pin name="IO_22"/>
<pin name="GNDIO_2" direction="pas"/>
<pin name="GNDIO_3" direction="pas"/>
<pin name="GNDIO" direction="pas"/>
<pin name="GNDINT_2" direction="pas"/>
<pin name="GNDINT" direction="pas"/>
<pin name="IO/TCK"/>
<pin name="IO/TDO"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="IO_27"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="IO_31"/>
<pin name="IO_32"/>
<pin name="IO_33"/>
<pin name="IO_34"/>
<pin name="IO_35"/>
<pin name="IO_36"/>
<pin name="IO_37"/>
<pin name="IO_38"/>
<pin name="IO_39"/>
<pin name="IO_40"/>
<pin name="IO_41"/>
<pin name="IO_42"/>
<pin name="IO_43"/>
<pin name="IO_44"/>
<pin name="IO_45"/>
<pin name="IO_46"/>
<pin name="IO_47"/>
<pin name="IO_48"/>
<pin name="IO_49"/>
<pin name="IO_50"/>
<pin name="IO_51"/>
<pin name="IO_52"/>
<pin name="IO_53"/>
<pin name="IO_54"/>
<pin name="IO"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="EP1C12F256C8N">
<description>IC, CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C12F256C8N_A"/>
<gate name="B" symbol="EP1C12F256C8N_B"/>
<gate name="C" symbol="EP1C12F256C8N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="CLK0" pad="G1"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="DATA0" pad="H2"/>
<connect gate="A" pin="DCLK" pad="K4"/>
<connect gate="A" pin="GND" pad="J9"/>
<connect gate="A" pin="GNDA_PLL1" pad="J6"/>
<connect gate="A" pin="GNDG_PLL1" pad="J5"/>
<connect gate="A" pin="GND_10" pad="G9"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="A5"/>
<connect gate="A" pin="GND_4" pad="F8"/>
<connect gate="A" pin="GND_5" pad="F9"/>
<connect gate="A" pin="GND_6" pad="J7"/>
<connect gate="A" pin="GND_7" pad="F6"/>
<connect gate="A" pin="GND_8" pad="G7"/>
<connect gate="A" pin="GND_9" pad="H8"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="A2"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="C4"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D1"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="D3"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D5"/>
<connect gate="A" pin="IO_29" pad="D6"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D7"/>
<connect gate="A" pin="IO_31" pad="D8"/>
<connect gate="A" pin="IO_32" pad="D9"/>
<connect gate="A" pin="IO_33" pad="E1"/>
<connect gate="A" pin="IO_34" pad="E2"/>
<connect gate="A" pin="IO_35" pad="E3"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E5"/>
<connect gate="A" pin="IO_38" pad="E6"/>
<connect gate="A" pin="IO_39" pad="E7"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_40" pad="E8"/>
<connect gate="A" pin="IO_41" pad="E9"/>
<connect gate="A" pin="IO_42" pad="F1"/>
<connect gate="A" pin="IO_43" pad="F2"/>
<connect gate="A" pin="IO_44" pad="F3"/>
<connect gate="A" pin="IO_45" pad="F4"/>
<connect gate="A" pin="IO_46" pad="F5"/>
<connect gate="A" pin="IO_47" pad="G2"/>
<connect gate="A" pin="IO_48" pad="G3"/>
<connect gate="A" pin="IO_49" pad="G4"/>
<connect gate="A" pin="IO_5" pad="B1"/>
<connect gate="A" pin="IO_50" pad="G5"/>
<connect gate="A" pin="IO_51" pad="H5"/>
<connect gate="A" pin="IO_52" pad="J1"/>
<connect gate="A" pin="IO_53" pad="K1"/>
<connect gate="A" pin="IO_54" pad="K2"/>
<connect gate="A" pin="IO_55" pad="K3"/>
<connect gate="A" pin="IO_6" pad="A6"/>
<connect gate="A" pin="IO_7" pad="B2"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="J3"/>
<connect gate="A" pin="MSEL1" pad="J2"/>
<connect gate="A" pin="NCE" pad="J4"/>
<connect gate="A" pin="NCEO" pad="H4"/>
<connect gate="A" pin="NCONFIG" pad="H3"/>
<connect gate="A" pin="VCCA_PLL1" pad="H6"/>
<connect gate="A" pin="VCCINT" pad="H7"/>
<connect gate="A" pin="VCCINT_2" pad="A7"/>
<connect gate="A" pin="VCCINT_3" pad="J8"/>
<connect gate="A" pin="VCCINT_4" pad="G8"/>
<connect gate="A" pin="VCCINT_5" pad="H9"/>
<connect gate="A" pin="VCCIO1" pad="G6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F7"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="B" pin="GND" pad="T1"/>
<connect gate="B" pin="GND_2" pad="K6"/>
<connect gate="B" pin="GND_3" pad="L6"/>
<connect gate="B" pin="GND_4" pad="K8"/>
<connect gate="B" pin="GND_5" pad="A12"/>
<connect gate="B" pin="GND_6" pad="L8"/>
<connect gate="B" pin="GND_7" pad="T5"/>
<connect gate="B" pin="GND_8" pad="L9"/>
<connect gate="B" pin="GND_9" pad="A16"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="M9"/>
<connect gate="B" pin="IO_11" pad="N1"/>
<connect gate="B" pin="IO_12" pad="N2"/>
<connect gate="B" pin="IO_13" pad="N3"/>
<connect gate="B" pin="IO_14" pad="N4"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="N6"/>
<connect gate="B" pin="IO_17" pad="L1"/>
<connect gate="B" pin="IO_18" pad="N7"/>
<connect gate="B" pin="IO_19" pad="L2"/>
<connect gate="B" pin="IO_2" pad="M1"/>
<connect gate="B" pin="IO_20" pad="N8"/>
<connect gate="B" pin="IO_21" pad="L3"/>
<connect gate="B" pin="IO_22" pad="N9"/>
<connect gate="B" pin="IO_23" pad="L4"/>
<connect gate="B" pin="IO_24" pad="L5"/>
<connect gate="B" pin="IO_25" pad="P2"/>
<connect gate="B" pin="IO_26" pad="P3"/>
<connect gate="B" pin="IO_27" pad="P4"/>
<connect gate="B" pin="IO_28" pad="P5"/>
<connect gate="B" pin="IO_29" pad="P6"/>
<connect gate="B" pin="IO_3" pad="M2"/>
<connect gate="B" pin="IO_30" pad="P7"/>
<connect gate="B" pin="IO_31" pad="P8"/>
<connect gate="B" pin="IO_32" pad="P9"/>
<connect gate="B" pin="IO_33" pad="R1"/>
<connect gate="B" pin="IO_34" pad="R2"/>
<connect gate="B" pin="IO_35" pad="R3"/>
<connect gate="B" pin="IO_36" pad="R4"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="M3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T4"/>
<connect gate="B" pin="IO_44" pad="T6"/>
<connect gate="B" pin="IO_45" pad="T8"/>
<connect gate="B" pin="IO_46" pad="T9"/>
<connect gate="B" pin="IO_47" pad="A11"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="M4"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B15"/>
<connect gate="B" pin="IO_56" pad="B16"/>
<connect gate="B" pin="IO_57" pad="C10"/>
<connect gate="B" pin="IO_58" pad="C11"/>
<connect gate="B" pin="IO_59" pad="C12"/>
<connect gate="B" pin="IO_6" pad="M5"/>
<connect gate="B" pin="IO_60" pad="C13"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="C15"/>
<connect gate="B" pin="IO_63" pad="D10"/>
<connect gate="B" pin="IO_64" pad="D11"/>
<connect gate="B" pin="IO_65" pad="D12"/>
<connect gate="B" pin="IO_66" pad="D13"/>
<connect gate="B" pin="IO_67" pad="D14"/>
<connect gate="B" pin="IO_68" pad="D15"/>
<connect gate="B" pin="IO_7" pad="M6"/>
<connect gate="B" pin="IO_8" pad="M7"/>
<connect gate="B" pin="IO_9" pad="M8"/>
<connect gate="B" pin="VCCINT" pad="K7"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="T7"/>
<connect gate="B" pin="VCCINT_4" pad="A10"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L7"/>
<connect gate="C" pin="CLK2" pad="G16"/>
<connect gate="C" pin="CLK3" pad="H16"/>
<connect gate="C" pin="CONF_DONE" pad="K13"/>
<connect gate="C" pin="GND" pad="T16"/>
<connect gate="C" pin="GNDA_PLL2" pad="J11"/>
<connect gate="C" pin="GNDG_PLL2" pad="J12"/>
<connect gate="C" pin="GND_2" pad="L11"/>
<connect gate="C" pin="GND_3" pad="H10"/>
<connect gate="C" pin="GND_4" pad="K10"/>
<connect gate="C" pin="GND_5" pad="T12"/>
<connect gate="C" pin="GND_6" pad="G11"/>
<connect gate="C" pin="GND_7" pad="F11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO_10" pad="F13"/>
<connect gate="C" pin="IO_11" pad="F14"/>
<connect gate="C" pin="IO_12" pad="F15"/>
<connect gate="C" pin="IO_13" pad="F16"/>
<connect gate="C" pin="IO_14" pad="G12"/>
<connect gate="C" pin="IO_15" pad="G13"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="K12"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="G15"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="H12"/>
<connect gate="C" pin="IO_21" pad="K14"/>
<connect gate="C" pin="IO_22" pad="H13"/>
<connect gate="C" pin="IO_23" pad="K15"/>
<connect gate="C" pin="IO_24" pad="K16"/>
<connect gate="C" pin="IO_25" pad="L12"/>
<connect gate="C" pin="IO_26" pad="L13"/>
<connect gate="C" pin="IO_27" pad="L14"/>
<connect gate="C" pin="IO_28" pad="L15"/>
<connect gate="C" pin="IO_29" pad="L16"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="M10"/>
<connect gate="C" pin="IO_31" pad="M11"/>
<connect gate="C" pin="IO_32" pad="M12"/>
<connect gate="C" pin="IO_33" pad="M13"/>
<connect gate="C" pin="IO_34" pad="M14"/>
<connect gate="C" pin="IO_35" pad="M15"/>
<connect gate="C" pin="IO_36" pad="M16"/>
<connect gate="C" pin="IO_37" pad="N10"/>
<connect gate="C" pin="IO_38" pad="N11"/>
<connect gate="C" pin="IO_39" pad="N12"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="N13"/>
<connect gate="C" pin="IO_41" pad="N14"/>
<connect gate="C" pin="IO_42" pad="N15"/>
<connect gate="C" pin="IO_43" pad="N16"/>
<connect gate="C" pin="IO_44" pad="P10"/>
<connect gate="C" pin="IO_45" pad="P11"/>
<connect gate="C" pin="IO_46" pad="P12"/>
<connect gate="C" pin="IO_47" pad="P13"/>
<connect gate="C" pin="IO_48" pad="P14"/>
<connect gate="C" pin="IO_49" pad="P15"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="R10"/>
<connect gate="C" pin="IO_51" pad="R11"/>
<connect gate="C" pin="IO_52" pad="R12"/>
<connect gate="C" pin="IO_53" pad="R13"/>
<connect gate="C" pin="IO_54" pad="R14"/>
<connect gate="C" pin="IO_55" pad="R15"/>
<connect gate="C" pin="IO_56" pad="R16"/>
<connect gate="C" pin="IO_57" pad="T11"/>
<connect gate="C" pin="IO_58" pad="T13"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="F12"/>
<connect gate="C" pin="NSTATUS" pad="J13"/>
<connect gate="C" pin="TCK" pad="J14"/>
<connect gate="C" pin="TDI" pad="H14"/>
<connect gate="C" pin="TDO" pad="H15"/>
<connect gate="C" pin="TMS" pad="J15"/>
<connect gate="C" pin="VCCA_PLL2" pad="H11"/>
<connect gate="C" pin="VCCINT" pad="T10"/>
<connect gate="C" pin="VCCINT_2" pad="G10"/>
<connect gate="C" pin="VCCINT_3" pad="J10"/>
<connect gate="C" pin="VCCIO2" pad="F10"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="K11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
<connect gate="C" pin="VCCIO4_2" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C12F256C8N"/>
<attribute name="OC_FARNELL" value="1453475"/>
<attribute name="OC_NEWARK" value="51R0538"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C12F256I7N">
<description>IC, CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C12F256I7N_A"/>
<gate name="B" symbol="EP1C12F256I7N_B"/>
<gate name="C" symbol="EP1C12F256I7N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="CLK0" pad="G1"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="DATA0" pad="H2"/>
<connect gate="A" pin="DCLK" pad="K4"/>
<connect gate="A" pin="GND" pad="J9"/>
<connect gate="A" pin="GNDA_PLL1" pad="J6"/>
<connect gate="A" pin="GNDG_PLL1" pad="J5"/>
<connect gate="A" pin="GND_10" pad="G9"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="A5"/>
<connect gate="A" pin="GND_4" pad="F8"/>
<connect gate="A" pin="GND_5" pad="F9"/>
<connect gate="A" pin="GND_6" pad="J7"/>
<connect gate="A" pin="GND_7" pad="F6"/>
<connect gate="A" pin="GND_8" pad="G7"/>
<connect gate="A" pin="GND_9" pad="H8"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="A2"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="C4"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D1"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="D3"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D5"/>
<connect gate="A" pin="IO_29" pad="D6"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D7"/>
<connect gate="A" pin="IO_31" pad="D8"/>
<connect gate="A" pin="IO_32" pad="D9"/>
<connect gate="A" pin="IO_33" pad="E1"/>
<connect gate="A" pin="IO_34" pad="E2"/>
<connect gate="A" pin="IO_35" pad="E3"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E5"/>
<connect gate="A" pin="IO_38" pad="E6"/>
<connect gate="A" pin="IO_39" pad="E7"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_40" pad="E8"/>
<connect gate="A" pin="IO_41" pad="E9"/>
<connect gate="A" pin="IO_42" pad="F1"/>
<connect gate="A" pin="IO_43" pad="F2"/>
<connect gate="A" pin="IO_44" pad="F3"/>
<connect gate="A" pin="IO_45" pad="F4"/>
<connect gate="A" pin="IO_46" pad="F5"/>
<connect gate="A" pin="IO_47" pad="G2"/>
<connect gate="A" pin="IO_48" pad="G3"/>
<connect gate="A" pin="IO_49" pad="G4"/>
<connect gate="A" pin="IO_5" pad="B1"/>
<connect gate="A" pin="IO_50" pad="G5"/>
<connect gate="A" pin="IO_51" pad="H5"/>
<connect gate="A" pin="IO_52" pad="J1"/>
<connect gate="A" pin="IO_53" pad="K1"/>
<connect gate="A" pin="IO_54" pad="K2"/>
<connect gate="A" pin="IO_55" pad="K3"/>
<connect gate="A" pin="IO_6" pad="A6"/>
<connect gate="A" pin="IO_7" pad="B2"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="J3"/>
<connect gate="A" pin="MSEL1" pad="J2"/>
<connect gate="A" pin="NCE" pad="J4"/>
<connect gate="A" pin="NCEO" pad="H4"/>
<connect gate="A" pin="NCONFIG" pad="H3"/>
<connect gate="A" pin="VCCA_PLL1" pad="H6"/>
<connect gate="A" pin="VCCINT" pad="H7"/>
<connect gate="A" pin="VCCINT_2" pad="A7"/>
<connect gate="A" pin="VCCINT_3" pad="J8"/>
<connect gate="A" pin="VCCINT_4" pad="G8"/>
<connect gate="A" pin="VCCINT_5" pad="H9"/>
<connect gate="A" pin="VCCIO1" pad="G6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F7"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="B" pin="GND" pad="T1"/>
<connect gate="B" pin="GND_2" pad="K6"/>
<connect gate="B" pin="GND_3" pad="L6"/>
<connect gate="B" pin="GND_4" pad="K8"/>
<connect gate="B" pin="GND_5" pad="A12"/>
<connect gate="B" pin="GND_6" pad="L8"/>
<connect gate="B" pin="GND_7" pad="T5"/>
<connect gate="B" pin="GND_8" pad="L9"/>
<connect gate="B" pin="GND_9" pad="A16"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="M9"/>
<connect gate="B" pin="IO_11" pad="N1"/>
<connect gate="B" pin="IO_12" pad="N2"/>
<connect gate="B" pin="IO_13" pad="N3"/>
<connect gate="B" pin="IO_14" pad="N4"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="N6"/>
<connect gate="B" pin="IO_17" pad="L1"/>
<connect gate="B" pin="IO_18" pad="N7"/>
<connect gate="B" pin="IO_19" pad="L2"/>
<connect gate="B" pin="IO_2" pad="M1"/>
<connect gate="B" pin="IO_20" pad="N8"/>
<connect gate="B" pin="IO_21" pad="L3"/>
<connect gate="B" pin="IO_22" pad="N9"/>
<connect gate="B" pin="IO_23" pad="L4"/>
<connect gate="B" pin="IO_24" pad="L5"/>
<connect gate="B" pin="IO_25" pad="P2"/>
<connect gate="B" pin="IO_26" pad="P3"/>
<connect gate="B" pin="IO_27" pad="P4"/>
<connect gate="B" pin="IO_28" pad="P5"/>
<connect gate="B" pin="IO_29" pad="P6"/>
<connect gate="B" pin="IO_3" pad="M2"/>
<connect gate="B" pin="IO_30" pad="P7"/>
<connect gate="B" pin="IO_31" pad="P8"/>
<connect gate="B" pin="IO_32" pad="P9"/>
<connect gate="B" pin="IO_33" pad="R1"/>
<connect gate="B" pin="IO_34" pad="R2"/>
<connect gate="B" pin="IO_35" pad="R3"/>
<connect gate="B" pin="IO_36" pad="R4"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="M3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T4"/>
<connect gate="B" pin="IO_44" pad="T6"/>
<connect gate="B" pin="IO_45" pad="T8"/>
<connect gate="B" pin="IO_46" pad="T9"/>
<connect gate="B" pin="IO_47" pad="A11"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="M4"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B15"/>
<connect gate="B" pin="IO_56" pad="B16"/>
<connect gate="B" pin="IO_57" pad="C10"/>
<connect gate="B" pin="IO_58" pad="C11"/>
<connect gate="B" pin="IO_59" pad="C12"/>
<connect gate="B" pin="IO_6" pad="M5"/>
<connect gate="B" pin="IO_60" pad="C13"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="C15"/>
<connect gate="B" pin="IO_63" pad="D10"/>
<connect gate="B" pin="IO_64" pad="D11"/>
<connect gate="B" pin="IO_65" pad="D12"/>
<connect gate="B" pin="IO_66" pad="D13"/>
<connect gate="B" pin="IO_67" pad="D14"/>
<connect gate="B" pin="IO_68" pad="D15"/>
<connect gate="B" pin="IO_7" pad="M6"/>
<connect gate="B" pin="IO_8" pad="M7"/>
<connect gate="B" pin="IO_9" pad="M8"/>
<connect gate="B" pin="VCCINT" pad="K7"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="T7"/>
<connect gate="B" pin="VCCINT_4" pad="A10"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L7"/>
<connect gate="C" pin="CLK2" pad="G16"/>
<connect gate="C" pin="CLK3" pad="H16"/>
<connect gate="C" pin="CONF_DONE" pad="K13"/>
<connect gate="C" pin="GND" pad="T16"/>
<connect gate="C" pin="GNDA_PLL2" pad="J11"/>
<connect gate="C" pin="GNDG_PLL2" pad="J12"/>
<connect gate="C" pin="GND_2" pad="L11"/>
<connect gate="C" pin="GND_3" pad="H10"/>
<connect gate="C" pin="GND_4" pad="K10"/>
<connect gate="C" pin="GND_5" pad="T12"/>
<connect gate="C" pin="GND_6" pad="G11"/>
<connect gate="C" pin="GND_7" pad="F11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO_10" pad="F13"/>
<connect gate="C" pin="IO_11" pad="F14"/>
<connect gate="C" pin="IO_12" pad="F15"/>
<connect gate="C" pin="IO_13" pad="F16"/>
<connect gate="C" pin="IO_14" pad="G12"/>
<connect gate="C" pin="IO_15" pad="G13"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="K12"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="G15"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="H12"/>
<connect gate="C" pin="IO_21" pad="K14"/>
<connect gate="C" pin="IO_22" pad="H13"/>
<connect gate="C" pin="IO_23" pad="K15"/>
<connect gate="C" pin="IO_24" pad="K16"/>
<connect gate="C" pin="IO_25" pad="L12"/>
<connect gate="C" pin="IO_26" pad="L13"/>
<connect gate="C" pin="IO_27" pad="L14"/>
<connect gate="C" pin="IO_28" pad="L15"/>
<connect gate="C" pin="IO_29" pad="L16"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="M10"/>
<connect gate="C" pin="IO_31" pad="M11"/>
<connect gate="C" pin="IO_32" pad="M12"/>
<connect gate="C" pin="IO_33" pad="M13"/>
<connect gate="C" pin="IO_34" pad="M14"/>
<connect gate="C" pin="IO_35" pad="M15"/>
<connect gate="C" pin="IO_36" pad="M16"/>
<connect gate="C" pin="IO_37" pad="N10"/>
<connect gate="C" pin="IO_38" pad="N11"/>
<connect gate="C" pin="IO_39" pad="N12"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="N13"/>
<connect gate="C" pin="IO_41" pad="N14"/>
<connect gate="C" pin="IO_42" pad="N15"/>
<connect gate="C" pin="IO_43" pad="N16"/>
<connect gate="C" pin="IO_44" pad="P10"/>
<connect gate="C" pin="IO_45" pad="P11"/>
<connect gate="C" pin="IO_46" pad="P12"/>
<connect gate="C" pin="IO_47" pad="P13"/>
<connect gate="C" pin="IO_48" pad="P14"/>
<connect gate="C" pin="IO_49" pad="P15"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="R10"/>
<connect gate="C" pin="IO_51" pad="R11"/>
<connect gate="C" pin="IO_52" pad="R12"/>
<connect gate="C" pin="IO_53" pad="R13"/>
<connect gate="C" pin="IO_54" pad="R14"/>
<connect gate="C" pin="IO_55" pad="R15"/>
<connect gate="C" pin="IO_56" pad="R16"/>
<connect gate="C" pin="IO_57" pad="T11"/>
<connect gate="C" pin="IO_58" pad="T13"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="F12"/>
<connect gate="C" pin="NSTATUS" pad="J13"/>
<connect gate="C" pin="TCK" pad="J14"/>
<connect gate="C" pin="TDI" pad="H14"/>
<connect gate="C" pin="TDO" pad="H15"/>
<connect gate="C" pin="TMS" pad="J15"/>
<connect gate="C" pin="VCCA_PLL2" pad="H11"/>
<connect gate="C" pin="VCCINT" pad="T10"/>
<connect gate="C" pin="VCCINT_2" pad="G10"/>
<connect gate="C" pin="VCCINT_3" pad="J10"/>
<connect gate="C" pin="VCCIO2" pad="F10"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="K11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
<connect gate="C" pin="VCCIO4_2" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C12F256I7N"/>
<attribute name="OC_FARNELL" value="1453467"/>
<attribute name="OC_NEWARK" value="52R0012"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C12F324C8N">
<description>FPGA, CYCLONE</description>
<gates>
<gate name="A" symbol="EP1C12F324C8N_A"/>
<gate name="B" symbol="EP1C12F324C8N_B"/>
<gate name="C" symbol="EP1C12F324C8N_C"/>
<gate name="D" symbol="EP1C12F324C8N_D"/>
</gates>
<devices>
<device name="" package="BGA324C100P18X18_1900X1900X220">
<connects>
<connect gate="A" pin="CLK0" pad="J3"/>
<connect gate="A" pin="CLK1" pad="J4"/>
<connect gate="A" pin="DATA0" pad="H7"/>
<connect gate="A" pin="GND" pad="J8"/>
<connect gate="A" pin="GNDG_PLL1" pad="J6"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="C1"/>
<connect gate="A" pin="GND_4" pad="A3"/>
<connect gate="A" pin="GND_5" pad="B2"/>
<connect gate="A" pin="GND_6" pad="H8"/>
<connect gate="A" pin="GND_7" pad="H9"/>
<connect gate="A" pin="IO" pad="J1"/>
<connect gate="A" pin="IO_10" pad="A6"/>
<connect gate="A" pin="IO_11" pad="B8"/>
<connect gate="A" pin="IO_12" pad="A7"/>
<connect gate="A" pin="IO_13" pad="B9"/>
<connect gate="A" pin="IO_14" pad="A8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="A4"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="E2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="E3"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E5"/>
<connect gate="A" pin="IO_35" pad="E6"/>
<connect gate="A" pin="IO_36" pad="E7"/>
<connect gate="A" pin="IO_37" pad="E8"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="E4"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F5"/>
<connect gate="A" pin="IO_43" pad="F6"/>
<connect gate="A" pin="IO_44" pad="F7"/>
<connect gate="A" pin="IO_45" pad="F8"/>
<connect gate="A" pin="IO_46" pad="F9"/>
<connect gate="A" pin="IO_47" pad="G1"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="G3"/>
<connect gate="A" pin="IO_5" pad="B3"/>
<connect gate="A" pin="IO_50" pad="G4"/>
<connect gate="A" pin="IO_51" pad="G5"/>
<connect gate="A" pin="IO_52" pad="G6"/>
<connect gate="A" pin="IO_53" pad="G8"/>
<connect gate="A" pin="IO_54" pad="G9"/>
<connect gate="A" pin="IO_55" pad="H1"/>
<connect gate="A" pin="IO_56" pad="H2"/>
<connect gate="A" pin="IO_57" pad="H3"/>
<connect gate="A" pin="IO_58" pad="H4"/>
<connect gate="A" pin="IO_59" pad="H5"/>
<connect gate="A" pin="IO_6" pad="B4"/>
<connect gate="A" pin="IO_60" pad="H6"/>
<connect gate="A" pin="IO_7" pad="B5"/>
<connect gate="A" pin="IO_8" pad="B6"/>
<connect gate="A" pin="IO_9" pad="B7"/>
<connect gate="A" pin="NCE" pad="J7"/>
<connect gate="A" pin="NCONFIG" pad="J2"/>
<connect gate="A" pin="VCCA_PLL1" pad="J5"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="A2"/>
<connect gate="A" pin="VCCINT_3" pad="B1"/>
<connect gate="A" pin="VCCIO1" pad="G7"/>
<connect gate="A" pin="VCCIO1_2" pad="E1"/>
<connect gate="A" pin="VCCIO2" pad="A5"/>
<connect gate="A" pin="VCCIO2_2" pad="E9"/>
<connect gate="B" pin="DCLK" pad="L1"/>
<connect gate="B" pin="GND" pad="V1"/>
<connect gate="B" pin="GNDA_PLL1" pad="K1"/>
<connect gate="B" pin="GND_2" pad="K8"/>
<connect gate="B" pin="GND_3" pad="K9"/>
<connect gate="B" pin="GND_4" pad="T1"/>
<connect gate="B" pin="GND_5" pad="U2"/>
<connect gate="B" pin="GND_6" pad="V3"/>
<connect gate="B" pin="GND_7" pad="L8"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO_10" pad="M2"/>
<connect gate="B" pin="IO_11" pad="L5"/>
<connect gate="B" pin="IO_12" pad="M3"/>
<connect gate="B" pin="IO_13" pad="L6"/>
<connect gate="B" pin="IO_14" pad="M4"/>
<connect gate="B" pin="IO_15" pad="N9"/>
<connect gate="B" pin="IO_16" pad="M5"/>
<connect gate="B" pin="IO_17" pad="M6"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="P3"/>
<connect gate="B" pin="IO_2" pad="K4"/>
<connect gate="B" pin="IO_20" pad="M8"/>
<connect gate="B" pin="IO_21" pad="P4"/>
<connect gate="B" pin="IO_22" pad="M9"/>
<connect gate="B" pin="IO_23" pad="N1"/>
<connect gate="B" pin="IO_24" pad="N2"/>
<connect gate="B" pin="IO_25" pad="N3"/>
<connect gate="B" pin="IO_26" pad="N4"/>
<connect gate="B" pin="IO_27" pad="N5"/>
<connect gate="B" pin="IO_28" pad="N6"/>
<connect gate="B" pin="IO_29" pad="N7"/>
<connect gate="B" pin="IO_3" pad="L2"/>
<connect gate="B" pin="IO_30" pad="N8"/>
<connect gate="B" pin="IO_31" pad="P5"/>
<connect gate="B" pin="IO_32" pad="P6"/>
<connect gate="B" pin="IO_33" pad="P7"/>
<connect gate="B" pin="IO_34" pad="P9"/>
<connect gate="B" pin="IO_35" pad="R1"/>
<connect gate="B" pin="IO_36" pad="R2"/>
<connect gate="B" pin="IO_37" pad="R3"/>
<connect gate="B" pin="IO_38" pad="R4"/>
<connect gate="B" pin="IO_39" pad="R5"/>
<connect gate="B" pin="IO_4" pad="L7"/>
<connect gate="B" pin="IO_40" pad="R6"/>
<connect gate="B" pin="IO_41" pad="R7"/>
<connect gate="B" pin="IO_42" pad="R8"/>
<connect gate="B" pin="IO_43" pad="R9"/>
<connect gate="B" pin="IO_44" pad="T2"/>
<connect gate="B" pin="IO_45" pad="T3"/>
<connect gate="B" pin="IO_46" pad="T4"/>
<connect gate="B" pin="IO_47" pad="T5"/>
<connect gate="B" pin="IO_48" pad="T6"/>
<connect gate="B" pin="IO_49" pad="T7"/>
<connect gate="B" pin="IO_5" pad="K5"/>
<connect gate="B" pin="IO_50" pad="T8"/>
<connect gate="B" pin="IO_51" pad="T9"/>
<connect gate="B" pin="IO_52" pad="U3"/>
<connect gate="B" pin="IO_53" pad="U4"/>
<connect gate="B" pin="IO_54" pad="U5"/>
<connect gate="B" pin="IO_55" pad="U6"/>
<connect gate="B" pin="IO_56" pad="U7"/>
<connect gate="B" pin="IO_57" pad="U8"/>
<connect gate="B" pin="IO_58" pad="U9"/>
<connect gate="B" pin="IO_59" pad="V4"/>
<connect gate="B" pin="IO_6" pad="L3"/>
<connect gate="B" pin="IO_60" pad="V6"/>
<connect gate="B" pin="IO_61" pad="V7"/>
<connect gate="B" pin="IO_62" pad="V8"/>
<connect gate="B" pin="IO_7" pad="K6"/>
<connect gate="B" pin="IO_8" pad="M1"/>
<connect gate="B" pin="IO_9" pad="L4"/>
<connect gate="B" pin="MSEL0" pad="K3"/>
<connect gate="B" pin="MSEL1" pad="K7"/>
<connect gate="B" pin="NCEO" pad="K2"/>
<connect gate="B" pin="VCCINT" pad="U1"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="V2"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO1_2" pad="M7"/>
<connect gate="B" pin="VCCIO4" pad="V5"/>
<connect gate="B" pin="VCCIO4_2" pad="P8"/>
<connect gate="C" pin="CLK2" pad="J15"/>
<connect gate="C" pin="CLK3" pad="J16"/>
<connect gate="C" pin="GND" pad="J11"/>
<connect gate="C" pin="GNDG_PLL2" pad="J18"/>
<connect gate="C" pin="GND_2" pad="B17"/>
<connect gate="C" pin="GND_3" pad="H11"/>
<connect gate="C" pin="GND_4" pad="A16"/>
<connect gate="C" pin="GND_5" pad="A18"/>
<connect gate="C" pin="GND_6" pad="J10"/>
<connect gate="C" pin="GND_7" pad="C18"/>
<connect gate="C" pin="IO" pad="J14"/>
<connect gate="C" pin="IO_10" pad="B14"/>
<connect gate="C" pin="IO_11" pad="A15"/>
<connect gate="C" pin="IO_12" pad="B15"/>
<connect gate="C" pin="IO_13" pad="B16"/>
<connect gate="C" pin="IO_14" pad="C10"/>
<connect gate="C" pin="IO_15" pad="C11"/>
<connect gate="C" pin="IO_16" pad="C12"/>
<connect gate="C" pin="IO_17" pad="C13"/>
<connect gate="C" pin="IO_18" pad="C14"/>
<connect gate="C" pin="IO_19" pad="C15"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C16"/>
<connect gate="C" pin="IO_21" pad="C17"/>
<connect gate="C" pin="IO_22" pad="D10"/>
<connect gate="C" pin="IO_23" pad="D11"/>
<connect gate="C" pin="IO_24" pad="D12"/>
<connect gate="C" pin="IO_25" pad="D13"/>
<connect gate="C" pin="IO_26" pad="D14"/>
<connect gate="C" pin="IO_27" pad="D15"/>
<connect gate="C" pin="IO_28" pad="D16"/>
<connect gate="C" pin="IO_29" pad="D17"/>
<connect gate="C" pin="IO_3" pad="B10"/>
<connect gate="C" pin="IO_30" pad="D18"/>
<connect gate="C" pin="IO_31" pad="E10"/>
<connect gate="C" pin="IO_32" pad="E11"/>
<connect gate="C" pin="IO_33" pad="E13"/>
<connect gate="C" pin="IO_34" pad="E14"/>
<connect gate="C" pin="IO_35" pad="E15"/>
<connect gate="C" pin="IO_36" pad="E16"/>
<connect gate="C" pin="IO_37" pad="E17"/>
<connect gate="C" pin="IO_38" pad="F10"/>
<connect gate="C" pin="IO_39" pad="F11"/>
<connect gate="C" pin="IO_4" pad="A11"/>
<connect gate="C" pin="IO_40" pad="F12"/>
<connect gate="C" pin="IO_41" pad="F13"/>
<connect gate="C" pin="IO_42" pad="F14"/>
<connect gate="C" pin="IO_43" pad="F15"/>
<connect gate="C" pin="IO_44" pad="F16"/>
<connect gate="C" pin="IO_45" pad="F17"/>
<connect gate="C" pin="IO_46" pad="F18"/>
<connect gate="C" pin="IO_47" pad="G10"/>
<connect gate="C" pin="IO_48" pad="G11"/>
<connect gate="C" pin="IO_49" pad="G12"/>
<connect gate="C" pin="IO_5" pad="B11"/>
<connect gate="C" pin="IO_50" pad="G13"/>
<connect gate="C" pin="IO_51" pad="G14"/>
<connect gate="C" pin="IO_52" pad="G15"/>
<connect gate="C" pin="IO_53" pad="G16"/>
<connect gate="C" pin="IO_54" pad="G17"/>
<connect gate="C" pin="IO_55" pad="G18"/>
<connect gate="C" pin="IO_56" pad="H13"/>
<connect gate="C" pin="IO_57" pad="H14"/>
<connect gate="C" pin="IO_58" pad="H15"/>
<connect gate="C" pin="IO_59" pad="H16"/>
<connect gate="C" pin="IO_6" pad="A12"/>
<connect gate="C" pin="IO_60" pad="H17"/>
<connect gate="C" pin="IO_61" pad="H18"/>
<connect gate="C" pin="IO_62" pad="J13"/>
<connect gate="C" pin="IO_7" pad="B12"/>
<connect gate="C" pin="IO_8" pad="A13"/>
<connect gate="C" pin="IO_9" pad="B13"/>
<connect gate="C" pin="TDI" pad="J17"/>
<connect gate="C" pin="VCCA_PLL2" pad="J12"/>
<connect gate="C" pin="VCCINT" pad="A17"/>
<connect gate="C" pin="VCCINT_2" pad="B18"/>
<connect gate="C" pin="VCCINT_3" pad="H10"/>
<connect gate="C" pin="VCCIO2" pad="E12"/>
<connect gate="C" pin="VCCIO2_2" pad="A14"/>
<connect gate="C" pin="VCCIO3" pad="E18"/>
<connect gate="C" pin="VCCIO3_2" pad="H12"/>
<connect gate="D" pin="CONF_DONE" pad="K17"/>
<connect gate="D" pin="GND" pad="K11"/>
<connect gate="D" pin="GNDA_PLL2" pad="K12"/>
<connect gate="D" pin="GND_2" pad="T18"/>
<connect gate="D" pin="GND_3" pad="U17"/>
<connect gate="D" pin="GND_4" pad="L10"/>
<connect gate="D" pin="GND_5" pad="L11"/>
<connect gate="D" pin="GND_6" pad="V16"/>
<connect gate="D" pin="GND_7" pad="V18"/>
<connect gate="D" pin="IO" pad="V15"/>
<connect gate="D" pin="IO_10" pad="M10"/>
<connect gate="D" pin="IO_11" pad="M11"/>
<connect gate="D" pin="IO_12" pad="M13"/>
<connect gate="D" pin="IO_13" pad="M14"/>
<connect gate="D" pin="IO_14" pad="M15"/>
<connect gate="D" pin="IO_15" pad="M16"/>
<connect gate="D" pin="IO_16" pad="M17"/>
<connect gate="D" pin="IO_17" pad="M18"/>
<connect gate="D" pin="IO_18" pad="N10"/>
<connect gate="D" pin="IO_19" pad="N11"/>
<connect gate="D" pin="IO_2" pad="L13"/>
<connect gate="D" pin="IO_20" pad="N12"/>
<connect gate="D" pin="IO_21" pad="N13"/>
<connect gate="D" pin="IO_22" pad="N14"/>
<connect gate="D" pin="IO_23" pad="N15"/>
<connect gate="D" pin="IO_24" pad="N16"/>
<connect gate="D" pin="IO_25" pad="N17"/>
<connect gate="D" pin="IO_26" pad="N18"/>
<connect gate="D" pin="IO_27" pad="P10"/>
<connect gate="D" pin="IO_28" pad="P12"/>
<connect gate="D" pin="IO_29" pad="P13"/>
<connect gate="D" pin="IO_3" pad="L14"/>
<connect gate="D" pin="IO_30" pad="P14"/>
<connect gate="D" pin="IO_31" pad="P15"/>
<connect gate="D" pin="IO_32" pad="P16"/>
<connect gate="D" pin="IO_33" pad="P17"/>
<connect gate="D" pin="IO_34" pad="R10"/>
<connect gate="D" pin="IO_35" pad="R11"/>
<connect gate="D" pin="IO_36" pad="R12"/>
<connect gate="D" pin="IO_37" pad="R13"/>
<connect gate="D" pin="IO_38" pad="R14"/>
<connect gate="D" pin="IO_39" pad="R15"/>
<connect gate="D" pin="IO_4" pad="L15"/>
<connect gate="D" pin="IO_40" pad="R16"/>
<connect gate="D" pin="IO_41" pad="R17"/>
<connect gate="D" pin="IO_42" pad="R18"/>
<connect gate="D" pin="IO_43" pad="T10"/>
<connect gate="D" pin="IO_44" pad="T11"/>
<connect gate="D" pin="IO_45" pad="T12"/>
<connect gate="D" pin="IO_46" pad="T13"/>
<connect gate="D" pin="IO_47" pad="T14"/>
<connect gate="D" pin="IO_48" pad="T15"/>
<connect gate="D" pin="IO_49" pad="T16"/>
<connect gate="D" pin="IO_5" pad="L16"/>
<connect gate="D" pin="IO_50" pad="T17"/>
<connect gate="D" pin="IO_51" pad="U10"/>
<connect gate="D" pin="IO_52" pad="U11"/>
<connect gate="D" pin="IO_53" pad="U12"/>
<connect gate="D" pin="IO_54" pad="U13"/>
<connect gate="D" pin="IO_55" pad="U14"/>
<connect gate="D" pin="IO_56" pad="U15"/>
<connect gate="D" pin="IO_57" pad="U16"/>
<connect gate="D" pin="IO_58" pad="V10"/>
<connect gate="D" pin="IO_59" pad="V11"/>
<connect gate="D" pin="IO_6" pad="L17"/>
<connect gate="D" pin="IO_60" pad="V12"/>
<connect gate="D" pin="IO_61" pad="V13"/>
<connect gate="D" pin="IO_7" pad="K15"/>
<connect gate="D" pin="IO_8" pad="L18"/>
<connect gate="D" pin="IO_9" pad="K16"/>
<connect gate="D" pin="NSTATUS" pad="L12"/>
<connect gate="D" pin="TCK" pad="K18"/>
<connect gate="D" pin="TDO" pad="K13"/>
<connect gate="D" pin="TMS" pad="K14"/>
<connect gate="D" pin="VCCINT" pad="V17"/>
<connect gate="D" pin="VCCINT_2" pad="K10"/>
<connect gate="D" pin="VCCINT_3" pad="U18"/>
<connect gate="D" pin="VCCIO3" pad="P18"/>
<connect gate="D" pin="VCCIO3_2" pad="M12"/>
<connect gate="D" pin="VCCIO4" pad="V14"/>
<connect gate="D" pin="VCCIO4_2" pad="P11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C12F324C8N"/>
<attribute name="OC_FARNELL" value="1549372"/>
<attribute name="OC_NEWARK" value="51R0539"/>
<attribute name="PACKAGE" value="FBGA-324"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C12Q240C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C12Q240C8N_A"/>
<gate name="B" symbol="EP1C12Q240C8N_B"/>
<gate name="C" symbol="EP1C12Q240C8N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3460X3460X410-240N">
<connects>
<connect gate="A" pin="CLK0" pad="28"/>
<connect gate="A" pin="CLK1" pad="29"/>
<connect gate="A" pin="DATA0" pad="25"/>
<connect gate="A" pin="DCLK" pad="36"/>
<connect gate="A" pin="GND" pad="71"/>
<connect gate="A" pin="GNDA_PLL1" pad="30"/>
<connect gate="A" pin="GNDG_PLL1" pad="31"/>
<connect gate="A" pin="GND_2" pad="80"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="GND_4" pad="40"/>
<connect gate="A" pin="GND_5" pad="52"/>
<connect gate="A" pin="GND_6" pad="69"/>
<connect gate="A" pin="IO" pad="79"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="17"/>
<connect gate="A" pin="IO_17" pad="18"/>
<connect gate="A" pin="IO_18" pad="19"/>
<connect gate="A" pin="IO_19" pad="20"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="21"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="24"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="46"/>
<connect gate="A" pin="IO_32" pad="47"/>
<connect gate="A" pin="IO_33" pad="48"/>
<connect gate="A" pin="IO_34" pad="49"/>
<connect gate="A" pin="IO_35" pad="50"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="59"/>
<connect gate="A" pin="IO_43" pad="60"/>
<connect gate="A" pin="IO_44" pad="61"/>
<connect gate="A" pin="IO_45" pad="62"/>
<connect gate="A" pin="IO_46" pad="63"/>
<connect gate="A" pin="IO_47" pad="64"/>
<connect gate="A" pin="IO_48" pad="65"/>
<connect gate="A" pin="IO_49" pad="66"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="67"/>
<connect gate="A" pin="IO_51" pad="68"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="MSEL0" pad="34"/>
<connect gate="A" pin="MSEL1" pad="35"/>
<connect gate="A" pin="NCE" pad="33"/>
<connect gate="A" pin="NCEO" pad="32"/>
<connect gate="A" pin="NCONFIG" pad="26"/>
<connect gate="A" pin="VCCA_PLL1" pad="27"/>
<connect gate="A" pin="VCCINT" pad="72"/>
<connect gate="A" pin="VCCIO1" pad="9"/>
<connect gate="A" pin="VCCIO1_2" pad="22"/>
<connect gate="A" pin="VCCIO1_3" pad="51"/>
<connect gate="A" pin="VCCIO4" pad="70"/>
<connect gate="B" pin="CLK2" pad="153"/>
<connect gate="B" pin="CLK3" pad="152"/>
<connect gate="B" pin="CONF_DONE" pad="145"/>
<connect gate="B" pin="GND" pad="129"/>
<connect gate="B" pin="GNDA_PLL2" pad="151"/>
<connect gate="B" pin="GNDG_PLL2" pad="150"/>
<connect gate="B" pin="GND_2" pad="89"/>
<connect gate="B" pin="GND_3" pad="142"/>
<connect gate="B" pin="GND_4" pad="91"/>
<connect gate="B" pin="GND_5" pad="96"/>
<connect gate="B" pin="GND_6" pad="102"/>
<connect gate="B" pin="GND_7" pad="109"/>
<connect gate="B" pin="GND_8" pad="111"/>
<connect gate="B" pin="IO" pad="160"/>
<connect gate="B" pin="IO_10" pad="94"/>
<connect gate="B" pin="IO_11" pad="95"/>
<connect gate="B" pin="IO_12" pad="98"/>
<connect gate="B" pin="IO_13" pad="99"/>
<connect gate="B" pin="IO_14" pad="100"/>
<connect gate="B" pin="IO_15" pad="101"/>
<connect gate="B" pin="IO_16" pad="104"/>
<connect gate="B" pin="IO_17" pad="105"/>
<connect gate="B" pin="IO_18" pad="106"/>
<connect gate="B" pin="IO_19" pad="107"/>
<connect gate="B" pin="IO_2" pad="82"/>
<connect gate="B" pin="IO_20" pad="108"/>
<connect gate="B" pin="IO_21" pad="113"/>
<connect gate="B" pin="IO_22" pad="114"/>
<connect gate="B" pin="IO_23" pad="115"/>
<connect gate="B" pin="IO_24" pad="116"/>
<connect gate="B" pin="IO_25" pad="117"/>
<connect gate="B" pin="IO_26" pad="118"/>
<connect gate="B" pin="IO_27" pad="119"/>
<connect gate="B" pin="IO_28" pad="120"/>
<connect gate="B" pin="IO_29" pad="121"/>
<connect gate="B" pin="IO_3" pad="83"/>
<connect gate="B" pin="IO_30" pad="122"/>
<connect gate="B" pin="IO_31" pad="123"/>
<connect gate="B" pin="IO_32" pad="124"/>
<connect gate="B" pin="IO_33" pad="125"/>
<connect gate="B" pin="IO_34" pad="126"/>
<connect gate="B" pin="IO_35" pad="127"/>
<connect gate="B" pin="IO_36" pad="128"/>
<connect gate="B" pin="IO_37" pad="131"/>
<connect gate="B" pin="IO_38" pad="132"/>
<connect gate="B" pin="IO_39" pad="133"/>
<connect gate="B" pin="IO_4" pad="84"/>
<connect gate="B" pin="IO_40" pad="134"/>
<connect gate="B" pin="IO_41" pad="135"/>
<connect gate="B" pin="IO_42" pad="136"/>
<connect gate="B" pin="IO_43" pad="137"/>
<connect gate="B" pin="IO_44" pad="138"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_46" pad="140"/>
<connect gate="B" pin="IO_47" pad="141"/>
<connect gate="B" pin="IO_48" pad="143"/>
<connect gate="B" pin="IO_49" pad="144"/>
<connect gate="B" pin="IO_5" pad="85"/>
<connect gate="B" pin="IO_50" pad="156"/>
<connect gate="B" pin="IO_51" pad="158"/>
<connect gate="B" pin="IO_52" pad="159"/>
<connect gate="B" pin="IO_6" pad="86"/>
<connect gate="B" pin="IO_7" pad="87"/>
<connect gate="B" pin="IO_8" pad="88"/>
<connect gate="B" pin="IO_9" pad="93"/>
<connect gate="B" pin="NSTATUS" pad="146"/>
<connect gate="B" pin="TCK" pad="147"/>
<connect gate="B" pin="TDI" pad="155"/>
<connect gate="B" pin="TDO" pad="149"/>
<connect gate="B" pin="TMS" pad="148"/>
<connect gate="B" pin="VCCA_PLL2" pad="154"/>
<connect gate="B" pin="VCCINT" pad="90"/>
<connect gate="B" pin="VCCINT_2" pad="97"/>
<connect gate="B" pin="VCCINT_3" pad="110"/>
<connect gate="B" pin="VCCINT_4" pad="103"/>
<connect gate="B" pin="VCCINT_5" pad="81"/>
<connect gate="B" pin="VCCIO3" pad="157"/>
<connect gate="B" pin="VCCIO3_2" pad="130"/>
<connect gate="B" pin="VCCIO4" pad="112"/>
<connect gate="B" pin="VCCIO4_2" pad="92"/>
<connect gate="C" pin="GND" pad="212"/>
<connect gate="C" pin="GND_10" pad="232"/>
<connect gate="C" pin="GND_2" pad="171"/>
<connect gate="C" pin="GND_3" pad="192"/>
<connect gate="C" pin="GND_4" pad="190"/>
<connect gate="C" pin="GND_5" pad="199"/>
<connect gate="C" pin="GND_6" pad="205"/>
<connect gate="C" pin="GND_7" pad="230"/>
<connect gate="C" pin="GND_8" pad="210"/>
<connect gate="C" pin="GND_9" pad="221"/>
<connect gate="C" pin="IO" pad="240"/>
<connect gate="C" pin="IO_10" pad="169"/>
<connect gate="C" pin="IO_11" pad="170"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="174"/>
<connect gate="C" pin="IO_14" pad="175"/>
<connect gate="C" pin="IO_15" pad="176"/>
<connect gate="C" pin="IO_16" pad="177"/>
<connect gate="C" pin="IO_17" pad="178"/>
<connect gate="C" pin="IO_18" pad="179"/>
<connect gate="C" pin="IO_19" pad="180"/>
<connect gate="C" pin="IO_2" pad="161"/>
<connect gate="C" pin="IO_20" pad="181"/>
<connect gate="C" pin="IO_21" pad="182"/>
<connect gate="C" pin="IO_22" pad="183"/>
<connect gate="C" pin="IO_23" pad="184"/>
<connect gate="C" pin="IO_24" pad="185"/>
<connect gate="C" pin="IO_25" pad="186"/>
<connect gate="C" pin="IO_26" pad="187"/>
<connect gate="C" pin="IO_27" pad="188"/>
<connect gate="C" pin="IO_28" pad="193"/>
<connect gate="C" pin="IO_29" pad="194"/>
<connect gate="C" pin="IO_3" pad="162"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="200"/>
<connect gate="C" pin="IO_34" pad="201"/>
<connect gate="C" pin="IO_35" pad="202"/>
<connect gate="C" pin="IO_36" pad="203"/>
<connect gate="C" pin="IO_37" pad="206"/>
<connect gate="C" pin="IO_38" pad="207"/>
<connect gate="C" pin="IO_39" pad="208"/>
<connect gate="C" pin="IO_4" pad="163"/>
<connect gate="C" pin="IO_40" pad="213"/>
<connect gate="C" pin="IO_41" pad="214"/>
<connect gate="C" pin="IO_42" pad="215"/>
<connect gate="C" pin="IO_43" pad="216"/>
<connect gate="C" pin="IO_44" pad="217"/>
<connect gate="C" pin="IO_45" pad="218"/>
<connect gate="C" pin="IO_46" pad="219"/>
<connect gate="C" pin="IO_47" pad="222"/>
<connect gate="C" pin="IO_48" pad="223"/>
<connect gate="C" pin="IO_49" pad="224"/>
<connect gate="C" pin="IO_5" pad="164"/>
<connect gate="C" pin="IO_50" pad="225"/>
<connect gate="C" pin="IO_51" pad="226"/>
<connect gate="C" pin="IO_52" pad="227"/>
<connect gate="C" pin="IO_53" pad="228"/>
<connect gate="C" pin="IO_54" pad="233"/>
<connect gate="C" pin="IO_55" pad="234"/>
<connect gate="C" pin="IO_56" pad="235"/>
<connect gate="C" pin="IO_57" pad="236"/>
<connect gate="C" pin="IO_58" pad="237"/>
<connect gate="C" pin="IO_59" pad="238"/>
<connect gate="C" pin="IO_6" pad="165"/>
<connect gate="C" pin="IO_60" pad="239"/>
<connect gate="C" pin="IO_7" pad="166"/>
<connect gate="C" pin="IO_8" pad="167"/>
<connect gate="C" pin="IO_9" pad="168"/>
<connect gate="C" pin="VCCINT" pad="229"/>
<connect gate="C" pin="VCCINT_2" pad="191"/>
<connect gate="C" pin="VCCINT_3" pad="198"/>
<connect gate="C" pin="VCCINT_4" pad="204"/>
<connect gate="C" pin="VCCINT_5" pad="211"/>
<connect gate="C" pin="VCCINT_6" pad="220"/>
<connect gate="C" pin="VCCIO2" pad="189"/>
<connect gate="C" pin="VCCIO2_2" pad="209"/>
<connect gate="C" pin="VCCIO2_3" pad="231"/>
<connect gate="C" pin="VCCIO3" pad="172"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C12Q240C8N"/>
<attribute name="OC_FARNELL" value="1662252"/>
<attribute name="OC_NEWARK" value="51R0540"/>
<attribute name="PACKAGE" value="240-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C20F324C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C20F324C8N_A"/>
<gate name="B" symbol="EP1C20F324C8N_B"/>
<gate name="C" symbol="EP1C20F324C8N_C"/>
<gate name="D" symbol="EP1C20F324C8N_D"/>
</gates>
<devices>
<device name="" package="BGA324C18X18X100P_1900X1900X22">
<connects>
<connect gate="A" pin="CLK0" pad="J3"/>
<connect gate="A" pin="CLK1" pad="J4"/>
<connect gate="A" pin="DATA0" pad="H7"/>
<connect gate="A" pin="GND" pad="G8"/>
<connect gate="A" pin="GNDG_PLL1" pad="J6"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="A3"/>
<connect gate="A" pin="GND_4" pad="B2"/>
<connect gate="A" pin="GND_5" pad="F9"/>
<connect gate="A" pin="GND_6" pad="H8"/>
<connect gate="A" pin="GND_7" pad="J8"/>
<connect gate="A" pin="GND_8" pad="C1"/>
<connect gate="A" pin="GND_9" pad="H9"/>
<connect gate="A" pin="IO" pad="J1"/>
<connect gate="A" pin="IO_10" pad="B6"/>
<connect gate="A" pin="IO_11" pad="B7"/>
<connect gate="A" pin="IO_12" pad="B8"/>
<connect gate="A" pin="IO_13" pad="B9"/>
<connect gate="A" pin="IO_14" pad="C2"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D1"/>
<connect gate="A" pin="IO_23" pad="D2"/>
<connect gate="A" pin="IO_24" pad="D3"/>
<connect gate="A" pin="IO_25" pad="D4"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="E5"/>
<connect gate="A" pin="IO_35" pad="E6"/>
<connect gate="A" pin="IO_36" pad="E7"/>
<connect gate="A" pin="IO_37" pad="E8"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F5"/>
<connect gate="A" pin="IO_43" pad="F6"/>
<connect gate="A" pin="IO_44" pad="F7"/>
<connect gate="A" pin="IO_45" pad="G1"/>
<connect gate="A" pin="IO_46" pad="G2"/>
<connect gate="A" pin="IO_47" pad="G3"/>
<connect gate="A" pin="IO_48" pad="G4"/>
<connect gate="A" pin="IO_49" pad="G5"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_50" pad="G6"/>
<connect gate="A" pin="IO_51" pad="H1"/>
<connect gate="A" pin="IO_52" pad="H2"/>
<connect gate="A" pin="IO_53" pad="H3"/>
<connect gate="A" pin="IO_54" pad="H4"/>
<connect gate="A" pin="IO_55" pad="H5"/>
<connect gate="A" pin="IO_56" pad="H6"/>
<connect gate="A" pin="IO_6" pad="A9"/>
<connect gate="A" pin="IO_7" pad="B3"/>
<connect gate="A" pin="IO_8" pad="B4"/>
<connect gate="A" pin="IO_9" pad="B5"/>
<connect gate="A" pin="NCE" pad="J7"/>
<connect gate="A" pin="NCONFIG" pad="J2"/>
<connect gate="A" pin="VCCA_PLL1" pad="J5"/>
<connect gate="A" pin="VCCINT" pad="G9"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCINT_3" pad="A2"/>
<connect gate="A" pin="VCCINT_4" pad="B1"/>
<connect gate="A" pin="VCCINT_5" pad="F8"/>
<connect gate="A" pin="VCCIO1" pad="G7"/>
<connect gate="A" pin="VCCIO1_2" pad="E1"/>
<connect gate="A" pin="VCCIO2" pad="A5"/>
<connect gate="A" pin="VCCIO2_2" pad="E9"/>
<connect gate="B" pin="DCLK" pad="L1"/>
<connect gate="B" pin="GND" pad="V3"/>
<connect gate="B" pin="GNDA_PLL1" pad="K1"/>
<connect gate="B" pin="GND_2" pad="U2"/>
<connect gate="B" pin="GND_3" pad="K8"/>
<connect gate="B" pin="GND_4" pad="M9"/>
<connect gate="B" pin="GND_5" pad="K9"/>
<connect gate="B" pin="GND_6" pad="T1"/>
<connect gate="B" pin="GND_7" pad="N8"/>
<connect gate="B" pin="GND_8" pad="L8"/>
<connect gate="B" pin="GND_9" pad="V1"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO_10" pad="L7"/>
<connect gate="B" pin="IO_11" pad="M1"/>
<connect gate="B" pin="IO_12" pad="M2"/>
<connect gate="B" pin="IO_13" pad="M3"/>
<connect gate="B" pin="IO_14" pad="M4"/>
<connect gate="B" pin="IO_15" pad="M5"/>
<connect gate="B" pin="IO_16" pad="M6"/>
<connect gate="B" pin="IO_17" pad="N1"/>
<connect gate="B" pin="IO_18" pad="N2"/>
<connect gate="B" pin="IO_19" pad="N3"/>
<connect gate="B" pin="IO_2" pad="K4"/>
<connect gate="B" pin="IO_20" pad="N4"/>
<connect gate="B" pin="IO_21" pad="N5"/>
<connect gate="B" pin="IO_22" pad="N6"/>
<connect gate="B" pin="IO_23" pad="N7"/>
<connect gate="B" pin="IO_24" pad="P2"/>
<connect gate="B" pin="IO_25" pad="P3"/>
<connect gate="B" pin="IO_26" pad="P4"/>
<connect gate="B" pin="IO_27" pad="P5"/>
<connect gate="B" pin="IO_28" pad="P6"/>
<connect gate="B" pin="IO_29" pad="P7"/>
<connect gate="B" pin="IO_3" pad="K5"/>
<connect gate="B" pin="IO_30" pad="P9"/>
<connect gate="B" pin="IO_31" pad="R1"/>
<connect gate="B" pin="IO_32" pad="R2"/>
<connect gate="B" pin="IO_33" pad="R3"/>
<connect gate="B" pin="IO_34" pad="R4"/>
<connect gate="B" pin="IO_35" pad="R5"/>
<connect gate="B" pin="IO_36" pad="R6"/>
<connect gate="B" pin="IO_37" pad="R7"/>
<connect gate="B" pin="IO_38" pad="R8"/>
<connect gate="B" pin="IO_39" pad="R9"/>
<connect gate="B" pin="IO_4" pad="K6"/>
<connect gate="B" pin="IO_40" pad="T2"/>
<connect gate="B" pin="IO_41" pad="T3"/>
<connect gate="B" pin="IO_42" pad="T4"/>
<connect gate="B" pin="IO_43" pad="T5"/>
<connect gate="B" pin="IO_44" pad="T6"/>
<connect gate="B" pin="IO_45" pad="T7"/>
<connect gate="B" pin="IO_46" pad="T8"/>
<connect gate="B" pin="IO_47" pad="T9"/>
<connect gate="B" pin="IO_48" pad="U3"/>
<connect gate="B" pin="IO_49" pad="U4"/>
<connect gate="B" pin="IO_5" pad="L2"/>
<connect gate="B" pin="IO_50" pad="U5"/>
<connect gate="B" pin="IO_51" pad="U6"/>
<connect gate="B" pin="IO_52" pad="U7"/>
<connect gate="B" pin="IO_53" pad="U8"/>
<connect gate="B" pin="IO_54" pad="U9"/>
<connect gate="B" pin="IO_55" pad="V4"/>
<connect gate="B" pin="IO_56" pad="V6"/>
<connect gate="B" pin="IO_57" pad="V7"/>
<connect gate="B" pin="IO_58" pad="V8"/>
<connect gate="B" pin="IO_6" pad="L3"/>
<connect gate="B" pin="IO_7" pad="L4"/>
<connect gate="B" pin="IO_8" pad="L5"/>
<connect gate="B" pin="IO_9" pad="L6"/>
<connect gate="B" pin="MSEL0" pad="K3"/>
<connect gate="B" pin="MSEL1" pad="K7"/>
<connect gate="B" pin="NCEO" pad="K2"/>
<connect gate="B" pin="VCCINT" pad="V2"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="M8"/>
<connect gate="B" pin="VCCINT_4" pad="N9"/>
<connect gate="B" pin="VCCINT_5" pad="U1"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO1_2" pad="M7"/>
<connect gate="B" pin="VCCIO4" pad="P8"/>
<connect gate="B" pin="VCCIO4_2" pad="V5"/>
<connect gate="C" pin="CLK2" pad="J15"/>
<connect gate="C" pin="CLK3" pad="J16"/>
<connect gate="C" pin="GND" pad="A16"/>
<connect gate="C" pin="GNDG_PLL2" pad="J18"/>
<connect gate="C" pin="GND_2" pad="F11"/>
<connect gate="C" pin="GND_3" pad="C18"/>
<connect gate="C" pin="GND_4" pad="G10"/>
<connect gate="C" pin="GND_5" pad="H11"/>
<connect gate="C" pin="GND_6" pad="A18"/>
<connect gate="C" pin="GND_7" pad="B17"/>
<connect gate="C" pin="GND_8" pad="J10"/>
<connect gate="C" pin="GND_9" pad="J11"/>
<connect gate="C" pin="IO" pad="J14"/>
<connect gate="C" pin="IO_10" pad="B13"/>
<connect gate="C" pin="IO_11" pad="B14"/>
<connect gate="C" pin="IO_12" pad="B15"/>
<connect gate="C" pin="IO_13" pad="B16"/>
<connect gate="C" pin="IO_14" pad="C10"/>
<connect gate="C" pin="IO_15" pad="C11"/>
<connect gate="C" pin="IO_16" pad="C12"/>
<connect gate="C" pin="IO_17" pad="C13"/>
<connect gate="C" pin="IO_18" pad="C14"/>
<connect gate="C" pin="IO_19" pad="C15"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C16"/>
<connect gate="C" pin="IO_21" pad="C17"/>
<connect gate="C" pin="IO_22" pad="D10"/>
<connect gate="C" pin="IO_23" pad="D11"/>
<connect gate="C" pin="IO_24" pad="D12"/>
<connect gate="C" pin="IO_25" pad="D13"/>
<connect gate="C" pin="IO_26" pad="D14"/>
<connect gate="C" pin="IO_27" pad="D15"/>
<connect gate="C" pin="IO_28" pad="D16"/>
<connect gate="C" pin="IO_29" pad="D17"/>
<connect gate="C" pin="IO_3" pad="A11"/>
<connect gate="C" pin="IO_30" pad="D18"/>
<connect gate="C" pin="IO_31" pad="E10"/>
<connect gate="C" pin="IO_32" pad="E11"/>
<connect gate="C" pin="IO_33" pad="E13"/>
<connect gate="C" pin="IO_34" pad="E14"/>
<connect gate="C" pin="IO_35" pad="E15"/>
<connect gate="C" pin="IO_36" pad="E16"/>
<connect gate="C" pin="IO_37" pad="E17"/>
<connect gate="C" pin="IO_38" pad="F12"/>
<connect gate="C" pin="IO_39" pad="F13"/>
<connect gate="C" pin="IO_4" pad="A12"/>
<connect gate="C" pin="IO_40" pad="F14"/>
<connect gate="C" pin="IO_41" pad="F15"/>
<connect gate="C" pin="IO_42" pad="F16"/>
<connect gate="C" pin="IO_43" pad="F17"/>
<connect gate="C" pin="IO_44" pad="F18"/>
<connect gate="C" pin="IO_45" pad="G12"/>
<connect gate="C" pin="IO_46" pad="G13"/>
<connect gate="C" pin="IO_47" pad="G14"/>
<connect gate="C" pin="IO_48" pad="G15"/>
<connect gate="C" pin="IO_49" pad="G16"/>
<connect gate="C" pin="IO_5" pad="A13"/>
<connect gate="C" pin="IO_50" pad="G17"/>
<connect gate="C" pin="IO_51" pad="G18"/>
<connect gate="C" pin="IO_52" pad="H13"/>
<connect gate="C" pin="IO_53" pad="H14"/>
<connect gate="C" pin="IO_54" pad="H15"/>
<connect gate="C" pin="IO_55" pad="H16"/>
<connect gate="C" pin="IO_56" pad="H17"/>
<connect gate="C" pin="IO_57" pad="H18"/>
<connect gate="C" pin="IO_58" pad="J13"/>
<connect gate="C" pin="IO_6" pad="A15"/>
<connect gate="C" pin="IO_7" pad="B10"/>
<connect gate="C" pin="IO_8" pad="B11"/>
<connect gate="C" pin="IO_9" pad="B12"/>
<connect gate="C" pin="TDI" pad="J17"/>
<connect gate="C" pin="VCCA_PLL2" pad="J12"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCINT_2" pad="A17"/>
<connect gate="C" pin="VCCINT_3" pad="B18"/>
<connect gate="C" pin="VCCINT_4" pad="G11"/>
<connect gate="C" pin="VCCINT_5" pad="F10"/>
<connect gate="C" pin="VCCIO2" pad="E12"/>
<connect gate="C" pin="VCCIO2_2" pad="A14"/>
<connect gate="C" pin="VCCIO3" pad="H12"/>
<connect gate="C" pin="VCCIO3_2" pad="E18"/>
<connect gate="D" pin="CONF_DONE" pad="K17"/>
<connect gate="D" pin="GND" pad="U17"/>
<connect gate="D" pin="GNDA_PLL2" pad="K12"/>
<connect gate="D" pin="GND_2" pad="K11"/>
<connect gate="D" pin="GND_3" pad="L10"/>
<connect gate="D" pin="GND_4" pad="L11"/>
<connect gate="D" pin="GND_5" pad="M11"/>
<connect gate="D" pin="GND_6" pad="V18"/>
<connect gate="D" pin="GND_7" pad="T18"/>
<connect gate="D" pin="GND_8" pad="N10"/>
<connect gate="D" pin="GND_9" pad="V16"/>
<connect gate="D" pin="IO" pad="V15"/>
<connect gate="D" pin="IO_10" pad="M13"/>
<connect gate="D" pin="IO_11" pad="M14"/>
<connect gate="D" pin="IO_12" pad="M15"/>
<connect gate="D" pin="IO_13" pad="M16"/>
<connect gate="D" pin="IO_14" pad="M17"/>
<connect gate="D" pin="IO_15" pad="M18"/>
<connect gate="D" pin="IO_16" pad="N12"/>
<connect gate="D" pin="IO_17" pad="N13"/>
<connect gate="D" pin="IO_18" pad="N14"/>
<connect gate="D" pin="IO_19" pad="N15"/>
<connect gate="D" pin="IO_2" pad="K15"/>
<connect gate="D" pin="IO_20" pad="N16"/>
<connect gate="D" pin="IO_21" pad="N17"/>
<connect gate="D" pin="IO_22" pad="N18"/>
<connect gate="D" pin="IO_23" pad="P10"/>
<connect gate="D" pin="IO_24" pad="P12"/>
<connect gate="D" pin="IO_25" pad="P13"/>
<connect gate="D" pin="IO_26" pad="P14"/>
<connect gate="D" pin="IO_27" pad="P15"/>
<connect gate="D" pin="IO_28" pad="P16"/>
<connect gate="D" pin="IO_29" pad="P17"/>
<connect gate="D" pin="IO_3" pad="K16"/>
<connect gate="D" pin="IO_30" pad="R10"/>
<connect gate="D" pin="IO_31" pad="R11"/>
<connect gate="D" pin="IO_32" pad="R12"/>
<connect gate="D" pin="IO_33" pad="R13"/>
<connect gate="D" pin="IO_34" pad="R14"/>
<connect gate="D" pin="IO_35" pad="R15"/>
<connect gate="D" pin="IO_36" pad="R16"/>
<connect gate="D" pin="IO_37" pad="R17"/>
<connect gate="D" pin="IO_38" pad="R18"/>
<connect gate="D" pin="IO_39" pad="T10"/>
<connect gate="D" pin="IO_4" pad="L13"/>
<connect gate="D" pin="IO_40" pad="T11"/>
<connect gate="D" pin="IO_41" pad="T12"/>
<connect gate="D" pin="IO_42" pad="T13"/>
<connect gate="D" pin="IO_43" pad="T14"/>
<connect gate="D" pin="IO_44" pad="T15"/>
<connect gate="D" pin="IO_45" pad="T16"/>
<connect gate="D" pin="IO_46" pad="T17"/>
<connect gate="D" pin="IO_47" pad="U10"/>
<connect gate="D" pin="IO_48" pad="U11"/>
<connect gate="D" pin="IO_49" pad="U12"/>
<connect gate="D" pin="IO_5" pad="L14"/>
<connect gate="D" pin="IO_50" pad="U13"/>
<connect gate="D" pin="IO_51" pad="U14"/>
<connect gate="D" pin="IO_52" pad="U15"/>
<connect gate="D" pin="IO_53" pad="U16"/>
<connect gate="D" pin="IO_54" pad="V10"/>
<connect gate="D" pin="IO_55" pad="V11"/>
<connect gate="D" pin="IO_56" pad="V12"/>
<connect gate="D" pin="IO_57" pad="V13"/>
<connect gate="D" pin="IO_6" pad="L15"/>
<connect gate="D" pin="IO_7" pad="L16"/>
<connect gate="D" pin="IO_8" pad="L17"/>
<connect gate="D" pin="IO_9" pad="L18"/>
<connect gate="D" pin="NSTATUS" pad="L12"/>
<connect gate="D" pin="TCK" pad="K18"/>
<connect gate="D" pin="TDO" pad="K13"/>
<connect gate="D" pin="TMS" pad="K14"/>
<connect gate="D" pin="VCCINT" pad="U18"/>
<connect gate="D" pin="VCCINT_2" pad="K10"/>
<connect gate="D" pin="VCCINT_3" pad="M10"/>
<connect gate="D" pin="VCCINT_4" pad="V17"/>
<connect gate="D" pin="VCCINT_5" pad="N11"/>
<connect gate="D" pin="VCCIO3" pad="P18"/>
<connect gate="D" pin="VCCIO3_2" pad="M12"/>
<connect gate="D" pin="VCCIO4" pad="V14"/>
<connect gate="D" pin="VCCIO4_2" pad="P11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C20F324C8N"/>
<attribute name="OC_FARNELL" value="1662280"/>
<attribute name="OC_NEWARK" value="51R0541"/>
<attribute name="PACKAGE" value="324-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C20F400C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C20F400C8N_A"/>
<gate name="B" symbol="EP1C20F400C8N_B"/>
<gate name="C" symbol="EP1C20F400C8N_C"/>
<gate name="D" symbol="EP1C20F400C8N_D"/>
</gates>
<devices>
<device name="" package="BGA400C20X20X100P_2100X2100X22">
<connects>
<connect gate="A" pin="CLK0/LVDSCLK1P" pad="K5"/>
<connect gate="A" pin="CLK1/LVDSCLK1N" pad="K6"/>
<connect gate="A" pin="DATA0" pad="K3"/>
<connect gate="A" pin="DCLK" pad="L3"/>
<connect gate="A" pin="GND" pad="H9"/>
<connect gate="A" pin="GNDA_PLL1" pad="K7"/>
<connect gate="A" pin="GNDG_PLL1" pad="L7"/>
<connect gate="A" pin="GND_2" pad="A3"/>
<connect gate="A" pin="GND_3" pad="B2"/>
<connect gate="A" pin="GND_4" pad="K9"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="GND_6" pad="C1"/>
<connect gate="A" pin="GND_7" pad="G8"/>
<connect gate="A" pin="GND_8" pad="G9"/>
<connect gate="A" pin="IO" pad="M1"/>
<connect gate="A" pin="IO/ASDO" pad="L4"/>
<connect gate="A" pin="IO_10" pad="B6"/>
<connect gate="A" pin="IO_11" pad="B7"/>
<connect gate="A" pin="IO_12" pad="B8"/>
<connect gate="A" pin="IO_13" pad="B9"/>
<connect gate="A" pin="IO_14" pad="C2"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D1"/>
<connect gate="A" pin="IO_23" pad="D2"/>
<connect gate="A" pin="IO_24" pad="D3"/>
<connect gate="A" pin="IO_25" pad="D4"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="E5"/>
<connect gate="A" pin="IO_35" pad="E6"/>
<connect gate="A" pin="IO_36" pad="E7"/>
<connect gate="A" pin="IO_37" pad="E8"/>
<connect gate="A" pin="IO_38" pad="E9"/>
<connect gate="A" pin="IO_39" pad="F1"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="F2"/>
<connect gate="A" pin="IO_41" pad="F3"/>
<connect gate="A" pin="IO_42" pad="F4"/>
<connect gate="A" pin="IO_43" pad="F5"/>
<connect gate="A" pin="IO_44" pad="F6"/>
<connect gate="A" pin="IO_45" pad="F7"/>
<connect gate="A" pin="IO_46" pad="F8"/>
<connect gate="A" pin="IO_47" pad="G1"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="G3"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_50" pad="G4"/>
<connect gate="A" pin="IO_51" pad="G5"/>
<connect gate="A" pin="IO_52" pad="G6"/>
<connect gate="A" pin="IO_53" pad="G7"/>
<connect gate="A" pin="IO_54" pad="H1"/>
<connect gate="A" pin="IO_55" pad="H2"/>
<connect gate="A" pin="IO_56" pad="H3"/>
<connect gate="A" pin="IO_57" pad="H4"/>
<connect gate="A" pin="IO_58" pad="H5"/>
<connect gate="A" pin="IO_59" pad="H6"/>
<connect gate="A" pin="IO_6" pad="A9"/>
<connect gate="A" pin="IO_60" pad="H7"/>
<connect gate="A" pin="IO_61" pad="J1"/>
<connect gate="A" pin="IO_62" pad="J2"/>
<connect gate="A" pin="IO_63" pad="J3"/>
<connect gate="A" pin="IO_64" pad="J4"/>
<connect gate="A" pin="IO_65" pad="J5"/>
<connect gate="A" pin="IO_66" pad="J6"/>
<connect gate="A" pin="IO_67" pad="J7"/>
<connect gate="A" pin="IO_68" pad="J8"/>
<connect gate="A" pin="IO_69" pad="K2"/>
<connect gate="A" pin="IO_7" pad="B3"/>
<connect gate="A" pin="IO_70" pad="L8"/>
<connect gate="A" pin="IO_8" pad="B4"/>
<connect gate="A" pin="IO_9" pad="B5"/>
<connect gate="A" pin="MSEL0" pad="L1"/>
<connect gate="A" pin="MSEL1" pad="L6"/>
<connect gate="A" pin="NCE" pad="L5"/>
<connect gate="A" pin="NCEO" pad="L2"/>
<connect gate="A" pin="NCONFIG" pad="K1"/>
<connect gate="A" pin="VCCA_PLL1" pad="K4"/>
<connect gate="A" pin="VCCINT" pad="A2"/>
<connect gate="A" pin="VCCINT_2" pad="B1"/>
<connect gate="A" pin="VCCINT_3" pad="J9"/>
<connect gate="A" pin="VCCINT_4" pad="L9"/>
<connect gate="A" pin="VCCIO1" pad="E1"/>
<connect gate="A" pin="VCCIO1_2" pad="H8"/>
<connect gate="A" pin="VCCIO1_3" pad="K8"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A5"/>
<connect gate="B" pin="GND" pad="A18"/>
<connect gate="B" pin="GND_2" pad="V1"/>
<connect gate="B" pin="GND_3" pad="A20"/>
<connect gate="B" pin="GND_4" pad="M9"/>
<connect gate="B" pin="GND_5" pad="W2"/>
<connect gate="B" pin="GND_6" pad="P8"/>
<connect gate="B" pin="GND_7" pad="Y1"/>
<connect gate="B" pin="GND_8" pad="P9"/>
<connect gate="B" pin="GND_9" pad="Y3"/>
<connect gate="B" pin="IO" pad="B18"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N4"/>
<connect gate="B" pin="IO_13" pad="N5"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="P1"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="M2"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="R1"/>
<connect gate="B" pin="IO_24" pad="R2"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M3"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T2"/>
<connect gate="B" pin="IO_32" pad="T3"/>
<connect gate="B" pin="IO_33" pad="T4"/>
<connect gate="B" pin="IO_34" pad="T5"/>
<connect gate="B" pin="IO_35" pad="T6"/>
<connect gate="B" pin="IO_36" pad="T7"/>
<connect gate="B" pin="IO_37" pad="T8"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="U1"/>
<connect gate="B" pin="IO_4" pad="M4"/>
<connect gate="B" pin="IO_40" pad="U2"/>
<connect gate="B" pin="IO_41" pad="U3"/>
<connect gate="B" pin="IO_42" pad="U4"/>
<connect gate="B" pin="IO_43" pad="U5"/>
<connect gate="B" pin="IO_44" pad="U6"/>
<connect gate="B" pin="IO_45" pad="U7"/>
<connect gate="B" pin="IO_46" pad="U8"/>
<connect gate="B" pin="IO_47" pad="U9"/>
<connect gate="B" pin="IO_48" pad="V2"/>
<connect gate="B" pin="IO_49" pad="V3"/>
<connect gate="B" pin="IO_5" pad="M5"/>
<connect gate="B" pin="IO_50" pad="V4"/>
<connect gate="B" pin="IO_51" pad="V5"/>
<connect gate="B" pin="IO_52" pad="V6"/>
<connect gate="B" pin="IO_53" pad="V7"/>
<connect gate="B" pin="IO_54" pad="V8"/>
<connect gate="B" pin="IO_55" pad="V9"/>
<connect gate="B" pin="IO_56" pad="W3"/>
<connect gate="B" pin="IO_57" pad="W4"/>
<connect gate="B" pin="IO_58" pad="W5"/>
<connect gate="B" pin="IO_59" pad="W6"/>
<connect gate="B" pin="IO_6" pad="M6"/>
<connect gate="B" pin="IO_60" pad="W7"/>
<connect gate="B" pin="IO_61" pad="W8"/>
<connect gate="B" pin="IO_62" pad="W9"/>
<connect gate="B" pin="IO_63" pad="Y4"/>
<connect gate="B" pin="IO_64" pad="Y6"/>
<connect gate="B" pin="IO_65" pad="Y7"/>
<connect gate="B" pin="IO_66" pad="Y8"/>
<connect gate="B" pin="IO_67" pad="Y9"/>
<connect gate="B" pin="IO_68" pad="A10"/>
<connect gate="B" pin="IO_69" pad="A11"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_70" pad="A12"/>
<connect gate="B" pin="IO_71" pad="A13"/>
<connect gate="B" pin="IO_72" pad="A14"/>
<connect gate="B" pin="IO_73" pad="A15"/>
<connect gate="B" pin="IO_74" pad="A17"/>
<connect gate="B" pin="IO_75" pad="B10"/>
<connect gate="B" pin="IO_76" pad="B11"/>
<connect gate="B" pin="IO_77" pad="B12"/>
<connect gate="B" pin="IO_78" pad="B13"/>
<connect gate="B" pin="IO_79" pad="B14"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_80" pad="B15"/>
<connect gate="B" pin="IO_81" pad="B16"/>
<connect gate="B" pin="IO_82" pad="B17"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="VCCINT" pad="A19"/>
<connect gate="B" pin="VCCINT_2" pad="N9"/>
<connect gate="B" pin="VCCINT_3" pad="W1"/>
<connect gate="B" pin="VCCINT_4" pad="Y2"/>
<connect gate="B" pin="VCCIO1" pad="N8"/>
<connect gate="B" pin="VCCIO1_2" pad="T1"/>
<connect gate="B" pin="VCCIO2" pad="A16"/>
<connect gate="B" pin="VCCIO4" pad="Y5"/>
<connect gate="B" pin="VCCIO4_2" pad="R8"/>
<connect gate="C" pin="CLK2" pad="L14"/>
<connect gate="C" pin="CLK3" pad="K14"/>
<connect gate="C" pin="CONF_DONE" pad="L18"/>
<connect gate="C" pin="GND" pad="J10"/>
<connect gate="C" pin="GNDA_PLL2" pad="K20"/>
<connect gate="C" pin="GNDG_PLL2" pad="L15"/>
<connect gate="C" pin="GND_10" pad="J12"/>
<connect gate="C" pin="GND_11" pad="G13"/>
<connect gate="C" pin="GND_12" pad="K11"/>
<connect gate="C" pin="GND_2" pad="C20"/>
<connect gate="C" pin="GND_3" pad="B19"/>
<connect gate="C" pin="GND_4" pad="G11"/>
<connect gate="C" pin="GND_5" pad="L12"/>
<connect gate="C" pin="GND_6" pad="G12"/>
<connect gate="C" pin="GND_7" pad="G10"/>
<connect gate="C" pin="GND_8" pad="H11"/>
<connect gate="C" pin="GND_9" pad="L10"/>
<connect gate="C" pin="IO" pad="L13"/>
<connect gate="C" pin="IO_10" pad="C18"/>
<connect gate="C" pin="IO_11" pad="C19"/>
<connect gate="C" pin="IO_12" pad="D10"/>
<connect gate="C" pin="IO_13" pad="D11"/>
<connect gate="C" pin="IO_14" pad="D12"/>
<connect gate="C" pin="IO_15" pad="D13"/>
<connect gate="C" pin="IO_16" pad="D14"/>
<connect gate="C" pin="IO_17" pad="D15"/>
<connect gate="C" pin="IO_18" pad="D16"/>
<connect gate="C" pin="IO_19" pad="D17"/>
<connect gate="C" pin="IO_2" pad="C10"/>
<connect gate="C" pin="IO_20" pad="D18"/>
<connect gate="C" pin="IO_21" pad="D19"/>
<connect gate="C" pin="IO_22" pad="D20"/>
<connect gate="C" pin="IO_23" pad="E10"/>
<connect gate="C" pin="IO_24" pad="E11"/>
<connect gate="C" pin="IO_25" pad="E12"/>
<connect gate="C" pin="IO_26" pad="E13"/>
<connect gate="C" pin="IO_27" pad="E14"/>
<connect gate="C" pin="IO_28" pad="E15"/>
<connect gate="C" pin="IO_29" pad="E16"/>
<connect gate="C" pin="IO_3" pad="C11"/>
<connect gate="C" pin="IO_30" pad="E17"/>
<connect gate="C" pin="IO_31" pad="E18"/>
<connect gate="C" pin="IO_32" pad="E19"/>
<connect gate="C" pin="IO_33" pad="F10"/>
<connect gate="C" pin="IO_34" pad="F12"/>
<connect gate="C" pin="IO_35" pad="F14"/>
<connect gate="C" pin="IO_36" pad="F15"/>
<connect gate="C" pin="IO_37" pad="F16"/>
<connect gate="C" pin="IO_38" pad="F17"/>
<connect gate="C" pin="IO_39" pad="F18"/>
<connect gate="C" pin="IO_4" pad="C12"/>
<connect gate="C" pin="IO_40" pad="F19"/>
<connect gate="C" pin="IO_41" pad="F20"/>
<connect gate="C" pin="IO_42" pad="G14"/>
<connect gate="C" pin="IO_43" pad="G15"/>
<connect gate="C" pin="IO_44" pad="G16"/>
<connect gate="C" pin="IO_45" pad="G17"/>
<connect gate="C" pin="IO_46" pad="G18"/>
<connect gate="C" pin="IO_47" pad="G19"/>
<connect gate="C" pin="IO_48" pad="G20"/>
<connect gate="C" pin="IO_49" pad="H14"/>
<connect gate="C" pin="IO_5" pad="C13"/>
<connect gate="C" pin="IO_50" pad="H15"/>
<connect gate="C" pin="IO_51" pad="H16"/>
<connect gate="C" pin="IO_52" pad="H17"/>
<connect gate="C" pin="IO_53" pad="H18"/>
<connect gate="C" pin="IO_54" pad="H19"/>
<connect gate="C" pin="IO_55" pad="H20"/>
<connect gate="C" pin="IO_56" pad="J13"/>
<connect gate="C" pin="IO_57" pad="J14"/>
<connect gate="C" pin="IO_58" pad="J15"/>
<connect gate="C" pin="IO_59" pad="J16"/>
<connect gate="C" pin="IO_6" pad="C14"/>
<connect gate="C" pin="IO_60" pad="J17"/>
<connect gate="C" pin="IO_61" pad="J18"/>
<connect gate="C" pin="IO_62" pad="J19"/>
<connect gate="C" pin="IO_63" pad="J20"/>
<connect gate="C" pin="IO_64" pad="K15"/>
<connect gate="C" pin="IO_65" pad="K16"/>
<connect gate="C" pin="IO_66" pad="K19"/>
<connect gate="C" pin="IO_7" pad="C15"/>
<connect gate="C" pin="IO_8" pad="C16"/>
<connect gate="C" pin="IO_9" pad="C17"/>
<connect gate="C" pin="NSTATUS" pad="L17"/>
<connect gate="C" pin="TCK" pad="L19"/>
<connect gate="C" pin="TDI" pad="K18"/>
<connect gate="C" pin="TMS" pad="L16"/>
<connect gate="C" pin="VCCA_PLL2" pad="K17"/>
<connect gate="C" pin="VCCINT" pad="B20"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="K10"/>
<connect gate="C" pin="VCCINT_4" pad="H12"/>
<connect gate="C" pin="VCCINT_5" pad="L11"/>
<connect gate="C" pin="VCCINT_6" pad="K12"/>
<connect gate="C" pin="VCCINT_7" pad="J11"/>
<connect gate="C" pin="VCCIO2" pad="F13"/>
<connect gate="C" pin="VCCIO2_2" pad="F11"/>
<connect gate="C" pin="VCCIO3" pad="K13"/>
<connect gate="C" pin="VCCIO3_2" pad="H13"/>
<connect gate="C" pin="VCCIO3_3" pad="E20"/>
<connect gate="D" pin="GND" pad="P13"/>
<connect gate="D" pin="GND_10" pad="P11"/>
<connect gate="D" pin="GND_11" pad="P12"/>
<connect gate="D" pin="GND_2" pad="V20"/>
<connect gate="D" pin="GND_3" pad="Y20"/>
<connect gate="D" pin="GND_4" pad="N10"/>
<connect gate="D" pin="GND_5" pad="W19"/>
<connect gate="D" pin="GND_6" pad="Y18"/>
<connect gate="D" pin="GND_7" pad="N12"/>
<connect gate="D" pin="GND_8" pad="P10"/>
<connect gate="D" pin="GND_9" pad="M11"/>
<connect gate="D" pin="IO" pad="Y17"/>
<connect gate="D" pin="IO_10" pad="N14"/>
<connect gate="D" pin="IO_11" pad="N15"/>
<connect gate="D" pin="IO_12" pad="N16"/>
<connect gate="D" pin="IO_13" pad="N17"/>
<connect gate="D" pin="IO_14" pad="N18"/>
<connect gate="D" pin="IO_15" pad="N19"/>
<connect gate="D" pin="IO_16" pad="N20"/>
<connect gate="D" pin="IO_17" pad="P14"/>
<connect gate="D" pin="IO_18" pad="P15"/>
<connect gate="D" pin="IO_19" pad="P16"/>
<connect gate="D" pin="IO_2" pad="M13"/>
<connect gate="D" pin="IO_20" pad="P17"/>
<connect gate="D" pin="IO_21" pad="P18"/>
<connect gate="D" pin="IO_22" pad="P19"/>
<connect gate="D" pin="IO_23" pad="P20"/>
<connect gate="D" pin="IO_24" pad="R11"/>
<connect gate="D" pin="IO_25" pad="R13"/>
<connect gate="D" pin="IO_26" pad="R14"/>
<connect gate="D" pin="IO_27" pad="R15"/>
<connect gate="D" pin="IO_28" pad="R16"/>
<connect gate="D" pin="IO_29" pad="R17"/>
<connect gate="D" pin="IO_3" pad="M14"/>
<connect gate="D" pin="IO_30" pad="R18"/>
<connect gate="D" pin="IO_31" pad="R19"/>
<connect gate="D" pin="IO_32" pad="R20"/>
<connect gate="D" pin="IO_33" pad="T10"/>
<connect gate="D" pin="IO_34" pad="T11"/>
<connect gate="D" pin="IO_35" pad="T12"/>
<connect gate="D" pin="IO_36" pad="T13"/>
<connect gate="D" pin="IO_37" pad="T14"/>
<connect gate="D" pin="IO_38" pad="T15"/>
<connect gate="D" pin="IO_39" pad="T16"/>
<connect gate="D" pin="IO_4" pad="M15"/>
<connect gate="D" pin="IO_40" pad="T17"/>
<connect gate="D" pin="IO_41" pad="T18"/>
<connect gate="D" pin="IO_42" pad="T19"/>
<connect gate="D" pin="IO_43" pad="U10"/>
<connect gate="D" pin="IO_44" pad="U11"/>
<connect gate="D" pin="IO_45" pad="U12"/>
<connect gate="D" pin="IO_46" pad="U13"/>
<connect gate="D" pin="IO_47" pad="U14"/>
<connect gate="D" pin="IO_48" pad="U15"/>
<connect gate="D" pin="IO_49" pad="U16"/>
<connect gate="D" pin="IO_5" pad="M16"/>
<connect gate="D" pin="IO_50" pad="U17"/>
<connect gate="D" pin="IO_51" pad="U18"/>
<connect gate="D" pin="IO_52" pad="U19"/>
<connect gate="D" pin="IO_53" pad="U20"/>
<connect gate="D" pin="IO_54" pad="V10"/>
<connect gate="D" pin="IO_55" pad="V11"/>
<connect gate="D" pin="IO_56" pad="V12"/>
<connect gate="D" pin="IO_57" pad="V13"/>
<connect gate="D" pin="IO_58" pad="V14"/>
<connect gate="D" pin="IO_59" pad="V15"/>
<connect gate="D" pin="IO_6" pad="M17"/>
<connect gate="D" pin="IO_60" pad="V16"/>
<connect gate="D" pin="IO_61" pad="V17"/>
<connect gate="D" pin="IO_62" pad="V18"/>
<connect gate="D" pin="IO_63" pad="V19"/>
<connect gate="D" pin="IO_64" pad="W10"/>
<connect gate="D" pin="IO_65" pad="W11"/>
<connect gate="D" pin="IO_66" pad="W12"/>
<connect gate="D" pin="IO_67" pad="W13"/>
<connect gate="D" pin="IO_68" pad="W14"/>
<connect gate="D" pin="IO_69" pad="W15"/>
<connect gate="D" pin="IO_7" pad="M18"/>
<connect gate="D" pin="IO_70" pad="W16"/>
<connect gate="D" pin="IO_71" pad="W17"/>
<connect gate="D" pin="IO_72" pad="W18"/>
<connect gate="D" pin="IO_73" pad="Y10"/>
<connect gate="D" pin="IO_74" pad="Y11"/>
<connect gate="D" pin="IO_75" pad="Y12"/>
<connect gate="D" pin="IO_76" pad="Y13"/>
<connect gate="D" pin="IO_77" pad="Y14"/>
<connect gate="D" pin="IO_78" pad="Y15"/>
<connect gate="D" pin="IO_8" pad="M19"/>
<connect gate="D" pin="IO_9" pad="M20"/>
<connect gate="D" pin="TDO" pad="L20"/>
<connect gate="D" pin="VCCINT" pad="N11"/>
<connect gate="D" pin="VCCINT_2" pad="M10"/>
<connect gate="D" pin="VCCINT_3" pad="Y19"/>
<connect gate="D" pin="VCCINT_4" pad="W20"/>
<connect gate="D" pin="VCCINT_5" pad="M12"/>
<connect gate="D" pin="VCCIO3" pad="T20"/>
<connect gate="D" pin="VCCIO3_2" pad="N13"/>
<connect gate="D" pin="VCCIO4" pad="R12"/>
<connect gate="D" pin="VCCIO4_2" pad="Y16"/>
<connect gate="D" pin="VCCIO4_3" pad="R10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C20F400C8N"/>
<attribute name="OC_FARNELL" value="1549374"/>
<attribute name="OC_NEWARK" value="51R0542"/>
<attribute name="PACKAGE" value="400-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C3T100C7N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C3T100C7N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CLK0" pad="10"/>
<connect gate="A" pin="CLK2" pad="66"/>
<connect gate="A" pin="CONF_DONE" pad="60"/>
<connect gate="A" pin="DATA0" pad="7"/>
<connect gate="A" pin="DCLK" pad="16"/>
<connect gate="A" pin="GND" pad="96"/>
<connect gate="A" pin="GNDA_PLL1" pad="11"/>
<connect gate="A" pin="GND_10" pad="45"/>
<connect gate="A" pin="GND_2" pad="43"/>
<connect gate="A" pin="GND_3" pad="58"/>
<connect gate="A" pin="GND_4" pad="81"/>
<connect gate="A" pin="GND_5" pad="83"/>
<connect gate="A" pin="GND_6" pad="19"/>
<connect gate="A" pin="GND_7" pad="32"/>
<connect gate="A" pin="GND_8" pad="30"/>
<connect gate="A" pin="GND_9" pad="94"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO_10" pad="21"/>
<connect gate="A" pin="IO_11" pad="22"/>
<connect gate="A" pin="IO_12" pad="23"/>
<connect gate="A" pin="IO_13" pad="24"/>
<connect gate="A" pin="IO_14" pad="25"/>
<connect gate="A" pin="IO_15" pad="26"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="29"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="54"/>
<connect gate="A" pin="IO_36" pad="55"/>
<connect gate="A" pin="IO_37" pad="56"/>
<connect gate="A" pin="IO_38" pad="57"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="68"/>
<connect gate="A" pin="IO_41" pad="69"/>
<connect gate="A" pin="IO_42" pad="70"/>
<connect gate="A" pin="IO_43" pad="71"/>
<connect gate="A" pin="IO_44" pad="72"/>
<connect gate="A" pin="IO_45" pad="73"/>
<connect gate="A" pin="IO_46" pad="74"/>
<connect gate="A" pin="IO_47" pad="75"/>
<connect gate="A" pin="IO_48" pad="76"/>
<connect gate="A" pin="IO_49" pad="77"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="78"/>
<connect gate="A" pin="IO_51" pad="79"/>
<connect gate="A" pin="IO_52" pad="84"/>
<connect gate="A" pin="IO_53" pad="85"/>
<connect gate="A" pin="IO_54" pad="86"/>
<connect gate="A" pin="IO_55" pad="87"/>
<connect gate="A" pin="IO_56" pad="88"/>
<connect gate="A" pin="IO_57" pad="89"/>
<connect gate="A" pin="IO_58" pad="90"/>
<connect gate="A" pin="IO_59" pad="91"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_60" pad="92"/>
<connect gate="A" pin="IO_61" pad="97"/>
<connect gate="A" pin="IO_62" pad="98"/>
<connect gate="A" pin="IO_63" pad="99"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="17"/>
<connect gate="A" pin="IO_9" pad="20"/>
<connect gate="A" pin="MSEL0" pad="14"/>
<connect gate="A" pin="MSEL1" pad="15"/>
<connect gate="A" pin="NCE" pad="13"/>
<connect gate="A" pin="NCEO" pad="12"/>
<connect gate="A" pin="NCONFIG" pad="8"/>
<connect gate="A" pin="NSTATUS" pad="61"/>
<connect gate="A" pin="TCK" pad="62"/>
<connect gate="A" pin="TDI" pad="67"/>
<connect gate="A" pin="TDO" pad="64"/>
<connect gate="A" pin="TMS" pad="63"/>
<connect gate="A" pin="VCCA_PLL1" pad="9"/>
<connect gate="A" pin="VCCINT" pad="44"/>
<connect gate="A" pin="VCCINT_2" pad="82"/>
<connect gate="A" pin="VCCINT_3" pad="93"/>
<connect gate="A" pin="VCCINT_4" pad="33"/>
<connect gate="A" pin="VCCIO1" pad="18"/>
<connect gate="A" pin="VCCIO2" pad="95"/>
<connect gate="A" pin="VCCIO2_2" pad="80"/>
<connect gate="A" pin="VCCIO3" pad="59"/>
<connect gate="A" pin="VCCIO4" pad="31"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C3T100C7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0045"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C3T100C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C3T100C8N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CLK0" pad="10"/>
<connect gate="A" pin="CLK2" pad="66"/>
<connect gate="A" pin="CONF_DONE" pad="60"/>
<connect gate="A" pin="DATA0" pad="7"/>
<connect gate="A" pin="DCLK" pad="16"/>
<connect gate="A" pin="GND" pad="96"/>
<connect gate="A" pin="GNDA_PLL1" pad="11"/>
<connect gate="A" pin="GND_10" pad="45"/>
<connect gate="A" pin="GND_2" pad="43"/>
<connect gate="A" pin="GND_3" pad="58"/>
<connect gate="A" pin="GND_4" pad="81"/>
<connect gate="A" pin="GND_5" pad="83"/>
<connect gate="A" pin="GND_6" pad="19"/>
<connect gate="A" pin="GND_7" pad="32"/>
<connect gate="A" pin="GND_8" pad="30"/>
<connect gate="A" pin="GND_9" pad="94"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO_10" pad="21"/>
<connect gate="A" pin="IO_11" pad="22"/>
<connect gate="A" pin="IO_12" pad="23"/>
<connect gate="A" pin="IO_13" pad="24"/>
<connect gate="A" pin="IO_14" pad="25"/>
<connect gate="A" pin="IO_15" pad="26"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="29"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="54"/>
<connect gate="A" pin="IO_36" pad="55"/>
<connect gate="A" pin="IO_37" pad="56"/>
<connect gate="A" pin="IO_38" pad="57"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="68"/>
<connect gate="A" pin="IO_41" pad="69"/>
<connect gate="A" pin="IO_42" pad="70"/>
<connect gate="A" pin="IO_43" pad="71"/>
<connect gate="A" pin="IO_44" pad="72"/>
<connect gate="A" pin="IO_45" pad="73"/>
<connect gate="A" pin="IO_46" pad="74"/>
<connect gate="A" pin="IO_47" pad="75"/>
<connect gate="A" pin="IO_48" pad="76"/>
<connect gate="A" pin="IO_49" pad="77"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="78"/>
<connect gate="A" pin="IO_51" pad="79"/>
<connect gate="A" pin="IO_52" pad="84"/>
<connect gate="A" pin="IO_53" pad="85"/>
<connect gate="A" pin="IO_54" pad="86"/>
<connect gate="A" pin="IO_55" pad="87"/>
<connect gate="A" pin="IO_56" pad="88"/>
<connect gate="A" pin="IO_57" pad="89"/>
<connect gate="A" pin="IO_58" pad="90"/>
<connect gate="A" pin="IO_59" pad="91"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_60" pad="92"/>
<connect gate="A" pin="IO_61" pad="97"/>
<connect gate="A" pin="IO_62" pad="98"/>
<connect gate="A" pin="IO_63" pad="99"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="17"/>
<connect gate="A" pin="IO_9" pad="20"/>
<connect gate="A" pin="MSEL0" pad="14"/>
<connect gate="A" pin="MSEL1" pad="15"/>
<connect gate="A" pin="NCE" pad="13"/>
<connect gate="A" pin="NCEO" pad="12"/>
<connect gate="A" pin="NCONFIG" pad="8"/>
<connect gate="A" pin="NSTATUS" pad="61"/>
<connect gate="A" pin="TCK" pad="62"/>
<connect gate="A" pin="TDI" pad="67"/>
<connect gate="A" pin="TDO" pad="64"/>
<connect gate="A" pin="TMS" pad="63"/>
<connect gate="A" pin="VCCA_PLL1" pad="9"/>
<connect gate="A" pin="VCCINT" pad="44"/>
<connect gate="A" pin="VCCINT_2" pad="82"/>
<connect gate="A" pin="VCCINT_3" pad="93"/>
<connect gate="A" pin="VCCINT_4" pad="33"/>
<connect gate="A" pin="VCCIO1" pad="18"/>
<connect gate="A" pin="VCCIO2" pad="95"/>
<connect gate="A" pin="VCCIO2_2" pad="80"/>
<connect gate="A" pin="VCCIO3" pad="59"/>
<connect gate="A" pin="VCCIO4" pad="31"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C3T100C8N"/>
<attribute name="OC_FARNELL" value="1662267"/>
<attribute name="OC_NEWARK" value="51R0543"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C3T100I7N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C3T100I7N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CLK0" pad="10"/>
<connect gate="A" pin="CLK2" pad="66"/>
<connect gate="A" pin="CONF_DONE" pad="60"/>
<connect gate="A" pin="DATA0" pad="7"/>
<connect gate="A" pin="DCLK" pad="16"/>
<connect gate="A" pin="GND" pad="96"/>
<connect gate="A" pin="GNDA_PLL1" pad="11"/>
<connect gate="A" pin="GND_10" pad="45"/>
<connect gate="A" pin="GND_2" pad="43"/>
<connect gate="A" pin="GND_3" pad="58"/>
<connect gate="A" pin="GND_4" pad="81"/>
<connect gate="A" pin="GND_5" pad="83"/>
<connect gate="A" pin="GND_6" pad="19"/>
<connect gate="A" pin="GND_7" pad="32"/>
<connect gate="A" pin="GND_8" pad="30"/>
<connect gate="A" pin="GND_9" pad="94"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO_10" pad="21"/>
<connect gate="A" pin="IO_11" pad="22"/>
<connect gate="A" pin="IO_12" pad="23"/>
<connect gate="A" pin="IO_13" pad="24"/>
<connect gate="A" pin="IO_14" pad="25"/>
<connect gate="A" pin="IO_15" pad="26"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="29"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="54"/>
<connect gate="A" pin="IO_36" pad="55"/>
<connect gate="A" pin="IO_37" pad="56"/>
<connect gate="A" pin="IO_38" pad="57"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="68"/>
<connect gate="A" pin="IO_41" pad="69"/>
<connect gate="A" pin="IO_42" pad="70"/>
<connect gate="A" pin="IO_43" pad="71"/>
<connect gate="A" pin="IO_44" pad="72"/>
<connect gate="A" pin="IO_45" pad="73"/>
<connect gate="A" pin="IO_46" pad="74"/>
<connect gate="A" pin="IO_47" pad="75"/>
<connect gate="A" pin="IO_48" pad="76"/>
<connect gate="A" pin="IO_49" pad="77"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="78"/>
<connect gate="A" pin="IO_51" pad="79"/>
<connect gate="A" pin="IO_52" pad="84"/>
<connect gate="A" pin="IO_53" pad="85"/>
<connect gate="A" pin="IO_54" pad="86"/>
<connect gate="A" pin="IO_55" pad="87"/>
<connect gate="A" pin="IO_56" pad="88"/>
<connect gate="A" pin="IO_57" pad="89"/>
<connect gate="A" pin="IO_58" pad="90"/>
<connect gate="A" pin="IO_59" pad="91"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_60" pad="92"/>
<connect gate="A" pin="IO_61" pad="97"/>
<connect gate="A" pin="IO_62" pad="98"/>
<connect gate="A" pin="IO_63" pad="99"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="17"/>
<connect gate="A" pin="IO_9" pad="20"/>
<connect gate="A" pin="MSEL0" pad="14"/>
<connect gate="A" pin="MSEL1" pad="15"/>
<connect gate="A" pin="NCE" pad="13"/>
<connect gate="A" pin="NCEO" pad="12"/>
<connect gate="A" pin="NCONFIG" pad="8"/>
<connect gate="A" pin="NSTATUS" pad="61"/>
<connect gate="A" pin="TCK" pad="62"/>
<connect gate="A" pin="TDI" pad="67"/>
<connect gate="A" pin="TDO" pad="64"/>
<connect gate="A" pin="TMS" pad="63"/>
<connect gate="A" pin="VCCA_PLL1" pad="9"/>
<connect gate="A" pin="VCCINT" pad="44"/>
<connect gate="A" pin="VCCINT_2" pad="82"/>
<connect gate="A" pin="VCCINT_3" pad="93"/>
<connect gate="A" pin="VCCINT_4" pad="33"/>
<connect gate="A" pin="VCCIO1" pad="18"/>
<connect gate="A" pin="VCCIO2" pad="95"/>
<connect gate="A" pin="VCCIO2_2" pad="80"/>
<connect gate="A" pin="VCCIO3" pad="59"/>
<connect gate="A" pin="VCCIO4" pad="31"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C3T100I7N"/>
<attribute name="OC_FARNELL" value="1453494"/>
<attribute name="OC_NEWARK" value="52R0048"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C3T144C7">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C3T144C7_A"/>
<gate name="B" symbol="EP1C3T144C7_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLK0" pad="16"/>
<connect gate="A" pin="CLK1" pad="17"/>
<connect gate="A" pin="DATA0" pad="13"/>
<connect gate="A" pin="DCLK" pad="24"/>
<connect gate="A" pin="GND" pad="63"/>
<connect gate="A" pin="GNDA_PLL1" pad="18"/>
<connect gate="A" pin="GNDG_PLL1" pad="19"/>
<connect gate="A" pin="GND_2" pad="30"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="43"/>
<connect gate="A" pin="GND_5" pad="45"/>
<connect gate="A" pin="GND_6" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="25"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="27"/>
<connect gate="A" pin="IO_15" pad="28"/>
<connect gate="A" pin="IO_16" pad="31"/>
<connect gate="A" pin="IO_17" pad="32"/>
<connect gate="A" pin="IO_18" pad="33"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="54"/>
<connect gate="A" pin="IO_36" pad="55"/>
<connect gate="A" pin="IO_37" pad="56"/>
<connect gate="A" pin="IO_38" pad="57"/>
<connect gate="A" pin="IO_39" pad="58"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="59"/>
<connect gate="A" pin="IO_41" pad="60"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="62"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="MSEL0" pad="22"/>
<connect gate="A" pin="MSEL1" pad="23"/>
<connect gate="A" pin="NCE" pad="21"/>
<connect gate="A" pin="NCEO" pad="20"/>
<connect gate="A" pin="NCONFIG" pad="14"/>
<connect gate="A" pin="VCCA_PLL1" pad="15"/>
<connect gate="A" pin="VCCINT" pad="64"/>
<connect gate="A" pin="VCCINT_2" pad="46"/>
<connect gate="A" pin="VCCIO1" pad="29"/>
<connect gate="A" pin="VCCIO1_2" pad="8"/>
<connect gate="A" pin="VCCIO4" pad="66"/>
<connect gate="A" pin="VCCIO4_2" pad="44"/>
<connect gate="B" pin="CLK2" pad="93"/>
<connect gate="B" pin="CLK3" pad="92"/>
<connect gate="B" pin="CONF_DONE" pad="86"/>
<connect gate="B" pin="GND" pad="138"/>
<connect gate="B" pin="GND_2" pad="80"/>
<connect gate="B" pin="GND_3" pad="116"/>
<connect gate="B" pin="GND_4" pad="101"/>
<connect gate="B" pin="GND_5" pad="118"/>
<connect gate="B" pin="GND_6" pad="136"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="83"/>
<connect gate="B" pin="IO_11" pad="84"/>
<connect gate="B" pin="IO_12" pad="85"/>
<connect gate="B" pin="IO_13" pad="91"/>
<connect gate="B" pin="IO_14" pad="94"/>
<connect gate="B" pin="IO_15" pad="96"/>
<connect gate="B" pin="IO_16" pad="97"/>
<connect gate="B" pin="IO_17" pad="98"/>
<connect gate="B" pin="IO_18" pad="99"/>
<connect gate="B" pin="IO_19" pad="100"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="103"/>
<connect gate="B" pin="IO_21" pad="104"/>
<connect gate="B" pin="IO_22" pad="105"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="108"/>
<connect gate="B" pin="IO_26" pad="109"/>
<connect gate="B" pin="IO_27" pad="110"/>
<connect gate="B" pin="IO_28" pad="111"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="114"/>
<connect gate="B" pin="IO_32" pad="119"/>
<connect gate="B" pin="IO_33" pad="120"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="122"/>
<connect gate="B" pin="IO_36" pad="123"/>
<connect gate="B" pin="IO_37" pad="124"/>
<connect gate="B" pin="IO_38" pad="125"/>
<connect gate="B" pin="IO_39" pad="126"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="129"/>
<connect gate="B" pin="IO_43" pad="130"/>
<connect gate="B" pin="IO_44" pad="131"/>
<connect gate="B" pin="IO_45" pad="132"/>
<connect gate="B" pin="IO_46" pad="133"/>
<connect gate="B" pin="IO_47" pad="134"/>
<connect gate="B" pin="IO_48" pad="139"/>
<connect gate="B" pin="IO_49" pad="140"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="141"/>
<connect gate="B" pin="IO_51" pad="142"/>
<connect gate="B" pin="IO_52" pad="143"/>
<connect gate="B" pin="IO_6" pad="77"/>
<connect gate="B" pin="IO_7" pad="78"/>
<connect gate="B" pin="IO_8" pad="79"/>
<connect gate="B" pin="IO_9" pad="82"/>
<connect gate="B" pin="NSTATUS" pad="87"/>
<connect gate="B" pin="TCK" pad="88"/>
<connect gate="B" pin="TDI" pad="95"/>
<connect gate="B" pin="TDO" pad="90"/>
<connect gate="B" pin="TMS" pad="89"/>
<connect gate="B" pin="VCCINT" pad="117"/>
<connect gate="B" pin="VCCINT_2" pad="135"/>
<connect gate="B" pin="VCCIO2" pad="137"/>
<connect gate="B" pin="VCCIO2_2" pad="115"/>
<connect gate="B" pin="VCCIO3" pad="102"/>
<connect gate="B" pin="VCCIO3_2" pad="81"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C3T144C7"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0052"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C3T144C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C3T144C8N_A"/>
<gate name="B" symbol="EP1C3T144C8N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLK0" pad="16"/>
<connect gate="A" pin="CLK1" pad="17"/>
<connect gate="A" pin="DATA0" pad="13"/>
<connect gate="A" pin="DCLK" pad="24"/>
<connect gate="A" pin="GND" pad="63"/>
<connect gate="A" pin="GNDA_PLL1" pad="18"/>
<connect gate="A" pin="GNDG_PLL1" pad="19"/>
<connect gate="A" pin="GND_2" pad="30"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="43"/>
<connect gate="A" pin="GND_5" pad="45"/>
<connect gate="A" pin="GND_6" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="25"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="27"/>
<connect gate="A" pin="IO_15" pad="28"/>
<connect gate="A" pin="IO_16" pad="31"/>
<connect gate="A" pin="IO_17" pad="32"/>
<connect gate="A" pin="IO_18" pad="33"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="54"/>
<connect gate="A" pin="IO_36" pad="55"/>
<connect gate="A" pin="IO_37" pad="56"/>
<connect gate="A" pin="IO_38" pad="57"/>
<connect gate="A" pin="IO_39" pad="58"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="59"/>
<connect gate="A" pin="IO_41" pad="60"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="62"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="MSEL0" pad="22"/>
<connect gate="A" pin="MSEL1" pad="23"/>
<connect gate="A" pin="NCE" pad="21"/>
<connect gate="A" pin="NCEO" pad="20"/>
<connect gate="A" pin="NCONFIG" pad="14"/>
<connect gate="A" pin="VCCA_PLL1" pad="15"/>
<connect gate="A" pin="VCCINT" pad="64"/>
<connect gate="A" pin="VCCINT_2" pad="46"/>
<connect gate="A" pin="VCCIO1" pad="29"/>
<connect gate="A" pin="VCCIO1_2" pad="8"/>
<connect gate="A" pin="VCCIO4" pad="66"/>
<connect gate="A" pin="VCCIO4_2" pad="44"/>
<connect gate="B" pin="CLK2" pad="93"/>
<connect gate="B" pin="CLK3" pad="92"/>
<connect gate="B" pin="CONF_DONE" pad="86"/>
<connect gate="B" pin="GND" pad="138"/>
<connect gate="B" pin="GND_2" pad="80"/>
<connect gate="B" pin="GND_3" pad="116"/>
<connect gate="B" pin="GND_4" pad="101"/>
<connect gate="B" pin="GND_5" pad="118"/>
<connect gate="B" pin="GND_6" pad="136"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="83"/>
<connect gate="B" pin="IO_11" pad="84"/>
<connect gate="B" pin="IO_12" pad="85"/>
<connect gate="B" pin="IO_13" pad="91"/>
<connect gate="B" pin="IO_14" pad="94"/>
<connect gate="B" pin="IO_15" pad="96"/>
<connect gate="B" pin="IO_16" pad="97"/>
<connect gate="B" pin="IO_17" pad="98"/>
<connect gate="B" pin="IO_18" pad="99"/>
<connect gate="B" pin="IO_19" pad="100"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="103"/>
<connect gate="B" pin="IO_21" pad="104"/>
<connect gate="B" pin="IO_22" pad="105"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="108"/>
<connect gate="B" pin="IO_26" pad="109"/>
<connect gate="B" pin="IO_27" pad="110"/>
<connect gate="B" pin="IO_28" pad="111"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="114"/>
<connect gate="B" pin="IO_32" pad="119"/>
<connect gate="B" pin="IO_33" pad="120"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="122"/>
<connect gate="B" pin="IO_36" pad="123"/>
<connect gate="B" pin="IO_37" pad="124"/>
<connect gate="B" pin="IO_38" pad="125"/>
<connect gate="B" pin="IO_39" pad="126"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="129"/>
<connect gate="B" pin="IO_43" pad="130"/>
<connect gate="B" pin="IO_44" pad="131"/>
<connect gate="B" pin="IO_45" pad="132"/>
<connect gate="B" pin="IO_46" pad="133"/>
<connect gate="B" pin="IO_47" pad="134"/>
<connect gate="B" pin="IO_48" pad="139"/>
<connect gate="B" pin="IO_49" pad="140"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="141"/>
<connect gate="B" pin="IO_51" pad="142"/>
<connect gate="B" pin="IO_52" pad="143"/>
<connect gate="B" pin="IO_6" pad="77"/>
<connect gate="B" pin="IO_7" pad="78"/>
<connect gate="B" pin="IO_8" pad="79"/>
<connect gate="B" pin="IO_9" pad="82"/>
<connect gate="B" pin="NSTATUS" pad="87"/>
<connect gate="B" pin="TCK" pad="88"/>
<connect gate="B" pin="TDI" pad="95"/>
<connect gate="B" pin="TDO" pad="90"/>
<connect gate="B" pin="TMS" pad="89"/>
<connect gate="B" pin="VCCINT" pad="117"/>
<connect gate="B" pin="VCCINT_2" pad="135"/>
<connect gate="B" pin="VCCIO2" pad="137"/>
<connect gate="B" pin="VCCIO2_2" pad="115"/>
<connect gate="B" pin="VCCIO3" pad="102"/>
<connect gate="B" pin="VCCIO3_2" pad="81"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C3T144C8N"/>
<attribute name="OC_FARNELL" value="1662265"/>
<attribute name="OC_NEWARK" value="51R0544"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C3T144I7N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C3T144I7N_A"/>
<gate name="B" symbol="EP1C3T144I7N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLK0" pad="16"/>
<connect gate="A" pin="CLK1" pad="17"/>
<connect gate="A" pin="DATA0" pad="13"/>
<connect gate="A" pin="DCLK" pad="24"/>
<connect gate="A" pin="GND" pad="63"/>
<connect gate="A" pin="GNDA_PLL1" pad="18"/>
<connect gate="A" pin="GNDG_PLL1" pad="19"/>
<connect gate="A" pin="GND_2" pad="30"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="43"/>
<connect gate="A" pin="GND_5" pad="45"/>
<connect gate="A" pin="GND_6" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="25"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="27"/>
<connect gate="A" pin="IO_15" pad="28"/>
<connect gate="A" pin="IO_16" pad="31"/>
<connect gate="A" pin="IO_17" pad="32"/>
<connect gate="A" pin="IO_18" pad="33"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="54"/>
<connect gate="A" pin="IO_36" pad="55"/>
<connect gate="A" pin="IO_37" pad="56"/>
<connect gate="A" pin="IO_38" pad="57"/>
<connect gate="A" pin="IO_39" pad="58"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="59"/>
<connect gate="A" pin="IO_41" pad="60"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="62"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="MSEL0" pad="22"/>
<connect gate="A" pin="MSEL1" pad="23"/>
<connect gate="A" pin="NCE" pad="21"/>
<connect gate="A" pin="NCEO" pad="20"/>
<connect gate="A" pin="NCONFIG" pad="14"/>
<connect gate="A" pin="VCCA_PLL1" pad="15"/>
<connect gate="A" pin="VCCINT" pad="64"/>
<connect gate="A" pin="VCCINT_2" pad="46"/>
<connect gate="A" pin="VCCIO1" pad="29"/>
<connect gate="A" pin="VCCIO1_2" pad="8"/>
<connect gate="A" pin="VCCIO4" pad="66"/>
<connect gate="A" pin="VCCIO4_2" pad="44"/>
<connect gate="B" pin="CLK2" pad="93"/>
<connect gate="B" pin="CLK3" pad="92"/>
<connect gate="B" pin="CONF_DONE" pad="86"/>
<connect gate="B" pin="GND" pad="138"/>
<connect gate="B" pin="GND_2" pad="80"/>
<connect gate="B" pin="GND_3" pad="116"/>
<connect gate="B" pin="GND_4" pad="101"/>
<connect gate="B" pin="GND_5" pad="118"/>
<connect gate="B" pin="GND_6" pad="136"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="83"/>
<connect gate="B" pin="IO_11" pad="84"/>
<connect gate="B" pin="IO_12" pad="85"/>
<connect gate="B" pin="IO_13" pad="91"/>
<connect gate="B" pin="IO_14" pad="94"/>
<connect gate="B" pin="IO_15" pad="96"/>
<connect gate="B" pin="IO_16" pad="97"/>
<connect gate="B" pin="IO_17" pad="98"/>
<connect gate="B" pin="IO_18" pad="99"/>
<connect gate="B" pin="IO_19" pad="100"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="103"/>
<connect gate="B" pin="IO_21" pad="104"/>
<connect gate="B" pin="IO_22" pad="105"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="108"/>
<connect gate="B" pin="IO_26" pad="109"/>
<connect gate="B" pin="IO_27" pad="110"/>
<connect gate="B" pin="IO_28" pad="111"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="114"/>
<connect gate="B" pin="IO_32" pad="119"/>
<connect gate="B" pin="IO_33" pad="120"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="122"/>
<connect gate="B" pin="IO_36" pad="123"/>
<connect gate="B" pin="IO_37" pad="124"/>
<connect gate="B" pin="IO_38" pad="125"/>
<connect gate="B" pin="IO_39" pad="126"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="129"/>
<connect gate="B" pin="IO_43" pad="130"/>
<connect gate="B" pin="IO_44" pad="131"/>
<connect gate="B" pin="IO_45" pad="132"/>
<connect gate="B" pin="IO_46" pad="133"/>
<connect gate="B" pin="IO_47" pad="134"/>
<connect gate="B" pin="IO_48" pad="139"/>
<connect gate="B" pin="IO_49" pad="140"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="141"/>
<connect gate="B" pin="IO_51" pad="142"/>
<connect gate="B" pin="IO_52" pad="143"/>
<connect gate="B" pin="IO_6" pad="77"/>
<connect gate="B" pin="IO_7" pad="78"/>
<connect gate="B" pin="IO_8" pad="79"/>
<connect gate="B" pin="IO_9" pad="82"/>
<connect gate="B" pin="NSTATUS" pad="87"/>
<connect gate="B" pin="TCK" pad="88"/>
<connect gate="B" pin="TDI" pad="95"/>
<connect gate="B" pin="TDO" pad="90"/>
<connect gate="B" pin="TMS" pad="89"/>
<connect gate="B" pin="VCCINT" pad="117"/>
<connect gate="B" pin="VCCINT_2" pad="135"/>
<connect gate="B" pin="VCCIO2" pad="137"/>
<connect gate="B" pin="VCCIO2_2" pad="115"/>
<connect gate="B" pin="VCCIO3" pad="102"/>
<connect gate="B" pin="VCCIO3_2" pad="81"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C3T144I7N"/>
<attribute name="OC_FARNELL" value="1453485"/>
<attribute name="OC_NEWARK" value="52R0056"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C4F324C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C4F324C8N_A"/>
<gate name="B" symbol="EP1C4F324C8N_B"/>
<gate name="C" symbol="EP1C4F324C8N_C"/>
<gate name="D" symbol="EP1C4F324C8N_D"/>
</gates>
<devices>
<device name="" package="BGA324C18X18X100P_1900X1900X22">
<connects>
<connect gate="A" pin="CLK0" pad="J3"/>
<connect gate="A" pin="CLK1" pad="J4"/>
<connect gate="A" pin="DATA0" pad="H7"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="GNDG_PLL1" pad="J6"/>
<connect gate="A" pin="GND_2" pad="J8"/>
<connect gate="A" pin="GND_3" pad="H8"/>
<connect gate="A" pin="GND_4" pad="C1"/>
<connect gate="A" pin="GND_5" pad="H9"/>
<connect gate="A" pin="GND_6" pad="A1"/>
<connect gate="A" pin="GND_7" pad="B2"/>
<connect gate="A" pin="IO" pad="E4"/>
<connect gate="A" pin="IO_10" pad="F4"/>
<connect gate="A" pin="IO_11" pad="F5"/>
<connect gate="A" pin="IO_12" pad="A6"/>
<connect gate="A" pin="IO_13" pad="F6"/>
<connect gate="A" pin="IO_14" pad="A7"/>
<connect gate="A" pin="IO_15" pad="F7"/>
<connect gate="A" pin="IO_16" pad="A8"/>
<connect gate="A" pin="IO_17" pad="F8"/>
<connect gate="A" pin="IO_18" pad="A9"/>
<connect gate="A" pin="IO_19" pad="F9"/>
<connect gate="A" pin="IO_2" pad="E5"/>
<connect gate="A" pin="IO_20" pad="G1"/>
<connect gate="A" pin="IO_21" pad="G2"/>
<connect gate="A" pin="IO_22" pad="B3"/>
<connect gate="A" pin="IO_23" pad="G3"/>
<connect gate="A" pin="IO_24" pad="B4"/>
<connect gate="A" pin="IO_25" pad="G4"/>
<connect gate="A" pin="IO_26" pad="B5"/>
<connect gate="A" pin="IO_27" pad="G5"/>
<connect gate="A" pin="IO_28" pad="B6"/>
<connect gate="A" pin="IO_29" pad="G6"/>
<connect gate="A" pin="IO_3" pad="E6"/>
<connect gate="A" pin="IO_30" pad="B7"/>
<connect gate="A" pin="IO_31" pad="G8"/>
<connect gate="A" pin="IO_32" pad="B8"/>
<connect gate="A" pin="IO_33" pad="G9"/>
<connect gate="A" pin="IO_34" pad="B9"/>
<connect gate="A" pin="IO_35" pad="H1"/>
<connect gate="A" pin="IO_36" pad="H2"/>
<connect gate="A" pin="IO_37" pad="C2"/>
<connect gate="A" pin="IO_38" pad="H3"/>
<connect gate="A" pin="IO_39" pad="C3"/>
<connect gate="A" pin="IO_4" pad="E7"/>
<connect gate="A" pin="IO_40" pad="H4"/>
<connect gate="A" pin="IO_41" pad="C4"/>
<connect gate="A" pin="IO_42" pad="H5"/>
<connect gate="A" pin="IO_43" pad="C5"/>
<connect gate="A" pin="IO_44" pad="H6"/>
<connect gate="A" pin="IO_45" pad="C6"/>
<connect gate="A" pin="IO_46" pad="J1"/>
<connect gate="A" pin="IO_47" pad="C7"/>
<connect gate="A" pin="IO_48" pad="C8"/>
<connect gate="A" pin="IO_49" pad="C9"/>
<connect gate="A" pin="IO_5" pad="E8"/>
<connect gate="A" pin="IO_50" pad="D1"/>
<connect gate="A" pin="IO_51" pad="D2"/>
<connect gate="A" pin="IO_52" pad="D3"/>
<connect gate="A" pin="IO_53" pad="D4"/>
<connect gate="A" pin="IO_54" pad="D5"/>
<connect gate="A" pin="IO_55" pad="D6"/>
<connect gate="A" pin="IO_56" pad="D7"/>
<connect gate="A" pin="IO_57" pad="D8"/>
<connect gate="A" pin="IO_58" pad="D9"/>
<connect gate="A" pin="IO_59" pad="E2"/>
<connect gate="A" pin="IO_6" pad="F1"/>
<connect gate="A" pin="IO_60" pad="E3"/>
<connect gate="A" pin="IO_7" pad="F2"/>
<connect gate="A" pin="IO_8" pad="F3"/>
<connect gate="A" pin="IO_9" pad="A4"/>
<connect gate="A" pin="NCE" pad="J7"/>
<connect gate="A" pin="NCONFIG" pad="J2"/>
<connect gate="A" pin="VCCA_PLL1" pad="J5"/>
<connect gate="A" pin="VCCINT" pad="A2"/>
<connect gate="A" pin="VCCINT_2" pad="B1"/>
<connect gate="A" pin="VCCINT_3" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="E1"/>
<connect gate="A" pin="VCCIO1_2" pad="G7"/>
<connect gate="A" pin="VCCIO2" pad="E9"/>
<connect gate="A" pin="VCCIO2_2" pad="A5"/>
<connect gate="B" pin="DCLK" pad="L1"/>
<connect gate="B" pin="GND" pad="V3"/>
<connect gate="B" pin="GNDA_PLL1" pad="K1"/>
<connect gate="B" pin="GND_2" pad="K8"/>
<connect gate="B" pin="GND_3" pad="T1"/>
<connect gate="B" pin="GND_4" pad="K9"/>
<connect gate="B" pin="GND_5" pad="U2"/>
<connect gate="B" pin="GND_6" pad="L8"/>
<connect gate="B" pin="GND_7" pad="V1"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO_10" pad="L7"/>
<connect gate="B" pin="IO_11" pad="M1"/>
<connect gate="B" pin="IO_12" pad="M2"/>
<connect gate="B" pin="IO_13" pad="M3"/>
<connect gate="B" pin="IO_14" pad="M4"/>
<connect gate="B" pin="IO_15" pad="M5"/>
<connect gate="B" pin="IO_16" pad="M6"/>
<connect gate="B" pin="IO_17" pad="M8"/>
<connect gate="B" pin="IO_18" pad="M9"/>
<connect gate="B" pin="IO_19" pad="N1"/>
<connect gate="B" pin="IO_2" pad="K4"/>
<connect gate="B" pin="IO_20" pad="N2"/>
<connect gate="B" pin="IO_21" pad="N3"/>
<connect gate="B" pin="IO_22" pad="N4"/>
<connect gate="B" pin="IO_23" pad="N5"/>
<connect gate="B" pin="IO_24" pad="N6"/>
<connect gate="B" pin="IO_25" pad="N7"/>
<connect gate="B" pin="IO_26" pad="N8"/>
<connect gate="B" pin="IO_27" pad="N9"/>
<connect gate="B" pin="IO_28" pad="P2"/>
<connect gate="B" pin="IO_29" pad="P3"/>
<connect gate="B" pin="IO_3" pad="K5"/>
<connect gate="B" pin="IO_30" pad="P4"/>
<connect gate="B" pin="IO_31" pad="P5"/>
<connect gate="B" pin="IO_32" pad="P6"/>
<connect gate="B" pin="IO_33" pad="P7"/>
<connect gate="B" pin="IO_34" pad="P9"/>
<connect gate="B" pin="IO_35" pad="R1"/>
<connect gate="B" pin="IO_36" pad="R2"/>
<connect gate="B" pin="IO_37" pad="R3"/>
<connect gate="B" pin="IO_38" pad="R4"/>
<connect gate="B" pin="IO_39" pad="R5"/>
<connect gate="B" pin="IO_4" pad="K6"/>
<connect gate="B" pin="IO_40" pad="R6"/>
<connect gate="B" pin="IO_41" pad="R7"/>
<connect gate="B" pin="IO_42" pad="R8"/>
<connect gate="B" pin="IO_43" pad="R9"/>
<connect gate="B" pin="IO_44" pad="T2"/>
<connect gate="B" pin="IO_45" pad="T3"/>
<connect gate="B" pin="IO_46" pad="T4"/>
<connect gate="B" pin="IO_47" pad="T5"/>
<connect gate="B" pin="IO_48" pad="T6"/>
<connect gate="B" pin="IO_49" pad="T7"/>
<connect gate="B" pin="IO_5" pad="L2"/>
<connect gate="B" pin="IO_50" pad="T8"/>
<connect gate="B" pin="IO_51" pad="T9"/>
<connect gate="B" pin="IO_52" pad="U3"/>
<connect gate="B" pin="IO_53" pad="U4"/>
<connect gate="B" pin="IO_54" pad="U5"/>
<connect gate="B" pin="IO_55" pad="U6"/>
<connect gate="B" pin="IO_56" pad="U7"/>
<connect gate="B" pin="IO_57" pad="U8"/>
<connect gate="B" pin="IO_58" pad="U9"/>
<connect gate="B" pin="IO_59" pad="V4"/>
<connect gate="B" pin="IO_6" pad="L3"/>
<connect gate="B" pin="IO_60" pad="V6"/>
<connect gate="B" pin="IO_61" pad="V7"/>
<connect gate="B" pin="IO_62" pad="V8"/>
<connect gate="B" pin="IO_7" pad="L4"/>
<connect gate="B" pin="IO_8" pad="L5"/>
<connect gate="B" pin="IO_9" pad="L6"/>
<connect gate="B" pin="MSEL0" pad="K3"/>
<connect gate="B" pin="MSEL1" pad="K7"/>
<connect gate="B" pin="NCEO" pad="K2"/>
<connect gate="B" pin="VCCINT" pad="L9"/>
<connect gate="B" pin="VCCINT_2" pad="U1"/>
<connect gate="B" pin="VCCINT_3" pad="V2"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO1_2" pad="M7"/>
<connect gate="B" pin="VCCIO4" pad="V5"/>
<connect gate="B" pin="VCCIO4_2" pad="P8"/>
<connect gate="C" pin="CLK2" pad="J15"/>
<connect gate="C" pin="CLK3" pad="J16"/>
<connect gate="C" pin="GND" pad="B17"/>
<connect gate="C" pin="GNDG_PLL2" pad="J18"/>
<connect gate="C" pin="GND_2" pad="J10"/>
<connect gate="C" pin="GND_3" pad="A16"/>
<connect gate="C" pin="GND_4" pad="J11"/>
<connect gate="C" pin="GND_5" pad="A18"/>
<connect gate="C" pin="GND_6" pad="C18"/>
<connect gate="C" pin="GND_7" pad="H11"/>
<connect gate="C" pin="IO" pad="J14"/>
<connect gate="C" pin="IO_10" pad="B13"/>
<connect gate="C" pin="IO_11" pad="B14"/>
<connect gate="C" pin="IO_12" pad="B15"/>
<connect gate="C" pin="IO_13" pad="B16"/>
<connect gate="C" pin="IO_14" pad="C10"/>
<connect gate="C" pin="IO_15" pad="C11"/>
<connect gate="C" pin="IO_16" pad="C12"/>
<connect gate="C" pin="IO_17" pad="C13"/>
<connect gate="C" pin="IO_18" pad="C14"/>
<connect gate="C" pin="IO_19" pad="C15"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C16"/>
<connect gate="C" pin="IO_21" pad="C17"/>
<connect gate="C" pin="IO_22" pad="D10"/>
<connect gate="C" pin="IO_23" pad="D11"/>
<connect gate="C" pin="IO_24" pad="D12"/>
<connect gate="C" pin="IO_25" pad="D13"/>
<connect gate="C" pin="IO_26" pad="D14"/>
<connect gate="C" pin="IO_27" pad="D15"/>
<connect gate="C" pin="IO_28" pad="D16"/>
<connect gate="C" pin="IO_29" pad="D17"/>
<connect gate="C" pin="IO_3" pad="A11"/>
<connect gate="C" pin="IO_30" pad="D18"/>
<connect gate="C" pin="IO_31" pad="E10"/>
<connect gate="C" pin="IO_32" pad="E11"/>
<connect gate="C" pin="IO_33" pad="E13"/>
<connect gate="C" pin="IO_34" pad="E14"/>
<connect gate="C" pin="IO_35" pad="E15"/>
<connect gate="C" pin="IO_36" pad="E16"/>
<connect gate="C" pin="IO_37" pad="E17"/>
<connect gate="C" pin="IO_38" pad="F10"/>
<connect gate="C" pin="IO_39" pad="F11"/>
<connect gate="C" pin="IO_4" pad="A12"/>
<connect gate="C" pin="IO_40" pad="F12"/>
<connect gate="C" pin="IO_41" pad="F13"/>
<connect gate="C" pin="IO_42" pad="F14"/>
<connect gate="C" pin="IO_43" pad="F15"/>
<connect gate="C" pin="IO_44" pad="F16"/>
<connect gate="C" pin="IO_45" pad="F17"/>
<connect gate="C" pin="IO_46" pad="F18"/>
<connect gate="C" pin="IO_47" pad="G10"/>
<connect gate="C" pin="IO_48" pad="G11"/>
<connect gate="C" pin="IO_49" pad="G12"/>
<connect gate="C" pin="IO_5" pad="A13"/>
<connect gate="C" pin="IO_50" pad="G13"/>
<connect gate="C" pin="IO_51" pad="G14"/>
<connect gate="C" pin="IO_52" pad="G15"/>
<connect gate="C" pin="IO_53" pad="G16"/>
<connect gate="C" pin="IO_54" pad="G17"/>
<connect gate="C" pin="IO_55" pad="G18"/>
<connect gate="C" pin="IO_56" pad="H13"/>
<connect gate="C" pin="IO_57" pad="H14"/>
<connect gate="C" pin="IO_58" pad="H15"/>
<connect gate="C" pin="IO_59" pad="H16"/>
<connect gate="C" pin="IO_6" pad="A15"/>
<connect gate="C" pin="IO_60" pad="H17"/>
<connect gate="C" pin="IO_61" pad="H18"/>
<connect gate="C" pin="IO_62" pad="J13"/>
<connect gate="C" pin="IO_7" pad="B10"/>
<connect gate="C" pin="IO_8" pad="B11"/>
<connect gate="C" pin="IO_9" pad="B12"/>
<connect gate="C" pin="TDI" pad="J17"/>
<connect gate="C" pin="VCCA_PLL2" pad="J12"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCINT_2" pad="B18"/>
<connect gate="C" pin="VCCINT_3" pad="A17"/>
<connect gate="C" pin="VCCIO2" pad="E12"/>
<connect gate="C" pin="VCCIO2_2" pad="A14"/>
<connect gate="C" pin="VCCIO3" pad="H12"/>
<connect gate="C" pin="VCCIO3_2" pad="E18"/>
<connect gate="D" pin="CONF_DONE" pad="K17"/>
<connect gate="D" pin="GND" pad="U17"/>
<connect gate="D" pin="GNDA_PLL2" pad="K12"/>
<connect gate="D" pin="GND_2" pad="T18"/>
<connect gate="D" pin="GND_3" pad="L10"/>
<connect gate="D" pin="GND_4" pad="V18"/>
<connect gate="D" pin="GND_5" pad="K11"/>
<connect gate="D" pin="GND_6" pad="L11"/>
<connect gate="D" pin="GND_7" pad="V16"/>
<connect gate="D" pin="IO" pad="V15"/>
<connect gate="D" pin="IO/LVDS104P" pad="T13"/>
<connect gate="D" pin="IO/LVDS105N/DQ0B4" pad="U13"/>
<connect gate="D" pin="IO/LVDS105P/DQ0B5" pad="V13"/>
<connect gate="D" pin="IO/LVDS106N/DQ0B6" pad="R12"/>
<connect gate="D" pin="IO/LVDS106P/DQ0B7" pad="T12"/>
<connect gate="D" pin="IO/LVDS107N" pad="U12"/>
<connect gate="D" pin="IO_10" pad="M10"/>
<connect gate="D" pin="IO_11" pad="M11"/>
<connect gate="D" pin="IO_12" pad="M13"/>
<connect gate="D" pin="IO_13" pad="M14"/>
<connect gate="D" pin="IO_14" pad="M15"/>
<connect gate="D" pin="IO_15" pad="M16"/>
<connect gate="D" pin="IO_16" pad="M17"/>
<connect gate="D" pin="IO_17" pad="M18"/>
<connect gate="D" pin="IO_18" pad="N10"/>
<connect gate="D" pin="IO_19" pad="N11"/>
<connect gate="D" pin="IO_2" pad="K15"/>
<connect gate="D" pin="IO_20" pad="N12"/>
<connect gate="D" pin="IO_21" pad="N13"/>
<connect gate="D" pin="IO_22" pad="N14"/>
<connect gate="D" pin="IO_23" pad="N15"/>
<connect gate="D" pin="IO_24" pad="N16"/>
<connect gate="D" pin="IO_25" pad="N17"/>
<connect gate="D" pin="IO_26" pad="N18"/>
<connect gate="D" pin="IO_27" pad="P10"/>
<connect gate="D" pin="IO_28" pad="P12"/>
<connect gate="D" pin="IO_29" pad="P13"/>
<connect gate="D" pin="IO_3" pad="K16"/>
<connect gate="D" pin="IO_30" pad="P14"/>
<connect gate="D" pin="IO_31" pad="P15"/>
<connect gate="D" pin="IO_32" pad="P16"/>
<connect gate="D" pin="IO_33" pad="P17"/>
<connect gate="D" pin="IO_34" pad="R10"/>
<connect gate="D" pin="IO_35" pad="R11"/>
<connect gate="D" pin="IO_36" pad="R13"/>
<connect gate="D" pin="IO_37" pad="R14"/>
<connect gate="D" pin="IO_38" pad="R15"/>
<connect gate="D" pin="IO_39" pad="R16"/>
<connect gate="D" pin="IO_4" pad="L13"/>
<connect gate="D" pin="IO_40" pad="R17"/>
<connect gate="D" pin="IO_41" pad="R18"/>
<connect gate="D" pin="IO_42" pad="T10"/>
<connect gate="D" pin="IO_43" pad="T11"/>
<connect gate="D" pin="IO_44" pad="T14"/>
<connect gate="D" pin="IO_45" pad="T15"/>
<connect gate="D" pin="IO_46" pad="T16"/>
<connect gate="D" pin="IO_47" pad="T17"/>
<connect gate="D" pin="IO_48" pad="U10"/>
<connect gate="D" pin="IO_49" pad="U11"/>
<connect gate="D" pin="IO_5" pad="L14"/>
<connect gate="D" pin="IO_50" pad="U14"/>
<connect gate="D" pin="IO_51" pad="U15"/>
<connect gate="D" pin="IO_52" pad="U16"/>
<connect gate="D" pin="IO_53" pad="V10"/>
<connect gate="D" pin="IO_54" pad="V11"/>
<connect gate="D" pin="IO_55" pad="V12"/>
<connect gate="D" pin="IO_6" pad="L15"/>
<connect gate="D" pin="IO_7" pad="L16"/>
<connect gate="D" pin="IO_8" pad="L17"/>
<connect gate="D" pin="IO_9" pad="L18"/>
<connect gate="D" pin="NSTATUS" pad="L12"/>
<connect gate="D" pin="TCK" pad="K18"/>
<connect gate="D" pin="TDO" pad="K13"/>
<connect gate="D" pin="TMS" pad="K14"/>
<connect gate="D" pin="VCCINT" pad="V17"/>
<connect gate="D" pin="VCCINT_2" pad="U18"/>
<connect gate="D" pin="VCCINT_3" pad="K10"/>
<connect gate="D" pin="VCCIO3" pad="M12"/>
<connect gate="D" pin="VCCIO3_2" pad="P18"/>
<connect gate="D" pin="VCCIO4" pad="V14"/>
<connect gate="D" pin="VCCIO4_2" pad="P11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C4F324C8N"/>
<attribute name="OC_FARNELL" value="1453486"/>
<attribute name="OC_NEWARK" value="51R0545"/>
<attribute name="PACKAGE" value="324-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C4F400C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1C4F400C8N_A"/>
<gate name="B" symbol="EP1C4F400C8N_B"/>
<gate name="C" symbol="EP1C4F400C8N_C"/>
<gate name="D" symbol="EP1C4F400C8N_D"/>
</gates>
<devices>
<device name="" package="BGA400C20X20X100P_2100X2100X22">
<connects>
<connect gate="A" pin="CLK0" pad="K5"/>
<connect gate="A" pin="CLK1" pad="K6"/>
<connect gate="A" pin="DATA0" pad="K3"/>
<connect gate="A" pin="DCLK" pad="L3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="GNDA_PLL1" pad="K7"/>
<connect gate="A" pin="GNDG_PLL1" pad="L7"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="G8"/>
<connect gate="A" pin="GND_4" pad="C1"/>
<connect gate="A" pin="GND_5" pad="G9"/>
<connect gate="A" pin="GND_6" pad="H9"/>
<connect gate="A" pin="GND_7" pad="K9"/>
<connect gate="A" pin="GND_8" pad="A1"/>
<connect gate="A" pin="IO" pad="M1"/>
<connect gate="A" pin="IO_10" pad="B6"/>
<connect gate="A" pin="IO_11" pad="B7"/>
<connect gate="A" pin="IO_12" pad="B8"/>
<connect gate="A" pin="IO_13" pad="B9"/>
<connect gate="A" pin="IO_14" pad="C2"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D1"/>
<connect gate="A" pin="IO_23" pad="D2"/>
<connect gate="A" pin="IO_24" pad="D3"/>
<connect gate="A" pin="IO_25" pad="D4"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="E5"/>
<connect gate="A" pin="IO_35" pad="E6"/>
<connect gate="A" pin="IO_36" pad="E7"/>
<connect gate="A" pin="IO_37" pad="E8"/>
<connect gate="A" pin="IO_38" pad="E9"/>
<connect gate="A" pin="IO_39" pad="F1"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="F2"/>
<connect gate="A" pin="IO_41" pad="F3"/>
<connect gate="A" pin="IO_42" pad="F4"/>
<connect gate="A" pin="IO_43" pad="F5"/>
<connect gate="A" pin="IO_44" pad="F6"/>
<connect gate="A" pin="IO_45" pad="F7"/>
<connect gate="A" pin="IO_46" pad="F8"/>
<connect gate="A" pin="IO_47" pad="G1"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="G3"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_50" pad="G4"/>
<connect gate="A" pin="IO_51" pad="G5"/>
<connect gate="A" pin="IO_52" pad="G6"/>
<connect gate="A" pin="IO_53" pad="G7"/>
<connect gate="A" pin="IO_54" pad="H1"/>
<connect gate="A" pin="IO_55" pad="H2"/>
<connect gate="A" pin="IO_56" pad="H3"/>
<connect gate="A" pin="IO_57" pad="H4"/>
<connect gate="A" pin="IO_58" pad="H5"/>
<connect gate="A" pin="IO_59" pad="H6"/>
<connect gate="A" pin="IO_6" pad="A9"/>
<connect gate="A" pin="IO_60" pad="H7"/>
<connect gate="A" pin="IO_61" pad="J1"/>
<connect gate="A" pin="IO_62" pad="J2"/>
<connect gate="A" pin="IO_63" pad="J3"/>
<connect gate="A" pin="IO_64" pad="J4"/>
<connect gate="A" pin="IO_65" pad="J5"/>
<connect gate="A" pin="IO_66" pad="J6"/>
<connect gate="A" pin="IO_67" pad="J7"/>
<connect gate="A" pin="IO_68" pad="J8"/>
<connect gate="A" pin="IO_69" pad="K2"/>
<connect gate="A" pin="IO_7" pad="B3"/>
<connect gate="A" pin="IO_70" pad="L4"/>
<connect gate="A" pin="IO_71" pad="L8"/>
<connect gate="A" pin="IO_8" pad="B4"/>
<connect gate="A" pin="IO_9" pad="B5"/>
<connect gate="A" pin="MSEL0" pad="L1"/>
<connect gate="A" pin="MSEL1" pad="L6"/>
<connect gate="A" pin="NCE" pad="L5"/>
<connect gate="A" pin="NCEO" pad="L2"/>
<connect gate="A" pin="NCONFIG" pad="K1"/>
<connect gate="A" pin="VCCA_PLL1" pad="K4"/>
<connect gate="A" pin="VCCINT" pad="L9"/>
<connect gate="A" pin="VCCINT_2" pad="A2"/>
<connect gate="A" pin="VCCINT_3" pad="B1"/>
<connect gate="A" pin="VCCINT_4" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="E1"/>
<connect gate="A" pin="VCCIO1_2" pad="H8"/>
<connect gate="A" pin="VCCIO1_3" pad="K8"/>
<connect gate="A" pin="VCCIO2" pad="A5"/>
<connect gate="A" pin="VCCIO2_2" pad="F9"/>
<connect gate="B" pin="GND" pad="A18"/>
<connect gate="B" pin="GND_2" pad="P8"/>
<connect gate="B" pin="GND_3" pad="P9"/>
<connect gate="B" pin="GND_4" pad="V1"/>
<connect gate="B" pin="GND_5" pad="W2"/>
<connect gate="B" pin="GND_6" pad="Y1"/>
<connect gate="B" pin="GND_7" pad="Y3"/>
<connect gate="B" pin="GND_8" pad="A20"/>
<connect gate="B" pin="GND_9" pad="M9"/>
<connect gate="B" pin="IO" pad="B18"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N4"/>
<connect gate="B" pin="IO_13" pad="N5"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="P1"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="M2"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="R1"/>
<connect gate="B" pin="IO_24" pad="R2"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M3"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T2"/>
<connect gate="B" pin="IO_32" pad="T3"/>
<connect gate="B" pin="IO_33" pad="T4"/>
<connect gate="B" pin="IO_34" pad="T5"/>
<connect gate="B" pin="IO_35" pad="T6"/>
<connect gate="B" pin="IO_36" pad="T7"/>
<connect gate="B" pin="IO_37" pad="T8"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="U1"/>
<connect gate="B" pin="IO_4" pad="M4"/>
<connect gate="B" pin="IO_40" pad="U2"/>
<connect gate="B" pin="IO_41" pad="U3"/>
<connect gate="B" pin="IO_42" pad="U4"/>
<connect gate="B" pin="IO_43" pad="U5"/>
<connect gate="B" pin="IO_44" pad="U6"/>
<connect gate="B" pin="IO_45" pad="U7"/>
<connect gate="B" pin="IO_46" pad="U8"/>
<connect gate="B" pin="IO_47" pad="U9"/>
<connect gate="B" pin="IO_48" pad="V2"/>
<connect gate="B" pin="IO_49" pad="V3"/>
<connect gate="B" pin="IO_5" pad="M5"/>
<connect gate="B" pin="IO_50" pad="V4"/>
<connect gate="B" pin="IO_51" pad="V5"/>
<connect gate="B" pin="IO_52" pad="V6"/>
<connect gate="B" pin="IO_53" pad="V7"/>
<connect gate="B" pin="IO_54" pad="V8"/>
<connect gate="B" pin="IO_55" pad="V9"/>
<connect gate="B" pin="IO_56" pad="W3"/>
<connect gate="B" pin="IO_57" pad="W4"/>
<connect gate="B" pin="IO_58" pad="W5"/>
<connect gate="B" pin="IO_59" pad="W6"/>
<connect gate="B" pin="IO_6" pad="M6"/>
<connect gate="B" pin="IO_60" pad="W7"/>
<connect gate="B" pin="IO_61" pad="W8"/>
<connect gate="B" pin="IO_62" pad="W9"/>
<connect gate="B" pin="IO_63" pad="Y4"/>
<connect gate="B" pin="IO_64" pad="Y6"/>
<connect gate="B" pin="IO_65" pad="Y7"/>
<connect gate="B" pin="IO_66" pad="Y8"/>
<connect gate="B" pin="IO_67" pad="Y9"/>
<connect gate="B" pin="IO_68" pad="A10"/>
<connect gate="B" pin="IO_69" pad="A11"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_70" pad="A12"/>
<connect gate="B" pin="IO_71" pad="A13"/>
<connect gate="B" pin="IO_72" pad="A14"/>
<connect gate="B" pin="IO_73" pad="A15"/>
<connect gate="B" pin="IO_74" pad="A17"/>
<connect gate="B" pin="IO_75" pad="B10"/>
<connect gate="B" pin="IO_76" pad="B11"/>
<connect gate="B" pin="IO_77" pad="B12"/>
<connect gate="B" pin="IO_78" pad="B13"/>
<connect gate="B" pin="IO_79" pad="B14"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_80" pad="B15"/>
<connect gate="B" pin="IO_81" pad="B16"/>
<connect gate="B" pin="IO_82" pad="B17"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="VCCINT" pad="A19"/>
<connect gate="B" pin="VCCINT_2" pad="W1"/>
<connect gate="B" pin="VCCINT_3" pad="Y2"/>
<connect gate="B" pin="VCCINT_4" pad="N9"/>
<connect gate="B" pin="VCCIO1" pad="N8"/>
<connect gate="B" pin="VCCIO1_2" pad="T1"/>
<connect gate="B" pin="VCCIO2" pad="A16"/>
<connect gate="B" pin="VCCIO4" pad="R8"/>
<connect gate="B" pin="VCCIO4_2" pad="Y5"/>
<connect gate="C" pin="CLK2" pad="L14"/>
<connect gate="C" pin="CLK3" pad="K14"/>
<connect gate="C" pin="CONF_DONE" pad="L18"/>
<connect gate="C" pin="GND" pad="C20"/>
<connect gate="C" pin="GNDA_PLL2" pad="K20"/>
<connect gate="C" pin="GNDG_PLL2" pad="L15"/>
<connect gate="C" pin="GND_10" pad="H11"/>
<connect gate="C" pin="GND_11" pad="B19"/>
<connect gate="C" pin="GND_12" pad="L10"/>
<connect gate="C" pin="GND_2" pad="G10"/>
<connect gate="C" pin="GND_3" pad="G11"/>
<connect gate="C" pin="GND_4" pad="G12"/>
<connect gate="C" pin="GND_5" pad="K11"/>
<connect gate="C" pin="GND_6" pad="L12"/>
<connect gate="C" pin="GND_7" pad="J12"/>
<connect gate="C" pin="GND_8" pad="G13"/>
<connect gate="C" pin="GND_9" pad="J10"/>
<connect gate="C" pin="IO" pad="L13"/>
<connect gate="C" pin="IO_10" pad="C18"/>
<connect gate="C" pin="IO_11" pad="C19"/>
<connect gate="C" pin="IO_12" pad="D10"/>
<connect gate="C" pin="IO_13" pad="D11"/>
<connect gate="C" pin="IO_14" pad="D12"/>
<connect gate="C" pin="IO_15" pad="D13"/>
<connect gate="C" pin="IO_16" pad="D14"/>
<connect gate="C" pin="IO_17" pad="D15"/>
<connect gate="C" pin="IO_18" pad="D16"/>
<connect gate="C" pin="IO_19" pad="D17"/>
<connect gate="C" pin="IO_2" pad="C10"/>
<connect gate="C" pin="IO_20" pad="D18"/>
<connect gate="C" pin="IO_21" pad="D19"/>
<connect gate="C" pin="IO_22" pad="D20"/>
<connect gate="C" pin="IO_23" pad="E10"/>
<connect gate="C" pin="IO_24" pad="E11"/>
<connect gate="C" pin="IO_25" pad="E12"/>
<connect gate="C" pin="IO_26" pad="E13"/>
<connect gate="C" pin="IO_27" pad="E14"/>
<connect gate="C" pin="IO_28" pad="E15"/>
<connect gate="C" pin="IO_29" pad="E16"/>
<connect gate="C" pin="IO_3" pad="C11"/>
<connect gate="C" pin="IO_30" pad="E17"/>
<connect gate="C" pin="IO_31" pad="E18"/>
<connect gate="C" pin="IO_32" pad="E19"/>
<connect gate="C" pin="IO_33" pad="F10"/>
<connect gate="C" pin="IO_34" pad="F12"/>
<connect gate="C" pin="IO_35" pad="F14"/>
<connect gate="C" pin="IO_36" pad="F15"/>
<connect gate="C" pin="IO_37" pad="F16"/>
<connect gate="C" pin="IO_38" pad="F17"/>
<connect gate="C" pin="IO_39" pad="F18"/>
<connect gate="C" pin="IO_4" pad="C12"/>
<connect gate="C" pin="IO_40" pad="F19"/>
<connect gate="C" pin="IO_41" pad="F20"/>
<connect gate="C" pin="IO_42" pad="G14"/>
<connect gate="C" pin="IO_43" pad="G15"/>
<connect gate="C" pin="IO_44" pad="G16"/>
<connect gate="C" pin="IO_45" pad="G17"/>
<connect gate="C" pin="IO_46" pad="G18"/>
<connect gate="C" pin="IO_47" pad="G19"/>
<connect gate="C" pin="IO_48" pad="G20"/>
<connect gate="C" pin="IO_49" pad="H14"/>
<connect gate="C" pin="IO_5" pad="C13"/>
<connect gate="C" pin="IO_50" pad="H15"/>
<connect gate="C" pin="IO_51" pad="H16"/>
<connect gate="C" pin="IO_52" pad="H17"/>
<connect gate="C" pin="IO_53" pad="H18"/>
<connect gate="C" pin="IO_54" pad="H19"/>
<connect gate="C" pin="IO_55" pad="H20"/>
<connect gate="C" pin="IO_56" pad="J13"/>
<connect gate="C" pin="IO_57" pad="J14"/>
<connect gate="C" pin="IO_58" pad="J15"/>
<connect gate="C" pin="IO_59" pad="J16"/>
<connect gate="C" pin="IO_6" pad="C14"/>
<connect gate="C" pin="IO_60" pad="J17"/>
<connect gate="C" pin="IO_61" pad="J18"/>
<connect gate="C" pin="IO_62" pad="J19"/>
<connect gate="C" pin="IO_63" pad="J20"/>
<connect gate="C" pin="IO_64" pad="K15"/>
<connect gate="C" pin="IO_65" pad="K16"/>
<connect gate="C" pin="IO_66" pad="K19"/>
<connect gate="C" pin="IO_7" pad="C15"/>
<connect gate="C" pin="IO_8" pad="C16"/>
<connect gate="C" pin="IO_9" pad="C17"/>
<connect gate="C" pin="NSTATUS" pad="L17"/>
<connect gate="C" pin="TCK" pad="L19"/>
<connect gate="C" pin="TDI" pad="K18"/>
<connect gate="C" pin="TMS" pad="L16"/>
<connect gate="C" pin="VCCA_PLL2" pad="K17"/>
<connect gate="C" pin="VCCINT" pad="B20"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="K12"/>
<connect gate="C" pin="VCCINT_4" pad="H12"/>
<connect gate="C" pin="VCCINT_5" pad="K10"/>
<connect gate="C" pin="VCCINT_6" pad="J11"/>
<connect gate="C" pin="VCCINT_7" pad="L11"/>
<connect gate="C" pin="VCCIO2" pad="F13"/>
<connect gate="C" pin="VCCIO2_2" pad="F11"/>
<connect gate="C" pin="VCCIO3" pad="E20"/>
<connect gate="C" pin="VCCIO3_2" pad="H13"/>
<connect gate="C" pin="VCCIO3_3" pad="K13"/>
<connect gate="D" pin="GND" pad="Y20"/>
<connect gate="D" pin="GND_10" pad="P13"/>
<connect gate="D" pin="GND_11" pad="W19"/>
<connect gate="D" pin="GND_2" pad="N10"/>
<connect gate="D" pin="GND_3" pad="M11"/>
<connect gate="D" pin="GND_4" pad="N12"/>
<connect gate="D" pin="GND_5" pad="P10"/>
<connect gate="D" pin="GND_6" pad="P11"/>
<connect gate="D" pin="GND_7" pad="P12"/>
<connect gate="D" pin="GND_8" pad="V20"/>
<connect gate="D" pin="GND_9" pad="Y18"/>
<connect gate="D" pin="IO" pad="Y17"/>
<connect gate="D" pin="IO_10" pad="N14"/>
<connect gate="D" pin="IO_11" pad="N15"/>
<connect gate="D" pin="IO_12" pad="N16"/>
<connect gate="D" pin="IO_13" pad="N17"/>
<connect gate="D" pin="IO_14" pad="N18"/>
<connect gate="D" pin="IO_15" pad="N19"/>
<connect gate="D" pin="IO_16" pad="N20"/>
<connect gate="D" pin="IO_17" pad="P14"/>
<connect gate="D" pin="IO_18" pad="P15"/>
<connect gate="D" pin="IO_19" pad="P16"/>
<connect gate="D" pin="IO_2" pad="M13"/>
<connect gate="D" pin="IO_20" pad="P17"/>
<connect gate="D" pin="IO_21" pad="P18"/>
<connect gate="D" pin="IO_22" pad="P19"/>
<connect gate="D" pin="IO_23" pad="P20"/>
<connect gate="D" pin="IO_24" pad="R11"/>
<connect gate="D" pin="IO_25" pad="R13"/>
<connect gate="D" pin="IO_26" pad="R14"/>
<connect gate="D" pin="IO_27" pad="R15"/>
<connect gate="D" pin="IO_28" pad="R16"/>
<connect gate="D" pin="IO_29" pad="R17"/>
<connect gate="D" pin="IO_3" pad="M14"/>
<connect gate="D" pin="IO_30" pad="R18"/>
<connect gate="D" pin="IO_31" pad="R19"/>
<connect gate="D" pin="IO_32" pad="R20"/>
<connect gate="D" pin="IO_33" pad="T10"/>
<connect gate="D" pin="IO_34" pad="T11"/>
<connect gate="D" pin="IO_35" pad="T12"/>
<connect gate="D" pin="IO_36" pad="T13"/>
<connect gate="D" pin="IO_37" pad="T14"/>
<connect gate="D" pin="IO_38" pad="T15"/>
<connect gate="D" pin="IO_39" pad="T16"/>
<connect gate="D" pin="IO_4" pad="M15"/>
<connect gate="D" pin="IO_40" pad="T17"/>
<connect gate="D" pin="IO_41" pad="T18"/>
<connect gate="D" pin="IO_42" pad="T19"/>
<connect gate="D" pin="IO_43" pad="U10"/>
<connect gate="D" pin="IO_44" pad="U11"/>
<connect gate="D" pin="IO_45" pad="U12"/>
<connect gate="D" pin="IO_46" pad="U13"/>
<connect gate="D" pin="IO_47" pad="U14"/>
<connect gate="D" pin="IO_48" pad="U15"/>
<connect gate="D" pin="IO_49" pad="U16"/>
<connect gate="D" pin="IO_5" pad="M16"/>
<connect gate="D" pin="IO_50" pad="U17"/>
<connect gate="D" pin="IO_51" pad="U18"/>
<connect gate="D" pin="IO_52" pad="U19"/>
<connect gate="D" pin="IO_53" pad="U20"/>
<connect gate="D" pin="IO_54" pad="V10"/>
<connect gate="D" pin="IO_55" pad="V11"/>
<connect gate="D" pin="IO_56" pad="V12"/>
<connect gate="D" pin="IO_57" pad="V13"/>
<connect gate="D" pin="IO_58" pad="V14"/>
<connect gate="D" pin="IO_59" pad="V15"/>
<connect gate="D" pin="IO_6" pad="M17"/>
<connect gate="D" pin="IO_60" pad="V16"/>
<connect gate="D" pin="IO_61" pad="V17"/>
<connect gate="D" pin="IO_62" pad="V18"/>
<connect gate="D" pin="IO_63" pad="V19"/>
<connect gate="D" pin="IO_64" pad="W10"/>
<connect gate="D" pin="IO_65" pad="W11"/>
<connect gate="D" pin="IO_66" pad="W12"/>
<connect gate="D" pin="IO_67" pad="W13"/>
<connect gate="D" pin="IO_68" pad="W14"/>
<connect gate="D" pin="IO_69" pad="W15"/>
<connect gate="D" pin="IO_7" pad="M18"/>
<connect gate="D" pin="IO_70" pad="W16"/>
<connect gate="D" pin="IO_71" pad="W17"/>
<connect gate="D" pin="IO_72" pad="W18"/>
<connect gate="D" pin="IO_73" pad="Y10"/>
<connect gate="D" pin="IO_74" pad="Y11"/>
<connect gate="D" pin="IO_75" pad="Y12"/>
<connect gate="D" pin="IO_76" pad="Y13"/>
<connect gate="D" pin="IO_77" pad="Y14"/>
<connect gate="D" pin="IO_78" pad="Y15"/>
<connect gate="D" pin="IO_8" pad="M19"/>
<connect gate="D" pin="IO_9" pad="M20"/>
<connect gate="D" pin="TDO" pad="L20"/>
<connect gate="D" pin="VCCINT" pad="N11"/>
<connect gate="D" pin="VCCINT_2" pad="M10"/>
<connect gate="D" pin="VCCINT_3" pad="Y19"/>
<connect gate="D" pin="VCCINT_4" pad="M12"/>
<connect gate="D" pin="VCCINT_5" pad="W20"/>
<connect gate="D" pin="VCCIO3" pad="T20"/>
<connect gate="D" pin="VCCIO3_2" pad="N13"/>
<connect gate="D" pin="VCCIO4" pad="Y16"/>
<connect gate="D" pin="VCCIO4_2" pad="R10"/>
<connect gate="D" pin="VCCIO4_3" pad="R12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C4F400C8N"/>
<attribute name="OC_FARNELL" value="1662282"/>
<attribute name="OC_NEWARK" value="51R0546"/>
<attribute name="PACKAGE" value="400-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C6F256C8N">
<description>IC, CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C6F256C8N_A"/>
<gate name="B" symbol="EP1C6F256C8N_B"/>
<gate name="C" symbol="EP1C6F256C8N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="CLK0" pad="G1"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="DATA0" pad="H2"/>
<connect gate="A" pin="DCLK" pad="K4"/>
<connect gate="A" pin="GND" pad="G7"/>
<connect gate="A" pin="GNDA_PLL1" pad="J6"/>
<connect gate="A" pin="GNDG_PLL1" pad="J5"/>
<connect gate="A" pin="GND_10" pad="G9"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="A5"/>
<connect gate="A" pin="GND_4" pad="J7"/>
<connect gate="A" pin="GND_5" pad="J9"/>
<connect gate="A" pin="GND_6" pad="F6"/>
<connect gate="A" pin="GND_7" pad="H8"/>
<connect gate="A" pin="GND_8" pad="F8"/>
<connect gate="A" pin="GND_9" pad="F9"/>
<connect gate="A" pin="IO" pad="G5"/>
<connect gate="A" pin="IO_10" pad="B9"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B6"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C4"/>
<connect gate="A" pin="IO_18" pad="B7"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D1"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="D3"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D5"/>
<connect gate="A" pin="IO_29" pad="D6"/>
<connect gate="A" pin="IO_3" pad="A9"/>
<connect gate="A" pin="IO_30" pad="D7"/>
<connect gate="A" pin="IO_31" pad="D8"/>
<connect gate="A" pin="IO_32" pad="D9"/>
<connect gate="A" pin="IO_33" pad="E1"/>
<connect gate="A" pin="IO_34" pad="E2"/>
<connect gate="A" pin="IO_35" pad="E3"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E5"/>
<connect gate="A" pin="IO_38" pad="E6"/>
<connect gate="A" pin="IO_39" pad="E7"/>
<connect gate="A" pin="IO_4" pad="B1"/>
<connect gate="A" pin="IO_40" pad="E8"/>
<connect gate="A" pin="IO_41" pad="E9"/>
<connect gate="A" pin="IO_42" pad="F1"/>
<connect gate="A" pin="IO_43" pad="F2"/>
<connect gate="A" pin="IO_44" pad="F3"/>
<connect gate="A" pin="IO_45" pad="F4"/>
<connect gate="A" pin="IO_46" pad="F5"/>
<connect gate="A" pin="IO_47" pad="H5"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="K1"/>
<connect gate="A" pin="IO_5" pad="B2"/>
<connect gate="A" pin="IO_50" pad="G3"/>
<connect gate="A" pin="IO_51" pad="K2"/>
<connect gate="A" pin="IO_52" pad="G4"/>
<connect gate="A" pin="IO_53" pad="K3"/>
<connect gate="A" pin="IO_54" pad="J1"/>
<connect gate="A" pin="IO_55" pad="K5"/>
<connect gate="A" pin="IO_6" pad="A2"/>
<connect gate="A" pin="IO_7" pad="B3"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="J3"/>
<connect gate="A" pin="MSEL1" pad="J2"/>
<connect gate="A" pin="NCE" pad="J4"/>
<connect gate="A" pin="NCEO" pad="H4"/>
<connect gate="A" pin="NCONFIG" pad="H3"/>
<connect gate="A" pin="VCCA_PLL1" pad="H6"/>
<connect gate="A" pin="VCCINT" pad="J8"/>
<connect gate="A" pin="VCCINT_2" pad="A7"/>
<connect gate="A" pin="VCCINT_3" pad="H7"/>
<connect gate="A" pin="VCCINT_4" pad="H9"/>
<connect gate="A" pin="VCCINT_5" pad="G8"/>
<connect gate="A" pin="VCCIO1" pad="G6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F7"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="B" pin="GND" pad="A16"/>
<connect gate="B" pin="GND_2" pad="T1"/>
<connect gate="B" pin="GND_3" pad="T5"/>
<connect gate="B" pin="GND_4" pad="K6"/>
<connect gate="B" pin="GND_5" pad="L6"/>
<connect gate="B" pin="GND_6" pad="K8"/>
<connect gate="B" pin="GND_7" pad="L8"/>
<connect gate="B" pin="GND_8" pad="A12"/>
<connect gate="B" pin="GND_9" pad="L9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="P5"/>
<connect gate="B" pin="IO_11" pad="P6"/>
<connect gate="B" pin="IO_12" pad="P7"/>
<connect gate="B" pin="IO_13" pad="M1"/>
<connect gate="B" pin="IO_14" pad="P8"/>
<connect gate="B" pin="IO_15" pad="M2"/>
<connect gate="B" pin="IO_16" pad="P9"/>
<connect gate="B" pin="IO_17" pad="M3"/>
<connect gate="B" pin="IO_18" pad="R1"/>
<connect gate="B" pin="IO_19" pad="M4"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="R2"/>
<connect gate="B" pin="IO_21" pad="M5"/>
<connect gate="B" pin="IO_22" pad="R3"/>
<connect gate="B" pin="IO_23" pad="M6"/>
<connect gate="B" pin="IO_24" pad="M7"/>
<connect gate="B" pin="IO_25" pad="M8"/>
<connect gate="B" pin="IO_26" pad="M9"/>
<connect gate="B" pin="IO_27" pad="N1"/>
<connect gate="B" pin="IO_28" pad="N2"/>
<connect gate="B" pin="IO_29" pad="N3"/>
<connect gate="B" pin="IO_3" pad="L2"/>
<connect gate="B" pin="IO_30" pad="N4"/>
<connect gate="B" pin="IO_31" pad="N5"/>
<connect gate="B" pin="IO_32" pad="N6"/>
<connect gate="B" pin="IO_33" pad="N7"/>
<connect gate="B" pin="IO_34" pad="N8"/>
<connect gate="B" pin="IO_35" pad="N9"/>
<connect gate="B" pin="IO_36" pad="R4"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="L3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T4"/>
<connect gate="B" pin="IO_44" pad="T6"/>
<connect gate="B" pin="IO_45" pad="T8"/>
<connect gate="B" pin="IO_46" pad="T9"/>
<connect gate="B" pin="IO_47" pad="A11"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="L4"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B15"/>
<connect gate="B" pin="IO_56" pad="B16"/>
<connect gate="B" pin="IO_57" pad="C10"/>
<connect gate="B" pin="IO_58" pad="C11"/>
<connect gate="B" pin="IO_59" pad="C12"/>
<connect gate="B" pin="IO_6" pad="P2"/>
<connect gate="B" pin="IO_60" pad="C13"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="C15"/>
<connect gate="B" pin="IO_63" pad="D10"/>
<connect gate="B" pin="IO_64" pad="D11"/>
<connect gate="B" pin="IO_65" pad="D12"/>
<connect gate="B" pin="IO_66" pad="D13"/>
<connect gate="B" pin="IO_67" pad="D14"/>
<connect gate="B" pin="IO_68" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L5"/>
<connect gate="B" pin="IO_8" pad="P3"/>
<connect gate="B" pin="IO_9" pad="P4"/>
<connect gate="B" pin="VCCINT" pad="A10"/>
<connect gate="B" pin="VCCINT_2" pad="K7"/>
<connect gate="B" pin="VCCINT_3" pad="T7"/>
<connect gate="B" pin="VCCINT_4" pad="K9"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L7"/>
<connect gate="C" pin="CLK2" pad="G16"/>
<connect gate="C" pin="CLK3" pad="H16"/>
<connect gate="C" pin="CONF_DONE" pad="K13"/>
<connect gate="C" pin="GND" pad="T16"/>
<connect gate="C" pin="GNDA_PLL2" pad="J11"/>
<connect gate="C" pin="GNDG_PLL2" pad="J12"/>
<connect gate="C" pin="GND_2" pad="K10"/>
<connect gate="C" pin="GND_3" pad="L11"/>
<connect gate="C" pin="GND_4" pad="G11"/>
<connect gate="C" pin="GND_5" pad="H10"/>
<connect gate="C" pin="GND_6" pad="F11"/>
<connect gate="C" pin="GND_7" pad="T12"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO_10" pad="E10"/>
<connect gate="C" pin="IO_11" pad="F15"/>
<connect gate="C" pin="IO_12" pad="E11"/>
<connect gate="C" pin="IO_13" pad="F16"/>
<connect gate="C" pin="IO_14" pad="E12"/>
<connect gate="C" pin="IO_15" pad="E13"/>
<connect gate="C" pin="IO_16" pad="E14"/>
<connect gate="C" pin="IO_17" pad="G12"/>
<connect gate="C" pin="IO_18" pad="E15"/>
<connect gate="C" pin="IO_19" pad="G13"/>
<connect gate="C" pin="IO_2" pad="K12"/>
<connect gate="C" pin="IO_20" pad="E16"/>
<connect gate="C" pin="IO_21" pad="G14"/>
<connect gate="C" pin="IO_22" pad="G15"/>
<connect gate="C" pin="IO_23" pad="H12"/>
<connect gate="C" pin="IO_24" pad="H13"/>
<connect gate="C" pin="IO_25" pad="L12"/>
<connect gate="C" pin="IO_26" pad="L13"/>
<connect gate="C" pin="IO_27" pad="L14"/>
<connect gate="C" pin="IO_28" pad="L15"/>
<connect gate="C" pin="IO_29" pad="L16"/>
<connect gate="C" pin="IO_3" pad="J16"/>
<connect gate="C" pin="IO_30" pad="M10"/>
<connect gate="C" pin="IO_31" pad="M11"/>
<connect gate="C" pin="IO_32" pad="M12"/>
<connect gate="C" pin="IO_33" pad="M13"/>
<connect gate="C" pin="IO_34" pad="M14"/>
<connect gate="C" pin="IO_35" pad="M15"/>
<connect gate="C" pin="IO_36" pad="M16"/>
<connect gate="C" pin="IO_37" pad="N10"/>
<connect gate="C" pin="IO_38" pad="N11"/>
<connect gate="C" pin="IO_39" pad="N12"/>
<connect gate="C" pin="IO_4" pad="K14"/>
<connect gate="C" pin="IO_40" pad="N13"/>
<connect gate="C" pin="IO_41" pad="N14"/>
<connect gate="C" pin="IO_42" pad="N15"/>
<connect gate="C" pin="IO_43" pad="N16"/>
<connect gate="C" pin="IO_44" pad="P10"/>
<connect gate="C" pin="IO_45" pad="P11"/>
<connect gate="C" pin="IO_46" pad="P12"/>
<connect gate="C" pin="IO_47" pad="P13"/>
<connect gate="C" pin="IO_48" pad="P14"/>
<connect gate="C" pin="IO_49" pad="P15"/>
<connect gate="C" pin="IO_5" pad="K15"/>
<connect gate="C" pin="IO_50" pad="R10"/>
<connect gate="C" pin="IO_51" pad="R11"/>
<connect gate="C" pin="IO_52" pad="R12"/>
<connect gate="C" pin="IO_53" pad="R13"/>
<connect gate="C" pin="IO_54" pad="R14"/>
<connect gate="C" pin="IO_55" pad="R15"/>
<connect gate="C" pin="IO_56" pad="R16"/>
<connect gate="C" pin="IO_57" pad="T11"/>
<connect gate="C" pin="IO_58" pad="T13"/>
<connect gate="C" pin="IO_6" pad="K16"/>
<connect gate="C" pin="IO_7" pad="F12"/>
<connect gate="C" pin="IO_8" pad="F13"/>
<connect gate="C" pin="IO_9" pad="F14"/>
<connect gate="C" pin="NSTATUS" pad="J13"/>
<connect gate="C" pin="TCK" pad="J14"/>
<connect gate="C" pin="TDI" pad="H14"/>
<connect gate="C" pin="TDO" pad="H15"/>
<connect gate="C" pin="TMS" pad="J15"/>
<connect gate="C" pin="VCCA_PLL2" pad="H11"/>
<connect gate="C" pin="VCCINT" pad="G10"/>
<connect gate="C" pin="VCCINT_2" pad="T10"/>
<connect gate="C" pin="VCCINT_3" pad="J10"/>
<connect gate="C" pin="VCCIO2" pad="F10"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="K11"/>
<connect gate="C" pin="VCCIO4" pad="L10"/>
<connect gate="C" pin="VCCIO4_2" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C6F256C8N"/>
<attribute name="OC_FARNELL" value="1453482"/>
<attribute name="OC_NEWARK" value="51R0547"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C6F256I7N">
<description>IC, CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C6F256I7N_A"/>
<gate name="B" symbol="EP1C6F256I7N_B"/>
<gate name="C" symbol="EP1C6F256I7N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="CLK0" pad="G1"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="DATA0" pad="H2"/>
<connect gate="A" pin="DCLK" pad="K4"/>
<connect gate="A" pin="GND" pad="G7"/>
<connect gate="A" pin="GNDA_PLL1" pad="J6"/>
<connect gate="A" pin="GNDG_PLL1" pad="J5"/>
<connect gate="A" pin="GND_10" pad="G9"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="A5"/>
<connect gate="A" pin="GND_4" pad="J7"/>
<connect gate="A" pin="GND_5" pad="J9"/>
<connect gate="A" pin="GND_6" pad="F6"/>
<connect gate="A" pin="GND_7" pad="H8"/>
<connect gate="A" pin="GND_8" pad="F8"/>
<connect gate="A" pin="GND_9" pad="F9"/>
<connect gate="A" pin="IO" pad="G5"/>
<connect gate="A" pin="IO_10" pad="B9"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B6"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C4"/>
<connect gate="A" pin="IO_18" pad="B7"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D1"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="D3"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D5"/>
<connect gate="A" pin="IO_29" pad="D6"/>
<connect gate="A" pin="IO_3" pad="A9"/>
<connect gate="A" pin="IO_30" pad="D7"/>
<connect gate="A" pin="IO_31" pad="D8"/>
<connect gate="A" pin="IO_32" pad="D9"/>
<connect gate="A" pin="IO_33" pad="E1"/>
<connect gate="A" pin="IO_34" pad="E2"/>
<connect gate="A" pin="IO_35" pad="E3"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E5"/>
<connect gate="A" pin="IO_38" pad="E6"/>
<connect gate="A" pin="IO_39" pad="E7"/>
<connect gate="A" pin="IO_4" pad="B1"/>
<connect gate="A" pin="IO_40" pad="E8"/>
<connect gate="A" pin="IO_41" pad="E9"/>
<connect gate="A" pin="IO_42" pad="F1"/>
<connect gate="A" pin="IO_43" pad="F2"/>
<connect gate="A" pin="IO_44" pad="F3"/>
<connect gate="A" pin="IO_45" pad="F4"/>
<connect gate="A" pin="IO_46" pad="F5"/>
<connect gate="A" pin="IO_47" pad="H5"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="K1"/>
<connect gate="A" pin="IO_5" pad="B2"/>
<connect gate="A" pin="IO_50" pad="G3"/>
<connect gate="A" pin="IO_51" pad="K2"/>
<connect gate="A" pin="IO_52" pad="G4"/>
<connect gate="A" pin="IO_53" pad="K3"/>
<connect gate="A" pin="IO_54" pad="J1"/>
<connect gate="A" pin="IO_55" pad="K5"/>
<connect gate="A" pin="IO_6" pad="A2"/>
<connect gate="A" pin="IO_7" pad="B3"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="J3"/>
<connect gate="A" pin="MSEL1" pad="J2"/>
<connect gate="A" pin="NCE" pad="J4"/>
<connect gate="A" pin="NCEO" pad="H4"/>
<connect gate="A" pin="NCONFIG" pad="H3"/>
<connect gate="A" pin="VCCA_PLL1" pad="H6"/>
<connect gate="A" pin="VCCINT" pad="J8"/>
<connect gate="A" pin="VCCINT_2" pad="A7"/>
<connect gate="A" pin="VCCINT_3" pad="H7"/>
<connect gate="A" pin="VCCINT_4" pad="H9"/>
<connect gate="A" pin="VCCINT_5" pad="G8"/>
<connect gate="A" pin="VCCIO1" pad="G6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F7"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="B" pin="GND" pad="A16"/>
<connect gate="B" pin="GND_2" pad="T1"/>
<connect gate="B" pin="GND_3" pad="T5"/>
<connect gate="B" pin="GND_4" pad="K6"/>
<connect gate="B" pin="GND_5" pad="L6"/>
<connect gate="B" pin="GND_6" pad="K8"/>
<connect gate="B" pin="GND_7" pad="L8"/>
<connect gate="B" pin="GND_8" pad="A12"/>
<connect gate="B" pin="GND_9" pad="L9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="P5"/>
<connect gate="B" pin="IO_11" pad="P6"/>
<connect gate="B" pin="IO_12" pad="P7"/>
<connect gate="B" pin="IO_13" pad="M1"/>
<connect gate="B" pin="IO_14" pad="P8"/>
<connect gate="B" pin="IO_15" pad="M2"/>
<connect gate="B" pin="IO_16" pad="P9"/>
<connect gate="B" pin="IO_17" pad="M3"/>
<connect gate="B" pin="IO_18" pad="R1"/>
<connect gate="B" pin="IO_19" pad="M4"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="R2"/>
<connect gate="B" pin="IO_21" pad="M5"/>
<connect gate="B" pin="IO_22" pad="R3"/>
<connect gate="B" pin="IO_23" pad="M6"/>
<connect gate="B" pin="IO_24" pad="M7"/>
<connect gate="B" pin="IO_25" pad="M8"/>
<connect gate="B" pin="IO_26" pad="M9"/>
<connect gate="B" pin="IO_27" pad="N1"/>
<connect gate="B" pin="IO_28" pad="N2"/>
<connect gate="B" pin="IO_29" pad="N3"/>
<connect gate="B" pin="IO_3" pad="L2"/>
<connect gate="B" pin="IO_30" pad="N4"/>
<connect gate="B" pin="IO_31" pad="N5"/>
<connect gate="B" pin="IO_32" pad="N6"/>
<connect gate="B" pin="IO_33" pad="N7"/>
<connect gate="B" pin="IO_34" pad="N8"/>
<connect gate="B" pin="IO_35" pad="N9"/>
<connect gate="B" pin="IO_36" pad="R4"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="L3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T4"/>
<connect gate="B" pin="IO_44" pad="T6"/>
<connect gate="B" pin="IO_45" pad="T8"/>
<connect gate="B" pin="IO_46" pad="T9"/>
<connect gate="B" pin="IO_47" pad="A11"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="L4"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B15"/>
<connect gate="B" pin="IO_56" pad="B16"/>
<connect gate="B" pin="IO_57" pad="C10"/>
<connect gate="B" pin="IO_58" pad="C11"/>
<connect gate="B" pin="IO_59" pad="C12"/>
<connect gate="B" pin="IO_6" pad="P2"/>
<connect gate="B" pin="IO_60" pad="C13"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="C15"/>
<connect gate="B" pin="IO_63" pad="D10"/>
<connect gate="B" pin="IO_64" pad="D11"/>
<connect gate="B" pin="IO_65" pad="D12"/>
<connect gate="B" pin="IO_66" pad="D13"/>
<connect gate="B" pin="IO_67" pad="D14"/>
<connect gate="B" pin="IO_68" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L5"/>
<connect gate="B" pin="IO_8" pad="P3"/>
<connect gate="B" pin="IO_9" pad="P4"/>
<connect gate="B" pin="VCCINT" pad="A10"/>
<connect gate="B" pin="VCCINT_2" pad="K7"/>
<connect gate="B" pin="VCCINT_3" pad="T7"/>
<connect gate="B" pin="VCCINT_4" pad="K9"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L7"/>
<connect gate="C" pin="CLK2" pad="G16"/>
<connect gate="C" pin="CLK3" pad="H16"/>
<connect gate="C" pin="CONF_DONE" pad="K13"/>
<connect gate="C" pin="GND" pad="T16"/>
<connect gate="C" pin="GNDA_PLL2" pad="J11"/>
<connect gate="C" pin="GNDG_PLL2" pad="J12"/>
<connect gate="C" pin="GND_2" pad="K10"/>
<connect gate="C" pin="GND_3" pad="L11"/>
<connect gate="C" pin="GND_4" pad="G11"/>
<connect gate="C" pin="GND_5" pad="H10"/>
<connect gate="C" pin="GND_6" pad="F11"/>
<connect gate="C" pin="GND_7" pad="T12"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO_10" pad="E10"/>
<connect gate="C" pin="IO_11" pad="F15"/>
<connect gate="C" pin="IO_12" pad="E11"/>
<connect gate="C" pin="IO_13" pad="F16"/>
<connect gate="C" pin="IO_14" pad="E12"/>
<connect gate="C" pin="IO_15" pad="E13"/>
<connect gate="C" pin="IO_16" pad="E14"/>
<connect gate="C" pin="IO_17" pad="G12"/>
<connect gate="C" pin="IO_18" pad="E15"/>
<connect gate="C" pin="IO_19" pad="G13"/>
<connect gate="C" pin="IO_2" pad="K12"/>
<connect gate="C" pin="IO_20" pad="E16"/>
<connect gate="C" pin="IO_21" pad="G14"/>
<connect gate="C" pin="IO_22" pad="G15"/>
<connect gate="C" pin="IO_23" pad="H12"/>
<connect gate="C" pin="IO_24" pad="H13"/>
<connect gate="C" pin="IO_25" pad="L12"/>
<connect gate="C" pin="IO_26" pad="L13"/>
<connect gate="C" pin="IO_27" pad="L14"/>
<connect gate="C" pin="IO_28" pad="L15"/>
<connect gate="C" pin="IO_29" pad="L16"/>
<connect gate="C" pin="IO_3" pad="J16"/>
<connect gate="C" pin="IO_30" pad="M10"/>
<connect gate="C" pin="IO_31" pad="M11"/>
<connect gate="C" pin="IO_32" pad="M12"/>
<connect gate="C" pin="IO_33" pad="M13"/>
<connect gate="C" pin="IO_34" pad="M14"/>
<connect gate="C" pin="IO_35" pad="M15"/>
<connect gate="C" pin="IO_36" pad="M16"/>
<connect gate="C" pin="IO_37" pad="N10"/>
<connect gate="C" pin="IO_38" pad="N11"/>
<connect gate="C" pin="IO_39" pad="N12"/>
<connect gate="C" pin="IO_4" pad="K14"/>
<connect gate="C" pin="IO_40" pad="N13"/>
<connect gate="C" pin="IO_41" pad="N14"/>
<connect gate="C" pin="IO_42" pad="N15"/>
<connect gate="C" pin="IO_43" pad="N16"/>
<connect gate="C" pin="IO_44" pad="P10"/>
<connect gate="C" pin="IO_45" pad="P11"/>
<connect gate="C" pin="IO_46" pad="P12"/>
<connect gate="C" pin="IO_47" pad="P13"/>
<connect gate="C" pin="IO_48" pad="P14"/>
<connect gate="C" pin="IO_49" pad="P15"/>
<connect gate="C" pin="IO_5" pad="K15"/>
<connect gate="C" pin="IO_50" pad="R10"/>
<connect gate="C" pin="IO_51" pad="R11"/>
<connect gate="C" pin="IO_52" pad="R12"/>
<connect gate="C" pin="IO_53" pad="R13"/>
<connect gate="C" pin="IO_54" pad="R14"/>
<connect gate="C" pin="IO_55" pad="R15"/>
<connect gate="C" pin="IO_56" pad="R16"/>
<connect gate="C" pin="IO_57" pad="T11"/>
<connect gate="C" pin="IO_58" pad="T13"/>
<connect gate="C" pin="IO_6" pad="K16"/>
<connect gate="C" pin="IO_7" pad="F12"/>
<connect gate="C" pin="IO_8" pad="F13"/>
<connect gate="C" pin="IO_9" pad="F14"/>
<connect gate="C" pin="NSTATUS" pad="J13"/>
<connect gate="C" pin="TCK" pad="J14"/>
<connect gate="C" pin="TDI" pad="H14"/>
<connect gate="C" pin="TDO" pad="H15"/>
<connect gate="C" pin="TMS" pad="J15"/>
<connect gate="C" pin="VCCA_PLL2" pad="H11"/>
<connect gate="C" pin="VCCINT" pad="G10"/>
<connect gate="C" pin="VCCINT_2" pad="T10"/>
<connect gate="C" pin="VCCINT_3" pad="J10"/>
<connect gate="C" pin="VCCIO2" pad="F10"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="K11"/>
<connect gate="C" pin="VCCIO4" pad="L10"/>
<connect gate="C" pin="VCCIO4_2" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C6F256I7N"/>
<attribute name="OC_FARNELL" value="1453478"/>
<attribute name="OC_NEWARK" value="52R0077"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C6Q240C6N">
<description>IC CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C6Q240C6N_A"/>
<gate name="B" symbol="EP1C6Q240C6N_B"/>
<gate name="C" symbol="EP1C6Q240C6N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3460X3460X410-240N">
<connects>
<connect gate="A" pin="CLK0" pad="28"/>
<connect gate="A" pin="CLK1" pad="29"/>
<connect gate="A" pin="DATA0" pad="25"/>
<connect gate="A" pin="DCLK" pad="36"/>
<connect gate="A" pin="GND" pad="40"/>
<connect gate="A" pin="GNDA_PLL1" pad="30"/>
<connect gate="A" pin="GNDG_PLL1" pad="31"/>
<connect gate="A" pin="GND_2" pad="52"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="GND_4" pad="71"/>
<connect gate="A" pin="GND_5" pad="69"/>
<connect gate="A" pin="IO" pad="80"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="17"/>
<connect gate="A" pin="IO_17" pad="18"/>
<connect gate="A" pin="IO_18" pad="19"/>
<connect gate="A" pin="IO_19" pad="20"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="21"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="24"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="46"/>
<connect gate="A" pin="IO_32" pad="47"/>
<connect gate="A" pin="IO_33" pad="48"/>
<connect gate="A" pin="IO_34" pad="49"/>
<connect gate="A" pin="IO_35" pad="50"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="59"/>
<connect gate="A" pin="IO_43" pad="60"/>
<connect gate="A" pin="IO_44" pad="61"/>
<connect gate="A" pin="IO_45" pad="62"/>
<connect gate="A" pin="IO_46" pad="63"/>
<connect gate="A" pin="IO_47" pad="64"/>
<connect gate="A" pin="IO_48" pad="65"/>
<connect gate="A" pin="IO_49" pad="66"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="67"/>
<connect gate="A" pin="IO_51" pad="68"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_58" pad="79"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="MSEL0" pad="34"/>
<connect gate="A" pin="MSEL1" pad="35"/>
<connect gate="A" pin="NCE" pad="33"/>
<connect gate="A" pin="NCEO" pad="32"/>
<connect gate="A" pin="NCONFIG" pad="26"/>
<connect gate="A" pin="VCCA_PLL1" pad="27"/>
<connect gate="A" pin="VCCINT" pad="72"/>
<connect gate="A" pin="VCCIO1" pad="22"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="51"/>
<connect gate="A" pin="VCCIO4" pad="70"/>
<connect gate="B" pin="CLK2" pad="153"/>
<connect gate="B" pin="CLK3" pad="152"/>
<connect gate="B" pin="CONF_DONE" pad="145"/>
<connect gate="B" pin="GND" pad="111"/>
<connect gate="B" pin="GNDA_PLL2" pad="151"/>
<connect gate="B" pin="GNDG_PLL2" pad="150"/>
<connect gate="B" pin="GND_2" pad="89"/>
<connect gate="B" pin="GND_3" pad="142"/>
<connect gate="B" pin="GND_4" pad="129"/>
<connect gate="B" pin="GND_5" pad="91"/>
<connect gate="B" pin="GND_6" pad="109"/>
<connect gate="B" pin="IO" pad="160"/>
<connect gate="B" pin="IO_10" pad="93"/>
<connect gate="B" pin="IO_11" pad="94"/>
<connect gate="B" pin="IO_12" pad="95"/>
<connect gate="B" pin="IO_13" pad="96"/>
<connect gate="B" pin="IO_14" pad="97"/>
<connect gate="B" pin="IO_15" pad="98"/>
<connect gate="B" pin="IO_16" pad="99"/>
<connect gate="B" pin="IO_17" pad="100"/>
<connect gate="B" pin="IO_18" pad="101"/>
<connect gate="B" pin="IO_19" pad="102"/>
<connect gate="B" pin="IO_2" pad="81"/>
<connect gate="B" pin="IO_20" pad="103"/>
<connect gate="B" pin="IO_21" pad="104"/>
<connect gate="B" pin="IO_22" pad="105"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="108"/>
<connect gate="B" pin="IO_26" pad="113"/>
<connect gate="B" pin="IO_27" pad="114"/>
<connect gate="B" pin="IO_28" pad="115"/>
<connect gate="B" pin="IO_29" pad="116"/>
<connect gate="B" pin="IO_3" pad="82"/>
<connect gate="B" pin="IO_30" pad="117"/>
<connect gate="B" pin="IO_31" pad="118"/>
<connect gate="B" pin="IO_32" pad="119"/>
<connect gate="B" pin="IO_33" pad="120"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="122"/>
<connect gate="B" pin="IO_36" pad="123"/>
<connect gate="B" pin="IO_37" pad="124"/>
<connect gate="B" pin="IO_38" pad="125"/>
<connect gate="B" pin="IO_39" pad="126"/>
<connect gate="B" pin="IO_4" pad="83"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="131"/>
<connect gate="B" pin="IO_43" pad="132"/>
<connect gate="B" pin="IO_44" pad="133"/>
<connect gate="B" pin="IO_45" pad="134"/>
<connect gate="B" pin="IO_46" pad="135"/>
<connect gate="B" pin="IO_47" pad="136"/>
<connect gate="B" pin="IO_48" pad="137"/>
<connect gate="B" pin="IO_49" pad="138"/>
<connect gate="B" pin="IO_5" pad="84"/>
<connect gate="B" pin="IO_50" pad="139"/>
<connect gate="B" pin="IO_51" pad="140"/>
<connect gate="B" pin="IO_52" pad="141"/>
<connect gate="B" pin="IO_53" pad="143"/>
<connect gate="B" pin="IO_54" pad="144"/>
<connect gate="B" pin="IO_55" pad="156"/>
<connect gate="B" pin="IO_56" pad="158"/>
<connect gate="B" pin="IO_57" pad="159"/>
<connect gate="B" pin="IO_6" pad="85"/>
<connect gate="B" pin="IO_7" pad="86"/>
<connect gate="B" pin="IO_8" pad="87"/>
<connect gate="B" pin="IO_9" pad="88"/>
<connect gate="B" pin="NSTATUS" pad="146"/>
<connect gate="B" pin="TCK" pad="147"/>
<connect gate="B" pin="TDI" pad="155"/>
<connect gate="B" pin="TDO" pad="149"/>
<connect gate="B" pin="TMS" pad="148"/>
<connect gate="B" pin="VCCA_PLL2" pad="154"/>
<connect gate="B" pin="VCCINT" pad="110"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO3" pad="130"/>
<connect gate="B" pin="VCCIO3_2" pad="157"/>
<connect gate="B" pin="VCCIO4" pad="92"/>
<connect gate="B" pin="VCCIO4_2" pad="112"/>
<connect gate="C" pin="GND" pad="230"/>
<connect gate="C" pin="GND_2" pad="232"/>
<connect gate="C" pin="GND_3" pad="171"/>
<connect gate="C" pin="GND_4" pad="210"/>
<connect gate="C" pin="GND_5" pad="212"/>
<connect gate="C" pin="GND_6" pad="190"/>
<connect gate="C" pin="GND_7" pad="192"/>
<connect gate="C" pin="IO" pad="240"/>
<connect gate="C" pin="IO_10" pad="169"/>
<connect gate="C" pin="IO_11" pad="170"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="174"/>
<connect gate="C" pin="IO_14" pad="175"/>
<connect gate="C" pin="IO_15" pad="176"/>
<connect gate="C" pin="IO_16" pad="177"/>
<connect gate="C" pin="IO_17" pad="178"/>
<connect gate="C" pin="IO_18" pad="179"/>
<connect gate="C" pin="IO_19" pad="180"/>
<connect gate="C" pin="IO_2" pad="161"/>
<connect gate="C" pin="IO_20" pad="181"/>
<connect gate="C" pin="IO_21" pad="182"/>
<connect gate="C" pin="IO_22" pad="183"/>
<connect gate="C" pin="IO_23" pad="184"/>
<connect gate="C" pin="IO_24" pad="185"/>
<connect gate="C" pin="IO_25" pad="186"/>
<connect gate="C" pin="IO_26" pad="187"/>
<connect gate="C" pin="IO_27" pad="188"/>
<connect gate="C" pin="IO_28" pad="193"/>
<connect gate="C" pin="IO_29" pad="194"/>
<connect gate="C" pin="IO_3" pad="162"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="198"/>
<connect gate="C" pin="IO_34" pad="199"/>
<connect gate="C" pin="IO_35" pad="200"/>
<connect gate="C" pin="IO_36" pad="201"/>
<connect gate="C" pin="IO_37" pad="202"/>
<connect gate="C" pin="IO_38" pad="203"/>
<connect gate="C" pin="IO_39" pad="204"/>
<connect gate="C" pin="IO_4" pad="163"/>
<connect gate="C" pin="IO_40" pad="205"/>
<connect gate="C" pin="IO_41" pad="206"/>
<connect gate="C" pin="IO_42" pad="207"/>
<connect gate="C" pin="IO_43" pad="208"/>
<connect gate="C" pin="IO_44" pad="213"/>
<connect gate="C" pin="IO_45" pad="214"/>
<connect gate="C" pin="IO_46" pad="215"/>
<connect gate="C" pin="IO_47" pad="216"/>
<connect gate="C" pin="IO_48" pad="217"/>
<connect gate="C" pin="IO_49" pad="218"/>
<connect gate="C" pin="IO_5" pad="164"/>
<connect gate="C" pin="IO_50" pad="219"/>
<connect gate="C" pin="IO_51" pad="220"/>
<connect gate="C" pin="IO_52" pad="221"/>
<connect gate="C" pin="IO_53" pad="222"/>
<connect gate="C" pin="IO_54" pad="223"/>
<connect gate="C" pin="IO_55" pad="224"/>
<connect gate="C" pin="IO_56" pad="225"/>
<connect gate="C" pin="IO_57" pad="226"/>
<connect gate="C" pin="IO_58" pad="227"/>
<connect gate="C" pin="IO_59" pad="228"/>
<connect gate="C" pin="IO_6" pad="165"/>
<connect gate="C" pin="IO_60" pad="233"/>
<connect gate="C" pin="IO_61" pad="234"/>
<connect gate="C" pin="IO_62" pad="235"/>
<connect gate="C" pin="IO_63" pad="236"/>
<connect gate="C" pin="IO_64" pad="237"/>
<connect gate="C" pin="IO_65" pad="238"/>
<connect gate="C" pin="IO_66" pad="239"/>
<connect gate="C" pin="IO_7" pad="166"/>
<connect gate="C" pin="IO_8" pad="167"/>
<connect gate="C" pin="IO_9" pad="168"/>
<connect gate="C" pin="VCCINT" pad="191"/>
<connect gate="C" pin="VCCINT_2" pad="211"/>
<connect gate="C" pin="VCCINT_3" pad="229"/>
<connect gate="C" pin="VCCIO2" pad="209"/>
<connect gate="C" pin="VCCIO2_2" pad="231"/>
<connect gate="C" pin="VCCIO2_3" pad="189"/>
<connect gate="C" pin="VCCIO3" pad="172"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C6Q240C6N"/>
<attribute name="OC_FARNELL" value="1700722"/>
<attribute name="OC_NEWARK" value="51R0548"/>
<attribute name="PACKAGE" value="PQFP-240"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C6Q240C8N">
<description>IC CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C6Q240C8N_A"/>
<gate name="B" symbol="EP1C6Q240C8N_B"/>
<gate name="C" symbol="EP1C6Q240C8N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3460X3460X410-240N">
<connects>
<connect gate="A" pin="CLK0" pad="28"/>
<connect gate="A" pin="CLK1" pad="29"/>
<connect gate="A" pin="DATA0" pad="25"/>
<connect gate="A" pin="DCLK" pad="36"/>
<connect gate="A" pin="GND" pad="40"/>
<connect gate="A" pin="GNDA_PLL1" pad="30"/>
<connect gate="A" pin="GNDG_PLL1" pad="31"/>
<connect gate="A" pin="GND_2" pad="52"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="GND_4" pad="71"/>
<connect gate="A" pin="GND_5" pad="69"/>
<connect gate="A" pin="IO" pad="80"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="17"/>
<connect gate="A" pin="IO_17" pad="18"/>
<connect gate="A" pin="IO_18" pad="19"/>
<connect gate="A" pin="IO_19" pad="20"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="21"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="24"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="46"/>
<connect gate="A" pin="IO_32" pad="47"/>
<connect gate="A" pin="IO_33" pad="48"/>
<connect gate="A" pin="IO_34" pad="49"/>
<connect gate="A" pin="IO_35" pad="50"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="59"/>
<connect gate="A" pin="IO_43" pad="60"/>
<connect gate="A" pin="IO_44" pad="61"/>
<connect gate="A" pin="IO_45" pad="62"/>
<connect gate="A" pin="IO_46" pad="63"/>
<connect gate="A" pin="IO_47" pad="64"/>
<connect gate="A" pin="IO_48" pad="65"/>
<connect gate="A" pin="IO_49" pad="66"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="67"/>
<connect gate="A" pin="IO_51" pad="68"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_58" pad="79"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="MSEL0" pad="34"/>
<connect gate="A" pin="MSEL1" pad="35"/>
<connect gate="A" pin="NCE" pad="33"/>
<connect gate="A" pin="NCEO" pad="32"/>
<connect gate="A" pin="NCONFIG" pad="26"/>
<connect gate="A" pin="VCCA_PLL1" pad="27"/>
<connect gate="A" pin="VCCINT" pad="72"/>
<connect gate="A" pin="VCCIO1" pad="22"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="51"/>
<connect gate="A" pin="VCCIO4" pad="70"/>
<connect gate="B" pin="CLK2" pad="153"/>
<connect gate="B" pin="CLK3" pad="152"/>
<connect gate="B" pin="CONF_DONE" pad="145"/>
<connect gate="B" pin="GND" pad="111"/>
<connect gate="B" pin="GNDA_PLL2" pad="151"/>
<connect gate="B" pin="GNDG_PLL2" pad="150"/>
<connect gate="B" pin="GND_2" pad="89"/>
<connect gate="B" pin="GND_3" pad="142"/>
<connect gate="B" pin="GND_4" pad="129"/>
<connect gate="B" pin="GND_5" pad="91"/>
<connect gate="B" pin="GND_6" pad="109"/>
<connect gate="B" pin="IO" pad="160"/>
<connect gate="B" pin="IO_10" pad="93"/>
<connect gate="B" pin="IO_11" pad="94"/>
<connect gate="B" pin="IO_12" pad="95"/>
<connect gate="B" pin="IO_13" pad="96"/>
<connect gate="B" pin="IO_14" pad="97"/>
<connect gate="B" pin="IO_15" pad="98"/>
<connect gate="B" pin="IO_16" pad="99"/>
<connect gate="B" pin="IO_17" pad="100"/>
<connect gate="B" pin="IO_18" pad="101"/>
<connect gate="B" pin="IO_19" pad="102"/>
<connect gate="B" pin="IO_2" pad="81"/>
<connect gate="B" pin="IO_20" pad="103"/>
<connect gate="B" pin="IO_21" pad="104"/>
<connect gate="B" pin="IO_22" pad="105"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="108"/>
<connect gate="B" pin="IO_26" pad="113"/>
<connect gate="B" pin="IO_27" pad="114"/>
<connect gate="B" pin="IO_28" pad="115"/>
<connect gate="B" pin="IO_29" pad="116"/>
<connect gate="B" pin="IO_3" pad="82"/>
<connect gate="B" pin="IO_30" pad="117"/>
<connect gate="B" pin="IO_31" pad="118"/>
<connect gate="B" pin="IO_32" pad="119"/>
<connect gate="B" pin="IO_33" pad="120"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="122"/>
<connect gate="B" pin="IO_36" pad="123"/>
<connect gate="B" pin="IO_37" pad="124"/>
<connect gate="B" pin="IO_38" pad="125"/>
<connect gate="B" pin="IO_39" pad="126"/>
<connect gate="B" pin="IO_4" pad="83"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="131"/>
<connect gate="B" pin="IO_43" pad="132"/>
<connect gate="B" pin="IO_44" pad="133"/>
<connect gate="B" pin="IO_45" pad="134"/>
<connect gate="B" pin="IO_46" pad="135"/>
<connect gate="B" pin="IO_47" pad="136"/>
<connect gate="B" pin="IO_48" pad="137"/>
<connect gate="B" pin="IO_49" pad="138"/>
<connect gate="B" pin="IO_5" pad="84"/>
<connect gate="B" pin="IO_50" pad="139"/>
<connect gate="B" pin="IO_51" pad="140"/>
<connect gate="B" pin="IO_52" pad="141"/>
<connect gate="B" pin="IO_53" pad="143"/>
<connect gate="B" pin="IO_54" pad="144"/>
<connect gate="B" pin="IO_55" pad="156"/>
<connect gate="B" pin="IO_56" pad="158"/>
<connect gate="B" pin="IO_57" pad="159"/>
<connect gate="B" pin="IO_6" pad="85"/>
<connect gate="B" pin="IO_7" pad="86"/>
<connect gate="B" pin="IO_8" pad="87"/>
<connect gate="B" pin="IO_9" pad="88"/>
<connect gate="B" pin="NSTATUS" pad="146"/>
<connect gate="B" pin="TCK" pad="147"/>
<connect gate="B" pin="TDI" pad="155"/>
<connect gate="B" pin="TDO" pad="149"/>
<connect gate="B" pin="TMS" pad="148"/>
<connect gate="B" pin="VCCA_PLL2" pad="154"/>
<connect gate="B" pin="VCCINT" pad="110"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO3" pad="130"/>
<connect gate="B" pin="VCCIO3_2" pad="157"/>
<connect gate="B" pin="VCCIO4" pad="92"/>
<connect gate="B" pin="VCCIO4_2" pad="112"/>
<connect gate="C" pin="GND" pad="230"/>
<connect gate="C" pin="GND_2" pad="232"/>
<connect gate="C" pin="GND_3" pad="171"/>
<connect gate="C" pin="GND_4" pad="210"/>
<connect gate="C" pin="GND_5" pad="212"/>
<connect gate="C" pin="GND_6" pad="190"/>
<connect gate="C" pin="GND_7" pad="192"/>
<connect gate="C" pin="IO" pad="240"/>
<connect gate="C" pin="IO_10" pad="169"/>
<connect gate="C" pin="IO_11" pad="170"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="174"/>
<connect gate="C" pin="IO_14" pad="175"/>
<connect gate="C" pin="IO_15" pad="176"/>
<connect gate="C" pin="IO_16" pad="177"/>
<connect gate="C" pin="IO_17" pad="178"/>
<connect gate="C" pin="IO_18" pad="179"/>
<connect gate="C" pin="IO_19" pad="180"/>
<connect gate="C" pin="IO_2" pad="161"/>
<connect gate="C" pin="IO_20" pad="181"/>
<connect gate="C" pin="IO_21" pad="182"/>
<connect gate="C" pin="IO_22" pad="183"/>
<connect gate="C" pin="IO_23" pad="184"/>
<connect gate="C" pin="IO_24" pad="185"/>
<connect gate="C" pin="IO_25" pad="186"/>
<connect gate="C" pin="IO_26" pad="187"/>
<connect gate="C" pin="IO_27" pad="188"/>
<connect gate="C" pin="IO_28" pad="193"/>
<connect gate="C" pin="IO_29" pad="194"/>
<connect gate="C" pin="IO_3" pad="162"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="198"/>
<connect gate="C" pin="IO_34" pad="199"/>
<connect gate="C" pin="IO_35" pad="200"/>
<connect gate="C" pin="IO_36" pad="201"/>
<connect gate="C" pin="IO_37" pad="202"/>
<connect gate="C" pin="IO_38" pad="203"/>
<connect gate="C" pin="IO_39" pad="204"/>
<connect gate="C" pin="IO_4" pad="163"/>
<connect gate="C" pin="IO_40" pad="205"/>
<connect gate="C" pin="IO_41" pad="206"/>
<connect gate="C" pin="IO_42" pad="207"/>
<connect gate="C" pin="IO_43" pad="208"/>
<connect gate="C" pin="IO_44" pad="213"/>
<connect gate="C" pin="IO_45" pad="214"/>
<connect gate="C" pin="IO_46" pad="215"/>
<connect gate="C" pin="IO_47" pad="216"/>
<connect gate="C" pin="IO_48" pad="217"/>
<connect gate="C" pin="IO_49" pad="218"/>
<connect gate="C" pin="IO_5" pad="164"/>
<connect gate="C" pin="IO_50" pad="219"/>
<connect gate="C" pin="IO_51" pad="220"/>
<connect gate="C" pin="IO_52" pad="221"/>
<connect gate="C" pin="IO_53" pad="222"/>
<connect gate="C" pin="IO_54" pad="223"/>
<connect gate="C" pin="IO_55" pad="224"/>
<connect gate="C" pin="IO_56" pad="225"/>
<connect gate="C" pin="IO_57" pad="226"/>
<connect gate="C" pin="IO_58" pad="227"/>
<connect gate="C" pin="IO_59" pad="228"/>
<connect gate="C" pin="IO_6" pad="165"/>
<connect gate="C" pin="IO_60" pad="233"/>
<connect gate="C" pin="IO_61" pad="234"/>
<connect gate="C" pin="IO_62" pad="235"/>
<connect gate="C" pin="IO_63" pad="236"/>
<connect gate="C" pin="IO_64" pad="237"/>
<connect gate="C" pin="IO_65" pad="238"/>
<connect gate="C" pin="IO_66" pad="239"/>
<connect gate="C" pin="IO_7" pad="166"/>
<connect gate="C" pin="IO_8" pad="167"/>
<connect gate="C" pin="IO_9" pad="168"/>
<connect gate="C" pin="VCCINT" pad="191"/>
<connect gate="C" pin="VCCINT_2" pad="211"/>
<connect gate="C" pin="VCCINT_3" pad="229"/>
<connect gate="C" pin="VCCIO2" pad="209"/>
<connect gate="C" pin="VCCIO2_2" pad="231"/>
<connect gate="C" pin="VCCIO2_3" pad="189"/>
<connect gate="C" pin="VCCIO3" pad="172"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C6Q240C8N"/>
<attribute name="OC_FARNELL" value="1635093"/>
<attribute name="OC_NEWARK" value="51R0549"/>
<attribute name="PACKAGE" value="PQFP-240"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1C6T144C8N">
<description>IC CYCLONE FPGA</description>
<gates>
<gate name="A" symbol="EP1C6T144C8N_A"/>
<gate name="B" symbol="EP1C6T144C8N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLK0" pad="16"/>
<connect gate="A" pin="CLK1" pad="17"/>
<connect gate="A" pin="DATA0" pad="13"/>
<connect gate="A" pin="DCLK" pad="24"/>
<connect gate="A" pin="GND" pad="65"/>
<connect gate="A" pin="GNDA_PLL1" pad="18"/>
<connect gate="A" pin="GNDG_PLL1" pad="19"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="30"/>
<connect gate="A" pin="GND_4" pad="43"/>
<connect gate="A" pin="GND_5" pad="45"/>
<connect gate="A" pin="GND_6" pad="63"/>
<connect gate="A" pin="GND_7" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="25"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="27"/>
<connect gate="A" pin="IO_15" pad="28"/>
<connect gate="A" pin="IO_16" pad="31"/>
<connect gate="A" pin="IO_17" pad="32"/>
<connect gate="A" pin="IO_18" pad="33"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="38"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="50"/>
<connect gate="A" pin="IO_32" pad="51"/>
<connect gate="A" pin="IO_33" pad="52"/>
<connect gate="A" pin="IO_34" pad="53"/>
<connect gate="A" pin="IO_35" pad="56"/>
<connect gate="A" pin="IO_36" pad="57"/>
<connect gate="A" pin="IO_37" pad="58"/>
<connect gate="A" pin="IO_38" pad="59"/>
<connect gate="A" pin="IO_39" pad="60"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="61"/>
<connect gate="A" pin="IO_41" pad="62"/>
<connect gate="A" pin="IO_42" pad="67"/>
<connect gate="A" pin="IO_43" pad="68"/>
<connect gate="A" pin="IO_44" pad="69"/>
<connect gate="A" pin="IO_45" pad="70"/>
<connect gate="A" pin="IO_46" pad="71"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="MSEL0" pad="22"/>
<connect gate="A" pin="MSEL1" pad="23"/>
<connect gate="A" pin="NCE" pad="21"/>
<connect gate="A" pin="NCEO" pad="20"/>
<connect gate="A" pin="NCONFIG" pad="14"/>
<connect gate="A" pin="VCCA_PLL1" pad="15"/>
<connect gate="A" pin="VCCINT" pad="55"/>
<connect gate="A" pin="VCCINT_2" pad="46"/>
<connect gate="A" pin="VCCINT_3" pad="64"/>
<connect gate="A" pin="VCCIO1" pad="8"/>
<connect gate="A" pin="VCCIO1_2" pad="29"/>
<connect gate="A" pin="VCCIO4" pad="66"/>
<connect gate="A" pin="VCCIO4_2" pad="44"/>
<connect gate="B" pin="CLK2" pad="93"/>
<connect gate="B" pin="CLK3" pad="92"/>
<connect gate="B" pin="CONF_DONE" pad="86"/>
<connect gate="B" pin="GND" pad="138"/>
<connect gate="B" pin="GNDG_PLL2" pad="91"/>
<connect gate="B" pin="GND_2" pad="118"/>
<connect gate="B" pin="GND_3" pad="136"/>
<connect gate="B" pin="GND_4" pad="127"/>
<connect gate="B" pin="GND_5" pad="80"/>
<connect gate="B" pin="GND_6" pad="101"/>
<connect gate="B" pin="GND_7" pad="116"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="83"/>
<connect gate="B" pin="IO_11" pad="84"/>
<connect gate="B" pin="IO_12" pad="85"/>
<connect gate="B" pin="IO_13" pad="96"/>
<connect gate="B" pin="IO_14" pad="97"/>
<connect gate="B" pin="IO_15" pad="98"/>
<connect gate="B" pin="IO_16" pad="99"/>
<connect gate="B" pin="IO_17" pad="100"/>
<connect gate="B" pin="IO_18" pad="103"/>
<connect gate="B" pin="IO_19" pad="104"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="105"/>
<connect gate="B" pin="IO_21" pad="106"/>
<connect gate="B" pin="IO_22" pad="107"/>
<connect gate="B" pin="IO_23" pad="108"/>
<connect gate="B" pin="IO_24" pad="109"/>
<connect gate="B" pin="IO_25" pad="110"/>
<connect gate="B" pin="IO_26" pad="111"/>
<connect gate="B" pin="IO_27" pad="112"/>
<connect gate="B" pin="IO_28" pad="113"/>
<connect gate="B" pin="IO_29" pad="114"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="119"/>
<connect gate="B" pin="IO_31" pad="120"/>
<connect gate="B" pin="IO_32" pad="121"/>
<connect gate="B" pin="IO_33" pad="122"/>
<connect gate="B" pin="IO_34" pad="123"/>
<connect gate="B" pin="IO_35" pad="124"/>
<connect gate="B" pin="IO_36" pad="125"/>
<connect gate="B" pin="IO_37" pad="128"/>
<connect gate="B" pin="IO_38" pad="129"/>
<connect gate="B" pin="IO_39" pad="130"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="131"/>
<connect gate="B" pin="IO_41" pad="132"/>
<connect gate="B" pin="IO_42" pad="133"/>
<connect gate="B" pin="IO_43" pad="134"/>
<connect gate="B" pin="IO_44" pad="139"/>
<connect gate="B" pin="IO_45" pad="140"/>
<connect gate="B" pin="IO_46" pad="141"/>
<connect gate="B" pin="IO_47" pad="142"/>
<connect gate="B" pin="IO_48" pad="143"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_6" pad="77"/>
<connect gate="B" pin="IO_7" pad="78"/>
<connect gate="B" pin="IO_8" pad="79"/>
<connect gate="B" pin="IO_9" pad="82"/>
<connect gate="B" pin="NSTATUS" pad="87"/>
<connect gate="B" pin="TCK" pad="88"/>
<connect gate="B" pin="TDI" pad="95"/>
<connect gate="B" pin="TDO" pad="90"/>
<connect gate="B" pin="TMS" pad="89"/>
<connect gate="B" pin="VCCA_PLL2" pad="94"/>
<connect gate="B" pin="VCCINT" pad="135"/>
<connect gate="B" pin="VCCINT_2" pad="117"/>
<connect gate="B" pin="VCCINT_3" pad="126"/>
<connect gate="B" pin="VCCIO2" pad="115"/>
<connect gate="B" pin="VCCIO2_2" pad="137"/>
<connect gate="B" pin="VCCIO3" pad="81"/>
<connect gate="B" pin="VCCIO3_2" pad="102"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1C6T144C8N"/>
<attribute name="OC_FARNELL" value="1662258"/>
<attribute name="OC_NEWARK" value="51R0550"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K100FI256-2N">
<description>IC ACEX 1K FPGA</description>
<gates>
<gate name="A" symbol="EP1K100FI256-2N_A"/>
<gate name="B" symbol="EP1K100FI256-2N_B"/>
<gate name="C" symbol="EP1K100FI256-2N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16X_1700X1700X22">
<connects>
<connect gate="A" pin="CLOCK" pad="A9"/>
<connect gate="A" pin="DATA0" pad="A1"/>
<connect gate="A" pin="DCLK" pad="B2"/>
<connect gate="A" pin="GNDINT" pad="K5"/>
<connect gate="A" pin="GNDINT_10" pad="J8"/>
<connect gate="A" pin="GNDINT_11" pad="J9"/>
<connect gate="A" pin="GNDINT_2" pad="A3"/>
<connect gate="A" pin="GNDINT_3" pad="C7"/>
<connect gate="A" pin="GNDINT_4" pad="E5"/>
<connect gate="A" pin="GNDINT_5" pad="F6"/>
<connect gate="A" pin="GNDINT_6" pad="G7"/>
<connect gate="A" pin="GNDINT_7" pad="G9"/>
<connect gate="A" pin="GNDINT_8" pad="H8"/>
<connect gate="A" pin="GNDINT_9" pad="H9"/>
<connect gate="A" pin="INPUT" pad="E8"/>
<connect gate="A" pin="INPUT_2" pad="B9"/>
<connect gate="A" pin="IO" pad="K4"/>
<connect gate="A" pin="IO/DATA1" pad="B3"/>
<connect gate="A" pin="IO/DATA2" pad="A2"/>
<connect gate="A" pin="IO/DATA3" pad="C3"/>
<connect gate="A" pin="IO/DATA4" pad="B4"/>
<connect gate="A" pin="IO/DATA5" pad="A4"/>
<connect gate="A" pin="IO/DATA6" pad="D4"/>
<connect gate="A" pin="IO/DATA7" pad="B5"/>
<connect gate="A" pin="IO/DEV_NCLR" pad="D8"/>
<connect gate="A" pin="IO/DEV_OE" pad="C9"/>
<connect gate="A" pin="IO_10" pad="C4"/>
<connect gate="A" pin="IO_11" pad="C5"/>
<connect gate="A" pin="IO_12" pad="C6"/>
<connect gate="A" pin="IO_13" pad="C8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="D3"/>
<connect gate="A" pin="IO_16" pad="D5"/>
<connect gate="A" pin="IO_17" pad="D6"/>
<connect gate="A" pin="IO_18" pad="D7"/>
<connect gate="A" pin="IO_19" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="E1"/>
<connect gate="A" pin="IO_21" pad="E2"/>
<connect gate="A" pin="IO_22" pad="E4"/>
<connect gate="A" pin="IO_23" pad="E7"/>
<connect gate="A" pin="IO_24" pad="E9"/>
<connect gate="A" pin="IO_25" pad="F1"/>
<connect gate="A" pin="IO_26" pad="F2"/>
<connect gate="A" pin="IO_27" pad="F3"/>
<connect gate="A" pin="IO_28" pad="F4"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G4"/>
<connect gate="A" pin="IO_32" pad="G5"/>
<connect gate="A" pin="IO_33" pad="H2"/>
<connect gate="A" pin="IO_34" pad="H3"/>
<connect gate="A" pin="IO_35" pad="H4"/>
<connect gate="A" pin="IO_36" pad="H5"/>
<connect gate="A" pin="IO_37" pad="J2"/>
<connect gate="A" pin="IO_38" pad="J3"/>
<connect gate="A" pin="IO_39" pad="J4"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="J5"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_7" pad="B7"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="C1"/>
<connect gate="A" pin="NC" pad="K3"/>
<connect gate="A" pin="NCE" pad="B1"/>
<connect gate="A" pin="NC_2" pad="D1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="G3"/>
<connect gate="A" pin="NC_5" pad="H1"/>
<connect gate="A" pin="NC_6" pad="J1"/>
<connect gate="A" pin="TDI" pad="C2"/>
<connect gate="A" pin="VCCINT" pad="J7"/>
<connect gate="A" pin="VCCINT_2" pad="F5"/>
<connect gate="A" pin="VCCINT_3" pad="F7"/>
<connect gate="A" pin="VCCINT_4" pad="F9"/>
<connect gate="A" pin="VCCINT_5" pad="H6"/>
<connect gate="A" pin="VCCINT_6" pad="H7"/>
<connect gate="A" pin="VCCIO" pad="J6"/>
<connect gate="A" pin="VCCIO_2" pad="E6"/>
<connect gate="A" pin="VCCIO_3" pad="F8"/>
<connect gate="A" pin="VCCIO_4" pad="G6"/>
<connect gate="A" pin="VCCIO_5" pad="G8"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="L8"/>
<connect gate="B" pin="CONF_DONE" pad="C15"/>
<connect gate="B" pin="GNDINT" pad="A14"/>
<connect gate="B" pin="GNDINT_2" pad="K7"/>
<connect gate="B" pin="GNDINT_3" pad="L1"/>
<connect gate="B" pin="GNDINT_4" pad="L6"/>
<connect gate="B" pin="GNDINT_5" pad="M5"/>
<connect gate="B" pin="GND_CKLK" pad="T8"/>
<connect gate="B" pin="INPUT" pad="R8"/>
<connect gate="B" pin="INPUT_2" pad="M9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/CLKUSR" pad="D15"/>
<connect gate="B" pin="IO/CS" pad="A15"/>
<connect gate="B" pin="IO/NCS" pad="A16"/>
<connect gate="B" pin="IO/NRS" pad="C14"/>
<connect gate="B" pin="IO/NWS" pad="B14"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="N7"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="N9"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="L3"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="P8"/>
<connect gate="B" pin="IO_24" pad="P9"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M1"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T1"/>
<connect gate="B" pin="IO_32" pad="T2"/>
<connect gate="B" pin="IO_33" pad="T3"/>
<connect gate="B" pin="IO_34" pad="T4"/>
<connect gate="B" pin="IO_35" pad="T5"/>
<connect gate="B" pin="IO_36" pad="T6"/>
<connect gate="B" pin="IO_37" pad="T7"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="A10"/>
<connect gate="B" pin="IO_4" pad="M2"/>
<connect gate="B" pin="IO_40" pad="A11"/>
<connect gate="B" pin="IO_41" pad="A12"/>
<connect gate="B" pin="IO_42" pad="A13"/>
<connect gate="B" pin="IO_43" pad="B10"/>
<connect gate="B" pin="IO_44" pad="B11"/>
<connect gate="B" pin="IO_45" pad="B12"/>
<connect gate="B" pin="IO_46" pad="B13"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="C13"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_6" pad="M4"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="MSEL0" pad="P1"/>
<connect gate="B" pin="MSEL1" pad="R1"/>
<connect gate="B" pin="NC" pad="L4"/>
<connect gate="B" pin="NCEO" pad="B16"/>
<connect gate="B" pin="NCONFIG" pad="N4"/>
<connect gate="B" pin="NC_2" pad="L2"/>
<connect gate="B" pin="TCK" pad="B15"/>
<connect gate="B" pin="TDO" pad="C16"/>
<connect gate="B" pin="VCCINT" pad="R2"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="L5"/>
<connect gate="B" pin="VCCINT_4" pad="L7"/>
<connect gate="B" pin="VCCIO" pad="D12"/>
<connect gate="B" pin="VCCIO_2" pad="K6"/>
<connect gate="B" pin="VCCIO_3" pad="K8"/>
<connect gate="B" pin="VCCIO_4" pad="M6"/>
<connect gate="B" pin="VCC_CKLK" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="M12"/>
<connect gate="C" pin="GNDINT_2" pad="E12"/>
<connect gate="C" pin="GNDINT_3" pad="F11"/>
<connect gate="C" pin="GNDINT_4" pad="G10"/>
<connect gate="C" pin="GNDINT_5" pad="K10"/>
<connect gate="C" pin="GNDINT_6" pad="L11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/INIT_DONE" pad="G16"/>
<connect gate="C" pin="IO/LOCK" pad="P12"/>
<connect gate="C" pin="IO/RDY/NBUSY" pad="G14"/>
<connect gate="C" pin="IO_10" pad="G12"/>
<connect gate="C" pin="IO_11" pad="G13"/>
<connect gate="C" pin="IO_12" pad="G15"/>
<connect gate="C" pin="IO_13" pad="H12"/>
<connect gate="C" pin="IO_14" pad="H13"/>
<connect gate="C" pin="IO_15" pad="H14"/>
<connect gate="C" pin="IO_16" pad="H15"/>
<connect gate="C" pin="IO_17" pad="J12"/>
<connect gate="C" pin="IO_18" pad="J13"/>
<connect gate="C" pin="IO_19" pad="J14"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="J15"/>
<connect gate="C" pin="IO_21" pad="J16"/>
<connect gate="C" pin="IO_22" pad="K12"/>
<connect gate="C" pin="IO_23" pad="K13"/>
<connect gate="C" pin="IO_24" pad="K15"/>
<connect gate="C" pin="IO_25" pad="L13"/>
<connect gate="C" pin="IO_26" pad="L14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="L16"/>
<connect gate="C" pin="IO_29" pad="M10"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="M13"/>
<connect gate="C" pin="IO_31" pad="M15"/>
<connect gate="C" pin="IO_32" pad="N10"/>
<connect gate="C" pin="IO_33" pad="N11"/>
<connect gate="C" pin="IO_34" pad="N13"/>
<connect gate="C" pin="IO_35" pad="N14"/>
<connect gate="C" pin="IO_36" pad="N16"/>
<connect gate="C" pin="IO_37" pad="P10"/>
<connect gate="C" pin="IO_38" pad="P11"/>
<connect gate="C" pin="IO_39" pad="P13"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="P14"/>
<connect gate="C" pin="IO_41" pad="P16"/>
<connect gate="C" pin="IO_42" pad="R10"/>
<connect gate="C" pin="IO_43" pad="R11"/>
<connect gate="C" pin="IO_44" pad="R12"/>
<connect gate="C" pin="IO_45" pad="R13"/>
<connect gate="C" pin="IO_46" pad="R14"/>
<connect gate="C" pin="IO_47" pad="R15"/>
<connect gate="C" pin="IO_48" pad="T10"/>
<connect gate="C" pin="IO_49" pad="T11"/>
<connect gate="C" pin="IO_5" pad="E15"/>
<connect gate="C" pin="IO_50" pad="T12"/>
<connect gate="C" pin="IO_51" pad="T13"/>
<connect gate="C" pin="IO_52" pad="T14"/>
<connect gate="C" pin="IO_6" pad="F13"/>
<connect gate="C" pin="IO_7" pad="F14"/>
<connect gate="C" pin="IO_8" pad="F15"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="N15"/>
<connect gate="C" pin="NC_2" pad="E16"/>
<connect gate="C" pin="NC_3" pad="H16"/>
<connect gate="C" pin="NC_4" pad="K14"/>
<connect gate="C" pin="NC_5" pad="K16"/>
<connect gate="C" pin="NC_6" pad="M14"/>
<connect gate="C" pin="NC_7" pad="M16"/>
<connect gate="C" pin="NSTATUS" pad="T16"/>
<connect gate="C" pin="TMS" pad="P15"/>
<connect gate="C" pin="TRST" pad="R16"/>
<connect gate="C" pin="VCCINT" pad="M11"/>
<connect gate="C" pin="VCCINT_2" pad="E11"/>
<connect gate="C" pin="VCCINT_3" pad="F12"/>
<connect gate="C" pin="VCCINT_4" pad="H10"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="J11"/>
<connect gate="C" pin="VCCINT_7" pad="L12"/>
<connect gate="C" pin="VCCIO" pad="N12"/>
<connect gate="C" pin="VCCIO_2" pad="F10"/>
<connect gate="C" pin="VCCIO_3" pad="G11"/>
<connect gate="C" pin="VCCIO_4" pad="H11"/>
<connect gate="C" pin="VCCIO_5" pad="K11"/>
<connect gate="C" pin="VCCIO_6" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K100FI256-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0131"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K100FI484-2N" prefix="U">
<description>IC ACEX 1K FPGA 100K 484-FBGA</description>
<gates>
<gate name="A" symbol="EP1K100FC484-1_A"/>
<gate name="B" symbol="EP1K100FC484-1_B"/>
<gate name="C" symbol="EP1K100FC484-1_C"/>
<gate name="D" symbol="EP1K100FC484-1_D"/>
<gate name="E" symbol="EP1K100FC484-1_E"/>
</gates>
<devices>
<device name="" package="BGA484N100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="*CE" pad="E4"/>
<connect gate="A" pin="DATA0" pad="D4"/>
<connect gate="A" pin="DCLK" pad="E5"/>
<connect gate="A" pin="GND" pad="G3"/>
<connect gate="A" pin="GND_10" pad="C2"/>
<connect gate="A" pin="GND_11" pad="B2"/>
<connect gate="A" pin="GND_2" pad="D6"/>
<connect gate="A" pin="GND_3" pad="B1"/>
<connect gate="A" pin="GND_4" pad="A8"/>
<connect gate="A" pin="GND_5" pad="H2"/>
<connect gate="A" pin="GND_6" pad="J9"/>
<connect gate="A" pin="GND_7" pad="K3"/>
<connect gate="A" pin="GND_8" pad="H8"/>
<connect gate="A" pin="GND_9" pad="A1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO/DATA1" pad="E6"/>
<connect gate="A" pin="IO/DATA2" pad="D5"/>
<connect gate="A" pin="IO/DATA3" pad="F6"/>
<connect gate="A" pin="IO/DATA4" pad="E7"/>
<connect gate="A" pin="IO/DATA5" pad="D7"/>
<connect gate="A" pin="IO/DATA6" pad="G7"/>
<connect gate="A" pin="IO/DATA7" pad="E8"/>
<connect gate="A" pin="IO_10" pad="C4"/>
<connect gate="A" pin="IO_11" pad="C5"/>
<connect gate="A" pin="IO_12" pad="C6"/>
<connect gate="A" pin="IO_13" pad="C7"/>
<connect gate="A" pin="IO_14" pad="C8"/>
<connect gate="A" pin="IO_15" pad="C9"/>
<connect gate="A" pin="IO_16" pad="D1"/>
<connect gate="A" pin="IO_17" pad="D2"/>
<connect gate="A" pin="IO_18" pad="D3"/>
<connect gate="A" pin="IO_19" pad="D8"/>
<connect gate="A" pin="IO_2" pad="A7"/>
<connect gate="A" pin="IO_20" pad="D9"/>
<connect gate="A" pin="IO_21" pad="E2"/>
<connect gate="A" pin="IO_22" pad="E3"/>
<connect gate="A" pin="IO_23" pad="E9"/>
<connect gate="A" pin="IO_24" pad="F1"/>
<connect gate="A" pin="IO_25" pad="F3"/>
<connect gate="A" pin="IO_26" pad="F4"/>
<connect gate="A" pin="IO_27" pad="F7"/>
<connect gate="A" pin="IO_28" pad="F8"/>
<connect gate="A" pin="IO_29" pad="F9"/>
<connect gate="A" pin="IO_3" pad="A9"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G4"/>
<connect gate="A" pin="IO_32" pad="G5"/>
<connect gate="A" pin="IO_33" pad="G6"/>
<connect gate="A" pin="IO_34" pad="G8"/>
<connect gate="A" pin="IO_35" pad="G9"/>
<connect gate="A" pin="IO_36" pad="H1"/>
<connect gate="A" pin="IO_37" pad="H3"/>
<connect gate="A" pin="IO_38" pad="H4"/>
<connect gate="A" pin="IO_39" pad="H5"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="H6"/>
<connect gate="A" pin="IO_41" pad="J1"/>
<connect gate="A" pin="IO_42" pad="H7"/>
<connect gate="A" pin="IO_43" pad="J3"/>
<connect gate="A" pin="IO_44" pad="J4"/>
<connect gate="A" pin="IO_45" pad="J5"/>
<connect gate="A" pin="IO_46" pad="J6"/>
<connect gate="A" pin="IO_47" pad="J7"/>
<connect gate="A" pin="IO_48" pad="K1"/>
<connect gate="A" pin="IO_49" pad="K4"/>
<connect gate="A" pin="IO_5" pad="B7"/>
<connect gate="A" pin="IO_50" pad="K5"/>
<connect gate="A" pin="IO_51" pad="K6"/>
<connect gate="A" pin="IO_52" pad="K7"/>
<connect gate="A" pin="IO_53" pad="K8"/>
<connect gate="A" pin="IO_54" pad="L1"/>
<connect gate="A" pin="IO_55" pad="L3"/>
<connect gate="A" pin="IO_56" pad="L4"/>
<connect gate="A" pin="IO_57" pad="L5"/>
<connect gate="A" pin="IO_58" pad="L6"/>
<connect gate="A" pin="IO_6" pad="B8"/>
<connect gate="A" pin="IO_7" pad="B9"/>
<connect gate="A" pin="IO_8" pad="C1"/>
<connect gate="A" pin="IO_9" pad="C3"/>
<connect gate="A" pin="NC" pad="A5"/>
<connect gate="A" pin="NC_10" pad="A4"/>
<connect gate="A" pin="NC_2" pad="F2"/>
<connect gate="A" pin="NC_3" pad="B3"/>
<connect gate="A" pin="NC_4" pad="A2"/>
<connect gate="A" pin="NC_5" pad="B4"/>
<connect gate="A" pin="NC_6" pad="A3"/>
<connect gate="A" pin="NC_7" pad="K2"/>
<connect gate="A" pin="NC_8" pad="L2"/>
<connect gate="A" pin="NC_9" pad="J2"/>
<connect gate="A" pin="TDI" pad="F5"/>
<connect gate="A" pin="VCCINT" pad="J8"/>
<connect gate="A" pin="VCCIO" pad="E1"/>
<connect gate="A" pin="VCCIO_2" pad="A6"/>
<connect gate="A" pin="VCCIO_3" pad="B5"/>
<connect gate="A" pin="VCCIO_4" pad="H9"/>
<connect gate="A" pin="VCCIO_5" pad="K9"/>
<connect gate="A" pin="VCCIO_6" pad="G1"/>
<connect gate="B" pin="GND" pad="Y3"/>
<connect gate="B" pin="GND_10" pad="AA1"/>
<connect gate="B" pin="GND_11" pad="P9"/>
<connect gate="B" pin="GND_2" pad="V3"/>
<connect gate="B" pin="GND_3" pad="Y1"/>
<connect gate="B" pin="GND_4" pad="N8"/>
<connect gate="B" pin="GND_5" pad="T1"/>
<connect gate="B" pin="GND_6" pad="P4"/>
<connect gate="B" pin="GND_7" pad="R8"/>
<connect gate="B" pin="GND_8" pad="A22"/>
<connect gate="B" pin="GND_9" pad="Y2"/>
<connect gate="B" pin="IO" pad="A21"/>
<connect gate="B" pin="IO_10" pad="M8"/>
<connect gate="B" pin="IO_11" pad="N2"/>
<connect gate="B" pin="IO_12" pad="R2"/>
<connect gate="B" pin="IO_13" pad="R4"/>
<connect gate="B" pin="IO_14" pad="P1"/>
<connect gate="B" pin="IO_15" pad="R5"/>
<connect gate="B" pin="IO_16" pad="P2"/>
<connect gate="B" pin="IO_17" pad="N4"/>
<connect gate="B" pin="IO_18" pad="R6"/>
<connect gate="B" pin="IO_19" pad="N5"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="P3"/>
<connect gate="B" pin="IO_21" pad="N6"/>
<connect gate="B" pin="IO_22" pad="R7"/>
<connect gate="B" pin="IO_23" pad="N7"/>
<connect gate="B" pin="IO_24" pad="T2"/>
<connect gate="B" pin="IO_25" pad="P5"/>
<connect gate="B" pin="IO_26" pad="T4"/>
<connect gate="B" pin="IO_27" pad="P6"/>
<connect gate="B" pin="IO_28" pad="T5"/>
<connect gate="B" pin="IO_29" pad="P7"/>
<connect gate="B" pin="IO_3" pad="M1"/>
<connect gate="B" pin="IO_30" pad="T6"/>
<connect gate="B" pin="IO_31" pad="T7"/>
<connect gate="B" pin="IO_32" pad="T8"/>
<connect gate="B" pin="IO_33" pad="T9"/>
<connect gate="B" pin="IO_34" pad="U2"/>
<connect gate="B" pin="IO_35" pad="U3"/>
<connect gate="B" pin="IO_36" pad="U5"/>
<connect gate="B" pin="IO_37" pad="U6"/>
<connect gate="B" pin="IO_38" pad="U7"/>
<connect gate="B" pin="IO_39" pad="U8"/>
<connect gate="B" pin="IO_4" pad="M2"/>
<connect gate="B" pin="IO_40" pad="U9"/>
<connect gate="B" pin="IO_41" pad="V1"/>
<connect gate="B" pin="IO_42" pad="V2"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="V9"/>
<connect gate="B" pin="IO_47" pad="W1"/>
<connect gate="B" pin="IO_48" pad="W2"/>
<connect gate="B" pin="IO_49" pad="W3"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="W4"/>
<connect gate="B" pin="IO_51" pad="W5"/>
<connect gate="B" pin="IO_52" pad="W6"/>
<connect gate="B" pin="IO_53" pad="W7"/>
<connect gate="B" pin="IO_54" pad="W8"/>
<connect gate="B" pin="IO_55" pad="W9"/>
<connect gate="B" pin="IO_56" pad="Y4"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="M4"/>
<connect gate="B" pin="IO_60" pad="Y9"/>
<connect gate="B" pin="IO_61" pad="A10"/>
<connect gate="B" pin="IO_62" pad="A11"/>
<connect gate="B" pin="IO_63" pad="A12"/>
<connect gate="B" pin="IO_64" pad="A14"/>
<connect gate="B" pin="IO_65" pad="A15"/>
<connect gate="B" pin="IO_66" pad="A16"/>
<connect gate="B" pin="IO_67" pad="A17"/>
<connect gate="B" pin="IO_68" pad="A18"/>
<connect gate="B" pin="IO_69" pad="A19"/>
<connect gate="B" pin="IO_7" pad="M5"/>
<connect gate="B" pin="IO_70" pad="A20"/>
<connect gate="B" pin="IO_8" pad="M6"/>
<connect gate="B" pin="IO_9" pad="M7"/>
<connect gate="B" pin="MSEL0" pad="U4"/>
<connect gate="B" pin="MSEL1" pad="V4"/>
<connect gate="B" pin="NC" pad="N1"/>
<connect gate="B" pin="NC_2" pad="R3"/>
<connect gate="B" pin="NC_3" pad="U1"/>
<connect gate="B" pin="VCCINT" pad="V5"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="P8"/>
<connect gate="B" pin="VCCINT_4" pad="Y8"/>
<connect gate="B" pin="VCCIO" pad="N9"/>
<connect gate="B" pin="VCCIO_2" pad="A13"/>
<connect gate="B" pin="VCCIO_3" pad="N3"/>
<connect gate="B" pin="VCCIO_4" pad="M9"/>
<connect gate="B" pin="VCCIO_5" pad="R9"/>
<connect gate="B" pin="VCCIO_6" pad="R1"/>
<connect gate="B" pin="VCCIO_7" pad="T3"/>
<connect gate="C" pin="*CEO" pad="E19"/>
<connect gate="C" pin="CLOCK" pad="D12"/>
<connect gate="C" pin="CONF_DONE" pad="F18"/>
<connect gate="C" pin="GND" pad="C21"/>
<connect gate="C" pin="GND_2" pad="AA6"/>
<connect gate="C" pin="GND_3" pad="B17"/>
<connect gate="C" pin="GND_4" pad="B21"/>
<connect gate="C" pin="GND_5" pad="D17"/>
<connect gate="C" pin="GND_6" pad="E21"/>
<connect gate="C" pin="GND_7" pad="G21"/>
<connect gate="C" pin="GND_8" pad="B22"/>
<connect gate="C" pin="GND_9" pad="F10"/>
<connect gate="C" pin="INPUT" pad="H11"/>
<connect gate="C" pin="INPUT_2" pad="E12"/>
<connect gate="C" pin="IO" pad="H10"/>
<connect gate="C" pin="IO/*CS" pad="D19"/>
<connect gate="C" pin="IO/*DEV_CLR" pad="G11"/>
<connect gate="C" pin="IO/*RS" pad="F17"/>
<connect gate="C" pin="IO/*WS" pad="E17"/>
<connect gate="C" pin="IO/CLKUSR" pad="G18"/>
<connect gate="C" pin="IO/CS" pad="D18"/>
<connect gate="C" pin="IO/DEV_OE" pad="F12"/>
<connect gate="C" pin="IO_10" pad="AB2"/>
<connect gate="C" pin="IO_11" pad="AB6"/>
<connect gate="C" pin="IO_12" pad="AB8"/>
<connect gate="C" pin="IO_13" pad="AB9"/>
<connect gate="C" pin="IO_14" pad="B11"/>
<connect gate="C" pin="IO_15" pad="B12"/>
<connect gate="C" pin="IO_16" pad="B13"/>
<connect gate="C" pin="IO_17" pad="B14"/>
<connect gate="C" pin="IO_18" pad="B15"/>
<connect gate="C" pin="IO_19" pad="B16"/>
<connect gate="C" pin="IO_2" pad="AA2"/>
<connect gate="C" pin="IO_20" pad="B18"/>
<connect gate="C" pin="IO_21" pad="B19"/>
<connect gate="C" pin="IO_22" pad="B20"/>
<connect gate="C" pin="IO_23" pad="C10"/>
<connect gate="C" pin="IO_24" pad="C12"/>
<connect gate="C" pin="IO_25" pad="C13"/>
<connect gate="C" pin="IO_26" pad="C14"/>
<connect gate="C" pin="IO_27" pad="C16"/>
<connect gate="C" pin="IO_28" pad="C18"/>
<connect gate="C" pin="IO_29" pad="C19"/>
<connect gate="C" pin="IO_3" pad="AA3"/>
<connect gate="C" pin="IO_30" pad="C20"/>
<connect gate="C" pin="IO_31" pad="C22"/>
<connect gate="C" pin="IO_32" pad="D10"/>
<connect gate="C" pin="IO_33" pad="D11"/>
<connect gate="C" pin="IO_34" pad="D13"/>
<connect gate="C" pin="IO_35" pad="D14"/>
<connect gate="C" pin="IO_36" pad="D15"/>
<connect gate="C" pin="IO_37" pad="D16"/>
<connect gate="C" pin="IO_38" pad="D20"/>
<connect gate="C" pin="IO_39" pad="D21"/>
<connect gate="C" pin="IO_4" pad="AA4"/>
<connect gate="C" pin="IO_40" pad="D22"/>
<connect gate="C" pin="IO_41" pad="E10"/>
<connect gate="C" pin="IO_42" pad="E11"/>
<connect gate="C" pin="IO_43" pad="E13"/>
<connect gate="C" pin="IO_44" pad="E14"/>
<connect gate="C" pin="IO_45" pad="E15"/>
<connect gate="C" pin="IO_46" pad="E16"/>
<connect gate="C" pin="IO_47" pad="E20"/>
<connect gate="C" pin="IO_48" pad="E22"/>
<connect gate="C" pin="IO_49" pad="F11"/>
<connect gate="C" pin="IO_5" pad="AA5"/>
<connect gate="C" pin="IO_50" pad="F13"/>
<connect gate="C" pin="IO_51" pad="F14"/>
<connect gate="C" pin="IO_52" pad="F15"/>
<connect gate="C" pin="IO_53" pad="F16"/>
<connect gate="C" pin="IO_54" pad="F20"/>
<connect gate="C" pin="IO_55" pad="F21"/>
<connect gate="C" pin="IO_56" pad="F22"/>
<connect gate="C" pin="IO_57" pad="G10"/>
<connect gate="C" pin="IO_58" pad="G12"/>
<connect gate="C" pin="IO_59" pad="G13"/>
<connect gate="C" pin="IO_6" pad="AA7"/>
<connect gate="C" pin="IO_60" pad="G14"/>
<connect gate="C" pin="IO_61" pad="G16"/>
<connect gate="C" pin="IO_62" pad="G17"/>
<connect gate="C" pin="IO_63" pad="G19"/>
<connect gate="C" pin="IO_64" pad="G20"/>
<connect gate="C" pin="IO_65" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AA8"/>
<connect gate="C" pin="IO_8" pad="AA9"/>
<connect gate="C" pin="IO_9" pad="AB1"/>
<connect gate="C" pin="NC" pad="C17"/>
<connect gate="C" pin="NC_2" pad="AB3"/>
<connect gate="C" pin="NC_3" pad="AB4"/>
<connect gate="C" pin="NC_4" pad="B10"/>
<connect gate="C" pin="NC_5" pad="AB5"/>
<connect gate="C" pin="NC_6" pad="AB7"/>
<connect gate="C" pin="TCK" pad="E18"/>
<connect gate="C" pin="TDO" pad="F19"/>
<connect gate="C" pin="VCCINT" pad="C11"/>
<connect gate="C" pin="VCCINT_2" pad="C15"/>
<connect gate="C" pin="VCCIO" pad="G15"/>
<connect gate="D" pin="CLOCK/GCLK1" pad="P11"/>
<connect gate="D" pin="GND" pad="L12"/>
<connect gate="D" pin="GND_10" pad="M12"/>
<connect gate="D" pin="GND_11" pad="H15"/>
<connect gate="D" pin="GND_12" pad="M20"/>
<connect gate="D" pin="GND_13" pad="R15"/>
<connect gate="D" pin="GND_14" pad="L11"/>
<connect gate="D" pin="GND_15" pad="K13"/>
<connect gate="D" pin="GND_2" pad="K12"/>
<connect gate="D" pin="GND_3" pad="J20"/>
<connect gate="D" pin="GND_4" pad="J14"/>
<connect gate="D" pin="GND_5" pad="N10"/>
<connect gate="D" pin="GND_6" pad="M11"/>
<connect gate="D" pin="GND_7" pad="P14"/>
<connect gate="D" pin="GND_8" pad="N13"/>
<connect gate="D" pin="GND_9" pad="K10"/>
<connect gate="D" pin="INPUT" pad="R12"/>
<connect gate="D" pin="IO" pad="H22"/>
<connect gate="D" pin="IO/INIT_DONE" pad="K19"/>
<connect gate="D" pin="IO/RDY/*BSY" pad="K17"/>
<connect gate="D" pin="IO_10" pad="L15"/>
<connect gate="D" pin="IO_11" pad="K18"/>
<connect gate="D" pin="IO_12" pad="L16"/>
<connect gate="D" pin="IO_13" pad="L17"/>
<connect gate="D" pin="IO_14" pad="L21"/>
<connect gate="D" pin="IO_15" pad="L22"/>
<connect gate="D" pin="IO_16" pad="M15"/>
<connect gate="D" pin="IO_17" pad="M16"/>
<connect gate="D" pin="IO_18" pad="M17"/>
<connect gate="D" pin="IO_19" pad="M18"/>
<connect gate="D" pin="IO_2" pad="J16"/>
<connect gate="D" pin="IO_20" pad="M19"/>
<connect gate="D" pin="IO_21" pad="M21"/>
<connect gate="D" pin="IO_22" pad="M22"/>
<connect gate="D" pin="IO_23" pad="N15"/>
<connect gate="D" pin="IO_24" pad="N16"/>
<connect gate="D" pin="IO_25" pad="N17"/>
<connect gate="D" pin="IO_26" pad="N18"/>
<connect gate="D" pin="IO_27" pad="N19"/>
<connect gate="D" pin="IO_28" pad="N21"/>
<connect gate="D" pin="IO_29" pad="N22"/>
<connect gate="D" pin="IO_3" pad="J17"/>
<connect gate="D" pin="IO_30" pad="P16"/>
<connect gate="D" pin="IO_31" pad="P21"/>
<connect gate="D" pin="IO_32" pad="P17"/>
<connect gate="D" pin="IO_33" pad="P18"/>
<connect gate="D" pin="IO_34" pad="R10"/>
<connect gate="D" pin="IO_35" pad="P19"/>
<connect gate="D" pin="IO_36" pad="R11"/>
<connect gate="D" pin="IO_37" pad="R13"/>
<connect gate="D" pin="IO_38" pad="R16"/>
<connect gate="D" pin="IO_39" pad="R17"/>
<connect gate="D" pin="IO_4" pad="J18"/>
<connect gate="D" pin="IO_40" pad="H12"/>
<connect gate="D" pin="IO_41" pad="H13"/>
<connect gate="D" pin="IO_42" pad="L18"/>
<connect gate="D" pin="IO_43" pad="H16"/>
<connect gate="D" pin="IO_44" pad="K21"/>
<connect gate="D" pin="IO_45" pad="H17"/>
<connect gate="D" pin="IO_46" pad="L19"/>
<connect gate="D" pin="IO_47" pad="H18"/>
<connect gate="D" pin="IO_48" pad="K22"/>
<connect gate="D" pin="IO_49" pad="H19"/>
<connect gate="D" pin="IO_5" pad="J19"/>
<connect gate="D" pin="IO_50" pad="L20"/>
<connect gate="D" pin="IO_51" pad="H21"/>
<connect gate="D" pin="IO_6" pad="J21"/>
<connect gate="D" pin="IO_7" pad="J22"/>
<connect gate="D" pin="IO_8" pad="K15"/>
<connect gate="D" pin="IO_9" pad="K16"/>
<connect gate="D" pin="NC" pad="P20"/>
<connect gate="D" pin="NC_2" pad="P22"/>
<connect gate="D" pin="VCCINT" pad="N12"/>
<connect gate="D" pin="VCCINT_10" pad="P15"/>
<connect gate="D" pin="VCCINT_11" pad="J15"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="R14"/>
<connect gate="D" pin="VCCINT_2" pad="J10"/>
<connect gate="D" pin="VCCINT_3" pad="L10"/>
<connect gate="D" pin="VCCINT_4" pad="J12"/>
<connect gate="D" pin="VCCINT_5" pad="H14"/>
<connect gate="D" pin="VCCINT_6" pad="L13"/>
<connect gate="D" pin="VCCINT_7" pad="M10"/>
<connect gate="D" pin="VCCINT_8" pad="P10"/>
<connect gate="D" pin="VCCINT_9" pad="M13"/>
<connect gate="D" pin="VCCIO" pad="L14"/>
<connect gate="D" pin="VCCIO_10" pad="J13"/>
<connect gate="D" pin="VCCIO_11" pad="K20"/>
<connect gate="D" pin="VCCIO_2" pad="K14"/>
<connect gate="D" pin="VCCIO_3" pad="K11"/>
<connect gate="D" pin="VCCIO_4" pad="H20"/>
<connect gate="D" pin="VCCIO_5" pad="J11"/>
<connect gate="D" pin="VCCIO_6" pad="P13"/>
<connect gate="D" pin="VCCIO_7" pad="N11"/>
<connect gate="D" pin="VCCIO_8" pad="N20"/>
<connect gate="D" pin="VCCIO_9" pad="N14"/>
<connect gate="D" pin="VCC_CKLK" pad="P12"/>
<connect gate="E" pin="*CONFIG" pad="T17"/>
<connect gate="E" pin="*STATUS" pad="W19"/>
<connect gate="E" pin="GND" pad="Y22"/>
<connect gate="E" pin="GND_2" pad="W20"/>
<connect gate="E" pin="GND_3" pad="Y21"/>
<connect gate="E" pin="GND_4" pad="AA22"/>
<connect gate="E" pin="GND_5" pad="AB11"/>
<connect gate="E" pin="GND_6" pad="R22"/>
<connect gate="E" pin="GND_7" pad="AB16"/>
<connect gate="E" pin="GND_CKLK" pad="W11"/>
<connect gate="E" pin="INPUT" pad="V11"/>
<connect gate="E" pin="IO" pad="AB22"/>
<connect gate="E" pin="IO/LOCK" pad="U15"/>
<connect gate="E" pin="IO_10" pad="T14"/>
<connect gate="E" pin="IO_11" pad="T16"/>
<connect gate="E" pin="IO_12" pad="T18"/>
<connect gate="E" pin="IO_13" pad="T19"/>
<connect gate="E" pin="IO_14" pad="U10"/>
<connect gate="E" pin="IO_15" pad="U11"/>
<connect gate="E" pin="IO_16" pad="U12"/>
<connect gate="E" pin="IO_17" pad="U13"/>
<connect gate="E" pin="IO_18" pad="U14"/>
<connect gate="E" pin="IO_19" pad="U16"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="U17"/>
<connect gate="E" pin="IO_21" pad="U19"/>
<connect gate="E" pin="IO_22" pad="U20"/>
<connect gate="E" pin="IO_23" pad="U21"/>
<connect gate="E" pin="IO_24" pad="U22"/>
<connect gate="E" pin="IO_25" pad="V10"/>
<connect gate="E" pin="IO_26" pad="V12"/>
<connect gate="E" pin="IO_27" pad="V13"/>
<connect gate="E" pin="IO_28" pad="V14"/>
<connect gate="E" pin="IO_29" pad="V15"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="V16"/>
<connect gate="E" pin="IO_31" pad="V17"/>
<connect gate="E" pin="IO_32" pad="V18"/>
<connect gate="E" pin="IO_33" pad="V20"/>
<connect gate="E" pin="IO_34" pad="V21"/>
<connect gate="E" pin="IO_35" pad="W12"/>
<connect gate="E" pin="IO_36" pad="W10"/>
<connect gate="E" pin="IO_37" pad="W13"/>
<connect gate="E" pin="IO_38" pad="W14"/>
<connect gate="E" pin="IO_39" pad="W15"/>
<connect gate="E" pin="IO_4" pad="R20"/>
<connect gate="E" pin="IO_40" pad="W16"/>
<connect gate="E" pin="IO_41" pad="W17"/>
<connect gate="E" pin="IO_42" pad="W18"/>
<connect gate="E" pin="IO_43" pad="Y10"/>
<connect gate="E" pin="IO_44" pad="Y11"/>
<connect gate="E" pin="IO_45" pad="Y12"/>
<connect gate="E" pin="IO_46" pad="Y13"/>
<connect gate="E" pin="IO_47" pad="Y14"/>
<connect gate="E" pin="IO_48" pad="Y15"/>
<connect gate="E" pin="IO_49" pad="Y17"/>
<connect gate="E" pin="IO_5" pad="R21"/>
<connect gate="E" pin="IO_50" pad="Y18"/>
<connect gate="E" pin="IO_51" pad="Y19"/>
<connect gate="E" pin="IO_52" pad="Y20"/>
<connect gate="E" pin="IO_53" pad="AA10"/>
<connect gate="E" pin="IO_54" pad="AA11"/>
<connect gate="E" pin="IO_55" pad="AA13"/>
<connect gate="E" pin="IO_56" pad="AA14"/>
<connect gate="E" pin="IO_57" pad="AA16"/>
<connect gate="E" pin="IO_58" pad="AA17"/>
<connect gate="E" pin="IO_59" pad="AA18"/>
<connect gate="E" pin="IO_6" pad="T10"/>
<connect gate="E" pin="IO_60" pad="AA19"/>
<connect gate="E" pin="IO_61" pad="AA20"/>
<connect gate="E" pin="IO_62" pad="AA21"/>
<connect gate="E" pin="IO_63" pad="AB10"/>
<connect gate="E" pin="IO_64" pad="AB12"/>
<connect gate="E" pin="IO_65" pad="AB14"/>
<connect gate="E" pin="IO_66" pad="AB21"/>
<connect gate="E" pin="IO_7" pad="T11"/>
<connect gate="E" pin="IO_8" pad="T12"/>
<connect gate="E" pin="IO_9" pad="T13"/>
<connect gate="E" pin="NC" pad="AA15"/>
<connect gate="E" pin="NC_10" pad="Y16"/>
<connect gate="E" pin="NC_2" pad="T20"/>
<connect gate="E" pin="NC_3" pad="AB17"/>
<connect gate="E" pin="NC_4" pad="W22"/>
<connect gate="E" pin="NC_5" pad="AB15"/>
<connect gate="E" pin="NC_6" pad="AB18"/>
<connect gate="E" pin="NC_7" pad="T21"/>
<connect gate="E" pin="NC_8" pad="AB19"/>
<connect gate="E" pin="NC_9" pad="AB20"/>
<connect gate="E" pin="TMS" pad="U18"/>
<connect gate="E" pin="TRST" pad="V19"/>
<connect gate="E" pin="VCCINT" pad="W21"/>
<connect gate="E" pin="VCCINT_2" pad="AA12"/>
<connect gate="E" pin="VCCIO" pad="V22"/>
<connect gate="E" pin="VCCIO_2" pad="T15"/>
<connect gate="E" pin="VCCIO_3" pad="T22"/>
<connect gate="E" pin="VCCIO_4" pad="AB13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K100FI484-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0133"/>
<attribute name="PACKAGE" value="484-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K100QC208-3N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K100QC208-3N_A"/>
<gate name="B" symbol="EP1K100QC208-3N_B"/>
<gate name="C" symbol="EP1K100QC208-3N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="43"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="20"/>
<connect gate="A" pin="GNDINT_4" pad="23"/>
<connect gate="A" pin="GNDINT_5" pad="32"/>
<connect gate="A" pin="GNDINT_6" pad="59"/>
<connect gate="A" pin="GNDINT_7" pad="35"/>
<connect gate="A" pin="GNDINT_8" pad="49"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/LOCK" pad="62"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="17"/>
<connect gate="A" pin="IO_11" pad="18"/>
<connect gate="A" pin="IO_12" pad="24"/>
<connect gate="A" pin="IO_13" pad="25"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="36"/>
<connect gate="A" pin="IO_21" pad="37"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="44"/>
<connect gate="A" pin="IO_27" pad="45"/>
<connect gate="A" pin="IO_28" pad="46"/>
<connect gate="A" pin="IO_29" pad="47"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="53"/>
<connect gate="A" pin="IO_31" pad="54"/>
<connect gate="A" pin="IO_32" pad="55"/>
<connect gate="A" pin="IO_33" pad="56"/>
<connect gate="A" pin="IO_34" pad="57"/>
<connect gate="A" pin="IO_35" pad="58"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_5" pad="11"/>
<connect gate="A" pin="IO_6" pad="12"/>
<connect gate="A" pin="IO_7" pad="13"/>
<connect gate="A" pin="IO_8" pad="14"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="48"/>
<connect gate="A" pin="VCCINT_2" pad="21"/>
<connect gate="A" pin="VCCINT_3" pad="33"/>
<connect gate="A" pin="VCCIO" pad="5"/>
<connect gate="A" pin="VCCIO_2" pad="42"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="79"/>
<connect gate="B" pin="GNDINT" pad="109"/>
<connect gate="B" pin="GNDINT_2" pad="76"/>
<connect gate="B" pin="GNDINT_3" pad="82"/>
<connect gate="B" pin="GNDINT_4" pad="117"/>
<connect gate="B" pin="GNDINT_5" pad="123"/>
<connect gate="B" pin="GNDINT_6" pad="129"/>
<connect gate="B" pin="GNDINT_7" pad="137"/>
<connect gate="B" pin="GND_CKLK" pad="81"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="114"/>
<connect gate="B" pin="IO_29" pad="115"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="120"/>
<connect gate="B" pin="IO_33" pad="121"/>
<connect gate="B" pin="IO_34" pad="122"/>
<connect gate="B" pin="IO_35" pad="125"/>
<connect gate="B" pin="IO_36" pad="126"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="131"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_40" pad="132"/>
<connect gate="B" pin="IO_41" pad="133"/>
<connect gate="B" pin="IO_42" pad="134"/>
<connect gate="B" pin="IO_43" pad="135"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="91"/>
<connect gate="B" pin="VCCINT_3" pad="106"/>
<connect gate="B" pin="VCCINT_4" pad="72"/>
<connect gate="B" pin="VCCINT_5" pad="124"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="110"/>
<connect gate="B" pin="VCCIO_4" pad="98"/>
<connect gate="B" pin="VCCIO_5" pad="138"/>
<connect gate="B" pin="VCC_CKLK" pad="77"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="188"/>
<connect gate="C" pin="GNDINT_2" pad="145"/>
<connect gate="C" pin="GNDINT_3" pad="151"/>
<connect gate="C" pin="GNDINT_4" pad="171"/>
<connect gate="C" pin="GNDINT_5" pad="181"/>
<connect gate="C" pin="INPUT" pad="182"/>
<connect gate="C" pin="INPUT_2" pad="184"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_CLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="172"/>
<connect gate="C" pin="IO_11" pad="144"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="147"/>
<connect gate="C" pin="IO_14" pad="174"/>
<connect gate="C" pin="IO_15" pad="148"/>
<connect gate="C" pin="IO_16" pad="175"/>
<connect gate="C" pin="IO_17" pad="160"/>
<connect gate="C" pin="IO_18" pad="176"/>
<connect gate="C" pin="IO_19" pad="149"/>
<connect gate="C" pin="IO_2" pad="167"/>
<connect gate="C" pin="IO_20" pad="177"/>
<connect gate="C" pin="IO_21" pad="150"/>
<connect gate="C" pin="IO_22" pad="179"/>
<connect gate="C" pin="IO_23" pad="187"/>
<connect gate="C" pin="IO_24" pad="189"/>
<connect gate="C" pin="IO_25" pad="205"/>
<connect gate="C" pin="IO_26" pad="190"/>
<connect gate="C" pin="IO_27" pad="191"/>
<connect gate="C" pin="IO_28" pad="192"/>
<connect gate="C" pin="IO_29" pad="193"/>
<connect gate="C" pin="IO_3" pad="163"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="198"/>
<connect gate="C" pin="IO_34" pad="199"/>
<connect gate="C" pin="IO_35" pad="200"/>
<connect gate="C" pin="IO_36" pad="202"/>
<connect gate="C" pin="IO_4" pad="168"/>
<connect gate="C" pin="IO_5" pad="141"/>
<connect gate="C" pin="IO_6" pad="169"/>
<connect gate="C" pin="IO_7" pad="142"/>
<connect gate="C" pin="IO_8" pad="170"/>
<connect gate="C" pin="IO_9" pad="143"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="185"/>
<connect gate="C" pin="VCCINT_2" pad="152"/>
<connect gate="C" pin="VCCINT_3" pad="201"/>
<connect gate="C" pin="VCCIO" pad="165"/>
<connect gate="C" pin="VCCIO_2" pad="194"/>
<connect gate="C" pin="VCCIO_3" pad="146"/>
<connect gate="C" pin="VCCIO_4" pad="178"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K100QC208-3N"/>
<attribute name="OC_FARNELL" value="1549325"/>
<attribute name="OC_NEWARK" value="51R0552"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K100QI208-2N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K100QI208-2N_A"/>
<gate name="B" symbol="EP1K100QI208-2N_B"/>
<gate name="C" symbol="EP1K100QI208-2N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="43"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="20"/>
<connect gate="A" pin="GNDINT_4" pad="23"/>
<connect gate="A" pin="GNDINT_5" pad="32"/>
<connect gate="A" pin="GNDINT_6" pad="59"/>
<connect gate="A" pin="GNDINT_7" pad="35"/>
<connect gate="A" pin="GNDINT_8" pad="49"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/LOCK" pad="62"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="17"/>
<connect gate="A" pin="IO_11" pad="18"/>
<connect gate="A" pin="IO_12" pad="24"/>
<connect gate="A" pin="IO_13" pad="25"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="36"/>
<connect gate="A" pin="IO_21" pad="37"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="44"/>
<connect gate="A" pin="IO_27" pad="45"/>
<connect gate="A" pin="IO_28" pad="46"/>
<connect gate="A" pin="IO_29" pad="47"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="53"/>
<connect gate="A" pin="IO_31" pad="54"/>
<connect gate="A" pin="IO_32" pad="55"/>
<connect gate="A" pin="IO_33" pad="56"/>
<connect gate="A" pin="IO_34" pad="57"/>
<connect gate="A" pin="IO_35" pad="58"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_5" pad="11"/>
<connect gate="A" pin="IO_6" pad="12"/>
<connect gate="A" pin="IO_7" pad="13"/>
<connect gate="A" pin="IO_8" pad="14"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="48"/>
<connect gate="A" pin="VCCINT_2" pad="21"/>
<connect gate="A" pin="VCCINT_3" pad="33"/>
<connect gate="A" pin="VCCIO" pad="5"/>
<connect gate="A" pin="VCCIO_2" pad="42"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="79"/>
<connect gate="B" pin="GNDINT" pad="109"/>
<connect gate="B" pin="GNDINT_2" pad="76"/>
<connect gate="B" pin="GNDINT_3" pad="82"/>
<connect gate="B" pin="GNDINT_4" pad="117"/>
<connect gate="B" pin="GNDINT_5" pad="123"/>
<connect gate="B" pin="GNDINT_6" pad="129"/>
<connect gate="B" pin="GNDINT_7" pad="137"/>
<connect gate="B" pin="GND_CKLK" pad="81"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="114"/>
<connect gate="B" pin="IO_29" pad="115"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="120"/>
<connect gate="B" pin="IO_33" pad="121"/>
<connect gate="B" pin="IO_34" pad="122"/>
<connect gate="B" pin="IO_35" pad="125"/>
<connect gate="B" pin="IO_36" pad="126"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="131"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_40" pad="132"/>
<connect gate="B" pin="IO_41" pad="133"/>
<connect gate="B" pin="IO_42" pad="134"/>
<connect gate="B" pin="IO_43" pad="135"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="91"/>
<connect gate="B" pin="VCCINT_3" pad="106"/>
<connect gate="B" pin="VCCINT_4" pad="72"/>
<connect gate="B" pin="VCCINT_5" pad="124"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="110"/>
<connect gate="B" pin="VCCIO_4" pad="98"/>
<connect gate="B" pin="VCCIO_5" pad="138"/>
<connect gate="B" pin="VCC_CKLK" pad="77"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="188"/>
<connect gate="C" pin="GNDINT_2" pad="145"/>
<connect gate="C" pin="GNDINT_3" pad="151"/>
<connect gate="C" pin="GNDINT_4" pad="171"/>
<connect gate="C" pin="GNDINT_5" pad="181"/>
<connect gate="C" pin="INPUT" pad="182"/>
<connect gate="C" pin="INPUT_2" pad="184"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_CLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="172"/>
<connect gate="C" pin="IO_11" pad="144"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="147"/>
<connect gate="C" pin="IO_14" pad="174"/>
<connect gate="C" pin="IO_15" pad="148"/>
<connect gate="C" pin="IO_16" pad="175"/>
<connect gate="C" pin="IO_17" pad="160"/>
<connect gate="C" pin="IO_18" pad="176"/>
<connect gate="C" pin="IO_19" pad="149"/>
<connect gate="C" pin="IO_2" pad="167"/>
<connect gate="C" pin="IO_20" pad="177"/>
<connect gate="C" pin="IO_21" pad="150"/>
<connect gate="C" pin="IO_22" pad="179"/>
<connect gate="C" pin="IO_23" pad="187"/>
<connect gate="C" pin="IO_24" pad="189"/>
<connect gate="C" pin="IO_25" pad="205"/>
<connect gate="C" pin="IO_26" pad="190"/>
<connect gate="C" pin="IO_27" pad="191"/>
<connect gate="C" pin="IO_28" pad="192"/>
<connect gate="C" pin="IO_29" pad="193"/>
<connect gate="C" pin="IO_3" pad="163"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="198"/>
<connect gate="C" pin="IO_34" pad="199"/>
<connect gate="C" pin="IO_35" pad="200"/>
<connect gate="C" pin="IO_36" pad="202"/>
<connect gate="C" pin="IO_4" pad="168"/>
<connect gate="C" pin="IO_5" pad="141"/>
<connect gate="C" pin="IO_6" pad="169"/>
<connect gate="C" pin="IO_7" pad="142"/>
<connect gate="C" pin="IO_8" pad="170"/>
<connect gate="C" pin="IO_9" pad="143"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="185"/>
<connect gate="C" pin="VCCINT_2" pad="152"/>
<connect gate="C" pin="VCCINT_3" pad="201"/>
<connect gate="C" pin="VCCIO" pad="165"/>
<connect gate="C" pin="VCCIO_2" pad="194"/>
<connect gate="C" pin="VCCIO_3" pad="146"/>
<connect gate="C" pin="VCCIO_4" pad="178"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K100QI208-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0140"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K10QC208-2N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K10QC208-2N_A"/>
<gate name="B" symbol="EP1K10QC208-2N_B"/>
<gate name="C" symbol="EP1K10QC208-2N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="43"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="20"/>
<connect gate="A" pin="GNDINT_4" pad="23"/>
<connect gate="A" pin="GNDINT_5" pad="32"/>
<connect gate="A" pin="GNDINT_6" pad="59"/>
<connect gate="A" pin="GNDINT_7" pad="35"/>
<connect gate="A" pin="GNDINT_8" pad="49"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/LOCK" pad="62"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="17"/>
<connect gate="A" pin="IO_11" pad="18"/>
<connect gate="A" pin="IO_12" pad="24"/>
<connect gate="A" pin="IO_13" pad="25"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="36"/>
<connect gate="A" pin="IO_21" pad="37"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="44"/>
<connect gate="A" pin="IO_27" pad="45"/>
<connect gate="A" pin="IO_28" pad="46"/>
<connect gate="A" pin="IO_29" pad="47"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="53"/>
<connect gate="A" pin="IO_31" pad="54"/>
<connect gate="A" pin="IO_32" pad="55"/>
<connect gate="A" pin="IO_33" pad="56"/>
<connect gate="A" pin="IO_34" pad="57"/>
<connect gate="A" pin="IO_35" pad="58"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_5" pad="11"/>
<connect gate="A" pin="IO_6" pad="12"/>
<connect gate="A" pin="IO_7" pad="13"/>
<connect gate="A" pin="IO_8" pad="14"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="48"/>
<connect gate="A" pin="VCCINT_2" pad="21"/>
<connect gate="A" pin="VCCINT_3" pad="33"/>
<connect gate="A" pin="VCCIO" pad="5"/>
<connect gate="A" pin="VCCIO_2" pad="42"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="79"/>
<connect gate="B" pin="GNDINT" pad="109"/>
<connect gate="B" pin="GNDINT_2" pad="76"/>
<connect gate="B" pin="GNDINT_3" pad="82"/>
<connect gate="B" pin="GNDINT_4" pad="117"/>
<connect gate="B" pin="GNDINT_5" pad="123"/>
<connect gate="B" pin="GNDINT_6" pad="129"/>
<connect gate="B" pin="GNDINT_7" pad="137"/>
<connect gate="B" pin="GND_CKLK" pad="81"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="114"/>
<connect gate="B" pin="IO_29" pad="115"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="120"/>
<connect gate="B" pin="IO_33" pad="121"/>
<connect gate="B" pin="IO_34" pad="122"/>
<connect gate="B" pin="IO_35" pad="125"/>
<connect gate="B" pin="IO_36" pad="126"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="131"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_40" pad="132"/>
<connect gate="B" pin="IO_41" pad="133"/>
<connect gate="B" pin="IO_42" pad="134"/>
<connect gate="B" pin="IO_43" pad="135"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="91"/>
<connect gate="B" pin="VCCINT_3" pad="106"/>
<connect gate="B" pin="VCCINT_4" pad="72"/>
<connect gate="B" pin="VCCINT_5" pad="124"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="110"/>
<connect gate="B" pin="VCCIO_4" pad="98"/>
<connect gate="B" pin="VCCIO_5" pad="138"/>
<connect gate="B" pin="VCC_CKLK" pad="77"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="188"/>
<connect gate="C" pin="GNDINT_2" pad="145"/>
<connect gate="C" pin="GNDINT_3" pad="151"/>
<connect gate="C" pin="GNDINT_4" pad="171"/>
<connect gate="C" pin="GNDINT_5" pad="181"/>
<connect gate="C" pin="INPUT" pad="182"/>
<connect gate="C" pin="INPUT_2" pad="184"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_CLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="172"/>
<connect gate="C" pin="IO_11" pad="144"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="147"/>
<connect gate="C" pin="IO_14" pad="174"/>
<connect gate="C" pin="IO_15" pad="148"/>
<connect gate="C" pin="IO_16" pad="175"/>
<connect gate="C" pin="IO_17" pad="160"/>
<connect gate="C" pin="IO_18" pad="176"/>
<connect gate="C" pin="IO_19" pad="149"/>
<connect gate="C" pin="IO_2" pad="167"/>
<connect gate="C" pin="IO_20" pad="177"/>
<connect gate="C" pin="IO_21" pad="150"/>
<connect gate="C" pin="IO_22" pad="179"/>
<connect gate="C" pin="IO_23" pad="187"/>
<connect gate="C" pin="IO_24" pad="189"/>
<connect gate="C" pin="IO_25" pad="205"/>
<connect gate="C" pin="IO_26" pad="190"/>
<connect gate="C" pin="IO_27" pad="191"/>
<connect gate="C" pin="IO_28" pad="192"/>
<connect gate="C" pin="IO_29" pad="193"/>
<connect gate="C" pin="IO_3" pad="163"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="198"/>
<connect gate="C" pin="IO_34" pad="199"/>
<connect gate="C" pin="IO_35" pad="200"/>
<connect gate="C" pin="IO_36" pad="202"/>
<connect gate="C" pin="IO_4" pad="168"/>
<connect gate="C" pin="IO_5" pad="141"/>
<connect gate="C" pin="IO_6" pad="169"/>
<connect gate="C" pin="IO_7" pad="142"/>
<connect gate="C" pin="IO_8" pad="170"/>
<connect gate="C" pin="IO_9" pad="143"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="185"/>
<connect gate="C" pin="VCCINT_2" pad="152"/>
<connect gate="C" pin="VCCINT_3" pad="201"/>
<connect gate="C" pin="VCCIO" pad="165"/>
<connect gate="C" pin="VCCIO_2" pad="194"/>
<connect gate="C" pin="VCCIO_3" pad="146"/>
<connect gate="C" pin="VCCIO_4" pad="178"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K10QC208-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0102"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K10TC100-1N">
<description>IC ACEX</description>
<gates>
<gate name="A" symbol="EP1K10TC100-1N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CLKUSR" pad="5"/>
<connect gate="A" pin="CLOCK" pad="90"/>
<connect gate="A" pin="CONF_DONE" pad="1"/>
<connect gate="A" pin="CS" pad="98"/>
<connect gate="A" pin="DATA0" pad="76"/>
<connect gate="A" pin="DATA1" pad="77"/>
<connect gate="A" pin="DATA2" pad="78"/>
<connect gate="A" pin="DATA3" pad="79"/>
<connect gate="A" pin="DATA4" pad="80"/>
<connect gate="A" pin="DATA5" pad="81"/>
<connect gate="A" pin="DATA6" pad="82"/>
<connect gate="A" pin="DATA7" pad="84"/>
<connect gate="A" pin="DCLK" pad="75"/>
<connect gate="A" pin="DEV_OE" pad="93"/>
<connect gate="A" pin="GCLK1" pad="39"/>
<connect gate="A" pin="GNDINT" pad="36"/>
<connect gate="A" pin="GNDINT_2" pad="59"/>
<connect gate="A" pin="GNDINT_3" pad="42"/>
<connect gate="A" pin="GNDINT_4" pad="95"/>
<connect gate="A" pin="GNDINT_5" pad="11"/>
<connect gate="A" pin="GNDINT_6" pad="66"/>
<connect gate="A" pin="GNDINT_7" pad="18"/>
<connect gate="A" pin="GNDINT_8" pad="88"/>
<connect gate="A" pin="GND_CKLK" pad="41"/>
<connect gate="A" pin="INIT_DONE" pad="10"/>
<connect gate="A" pin="INPUT" pad="40"/>
<connect gate="A" pin="INPUT_2" pad="38"/>
<connect gate="A" pin="INPUT_3" pad="89"/>
<connect gate="A" pin="INPUT_4" pad="91"/>
<connect gate="A" pin="IO" pad="71"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="87"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="23"/>
<connect gate="A" pin="IO_12" pad="26"/>
<connect gate="A" pin="IO_13" pad="27"/>
<connect gate="A" pin="IO_14" pad="28"/>
<connect gate="A" pin="IO_15" pad="6"/>
<connect gate="A" pin="IO_16" pad="7"/>
<connect gate="A" pin="IO_17" pad="30"/>
<connect gate="A" pin="IO_18" pad="31"/>
<connect gate="A" pin="IO_19" pad="32"/>
<connect gate="A" pin="IO_2" pad="9"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="45"/>
<connect gate="A" pin="IO_22" pad="43"/>
<connect gate="A" pin="IO_23" pad="46"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="47"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="49"/>
<connect gate="A" pin="IO_28" pad="50"/>
<connect gate="A" pin="IO_29" pad="85"/>
<connect gate="A" pin="IO_3" pad="19"/>
<connect gate="A" pin="IO_30" pad="86"/>
<connect gate="A" pin="IO_31" pad="55"/>
<connect gate="A" pin="IO_32" pad="56"/>
<connect gate="A" pin="IO_33" pad="57"/>
<connect gate="A" pin="IO_34" pad="58"/>
<connect gate="A" pin="IO_35" pad="61"/>
<connect gate="A" pin="IO_36" pad="62"/>
<connect gate="A" pin="IO_37" pad="63"/>
<connect gate="A" pin="IO_38" pad="64"/>
<connect gate="A" pin="IO_39" pad="94"/>
<connect gate="A" pin="IO_4" pad="20"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_5" pad="22"/>
<connect gate="A" pin="IO_6" pad="14"/>
<connect gate="A" pin="IO_7" pad="21"/>
<connect gate="A" pin="IO_8" pad="13"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="LOCK" pad="29"/>
<connect gate="A" pin="MSEL0" pad="54"/>
<connect gate="A" pin="MSEL1" pad="53"/>
<connect gate="A" pin="NCE" pad="74"/>
<connect gate="A" pin="NCEO" pad="2"/>
<connect gate="A" pin="NCONFIG" pad="51"/>
<connect gate="A" pin="NCS" pad="99"/>
<connect gate="A" pin="NRS" pad="96"/>
<connect gate="A" pin="NSTATUS" pad="25"/>
<connect gate="A" pin="NWS" pad="97"/>
<connect gate="A" pin="RDYNBUSY" pad="8"/>
<connect gate="A" pin="TCK" pad="100"/>
<connect gate="A" pin="TDI" pad="73"/>
<connect gate="A" pin="TDO" pad="3"/>
<connect gate="A" pin="TMS" pad="24"/>
<connect gate="A" pin="VCCINT" pad="72"/>
<connect gate="A" pin="VCCINT_2" pad="12"/>
<connect gate="A" pin="VCCINT_3" pad="35"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCINT_5" pad="92"/>
<connect gate="A" pin="VCCINT_6" pad="60"/>
<connect gate="A" pin="VCCIO" pad="4"/>
<connect gate="A" pin="VCCIO_2" pad="44"/>
<connect gate="A" pin="VCCIO_3" pad="67"/>
<connect gate="A" pin="VCCIO_4" pad="83"/>
<connect gate="A" pin="VCCIO_5" pad="17"/>
<connect gate="A" pin="VCC_CKLK" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K10TC100-1N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0106"/>
<attribute name="PACKAGE" value="TQP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K10TC100-3N">
<description>IC ACEX</description>
<gates>
<gate name="A" symbol="EP1K10TC100-3N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CLKUSR" pad="5"/>
<connect gate="A" pin="CLOCK" pad="90"/>
<connect gate="A" pin="CONF_DONE" pad="1"/>
<connect gate="A" pin="CS" pad="98"/>
<connect gate="A" pin="DATA0" pad="76"/>
<connect gate="A" pin="DATA1" pad="77"/>
<connect gate="A" pin="DATA2" pad="78"/>
<connect gate="A" pin="DATA3" pad="79"/>
<connect gate="A" pin="DATA4" pad="80"/>
<connect gate="A" pin="DATA5" pad="81"/>
<connect gate="A" pin="DATA6" pad="82"/>
<connect gate="A" pin="DATA7" pad="84"/>
<connect gate="A" pin="DCLK" pad="75"/>
<connect gate="A" pin="DEV_OE" pad="93"/>
<connect gate="A" pin="GCLK1" pad="39"/>
<connect gate="A" pin="GNDINT" pad="36"/>
<connect gate="A" pin="GNDINT_2" pad="59"/>
<connect gate="A" pin="GNDINT_3" pad="42"/>
<connect gate="A" pin="GNDINT_4" pad="95"/>
<connect gate="A" pin="GNDINT_5" pad="11"/>
<connect gate="A" pin="GNDINT_6" pad="66"/>
<connect gate="A" pin="GNDINT_7" pad="18"/>
<connect gate="A" pin="GNDINT_8" pad="88"/>
<connect gate="A" pin="GND_CKLK" pad="41"/>
<connect gate="A" pin="INIT_DONE" pad="10"/>
<connect gate="A" pin="INPUT" pad="40"/>
<connect gate="A" pin="INPUT_2" pad="38"/>
<connect gate="A" pin="INPUT_3" pad="89"/>
<connect gate="A" pin="INPUT_4" pad="91"/>
<connect gate="A" pin="IO" pad="71"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="87"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="23"/>
<connect gate="A" pin="IO_12" pad="26"/>
<connect gate="A" pin="IO_13" pad="27"/>
<connect gate="A" pin="IO_14" pad="28"/>
<connect gate="A" pin="IO_15" pad="6"/>
<connect gate="A" pin="IO_16" pad="7"/>
<connect gate="A" pin="IO_17" pad="30"/>
<connect gate="A" pin="IO_18" pad="31"/>
<connect gate="A" pin="IO_19" pad="32"/>
<connect gate="A" pin="IO_2" pad="9"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="45"/>
<connect gate="A" pin="IO_22" pad="43"/>
<connect gate="A" pin="IO_23" pad="46"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="47"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="49"/>
<connect gate="A" pin="IO_28" pad="50"/>
<connect gate="A" pin="IO_29" pad="85"/>
<connect gate="A" pin="IO_3" pad="19"/>
<connect gate="A" pin="IO_30" pad="86"/>
<connect gate="A" pin="IO_31" pad="55"/>
<connect gate="A" pin="IO_32" pad="56"/>
<connect gate="A" pin="IO_33" pad="57"/>
<connect gate="A" pin="IO_34" pad="58"/>
<connect gate="A" pin="IO_35" pad="61"/>
<connect gate="A" pin="IO_36" pad="62"/>
<connect gate="A" pin="IO_37" pad="63"/>
<connect gate="A" pin="IO_38" pad="64"/>
<connect gate="A" pin="IO_39" pad="94"/>
<connect gate="A" pin="IO_4" pad="20"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_5" pad="22"/>
<connect gate="A" pin="IO_6" pad="14"/>
<connect gate="A" pin="IO_7" pad="21"/>
<connect gate="A" pin="IO_8" pad="13"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="LOCK" pad="29"/>
<connect gate="A" pin="MSEL0" pad="54"/>
<connect gate="A" pin="MSEL1" pad="53"/>
<connect gate="A" pin="NCE" pad="74"/>
<connect gate="A" pin="NCEO" pad="2"/>
<connect gate="A" pin="NCONFIG" pad="51"/>
<connect gate="A" pin="NCS" pad="99"/>
<connect gate="A" pin="NRS" pad="96"/>
<connect gate="A" pin="NSTATUS" pad="25"/>
<connect gate="A" pin="NWS" pad="97"/>
<connect gate="A" pin="RDYNBUSY" pad="8"/>
<connect gate="A" pin="TCK" pad="100"/>
<connect gate="A" pin="TDI" pad="73"/>
<connect gate="A" pin="TDO" pad="3"/>
<connect gate="A" pin="TMS" pad="24"/>
<connect gate="A" pin="VCCINT" pad="72"/>
<connect gate="A" pin="VCCINT_2" pad="12"/>
<connect gate="A" pin="VCCINT_3" pad="35"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCINT_5" pad="92"/>
<connect gate="A" pin="VCCINT_6" pad="60"/>
<connect gate="A" pin="VCCIO" pad="4"/>
<connect gate="A" pin="VCCIO_2" pad="44"/>
<connect gate="A" pin="VCCIO_3" pad="67"/>
<connect gate="A" pin="VCCIO_4" pad="83"/>
<connect gate="A" pin="VCCIO_5" pad="17"/>
<connect gate="A" pin="VCC_CKLK" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K10TC100-3N"/>
<attribute name="OC_FARNELL" value="1549323"/>
<attribute name="OC_NEWARK" value="52R0110"/>
<attribute name="PACKAGE" value="TQP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K10TC144-3N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K10TC144-3N_A"/>
<gate name="B" symbol="EP1K10TC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK/GCLK1" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="40"/>
<connect gate="A" pin="GNDINT_2" pad="58"/>
<connect gate="A" pin="GNDINT_3" pad="66"/>
<connect gate="A" pin="GNDINT_4" pad="15"/>
<connect gate="A" pin="GNDINT_5" pad="25"/>
<connect gate="A" pin="GNDINT_6" pad="52"/>
<connect gate="A" pin="GND_CKLK" pad="57"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/LOCK" pad="42"/>
<connect gate="A" pin="IO/RDY/NBUSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="26"/>
<connect gate="A" pin="IO_11" pad="27"/>
<connect gate="A" pin="IO_12" pad="29"/>
<connect gate="A" pin="IO_13" pad="30"/>
<connect gate="A" pin="IO_14" pad="32"/>
<connect gate="A" pin="IO_15" pad="33"/>
<connect gate="A" pin="IO_16" pad="36"/>
<connect gate="A" pin="IO_17" pad="37"/>
<connect gate="A" pin="IO_18" pad="38"/>
<connect gate="A" pin="IO_19" pad="39"/>
<connect gate="A" pin="IO_2" pad="9"/>
<connect gate="A" pin="IO_20" pad="41"/>
<connect gate="A" pin="IO_21" pad="43"/>
<connect gate="A" pin="IO_22" pad="44"/>
<connect gate="A" pin="IO_23" pad="46"/>
<connect gate="A" pin="IO_24" pad="47"/>
<connect gate="A" pin="IO_25" pad="48"/>
<connect gate="A" pin="IO_26" pad="49"/>
<connect gate="A" pin="IO_27" pad="51"/>
<connect gate="A" pin="IO_28" pad="59"/>
<connect gate="A" pin="IO_29" pad="60"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="62"/>
<connect gate="A" pin="IO_31" pad="63"/>
<connect gate="A" pin="IO_32" pad="64"/>
<connect gate="A" pin="IO_33" pad="65"/>
<connect gate="A" pin="IO_34" pad="67"/>
<connect gate="A" pin="IO_35" pad="68"/>
<connect gate="A" pin="IO_36" pad="69"/>
<connect gate="A" pin="IO_37" pad="70"/>
<connect gate="A" pin="IO_4" pad="13"/>
<connect gate="A" pin="IO_5" pad="17"/>
<connect gate="A" pin="IO_6" pad="18"/>
<connect gate="A" pin="IO_7" pad="19"/>
<connect gate="A" pin="IO_8" pad="21"/>
<connect gate="A" pin="IO_9" pad="23"/>
<connect gate="A" pin="N.C." pad="31"/>
<connect gate="A" pin="N.C._2" pad="6"/>
<connect gate="A" pin="N.C._3" pad="10"/>
<connect gate="A" pin="N.C._4" pad="12"/>
<connect gate="A" pin="N.C._5" pad="20"/>
<connect gate="A" pin="N.C._6" pad="22"/>
<connect gate="A" pin="N.C._7" pad="28"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="50"/>
<connect gate="A" pin="VCCINT_2" pad="16"/>
<connect gate="A" pin="VCCIO" pad="61"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="71"/>
<connect gate="A" pin="VCCIO_5" pad="45"/>
<connect gate="A" pin="VCC_CKLK" pad="53"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="93"/>
<connect gate="B" pin="GNDINT_2" pad="129"/>
<connect gate="B" pin="GNDINT_3" pad="139"/>
<connect gate="B" pin="GNDINT_4" pad="123"/>
<connect gate="B" pin="GNDINT_5" pad="84"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="90"/>
<connect gate="B" pin="IO_12" pad="91"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="95"/>
<connect gate="B" pin="IO_15" pad="96"/>
<connect gate="B" pin="IO_16" pad="97"/>
<connect gate="B" pin="IO_17" pad="98"/>
<connect gate="B" pin="IO_18" pad="100"/>
<connect gate="B" pin="IO_19" pad="102"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="117"/>
<connect gate="B" pin="IO_21" pad="118"/>
<connect gate="B" pin="IO_22" pad="119"/>
<connect gate="B" pin="IO_23" pad="120"/>
<connect gate="B" pin="IO_24" pad="121"/>
<connect gate="B" pin="IO_25" pad="130"/>
<connect gate="B" pin="IO_26" pad="131"/>
<connect gate="B" pin="IO_27" pad="132"/>
<connect gate="B" pin="IO_28" pad="133"/>
<connect gate="B" pin="IO_29" pad="135"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="136"/>
<connect gate="B" pin="IO_31" pad="137"/>
<connect gate="B" pin="IO_32" pad="138"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="83"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="N.C." pad="101"/>
<connect gate="B" pin="N.C._2" pad="99"/>
<connect gate="B" pin="N.C._3" pad="89"/>
<connect gate="B" pin="N.C._4" pad="104"/>
<connect gate="B" pin="N.C._5" pad="82"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="75"/>
<connect gate="B" pin="VCCINT_2" pad="103"/>
<connect gate="B" pin="VCCINT_3" pad="85"/>
<connect gate="B" pin="VCCINT_4" pad="127"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K10TC144-3N"/>
<attribute name="OC_FARNELL" value="1453500"/>
<attribute name="OC_NEWARK" value="51R0551"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K30FC256-1N">
<description>IC ACEX 1K FPGA</description>
<gates>
<gate name="A" symbol="EP1K30FC256-1N_A"/>
<gate name="B" symbol="EP1K30FC256-1N_B"/>
<gate name="C" symbol="EP1K30FC256-1N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16X_1700X1700X22">
<connects>
<connect gate="A" pin="CLOCK" pad="A9"/>
<connect gate="A" pin="DATA0" pad="A1"/>
<connect gate="A" pin="DCLK" pad="B2"/>
<connect gate="A" pin="GNDINT" pad="K5"/>
<connect gate="A" pin="GNDINT_10" pad="J8"/>
<connect gate="A" pin="GNDINT_11" pad="J9"/>
<connect gate="A" pin="GNDINT_2" pad="A3"/>
<connect gate="A" pin="GNDINT_3" pad="C7"/>
<connect gate="A" pin="GNDINT_4" pad="E5"/>
<connect gate="A" pin="GNDINT_5" pad="F6"/>
<connect gate="A" pin="GNDINT_6" pad="G7"/>
<connect gate="A" pin="GNDINT_7" pad="G9"/>
<connect gate="A" pin="GNDINT_8" pad="H8"/>
<connect gate="A" pin="GNDINT_9" pad="H9"/>
<connect gate="A" pin="INPUT" pad="E8"/>
<connect gate="A" pin="INPUT_2" pad="B9"/>
<connect gate="A" pin="IO" pad="K4"/>
<connect gate="A" pin="IO/DATA1" pad="B3"/>
<connect gate="A" pin="IO/DATA2" pad="A2"/>
<connect gate="A" pin="IO/DATA3" pad="C3"/>
<connect gate="A" pin="IO/DATA4" pad="B4"/>
<connect gate="A" pin="IO/DATA5" pad="A4"/>
<connect gate="A" pin="IO/DATA6" pad="D4"/>
<connect gate="A" pin="IO/DATA7" pad="B5"/>
<connect gate="A" pin="IO/DEV_NCLR" pad="D8"/>
<connect gate="A" pin="IO/DEV_OE" pad="C9"/>
<connect gate="A" pin="IO_10" pad="C4"/>
<connect gate="A" pin="IO_11" pad="C5"/>
<connect gate="A" pin="IO_12" pad="C6"/>
<connect gate="A" pin="IO_13" pad="C8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="D3"/>
<connect gate="A" pin="IO_16" pad="D5"/>
<connect gate="A" pin="IO_17" pad="D6"/>
<connect gate="A" pin="IO_18" pad="D7"/>
<connect gate="A" pin="IO_19" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="E1"/>
<connect gate="A" pin="IO_21" pad="E2"/>
<connect gate="A" pin="IO_22" pad="E4"/>
<connect gate="A" pin="IO_23" pad="E7"/>
<connect gate="A" pin="IO_24" pad="E9"/>
<connect gate="A" pin="IO_25" pad="F1"/>
<connect gate="A" pin="IO_26" pad="F2"/>
<connect gate="A" pin="IO_27" pad="F3"/>
<connect gate="A" pin="IO_28" pad="F4"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G4"/>
<connect gate="A" pin="IO_32" pad="G5"/>
<connect gate="A" pin="IO_33" pad="H2"/>
<connect gate="A" pin="IO_34" pad="H3"/>
<connect gate="A" pin="IO_35" pad="H4"/>
<connect gate="A" pin="IO_36" pad="H5"/>
<connect gate="A" pin="IO_37" pad="J2"/>
<connect gate="A" pin="IO_38" pad="J3"/>
<connect gate="A" pin="IO_39" pad="J4"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="J5"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_7" pad="B7"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="C1"/>
<connect gate="A" pin="NC" pad="K3"/>
<connect gate="A" pin="NCE" pad="B1"/>
<connect gate="A" pin="NC_2" pad="D1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="G3"/>
<connect gate="A" pin="NC_5" pad="H1"/>
<connect gate="A" pin="NC_6" pad="J1"/>
<connect gate="A" pin="TDI" pad="C2"/>
<connect gate="A" pin="VCCINT" pad="J7"/>
<connect gate="A" pin="VCCINT_2" pad="F5"/>
<connect gate="A" pin="VCCINT_3" pad="F7"/>
<connect gate="A" pin="VCCINT_4" pad="F9"/>
<connect gate="A" pin="VCCINT_5" pad="H6"/>
<connect gate="A" pin="VCCINT_6" pad="H7"/>
<connect gate="A" pin="VCCIO" pad="J6"/>
<connect gate="A" pin="VCCIO_2" pad="E6"/>
<connect gate="A" pin="VCCIO_3" pad="F8"/>
<connect gate="A" pin="VCCIO_4" pad="G6"/>
<connect gate="A" pin="VCCIO_5" pad="G8"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="L8"/>
<connect gate="B" pin="CONF_DONE" pad="C15"/>
<connect gate="B" pin="GNDINT" pad="A14"/>
<connect gate="B" pin="GNDINT_2" pad="K7"/>
<connect gate="B" pin="GNDINT_3" pad="L1"/>
<connect gate="B" pin="GNDINT_4" pad="L6"/>
<connect gate="B" pin="GNDINT_5" pad="M5"/>
<connect gate="B" pin="GND_CKLK" pad="T8"/>
<connect gate="B" pin="INPUT" pad="R8"/>
<connect gate="B" pin="INPUT_2" pad="M9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/CLKUSR" pad="D15"/>
<connect gate="B" pin="IO/CS" pad="A15"/>
<connect gate="B" pin="IO/NCS" pad="A16"/>
<connect gate="B" pin="IO/NRS" pad="C14"/>
<connect gate="B" pin="IO/NWS" pad="B14"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="N7"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="N9"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="L3"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="P8"/>
<connect gate="B" pin="IO_24" pad="P9"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M1"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T1"/>
<connect gate="B" pin="IO_32" pad="T2"/>
<connect gate="B" pin="IO_33" pad="T3"/>
<connect gate="B" pin="IO_34" pad="T4"/>
<connect gate="B" pin="IO_35" pad="T5"/>
<connect gate="B" pin="IO_36" pad="T6"/>
<connect gate="B" pin="IO_37" pad="T7"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="A10"/>
<connect gate="B" pin="IO_4" pad="M2"/>
<connect gate="B" pin="IO_40" pad="A11"/>
<connect gate="B" pin="IO_41" pad="A12"/>
<connect gate="B" pin="IO_42" pad="A13"/>
<connect gate="B" pin="IO_43" pad="B10"/>
<connect gate="B" pin="IO_44" pad="B11"/>
<connect gate="B" pin="IO_45" pad="B12"/>
<connect gate="B" pin="IO_46" pad="B13"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="C13"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_6" pad="M4"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="MSEL0" pad="P1"/>
<connect gate="B" pin="MSEL1" pad="R1"/>
<connect gate="B" pin="NC" pad="L4"/>
<connect gate="B" pin="NCEO" pad="B16"/>
<connect gate="B" pin="NCONFIG" pad="N4"/>
<connect gate="B" pin="NC_2" pad="L2"/>
<connect gate="B" pin="TCK" pad="B15"/>
<connect gate="B" pin="TDO" pad="C16"/>
<connect gate="B" pin="VCCINT" pad="R2"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="L5"/>
<connect gate="B" pin="VCCINT_4" pad="L7"/>
<connect gate="B" pin="VCCIO" pad="D12"/>
<connect gate="B" pin="VCCIO_2" pad="K6"/>
<connect gate="B" pin="VCCIO_3" pad="K8"/>
<connect gate="B" pin="VCCIO_4" pad="M6"/>
<connect gate="B" pin="VCC_CKLK" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="M12"/>
<connect gate="C" pin="GNDINT_2" pad="E12"/>
<connect gate="C" pin="GNDINT_3" pad="F11"/>
<connect gate="C" pin="GNDINT_4" pad="G10"/>
<connect gate="C" pin="GNDINT_5" pad="K10"/>
<connect gate="C" pin="GNDINT_6" pad="L11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/INIT_DONE" pad="G16"/>
<connect gate="C" pin="IO/LOCK" pad="P12"/>
<connect gate="C" pin="IO/RDY/NBUSY" pad="G14"/>
<connect gate="C" pin="IO_10" pad="G12"/>
<connect gate="C" pin="IO_11" pad="G13"/>
<connect gate="C" pin="IO_12" pad="G15"/>
<connect gate="C" pin="IO_13" pad="H12"/>
<connect gate="C" pin="IO_14" pad="H13"/>
<connect gate="C" pin="IO_15" pad="H14"/>
<connect gate="C" pin="IO_16" pad="H15"/>
<connect gate="C" pin="IO_17" pad="J12"/>
<connect gate="C" pin="IO_18" pad="J13"/>
<connect gate="C" pin="IO_19" pad="J14"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="J15"/>
<connect gate="C" pin="IO_21" pad="J16"/>
<connect gate="C" pin="IO_22" pad="K12"/>
<connect gate="C" pin="IO_23" pad="K13"/>
<connect gate="C" pin="IO_24" pad="K15"/>
<connect gate="C" pin="IO_25" pad="L13"/>
<connect gate="C" pin="IO_26" pad="L14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="L16"/>
<connect gate="C" pin="IO_29" pad="M10"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="M13"/>
<connect gate="C" pin="IO_31" pad="M15"/>
<connect gate="C" pin="IO_32" pad="N10"/>
<connect gate="C" pin="IO_33" pad="N11"/>
<connect gate="C" pin="IO_34" pad="N13"/>
<connect gate="C" pin="IO_35" pad="N14"/>
<connect gate="C" pin="IO_36" pad="N16"/>
<connect gate="C" pin="IO_37" pad="P10"/>
<connect gate="C" pin="IO_38" pad="P11"/>
<connect gate="C" pin="IO_39" pad="P13"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="P14"/>
<connect gate="C" pin="IO_41" pad="P16"/>
<connect gate="C" pin="IO_42" pad="R10"/>
<connect gate="C" pin="IO_43" pad="R11"/>
<connect gate="C" pin="IO_44" pad="R12"/>
<connect gate="C" pin="IO_45" pad="R13"/>
<connect gate="C" pin="IO_46" pad="R14"/>
<connect gate="C" pin="IO_47" pad="R15"/>
<connect gate="C" pin="IO_48" pad="T10"/>
<connect gate="C" pin="IO_49" pad="T11"/>
<connect gate="C" pin="IO_5" pad="E15"/>
<connect gate="C" pin="IO_50" pad="T12"/>
<connect gate="C" pin="IO_51" pad="T13"/>
<connect gate="C" pin="IO_52" pad="T14"/>
<connect gate="C" pin="IO_6" pad="F13"/>
<connect gate="C" pin="IO_7" pad="F14"/>
<connect gate="C" pin="IO_8" pad="F15"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="N15"/>
<connect gate="C" pin="NC_2" pad="E16"/>
<connect gate="C" pin="NC_3" pad="H16"/>
<connect gate="C" pin="NC_4" pad="K14"/>
<connect gate="C" pin="NC_5" pad="K16"/>
<connect gate="C" pin="NC_6" pad="M14"/>
<connect gate="C" pin="NC_7" pad="M16"/>
<connect gate="C" pin="NSTATUS" pad="T16"/>
<connect gate="C" pin="TMS" pad="P15"/>
<connect gate="C" pin="TRST" pad="R16"/>
<connect gate="C" pin="VCCINT" pad="M11"/>
<connect gate="C" pin="VCCINT_2" pad="E11"/>
<connect gate="C" pin="VCCINT_3" pad="F12"/>
<connect gate="C" pin="VCCINT_4" pad="H10"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="J11"/>
<connect gate="C" pin="VCCINT_7" pad="L12"/>
<connect gate="C" pin="VCCIO" pad="N12"/>
<connect gate="C" pin="VCCIO_2" pad="F10"/>
<connect gate="C" pin="VCCIO_3" pad="G11"/>
<connect gate="C" pin="VCCIO_4" pad="H11"/>
<connect gate="C" pin="VCCIO_5" pad="K11"/>
<connect gate="C" pin="VCCIO_6" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K30FC256-1N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0142"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K30FI256-2N">
<description>IC ACEX 1K FPGA</description>
<gates>
<gate name="A" symbol="EP1K30FI256-2N_A"/>
<gate name="B" symbol="EP1K30FI256-2N_B"/>
<gate name="C" symbol="EP1K30FI256-2N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16X_1700X1700X22">
<connects>
<connect gate="A" pin="CLOCK" pad="A9"/>
<connect gate="A" pin="DATA0" pad="A1"/>
<connect gate="A" pin="DCLK" pad="B2"/>
<connect gate="A" pin="GNDINT" pad="K5"/>
<connect gate="A" pin="GNDINT_10" pad="J8"/>
<connect gate="A" pin="GNDINT_11" pad="J9"/>
<connect gate="A" pin="GNDINT_2" pad="A3"/>
<connect gate="A" pin="GNDINT_3" pad="C7"/>
<connect gate="A" pin="GNDINT_4" pad="E5"/>
<connect gate="A" pin="GNDINT_5" pad="F6"/>
<connect gate="A" pin="GNDINT_6" pad="G7"/>
<connect gate="A" pin="GNDINT_7" pad="G9"/>
<connect gate="A" pin="GNDINT_8" pad="H8"/>
<connect gate="A" pin="GNDINT_9" pad="H9"/>
<connect gate="A" pin="INPUT" pad="E8"/>
<connect gate="A" pin="INPUT_2" pad="B9"/>
<connect gate="A" pin="IO" pad="K4"/>
<connect gate="A" pin="IO/DATA1" pad="B3"/>
<connect gate="A" pin="IO/DATA2" pad="A2"/>
<connect gate="A" pin="IO/DATA3" pad="C3"/>
<connect gate="A" pin="IO/DATA4" pad="B4"/>
<connect gate="A" pin="IO/DATA5" pad="A4"/>
<connect gate="A" pin="IO/DATA6" pad="D4"/>
<connect gate="A" pin="IO/DATA7" pad="B5"/>
<connect gate="A" pin="IO/DEV_NCLR" pad="D8"/>
<connect gate="A" pin="IO/DEV_OE" pad="C9"/>
<connect gate="A" pin="IO_10" pad="C4"/>
<connect gate="A" pin="IO_11" pad="C5"/>
<connect gate="A" pin="IO_12" pad="C6"/>
<connect gate="A" pin="IO_13" pad="C8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="D3"/>
<connect gate="A" pin="IO_16" pad="D5"/>
<connect gate="A" pin="IO_17" pad="D6"/>
<connect gate="A" pin="IO_18" pad="D7"/>
<connect gate="A" pin="IO_19" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="E1"/>
<connect gate="A" pin="IO_21" pad="E2"/>
<connect gate="A" pin="IO_22" pad="E4"/>
<connect gate="A" pin="IO_23" pad="E7"/>
<connect gate="A" pin="IO_24" pad="E9"/>
<connect gate="A" pin="IO_25" pad="F1"/>
<connect gate="A" pin="IO_26" pad="F2"/>
<connect gate="A" pin="IO_27" pad="F3"/>
<connect gate="A" pin="IO_28" pad="F4"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G4"/>
<connect gate="A" pin="IO_32" pad="G5"/>
<connect gate="A" pin="IO_33" pad="H2"/>
<connect gate="A" pin="IO_34" pad="H3"/>
<connect gate="A" pin="IO_35" pad="H4"/>
<connect gate="A" pin="IO_36" pad="H5"/>
<connect gate="A" pin="IO_37" pad="J2"/>
<connect gate="A" pin="IO_38" pad="J3"/>
<connect gate="A" pin="IO_39" pad="J4"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="J5"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_7" pad="B7"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="C1"/>
<connect gate="A" pin="NC" pad="K3"/>
<connect gate="A" pin="NCE" pad="B1"/>
<connect gate="A" pin="NC_2" pad="D1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="G3"/>
<connect gate="A" pin="NC_5" pad="H1"/>
<connect gate="A" pin="NC_6" pad="J1"/>
<connect gate="A" pin="TDI" pad="C2"/>
<connect gate="A" pin="VCCINT" pad="J7"/>
<connect gate="A" pin="VCCINT_2" pad="F5"/>
<connect gate="A" pin="VCCINT_3" pad="F7"/>
<connect gate="A" pin="VCCINT_4" pad="F9"/>
<connect gate="A" pin="VCCINT_5" pad="H6"/>
<connect gate="A" pin="VCCINT_6" pad="H7"/>
<connect gate="A" pin="VCCIO" pad="J6"/>
<connect gate="A" pin="VCCIO_2" pad="E6"/>
<connect gate="A" pin="VCCIO_3" pad="F8"/>
<connect gate="A" pin="VCCIO_4" pad="G6"/>
<connect gate="A" pin="VCCIO_5" pad="G8"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="L8"/>
<connect gate="B" pin="CONF_DONE" pad="C15"/>
<connect gate="B" pin="GNDINT" pad="A14"/>
<connect gate="B" pin="GNDINT_2" pad="K7"/>
<connect gate="B" pin="GNDINT_3" pad="L1"/>
<connect gate="B" pin="GNDINT_4" pad="L6"/>
<connect gate="B" pin="GNDINT_5" pad="M5"/>
<connect gate="B" pin="GND_CKLK" pad="T8"/>
<connect gate="B" pin="INPUT" pad="R8"/>
<connect gate="B" pin="INPUT_2" pad="M9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/CLKUSR" pad="D15"/>
<connect gate="B" pin="IO/CS" pad="A15"/>
<connect gate="B" pin="IO/NCS" pad="A16"/>
<connect gate="B" pin="IO/NRS" pad="C14"/>
<connect gate="B" pin="IO/NWS" pad="B14"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="N7"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="N9"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="L3"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="P8"/>
<connect gate="B" pin="IO_24" pad="P9"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M1"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T1"/>
<connect gate="B" pin="IO_32" pad="T2"/>
<connect gate="B" pin="IO_33" pad="T3"/>
<connect gate="B" pin="IO_34" pad="T4"/>
<connect gate="B" pin="IO_35" pad="T5"/>
<connect gate="B" pin="IO_36" pad="T6"/>
<connect gate="B" pin="IO_37" pad="T7"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="A10"/>
<connect gate="B" pin="IO_4" pad="M2"/>
<connect gate="B" pin="IO_40" pad="A11"/>
<connect gate="B" pin="IO_41" pad="A12"/>
<connect gate="B" pin="IO_42" pad="A13"/>
<connect gate="B" pin="IO_43" pad="B10"/>
<connect gate="B" pin="IO_44" pad="B11"/>
<connect gate="B" pin="IO_45" pad="B12"/>
<connect gate="B" pin="IO_46" pad="B13"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="C13"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_6" pad="M4"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="MSEL0" pad="P1"/>
<connect gate="B" pin="MSEL1" pad="R1"/>
<connect gate="B" pin="NC" pad="L4"/>
<connect gate="B" pin="NCEO" pad="B16"/>
<connect gate="B" pin="NCONFIG" pad="N4"/>
<connect gate="B" pin="NC_2" pad="L2"/>
<connect gate="B" pin="TCK" pad="B15"/>
<connect gate="B" pin="TDO" pad="C16"/>
<connect gate="B" pin="VCCINT" pad="R2"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="L5"/>
<connect gate="B" pin="VCCINT_4" pad="L7"/>
<connect gate="B" pin="VCCIO" pad="D12"/>
<connect gate="B" pin="VCCIO_2" pad="K6"/>
<connect gate="B" pin="VCCIO_3" pad="K8"/>
<connect gate="B" pin="VCCIO_4" pad="M6"/>
<connect gate="B" pin="VCC_CKLK" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="M12"/>
<connect gate="C" pin="GNDINT_2" pad="E12"/>
<connect gate="C" pin="GNDINT_3" pad="F11"/>
<connect gate="C" pin="GNDINT_4" pad="G10"/>
<connect gate="C" pin="GNDINT_5" pad="K10"/>
<connect gate="C" pin="GNDINT_6" pad="L11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/INIT_DONE" pad="G16"/>
<connect gate="C" pin="IO/LOCK" pad="P12"/>
<connect gate="C" pin="IO/RDY/NBUSY" pad="G14"/>
<connect gate="C" pin="IO_10" pad="G12"/>
<connect gate="C" pin="IO_11" pad="G13"/>
<connect gate="C" pin="IO_12" pad="G15"/>
<connect gate="C" pin="IO_13" pad="H12"/>
<connect gate="C" pin="IO_14" pad="H13"/>
<connect gate="C" pin="IO_15" pad="H14"/>
<connect gate="C" pin="IO_16" pad="H15"/>
<connect gate="C" pin="IO_17" pad="J12"/>
<connect gate="C" pin="IO_18" pad="J13"/>
<connect gate="C" pin="IO_19" pad="J14"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="J15"/>
<connect gate="C" pin="IO_21" pad="J16"/>
<connect gate="C" pin="IO_22" pad="K12"/>
<connect gate="C" pin="IO_23" pad="K13"/>
<connect gate="C" pin="IO_24" pad="K15"/>
<connect gate="C" pin="IO_25" pad="L13"/>
<connect gate="C" pin="IO_26" pad="L14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="L16"/>
<connect gate="C" pin="IO_29" pad="M10"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="M13"/>
<connect gate="C" pin="IO_31" pad="M15"/>
<connect gate="C" pin="IO_32" pad="N10"/>
<connect gate="C" pin="IO_33" pad="N11"/>
<connect gate="C" pin="IO_34" pad="N13"/>
<connect gate="C" pin="IO_35" pad="N14"/>
<connect gate="C" pin="IO_36" pad="N16"/>
<connect gate="C" pin="IO_37" pad="P10"/>
<connect gate="C" pin="IO_38" pad="P11"/>
<connect gate="C" pin="IO_39" pad="P13"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="P14"/>
<connect gate="C" pin="IO_41" pad="P16"/>
<connect gate="C" pin="IO_42" pad="R10"/>
<connect gate="C" pin="IO_43" pad="R11"/>
<connect gate="C" pin="IO_44" pad="R12"/>
<connect gate="C" pin="IO_45" pad="R13"/>
<connect gate="C" pin="IO_46" pad="R14"/>
<connect gate="C" pin="IO_47" pad="R15"/>
<connect gate="C" pin="IO_48" pad="T10"/>
<connect gate="C" pin="IO_49" pad="T11"/>
<connect gate="C" pin="IO_5" pad="E15"/>
<connect gate="C" pin="IO_50" pad="T12"/>
<connect gate="C" pin="IO_51" pad="T13"/>
<connect gate="C" pin="IO_52" pad="T14"/>
<connect gate="C" pin="IO_6" pad="F13"/>
<connect gate="C" pin="IO_7" pad="F14"/>
<connect gate="C" pin="IO_8" pad="F15"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="N15"/>
<connect gate="C" pin="NC_2" pad="E16"/>
<connect gate="C" pin="NC_3" pad="H16"/>
<connect gate="C" pin="NC_4" pad="K14"/>
<connect gate="C" pin="NC_5" pad="K16"/>
<connect gate="C" pin="NC_6" pad="M14"/>
<connect gate="C" pin="NC_7" pad="M16"/>
<connect gate="C" pin="NSTATUS" pad="T16"/>
<connect gate="C" pin="TMS" pad="P15"/>
<connect gate="C" pin="TRST" pad="R16"/>
<connect gate="C" pin="VCCINT" pad="M11"/>
<connect gate="C" pin="VCCINT_2" pad="E11"/>
<connect gate="C" pin="VCCINT_3" pad="F12"/>
<connect gate="C" pin="VCCINT_4" pad="H10"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="J11"/>
<connect gate="C" pin="VCCINT_7" pad="L12"/>
<connect gate="C" pin="VCCIO" pad="N12"/>
<connect gate="C" pin="VCCIO_2" pad="F10"/>
<connect gate="C" pin="VCCIO_3" pad="G11"/>
<connect gate="C" pin="VCCIO_4" pad="H11"/>
<connect gate="C" pin="VCCIO_5" pad="K11"/>
<connect gate="C" pin="VCCIO_6" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K30FI256-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0148"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K30QC208-3N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K30QC208-3N_A"/>
<gate name="B" symbol="EP1K30QC208-3N_B"/>
<gate name="C" symbol="EP1K30QC208-3N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="43"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="20"/>
<connect gate="A" pin="GNDINT_4" pad="23"/>
<connect gate="A" pin="GNDINT_5" pad="32"/>
<connect gate="A" pin="GNDINT_6" pad="59"/>
<connect gate="A" pin="GNDINT_7" pad="35"/>
<connect gate="A" pin="GNDINT_8" pad="49"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/LOCK" pad="62"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="17"/>
<connect gate="A" pin="IO_11" pad="18"/>
<connect gate="A" pin="IO_12" pad="24"/>
<connect gate="A" pin="IO_13" pad="25"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="36"/>
<connect gate="A" pin="IO_21" pad="37"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="44"/>
<connect gate="A" pin="IO_27" pad="45"/>
<connect gate="A" pin="IO_28" pad="46"/>
<connect gate="A" pin="IO_29" pad="47"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="53"/>
<connect gate="A" pin="IO_31" pad="54"/>
<connect gate="A" pin="IO_32" pad="55"/>
<connect gate="A" pin="IO_33" pad="56"/>
<connect gate="A" pin="IO_34" pad="57"/>
<connect gate="A" pin="IO_35" pad="58"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_5" pad="11"/>
<connect gate="A" pin="IO_6" pad="12"/>
<connect gate="A" pin="IO_7" pad="13"/>
<connect gate="A" pin="IO_8" pad="14"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="48"/>
<connect gate="A" pin="VCCINT_2" pad="21"/>
<connect gate="A" pin="VCCINT_3" pad="33"/>
<connect gate="A" pin="VCCIO" pad="5"/>
<connect gate="A" pin="VCCIO_2" pad="42"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="79"/>
<connect gate="B" pin="GNDINT" pad="109"/>
<connect gate="B" pin="GNDINT_2" pad="76"/>
<connect gate="B" pin="GNDINT_3" pad="82"/>
<connect gate="B" pin="GNDINT_4" pad="117"/>
<connect gate="B" pin="GNDINT_5" pad="123"/>
<connect gate="B" pin="GNDINT_6" pad="129"/>
<connect gate="B" pin="GNDINT_7" pad="137"/>
<connect gate="B" pin="GND_CKLK" pad="81"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="114"/>
<connect gate="B" pin="IO_29" pad="115"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="120"/>
<connect gate="B" pin="IO_33" pad="121"/>
<connect gate="B" pin="IO_34" pad="122"/>
<connect gate="B" pin="IO_35" pad="125"/>
<connect gate="B" pin="IO_36" pad="126"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="131"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_40" pad="132"/>
<connect gate="B" pin="IO_41" pad="133"/>
<connect gate="B" pin="IO_42" pad="134"/>
<connect gate="B" pin="IO_43" pad="135"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="91"/>
<connect gate="B" pin="VCCINT_3" pad="106"/>
<connect gate="B" pin="VCCINT_4" pad="72"/>
<connect gate="B" pin="VCCINT_5" pad="124"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="110"/>
<connect gate="B" pin="VCCIO_4" pad="98"/>
<connect gate="B" pin="VCCIO_5" pad="138"/>
<connect gate="B" pin="VCC_CKLK" pad="77"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="188"/>
<connect gate="C" pin="GNDINT_2" pad="145"/>
<connect gate="C" pin="GNDINT_3" pad="151"/>
<connect gate="C" pin="GNDINT_4" pad="171"/>
<connect gate="C" pin="GNDINT_5" pad="181"/>
<connect gate="C" pin="INPUT" pad="182"/>
<connect gate="C" pin="INPUT_2" pad="184"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_CLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="172"/>
<connect gate="C" pin="IO_11" pad="144"/>
<connect gate="C" pin="IO_12" pad="173"/>
<connect gate="C" pin="IO_13" pad="147"/>
<connect gate="C" pin="IO_14" pad="174"/>
<connect gate="C" pin="IO_15" pad="148"/>
<connect gate="C" pin="IO_16" pad="175"/>
<connect gate="C" pin="IO_17" pad="160"/>
<connect gate="C" pin="IO_18" pad="176"/>
<connect gate="C" pin="IO_19" pad="149"/>
<connect gate="C" pin="IO_2" pad="167"/>
<connect gate="C" pin="IO_20" pad="177"/>
<connect gate="C" pin="IO_21" pad="150"/>
<connect gate="C" pin="IO_22" pad="179"/>
<connect gate="C" pin="IO_23" pad="187"/>
<connect gate="C" pin="IO_24" pad="189"/>
<connect gate="C" pin="IO_25" pad="205"/>
<connect gate="C" pin="IO_26" pad="190"/>
<connect gate="C" pin="IO_27" pad="191"/>
<connect gate="C" pin="IO_28" pad="192"/>
<connect gate="C" pin="IO_29" pad="193"/>
<connect gate="C" pin="IO_3" pad="163"/>
<connect gate="C" pin="IO_30" pad="195"/>
<connect gate="C" pin="IO_31" pad="196"/>
<connect gate="C" pin="IO_32" pad="197"/>
<connect gate="C" pin="IO_33" pad="198"/>
<connect gate="C" pin="IO_34" pad="199"/>
<connect gate="C" pin="IO_35" pad="200"/>
<connect gate="C" pin="IO_36" pad="202"/>
<connect gate="C" pin="IO_4" pad="168"/>
<connect gate="C" pin="IO_5" pad="141"/>
<connect gate="C" pin="IO_6" pad="169"/>
<connect gate="C" pin="IO_7" pad="142"/>
<connect gate="C" pin="IO_8" pad="170"/>
<connect gate="C" pin="IO_9" pad="143"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="185"/>
<connect gate="C" pin="VCCINT_2" pad="152"/>
<connect gate="C" pin="VCCINT_3" pad="201"/>
<connect gate="C" pin="VCCIO" pad="165"/>
<connect gate="C" pin="VCCIO_2" pad="194"/>
<connect gate="C" pin="VCCIO_3" pad="146"/>
<connect gate="C" pin="VCCIO_4" pad="178"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K30QC208-3N"/>
<attribute name="OC_FARNELL" value="1662257"/>
<attribute name="OC_NEWARK" value="51R0553"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K30TC144-3N" prefix="U">
<description>IC ACEX 1K FPGA 30K 144-TQFP</description>
<gates>
<gate name="A" symbol="EP1K30TC144-3N_A"/>
<gate name="B" symbol="EP1K30TC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="*CEO" pad="3"/>
<connect gate="A" pin="*STATUS" pad="35"/>
<connect gate="A" pin="CLOCK/GCLK1" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="40"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="15"/>
<connect gate="A" pin="GNDINT_4" pad="66"/>
<connect gate="A" pin="GNDINT_5" pad="25"/>
<connect gate="A" pin="GNDINT_6" pad="58"/>
<connect gate="A" pin="GNDINT_7" pad="52"/>
<connect gate="A" pin="GND_CKLK" pad="57"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="23"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/LOCK" pad="42"/>
<connect gate="A" pin="IO/RDY/*BUSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="29"/>
<connect gate="A" pin="IO_11" pad="30"/>
<connect gate="A" pin="IO_12" pad="31"/>
<connect gate="A" pin="IO_13" pad="32"/>
<connect gate="A" pin="IO_14" pad="33"/>
<connect gate="A" pin="IO_15" pad="36"/>
<connect gate="A" pin="IO_16" pad="37"/>
<connect gate="A" pin="IO_17" pad="38"/>
<connect gate="A" pin="IO_18" pad="39"/>
<connect gate="A" pin="IO_19" pad="41"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="43"/>
<connect gate="A" pin="IO_21" pad="44"/>
<connect gate="A" pin="IO_22" pad="46"/>
<connect gate="A" pin="IO_23" pad="47"/>
<connect gate="A" pin="IO_24" pad="48"/>
<connect gate="A" pin="IO_25" pad="49"/>
<connect gate="A" pin="IO_26" pad="51"/>
<connect gate="A" pin="IO_27" pad="59"/>
<connect gate="A" pin="IO_28" pad="60"/>
<connect gate="A" pin="IO_29" pad="62"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="63"/>
<connect gate="A" pin="IO_31" pad="64"/>
<connect gate="A" pin="IO_32" pad="65"/>
<connect gate="A" pin="IO_33" pad="67"/>
<connect gate="A" pin="IO_34" pad="68"/>
<connect gate="A" pin="IO_35" pad="69"/>
<connect gate="A" pin="IO_36" pad="70"/>
<connect gate="A" pin="IO_37" pad="72"/>
<connect gate="A" pin="IO_38" pad="17"/>
<connect gate="A" pin="IO_39" pad="18"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="19"/>
<connect gate="A" pin="IO_41" pad="20"/>
<connect gate="A" pin="IO_42" pad="21"/>
<connect gate="A" pin="IO_43" pad="22"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="26"/>
<connect gate="A" pin="IO_8" pad="27"/>
<connect gate="A" pin="IO_9" pad="28"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="16"/>
<connect gate="A" pin="VCCINT_2" pad="50"/>
<connect gate="A" pin="VCCIO" pad="5"/>
<connect gate="A" pin="VCCIO_2" pad="61"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="45"/>
<connect gate="A" pin="VCCIO_5" pad="71"/>
<connect gate="A" pin="VCC_CKLK" pad="53"/>
<connect gate="B" pin="*CE" pad="106"/>
<connect gate="B" pin="*CONFIG" pad="74"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="93"/>
<connect gate="B" pin="GNDINT_2" pad="123"/>
<connect gate="B" pin="GNDINT_3" pad="129"/>
<connect gate="B" pin="GNDINT_4" pad="139"/>
<connect gate="B" pin="GNDINT_5" pad="104"/>
<connect gate="B" pin="GNDINT_6" pad="84"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/*CS" pad="144"/>
<connect gate="B" pin="IO/*DEV_CLR" pad="122"/>
<connect gate="B" pin="IO/*RS" pad="141"/>
<connect gate="B" pin="IO/*WS" pad="142"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO_10" pad="96"/>
<connect gate="B" pin="IO_11" pad="97"/>
<connect gate="B" pin="IO_12" pad="98"/>
<connect gate="B" pin="IO_13" pad="99"/>
<connect gate="B" pin="IO_14" pad="100"/>
<connect gate="B" pin="IO_15" pad="101"/>
<connect gate="B" pin="IO_16" pad="102"/>
<connect gate="B" pin="IO_17" pad="117"/>
<connect gate="B" pin="IO_18" pad="118"/>
<connect gate="B" pin="IO_19" pad="119"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="120"/>
<connect gate="B" pin="IO_21" pad="121"/>
<connect gate="B" pin="IO_22" pad="130"/>
<connect gate="B" pin="IO_23" pad="131"/>
<connect gate="B" pin="IO_24" pad="132"/>
<connect gate="B" pin="IO_25" pad="133"/>
<connect gate="B" pin="IO_26" pad="135"/>
<connect gate="B" pin="IO_27" pad="136"/>
<connect gate="B" pin="IO_28" pad="137"/>
<connect gate="B" pin="IO_29" pad="138"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="86"/>
<connect gate="B" pin="IO_31" pad="87"/>
<connect gate="B" pin="IO_32" pad="88"/>
<connect gate="B" pin="IO_33" pad="89"/>
<connect gate="B" pin="IO_34" pad="90"/>
<connect gate="B" pin="IO_35" pad="91"/>
<connect gate="B" pin="IO_36" pad="92"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="95"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="127"/>
<connect gate="B" pin="VCCINT_2" pad="103"/>
<connect gate="B" pin="VCCINT_3" pad="75"/>
<connect gate="B" pin="VCCINT_4" pad="85"/>
<connect gate="B" pin="VCCIO" pad="94"/>
<connect gate="B" pin="VCCIO_2" pad="134"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K30TC144-3N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R0554"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K30TI144-2N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K30TI144-2N_A"/>
<gate name="B" symbol="EP1K30TI144-2N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK/GCLK" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="66"/>
<connect gate="A" pin="GNDINT_2" pad="40"/>
<connect gate="A" pin="GNDINT_3" pad="6"/>
<connect gate="A" pin="GNDINT_4" pad="15"/>
<connect gate="A" pin="GNDINT_5" pad="25"/>
<connect gate="A" pin="GNDINT_6" pad="52"/>
<connect gate="A" pin="GNDINT_7" pad="58"/>
<connect gate="A" pin="GND_CKLK" pad="57"/>
<connect gate="A" pin="INPUT" pad="54"/>
<connect gate="A" pin="INPUT_2" pad="56"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/LOCK" pad="42"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="43"/>
<connect gate="A" pin="IO_28" pad="44"/>
<connect gate="A" pin="IO_29" pad="46"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="47"/>
<connect gate="A" pin="IO_31" pad="48"/>
<connect gate="A" pin="IO_32" pad="49"/>
<connect gate="A" pin="IO_33" pad="51"/>
<connect gate="A" pin="IO_34" pad="59"/>
<connect gate="A" pin="IO_35" pad="60"/>
<connect gate="A" pin="IO_36" pad="62"/>
<connect gate="A" pin="IO_37" pad="63"/>
<connect gate="A" pin="IO_38" pad="64"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="50"/>
<connect gate="A" pin="VCCINT_2" pad="16"/>
<connect gate="A" pin="VCCIO" pad="5"/>
<connect gate="A" pin="VCCIO_2" pad="45"/>
<connect gate="A" pin="VCCIO_3" pad="61"/>
<connect gate="A" pin="VCCIO_4" pad="24"/>
<connect gate="A" pin="VCCIO_5" pad="71"/>
<connect gate="A" pin="VCC_CKLK" pad="53"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="129"/>
<connect gate="B" pin="GNDINT_2" pad="84"/>
<connect gate="B" pin="GNDINT_3" pad="93"/>
<connect gate="B" pin="GNDINT_4" pad="104"/>
<connect gate="B" pin="GNDINT_5" pad="123"/>
<connect gate="B" pin="GNDINT_6" pad="139"/>
<connect gate="B" pin="INPUT" pad="124"/>
<connect gate="B" pin="INPUT_2" pad="126"/>
<connect gate="B" pin="IO" pad="102"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NDEV_CLR" pad="122"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO/RS" pad="141"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="130"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="131"/>
<connect gate="B" pin="IO_16" pad="117"/>
<connect gate="B" pin="IO_17" pad="132"/>
<connect gate="B" pin="IO_18" pad="91"/>
<connect gate="B" pin="IO_19" pad="133"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="118"/>
<connect gate="B" pin="IO_21" pad="135"/>
<connect gate="B" pin="IO_22" pad="92"/>
<connect gate="B" pin="IO_23" pad="136"/>
<connect gate="B" pin="IO_24" pad="119"/>
<connect gate="B" pin="IO_25" pad="137"/>
<connect gate="B" pin="IO_26" pad="95"/>
<connect gate="B" pin="IO_27" pad="138"/>
<connect gate="B" pin="IO_28" pad="120"/>
<connect gate="B" pin="IO_29" pad="140"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="96"/>
<connect gate="B" pin="IO_31" pad="121"/>
<connect gate="B" pin="IO_32" pad="97"/>
<connect gate="B" pin="IO_33" pad="98"/>
<connect gate="B" pin="IO_34" pad="99"/>
<connect gate="B" pin="IO_35" pad="100"/>
<connect gate="B" pin="IO_36" pad="101"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="103"/>
<connect gate="B" pin="VCCINT_2" pad="127"/>
<connect gate="B" pin="VCCINT_3" pad="75"/>
<connect gate="B" pin="VCCINT_4" pad="85"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K30TI144-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0162"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K50FC256-1N">
<description>IC ACEX 1K FPGA</description>
<gates>
<gate name="A" symbol="EP1K50FC256-1N_A"/>
<gate name="B" symbol="EP1K50FC256-1N_B"/>
<gate name="C" symbol="EP1K50FC256-1N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16X_1700X1700X22">
<connects>
<connect gate="A" pin="CLOCK" pad="A9"/>
<connect gate="A" pin="DATA0" pad="A1"/>
<connect gate="A" pin="DCLK" pad="B2"/>
<connect gate="A" pin="GNDINT" pad="K5"/>
<connect gate="A" pin="GNDINT_10" pad="J8"/>
<connect gate="A" pin="GNDINT_11" pad="J9"/>
<connect gate="A" pin="GNDINT_2" pad="A3"/>
<connect gate="A" pin="GNDINT_3" pad="C7"/>
<connect gate="A" pin="GNDINT_4" pad="E5"/>
<connect gate="A" pin="GNDINT_5" pad="F6"/>
<connect gate="A" pin="GNDINT_6" pad="G7"/>
<connect gate="A" pin="GNDINT_7" pad="G9"/>
<connect gate="A" pin="GNDINT_8" pad="H8"/>
<connect gate="A" pin="GNDINT_9" pad="H9"/>
<connect gate="A" pin="INPUT" pad="E8"/>
<connect gate="A" pin="INPUT_2" pad="B9"/>
<connect gate="A" pin="IO" pad="K4"/>
<connect gate="A" pin="IO/DATA1" pad="B3"/>
<connect gate="A" pin="IO/DATA2" pad="A2"/>
<connect gate="A" pin="IO/DATA3" pad="C3"/>
<connect gate="A" pin="IO/DATA4" pad="B4"/>
<connect gate="A" pin="IO/DATA5" pad="A4"/>
<connect gate="A" pin="IO/DATA6" pad="D4"/>
<connect gate="A" pin="IO/DATA7" pad="B5"/>
<connect gate="A" pin="IO/DEV_NCLR" pad="D8"/>
<connect gate="A" pin="IO/DEV_OE" pad="C9"/>
<connect gate="A" pin="IO_10" pad="C4"/>
<connect gate="A" pin="IO_11" pad="C5"/>
<connect gate="A" pin="IO_12" pad="C6"/>
<connect gate="A" pin="IO_13" pad="C8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="D3"/>
<connect gate="A" pin="IO_16" pad="D5"/>
<connect gate="A" pin="IO_17" pad="D6"/>
<connect gate="A" pin="IO_18" pad="D7"/>
<connect gate="A" pin="IO_19" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="E1"/>
<connect gate="A" pin="IO_21" pad="E2"/>
<connect gate="A" pin="IO_22" pad="E4"/>
<connect gate="A" pin="IO_23" pad="E7"/>
<connect gate="A" pin="IO_24" pad="E9"/>
<connect gate="A" pin="IO_25" pad="F1"/>
<connect gate="A" pin="IO_26" pad="F2"/>
<connect gate="A" pin="IO_27" pad="F3"/>
<connect gate="A" pin="IO_28" pad="F4"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G4"/>
<connect gate="A" pin="IO_32" pad="G5"/>
<connect gate="A" pin="IO_33" pad="H2"/>
<connect gate="A" pin="IO_34" pad="H3"/>
<connect gate="A" pin="IO_35" pad="H4"/>
<connect gate="A" pin="IO_36" pad="H5"/>
<connect gate="A" pin="IO_37" pad="J2"/>
<connect gate="A" pin="IO_38" pad="J3"/>
<connect gate="A" pin="IO_39" pad="J4"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="J5"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_7" pad="B7"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="C1"/>
<connect gate="A" pin="NC" pad="K3"/>
<connect gate="A" pin="NCE" pad="B1"/>
<connect gate="A" pin="NC_2" pad="D1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="G3"/>
<connect gate="A" pin="NC_5" pad="H1"/>
<connect gate="A" pin="NC_6" pad="J1"/>
<connect gate="A" pin="TDI" pad="C2"/>
<connect gate="A" pin="VCCINT" pad="J7"/>
<connect gate="A" pin="VCCINT_2" pad="F5"/>
<connect gate="A" pin="VCCINT_3" pad="F7"/>
<connect gate="A" pin="VCCINT_4" pad="F9"/>
<connect gate="A" pin="VCCINT_5" pad="H6"/>
<connect gate="A" pin="VCCINT_6" pad="H7"/>
<connect gate="A" pin="VCCIO" pad="J6"/>
<connect gate="A" pin="VCCIO_2" pad="E6"/>
<connect gate="A" pin="VCCIO_3" pad="F8"/>
<connect gate="A" pin="VCCIO_4" pad="G6"/>
<connect gate="A" pin="VCCIO_5" pad="G8"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="L8"/>
<connect gate="B" pin="CONF_DONE" pad="C15"/>
<connect gate="B" pin="GNDINT" pad="A14"/>
<connect gate="B" pin="GNDINT_2" pad="K7"/>
<connect gate="B" pin="GNDINT_3" pad="L1"/>
<connect gate="B" pin="GNDINT_4" pad="L6"/>
<connect gate="B" pin="GNDINT_5" pad="M5"/>
<connect gate="B" pin="GND_CKLK" pad="T8"/>
<connect gate="B" pin="INPUT" pad="R8"/>
<connect gate="B" pin="INPUT_2" pad="M9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/CLKUSR" pad="D15"/>
<connect gate="B" pin="IO/CS" pad="A15"/>
<connect gate="B" pin="IO/NCS" pad="A16"/>
<connect gate="B" pin="IO/NRS" pad="C14"/>
<connect gate="B" pin="IO/NWS" pad="B14"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="N7"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="N9"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="L3"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="P8"/>
<connect gate="B" pin="IO_24" pad="P9"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M1"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T1"/>
<connect gate="B" pin="IO_32" pad="T2"/>
<connect gate="B" pin="IO_33" pad="T3"/>
<connect gate="B" pin="IO_34" pad="T4"/>
<connect gate="B" pin="IO_35" pad="T5"/>
<connect gate="B" pin="IO_36" pad="T6"/>
<connect gate="B" pin="IO_37" pad="T7"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="A10"/>
<connect gate="B" pin="IO_4" pad="M2"/>
<connect gate="B" pin="IO_40" pad="A11"/>
<connect gate="B" pin="IO_41" pad="A12"/>
<connect gate="B" pin="IO_42" pad="A13"/>
<connect gate="B" pin="IO_43" pad="B10"/>
<connect gate="B" pin="IO_44" pad="B11"/>
<connect gate="B" pin="IO_45" pad="B12"/>
<connect gate="B" pin="IO_46" pad="B13"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="C13"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_6" pad="M4"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="MSEL0" pad="P1"/>
<connect gate="B" pin="MSEL1" pad="R1"/>
<connect gate="B" pin="NC" pad="L4"/>
<connect gate="B" pin="NCEO" pad="B16"/>
<connect gate="B" pin="NCONFIG" pad="N4"/>
<connect gate="B" pin="NC_2" pad="L2"/>
<connect gate="B" pin="TCK" pad="B15"/>
<connect gate="B" pin="TDO" pad="C16"/>
<connect gate="B" pin="VCCINT" pad="R2"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="L5"/>
<connect gate="B" pin="VCCINT_4" pad="L7"/>
<connect gate="B" pin="VCCIO" pad="D12"/>
<connect gate="B" pin="VCCIO_2" pad="K6"/>
<connect gate="B" pin="VCCIO_3" pad="K8"/>
<connect gate="B" pin="VCCIO_4" pad="M6"/>
<connect gate="B" pin="VCC_CKLK" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="M12"/>
<connect gate="C" pin="GNDINT_2" pad="E12"/>
<connect gate="C" pin="GNDINT_3" pad="F11"/>
<connect gate="C" pin="GNDINT_4" pad="G10"/>
<connect gate="C" pin="GNDINT_5" pad="K10"/>
<connect gate="C" pin="GNDINT_6" pad="L11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/INIT_DONE" pad="G16"/>
<connect gate="C" pin="IO/LOCK" pad="P12"/>
<connect gate="C" pin="IO/RDY/NBUSY" pad="G14"/>
<connect gate="C" pin="IO_10" pad="G12"/>
<connect gate="C" pin="IO_11" pad="G13"/>
<connect gate="C" pin="IO_12" pad="G15"/>
<connect gate="C" pin="IO_13" pad="H12"/>
<connect gate="C" pin="IO_14" pad="H13"/>
<connect gate="C" pin="IO_15" pad="H14"/>
<connect gate="C" pin="IO_16" pad="H15"/>
<connect gate="C" pin="IO_17" pad="J12"/>
<connect gate="C" pin="IO_18" pad="J13"/>
<connect gate="C" pin="IO_19" pad="J14"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="J15"/>
<connect gate="C" pin="IO_21" pad="J16"/>
<connect gate="C" pin="IO_22" pad="K12"/>
<connect gate="C" pin="IO_23" pad="K13"/>
<connect gate="C" pin="IO_24" pad="K15"/>
<connect gate="C" pin="IO_25" pad="L13"/>
<connect gate="C" pin="IO_26" pad="L14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="L16"/>
<connect gate="C" pin="IO_29" pad="M10"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="M13"/>
<connect gate="C" pin="IO_31" pad="M15"/>
<connect gate="C" pin="IO_32" pad="N10"/>
<connect gate="C" pin="IO_33" pad="N11"/>
<connect gate="C" pin="IO_34" pad="N13"/>
<connect gate="C" pin="IO_35" pad="N14"/>
<connect gate="C" pin="IO_36" pad="N16"/>
<connect gate="C" pin="IO_37" pad="P10"/>
<connect gate="C" pin="IO_38" pad="P11"/>
<connect gate="C" pin="IO_39" pad="P13"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="P14"/>
<connect gate="C" pin="IO_41" pad="P16"/>
<connect gate="C" pin="IO_42" pad="R10"/>
<connect gate="C" pin="IO_43" pad="R11"/>
<connect gate="C" pin="IO_44" pad="R12"/>
<connect gate="C" pin="IO_45" pad="R13"/>
<connect gate="C" pin="IO_46" pad="R14"/>
<connect gate="C" pin="IO_47" pad="R15"/>
<connect gate="C" pin="IO_48" pad="T10"/>
<connect gate="C" pin="IO_49" pad="T11"/>
<connect gate="C" pin="IO_5" pad="E15"/>
<connect gate="C" pin="IO_50" pad="T12"/>
<connect gate="C" pin="IO_51" pad="T13"/>
<connect gate="C" pin="IO_52" pad="T14"/>
<connect gate="C" pin="IO_6" pad="F13"/>
<connect gate="C" pin="IO_7" pad="F14"/>
<connect gate="C" pin="IO_8" pad="F15"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="N15"/>
<connect gate="C" pin="NC_2" pad="E16"/>
<connect gate="C" pin="NC_3" pad="H16"/>
<connect gate="C" pin="NC_4" pad="K14"/>
<connect gate="C" pin="NC_5" pad="K16"/>
<connect gate="C" pin="NC_6" pad="M14"/>
<connect gate="C" pin="NC_7" pad="M16"/>
<connect gate="C" pin="NSTATUS" pad="T16"/>
<connect gate="C" pin="TMS" pad="P15"/>
<connect gate="C" pin="TRST" pad="R16"/>
<connect gate="C" pin="VCCINT" pad="M11"/>
<connect gate="C" pin="VCCINT_2" pad="E11"/>
<connect gate="C" pin="VCCINT_3" pad="F12"/>
<connect gate="C" pin="VCCINT_4" pad="H10"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="J11"/>
<connect gate="C" pin="VCCINT_7" pad="L12"/>
<connect gate="C" pin="VCCIO" pad="N12"/>
<connect gate="C" pin="VCCIO_2" pad="F10"/>
<connect gate="C" pin="VCCIO_3" pad="G11"/>
<connect gate="C" pin="VCCIO_4" pad="H11"/>
<connect gate="C" pin="VCCIO_5" pad="K11"/>
<connect gate="C" pin="VCCIO_6" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K50FC256-1N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0164"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K50FI256-2N">
<description>IC ACEX 1K FPGA</description>
<gates>
<gate name="A" symbol="EP1K50FI256-2N_A"/>
<gate name="B" symbol="EP1K50FI256-2N_B"/>
<gate name="C" symbol="EP1K50FI256-2N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16X_1700X1700X22">
<connects>
<connect gate="A" pin="CLOCK" pad="A9"/>
<connect gate="A" pin="DATA0" pad="A1"/>
<connect gate="A" pin="DCLK" pad="B2"/>
<connect gate="A" pin="GNDINT" pad="K5"/>
<connect gate="A" pin="GNDINT_10" pad="J8"/>
<connect gate="A" pin="GNDINT_11" pad="J9"/>
<connect gate="A" pin="GNDINT_2" pad="A3"/>
<connect gate="A" pin="GNDINT_3" pad="C7"/>
<connect gate="A" pin="GNDINT_4" pad="E5"/>
<connect gate="A" pin="GNDINT_5" pad="F6"/>
<connect gate="A" pin="GNDINT_6" pad="G7"/>
<connect gate="A" pin="GNDINT_7" pad="G9"/>
<connect gate="A" pin="GNDINT_8" pad="H8"/>
<connect gate="A" pin="GNDINT_9" pad="H9"/>
<connect gate="A" pin="INPUT" pad="E8"/>
<connect gate="A" pin="INPUT_2" pad="B9"/>
<connect gate="A" pin="IO" pad="K4"/>
<connect gate="A" pin="IO/DATA1" pad="B3"/>
<connect gate="A" pin="IO/DATA2" pad="A2"/>
<connect gate="A" pin="IO/DATA3" pad="C3"/>
<connect gate="A" pin="IO/DATA4" pad="B4"/>
<connect gate="A" pin="IO/DATA5" pad="A4"/>
<connect gate="A" pin="IO/DATA6" pad="D4"/>
<connect gate="A" pin="IO/DATA7" pad="B5"/>
<connect gate="A" pin="IO/DEV_NCLR" pad="D8"/>
<connect gate="A" pin="IO/DEV_OE" pad="C9"/>
<connect gate="A" pin="IO_10" pad="C4"/>
<connect gate="A" pin="IO_11" pad="C5"/>
<connect gate="A" pin="IO_12" pad="C6"/>
<connect gate="A" pin="IO_13" pad="C8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="D3"/>
<connect gate="A" pin="IO_16" pad="D5"/>
<connect gate="A" pin="IO_17" pad="D6"/>
<connect gate="A" pin="IO_18" pad="D7"/>
<connect gate="A" pin="IO_19" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="E1"/>
<connect gate="A" pin="IO_21" pad="E2"/>
<connect gate="A" pin="IO_22" pad="E4"/>
<connect gate="A" pin="IO_23" pad="E7"/>
<connect gate="A" pin="IO_24" pad="E9"/>
<connect gate="A" pin="IO_25" pad="F1"/>
<connect gate="A" pin="IO_26" pad="F2"/>
<connect gate="A" pin="IO_27" pad="F3"/>
<connect gate="A" pin="IO_28" pad="F4"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G4"/>
<connect gate="A" pin="IO_32" pad="G5"/>
<connect gate="A" pin="IO_33" pad="H2"/>
<connect gate="A" pin="IO_34" pad="H3"/>
<connect gate="A" pin="IO_35" pad="H4"/>
<connect gate="A" pin="IO_36" pad="H5"/>
<connect gate="A" pin="IO_37" pad="J2"/>
<connect gate="A" pin="IO_38" pad="J3"/>
<connect gate="A" pin="IO_39" pad="J4"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="J5"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_7" pad="B7"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="C1"/>
<connect gate="A" pin="NC" pad="K3"/>
<connect gate="A" pin="NCE" pad="B1"/>
<connect gate="A" pin="NC_2" pad="D1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="G3"/>
<connect gate="A" pin="NC_5" pad="H1"/>
<connect gate="A" pin="NC_6" pad="J1"/>
<connect gate="A" pin="TDI" pad="C2"/>
<connect gate="A" pin="VCCINT" pad="J7"/>
<connect gate="A" pin="VCCINT_2" pad="F5"/>
<connect gate="A" pin="VCCINT_3" pad="F7"/>
<connect gate="A" pin="VCCINT_4" pad="F9"/>
<connect gate="A" pin="VCCINT_5" pad="H6"/>
<connect gate="A" pin="VCCINT_6" pad="H7"/>
<connect gate="A" pin="VCCIO" pad="J6"/>
<connect gate="A" pin="VCCIO_2" pad="E6"/>
<connect gate="A" pin="VCCIO_3" pad="F8"/>
<connect gate="A" pin="VCCIO_4" pad="G6"/>
<connect gate="A" pin="VCCIO_5" pad="G8"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="L8"/>
<connect gate="B" pin="CONF_DONE" pad="C15"/>
<connect gate="B" pin="GNDINT" pad="A14"/>
<connect gate="B" pin="GNDINT_2" pad="K7"/>
<connect gate="B" pin="GNDINT_3" pad="L1"/>
<connect gate="B" pin="GNDINT_4" pad="L6"/>
<connect gate="B" pin="GNDINT_5" pad="M5"/>
<connect gate="B" pin="GND_CKLK" pad="T8"/>
<connect gate="B" pin="INPUT" pad="R8"/>
<connect gate="B" pin="INPUT_2" pad="M9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/CLKUSR" pad="D15"/>
<connect gate="B" pin="IO/CS" pad="A15"/>
<connect gate="B" pin="IO/NCS" pad="A16"/>
<connect gate="B" pin="IO/NRS" pad="C14"/>
<connect gate="B" pin="IO/NWS" pad="B14"/>
<connect gate="B" pin="IO_10" pad="N2"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="N7"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="N9"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="P4"/>
<connect gate="B" pin="IO_2" pad="L3"/>
<connect gate="B" pin="IO_20" pad="P5"/>
<connect gate="B" pin="IO_21" pad="P6"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="P8"/>
<connect gate="B" pin="IO_24" pad="P9"/>
<connect gate="B" pin="IO_25" pad="R3"/>
<connect gate="B" pin="IO_26" pad="R4"/>
<connect gate="B" pin="IO_27" pad="R5"/>
<connect gate="B" pin="IO_28" pad="R6"/>
<connect gate="B" pin="IO_29" pad="R7"/>
<connect gate="B" pin="IO_3" pad="M1"/>
<connect gate="B" pin="IO_30" pad="R9"/>
<connect gate="B" pin="IO_31" pad="T1"/>
<connect gate="B" pin="IO_32" pad="T2"/>
<connect gate="B" pin="IO_33" pad="T3"/>
<connect gate="B" pin="IO_34" pad="T4"/>
<connect gate="B" pin="IO_35" pad="T5"/>
<connect gate="B" pin="IO_36" pad="T6"/>
<connect gate="B" pin="IO_37" pad="T7"/>
<connect gate="B" pin="IO_38" pad="T9"/>
<connect gate="B" pin="IO_39" pad="A10"/>
<connect gate="B" pin="IO_4" pad="M2"/>
<connect gate="B" pin="IO_40" pad="A11"/>
<connect gate="B" pin="IO_41" pad="A12"/>
<connect gate="B" pin="IO_42" pad="A13"/>
<connect gate="B" pin="IO_43" pad="B10"/>
<connect gate="B" pin="IO_44" pad="B11"/>
<connect gate="B" pin="IO_45" pad="B12"/>
<connect gate="B" pin="IO_46" pad="B13"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="C13"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_6" pad="M4"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_9" pad="N1"/>
<connect gate="B" pin="MSEL0" pad="P1"/>
<connect gate="B" pin="MSEL1" pad="R1"/>
<connect gate="B" pin="NC" pad="L4"/>
<connect gate="B" pin="NCEO" pad="B16"/>
<connect gate="B" pin="NCONFIG" pad="N4"/>
<connect gate="B" pin="NC_2" pad="L2"/>
<connect gate="B" pin="TCK" pad="B15"/>
<connect gate="B" pin="TDO" pad="C16"/>
<connect gate="B" pin="VCCINT" pad="R2"/>
<connect gate="B" pin="VCCINT_2" pad="K9"/>
<connect gate="B" pin="VCCINT_3" pad="L5"/>
<connect gate="B" pin="VCCINT_4" pad="L7"/>
<connect gate="B" pin="VCCIO" pad="D12"/>
<connect gate="B" pin="VCCIO_2" pad="K6"/>
<connect gate="B" pin="VCCIO_3" pad="K8"/>
<connect gate="B" pin="VCCIO_4" pad="M6"/>
<connect gate="B" pin="VCC_CKLK" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="M12"/>
<connect gate="C" pin="GNDINT_2" pad="E12"/>
<connect gate="C" pin="GNDINT_3" pad="F11"/>
<connect gate="C" pin="GNDINT_4" pad="G10"/>
<connect gate="C" pin="GNDINT_5" pad="K10"/>
<connect gate="C" pin="GNDINT_6" pad="L11"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/INIT_DONE" pad="G16"/>
<connect gate="C" pin="IO/LOCK" pad="P12"/>
<connect gate="C" pin="IO/RDY/NBUSY" pad="G14"/>
<connect gate="C" pin="IO_10" pad="G12"/>
<connect gate="C" pin="IO_11" pad="G13"/>
<connect gate="C" pin="IO_12" pad="G15"/>
<connect gate="C" pin="IO_13" pad="H12"/>
<connect gate="C" pin="IO_14" pad="H13"/>
<connect gate="C" pin="IO_15" pad="H14"/>
<connect gate="C" pin="IO_16" pad="H15"/>
<connect gate="C" pin="IO_17" pad="J12"/>
<connect gate="C" pin="IO_18" pad="J13"/>
<connect gate="C" pin="IO_19" pad="J14"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="J15"/>
<connect gate="C" pin="IO_21" pad="J16"/>
<connect gate="C" pin="IO_22" pad="K12"/>
<connect gate="C" pin="IO_23" pad="K13"/>
<connect gate="C" pin="IO_24" pad="K15"/>
<connect gate="C" pin="IO_25" pad="L13"/>
<connect gate="C" pin="IO_26" pad="L14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="L16"/>
<connect gate="C" pin="IO_29" pad="M10"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="M13"/>
<connect gate="C" pin="IO_31" pad="M15"/>
<connect gate="C" pin="IO_32" pad="N10"/>
<connect gate="C" pin="IO_33" pad="N11"/>
<connect gate="C" pin="IO_34" pad="N13"/>
<connect gate="C" pin="IO_35" pad="N14"/>
<connect gate="C" pin="IO_36" pad="N16"/>
<connect gate="C" pin="IO_37" pad="P10"/>
<connect gate="C" pin="IO_38" pad="P11"/>
<connect gate="C" pin="IO_39" pad="P13"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="P14"/>
<connect gate="C" pin="IO_41" pad="P16"/>
<connect gate="C" pin="IO_42" pad="R10"/>
<connect gate="C" pin="IO_43" pad="R11"/>
<connect gate="C" pin="IO_44" pad="R12"/>
<connect gate="C" pin="IO_45" pad="R13"/>
<connect gate="C" pin="IO_46" pad="R14"/>
<connect gate="C" pin="IO_47" pad="R15"/>
<connect gate="C" pin="IO_48" pad="T10"/>
<connect gate="C" pin="IO_49" pad="T11"/>
<connect gate="C" pin="IO_5" pad="E15"/>
<connect gate="C" pin="IO_50" pad="T12"/>
<connect gate="C" pin="IO_51" pad="T13"/>
<connect gate="C" pin="IO_52" pad="T14"/>
<connect gate="C" pin="IO_6" pad="F13"/>
<connect gate="C" pin="IO_7" pad="F14"/>
<connect gate="C" pin="IO_8" pad="F15"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="N15"/>
<connect gate="C" pin="NC_2" pad="E16"/>
<connect gate="C" pin="NC_3" pad="H16"/>
<connect gate="C" pin="NC_4" pad="K14"/>
<connect gate="C" pin="NC_5" pad="K16"/>
<connect gate="C" pin="NC_6" pad="M14"/>
<connect gate="C" pin="NC_7" pad="M16"/>
<connect gate="C" pin="NSTATUS" pad="T16"/>
<connect gate="C" pin="TMS" pad="P15"/>
<connect gate="C" pin="TRST" pad="R16"/>
<connect gate="C" pin="VCCINT" pad="M11"/>
<connect gate="C" pin="VCCINT_2" pad="E11"/>
<connect gate="C" pin="VCCINT_3" pad="F12"/>
<connect gate="C" pin="VCCINT_4" pad="H10"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="J11"/>
<connect gate="C" pin="VCCINT_7" pad="L12"/>
<connect gate="C" pin="VCCIO" pad="N12"/>
<connect gate="C" pin="VCCIO_2" pad="F10"/>
<connect gate="C" pin="VCCIO_3" pad="G11"/>
<connect gate="C" pin="VCCIO_4" pad="H11"/>
<connect gate="C" pin="VCCIO_5" pad="K11"/>
<connect gate="C" pin="VCCIO_6" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K50FI256-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0176"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K50QC208-1N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1K50QC208-1N_A"/>
<gate name="B" symbol="EP1K50QC208-1N_B"/>
<gate name="C" symbol="EP1K50QC208-1N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="49"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="59"/>
<connect gate="A" pin="GNDINT_4" pad="20"/>
<connect gate="A" pin="GNDINT_5" pad="23"/>
<connect gate="A" pin="GNDINT_6" pad="32"/>
<connect gate="A" pin="GNDINT_7" pad="35"/>
<connect gate="A" pin="GNDINT_8" pad="43"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/LOCK" pad="62"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="17"/>
<connect gate="A" pin="IO_11" pad="24"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="25"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="36"/>
<connect gate="A" pin="IO_19" pad="30"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="37"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="44"/>
<connect gate="A" pin="IO_27" pad="45"/>
<connect gate="A" pin="IO_28" pad="46"/>
<connect gate="A" pin="IO_29" pad="47"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="53"/>
<connect gate="A" pin="IO_31" pad="54"/>
<connect gate="A" pin="IO_32" pad="55"/>
<connect gate="A" pin="IO_33" pad="63"/>
<connect gate="A" pin="IO_34" pad="56"/>
<connect gate="A" pin="IO_35" pad="64"/>
<connect gate="A" pin="IO_36" pad="57"/>
<connect gate="A" pin="IO_37" pad="65"/>
<connect gate="A" pin="IO_38" pad="58"/>
<connect gate="A" pin="IO_39" pad="60"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="61"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_5" pad="11"/>
<connect gate="A" pin="IO_6" pad="12"/>
<connect gate="A" pin="IO_7" pad="13"/>
<connect gate="A" pin="IO_8" pad="14"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="21"/>
<connect gate="A" pin="VCCINT_2" pad="33"/>
<connect gate="A" pin="VCCINT_3" pad="48"/>
<connect gate="A" pin="VCCIO" pad="42"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="79"/>
<connect gate="B" pin="GNDINT" pad="137"/>
<connect gate="B" pin="GNDINT_2" pad="82"/>
<connect gate="B" pin="GNDINT_3" pad="76"/>
<connect gate="B" pin="GNDINT_4" pad="109"/>
<connect gate="B" pin="GNDINT_5" pad="117"/>
<connect gate="B" pin="GNDINT_6" pad="129"/>
<connect gate="B" pin="GNDINT_7" pad="123"/>
<connect gate="B" pin="GND_CKLK" pad="81"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="114"/>
<connect gate="B" pin="IO_29" pad="115"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="120"/>
<connect gate="B" pin="IO_33" pad="121"/>
<connect gate="B" pin="IO_34" pad="122"/>
<connect gate="B" pin="IO_35" pad="125"/>
<connect gate="B" pin="IO_36" pad="126"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="131"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_40" pad="132"/>
<connect gate="B" pin="IO_41" pad="133"/>
<connect gate="B" pin="IO_42" pad="134"/>
<connect gate="B" pin="IO_43" pad="135"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="106"/>
<connect gate="B" pin="VCCINT_3" pad="91"/>
<connect gate="B" pin="VCCINT_4" pad="72"/>
<connect gate="B" pin="VCCINT_5" pad="124"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="110"/>
<connect gate="B" pin="VCCIO_4" pad="138"/>
<connect gate="B" pin="VCCIO_5" pad="98"/>
<connect gate="B" pin="VCC_CKLK" pad="77"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="188"/>
<connect gate="C" pin="GNDINT_2" pad="145"/>
<connect gate="C" pin="GNDINT_3" pad="151"/>
<connect gate="C" pin="GNDINT_4" pad="171"/>
<connect gate="C" pin="GNDINT_5" pad="181"/>
<connect gate="C" pin="INPUT" pad="182"/>
<connect gate="C" pin="INPUT_2" pad="184"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_CLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="148"/>
<connect gate="C" pin="IO_11" pad="163"/>
<connect gate="C" pin="IO_12" pad="149"/>
<connect gate="C" pin="IO_13" pad="169"/>
<connect gate="C" pin="IO_14" pad="150"/>
<connect gate="C" pin="IO_15" pad="170"/>
<connect gate="C" pin="IO_16" pad="172"/>
<connect gate="C" pin="IO_17" pad="173"/>
<connect gate="C" pin="IO_18" pad="174"/>
<connect gate="C" pin="IO_19" pad="175"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="176"/>
<connect gate="C" pin="IO_21" pad="187"/>
<connect gate="C" pin="IO_22" pad="177"/>
<connect gate="C" pin="IO_23" pad="189"/>
<connect gate="C" pin="IO_24" pad="179"/>
<connect gate="C" pin="IO_25" pad="190"/>
<connect gate="C" pin="IO_26" pad="191"/>
<connect gate="C" pin="IO_27" pad="192"/>
<connect gate="C" pin="IO_28" pad="193"/>
<connect gate="C" pin="IO_29" pad="195"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="196"/>
<connect gate="C" pin="IO_31" pad="197"/>
<connect gate="C" pin="IO_32" pad="198"/>
<connect gate="C" pin="IO_33" pad="199"/>
<connect gate="C" pin="IO_34" pad="200"/>
<connect gate="C" pin="IO_35" pad="202"/>
<connect gate="C" pin="IO_36" pad="205"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_5" pad="167"/>
<connect gate="C" pin="IO_6" pad="144"/>
<connect gate="C" pin="IO_7" pad="168"/>
<connect gate="C" pin="IO_8" pad="147"/>
<connect gate="C" pin="IO_9" pad="160"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="201"/>
<connect gate="C" pin="VCCINT_2" pad="185"/>
<connect gate="C" pin="VCCINT_3" pad="152"/>
<connect gate="C" pin="VCCIO" pad="165"/>
<connect gate="C" pin="VCCIO_2" pad="194"/>
<connect gate="C" pin="VCCIO_3" pad="146"/>
<connect gate="C" pin="VCCIO_4" pad="178"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K50QC208-1N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0178"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K50QC208-2N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP1K50QC208-2N_A"/>
<gate name="B" symbol="EP1K50QC208-2N_B"/>
<gate name="C" symbol="EP1K50QC208-2N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="49"/>
<connect gate="A" pin="GNDINT_2" pad="6"/>
<connect gate="A" pin="GNDINT_3" pad="59"/>
<connect gate="A" pin="GNDINT_4" pad="20"/>
<connect gate="A" pin="GNDINT_5" pad="23"/>
<connect gate="A" pin="GNDINT_6" pad="32"/>
<connect gate="A" pin="GNDINT_7" pad="35"/>
<connect gate="A" pin="GNDINT_8" pad="43"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/LOCK" pad="62"/>
<connect gate="A" pin="IO/RDYNBUSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="17"/>
<connect gate="A" pin="IO_11" pad="24"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="25"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="36"/>
<connect gate="A" pin="IO_19" pad="30"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="37"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="44"/>
<connect gate="A" pin="IO_27" pad="45"/>
<connect gate="A" pin="IO_28" pad="46"/>
<connect gate="A" pin="IO_29" pad="47"/>
<connect gate="A" pin="IO_3" pad="8"/>
<connect gate="A" pin="IO_30" pad="53"/>
<connect gate="A" pin="IO_31" pad="54"/>
<connect gate="A" pin="IO_32" pad="55"/>
<connect gate="A" pin="IO_33" pad="63"/>
<connect gate="A" pin="IO_34" pad="56"/>
<connect gate="A" pin="IO_35" pad="64"/>
<connect gate="A" pin="IO_36" pad="57"/>
<connect gate="A" pin="IO_37" pad="65"/>
<connect gate="A" pin="IO_38" pad="58"/>
<connect gate="A" pin="IO_39" pad="60"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="61"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_5" pad="11"/>
<connect gate="A" pin="IO_6" pad="12"/>
<connect gate="A" pin="IO_7" pad="13"/>
<connect gate="A" pin="IO_8" pad="14"/>
<connect gate="A" pin="IO_9" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="21"/>
<connect gate="A" pin="VCCINT_2" pad="33"/>
<connect gate="A" pin="VCCINT_3" pad="48"/>
<connect gate="A" pin="VCCIO" pad="42"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK/GCLK1" pad="79"/>
<connect gate="B" pin="GNDINT" pad="137"/>
<connect gate="B" pin="GNDINT_2" pad="82"/>
<connect gate="B" pin="GNDINT_3" pad="76"/>
<connect gate="B" pin="GNDINT_4" pad="109"/>
<connect gate="B" pin="GNDINT_5" pad="117"/>
<connect gate="B" pin="GNDINT_6" pad="129"/>
<connect gate="B" pin="GNDINT_7" pad="123"/>
<connect gate="B" pin="GND_CKLK" pad="81"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="114"/>
<connect gate="B" pin="IO_29" pad="115"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="120"/>
<connect gate="B" pin="IO_33" pad="121"/>
<connect gate="B" pin="IO_34" pad="122"/>
<connect gate="B" pin="IO_35" pad="125"/>
<connect gate="B" pin="IO_36" pad="126"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="131"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_40" pad="132"/>
<connect gate="B" pin="IO_41" pad="133"/>
<connect gate="B" pin="IO_42" pad="134"/>
<connect gate="B" pin="IO_43" pad="135"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="139"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="106"/>
<connect gate="B" pin="VCCINT_3" pad="91"/>
<connect gate="B" pin="VCCINT_4" pad="72"/>
<connect gate="B" pin="VCCINT_5" pad="124"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="110"/>
<connect gate="B" pin="VCCIO_4" pad="138"/>
<connect gate="B" pin="VCCIO_5" pad="98"/>
<connect gate="B" pin="VCC_CKLK" pad="77"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="188"/>
<connect gate="C" pin="GNDINT_2" pad="145"/>
<connect gate="C" pin="GNDINT_3" pad="151"/>
<connect gate="C" pin="GNDINT_4" pad="171"/>
<connect gate="C" pin="GNDINT_5" pad="181"/>
<connect gate="C" pin="INPUT" pad="182"/>
<connect gate="C" pin="INPUT_2" pad="184"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_CLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="148"/>
<connect gate="C" pin="IO_11" pad="163"/>
<connect gate="C" pin="IO_12" pad="149"/>
<connect gate="C" pin="IO_13" pad="169"/>
<connect gate="C" pin="IO_14" pad="150"/>
<connect gate="C" pin="IO_15" pad="170"/>
<connect gate="C" pin="IO_16" pad="172"/>
<connect gate="C" pin="IO_17" pad="173"/>
<connect gate="C" pin="IO_18" pad="174"/>
<connect gate="C" pin="IO_19" pad="175"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="176"/>
<connect gate="C" pin="IO_21" pad="187"/>
<connect gate="C" pin="IO_22" pad="177"/>
<connect gate="C" pin="IO_23" pad="189"/>
<connect gate="C" pin="IO_24" pad="179"/>
<connect gate="C" pin="IO_25" pad="190"/>
<connect gate="C" pin="IO_26" pad="191"/>
<connect gate="C" pin="IO_27" pad="192"/>
<connect gate="C" pin="IO_28" pad="193"/>
<connect gate="C" pin="IO_29" pad="195"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="196"/>
<connect gate="C" pin="IO_31" pad="197"/>
<connect gate="C" pin="IO_32" pad="198"/>
<connect gate="C" pin="IO_33" pad="199"/>
<connect gate="C" pin="IO_34" pad="200"/>
<connect gate="C" pin="IO_35" pad="202"/>
<connect gate="C" pin="IO_36" pad="205"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_5" pad="167"/>
<connect gate="C" pin="IO_6" pad="144"/>
<connect gate="C" pin="IO_7" pad="168"/>
<connect gate="C" pin="IO_8" pad="147"/>
<connect gate="C" pin="IO_9" pad="160"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="201"/>
<connect gate="C" pin="VCCINT_2" pad="185"/>
<connect gate="C" pin="VCCINT_3" pad="152"/>
<connect gate="C" pin="VCCIO" pad="165"/>
<connect gate="C" pin="VCCIO_2" pad="194"/>
<connect gate="C" pin="VCCIO_3" pad="146"/>
<connect gate="C" pin="VCCIO_4" pad="178"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K50QC208-2N"/>
<attribute name="OC_FARNELL" value="1700721"/>
<attribute name="OC_NEWARK" value="51R0555"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1K50TC144-1N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EP1K50TC144-1N_A"/>
<gate name="B" symbol="EP1K50TC144-1N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK/GCLK1" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="15"/>
<connect gate="A" pin="GNDINT_2" pad="40"/>
<connect gate="A" pin="GNDINT_3" pad="52"/>
<connect gate="A" pin="GNDINT_4" pad="58"/>
<connect gate="A" pin="GNDINT_5" pad="66"/>
<connect gate="A" pin="GNDINT_6" pad="6"/>
<connect gate="A" pin="GNDINT_7" pad="25"/>
<connect gate="A" pin="GND_CKLK" pad="57"/>
<connect gate="A" pin="INPUT" pad="54"/>
<connect gate="A" pin="INPUT_2" pad="56"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/LOCK" pad="42"/>
<connect gate="A" pin="IO/RDY/NBUSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="43"/>
<connect gate="A" pin="IO_28" pad="44"/>
<connect gate="A" pin="IO_29" pad="46"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="47"/>
<connect gate="A" pin="IO_31" pad="48"/>
<connect gate="A" pin="IO_32" pad="49"/>
<connect gate="A" pin="IO_33" pad="51"/>
<connect gate="A" pin="IO_34" pad="59"/>
<connect gate="A" pin="IO_35" pad="60"/>
<connect gate="A" pin="IO_36" pad="62"/>
<connect gate="A" pin="IO_37" pad="63"/>
<connect gate="A" pin="IO_38" pad="64"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="50"/>
<connect gate="A" pin="VCCINT_2" pad="16"/>
<connect gate="A" pin="VCCIO" pad="45"/>
<connect gate="A" pin="VCCIO_2" pad="61"/>
<connect gate="A" pin="VCCIO_3" pad="5"/>
<connect gate="A" pin="VCCIO_4" pad="71"/>
<connect gate="A" pin="VCCIO_5" pad="24"/>
<connect gate="A" pin="VCC_CKLK" pad="53"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="84"/>
<connect gate="B" pin="GNDINT_2" pad="93"/>
<connect gate="B" pin="GNDINT_3" pad="123"/>
<connect gate="B" pin="GNDINT_4" pad="139"/>
<connect gate="B" pin="GNDINT_5" pad="129"/>
<connect gate="B" pin="GNDINT_6" pad="104"/>
<connect gate="B" pin="INPUT" pad="124"/>
<connect gate="B" pin="INPUT_2" pad="126"/>
<connect gate="B" pin="IO" pad="121"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLR" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="90"/>
<connect gate="B" pin="IO_14" pad="95"/>
<connect gate="B" pin="IO_15" pad="91"/>
<connect gate="B" pin="IO_16" pad="96"/>
<connect gate="B" pin="IO_17" pad="92"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="98"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="102"/>
<connect gate="B" pin="IO_21" pad="131"/>
<connect gate="B" pin="IO_22" pad="99"/>
<connect gate="B" pin="IO_23" pad="132"/>
<connect gate="B" pin="IO_24" pad="100"/>
<connect gate="B" pin="IO_25" pad="133"/>
<connect gate="B" pin="IO_26" pad="101"/>
<connect gate="B" pin="IO_27" pad="135"/>
<connect gate="B" pin="IO_28" pad="117"/>
<connect gate="B" pin="IO_29" pad="136"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="118"/>
<connect gate="B" pin="IO_31" pad="137"/>
<connect gate="B" pin="IO_32" pad="119"/>
<connect gate="B" pin="IO_33" pad="130"/>
<connect gate="B" pin="IO_34" pad="138"/>
<connect gate="B" pin="IO_35" pad="120"/>
<connect gate="B" pin="IO_36" pad="140"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="127"/>
<connect gate="B" pin="VCCINT_2" pad="75"/>
<connect gate="B" pin="VCCINT_3" pad="85"/>
<connect gate="B" pin="VCCINT_4" pad="103"/>
<connect gate="B" pin="VCCIO" pad="115"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="134"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1K50TC144-1N"/>
<attribute name="OC_FARNELL" value="1549324"/>
<attribute name="OC_NEWARK" value="52R0184"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1S10F484C7N">
<description>Stratix Device</description>
<gates>
<gate name="A" symbol="EP1S10F484C7N_A"/>
<gate name="B" symbol="EP1S10F484C7N_B"/>
<gate name="C" symbol="EP1S10F484C7N_C"/>
<gate name="D" symbol="EP1S10F484C7N_D"/>
<gate name="E" symbol="EP1S10F484C7N_E"/>
</gates>
<devices>
<device name="" package="BGA484C22X22X100P_2300X2300X35">
<connects>
<connect gate="A" pin="CLK10P" pad="L3"/>
<connect gate="A" pin="CLK11N" pad="L1"/>
<connect gate="A" pin="CLK11P" pad="L2"/>
<connect gate="A" pin="GND" pad="J1"/>
<connect gate="A" pin="GNDA_PLL4" pad="L4"/>
<connect gate="A" pin="GNDG_PLL4" pad="L5"/>
<connect gate="A" pin="GND_2" pad="A9"/>
<connect gate="A" pin="GND_3" pad="A2"/>
<connect gate="A" pin="GND_4" pad="G6"/>
<connect gate="A" pin="GND_5" pad="B1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="C2"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D1"/>
<connect gate="A" pin="IO_23" pad="D2"/>
<connect gate="A" pin="IO_24" pad="D3"/>
<connect gate="A" pin="IO_25" pad="D4"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E1"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E5"/>
<connect gate="A" pin="IO_34" pad="E6"/>
<connect gate="A" pin="IO_35" pad="E7"/>
<connect gate="A" pin="IO_36" pad="E8"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F5"/>
<connect gate="A" pin="IO_43" pad="F6"/>
<connect gate="A" pin="IO_44" pad="F7"/>
<connect gate="A" pin="IO_45" pad="F8"/>
<connect gate="A" pin="IO_46" pad="F9"/>
<connect gate="A" pin="IO_47" pad="G1"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="G3"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="G4"/>
<connect gate="A" pin="IO_51" pad="G5"/>
<connect gate="A" pin="IO_52" pad="G7"/>
<connect gate="A" pin="IO_53" pad="G8"/>
<connect gate="A" pin="IO_54" pad="G9"/>
<connect gate="A" pin="IO_55" pad="H1"/>
<connect gate="A" pin="IO_56" pad="H2"/>
<connect gate="A" pin="IO_57" pad="H3"/>
<connect gate="A" pin="IO_58" pad="H4"/>
<connect gate="A" pin="IO_59" pad="H8"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_60" pad="J2"/>
<connect gate="A" pin="IO_61" pad="J3"/>
<connect gate="A" pin="IO_62" pad="J4"/>
<connect gate="A" pin="IO_63" pad="J6"/>
<connect gate="A" pin="IO_64" pad="J7"/>
<connect gate="A" pin="IO_65" pad="J8"/>
<connect gate="A" pin="IO_66" pad="J9"/>
<connect gate="A" pin="IO_67" pad="K2"/>
<connect gate="A" pin="IO_68" pad="K3"/>
<connect gate="A" pin="IO_69" pad="K6"/>
<connect gate="A" pin="IO_7" pad="B2"/>
<connect gate="A" pin="IO_70" pad="K7"/>
<connect gate="A" pin="IO_71" pad="K8"/>
<connect gate="A" pin="IO_72" pad="L6"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="NC" pad="E4"/>
<connect gate="A" pin="NC_2" pad="B9"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="H9"/>
<connect gate="A" pin="TCK" pad="K9"/>
<connect gate="A" pin="VCCA_PLL4" pad="K4"/>
<connect gate="A" pin="VCCG_PLL4" pad="K5"/>
<connect gate="A" pin="VCCINT" pad="A1"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="K1"/>
<connect gate="A" pin="VCCIO5_2" pad="C1"/>
<connect gate="A" pin="VREF0B4" pad="H6"/>
<connect gate="A" pin="VREF0B5" pad="J5"/>
<connect gate="A" pin="VREF1B4" pad="H7"/>
<connect gate="A" pin="VREF1B5" pad="H5"/>
<connect gate="B" pin="CLK12P" pad="A11"/>
<connect gate="B" pin="CLK8P" pad="M3"/>
<connect gate="B" pin="CLK9N" pad="M1"/>
<connect gate="B" pin="CLK9P" pad="M2"/>
<connect gate="B" pin="GND" pad="AA1"/>
<connect gate="B" pin="GNDA_PLL3" pad="M4"/>
<connect gate="B" pin="GNDG_PLL3" pad="N4"/>
<connect gate="B" pin="GND_2" pad="M9"/>
<connect gate="B" pin="GND_3" pad="A21"/>
<connect gate="B" pin="GND_4" pad="P1"/>
<connect gate="B" pin="GND_5" pad="T6"/>
<connect gate="B" pin="GND_6" pad="A14"/>
<connect gate="B" pin="IO" pad="A19"/>
<connect gate="B" pin="IO_10" pad="N8"/>
<connect gate="B" pin="IO_11" pad="P2"/>
<connect gate="B" pin="IO_12" pad="P3"/>
<connect gate="B" pin="IO_13" pad="P4"/>
<connect gate="B" pin="IO_14" pad="P6"/>
<connect gate="B" pin="IO_15" pad="P7"/>
<connect gate="B" pin="IO_16" pad="P8"/>
<connect gate="B" pin="IO_17" pad="P9"/>
<connect gate="B" pin="IO_18" pad="R1"/>
<connect gate="B" pin="IO_19" pad="R2"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R3"/>
<connect gate="B" pin="IO_21" pad="R4"/>
<connect gate="B" pin="IO_22" pad="R8"/>
<connect gate="B" pin="IO_23" pad="T1"/>
<connect gate="B" pin="IO_24" pad="T2"/>
<connect gate="B" pin="IO_25" pad="T3"/>
<connect gate="B" pin="IO_26" pad="T4"/>
<connect gate="B" pin="IO_27" pad="T5"/>
<connect gate="B" pin="IO_28" pad="T7"/>
<connect gate="B" pin="IO_29" pad="T8"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="T9"/>
<connect gate="B" pin="IO_31" pad="U1"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U5"/>
<connect gate="B" pin="IO_34" pad="U6"/>
<connect gate="B" pin="IO_35" pad="U7"/>
<connect gate="B" pin="IO_36" pad="U8"/>
<connect gate="B" pin="IO_37" pad="U9"/>
<connect gate="B" pin="IO_38" pad="V1"/>
<connect gate="B" pin="IO_39" pad="V2"/>
<connect gate="B" pin="IO_4" pad="M7"/>
<connect gate="B" pin="IO_40" pad="V3"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V5"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="V9"/>
<connect gate="B" pin="IO_47" pad="W1"/>
<connect gate="B" pin="IO_48" pad="W2"/>
<connect gate="B" pin="IO_49" pad="W3"/>
<connect gate="B" pin="IO_5" pad="M8"/>
<connect gate="B" pin="IO_50" pad="W4"/>
<connect gate="B" pin="IO_51" pad="W5"/>
<connect gate="B" pin="IO_52" pad="W6"/>
<connect gate="B" pin="IO_53" pad="W7"/>
<connect gate="B" pin="IO_54" pad="W8"/>
<connect gate="B" pin="IO_55" pad="W9"/>
<connect gate="B" pin="IO_56" pad="Y2"/>
<connect gate="B" pin="IO_57" pad="Y3"/>
<connect gate="B" pin="IO_58" pad="Y4"/>
<connect gate="B" pin="IO_59" pad="Y5"/>
<connect gate="B" pin="IO_6" pad="N2"/>
<connect gate="B" pin="IO_60" pad="Y6"/>
<connect gate="B" pin="IO_61" pad="Y7"/>
<connect gate="B" pin="IO_62" pad="Y8"/>
<connect gate="B" pin="IO_63" pad="Y9"/>
<connect gate="B" pin="IO_64" pad="A12"/>
<connect gate="B" pin="IO_65" pad="A15"/>
<connect gate="B" pin="IO_66" pad="A16"/>
<connect gate="B" pin="IO_67" pad="A17"/>
<connect gate="B" pin="IO_68" pad="A18"/>
<connect gate="B" pin="IO_7" pad="N3"/>
<connect gate="B" pin="IO_8" pad="N6"/>
<connect gate="B" pin="IO_9" pad="N7"/>
<connect gate="B" pin="NC" pad="U4"/>
<connect gate="B" pin="NC_2" pad="U3"/>
<connect gate="B" pin="NC_3" pad="R5"/>
<connect gate="B" pin="NIO_PULLUP" pad="N9"/>
<connect gate="B" pin="VCCA_PLL3" pad="M5"/>
<connect gate="B" pin="VCCG_PLL3" pad="N5"/>
<connect gate="B" pin="VCCINT" pad="A22"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCIO3" pad="A13"/>
<connect gate="B" pin="VCCIO3_2" pad="A20"/>
<connect gate="B" pin="VCCIO4" pad="A10"/>
<connect gate="B" pin="VCCIO6" pad="Y1"/>
<connect gate="B" pin="VCCIO6_2" pad="N1"/>
<connect gate="B" pin="VREF0B6" pad="R6"/>
<connect gate="B" pin="VREF0B7" pad="R9"/>
<connect gate="B" pin="VREF1B6" pad="P5"/>
<connect gate="B" pin="VREF1B7" pad="R7"/>
<connect gate="C" pin="CLK13P" pad="B11"/>
<connect gate="C" pin="CLK14P" pad="B14"/>
<connect gate="C" pin="CLK15P" pad="E13"/>
<connect gate="C" pin="GND" pad="G17"/>
<connect gate="C" pin="GNDA_PLL5" pad="F12"/>
<connect gate="C" pin="GNDG_PLL5" pad="G11"/>
<connect gate="C" pin="GND_2" pad="AB2"/>
<connect gate="C" pin="GND_3" pad="B22"/>
<connect gate="C" pin="GND_4" pad="AB9"/>
<connect gate="C" pin="GND_5" pad="G15"/>
<connect gate="C" pin="IO" pad="H10"/>
<connect gate="C" pin="IO_10" pad="AB5"/>
<connect gate="C" pin="IO_11" pad="AB6"/>
<connect gate="C" pin="IO_12" pad="AB7"/>
<connect gate="C" pin="IO_13" pad="AB8"/>
<connect gate="C" pin="IO_14" pad="B12"/>
<connect gate="C" pin="IO_15" pad="B13"/>
<connect gate="C" pin="IO_16" pad="B15"/>
<connect gate="C" pin="IO_17" pad="B16"/>
<connect gate="C" pin="IO_18" pad="B17"/>
<connect gate="C" pin="IO_19" pad="B18"/>
<connect gate="C" pin="IO_2" pad="AA2"/>
<connect gate="C" pin="IO_20" pad="B19"/>
<connect gate="C" pin="IO_21" pad="B20"/>
<connect gate="C" pin="IO_22" pad="B21"/>
<connect gate="C" pin="IO_23" pad="C12"/>
<connect gate="C" pin="IO_24" pad="C13"/>
<connect gate="C" pin="IO_25" pad="C14"/>
<connect gate="C" pin="IO_26" pad="C15"/>
<connect gate="C" pin="IO_27" pad="C16"/>
<connect gate="C" pin="IO_28" pad="C17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="AA3"/>
<connect gate="C" pin="IO_30" pad="C19"/>
<connect gate="C" pin="IO_31" pad="C20"/>
<connect gate="C" pin="IO_32" pad="C21"/>
<connect gate="C" pin="IO_33" pad="D12"/>
<connect gate="C" pin="IO_34" pad="D13"/>
<connect gate="C" pin="IO_35" pad="D14"/>
<connect gate="C" pin="IO_36" pad="D15"/>
<connect gate="C" pin="IO_37" pad="D16"/>
<connect gate="C" pin="IO_38" pad="D17"/>
<connect gate="C" pin="IO_39" pad="D18"/>
<connect gate="C" pin="IO_4" pad="AA4"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E14"/>
<connect gate="C" pin="IO_45" pad="E15"/>
<connect gate="C" pin="IO_46" pad="E16"/>
<connect gate="C" pin="IO_47" pad="E17"/>
<connect gate="C" pin="IO_48" pad="E18"/>
<connect gate="C" pin="IO_49" pad="E19"/>
<connect gate="C" pin="IO_5" pad="AA5"/>
<connect gate="C" pin="IO_50" pad="E20"/>
<connect gate="C" pin="IO_51" pad="E21"/>
<connect gate="C" pin="IO_52" pad="E22"/>
<connect gate="C" pin="IO_53" pad="F10"/>
<connect gate="C" pin="IO_54" pad="F14"/>
<connect gate="C" pin="IO_55" pad="F15"/>
<connect gate="C" pin="IO_56" pad="F16"/>
<connect gate="C" pin="IO_57" pad="F17"/>
<connect gate="C" pin="IO_58" pad="F18"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AA6"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G14"/>
<connect gate="C" pin="IO_62" pad="G16"/>
<connect gate="C" pin="IO_63" pad="G18"/>
<connect gate="C" pin="IO_64" pad="G19"/>
<connect gate="C" pin="IO_65" pad="G20"/>
<connect gate="C" pin="IO_66" pad="G21"/>
<connect gate="C" pin="IO_67" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AA7"/>
<connect gate="C" pin="IO_8" pad="AA8"/>
<connect gate="C" pin="IO_9" pad="AB4"/>
<connect gate="C" pin="NC" pad="F20"/>
<connect gate="C" pin="NC_10" pad="AA9"/>
<connect gate="C" pin="NC_11" pad="F19"/>
<connect gate="C" pin="NC_2" pad="C10"/>
<connect gate="C" pin="NC_3" pad="C11"/>
<connect gate="C" pin="NC_4" pad="D10"/>
<connect gate="C" pin="NC_5" pad="D11"/>
<connect gate="C" pin="NC_6" pad="E10"/>
<connect gate="C" pin="NC_7" pad="E11"/>
<connect gate="C" pin="NC_8" pad="E12"/>
<connect gate="C" pin="NC_9" pad="B10"/>
<connect gate="C" pin="TDO" pad="H11"/>
<connect gate="C" pin="TEMPDIODEP" pad="G12"/>
<connect gate="C" pin="TMS" pad="G10"/>
<connect gate="C" pin="VCCA_PLL5" pad="G13"/>
<connect gate="C" pin="VCCG_PLL5" pad="F11"/>
<connect gate="C" pin="VCCINT" pad="AB1"/>
<connect gate="C" pin="VCCIO2" pad="C22"/>
<connect gate="C" pin="VCCIO7" pad="AB3"/>
<connect gate="C" pin="VCC_PLL5_OUTA" pad="F13"/>
<connect gate="D" pin="CLK0N" pad="L22"/>
<connect gate="D" pin="CLK0P" pad="L21"/>
<connect gate="D" pin="CLK1P" pad="L20"/>
<connect gate="D" pin="CLK2N" pad="M22"/>
<connect gate="D" pin="CLK2P" pad="M21"/>
<connect gate="D" pin="CLK3P" pad="M20"/>
<connect gate="D" pin="CONF_DONE" pad="K13"/>
<connect gate="D" pin="DCLK" pad="J13"/>
<connect gate="D" pin="GND" pad="L14"/>
<connect gate="D" pin="GNDA_PLL1" pad="L19"/>
<connect gate="D" pin="GNDA_PLL2" pad="M19"/>
<connect gate="D" pin="GNDG_PLL1" pad="L18"/>
<connect gate="D" pin="GNDG_PLL2" pad="N19"/>
<connect gate="D" pin="GND_2" pad="L10"/>
<connect gate="D" pin="GND_3" pad="M13"/>
<connect gate="D" pin="GND_4" pad="J22"/>
<connect gate="D" pin="GND_5" pad="L12"/>
<connect gate="D" pin="GND_6" pad="K11"/>
<connect gate="D" pin="GND_7" pad="N12"/>
<connect gate="D" pin="GND_8" pad="P22"/>
<connect gate="D" pin="GND_9" pad="M11"/>
<connect gate="D" pin="IO" pad="R15"/>
<connect gate="D" pin="IO_10" pad="J17"/>
<connect gate="D" pin="IO_11" pad="J19"/>
<connect gate="D" pin="IO_12" pad="J20"/>
<connect gate="D" pin="IO_13" pad="J21"/>
<connect gate="D" pin="IO_14" pad="K10"/>
<connect gate="D" pin="IO_15" pad="K14"/>
<connect gate="D" pin="IO_16" pad="K15"/>
<connect gate="D" pin="IO_17" pad="K16"/>
<connect gate="D" pin="IO_18" pad="K17"/>
<connect gate="D" pin="IO_19" pad="K20"/>
<connect gate="D" pin="IO_2" pad="H17"/>
<connect gate="D" pin="IO_20" pad="K21"/>
<connect gate="D" pin="IO_21" pad="L15"/>
<connect gate="D" pin="IO_22" pad="L16"/>
<connect gate="D" pin="IO_23" pad="L17"/>
<connect gate="D" pin="IO_24" pad="M15"/>
<connect gate="D" pin="IO_25" pad="M16"/>
<connect gate="D" pin="IO_26" pad="M17"/>
<connect gate="D" pin="IO_27" pad="N10"/>
<connect gate="D" pin="IO_28" pad="N13"/>
<connect gate="D" pin="IO_29" pad="N14"/>
<connect gate="D" pin="IO_3" pad="H19"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N16"/>
<connect gate="D" pin="IO_32" pad="N17"/>
<connect gate="D" pin="IO_33" pad="N20"/>
<connect gate="D" pin="IO_34" pad="N21"/>
<connect gate="D" pin="IO_35" pad="P10"/>
<connect gate="D" pin="IO_36" pad="P13"/>
<connect gate="D" pin="IO_37" pad="P14"/>
<connect gate="D" pin="IO_38" pad="P15"/>
<connect gate="D" pin="IO_39" pad="P16"/>
<connect gate="D" pin="IO_4" pad="H20"/>
<connect gate="D" pin="IO_40" pad="P17"/>
<connect gate="D" pin="IO_41" pad="P19"/>
<connect gate="D" pin="IO_42" pad="P20"/>
<connect gate="D" pin="IO_43" pad="P21"/>
<connect gate="D" pin="IO_5" pad="H21"/>
<connect gate="D" pin="IO_6" pad="H22"/>
<connect gate="D" pin="IO_7" pad="J14"/>
<connect gate="D" pin="IO_8" pad="J15"/>
<connect gate="D" pin="IO_9" pad="J16"/>
<connect gate="D" pin="MSEL1" pad="P12"/>
<connect gate="D" pin="MSEL2" pad="R12"/>
<connect gate="D" pin="NC" pad="R14"/>
<connect gate="D" pin="NCE" pad="R11"/>
<connect gate="D" pin="NCEO" pad="P11"/>
<connect gate="D" pin="NCONFIG" pad="H13"/>
<connect gate="D" pin="NC_2" pad="H16"/>
<connect gate="D" pin="NSTATUS" pad="J12"/>
<connect gate="D" pin="PLL_ENA" pad="R13"/>
<connect gate="D" pin="TDI" pad="J11"/>
<connect gate="D" pin="TEMPDIODEN" pad="H12"/>
<connect gate="D" pin="TRST" pad="J10"/>
<connect gate="D" pin="VCCA_PLL1" pad="K19"/>
<connect gate="D" pin="VCCA_PLL2" pad="M18"/>
<connect gate="D" pin="VCCG_PLL1" pad="K18"/>
<connect gate="D" pin="VCCG_PLL2" pad="N18"/>
<connect gate="D" pin="VCCINT" pad="M10"/>
<connect gate="D" pin="VCCINT_2" pad="L13"/>
<connect gate="D" pin="VCCINT_3" pad="K12"/>
<connect gate="D" pin="VCCINT_4" pad="M14"/>
<connect gate="D" pin="VCCINT_5" pad="M12"/>
<connect gate="D" pin="VCCINT_6" pad="N11"/>
<connect gate="D" pin="VCCINT_7" pad="L11"/>
<connect gate="D" pin="VCCIO1" pad="N22"/>
<connect gate="D" pin="VCCIO2" pad="K22"/>
<connect gate="D" pin="VCCSEL" pad="R10"/>
<connect gate="D" pin="VREF0B1" pad="P18"/>
<connect gate="D" pin="VREF0B2" pad="H18"/>
<connect gate="D" pin="VREF0B3" pad="H14"/>
<connect gate="D" pin="VREF1B1" pad="R17"/>
<connect gate="D" pin="VREF1B2" pad="J18"/>
<connect gate="D" pin="VREF1B3" pad="H15"/>
<connect gate="D" pin="VREF1B8" pad="R16"/>
<connect gate="E" pin="CLK4P" pad="AA14"/>
<connect gate="E" pin="CLK5P" pad="V13"/>
<connect gate="E" pin="CLK6P" pad="AB11"/>
<connect gate="E" pin="CLK7P" pad="AA11"/>
<connect gate="E" pin="GND" pad="AA22"/>
<connect gate="E" pin="GNDA_PLL6" pad="U12"/>
<connect gate="E" pin="GNDG_PLL6" pad="T11"/>
<connect gate="E" pin="GND_2" pad="T17"/>
<connect gate="E" pin="GND_3" pad="AB14"/>
<connect gate="E" pin="GND_4" pad="AB21"/>
<connect gate="E" pin="IO" pad="AB19"/>
<connect gate="E" pin="IO_10" pad="T18"/>
<connect gate="E" pin="IO_11" pad="T19"/>
<connect gate="E" pin="IO_12" pad="T20"/>
<connect gate="E" pin="IO_13" pad="T21"/>
<connect gate="E" pin="IO_14" pad="T22"/>
<connect gate="E" pin="IO_15" pad="U14"/>
<connect gate="E" pin="IO_16" pad="U15"/>
<connect gate="E" pin="IO_17" pad="U16"/>
<connect gate="E" pin="IO_18" pad="U17"/>
<connect gate="E" pin="IO_19" pad="U18"/>
<connect gate="E" pin="IO_2" pad="R19"/>
<connect gate="E" pin="IO_20" pad="U19"/>
<connect gate="E" pin="IO_21" pad="U20"/>
<connect gate="E" pin="IO_22" pad="U21"/>
<connect gate="E" pin="IO_23" pad="U22"/>
<connect gate="E" pin="IO_24" pad="V14"/>
<connect gate="E" pin="IO_25" pad="V15"/>
<connect gate="E" pin="IO_26" pad="V16"/>
<connect gate="E" pin="IO_27" pad="V17"/>
<connect gate="E" pin="IO_28" pad="V18"/>
<connect gate="E" pin="IO_29" pad="V21"/>
<connect gate="E" pin="IO_3" pad="R20"/>
<connect gate="E" pin="IO_30" pad="V22"/>
<connect gate="E" pin="IO_31" pad="W12"/>
<connect gate="E" pin="IO_32" pad="W13"/>
<connect gate="E" pin="IO_33" pad="W14"/>
<connect gate="E" pin="IO_34" pad="W15"/>
<connect gate="E" pin="IO_35" pad="W16"/>
<connect gate="E" pin="IO_36" pad="W17"/>
<connect gate="E" pin="IO_37" pad="W18"/>
<connect gate="E" pin="IO_38" pad="W19"/>
<connect gate="E" pin="IO_39" pad="W20"/>
<connect gate="E" pin="IO_4" pad="R21"/>
<connect gate="E" pin="IO_40" pad="W21"/>
<connect gate="E" pin="IO_41" pad="W22"/>
<connect gate="E" pin="IO_42" pad="Y12"/>
<connect gate="E" pin="IO_43" pad="Y13"/>
<connect gate="E" pin="IO_44" pad="Y14"/>
<connect gate="E" pin="IO_45" pad="Y15"/>
<connect gate="E" pin="IO_46" pad="Y16"/>
<connect gate="E" pin="IO_47" pad="Y17"/>
<connect gate="E" pin="IO_48" pad="Y18"/>
<connect gate="E" pin="IO_49" pad="Y19"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="Y20"/>
<connect gate="E" pin="IO_51" pad="Y21"/>
<connect gate="E" pin="IO_52" pad="AA12"/>
<connect gate="E" pin="IO_53" pad="AA13"/>
<connect gate="E" pin="IO_54" pad="AA15"/>
<connect gate="E" pin="IO_55" pad="AA16"/>
<connect gate="E" pin="IO_56" pad="AA17"/>
<connect gate="E" pin="IO_57" pad="AA18"/>
<connect gate="E" pin="IO_58" pad="AA19"/>
<connect gate="E" pin="IO_59" pad="AA20"/>
<connect gate="E" pin="IO_6" pad="T10"/>
<connect gate="E" pin="IO_60" pad="AA21"/>
<connect gate="E" pin="IO_61" pad="AB12"/>
<connect gate="E" pin="IO_62" pad="AB15"/>
<connect gate="E" pin="IO_63" pad="AB16"/>
<connect gate="E" pin="IO_64" pad="AB17"/>
<connect gate="E" pin="IO_65" pad="AB18"/>
<connect gate="E" pin="IO_7" pad="T14"/>
<connect gate="E" pin="IO_8" pad="T15"/>
<connect gate="E" pin="IO_9" pad="T16"/>
<connect gate="E" pin="MSEL0" pad="T13"/>
<connect gate="E" pin="NC" pad="AA10"/>
<connect gate="E" pin="NC_10" pad="Y11"/>
<connect gate="E" pin="NC_2" pad="V10"/>
<connect gate="E" pin="NC_3" pad="V11"/>
<connect gate="E" pin="NC_4" pad="V12"/>
<connect gate="E" pin="NC_5" pad="V19"/>
<connect gate="E" pin="NC_6" pad="V20"/>
<connect gate="E" pin="NC_7" pad="W10"/>
<connect gate="E" pin="NC_8" pad="W11"/>
<connect gate="E" pin="NC_9" pad="Y10"/>
<connect gate="E" pin="PORSEL" pad="U10"/>
<connect gate="E" pin="VCCA_PLL6" pad="T12"/>
<connect gate="E" pin="VCCG_PLL6" pad="U11"/>
<connect gate="E" pin="VCCINT" pad="AB22"/>
<connect gate="E" pin="VCCIO1" pad="Y22"/>
<connect gate="E" pin="VCCIO7" pad="AB10"/>
<connect gate="E" pin="VCCIO8" pad="AB20"/>
<connect gate="E" pin="VCCIO8_2" pad="AB13"/>
<connect gate="E" pin="VCC_PLL6_OUTA" pad="U13"/>
<connect gate="E" pin="VREF0B8" pad="R18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1S10F484C7N"/>
<attribute name="OC_FARNELL" value="1549494"/>
<attribute name="OC_NEWARK" value="51R8597"/>
<attribute name="PACKAGE" value="484-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1S20F780C7N">
<description>FPGA, STRATIX</description>
<gates>
<gate name="A" symbol="EP1S20F780C7N_A"/>
<gate name="B" symbol="EP1S20F780C7N_B"/>
<gate name="C" symbol="EP1S20F780C7N_C"/>
<gate name="D" symbol="EP1S20F780C7N_D"/>
<gate name="E" symbol="EP1S20F780C7N_E"/>
<gate name="F" symbol="EP1S20F780C7N_F"/>
<gate name="G" symbol="EP1S20F780C7N_G"/>
<gate name="H" symbol="EP1S20F780C7N_H"/>
</gates>
<devices>
<device name="" package="BGA780C100P28X28_2900X2900X350">
<connects>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="IO" pad="L9"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="A9"/>
<connect gate="A" pin="IO_12" pad="B6"/>
<connect gate="A" pin="IO_13" pad="B7"/>
<connect gate="A" pin="IO_14" pad="F1"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="E8"/>
<connect gate="A" pin="IO_17" pad="B9"/>
<connect gate="A" pin="IO_18" pad="C1"/>
<connect gate="A" pin="IO_19" pad="F2"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C2"/>
<connect gate="A" pin="IO_21" pad="F3"/>
<connect gate="A" pin="IO_22" pad="F4"/>
<connect gate="A" pin="IO_23" pad="C4"/>
<connect gate="A" pin="IO_24" pad="C5"/>
<connect gate="A" pin="IO_25" pad="C6"/>
<connect gate="A" pin="IO_26" pad="C7"/>
<connect gate="A" pin="IO_27" pad="C8"/>
<connect gate="A" pin="IO_28" pad="C9"/>
<connect gate="A" pin="IO_29" pad="D1"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D5"/>
<connect gate="A" pin="IO_31" pad="D2"/>
<connect gate="A" pin="IO_32" pad="D6"/>
<connect gate="A" pin="IO_33" pad="D7"/>
<connect gate="A" pin="IO_34" pad="D8"/>
<connect gate="A" pin="IO_35" pad="D9"/>
<connect gate="A" pin="IO_36" pad="E1"/>
<connect gate="A" pin="IO_37" pad="E6"/>
<connect gate="A" pin="IO_38" pad="E2"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="G9"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="H8"/>
<connect gate="A" pin="IO_58" pad="H9"/>
<connect gate="A" pin="IO_59" pad="J1"/>
<connect gate="A" pin="IO_6" pad="B3"/>
<connect gate="A" pin="IO_60" pad="J2"/>
<connect gate="A" pin="IO_61" pad="J3"/>
<connect gate="A" pin="IO_62" pad="J4"/>
<connect gate="A" pin="IO_63" pad="J5"/>
<connect gate="A" pin="IO_64" pad="J6"/>
<connect gate="A" pin="IO_65" pad="J7"/>
<connect gate="A" pin="IO_66" pad="J8"/>
<connect gate="A" pin="IO_67" pad="J9"/>
<connect gate="A" pin="IO_68" pad="K1"/>
<connect gate="A" pin="IO_69" pad="K2"/>
<connect gate="A" pin="IO_7" pad="A7"/>
<connect gate="A" pin="IO_70" pad="K3"/>
<connect gate="A" pin="IO_71" pad="K4"/>
<connect gate="A" pin="IO_72" pad="K5"/>
<connect gate="A" pin="IO_73" pad="K6"/>
<connect gate="A" pin="IO_74" pad="K7"/>
<connect gate="A" pin="IO_75" pad="K8"/>
<connect gate="A" pin="IO_76" pad="L1"/>
<connect gate="A" pin="IO_77" pad="L2"/>
<connect gate="A" pin="IO_78" pad="L3"/>
<connect gate="A" pin="IO_79" pad="L4"/>
<connect gate="A" pin="IO_8" pad="B4"/>
<connect gate="A" pin="IO_80" pad="L5"/>
<connect gate="A" pin="IO_81" pad="L6"/>
<connect gate="A" pin="IO_82" pad="L7"/>
<connect gate="A" pin="IO_83" pad="L8"/>
<connect gate="A" pin="IO_9" pad="A8"/>
<connect gate="A" pin="NC" pad="F5"/>
<connect gate="A" pin="NC_2" pad="F6"/>
<connect gate="A" pin="NC_3" pad="F7"/>
<connect gate="A" pin="NC_4" pad="E3"/>
<connect gate="A" pin="NC_5" pad="D3"/>
<connect gate="A" pin="NC_6" pad="E5"/>
<connect gate="A" pin="NC_7" pad="E4"/>
<connect gate="A" pin="NC_8" pad="D4"/>
<connect gate="A" pin="VCCIO4" pad="A2"/>
<connect gate="A" pin="VCCIO5" pad="B1"/>
<connect gate="A" pin="VREF0B4" pad="E7"/>
<connect gate="A" pin="VREF1B4" pad="E9"/>
<connect gate="A" pin="VREF1B5" pad="K9"/>
<connect gate="B" pin="CLK10P" pad="P4"/>
<connect gate="B" pin="CLK11N" pad="N2"/>
<connect gate="B" pin="CLK11P" pad="P2"/>
<connect gate="B" pin="CLK8P" pad="R4"/>
<connect gate="B" pin="CLK9N" pad="T2"/>
<connect gate="B" pin="CLK9P" pad="R2"/>
<connect gate="B" pin="GND" pad="P1"/>
<connect gate="B" pin="GNDA_PLL3" pad="R5"/>
<connect gate="B" pin="GNDA_PLL4" pad="P5"/>
<connect gate="B" pin="GNDG_PLL3" pad="R7"/>
<connect gate="B" pin="GNDG_PLL4" pad="P7"/>
<connect gate="B" pin="GND_2" pad="R1"/>
<connect gate="B" pin="GND_3" pad="A14"/>
<connect gate="B" pin="GND_4" pad="A15"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="T1"/>
<connect gate="B" pin="IO_11" pad="N4"/>
<connect gate="B" pin="IO_12" pad="T3"/>
<connect gate="B" pin="IO_13" pad="M9"/>
<connect gate="B" pin="IO_14" pad="T4"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="T5"/>
<connect gate="B" pin="IO_17" pad="N1"/>
<connect gate="B" pin="IO_18" pad="T6"/>
<connect gate="B" pin="IO_19" pad="P3"/>
<connect gate="B" pin="IO_2" pad="M2"/>
<connect gate="B" pin="IO_20" pad="T7"/>
<connect gate="B" pin="IO_21" pad="N6"/>
<connect gate="B" pin="IO_22" pad="T8"/>
<connect gate="B" pin="IO_23" pad="U2"/>
<connect gate="B" pin="IO_24" pad="N7"/>
<connect gate="B" pin="IO_25" pad="U3"/>
<connect gate="B" pin="IO_26" pad="T9"/>
<connect gate="B" pin="IO_27" pad="N9"/>
<connect gate="B" pin="IO_28" pad="U4"/>
<connect gate="B" pin="IO_29" pad="R3"/>
<connect gate="B" pin="IO_3" pad="M3"/>
<connect gate="B" pin="IO_30" pad="N8"/>
<connect gate="B" pin="IO_31" pad="U5"/>
<connect gate="B" pin="IO_32" pad="U6"/>
<connect gate="B" pin="IO_33" pad="U7"/>
<connect gate="B" pin="IO_34" pad="U8"/>
<connect gate="B" pin="IO_35" pad="U9"/>
<connect gate="B" pin="IO_36" pad="V1"/>
<connect gate="B" pin="IO_37" pad="V2"/>
<connect gate="B" pin="IO_38" pad="V3"/>
<connect gate="B" pin="IO_39" pad="V4"/>
<connect gate="B" pin="IO_4" pad="M4"/>
<connect gate="B" pin="IO_40" pad="V5"/>
<connect gate="B" pin="IO_41" pad="V6"/>
<connect gate="B" pin="IO_42" pad="V7"/>
<connect gate="B" pin="IO_43" pad="V8"/>
<connect gate="B" pin="IO_44" pad="V9"/>
<connect gate="B" pin="IO_45" pad="W1"/>
<connect gate="B" pin="IO_46" pad="W2"/>
<connect gate="B" pin="IO_47" pad="W3"/>
<connect gate="B" pin="IO_48" pad="W4"/>
<connect gate="B" pin="IO_49" pad="W5"/>
<connect gate="B" pin="IO_5" pad="M5"/>
<connect gate="B" pin="IO_50" pad="W6"/>
<connect gate="B" pin="IO_51" pad="W7"/>
<connect gate="B" pin="IO_52" pad="W8"/>
<connect gate="B" pin="IO_53" pad="Y1"/>
<connect gate="B" pin="IO_54" pad="Y2"/>
<connect gate="B" pin="IO_55" pad="Y3"/>
<connect gate="B" pin="IO_56" pad="Y4"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="M6"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A11"/>
<connect gate="B" pin="IO_64" pad="A13"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A18"/>
<connect gate="B" pin="IO_67" pad="A19"/>
<connect gate="B" pin="IO_68" pad="A20"/>
<connect gate="B" pin="IO_69" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_70" pad="A22"/>
<connect gate="B" pin="IO_71" pad="A23"/>
<connect gate="B" pin="IO_72" pad="A24"/>
<connect gate="B" pin="IO_73" pad="A25"/>
<connect gate="B" pin="IO_8" pad="N3"/>
<connect gate="B" pin="IO_9" pad="M8"/>
<connect gate="B" pin="VCCA_PLL3" pad="R6"/>
<connect gate="B" pin="VCCA_PLL4" pad="P6"/>
<connect gate="B" pin="VCCG_PLL3" pad="R8"/>
<connect gate="B" pin="VCCG_PLL4" pad="P8"/>
<connect gate="B" pin="VCCIO3" pad="A17"/>
<connect gate="B" pin="VCCIO4" pad="A12"/>
<connect gate="B" pin="VCCIO5" pad="P9"/>
<connect gate="B" pin="VCCIO5_2" pad="M1"/>
<connect gate="B" pin="VCCIO6" pad="U1"/>
<connect gate="B" pin="VCCIO6_2" pad="R9"/>
<connect gate="B" pin="VREF1B6" pad="W9"/>
<connect gate="C" pin="GND" pad="B27"/>
<connect gate="C" pin="GND_2" pad="AF3"/>
<connect gate="C" pin="GND_3" pad="AG2"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AE9"/>
<connect gate="C" pin="IO_11" pad="AB8"/>
<connect gate="C" pin="IO_12" pad="AF1"/>
<connect gate="C" pin="IO_13" pad="AB9"/>
<connect gate="C" pin="IO_14" pad="AA1"/>
<connect gate="C" pin="IO_15" pad="AC1"/>
<connect gate="C" pin="IO_16" pad="AA2"/>
<connect gate="C" pin="IO_17" pad="AC2"/>
<connect gate="C" pin="IO_18" pad="AA3"/>
<connect gate="C" pin="IO_19" pad="AA4"/>
<connect gate="C" pin="IO_2" pad="AE1"/>
<connect gate="C" pin="IO_20" pad="AA5"/>
<connect gate="C" pin="IO_21" pad="AC5"/>
<connect gate="C" pin="IO_22" pad="AA6"/>
<connect gate="C" pin="IO_23" pad="AA7"/>
<connect gate="C" pin="IO_24" pad="AC7"/>
<connect gate="C" pin="IO_25" pad="AA8"/>
<connect gate="C" pin="IO_26" pad="AC8"/>
<connect gate="C" pin="IO_27" pad="AA9"/>
<connect gate="C" pin="IO_28" pad="AC9"/>
<connect gate="C" pin="IO_29" pad="AB1"/>
<connect gate="C" pin="IO_3" pad="AE2"/>
<connect gate="C" pin="IO_30" pad="AD1"/>
<connect gate="C" pin="IO_31" pad="AB2"/>
<connect gate="C" pin="IO_32" pad="AD2"/>
<connect gate="C" pin="IO_33" pad="AB3"/>
<connect gate="C" pin="IO_34" pad="AB4"/>
<connect gate="C" pin="IO_35" pad="AD5"/>
<connect gate="C" pin="IO_36" pad="AD6"/>
<connect gate="C" pin="IO_37" pad="AD8"/>
<connect gate="C" pin="IO_38" pad="AF2"/>
<connect gate="C" pin="IO_39" pad="AF4"/>
<connect gate="C" pin="IO_4" pad="AE4"/>
<connect gate="C" pin="IO_40" pad="AF5"/>
<connect gate="C" pin="IO_41" pad="AF6"/>
<connect gate="C" pin="IO_42" pad="AF7"/>
<connect gate="C" pin="IO_43" pad="AF8"/>
<connect gate="C" pin="IO_44" pad="AF9"/>
<connect gate="C" pin="IO_45" pad="AG3"/>
<connect gate="C" pin="IO_46" pad="AG4"/>
<connect gate="C" pin="IO_47" pad="AG5"/>
<connect gate="C" pin="IO_48" pad="AG6"/>
<connect gate="C" pin="IO_49" pad="AG7"/>
<connect gate="C" pin="IO_5" pad="AE5"/>
<connect gate="C" pin="IO_50" pad="AG8"/>
<connect gate="C" pin="IO_51" pad="AG9"/>
<connect gate="C" pin="IO_52" pad="AH3"/>
<connect gate="C" pin="IO_53" pad="AH4"/>
<connect gate="C" pin="IO_54" pad="AH5"/>
<connect gate="C" pin="IO_55" pad="AH6"/>
<connect gate="C" pin="IO_56" pad="AH7"/>
<connect gate="C" pin="IO_57" pad="AH8"/>
<connect gate="C" pin="IO_58" pad="AH9"/>
<connect gate="C" pin="IO_59" pad="B10"/>
<connect gate="C" pin="IO_6" pad="AE6"/>
<connect gate="C" pin="IO_60" pad="B11"/>
<connect gate="C" pin="IO_61" pad="B12"/>
<connect gate="C" pin="IO_62" pad="B13"/>
<connect gate="C" pin="IO_63" pad="B15"/>
<connect gate="C" pin="IO_64" pad="B16"/>
<connect gate="C" pin="IO_65" pad="B17"/>
<connect gate="C" pin="IO_66" pad="B18"/>
<connect gate="C" pin="IO_67" pad="B19"/>
<connect gate="C" pin="IO_68" pad="B20"/>
<connect gate="C" pin="IO_69" pad="B21"/>
<connect gate="C" pin="IO_7" pad="AE7"/>
<connect gate="C" pin="IO_70" pad="B22"/>
<connect gate="C" pin="IO_71" pad="B23"/>
<connect gate="C" pin="IO_72" pad="B24"/>
<connect gate="C" pin="IO_73" pad="B25"/>
<connect gate="C" pin="IO_74" pad="B26"/>
<connect gate="C" pin="IO_75" pad="C10"/>
<connect gate="C" pin="IO_76" pad="C11"/>
<connect gate="C" pin="IO_77" pad="C12"/>
<connect gate="C" pin="IO_78" pad="C13"/>
<connect gate="C" pin="IO_79" pad="C15"/>
<connect gate="C" pin="IO_8" pad="AE8"/>
<connect gate="C" pin="IO_9" pad="AB7"/>
<connect gate="C" pin="NC" pad="AD4"/>
<connect gate="C" pin="NC_2" pad="AB5"/>
<connect gate="C" pin="NC_3" pad="AB6"/>
<connect gate="C" pin="NC_4" pad="AC6"/>
<connect gate="C" pin="NC_5" pad="AC3"/>
<connect gate="C" pin="NC_6" pad="AC4"/>
<connect gate="C" pin="NC_7" pad="AD3"/>
<connect gate="C" pin="TEMPDIODEN" pad="C14"/>
<connect gate="C" pin="TEMPDIODEP" pad="B14"/>
<connect gate="C" pin="VCCIO2" pad="B28"/>
<connect gate="C" pin="VCCIO3" pad="A27"/>
<connect gate="C" pin="VCCIO6" pad="AG1"/>
<connect gate="C" pin="VCCIO7" pad="AH2"/>
<connect gate="C" pin="VREF0B6" pad="AE3"/>
<connect gate="C" pin="VREF1B7" pad="AD9"/>
<connect gate="C" pin="VREF2B7" pad="AD7"/>
<connect gate="D" pin="CONF_DONE" pad="G17"/>
<connect gate="D" pin="DCLK" pad="F16"/>
<connect gate="D" pin="GND" pad="C26"/>
<connect gate="D" pin="GNDA_PLL5" pad="G14"/>
<connect gate="D" pin="GNDG_PLL5" pad="E14"/>
<connect gate="D" pin="GND_2" pad="G15"/>
<connect gate="D" pin="GND_3" pad="G20"/>
<connect gate="D" pin="GND_4" pad="H16"/>
<connect gate="D" pin="IO" pad="H19"/>
<connect gate="D" pin="IO_10" pad="C20"/>
<connect gate="D" pin="IO_11" pad="D13"/>
<connect gate="D" pin="IO_12" pad="C21"/>
<connect gate="D" pin="IO_13" pad="D27"/>
<connect gate="D" pin="IO_14" pad="C22"/>
<connect gate="D" pin="IO_15" pad="D28"/>
<connect gate="D" pin="IO_16" pad="D15"/>
<connect gate="D" pin="IO_17" pad="E10"/>
<connect gate="D" pin="IO_18" pad="C23"/>
<connect gate="D" pin="IO_19" pad="D16"/>
<connect gate="D" pin="IO_2" pad="C27"/>
<connect gate="D" pin="IO_20" pad="E12"/>
<connect gate="D" pin="IO_21" pad="C24"/>
<connect gate="D" pin="IO_22" pad="E13"/>
<connect gate="D" pin="IO_23" pad="D17"/>
<connect gate="D" pin="IO_24" pad="C25"/>
<connect gate="D" pin="IO_25" pad="E15"/>
<connect gate="D" pin="IO_26" pad="D18"/>
<connect gate="D" pin="IO_27" pad="E16"/>
<connect gate="D" pin="IO_28" pad="D19"/>
<connect gate="D" pin="IO_29" pad="E17"/>
<connect gate="D" pin="IO_3" pad="C28"/>
<connect gate="D" pin="IO_30" pad="D20"/>
<connect gate="D" pin="IO_31" pad="D21"/>
<connect gate="D" pin="IO_32" pad="E27"/>
<connect gate="D" pin="IO_33" pad="D22"/>
<connect gate="D" pin="IO_34" pad="E19"/>
<connect gate="D" pin="IO_35" pad="D23"/>
<connect gate="D" pin="IO_36" pad="E23"/>
<connect gate="D" pin="IO_37" pad="D24"/>
<connect gate="D" pin="IO_38" pad="E21"/>
<connect gate="D" pin="IO_39" pad="E28"/>
<connect gate="D" pin="IO_4" pad="C17"/>
<connect gate="D" pin="IO_40" pad="F10"/>
<connect gate="D" pin="IO_41" pad="F11"/>
<connect gate="D" pin="IO_42" pad="F12"/>
<connect gate="D" pin="IO_43" pad="F17"/>
<connect gate="D" pin="IO_44" pad="F25"/>
<connect gate="D" pin="IO_45" pad="F18"/>
<connect gate="D" pin="IO_46" pad="F26"/>
<connect gate="D" pin="IO_47" pad="F19"/>
<connect gate="D" pin="IO_48" pad="F27"/>
<connect gate="D" pin="IO_49" pad="F20"/>
<connect gate="D" pin="IO_5" pad="D10"/>
<connect gate="D" pin="IO_50" pad="F28"/>
<connect gate="D" pin="IO_51" pad="F21"/>
<connect gate="D" pin="IO_52" pad="G10"/>
<connect gate="D" pin="IO_53" pad="F22"/>
<connect gate="D" pin="IO_54" pad="G18"/>
<connect gate="D" pin="IO_55" pad="G11"/>
<connect gate="D" pin="IO_56" pad="G19"/>
<connect gate="D" pin="IO_57" pad="G12"/>
<connect gate="D" pin="IO_58" pad="G21"/>
<connect gate="D" pin="IO_59" pad="G22"/>
<connect gate="D" pin="IO_6" pad="C18"/>
<connect gate="D" pin="IO_60" pad="G23"/>
<connect gate="D" pin="IO_61" pad="G24"/>
<connect gate="D" pin="IO_62" pad="G25"/>
<connect gate="D" pin="IO_63" pad="G26"/>
<connect gate="D" pin="IO_64" pad="G27"/>
<connect gate="D" pin="IO_65" pad="G28"/>
<connect gate="D" pin="IO_66" pad="H10"/>
<connect gate="D" pin="IO_67" pad="H11"/>
<connect gate="D" pin="IO_68" pad="H12"/>
<connect gate="D" pin="IO_69" pad="H14"/>
<connect gate="D" pin="IO_7" pad="D11"/>
<connect gate="D" pin="IO_70" pad="H15"/>
<connect gate="D" pin="IO_71" pad="H17"/>
<connect gate="D" pin="IO_72" pad="H18"/>
<connect gate="D" pin="IO_8" pad="C19"/>
<connect gate="D" pin="IO_9" pad="D12"/>
<connect gate="D" pin="NC" pad="F24"/>
<connect gate="D" pin="NC_2" pad="E25"/>
<connect gate="D" pin="NC_3" pad="F23"/>
<connect gate="D" pin="NC_4" pad="D25"/>
<connect gate="D" pin="NC_5" pad="E26"/>
<connect gate="D" pin="NC_6" pad="D26"/>
<connect gate="D" pin="TDI" pad="G13"/>
<connect gate="D" pin="TDO" pad="H13"/>
<connect gate="D" pin="TMS" pad="F13"/>
<connect gate="D" pin="VCCA_PLL5" pad="F14"/>
<connect gate="D" pin="VCCG_PLL5" pad="D14"/>
<connect gate="D" pin="VCC_PLL5_OUTA" pad="F15"/>
<connect gate="D" pin="VCC_PLL5_OUTB" pad="G16"/>
<connect gate="D" pin="VREF0B2" pad="E24"/>
<connect gate="D" pin="VREF0B3" pad="E18"/>
<connect gate="D" pin="VREF1B3" pad="E20"/>
<connect gate="D" pin="VREF2B3" pad="E22"/>
<connect gate="D" pin="VREF2B4" pad="E11"/>
<connect gate="E" pin="CLK12P" pad="K13"/>
<connect gate="E" pin="CLK13P" pad="M13"/>
<connect gate="E" pin="CLK14P" pad="K17"/>
<connect gate="E" pin="CLK15P" pad="M17"/>
<connect gate="E" pin="GND" pad="L15"/>
<connect gate="E" pin="GND_2" pad="N14"/>
<connect gate="E" pin="GND_3" pad="N18"/>
<connect gate="E" pin="GND_4" pad="L14"/>
<connect gate="E" pin="GND_5" pad="N16"/>
<connect gate="E" pin="GND_6" pad="N12"/>
<connect gate="E" pin="GND_7" pad="M15"/>
<connect gate="E" pin="IO" pad="N22"/>
<connect gate="E" pin="IO_10" pad="J18"/>
<connect gate="E" pin="IO_11" pad="H26"/>
<connect gate="E" pin="IO_12" pad="J19"/>
<connect gate="E" pin="IO_13" pad="H27"/>
<connect gate="E" pin="IO_14" pad="J20"/>
<connect gate="E" pin="IO_15" pad="H28"/>
<connect gate="E" pin="IO_16" pad="J21"/>
<connect gate="E" pin="IO_17" pad="J10"/>
<connect gate="E" pin="IO_18" pad="J22"/>
<connect gate="E" pin="IO_19" pad="J11"/>
<connect gate="E" pin="IO_2" pad="H21"/>
<connect gate="E" pin="IO_20" pad="J23"/>
<connect gate="E" pin="IO_21" pad="J12"/>
<connect gate="E" pin="IO_22" pad="J24"/>
<connect gate="E" pin="IO_23" pad="K14"/>
<connect gate="E" pin="IO_24" pad="J13"/>
<connect gate="E" pin="IO_25" pad="K15"/>
<connect gate="E" pin="IO_26" pad="J25"/>
<connect gate="E" pin="IO_27" pad="K16"/>
<connect gate="E" pin="IO_28" pad="J26"/>
<connect gate="E" pin="IO_29" pad="J27"/>
<connect gate="E" pin="IO_3" pad="H20"/>
<connect gate="E" pin="IO_30" pad="K18"/>
<connect gate="E" pin="IO_31" pad="J28"/>
<connect gate="E" pin="IO_32" pad="K19"/>
<connect gate="E" pin="IO_33" pad="K10"/>
<connect gate="E" pin="IO_34" pad="K11"/>
<connect gate="E" pin="IO_35" pad="K21"/>
<connect gate="E" pin="IO_36" pad="K22"/>
<connect gate="E" pin="IO_37" pad="K23"/>
<connect gate="E" pin="IO_38" pad="K24"/>
<connect gate="E" pin="IO_39" pad="K25"/>
<connect gate="E" pin="IO_4" pad="H22"/>
<connect gate="E" pin="IO_40" pad="K26"/>
<connect gate="E" pin="IO_41" pad="K27"/>
<connect gate="E" pin="IO_42" pad="K28"/>
<connect gate="E" pin="IO_43" pad="L10"/>
<connect gate="E" pin="IO_44" pad="L11"/>
<connect gate="E" pin="IO_45" pad="L13"/>
<connect gate="E" pin="IO_46" pad="L17"/>
<connect gate="E" pin="IO_47" pad="L18"/>
<connect gate="E" pin="IO_48" pad="L19"/>
<connect gate="E" pin="IO_49" pad="L20"/>
<connect gate="E" pin="IO_5" pad="H23"/>
<connect gate="E" pin="IO_50" pad="L21"/>
<connect gate="E" pin="IO_51" pad="L22"/>
<connect gate="E" pin="IO_52" pad="L23"/>
<connect gate="E" pin="IO_53" pad="L24"/>
<connect gate="E" pin="IO_54" pad="L25"/>
<connect gate="E" pin="IO_55" pad="L26"/>
<connect gate="E" pin="IO_56" pad="L27"/>
<connect gate="E" pin="IO_57" pad="L28"/>
<connect gate="E" pin="IO_58" pad="M10"/>
<connect gate="E" pin="IO_59" pad="M11"/>
<connect gate="E" pin="IO_6" pad="J16"/>
<connect gate="E" pin="IO_60" pad="M12"/>
<connect gate="E" pin="IO_61" pad="M18"/>
<connect gate="E" pin="IO_62" pad="M19"/>
<connect gate="E" pin="IO_63" pad="M20"/>
<connect gate="E" pin="IO_64" pad="M21"/>
<connect gate="E" pin="IO_65" pad="M22"/>
<connect gate="E" pin="IO_66" pad="M23"/>
<connect gate="E" pin="IO_67" pad="M24"/>
<connect gate="E" pin="IO_68" pad="M25"/>
<connect gate="E" pin="IO_69" pad="M26"/>
<connect gate="E" pin="IO_7" pad="H24"/>
<connect gate="E" pin="IO_70" pad="M27"/>
<connect gate="E" pin="IO_71" pad="N10"/>
<connect gate="E" pin="IO_72" pad="N19"/>
<connect gate="E" pin="IO_73" pad="N20"/>
<connect gate="E" pin="IO_74" pad="N21"/>
<connect gate="E" pin="IO_8" pad="J17"/>
<connect gate="E" pin="IO_9" pad="H25"/>
<connect gate="E" pin="NCONFIG" pad="L16"/>
<connect gate="E" pin="NSTATUS" pad="M16"/>
<connect gate="E" pin="TCK" pad="K12"/>
<connect gate="E" pin="TRST" pad="L12"/>
<connect gate="E" pin="VCCINT" pad="N17"/>
<connect gate="E" pin="VCCINT_2" pad="M14"/>
<connect gate="E" pin="VCCINT_3" pad="N13"/>
<connect gate="E" pin="VCCINT_4" pad="N11"/>
<connect gate="E" pin="VCCINT_5" pad="N15"/>
<connect gate="E" pin="VCCIO2" pad="M28"/>
<connect gate="E" pin="VCCIO3" pad="J15"/>
<connect gate="E" pin="VCCIO4" pad="J14"/>
<connect gate="E" pin="VREF1B2" pad="K20"/>
<connect gate="F" pin="CLK0N" pad="N27"/>
<connect gate="F" pin="CLK0P" pad="P27"/>
<connect gate="F" pin="CLK1P" pad="P25"/>
<connect gate="F" pin="CLK2N" pad="T27"/>
<connect gate="F" pin="CLK2P" pad="R27"/>
<connect gate="F" pin="CLK3P" pad="R25"/>
<connect gate="F" pin="GND" pad="U18"/>
<connect gate="F" pin="GNDA_PLL1" pad="P24"/>
<connect gate="F" pin="GNDA_PLL2" pad="R24"/>
<connect gate="F" pin="GNDG_PLL1" pad="P22"/>
<connect gate="F" pin="GNDG_PLL2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="R18"/>
<connect gate="F" pin="GND_11" pad="R16"/>
<connect gate="F" pin="GND_12" pad="T11"/>
<connect gate="F" pin="GND_13" pad="R12"/>
<connect gate="F" pin="GND_14" pad="R14"/>
<connect gate="F" pin="GND_15" pad="V15"/>
<connect gate="F" pin="GND_16" pad="U12"/>
<connect gate="F" pin="GND_17" pad="V17"/>
<connect gate="F" pin="GND_18" pad="P17"/>
<connect gate="F" pin="GND_19" pad="T13"/>
<connect gate="F" pin="GND_2" pad="P11"/>
<connect gate="F" pin="GND_20" pad="P18"/>
<connect gate="F" pin="GND_21" pad="U14"/>
<connect gate="F" pin="GND_22" pad="T15"/>
<connect gate="F" pin="GND_23" pad="U16"/>
<connect gate="F" pin="GND_24" pad="T17"/>
<connect gate="F" pin="GND_3" pad="P28"/>
<connect gate="F" pin="GND_4" pad="P15"/>
<connect gate="F" pin="GND_5" pad="P13"/>
<connect gate="F" pin="GND_6" pad="R28"/>
<connect gate="F" pin="GND_7" pad="V13"/>
<connect gate="F" pin="GND_8" pad="R11"/>
<connect gate="F" pin="GND_9" pad="V14"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="T19"/>
<connect gate="F" pin="IO_11" pad="T20"/>
<connect gate="F" pin="IO_12" pad="T21"/>
<connect gate="F" pin="IO_13" pad="T22"/>
<connect gate="F" pin="IO_14" pad="T23"/>
<connect gate="F" pin="IO_15" pad="T24"/>
<connect gate="F" pin="IO_16" pad="T25"/>
<connect gate="F" pin="IO_17" pad="T26"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U10"/>
<connect gate="F" pin="IO_2" pad="N23"/>
<connect gate="F" pin="IO_20" pad="U19"/>
<connect gate="F" pin="IO_21" pad="U20"/>
<connect gate="F" pin="IO_22" pad="U21"/>
<connect gate="F" pin="IO_23" pad="U22"/>
<connect gate="F" pin="IO_24" pad="U23"/>
<connect gate="F" pin="IO_25" pad="U24"/>
<connect gate="F" pin="IO_26" pad="U25"/>
<connect gate="F" pin="IO_27" pad="U26"/>
<connect gate="F" pin="IO_28" pad="U27"/>
<connect gate="F" pin="IO_29" pad="V10"/>
<connect gate="F" pin="IO_3" pad="R26"/>
<connect gate="F" pin="IO_30" pad="V11"/>
<connect gate="F" pin="IO_31" pad="V18"/>
<connect gate="F" pin="IO_32" pad="V19"/>
<connect gate="F" pin="IO_33" pad="V20"/>
<connect gate="F" pin="IO_34" pad="V21"/>
<connect gate="F" pin="IO_35" pad="V22"/>
<connect gate="F" pin="IO_36" pad="V23"/>
<connect gate="F" pin="IO_37" pad="V24"/>
<connect gate="F" pin="IO_4" pad="N24"/>
<connect gate="F" pin="IO_5" pad="N28"/>
<connect gate="F" pin="IO_6" pad="P26"/>
<connect gate="F" pin="IO_7" pad="T10"/>
<connect gate="F" pin="IO_8" pad="N25"/>
<connect gate="F" pin="IO_9" pad="N26"/>
<connect gate="F" pin="NC" pad="R10"/>
<connect gate="F" pin="NC_2" pad="P19"/>
<connect gate="F" pin="VCCA_PLL1" pad="P23"/>
<connect gate="F" pin="VCCA_PLL2" pad="R23"/>
<connect gate="F" pin="VCCA_PLL3" pad="R19"/>
<connect gate="F" pin="VCCG_PLL1" pad="P21"/>
<connect gate="F" pin="VCCG_PLL2" pad="R21"/>
<connect gate="F" pin="VCCINT" pad="T14"/>
<connect gate="F" pin="VCCINT_10" pad="R17"/>
<connect gate="F" pin="VCCINT_11" pad="R15"/>
<connect gate="F" pin="VCCINT_12" pad="T18"/>
<connect gate="F" pin="VCCINT_13" pad="T12"/>
<connect gate="F" pin="VCCINT_14" pad="P16"/>
<connect gate="F" pin="VCCINT_15" pad="U13"/>
<connect gate="F" pin="VCCINT_16" pad="U17"/>
<connect gate="F" pin="VCCINT_2" pad="V16"/>
<connect gate="F" pin="VCCINT_3" pad="V12"/>
<connect gate="F" pin="VCCINT_4" pad="U11"/>
<connect gate="F" pin="VCCINT_5" pad="P12"/>
<connect gate="F" pin="VCCINT_6" pad="U15"/>
<connect gate="F" pin="VCCINT_7" pad="R13"/>
<connect gate="F" pin="VCCINT_8" pad="T16"/>
<connect gate="F" pin="VCCINT_9" pad="P14"/>
<connect gate="F" pin="VCCIO1" pad="R20"/>
<connect gate="F" pin="VCCIO1_2" pad="U28"/>
<connect gate="F" pin="VCCIO2" pad="P20"/>
<connect gate="F" pin="VREF0B5" pad="P10"/>
<connect gate="G" pin="CLK4P" pad="AC17"/>
<connect gate="G" pin="CLK5P" pad="AA17"/>
<connect gate="G" pin="CLK7P" pad="W13"/>
<connect gate="G" pin="GND" pad="AC15"/>
<connect gate="G" pin="GNDG_PLL6" pad="AB14"/>
<connect gate="G" pin="GND_2" pad="AA16"/>
<connect gate="G" pin="IO" pad="AC28"/>
<connect gate="G" pin="IO_10" pad="W27"/>
<connect gate="G" pin="IO_11" pad="W14"/>
<connect gate="G" pin="IO_12" pad="W28"/>
<connect gate="G" pin="IO_13" pad="V28"/>
<connect gate="G" pin="IO_14" pad="Y10"/>
<connect gate="G" pin="IO_15" pad="W15"/>
<connect gate="G" pin="IO_16" pad="Y11"/>
<connect gate="G" pin="IO_17" pad="W10"/>
<connect gate="G" pin="IO_18" pad="W16"/>
<connect gate="G" pin="IO_19" pad="Y13"/>
<connect gate="G" pin="IO_2" pad="W21"/>
<connect gate="G" pin="IO_20" pad="W11"/>
<connect gate="G" pin="IO_21" pad="W12"/>
<connect gate="G" pin="IO_22" pad="W18"/>
<connect gate="G" pin="IO_23" pad="Y16"/>
<connect gate="G" pin="IO_24" pad="W19"/>
<connect gate="G" pin="IO_25" pad="Y17"/>
<connect gate="G" pin="IO_26" pad="Y18"/>
<connect gate="G" pin="IO_27" pad="Y19"/>
<connect gate="G" pin="IO_28" pad="Y20"/>
<connect gate="G" pin="IO_29" pad="Y21"/>
<connect gate="G" pin="IO_3" pad="W22"/>
<connect gate="G" pin="IO_30" pad="Y22"/>
<connect gate="G" pin="IO_31" pad="Y23"/>
<connect gate="G" pin="IO_32" pad="Y24"/>
<connect gate="G" pin="IO_33" pad="Y25"/>
<connect gate="G" pin="IO_34" pad="Y26"/>
<connect gate="G" pin="IO_35" pad="Y27"/>
<connect gate="G" pin="IO_36" pad="Y28"/>
<connect gate="G" pin="IO_37" pad="AA10"/>
<connect gate="G" pin="IO_38" pad="AA11"/>
<connect gate="G" pin="IO_39" pad="AA14"/>
<connect gate="G" pin="IO_4" pad="W23"/>
<connect gate="G" pin="IO_40" pad="AA15"/>
<connect gate="G" pin="IO_41" pad="AA18"/>
<connect gate="G" pin="IO_42" pad="AA19"/>
<connect gate="G" pin="IO_43" pad="AA20"/>
<connect gate="G" pin="IO_44" pad="AA21"/>
<connect gate="G" pin="IO_45" pad="AA22"/>
<connect gate="G" pin="IO_46" pad="AA23"/>
<connect gate="G" pin="IO_47" pad="AA24"/>
<connect gate="G" pin="IO_48" pad="AA25"/>
<connect gate="G" pin="IO_49" pad="AA26"/>
<connect gate="G" pin="IO_5" pad="W24"/>
<connect gate="G" pin="IO_50" pad="AA27"/>
<connect gate="G" pin="IO_51" pad="AA28"/>
<connect gate="G" pin="IO_52" pad="AB10"/>
<connect gate="G" pin="IO_53" pad="AB11"/>
<connect gate="G" pin="IO_54" pad="AB12"/>
<connect gate="G" pin="IO_55" pad="AB17"/>
<connect gate="G" pin="IO_56" pad="AB18"/>
<connect gate="G" pin="IO_57" pad="AB19"/>
<connect gate="G" pin="IO_58" pad="AB20"/>
<connect gate="G" pin="IO_59" pad="AB21"/>
<connect gate="G" pin="IO_6" pad="W25"/>
<connect gate="G" pin="IO_60" pad="AB22"/>
<connect gate="G" pin="IO_61" pad="AB25"/>
<connect gate="G" pin="IO_62" pad="AB26"/>
<connect gate="G" pin="IO_63" pad="AB27"/>
<connect gate="G" pin="IO_64" pad="AB28"/>
<connect gate="G" pin="IO_65" pad="AC10"/>
<connect gate="G" pin="IO_66" pad="AC11"/>
<connect gate="G" pin="IO_67" pad="AC19"/>
<connect gate="G" pin="IO_68" pad="AC20"/>
<connect gate="G" pin="IO_69" pad="AC21"/>
<connect gate="G" pin="IO_7" pad="V26"/>
<connect gate="G" pin="IO_70" pad="AC22"/>
<connect gate="G" pin="IO_71" pad="AC23"/>
<connect gate="G" pin="IO_72" pad="AC27"/>
<connect gate="G" pin="IO_8" pad="W26"/>
<connect gate="G" pin="IO_9" pad="V27"/>
<connect gate="G" pin="MSEL0" pad="AC16"/>
<connect gate="G" pin="MSEL1" pad="W17"/>
<connect gate="G" pin="MSEL2" pad="AB15"/>
<connect gate="G" pin="NC" pad="AB24"/>
<connect gate="G" pin="NCE" pad="AB13"/>
<connect gate="G" pin="NCEO" pad="AC13"/>
<connect gate="G" pin="NC_2" pad="AC24"/>
<connect gate="G" pin="NC_3" pad="AC25"/>
<connect gate="G" pin="NC_4" pad="AB23"/>
<connect gate="G" pin="NC_5" pad="AC26"/>
<connect gate="G" pin="NIO_PULLUP" pad="Y12"/>
<connect gate="G" pin="PLL_ENA" pad="AC18"/>
<connect gate="G" pin="PORSEL" pad="AC12"/>
<connect gate="G" pin="VCCG_PLL6" pad="AA13"/>
<connect gate="G" pin="VCCIO7" pad="Y14"/>
<connect gate="G" pin="VCCIO8" pad="Y15"/>
<connect gate="G" pin="VCCSEL" pad="AA12"/>
<connect gate="G" pin="VCC_PLL6_OUTA" pad="AC14"/>
<connect gate="G" pin="VCC_PLL6_OUTB" pad="AB16"/>
<connect gate="G" pin="VREF1B1" pad="W20"/>
<connect gate="H" pin="CLK6P" pad="AD14"/>
<connect gate="H" pin="GND" pad="AH15"/>
<connect gate="H" pin="GNDA_PLL6" pad="AF14"/>
<connect gate="H" pin="GND_2" pad="AG27"/>
<connect gate="H" pin="GND_3" pad="AF26"/>
<connect gate="H" pin="GND_4" pad="AH14"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD13"/>
<connect gate="H" pin="IO_11" pad="AD18"/>
<connect gate="H" pin="IO_12" pad="AD19"/>
<connect gate="H" pin="IO_13" pad="AD27"/>
<connect gate="H" pin="IO_14" pad="AD28"/>
<connect gate="H" pin="IO_15" pad="AE10"/>
<connect gate="H" pin="IO_16" pad="AE11"/>
<connect gate="H" pin="IO_17" pad="AE12"/>
<connect gate="H" pin="IO_18" pad="AE13"/>
<connect gate="H" pin="IO_19" pad="AE14"/>
<connect gate="H" pin="IO_2" pad="AD23"/>
<connect gate="H" pin="IO_20" pad="AE15"/>
<connect gate="H" pin="IO_21" pad="AE16"/>
<connect gate="H" pin="IO_22" pad="AE17"/>
<connect gate="H" pin="IO_23" pad="AE18"/>
<connect gate="H" pin="IO_24" pad="AE19"/>
<connect gate="H" pin="IO_25" pad="AE20"/>
<connect gate="H" pin="IO_26" pad="AE21"/>
<connect gate="H" pin="IO_27" pad="AE22"/>
<connect gate="H" pin="IO_28" pad="AE23"/>
<connect gate="H" pin="IO_29" pad="AE24"/>
<connect gate="H" pin="IO_3" pad="AD10"/>
<connect gate="H" pin="IO_30" pad="AE25"/>
<connect gate="H" pin="IO_31" pad="AF15"/>
<connect gate="H" pin="IO_32" pad="AF16"/>
<connect gate="H" pin="IO_33" pad="AE27"/>
<connect gate="H" pin="IO_34" pad="AF17"/>
<connect gate="H" pin="IO_35" pad="AE28"/>
<connect gate="H" pin="IO_36" pad="AF18"/>
<connect gate="H" pin="IO_37" pad="AF10"/>
<connect gate="H" pin="IO_38" pad="AF19"/>
<connect gate="H" pin="IO_39" pad="AF11"/>
<connect gate="H" pin="IO_4" pad="AD15"/>
<connect gate="H" pin="IO_40" pad="AF20"/>
<connect gate="H" pin="IO_41" pad="AF12"/>
<connect gate="H" pin="IO_42" pad="AF13"/>
<connect gate="H" pin="IO_43" pad="AF21"/>
<connect gate="H" pin="IO_44" pad="AF22"/>
<connect gate="H" pin="IO_45" pad="AF23"/>
<connect gate="H" pin="IO_46" pad="AF24"/>
<connect gate="H" pin="IO_47" pad="AF25"/>
<connect gate="H" pin="IO_48" pad="AF27"/>
<connect gate="H" pin="IO_49" pad="AF28"/>
<connect gate="H" pin="IO_5" pad="AD21"/>
<connect gate="H" pin="IO_50" pad="AG10"/>
<connect gate="H" pin="IO_51" pad="AG11"/>
<connect gate="H" pin="IO_52" pad="AG12"/>
<connect gate="H" pin="IO_53" pad="AG13"/>
<connect gate="H" pin="IO_54" pad="AG15"/>
<connect gate="H" pin="IO_55" pad="AG16"/>
<connect gate="H" pin="IO_56" pad="AG17"/>
<connect gate="H" pin="IO_57" pad="AG18"/>
<connect gate="H" pin="IO_58" pad="AG19"/>
<connect gate="H" pin="IO_59" pad="AG20"/>
<connect gate="H" pin="IO_6" pad="AD24"/>
<connect gate="H" pin="IO_60" pad="AG21"/>
<connect gate="H" pin="IO_61" pad="AG22"/>
<connect gate="H" pin="IO_62" pad="AG23"/>
<connect gate="H" pin="IO_63" pad="AG24"/>
<connect gate="H" pin="IO_64" pad="AG25"/>
<connect gate="H" pin="IO_65" pad="AG26"/>
<connect gate="H" pin="IO_66" pad="AH10"/>
<connect gate="H" pin="IO_67" pad="AH11"/>
<connect gate="H" pin="IO_68" pad="AH13"/>
<connect gate="H" pin="IO_69" pad="AH16"/>
<connect gate="H" pin="IO_7" pad="AD16"/>
<connect gate="H" pin="IO_70" pad="AH19"/>
<connect gate="H" pin="IO_71" pad="AH20"/>
<connect gate="H" pin="IO_72" pad="AH21"/>
<connect gate="H" pin="IO_73" pad="AH22"/>
<connect gate="H" pin="IO_74" pad="AH23"/>
<connect gate="H" pin="IO_75" pad="AH24"/>
<connect gate="H" pin="IO_76" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD12"/>
<connect gate="H" pin="IO_9" pad="AD17"/>
<connect gate="H" pin="NC" pad="AE26"/>
<connect gate="H" pin="NC_2" pad="AD25"/>
<connect gate="H" pin="NC_3" pad="AD26"/>
<connect gate="H" pin="VCCA_PLL6" pad="AG14"/>
<connect gate="H" pin="VCCIO1" pad="AG28"/>
<connect gate="H" pin="VCCIO7" pad="AH12"/>
<connect gate="H" pin="VCCIO8" pad="AH17"/>
<connect gate="H" pin="VCCIO8_2" pad="AH27"/>
<connect gate="H" pin="VREF0B7" pad="AD11"/>
<connect gate="H" pin="VREF0B8" pad="AD22"/>
<connect gate="H" pin="VREF1B8" pad="AD20"/>
<connect gate="H" pin="VREF2B8" pad="AH18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1S20F780C7N"/>
<attribute name="OC_FARNELL" value="1549495"/>
<attribute name="OC_NEWARK" value="52R0304"/>
<attribute name="PACKAGE" value="BGA-780"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1S25F672C7N">
<description>IC, FPGA, STRATIX</description>
<gates>
<gate name="A" symbol="EP1S25F672C7N_A"/>
<gate name="B" symbol="EP1S25F672C7N_B"/>
<gate name="C" symbol="EP1S25F672C7N_C"/>
<gate name="D" symbol="EP1S25F672C7N_D"/>
<gate name="E" symbol="EP1S25F672C7N_E"/>
<gate name="F" symbol="EP1S25F672C7N_F"/>
<gate name="G" symbol="EP1S25F672C7N_G"/>
</gates>
<devices>
<device name="" package="BGA672C100P26X26_2700X2700X350">
<connects>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="GND_2" pad="F8"/>
<connect gate="A" pin="GND_3" pad="G8"/>
<connect gate="A" pin="GND_4" pad="H9"/>
<connect gate="A" pin="GND_5" pad="J9"/>
<connect gate="A" pin="GND_6" pad="A2"/>
<connect gate="A" pin="GND_7" pad="B1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="C1"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="C4"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D2"/>
<connect gate="A" pin="IO_25" pad="D3"/>
<connect gate="A" pin="IO_26" pad="D4"/>
<connect gate="A" pin="IO_27" pad="D5"/>
<connect gate="A" pin="IO_28" pad="D6"/>
<connect gate="A" pin="IO_29" pad="E2"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="D8"/>
<connect gate="A" pin="IO_31" pad="E3"/>
<connect gate="A" pin="IO_32" pad="E4"/>
<connect gate="A" pin="IO_33" pad="E5"/>
<connect gate="A" pin="IO_34" pad="E6"/>
<connect gate="A" pin="IO_35" pad="E7"/>
<connect gate="A" pin="IO_36" pad="E8"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="E1"/>
<connect gate="A" pin="IO_39" pad="F1"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="F2"/>
<connect gate="A" pin="IO_41" pad="F3"/>
<connect gate="A" pin="IO_42" pad="F4"/>
<connect gate="A" pin="IO_43" pad="F5"/>
<connect gate="A" pin="IO_44" pad="F6"/>
<connect gate="A" pin="IO_45" pad="F7"/>
<connect gate="A" pin="IO_46" pad="F9"/>
<connect gate="A" pin="IO_47" pad="G1"/>
<connect gate="A" pin="IO_48" pad="G2"/>
<connect gate="A" pin="IO_49" pad="G3"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="G4"/>
<connect gate="A" pin="IO_51" pad="G5"/>
<connect gate="A" pin="IO_52" pad="G6"/>
<connect gate="A" pin="IO_53" pad="G7"/>
<connect gate="A" pin="IO_54" pad="G9"/>
<connect gate="A" pin="IO_55" pad="H1"/>
<connect gate="A" pin="IO_56" pad="H2"/>
<connect gate="A" pin="IO_57" pad="H3"/>
<connect gate="A" pin="IO_58" pad="H4"/>
<connect gate="A" pin="IO_59" pad="H5"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_60" pad="H6"/>
<connect gate="A" pin="IO_61" pad="H7"/>
<connect gate="A" pin="IO_62" pad="J1"/>
<connect gate="A" pin="IO_63" pad="J2"/>
<connect gate="A" pin="IO_64" pad="J3"/>
<connect gate="A" pin="IO_65" pad="J4"/>
<connect gate="A" pin="IO_66" pad="J5"/>
<connect gate="A" pin="IO_67" pad="J6"/>
<connect gate="A" pin="IO_68" pad="J7"/>
<connect gate="A" pin="IO_69" pad="J8"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_70" pad="K1"/>
<connect gate="A" pin="IO_71" pad="K2"/>
<connect gate="A" pin="IO_72" pad="K3"/>
<connect gate="A" pin="IO_73" pad="K4"/>
<connect gate="A" pin="IO_74" pad="K5"/>
<connect gate="A" pin="IO_75" pad="K6"/>
<connect gate="A" pin="IO_76" pad="K7"/>
<connect gate="A" pin="IO_77" pad="K8"/>
<connect gate="A" pin="IO_78" pad="K9"/>
<connect gate="A" pin="IO_79" pad="L2"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_80" pad="L3"/>
<connect gate="A" pin="IO_81" pad="L4"/>
<connect gate="A" pin="IO_82" pad="L5"/>
<connect gate="A" pin="IO_83" pad="L6"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="VCCIO2" pad="L1"/>
<connect gate="A" pin="VCCIO2_2" pad="D1"/>
<connect gate="A" pin="VCCIO3" pad="A4"/>
<connect gate="A" pin="VREF0B2" pad="H8"/>
<connect gate="A" pin="VREF1B3" pad="D9"/>
<connect gate="A" pin="VREF2B3" pad="D7"/>
<connect gate="B" pin="CLK0N" pad="N2"/>
<connect gate="B" pin="CLK0P" pad="N3"/>
<connect gate="B" pin="CLK13P" pad="A15"/>
<connect gate="B" pin="CLK1P" pad="M1"/>
<connect gate="B" pin="CLK2N" pad="R2"/>
<connect gate="B" pin="CLK2P" pad="R1"/>
<connect gate="B" pin="CLK3P" pad="R3"/>
<connect gate="B" pin="GND" pad="A14"/>
<connect gate="B" pin="GNDA_PLL1" pad="N5"/>
<connect gate="B" pin="GNDA_PLL2" pad="P3"/>
<connect gate="B" pin="GNDG_PLL1" pad="N4"/>
<connect gate="B" pin="GNDG_PLL2" pad="P2"/>
<connect gate="B" pin="GND_2" pad="N1"/>
<connect gate="B" pin="GND_3" pad="P9"/>
<connect gate="B" pin="GND_4" pad="V9"/>
<connect gate="B" pin="GND_5" pad="N9"/>
<connect gate="B" pin="GND_6" pad="A13"/>
<connect gate="B" pin="GND_7" pad="P1"/>
<connect gate="B" pin="IO" pad="A22"/>
<connect gate="B" pin="IO_10" pad="R8"/>
<connect gate="B" pin="IO_11" pad="M8"/>
<connect gate="B" pin="IO_12" pad="R9"/>
<connect gate="B" pin="IO_13" pad="M9"/>
<connect gate="B" pin="IO_14" pad="P6"/>
<connect gate="B" pin="IO_15" pad="N6"/>
<connect gate="B" pin="IO_16" pad="P7"/>
<connect gate="B" pin="IO_17" pad="U1"/>
<connect gate="B" pin="IO_18" pad="N7"/>
<connect gate="B" pin="IO_19" pad="T2"/>
<connect gate="B" pin="IO_2" pad="R4"/>
<connect gate="B" pin="IO_20" pad="P8"/>
<connect gate="B" pin="IO_21" pad="T3"/>
<connect gate="B" pin="IO_22" pad="N8"/>
<connect gate="B" pin="IO_23" pad="T4"/>
<connect gate="B" pin="IO_24" pad="T5"/>
<connect gate="B" pin="IO_25" pad="T6"/>
<connect gate="B" pin="IO_26" pad="T7"/>
<connect gate="B" pin="IO_27" pad="U2"/>
<connect gate="B" pin="IO_28" pad="U3"/>
<connect gate="B" pin="IO_29" pad="U4"/>
<connect gate="B" pin="IO_3" pad="M4"/>
<connect gate="B" pin="IO_30" pad="U5"/>
<connect gate="B" pin="IO_31" pad="U6"/>
<connect gate="B" pin="IO_32" pad="U7"/>
<connect gate="B" pin="IO_33" pad="U8"/>
<connect gate="B" pin="IO_34" pad="U9"/>
<connect gate="B" pin="IO_35" pad="V1"/>
<connect gate="B" pin="IO_36" pad="V2"/>
<connect gate="B" pin="IO_37" pad="V3"/>
<connect gate="B" pin="IO_38" pad="V4"/>
<connect gate="B" pin="IO_39" pad="V5"/>
<connect gate="B" pin="IO_4" pad="R5"/>
<connect gate="B" pin="IO_40" pad="V6"/>
<connect gate="B" pin="IO_41" pad="V8"/>
<connect gate="B" pin="IO_42" pad="W1"/>
<connect gate="B" pin="IO_43" pad="W2"/>
<connect gate="B" pin="IO_44" pad="W3"/>
<connect gate="B" pin="IO_45" pad="W4"/>
<connect gate="B" pin="IO_46" pad="W5"/>
<connect gate="B" pin="IO_47" pad="W6"/>
<connect gate="B" pin="IO_48" pad="W7"/>
<connect gate="B" pin="IO_49" pad="W8"/>
<connect gate="B" pin="IO_5" pad="M5"/>
<connect gate="B" pin="IO_50" pad="W9"/>
<connect gate="B" pin="IO_51" pad="Y1"/>
<connect gate="B" pin="IO_52" pad="Y2"/>
<connect gate="B" pin="IO_53" pad="Y3"/>
<connect gate="B" pin="IO_54" pad="Y4"/>
<connect gate="B" pin="IO_55" pad="Y5"/>
<connect gate="B" pin="IO_56" pad="Y6"/>
<connect gate="B" pin="IO_57" pad="Y8"/>
<connect gate="B" pin="IO_58" pad="Y9"/>
<connect gate="B" pin="IO_59" pad="A10"/>
<connect gate="B" pin="IO_6" pad="R6"/>
<connect gate="B" pin="IO_60" pad="A12"/>
<connect gate="B" pin="IO_61" pad="A17"/>
<connect gate="B" pin="IO_62" pad="A18"/>
<connect gate="B" pin="IO_63" pad="A19"/>
<connect gate="B" pin="IO_64" pad="A20"/>
<connect gate="B" pin="IO_65" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M6"/>
<connect gate="B" pin="IO_8" pad="R7"/>
<connect gate="B" pin="IO_9" pad="M7"/>
<connect gate="B" pin="VCCA_PLL1" pad="M3"/>
<connect gate="B" pin="VCCA_PLL2" pad="P5"/>
<connect gate="B" pin="VCCG_PLL1" pad="M2"/>
<connect gate="B" pin="VCCG_PLL2" pad="P4"/>
<connect gate="B" pin="VCCIO1" pad="T9"/>
<connect gate="B" pin="VCCIO1_2" pad="T1"/>
<connect gate="B" pin="VCCIO2" pad="L9"/>
<connect gate="B" pin="VCCIO3" pad="A11"/>
<connect gate="B" pin="VCCIO4" pad="A16"/>
<connect gate="B" pin="VREF0B1" pad="T8"/>
<connect gate="B" pin="VREF1B1" pad="V7"/>
<connect gate="B" pin="VREF1B2" pad="L8"/>
<connect gate="B" pin="VREF2B1" pad="Y7"/>
<connect gate="C" pin="CLK12P" pad="B15"/>
<connect gate="C" pin="CLK14P" pad="B12"/>
<connect gate="C" pin="CLK15P" pad="D12"/>
<connect gate="C" pin="GND" pad="AE1"/>
<connect gate="C" pin="GNDA_PLL5" pad="B14"/>
<connect gate="C" pin="GNDG_PLL5" pad="B13"/>
<connect gate="C" pin="GND_2" pad="B26"/>
<connect gate="C" pin="GND_3" pad="C13"/>
<connect gate="C" pin="GND_4" pad="AF2"/>
<connect gate="C" pin="GND_5" pad="A25"/>
<connect gate="C" pin="IO" pad="D11"/>
<connect gate="C" pin="IO_10" pad="AA8"/>
<connect gate="C" pin="IO_11" pad="AA9"/>
<connect gate="C" pin="IO_12" pad="AB1"/>
<connect gate="C" pin="IO_13" pad="AB2"/>
<connect gate="C" pin="IO_14" pad="AB3"/>
<connect gate="C" pin="IO_15" pad="AB4"/>
<connect gate="C" pin="IO_16" pad="AB5"/>
<connect gate="C" pin="IO_17" pad="AB6"/>
<connect gate="C" pin="IO_18" pad="AB7"/>
<connect gate="C" pin="IO_19" pad="AB8"/>
<connect gate="C" pin="IO_2" pad="AA1"/>
<connect gate="C" pin="IO_20" pad="AB9"/>
<connect gate="C" pin="IO_21" pad="AC2"/>
<connect gate="C" pin="IO_22" pad="AC3"/>
<connect gate="C" pin="IO_23" pad="AC4"/>
<connect gate="C" pin="IO_24" pad="AC5"/>
<connect gate="C" pin="IO_25" pad="AC6"/>
<connect gate="C" pin="IO_26" pad="AC7"/>
<connect gate="C" pin="IO_27" pad="AC8"/>
<connect gate="C" pin="IO_28" pad="AC9"/>
<connect gate="C" pin="IO_29" pad="AD1"/>
<connect gate="C" pin="IO_3" pad="AA2"/>
<connect gate="C" pin="IO_30" pad="AD2"/>
<connect gate="C" pin="IO_31" pad="AD3"/>
<connect gate="C" pin="IO_32" pad="AD4"/>
<connect gate="C" pin="IO_33" pad="AD5"/>
<connect gate="C" pin="IO_34" pad="AE2"/>
<connect gate="C" pin="IO_35" pad="AD6"/>
<connect gate="C" pin="IO_36" pad="AE3"/>
<connect gate="C" pin="IO_37" pad="AD7"/>
<connect gate="C" pin="IO_38" pad="AE4"/>
<connect gate="C" pin="IO_39" pad="AD8"/>
<connect gate="C" pin="IO_4" pad="AA3"/>
<connect gate="C" pin="IO_40" pad="AD9"/>
<connect gate="C" pin="IO_41" pad="AE6"/>
<connect gate="C" pin="IO_42" pad="AE7"/>
<connect gate="C" pin="IO_43" pad="AE8"/>
<connect gate="C" pin="IO_44" pad="AF3"/>
<connect gate="C" pin="IO_45" pad="AF5"/>
<connect gate="C" pin="IO_46" pad="AF6"/>
<connect gate="C" pin="IO_47" pad="AF7"/>
<connect gate="C" pin="IO_48" pad="AF8"/>
<connect gate="C" pin="IO_49" pad="AF9"/>
<connect gate="C" pin="IO_5" pad="A24"/>
<connect gate="C" pin="IO_50" pad="B10"/>
<connect gate="C" pin="IO_51" pad="B11"/>
<connect gate="C" pin="IO_52" pad="B16"/>
<connect gate="C" pin="IO_53" pad="B17"/>
<connect gate="C" pin="IO_54" pad="B18"/>
<connect gate="C" pin="IO_55" pad="B19"/>
<connect gate="C" pin="IO_56" pad="B20"/>
<connect gate="C" pin="IO_57" pad="B21"/>
<connect gate="C" pin="IO_58" pad="B22"/>
<connect gate="C" pin="IO_59" pad="B23"/>
<connect gate="C" pin="IO_6" pad="AA4"/>
<connect gate="C" pin="IO_60" pad="B24"/>
<connect gate="C" pin="IO_61" pad="B25"/>
<connect gate="C" pin="IO_62" pad="C10"/>
<connect gate="C" pin="IO_63" pad="C11"/>
<connect gate="C" pin="IO_64" pad="C12"/>
<connect gate="C" pin="IO_65" pad="C15"/>
<connect gate="C" pin="IO_66" pad="C16"/>
<connect gate="C" pin="IO_67" pad="C17"/>
<connect gate="C" pin="IO_68" pad="C18"/>
<connect gate="C" pin="IO_69" pad="C19"/>
<connect gate="C" pin="IO_7" pad="AA5"/>
<connect gate="C" pin="IO_70" pad="C20"/>
<connect gate="C" pin="IO_71" pad="C21"/>
<connect gate="C" pin="IO_72" pad="C22"/>
<connect gate="C" pin="IO_73" pad="C23"/>
<connect gate="C" pin="IO_74" pad="C24"/>
<connect gate="C" pin="IO_75" pad="C25"/>
<connect gate="C" pin="IO_76" pad="C26"/>
<connect gate="C" pin="IO_77" pad="D10"/>
<connect gate="C" pin="IO_8" pad="AA6"/>
<connect gate="C" pin="IO_9" pad="AA7"/>
<connect gate="C" pin="TRST" pad="D15"/>
<connect gate="C" pin="VCCA_PLL5" pad="D14"/>
<connect gate="C" pin="VCCG_PLL5" pad="C14"/>
<connect gate="C" pin="VCCIO1" pad="AC1"/>
<connect gate="C" pin="VCCIO4" pad="A23"/>
<connect gate="C" pin="VCCIO8" pad="AF4"/>
<connect gate="C" pin="VCC_PLL5_OUTA" pad="D13"/>
<connect gate="C" pin="VREF0B8" pad="AE5"/>
<connect gate="C" pin="VREF1B8" pad="AE9"/>
<connect gate="D" pin="CONF_DONE" pad="H11"/>
<connect gate="D" pin="DCLK" pad="G12"/>
<connect gate="D" pin="GND" pad="J14"/>
<connect gate="D" pin="GND_2" pad="J17"/>
<connect gate="D" pin="GND_3" pad="H17"/>
<connect gate="D" pin="GND_4" pad="J10"/>
<connect gate="D" pin="GND_5" pad="J13"/>
<connect gate="D" pin="IO" pad="J26"/>
<connect gate="D" pin="IO_10" pad="D20"/>
<connect gate="D" pin="IO_11" pad="E14"/>
<connect gate="D" pin="IO_12" pad="D21"/>
<connect gate="D" pin="IO_13" pad="D22"/>
<connect gate="D" pin="IO_14" pad="E16"/>
<connect gate="D" pin="IO_15" pad="D23"/>
<connect gate="D" pin="IO_16" pad="E17"/>
<connect gate="D" pin="IO_17" pad="D24"/>
<connect gate="D" pin="IO_18" pad="E18"/>
<connect gate="D" pin="IO_19" pad="D25"/>
<connect gate="D" pin="IO_2" pad="D16"/>
<connect gate="D" pin="IO_20" pad="E19"/>
<connect gate="D" pin="IO_21" pad="E20"/>
<connect gate="D" pin="IO_22" pad="E21"/>
<connect gate="D" pin="IO_23" pad="E22"/>
<connect gate="D" pin="IO_24" pad="E23"/>
<connect gate="D" pin="IO_25" pad="E24"/>
<connect gate="D" pin="IO_26" pad="E25"/>
<connect gate="D" pin="IO_27" pad="E26"/>
<connect gate="D" pin="IO_28" pad="F10"/>
<connect gate="D" pin="IO_29" pad="F12"/>
<connect gate="D" pin="IO_3" pad="E10"/>
<connect gate="D" pin="IO_30" pad="F13"/>
<connect gate="D" pin="IO_31" pad="F14"/>
<connect gate="D" pin="IO_32" pad="F15"/>
<connect gate="D" pin="IO_33" pad="F16"/>
<connect gate="D" pin="IO_34" pad="F17"/>
<connect gate="D" pin="IO_35" pad="F19"/>
<connect gate="D" pin="IO_36" pad="F20"/>
<connect gate="D" pin="IO_37" pad="F21"/>
<connect gate="D" pin="IO_38" pad="F23"/>
<connect gate="D" pin="IO_39" pad="F24"/>
<connect gate="D" pin="IO_4" pad="D17"/>
<connect gate="D" pin="IO_40" pad="F25"/>
<connect gate="D" pin="IO_41" pad="F26"/>
<connect gate="D" pin="IO_42" pad="G10"/>
<connect gate="D" pin="IO_43" pad="G11"/>
<connect gate="D" pin="IO_44" pad="G17"/>
<connect gate="D" pin="IO_45" pad="G18"/>
<connect gate="D" pin="IO_46" pad="G19"/>
<connect gate="D" pin="IO_47" pad="G20"/>
<connect gate="D" pin="IO_48" pad="G21"/>
<connect gate="D" pin="IO_49" pad="G22"/>
<connect gate="D" pin="IO_5" pad="E11"/>
<connect gate="D" pin="IO_50" pad="G23"/>
<connect gate="D" pin="IO_51" pad="G24"/>
<connect gate="D" pin="IO_52" pad="G25"/>
<connect gate="D" pin="IO_53" pad="G26"/>
<connect gate="D" pin="IO_54" pad="H10"/>
<connect gate="D" pin="IO_55" pad="H16"/>
<connect gate="D" pin="IO_56" pad="H18"/>
<connect gate="D" pin="IO_57" pad="H19"/>
<connect gate="D" pin="IO_58" pad="H20"/>
<connect gate="D" pin="IO_59" pad="H21"/>
<connect gate="D" pin="IO_6" pad="D18"/>
<connect gate="D" pin="IO_60" pad="H22"/>
<connect gate="D" pin="IO_61" pad="H23"/>
<connect gate="D" pin="IO_62" pad="H24"/>
<connect gate="D" pin="IO_63" pad="H25"/>
<connect gate="D" pin="IO_64" pad="H26"/>
<connect gate="D" pin="IO_65" pad="J19"/>
<connect gate="D" pin="IO_66" pad="J20"/>
<connect gate="D" pin="IO_67" pad="J21"/>
<connect gate="D" pin="IO_68" pad="J22"/>
<connect gate="D" pin="IO_69" pad="J23"/>
<connect gate="D" pin="IO_7" pad="E12"/>
<connect gate="D" pin="IO_70" pad="J24"/>
<connect gate="D" pin="IO_71" pad="J25"/>
<connect gate="D" pin="IO_8" pad="D19"/>
<connect gate="D" pin="IO_9" pad="E13"/>
<connect gate="D" pin="NCONFIG" pad="H12"/>
<connect gate="D" pin="NSTATUS" pad="H13"/>
<connect gate="D" pin="TCK" pad="G15"/>
<connect gate="D" pin="TDI" pad="H15"/>
<connect gate="D" pin="TDO" pad="G14"/>
<connect gate="D" pin="TEMPDIODEN" pad="G13"/>
<connect gate="D" pin="TEMPDIODEP" pad="H14"/>
<connect gate="D" pin="TMS" pad="E15"/>
<connect gate="D" pin="VCCIO3" pad="J12"/>
<connect gate="D" pin="VCCIO3_2" pad="J11"/>
<connect gate="D" pin="VCCIO4" pad="J16"/>
<connect gate="D" pin="VCCIO4_2" pad="J15"/>
<connect gate="D" pin="VCCIO5" pad="D26"/>
<connect gate="D" pin="VREF0B3" pad="F11"/>
<connect gate="D" pin="VREF0B4" pad="F22"/>
<connect gate="D" pin="VREF1B4" pad="F18"/>
<connect gate="D" pin="VREF1B5" pad="J18"/>
<connect gate="D" pin="VREF2B4" pad="G16"/>
<connect gate="E" pin="CLK10P" pad="M26"/>
<connect gate="E" pin="CLK11N" pad="M25"/>
<connect gate="E" pin="CLK11P" pad="M24"/>
<connect gate="E" pin="CLK8P" pad="P24"/>
<connect gate="E" pin="CLK9N" pad="P25"/>
<connect gate="E" pin="GND" pad="P18"/>
<connect gate="E" pin="GNDA_PLL4" pad="N23"/>
<connect gate="E" pin="GNDG_PLL4" pad="N22"/>
<connect gate="E" pin="GND_10" pad="N18"/>
<connect gate="E" pin="GND_11" pad="L11"/>
<connect gate="E" pin="GND_12" pad="M10"/>
<connect gate="E" pin="GND_13" pad="L13"/>
<connect gate="E" pin="GND_14" pad="P26"/>
<connect gate="E" pin="GND_15" pad="L15"/>
<connect gate="E" pin="GND_16" pad="P12"/>
<connect gate="E" pin="GND_17" pad="K16"/>
<connect gate="E" pin="GND_18" pad="N11"/>
<connect gate="E" pin="GND_19" pad="L17"/>
<connect gate="E" pin="GND_2" pad="N15"/>
<connect gate="E" pin="GND_20" pad="R11"/>
<connect gate="E" pin="GND_21" pad="M12"/>
<connect gate="E" pin="GND_22" pad="P14"/>
<connect gate="E" pin="GND_23" pad="R13"/>
<connect gate="E" pin="GND_24" pad="N13"/>
<connect gate="E" pin="GND_25" pad="M16"/>
<connect gate="E" pin="GND_26" pad="R15"/>
<connect gate="E" pin="GND_27" pad="P16"/>
<connect gate="E" pin="GND_28" pad="M14"/>
<connect gate="E" pin="GND_29" pad="R17"/>
<connect gate="E" pin="GND_3" pad="K12"/>
<connect gate="E" pin="GND_4" pad="N26"/>
<connect gate="E" pin="GND_5" pad="K10"/>
<connect gate="E" pin="GND_6" pad="N17"/>
<connect gate="E" pin="GND_7" pad="K14"/>
<connect gate="E" pin="GND_8" pad="P10"/>
<connect gate="E" pin="GND_9" pad="K18"/>
<connect gate="E" pin="IO" pad="R20"/>
<connect gate="E" pin="IO_10" pad="K26"/>
<connect gate="E" pin="IO_11" pad="M19"/>
<connect gate="E" pin="IO_12" pad="L20"/>
<connect gate="E" pin="IO_13" pad="M20"/>
<connect gate="E" pin="IO_14" pad="L21"/>
<connect gate="E" pin="IO_15" pad="M21"/>
<connect gate="E" pin="IO_16" pad="L22"/>
<connect gate="E" pin="IO_17" pad="M22"/>
<connect gate="E" pin="IO_18" pad="L23"/>
<connect gate="E" pin="IO_19" pad="M23"/>
<connect gate="E" pin="IO_2" pad="K19"/>
<connect gate="E" pin="IO_20" pad="L24"/>
<connect gate="E" pin="IO_21" pad="L25"/>
<connect gate="E" pin="IO_22" pad="N19"/>
<connect gate="E" pin="IO_23" pad="N20"/>
<connect gate="E" pin="IO_24" pad="N21"/>
<connect gate="E" pin="IO_25" pad="P19"/>
<connect gate="E" pin="IO_26" pad="P20"/>
<connect gate="E" pin="IO_27" pad="P21"/>
<connect gate="E" pin="IO_28" pad="R19"/>
<connect gate="E" pin="IO_3" pad="K20"/>
<connect gate="E" pin="IO_4" pad="K21"/>
<connect gate="E" pin="IO_5" pad="K22"/>
<connect gate="E" pin="IO_6" pad="K23"/>
<connect gate="E" pin="IO_7" pad="K24"/>
<connect gate="E" pin="IO_8" pad="K25"/>
<connect gate="E" pin="IO_9" pad="M18"/>
<connect gate="E" pin="VCCA_PLL3" pad="P22"/>
<connect gate="E" pin="VCCA_PLL4" pad="N25"/>
<connect gate="E" pin="VCCG_PLL3" pad="P23"/>
<connect gate="E" pin="VCCG_PLL4" pad="N24"/>
<connect gate="E" pin="VCCINT" pad="K17"/>
<connect gate="E" pin="VCCINT_10" pad="L14"/>
<connect gate="E" pin="VCCINT_11" pad="R10"/>
<connect gate="E" pin="VCCINT_12" pad="M13"/>
<connect gate="E" pin="VCCINT_13" pad="P13"/>
<connect gate="E" pin="VCCINT_14" pad="N14"/>
<connect gate="E" pin="VCCINT_15" pad="R16"/>
<connect gate="E" pin="VCCINT_16" pad="K15"/>
<connect gate="E" pin="VCCINT_17" pad="P17"/>
<connect gate="E" pin="VCCINT_18" pad="M11"/>
<connect gate="E" pin="VCCINT_19" pad="R12"/>
<connect gate="E" pin="VCCINT_2" pad="L10"/>
<connect gate="E" pin="VCCINT_20" pad="N16"/>
<connect gate="E" pin="VCCINT_21" pad="R14"/>
<connect gate="E" pin="VCCINT_22" pad="M15"/>
<connect gate="E" pin="VCCINT_23" pad="M17"/>
<connect gate="E" pin="VCCINT_24" pad="L16"/>
<connect gate="E" pin="VCCINT_3" pad="K11"/>
<connect gate="E" pin="VCCINT_4" pad="N10"/>
<connect gate="E" pin="VCCINT_5" pad="L12"/>
<connect gate="E" pin="VCCINT_6" pad="K13"/>
<connect gate="E" pin="VCCINT_7" pad="P11"/>
<connect gate="E" pin="VCCINT_8" pad="N12"/>
<connect gate="E" pin="VCCINT_9" pad="P15"/>
<connect gate="E" pin="VCCIO5" pad="L26"/>
<connect gate="E" pin="VCCIO5_2" pad="L18"/>
<connect gate="E" pin="VREF0B5" pad="L19"/>
<connect gate="E" pin="VREF2B6" pad="R18"/>
<connect gate="F" pin="CLK9P" pad="R26"/>
<connect gate="F" pin="GND" pad="V18"/>
<connect gate="F" pin="GNDA_PLL3" pad="R24"/>
<connect gate="F" pin="GNDG_PLL3" pad="R25"/>
<connect gate="F" pin="GND_10" pad="U13"/>
<connect gate="F" pin="GND_11" pad="V17"/>
<connect gate="F" pin="GND_12" pad="T16"/>
<connect gate="F" pin="GND_13" pad="U17"/>
<connect gate="F" pin="GND_2" pad="V10"/>
<connect gate="F" pin="GND_3" pad="V13"/>
<connect gate="F" pin="GND_4" pad="V14"/>
<connect gate="F" pin="GND_5" pad="T12"/>
<connect gate="F" pin="GND_6" pad="T14"/>
<connect gate="F" pin="GND_7" pad="U11"/>
<connect gate="F" pin="GND_8" pad="T10"/>
<connect gate="F" pin="GND_9" pad="U15"/>
<connect gate="F" pin="IO" pad="AA14"/>
<connect gate="F" pin="IO_10" pad="U24"/>
<connect gate="F" pin="IO_11" pad="T21"/>
<connect gate="F" pin="IO_12" pad="U25"/>
<connect gate="F" pin="IO_13" pad="T22"/>
<connect gate="F" pin="IO_14" pad="U26"/>
<connect gate="F" pin="IO_15" pad="T23"/>
<connect gate="F" pin="IO_16" pad="R21"/>
<connect gate="F" pin="IO_17" pad="T24"/>
<connect gate="F" pin="IO_18" pad="R22"/>
<connect gate="F" pin="IO_19" pad="T25"/>
<connect gate="F" pin="IO_2" pad="U18"/>
<connect gate="F" pin="IO_20" pad="R23"/>
<connect gate="F" pin="IO_21" pad="V19"/>
<connect gate="F" pin="IO_22" pad="V21"/>
<connect gate="F" pin="IO_23" pad="V22"/>
<connect gate="F" pin="IO_24" pad="V23"/>
<connect gate="F" pin="IO_25" pad="V24"/>
<connect gate="F" pin="IO_26" pad="V25"/>
<connect gate="F" pin="IO_27" pad="V26"/>
<connect gate="F" pin="IO_28" pad="W10"/>
<connect gate="F" pin="IO_29" pad="W15"/>
<connect gate="F" pin="IO_3" pad="U19"/>
<connect gate="F" pin="IO_30" pad="W17"/>
<connect gate="F" pin="IO_31" pad="W18"/>
<connect gate="F" pin="IO_32" pad="W19"/>
<connect gate="F" pin="IO_33" pad="W20"/>
<connect gate="F" pin="IO_34" pad="W21"/>
<connect gate="F" pin="IO_35" pad="W22"/>
<connect gate="F" pin="IO_36" pad="W23"/>
<connect gate="F" pin="IO_37" pad="W24"/>
<connect gate="F" pin="IO_38" pad="W25"/>
<connect gate="F" pin="IO_39" pad="W26"/>
<connect gate="F" pin="IO_4" pad="U20"/>
<connect gate="F" pin="IO_40" pad="Y10"/>
<connect gate="F" pin="IO_41" pad="Y11"/>
<connect gate="F" pin="IO_42" pad="Y16"/>
<connect gate="F" pin="IO_43" pad="Y17"/>
<connect gate="F" pin="IO_44" pad="Y18"/>
<connect gate="F" pin="IO_45" pad="Y19"/>
<connect gate="F" pin="IO_46" pad="Y20"/>
<connect gate="F" pin="IO_47" pad="Y22"/>
<connect gate="F" pin="IO_48" pad="Y23"/>
<connect gate="F" pin="IO_49" pad="Y24"/>
<connect gate="F" pin="IO_5" pad="U21"/>
<connect gate="F" pin="IO_50" pad="Y25"/>
<connect gate="F" pin="IO_51" pad="Y26"/>
<connect gate="F" pin="IO_52" pad="AA10"/>
<connect gate="F" pin="IO_53" pad="AA11"/>
<connect gate="F" pin="IO_54" pad="AA12"/>
<connect gate="F" pin="IO_55" pad="AA13"/>
<connect gate="F" pin="IO_6" pad="U22"/>
<connect gate="F" pin="IO_7" pad="T19"/>
<connect gate="F" pin="IO_8" pad="U23"/>
<connect gate="F" pin="IO_9" pad="T20"/>
<connect gate="F" pin="MSEL0" pad="Y12"/>
<connect gate="F" pin="MSEL1" pad="Y13"/>
<connect gate="F" pin="MSEL2" pad="W13"/>
<connect gate="F" pin="NCE" pad="Y14"/>
<connect gate="F" pin="NCEO" pad="W14"/>
<connect gate="F" pin="PLL_ENA" pad="W12"/>
<connect gate="F" pin="PORSEL" pad="W16"/>
<connect gate="F" pin="VCCINT" pad="T15"/>
<connect gate="F" pin="VCCINT_2" pad="U10"/>
<connect gate="F" pin="VCCINT_3" pad="U12"/>
<connect gate="F" pin="VCCINT_4" pad="T11"/>
<connect gate="F" pin="VCCINT_5" pad="U16"/>
<connect gate="F" pin="VCCINT_6" pad="U14"/>
<connect gate="F" pin="VCCINT_7" pad="T17"/>
<connect gate="F" pin="VCCINT_8" pad="T13"/>
<connect gate="F" pin="VCCIO6" pad="T18"/>
<connect gate="F" pin="VCCIO6_2" pad="T26"/>
<connect gate="F" pin="VCCIO7" pad="V16"/>
<connect gate="F" pin="VCCIO7_2" pad="V15"/>
<connect gate="F" pin="VCCIO8" pad="V12"/>
<connect gate="F" pin="VCCIO8_2" pad="V11"/>
<connect gate="F" pin="VCCSEL" pad="Y15"/>
<connect gate="F" pin="VREF0B6" pad="Y21"/>
<connect gate="F" pin="VREF1B6" pad="V20"/>
<connect gate="F" pin="VREF2B8" pad="W11"/>
<connect gate="G" pin="CLK4P" pad="AE12"/>
<connect gate="G" pin="CLK5P" pad="AC12"/>
<connect gate="G" pin="CLK6P" pad="AF15"/>
<connect gate="G" pin="CLK7P" pad="AE15"/>
<connect gate="G" pin="GND" pad="AF14"/>
<connect gate="G" pin="GNDA_PLL6" pad="AC14"/>
<connect gate="G" pin="GNDG_PLL6" pad="AE14"/>
<connect gate="G" pin="GND_2" pad="AF13"/>
<connect gate="G" pin="GND_3" pad="AF25"/>
<connect gate="G" pin="GND_4" pad="AC13"/>
<connect gate="G" pin="GND_5" pad="AE26"/>
<connect gate="G" pin="IO" pad="AF24"/>
<connect gate="G" pin="IO_10" pad="AA16"/>
<connect gate="G" pin="IO_11" pad="AA26"/>
<connect gate="G" pin="IO_12" pad="AA17"/>
<connect gate="G" pin="IO_13" pad="AB10"/>
<connect gate="G" pin="IO_14" pad="AB11"/>
<connect gate="G" pin="IO_15" pad="AB16"/>
<connect gate="G" pin="IO_16" pad="AB12"/>
<connect gate="G" pin="IO_17" pad="AB17"/>
<connect gate="G" pin="IO_18" pad="AB13"/>
<connect gate="G" pin="IO_19" pad="AB14"/>
<connect gate="G" pin="IO_2" pad="AA18"/>
<connect gate="G" pin="IO_20" pad="AB19"/>
<connect gate="G" pin="IO_21" pad="AB20"/>
<connect gate="G" pin="IO_22" pad="AC11"/>
<connect gate="G" pin="IO_23" pad="AB21"/>
<connect gate="G" pin="IO_24" pad="AB22"/>
<connect gate="G" pin="IO_25" pad="AB23"/>
<connect gate="G" pin="IO_26" pad="AB24"/>
<connect gate="G" pin="IO_27" pad="AC15"/>
<connect gate="G" pin="IO_28" pad="AB25"/>
<connect gate="G" pin="IO_29" pad="AC16"/>
<connect gate="G" pin="IO_3" pad="AA19"/>
<connect gate="G" pin="IO_30" pad="AB26"/>
<connect gate="G" pin="IO_31" pad="AC17"/>
<connect gate="G" pin="IO_32" pad="AC10"/>
<connect gate="G" pin="IO_33" pad="AC18"/>
<connect gate="G" pin="IO_34" pad="AC19"/>
<connect gate="G" pin="IO_35" pad="AC20"/>
<connect gate="G" pin="IO_36" pad="AC21"/>
<connect gate="G" pin="IO_37" pad="AC22"/>
<connect gate="G" pin="IO_38" pad="AC23"/>
<connect gate="G" pin="IO_39" pad="AC24"/>
<connect gate="G" pin="IO_4" pad="AA20"/>
<connect gate="G" pin="IO_40" pad="AC25"/>
<connect gate="G" pin="IO_41" pad="AD10"/>
<connect gate="G" pin="IO_42" pad="AD11"/>
<connect gate="G" pin="IO_43" pad="AD12"/>
<connect gate="G" pin="IO_44" pad="AD15"/>
<connect gate="G" pin="IO_45" pad="AD16"/>
<connect gate="G" pin="IO_46" pad="AD17"/>
<connect gate="G" pin="IO_47" pad="AD18"/>
<connect gate="G" pin="IO_48" pad="AD19"/>
<connect gate="G" pin="IO_49" pad="AD20"/>
<connect gate="G" pin="IO_5" pad="AA21"/>
<connect gate="G" pin="IO_50" pad="AD22"/>
<connect gate="G" pin="IO_51" pad="AD23"/>
<connect gate="G" pin="IO_52" pad="AD24"/>
<connect gate="G" pin="IO_53" pad="AD25"/>
<connect gate="G" pin="IO_54" pad="AD26"/>
<connect gate="G" pin="IO_55" pad="AE10"/>
<connect gate="G" pin="IO_56" pad="AE11"/>
<connect gate="G" pin="IO_57" pad="AE16"/>
<connect gate="G" pin="IO_58" pad="AE17"/>
<connect gate="G" pin="IO_59" pad="AE18"/>
<connect gate="G" pin="IO_6" pad="AA22"/>
<connect gate="G" pin="IO_60" pad="AE19"/>
<connect gate="G" pin="IO_61" pad="AE20"/>
<connect gate="G" pin="IO_62" pad="AE21"/>
<connect gate="G" pin="IO_63" pad="AE22"/>
<connect gate="G" pin="IO_64" pad="AE23"/>
<connect gate="G" pin="IO_65" pad="AE24"/>
<connect gate="G" pin="IO_66" pad="AE25"/>
<connect gate="G" pin="IO_67" pad="AF10"/>
<connect gate="G" pin="IO_68" pad="AF12"/>
<connect gate="G" pin="IO_69" pad="AF17"/>
<connect gate="G" pin="IO_7" pad="AA23"/>
<connect gate="G" pin="IO_70" pad="AF18"/>
<connect gate="G" pin="IO_71" pad="AF19"/>
<connect gate="G" pin="IO_72" pad="AF20"/>
<connect gate="G" pin="IO_73" pad="AF21"/>
<connect gate="G" pin="IO_74" pad="AF22"/>
<connect gate="G" pin="IO_8" pad="AA24"/>
<connect gate="G" pin="IO_9" pad="AA25"/>
<connect gate="G" pin="NIO_PULLUP" pad="AA15"/>
<connect gate="G" pin="VCCA_PLL6" pad="AD14"/>
<connect gate="G" pin="VCCG_PLL6" pad="AD13"/>
<connect gate="G" pin="VCCIO6" pad="AC26"/>
<connect gate="G" pin="VCCIO7" pad="AF16"/>
<connect gate="G" pin="VCCIO7_2" pad="AF23"/>
<connect gate="G" pin="VCCIO8" pad="AF11"/>
<connect gate="G" pin="VCC_PLL6_OUTA" pad="AE13"/>
<connect gate="G" pin="VREF0B7" pad="AB15"/>
<connect gate="G" pin="VREF1B7" pad="AB18"/>
<connect gate="G" pin="VREF2B7" pad="AD21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1S25F672C7N"/>
<attribute name="OC_FARNELL" value="1637227"/>
<attribute name="OC_NEWARK" value="51R4689"/>
<attribute name="PACKAGE" value="FBGA-672"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1S25F780C6N">
<description>FPGA, STRATIX</description>
<gates>
<gate name="A" symbol="EP1S25F780C6N_A"/>
<gate name="B" symbol="EP1S25F780C6N_B"/>
<gate name="C" symbol="EP1S25F780C6N_C"/>
<gate name="D" symbol="EP1S25F780C6N_D"/>
<gate name="E" symbol="EP1S25F780C6N_E"/>
<gate name="F" symbol="EP1S25F780C6N_F"/>
<gate name="G" symbol="EP1S25F780C6N_G"/>
<gate name="H" symbol="EP1S25F780C6N_H"/>
</gates>
<devices>
<device name="" package="BGA780C100P28X28_2900X2900X350">
<connects>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="IO" pad="L9"/>
<connect gate="A" pin="IO_10" pad="B4"/>
<connect gate="A" pin="IO_11" pad="B5"/>
<connect gate="A" pin="IO_12" pad="B6"/>
<connect gate="A" pin="IO_13" pad="B7"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="B9"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C1"/>
<connect gate="A" pin="IO_18" pad="C5"/>
<connect gate="A" pin="IO_19" pad="C2"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D1"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="E6"/>
<connect gate="A" pin="IO_29" pad="D7"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D8"/>
<connect gate="A" pin="IO_31" pad="E8"/>
<connect gate="A" pin="IO_32" pad="D9"/>
<connect gate="A" pin="IO_33" pad="F1"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="F2"/>
<connect gate="A" pin="IO_37" pad="F3"/>
<connect gate="A" pin="IO_38" pad="F4"/>
<connect gate="A" pin="IO_39" pad="F5"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="F6"/>
<connect gate="A" pin="IO_41" pad="F7"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G4"/>
<connect gate="A" pin="IO_48" pad="G5"/>
<connect gate="A" pin="IO_49" pad="G6"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="G7"/>
<connect gate="A" pin="IO_51" pad="G8"/>
<connect gate="A" pin="IO_52" pad="G9"/>
<connect gate="A" pin="IO_53" pad="H1"/>
<connect gate="A" pin="IO_54" pad="H2"/>
<connect gate="A" pin="IO_55" pad="H3"/>
<connect gate="A" pin="IO_56" pad="H4"/>
<connect gate="A" pin="IO_57" pad="H5"/>
<connect gate="A" pin="IO_58" pad="H6"/>
<connect gate="A" pin="IO_59" pad="H7"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="H8"/>
<connect gate="A" pin="IO_61" pad="H9"/>
<connect gate="A" pin="IO_62" pad="J1"/>
<connect gate="A" pin="IO_63" pad="J2"/>
<connect gate="A" pin="IO_64" pad="J3"/>
<connect gate="A" pin="IO_65" pad="J4"/>
<connect gate="A" pin="IO_66" pad="J5"/>
<connect gate="A" pin="IO_67" pad="J6"/>
<connect gate="A" pin="IO_68" pad="J7"/>
<connect gate="A" pin="IO_69" pad="J8"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_70" pad="J9"/>
<connect gate="A" pin="IO_71" pad="K1"/>
<connect gate="A" pin="IO_72" pad="K2"/>
<connect gate="A" pin="IO_73" pad="K3"/>
<connect gate="A" pin="IO_74" pad="K4"/>
<connect gate="A" pin="IO_75" pad="K5"/>
<connect gate="A" pin="IO_76" pad="K6"/>
<connect gate="A" pin="IO_77" pad="K7"/>
<connect gate="A" pin="IO_78" pad="K8"/>
<connect gate="A" pin="IO_79" pad="L1"/>
<connect gate="A" pin="IO_8" pad="A8"/>
<connect gate="A" pin="IO_80" pad="L2"/>
<connect gate="A" pin="IO_81" pad="L3"/>
<connect gate="A" pin="IO_82" pad="L4"/>
<connect gate="A" pin="IO_83" pad="L5"/>
<connect gate="A" pin="IO_84" pad="L6"/>
<connect gate="A" pin="IO_85" pad="L7"/>
<connect gate="A" pin="IO_86" pad="L8"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="NC" pad="E4"/>
<connect gate="A" pin="NC_2" pad="D3"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="D4"/>
<connect gate="A" pin="NC_5" pad="E5"/>
<connect gate="A" pin="VCCIO4" pad="A2"/>
<connect gate="A" pin="VCCIO5" pad="B1"/>
<connect gate="A" pin="VREF0B4" pad="E7"/>
<connect gate="A" pin="VREF1B4" pad="E9"/>
<connect gate="A" pin="VREF1B5" pad="K9"/>
<connect gate="B" pin="CLK10P" pad="P4"/>
<connect gate="B" pin="CLK11N" pad="N2"/>
<connect gate="B" pin="CLK11P" pad="P2"/>
<connect gate="B" pin="CLK8P" pad="R4"/>
<connect gate="B" pin="CLK9N" pad="T2"/>
<connect gate="B" pin="CLK9P" pad="R2"/>
<connect gate="B" pin="GND" pad="A15"/>
<connect gate="B" pin="GNDA_PLL3" pad="R5"/>
<connect gate="B" pin="GNDA_PLL4" pad="P5"/>
<connect gate="B" pin="GNDG_PLL3" pad="R7"/>
<connect gate="B" pin="GNDG_PLL4" pad="P7"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="A14"/>
<connect gate="B" pin="GND_4" pad="R1"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="N7"/>
<connect gate="B" pin="IO_11" pad="M6"/>
<connect gate="B" pin="IO_12" pad="N8"/>
<connect gate="B" pin="IO_13" pad="M7"/>
<connect gate="B" pin="IO_14" pad="T3"/>
<connect gate="B" pin="IO_15" pad="N9"/>
<connect gate="B" pin="IO_16" pad="T4"/>
<connect gate="B" pin="IO_17" pad="M8"/>
<connect gate="B" pin="IO_18" pad="T5"/>
<connect gate="B" pin="IO_19" pad="M9"/>
<connect gate="B" pin="IO_2" pad="N3"/>
<connect gate="B" pin="IO_20" pad="T6"/>
<connect gate="B" pin="IO_21" pad="N1"/>
<connect gate="B" pin="IO_22" pad="T7"/>
<connect gate="B" pin="IO_23" pad="P3"/>
<connect gate="B" pin="IO_24" pad="T8"/>
<connect gate="B" pin="IO_25" pad="T9"/>
<connect gate="B" pin="IO_26" pad="R3"/>
<connect gate="B" pin="IO_27" pad="T1"/>
<connect gate="B" pin="IO_28" pad="U2"/>
<connect gate="B" pin="IO_29" pad="U3"/>
<connect gate="B" pin="IO_3" pad="M3"/>
<connect gate="B" pin="IO_30" pad="U4"/>
<connect gate="B" pin="IO_31" pad="U5"/>
<connect gate="B" pin="IO_32" pad="U6"/>
<connect gate="B" pin="IO_33" pad="U7"/>
<connect gate="B" pin="IO_34" pad="U8"/>
<connect gate="B" pin="IO_35" pad="U9"/>
<connect gate="B" pin="IO_36" pad="V1"/>
<connect gate="B" pin="IO_37" pad="V2"/>
<connect gate="B" pin="IO_38" pad="V3"/>
<connect gate="B" pin="IO_39" pad="V4"/>
<connect gate="B" pin="IO_4" pad="N4"/>
<connect gate="B" pin="IO_40" pad="V5"/>
<connect gate="B" pin="IO_41" pad="V6"/>
<connect gate="B" pin="IO_42" pad="V7"/>
<connect gate="B" pin="IO_43" pad="V8"/>
<connect gate="B" pin="IO_44" pad="V9"/>
<connect gate="B" pin="IO_45" pad="W1"/>
<connect gate="B" pin="IO_46" pad="W2"/>
<connect gate="B" pin="IO_47" pad="W3"/>
<connect gate="B" pin="IO_48" pad="W4"/>
<connect gate="B" pin="IO_49" pad="W5"/>
<connect gate="B" pin="IO_5" pad="M4"/>
<connect gate="B" pin="IO_50" pad="W6"/>
<connect gate="B" pin="IO_51" pad="W7"/>
<connect gate="B" pin="IO_52" pad="W8"/>
<connect gate="B" pin="IO_53" pad="Y1"/>
<connect gate="B" pin="IO_54" pad="Y2"/>
<connect gate="B" pin="IO_55" pad="Y3"/>
<connect gate="B" pin="IO_56" pad="Y4"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="N5"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A11"/>
<connect gate="B" pin="IO_64" pad="A13"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A18"/>
<connect gate="B" pin="IO_67" pad="A19"/>
<connect gate="B" pin="IO_68" pad="A20"/>
<connect gate="B" pin="IO_69" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M5"/>
<connect gate="B" pin="IO_70" pad="A22"/>
<connect gate="B" pin="IO_71" pad="A23"/>
<connect gate="B" pin="IO_72" pad="A24"/>
<connect gate="B" pin="IO_73" pad="A25"/>
<connect gate="B" pin="IO_8" pad="N6"/>
<connect gate="B" pin="IO_9" pad="M2"/>
<connect gate="B" pin="VCCA_PLL3" pad="R6"/>
<connect gate="B" pin="VCCA_PLL4" pad="P6"/>
<connect gate="B" pin="VCCG_PLL3" pad="R8"/>
<connect gate="B" pin="VCCG_PLL4" pad="P8"/>
<connect gate="B" pin="VCCIO3" pad="A17"/>
<connect gate="B" pin="VCCIO4" pad="A12"/>
<connect gate="B" pin="VCCIO5" pad="P9"/>
<connect gate="B" pin="VCCIO5_2" pad="M1"/>
<connect gate="B" pin="VCCIO6" pad="U1"/>
<connect gate="B" pin="VCCIO6_2" pad="R9"/>
<connect gate="B" pin="VREF1B6" pad="W9"/>
<connect gate="C" pin="GND" pad="AG2"/>
<connect gate="C" pin="GND_2" pad="AF3"/>
<connect gate="C" pin="GND_3" pad="B27"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AD1"/>
<connect gate="C" pin="IO_11" pad="AA4"/>
<connect gate="C" pin="IO_12" pad="AD2"/>
<connect gate="C" pin="IO_13" pad="AA5"/>
<connect gate="C" pin="IO_14" pad="AA6"/>
<connect gate="C" pin="IO_15" pad="AA7"/>
<connect gate="C" pin="IO_16" pad="AA8"/>
<connect gate="C" pin="IO_17" pad="AA9"/>
<connect gate="C" pin="IO_18" pad="AB1"/>
<connect gate="C" pin="IO_19" pad="AB2"/>
<connect gate="C" pin="IO_2" pad="AC5"/>
<connect gate="C" pin="IO_20" pad="AB3"/>
<connect gate="C" pin="IO_21" pad="AB4"/>
<connect gate="C" pin="IO_22" pad="AB5"/>
<connect gate="C" pin="IO_23" pad="AB8"/>
<connect gate="C" pin="IO_24" pad="AE1"/>
<connect gate="C" pin="IO_25" pad="AD5"/>
<connect gate="C" pin="IO_26" pad="AE2"/>
<connect gate="C" pin="IO_27" pad="AB6"/>
<connect gate="C" pin="IO_28" pad="AD6"/>
<connect gate="C" pin="IO_29" pad="AE4"/>
<connect gate="C" pin="IO_3" pad="AC6"/>
<connect gate="C" pin="IO_30" pad="AB9"/>
<connect gate="C" pin="IO_31" pad="AE5"/>
<connect gate="C" pin="IO_32" pad="AB7"/>
<connect gate="C" pin="IO_33" pad="AE6"/>
<connect gate="C" pin="IO_34" pad="AD8"/>
<connect gate="C" pin="IO_35" pad="AE7"/>
<connect gate="C" pin="IO_36" pad="AC1"/>
<connect gate="C" pin="IO_37" pad="AE8"/>
<connect gate="C" pin="IO_38" pad="AC2"/>
<connect gate="C" pin="IO_39" pad="AE9"/>
<connect gate="C" pin="IO_4" pad="AC7"/>
<connect gate="C" pin="IO_40" pad="AF1"/>
<connect gate="C" pin="IO_41" pad="AF2"/>
<connect gate="C" pin="IO_42" pad="AF4"/>
<connect gate="C" pin="IO_43" pad="AF5"/>
<connect gate="C" pin="IO_44" pad="AF6"/>
<connect gate="C" pin="IO_45" pad="AF7"/>
<connect gate="C" pin="IO_46" pad="AF8"/>
<connect gate="C" pin="IO_47" pad="AF9"/>
<connect gate="C" pin="IO_48" pad="AG3"/>
<connect gate="C" pin="IO_49" pad="AG4"/>
<connect gate="C" pin="IO_5" pad="AA1"/>
<connect gate="C" pin="IO_50" pad="AG5"/>
<connect gate="C" pin="IO_51" pad="AG6"/>
<connect gate="C" pin="IO_52" pad="AG7"/>
<connect gate="C" pin="IO_53" pad="AG8"/>
<connect gate="C" pin="IO_54" pad="AG9"/>
<connect gate="C" pin="IO_55" pad="AH3"/>
<connect gate="C" pin="IO_56" pad="AH4"/>
<connect gate="C" pin="IO_57" pad="AH5"/>
<connect gate="C" pin="IO_58" pad="AH6"/>
<connect gate="C" pin="IO_59" pad="AH7"/>
<connect gate="C" pin="IO_6" pad="AC8"/>
<connect gate="C" pin="IO_60" pad="AH8"/>
<connect gate="C" pin="IO_61" pad="AH9"/>
<connect gate="C" pin="IO_62" pad="B10"/>
<connect gate="C" pin="IO_63" pad="B11"/>
<connect gate="C" pin="IO_64" pad="B12"/>
<connect gate="C" pin="IO_65" pad="B13"/>
<connect gate="C" pin="IO_66" pad="B15"/>
<connect gate="C" pin="IO_67" pad="B16"/>
<connect gate="C" pin="IO_68" pad="B17"/>
<connect gate="C" pin="IO_69" pad="B18"/>
<connect gate="C" pin="IO_7" pad="AA2"/>
<connect gate="C" pin="IO_70" pad="B19"/>
<connect gate="C" pin="IO_71" pad="B20"/>
<connect gate="C" pin="IO_72" pad="B21"/>
<connect gate="C" pin="IO_73" pad="B22"/>
<connect gate="C" pin="IO_74" pad="B23"/>
<connect gate="C" pin="IO_75" pad="B24"/>
<connect gate="C" pin="IO_76" pad="B25"/>
<connect gate="C" pin="IO_77" pad="B26"/>
<connect gate="C" pin="IO_78" pad="C10"/>
<connect gate="C" pin="IO_79" pad="C11"/>
<connect gate="C" pin="IO_8" pad="AC9"/>
<connect gate="C" pin="IO_80" pad="C12"/>
<connect gate="C" pin="IO_81" pad="C13"/>
<connect gate="C" pin="IO_82" pad="C15"/>
<connect gate="C" pin="IO_9" pad="AA3"/>
<connect gate="C" pin="NC" pad="AD4"/>
<connect gate="C" pin="NC_2" pad="AC3"/>
<connect gate="C" pin="NC_3" pad="AC4"/>
<connect gate="C" pin="NC_4" pad="AD3"/>
<connect gate="C" pin="TEMPDIODEN" pad="C14"/>
<connect gate="C" pin="TEMPDIODEP" pad="B14"/>
<connect gate="C" pin="VCCIO2" pad="B28"/>
<connect gate="C" pin="VCCIO3" pad="A27"/>
<connect gate="C" pin="VCCIO6" pad="AG1"/>
<connect gate="C" pin="VCCIO7" pad="AH2"/>
<connect gate="C" pin="VREF0B6" pad="AE3"/>
<connect gate="C" pin="VREF1B7" pad="AD9"/>
<connect gate="C" pin="VREF2B7" pad="AD7"/>
<connect gate="D" pin="CONF_DONE" pad="G17"/>
<connect gate="D" pin="DCLK" pad="F16"/>
<connect gate="D" pin="GND" pad="C26"/>
<connect gate="D" pin="GNDA_PLL5" pad="G14"/>
<connect gate="D" pin="GNDG_PLL5" pad="E14"/>
<connect gate="D" pin="GND_2" pad="G15"/>
<connect gate="D" pin="GND_3" pad="G20"/>
<connect gate="D" pin="GND_4" pad="H16"/>
<connect gate="D" pin="IO" pad="H19"/>
<connect gate="D" pin="IO_10" pad="C17"/>
<connect gate="D" pin="IO_11" pad="C27"/>
<connect gate="D" pin="IO_12" pad="C28"/>
<connect gate="D" pin="IO_13" pad="D10"/>
<connect gate="D" pin="IO_14" pad="D11"/>
<connect gate="D" pin="IO_15" pad="D12"/>
<connect gate="D" pin="IO_16" pad="D13"/>
<connect gate="D" pin="IO_17" pad="D15"/>
<connect gate="D" pin="IO_18" pad="D16"/>
<connect gate="D" pin="IO_19" pad="D17"/>
<connect gate="D" pin="IO_2" pad="C18"/>
<connect gate="D" pin="IO_20" pad="D18"/>
<connect gate="D" pin="IO_21" pad="D19"/>
<connect gate="D" pin="IO_22" pad="D20"/>
<connect gate="D" pin="IO_23" pad="D21"/>
<connect gate="D" pin="IO_24" pad="E15"/>
<connect gate="D" pin="IO_25" pad="D22"/>
<connect gate="D" pin="IO_26" pad="E16"/>
<connect gate="D" pin="IO_27" pad="D23"/>
<connect gate="D" pin="IO_28" pad="E17"/>
<connect gate="D" pin="IO_29" pad="D24"/>
<connect gate="D" pin="IO_3" pad="C19"/>
<connect gate="D" pin="IO_30" pad="D27"/>
<connect gate="D" pin="IO_31" pad="E19"/>
<connect gate="D" pin="IO_32" pad="D28"/>
<connect gate="D" pin="IO_33" pad="E10"/>
<connect gate="D" pin="IO_34" pad="E21"/>
<connect gate="D" pin="IO_35" pad="E12"/>
<connect gate="D" pin="IO_36" pad="E13"/>
<connect gate="D" pin="IO_37" pad="E27"/>
<connect gate="D" pin="IO_38" pad="E23"/>
<connect gate="D" pin="IO_39" pad="F17"/>
<connect gate="D" pin="IO_4" pad="C20"/>
<connect gate="D" pin="IO_40" pad="F18"/>
<connect gate="D" pin="IO_41" pad="F19"/>
<connect gate="D" pin="IO_42" pad="F20"/>
<connect gate="D" pin="IO_43" pad="E28"/>
<connect gate="D" pin="IO_44" pad="F21"/>
<connect gate="D" pin="IO_45" pad="F10"/>
<connect gate="D" pin="IO_46" pad="F22"/>
<connect gate="D" pin="IO_47" pad="F11"/>
<connect gate="D" pin="IO_48" pad="F23"/>
<connect gate="D" pin="IO_49" pad="F24"/>
<connect gate="D" pin="IO_5" pad="C21"/>
<connect gate="D" pin="IO_50" pad="F25"/>
<connect gate="D" pin="IO_51" pad="F26"/>
<connect gate="D" pin="IO_52" pad="F27"/>
<connect gate="D" pin="IO_53" pad="F28"/>
<connect gate="D" pin="IO_54" pad="G10"/>
<connect gate="D" pin="IO_55" pad="G11"/>
<connect gate="D" pin="IO_56" pad="G12"/>
<connect gate="D" pin="IO_57" pad="F12"/>
<connect gate="D" pin="IO_58" pad="G18"/>
<connect gate="D" pin="IO_59" pad="G19"/>
<connect gate="D" pin="IO_6" pad="C22"/>
<connect gate="D" pin="IO_60" pad="G21"/>
<connect gate="D" pin="IO_61" pad="G22"/>
<connect gate="D" pin="IO_62" pad="G23"/>
<connect gate="D" pin="IO_63" pad="G24"/>
<connect gate="D" pin="IO_64" pad="G25"/>
<connect gate="D" pin="IO_65" pad="G26"/>
<connect gate="D" pin="IO_66" pad="G27"/>
<connect gate="D" pin="IO_67" pad="G28"/>
<connect gate="D" pin="IO_68" pad="H10"/>
<connect gate="D" pin="IO_69" pad="H11"/>
<connect gate="D" pin="IO_7" pad="C23"/>
<connect gate="D" pin="IO_70" pad="H12"/>
<connect gate="D" pin="IO_71" pad="H14"/>
<connect gate="D" pin="IO_72" pad="H15"/>
<connect gate="D" pin="IO_73" pad="H17"/>
<connect gate="D" pin="IO_74" pad="H18"/>
<connect gate="D" pin="IO_8" pad="C24"/>
<connect gate="D" pin="IO_9" pad="C25"/>
<connect gate="D" pin="NC" pad="E26"/>
<connect gate="D" pin="NC_2" pad="D25"/>
<connect gate="D" pin="NC_3" pad="E25"/>
<connect gate="D" pin="NC_4" pad="D26"/>
<connect gate="D" pin="TDI" pad="G13"/>
<connect gate="D" pin="TDO" pad="H13"/>
<connect gate="D" pin="TMS" pad="F13"/>
<connect gate="D" pin="VCCA_PLL5" pad="F14"/>
<connect gate="D" pin="VCCG_PLL5" pad="D14"/>
<connect gate="D" pin="VCC_PLL5_OUTA" pad="F15"/>
<connect gate="D" pin="VCC_PLL5_OUTB" pad="G16"/>
<connect gate="D" pin="VREF0B2" pad="E24"/>
<connect gate="D" pin="VREF0B3" pad="E18"/>
<connect gate="D" pin="VREF1B3" pad="E20"/>
<connect gate="D" pin="VREF2B3" pad="E22"/>
<connect gate="D" pin="VREF2B4" pad="E11"/>
<connect gate="E" pin="CLK12P" pad="K13"/>
<connect gate="E" pin="CLK13P" pad="M13"/>
<connect gate="E" pin="CLK14P" pad="K17"/>
<connect gate="E" pin="CLK15P" pad="M17"/>
<connect gate="E" pin="GND" pad="L15"/>
<connect gate="E" pin="GND_2" pad="N18"/>
<connect gate="E" pin="GND_3" pad="N14"/>
<connect gate="E" pin="GND_4" pad="M15"/>
<connect gate="E" pin="GND_5" pad="N16"/>
<connect gate="E" pin="GND_6" pad="N12"/>
<connect gate="E" pin="GND_7" pad="L14"/>
<connect gate="E" pin="IO" pad="N22"/>
<connect gate="E" pin="IO_10" pad="J10"/>
<connect gate="E" pin="IO_11" pad="J11"/>
<connect gate="E" pin="IO_12" pad="J12"/>
<connect gate="E" pin="IO_13" pad="J13"/>
<connect gate="E" pin="IO_14" pad="J16"/>
<connect gate="E" pin="IO_15" pad="J17"/>
<connect gate="E" pin="IO_16" pad="J18"/>
<connect gate="E" pin="IO_17" pad="J19"/>
<connect gate="E" pin="IO_18" pad="J20"/>
<connect gate="E" pin="IO_19" pad="J21"/>
<connect gate="E" pin="IO_2" pad="H21"/>
<connect gate="E" pin="IO_20" pad="J22"/>
<connect gate="E" pin="IO_21" pad="J23"/>
<connect gate="E" pin="IO_22" pad="J24"/>
<connect gate="E" pin="IO_23" pad="J25"/>
<connect gate="E" pin="IO_24" pad="J26"/>
<connect gate="E" pin="IO_25" pad="J27"/>
<connect gate="E" pin="IO_26" pad="J28"/>
<connect gate="E" pin="IO_27" pad="K10"/>
<connect gate="E" pin="IO_28" pad="K21"/>
<connect gate="E" pin="IO_29" pad="K11"/>
<connect gate="E" pin="IO_3" pad="H22"/>
<connect gate="E" pin="IO_30" pad="K22"/>
<connect gate="E" pin="IO_31" pad="K23"/>
<connect gate="E" pin="IO_32" pad="H20"/>
<connect gate="E" pin="IO_33" pad="K24"/>
<connect gate="E" pin="IO_34" pad="K14"/>
<connect gate="E" pin="IO_35" pad="K25"/>
<connect gate="E" pin="IO_36" pad="K15"/>
<connect gate="E" pin="IO_37" pad="K26"/>
<connect gate="E" pin="IO_38" pad="K16"/>
<connect gate="E" pin="IO_39" pad="K27"/>
<connect gate="E" pin="IO_4" pad="H23"/>
<connect gate="E" pin="IO_40" pad="K28"/>
<connect gate="E" pin="IO_41" pad="K18"/>
<connect gate="E" pin="IO_42" pad="L10"/>
<connect gate="E" pin="IO_43" pad="K19"/>
<connect gate="E" pin="IO_44" pad="L11"/>
<connect gate="E" pin="IO_45" pad="L13"/>
<connect gate="E" pin="IO_46" pad="L17"/>
<connect gate="E" pin="IO_47" pad="L18"/>
<connect gate="E" pin="IO_48" pad="L19"/>
<connect gate="E" pin="IO_49" pad="L20"/>
<connect gate="E" pin="IO_5" pad="H24"/>
<connect gate="E" pin="IO_50" pad="L21"/>
<connect gate="E" pin="IO_51" pad="L22"/>
<connect gate="E" pin="IO_52" pad="L23"/>
<connect gate="E" pin="IO_53" pad="L24"/>
<connect gate="E" pin="IO_54" pad="L25"/>
<connect gate="E" pin="IO_55" pad="L26"/>
<connect gate="E" pin="IO_56" pad="L27"/>
<connect gate="E" pin="IO_57" pad="L28"/>
<connect gate="E" pin="IO_58" pad="M10"/>
<connect gate="E" pin="IO_59" pad="M11"/>
<connect gate="E" pin="IO_6" pad="H25"/>
<connect gate="E" pin="IO_60" pad="M12"/>
<connect gate="E" pin="IO_61" pad="M18"/>
<connect gate="E" pin="IO_62" pad="M19"/>
<connect gate="E" pin="IO_63" pad="M20"/>
<connect gate="E" pin="IO_64" pad="M21"/>
<connect gate="E" pin="IO_65" pad="M22"/>
<connect gate="E" pin="IO_66" pad="M23"/>
<connect gate="E" pin="IO_67" pad="M24"/>
<connect gate="E" pin="IO_68" pad="M25"/>
<connect gate="E" pin="IO_69" pad="M26"/>
<connect gate="E" pin="IO_7" pad="H26"/>
<connect gate="E" pin="IO_70" pad="M27"/>
<connect gate="E" pin="IO_71" pad="N10"/>
<connect gate="E" pin="IO_72" pad="N19"/>
<connect gate="E" pin="IO_73" pad="N20"/>
<connect gate="E" pin="IO_74" pad="N21"/>
<connect gate="E" pin="IO_8" pad="H27"/>
<connect gate="E" pin="IO_9" pad="H28"/>
<connect gate="E" pin="NCONFIG" pad="L16"/>
<connect gate="E" pin="NSTATUS" pad="M16"/>
<connect gate="E" pin="TCK" pad="K12"/>
<connect gate="E" pin="TRST" pad="L12"/>
<connect gate="E" pin="VCCINT" pad="N17"/>
<connect gate="E" pin="VCCINT_2" pad="N13"/>
<connect gate="E" pin="VCCINT_3" pad="N11"/>
<connect gate="E" pin="VCCINT_4" pad="N15"/>
<connect gate="E" pin="VCCINT_5" pad="M14"/>
<connect gate="E" pin="VCCIO2" pad="M28"/>
<connect gate="E" pin="VCCIO3" pad="J15"/>
<connect gate="E" pin="VCCIO4" pad="J14"/>
<connect gate="E" pin="VREF1B2" pad="K20"/>
<connect gate="F" pin="CLK0N" pad="N27"/>
<connect gate="F" pin="CLK0P" pad="P27"/>
<connect gate="F" pin="CLK1P" pad="P25"/>
<connect gate="F" pin="CLK2N" pad="T27"/>
<connect gate="F" pin="CLK2P" pad="R27"/>
<connect gate="F" pin="CLK3P" pad="R25"/>
<connect gate="F" pin="GND" pad="V15"/>
<connect gate="F" pin="GNDA_PLL1" pad="P24"/>
<connect gate="F" pin="GNDA_PLL2" pad="R24"/>
<connect gate="F" pin="GNDG_PLL1" pad="P22"/>
<connect gate="F" pin="GNDG_PLL2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="P17"/>
<connect gate="F" pin="GND_11" pad="T17"/>
<connect gate="F" pin="GND_12" pad="P15"/>
<connect gate="F" pin="GND_13" pad="T15"/>
<connect gate="F" pin="GND_14" pad="P18"/>
<connect gate="F" pin="GND_15" pad="U16"/>
<connect gate="F" pin="GND_16" pad="T13"/>
<connect gate="F" pin="GND_17" pad="U18"/>
<connect gate="F" pin="GND_18" pad="R28"/>
<connect gate="F" pin="GND_19" pad="T11"/>
<connect gate="F" pin="GND_2" pad="R11"/>
<connect gate="F" pin="GND_20" pad="V14"/>
<connect gate="F" pin="GND_21" pad="U14"/>
<connect gate="F" pin="GND_22" pad="V17"/>
<connect gate="F" pin="GND_23" pad="P11"/>
<connect gate="F" pin="GND_24" pad="U12"/>
<connect gate="F" pin="GND_3" pad="R12"/>
<connect gate="F" pin="GND_4" pad="P13"/>
<connect gate="F" pin="GND_5" pad="P28"/>
<connect gate="F" pin="GND_6" pad="R14"/>
<connect gate="F" pin="GND_7" pad="R16"/>
<connect gate="F" pin="GND_8" pad="R18"/>
<connect gate="F" pin="GND_9" pad="V13"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="T19"/>
<connect gate="F" pin="IO_11" pad="T20"/>
<connect gate="F" pin="IO_12" pad="T21"/>
<connect gate="F" pin="IO_13" pad="T22"/>
<connect gate="F" pin="IO_14" pad="T23"/>
<connect gate="F" pin="IO_15" pad="T24"/>
<connect gate="F" pin="IO_16" pad="T25"/>
<connect gate="F" pin="IO_17" pad="T26"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U10"/>
<connect gate="F" pin="IO_2" pad="N23"/>
<connect gate="F" pin="IO_20" pad="U19"/>
<connect gate="F" pin="IO_21" pad="U20"/>
<connect gate="F" pin="IO_22" pad="U21"/>
<connect gate="F" pin="IO_23" pad="U22"/>
<connect gate="F" pin="IO_24" pad="U23"/>
<connect gate="F" pin="IO_25" pad="U24"/>
<connect gate="F" pin="IO_26" pad="U25"/>
<connect gate="F" pin="IO_27" pad="U26"/>
<connect gate="F" pin="IO_28" pad="U27"/>
<connect gate="F" pin="IO_29" pad="V10"/>
<connect gate="F" pin="IO_3" pad="N28"/>
<connect gate="F" pin="IO_30" pad="V11"/>
<connect gate="F" pin="IO_31" pad="V18"/>
<connect gate="F" pin="IO_32" pad="V19"/>
<connect gate="F" pin="IO_33" pad="V20"/>
<connect gate="F" pin="IO_34" pad="V21"/>
<connect gate="F" pin="IO_35" pad="V22"/>
<connect gate="F" pin="IO_36" pad="V23"/>
<connect gate="F" pin="IO_37" pad="V24"/>
<connect gate="F" pin="IO_4" pad="N24"/>
<connect gate="F" pin="IO_5" pad="P26"/>
<connect gate="F" pin="IO_6" pad="R26"/>
<connect gate="F" pin="IO_7" pad="N25"/>
<connect gate="F" pin="IO_8" pad="T10"/>
<connect gate="F" pin="IO_9" pad="N26"/>
<connect gate="F" pin="NC" pad="P19"/>
<connect gate="F" pin="VCCA_PLL1" pad="P23"/>
<connect gate="F" pin="VCCA_PLL2" pad="R23"/>
<connect gate="F" pin="VCCG_PLL1" pad="P21"/>
<connect gate="F" pin="VCCG_PLL2" pad="R21"/>
<connect gate="F" pin="VCCINT" pad="U11"/>
<connect gate="F" pin="VCCINT_10" pad="U17"/>
<connect gate="F" pin="VCCINT_11" pad="T16"/>
<connect gate="F" pin="VCCINT_12" pad="R17"/>
<connect gate="F" pin="VCCINT_13" pad="V12"/>
<connect gate="F" pin="VCCINT_14" pad="T18"/>
<connect gate="F" pin="VCCINT_15" pad="V16"/>
<connect gate="F" pin="VCCINT_16" pad="P16"/>
<connect gate="F" pin="VCCINT_2" pad="T12"/>
<connect gate="F" pin="VCCINT_3" pad="P12"/>
<connect gate="F" pin="VCCINT_4" pad="U13"/>
<connect gate="F" pin="VCCINT_5" pad="P14"/>
<connect gate="F" pin="VCCINT_6" pad="T14"/>
<connect gate="F" pin="VCCINT_7" pad="U15"/>
<connect gate="F" pin="VCCINT_8" pad="R13"/>
<connect gate="F" pin="VCCINT_9" pad="R15"/>
<connect gate="F" pin="VCCIO1" pad="U28"/>
<connect gate="F" pin="VCCIO1_2" pad="R20"/>
<connect gate="F" pin="VCCIO2" pad="P20"/>
<connect gate="F" pin="VREF0B1" pad="R19"/>
<connect gate="F" pin="VREF0B5" pad="P10"/>
<connect gate="F" pin="VREF2B6" pad="R10"/>
<connect gate="G" pin="CLK4P" pad="AC17"/>
<connect gate="G" pin="CLK5P" pad="AA17"/>
<connect gate="G" pin="CLK7P" pad="W13"/>
<connect gate="G" pin="GND" pad="AA16"/>
<connect gate="G" pin="GNDG_PLL6" pad="AB14"/>
<connect gate="G" pin="GND_2" pad="AC15"/>
<connect gate="G" pin="IO" pad="AB12"/>
<connect gate="G" pin="IO_10" pad="W24"/>
<connect gate="G" pin="IO_11" pad="V28"/>
<connect gate="G" pin="IO_12" pad="W19"/>
<connect gate="G" pin="IO_13" pad="W16"/>
<connect gate="G" pin="IO_14" pad="W25"/>
<connect gate="G" pin="IO_15" pad="W10"/>
<connect gate="G" pin="IO_16" pad="W26"/>
<connect gate="G" pin="IO_17" pad="W11"/>
<connect gate="G" pin="IO_18" pad="W27"/>
<connect gate="G" pin="IO_19" pad="W12"/>
<connect gate="G" pin="IO_2" pad="W21"/>
<connect gate="G" pin="IO_20" pad="W28"/>
<connect gate="G" pin="IO_21" pad="Y16"/>
<connect gate="G" pin="IO_22" pad="Y10"/>
<connect gate="G" pin="IO_23" pad="Y17"/>
<connect gate="G" pin="IO_24" pad="Y11"/>
<connect gate="G" pin="IO_25" pad="Y18"/>
<connect gate="G" pin="IO_26" pad="Y19"/>
<connect gate="G" pin="IO_27" pad="Y13"/>
<connect gate="G" pin="IO_28" pad="Y20"/>
<connect gate="G" pin="IO_29" pad="Y21"/>
<connect gate="G" pin="IO_3" pad="W22"/>
<connect gate="G" pin="IO_30" pad="Y22"/>
<connect gate="G" pin="IO_31" pad="Y23"/>
<connect gate="G" pin="IO_32" pad="Y24"/>
<connect gate="G" pin="IO_33" pad="Y25"/>
<connect gate="G" pin="IO_34" pad="Y26"/>
<connect gate="G" pin="IO_35" pad="Y27"/>
<connect gate="G" pin="IO_36" pad="AA14"/>
<connect gate="G" pin="IO_37" pad="Y28"/>
<connect gate="G" pin="IO_38" pad="AA15"/>
<connect gate="G" pin="IO_39" pad="AA10"/>
<connect gate="G" pin="IO_4" pad="V26"/>
<connect gate="G" pin="IO_40" pad="AA11"/>
<connect gate="G" pin="IO_41" pad="AB17"/>
<connect gate="G" pin="IO_42" pad="AB18"/>
<connect gate="G" pin="IO_43" pad="AB19"/>
<connect gate="G" pin="IO_44" pad="AB20"/>
<connect gate="G" pin="IO_45" pad="AB21"/>
<connect gate="G" pin="IO_46" pad="AB22"/>
<connect gate="G" pin="IO_47" pad="AB23"/>
<connect gate="G" pin="IO_48" pad="AB24"/>
<connect gate="G" pin="IO_49" pad="AB25"/>
<connect gate="G" pin="IO_5" pad="W23"/>
<connect gate="G" pin="IO_50" pad="AB26"/>
<connect gate="G" pin="IO_51" pad="AB27"/>
<connect gate="G" pin="IO_52" pad="AA18"/>
<connect gate="G" pin="IO_53" pad="AB28"/>
<connect gate="G" pin="IO_54" pad="AA19"/>
<connect gate="G" pin="IO_55" pad="AC10"/>
<connect gate="G" pin="IO_56" pad="AA20"/>
<connect gate="G" pin="IO_57" pad="AC11"/>
<connect gate="G" pin="IO_58" pad="AA21"/>
<connect gate="G" pin="IO_59" pad="AA22"/>
<connect gate="G" pin="IO_6" pad="V27"/>
<connect gate="G" pin="IO_60" pad="AC19"/>
<connect gate="G" pin="IO_61" pad="AA23"/>
<connect gate="G" pin="IO_62" pad="AC20"/>
<connect gate="G" pin="IO_63" pad="AA24"/>
<connect gate="G" pin="IO_64" pad="AC21"/>
<connect gate="G" pin="IO_65" pad="AA25"/>
<connect gate="G" pin="IO_66" pad="AC22"/>
<connect gate="G" pin="IO_67" pad="AA26"/>
<connect gate="G" pin="IO_68" pad="AC23"/>
<connect gate="G" pin="IO_69" pad="AA27"/>
<connect gate="G" pin="IO_7" pad="W14"/>
<connect gate="G" pin="IO_70" pad="AC24"/>
<connect gate="G" pin="IO_71" pad="AA28"/>
<connect gate="G" pin="IO_72" pad="AC27"/>
<connect gate="G" pin="IO_73" pad="AB10"/>
<connect gate="G" pin="IO_74" pad="AC28"/>
<connect gate="G" pin="IO_75" pad="AB11"/>
<connect gate="G" pin="IO_8" pad="W15"/>
<connect gate="G" pin="IO_9" pad="W18"/>
<connect gate="G" pin="MSEL0" pad="AC16"/>
<connect gate="G" pin="MSEL1" pad="W17"/>
<connect gate="G" pin="MSEL2" pad="AB15"/>
<connect gate="G" pin="NC" pad="AC26"/>
<connect gate="G" pin="NCE" pad="AB13"/>
<connect gate="G" pin="NCEO" pad="AC13"/>
<connect gate="G" pin="NC_2" pad="AC25"/>
<connect gate="G" pin="NIO_PULLUP" pad="Y12"/>
<connect gate="G" pin="PLL_ENA" pad="AC18"/>
<connect gate="G" pin="PORSEL" pad="AC12"/>
<connect gate="G" pin="VCCG_PLL6" pad="AA13"/>
<connect gate="G" pin="VCCIO7" pad="Y14"/>
<connect gate="G" pin="VCCIO8" pad="Y15"/>
<connect gate="G" pin="VCCSEL" pad="AA12"/>
<connect gate="G" pin="VCC_PLL6_OUTA" pad="AC14"/>
<connect gate="G" pin="VCC_PLL6_OUTB" pad="AB16"/>
<connect gate="G" pin="VREF1B1" pad="W20"/>
<connect gate="H" pin="CLK6P" pad="AD14"/>
<connect gate="H" pin="GND" pad="AH15"/>
<connect gate="H" pin="GNDA_PLL6" pad="AF14"/>
<connect gate="H" pin="GND_2" pad="AF26"/>
<connect gate="H" pin="GND_3" pad="AH14"/>
<connect gate="H" pin="GND_4" pad="AG27"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD13"/>
<connect gate="H" pin="IO_11" pad="AE12"/>
<connect gate="H" pin="IO_12" pad="AD10"/>
<connect gate="H" pin="IO_13" pad="AE13"/>
<connect gate="H" pin="IO_14" pad="AD15"/>
<connect gate="H" pin="IO_15" pad="AE14"/>
<connect gate="H" pin="IO_16" pad="AD16"/>
<connect gate="H" pin="IO_17" pad="AE15"/>
<connect gate="H" pin="IO_18" pad="AD17"/>
<connect gate="H" pin="IO_19" pad="AE16"/>
<connect gate="H" pin="IO_2" pad="AD23"/>
<connect gate="H" pin="IO_20" pad="AD18"/>
<connect gate="H" pin="IO_21" pad="AE17"/>
<connect gate="H" pin="IO_22" pad="AD19"/>
<connect gate="H" pin="IO_23" pad="AE18"/>
<connect gate="H" pin="IO_24" pad="AE19"/>
<connect gate="H" pin="IO_25" pad="AE20"/>
<connect gate="H" pin="IO_26" pad="AE21"/>
<connect gate="H" pin="IO_27" pad="AE27"/>
<connect gate="H" pin="IO_28" pad="AE22"/>
<connect gate="H" pin="IO_29" pad="AE28"/>
<connect gate="H" pin="IO_3" pad="AD24"/>
<connect gate="H" pin="IO_30" pad="AE23"/>
<connect gate="H" pin="IO_31" pad="AF10"/>
<connect gate="H" pin="IO_32" pad="AE24"/>
<connect gate="H" pin="IO_33" pad="AF15"/>
<connect gate="H" pin="IO_34" pad="AF11"/>
<connect gate="H" pin="IO_35" pad="AF16"/>
<connect gate="H" pin="IO_36" pad="AE25"/>
<connect gate="H" pin="IO_37" pad="AF17"/>
<connect gate="H" pin="IO_38" pad="AF12"/>
<connect gate="H" pin="IO_39" pad="AF18"/>
<connect gate="H" pin="IO_4" pad="AD27"/>
<connect gate="H" pin="IO_40" pad="AF13"/>
<connect gate="H" pin="IO_41" pad="AF19"/>
<connect gate="H" pin="IO_42" pad="AF20"/>
<connect gate="H" pin="IO_43" pad="AF21"/>
<connect gate="H" pin="IO_44" pad="AF22"/>
<connect gate="H" pin="IO_45" pad="AF23"/>
<connect gate="H" pin="IO_46" pad="AF24"/>
<connect gate="H" pin="IO_47" pad="AF25"/>
<connect gate="H" pin="IO_48" pad="AF27"/>
<connect gate="H" pin="IO_49" pad="AF28"/>
<connect gate="H" pin="IO_5" pad="AD28"/>
<connect gate="H" pin="IO_50" pad="AG10"/>
<connect gate="H" pin="IO_51" pad="AG11"/>
<connect gate="H" pin="IO_52" pad="AG12"/>
<connect gate="H" pin="IO_53" pad="AG13"/>
<connect gate="H" pin="IO_54" pad="AG15"/>
<connect gate="H" pin="IO_55" pad="AG16"/>
<connect gate="H" pin="IO_56" pad="AG17"/>
<connect gate="H" pin="IO_57" pad="AG18"/>
<connect gate="H" pin="IO_58" pad="AG19"/>
<connect gate="H" pin="IO_59" pad="AG20"/>
<connect gate="H" pin="IO_6" pad="AE10"/>
<connect gate="H" pin="IO_60" pad="AG21"/>
<connect gate="H" pin="IO_61" pad="AG22"/>
<connect gate="H" pin="IO_62" pad="AG23"/>
<connect gate="H" pin="IO_63" pad="AG24"/>
<connect gate="H" pin="IO_64" pad="AG25"/>
<connect gate="H" pin="IO_65" pad="AG26"/>
<connect gate="H" pin="IO_66" pad="AH10"/>
<connect gate="H" pin="IO_67" pad="AH11"/>
<connect gate="H" pin="IO_68" pad="AH13"/>
<connect gate="H" pin="IO_69" pad="AH16"/>
<connect gate="H" pin="IO_7" pad="AD21"/>
<connect gate="H" pin="IO_70" pad="AH19"/>
<connect gate="H" pin="IO_71" pad="AH20"/>
<connect gate="H" pin="IO_72" pad="AH21"/>
<connect gate="H" pin="IO_73" pad="AH22"/>
<connect gate="H" pin="IO_74" pad="AH23"/>
<connect gate="H" pin="IO_75" pad="AH24"/>
<connect gate="H" pin="IO_76" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD12"/>
<connect gate="H" pin="IO_9" pad="AE11"/>
<connect gate="H" pin="NC" pad="AD26"/>
<connect gate="H" pin="NC_2" pad="AD25"/>
<connect gate="H" pin="VCCA_PLL6" pad="AG14"/>
<connect gate="H" pin="VCCIO1" pad="AG28"/>
<connect gate="H" pin="VCCIO7" pad="AH12"/>
<connect gate="H" pin="VCCIO8" pad="AH27"/>
<connect gate="H" pin="VCCIO8_2" pad="AH17"/>
<connect gate="H" pin="VREF0B7" pad="AD11"/>
<connect gate="H" pin="VREF0B8" pad="AD22"/>
<connect gate="H" pin="VREF1B8" pad="AD20"/>
<connect gate="H" pin="VREF2B1" pad="AE26"/>
<connect gate="H" pin="VREF2B8" pad="AH18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1S25F780C6N"/>
<attribute name="OC_FARNELL" value="1549496"/>
<attribute name="OC_NEWARK" value="52R0329"/>
<attribute name="PACKAGE" value="BGA-780"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1S30F780C7N">
<description>Stratix Device</description>
<gates>
<gate name="A" symbol="EP1S30F780C7N_A"/>
<gate name="B" symbol="EP1S30F780C7N_B"/>
<gate name="C" symbol="EP1S30F780C7N_C"/>
<gate name="D" symbol="EP1S30F780C7N_D"/>
<gate name="E" symbol="EP1S30F780C7N_E"/>
<gate name="F" symbol="EP1S30F780C7N_F"/>
<gate name="G" symbol="EP1S30F780C7N_G"/>
<gate name="H" symbol="EP1S30F780C7N_H"/>
</gates>
<devices>
<device name="" package="BGA780C28X28X100P_2900X2900X35">
<connects>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="IO" pad="L9"/>
<connect gate="A" pin="IO_10" pad="B4"/>
<connect gate="A" pin="IO_11" pad="B5"/>
<connect gate="A" pin="IO_12" pad="B6"/>
<connect gate="A" pin="IO_13" pad="B7"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="B9"/>
<connect gate="A" pin="IO_16" pad="C1"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C4"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="D1"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E1"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E6"/>
<connect gate="A" pin="IO_34" pad="E8"/>
<connect gate="A" pin="IO_35" pad="F1"/>
<connect gate="A" pin="IO_36" pad="F2"/>
<connect gate="A" pin="IO_37" pad="F3"/>
<connect gate="A" pin="IO_38" pad="F4"/>
<connect gate="A" pin="IO_39" pad="F5"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="F6"/>
<connect gate="A" pin="IO_41" pad="F7"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G4"/>
<connect gate="A" pin="IO_48" pad="G5"/>
<connect gate="A" pin="IO_49" pad="G6"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="G7"/>
<connect gate="A" pin="IO_51" pad="G8"/>
<connect gate="A" pin="IO_52" pad="G9"/>
<connect gate="A" pin="IO_53" pad="H1"/>
<connect gate="A" pin="IO_54" pad="H2"/>
<connect gate="A" pin="IO_55" pad="H3"/>
<connect gate="A" pin="IO_56" pad="H4"/>
<connect gate="A" pin="IO_57" pad="H5"/>
<connect gate="A" pin="IO_58" pad="H6"/>
<connect gate="A" pin="IO_59" pad="H7"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="H8"/>
<connect gate="A" pin="IO_61" pad="H9"/>
<connect gate="A" pin="IO_62" pad="J1"/>
<connect gate="A" pin="IO_63" pad="J2"/>
<connect gate="A" pin="IO_64" pad="J3"/>
<connect gate="A" pin="IO_65" pad="J4"/>
<connect gate="A" pin="IO_66" pad="J5"/>
<connect gate="A" pin="IO_67" pad="J6"/>
<connect gate="A" pin="IO_68" pad="J7"/>
<connect gate="A" pin="IO_69" pad="J8"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_70" pad="J9"/>
<connect gate="A" pin="IO_71" pad="K1"/>
<connect gate="A" pin="IO_72" pad="K2"/>
<connect gate="A" pin="IO_73" pad="K3"/>
<connect gate="A" pin="IO_74" pad="K4"/>
<connect gate="A" pin="IO_75" pad="K5"/>
<connect gate="A" pin="IO_76" pad="K6"/>
<connect gate="A" pin="IO_77" pad="K7"/>
<connect gate="A" pin="IO_78" pad="K8"/>
<connect gate="A" pin="IO_79" pad="L1"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_80" pad="L2"/>
<connect gate="A" pin="IO_81" pad="L3"/>
<connect gate="A" pin="IO_82" pad="L4"/>
<connect gate="A" pin="IO_83" pad="L5"/>
<connect gate="A" pin="IO_84" pad="L6"/>
<connect gate="A" pin="IO_85" pad="L7"/>
<connect gate="A" pin="IO_86" pad="L8"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="NC" pad="E4"/>
<connect gate="A" pin="NC_2" pad="D3"/>
<connect gate="A" pin="NC_3" pad="D4"/>
<connect gate="A" pin="NC_4" pad="E3"/>
<connect gate="A" pin="VCCIO4" pad="A2"/>
<connect gate="A" pin="VCCIO5" pad="B1"/>
<connect gate="A" pin="VREF0B4" pad="E7"/>
<connect gate="A" pin="VREF1B4" pad="E9"/>
<connect gate="A" pin="VREF1B5" pad="K9"/>
<connect gate="A" pin="VREF2B5" pad="E5"/>
<connect gate="B" pin="CLK10P" pad="P4"/>
<connect gate="B" pin="CLK11N" pad="N2"/>
<connect gate="B" pin="CLK11P" pad="P2"/>
<connect gate="B" pin="CLK8P" pad="R4"/>
<connect gate="B" pin="CLK9N" pad="T2"/>
<connect gate="B" pin="CLK9P" pad="R2"/>
<connect gate="B" pin="GND" pad="A14"/>
<connect gate="B" pin="GNDA_PLL3" pad="R5"/>
<connect gate="B" pin="GNDA_PLL4" pad="P5"/>
<connect gate="B" pin="GNDG_PLL3" pad="R7"/>
<connect gate="B" pin="GNDG_PLL4" pad="P7"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="R1"/>
<connect gate="B" pin="GND_4" pad="A15"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="N1"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="N4"/>
<connect gate="B" pin="IO_13" pad="N5"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="N8"/>
<connect gate="B" pin="IO_17" pad="N9"/>
<connect gate="B" pin="IO_18" pad="P3"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="M2"/>
<connect gate="B" pin="IO_20" pad="T1"/>
<connect gate="B" pin="IO_21" pad="T3"/>
<connect gate="B" pin="IO_22" pad="T4"/>
<connect gate="B" pin="IO_23" pad="T5"/>
<connect gate="B" pin="IO_24" pad="T6"/>
<connect gate="B" pin="IO_25" pad="T7"/>
<connect gate="B" pin="IO_26" pad="T8"/>
<connect gate="B" pin="IO_27" pad="T9"/>
<connect gate="B" pin="IO_28" pad="U2"/>
<connect gate="B" pin="IO_29" pad="U3"/>
<connect gate="B" pin="IO_3" pad="M3"/>
<connect gate="B" pin="IO_30" pad="U4"/>
<connect gate="B" pin="IO_31" pad="U5"/>
<connect gate="B" pin="IO_32" pad="U6"/>
<connect gate="B" pin="IO_33" pad="U7"/>
<connect gate="B" pin="IO_34" pad="U8"/>
<connect gate="B" pin="IO_35" pad="U9"/>
<connect gate="B" pin="IO_36" pad="V1"/>
<connect gate="B" pin="IO_37" pad="V2"/>
<connect gate="B" pin="IO_38" pad="V3"/>
<connect gate="B" pin="IO_39" pad="V4"/>
<connect gate="B" pin="IO_4" pad="M4"/>
<connect gate="B" pin="IO_40" pad="V5"/>
<connect gate="B" pin="IO_41" pad="V6"/>
<connect gate="B" pin="IO_42" pad="V7"/>
<connect gate="B" pin="IO_43" pad="V8"/>
<connect gate="B" pin="IO_44" pad="V9"/>
<connect gate="B" pin="IO_45" pad="W1"/>
<connect gate="B" pin="IO_46" pad="W2"/>
<connect gate="B" pin="IO_47" pad="W3"/>
<connect gate="B" pin="IO_48" pad="W4"/>
<connect gate="B" pin="IO_49" pad="W5"/>
<connect gate="B" pin="IO_5" pad="M5"/>
<connect gate="B" pin="IO_50" pad="W6"/>
<connect gate="B" pin="IO_51" pad="W7"/>
<connect gate="B" pin="IO_52" pad="W8"/>
<connect gate="B" pin="IO_53" pad="Y1"/>
<connect gate="B" pin="IO_54" pad="Y2"/>
<connect gate="B" pin="IO_55" pad="Y3"/>
<connect gate="B" pin="IO_56" pad="Y4"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="M6"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A11"/>
<connect gate="B" pin="IO_64" pad="A13"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A18"/>
<connect gate="B" pin="IO_67" pad="A19"/>
<connect gate="B" pin="IO_68" pad="A20"/>
<connect gate="B" pin="IO_69" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M7"/>
<connect gate="B" pin="IO_70" pad="A22"/>
<connect gate="B" pin="IO_71" pad="A23"/>
<connect gate="B" pin="IO_72" pad="A24"/>
<connect gate="B" pin="IO_73" pad="A25"/>
<connect gate="B" pin="IO_8" pad="M8"/>
<connect gate="B" pin="IO_9" pad="M9"/>
<connect gate="B" pin="VCCA_PLL3" pad="R6"/>
<connect gate="B" pin="VCCA_PLL4" pad="P6"/>
<connect gate="B" pin="VCCG_PLL3" pad="R8"/>
<connect gate="B" pin="VCCG_PLL4" pad="P8"/>
<connect gate="B" pin="VCCIO3" pad="A17"/>
<connect gate="B" pin="VCCIO4" pad="A12"/>
<connect gate="B" pin="VCCIO5" pad="M1"/>
<connect gate="B" pin="VCCIO5_2" pad="P9"/>
<connect gate="B" pin="VCCIO6" pad="R9"/>
<connect gate="B" pin="VCCIO6_2" pad="U1"/>
<connect gate="B" pin="VREF1B6" pad="W9"/>
<connect gate="C" pin="GND" pad="B27"/>
<connect gate="C" pin="GND_2" pad="AF3"/>
<connect gate="C" pin="GND_3" pad="AG2"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AA9"/>
<connect gate="C" pin="IO_11" pad="AB1"/>
<connect gate="C" pin="IO_12" pad="AB2"/>
<connect gate="C" pin="IO_13" pad="AB3"/>
<connect gate="C" pin="IO_14" pad="AB4"/>
<connect gate="C" pin="IO_15" pad="AB5"/>
<connect gate="C" pin="IO_16" pad="AB6"/>
<connect gate="C" pin="IO_17" pad="AB7"/>
<connect gate="C" pin="IO_18" pad="AB8"/>
<connect gate="C" pin="IO_19" pad="AB9"/>
<connect gate="C" pin="IO_2" pad="AA1"/>
<connect gate="C" pin="IO_20" pad="AC1"/>
<connect gate="C" pin="IO_21" pad="AC2"/>
<connect gate="C" pin="IO_22" pad="AC5"/>
<connect gate="C" pin="IO_23" pad="AC6"/>
<connect gate="C" pin="IO_24" pad="AC7"/>
<connect gate="C" pin="IO_25" pad="AC8"/>
<connect gate="C" pin="IO_26" pad="AC9"/>
<connect gate="C" pin="IO_27" pad="AD1"/>
<connect gate="C" pin="IO_28" pad="AD2"/>
<connect gate="C" pin="IO_29" pad="AD5"/>
<connect gate="C" pin="IO_3" pad="AA2"/>
<connect gate="C" pin="IO_30" pad="AD6"/>
<connect gate="C" pin="IO_31" pad="AD8"/>
<connect gate="C" pin="IO_32" pad="AE1"/>
<connect gate="C" pin="IO_33" pad="AE2"/>
<connect gate="C" pin="IO_34" pad="AE4"/>
<connect gate="C" pin="IO_35" pad="AE5"/>
<connect gate="C" pin="IO_36" pad="AE6"/>
<connect gate="C" pin="IO_37" pad="AE7"/>
<connect gate="C" pin="IO_38" pad="AE8"/>
<connect gate="C" pin="IO_39" pad="AE9"/>
<connect gate="C" pin="IO_4" pad="AA3"/>
<connect gate="C" pin="IO_40" pad="AF1"/>
<connect gate="C" pin="IO_41" pad="AF2"/>
<connect gate="C" pin="IO_42" pad="AF4"/>
<connect gate="C" pin="IO_43" pad="AF5"/>
<connect gate="C" pin="IO_44" pad="AF6"/>
<connect gate="C" pin="IO_45" pad="AF7"/>
<connect gate="C" pin="IO_46" pad="AF8"/>
<connect gate="C" pin="IO_47" pad="AF9"/>
<connect gate="C" pin="IO_48" pad="AG3"/>
<connect gate="C" pin="IO_49" pad="AG4"/>
<connect gate="C" pin="IO_5" pad="AA4"/>
<connect gate="C" pin="IO_50" pad="AG5"/>
<connect gate="C" pin="IO_51" pad="AG6"/>
<connect gate="C" pin="IO_52" pad="AG7"/>
<connect gate="C" pin="IO_53" pad="AG8"/>
<connect gate="C" pin="IO_54" pad="AG9"/>
<connect gate="C" pin="IO_55" pad="AH3"/>
<connect gate="C" pin="IO_56" pad="AH4"/>
<connect gate="C" pin="IO_57" pad="AH5"/>
<connect gate="C" pin="IO_58" pad="AH6"/>
<connect gate="C" pin="IO_59" pad="AH7"/>
<connect gate="C" pin="IO_6" pad="AA5"/>
<connect gate="C" pin="IO_60" pad="AH8"/>
<connect gate="C" pin="IO_61" pad="AH9"/>
<connect gate="C" pin="IO_62" pad="B10"/>
<connect gate="C" pin="IO_63" pad="B11"/>
<connect gate="C" pin="IO_64" pad="B12"/>
<connect gate="C" pin="IO_65" pad="B13"/>
<connect gate="C" pin="IO_66" pad="B15"/>
<connect gate="C" pin="IO_67" pad="B16"/>
<connect gate="C" pin="IO_68" pad="B17"/>
<connect gate="C" pin="IO_69" pad="B18"/>
<connect gate="C" pin="IO_7" pad="AA6"/>
<connect gate="C" pin="IO_70" pad="B19"/>
<connect gate="C" pin="IO_71" pad="B20"/>
<connect gate="C" pin="IO_72" pad="B21"/>
<connect gate="C" pin="IO_73" pad="B22"/>
<connect gate="C" pin="IO_74" pad="B23"/>
<connect gate="C" pin="IO_75" pad="B24"/>
<connect gate="C" pin="IO_76" pad="B25"/>
<connect gate="C" pin="IO_77" pad="B26"/>
<connect gate="C" pin="IO_78" pad="C10"/>
<connect gate="C" pin="IO_79" pad="C11"/>
<connect gate="C" pin="IO_8" pad="AA7"/>
<connect gate="C" pin="IO_80" pad="C12"/>
<connect gate="C" pin="IO_81" pad="C13"/>
<connect gate="C" pin="IO_82" pad="C15"/>
<connect gate="C" pin="IO_9" pad="AA8"/>
<connect gate="C" pin="NC" pad="AD4"/>
<connect gate="C" pin="NC_2" pad="AC3"/>
<connect gate="C" pin="NC_3" pad="AC4"/>
<connect gate="C" pin="NC_4" pad="AD3"/>
<connect gate="C" pin="TEMPDIODEN" pad="C14"/>
<connect gate="C" pin="TEMPDIODEP" pad="B14"/>
<connect gate="C" pin="VCCIO2" pad="B28"/>
<connect gate="C" pin="VCCIO3" pad="A27"/>
<connect gate="C" pin="VCCIO6" pad="AG1"/>
<connect gate="C" pin="VCCIO7" pad="AH2"/>
<connect gate="C" pin="VREF0B6" pad="AE3"/>
<connect gate="C" pin="VREF1B7" pad="AD9"/>
<connect gate="C" pin="VREF2B7" pad="AD7"/>
<connect gate="D" pin="CONF_DONE" pad="G17"/>
<connect gate="D" pin="DCLK" pad="F16"/>
<connect gate="D" pin="GND" pad="C26"/>
<connect gate="D" pin="GNDA_PLL5" pad="G14"/>
<connect gate="D" pin="GNDG_PLL5" pad="E14"/>
<connect gate="D" pin="GND_2" pad="H16"/>
<connect gate="D" pin="GND_3" pad="G15"/>
<connect gate="D" pin="GND_4" pad="G20"/>
<connect gate="D" pin="IO" pad="H19"/>
<connect gate="D" pin="IO_10" pad="C25"/>
<connect gate="D" pin="IO_11" pad="C27"/>
<connect gate="D" pin="IO_12" pad="C28"/>
<connect gate="D" pin="IO_13" pad="D10"/>
<connect gate="D" pin="IO_14" pad="D11"/>
<connect gate="D" pin="IO_15" pad="D12"/>
<connect gate="D" pin="IO_16" pad="D13"/>
<connect gate="D" pin="IO_17" pad="D15"/>
<connect gate="D" pin="IO_18" pad="D16"/>
<connect gate="D" pin="IO_19" pad="D17"/>
<connect gate="D" pin="IO_2" pad="C17"/>
<connect gate="D" pin="IO_20" pad="D18"/>
<connect gate="D" pin="IO_21" pad="D19"/>
<connect gate="D" pin="IO_22" pad="D20"/>
<connect gate="D" pin="IO_23" pad="D21"/>
<connect gate="D" pin="IO_24" pad="D22"/>
<connect gate="D" pin="IO_25" pad="D23"/>
<connect gate="D" pin="IO_26" pad="D24"/>
<connect gate="D" pin="IO_27" pad="D27"/>
<connect gate="D" pin="IO_28" pad="D28"/>
<connect gate="D" pin="IO_29" pad="E10"/>
<connect gate="D" pin="IO_3" pad="C18"/>
<connect gate="D" pin="IO_30" pad="E12"/>
<connect gate="D" pin="IO_31" pad="E13"/>
<connect gate="D" pin="IO_32" pad="E15"/>
<connect gate="D" pin="IO_33" pad="E16"/>
<connect gate="D" pin="IO_34" pad="E17"/>
<connect gate="D" pin="IO_35" pad="E19"/>
<connect gate="D" pin="IO_36" pad="E21"/>
<connect gate="D" pin="IO_37" pad="E23"/>
<connect gate="D" pin="IO_38" pad="E27"/>
<connect gate="D" pin="IO_39" pad="E28"/>
<connect gate="D" pin="IO_4" pad="C19"/>
<connect gate="D" pin="IO_40" pad="F10"/>
<connect gate="D" pin="IO_41" pad="F11"/>
<connect gate="D" pin="IO_42" pad="F12"/>
<connect gate="D" pin="IO_43" pad="F17"/>
<connect gate="D" pin="IO_44" pad="F18"/>
<connect gate="D" pin="IO_45" pad="F19"/>
<connect gate="D" pin="IO_46" pad="F20"/>
<connect gate="D" pin="IO_47" pad="F21"/>
<connect gate="D" pin="IO_48" pad="F22"/>
<connect gate="D" pin="IO_49" pad="F23"/>
<connect gate="D" pin="IO_5" pad="C20"/>
<connect gate="D" pin="IO_50" pad="F24"/>
<connect gate="D" pin="IO_51" pad="F25"/>
<connect gate="D" pin="IO_52" pad="F26"/>
<connect gate="D" pin="IO_53" pad="F27"/>
<connect gate="D" pin="IO_54" pad="F28"/>
<connect gate="D" pin="IO_55" pad="G10"/>
<connect gate="D" pin="IO_56" pad="G11"/>
<connect gate="D" pin="IO_57" pad="G12"/>
<connect gate="D" pin="IO_58" pad="G18"/>
<connect gate="D" pin="IO_59" pad="G19"/>
<connect gate="D" pin="IO_6" pad="C21"/>
<connect gate="D" pin="IO_60" pad="G21"/>
<connect gate="D" pin="IO_61" pad="G22"/>
<connect gate="D" pin="IO_62" pad="G23"/>
<connect gate="D" pin="IO_63" pad="G24"/>
<connect gate="D" pin="IO_64" pad="G25"/>
<connect gate="D" pin="IO_65" pad="G26"/>
<connect gate="D" pin="IO_66" pad="G27"/>
<connect gate="D" pin="IO_67" pad="G28"/>
<connect gate="D" pin="IO_68" pad="H10"/>
<connect gate="D" pin="IO_69" pad="H11"/>
<connect gate="D" pin="IO_7" pad="C22"/>
<connect gate="D" pin="IO_70" pad="H12"/>
<connect gate="D" pin="IO_71" pad="H14"/>
<connect gate="D" pin="IO_72" pad="H15"/>
<connect gate="D" pin="IO_73" pad="H17"/>
<connect gate="D" pin="IO_74" pad="H18"/>
<connect gate="D" pin="IO_8" pad="C23"/>
<connect gate="D" pin="IO_9" pad="C24"/>
<connect gate="D" pin="NC" pad="E26"/>
<connect gate="D" pin="NC_2" pad="D25"/>
<connect gate="D" pin="NC_3" pad="D26"/>
<connect gate="D" pin="NC_4" pad="E25"/>
<connect gate="D" pin="TDI" pad="G13"/>
<connect gate="D" pin="TDO" pad="H13"/>
<connect gate="D" pin="TMS" pad="F13"/>
<connect gate="D" pin="VCCA_PLL5" pad="F14"/>
<connect gate="D" pin="VCCG_PLL5" pad="D14"/>
<connect gate="D" pin="VCC_PLL5_OUTA" pad="F15"/>
<connect gate="D" pin="VCC_PLL5_OUTB" pad="G16"/>
<connect gate="D" pin="VREF0B2" pad="E24"/>
<connect gate="D" pin="VREF0B3" pad="E18"/>
<connect gate="D" pin="VREF1B3" pad="E20"/>
<connect gate="D" pin="VREF2B3" pad="E22"/>
<connect gate="D" pin="VREF2B4" pad="E11"/>
<connect gate="E" pin="CLK12P" pad="K13"/>
<connect gate="E" pin="CLK13P" pad="M13"/>
<connect gate="E" pin="CLK14P" pad="K17"/>
<connect gate="E" pin="CLK15P" pad="M17"/>
<connect gate="E" pin="GND" pad="L15"/>
<connect gate="E" pin="GND_2" pad="M15"/>
<connect gate="E" pin="GND_3" pad="N12"/>
<connect gate="E" pin="GND_4" pad="N14"/>
<connect gate="E" pin="GND_5" pad="N16"/>
<connect gate="E" pin="GND_6" pad="N18"/>
<connect gate="E" pin="GND_7" pad="L14"/>
<connect gate="E" pin="IO" pad="N22"/>
<connect gate="E" pin="IO_10" pad="H28"/>
<connect gate="E" pin="IO_11" pad="J10"/>
<connect gate="E" pin="IO_12" pad="J11"/>
<connect gate="E" pin="IO_13" pad="J12"/>
<connect gate="E" pin="IO_14" pad="J13"/>
<connect gate="E" pin="IO_15" pad="J16"/>
<connect gate="E" pin="IO_16" pad="J17"/>
<connect gate="E" pin="IO_17" pad="J18"/>
<connect gate="E" pin="IO_18" pad="J19"/>
<connect gate="E" pin="IO_19" pad="J20"/>
<connect gate="E" pin="IO_2" pad="H20"/>
<connect gate="E" pin="IO_20" pad="J21"/>
<connect gate="E" pin="IO_21" pad="J22"/>
<connect gate="E" pin="IO_22" pad="J23"/>
<connect gate="E" pin="IO_23" pad="J24"/>
<connect gate="E" pin="IO_24" pad="J25"/>
<connect gate="E" pin="IO_25" pad="J26"/>
<connect gate="E" pin="IO_26" pad="J27"/>
<connect gate="E" pin="IO_27" pad="J28"/>
<connect gate="E" pin="IO_28" pad="K10"/>
<connect gate="E" pin="IO_29" pad="K11"/>
<connect gate="E" pin="IO_3" pad="H21"/>
<connect gate="E" pin="IO_30" pad="K14"/>
<connect gate="E" pin="IO_31" pad="K15"/>
<connect gate="E" pin="IO_32" pad="K16"/>
<connect gate="E" pin="IO_33" pad="K18"/>
<connect gate="E" pin="IO_34" pad="K19"/>
<connect gate="E" pin="IO_35" pad="K21"/>
<connect gate="E" pin="IO_36" pad="K22"/>
<connect gate="E" pin="IO_37" pad="K23"/>
<connect gate="E" pin="IO_38" pad="K24"/>
<connect gate="E" pin="IO_39" pad="K25"/>
<connect gate="E" pin="IO_4" pad="H22"/>
<connect gate="E" pin="IO_40" pad="K26"/>
<connect gate="E" pin="IO_41" pad="K27"/>
<connect gate="E" pin="IO_42" pad="K28"/>
<connect gate="E" pin="IO_43" pad="L10"/>
<connect gate="E" pin="IO_44" pad="L11"/>
<connect gate="E" pin="IO_45" pad="L13"/>
<connect gate="E" pin="IO_46" pad="L17"/>
<connect gate="E" pin="IO_47" pad="L18"/>
<connect gate="E" pin="IO_48" pad="L19"/>
<connect gate="E" pin="IO_49" pad="L20"/>
<connect gate="E" pin="IO_5" pad="H23"/>
<connect gate="E" pin="IO_50" pad="L21"/>
<connect gate="E" pin="IO_51" pad="L22"/>
<connect gate="E" pin="IO_52" pad="L23"/>
<connect gate="E" pin="IO_53" pad="L24"/>
<connect gate="E" pin="IO_54" pad="L25"/>
<connect gate="E" pin="IO_55" pad="L26"/>
<connect gate="E" pin="IO_56" pad="L27"/>
<connect gate="E" pin="IO_57" pad="L28"/>
<connect gate="E" pin="IO_58" pad="M10"/>
<connect gate="E" pin="IO_59" pad="M11"/>
<connect gate="E" pin="IO_6" pad="H24"/>
<connect gate="E" pin="IO_60" pad="M12"/>
<connect gate="E" pin="IO_61" pad="M18"/>
<connect gate="E" pin="IO_62" pad="M19"/>
<connect gate="E" pin="IO_63" pad="M20"/>
<connect gate="E" pin="IO_64" pad="M21"/>
<connect gate="E" pin="IO_65" pad="M22"/>
<connect gate="E" pin="IO_66" pad="M23"/>
<connect gate="E" pin="IO_67" pad="M24"/>
<connect gate="E" pin="IO_68" pad="M25"/>
<connect gate="E" pin="IO_69" pad="M26"/>
<connect gate="E" pin="IO_7" pad="H25"/>
<connect gate="E" pin="IO_70" pad="M27"/>
<connect gate="E" pin="IO_71" pad="N10"/>
<connect gate="E" pin="IO_72" pad="N19"/>
<connect gate="E" pin="IO_73" pad="N20"/>
<connect gate="E" pin="IO_74" pad="N21"/>
<connect gate="E" pin="IO_8" pad="H26"/>
<connect gate="E" pin="IO_9" pad="H27"/>
<connect gate="E" pin="NCONFIG" pad="L16"/>
<connect gate="E" pin="NSTATUS" pad="M16"/>
<connect gate="E" pin="TCK" pad="K12"/>
<connect gate="E" pin="TRST" pad="L12"/>
<connect gate="E" pin="VCCINT" pad="N15"/>
<connect gate="E" pin="VCCINT_2" pad="N11"/>
<connect gate="E" pin="VCCINT_3" pad="N13"/>
<connect gate="E" pin="VCCINT_4" pad="M14"/>
<connect gate="E" pin="VCCINT_5" pad="N17"/>
<connect gate="E" pin="VCCIO2" pad="M28"/>
<connect gate="E" pin="VCCIO3" pad="J15"/>
<connect gate="E" pin="VCCIO4" pad="J14"/>
<connect gate="E" pin="VREF1B2" pad="K20"/>
<connect gate="F" pin="CLK0N" pad="N27"/>
<connect gate="F" pin="CLK0P" pad="P27"/>
<connect gate="F" pin="CLK1P" pad="P25"/>
<connect gate="F" pin="CLK2N" pad="T27"/>
<connect gate="F" pin="CLK2P" pad="R27"/>
<connect gate="F" pin="CLK3P" pad="R25"/>
<connect gate="F" pin="GND" pad="R12"/>
<connect gate="F" pin="GNDA_PLL1" pad="P24"/>
<connect gate="F" pin="GNDA_PLL2" pad="R24"/>
<connect gate="F" pin="GNDG_PLL1" pad="P22"/>
<connect gate="F" pin="GNDG_PLL2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="U16"/>
<connect gate="F" pin="GND_11" pad="V14"/>
<connect gate="F" pin="GND_12" pad="V15"/>
<connect gate="F" pin="GND_13" pad="P13"/>
<connect gate="F" pin="GND_14" pad="P11"/>
<connect gate="F" pin="GND_15" pad="P15"/>
<connect gate="F" pin="GND_16" pad="P17"/>
<connect gate="F" pin="GND_17" pad="P28"/>
<connect gate="F" pin="GND_18" pad="R28"/>
<connect gate="F" pin="GND_19" pad="R11"/>
<connect gate="F" pin="GND_2" pad="T13"/>
<connect gate="F" pin="GND_20" pad="T11"/>
<connect gate="F" pin="GND_21" pad="R16"/>
<connect gate="F" pin="GND_22" pad="R18"/>
<connect gate="F" pin="GND_23" pad="R14"/>
<connect gate="F" pin="GND_24" pad="P18"/>
<connect gate="F" pin="GND_3" pad="U12"/>
<connect gate="F" pin="GND_4" pad="U18"/>
<connect gate="F" pin="GND_5" pad="T15"/>
<connect gate="F" pin="GND_6" pad="T17"/>
<connect gate="F" pin="GND_7" pad="U14"/>
<connect gate="F" pin="GND_8" pad="V17"/>
<connect gate="F" pin="GND_9" pad="V13"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="T19"/>
<connect gate="F" pin="IO_11" pad="T20"/>
<connect gate="F" pin="IO_12" pad="T21"/>
<connect gate="F" pin="IO_13" pad="T22"/>
<connect gate="F" pin="IO_14" pad="T23"/>
<connect gate="F" pin="IO_15" pad="T24"/>
<connect gate="F" pin="IO_16" pad="T25"/>
<connect gate="F" pin="IO_17" pad="T26"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U10"/>
<connect gate="F" pin="IO_2" pad="N23"/>
<connect gate="F" pin="IO_20" pad="U19"/>
<connect gate="F" pin="IO_21" pad="U20"/>
<connect gate="F" pin="IO_22" pad="U21"/>
<connect gate="F" pin="IO_23" pad="U22"/>
<connect gate="F" pin="IO_24" pad="U23"/>
<connect gate="F" pin="IO_25" pad="U24"/>
<connect gate="F" pin="IO_26" pad="U25"/>
<connect gate="F" pin="IO_27" pad="U26"/>
<connect gate="F" pin="IO_28" pad="U27"/>
<connect gate="F" pin="IO_29" pad="V10"/>
<connect gate="F" pin="IO_3" pad="N24"/>
<connect gate="F" pin="IO_30" pad="V11"/>
<connect gate="F" pin="IO_31" pad="V18"/>
<connect gate="F" pin="IO_32" pad="V19"/>
<connect gate="F" pin="IO_33" pad="V20"/>
<connect gate="F" pin="IO_34" pad="V21"/>
<connect gate="F" pin="IO_35" pad="V22"/>
<connect gate="F" pin="IO_36" pad="V23"/>
<connect gate="F" pin="IO_37" pad="V24"/>
<connect gate="F" pin="IO_4" pad="N25"/>
<connect gate="F" pin="IO_5" pad="N26"/>
<connect gate="F" pin="IO_6" pad="N28"/>
<connect gate="F" pin="IO_7" pad="P26"/>
<connect gate="F" pin="IO_8" pad="R26"/>
<connect gate="F" pin="IO_9" pad="T10"/>
<connect gate="F" pin="VCCA_PLL1" pad="P23"/>
<connect gate="F" pin="VCCA_PLL2" pad="R23"/>
<connect gate="F" pin="VCCG_PLL1" pad="P21"/>
<connect gate="F" pin="VCCG_PLL2" pad="R21"/>
<connect gate="F" pin="VCCINT" pad="P16"/>
<connect gate="F" pin="VCCINT_10" pad="V12"/>
<connect gate="F" pin="VCCINT_11" pad="R13"/>
<connect gate="F" pin="VCCINT_12" pad="V16"/>
<connect gate="F" pin="VCCINT_13" pad="P12"/>
<connect gate="F" pin="VCCINT_14" pad="U17"/>
<connect gate="F" pin="VCCINT_15" pad="R17"/>
<connect gate="F" pin="VCCINT_16" pad="U11"/>
<connect gate="F" pin="VCCINT_2" pad="T12"/>
<connect gate="F" pin="VCCINT_3" pad="T14"/>
<connect gate="F" pin="VCCINT_4" pad="T18"/>
<connect gate="F" pin="VCCINT_5" pad="U13"/>
<connect gate="F" pin="VCCINT_6" pad="T16"/>
<connect gate="F" pin="VCCINT_7" pad="R15"/>
<connect gate="F" pin="VCCINT_8" pad="U15"/>
<connect gate="F" pin="VCCINT_9" pad="P14"/>
<connect gate="F" pin="VCCIO1" pad="U28"/>
<connect gate="F" pin="VCCIO1_2" pad="R20"/>
<connect gate="F" pin="VCCIO2" pad="P20"/>
<connect gate="F" pin="VREF0B1" pad="R19"/>
<connect gate="F" pin="VREF0B5" pad="P10"/>
<connect gate="F" pin="VREF2B2" pad="P19"/>
<connect gate="F" pin="VREF2B6" pad="R10"/>
<connect gate="G" pin="CLK4P" pad="AC17"/>
<connect gate="G" pin="CLK5P" pad="AA17"/>
<connect gate="G" pin="CLK7P" pad="W13"/>
<connect gate="G" pin="GND" pad="AC15"/>
<connect gate="G" pin="GNDG_PLL6" pad="AB14"/>
<connect gate="G" pin="GND_2" pad="AA16"/>
<connect gate="G" pin="IO" pad="AC28"/>
<connect gate="G" pin="IO_10" pad="W16"/>
<connect gate="G" pin="IO_11" pad="W18"/>
<connect gate="G" pin="IO_12" pad="W19"/>
<connect gate="G" pin="IO_13" pad="W21"/>
<connect gate="G" pin="IO_14" pad="W22"/>
<connect gate="G" pin="IO_15" pad="W23"/>
<connect gate="G" pin="IO_16" pad="W24"/>
<connect gate="G" pin="IO_17" pad="W25"/>
<connect gate="G" pin="IO_18" pad="W26"/>
<connect gate="G" pin="IO_19" pad="W27"/>
<connect gate="G" pin="IO_2" pad="V26"/>
<connect gate="G" pin="IO_20" pad="W28"/>
<connect gate="G" pin="IO_21" pad="Y10"/>
<connect gate="G" pin="IO_22" pad="Y11"/>
<connect gate="G" pin="IO_23" pad="Y13"/>
<connect gate="G" pin="IO_24" pad="Y16"/>
<connect gate="G" pin="IO_25" pad="Y17"/>
<connect gate="G" pin="IO_26" pad="Y18"/>
<connect gate="G" pin="IO_27" pad="Y19"/>
<connect gate="G" pin="IO_28" pad="Y20"/>
<connect gate="G" pin="IO_29" pad="Y21"/>
<connect gate="G" pin="IO_3" pad="V27"/>
<connect gate="G" pin="IO_30" pad="Y22"/>
<connect gate="G" pin="IO_31" pad="Y23"/>
<connect gate="G" pin="IO_32" pad="Y24"/>
<connect gate="G" pin="IO_33" pad="Y25"/>
<connect gate="G" pin="IO_34" pad="Y26"/>
<connect gate="G" pin="IO_35" pad="Y27"/>
<connect gate="G" pin="IO_36" pad="Y28"/>
<connect gate="G" pin="IO_37" pad="AA10"/>
<connect gate="G" pin="IO_38" pad="AA11"/>
<connect gate="G" pin="IO_39" pad="AA14"/>
<connect gate="G" pin="IO_4" pad="V28"/>
<connect gate="G" pin="IO_40" pad="AA15"/>
<connect gate="G" pin="IO_41" pad="AA18"/>
<connect gate="G" pin="IO_42" pad="AA19"/>
<connect gate="G" pin="IO_43" pad="AA20"/>
<connect gate="G" pin="IO_44" pad="AA21"/>
<connect gate="G" pin="IO_45" pad="AA22"/>
<connect gate="G" pin="IO_46" pad="AA23"/>
<connect gate="G" pin="IO_47" pad="AA24"/>
<connect gate="G" pin="IO_48" pad="AA25"/>
<connect gate="G" pin="IO_49" pad="AA26"/>
<connect gate="G" pin="IO_5" pad="W10"/>
<connect gate="G" pin="IO_50" pad="AA27"/>
<connect gate="G" pin="IO_51" pad="AA28"/>
<connect gate="G" pin="IO_52" pad="AB10"/>
<connect gate="G" pin="IO_53" pad="AB11"/>
<connect gate="G" pin="IO_54" pad="AB12"/>
<connect gate="G" pin="IO_55" pad="AB17"/>
<connect gate="G" pin="IO_56" pad="AB18"/>
<connect gate="G" pin="IO_57" pad="AB19"/>
<connect gate="G" pin="IO_58" pad="AB20"/>
<connect gate="G" pin="IO_59" pad="AB21"/>
<connect gate="G" pin="IO_6" pad="W11"/>
<connect gate="G" pin="IO_60" pad="AB22"/>
<connect gate="G" pin="IO_61" pad="AB23"/>
<connect gate="G" pin="IO_62" pad="AB24"/>
<connect gate="G" pin="IO_63" pad="AB25"/>
<connect gate="G" pin="IO_64" pad="AB26"/>
<connect gate="G" pin="IO_65" pad="AB27"/>
<connect gate="G" pin="IO_66" pad="AB28"/>
<connect gate="G" pin="IO_67" pad="AC10"/>
<connect gate="G" pin="IO_68" pad="AC11"/>
<connect gate="G" pin="IO_69" pad="AC19"/>
<connect gate="G" pin="IO_7" pad="W12"/>
<connect gate="G" pin="IO_70" pad="AC20"/>
<connect gate="G" pin="IO_71" pad="AC21"/>
<connect gate="G" pin="IO_72" pad="AC22"/>
<connect gate="G" pin="IO_73" pad="AC23"/>
<connect gate="G" pin="IO_74" pad="AC24"/>
<connect gate="G" pin="IO_75" pad="AC27"/>
<connect gate="G" pin="IO_8" pad="W14"/>
<connect gate="G" pin="IO_9" pad="W15"/>
<connect gate="G" pin="MSEL0" pad="AC16"/>
<connect gate="G" pin="MSEL1" pad="W17"/>
<connect gate="G" pin="MSEL2" pad="AB15"/>
<connect gate="G" pin="NC" pad="AC26"/>
<connect gate="G" pin="NCE" pad="AB13"/>
<connect gate="G" pin="NCEO" pad="AC13"/>
<connect gate="G" pin="NC_2" pad="AC25"/>
<connect gate="G" pin="NO_PULLUP" pad="Y12"/>
<connect gate="G" pin="PLL_ENA" pad="AC18"/>
<connect gate="G" pin="PORSEL" pad="AC12"/>
<connect gate="G" pin="VCCG_PLL6" pad="AA13"/>
<connect gate="G" pin="VCCIO7" pad="Y14"/>
<connect gate="G" pin="VCCIO8" pad="Y15"/>
<connect gate="G" pin="VCCSEL" pad="AA12"/>
<connect gate="G" pin="VCC_PLL6_OUTA" pad="AC14"/>
<connect gate="G" pin="VCC_PLL6_OUTB" pad="AB16"/>
<connect gate="G" pin="VREF1B1" pad="W20"/>
<connect gate="H" pin="CLK6P" pad="AD14"/>
<connect gate="H" pin="GND" pad="AG27"/>
<connect gate="H" pin="GNDA_PLL6" pad="AF14"/>
<connect gate="H" pin="GND_2" pad="AH14"/>
<connect gate="H" pin="GND_3" pad="AF26"/>
<connect gate="H" pin="GND_4" pad="AH15"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD21"/>
<connect gate="H" pin="IO_11" pad="AD23"/>
<connect gate="H" pin="IO_12" pad="AD24"/>
<connect gate="H" pin="IO_13" pad="AD27"/>
<connect gate="H" pin="IO_14" pad="AD28"/>
<connect gate="H" pin="IO_15" pad="AE10"/>
<connect gate="H" pin="IO_16" pad="AE11"/>
<connect gate="H" pin="IO_17" pad="AE12"/>
<connect gate="H" pin="IO_18" pad="AE13"/>
<connect gate="H" pin="IO_19" pad="AE14"/>
<connect gate="H" pin="IO_2" pad="AD10"/>
<connect gate="H" pin="IO_20" pad="AE15"/>
<connect gate="H" pin="IO_21" pad="AE16"/>
<connect gate="H" pin="IO_22" pad="AE17"/>
<connect gate="H" pin="IO_23" pad="AE18"/>
<connect gate="H" pin="IO_24" pad="AE19"/>
<connect gate="H" pin="IO_25" pad="AE20"/>
<connect gate="H" pin="IO_26" pad="AE21"/>
<connect gate="H" pin="IO_27" pad="AE22"/>
<connect gate="H" pin="IO_28" pad="AE23"/>
<connect gate="H" pin="IO_29" pad="AE24"/>
<connect gate="H" pin="IO_3" pad="AD12"/>
<connect gate="H" pin="IO_30" pad="AE25"/>
<connect gate="H" pin="IO_31" pad="AE27"/>
<connect gate="H" pin="IO_32" pad="AE28"/>
<connect gate="H" pin="IO_33" pad="AF10"/>
<connect gate="H" pin="IO_34" pad="AF11"/>
<connect gate="H" pin="IO_35" pad="AF12"/>
<connect gate="H" pin="IO_36" pad="AF13"/>
<connect gate="H" pin="IO_37" pad="AF15"/>
<connect gate="H" pin="IO_38" pad="AF16"/>
<connect gate="H" pin="IO_39" pad="AF17"/>
<connect gate="H" pin="IO_4" pad="AD13"/>
<connect gate="H" pin="IO_40" pad="AF18"/>
<connect gate="H" pin="IO_41" pad="AF19"/>
<connect gate="H" pin="IO_42" pad="AF20"/>
<connect gate="H" pin="IO_43" pad="AF21"/>
<connect gate="H" pin="IO_44" pad="AF22"/>
<connect gate="H" pin="IO_45" pad="AF23"/>
<connect gate="H" pin="IO_46" pad="AF24"/>
<connect gate="H" pin="IO_47" pad="AF25"/>
<connect gate="H" pin="IO_48" pad="AF27"/>
<connect gate="H" pin="IO_49" pad="AF28"/>
<connect gate="H" pin="IO_5" pad="AD15"/>
<connect gate="H" pin="IO_50" pad="AG10"/>
<connect gate="H" pin="IO_51" pad="AG11"/>
<connect gate="H" pin="IO_52" pad="AG12"/>
<connect gate="H" pin="IO_53" pad="AG13"/>
<connect gate="H" pin="IO_54" pad="AG15"/>
<connect gate="H" pin="IO_55" pad="AG16"/>
<connect gate="H" pin="IO_56" pad="AG17"/>
<connect gate="H" pin="IO_57" pad="AG18"/>
<connect gate="H" pin="IO_58" pad="AG19"/>
<connect gate="H" pin="IO_59" pad="AG20"/>
<connect gate="H" pin="IO_6" pad="AD16"/>
<connect gate="H" pin="IO_60" pad="AG21"/>
<connect gate="H" pin="IO_61" pad="AG22"/>
<connect gate="H" pin="IO_62" pad="AG23"/>
<connect gate="H" pin="IO_63" pad="AG24"/>
<connect gate="H" pin="IO_64" pad="AG25"/>
<connect gate="H" pin="IO_65" pad="AG26"/>
<connect gate="H" pin="IO_66" pad="AH10"/>
<connect gate="H" pin="IO_67" pad="AH11"/>
<connect gate="H" pin="IO_68" pad="AH13"/>
<connect gate="H" pin="IO_69" pad="AH16"/>
<connect gate="H" pin="IO_7" pad="AD17"/>
<connect gate="H" pin="IO_70" pad="AH19"/>
<connect gate="H" pin="IO_71" pad="AH20"/>
<connect gate="H" pin="IO_72" pad="AH21"/>
<connect gate="H" pin="IO_73" pad="AH22"/>
<connect gate="H" pin="IO_74" pad="AH23"/>
<connect gate="H" pin="IO_75" pad="AH24"/>
<connect gate="H" pin="IO_76" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD18"/>
<connect gate="H" pin="IO_9" pad="AD19"/>
<connect gate="H" pin="NC" pad="AD26"/>
<connect gate="H" pin="NC_2" pad="AD25"/>
<connect gate="H" pin="VCCA_PLL6" pad="AG14"/>
<connect gate="H" pin="VCCIO1" pad="AG28"/>
<connect gate="H" pin="VCCIO7" pad="AH12"/>
<connect gate="H" pin="VCCIO8" pad="AH27"/>
<connect gate="H" pin="VCCIO8_2" pad="AH17"/>
<connect gate="H" pin="VREF0B7" pad="AD11"/>
<connect gate="H" pin="VREF0B8" pad="AD22"/>
<connect gate="H" pin="VREF1B8" pad="AD20"/>
<connect gate="H" pin="VREF2B1" pad="AE26"/>
<connect gate="H" pin="VREF2B8" pad="AH18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1S30F780C7N"/>
<attribute name="OC_FARNELL" value="1549497"/>
<attribute name="OC_NEWARK" value="52R0350"/>
<attribute name="PACKAGE" value="780-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1SGX10CF672C6N">
<description>StratixGX FPGA Family</description>
<gates>
<gate name="A" symbol="EP1SGX10CF672C6N_A"/>
<gate name="B" symbol="EP1SGX10CF672C6N_B"/>
<gate name="C" symbol="EP1SGX10CF672C6N_C"/>
<gate name="D" symbol="EP1SGX10CF672C6N_D"/>
<gate name="E" symbol="EP1SGX10CF672C6N_E"/>
<gate name="F" symbol="EP1SGX10CF672C6N_F"/>
<gate name="G" symbol="EP1SGX10CF672C6N_G"/>
</gates>
<devices>
<device name="" package="BGA672C26X26X100P_2700X2700X35">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GND/NC" pad="G2"/>
<connect gate="A" pin="GND/NC_10" pad="G4"/>
<connect gate="A" pin="GND/NC_11" pad="L4"/>
<connect gate="A" pin="GND/NC_12" pad="E2"/>
<connect gate="A" pin="GND/NC_13" pad="L5"/>
<connect gate="A" pin="GND/NC_14" pad="G5"/>
<connect gate="A" pin="GND/NC_2" pad="E1"/>
<connect gate="A" pin="GND/NC_3" pad="J1"/>
<connect gate="A" pin="GND/NC_4" pad="G1"/>
<connect gate="A" pin="GND/NC_5" pad="J4"/>
<connect gate="A" pin="GND/NC_6" pad="L1"/>
<connect gate="A" pin="GND/NC_7" pad="J2"/>
<connect gate="A" pin="GND/NC_8" pad="L2"/>
<connect gate="A" pin="GND/NC_9" pad="J5"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_3" pad="G6"/>
<connect gate="A" pin="GND_4" pad="D3"/>
<connect gate="A" pin="GND_5" pad="J6"/>
<connect gate="A" pin="GXB_GND" pad="H5"/>
<connect gate="A" pin="GXB_GND_10" pad="G3"/>
<connect gate="A" pin="GXB_GND_11" pad="K1"/>
<connect gate="A" pin="GXB_GND_12" pad="F5"/>
<connect gate="A" pin="GXB_GND_13" pad="K2"/>
<connect gate="A" pin="GXB_GND_14" pad="H1"/>
<connect gate="A" pin="GXB_GND_15" pad="K3"/>
<connect gate="A" pin="GXB_GND_16" pad="H2"/>
<connect gate="A" pin="GXB_GND_17" pad="K4"/>
<connect gate="A" pin="GXB_GND_18" pad="H3"/>
<connect gate="A" pin="GXB_GND_19" pad="L3"/>
<connect gate="A" pin="GXB_GND_2" pad="D1"/>
<connect gate="A" pin="GXB_GND_20" pad="K5"/>
<connect gate="A" pin="GXB_GND_21" pad="H4"/>
<connect gate="A" pin="GXB_GND_3" pad="E3"/>
<connect gate="A" pin="GXB_GND_4" pad="D2"/>
<connect gate="A" pin="GXB_GND_5" pad="J3"/>
<connect gate="A" pin="GXB_GND_6" pad="F1"/>
<connect gate="A" pin="GXB_GND_7" pad="F2"/>
<connect gate="A" pin="GXB_GND_8" pad="F3"/>
<connect gate="A" pin="GXB_GND_9" pad="F4"/>
<connect gate="A" pin="IO_4" pad="H8"/>
<connect gate="A" pin="IO_4_2" pad="G9"/>
<connect gate="A" pin="IO_4_3" pad="J9"/>
<connect gate="A" pin="IO_4_4" pad="F8"/>
<connect gate="A" pin="IO_4_5" pad="K8"/>
<connect gate="A" pin="IO_4_6" pad="H7"/>
<connect gate="A" pin="IO_4_DEV_OE" pad="J7"/>
<connect gate="A" pin="IO_4_DQ0T0" pad="B2"/>
<connect gate="A" pin="IO_4_DQ0T1" pad="C2"/>
<connect gate="A" pin="IO_4_DQ0T2" pad="C1"/>
<connect gate="A" pin="IO_4_DQ0T3" pad="B3"/>
<connect gate="A" pin="IO_4_DQ0T4" pad="D4"/>
<connect gate="A" pin="IO_4_DQ0T5" pad="E4"/>
<connect gate="A" pin="IO_4_DQ0T6" pad="B4"/>
<connect gate="A" pin="IO_4_DQ0T7" pad="C4"/>
<connect gate="A" pin="IO_4_DQ1T0" pad="E5"/>
<connect gate="A" pin="IO_4_DQ1T1" pad="C6"/>
<connect gate="A" pin="IO_4_DQ1T2" pad="B5"/>
<connect gate="A" pin="IO_4_DQ1T3" pad="D5"/>
<connect gate="A" pin="IO_4_DQ1T4" pad="A5"/>
<connect gate="A" pin="IO_4_DQ1T5" pad="A4"/>
<connect gate="A" pin="IO_4_DQ1T6" pad="E6"/>
<connect gate="A" pin="IO_4_DQ1T7" pad="D6"/>
<connect gate="A" pin="IO_4_DQ2T0" pad="B6"/>
<connect gate="A" pin="IO_4_DQ2T1" pad="E8"/>
<connect gate="A" pin="IO_4_DQ2T2" pad="F7"/>
<connect gate="A" pin="IO_4_DQ2T3" pad="A6"/>
<connect gate="A" pin="IO_4_DQ2T4" pad="B7"/>
<connect gate="A" pin="IO_4_DQ2T5" pad="D7"/>
<connect gate="A" pin="IO_4_DQ2T6" pad="E7"/>
<connect gate="A" pin="IO_4_DQ2T7" pad="A7"/>
<connect gate="A" pin="IO_4_DQ3T0" pad="D8"/>
<connect gate="A" pin="IO_4_DQ3T1" pad="A8"/>
<connect gate="A" pin="IO_4_DQ3T2" pad="C9"/>
<connect gate="A" pin="IO_4_DQ3T3" pad="C8"/>
<connect gate="A" pin="IO_4_DQ3T5" pad="A9"/>
<connect gate="A" pin="IO_4_DQ3T6" pad="B9"/>
<connect gate="A" pin="IO_4_DQ3T7" pad="D9"/>
<connect gate="A" pin="IO_4_DQS0T" pad="C3"/>
<connect gate="A" pin="IO_4_DQS1T" pad="C5"/>
<connect gate="A" pin="IO_4_DQS2T" pad="C7"/>
<connect gate="A" pin="IO_4_DQS3T" pad="B8"/>
<connect gate="A" pin="IO_4_FCLK7" pad="G7"/>
<connect gate="A" pin="IO_4_RDN4" pad="G8"/>
<connect gate="A" pin="NC" pad="E9"/>
<connect gate="A" pin="RREFB15A" pad="K7"/>
<connect gate="A" pin="TCK" pad="J8"/>
<connect gate="A" pin="TMS" pad="F9"/>
<connect gate="A" pin="TRST" pad="H9"/>
<connect gate="A" pin="VCCINT" pad="H6"/>
<connect gate="A" pin="VCCINT_2" pad="K6"/>
<connect gate="A" pin="VCCINT_3" pad="F6"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCR_B15" pad="L7"/>
<connect gate="A" pin="VCCT_B15" pad="L6"/>
<connect gate="A" pin="VREF0B4" pad="K9"/>
<connect gate="B" pin="GND" pad="A11"/>
<connect gate="B" pin="GND/NC" pad="N5"/>
<connect gate="B" pin="GND/NC_2" pad="N1"/>
<connect gate="B" pin="GND/NC_3" pad="N2"/>
<connect gate="B" pin="GND/NC_4" pad="N4"/>
<connect gate="B" pin="GND_2" pad="P6"/>
<connect gate="B" pin="GND_3" pad="N6"/>
<connect gate="B" pin="GND_4" pad="W6"/>
<connect gate="B" pin="GND_5" pad="U6"/>
<connect gate="B" pin="GND_6" pad="A16"/>
<connect gate="B" pin="GXB_GND" pad="Y5"/>
<connect gate="B" pin="GXB_GND_10" pad="T3"/>
<connect gate="B" pin="GXB_GND_11" pad="V1"/>
<connect gate="B" pin="GXB_GND_12" pad="T4"/>
<connect gate="B" pin="GXB_GND_13" pad="P1"/>
<connect gate="B" pin="GXB_GND_14" pad="V2"/>
<connect gate="B" pin="GXB_GND_15" pad="P2"/>
<connect gate="B" pin="GXB_GND_16" pad="T5"/>
<connect gate="B" pin="GXB_GND_17" pad="P3"/>
<connect gate="B" pin="GXB_GND_18" pad="U3"/>
<connect gate="B" pin="GXB_GND_19" pad="P4"/>
<connect gate="B" pin="GXB_GND_2" pad="M1"/>
<connect gate="B" pin="GXB_GND_20" pad="W3"/>
<connect gate="B" pin="GXB_GND_21" pad="M5"/>
<connect gate="B" pin="GXB_GND_22" pad="P5"/>
<connect gate="B" pin="GXB_GND_23" pad="V3"/>
<connect gate="B" pin="GXB_GND_24" pad="V4"/>
<connect gate="B" pin="GXB_GND_25" pad="Y1"/>
<connect gate="B" pin="GXB_GND_26" pad="V5"/>
<connect gate="B" pin="GXB_GND_27" pad="Y2"/>
<connect gate="B" pin="GXB_GND_28" pad="Y3"/>
<connect gate="B" pin="GXB_GND_29" pad="Y4"/>
<connect gate="B" pin="GXB_GND_3" pad="M2"/>
<connect gate="B" pin="GXB_GND_4" pad="M3"/>
<connect gate="B" pin="GXB_GND_5" pad="N3"/>
<connect gate="B" pin="GXB_GND_6" pad="T1"/>
<connect gate="B" pin="GXB_GND_7" pad="M4"/>
<connect gate="B" pin="GXB_GND_8" pad="R3"/>
<connect gate="B" pin="GXB_GND_9" pad="T2"/>
<connect gate="B" pin="GXB_RX8N" pad="U2"/>
<connect gate="B" pin="GXB_RX8P" pad="U1"/>
<connect gate="B" pin="GXB_RX9N" pad="R2"/>
<connect gate="B" pin="GXB_RX9P" pad="R1"/>
<connect gate="B" pin="GXB_TX10N" pad="W5"/>
<connect gate="B" pin="GXB_TX10P" pad="W4"/>
<connect gate="B" pin="GXB_TX8N" pad="U5"/>
<connect gate="B" pin="GXB_TX8P" pad="U4"/>
<connect gate="B" pin="GXB_TX9N" pad="R5"/>
<connect gate="B" pin="GXB_TX9P" pad="R4"/>
<connect gate="B" pin="IO_10_PLL5_OUT3N" pad="A13"/>
<connect gate="B" pin="IO_3_CLK14N" pad="A14"/>
<connect gate="B" pin="IO_3_DQ7T2" pad="A17"/>
<connect gate="B" pin="IO_3_DQ8T2" pad="A18"/>
<connect gate="B" pin="IO_3_DQ8T4" pad="A20"/>
<connect gate="B" pin="IO_3_DQ8T5" pad="A19"/>
<connect gate="B" pin="IO_3_DQ9T0" pad="A21"/>
<connect gate="B" pin="IO_3_DQ9T4" pad="A22"/>
<connect gate="B" pin="IO_4_DQ3T4" pad="A10"/>
<connect gate="B" pin="IO_7" pad="V7"/>
<connect gate="B" pin="IO_7_2" pad="U8"/>
<connect gate="B" pin="IO_7_3" pad="W7"/>
<connect gate="B" pin="IO_7_4" pad="U9"/>
<connect gate="B" pin="IO_7_5" pad="W8"/>
<connect gate="B" pin="IO_7_DQ2B2" pad="Y8"/>
<connect gate="B" pin="IO_7_DQ2B6" pad="Y7"/>
<connect gate="B" pin="IO_7_FCLK4" pad="Y9"/>
<connect gate="B" pin="IO_7_FCLK5" pad="W9"/>
<connect gate="B" pin="IO_7_RDN7" pad="V8"/>
<connect gate="B" pin="NC" pad="V9"/>
<connect gate="B" pin="NCE" pad="P9"/>
<connect gate="B" pin="NCEO" pad="T9"/>
<connect gate="B" pin="REFCLKB15N" pad="W2"/>
<connect gate="B" pin="REFCLKB15P" pad="W1"/>
<connect gate="B" pin="RREFB15" pad="U7"/>
<connect gate="B" pin="VCCA_B15" pad="N7"/>
<connect gate="B" pin="VCCA_B15_2" pad="P8"/>
<connect gate="B" pin="VCCG_B15" pad="N8"/>
<connect gate="B" pin="VCCG_B15_2" pad="P7"/>
<connect gate="B" pin="VCCINT" pad="M9"/>
<connect gate="B" pin="VCCINT_2" pad="N9"/>
<connect gate="B" pin="VCCINT_3" pad="V6"/>
<connect gate="B" pin="VCCINT_4" pad="L9"/>
<connect gate="B" pin="VCCINT_5" pad="Y6"/>
<connect gate="B" pin="VCCIO3" pad="A15"/>
<connect gate="B" pin="VCCIO4" pad="A12"/>
<connect gate="B" pin="VCCP_B15" pad="T8"/>
<connect gate="B" pin="VCCP_B15_2" pad="L8"/>
<connect gate="B" pin="VCCP_B15_3" pad="M8"/>
<connect gate="B" pin="VCCP_B15_4" pad="R8"/>
<connect gate="B" pin="VCCR_B15" pad="T7"/>
<connect gate="B" pin="VCCR_B15_2" pad="M7"/>
<connect gate="B" pin="VCCR_B15_3" pad="R7"/>
<connect gate="B" pin="VCCSEL" pad="R9"/>
<connect gate="B" pin="VCCT_B15" pad="T6"/>
<connect gate="B" pin="VCCT_B15_2" pad="M6"/>
<connect gate="B" pin="VCCT_B15_3" pad="R6"/>
<connect gate="C" pin="CLK14P" pad="B14"/>
<connect gate="C" pin="CLK15P" pad="D14"/>
<connect gate="C" pin="GND" pad="AF2"/>
<connect gate="C" pin="GND_2" pad="A25"/>
<connect gate="C" pin="GND_3" pad="AC3"/>
<connect gate="C" pin="GND_4" pad="AD3"/>
<connect gate="C" pin="GND_5" pad="AA6"/>
<connect gate="C" pin="GND_6" pad="B26"/>
<connect gate="C" pin="GND_7" pad="AE1"/>
<connect gate="C" pin="GXB_GND" pad="AA3"/>
<connect gate="C" pin="GXB_GND_2" pad="AD1"/>
<connect gate="C" pin="GXB_GND_3" pad="AD2"/>
<connect gate="C" pin="GXB_GND_4" pad="AB1"/>
<connect gate="C" pin="GXB_GND_5" pad="AB2"/>
<connect gate="C" pin="GXB_GND_6" pad="AB3"/>
<connect gate="C" pin="GXB_GND_7" pad="AB4"/>
<connect gate="C" pin="GXB_GND_8" pad="AB5"/>
<connect gate="C" pin="GXB_RX10N" pad="AA2"/>
<connect gate="C" pin="GXB_RX10P" pad="AA1"/>
<connect gate="C" pin="GXB_RX11N" pad="AC2"/>
<connect gate="C" pin="GXB_RX11P" pad="AC1"/>
<connect gate="C" pin="GXB_TX11N" pad="AA5"/>
<connect gate="C" pin="GXB_TX11P" pad="AA4"/>
<connect gate="C" pin="IO_10_PLL5_OUT3P" pad="B13"/>
<connect gate="C" pin="IO_3_CLK15N" pad="C14"/>
<connect gate="C" pin="IO_3_DQ6T1" pad="B15"/>
<connect gate="C" pin="IO_3_DQ6T3" pad="C16"/>
<connect gate="C" pin="IO_3_DQ6T6" pad="C15"/>
<connect gate="C" pin="IO_3_DQ6T7" pad="B16"/>
<connect gate="C" pin="IO_3_DQ7T1" pad="B17"/>
<connect gate="C" pin="IO_3_DQ7T4" pad="C18"/>
<connect gate="C" pin="IO_3_DQ7T5" pad="B18"/>
<connect gate="C" pin="IO_3_DQ8T0" pad="C19"/>
<connect gate="C" pin="IO_3_DQ8T3" pad="B20"/>
<connect gate="C" pin="IO_3_DQ8T6" pad="C20"/>
<connect gate="C" pin="IO_3_DQ9T1" pad="B21"/>
<connect gate="C" pin="IO_3_DQ9T2" pad="C21"/>
<connect gate="C" pin="IO_3_DQ9T3" pad="C22"/>
<connect gate="C" pin="IO_3_DQ9T5" pad="B23"/>
<connect gate="C" pin="IO_3_DQ9T6" pad="A23"/>
<connect gate="C" pin="IO_3_DQ9T7" pad="B24"/>
<connect gate="C" pin="IO_3_DQS6T" pad="D15"/>
<connect gate="C" pin="IO_3_DQS7T" pad="C17"/>
<connect gate="C" pin="IO_3_DQS8T" pad="B19"/>
<connect gate="C" pin="IO_3_DQS9T" pad="B22"/>
<connect gate="C" pin="IO_4_CLK12N" pad="D12"/>
<connect gate="C" pin="IO_7_DQ0B0" pad="AC5"/>
<connect gate="C" pin="IO_7_DQ0B1" pad="AE3"/>
<connect gate="C" pin="IO_7_DQ0B2" pad="AE2"/>
<connect gate="C" pin="IO_7_DQ0B3" pad="AD5"/>
<connect gate="C" pin="IO_7_DQ0B4" pad="AD4"/>
<connect gate="C" pin="IO_7_DQ0B5" pad="AC4"/>
<connect gate="C" pin="IO_7_DQ0B6" pad="AE5"/>
<connect gate="C" pin="IO_7_DQ0B7" pad="AF4"/>
<connect gate="C" pin="IO_7_DQ1B0" pad="AC6"/>
<connect gate="C" pin="IO_7_DQ1B1" pad="AC7"/>
<connect gate="C" pin="IO_7_DQ1B2" pad="AF6"/>
<connect gate="C" pin="IO_7_DQ1B3" pad="AD6"/>
<connect gate="C" pin="IO_7_DQ1B4" pad="AE7"/>
<connect gate="C" pin="IO_7_DQ1B5" pad="AF7"/>
<connect gate="C" pin="IO_7_DQ1B6" pad="AD7"/>
<connect gate="C" pin="IO_7_DQ1B7" pad="AF5"/>
<connect gate="C" pin="IO_7_DQ2B0" pad="AB8"/>
<connect gate="C" pin="IO_7_DQ2B1" pad="AA8"/>
<connect gate="C" pin="IO_7_DQ2B3" pad="AB9"/>
<connect gate="C" pin="IO_7_DQ2B4" pad="AC8"/>
<connect gate="C" pin="IO_7_DQ2B5" pad="AA7"/>
<connect gate="C" pin="IO_7_DQ2B7" pad="AC9"/>
<connect gate="C" pin="IO_7_DQ3B0" pad="AD8"/>
<connect gate="C" pin="IO_7_DQ3B1" pad="AD9"/>
<connect gate="C" pin="IO_7_DQ3B2" pad="AF9"/>
<connect gate="C" pin="IO_7_DQ3B3" pad="AE8"/>
<connect gate="C" pin="IO_7_DQ3B7" pad="AF8"/>
<connect gate="C" pin="IO_7_DQS0B" pad="AE4"/>
<connect gate="C" pin="IO_7_DQS1B" pad="AE6"/>
<connect gate="C" pin="IO_7_DQS2B" pad="AB7"/>
<connect gate="C" pin="IO_7_DQS3B" pad="AE9"/>
<connect gate="C" pin="IO_9_PLL5_OUT0N" pad="C13"/>
<connect gate="C" pin="IO_9_PLL5_OUT0P" pad="D13"/>
<connect gate="C" pin="IO_9_PLL5_OUT1N" pad="B12"/>
<connect gate="C" pin="IO_9_PLL5_OUT1P" pad="C12"/>
<connect gate="C" pin="NC" pad="C25"/>
<connect gate="C" pin="NC_10" pad="C24"/>
<connect gate="C" pin="NC_11" pad="B25"/>
<connect gate="C" pin="NC_2" pad="C10"/>
<connect gate="C" pin="NC_3" pad="D10"/>
<connect gate="C" pin="NC_4" pad="AA9"/>
<connect gate="C" pin="NC_5" pad="B10"/>
<connect gate="C" pin="NC_6" pad="C11"/>
<connect gate="C" pin="NC_7" pad="B11"/>
<connect gate="C" pin="NC_8" pad="D11"/>
<connect gate="C" pin="NC_9" pad="C23"/>
<connect gate="C" pin="VCCINT" pad="AB6"/>
<connect gate="C" pin="VCCIO2" pad="C26"/>
<connect gate="C" pin="VCCIO3" pad="A24"/>
<connect gate="C" pin="VCCIO7" pad="AF3"/>
<connect gate="D" pin="CLK12P" pad="E12"/>
<connect gate="D" pin="CLK13P" pad="G12"/>
<connect gate="D" pin="GND" pad="H17"/>
<connect gate="D" pin="GNDA_PLL5" pad="G13"/>
<connect gate="D" pin="GNDG_PLL5" pad="J12"/>
<connect gate="D" pin="INPUT" pad="H26"/>
<connect gate="D" pin="INPUT_10" pad="H23"/>
<connect gate="D" pin="INPUT_11" pad="H24"/>
<connect gate="D" pin="INPUT_12" pad="H25"/>
<connect gate="D" pin="INPUT_2" pad="F25"/>
<connect gate="D" pin="INPUT_3" pad="G25"/>
<connect gate="D" pin="INPUT_4" pad="G26"/>
<connect gate="D" pin="INPUT_5" pad="J23"/>
<connect gate="D" pin="INPUT_6" pad="F26"/>
<connect gate="D" pin="INPUT_7" pad="J24"/>
<connect gate="D" pin="INPUT_8" pad="J25"/>
<connect gate="D" pin="INPUT_9" pad="J26"/>
<connect gate="D" pin="IO_10_PLL5_OUT2N" pad="E14"/>
<connect gate="D" pin="IO_10_PLL5_OUT2P" pad="F14"/>
<connect gate="D" pin="IO_2_DIFFIO_TX18N" pad="J20"/>
<connect gate="D" pin="IO_2_DIFFIO_TX18P" pad="J19"/>
<connect gate="D" pin="IO_2_DIFFIO_TX20N" pad="J22"/>
<connect gate="D" pin="IO_2_DIFFIO_TX20P" pad="J21"/>
<connect gate="D" pin="IO_2_DIFFIO_TX21N" pad="H20"/>
<connect gate="D" pin="IO_2_DIFFIO_TX21P" pad="H19"/>
<connect gate="D" pin="IO_3" pad="G17"/>
<connect gate="D" pin="IO_3_2" pad="H16"/>
<connect gate="D" pin="IO_3_3" pad="G16"/>
<connect gate="D" pin="IO_3_4" pad="H18"/>
<connect gate="D" pin="IO_3_5" pad="F17"/>
<connect gate="D" pin="IO_3_DQ6T0" pad="E16"/>
<connect gate="D" pin="IO_3_DQ6T2" pad="E15"/>
<connect gate="D" pin="IO_3_DQ6T4" pad="D16"/>
<connect gate="D" pin="IO_3_DQ6T5" pad="F15"/>
<connect gate="D" pin="IO_3_DQ7T0" pad="E17"/>
<connect gate="D" pin="IO_3_DQ7T3" pad="D17"/>
<connect gate="D" pin="IO_3_DQ7T6" pad="D18"/>
<connect gate="D" pin="IO_3_DQ7T7" pad="E18"/>
<connect gate="D" pin="IO_3_DQ8T1" pad="D19"/>
<connect gate="D" pin="IO_3_DQ8T7" pad="D20"/>
<connect gate="D" pin="IO_3_FCLK0" pad="F18"/>
<connect gate="D" pin="IO_3_FCLK1" pad="G18"/>
<connect gate="D" pin="IO_4" pad="H11"/>
<connect gate="D" pin="IO_4_2" pad="E10"/>
<connect gate="D" pin="IO_4_3" pad="H10"/>
<connect gate="D" pin="IO_4_4" pad="E11"/>
<connect gate="D" pin="IO_4_CLK13N" pad="F12"/>
<connect gate="D" pin="IO_4_FCLK6" pad="G10"/>
<connect gate="D" pin="IO_4_RUP4" pad="G11"/>
<connect gate="D" pin="IO_9_PLL5_FBN" pad="E13"/>
<connect gate="D" pin="IO_9_PLL5_FBP" pad="F13"/>
<connect gate="D" pin="NC" pad="H22"/>
<connect gate="D" pin="NC_10" pad="F16"/>
<connect gate="D" pin="NC_11" pad="D24"/>
<connect gate="D" pin="NC_12" pad="H21"/>
<connect gate="D" pin="NC_13" pad="D21"/>
<connect gate="D" pin="NC_14" pad="H14"/>
<connect gate="D" pin="NC_15" pad="D25"/>
<connect gate="D" pin="NC_16" pad="E26"/>
<connect gate="D" pin="NC_17" pad="F19"/>
<connect gate="D" pin="NC_18" pad="J18"/>
<connect gate="D" pin="NC_19" pad="E19"/>
<connect gate="D" pin="NC_2" pad="G21"/>
<connect gate="D" pin="NC_20" pad="G15"/>
<connect gate="D" pin="NC_21" pad="D22"/>
<connect gate="D" pin="NC_22" pad="G20"/>
<connect gate="D" pin="NC_23" pad="E20"/>
<connect gate="D" pin="NC_24" pad="F20"/>
<connect gate="D" pin="NC_25" pad="F21"/>
<connect gate="D" pin="NC_26" pad="J15"/>
<connect gate="D" pin="NC_27" pad="E21"/>
<connect gate="D" pin="NC_28" pad="J14"/>
<connect gate="D" pin="NC_29" pad="D23"/>
<connect gate="D" pin="NC_3" pad="E23"/>
<connect gate="D" pin="NC_30" pad="H15"/>
<connect gate="D" pin="NC_31" pad="E22"/>
<connect gate="D" pin="NC_32" pad="F22"/>
<connect gate="D" pin="NC_33" pad="F23"/>
<connect gate="D" pin="NC_34" pad="G19"/>
<connect gate="D" pin="NC_35" pad="D26"/>
<connect gate="D" pin="NC_36" pad="F24"/>
<connect gate="D" pin="NC_4" pad="G22"/>
<connect gate="D" pin="NC_5" pad="E24"/>
<connect gate="D" pin="NC_6" pad="G23"/>
<connect gate="D" pin="NC_7" pad="E25"/>
<connect gate="D" pin="NC_8" pad="G14"/>
<connect gate="D" pin="NC_9" pad="G24"/>
<connect gate="D" pin="TDI" pad="F10"/>
<connect gate="D" pin="TDO" pad="F11"/>
<connect gate="D" pin="TEMPDIODEN" pad="J10"/>
<connect gate="D" pin="TEMPDIODEP" pad="J11"/>
<connect gate="D" pin="VCCA_PLL5" pad="H13"/>
<connect gate="D" pin="VCCG_PLL5" pad="H12"/>
<connect gate="D" pin="VCC_PLL5_OUTA" pad="J13"/>
<connect gate="D" pin="VREF0B3" pad="J16"/>
<connect gate="D" pin="VREF1B3" pad="J17"/>
<connect gate="E" pin="CLK0N" pad="N26"/>
<connect gate="E" pin="CLK0P" pad="N25"/>
<connect gate="E" pin="CLK1P" pad="N23"/>
<connect gate="E" pin="CLK2N" pad="P26"/>
<connect gate="E" pin="CLK2P" pad="P25"/>
<connect gate="E" pin="CLK3P" pad="P23"/>
<connect gate="E" pin="CONF_DONE" pad="K15"/>
<connect gate="E" pin="DCLK" pad="K13"/>
<connect gate="E" pin="GND" pad="P15"/>
<connect gate="E" pin="GNDA_PLL1" pad="N22"/>
<connect gate="E" pin="GNDA_PLL2" pad="P22"/>
<connect gate="E" pin="GNDG_PLL1" pad="N19"/>
<connect gate="E" pin="GNDG_PLL2" pad="P19"/>
<connect gate="E" pin="GND_10" pad="P11"/>
<connect gate="E" pin="GND_11" pad="R12"/>
<connect gate="E" pin="GND_12" pad="P13"/>
<connect gate="E" pin="GND_13" pad="R14"/>
<connect gate="E" pin="GND_14" pad="P17"/>
<connect gate="E" pin="GND_2" pad="M11"/>
<connect gate="E" pin="GND_3" pad="L26"/>
<connect gate="E" pin="GND_4" pad="M12"/>
<connect gate="E" pin="GND_5" pad="M13"/>
<connect gate="E" pin="GND_6" pad="N12"/>
<connect gate="E" pin="GND_7" pad="N17"/>
<connect gate="E" pin="GND_8" pad="N10"/>
<connect gate="E" pin="GND_9" pad="N14"/>
<connect gate="E" pin="INPUT" pad="M25"/>
<connect gate="E" pin="INPUT_10" pad="M24"/>
<connect gate="E" pin="INPUT_2" pad="K23"/>
<connect gate="E" pin="INPUT_3" pad="K24"/>
<connect gate="E" pin="INPUT_4" pad="L23"/>
<connect gate="E" pin="INPUT_5" pad="K25"/>
<connect gate="E" pin="INPUT_6" pad="L24"/>
<connect gate="E" pin="INPUT_7" pad="K26"/>
<connect gate="E" pin="INPUT_8" pad="M23"/>
<connect gate="E" pin="INPUT_9" pad="L25"/>
<connect gate="E" pin="IO_1_CLK3N" pad="P24"/>
<connect gate="E" pin="IO_1_DIFFIO_TX10N" pad="R18"/>
<connect gate="E" pin="IO_1_DIFFIO_TX10P" pad="R17"/>
<connect gate="E" pin="IO_1_DIFFIO_TX9N" pad="R20"/>
<connect gate="E" pin="IO_1_DIFFIO_TX9P" pad="R19"/>
<connect gate="E" pin="IO_2_CLK1N" pad="N24"/>
<connect gate="E" pin="IO_2_DIFFIO_TX11N" pad="M18"/>
<connect gate="E" pin="IO_2_DIFFIO_TX11P" pad="M17"/>
<connect gate="E" pin="IO_2_DIFFIO_TX12N" pad="M20"/>
<connect gate="E" pin="IO_2_DIFFIO_TX12P" pad="M19"/>
<connect gate="E" pin="IO_2_DIFFIO_TX13N" pad="M22"/>
<connect gate="E" pin="IO_2_DIFFIO_TX13P" pad="M21"/>
<connect gate="E" pin="IO_2_DIFFIO_TX14N" pad="L20"/>
<connect gate="E" pin="IO_2_DIFFIO_TX14P" pad="L19"/>
<connect gate="E" pin="IO_2_DIFFIO_TX15N" pad="K18"/>
<connect gate="E" pin="IO_2_DIFFIO_TX15P" pad="K17"/>
<connect gate="E" pin="IO_2_DIFFIO_TX16N" pad="L22"/>
<connect gate="E" pin="IO_2_DIFFIO_TX16P" pad="L21"/>
<connect gate="E" pin="IO_2_DIFFIO_TX17N" pad="K20"/>
<connect gate="E" pin="IO_2_DIFFIO_TX17P" pad="K19"/>
<connect gate="E" pin="IO_2_DIFFIO_TX19N" pad="K22"/>
<connect gate="E" pin="IO_2_DIFFIO_TX19P" pad="K21"/>
<connect gate="E" pin="IO_3" pad="K16"/>
<connect gate="E" pin="IO_3_2" pad="L15"/>
<connect gate="E" pin="IO_3_3" pad="M15"/>
<connect gate="E" pin="IO_3_RDN3" pad="M16"/>
<connect gate="E" pin="IO_3_RUP3" pad="L16"/>
<connect gate="E" pin="IO_7" pad="R10"/>
<connect gate="E" pin="IO_8" pad="R13"/>
<connect gate="E" pin="IO_8_RDN8" pad="R15"/>
<connect gate="E" pin="NC" pad="K11"/>
<connect gate="E" pin="NCONFIG" pad="L14"/>
<connect gate="E" pin="NSTATUS" pad="K14"/>
<connect gate="E" pin="VCCA_PLL1" pad="N20"/>
<connect gate="E" pin="VCCA_PLL2" pad="P21"/>
<connect gate="E" pin="VCCG_PLL1" pad="N21"/>
<connect gate="E" pin="VCCG_PLL2" pad="P20"/>
<connect gate="E" pin="VCCINT" pad="M10"/>
<connect gate="E" pin="VCCINT_10" pad="N11"/>
<connect gate="E" pin="VCCINT_11" pad="P14"/>
<connect gate="E" pin="VCCINT_12" pad="M14"/>
<connect gate="E" pin="VCCINT_2" pad="L10"/>
<connect gate="E" pin="VCCINT_3" pad="L11"/>
<connect gate="E" pin="VCCINT_4" pad="N15"/>
<connect gate="E" pin="VCCINT_5" pad="N13"/>
<connect gate="E" pin="VCCINT_6" pad="P10"/>
<connect gate="E" pin="VCCINT_7" pad="P12"/>
<connect gate="E" pin="VCCINT_8" pad="N16"/>
<connect gate="E" pin="VCCINT_9" pad="P16"/>
<connect gate="E" pin="VCCIO1" pad="P18"/>
<connect gate="E" pin="VCCIO2" pad="N18"/>
<connect gate="E" pin="VCCIO2_2" pad="M26"/>
<connect gate="E" pin="VCCIO3" pad="L13"/>
<connect gate="E" pin="VCCIO4" pad="L12"/>
<connect gate="E" pin="VCC_PLL5_OUTB" pad="K12"/>
<connect gate="E" pin="VCC_PLL6_OUTB" pad="R11"/>
<connect gate="E" pin="VREF0B1" pad="R16"/>
<connect gate="E" pin="VREF0B2" pad="L17"/>
<connect gate="E" pin="VREF1B2" pad="L18"/>
<connect gate="E" pin="VREF1B4" pad="K10"/>
<connect gate="F" pin="CLK7P" pad="Y12"/>
<connect gate="F" pin="GND" pad="T26"/>
<connect gate="F" pin="GNDA_PLL6" pad="W12"/>
<connect gate="F" pin="GNDG_PLL6" pad="U12"/>
<connect gate="F" pin="INPUT" pad="W26"/>
<connect gate="F" pin="INPUT_10" pad="Y24"/>
<connect gate="F" pin="INPUT_11" pad="T24"/>
<connect gate="F" pin="INPUT_12" pad="U25"/>
<connect gate="F" pin="INPUT_13" pad="V23"/>
<connect gate="F" pin="INPUT_14" pad="V24"/>
<connect gate="F" pin="INPUT_15" pad="T23"/>
<connect gate="F" pin="INPUT_16" pad="T25"/>
<connect gate="F" pin="INPUT_17" pad="U26"/>
<connect gate="F" pin="INPUT_18" pad="Y25"/>
<connect gate="F" pin="INPUT_19" pad="V25"/>
<connect gate="F" pin="INPUT_2" pad="R23"/>
<connect gate="F" pin="INPUT_20" pad="W25"/>
<connect gate="F" pin="INPUT_21" pad="V26"/>
<connect gate="F" pin="INPUT_22" pad="Y26"/>
<connect gate="F" pin="INPUT_3" pad="Y23"/>
<connect gate="F" pin="INPUT_4" pad="R24"/>
<connect gate="F" pin="INPUT_5" pad="W23"/>
<connect gate="F" pin="INPUT_6" pad="R25"/>
<connect gate="F" pin="INPUT_7" pad="U23"/>
<connect gate="F" pin="INPUT_8" pad="U24"/>
<connect gate="F" pin="INPUT_9" pad="W24"/>
<connect gate="F" pin="IO_11_PLL6_OUT1P" pad="AA13"/>
<connect gate="F" pin="IO_12_PLL6_OUT2P" pad="AA14"/>
<connect gate="F" pin="IO_1_DIFFIO_TX0N" pad="W20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX0P" pad="W19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX1N" pad="V22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX1P" pad="V21"/>
<connect gate="F" pin="IO_1_DIFFIO_TX2N" pad="U22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX2P" pad="U21"/>
<connect gate="F" pin="IO_1_DIFFIO_TX3N" pad="V20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX3P" pad="V19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX4N" pad="U20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX4P" pad="U19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX5N" pad="U18"/>
<connect gate="F" pin="IO_1_DIFFIO_TX5P" pad="U17"/>
<connect gate="F" pin="IO_1_DIFFIO_TX6N" pad="T22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX6P" pad="T21"/>
<connect gate="F" pin="IO_1_DIFFIO_TX7N" pad="T20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX7P" pad="T19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX8N" pad="R22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX8P" pad="R21"/>
<connect gate="F" pin="IO_7" pad="AA11"/>
<connect gate="F" pin="IO_7_2" pad="U11"/>
<connect gate="F" pin="IO_7_3" pad="W11"/>
<connect gate="F" pin="IO_7_4" pad="Y11"/>
<connect gate="F" pin="IO_7_CLK7N" pad="AA12"/>
<connect gate="F" pin="IO_7_DEV_CLRN" pad="W10"/>
<connect gate="F" pin="IO_7_RUP7" pad="Y10"/>
<connect gate="F" pin="IO_8" pad="Y16"/>
<connect gate="F" pin="IO_8_2" pad="T15"/>
<connect gate="F" pin="IO_8_3" pad="U14"/>
<connect gate="F" pin="IO_8_4" pad="U15"/>
<connect gate="F" pin="IO_8_5" pad="W16"/>
<connect gate="F" pin="IO_8_6" pad="Y15"/>
<connect gate="F" pin="IO_8_DQ7B0" pad="Y17"/>
<connect gate="F" pin="IO_8_DQ7B1" pad="W17"/>
<connect gate="F" pin="IO_8_DQ7B4" pad="W18"/>
<connect gate="F" pin="IO_8_DQ7B7" pad="Y18"/>
<connect gate="F" pin="IO_8_FCLK2" pad="U16"/>
<connect gate="F" pin="IO_8_FCLK3" pad="T16"/>
<connect gate="F" pin="IO_8_RUP8" pad="V16"/>
<connect gate="F" pin="MSEL0" pad="U13"/>
<connect gate="F" pin="MSEL1" pad="T13"/>
<connect gate="F" pin="MSEL2" pad="V14"/>
<connect gate="F" pin="NC" pad="AA10"/>
<connect gate="F" pin="NC_10" pad="W21"/>
<connect gate="F" pin="NC_11" pad="Y21"/>
<connect gate="F" pin="NC_12" pad="W22"/>
<connect gate="F" pin="NC_13" pad="Y22"/>
<connect gate="F" pin="NC_2" pad="T17"/>
<connect gate="F" pin="NC_3" pad="Y13"/>
<connect gate="F" pin="NC_4" pad="V15"/>
<connect gate="F" pin="NC_5" pad="Y14"/>
<connect gate="F" pin="NC_6" pad="Y19"/>
<connect gate="F" pin="NC_7" pad="W13"/>
<connect gate="F" pin="NC_8" pad="Y20"/>
<connect gate="F" pin="NC_9" pad="W14"/>
<connect gate="F" pin="NIO_PULLUP" pad="T10"/>
<connect gate="F" pin="PLL_ENA" pad="W15"/>
<connect gate="F" pin="PORSEL" pad="U10"/>
<connect gate="F" pin="VCCA_PLL6" pad="T11"/>
<connect gate="F" pin="VCCG_PLL6" pad="V12"/>
<connect gate="F" pin="VCCIO1" pad="R26"/>
<connect gate="F" pin="VCCIO7" pad="T12"/>
<connect gate="F" pin="VCCIO8" pad="T14"/>
<connect gate="F" pin="VCC_PLL6_OUTA" pad="V13"/>
<connect gate="F" pin="VREF0B7" pad="V11"/>
<connect gate="F" pin="VREF0B8" pad="V18"/>
<connect gate="F" pin="VREF1B1" pad="T18"/>
<connect gate="F" pin="VREF1B7" pad="V10"/>
<connect gate="F" pin="VREF1B8" pad="V17"/>
<connect gate="G" pin="CLK4P" pad="AE14"/>
<connect gate="G" pin="CLK5P" pad="AC14"/>
<connect gate="G" pin="CLK6P" pad="AB12"/>
<connect gate="G" pin="GND" pad="AF11"/>
<connect gate="G" pin="GND_2" pad="AF25"/>
<connect gate="G" pin="GND_3" pad="AE26"/>
<connect gate="G" pin="GND_4" pad="AF16"/>
<connect gate="G" pin="IO_11_PLL6_FBN" pad="AE12"/>
<connect gate="G" pin="IO_11_PLL6_FBP" pad="AD12"/>
<connect gate="G" pin="IO_11_PLL6_OUT0N" pad="AD13"/>
<connect gate="G" pin="IO_11_PLL6_OUT0P" pad="AC13"/>
<connect gate="G" pin="IO_11_PLL6_OUT1N" pad="AB13"/>
<connect gate="G" pin="IO_12_PLL6_OUT2N" pad="AB14"/>
<connect gate="G" pin="IO_12_PLL6_OUT3N" pad="AF13"/>
<connect gate="G" pin="IO_12_PLL6_OUT3P" pad="AE13"/>
<connect gate="G" pin="IO_7_CLK6N" pad="AC12"/>
<connect gate="G" pin="IO_7_DQ3B4" pad="AF10"/>
<connect gate="G" pin="IO_7_DQ3B5" pad="AE10"/>
<connect gate="G" pin="IO_7_DQ3B6" pad="AE11"/>
<connect gate="G" pin="IO_8" pad="AA16"/>
<connect gate="G" pin="IO_8_CLK4N" pad="AF14"/>
<connect gate="G" pin="IO_8_CLK5N" pad="AD14"/>
<connect gate="G" pin="IO_8_DQ6B0" pad="AE15"/>
<connect gate="G" pin="IO_8_DQ6B1" pad="AC16"/>
<connect gate="G" pin="IO_8_DQ6B2" pad="AC15"/>
<connect gate="G" pin="IO_8_DQ6B3" pad="AC17"/>
<connect gate="G" pin="IO_8_DQ6B4" pad="AE16"/>
<connect gate="G" pin="IO_8_DQ6B5" pad="AD15"/>
<connect gate="G" pin="IO_8_DQ6B6" pad="AD17"/>
<connect gate="G" pin="IO_8_DQ6B7" pad="AE17"/>
<connect gate="G" pin="IO_8_DQ7B2" pad="AB17"/>
<connect gate="G" pin="IO_8_DQ7B3" pad="AB16"/>
<connect gate="G" pin="IO_8_DQ7B5" pad="AB18"/>
<connect gate="G" pin="IO_8_DQ7B6" pad="AA18"/>
<connect gate="G" pin="IO_8_DQ8B0" pad="AF18"/>
<connect gate="G" pin="IO_8_DQ8B1" pad="AC18"/>
<connect gate="G" pin="IO_8_DQ8B2" pad="AF17"/>
<connect gate="G" pin="IO_8_DQ8B3" pad="AF19"/>
<connect gate="G" pin="IO_8_DQ8B4" pad="AD19"/>
<connect gate="G" pin="IO_8_DQ8B5" pad="AD18"/>
<connect gate="G" pin="IO_8_DQ8B6" pad="AE19"/>
<connect gate="G" pin="IO_8_DQ8B7" pad="AF20"/>
<connect gate="G" pin="IO_8_DQ9B0" pad="AE20"/>
<connect gate="G" pin="IO_8_DQ9B1" pad="AD20"/>
<connect gate="G" pin="IO_8_DQ9B2" pad="AD21"/>
<connect gate="G" pin="IO_8_DQ9B3" pad="AF21"/>
<connect gate="G" pin="IO_8_DQ9B4" pad="AF22"/>
<connect gate="G" pin="IO_8_DQ9B5" pad="AD22"/>
<connect gate="G" pin="IO_8_DQ9B6" pad="AE22"/>
<connect gate="G" pin="IO_8_DQ9B7" pad="AF23"/>
<connect gate="G" pin="IO_8_DQS6B" pad="AD16"/>
<connect gate="G" pin="IO_8_DQS7B" pad="AA17"/>
<connect gate="G" pin="IO_8_DQS8B" pad="AE18"/>
<connect gate="G" pin="IO_8_DQS9B" pad="AE21"/>
<connect gate="G" pin="NC" pad="AE25"/>
<connect gate="G" pin="NC_10" pad="AA26"/>
<connect gate="G" pin="NC_11" pad="AB10"/>
<connect gate="G" pin="NC_12" pad="AB11"/>
<connect gate="G" pin="NC_13" pad="AB15"/>
<connect gate="G" pin="NC_14" pad="AB19"/>
<connect gate="G" pin="NC_15" pad="AB20"/>
<connect gate="G" pin="NC_16" pad="AB21"/>
<connect gate="G" pin="NC_17" pad="AB22"/>
<connect gate="G" pin="NC_18" pad="AB23"/>
<connect gate="G" pin="NC_19" pad="AB24"/>
<connect gate="G" pin="NC_2" pad="AA15"/>
<connect gate="G" pin="NC_20" pad="AB25"/>
<connect gate="G" pin="NC_21" pad="AB26"/>
<connect gate="G" pin="NC_22" pad="AC10"/>
<connect gate="G" pin="NC_23" pad="AC19"/>
<connect gate="G" pin="NC_24" pad="AC11"/>
<connect gate="G" pin="NC_25" pad="AC20"/>
<connect gate="G" pin="NC_26" pad="AC21"/>
<connect gate="G" pin="NC_27" pad="AC22"/>
<connect gate="G" pin="NC_28" pad="AC23"/>
<connect gate="G" pin="NC_29" pad="AC24"/>
<connect gate="G" pin="NC_3" pad="AA19"/>
<connect gate="G" pin="NC_30" pad="AC25"/>
<connect gate="G" pin="NC_31" pad="AC26"/>
<connect gate="G" pin="NC_32" pad="AD10"/>
<connect gate="G" pin="NC_33" pad="AD11"/>
<connect gate="G" pin="NC_34" pad="AD23"/>
<connect gate="G" pin="NC_35" pad="AD24"/>
<connect gate="G" pin="NC_36" pad="AD25"/>
<connect gate="G" pin="NC_37" pad="AE23"/>
<connect gate="G" pin="NC_38" pad="AE24"/>
<connect gate="G" pin="NC_4" pad="AA20"/>
<connect gate="G" pin="NC_5" pad="AA21"/>
<connect gate="G" pin="NC_6" pad="AA22"/>
<connect gate="G" pin="NC_7" pad="AA23"/>
<connect gate="G" pin="NC_8" pad="AA24"/>
<connect gate="G" pin="NC_9" pad="AA25"/>
<connect gate="G" pin="VCCIO1" pad="AD26"/>
<connect gate="G" pin="VCCIO7" pad="AF12"/>
<connect gate="G" pin="VCCIO8" pad="AF24"/>
<connect gate="G" pin="VCCIO8_2" pad="AF15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1SGX10CF672C6N"/>
<attribute name="OC_FARNELL" value="1637229"/>
<attribute name="OC_NEWARK" value="51R0558"/>
<attribute name="PACKAGE" value="672-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1SGX25CF672C7N">
<description>StratixGX FPGA Family</description>
<gates>
<gate name="A" symbol="EP1SGX25CF672C7N_A"/>
<gate name="B" symbol="EP1SGX25CF672C7N_B"/>
<gate name="C" symbol="EP1SGX25CF672C7N_C"/>
<gate name="D" symbol="EP1SGX25CF672C7N_D"/>
<gate name="E" symbol="EP1SGX25CF672C7N_E"/>
<gate name="F" symbol="EP1SGX25CF672C7N_F"/>
<gate name="G" symbol="EP1SGX25CF672C7N_G"/>
</gates>
<devices>
<device name="" package="BGA672C26X26X100P_2700X2700X35">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GND/NC" pad="G2"/>
<connect gate="A" pin="GND/NC_10" pad="G4"/>
<connect gate="A" pin="GND/NC_11" pad="L4"/>
<connect gate="A" pin="GND/NC_12" pad="E2"/>
<connect gate="A" pin="GND/NC_13" pad="L5"/>
<connect gate="A" pin="GND/NC_14" pad="G5"/>
<connect gate="A" pin="GND/NC_2" pad="E1"/>
<connect gate="A" pin="GND/NC_3" pad="J1"/>
<connect gate="A" pin="GND/NC_4" pad="G1"/>
<connect gate="A" pin="GND/NC_5" pad="J4"/>
<connect gate="A" pin="GND/NC_6" pad="L1"/>
<connect gate="A" pin="GND/NC_7" pad="J2"/>
<connect gate="A" pin="GND/NC_8" pad="L2"/>
<connect gate="A" pin="GND/NC_9" pad="J5"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_3" pad="G6"/>
<connect gate="A" pin="GND_4" pad="D3"/>
<connect gate="A" pin="GND_5" pad="J6"/>
<connect gate="A" pin="GXB_GND" pad="H5"/>
<connect gate="A" pin="GXB_GND_10" pad="G3"/>
<connect gate="A" pin="GXB_GND_11" pad="K1"/>
<connect gate="A" pin="GXB_GND_12" pad="F5"/>
<connect gate="A" pin="GXB_GND_13" pad="K2"/>
<connect gate="A" pin="GXB_GND_14" pad="H1"/>
<connect gate="A" pin="GXB_GND_15" pad="K3"/>
<connect gate="A" pin="GXB_GND_16" pad="H2"/>
<connect gate="A" pin="GXB_GND_17" pad="K4"/>
<connect gate="A" pin="GXB_GND_18" pad="H3"/>
<connect gate="A" pin="GXB_GND_19" pad="L3"/>
<connect gate="A" pin="GXB_GND_2" pad="D1"/>
<connect gate="A" pin="GXB_GND_20" pad="K5"/>
<connect gate="A" pin="GXB_GND_21" pad="H4"/>
<connect gate="A" pin="GXB_GND_3" pad="E3"/>
<connect gate="A" pin="GXB_GND_4" pad="D2"/>
<connect gate="A" pin="GXB_GND_5" pad="J3"/>
<connect gate="A" pin="GXB_GND_6" pad="F1"/>
<connect gate="A" pin="GXB_GND_7" pad="F2"/>
<connect gate="A" pin="GXB_GND_8" pad="F3"/>
<connect gate="A" pin="GXB_GND_9" pad="F4"/>
<connect gate="A" pin="IO_4" pad="H8"/>
<connect gate="A" pin="IO_4_2" pad="G9"/>
<connect gate="A" pin="IO_4_3" pad="J9"/>
<connect gate="A" pin="IO_4_4" pad="F8"/>
<connect gate="A" pin="IO_4_5" pad="K8"/>
<connect gate="A" pin="IO_4_6" pad="H7"/>
<connect gate="A" pin="IO_4_DEV_OE" pad="J7"/>
<connect gate="A" pin="IO_4_DQ0T0" pad="B2"/>
<connect gate="A" pin="IO_4_DQ0T1" pad="C2"/>
<connect gate="A" pin="IO_4_DQ0T2" pad="C1"/>
<connect gate="A" pin="IO_4_DQ0T3" pad="B3"/>
<connect gate="A" pin="IO_4_DQ0T4" pad="D4"/>
<connect gate="A" pin="IO_4_DQ0T5" pad="E4"/>
<connect gate="A" pin="IO_4_DQ0T6" pad="B4"/>
<connect gate="A" pin="IO_4_DQ0T7" pad="C4"/>
<connect gate="A" pin="IO_4_DQ1T0" pad="E5"/>
<connect gate="A" pin="IO_4_DQ1T1" pad="C6"/>
<connect gate="A" pin="IO_4_DQ1T2" pad="B5"/>
<connect gate="A" pin="IO_4_DQ1T3" pad="D5"/>
<connect gate="A" pin="IO_4_DQ1T4" pad="A5"/>
<connect gate="A" pin="IO_4_DQ1T5" pad="A4"/>
<connect gate="A" pin="IO_4_DQ1T6" pad="E6"/>
<connect gate="A" pin="IO_4_DQ1T7" pad="D6"/>
<connect gate="A" pin="IO_4_DQ2T0" pad="B6"/>
<connect gate="A" pin="IO_4_DQ2T1" pad="E8"/>
<connect gate="A" pin="IO_4_DQ2T2" pad="F7"/>
<connect gate="A" pin="IO_4_DQ2T3" pad="A6"/>
<connect gate="A" pin="IO_4_DQ2T4" pad="B7"/>
<connect gate="A" pin="IO_4_DQ2T5" pad="D7"/>
<connect gate="A" pin="IO_4_DQ2T6" pad="E7"/>
<connect gate="A" pin="IO_4_DQ2T7" pad="A7"/>
<connect gate="A" pin="IO_4_DQ3T0" pad="D8"/>
<connect gate="A" pin="IO_4_DQ3T1" pad="A8"/>
<connect gate="A" pin="IO_4_DQ3T2" pad="C9"/>
<connect gate="A" pin="IO_4_DQ3T3" pad="C8"/>
<connect gate="A" pin="IO_4_DQ3T5" pad="A9"/>
<connect gate="A" pin="IO_4_DQ3T6" pad="B9"/>
<connect gate="A" pin="IO_4_DQ3T7" pad="D9"/>
<connect gate="A" pin="IO_4_DQS0T" pad="C3"/>
<connect gate="A" pin="IO_4_DQS1T" pad="C5"/>
<connect gate="A" pin="IO_4_DQS2T" pad="C7"/>
<connect gate="A" pin="IO_4_DQS3T" pad="B8"/>
<connect gate="A" pin="IO_4_FCLK7" pad="G7"/>
<connect gate="A" pin="IO_4_RDN4" pad="G8"/>
<connect gate="A" pin="NC" pad="E9"/>
<connect gate="A" pin="RREFB15A" pad="K7"/>
<connect gate="A" pin="TCK" pad="J8"/>
<connect gate="A" pin="TMS" pad="F9"/>
<connect gate="A" pin="TRST" pad="H9"/>
<connect gate="A" pin="VCCINT" pad="H6"/>
<connect gate="A" pin="VCCINT_2" pad="K6"/>
<connect gate="A" pin="VCCINT_3" pad="F6"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCR_B15" pad="L7"/>
<connect gate="A" pin="VCCT_B15" pad="L6"/>
<connect gate="A" pin="VREF0B4" pad="K9"/>
<connect gate="B" pin="GND" pad="A11"/>
<connect gate="B" pin="GND/NC" pad="N5"/>
<connect gate="B" pin="GND/NC_2" pad="N1"/>
<connect gate="B" pin="GND/NC_3" pad="N2"/>
<connect gate="B" pin="GND/NC_4" pad="N4"/>
<connect gate="B" pin="GND_2" pad="P6"/>
<connect gate="B" pin="GND_3" pad="N6"/>
<connect gate="B" pin="GND_4" pad="W6"/>
<connect gate="B" pin="GND_5" pad="U6"/>
<connect gate="B" pin="GND_6" pad="A16"/>
<connect gate="B" pin="GXB_GND" pad="Y5"/>
<connect gate="B" pin="GXB_GND_10" pad="T3"/>
<connect gate="B" pin="GXB_GND_11" pad="V1"/>
<connect gate="B" pin="GXB_GND_12" pad="T4"/>
<connect gate="B" pin="GXB_GND_13" pad="P1"/>
<connect gate="B" pin="GXB_GND_14" pad="V2"/>
<connect gate="B" pin="GXB_GND_15" pad="P2"/>
<connect gate="B" pin="GXB_GND_16" pad="T5"/>
<connect gate="B" pin="GXB_GND_17" pad="P3"/>
<connect gate="B" pin="GXB_GND_18" pad="U3"/>
<connect gate="B" pin="GXB_GND_19" pad="P4"/>
<connect gate="B" pin="GXB_GND_2" pad="M1"/>
<connect gate="B" pin="GXB_GND_20" pad="W3"/>
<connect gate="B" pin="GXB_GND_21" pad="M5"/>
<connect gate="B" pin="GXB_GND_22" pad="P5"/>
<connect gate="B" pin="GXB_GND_23" pad="V3"/>
<connect gate="B" pin="GXB_GND_24" pad="V4"/>
<connect gate="B" pin="GXB_GND_25" pad="Y1"/>
<connect gate="B" pin="GXB_GND_26" pad="V5"/>
<connect gate="B" pin="GXB_GND_27" pad="Y2"/>
<connect gate="B" pin="GXB_GND_28" pad="Y3"/>
<connect gate="B" pin="GXB_GND_29" pad="Y4"/>
<connect gate="B" pin="GXB_GND_3" pad="M2"/>
<connect gate="B" pin="GXB_GND_4" pad="M3"/>
<connect gate="B" pin="GXB_GND_5" pad="N3"/>
<connect gate="B" pin="GXB_GND_6" pad="T1"/>
<connect gate="B" pin="GXB_GND_7" pad="M4"/>
<connect gate="B" pin="GXB_GND_8" pad="R3"/>
<connect gate="B" pin="GXB_GND_9" pad="T2"/>
<connect gate="B" pin="GXB_RX8N" pad="U2"/>
<connect gate="B" pin="GXB_RX8P" pad="U1"/>
<connect gate="B" pin="GXB_RX9N" pad="R2"/>
<connect gate="B" pin="GXB_RX9P" pad="R1"/>
<connect gate="B" pin="GXB_TX10N" pad="W5"/>
<connect gate="B" pin="GXB_TX10P" pad="W4"/>
<connect gate="B" pin="GXB_TX8N" pad="U5"/>
<connect gate="B" pin="GXB_TX8P" pad="U4"/>
<connect gate="B" pin="GXB_TX9N" pad="R5"/>
<connect gate="B" pin="GXB_TX9P" pad="R4"/>
<connect gate="B" pin="IO_10_PLL5_OUT3N" pad="A13"/>
<connect gate="B" pin="IO_3_CLK14N" pad="A14"/>
<connect gate="B" pin="IO_3_DQ7T2" pad="A17"/>
<connect gate="B" pin="IO_3_DQ8T2" pad="A18"/>
<connect gate="B" pin="IO_3_DQ8T4" pad="A20"/>
<connect gate="B" pin="IO_3_DQ8T5" pad="A19"/>
<connect gate="B" pin="IO_3_DQ9T0" pad="A21"/>
<connect gate="B" pin="IO_3_DQ9T4" pad="A22"/>
<connect gate="B" pin="IO_4_DQ3T4" pad="A10"/>
<connect gate="B" pin="IO_7" pad="V7"/>
<connect gate="B" pin="IO_7_2" pad="U8"/>
<connect gate="B" pin="IO_7_3" pad="W7"/>
<connect gate="B" pin="IO_7_4" pad="U9"/>
<connect gate="B" pin="IO_7_5" pad="W8"/>
<connect gate="B" pin="IO_7_DQ2B2" pad="Y8"/>
<connect gate="B" pin="IO_7_DQ2B6" pad="Y7"/>
<connect gate="B" pin="IO_7_FCLK4" pad="Y9"/>
<connect gate="B" pin="IO_7_FCLK5" pad="W9"/>
<connect gate="B" pin="IO_7_RDN7" pad="V8"/>
<connect gate="B" pin="NC" pad="V9"/>
<connect gate="B" pin="NCE" pad="P9"/>
<connect gate="B" pin="NCEO" pad="T9"/>
<connect gate="B" pin="REFCLKB15N" pad="W2"/>
<connect gate="B" pin="REFCLKB15P" pad="W1"/>
<connect gate="B" pin="RREFB15" pad="U7"/>
<connect gate="B" pin="VCCA_B15" pad="N7"/>
<connect gate="B" pin="VCCA_B15_2" pad="P8"/>
<connect gate="B" pin="VCCG_B15" pad="N8"/>
<connect gate="B" pin="VCCG_B15_2" pad="P7"/>
<connect gate="B" pin="VCCINT" pad="M9"/>
<connect gate="B" pin="VCCINT_2" pad="N9"/>
<connect gate="B" pin="VCCINT_3" pad="V6"/>
<connect gate="B" pin="VCCINT_4" pad="L9"/>
<connect gate="B" pin="VCCINT_5" pad="Y6"/>
<connect gate="B" pin="VCCIO3" pad="A15"/>
<connect gate="B" pin="VCCIO4" pad="A12"/>
<connect gate="B" pin="VCCP_B15" pad="T8"/>
<connect gate="B" pin="VCCP_B15_2" pad="L8"/>
<connect gate="B" pin="VCCP_B15_3" pad="M8"/>
<connect gate="B" pin="VCCP_B15_4" pad="R8"/>
<connect gate="B" pin="VCCR_B15" pad="T7"/>
<connect gate="B" pin="VCCR_B15_2" pad="M7"/>
<connect gate="B" pin="VCCR_B15_3" pad="R7"/>
<connect gate="B" pin="VCCSEL" pad="R9"/>
<connect gate="B" pin="VCCT_B15" pad="T6"/>
<connect gate="B" pin="VCCT_B15_2" pad="M6"/>
<connect gate="B" pin="VCCT_B15_3" pad="R6"/>
<connect gate="C" pin="CLK14P" pad="B14"/>
<connect gate="C" pin="CLK15P" pad="D14"/>
<connect gate="C" pin="GND" pad="AF2"/>
<connect gate="C" pin="GND_2" pad="A25"/>
<connect gate="C" pin="GND_3" pad="AC3"/>
<connect gate="C" pin="GND_4" pad="AD3"/>
<connect gate="C" pin="GND_5" pad="AA6"/>
<connect gate="C" pin="GND_6" pad="B26"/>
<connect gate="C" pin="GND_7" pad="AE1"/>
<connect gate="C" pin="GXB_GND" pad="AA3"/>
<connect gate="C" pin="GXB_GND_2" pad="AD1"/>
<connect gate="C" pin="GXB_GND_3" pad="AD2"/>
<connect gate="C" pin="GXB_GND_4" pad="AB1"/>
<connect gate="C" pin="GXB_GND_5" pad="AB2"/>
<connect gate="C" pin="GXB_GND_6" pad="AB3"/>
<connect gate="C" pin="GXB_GND_7" pad="AB4"/>
<connect gate="C" pin="GXB_GND_8" pad="AB5"/>
<connect gate="C" pin="GXB_RX10N" pad="AA2"/>
<connect gate="C" pin="GXB_RX10P" pad="AA1"/>
<connect gate="C" pin="GXB_RX11N" pad="AC2"/>
<connect gate="C" pin="GXB_RX11P" pad="AC1"/>
<connect gate="C" pin="GXB_TX11N" pad="AA5"/>
<connect gate="C" pin="GXB_TX11P" pad="AA4"/>
<connect gate="C" pin="IO_10_PLL5_OUT3P" pad="B13"/>
<connect gate="C" pin="IO_3_CLK15N" pad="C14"/>
<connect gate="C" pin="IO_3_DQ6T1" pad="B15"/>
<connect gate="C" pin="IO_3_DQ6T3" pad="C16"/>
<connect gate="C" pin="IO_3_DQ6T6" pad="C15"/>
<connect gate="C" pin="IO_3_DQ6T7" pad="B16"/>
<connect gate="C" pin="IO_3_DQ7T1" pad="B17"/>
<connect gate="C" pin="IO_3_DQ7T4" pad="C18"/>
<connect gate="C" pin="IO_3_DQ7T5" pad="B18"/>
<connect gate="C" pin="IO_3_DQ8T0" pad="C19"/>
<connect gate="C" pin="IO_3_DQ8T3" pad="B20"/>
<connect gate="C" pin="IO_3_DQ8T6" pad="C20"/>
<connect gate="C" pin="IO_3_DQ9T1" pad="B21"/>
<connect gate="C" pin="IO_3_DQ9T2" pad="C21"/>
<connect gate="C" pin="IO_3_DQ9T3" pad="C22"/>
<connect gate="C" pin="IO_3_DQ9T5" pad="B23"/>
<connect gate="C" pin="IO_3_DQ9T6" pad="A23"/>
<connect gate="C" pin="IO_3_DQ9T7" pad="B24"/>
<connect gate="C" pin="IO_3_DQS6T" pad="D15"/>
<connect gate="C" pin="IO_3_DQS7T" pad="C17"/>
<connect gate="C" pin="IO_3_DQS8T" pad="B19"/>
<connect gate="C" pin="IO_3_DQS9T" pad="B22"/>
<connect gate="C" pin="IO_4_CLK12N" pad="D12"/>
<connect gate="C" pin="IO_7_DQ0B0" pad="AC5"/>
<connect gate="C" pin="IO_7_DQ0B1" pad="AE3"/>
<connect gate="C" pin="IO_7_DQ0B2" pad="AE2"/>
<connect gate="C" pin="IO_7_DQ0B3" pad="AD5"/>
<connect gate="C" pin="IO_7_DQ0B4" pad="AD4"/>
<connect gate="C" pin="IO_7_DQ0B5" pad="AC4"/>
<connect gate="C" pin="IO_7_DQ0B6" pad="AE5"/>
<connect gate="C" pin="IO_7_DQ0B7" pad="AF4"/>
<connect gate="C" pin="IO_7_DQ1B0" pad="AC6"/>
<connect gate="C" pin="IO_7_DQ1B1" pad="AC7"/>
<connect gate="C" pin="IO_7_DQ1B2" pad="AF6"/>
<connect gate="C" pin="IO_7_DQ1B3" pad="AD6"/>
<connect gate="C" pin="IO_7_DQ1B4" pad="AE7"/>
<connect gate="C" pin="IO_7_DQ1B5" pad="AF7"/>
<connect gate="C" pin="IO_7_DQ1B6" pad="AD7"/>
<connect gate="C" pin="IO_7_DQ1B7" pad="AF5"/>
<connect gate="C" pin="IO_7_DQ2B0" pad="AB8"/>
<connect gate="C" pin="IO_7_DQ2B1" pad="AA8"/>
<connect gate="C" pin="IO_7_DQ2B3" pad="AB9"/>
<connect gate="C" pin="IO_7_DQ2B4" pad="AC8"/>
<connect gate="C" pin="IO_7_DQ2B5" pad="AA7"/>
<connect gate="C" pin="IO_7_DQ2B7" pad="AC9"/>
<connect gate="C" pin="IO_7_DQ3B0" pad="AD8"/>
<connect gate="C" pin="IO_7_DQ3B1" pad="AD9"/>
<connect gate="C" pin="IO_7_DQ3B2" pad="AF9"/>
<connect gate="C" pin="IO_7_DQ3B3" pad="AE8"/>
<connect gate="C" pin="IO_7_DQ3B7" pad="AF8"/>
<connect gate="C" pin="IO_7_DQS0B" pad="AE4"/>
<connect gate="C" pin="IO_7_DQS1B" pad="AE6"/>
<connect gate="C" pin="IO_7_DQS2B" pad="AB7"/>
<connect gate="C" pin="IO_7_DQS3B" pad="AE9"/>
<connect gate="C" pin="IO_9_PLL5_OUT0N" pad="C13"/>
<connect gate="C" pin="IO_9_PLL5_OUT0P" pad="D13"/>
<connect gate="C" pin="IO_9_PLL5_OUT1N" pad="B12"/>
<connect gate="C" pin="IO_9_PLL5_OUT1P" pad="C12"/>
<connect gate="C" pin="NC" pad="C25"/>
<connect gate="C" pin="NC_10" pad="C24"/>
<connect gate="C" pin="NC_11" pad="B25"/>
<connect gate="C" pin="NC_2" pad="C10"/>
<connect gate="C" pin="NC_3" pad="D10"/>
<connect gate="C" pin="NC_4" pad="AA9"/>
<connect gate="C" pin="NC_5" pad="B10"/>
<connect gate="C" pin="NC_6" pad="C11"/>
<connect gate="C" pin="NC_7" pad="B11"/>
<connect gate="C" pin="NC_8" pad="D11"/>
<connect gate="C" pin="NC_9" pad="C23"/>
<connect gate="C" pin="VCCINT" pad="AB6"/>
<connect gate="C" pin="VCCIO2" pad="C26"/>
<connect gate="C" pin="VCCIO3" pad="A24"/>
<connect gate="C" pin="VCCIO7" pad="AF3"/>
<connect gate="D" pin="CLK12P" pad="E12"/>
<connect gate="D" pin="CLK13P" pad="G12"/>
<connect gate="D" pin="GND" pad="H17"/>
<connect gate="D" pin="GNDA_PLL5" pad="G13"/>
<connect gate="D" pin="GNDG_PLL5" pad="J12"/>
<connect gate="D" pin="INPUT" pad="H26"/>
<connect gate="D" pin="INPUT_10" pad="H23"/>
<connect gate="D" pin="INPUT_11" pad="H24"/>
<connect gate="D" pin="INPUT_12" pad="H25"/>
<connect gate="D" pin="INPUT_2" pad="F25"/>
<connect gate="D" pin="INPUT_3" pad="G25"/>
<connect gate="D" pin="INPUT_4" pad="G26"/>
<connect gate="D" pin="INPUT_5" pad="J23"/>
<connect gate="D" pin="INPUT_6" pad="F26"/>
<connect gate="D" pin="INPUT_7" pad="J24"/>
<connect gate="D" pin="INPUT_8" pad="J25"/>
<connect gate="D" pin="INPUT_9" pad="J26"/>
<connect gate="D" pin="IO_10_PLL5_OUT2N" pad="E14"/>
<connect gate="D" pin="IO_10_PLL5_OUT2P" pad="F14"/>
<connect gate="D" pin="IO_2_DIFFIO_TX18N" pad="J20"/>
<connect gate="D" pin="IO_2_DIFFIO_TX18P" pad="J19"/>
<connect gate="D" pin="IO_2_DIFFIO_TX20N" pad="J22"/>
<connect gate="D" pin="IO_2_DIFFIO_TX20P" pad="J21"/>
<connect gate="D" pin="IO_2_DIFFIO_TX21N" pad="H20"/>
<connect gate="D" pin="IO_2_DIFFIO_TX21P" pad="H19"/>
<connect gate="D" pin="IO_3" pad="G17"/>
<connect gate="D" pin="IO_3_2" pad="H16"/>
<connect gate="D" pin="IO_3_3" pad="G16"/>
<connect gate="D" pin="IO_3_4" pad="H18"/>
<connect gate="D" pin="IO_3_5" pad="F17"/>
<connect gate="D" pin="IO_3_DQ6T0" pad="E16"/>
<connect gate="D" pin="IO_3_DQ6T2" pad="E15"/>
<connect gate="D" pin="IO_3_DQ6T4" pad="D16"/>
<connect gate="D" pin="IO_3_DQ6T5" pad="F15"/>
<connect gate="D" pin="IO_3_DQ7T0" pad="E17"/>
<connect gate="D" pin="IO_3_DQ7T3" pad="D17"/>
<connect gate="D" pin="IO_3_DQ7T6" pad="D18"/>
<connect gate="D" pin="IO_3_DQ7T7" pad="E18"/>
<connect gate="D" pin="IO_3_DQ8T1" pad="D19"/>
<connect gate="D" pin="IO_3_DQ8T7" pad="D20"/>
<connect gate="D" pin="IO_3_FCLK0" pad="F18"/>
<connect gate="D" pin="IO_3_FCLK1" pad="G18"/>
<connect gate="D" pin="IO_4" pad="H11"/>
<connect gate="D" pin="IO_4_2" pad="E10"/>
<connect gate="D" pin="IO_4_3" pad="H10"/>
<connect gate="D" pin="IO_4_4" pad="E11"/>
<connect gate="D" pin="IO_4_CLK13N" pad="F12"/>
<connect gate="D" pin="IO_4_FCLK6" pad="G10"/>
<connect gate="D" pin="IO_4_RUP4" pad="G11"/>
<connect gate="D" pin="IO_9_PLL5_FBN" pad="E13"/>
<connect gate="D" pin="IO_9_PLL5_FBP" pad="F13"/>
<connect gate="D" pin="NC" pad="H22"/>
<connect gate="D" pin="NC_10" pad="F16"/>
<connect gate="D" pin="NC_11" pad="D24"/>
<connect gate="D" pin="NC_12" pad="H21"/>
<connect gate="D" pin="NC_13" pad="D21"/>
<connect gate="D" pin="NC_14" pad="H14"/>
<connect gate="D" pin="NC_15" pad="D25"/>
<connect gate="D" pin="NC_16" pad="E26"/>
<connect gate="D" pin="NC_17" pad="F19"/>
<connect gate="D" pin="NC_18" pad="J18"/>
<connect gate="D" pin="NC_19" pad="E19"/>
<connect gate="D" pin="NC_2" pad="G21"/>
<connect gate="D" pin="NC_20" pad="G15"/>
<connect gate="D" pin="NC_21" pad="D22"/>
<connect gate="D" pin="NC_22" pad="G20"/>
<connect gate="D" pin="NC_23" pad="E20"/>
<connect gate="D" pin="NC_24" pad="F20"/>
<connect gate="D" pin="NC_25" pad="F21"/>
<connect gate="D" pin="NC_26" pad="J15"/>
<connect gate="D" pin="NC_27" pad="E21"/>
<connect gate="D" pin="NC_28" pad="J14"/>
<connect gate="D" pin="NC_29" pad="D23"/>
<connect gate="D" pin="NC_3" pad="E23"/>
<connect gate="D" pin="NC_30" pad="H15"/>
<connect gate="D" pin="NC_31" pad="E22"/>
<connect gate="D" pin="NC_32" pad="F22"/>
<connect gate="D" pin="NC_33" pad="F23"/>
<connect gate="D" pin="NC_34" pad="G19"/>
<connect gate="D" pin="NC_35" pad="D26"/>
<connect gate="D" pin="NC_36" pad="F24"/>
<connect gate="D" pin="NC_4" pad="G22"/>
<connect gate="D" pin="NC_5" pad="E24"/>
<connect gate="D" pin="NC_6" pad="G23"/>
<connect gate="D" pin="NC_7" pad="E25"/>
<connect gate="D" pin="NC_8" pad="G14"/>
<connect gate="D" pin="NC_9" pad="G24"/>
<connect gate="D" pin="TDI" pad="F10"/>
<connect gate="D" pin="TDO" pad="F11"/>
<connect gate="D" pin="TEMPDIODEN" pad="J10"/>
<connect gate="D" pin="TEMPDIODEP" pad="J11"/>
<connect gate="D" pin="VCCA_PLL5" pad="H13"/>
<connect gate="D" pin="VCCG_PLL5" pad="H12"/>
<connect gate="D" pin="VCC_PLL5_OUTA" pad="J13"/>
<connect gate="D" pin="VREF0B3" pad="J16"/>
<connect gate="D" pin="VREF1B3" pad="J17"/>
<connect gate="E" pin="CLK0N" pad="N26"/>
<connect gate="E" pin="CLK0P" pad="N25"/>
<connect gate="E" pin="CLK1P" pad="N23"/>
<connect gate="E" pin="CLK2N" pad="P26"/>
<connect gate="E" pin="CLK2P" pad="P25"/>
<connect gate="E" pin="CLK3P" pad="P23"/>
<connect gate="E" pin="CONF_DONE" pad="K15"/>
<connect gate="E" pin="DCLK" pad="K13"/>
<connect gate="E" pin="GND" pad="P15"/>
<connect gate="E" pin="GNDA_PLL1" pad="N22"/>
<connect gate="E" pin="GNDA_PLL2" pad="P22"/>
<connect gate="E" pin="GNDG_PLL1" pad="N19"/>
<connect gate="E" pin="GNDG_PLL2" pad="P19"/>
<connect gate="E" pin="GND_10" pad="P11"/>
<connect gate="E" pin="GND_11" pad="R12"/>
<connect gate="E" pin="GND_12" pad="P13"/>
<connect gate="E" pin="GND_13" pad="R14"/>
<connect gate="E" pin="GND_14" pad="P17"/>
<connect gate="E" pin="GND_2" pad="M11"/>
<connect gate="E" pin="GND_3" pad="L26"/>
<connect gate="E" pin="GND_4" pad="M12"/>
<connect gate="E" pin="GND_5" pad="M13"/>
<connect gate="E" pin="GND_6" pad="N12"/>
<connect gate="E" pin="GND_7" pad="N17"/>
<connect gate="E" pin="GND_8" pad="N10"/>
<connect gate="E" pin="GND_9" pad="N14"/>
<connect gate="E" pin="INPUT" pad="M25"/>
<connect gate="E" pin="INPUT_10" pad="M24"/>
<connect gate="E" pin="INPUT_2" pad="K23"/>
<connect gate="E" pin="INPUT_3" pad="K24"/>
<connect gate="E" pin="INPUT_4" pad="L23"/>
<connect gate="E" pin="INPUT_5" pad="K25"/>
<connect gate="E" pin="INPUT_6" pad="L24"/>
<connect gate="E" pin="INPUT_7" pad="K26"/>
<connect gate="E" pin="INPUT_8" pad="M23"/>
<connect gate="E" pin="INPUT_9" pad="L25"/>
<connect gate="E" pin="IO_1_CLK3N" pad="P24"/>
<connect gate="E" pin="IO_1_DIFFIO_TX10N" pad="R18"/>
<connect gate="E" pin="IO_1_DIFFIO_TX10P" pad="R17"/>
<connect gate="E" pin="IO_1_DIFFIO_TX9N" pad="R20"/>
<connect gate="E" pin="IO_1_DIFFIO_TX9P" pad="R19"/>
<connect gate="E" pin="IO_2_CLK1N" pad="N24"/>
<connect gate="E" pin="IO_2_DIFFIO_TX11N" pad="M18"/>
<connect gate="E" pin="IO_2_DIFFIO_TX11P" pad="M17"/>
<connect gate="E" pin="IO_2_DIFFIO_TX12N" pad="M20"/>
<connect gate="E" pin="IO_2_DIFFIO_TX12P" pad="M19"/>
<connect gate="E" pin="IO_2_DIFFIO_TX13N" pad="M22"/>
<connect gate="E" pin="IO_2_DIFFIO_TX13P" pad="M21"/>
<connect gate="E" pin="IO_2_DIFFIO_TX14N" pad="L20"/>
<connect gate="E" pin="IO_2_DIFFIO_TX14P" pad="L19"/>
<connect gate="E" pin="IO_2_DIFFIO_TX15N" pad="K18"/>
<connect gate="E" pin="IO_2_DIFFIO_TX15P" pad="K17"/>
<connect gate="E" pin="IO_2_DIFFIO_TX16N" pad="L22"/>
<connect gate="E" pin="IO_2_DIFFIO_TX16P" pad="L21"/>
<connect gate="E" pin="IO_2_DIFFIO_TX17N" pad="K20"/>
<connect gate="E" pin="IO_2_DIFFIO_TX17P" pad="K19"/>
<connect gate="E" pin="IO_2_DIFFIO_TX19N" pad="K22"/>
<connect gate="E" pin="IO_2_DIFFIO_TX19P" pad="K21"/>
<connect gate="E" pin="IO_3" pad="K16"/>
<connect gate="E" pin="IO_3_2" pad="L15"/>
<connect gate="E" pin="IO_3_3" pad="M15"/>
<connect gate="E" pin="IO_3_RDN3" pad="M16"/>
<connect gate="E" pin="IO_3_RUP3" pad="L16"/>
<connect gate="E" pin="IO_7" pad="R10"/>
<connect gate="E" pin="IO_8" pad="R13"/>
<connect gate="E" pin="IO_8_RDN8" pad="R15"/>
<connect gate="E" pin="NC" pad="K11"/>
<connect gate="E" pin="NCONFIG" pad="L14"/>
<connect gate="E" pin="NSTATUS" pad="K14"/>
<connect gate="E" pin="VCCA_PLL1" pad="N20"/>
<connect gate="E" pin="VCCA_PLL2" pad="P21"/>
<connect gate="E" pin="VCCG_PLL1" pad="N21"/>
<connect gate="E" pin="VCCG_PLL2" pad="P20"/>
<connect gate="E" pin="VCCINT" pad="M10"/>
<connect gate="E" pin="VCCINT_10" pad="N11"/>
<connect gate="E" pin="VCCINT_11" pad="P14"/>
<connect gate="E" pin="VCCINT_12" pad="M14"/>
<connect gate="E" pin="VCCINT_2" pad="L10"/>
<connect gate="E" pin="VCCINT_3" pad="L11"/>
<connect gate="E" pin="VCCINT_4" pad="N15"/>
<connect gate="E" pin="VCCINT_5" pad="N13"/>
<connect gate="E" pin="VCCINT_6" pad="P10"/>
<connect gate="E" pin="VCCINT_7" pad="P12"/>
<connect gate="E" pin="VCCINT_8" pad="N16"/>
<connect gate="E" pin="VCCINT_9" pad="P16"/>
<connect gate="E" pin="VCCIO1" pad="P18"/>
<connect gate="E" pin="VCCIO2" pad="N18"/>
<connect gate="E" pin="VCCIO2_2" pad="M26"/>
<connect gate="E" pin="VCCIO3" pad="L13"/>
<connect gate="E" pin="VCCIO4" pad="L12"/>
<connect gate="E" pin="VCC_PLL5_OUTB" pad="K12"/>
<connect gate="E" pin="VCC_PLL6_OUTB" pad="R11"/>
<connect gate="E" pin="VREF0B1" pad="R16"/>
<connect gate="E" pin="VREF0B2" pad="L17"/>
<connect gate="E" pin="VREF1B2" pad="L18"/>
<connect gate="E" pin="VREF1B4" pad="K10"/>
<connect gate="F" pin="CLK7P" pad="Y12"/>
<connect gate="F" pin="GND" pad="T26"/>
<connect gate="F" pin="GNDA_PLL6" pad="W12"/>
<connect gate="F" pin="GNDG_PLL6" pad="U12"/>
<connect gate="F" pin="INPUT" pad="W26"/>
<connect gate="F" pin="INPUT_10" pad="Y24"/>
<connect gate="F" pin="INPUT_11" pad="T24"/>
<connect gate="F" pin="INPUT_12" pad="U25"/>
<connect gate="F" pin="INPUT_13" pad="V23"/>
<connect gate="F" pin="INPUT_14" pad="V24"/>
<connect gate="F" pin="INPUT_15" pad="T23"/>
<connect gate="F" pin="INPUT_16" pad="T25"/>
<connect gate="F" pin="INPUT_17" pad="U26"/>
<connect gate="F" pin="INPUT_18" pad="Y25"/>
<connect gate="F" pin="INPUT_19" pad="V25"/>
<connect gate="F" pin="INPUT_2" pad="R23"/>
<connect gate="F" pin="INPUT_20" pad="W25"/>
<connect gate="F" pin="INPUT_21" pad="V26"/>
<connect gate="F" pin="INPUT_22" pad="Y26"/>
<connect gate="F" pin="INPUT_3" pad="Y23"/>
<connect gate="F" pin="INPUT_4" pad="R24"/>
<connect gate="F" pin="INPUT_5" pad="W23"/>
<connect gate="F" pin="INPUT_6" pad="R25"/>
<connect gate="F" pin="INPUT_7" pad="U23"/>
<connect gate="F" pin="INPUT_8" pad="U24"/>
<connect gate="F" pin="INPUT_9" pad="W24"/>
<connect gate="F" pin="IO_11_PLL6_OUT1P" pad="AA13"/>
<connect gate="F" pin="IO_12_PLL6_OUT2P" pad="AA14"/>
<connect gate="F" pin="IO_1_DIFFIO_TX0N" pad="W20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX0P" pad="W19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX1N" pad="V22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX1P" pad="V21"/>
<connect gate="F" pin="IO_1_DIFFIO_TX2N" pad="U22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX2P" pad="U21"/>
<connect gate="F" pin="IO_1_DIFFIO_TX3N" pad="V20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX3P" pad="V19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX4N" pad="U20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX4P" pad="U19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX5N" pad="U18"/>
<connect gate="F" pin="IO_1_DIFFIO_TX5P" pad="U17"/>
<connect gate="F" pin="IO_1_DIFFIO_TX6N" pad="T22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX6P" pad="T21"/>
<connect gate="F" pin="IO_1_DIFFIO_TX7N" pad="T20"/>
<connect gate="F" pin="IO_1_DIFFIO_TX7P" pad="T19"/>
<connect gate="F" pin="IO_1_DIFFIO_TX8N" pad="R22"/>
<connect gate="F" pin="IO_1_DIFFIO_TX8P" pad="R21"/>
<connect gate="F" pin="IO_7" pad="AA11"/>
<connect gate="F" pin="IO_7_2" pad="U11"/>
<connect gate="F" pin="IO_7_3" pad="W11"/>
<connect gate="F" pin="IO_7_4" pad="Y11"/>
<connect gate="F" pin="IO_7_CLK7N" pad="AA12"/>
<connect gate="F" pin="IO_7_DEV_CLRN" pad="W10"/>
<connect gate="F" pin="IO_7_RUP7" pad="Y10"/>
<connect gate="F" pin="IO_8" pad="Y16"/>
<connect gate="F" pin="IO_8_2" pad="T15"/>
<connect gate="F" pin="IO_8_3" pad="U14"/>
<connect gate="F" pin="IO_8_4" pad="U15"/>
<connect gate="F" pin="IO_8_5" pad="W16"/>
<connect gate="F" pin="IO_8_6" pad="Y15"/>
<connect gate="F" pin="IO_8_DQ7B0" pad="Y17"/>
<connect gate="F" pin="IO_8_DQ7B1" pad="W17"/>
<connect gate="F" pin="IO_8_DQ7B4" pad="W18"/>
<connect gate="F" pin="IO_8_DQ7B7" pad="Y18"/>
<connect gate="F" pin="IO_8_FCLK2" pad="U16"/>
<connect gate="F" pin="IO_8_FCLK3" pad="T16"/>
<connect gate="F" pin="IO_8_RUP8" pad="V16"/>
<connect gate="F" pin="MSEL0" pad="U13"/>
<connect gate="F" pin="MSEL1" pad="T13"/>
<connect gate="F" pin="MSEL2" pad="V14"/>
<connect gate="F" pin="NC" pad="AA10"/>
<connect gate="F" pin="NC_10" pad="W21"/>
<connect gate="F" pin="NC_11" pad="Y21"/>
<connect gate="F" pin="NC_12" pad="W22"/>
<connect gate="F" pin="NC_13" pad="Y22"/>
<connect gate="F" pin="NC_2" pad="T17"/>
<connect gate="F" pin="NC_3" pad="Y13"/>
<connect gate="F" pin="NC_4" pad="V15"/>
<connect gate="F" pin="NC_5" pad="Y14"/>
<connect gate="F" pin="NC_6" pad="Y19"/>
<connect gate="F" pin="NC_7" pad="W13"/>
<connect gate="F" pin="NC_8" pad="Y20"/>
<connect gate="F" pin="NC_9" pad="W14"/>
<connect gate="F" pin="NIO_PULLUP" pad="T10"/>
<connect gate="F" pin="PLL_ENA" pad="W15"/>
<connect gate="F" pin="PORSEL" pad="U10"/>
<connect gate="F" pin="VCCA_PLL6" pad="T11"/>
<connect gate="F" pin="VCCG_PLL6" pad="V12"/>
<connect gate="F" pin="VCCIO1" pad="R26"/>
<connect gate="F" pin="VCCIO7" pad="T12"/>
<connect gate="F" pin="VCCIO8" pad="T14"/>
<connect gate="F" pin="VCC_PLL6_OUTA" pad="V13"/>
<connect gate="F" pin="VREF0B7" pad="V11"/>
<connect gate="F" pin="VREF0B8" pad="V18"/>
<connect gate="F" pin="VREF1B1" pad="T18"/>
<connect gate="F" pin="VREF1B7" pad="V10"/>
<connect gate="F" pin="VREF1B8" pad="V17"/>
<connect gate="G" pin="CLK4P" pad="AE14"/>
<connect gate="G" pin="CLK5P" pad="AC14"/>
<connect gate="G" pin="CLK6P" pad="AB12"/>
<connect gate="G" pin="GND" pad="AF11"/>
<connect gate="G" pin="GND_2" pad="AF25"/>
<connect gate="G" pin="GND_3" pad="AE26"/>
<connect gate="G" pin="GND_4" pad="AF16"/>
<connect gate="G" pin="IO_11_PLL6_FBN" pad="AE12"/>
<connect gate="G" pin="IO_11_PLL6_FBP" pad="AD12"/>
<connect gate="G" pin="IO_11_PLL6_OUT0N" pad="AD13"/>
<connect gate="G" pin="IO_11_PLL6_OUT0P" pad="AC13"/>
<connect gate="G" pin="IO_11_PLL6_OUT1N" pad="AB13"/>
<connect gate="G" pin="IO_12_PLL6_OUT2N" pad="AB14"/>
<connect gate="G" pin="IO_12_PLL6_OUT3N" pad="AF13"/>
<connect gate="G" pin="IO_12_PLL6_OUT3P" pad="AE13"/>
<connect gate="G" pin="IO_7_CLK6N" pad="AC12"/>
<connect gate="G" pin="IO_7_DQ3B4" pad="AF10"/>
<connect gate="G" pin="IO_7_DQ3B5" pad="AE10"/>
<connect gate="G" pin="IO_7_DQ3B6" pad="AE11"/>
<connect gate="G" pin="IO_8" pad="AA16"/>
<connect gate="G" pin="IO_8_CLK4N" pad="AF14"/>
<connect gate="G" pin="IO_8_CLK5N" pad="AD14"/>
<connect gate="G" pin="IO_8_DQ6B0" pad="AE15"/>
<connect gate="G" pin="IO_8_DQ6B1" pad="AC16"/>
<connect gate="G" pin="IO_8_DQ6B2" pad="AC15"/>
<connect gate="G" pin="IO_8_DQ6B3" pad="AC17"/>
<connect gate="G" pin="IO_8_DQ6B4" pad="AE16"/>
<connect gate="G" pin="IO_8_DQ6B5" pad="AD15"/>
<connect gate="G" pin="IO_8_DQ6B6" pad="AD17"/>
<connect gate="G" pin="IO_8_DQ6B7" pad="AE17"/>
<connect gate="G" pin="IO_8_DQ7B2" pad="AB17"/>
<connect gate="G" pin="IO_8_DQ7B3" pad="AB16"/>
<connect gate="G" pin="IO_8_DQ7B5" pad="AB18"/>
<connect gate="G" pin="IO_8_DQ7B6" pad="AA18"/>
<connect gate="G" pin="IO_8_DQ8B0" pad="AF18"/>
<connect gate="G" pin="IO_8_DQ8B1" pad="AC18"/>
<connect gate="G" pin="IO_8_DQ8B2" pad="AF17"/>
<connect gate="G" pin="IO_8_DQ8B3" pad="AF19"/>
<connect gate="G" pin="IO_8_DQ8B4" pad="AD19"/>
<connect gate="G" pin="IO_8_DQ8B5" pad="AD18"/>
<connect gate="G" pin="IO_8_DQ8B6" pad="AE19"/>
<connect gate="G" pin="IO_8_DQ8B7" pad="AF20"/>
<connect gate="G" pin="IO_8_DQ9B0" pad="AE20"/>
<connect gate="G" pin="IO_8_DQ9B1" pad="AD20"/>
<connect gate="G" pin="IO_8_DQ9B2" pad="AD21"/>
<connect gate="G" pin="IO_8_DQ9B3" pad="AF21"/>
<connect gate="G" pin="IO_8_DQ9B4" pad="AF22"/>
<connect gate="G" pin="IO_8_DQ9B5" pad="AD22"/>
<connect gate="G" pin="IO_8_DQ9B6" pad="AE22"/>
<connect gate="G" pin="IO_8_DQ9B7" pad="AF23"/>
<connect gate="G" pin="IO_8_DQS6B" pad="AD16"/>
<connect gate="G" pin="IO_8_DQS7B" pad="AA17"/>
<connect gate="G" pin="IO_8_DQS8B" pad="AE18"/>
<connect gate="G" pin="IO_8_DQS9B" pad="AE21"/>
<connect gate="G" pin="NC" pad="AE25"/>
<connect gate="G" pin="NC_10" pad="AA26"/>
<connect gate="G" pin="NC_11" pad="AB10"/>
<connect gate="G" pin="NC_12" pad="AB11"/>
<connect gate="G" pin="NC_13" pad="AB15"/>
<connect gate="G" pin="NC_14" pad="AB19"/>
<connect gate="G" pin="NC_15" pad="AB20"/>
<connect gate="G" pin="NC_16" pad="AB21"/>
<connect gate="G" pin="NC_17" pad="AB22"/>
<connect gate="G" pin="NC_18" pad="AB23"/>
<connect gate="G" pin="NC_19" pad="AB24"/>
<connect gate="G" pin="NC_2" pad="AA15"/>
<connect gate="G" pin="NC_20" pad="AB25"/>
<connect gate="G" pin="NC_21" pad="AB26"/>
<connect gate="G" pin="NC_22" pad="AC10"/>
<connect gate="G" pin="NC_23" pad="AC19"/>
<connect gate="G" pin="NC_24" pad="AC11"/>
<connect gate="G" pin="NC_25" pad="AC20"/>
<connect gate="G" pin="NC_26" pad="AC21"/>
<connect gate="G" pin="NC_27" pad="AC22"/>
<connect gate="G" pin="NC_28" pad="AC23"/>
<connect gate="G" pin="NC_29" pad="AC24"/>
<connect gate="G" pin="NC_3" pad="AA19"/>
<connect gate="G" pin="NC_30" pad="AC25"/>
<connect gate="G" pin="NC_31" pad="AC26"/>
<connect gate="G" pin="NC_32" pad="AD10"/>
<connect gate="G" pin="NC_33" pad="AD11"/>
<connect gate="G" pin="NC_34" pad="AD23"/>
<connect gate="G" pin="NC_35" pad="AD24"/>
<connect gate="G" pin="NC_36" pad="AD25"/>
<connect gate="G" pin="NC_37" pad="AE23"/>
<connect gate="G" pin="NC_38" pad="AE24"/>
<connect gate="G" pin="NC_4" pad="AA20"/>
<connect gate="G" pin="NC_5" pad="AA21"/>
<connect gate="G" pin="NC_6" pad="AA22"/>
<connect gate="G" pin="NC_7" pad="AA23"/>
<connect gate="G" pin="NC_8" pad="AA24"/>
<connect gate="G" pin="NC_9" pad="AA25"/>
<connect gate="G" pin="VCCIO1" pad="AD26"/>
<connect gate="G" pin="VCCIO7" pad="AF12"/>
<connect gate="G" pin="VCCIO8" pad="AF24"/>
<connect gate="G" pin="VCCIO8_2" pad="AF15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1SGX25CF672C7N"/>
<attribute name="OC_FARNELL" value="1549484"/>
<attribute name="OC_NEWARK" value="52R0221"/>
<attribute name="PACKAGE" value="672-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP1SGX40GF1020C6N">
<description>FPGA, STRATIX GX</description>
<gates>
<gate name="A" symbol="EP1SGX40GF1020C6N_A"/>
<gate name="B" symbol="EP1SGX40GF1020C6N_B"/>
<gate name="C" symbol="EP1SGX40GF1020C6N_C"/>
<gate name="D" symbol="EP1SGX40GF1020C6N_D"/>
<gate name="E" symbol="EP1SGX40GF1020C6N_E"/>
<gate name="F" symbol="EP1SGX40GF1020C6N_F"/>
<gate name="G" symbol="EP1SGX40GF1020C6N_G"/>
<gate name="H" symbol="EP1SGX40GF1020C6N_H"/>
<gate name="I" symbol="EP1SGX40GF1020C6N_I"/>
<gate name="J" symbol="EP1SGX40GF1020C6N_J"/>
<gate name="K" symbol="EP1SGX40GF1020C6N_K"/>
</gates>
<devices>
<device name="" package="BGA1020C100P32X32_3300X3300X35">
<connects>
<connect gate="A" pin="GND" pad="F8"/>
<connect gate="A" pin="GND/NC" pad="A4"/>
<connect gate="A" pin="GND/NC_2" pad="D8"/>
<connect gate="A" pin="GND/NC_3" pad="B4"/>
<connect gate="A" pin="GND/NC_4" pad="D6"/>
<connect gate="A" pin="GND/NC_5" pad="A6"/>
<connect gate="A" pin="GND/NC_6" pad="E6"/>
<connect gate="A" pin="GND/NC_7" pad="B6"/>
<connect gate="A" pin="GND/NC_8" pad="E8"/>
<connect gate="A" pin="GND/NC_9" pad="A8"/>
<connect gate="A" pin="GND_2" pad="F7"/>
<connect gate="A" pin="GXB_GND" pad="K5"/>
<connect gate="A" pin="GXB_GND_10" pad="D9"/>
<connect gate="A" pin="GXB_GND_11" pad="G3"/>
<connect gate="A" pin="GXB_GND_12" pad="B7"/>
<connect gate="A" pin="GXB_GND_13" pad="B9"/>
<connect gate="A" pin="GXB_GND_14" pad="E1"/>
<connect gate="A" pin="GXB_GND_15" pad="G6"/>
<connect gate="A" pin="GXB_GND_16" pad="E5"/>
<connect gate="A" pin="GXB_GND_17" pad="E7"/>
<connect gate="A" pin="GXB_GND_18" pad="D7"/>
<connect gate="A" pin="GXB_GND_19" pad="E9"/>
<connect gate="A" pin="GXB_GND_2" pad="A2"/>
<connect gate="A" pin="GXB_GND_20" pad="C2"/>
<connect gate="A" pin="GXB_GND_21" pad="F3"/>
<connect gate="A" pin="GXB_GND_22" pad="A9"/>
<connect gate="A" pin="GXB_GND_23" pad="C3"/>
<connect gate="A" pin="GXB_GND_24" pad="F4"/>
<connect gate="A" pin="GXB_GND_25" pad="H3"/>
<connect gate="A" pin="GXB_GND_26" pad="C4"/>
<connect gate="A" pin="GXB_GND_27" pad="E2"/>
<connect gate="A" pin="GXB_GND_28" pad="F5"/>
<connect gate="A" pin="GXB_GND_29" pad="H4"/>
<connect gate="A" pin="GXB_GND_3" pad="A5"/>
<connect gate="A" pin="GXB_GND_30" pad="C1"/>
<connect gate="A" pin="GXB_GND_31" pad="H5"/>
<connect gate="A" pin="GXB_GND_32" pad="F6"/>
<connect gate="A" pin="GXB_GND_33" pad="L1"/>
<connect gate="A" pin="GXB_GND_34" pad="D3"/>
<connect gate="A" pin="GXB_GND_35" pad="E3"/>
<connect gate="A" pin="GXB_GND_36" pad="H6"/>
<connect gate="A" pin="GXB_GND_37" pad="J1"/>
<connect gate="A" pin="GXB_GND_38" pad="L2"/>
<connect gate="A" pin="GXB_GND_39" pad="C5"/>
<connect gate="A" pin="GXB_GND_4" pad="A7"/>
<connect gate="A" pin="GXB_GND_40" pad="J2"/>
<connect gate="A" pin="GXB_GND_41" pad="J3"/>
<connect gate="A" pin="GXB_GND_42" pad="L3"/>
<connect gate="A" pin="GXB_GND_43" pad="D5"/>
<connect gate="A" pin="GXB_GND_44" pad="J6"/>
<connect gate="A" pin="GXB_GND_45" pad="C6"/>
<connect gate="A" pin="GXB_GND_46" pad="C7"/>
<connect gate="A" pin="GXB_GND_47" pad="K3"/>
<connect gate="A" pin="GXB_GND_48" pad="C8"/>
<connect gate="A" pin="GXB_GND_49" pad="C9"/>
<connect gate="A" pin="GXB_GND_5" pad="A3"/>
<connect gate="A" pin="GXB_GND_50" pad="K4"/>
<connect gate="A" pin="GXB_GND_6" pad="B3"/>
<connect gate="A" pin="GXB_GND_7" pad="G1"/>
<connect gate="A" pin="GXB_GND_8" pad="B5"/>
<connect gate="A" pin="GXB_GND_9" pad="G2"/>
<connect gate="A" pin="GXB_RX4N" pad="D2"/>
<connect gate="A" pin="GXB_RX4P" pad="D1"/>
<connect gate="A" pin="GXB_RX5N" pad="B2"/>
<connect gate="A" pin="GXB_RX5P" pad="B1"/>
<connect gate="A" pin="GXB_RX6N" pad="H2"/>
<connect gate="A" pin="GXB_RX6P" pad="H1"/>
<connect gate="A" pin="GXB_RX7N" pad="K2"/>
<connect gate="A" pin="GXB_RX7P" pad="K1"/>
<connect gate="A" pin="GXB_TX4N" pad="G5"/>
<connect gate="A" pin="GXB_TX4P" pad="G4"/>
<connect gate="A" pin="GXB_TX5N" pad="E4"/>
<connect gate="A" pin="GXB_TX5P" pad="D4"/>
<connect gate="A" pin="GXB_TX6N" pad="J5"/>
<connect gate="A" pin="GXB_TX6P" pad="J4"/>
<connect gate="A" pin="GXB_TX7P" pad="L4"/>
<connect gate="A" pin="IO_4" pad="K7"/>
<connect gate="A" pin="IO_4_2" pad="H7"/>
<connect gate="A" pin="IO_4_DQ0T0" pad="H9"/>
<connect gate="A" pin="IO_4_DQ0T1" pad="J8"/>
<connect gate="A" pin="IO_4_DQ0T2" pad="K8"/>
<connect gate="A" pin="IO_4_DQ0T3" pad="J9"/>
<connect gate="A" pin="IO_4_DQ0T4" pad="K9"/>
<connect gate="A" pin="IO_4_DQ0T5" pad="G9"/>
<connect gate="A" pin="IO_4_DQ0T6" pad="H8"/>
<connect gate="A" pin="IO_4_DQS0T" pad="G8"/>
<connect gate="A" pin="REFCLKB13N" pad="B8"/>
<connect gate="A" pin="REFCLKB14N" pad="F2"/>
<connect gate="A" pin="REFCLKB14P" pad="F1"/>
<connect gate="A" pin="RREFB13" pad="J7"/>
<connect gate="A" pin="VCCG_B13" pad="K6"/>
<connect gate="A" pin="VCCINT" pad="F9"/>
<connect gate="A" pin="VCCIO4" pad="G7"/>
<connect gate="B" pin="GND" pad="P6"/>
<connect gate="B" pin="GND/NC" pad="Y2"/>
<connect gate="B" pin="GND/NC_10" pad="M2"/>
<connect gate="B" pin="GND/NC_11" pad="V2"/>
<connect gate="B" pin="GND/NC_12" pad="U5"/>
<connect gate="B" pin="GND/NC_13" pad="A10"/>
<connect gate="B" pin="GND/NC_14" pad="W4"/>
<connect gate="B" pin="GND/NC_15" pad="R5"/>
<connect gate="B" pin="GND/NC_16" pad="A12"/>
<connect gate="B" pin="GND/NC_17" pad="W5"/>
<connect gate="B" pin="GND/NC_18" pad="Y1"/>
<connect gate="B" pin="GND/NC_2" pad="N4"/>
<connect gate="B" pin="GND/NC_3" pad="M1"/>
<connect gate="B" pin="GND/NC_4" pad="P1"/>
<connect gate="B" pin="GND/NC_5" pad="N5"/>
<connect gate="B" pin="GND/NC_6" pad="P2"/>
<connect gate="B" pin="GND/NC_7" pad="R4"/>
<connect gate="B" pin="GND/NC_8" pad="U4"/>
<connect gate="B" pin="GND/NC_9" pad="V1"/>
<connect gate="B" pin="GND_2" pad="L6"/>
<connect gate="B" pin="GND_3" pad="Y6"/>
<connect gate="B" pin="GND_4" pad="U6"/>
<connect gate="B" pin="GXB_GND" pad="A11"/>
<connect gate="B" pin="GXB_GND_10" pad="P5"/>
<connect gate="B" pin="GXB_GND_11" pad="M3"/>
<connect gate="B" pin="GXB_GND_12" pad="M4"/>
<connect gate="B" pin="GXB_GND_13" pad="M5"/>
<connect gate="B" pin="GXB_GND_14" pad="T3"/>
<connect gate="B" pin="GXB_GND_15" pad="T4"/>
<connect gate="B" pin="GXB_GND_16" pad="V3"/>
<connect gate="B" pin="GXB_GND_17" pad="U1"/>
<connect gate="B" pin="GXB_GND_18" pad="V4"/>
<connect gate="B" pin="GXB_GND_19" pad="T5"/>
<connect gate="B" pin="GXB_GND_2" pad="N1"/>
<connect gate="B" pin="GXB_GND_20" pad="V5"/>
<connect gate="B" pin="GXB_GND_21" pad="U2"/>
<connect gate="B" pin="GXB_GND_22" pad="U3"/>
<connect gate="B" pin="GXB_GND_23" pad="W1"/>
<connect gate="B" pin="GXB_GND_24" pad="W2"/>
<connect gate="B" pin="GXB_GND_25" pad="W3"/>
<connect gate="B" pin="GXB_GND_26" pad="Y3"/>
<connect gate="B" pin="GXB_GND_27" pad="Y4"/>
<connect gate="B" pin="GXB_GND_28" pad="Y5"/>
<connect gate="B" pin="GXB_GND_3" pad="P3"/>
<connect gate="B" pin="GXB_GND_4" pad="R1"/>
<connect gate="B" pin="GXB_GND_5" pad="N2"/>
<connect gate="B" pin="GXB_GND_6" pad="R2"/>
<connect gate="B" pin="GXB_GND_7" pad="P4"/>
<connect gate="B" pin="GXB_GND_8" pad="R3"/>
<connect gate="B" pin="GXB_GND_9" pad="N3"/>
<connect gate="B" pin="GXB_TX7N" pad="L5"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_4_DQ0T7" pad="L9"/>
<connect gate="B" pin="IO_4_DQ4T1" pad="A15"/>
<connect gate="B" pin="IO_4_DQ4T2" pad="A14"/>
<connect gate="B" pin="REFCLKB17N" pad="T2"/>
<connect gate="B" pin="REFCLKB17P" pad="T1"/>
<connect gate="B" pin="RREFB14" pad="L7"/>
<connect gate="B" pin="RREFB15" pad="T8"/>
<connect gate="B" pin="RREFB17" pad="T7"/>
<connect gate="B" pin="VCCA_B14" pad="R6"/>
<connect gate="B" pin="VCCA_B14_2" pad="M6"/>
<connect gate="B" pin="VCCA_B15" pad="V6"/>
<connect gate="B" pin="VCCG_B14" pad="N6"/>
<connect gate="B" pin="VCCG_B15" pad="W6"/>
<connect gate="B" pin="VCCG_B15_2" pad="T6"/>
<connect gate="B" pin="VCCINT" pad="T9"/>
<connect gate="B" pin="VCCIO4" pad="A16"/>
<connect gate="B" pin="VCCIO4_2" pad="A13"/>
<connect gate="B" pin="VCCP_B14" pad="R9"/>
<connect gate="B" pin="VCCP_B14_2" pad="M9"/>
<connect gate="B" pin="VCCP_B14_3" pad="N9"/>
<connect gate="B" pin="VCCP_B14_4" pad="P9"/>
<connect gate="B" pin="VCCP_B15" pad="Y9"/>
<connect gate="B" pin="VCCP_B15_2" pad="V9"/>
<connect gate="B" pin="VCCP_B15_3" pad="U9"/>
<connect gate="B" pin="VCCP_B15_4" pad="W9"/>
<connect gate="B" pin="VCCR_B14" pad="R8"/>
<connect gate="B" pin="VCCR_B14_2" pad="M8"/>
<connect gate="B" pin="VCCR_B14_3" pad="N8"/>
<connect gate="B" pin="VCCR_B14_4" pad="P8"/>
<connect gate="B" pin="VCCR_B15" pad="Y8"/>
<connect gate="B" pin="VCCR_B15_2" pad="V8"/>
<connect gate="B" pin="VCCR_B15_3" pad="U8"/>
<connect gate="B" pin="VCCR_B15_4" pad="W8"/>
<connect gate="B" pin="VCCT_B14" pad="R7"/>
<connect gate="B" pin="VCCT_B14_2" pad="M7"/>
<connect gate="B" pin="VCCT_B14_3" pad="N7"/>
<connect gate="B" pin="VCCT_B14_4" pad="P7"/>
<connect gate="B" pin="VCCT_B15" pad="Y7"/>
<connect gate="B" pin="VCCT_B15_2" pad="V7"/>
<connect gate="B" pin="VCCT_B15_3" pad="U7"/>
<connect gate="B" pin="VCCT_B15_4" pad="W7"/>
<connect gate="C" pin="GND" pad="AG9"/>
<connect gate="C" pin="GND/NC" pad="AH7"/>
<connect gate="C" pin="GND/NC_2" pad="AH9"/>
<connect gate="C" pin="GND/NC_3" pad="AJ4"/>
<connect gate="C" pin="GND/NC_4" pad="AJ5"/>
<connect gate="C" pin="GND_2" pad="A31"/>
<connect gate="C" pin="GND_3" pad="AB6"/>
<connect gate="C" pin="GND_4" pad="AE7"/>
<connect gate="C" pin="GND_5" pad="AG6"/>
<connect gate="C" pin="GND_6" pad="AF6"/>
<connect gate="C" pin="GND_7" pad="AG7"/>
<connect gate="C" pin="GND_8" pad="A20"/>
<connect gate="C" pin="GND_9" pad="AG8"/>
<connect gate="C" pin="GXB_GND" pad="AJ6"/>
<connect gate="C" pin="GXB_GND_10" pad="AD4"/>
<connect gate="C" pin="GXB_GND_11" pad="AC2"/>
<connect gate="C" pin="GXB_GND_12" pad="AD5"/>
<connect gate="C" pin="GXB_GND_13" pad="AC3"/>
<connect gate="C" pin="GXB_GND_14" pad="AE1"/>
<connect gate="C" pin="GXB_GND_15" pad="AE2"/>
<connect gate="C" pin="GXB_GND_16" pad="AE3"/>
<connect gate="C" pin="GXB_GND_17" pad="AE6"/>
<connect gate="C" pin="GXB_GND_18" pad="AF3"/>
<connect gate="C" pin="GXB_GND_19" pad="AF4"/>
<connect gate="C" pin="GXB_GND_2" pad="AA1"/>
<connect gate="C" pin="GXB_GND_20" pad="AF5"/>
<connect gate="C" pin="GXB_GND_21" pad="AH3"/>
<connect gate="C" pin="GXB_GND_22" pad="AG1"/>
<connect gate="C" pin="GXB_GND_23" pad="AH4"/>
<connect gate="C" pin="GXB_GND_24" pad="AG2"/>
<connect gate="C" pin="GXB_GND_25" pad="AH5"/>
<connect gate="C" pin="GXB_GND_26" pad="AG3"/>
<connect gate="C" pin="GXB_GND_27" pad="AH6"/>
<connect gate="C" pin="GXB_GND_28" pad="AJ1"/>
<connect gate="C" pin="GXB_GND_29" pad="AJ2"/>
<connect gate="C" pin="GXB_GND_3" pad="AA2"/>
<connect gate="C" pin="GXB_GND_30" pad="AH8"/>
<connect gate="C" pin="GXB_GND_31" pad="AJ3"/>
<connect gate="C" pin="GXB_GND_4" pad="AA3"/>
<connect gate="C" pin="GXB_GND_5" pad="AB3"/>
<connect gate="C" pin="GXB_GND_6" pad="AB4"/>
<connect gate="C" pin="GXB_GND_7" pad="AB5"/>
<connect gate="C" pin="GXB_GND_8" pad="AD3"/>
<connect gate="C" pin="GXB_GND_9" pad="AC1"/>
<connect gate="C" pin="GXB_RX10N" pad="AH2"/>
<connect gate="C" pin="GXB_RX10P" pad="AH1"/>
<connect gate="C" pin="GXB_RX8N" pad="AD2"/>
<connect gate="C" pin="GXB_RX8P" pad="AD1"/>
<connect gate="C" pin="GXB_RX9N" pad="AB2"/>
<connect gate="C" pin="GXB_RX9P" pad="AB1"/>
<connect gate="C" pin="GXB_TX10N" pad="AE5"/>
<connect gate="C" pin="GXB_TX10P" pad="AE4"/>
<connect gate="C" pin="GXB_TX11N" pad="AG5"/>
<connect gate="C" pin="GXB_TX11P" pad="AG4"/>
<connect gate="C" pin="GXB_TX8N" pad="AC5"/>
<connect gate="C" pin="GXB_TX8P" pad="AC4"/>
<connect gate="C" pin="GXB_TX9N" pad="AA5"/>
<connect gate="C" pin="GXB_TX9P" pad="AA4"/>
<connect gate="C" pin="IO_10_PLL5_OUT2N" pad="A17"/>
<connect gate="C" pin="IO_3_CLK14N" pad="A18"/>
<connect gate="C" pin="IO_3_DQ6T2" pad="A21"/>
<connect gate="C" pin="IO_3_DQ6T3" pad="A22"/>
<connect gate="C" pin="IO_3_DQ7T0" pad="A23"/>
<connect gate="C" pin="IO_3_DQ7T4" pad="A24"/>
<connect gate="C" pin="IO_3_DQ8T0" pad="A25"/>
<connect gate="C" pin="IO_3_DQ8T3" pad="A26"/>
<connect gate="C" pin="IO_3_DQ9T0" pad="A27"/>
<connect gate="C" pin="IO_3_DQ9T5" pad="A29"/>
<connect gate="C" pin="IO_3_DQS9T" pad="A28"/>
<connect gate="C" pin="IO_7" pad="AD7"/>
<connect gate="C" pin="IO_7_DQ0B0" pad="AE9"/>
<connect gate="C" pin="IO_7_DQ0B1" pad="AD9"/>
<connect gate="C" pin="IO_7_DQ0B2" pad="AD8"/>
<connect gate="C" pin="IO_7_DQ0B3" pad="AE8"/>
<connect gate="C" pin="IO_7_DQ0B4" pad="AC8"/>
<connect gate="C" pin="IO_7_DQ0B6" pad="AF8"/>
<connect gate="C" pin="IO_7_DQ0B7" pad="AC9"/>
<connect gate="C" pin="IO_7_DQS0B" pad="AF9"/>
<connect gate="C" pin="REFCLKB15N" pad="AF2"/>
<connect gate="C" pin="REFCLKB15P" pad="AF1"/>
<connect gate="C" pin="RREFB16" pad="AC7"/>
<connect gate="C" pin="VCCA_B15" pad="AD6"/>
<connect gate="C" pin="VCCA_B15_2" pad="AA6"/>
<connect gate="C" pin="VCCG_B15" pad="AC6"/>
<connect gate="C" pin="VCCIO3" pad="A19"/>
<connect gate="C" pin="VCCIO3_2" pad="A30"/>
<connect gate="C" pin="VCCIO7" pad="AF7"/>
<connect gate="C" pin="VCCP_B15" pad="AA9"/>
<connect gate="C" pin="VCCP_B15_2" pad="AB9"/>
<connect gate="C" pin="VCCR_B15" pad="AA8"/>
<connect gate="C" pin="VCCR_B15_2" pad="AB8"/>
<connect gate="C" pin="VCCT_B15" pad="AA7"/>
<connect gate="C" pin="VCCT_B15_2" pad="AB7"/>
<connect gate="D" pin="CLK12P" pad="D16"/>
<connect gate="D" pin="CLK14P" pad="B18"/>
<connect gate="D" pin="CLK15P" pad="C19"/>
<connect gate="D" pin="GND" pad="D13"/>
<connect gate="D" pin="GND/NC" pad="AL5"/>
<connect gate="D" pin="GND/NC_10" pad="B12"/>
<connect gate="D" pin="GND/NC_11" pad="D10"/>
<connect gate="D" pin="GND/NC_12" pad="B10"/>
<connect gate="D" pin="GND/NC_2" pad="AL9"/>
<connect gate="D" pin="GND/NC_3" pad="AJ7"/>
<connect gate="D" pin="GND/NC_4" pad="AJ9"/>
<connect gate="D" pin="GND/NC_5" pad="AM2"/>
<connect gate="D" pin="GND/NC_6" pad="AM5"/>
<connect gate="D" pin="GND/NC_7" pad="AM9"/>
<connect gate="D" pin="GND/NC_8" pad="AM3"/>
<connect gate="D" pin="GND/NC_9" pad="D12"/>
<connect gate="D" pin="GND_2" pad="B13"/>
<connect gate="D" pin="GND_3" pad="B32"/>
<connect gate="D" pin="GND_4" pad="C13"/>
<connect gate="D" pin="GND_5" pad="B16"/>
<connect gate="D" pin="GXB_GND" pad="D11"/>
<connect gate="D" pin="GXB_GND_10" pad="AK7"/>
<connect gate="D" pin="GXB_GND_11" pad="AL3"/>
<connect gate="D" pin="GXB_GND_12" pad="AK8"/>
<connect gate="D" pin="GXB_GND_13" pad="AL4"/>
<connect gate="D" pin="GXB_GND_14" pad="AK9"/>
<connect gate="D" pin="GXB_GND_15" pad="AL6"/>
<connect gate="D" pin="GXB_GND_16" pad="AL1"/>
<connect gate="D" pin="GXB_GND_17" pad="B11"/>
<connect gate="D" pin="GXB_GND_18" pad="AL8"/>
<connect gate="D" pin="GXB_GND_19" pad="C10"/>
<connect gate="D" pin="GXB_GND_2" pad="AK3"/>
<connect gate="D" pin="GXB_GND_20" pad="C11"/>
<connect gate="D" pin="GXB_GND_21" pad="C12"/>
<connect gate="D" pin="GXB_GND_22" pad="AM4"/>
<connect gate="D" pin="GXB_GND_3" pad="AK4"/>
<connect gate="D" pin="GXB_GND_4" pad="AJ8"/>
<connect gate="D" pin="GXB_GND_5" pad="AM6"/>
<connect gate="D" pin="GXB_GND_6" pad="AK5"/>
<connect gate="D" pin="GXB_GND_7" pad="AL2"/>
<connect gate="D" pin="GXB_GND_8" pad="AK6"/>
<connect gate="D" pin="GXB_GND_9" pad="AM8"/>
<connect gate="D" pin="GXB_RX11N" pad="AK2"/>
<connect gate="D" pin="GXB_RX11P" pad="AK1"/>
<connect gate="D" pin="IO_10_PLL5_OUT2P" pad="B17"/>
<connect gate="D" pin="IO_10_PLL5_OUT3N" pad="C18"/>
<connect gate="D" pin="IO_10_PLL5_OUT3P" pad="D18"/>
<connect gate="D" pin="IO_3" pad="D27"/>
<connect gate="D" pin="IO_3_2" pad="B30"/>
<connect gate="D" pin="IO_3_3" pad="B31"/>
<connect gate="D" pin="IO_3_4" pad="C30"/>
<connect gate="D" pin="IO_3_5" pad="C31"/>
<connect gate="D" pin="IO_3_CLK15N" pad="B19"/>
<connect gate="D" pin="IO_3_DQ5T3" pad="D19"/>
<connect gate="D" pin="IO_3_DQ5T4" pad="B20"/>
<connect gate="D" pin="IO_3_DQ5T5" pad="C20"/>
<connect gate="D" pin="IO_3_DQ5T6" pad="D20"/>
<connect gate="D" pin="IO_3_DQ6T0" pad="C21"/>
<connect gate="D" pin="IO_3_DQ6T1" pad="D21"/>
<connect gate="D" pin="IO_3_DQ6T4" pad="C22"/>
<connect gate="D" pin="IO_3_DQ6T5" pad="D22"/>
<connect gate="D" pin="IO_3_DQ6T6" pad="B22"/>
<connect gate="D" pin="IO_3_DQ7T1" pad="B23"/>
<connect gate="D" pin="IO_3_DQ7T2" pad="C23"/>
<connect gate="D" pin="IO_3_DQ7T5" pad="B24"/>
<connect gate="D" pin="IO_3_DQ7T6" pad="C24"/>
<connect gate="D" pin="IO_3_DQ7T7" pad="D24"/>
<connect gate="D" pin="IO_3_DQ8T1" pad="B25"/>
<connect gate="D" pin="IO_3_DQ8T2" pad="C25"/>
<connect gate="D" pin="IO_3_DQ8T5" pad="B26"/>
<connect gate="D" pin="IO_3_DQ8T6" pad="C26"/>
<connect gate="D" pin="IO_3_DQ8T7" pad="D26"/>
<connect gate="D" pin="IO_3_DQ9T1" pad="B27"/>
<connect gate="D" pin="IO_3_DQ9T2" pad="C27"/>
<connect gate="D" pin="IO_3_DQ9T3" pad="B28"/>
<connect gate="D" pin="IO_3_DQ9T4" pad="C28"/>
<connect gate="D" pin="IO_3_DQ9T6" pad="B29"/>
<connect gate="D" pin="IO_3_DQ9T7" pad="C29"/>
<connect gate="D" pin="IO_3_DQS6T" pad="B21"/>
<connect gate="D" pin="IO_3_DQS7T" pad="D23"/>
<connect gate="D" pin="IO_3_DQS8T" pad="D25"/>
<connect gate="D" pin="IO_4_CLK12N" pad="C16"/>
<connect gate="D" pin="IO_4_DQ3T1" pad="D14"/>
<connect gate="D" pin="IO_4_DQ4T0" pad="C14"/>
<connect gate="D" pin="IO_4_DQ4T3" pad="B15"/>
<connect gate="D" pin="IO_4_DQ4T4" pad="C15"/>
<connect gate="D" pin="IO_4_DQ4T6" pad="D15"/>
<connect gate="D" pin="IO_4_DQS4T" pad="B14"/>
<connect gate="D" pin="IO_9_PLL5_OUT1N" pad="C17"/>
<connect gate="D" pin="IO_9_PLL5_OUT1P" pad="D17"/>
<connect gate="D" pin="REFCLKB16N" pad="AL7"/>
<connect gate="D" pin="REFCLKB16P" pad="AM7"/>
<connect gate="D" pin="VCCIO2" pad="C32"/>
<connect gate="E" pin="CLK13P" pad="F16"/>
<connect gate="E" pin="FPLL7CLKN" pad="E30"/>
<connect gate="E" pin="FPLL7CLKP" pad="E29"/>
<connect gate="E" pin="GND" pad="F12"/>
<connect gate="E" pin="GND/NC" pad="E12"/>
<connect gate="E" pin="GND/NC_2" pad="E10"/>
<connect gate="E" pin="GND_2" pad="E13"/>
<connect gate="E" pin="GND_3" pad="F10"/>
<connect gate="E" pin="GXB_GND" pad="E11"/>
<connect gate="E" pin="IN_2_DIFFIO_RX38N" pad="G32"/>
<connect gate="E" pin="IN_2_DIFFIO_RX38P" pad="G31"/>
<connect gate="E" pin="IN_2_DIFFIO_RX39N" pad="G30"/>
<connect gate="E" pin="IN_2_DIFFIO_RX39P" pad="G29"/>
<connect gate="E" pin="IN_2_DIFFIO_RX40N" pad="F32"/>
<connect gate="E" pin="IN_2_DIFFIO_RX40P" pad="F31"/>
<connect gate="E" pin="IN_2_DIFFIO_RX41N" pad="E32"/>
<connect gate="E" pin="IN_2_DIFFIO_RX41P" pad="E31"/>
<connect gate="E" pin="IN_2_DIFFIO_RX42N" pad="F30"/>
<connect gate="E" pin="IN_2_DIFFIO_RX42P" pad="F29"/>
<connect gate="E" pin="IN_2_DIFFIO_RX43N" pad="D32"/>
<connect gate="E" pin="IN_2_DIFFIO_RX43P" pad="D31"/>
<connect gate="E" pin="IN_2_DIFFIO_RX44N" pad="D30"/>
<connect gate="E" pin="IN_2_DIFFIO_RX44P" pad="D29"/>
<connect gate="E" pin="IO_2_DIFFIO_TX39N" pad="H25"/>
<connect gate="E" pin="IO_2_DIFFIO_TX39P" pad="H24"/>
<connect gate="E" pin="IO_2_DIFFIO_TX40N" pad="H27"/>
<connect gate="E" pin="IO_2_DIFFIO_TX40P" pad="H26"/>
<connect gate="E" pin="IO_2_DIFFIO_TX41N" pad="H28"/>
<connect gate="E" pin="IO_2_DIFFIO_TX42N" pad="G26"/>
<connect gate="E" pin="IO_2_DIFFIO_TX42P" pad="G25"/>
<connect gate="E" pin="IO_2_DIFFIO_TX43N" pad="G28"/>
<connect gate="E" pin="IO_2_DIFFIO_TX43P" pad="G27"/>
<connect gate="E" pin="IO_2_DIFFIO_TX44N" pad="F28"/>
<connect gate="E" pin="IO_2_DIFFIO_TX44P" pad="F27"/>
<connect gate="E" pin="IO_3" pad="H23"/>
<connect gate="E" pin="IO_3_10" pad="F24"/>
<connect gate="E" pin="IO_3_11" pad="F25"/>
<connect gate="E" pin="IO_3_12" pad="F26"/>
<connect gate="E" pin="IO_3_13" pad="G20"/>
<connect gate="E" pin="IO_3_14" pad="G23"/>
<connect gate="E" pin="IO_3_15" pad="G24"/>
<connect gate="E" pin="IO_3_16" pad="H20"/>
<connect gate="E" pin="IO_3_2" pad="D28"/>
<connect gate="E" pin="IO_3_3" pad="E24"/>
<connect gate="E" pin="IO_3_4" pad="E26"/>
<connect gate="E" pin="IO_3_5" pad="E27"/>
<connect gate="E" pin="IO_3_6" pad="E28"/>
<connect gate="E" pin="IO_3_7" pad="F21"/>
<connect gate="E" pin="IO_3_8" pad="F22"/>
<connect gate="E" pin="IO_3_9" pad="F23"/>
<connect gate="E" pin="IO_3_DQ5T0" pad="E19"/>
<connect gate="E" pin="IO_3_DQ5T1" pad="F19"/>
<connect gate="E" pin="IO_3_DQ5T2" pad="E20"/>
<connect gate="E" pin="IO_3_DQ5T7" pad="E21"/>
<connect gate="E" pin="IO_3_DQ6T7" pad="E22"/>
<connect gate="E" pin="IO_3_DQ7T3" pad="E23"/>
<connect gate="E" pin="IO_3_DQ8T4" pad="E25"/>
<connect gate="E" pin="IO_3_DQS5T" pad="F20"/>
<connect gate="E" pin="IO_3_FCLK0" pad="G22"/>
<connect gate="E" pin="IO_3_FCLK1" pad="H22"/>
<connect gate="E" pin="IO_3_RDN3" pad="G21"/>
<connect gate="E" pin="IO_3_RUP3" pad="H21"/>
<connect gate="E" pin="IO_4" pad="H18"/>
<connect gate="E" pin="IO_4_2" pad="G17"/>
<connect gate="E" pin="IO_4_3" pad="G18"/>
<connect gate="E" pin="IO_4_4" pad="G19"/>
<connect gate="E" pin="IO_4_5" pad="H17"/>
<connect gate="E" pin="IO_4_CLK13N/PLL11_OUT" pad="E16"/>
<connect gate="E" pin="IO_4_DQ1T2" pad="G10"/>
<connect gate="E" pin="IO_4_DQ1T4" pad="H11"/>
<connect gate="E" pin="IO_4_DQ1T7" pad="G11"/>
<connect gate="E" pin="IO_4_DQ2T2" pad="G12"/>
<connect gate="E" pin="IO_4_DQ2T4" pad="H13"/>
<connect gate="E" pin="IO_4_DQ3T0" pad="G13"/>
<connect gate="E" pin="IO_4_DQ3T2" pad="F14"/>
<connect gate="E" pin="IO_4_DQ3T3" pad="E14"/>
<connect gate="E" pin="IO_4_DQ3T4" pad="H14"/>
<connect gate="E" pin="IO_4_DQ3T6" pad="G15"/>
<connect gate="E" pin="IO_4_DQ3T7" pad="H15"/>
<connect gate="E" pin="IO_4_DQ4T5" pad="F15"/>
<connect gate="E" pin="IO_4_DQ4T7" pad="E15"/>
<connect gate="E" pin="IO_4_DQS1T" pad="H10"/>
<connect gate="E" pin="IO_4_DQS2T" pad="H12"/>
<connect gate="E" pin="IO_4_DQS3T" pad="G14"/>
<connect gate="E" pin="IO_4_RUP4" pad="H19"/>
<connect gate="E" pin="IO_9_PLL5_FBN" pad="E17"/>
<connect gate="E" pin="IO_9_PLL5_FBP" pad="F17"/>
<connect gate="E" pin="IO_9_PLL5_OUT0N" pad="E18"/>
<connect gate="E" pin="IO_9_PLL5_OUT0P" pad="F18"/>
<connect gate="E" pin="TDI" pad="H16"/>
<connect gate="E" pin="TMS" pad="G16"/>
<connect gate="E" pin="VCCINT" pad="F11"/>
<connect gate="E" pin="VCCINT_2" pad="F13"/>
<connect gate="F" pin="CONF_DONE" pad="K21"/>
<connect gate="F" pin="DCLK" pad="J20"/>
<connect gate="F" pin="GND" pad="K22"/>
<connect gate="F" pin="GNDA_PLL11" pad="L16"/>
<connect gate="F" pin="GNDA_PLL5" pad="L17"/>
<connect gate="F" pin="GNDA_PLL7" pad="K27"/>
<connect gate="F" pin="GNDG_PLL11" pad="M16"/>
<connect gate="F" pin="GNDG_PLL5" pad="M17"/>
<connect gate="F" pin="GNDG_PLL7" pad="K26"/>
<connect gate="F" pin="IN_2_DIFFIO_RX28N" pad="K32"/>
<connect gate="F" pin="IN_2_DIFFIO_RX28P" pad="K31"/>
<connect gate="F" pin="IN_2_DIFFIO_RX30P" pad="M29"/>
<connect gate="F" pin="IN_2_DIFFIO_RX31N" pad="L32"/>
<connect gate="F" pin="IN_2_DIFFIO_RX31P" pad="L31"/>
<connect gate="F" pin="IN_2_DIFFIO_RX32N/RDN2" pad="L30"/>
<connect gate="F" pin="IN_2_DIFFIO_RX32P/RUP2" pad="L29"/>
<connect gate="F" pin="IN_2_DIFFIO_RX33N" pad="J30"/>
<connect gate="F" pin="IN_2_DIFFIO_RX33P" pad="J29"/>
<connect gate="F" pin="IN_2_DIFFIO_RX34N" pad="J32"/>
<connect gate="F" pin="IN_2_DIFFIO_RX34P" pad="J31"/>
<connect gate="F" pin="IN_2_DIFFIO_RX35N" pad="H32"/>
<connect gate="F" pin="IN_2_DIFFIO_RX35P" pad="H31"/>
<connect gate="F" pin="IN_2_DIFFIO_RX36N" pad="K30"/>
<connect gate="F" pin="IN_2_DIFFIO_RX36P" pad="K29"/>
<connect gate="F" pin="IN_2_DIFFIO_RX37N" pad="H30"/>
<connect gate="F" pin="IN_2_DIFFIO_RX37P" pad="H29"/>
<connect gate="F" pin="IO_2_DIFFIO_TX23N" pad="L23"/>
<connect gate="F" pin="IO_2_DIFFIO_TX23P" pad="M23"/>
<connect gate="F" pin="IO_2_DIFFIO_TX24N" pad="J23"/>
<connect gate="F" pin="IO_2_DIFFIO_TX24P" pad="K23"/>
<connect gate="F" pin="IO_2_DIFFIO_TX32N" pad="M28"/>
<connect gate="F" pin="IO_2_DIFFIO_TX32P" pad="M27"/>
<connect gate="F" pin="IO_2_DIFFIO_TX33N" pad="M26"/>
<connect gate="F" pin="IO_2_DIFFIO_TX33P" pad="M25"/>
<connect gate="F" pin="IO_2_DIFFIO_TX34N" pad="L27"/>
<connect gate="F" pin="IO_2_DIFFIO_TX34P" pad="L26"/>
<connect gate="F" pin="IO_2_DIFFIO_TX35N" pad="L25"/>
<connect gate="F" pin="IO_2_DIFFIO_TX35P" pad="L24"/>
<connect gate="F" pin="IO_2_DIFFIO_TX36N" pad="K25"/>
<connect gate="F" pin="IO_2_DIFFIO_TX36P" pad="K24"/>
<connect gate="F" pin="IO_2_DIFFIO_TX37N" pad="J25"/>
<connect gate="F" pin="IO_2_DIFFIO_TX37P" pad="J24"/>
<connect gate="F" pin="IO_2_DIFFIO_TX38N" pad="K28"/>
<connect gate="F" pin="IO_2_DIFFIO_TX38P" pad="L28"/>
<connect gate="F" pin="IO_2_DIFFIO_TX41P" pad="J28"/>
<connect gate="F" pin="IO_3" pad="J22"/>
<connect gate="F" pin="IO_3_2" pad="J21"/>
<connect gate="F" pin="IO_4" pad="M15"/>
<connect gate="F" pin="IO_4_10" pad="M11"/>
<connect gate="F" pin="IO_4_11" pad="M12"/>
<connect gate="F" pin="IO_4_2" pad="J18"/>
<connect gate="F" pin="IO_4_3" pad="J19"/>
<connect gate="F" pin="IO_4_4" pad="K19"/>
<connect gate="F" pin="IO_4_5" pad="L10"/>
<connect gate="F" pin="IO_4_6" pad="L14"/>
<connect gate="F" pin="IO_4_7" pad="L15"/>
<connect gate="F" pin="IO_4_8" pad="L19"/>
<connect gate="F" pin="IO_4_9" pad="M10"/>
<connect gate="F" pin="IO_4_DEV_OE" pad="M14"/>
<connect gate="F" pin="IO_4_DQ1T0" pad="J10"/>
<connect gate="F" pin="IO_4_DQ1T1" pad="K10"/>
<connect gate="F" pin="IO_4_DQ1T3" pad="K11"/>
<connect gate="F" pin="IO_4_DQ1T5" pad="J11"/>
<connect gate="F" pin="IO_4_DQ1T6" pad="L11"/>
<connect gate="F" pin="IO_4_DQ2T0" pad="J12"/>
<connect gate="F" pin="IO_4_DQ2T1" pad="K12"/>
<connect gate="F" pin="IO_4_DQ2T3" pad="L12"/>
<connect gate="F" pin="IO_4_DQ2T5" pad="J13"/>
<connect gate="F" pin="IO_4_DQ2T6" pad="L13"/>
<connect gate="F" pin="IO_4_DQ2T7" pad="K13"/>
<connect gate="F" pin="IO_4_DQ3T5" pad="J14"/>
<connect gate="F" pin="IO_4_FCLK6" pad="M13"/>
<connect gate="F" pin="IO_4_RDN4" pad="K14"/>
<connect gate="F" pin="NCONFIG" pad="K20"/>
<connect gate="F" pin="NSTATUS" pad="L22"/>
<connect gate="F" pin="TCK" pad="K15"/>
<connect gate="F" pin="TDO" pad="J16"/>
<connect gate="F" pin="TEMPDIODEN" pad="L20"/>
<connect gate="F" pin="TEMPDIODEP" pad="L21"/>
<connect gate="F" pin="TRST" pad="J15"/>
<connect gate="F" pin="VCCA_PLL11" pad="K16"/>
<connect gate="F" pin="VCCA_PLL5" pad="L18"/>
<connect gate="F" pin="VCCA_PLL7" pad="J27"/>
<connect gate="F" pin="VCCG_PLL11" pad="J17"/>
<connect gate="F" pin="VCCG_PLL5" pad="K17"/>
<connect gate="F" pin="VCCG_PLL7" pad="J26"/>
<connect gate="F" pin="VCC_PLL5_OUTA" pad="K18"/>
<connect gate="F" pin="VCC_PLL5_OUTB" pad="M18"/>
<connect gate="F" pin="VREF0B2" pad="M24"/>
<connect gate="F" pin="VREF0B3" pad="M19"/>
<connect gate="F" pin="VREF1B3" pad="M20"/>
<connect gate="F" pin="VREF2B3" pad="M21"/>
<connect gate="F" pin="VREF3B3" pad="M22"/>
<connect gate="G" pin="CLK1P" pad="T29"/>
<connect gate="G" pin="GND" pad="R19"/>
<connect gate="G" pin="GNDA_PLL1" pad="T28"/>
<connect gate="G" pin="GNDG_PLL1" pad="T26"/>
<connect gate="G" pin="GND_10" pad="R17"/>
<connect gate="G" pin="GND_11" pad="T20"/>
<connect gate="G" pin="GND_12" pad="T10"/>
<connect gate="G" pin="GND_13" pad="T22"/>
<connect gate="G" pin="GND_2" pad="N22"/>
<connect gate="G" pin="GND_3" pad="N20"/>
<connect gate="G" pin="GND_4" pad="P16"/>
<connect gate="G" pin="GND_5" pad="T16"/>
<connect gate="G" pin="GND_6" pad="P32"/>
<connect gate="G" pin="GND_7" pad="N24"/>
<connect gate="G" pin="GND_8" pad="T18"/>
<connect gate="G" pin="GND_9" pad="P18"/>
<connect gate="G" pin="IN_2_DIFFIO_RX23N" pad="R30"/>
<connect gate="G" pin="IN_2_DIFFIO_RX23P" pad="R29"/>
<connect gate="G" pin="IN_2_DIFFIO_RX24N" pad="R31"/>
<connect gate="G" pin="IN_2_DIFFIO_RX24P" pad="P31"/>
<connect gate="G" pin="IN_2_DIFFIO_RX25N" pad="N32"/>
<connect gate="G" pin="IN_2_DIFFIO_RX25P" pad="N31"/>
<connect gate="G" pin="IN_2_DIFFIO_RX26N" pad="P30"/>
<connect gate="G" pin="IN_2_DIFFIO_RX26P" pad="P29"/>
<connect gate="G" pin="IN_2_DIFFIO_RX27N" pad="M32"/>
<connect gate="G" pin="IN_2_DIFFIO_RX27P" pad="M31"/>
<connect gate="G" pin="IN_2_DIFFIO_RX29N" pad="N30"/>
<connect gate="G" pin="IN_2_DIFFIO_RX29P" pad="N29"/>
<connect gate="G" pin="IN_2_DIFFIO_RX30N" pad="M30"/>
<connect gate="G" pin="IO_1_DIFFIO_TX22P" pad="T23"/>
<connect gate="G" pin="IO_2_CLK1N" pad="T30"/>
<connect gate="G" pin="IO_2_DIFFIO_TX25N" pad="R26"/>
<connect gate="G" pin="IO_2_DIFFIO_TX25P" pad="R25"/>
<connect gate="G" pin="IO_2_DIFFIO_TX26N" pad="R28"/>
<connect gate="G" pin="IO_2_DIFFIO_TX26P" pad="R27"/>
<connect gate="G" pin="IO_2_DIFFIO_TX27N" pad="P28"/>
<connect gate="G" pin="IO_2_DIFFIO_TX27P" pad="P27"/>
<connect gate="G" pin="IO_2_DIFFIO_TX28N" pad="R24"/>
<connect gate="G" pin="IO_2_DIFFIO_TX28P" pad="P24"/>
<connect gate="G" pin="IO_2_DIFFIO_TX29N" pad="P26"/>
<connect gate="G" pin="IO_2_DIFFIO_TX29P" pad="P25"/>
<connect gate="G" pin="IO_2_DIFFIO_TX30N" pad="N28"/>
<connect gate="G" pin="IO_2_DIFFIO_TX30P" pad="N27"/>
<connect gate="G" pin="IO_2_DIFFIO_TX31N" pad="N26"/>
<connect gate="G" pin="IO_2_DIFFIO_TX31P" pad="N25"/>
<connect gate="G" pin="IO_4" pad="T13"/>
<connect gate="G" pin="IO_4_10" pad="P13"/>
<connect gate="G" pin="IO_4_11" pad="P14"/>
<connect gate="G" pin="IO_4_12" pad="R10"/>
<connect gate="G" pin="IO_4_13" pad="R11"/>
<connect gate="G" pin="IO_4_14" pad="R12"/>
<connect gate="G" pin="IO_4_15" pad="R13"/>
<connect gate="G" pin="IO_4_16" pad="R14"/>
<connect gate="G" pin="IO_4_17" pad="T12"/>
<connect gate="G" pin="IO_4_2" pad="N10"/>
<connect gate="G" pin="IO_4_3" pad="N11"/>
<connect gate="G" pin="IO_4_4" pad="N14"/>
<connect gate="G" pin="IO_4_5" pad="N17"/>
<connect gate="G" pin="IO_4_6" pad="N18"/>
<connect gate="G" pin="IO_4_7" pad="P10"/>
<connect gate="G" pin="IO_4_8" pad="P11"/>
<connect gate="G" pin="IO_4_9" pad="P12"/>
<connect gate="G" pin="IO_4_FCLK7" pad="T14"/>
<connect gate="G" pin="VCCA_PLL1" pad="T27"/>
<connect gate="G" pin="VCCG_PLL1" pad="T25"/>
<connect gate="G" pin="VCCINT" pad="T17"/>
<connect gate="G" pin="VCCINT_10" pad="R22"/>
<connect gate="G" pin="VCCINT_11" pad="R15"/>
<connect gate="G" pin="VCCINT_12" pad="T19"/>
<connect gate="G" pin="VCCINT_13" pad="P22"/>
<connect gate="G" pin="VCCINT_14" pad="T15"/>
<connect gate="G" pin="VCCINT_15" pad="R16"/>
<connect gate="G" pin="VCCINT_16" pad="T21"/>
<connect gate="G" pin="VCCINT_2" pad="P15"/>
<connect gate="G" pin="VCCINT_3" pad="P19"/>
<connect gate="G" pin="VCCINT_4" pad="R18"/>
<connect gate="G" pin="VCCINT_5" pad="P17"/>
<connect gate="G" pin="VCCINT_6" pad="R20"/>
<connect gate="G" pin="VCCINT_7" pad="P20"/>
<connect gate="G" pin="VCCINT_8" pad="R21"/>
<connect gate="G" pin="VCCINT_9" pad="P21"/>
<connect gate="G" pin="VCCIO2" pad="T24"/>
<connect gate="G" pin="VCCIO2_2" pad="N23"/>
<connect gate="G" pin="VCCIO2_3" pad="R32"/>
<connect gate="G" pin="VCCIO3" pad="N19"/>
<connect gate="G" pin="VCCIO3_2" pad="N21"/>
<connect gate="G" pin="VCCIO4" pad="T11"/>
<connect gate="G" pin="VREF0B4" pad="N12"/>
<connect gate="G" pin="VREF1B2" pad="P23"/>
<connect gate="G" pin="VREF1B4" pad="N13"/>
<connect gate="G" pin="VREF2B2" pad="R23"/>
<connect gate="G" pin="VREF2B4" pad="N15"/>
<connect gate="G" pin="VREF3B4" pad="N16"/>
<connect gate="H" pin="CLK0N" pad="T32"/>
<connect gate="H" pin="CLK0P" pad="T31"/>
<connect gate="H" pin="CLK2N" pad="U32"/>
<connect gate="H" pin="CLK2P" pad="U31"/>
<connect gate="H" pin="CLK3P" pad="U29"/>
<connect gate="H" pin="GND" pad="U19"/>
<connect gate="H" pin="GNDA_PLL2" pad="U28"/>
<connect gate="H" pin="GNDG_PLL2" pad="U26"/>
<connect gate="H" pin="GND_10" pad="W17"/>
<connect gate="H" pin="GND_11" pad="U22"/>
<connect gate="H" pin="GND_12" pad="Y24"/>
<connect gate="H" pin="GND_13" pad="W32"/>
<connect gate="H" pin="GND_2" pad="V18"/>
<connect gate="H" pin="GND_3" pad="U10"/>
<connect gate="H" pin="GND_4" pad="V20"/>
<connect gate="H" pin="GND_5" pad="U17"/>
<connect gate="H" pin="GND_6" pad="Y20"/>
<connect gate="H" pin="GND_7" pad="W19"/>
<connect gate="H" pin="GND_8" pad="V16"/>
<connect gate="H" pin="GND_9" pad="Y22"/>
<connect gate="H" pin="IN_1_DIFFIO_RX16N" pad="Y30"/>
<connect gate="H" pin="IN_1_DIFFIO_RX16P" pad="Y29"/>
<connect gate="H" pin="IN_1_DIFFIO_RX19N" pad="W30"/>
<connect gate="H" pin="IN_1_DIFFIO_RX19P" pad="W29"/>
<connect gate="H" pin="IN_1_DIFFIO_RX20P" pad="Y31"/>
<connect gate="H" pin="IN_1_DIFFIO_RX21N" pad="W31"/>
<connect gate="H" pin="IN_1_DIFFIO_RX21P" pad="V31"/>
<connect gate="H" pin="IN_1_DIFFIO_RX22N" pad="V30"/>
<connect gate="H" pin="IN_1_DIFFIO_RX22P" pad="V29"/>
<connect gate="H" pin="IO_1_CLK3N" pad="U30"/>
<connect gate="H" pin="IO_1_DIFFIO_TX13N" pad="Y28"/>
<connect gate="H" pin="IO_1_DIFFIO_TX13P" pad="Y27"/>
<connect gate="H" pin="IO_1_DIFFIO_TX14N" pad="Y26"/>
<connect gate="H" pin="IO_1_DIFFIO_TX14P" pad="Y25"/>
<connect gate="H" pin="IO_1_DIFFIO_TX15N" pad="W26"/>
<connect gate="H" pin="IO_1_DIFFIO_TX15P" pad="W25"/>
<connect gate="H" pin="IO_1_DIFFIO_TX16N" pad="W28"/>
<connect gate="H" pin="IO_1_DIFFIO_TX16P" pad="W27"/>
<connect gate="H" pin="IO_1_DIFFIO_TX17N" pad="W24"/>
<connect gate="H" pin="IO_1_DIFFIO_TX17P" pad="V24"/>
<connect gate="H" pin="IO_1_DIFFIO_TX18N" pad="V26"/>
<connect gate="H" pin="IO_1_DIFFIO_TX18P" pad="V25"/>
<connect gate="H" pin="IO_1_DIFFIO_TX19N" pad="V28"/>
<connect gate="H" pin="IO_1_DIFFIO_TX19P" pad="V27"/>
<connect gate="H" pin="IO_1_DIFFIO_TX22N" pad="U24"/>
<connect gate="H" pin="IO_4" pad="U12"/>
<connect gate="H" pin="IO_7" pad="Y18"/>
<connect gate="H" pin="IO_7_10" pad="W12"/>
<connect gate="H" pin="IO_7_11" pad="W13"/>
<connect gate="H" pin="IO_7_12" pad="W14"/>
<connect gate="H" pin="IO_7_13" pad="Y10"/>
<connect gate="H" pin="IO_7_14" pad="Y11"/>
<connect gate="H" pin="IO_7_15" pad="Y14"/>
<connect gate="H" pin="IO_7_16" pad="Y17"/>
<connect gate="H" pin="IO_7_2" pad="U13"/>
<connect gate="H" pin="IO_7_3" pad="V10"/>
<connect gate="H" pin="IO_7_4" pad="V11"/>
<connect gate="H" pin="IO_7_5" pad="V12"/>
<connect gate="H" pin="IO_7_6" pad="V13"/>
<connect gate="H" pin="IO_7_7" pad="V14"/>
<connect gate="H" pin="IO_7_8" pad="W10"/>
<connect gate="H" pin="IO_7_9" pad="W11"/>
<connect gate="H" pin="IO_7_FCLK4" pad="U14"/>
<connect gate="H" pin="VCCA_PLL2" pad="U27"/>
<connect gate="H" pin="VCCG_PLL2" pad="U25"/>
<connect gate="H" pin="VCCINT" pad="W22"/>
<connect gate="H" pin="VCCINT_10" pad="V17"/>
<connect gate="H" pin="VCCINT_11" pad="V19"/>
<connect gate="H" pin="VCCINT_12" pad="W18"/>
<connect gate="H" pin="VCCINT_13" pad="V21"/>
<connect gate="H" pin="VCCINT_14" pad="V22"/>
<connect gate="H" pin="VCCINT_15" pad="W20"/>
<connect gate="H" pin="VCCINT_16" pad="W21"/>
<connect gate="H" pin="VCCINT_2" pad="U15"/>
<connect gate="H" pin="VCCINT_3" pad="U20"/>
<connect gate="H" pin="VCCINT_4" pad="U18"/>
<connect gate="H" pin="VCCINT_5" pad="U21"/>
<connect gate="H" pin="VCCINT_6" pad="U16"/>
<connect gate="H" pin="VCCINT_7" pad="W15"/>
<connect gate="H" pin="VCCINT_8" pad="W16"/>
<connect gate="H" pin="VCCINT_9" pad="V15"/>
<connect gate="H" pin="VCCIO1" pad="V32"/>
<connect gate="H" pin="VCCIO1_2" pad="Y23"/>
<connect gate="H" pin="VCCIO1_3" pad="U23"/>
<connect gate="H" pin="VCCIO7" pad="U11"/>
<connect gate="H" pin="VCCIO8" pad="Y21"/>
<connect gate="H" pin="VCCIO8_2" pad="Y19"/>
<connect gate="H" pin="VREF0B1" pad="V23"/>
<connect gate="H" pin="VREF0B7" pad="Y16"/>
<connect gate="H" pin="VREF1B1" pad="W23"/>
<connect gate="H" pin="VREF1B7" pad="Y15"/>
<connect gate="H" pin="VREF2B7" pad="Y13"/>
<connect gate="H" pin="VREF3B7" pad="Y12"/>
<connect gate="I" pin="GNDA_PLL12" pad="AB16"/>
<connect gate="I" pin="GNDA_PLL6" pad="AB17"/>
<connect gate="I" pin="GNDA_PLL8" pad="AC27"/>
<connect gate="I" pin="GNDG_PLL12" pad="AA16"/>
<connect gate="I" pin="GNDG_PLL6" pad="AA17"/>
<connect gate="I" pin="GNDG_PLL8" pad="AC26"/>
<connect gate="I" pin="IN_1_DIFFIO_RX11N" pad="AD32"/>
<connect gate="I" pin="IN_1_DIFFIO_RX11P" pad="AD31"/>
<connect gate="I" pin="IN_1_DIFFIO_RX12N" pad="AC30"/>
<connect gate="I" pin="IN_1_DIFFIO_RX12P" pad="AC29"/>
<connect gate="I" pin="IN_1_DIFFIO_RX13N/RDN1" pad="AB30"/>
<connect gate="I" pin="IN_1_DIFFIO_RX13P/RUP1" pad="AB29"/>
<connect gate="I" pin="IN_1_DIFFIO_RX14N" pad="AA30"/>
<connect gate="I" pin="IN_1_DIFFIO_RX14P" pad="AA29"/>
<connect gate="I" pin="IN_1_DIFFIO_RX15N" pad="AB32"/>
<connect gate="I" pin="IN_1_DIFFIO_RX15P" pad="AB31"/>
<connect gate="I" pin="IN_1_DIFFIO_RX17N" pad="AC32"/>
<connect gate="I" pin="IN_1_DIFFIO_RX17P" pad="AC31"/>
<connect gate="I" pin="IN_1_DIFFIO_RX18N" pad="AA32"/>
<connect gate="I" pin="IN_1_DIFFIO_RX18P" pad="AA31"/>
<connect gate="I" pin="IN_1_DIFFIO_RX20N" pad="Y32"/>
<connect gate="I" pin="IN_1_DIFFIO_RX8N" pad="AD30"/>
<connect gate="I" pin="IN_1_DIFFIO_RX8P" pad="AD29"/>
<connect gate="I" pin="IO_1_DIFFIO_TX10N" pad="AB27"/>
<connect gate="I" pin="IO_1_DIFFIO_TX10P" pad="AB26"/>
<connect gate="I" pin="IO_1_DIFFIO_TX11N" pad="AA28"/>
<connect gate="I" pin="IO_1_DIFFIO_TX11P" pad="AA27"/>
<connect gate="I" pin="IO_1_DIFFIO_TX12N" pad="AA26"/>
<connect gate="I" pin="IO_1_DIFFIO_TX12P" pad="AA25"/>
<connect gate="I" pin="IO_1_DIFFIO_TX20N" pad="AD23"/>
<connect gate="I" pin="IO_1_DIFFIO_TX20P" pad="AC23"/>
<connect gate="I" pin="IO_1_DIFFIO_TX21N" pad="AB23"/>
<connect gate="I" pin="IO_1_DIFFIO_TX21P" pad="AA23"/>
<connect gate="I" pin="IO_1_DIFFIO_TX3P" pad="AD28"/>
<connect gate="I" pin="IO_1_DIFFIO_TX6N" pad="AC28"/>
<connect gate="I" pin="IO_1_DIFFIO_TX6P" pad="AB28"/>
<connect gate="I" pin="IO_1_DIFFIO_TX7N" pad="AD25"/>
<connect gate="I" pin="IO_1_DIFFIO_TX7P" pad="AD24"/>
<connect gate="I" pin="IO_1_DIFFIO_TX8N" pad="AC25"/>
<connect gate="I" pin="IO_1_DIFFIO_TX8P" pad="AC24"/>
<connect gate="I" pin="IO_1_DIFFIO_TX9N" pad="AB25"/>
<connect gate="I" pin="IO_1_DIFFIO_TX9P" pad="AB24"/>
<connect gate="I" pin="IO_7" pad="AD19"/>
<connect gate="I" pin="IO_7_10" pad="AD15"/>
<connect gate="I" pin="IO_7_11" pad="AD18"/>
<connect gate="I" pin="IO_7_2" pad="AA10"/>
<connect gate="I" pin="IO_7_3" pad="AA11"/>
<connect gate="I" pin="IO_7_4" pad="AA12"/>
<connect gate="I" pin="IO_7_5" pad="AA13"/>
<connect gate="I" pin="IO_7_6" pad="AA14"/>
<connect gate="I" pin="IO_7_7" pad="AB10"/>
<connect gate="I" pin="IO_7_8" pad="AB14"/>
<connect gate="I" pin="IO_7_9" pad="AC19"/>
<connect gate="I" pin="IO_7_DEV_CLRN" pad="AD14"/>
<connect gate="I" pin="IO_7_DQ1B0" pad="AD10"/>
<connect gate="I" pin="IO_7_DQ1B1" pad="AC10"/>
<connect gate="I" pin="IO_7_DQ1B3" pad="AC11"/>
<connect gate="I" pin="IO_7_DQ1B5" pad="AB12"/>
<connect gate="I" pin="IO_7_DQ1B6" pad="AB11"/>
<connect gate="I" pin="IO_7_DQ2B0" pad="AD12"/>
<connect gate="I" pin="IO_7_DQ2B1" pad="AC12"/>
<connect gate="I" pin="IO_7_DQ2B3" pad="AB13"/>
<connect gate="I" pin="IO_7_DQ2B6" pad="AC13"/>
<connect gate="I" pin="IO_7_DQ2B7" pad="AD13"/>
<connect gate="I" pin="IO_7_DQS1B" pad="AD11"/>
<connect gate="I" pin="IO_7_RDN7" pad="AC14"/>
<connect gate="I" pin="IO_8" pad="AD22"/>
<connect gate="I" pin="IO_8_2" pad="AB21"/>
<connect gate="I" pin="IO_8_3" pad="AB22"/>
<connect gate="I" pin="IO_8_4" pad="AC21"/>
<connect gate="I" pin="IO_8_5" pad="AC22"/>
<connect gate="I" pin="IO_8_RDN8" pad="AD21"/>
<connect gate="I" pin="MSEL0" pad="AD20"/>
<connect gate="I" pin="MSEL1" pad="AB20"/>
<connect gate="I" pin="MSEL2" pad="AB19"/>
<connect gate="I" pin="NCE" pad="AD16"/>
<connect gate="I" pin="NIO_PULLUP" pad="AB15"/>
<connect gate="I" pin="PLL_ENA" pad="AC20"/>
<connect gate="I" pin="PORSEL" pad="AC15"/>
<connect gate="I" pin="VCCA_PLL12" pad="AC16"/>
<connect gate="I" pin="VCCA_PLL6" pad="AC18"/>
<connect gate="I" pin="VCCA_PLL8" pad="AD27"/>
<connect gate="I" pin="VCCG_PLL12" pad="AD17"/>
<connect gate="I" pin="VCCG_PLL6" pad="AC17"/>
<connect gate="I" pin="VCCG_PLL8" pad="AD26"/>
<connect gate="I" pin="VCCSEL" pad="AA15"/>
<connect gate="I" pin="VCC_PLL6_OUTA" pad="AB18"/>
<connect gate="I" pin="VCC_PLL6_OUTB" pad="AA18"/>
<connect gate="I" pin="VREF0B8" pad="AA22"/>
<connect gate="I" pin="VREF1B8" pad="AA21"/>
<connect gate="I" pin="VREF2B1" pad="AA24"/>
<connect gate="I" pin="VREF2B8" pad="AA20"/>
<connect gate="I" pin="VREF3B8" pad="AA19"/>
<connect gate="J" pin="CLK7P" pad="AG16"/>
<connect gate="J" pin="FPLL8CLKN" pad="AH30"/>
<connect gate="J" pin="FPLL8CLKP" pad="AH29"/>
<connect gate="J" pin="GND" pad="AH12"/>
<connect gate="J" pin="GND/NC" pad="AH11"/>
<connect gate="J" pin="GND_2" pad="AG11"/>
<connect gate="J" pin="GXB_GND" pad="AJ10"/>
<connect gate="J" pin="GXB_GND_2" pad="AH10"/>
<connect gate="J" pin="IN_1_DIFFIO_RX0N" pad="AH28"/>
<connect gate="J" pin="IN_1_DIFFIO_RX0P" pad="AH27"/>
<connect gate="J" pin="IN_1_DIFFIO_RX10N" pad="AE32"/>
<connect gate="J" pin="IN_1_DIFFIO_RX10P" pad="AE31"/>
<connect gate="J" pin="IN_1_DIFFIO_RX3N" pad="AH32"/>
<connect gate="J" pin="IN_1_DIFFIO_RX3P" pad="AH31"/>
<connect gate="J" pin="IN_1_DIFFIO_RX4N" pad="AG30"/>
<connect gate="J" pin="IN_1_DIFFIO_RX4P" pad="AG29"/>
<connect gate="J" pin="IN_1_DIFFIO_RX5N" pad="AG32"/>
<connect gate="J" pin="IN_1_DIFFIO_RX5P" pad="AG31"/>
<connect gate="J" pin="IN_1_DIFFIO_RX6N" pad="AF32"/>
<connect gate="J" pin="IN_1_DIFFIO_RX6P" pad="AF31"/>
<connect gate="J" pin="IN_1_DIFFIO_RX7N" pad="AF30"/>
<connect gate="J" pin="IN_1_DIFFIO_RX7P" pad="AF29"/>
<connect gate="J" pin="IN_1_DIFFIO_RX9N" pad="AE30"/>
<connect gate="J" pin="IN_1_DIFFIO_RX9P" pad="AE29"/>
<connect gate="J" pin="IO_1" pad="AG26"/>
<connect gate="J" pin="IO_11_PLL6_FBN" pad="AH17"/>
<connect gate="J" pin="IO_11_PLL6_FBP" pad="AG17"/>
<connect gate="J" pin="IO_12_PLL6_OUT3N" pad="AH18"/>
<connect gate="J" pin="IO_12_PLL6_OUT3P" pad="AG18"/>
<connect gate="J" pin="IO_1_2" pad="AG25"/>
<connect gate="J" pin="IO_1_DIFFIO_TX0N" pad="AG28"/>
<connect gate="J" pin="IO_1_DIFFIO_TX0P" pad="AG27"/>
<connect gate="J" pin="IO_1_DIFFIO_TX1N" pad="AF28"/>
<connect gate="J" pin="IO_1_DIFFIO_TX1P" pad="AF27"/>
<connect gate="J" pin="IO_1_DIFFIO_TX2N" pad="AF26"/>
<connect gate="J" pin="IO_1_DIFFIO_TX2P" pad="AF25"/>
<connect gate="J" pin="IO_1_DIFFIO_TX3N" pad="AE28"/>
<connect gate="J" pin="IO_1_DIFFIO_TX4N" pad="AE27"/>
<connect gate="J" pin="IO_1_DIFFIO_TX4P" pad="AE26"/>
<connect gate="J" pin="IO_1_DIFFIO_TX5N" pad="AE25"/>
<connect gate="J" pin="IO_1_DIFFIO_TX5P" pad="AE24"/>
<connect gate="J" pin="IO_7" pad="AF18"/>
<connect gate="J" pin="IO_7_2" pad="AE14"/>
<connect gate="J" pin="IO_7_3" pad="AE15"/>
<connect gate="J" pin="IO_7_4" pad="AE17"/>
<connect gate="J" pin="IO_7_5" pad="AE18"/>
<connect gate="J" pin="IO_7_6" pad="AE19"/>
<connect gate="J" pin="IO_7_7" pad="AF14"/>
<connect gate="J" pin="IO_7_8" pad="AF16"/>
<connect gate="J" pin="IO_7_9" pad="AF17"/>
<connect gate="J" pin="IO_7_CLK7N" pad="AH16"/>
<connect gate="J" pin="IO_7_DQ0B5" pad="AF10"/>
<connect gate="J" pin="IO_7_DQ1B2" pad="AE10"/>
<connect gate="J" pin="IO_7_DQ1B4" pad="AE11"/>
<connect gate="J" pin="IO_7_DQ1B7" pad="AF11"/>
<connect gate="J" pin="IO_7_DQ2B2" pad="AF12"/>
<connect gate="J" pin="IO_7_DQ2B4" pad="AF13"/>
<connect gate="J" pin="IO_7_DQ2B5" pad="AE13"/>
<connect gate="J" pin="IO_7_DQ3B0" pad="AG13"/>
<connect gate="J" pin="IO_7_DQ3B6" pad="AH14"/>
<connect gate="J" pin="IO_7_DQ3B7" pad="AG14"/>
<connect gate="J" pin="IO_7_DQ4B5" pad="AH15"/>
<connect gate="J" pin="IO_7_DQ4B7" pad="AG15"/>
<connect gate="J" pin="IO_7_DQS2B" pad="AE12"/>
<connect gate="J" pin="IO_7_DQS3B" pad="AH13"/>
<connect gate="J" pin="IO_7_FCLK5" pad="AF15"/>
<connect gate="J" pin="IO_7_RUP7" pad="AF19"/>
<connect gate="J" pin="IO_8" pad="AH26"/>
<connect gate="J" pin="IO_8_10" pad="AG23"/>
<connect gate="J" pin="IO_8_11" pad="AG24"/>
<connect gate="J" pin="IO_8_12" pad="AH24"/>
<connect gate="J" pin="IO_8_2" pad="AE20"/>
<connect gate="J" pin="IO_8_3" pad="AE21"/>
<connect gate="J" pin="IO_8_4" pad="AE23"/>
<connect gate="J" pin="IO_8_5" pad="AF21"/>
<connect gate="J" pin="IO_8_6" pad="AF23"/>
<connect gate="J" pin="IO_8_7" pad="AF24"/>
<connect gate="J" pin="IO_8_8" pad="AG21"/>
<connect gate="J" pin="IO_8_9" pad="AG22"/>
<connect gate="J" pin="IO_8_DQ5B0" pad="AH19"/>
<connect gate="J" pin="IO_8_DQ5B1" pad="AG19"/>
<connect gate="J" pin="IO_8_DQ5B2" pad="AH20"/>
<connect gate="J" pin="IO_8_DQ5B7" pad="AH21"/>
<connect gate="J" pin="IO_8_DQ6B7" pad="AH22"/>
<connect gate="J" pin="IO_8_DQ7B3" pad="AH23"/>
<connect gate="J" pin="IO_8_DQ8B4" pad="AH25"/>
<connect gate="J" pin="IO_8_DQS5B" pad="AG20"/>
<connect gate="J" pin="IO_8_FCLK2" pad="AF22"/>
<connect gate="J" pin="IO_8_FCLK3" pad="AE22"/>
<connect gate="J" pin="IO_8_RUP8" pad="AF20"/>
<connect gate="J" pin="NCEO" pad="AE16"/>
<connect gate="J" pin="VCCINT" pad="AG12"/>
<connect gate="J" pin="VCCINT_2" pad="AG10"/>
<connect gate="K" pin="CLK4P" pad="AL18"/>
<connect gate="K" pin="CLK5P" pad="AK19"/>
<connect gate="K" pin="CLK6P" pad="AJ16"/>
<connect gate="K" pin="GND" pad="AL32"/>
<connect gate="K" pin="GND/NC" pad="AL11"/>
<connect gate="K" pin="GND/NC_2" pad="AM11"/>
<connect gate="K" pin="GND/NC_3" pad="AJ11"/>
<connect gate="K" pin="GND_2" pad="AL12"/>
<connect gate="K" pin="GND_3" pad="AK12"/>
<connect gate="K" pin="GND_4" pad="AM20"/>
<connect gate="K" pin="GND_5" pad="AL16"/>
<connect gate="K" pin="GND_6" pad="AJ12"/>
<connect gate="K" pin="GND_7" pad="AM31"/>
<connect gate="K" pin="GXB_GND" pad="AM10"/>
<connect gate="K" pin="GXB_GND_2" pad="AK11"/>
<connect gate="K" pin="GXB_GND_3" pad="AK10"/>
<connect gate="K" pin="GXB_GND_4" pad="AL10"/>
<connect gate="K" pin="IN_1_DIFFIO_RX1N" pad="AJ30"/>
<connect gate="K" pin="IN_1_DIFFIO_RX1P" pad="AJ29"/>
<connect gate="K" pin="IN_1_DIFFIO_RX2N" pad="AJ32"/>
<connect gate="K" pin="IN_1_DIFFIO_RX2P" pad="AJ31"/>
<connect gate="K" pin="IO_11_PLL6_OUT0N" pad="AM17"/>
<connect gate="K" pin="IO_11_PLL6_OUT0P" pad="AL17"/>
<connect gate="K" pin="IO_11_PLL6_OUT1N" pad="AK17"/>
<connect gate="K" pin="IO_11_PLL6_OUT1P" pad="AJ17"/>
<connect gate="K" pin="IO_12_PLL6_OUT2N" pad="AK18"/>
<connect gate="K" pin="IO_12_PLL6_OUT2P" pad="AJ18"/>
<connect gate="K" pin="IO_7_CLK6N/PLL12_OUT" pad="AK16"/>
<connect gate="K" pin="IO_7_DQ3B1" pad="AK13"/>
<connect gate="K" pin="IO_7_DQ3B2" pad="AJ13"/>
<connect gate="K" pin="IO_7_DQ3B3" pad="AJ14"/>
<connect gate="K" pin="IO_7_DQ3B4" pad="AM13"/>
<connect gate="K" pin="IO_7_DQ3B5" pad="AL13"/>
<connect gate="K" pin="IO_7_DQ4B0" pad="AK14"/>
<connect gate="K" pin="IO_7_DQ4B1" pad="AM15"/>
<connect gate="K" pin="IO_7_DQ4B2" pad="AM14"/>
<connect gate="K" pin="IO_7_DQ4B3" pad="AL15"/>
<connect gate="K" pin="IO_7_DQ4B4" pad="AK15"/>
<connect gate="K" pin="IO_7_DQ4B6" pad="AJ15"/>
<connect gate="K" pin="IO_7_DQS4B" pad="AL14"/>
<connect gate="K" pin="IO_8" pad="AL31"/>
<connect gate="K" pin="IO_8_2" pad="AJ27"/>
<connect gate="K" pin="IO_8_3" pad="AJ28"/>
<connect gate="K" pin="IO_8_4" pad="AK30"/>
<connect gate="K" pin="IO_8_5" pad="AK31"/>
<connect gate="K" pin="IO_8_6" pad="AL30"/>
<connect gate="K" pin="IO_8_CLK4N" pad="AM18"/>
<connect gate="K" pin="IO_8_CLK5N" pad="AL19"/>
<connect gate="K" pin="IO_8_DQ5B3" pad="AJ19"/>
<connect gate="K" pin="IO_8_DQ5B4" pad="AL20"/>
<connect gate="K" pin="IO_8_DQ5B5" pad="AK20"/>
<connect gate="K" pin="IO_8_DQ5B6" pad="AJ20"/>
<connect gate="K" pin="IO_8_DQ6B0" pad="AK21"/>
<connect gate="K" pin="IO_8_DQ6B1" pad="AJ21"/>
<connect gate="K" pin="IO_8_DQ6B2" pad="AM21"/>
<connect gate="K" pin="IO_8_DQ6B3" pad="AM22"/>
<connect gate="K" pin="IO_8_DQ6B4" pad="AK22"/>
<connect gate="K" pin="IO_8_DQ6B5" pad="AJ22"/>
<connect gate="K" pin="IO_8_DQ6B6" pad="AL22"/>
<connect gate="K" pin="IO_8_DQ7B0" pad="AM23"/>
<connect gate="K" pin="IO_8_DQ7B1" pad="AL23"/>
<connect gate="K" pin="IO_8_DQ7B2" pad="AK23"/>
<connect gate="K" pin="IO_8_DQ7B4" pad="AM24"/>
<connect gate="K" pin="IO_8_DQ7B5" pad="AL24"/>
<connect gate="K" pin="IO_8_DQ7B6" pad="AK24"/>
<connect gate="K" pin="IO_8_DQ7B7" pad="AJ24"/>
<connect gate="K" pin="IO_8_DQ8B0" pad="AM25"/>
<connect gate="K" pin="IO_8_DQ8B1" pad="AL25"/>
<connect gate="K" pin="IO_8_DQ8B2" pad="AK25"/>
<connect gate="K" pin="IO_8_DQ8B3" pad="AM26"/>
<connect gate="K" pin="IO_8_DQ8B5" pad="AL26"/>
<connect gate="K" pin="IO_8_DQ8B6" pad="AK26"/>
<connect gate="K" pin="IO_8_DQ8B7" pad="AJ26"/>
<connect gate="K" pin="IO_8_DQ9B0" pad="AM27"/>
<connect gate="K" pin="IO_8_DQ9B1" pad="AL27"/>
<connect gate="K" pin="IO_8_DQ9B2" pad="AK27"/>
<connect gate="K" pin="IO_8_DQ9B3" pad="AL28"/>
<connect gate="K" pin="IO_8_DQ9B4" pad="AK28"/>
<connect gate="K" pin="IO_8_DQ9B5" pad="AM29"/>
<connect gate="K" pin="IO_8_DQ9B6" pad="AL29"/>
<connect gate="K" pin="IO_8_DQ9B7" pad="AK29"/>
<connect gate="K" pin="IO_8_DQS6B" pad="AL21"/>
<connect gate="K" pin="IO_8_DQS7B" pad="AJ23"/>
<connect gate="K" pin="IO_8_DQS8B" pad="AJ25"/>
<connect gate="K" pin="IO_8_DQS9B" pad="AM28"/>
<connect gate="K" pin="VCCIO1" pad="AK32"/>
<connect gate="K" pin="VCCIO7" pad="AM16"/>
<connect gate="K" pin="VCCIO7_2" pad="AM12"/>
<connect gate="K" pin="VCCIO8" pad="AM19"/>
<connect gate="K" pin="VCCIO8_2" pad="AM30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP1SGX40GF1020C6N"/>
<attribute name="OC_FARNELL" value="1637231"/>
<attribute name="OC_NEWARK" value="51R0559"/>
<attribute name="PACKAGE" value="BGA-1020"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C15AF256I8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP2C15AF256I8N_A"/>
<gate name="B" symbol="EP2C15AF256I8N_B"/>
<gate name="C" symbol="EP2C15AF256I8N_C"/>
</gates>
<devices>
<device name="" package="BGA256C16X16X100C_1700X1700X22">
<connects>
<connect gate="A" pin="CLK0" pad="H2"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="CLK10" pad="A8"/>
<connect gate="A" pin="CLK11" pad="B8"/>
<connect gate="A" pin="CLK2" pad="J2"/>
<connect gate="A" pin="CLK3" pad="J1"/>
<connect gate="A" pin="CLK8" pad="A9"/>
<connect gate="A" pin="CLK9" pad="B9"/>
<connect gate="A" pin="DATA0" pad="F1"/>
<connect gate="A" pin="DCLK" pad="H4"/>
<connect gate="A" pin="GND" pad="J9"/>
<connect gate="A" pin="GNDA_PLL3" pad="E6"/>
<connect gate="A" pin="GND_10" pad="C9"/>
<connect gate="A" pin="GND_11" pad="F8"/>
<connect gate="A" pin="GND_12" pad="G6"/>
<connect gate="A" pin="GND_13" pad="H3"/>
<connect gate="A" pin="GND_14" pad="H8"/>
<connect gate="A" pin="GND_15" pad="H6"/>
<connect gate="A" pin="GND_16" pad="H9"/>
<connect gate="A" pin="GND_17" pad="J3"/>
<connect gate="A" pin="GND_2" pad="J8"/>
<connect gate="A" pin="GND_3" pad="A1"/>
<connect gate="A" pin="GND_4" pad="E8"/>
<connect gate="A" pin="GND_5" pad="G8"/>
<connect gate="A" pin="GND_6" pad="B2"/>
<connect gate="A" pin="GND_7" pad="C8"/>
<connect gate="A" pin="GND_8" pad="E9"/>
<connect gate="A" pin="GND_9" pad="F7"/>
<connect gate="A" pin="GND_PLL3" pad="D5"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO_10" pad="B6"/>
<connect gate="A" pin="IO_11" pad="B7"/>
<connect gate="A" pin="IO_12" pad="C1"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="C3"/>
<connect gate="A" pin="IO_15" pad="C4"/>
<connect gate="A" pin="IO_16" pad="C5"/>
<connect gate="A" pin="IO_17" pad="C6"/>
<connect gate="A" pin="IO_18" pad="D1"/>
<connect gate="A" pin="IO_19" pad="D2"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="D3"/>
<connect gate="A" pin="IO_21" pad="D4"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="D7"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D9"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="E2"/>
<connect gate="A" pin="IO_28" pad="E3"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="F3"/>
<connect gate="A" pin="IO_31" pad="F4"/>
<connect gate="A" pin="IO_32" pad="G4"/>
<connect gate="A" pin="IO_33" pad="J4"/>
<connect gate="A" pin="IO_34" pad="K1"/>
<connect gate="A" pin="IO_35" pad="K2"/>
<connect gate="A" pin="IO_36" pad="K4"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_7" pad="B3"/>
<connect gate="A" pin="IO_8" pad="B4"/>
<connect gate="A" pin="IO_9" pad="B5"/>
<connect gate="A" pin="NCE" pad="G5"/>
<connect gate="A" pin="NCONFIG" pad="J5"/>
<connect gate="A" pin="TCK" pad="F2"/>
<connect gate="A" pin="TDI" pad="H5"/>
<connect gate="A" pin="TDO" pad="G2"/>
<connect gate="A" pin="TMS" pad="G1"/>
<connect gate="A" pin="VCCA_PLL3" pad="F6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="F9"/>
<connect gate="A" pin="VCCINT_2" pad="J6"/>
<connect gate="A" pin="VCCINT_3" pad="G7"/>
<connect gate="A" pin="VCCINT_4" pad="J7"/>
<connect gate="A" pin="VCCINT_5" pad="G9"/>
<connect gate="A" pin="VCCINT_6" pad="H7"/>
<connect gate="A" pin="VCCIO1" pad="K3"/>
<connect gate="A" pin="VCCIO2" pad="G3"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO3" pad="E7"/>
<connect gate="A" pin="VCCIO3_2" pad="C7"/>
<connect gate="A" pin="VCCIO3_3" pad="A2"/>
<connect gate="B" pin="CLK13" pad="N9"/>
<connect gate="B" pin="CLK14" pad="R9"/>
<connect gate="B" pin="CLK15" pad="T9"/>
<connect gate="B" pin="GND" pad="B15"/>
<connect gate="B" pin="GNDA_PLL1" pad="M6"/>
<connect gate="B" pin="GND_10" pad="T1"/>
<connect gate="B" pin="GND_11" pad="A16"/>
<connect gate="B" pin="GND_2" pad="K7"/>
<connect gate="B" pin="GND_3" pad="K9"/>
<connect gate="B" pin="GND_4" pad="L9"/>
<connect gate="B" pin="GND_5" pad="M8"/>
<connect gate="B" pin="GND_6" pad="M9"/>
<connect gate="B" pin="GND_7" pad="P8"/>
<connect gate="B" pin="GND_8" pad="P9"/>
<connect gate="B" pin="GND_9" pad="R2"/>
<connect gate="B" pin="GND_PLL1" pad="N5"/>
<connect gate="B" pin="GND_PLL1_2" pad="L5"/>
<connect gate="B" pin="GND_PLL2" pad="D12"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="N1"/>
<connect gate="B" pin="IO_11" pad="N2"/>
<connect gate="B" pin="IO_12" pad="N3"/>
<connect gate="B" pin="IO_13" pad="N4"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="N8"/>
<connect gate="B" pin="IO_17" pad="P1"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="P3"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="P4"/>
<connect gate="B" pin="IO_21" pad="P5"/>
<connect gate="B" pin="IO_22" pad="P6"/>
<connect gate="B" pin="IO_23" pad="R3"/>
<connect gate="B" pin="IO_24" pad="R4"/>
<connect gate="B" pin="IO_25" pad="R5"/>
<connect gate="B" pin="IO_26" pad="R6"/>
<connect gate="B" pin="IO_27" pad="R7"/>
<connect gate="B" pin="IO_28" pad="R8"/>
<connect gate="B" pin="IO_29" pad="T3"/>
<connect gate="B" pin="IO_3" pad="L2"/>
<connect gate="B" pin="IO_30" pad="T4"/>
<connect gate="B" pin="IO_31" pad="T5"/>
<connect gate="B" pin="IO_32" pad="T6"/>
<connect gate="B" pin="IO_33" pad="T7"/>
<connect gate="B" pin="IO_34" pad="T8"/>
<connect gate="B" pin="IO_35" pad="A10"/>
<connect gate="B" pin="IO_36" pad="A11"/>
<connect gate="B" pin="IO_37" pad="A12"/>
<connect gate="B" pin="IO_38" pad="A13"/>
<connect gate="B" pin="IO_39" pad="A14"/>
<connect gate="B" pin="IO_4" pad="L3"/>
<connect gate="B" pin="IO_40" pad="B10"/>
<connect gate="B" pin="IO_41" pad="B11"/>
<connect gate="B" pin="IO_42" pad="B12"/>
<connect gate="B" pin="IO_43" pad="B13"/>
<connect gate="B" pin="IO_44" pad="B14"/>
<connect gate="B" pin="IO_45" pad="C11"/>
<connect gate="B" pin="IO_46" pad="C12"/>
<connect gate="B" pin="IO_47" pad="C13"/>
<connect gate="B" pin="IO_48" pad="C14"/>
<connect gate="B" pin="IO_49" pad="C15"/>
<connect gate="B" pin="IO_5" pad="L4"/>
<connect gate="B" pin="IO_50" pad="C16"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_55" pad="D15"/>
<connect gate="B" pin="IO_6" pad="M1"/>
<connect gate="B" pin="IO_7" pad="M2"/>
<connect gate="B" pin="IO_8" pad="M3"/>
<connect gate="B" pin="IO_9" pad="M4"/>
<connect gate="B" pin="VCCA_PLL1" pad="M5"/>
<connect gate="B" pin="VCCD_PLL1" pad="L6"/>
<connect gate="B" pin="VCCINT" pad="K8"/>
<connect gate="B" pin="VCCINT_2" pad="K6"/>
<connect gate="B" pin="VCCINT_3" pad="L7"/>
<connect gate="B" pin="VCCINT_4" pad="L8"/>
<connect gate="B" pin="VCCIO1" pad="R1"/>
<connect gate="B" pin="VCCIO4" pad="C10"/>
<connect gate="B" pin="VCCIO4_2" pad="A15"/>
<connect gate="B" pin="VCCIO5" pad="B16"/>
<connect gate="B" pin="VCCIO8" pad="M7"/>
<connect gate="B" pin="VCCIO8_2" pad="P7"/>
<connect gate="B" pin="VCCIO8_3" pad="T2"/>
<connect gate="C" pin="CLK12" pad="N10"/>
<connect gate="C" pin="CLK4" pad="H16"/>
<connect gate="C" pin="CLK5" pad="H15"/>
<connect gate="C" pin="CLK6" pad="J15"/>
<connect gate="C" pin="CLK7" pad="J16"/>
<connect gate="C" pin="CONF_DONE" pad="L13"/>
<connect gate="C" pin="GND" pad="L10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E11"/>
<connect gate="C" pin="GNDA_PLL4" pad="M11"/>
<connect gate="C" pin="GND_2" pad="G10"/>
<connect gate="C" pin="GND_3" pad="J14"/>
<connect gate="C" pin="GND_4" pad="K11"/>
<connect gate="C" pin="GND_5" pad="J11"/>
<connect gate="C" pin="GND_6" pad="T16"/>
<connect gate="C" pin="GND_7" pad="H14"/>
<connect gate="C" pin="GND_8" pad="R15"/>
<connect gate="C" pin="GND_PLL2" pad="F12"/>
<connect gate="C" pin="GND_PLL4" pad="N12"/>
<connect gate="C" pin="GND_PLL4_2" pad="L12"/>
<connect gate="C" pin="IO" pad="T14"/>
<connect gate="C" pin="IO_10" pad="G12"/>
<connect gate="C" pin="IO_11" pad="G13"/>
<connect gate="C" pin="IO_12" pad="G15"/>
<connect gate="C" pin="IO_13" pad="G16"/>
<connect gate="C" pin="IO_14" pad="H12"/>
<connect gate="C" pin="IO_15" pad="H13"/>
<connect gate="C" pin="IO_16" pad="J12"/>
<connect gate="C" pin="IO_17" pad="K13"/>
<connect gate="C" pin="IO_18" pad="K15"/>
<connect gate="C" pin="IO_19" pad="K16"/>
<connect gate="C" pin="IO_2" pad="E13"/>
<connect gate="C" pin="IO_20" pad="L14"/>
<connect gate="C" pin="IO_21" pad="L15"/>
<connect gate="C" pin="IO_22" pad="L16"/>
<connect gate="C" pin="IO_23" pad="M14"/>
<connect gate="C" pin="IO_24" pad="M15"/>
<connect gate="C" pin="IO_25" pad="M16"/>
<connect gate="C" pin="IO_26" pad="N11"/>
<connect gate="C" pin="IO_27" pad="N13"/>
<connect gate="C" pin="IO_28" pad="N14"/>
<connect gate="C" pin="IO_29" pad="N15"/>
<connect gate="C" pin="IO_3" pad="E14"/>
<connect gate="C" pin="IO_30" pad="N16"/>
<connect gate="C" pin="IO_31" pad="P11"/>
<connect gate="C" pin="IO_32" pad="P12"/>
<connect gate="C" pin="IO_33" pad="P13"/>
<connect gate="C" pin="IO_34" pad="P14"/>
<connect gate="C" pin="IO_35" pad="P15"/>
<connect gate="C" pin="IO_36" pad="P16"/>
<connect gate="C" pin="IO_37" pad="R10"/>
<connect gate="C" pin="IO_38" pad="R11"/>
<connect gate="C" pin="IO_39" pad="R12"/>
<connect gate="C" pin="IO_4" pad="E15"/>
<connect gate="C" pin="IO_40" pad="R13"/>
<connect gate="C" pin="IO_41" pad="R14"/>
<connect gate="C" pin="IO_42" pad="T10"/>
<connect gate="C" pin="IO_43" pad="T11"/>
<connect gate="C" pin="IO_44" pad="T12"/>
<connect gate="C" pin="IO_45" pad="T13"/>
<connect gate="C" pin="IO_5" pad="E16"/>
<connect gate="C" pin="IO_6" pad="F13"/>
<connect gate="C" pin="IO_7" pad="F14"/>
<connect gate="C" pin="IO_8" pad="F15"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="MSEL0" pad="J13"/>
<connect gate="C" pin="MSEL1" pad="K12"/>
<connect gate="C" pin="NSTATUS" pad="M13"/>
<connect gate="C" pin="VCCA_PLL2" pad="E12"/>
<connect gate="C" pin="VCCA_PLL4" pad="L11"/>
<connect gate="C" pin="VCCD_PLL2" pad="F11"/>
<connect gate="C" pin="VCCD_PLL4" pad="M12"/>
<connect gate="C" pin="VCCINT" pad="G11"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="H11"/>
<connect gate="C" pin="VCCINT_4" pad="J10"/>
<connect gate="C" pin="VCCINT_5" pad="K10"/>
<connect gate="C" pin="VCCINT_6" pad="F10"/>
<connect gate="C" pin="VCCIO4" pad="E10"/>
<connect gate="C" pin="VCCIO5" pad="G14"/>
<connect gate="C" pin="VCCIO6" pad="R16"/>
<connect gate="C" pin="VCCIO6_2" pad="K14"/>
<connect gate="C" pin="VCCIO7" pad="T15"/>
<connect gate="C" pin="VCCIO7_2" pad="P10"/>
<connect gate="C" pin="VCCIO7_3" pad="M10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C15AF256I8N"/>
<attribute name="OC_FARNELL" value="1549348"/>
<attribute name="OC_NEWARK" value="52R0489"/>
<attribute name="PACKAGE" value="256-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C20F256C8N">
<description>IC CYCLONE II FPGA</description>
<gates>
<gate name="A" symbol="EP2C20F256C8N_A"/>
<gate name="B" symbol="EP2C20F256C8N_B"/>
<gate name="C" symbol="EP2C20F256C8N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="CLK0" pad="H2"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="CLK10" pad="A8"/>
<connect gate="A" pin="CLK11" pad="B8"/>
<connect gate="A" pin="CLK2" pad="J2"/>
<connect gate="A" pin="CLK3" pad="J1"/>
<connect gate="A" pin="CLK8" pad="A9"/>
<connect gate="A" pin="CLK9" pad="B9"/>
<connect gate="A" pin="DATA0" pad="F1"/>
<connect gate="A" pin="DCLK" pad="H4"/>
<connect gate="A" pin="GND" pad="J9"/>
<connect gate="A" pin="GNDA_PLL3" pad="E6"/>
<connect gate="A" pin="GND_10" pad="F8"/>
<connect gate="A" pin="GND_11" pad="H3"/>
<connect gate="A" pin="GND_12" pad="H6"/>
<connect gate="A" pin="GND_13" pad="J8"/>
<connect gate="A" pin="GND_14" pad="C9"/>
<connect gate="A" pin="GND_15" pad="E8"/>
<connect gate="A" pin="GND_16" pad="J3"/>
<connect gate="A" pin="GND_17" pad="E9"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="H9"/>
<connect gate="A" pin="GND_4" pad="B2"/>
<connect gate="A" pin="GND_5" pad="H8"/>
<connect gate="A" pin="GND_6" pad="G8"/>
<connect gate="A" pin="GND_7" pad="G6"/>
<connect gate="A" pin="GND_8" pad="C8"/>
<connect gate="A" pin="GND_9" pad="F7"/>
<connect gate="A" pin="GND_PLL3" pad="F5"/>
<connect gate="A" pin="GND_PLL3_2" pad="D5"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO_10" pad="C6"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="D4"/>
<connect gate="A" pin="IO_13" pad="B5"/>
<connect gate="A" pin="IO_14" pad="A5"/>
<connect gate="A" pin="IO_15" pad="D6"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="D7"/>
<connect gate="A" pin="IO_18" pad="A6"/>
<connect gate="A" pin="IO_19" pad="D8"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="B6"/>
<connect gate="A" pin="IO_21" pad="D9"/>
<connect gate="A" pin="IO_22" pad="A7"/>
<connect gate="A" pin="IO_23" pad="E1"/>
<connect gate="A" pin="IO_24" pad="C3"/>
<connect gate="A" pin="IO_25" pad="E2"/>
<connect gate="A" pin="IO_26" pad="B7"/>
<connect gate="A" pin="IO_27" pad="E3"/>
<connect gate="A" pin="IO_28" pad="C4"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="D1"/>
<connect gate="A" pin="IO_30" pad="F3"/>
<connect gate="A" pin="IO_31" pad="J4"/>
<connect gate="A" pin="IO_32" pad="F4"/>
<connect gate="A" pin="IO_33" pad="K1"/>
<connect gate="A" pin="IO_34" pad="K2"/>
<connect gate="A" pin="IO_35" pad="K4"/>
<connect gate="A" pin="IO_36" pad="G4"/>
<connect gate="A" pin="IO_4" pad="B4"/>
<connect gate="A" pin="IO_5" pad="D2"/>
<connect gate="A" pin="IO_6" pad="A3"/>
<connect gate="A" pin="IO_7" pad="D3"/>
<connect gate="A" pin="IO_8" pad="C1"/>
<connect gate="A" pin="IO_9" pad="C5"/>
<connect gate="A" pin="NCE" pad="G5"/>
<connect gate="A" pin="NCONFIG" pad="J5"/>
<connect gate="A" pin="TCK" pad="F2"/>
<connect gate="A" pin="TDI" pad="H5"/>
<connect gate="A" pin="TDO" pad="G2"/>
<connect gate="A" pin="TMS" pad="G1"/>
<connect gate="A" pin="VCCA_PLL3" pad="F6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="J6"/>
<connect gate="A" pin="VCCINT_2" pad="F9"/>
<connect gate="A" pin="VCCINT_3" pad="H7"/>
<connect gate="A" pin="VCCINT_4" pad="G7"/>
<connect gate="A" pin="VCCINT_5" pad="G9"/>
<connect gate="A" pin="VCCINT_6" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="K3"/>
<connect gate="A" pin="VCCIO2" pad="G3"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO3" pad="C7"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="E7"/>
<connect gate="B" pin="CLK13" pad="N9"/>
<connect gate="B" pin="CLK14" pad="R9"/>
<connect gate="B" pin="CLK15" pad="T9"/>
<connect gate="B" pin="GND" pad="B15"/>
<connect gate="B" pin="GNDA_PLL1" pad="M6"/>
<connect gate="B" pin="GND_10" pad="T1"/>
<connect gate="B" pin="GND_11" pad="A16"/>
<connect gate="B" pin="GND_2" pad="K7"/>
<connect gate="B" pin="GND_3" pad="L9"/>
<connect gate="B" pin="GND_4" pad="M8"/>
<connect gate="B" pin="GND_5" pad="P8"/>
<connect gate="B" pin="GND_6" pad="M9"/>
<connect gate="B" pin="GND_7" pad="P9"/>
<connect gate="B" pin="GND_8" pad="R2"/>
<connect gate="B" pin="GND_9" pad="K9"/>
<connect gate="B" pin="GND_PLL1" pad="L5"/>
<connect gate="B" pin="GND_PLL1_2" pad="N5"/>
<connect gate="B" pin="GND_PLL2" pad="D12"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="M3"/>
<connect gate="B" pin="IO_11" pad="N6"/>
<connect gate="B" pin="IO_12" pad="L3"/>
<connect gate="B" pin="IO_13" pad="N7"/>
<connect gate="B" pin="IO_14" pad="L4"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P1"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N1"/>
<connect gate="B" pin="IO_20" pad="P3"/>
<connect gate="B" pin="IO_21" pad="P4"/>
<connect gate="B" pin="IO_22" pad="P5"/>
<connect gate="B" pin="IO_23" pad="P6"/>
<connect gate="B" pin="IO_24" pad="R4"/>
<connect gate="B" pin="IO_25" pad="R5"/>
<connect gate="B" pin="IO_26" pad="R6"/>
<connect gate="B" pin="IO_27" pad="R7"/>
<connect gate="B" pin="IO_28" pad="R8"/>
<connect gate="B" pin="IO_29" pad="T3"/>
<connect gate="B" pin="IO_3" pad="N2"/>
<connect gate="B" pin="IO_30" pad="T4"/>
<connect gate="B" pin="IO_31" pad="T5"/>
<connect gate="B" pin="IO_32" pad="T6"/>
<connect gate="B" pin="IO_33" pad="T7"/>
<connect gate="B" pin="IO_34" pad="T8"/>
<connect gate="B" pin="IO_35" pad="A10"/>
<connect gate="B" pin="IO_36" pad="A11"/>
<connect gate="B" pin="IO_37" pad="A12"/>
<connect gate="B" pin="IO_38" pad="A13"/>
<connect gate="B" pin="IO_39" pad="A14"/>
<connect gate="B" pin="IO_4" pad="N3"/>
<connect gate="B" pin="IO_40" pad="B10"/>
<connect gate="B" pin="IO_41" pad="B11"/>
<connect gate="B" pin="IO_42" pad="B12"/>
<connect gate="B" pin="IO_43" pad="B13"/>
<connect gate="B" pin="IO_44" pad="B14"/>
<connect gate="B" pin="IO_45" pad="C11"/>
<connect gate="B" pin="IO_46" pad="C12"/>
<connect gate="B" pin="IO_47" pad="C13"/>
<connect gate="B" pin="IO_48" pad="C14"/>
<connect gate="B" pin="IO_49" pad="C15"/>
<connect gate="B" pin="IO_5" pad="L1"/>
<connect gate="B" pin="IO_50" pad="C16"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_55" pad="D15"/>
<connect gate="B" pin="IO_6" pad="M1"/>
<connect gate="B" pin="IO_7" pad="N4"/>
<connect gate="B" pin="IO_8" pad="M2"/>
<connect gate="B" pin="IO_9" pad="L2"/>
<connect gate="B" pin="VCCA_PLL1" pad="M5"/>
<connect gate="B" pin="VCCD_PLL1" pad="L6"/>
<connect gate="B" pin="VCCINT" pad="K8"/>
<connect gate="B" pin="VCCINT_2" pad="L7"/>
<connect gate="B" pin="VCCINT_3" pad="K6"/>
<connect gate="B" pin="VCCINT_4" pad="L8"/>
<connect gate="B" pin="VCCIO1" pad="R1"/>
<connect gate="B" pin="VCCIO4" pad="A15"/>
<connect gate="B" pin="VCCIO4_2" pad="C10"/>
<connect gate="B" pin="VCCIO5" pad="B16"/>
<connect gate="B" pin="VCCIO8" pad="T2"/>
<connect gate="B" pin="VCCIO8_2" pad="P7"/>
<connect gate="B" pin="VCCIO8_3" pad="M7"/>
<connect gate="C" pin="CLK12" pad="N10"/>
<connect gate="C" pin="CLK4" pad="H16"/>
<connect gate="C" pin="CLK5" pad="H15"/>
<connect gate="C" pin="CLK6" pad="J15"/>
<connect gate="C" pin="CLK7" pad="J16"/>
<connect gate="C" pin="CONF_DONE" pad="L13"/>
<connect gate="C" pin="GND" pad="R15"/>
<connect gate="C" pin="GNDA_PLL2" pad="E11"/>
<connect gate="C" pin="GNDA_PLL4" pad="M11"/>
<connect gate="C" pin="GND_2" pad="J14"/>
<connect gate="C" pin="GND_3" pad="K11"/>
<connect gate="C" pin="GND_4" pad="J11"/>
<connect gate="C" pin="GND_5" pad="T16"/>
<connect gate="C" pin="GND_6" pad="L10"/>
<connect gate="C" pin="GND_7" pad="G10"/>
<connect gate="C" pin="GND_8" pad="H14"/>
<connect gate="C" pin="GND_PLL2" pad="F12"/>
<connect gate="C" pin="GND_PLL4" pad="N12"/>
<connect gate="C" pin="GND_PLL4_2" pad="L12"/>
<connect gate="C" pin="IO" pad="T14"/>
<connect gate="C" pin="IO_10" pad="F15"/>
<connect gate="C" pin="IO_11" pad="F16"/>
<connect gate="C" pin="IO_12" pad="K15"/>
<connect gate="C" pin="IO_13" pad="K16"/>
<connect gate="C" pin="IO_14" pad="G12"/>
<connect gate="C" pin="IO_15" pad="G13"/>
<connect gate="C" pin="IO_16" pad="H12"/>
<connect gate="C" pin="IO_17" pad="G15"/>
<connect gate="C" pin="IO_18" pad="H13"/>
<connect gate="C" pin="IO_19" pad="G16"/>
<connect gate="C" pin="IO_2" pad="J12"/>
<connect gate="C" pin="IO_20" pad="M14"/>
<connect gate="C" pin="IO_21" pad="M15"/>
<connect gate="C" pin="IO_22" pad="L14"/>
<connect gate="C" pin="IO_23" pad="M16"/>
<connect gate="C" pin="IO_24" pad="L15"/>
<connect gate="C" pin="IO_25" pad="N11"/>
<connect gate="C" pin="IO_26" pad="L16"/>
<connect gate="C" pin="IO_27" pad="N13"/>
<connect gate="C" pin="IO_28" pad="N14"/>
<connect gate="C" pin="IO_29" pad="N15"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="N16"/>
<connect gate="C" pin="IO_31" pad="P11"/>
<connect gate="C" pin="IO_32" pad="P12"/>
<connect gate="C" pin="IO_33" pad="P13"/>
<connect gate="C" pin="IO_34" pad="P14"/>
<connect gate="C" pin="IO_35" pad="P15"/>
<connect gate="C" pin="IO_36" pad="P16"/>
<connect gate="C" pin="IO_37" pad="R10"/>
<connect gate="C" pin="IO_38" pad="R11"/>
<connect gate="C" pin="IO_39" pad="R12"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="R13"/>
<connect gate="C" pin="IO_41" pad="R14"/>
<connect gate="C" pin="IO_42" pad="T10"/>
<connect gate="C" pin="IO_43" pad="T11"/>
<connect gate="C" pin="IO_44" pad="T12"/>
<connect gate="C" pin="IO_45" pad="T13"/>
<connect gate="C" pin="IO_5" pad="K13"/>
<connect gate="C" pin="IO_6" pad="E15"/>
<connect gate="C" pin="IO_7" pad="E16"/>
<connect gate="C" pin="IO_8" pad="F13"/>
<connect gate="C" pin="IO_9" pad="F14"/>
<connect gate="C" pin="MSEL0" pad="J13"/>
<connect gate="C" pin="MSEL1" pad="K12"/>
<connect gate="C" pin="NSTATUS" pad="M13"/>
<connect gate="C" pin="VCCA_PLL2" pad="E12"/>
<connect gate="C" pin="VCCA_PLL4" pad="L11"/>
<connect gate="C" pin="VCCD_PLL2" pad="F11"/>
<connect gate="C" pin="VCCD_PLL4" pad="M12"/>
<connect gate="C" pin="VCCINT" pad="G11"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="F10"/>
<connect gate="C" pin="VCCINT_4" pad="H11"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="K10"/>
<connect gate="C" pin="VCCIO4" pad="E10"/>
<connect gate="C" pin="VCCIO5" pad="G14"/>
<connect gate="C" pin="VCCIO6" pad="K14"/>
<connect gate="C" pin="VCCIO6_2" pad="R16"/>
<connect gate="C" pin="VCCIO7" pad="T15"/>
<connect gate="C" pin="VCCIO7_2" pad="P10"/>
<connect gate="C" pin="VCCIO7_3" pad="M10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C20F256C8N"/>
<attribute name="OC_FARNELL" value="1453473"/>
<attribute name="OC_NEWARK" value="51R0560"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C20F256I8N">
<description>IC CYCLONE II FPGA</description>
<gates>
<gate name="A" symbol="EP2C20F256I8N_A"/>
<gate name="B" symbol="EP2C20F256I8N_B"/>
<gate name="C" symbol="EP2C20F256I8N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="CLK0" pad="H2"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="CLK10" pad="A8"/>
<connect gate="A" pin="CLK11" pad="B8"/>
<connect gate="A" pin="CLK2" pad="J2"/>
<connect gate="A" pin="CLK3" pad="J1"/>
<connect gate="A" pin="CLK8" pad="A9"/>
<connect gate="A" pin="CLK9" pad="B9"/>
<connect gate="A" pin="DATA0" pad="F1"/>
<connect gate="A" pin="DCLK" pad="H4"/>
<connect gate="A" pin="GND" pad="J9"/>
<connect gate="A" pin="GNDA_PLL3" pad="E6"/>
<connect gate="A" pin="GND_10" pad="F8"/>
<connect gate="A" pin="GND_11" pad="H3"/>
<connect gate="A" pin="GND_12" pad="H6"/>
<connect gate="A" pin="GND_13" pad="J8"/>
<connect gate="A" pin="GND_14" pad="C9"/>
<connect gate="A" pin="GND_15" pad="E8"/>
<connect gate="A" pin="GND_16" pad="J3"/>
<connect gate="A" pin="GND_17" pad="E9"/>
<connect gate="A" pin="GND_2" pad="A1"/>
<connect gate="A" pin="GND_3" pad="H9"/>
<connect gate="A" pin="GND_4" pad="B2"/>
<connect gate="A" pin="GND_5" pad="H8"/>
<connect gate="A" pin="GND_6" pad="G8"/>
<connect gate="A" pin="GND_7" pad="G6"/>
<connect gate="A" pin="GND_8" pad="C8"/>
<connect gate="A" pin="GND_9" pad="F7"/>
<connect gate="A" pin="GND_PLL3" pad="F5"/>
<connect gate="A" pin="GND_PLL3_2" pad="D5"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO_10" pad="C6"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="D4"/>
<connect gate="A" pin="IO_13" pad="B5"/>
<connect gate="A" pin="IO_14" pad="A5"/>
<connect gate="A" pin="IO_15" pad="D6"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="D7"/>
<connect gate="A" pin="IO_18" pad="A6"/>
<connect gate="A" pin="IO_19" pad="D8"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="B6"/>
<connect gate="A" pin="IO_21" pad="D9"/>
<connect gate="A" pin="IO_22" pad="A7"/>
<connect gate="A" pin="IO_23" pad="E1"/>
<connect gate="A" pin="IO_24" pad="C3"/>
<connect gate="A" pin="IO_25" pad="E2"/>
<connect gate="A" pin="IO_26" pad="B7"/>
<connect gate="A" pin="IO_27" pad="E3"/>
<connect gate="A" pin="IO_28" pad="C4"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="D1"/>
<connect gate="A" pin="IO_30" pad="F3"/>
<connect gate="A" pin="IO_31" pad="J4"/>
<connect gate="A" pin="IO_32" pad="F4"/>
<connect gate="A" pin="IO_33" pad="K1"/>
<connect gate="A" pin="IO_34" pad="K2"/>
<connect gate="A" pin="IO_35" pad="K4"/>
<connect gate="A" pin="IO_36" pad="G4"/>
<connect gate="A" pin="IO_4" pad="B4"/>
<connect gate="A" pin="IO_5" pad="D2"/>
<connect gate="A" pin="IO_6" pad="A3"/>
<connect gate="A" pin="IO_7" pad="D3"/>
<connect gate="A" pin="IO_8" pad="C1"/>
<connect gate="A" pin="IO_9" pad="C5"/>
<connect gate="A" pin="NCE" pad="G5"/>
<connect gate="A" pin="NCONFIG" pad="J5"/>
<connect gate="A" pin="TCK" pad="F2"/>
<connect gate="A" pin="TDI" pad="H5"/>
<connect gate="A" pin="TDO" pad="G2"/>
<connect gate="A" pin="TMS" pad="G1"/>
<connect gate="A" pin="VCCA_PLL3" pad="F6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="J6"/>
<connect gate="A" pin="VCCINT_2" pad="F9"/>
<connect gate="A" pin="VCCINT_3" pad="H7"/>
<connect gate="A" pin="VCCINT_4" pad="G7"/>
<connect gate="A" pin="VCCINT_5" pad="G9"/>
<connect gate="A" pin="VCCINT_6" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="K3"/>
<connect gate="A" pin="VCCIO2" pad="G3"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO3" pad="C7"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="E7"/>
<connect gate="B" pin="CLK13" pad="N9"/>
<connect gate="B" pin="CLK14" pad="R9"/>
<connect gate="B" pin="CLK15" pad="T9"/>
<connect gate="B" pin="GND" pad="B15"/>
<connect gate="B" pin="GNDA_PLL1" pad="M6"/>
<connect gate="B" pin="GND_10" pad="T1"/>
<connect gate="B" pin="GND_11" pad="A16"/>
<connect gate="B" pin="GND_2" pad="K7"/>
<connect gate="B" pin="GND_3" pad="L9"/>
<connect gate="B" pin="GND_4" pad="M8"/>
<connect gate="B" pin="GND_5" pad="P8"/>
<connect gate="B" pin="GND_6" pad="M9"/>
<connect gate="B" pin="GND_7" pad="P9"/>
<connect gate="B" pin="GND_8" pad="R2"/>
<connect gate="B" pin="GND_9" pad="K9"/>
<connect gate="B" pin="GND_PLL1" pad="L5"/>
<connect gate="B" pin="GND_PLL1_2" pad="N5"/>
<connect gate="B" pin="GND_PLL2" pad="D12"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="M3"/>
<connect gate="B" pin="IO_11" pad="N6"/>
<connect gate="B" pin="IO_12" pad="L3"/>
<connect gate="B" pin="IO_13" pad="N7"/>
<connect gate="B" pin="IO_14" pad="L4"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P1"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N1"/>
<connect gate="B" pin="IO_20" pad="P3"/>
<connect gate="B" pin="IO_21" pad="P4"/>
<connect gate="B" pin="IO_22" pad="P5"/>
<connect gate="B" pin="IO_23" pad="P6"/>
<connect gate="B" pin="IO_24" pad="R4"/>
<connect gate="B" pin="IO_25" pad="R5"/>
<connect gate="B" pin="IO_26" pad="R6"/>
<connect gate="B" pin="IO_27" pad="R7"/>
<connect gate="B" pin="IO_28" pad="R8"/>
<connect gate="B" pin="IO_29" pad="T3"/>
<connect gate="B" pin="IO_3" pad="N2"/>
<connect gate="B" pin="IO_30" pad="T4"/>
<connect gate="B" pin="IO_31" pad="T5"/>
<connect gate="B" pin="IO_32" pad="T6"/>
<connect gate="B" pin="IO_33" pad="T7"/>
<connect gate="B" pin="IO_34" pad="T8"/>
<connect gate="B" pin="IO_35" pad="A10"/>
<connect gate="B" pin="IO_36" pad="A11"/>
<connect gate="B" pin="IO_37" pad="A12"/>
<connect gate="B" pin="IO_38" pad="A13"/>
<connect gate="B" pin="IO_39" pad="A14"/>
<connect gate="B" pin="IO_4" pad="N3"/>
<connect gate="B" pin="IO_40" pad="B10"/>
<connect gate="B" pin="IO_41" pad="B11"/>
<connect gate="B" pin="IO_42" pad="B12"/>
<connect gate="B" pin="IO_43" pad="B13"/>
<connect gate="B" pin="IO_44" pad="B14"/>
<connect gate="B" pin="IO_45" pad="C11"/>
<connect gate="B" pin="IO_46" pad="C12"/>
<connect gate="B" pin="IO_47" pad="C13"/>
<connect gate="B" pin="IO_48" pad="C14"/>
<connect gate="B" pin="IO_49" pad="C15"/>
<connect gate="B" pin="IO_5" pad="L1"/>
<connect gate="B" pin="IO_50" pad="C16"/>
<connect gate="B" pin="IO_51" pad="D10"/>
<connect gate="B" pin="IO_52" pad="D11"/>
<connect gate="B" pin="IO_53" pad="D13"/>
<connect gate="B" pin="IO_54" pad="D14"/>
<connect gate="B" pin="IO_55" pad="D15"/>
<connect gate="B" pin="IO_6" pad="M1"/>
<connect gate="B" pin="IO_7" pad="N4"/>
<connect gate="B" pin="IO_8" pad="M2"/>
<connect gate="B" pin="IO_9" pad="L2"/>
<connect gate="B" pin="VCCA_PLL1" pad="M5"/>
<connect gate="B" pin="VCCD_PLL1" pad="L6"/>
<connect gate="B" pin="VCCINT" pad="K8"/>
<connect gate="B" pin="VCCINT_2" pad="L7"/>
<connect gate="B" pin="VCCINT_3" pad="K6"/>
<connect gate="B" pin="VCCINT_4" pad="L8"/>
<connect gate="B" pin="VCCIO1" pad="R1"/>
<connect gate="B" pin="VCCIO4" pad="A15"/>
<connect gate="B" pin="VCCIO4_2" pad="C10"/>
<connect gate="B" pin="VCCIO5" pad="B16"/>
<connect gate="B" pin="VCCIO8" pad="T2"/>
<connect gate="B" pin="VCCIO8_2" pad="P7"/>
<connect gate="B" pin="VCCIO8_3" pad="M7"/>
<connect gate="C" pin="CLK12" pad="N10"/>
<connect gate="C" pin="CLK4" pad="H16"/>
<connect gate="C" pin="CLK5" pad="H15"/>
<connect gate="C" pin="CLK6" pad="J15"/>
<connect gate="C" pin="CLK7" pad="J16"/>
<connect gate="C" pin="CONF_DONE" pad="L13"/>
<connect gate="C" pin="GND" pad="R15"/>
<connect gate="C" pin="GNDA_PLL2" pad="E11"/>
<connect gate="C" pin="GNDA_PLL4" pad="M11"/>
<connect gate="C" pin="GND_2" pad="J14"/>
<connect gate="C" pin="GND_3" pad="K11"/>
<connect gate="C" pin="GND_4" pad="J11"/>
<connect gate="C" pin="GND_5" pad="T16"/>
<connect gate="C" pin="GND_6" pad="L10"/>
<connect gate="C" pin="GND_7" pad="G10"/>
<connect gate="C" pin="GND_8" pad="H14"/>
<connect gate="C" pin="GND_PLL2" pad="F12"/>
<connect gate="C" pin="GND_PLL4" pad="N12"/>
<connect gate="C" pin="GND_PLL4_2" pad="L12"/>
<connect gate="C" pin="IO" pad="T14"/>
<connect gate="C" pin="IO_10" pad="F15"/>
<connect gate="C" pin="IO_11" pad="F16"/>
<connect gate="C" pin="IO_12" pad="K15"/>
<connect gate="C" pin="IO_13" pad="K16"/>
<connect gate="C" pin="IO_14" pad="G12"/>
<connect gate="C" pin="IO_15" pad="G13"/>
<connect gate="C" pin="IO_16" pad="H12"/>
<connect gate="C" pin="IO_17" pad="G15"/>
<connect gate="C" pin="IO_18" pad="H13"/>
<connect gate="C" pin="IO_19" pad="G16"/>
<connect gate="C" pin="IO_2" pad="J12"/>
<connect gate="C" pin="IO_20" pad="M14"/>
<connect gate="C" pin="IO_21" pad="M15"/>
<connect gate="C" pin="IO_22" pad="L14"/>
<connect gate="C" pin="IO_23" pad="M16"/>
<connect gate="C" pin="IO_24" pad="L15"/>
<connect gate="C" pin="IO_25" pad="N11"/>
<connect gate="C" pin="IO_26" pad="L16"/>
<connect gate="C" pin="IO_27" pad="N13"/>
<connect gate="C" pin="IO_28" pad="N14"/>
<connect gate="C" pin="IO_29" pad="N15"/>
<connect gate="C" pin="IO_3" pad="E13"/>
<connect gate="C" pin="IO_30" pad="N16"/>
<connect gate="C" pin="IO_31" pad="P11"/>
<connect gate="C" pin="IO_32" pad="P12"/>
<connect gate="C" pin="IO_33" pad="P13"/>
<connect gate="C" pin="IO_34" pad="P14"/>
<connect gate="C" pin="IO_35" pad="P15"/>
<connect gate="C" pin="IO_36" pad="P16"/>
<connect gate="C" pin="IO_37" pad="R10"/>
<connect gate="C" pin="IO_38" pad="R11"/>
<connect gate="C" pin="IO_39" pad="R12"/>
<connect gate="C" pin="IO_4" pad="E14"/>
<connect gate="C" pin="IO_40" pad="R13"/>
<connect gate="C" pin="IO_41" pad="R14"/>
<connect gate="C" pin="IO_42" pad="T10"/>
<connect gate="C" pin="IO_43" pad="T11"/>
<connect gate="C" pin="IO_44" pad="T12"/>
<connect gate="C" pin="IO_45" pad="T13"/>
<connect gate="C" pin="IO_5" pad="K13"/>
<connect gate="C" pin="IO_6" pad="E15"/>
<connect gate="C" pin="IO_7" pad="E16"/>
<connect gate="C" pin="IO_8" pad="F13"/>
<connect gate="C" pin="IO_9" pad="F14"/>
<connect gate="C" pin="MSEL0" pad="J13"/>
<connect gate="C" pin="MSEL1" pad="K12"/>
<connect gate="C" pin="NSTATUS" pad="M13"/>
<connect gate="C" pin="VCCA_PLL2" pad="E12"/>
<connect gate="C" pin="VCCA_PLL4" pad="L11"/>
<connect gate="C" pin="VCCD_PLL2" pad="F11"/>
<connect gate="C" pin="VCCD_PLL4" pad="M12"/>
<connect gate="C" pin="VCCINT" pad="G11"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="F10"/>
<connect gate="C" pin="VCCINT_4" pad="H11"/>
<connect gate="C" pin="VCCINT_5" pad="J10"/>
<connect gate="C" pin="VCCINT_6" pad="K10"/>
<connect gate="C" pin="VCCIO4" pad="E10"/>
<connect gate="C" pin="VCCIO5" pad="G14"/>
<connect gate="C" pin="VCCIO6" pad="K14"/>
<connect gate="C" pin="VCCIO6_2" pad="R16"/>
<connect gate="C" pin="VCCIO7" pad="T15"/>
<connect gate="C" pin="VCCIO7_2" pad="P10"/>
<connect gate="C" pin="VCCIO7_3" pad="M10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C20F256I8N"/>
<attribute name="OC_FARNELL" value="1663195"/>
<attribute name="OC_NEWARK" value="52R0507"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C20F484C8N">
<description>IC CYCLONE II FPGA</description>
<gates>
<gate name="A" symbol="EP2C20F484C8N_A"/>
<gate name="B" symbol="EP2C20F484C8N_B"/>
<gate name="C" symbol="EP2C20F484C8N_C"/>
<gate name="D" symbol="EP2C20F484C8N_D"/>
<gate name="E" symbol="EP2C20F484C8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K7"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_2" pad="C5"/>
<connect gate="A" pin="GND_3" pad="K3"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="G4"/>
<connect gate="A" pin="GND_6" pad="A1"/>
<connect gate="A" pin="GND_7" pad="B2"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J4"/>
<connect gate="A" pin="IO_10" pad="A7"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="C9"/>
<connect gate="A" pin="IO_13" pad="A9"/>
<connect gate="A" pin="IO_14" pad="D1"/>
<connect gate="A" pin="IO_15" pad="D2"/>
<connect gate="A" pin="IO_16" pad="D3"/>
<connect gate="A" pin="IO_17" pad="D4"/>
<connect gate="A" pin="IO_18" pad="D5"/>
<connect gate="A" pin="IO_19" pad="D6"/>
<connect gate="A" pin="IO_2" pad="C2"/>
<connect gate="A" pin="IO_20" pad="D7"/>
<connect gate="A" pin="IO_21" pad="B3"/>
<connect gate="A" pin="IO_22" pad="D8"/>
<connect gate="A" pin="IO_23" pad="B4"/>
<connect gate="A" pin="IO_24" pad="D9"/>
<connect gate="A" pin="IO_25" pad="B5"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="B6"/>
<connect gate="A" pin="IO_28" pad="E2"/>
<connect gate="A" pin="IO_29" pad="B7"/>
<connect gate="A" pin="IO_3" pad="C3"/>
<connect gate="A" pin="IO_30" pad="E7"/>
<connect gate="A" pin="IO_31" pad="B8"/>
<connect gate="A" pin="IO_32" pad="B9"/>
<connect gate="A" pin="IO_33" pad="E3"/>
<connect gate="A" pin="IO_34" pad="E8"/>
<connect gate="A" pin="IO_35" pad="C1"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G3"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="H1"/>
<connect gate="A" pin="IO_5" pad="C4"/>
<connect gate="A" pin="IO_50" pad="H2"/>
<connect gate="A" pin="IO_51" pad="H3"/>
<connect gate="A" pin="IO_52" pad="H4"/>
<connect gate="A" pin="IO_53" pad="H5"/>
<connect gate="A" pin="IO_54" pad="H6"/>
<connect gate="A" pin="IO_55" pad="H7"/>
<connect gate="A" pin="IO_56" pad="H8"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J1"/>
<connect gate="A" pin="IO_59" pad="J2"/>
<connect gate="A" pin="IO_6" pad="A4"/>
<connect gate="A" pin="IO_7" pad="A5"/>
<connect gate="A" pin="IO_8" pad="A6"/>
<connect gate="A" pin="IO_9" pad="C7"/>
<connect gate="A" pin="NC" pad="K8"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="NC_2" pad="G1"/>
<connect gate="A" pin="NC_3" pad="G2"/>
<connect gate="A" pin="NC_4" pad="J3"/>
<connect gate="A" pin="NC_5" pad="J5"/>
<connect gate="A" pin="NC_6" pad="J6"/>
<connect gate="A" pin="NC_7" pad="L7"/>
<connect gate="A" pin="NC_8" pad="J8"/>
<connect gate="A" pin="NC_9" pad="J9"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="L3"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="J7"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="C6"/>
<connect gate="A" pin="VCCIO3_3" pad="A2"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="A22"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_2" pad="N7"/>
<connect gate="B" pin="GND_3" pad="M4"/>
<connect gate="B" pin="GND_4" pad="R3"/>
<connect gate="B" pin="GND_5" pad="Y8"/>
<connect gate="B" pin="GND_6" pad="V3"/>
<connect gate="B" pin="GND_7" pad="V6"/>
<connect gate="B" pin="GND_PLL1" pad="V5"/>
<connect gate="B" pin="GND_PLL1_2" pad="U5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="N1"/>
<connect gate="B" pin="IO_11" pad="R6"/>
<connect gate="B" pin="IO_12" pad="R1"/>
<connect gate="B" pin="IO_13" pad="R7"/>
<connect gate="B" pin="IO_14" pad="P6"/>
<connect gate="B" pin="IO_15" pad="R8"/>
<connect gate="B" pin="IO_16" pad="R2"/>
<connect gate="B" pin="IO_17" pad="R9"/>
<connect gate="B" pin="IO_18" pad="M5"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="P1"/>
<connect gate="B" pin="IO_20" pad="N2"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="M6"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="N3"/>
<connect gate="B" pin="IO_25" pad="U1"/>
<connect gate="B" pin="IO_26" pad="N4"/>
<connect gate="B" pin="IO_27" pad="T5"/>
<connect gate="B" pin="IO_28" pad="T6"/>
<connect gate="B" pin="IO_29" pad="N6"/>
<connect gate="B" pin="IO_3" pad="P2"/>
<connect gate="B" pin="IO_30" pad="T7"/>
<connect gate="B" pin="IO_31" pad="T8"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U3"/>
<connect gate="B" pin="IO_34" pad="U4"/>
<connect gate="B" pin="IO_35" pad="U8"/>
<connect gate="B" pin="IO_36" pad="U9"/>
<connect gate="B" pin="IO_37" pad="V1"/>
<connect gate="B" pin="IO_38" pad="V2"/>
<connect gate="B" pin="IO_39" pad="V4"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_40" pad="V8"/>
<connect gate="B" pin="IO_41" pad="V9"/>
<connect gate="B" pin="IO_42" pad="W1"/>
<connect gate="B" pin="IO_43" pad="W2"/>
<connect gate="B" pin="IO_44" pad="W3"/>
<connect gate="B" pin="IO_45" pad="W4"/>
<connect gate="B" pin="IO_46" pad="W5"/>
<connect gate="B" pin="IO_47" pad="W7"/>
<connect gate="B" pin="IO_48" pad="W8"/>
<connect gate="B" pin="IO_49" pad="W9"/>
<connect gate="B" pin="IO_5" pad="P3"/>
<connect gate="B" pin="IO_50" pad="Y1"/>
<connect gate="B" pin="IO_51" pad="Y2"/>
<connect gate="B" pin="IO_52" pad="Y3"/>
<connect gate="B" pin="IO_53" pad="Y4"/>
<connect gate="B" pin="IO_54" pad="Y5"/>
<connect gate="B" pin="IO_55" pad="Y6"/>
<connect gate="B" pin="IO_56" pad="Y7"/>
<connect gate="B" pin="IO_57" pad="Y9"/>
<connect gate="B" pin="IO_58" pad="A10"/>
<connect gate="B" pin="IO_59" pad="A11"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_60" pad="A13"/>
<connect gate="B" pin="IO_61" pad="A14"/>
<connect gate="B" pin="IO_62" pad="A15"/>
<connect gate="B" pin="IO_63" pad="A16"/>
<connect gate="B" pin="IO_64" pad="A17"/>
<connect gate="B" pin="IO_65" pad="A18"/>
<connect gate="B" pin="IO_66" pad="A19"/>
<connect gate="B" pin="IO_7" pad="P5"/>
<connect gate="B" pin="IO_8" pad="P9"/>
<connect gate="B" pin="IO_9" pad="R5"/>
<connect gate="B" pin="NC" pad="P4"/>
<connect gate="B" pin="NC_2" pad="M7"/>
<connect gate="B" pin="NC_3" pad="M8"/>
<connect gate="B" pin="NC_4" pad="N8"/>
<connect gate="B" pin="NC_5" pad="R4"/>
<connect gate="B" pin="NC_6" pad="N5"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="L9"/>
<connect gate="B" pin="VCCINT_2" pad="M9"/>
<connect gate="B" pin="VCCINT_3" pad="N9"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="M3"/>
<connect gate="B" pin="VCCIO1_3" pad="T4"/>
<connect gate="B" pin="VCCIO1_4" pad="P7"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="W6"/>
<connect gate="B" pin="VCCIO8_2" pad="T9"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="G13"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="C15"/>
<connect gate="C" pin="GND_2" pad="D10"/>
<connect gate="C" pin="GND_3" pad="D13"/>
<connect gate="C" pin="GND_4" pad="D18"/>
<connect gate="C" pin="GND_5" pad="F19"/>
<connect gate="C" pin="GND_6" pad="AA2"/>
<connect gate="C" pin="GND_7" pad="AB1"/>
<connect gate="C" pin="GND_8" pad="G10"/>
<connect gate="C" pin="GND_9" pad="B21"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="AB5"/>
<connect gate="C" pin="IO_11" pad="AB6"/>
<connect gate="C" pin="IO_12" pad="AB7"/>
<connect gate="C" pin="IO_13" pad="C10"/>
<connect gate="C" pin="IO_14" pad="AB3"/>
<connect gate="C" pin="IO_15" pad="AB8"/>
<connect gate="C" pin="IO_16" pad="AB9"/>
<connect gate="C" pin="IO_17" pad="C13"/>
<connect gate="C" pin="IO_18" pad="B10"/>
<connect gate="C" pin="IO_19" pad="C14"/>
<connect gate="C" pin="IO_2" pad="AA3"/>
<connect gate="C" pin="IO_20" pad="B11"/>
<connect gate="C" pin="IO_21" pad="C16"/>
<connect gate="C" pin="IO_22" pad="B13"/>
<connect gate="C" pin="IO_23" pad="C17"/>
<connect gate="C" pin="IO_24" pad="B14"/>
<connect gate="C" pin="IO_25" pad="C18"/>
<connect gate="C" pin="IO_26" pad="B15"/>
<connect gate="C" pin="IO_27" pad="C19"/>
<connect gate="C" pin="IO_28" pad="B16"/>
<connect gate="C" pin="IO_29" pad="C20"/>
<connect gate="C" pin="IO_3" pad="AA4"/>
<connect gate="C" pin="IO_30" pad="B17"/>
<connect gate="C" pin="IO_31" pad="C21"/>
<connect gate="C" pin="IO_32" pad="B18"/>
<connect gate="C" pin="IO_33" pad="C22"/>
<connect gate="C" pin="IO_34" pad="B19"/>
<connect gate="C" pin="IO_35" pad="D14"/>
<connect gate="C" pin="IO_36" pad="B20"/>
<connect gate="C" pin="IO_37" pad="D11"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AA5"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="AA6"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AA7"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G11"/>
<connect gate="C" pin="IO_62" pad="G12"/>
<connect gate="C" pin="IO_63" pad="G15"/>
<connect gate="C" pin="IO_64" pad="G16"/>
<connect gate="C" pin="IO_65" pad="G17"/>
<connect gate="C" pin="IO_66" pad="G18"/>
<connect gate="C" pin="IO_67" pad="G20"/>
<connect gate="C" pin="IO_68" pad="G21"/>
<connect gate="C" pin="IO_69" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AA8"/>
<connect gate="C" pin="IO_70" pad="H10"/>
<connect gate="C" pin="IO_8" pad="AB4"/>
<connect gate="C" pin="IO_9" pad="AA9"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="G14"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="D17"/>
<connect gate="C" pin="VCCIO5" pad="G19"/>
<connect gate="C" pin="VCCIO5_2" pad="B22"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="N19"/>
<connect gate="D" pin="GND_10" pad="L13"/>
<connect gate="D" pin="GND_11" pad="K12"/>
<connect gate="D" pin="GND_12" pad="H20"/>
<connect gate="D" pin="GND_13" pad="M10"/>
<connect gate="D" pin="GND_14" pad="M11"/>
<connect gate="D" pin="GND_15" pad="M12"/>
<connect gate="D" pin="GND_16" pad="N10"/>
<connect gate="D" pin="GND_17" pad="M13"/>
<connect gate="D" pin="GND_18" pad="N11"/>
<connect gate="D" pin="GND_19" pad="N12"/>
<connect gate="D" pin="GND_2" pad="K19"/>
<connect gate="D" pin="GND_20" pad="N16"/>
<connect gate="D" pin="GND_21" pad="N13"/>
<connect gate="D" pin="GND_3" pad="K13"/>
<connect gate="D" pin="GND_4" pad="K16"/>
<connect gate="D" pin="GND_5" pad="L10"/>
<connect gate="D" pin="GND_6" pad="K10"/>
<connect gate="D" pin="GND_7" pad="L11"/>
<connect gate="D" pin="GND_8" pad="K11"/>
<connect gate="D" pin="GND_9" pad="L12"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J14"/>
<connect gate="D" pin="IO_11" pad="J15"/>
<connect gate="D" pin="IO_12" pad="L18"/>
<connect gate="D" pin="IO_13" pad="L19"/>
<connect gate="D" pin="IO_14" pad="J17"/>
<connect gate="D" pin="IO_15" pad="J18"/>
<connect gate="D" pin="IO_16" pad="K20"/>
<connect gate="D" pin="IO_17" pad="J19"/>
<connect gate="D" pin="IO_18" pad="K21"/>
<connect gate="D" pin="IO_19" pad="J20"/>
<connect gate="D" pin="IO_2" pad="H12"/>
<connect gate="D" pin="IO_20" pad="K22"/>
<connect gate="D" pin="IO_21" pad="J21"/>
<connect gate="D" pin="IO_22" pad="J22"/>
<connect gate="D" pin="IO_23" pad="M18"/>
<connect gate="D" pin="IO_24" pad="M19"/>
<connect gate="D" pin="IO_25" pad="N15"/>
<connect gate="D" pin="IO_26" pad="N21"/>
<connect gate="D" pin="IO_27" pad="N22"/>
<connect gate="D" pin="IO_28" pad="P15"/>
<connect gate="D" pin="IO_29" pad="P17"/>
<connect gate="D" pin="IO_3" pad="H13"/>
<connect gate="D" pin="IO_30" pad="P18"/>
<connect gate="D" pin="IO_31" pad="R10"/>
<connect gate="D" pin="IO_32" pad="R11"/>
<connect gate="D" pin="IO_33" pad="R12"/>
<connect gate="D" pin="IO_34" pad="R13"/>
<connect gate="D" pin="IO_35" pad="R14"/>
<connect gate="D" pin="IO_36" pad="R15"/>
<connect gate="D" pin="IO_37" pad="R16"/>
<connect gate="D" pin="IO_4" pad="H14"/>
<connect gate="D" pin="IO_5" pad="H15"/>
<connect gate="D" pin="IO_6" pad="H16"/>
<connect gate="D" pin="IO_7" pad="H17"/>
<connect gate="D" pin="IO_8" pad="H18"/>
<connect gate="D" pin="IO_9" pad="H19"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NC" pad="M16"/>
<connect gate="D" pin="NC_10" pad="P21"/>
<connect gate="D" pin="NC_11" pad="K18"/>
<connect gate="D" pin="NC_12" pad="P22"/>
<connect gate="D" pin="NC_13" pad="L16"/>
<connect gate="D" pin="NC_14" pad="L17"/>
<connect gate="D" pin="NC_15" pad="M15"/>
<connect gate="D" pin="NC_2" pad="H22"/>
<connect gate="D" pin="NC_3" pad="P14"/>
<connect gate="D" pin="NC_4" pad="K15"/>
<connect gate="D" pin="NC_5" pad="H21"/>
<connect gate="D" pin="NC_6" pad="P19"/>
<connect gate="D" pin="NC_7" pad="K17"/>
<connect gate="D" pin="NC_8" pad="P20"/>
<connect gate="D" pin="NC_9" pad="L15"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="L14"/>
<connect gate="D" pin="VCCINT_10" pad="K14"/>
<connect gate="D" pin="VCCINT_11" pad="N14"/>
<connect gate="D" pin="VCCINT_12" pad="P13"/>
<connect gate="D" pin="VCCINT_2" pad="P10"/>
<connect gate="D" pin="VCCINT_3" pad="J10"/>
<connect gate="D" pin="VCCINT_4" pad="P11"/>
<connect gate="D" pin="VCCINT_5" pad="J11"/>
<connect gate="D" pin="VCCINT_6" pad="M14"/>
<connect gate="D" pin="VCCINT_7" pad="J12"/>
<connect gate="D" pin="VCCINT_8" pad="P12"/>
<connect gate="D" pin="VCCINT_9" pad="J13"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="M20"/>
<connect gate="D" pin="VCCIO6_2" pad="P16"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AA21"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="W19"/>
<connect gate="E" pin="GND_2" pad="Y15"/>
<connect gate="E" pin="GND_3" pad="T10"/>
<connect gate="E" pin="GND_4" pad="T20"/>
<connect gate="E" pin="GND_5" pad="T13"/>
<connect gate="E" pin="GND_6" pad="AB22"/>
<connect gate="E" pin="GND_7" pad="V17"/>
<connect gate="E" pin="GND_8" pad="W13"/>
<connect gate="E" pin="GND_9" pad="W10"/>
<connect gate="E" pin="GND_PLL4" pad="V18"/>
<connect gate="E" pin="GND_PLL4_2" pad="T17"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="T16"/>
<connect gate="E" pin="IO_11" pad="U18"/>
<connect gate="E" pin="IO_12" pad="R22"/>
<connect gate="E" pin="IO_13" pad="T18"/>
<connect gate="E" pin="IO_14" pad="U19"/>
<connect gate="E" pin="IO_15" pad="U20"/>
<connect gate="E" pin="IO_16" pad="T11"/>
<connect gate="E" pin="IO_17" pad="T21"/>
<connect gate="E" pin="IO_18" pad="U21"/>
<connect gate="E" pin="IO_19" pad="T12"/>
<connect gate="E" pin="IO_2" pad="U13"/>
<connect gate="E" pin="IO_20" pad="T22"/>
<connect gate="E" pin="IO_21" pad="V19"/>
<connect gate="E" pin="IO_22" pad="U10"/>
<connect gate="E" pin="IO_23" pad="V20"/>
<connect gate="E" pin="IO_24" pad="U22"/>
<connect gate="E" pin="IO_25" pad="V21"/>
<connect gate="E" pin="IO_26" pad="V14"/>
<connect gate="E" pin="IO_27" pad="V22"/>
<connect gate="E" pin="IO_28" pad="V15"/>
<connect gate="E" pin="IO_29" pad="W11"/>
<connect gate="E" pin="IO_3" pad="U14"/>
<connect gate="E" pin="IO_30" pad="V11"/>
<connect gate="E" pin="IO_31" pad="W14"/>
<connect gate="E" pin="IO_32" pad="W15"/>
<connect gate="E" pin="IO_33" pad="W16"/>
<connect gate="E" pin="IO_34" pad="W20"/>
<connect gate="E" pin="IO_35" pad="W21"/>
<connect gate="E" pin="IO_36" pad="W22"/>
<connect gate="E" pin="IO_37" pad="Y10"/>
<connect gate="E" pin="IO_38" pad="Y13"/>
<connect gate="E" pin="IO_39" pad="Y14"/>
<connect gate="E" pin="IO_4" pad="R18"/>
<connect gate="E" pin="IO_40" pad="Y16"/>
<connect gate="E" pin="IO_41" pad="Y17"/>
<connect gate="E" pin="IO_42" pad="Y18"/>
<connect gate="E" pin="IO_43" pad="Y19"/>
<connect gate="E" pin="IO_44" pad="Y20"/>
<connect gate="E" pin="IO_45" pad="Y21"/>
<connect gate="E" pin="IO_46" pad="Y22"/>
<connect gate="E" pin="IO_47" pad="AA10"/>
<connect gate="E" pin="IO_48" pad="AA11"/>
<connect gate="E" pin="IO_49" pad="AA12"/>
<connect gate="E" pin="IO_5" pad="U15"/>
<connect gate="E" pin="IO_50" pad="AA13"/>
<connect gate="E" pin="IO_51" pad="AA14"/>
<connect gate="E" pin="IO_52" pad="AA15"/>
<connect gate="E" pin="IO_53" pad="AA16"/>
<connect gate="E" pin="IO_54" pad="AA17"/>
<connect gate="E" pin="IO_55" pad="AA18"/>
<connect gate="E" pin="IO_56" pad="AA19"/>
<connect gate="E" pin="IO_57" pad="AA20"/>
<connect gate="E" pin="IO_58" pad="AB10"/>
<connect gate="E" pin="IO_59" pad="AB11"/>
<connect gate="E" pin="IO_6" pad="R19"/>
<connect gate="E" pin="IO_60" pad="AB12"/>
<connect gate="E" pin="IO_61" pad="AB13"/>
<connect gate="E" pin="IO_62" pad="AB14"/>
<connect gate="E" pin="IO_63" pad="AB15"/>
<connect gate="E" pin="IO_64" pad="AB16"/>
<connect gate="E" pin="IO_65" pad="AB17"/>
<connect gate="E" pin="IO_66" pad="AB18"/>
<connect gate="E" pin="IO_67" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="R20"/>
<connect gate="E" pin="IO_8" pad="R21"/>
<connect gate="E" pin="IO_9" pad="T15"/>
<connect gate="E" pin="NC" pad="W18"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCIO6" pad="T19"/>
<connect gate="E" pin="VCCIO6_2" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="Y12"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="AB21"/>
<connect gate="E" pin="VCCIO7_4" pad="V13"/>
<connect gate="E" pin="VCCIO7_5" pad="W17"/>
<connect gate="E" pin="VCCIO8" pad="Y11"/>
<connect gate="E" pin="VCCIO8_2" pad="V10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C20F484C8N"/>
<attribute name="OC_FARNELL" value="1635083"/>
<attribute name="OC_NEWARK" value="51R0561"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C20F484I8N">
<description>IC CYCLONE II FPGA</description>
<gates>
<gate name="A" symbol="EP2C20F484I8N_A"/>
<gate name="B" symbol="EP2C20F484I8N_B"/>
<gate name="C" symbol="EP2C20F484I8N_C"/>
<gate name="D" symbol="EP2C20F484I8N_D"/>
<gate name="E" symbol="EP2C20F484I8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K7"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_2" pad="C5"/>
<connect gate="A" pin="GND_3" pad="K3"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="G4"/>
<connect gate="A" pin="GND_6" pad="A1"/>
<connect gate="A" pin="GND_7" pad="B2"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J4"/>
<connect gate="A" pin="IO_10" pad="A7"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="C9"/>
<connect gate="A" pin="IO_13" pad="A9"/>
<connect gate="A" pin="IO_14" pad="D1"/>
<connect gate="A" pin="IO_15" pad="D2"/>
<connect gate="A" pin="IO_16" pad="D3"/>
<connect gate="A" pin="IO_17" pad="D4"/>
<connect gate="A" pin="IO_18" pad="D5"/>
<connect gate="A" pin="IO_19" pad="D6"/>
<connect gate="A" pin="IO_2" pad="C2"/>
<connect gate="A" pin="IO_20" pad="D7"/>
<connect gate="A" pin="IO_21" pad="B3"/>
<connect gate="A" pin="IO_22" pad="D8"/>
<connect gate="A" pin="IO_23" pad="B4"/>
<connect gate="A" pin="IO_24" pad="D9"/>
<connect gate="A" pin="IO_25" pad="B5"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="B6"/>
<connect gate="A" pin="IO_28" pad="E2"/>
<connect gate="A" pin="IO_29" pad="B7"/>
<connect gate="A" pin="IO_3" pad="C3"/>
<connect gate="A" pin="IO_30" pad="E7"/>
<connect gate="A" pin="IO_31" pad="B8"/>
<connect gate="A" pin="IO_32" pad="B9"/>
<connect gate="A" pin="IO_33" pad="E3"/>
<connect gate="A" pin="IO_34" pad="E8"/>
<connect gate="A" pin="IO_35" pad="C1"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G3"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="H1"/>
<connect gate="A" pin="IO_5" pad="C4"/>
<connect gate="A" pin="IO_50" pad="H2"/>
<connect gate="A" pin="IO_51" pad="H3"/>
<connect gate="A" pin="IO_52" pad="H4"/>
<connect gate="A" pin="IO_53" pad="H5"/>
<connect gate="A" pin="IO_54" pad="H6"/>
<connect gate="A" pin="IO_55" pad="H7"/>
<connect gate="A" pin="IO_56" pad="H8"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J1"/>
<connect gate="A" pin="IO_59" pad="J2"/>
<connect gate="A" pin="IO_6" pad="A4"/>
<connect gate="A" pin="IO_7" pad="A5"/>
<connect gate="A" pin="IO_8" pad="A6"/>
<connect gate="A" pin="IO_9" pad="C7"/>
<connect gate="A" pin="NC" pad="K8"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="NC_2" pad="G1"/>
<connect gate="A" pin="NC_3" pad="G2"/>
<connect gate="A" pin="NC_4" pad="J3"/>
<connect gate="A" pin="NC_5" pad="J5"/>
<connect gate="A" pin="NC_6" pad="J6"/>
<connect gate="A" pin="NC_7" pad="L7"/>
<connect gate="A" pin="NC_8" pad="J8"/>
<connect gate="A" pin="NC_9" pad="J9"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="L3"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="J7"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="C6"/>
<connect gate="A" pin="VCCIO3_3" pad="A2"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="A22"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_2" pad="N7"/>
<connect gate="B" pin="GND_3" pad="M4"/>
<connect gate="B" pin="GND_4" pad="R3"/>
<connect gate="B" pin="GND_5" pad="Y8"/>
<connect gate="B" pin="GND_6" pad="V3"/>
<connect gate="B" pin="GND_7" pad="V6"/>
<connect gate="B" pin="GND_PLL1" pad="V5"/>
<connect gate="B" pin="GND_PLL1_2" pad="U5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="N1"/>
<connect gate="B" pin="IO_11" pad="R6"/>
<connect gate="B" pin="IO_12" pad="R1"/>
<connect gate="B" pin="IO_13" pad="R7"/>
<connect gate="B" pin="IO_14" pad="P6"/>
<connect gate="B" pin="IO_15" pad="R8"/>
<connect gate="B" pin="IO_16" pad="R2"/>
<connect gate="B" pin="IO_17" pad="R9"/>
<connect gate="B" pin="IO_18" pad="M5"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="P1"/>
<connect gate="B" pin="IO_20" pad="N2"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="M6"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="N3"/>
<connect gate="B" pin="IO_25" pad="U1"/>
<connect gate="B" pin="IO_26" pad="N4"/>
<connect gate="B" pin="IO_27" pad="T5"/>
<connect gate="B" pin="IO_28" pad="T6"/>
<connect gate="B" pin="IO_29" pad="N6"/>
<connect gate="B" pin="IO_3" pad="P2"/>
<connect gate="B" pin="IO_30" pad="T7"/>
<connect gate="B" pin="IO_31" pad="T8"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U3"/>
<connect gate="B" pin="IO_34" pad="U4"/>
<connect gate="B" pin="IO_35" pad="U8"/>
<connect gate="B" pin="IO_36" pad="U9"/>
<connect gate="B" pin="IO_37" pad="V1"/>
<connect gate="B" pin="IO_38" pad="V2"/>
<connect gate="B" pin="IO_39" pad="V4"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_40" pad="V8"/>
<connect gate="B" pin="IO_41" pad="V9"/>
<connect gate="B" pin="IO_42" pad="W1"/>
<connect gate="B" pin="IO_43" pad="W2"/>
<connect gate="B" pin="IO_44" pad="W3"/>
<connect gate="B" pin="IO_45" pad="W4"/>
<connect gate="B" pin="IO_46" pad="W5"/>
<connect gate="B" pin="IO_47" pad="W7"/>
<connect gate="B" pin="IO_48" pad="W8"/>
<connect gate="B" pin="IO_49" pad="W9"/>
<connect gate="B" pin="IO_5" pad="P3"/>
<connect gate="B" pin="IO_50" pad="Y1"/>
<connect gate="B" pin="IO_51" pad="Y2"/>
<connect gate="B" pin="IO_52" pad="Y3"/>
<connect gate="B" pin="IO_53" pad="Y4"/>
<connect gate="B" pin="IO_54" pad="Y5"/>
<connect gate="B" pin="IO_55" pad="Y6"/>
<connect gate="B" pin="IO_56" pad="Y7"/>
<connect gate="B" pin="IO_57" pad="Y9"/>
<connect gate="B" pin="IO_58" pad="A10"/>
<connect gate="B" pin="IO_59" pad="A11"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_60" pad="A13"/>
<connect gate="B" pin="IO_61" pad="A14"/>
<connect gate="B" pin="IO_62" pad="A15"/>
<connect gate="B" pin="IO_63" pad="A16"/>
<connect gate="B" pin="IO_64" pad="A17"/>
<connect gate="B" pin="IO_65" pad="A18"/>
<connect gate="B" pin="IO_66" pad="A19"/>
<connect gate="B" pin="IO_7" pad="P5"/>
<connect gate="B" pin="IO_8" pad="P9"/>
<connect gate="B" pin="IO_9" pad="R5"/>
<connect gate="B" pin="NC" pad="P4"/>
<connect gate="B" pin="NC_2" pad="M7"/>
<connect gate="B" pin="NC_3" pad="M8"/>
<connect gate="B" pin="NC_4" pad="N8"/>
<connect gate="B" pin="NC_5" pad="R4"/>
<connect gate="B" pin="NC_6" pad="N5"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="L9"/>
<connect gate="B" pin="VCCINT_2" pad="M9"/>
<connect gate="B" pin="VCCINT_3" pad="N9"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="M3"/>
<connect gate="B" pin="VCCIO1_3" pad="T4"/>
<connect gate="B" pin="VCCIO1_4" pad="P7"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="W6"/>
<connect gate="B" pin="VCCIO8_2" pad="T9"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="G13"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="C15"/>
<connect gate="C" pin="GND_2" pad="D10"/>
<connect gate="C" pin="GND_3" pad="D13"/>
<connect gate="C" pin="GND_4" pad="D18"/>
<connect gate="C" pin="GND_5" pad="F19"/>
<connect gate="C" pin="GND_6" pad="AA2"/>
<connect gate="C" pin="GND_7" pad="AB1"/>
<connect gate="C" pin="GND_8" pad="G10"/>
<connect gate="C" pin="GND_9" pad="B21"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="AB5"/>
<connect gate="C" pin="IO_11" pad="AB6"/>
<connect gate="C" pin="IO_12" pad="AB7"/>
<connect gate="C" pin="IO_13" pad="C10"/>
<connect gate="C" pin="IO_14" pad="AB3"/>
<connect gate="C" pin="IO_15" pad="AB8"/>
<connect gate="C" pin="IO_16" pad="AB9"/>
<connect gate="C" pin="IO_17" pad="C13"/>
<connect gate="C" pin="IO_18" pad="B10"/>
<connect gate="C" pin="IO_19" pad="C14"/>
<connect gate="C" pin="IO_2" pad="AA3"/>
<connect gate="C" pin="IO_20" pad="B11"/>
<connect gate="C" pin="IO_21" pad="C16"/>
<connect gate="C" pin="IO_22" pad="B13"/>
<connect gate="C" pin="IO_23" pad="C17"/>
<connect gate="C" pin="IO_24" pad="B14"/>
<connect gate="C" pin="IO_25" pad="C18"/>
<connect gate="C" pin="IO_26" pad="B15"/>
<connect gate="C" pin="IO_27" pad="C19"/>
<connect gate="C" pin="IO_28" pad="B16"/>
<connect gate="C" pin="IO_29" pad="C20"/>
<connect gate="C" pin="IO_3" pad="AA4"/>
<connect gate="C" pin="IO_30" pad="B17"/>
<connect gate="C" pin="IO_31" pad="C21"/>
<connect gate="C" pin="IO_32" pad="B18"/>
<connect gate="C" pin="IO_33" pad="C22"/>
<connect gate="C" pin="IO_34" pad="B19"/>
<connect gate="C" pin="IO_35" pad="D14"/>
<connect gate="C" pin="IO_36" pad="B20"/>
<connect gate="C" pin="IO_37" pad="D11"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AA5"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="AA6"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AA7"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G11"/>
<connect gate="C" pin="IO_62" pad="G12"/>
<connect gate="C" pin="IO_63" pad="G15"/>
<connect gate="C" pin="IO_64" pad="G16"/>
<connect gate="C" pin="IO_65" pad="G17"/>
<connect gate="C" pin="IO_66" pad="G18"/>
<connect gate="C" pin="IO_67" pad="G20"/>
<connect gate="C" pin="IO_68" pad="G21"/>
<connect gate="C" pin="IO_69" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AA8"/>
<connect gate="C" pin="IO_70" pad="H10"/>
<connect gate="C" pin="IO_8" pad="AB4"/>
<connect gate="C" pin="IO_9" pad="AA9"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="G14"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="D17"/>
<connect gate="C" pin="VCCIO5" pad="G19"/>
<connect gate="C" pin="VCCIO5_2" pad="B22"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="N19"/>
<connect gate="D" pin="GND_10" pad="L13"/>
<connect gate="D" pin="GND_11" pad="K12"/>
<connect gate="D" pin="GND_12" pad="H20"/>
<connect gate="D" pin="GND_13" pad="M10"/>
<connect gate="D" pin="GND_14" pad="M11"/>
<connect gate="D" pin="GND_15" pad="M12"/>
<connect gate="D" pin="GND_16" pad="N10"/>
<connect gate="D" pin="GND_17" pad="M13"/>
<connect gate="D" pin="GND_18" pad="N11"/>
<connect gate="D" pin="GND_19" pad="N12"/>
<connect gate="D" pin="GND_2" pad="K19"/>
<connect gate="D" pin="GND_20" pad="N16"/>
<connect gate="D" pin="GND_21" pad="N13"/>
<connect gate="D" pin="GND_3" pad="K13"/>
<connect gate="D" pin="GND_4" pad="K16"/>
<connect gate="D" pin="GND_5" pad="L10"/>
<connect gate="D" pin="GND_6" pad="K10"/>
<connect gate="D" pin="GND_7" pad="L11"/>
<connect gate="D" pin="GND_8" pad="K11"/>
<connect gate="D" pin="GND_9" pad="L12"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J14"/>
<connect gate="D" pin="IO_11" pad="J15"/>
<connect gate="D" pin="IO_12" pad="L18"/>
<connect gate="D" pin="IO_13" pad="L19"/>
<connect gate="D" pin="IO_14" pad="J17"/>
<connect gate="D" pin="IO_15" pad="J18"/>
<connect gate="D" pin="IO_16" pad="K20"/>
<connect gate="D" pin="IO_17" pad="J19"/>
<connect gate="D" pin="IO_18" pad="K21"/>
<connect gate="D" pin="IO_19" pad="J20"/>
<connect gate="D" pin="IO_2" pad="H12"/>
<connect gate="D" pin="IO_20" pad="K22"/>
<connect gate="D" pin="IO_21" pad="J21"/>
<connect gate="D" pin="IO_22" pad="J22"/>
<connect gate="D" pin="IO_23" pad="M18"/>
<connect gate="D" pin="IO_24" pad="M19"/>
<connect gate="D" pin="IO_25" pad="N15"/>
<connect gate="D" pin="IO_26" pad="N21"/>
<connect gate="D" pin="IO_27" pad="N22"/>
<connect gate="D" pin="IO_28" pad="P15"/>
<connect gate="D" pin="IO_29" pad="P17"/>
<connect gate="D" pin="IO_3" pad="H13"/>
<connect gate="D" pin="IO_30" pad="P18"/>
<connect gate="D" pin="IO_31" pad="R10"/>
<connect gate="D" pin="IO_32" pad="R11"/>
<connect gate="D" pin="IO_33" pad="R12"/>
<connect gate="D" pin="IO_34" pad="R13"/>
<connect gate="D" pin="IO_35" pad="R14"/>
<connect gate="D" pin="IO_36" pad="R15"/>
<connect gate="D" pin="IO_37" pad="R16"/>
<connect gate="D" pin="IO_4" pad="H14"/>
<connect gate="D" pin="IO_5" pad="H15"/>
<connect gate="D" pin="IO_6" pad="H16"/>
<connect gate="D" pin="IO_7" pad="H17"/>
<connect gate="D" pin="IO_8" pad="H18"/>
<connect gate="D" pin="IO_9" pad="H19"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NC" pad="M16"/>
<connect gate="D" pin="NC_10" pad="P21"/>
<connect gate="D" pin="NC_11" pad="K18"/>
<connect gate="D" pin="NC_12" pad="P22"/>
<connect gate="D" pin="NC_13" pad="L16"/>
<connect gate="D" pin="NC_14" pad="L17"/>
<connect gate="D" pin="NC_15" pad="M15"/>
<connect gate="D" pin="NC_2" pad="H22"/>
<connect gate="D" pin="NC_3" pad="P14"/>
<connect gate="D" pin="NC_4" pad="K15"/>
<connect gate="D" pin="NC_5" pad="H21"/>
<connect gate="D" pin="NC_6" pad="P19"/>
<connect gate="D" pin="NC_7" pad="K17"/>
<connect gate="D" pin="NC_8" pad="P20"/>
<connect gate="D" pin="NC_9" pad="L15"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="L14"/>
<connect gate="D" pin="VCCINT_10" pad="K14"/>
<connect gate="D" pin="VCCINT_11" pad="N14"/>
<connect gate="D" pin="VCCINT_12" pad="P13"/>
<connect gate="D" pin="VCCINT_2" pad="P10"/>
<connect gate="D" pin="VCCINT_3" pad="J10"/>
<connect gate="D" pin="VCCINT_4" pad="P11"/>
<connect gate="D" pin="VCCINT_5" pad="J11"/>
<connect gate="D" pin="VCCINT_6" pad="M14"/>
<connect gate="D" pin="VCCINT_7" pad="J12"/>
<connect gate="D" pin="VCCINT_8" pad="P12"/>
<connect gate="D" pin="VCCINT_9" pad="J13"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="M20"/>
<connect gate="D" pin="VCCIO6_2" pad="P16"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AA21"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="W19"/>
<connect gate="E" pin="GND_2" pad="Y15"/>
<connect gate="E" pin="GND_3" pad="T10"/>
<connect gate="E" pin="GND_4" pad="T20"/>
<connect gate="E" pin="GND_5" pad="T13"/>
<connect gate="E" pin="GND_6" pad="AB22"/>
<connect gate="E" pin="GND_7" pad="V17"/>
<connect gate="E" pin="GND_8" pad="W13"/>
<connect gate="E" pin="GND_9" pad="W10"/>
<connect gate="E" pin="GND_PLL4" pad="V18"/>
<connect gate="E" pin="GND_PLL4_2" pad="T17"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="T16"/>
<connect gate="E" pin="IO_11" pad="U18"/>
<connect gate="E" pin="IO_12" pad="R22"/>
<connect gate="E" pin="IO_13" pad="T18"/>
<connect gate="E" pin="IO_14" pad="U19"/>
<connect gate="E" pin="IO_15" pad="U20"/>
<connect gate="E" pin="IO_16" pad="T11"/>
<connect gate="E" pin="IO_17" pad="T21"/>
<connect gate="E" pin="IO_18" pad="U21"/>
<connect gate="E" pin="IO_19" pad="T12"/>
<connect gate="E" pin="IO_2" pad="U13"/>
<connect gate="E" pin="IO_20" pad="T22"/>
<connect gate="E" pin="IO_21" pad="V19"/>
<connect gate="E" pin="IO_22" pad="U10"/>
<connect gate="E" pin="IO_23" pad="V20"/>
<connect gate="E" pin="IO_24" pad="U22"/>
<connect gate="E" pin="IO_25" pad="V21"/>
<connect gate="E" pin="IO_26" pad="V14"/>
<connect gate="E" pin="IO_27" pad="V22"/>
<connect gate="E" pin="IO_28" pad="V15"/>
<connect gate="E" pin="IO_29" pad="W11"/>
<connect gate="E" pin="IO_3" pad="U14"/>
<connect gate="E" pin="IO_30" pad="V11"/>
<connect gate="E" pin="IO_31" pad="W14"/>
<connect gate="E" pin="IO_32" pad="W15"/>
<connect gate="E" pin="IO_33" pad="W16"/>
<connect gate="E" pin="IO_34" pad="W20"/>
<connect gate="E" pin="IO_35" pad="W21"/>
<connect gate="E" pin="IO_36" pad="W22"/>
<connect gate="E" pin="IO_37" pad="Y10"/>
<connect gate="E" pin="IO_38" pad="Y13"/>
<connect gate="E" pin="IO_39" pad="Y14"/>
<connect gate="E" pin="IO_4" pad="R18"/>
<connect gate="E" pin="IO_40" pad="Y16"/>
<connect gate="E" pin="IO_41" pad="Y17"/>
<connect gate="E" pin="IO_42" pad="Y18"/>
<connect gate="E" pin="IO_43" pad="Y19"/>
<connect gate="E" pin="IO_44" pad="Y20"/>
<connect gate="E" pin="IO_45" pad="Y21"/>
<connect gate="E" pin="IO_46" pad="Y22"/>
<connect gate="E" pin="IO_47" pad="AA10"/>
<connect gate="E" pin="IO_48" pad="AA11"/>
<connect gate="E" pin="IO_49" pad="AA12"/>
<connect gate="E" pin="IO_5" pad="U15"/>
<connect gate="E" pin="IO_50" pad="AA13"/>
<connect gate="E" pin="IO_51" pad="AA14"/>
<connect gate="E" pin="IO_52" pad="AA15"/>
<connect gate="E" pin="IO_53" pad="AA16"/>
<connect gate="E" pin="IO_54" pad="AA17"/>
<connect gate="E" pin="IO_55" pad="AA18"/>
<connect gate="E" pin="IO_56" pad="AA19"/>
<connect gate="E" pin="IO_57" pad="AA20"/>
<connect gate="E" pin="IO_58" pad="AB10"/>
<connect gate="E" pin="IO_59" pad="AB11"/>
<connect gate="E" pin="IO_6" pad="R19"/>
<connect gate="E" pin="IO_60" pad="AB12"/>
<connect gate="E" pin="IO_61" pad="AB13"/>
<connect gate="E" pin="IO_62" pad="AB14"/>
<connect gate="E" pin="IO_63" pad="AB15"/>
<connect gate="E" pin="IO_64" pad="AB16"/>
<connect gate="E" pin="IO_65" pad="AB17"/>
<connect gate="E" pin="IO_66" pad="AB18"/>
<connect gate="E" pin="IO_67" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="R20"/>
<connect gate="E" pin="IO_8" pad="R21"/>
<connect gate="E" pin="IO_9" pad="T15"/>
<connect gate="E" pin="NC" pad="W18"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCIO6" pad="T19"/>
<connect gate="E" pin="VCCIO6_2" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="Y12"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="AB21"/>
<connect gate="E" pin="VCCIO7_4" pad="V13"/>
<connect gate="E" pin="VCCIO7_5" pad="W17"/>
<connect gate="E" pin="VCCIO8" pad="Y11"/>
<connect gate="E" pin="VCCIO8_2" pad="V10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C20F484I8N"/>
<attribute name="OC_FARNELL" value="1663196"/>
<attribute name="OC_NEWARK" value="52R0514"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C35F484C8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C35F484C8N_A"/>
<gate name="B" symbol="EP2C35F484C8N_B"/>
<gate name="C" symbol="EP2C35F484C8N_C"/>
<gate name="D" symbol="EP2C35F484C8N_D"/>
<gate name="E" symbol="EP2C35F484C8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K7"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="J9"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="C5"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="GND_6" pad="G4"/>
<connect gate="A" pin="GND_7" pad="K3"/>
<connect gate="A" pin="GND_8" pad="H9"/>
<connect gate="A" pin="GND_9" pad="J8"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="C9"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="D1"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="A5"/>
<connect gate="A" pin="IO_16" pad="D3"/>
<connect gate="A" pin="IO_17" pad="B9"/>
<connect gate="A" pin="IO_18" pad="D4"/>
<connect gate="A" pin="IO_19" pad="A6"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="D5"/>
<connect gate="A" pin="IO_21" pad="C1"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="A7"/>
<connect gate="A" pin="IO_24" pad="D7"/>
<connect gate="A" pin="IO_25" pad="C2"/>
<connect gate="A" pin="IO_26" pad="D8"/>
<connect gate="A" pin="IO_27" pad="A8"/>
<connect gate="A" pin="IO_28" pad="D9"/>
<connect gate="A" pin="IO_29" pad="C3"/>
<connect gate="A" pin="IO_3" pad="C4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E7"/>
<connect gate="A" pin="IO_34" pad="E3"/>
<connect gate="A" pin="IO_35" pad="E8"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="B4"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="G7"/>
<connect gate="A" pin="IO_5" pad="B5"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="J1"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_60" pad="J4"/>
<connect gate="A" pin="IO_61" pad="J5"/>
<connect gate="A" pin="IO_62" pad="L7"/>
<connect gate="A" pin="IO_7" pad="C7"/>
<connect gate="A" pin="IO_8" pad="A3"/>
<connect gate="A" pin="IO_9" pad="B7"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="G8"/>
<connect gate="A" pin="VCCINT_3" pad="K8"/>
<connect gate="A" pin="VCCINT_4" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="J7"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="L3"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="R3"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V6"/>
<connect gate="B" pin="GND_11" pad="V3"/>
<connect gate="B" pin="GND_2" pad="M4"/>
<connect gate="B" pin="GND_3" pad="Y8"/>
<connect gate="B" pin="GND_4" pad="P8"/>
<connect gate="B" pin="GND_5" pad="R9"/>
<connect gate="B" pin="GND_6" pad="N7"/>
<connect gate="B" pin="GND_7" pad="A22"/>
<connect gate="B" pin="GND_8" pad="P9"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GND_PLL1" pad="U5"/>
<connect gate="B" pin="GND_PLL1_2" pad="V5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="R5"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="R6"/>
<connect gate="B" pin="IO_13" pad="N4"/>
<connect gate="B" pin="IO_14" pad="R7"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="R8"/>
<connect gate="B" pin="IO_17" pad="U1"/>
<connect gate="B" pin="IO_18" pad="N6"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="M5"/>
<connect gate="B" pin="IO_20" pad="P1"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="P2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="P3"/>
<connect gate="B" pin="IO_25" pad="P4"/>
<connect gate="B" pin="IO_26" pad="P5"/>
<connect gate="B" pin="IO_27" pad="P6"/>
<connect gate="B" pin="IO_28" pad="T5"/>
<connect gate="B" pin="IO_29" pad="T6"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="T7"/>
<connect gate="B" pin="IO_31" pad="R1"/>
<connect gate="B" pin="IO_32" pad="T8"/>
<connect gate="B" pin="IO_33" pad="R2"/>
<connect gate="B" pin="IO_34" pad="U2"/>
<connect gate="B" pin="IO_35" pad="U3"/>
<connect gate="B" pin="IO_36" pad="U4"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V8"/>
<connect gate="B" pin="IO_43" pad="V9"/>
<connect gate="B" pin="IO_44" pad="W1"/>
<connect gate="B" pin="IO_45" pad="W2"/>
<connect gate="B" pin="IO_46" pad="W3"/>
<connect gate="B" pin="IO_47" pad="W4"/>
<connect gate="B" pin="IO_48" pad="W5"/>
<connect gate="B" pin="IO_49" pad="W7"/>
<connect gate="B" pin="IO_5" pad="M7"/>
<connect gate="B" pin="IO_50" pad="W8"/>
<connect gate="B" pin="IO_51" pad="W9"/>
<connect gate="B" pin="IO_52" pad="Y1"/>
<connect gate="B" pin="IO_53" pad="Y2"/>
<connect gate="B" pin="IO_54" pad="Y3"/>
<connect gate="B" pin="IO_55" pad="Y4"/>
<connect gate="B" pin="IO_56" pad="Y5"/>
<connect gate="B" pin="IO_57" pad="Y6"/>
<connect gate="B" pin="IO_58" pad="Y7"/>
<connect gate="B" pin="IO_59" pad="Y9"/>
<connect gate="B" pin="IO_6" pad="M8"/>
<connect gate="B" pin="IO_60" pad="A10"/>
<connect gate="B" pin="IO_61" pad="A11"/>
<connect gate="B" pin="IO_62" pad="A13"/>
<connect gate="B" pin="IO_63" pad="A14"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_68" pad="A19"/>
<connect gate="B" pin="IO_7" pad="N1"/>
<connect gate="B" pin="IO_8" pad="R4"/>
<connect gate="B" pin="IO_9" pad="N2"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="N9"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="M9"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="P7"/>
<connect gate="B" pin="VCCIO1_3" pad="T4"/>
<connect gate="B" pin="VCCIO1_4" pad="M3"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="T9"/>
<connect gate="B" pin="VCCIO8_2" pad="W6"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="H10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="C15"/>
<connect gate="C" pin="GND_11" pad="G15"/>
<connect gate="C" pin="GND_12" pad="G13"/>
<connect gate="C" pin="GND_2" pad="AB1"/>
<connect gate="C" pin="GND_3" pad="D10"/>
<connect gate="C" pin="GND_4" pad="D18"/>
<connect gate="C" pin="GND_5" pad="D13"/>
<connect gate="C" pin="GND_6" pad="F19"/>
<connect gate="C" pin="GND_7" pad="AA2"/>
<connect gate="C" pin="GND_8" pad="G10"/>
<connect gate="C" pin="GND_9" pad="B21"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="C13"/>
<connect gate="C" pin="IO_11" pad="AA3"/>
<connect gate="C" pin="IO_12" pad="AB9"/>
<connect gate="C" pin="IO_13" pad="AA4"/>
<connect gate="C" pin="IO_14" pad="B10"/>
<connect gate="C" pin="IO_15" pad="AA5"/>
<connect gate="C" pin="IO_16" pad="B11"/>
<connect gate="C" pin="IO_17" pad="AA6"/>
<connect gate="C" pin="IO_18" pad="AA7"/>
<connect gate="C" pin="IO_19" pad="B13"/>
<connect gate="C" pin="IO_2" pad="AB3"/>
<connect gate="C" pin="IO_20" pad="AA8"/>
<connect gate="C" pin="IO_21" pad="B14"/>
<connect gate="C" pin="IO_22" pad="C14"/>
<connect gate="C" pin="IO_23" pad="AA9"/>
<connect gate="C" pin="IO_24" pad="B15"/>
<connect gate="C" pin="IO_25" pad="C16"/>
<connect gate="C" pin="IO_26" pad="B16"/>
<connect gate="C" pin="IO_27" pad="C17"/>
<connect gate="C" pin="IO_28" pad="B17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="D14"/>
<connect gate="C" pin="IO_30" pad="B18"/>
<connect gate="C" pin="IO_31" pad="C19"/>
<connect gate="C" pin="IO_32" pad="B19"/>
<connect gate="C" pin="IO_33" pad="C20"/>
<connect gate="C" pin="IO_34" pad="B20"/>
<connect gate="C" pin="IO_35" pad="C10"/>
<connect gate="C" pin="IO_36" pad="C21"/>
<connect gate="C" pin="IO_37" pad="C22"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AB4"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="D11"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AB5"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G11"/>
<connect gate="C" pin="IO_62" pad="G16"/>
<connect gate="C" pin="IO_63" pad="G17"/>
<connect gate="C" pin="IO_64" pad="G18"/>
<connect gate="C" pin="IO_65" pad="G20"/>
<connect gate="C" pin="IO_66" pad="G21"/>
<connect gate="C" pin="IO_67" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AB6"/>
<connect gate="C" pin="IO_8" pad="AB7"/>
<connect gate="C" pin="IO_9" pad="AB8"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="G14"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="D17"/>
<connect gate="C" pin="VCCIO5" pad="B22"/>
<connect gate="C" pin="VCCIO5_2" pad="G19"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="N16"/>
<connect gate="D" pin="GND_10" pad="M10"/>
<connect gate="D" pin="GND_11" pad="N11"/>
<connect gate="D" pin="GND_12" pad="L13"/>
<connect gate="D" pin="GND_13" pad="N12"/>
<connect gate="D" pin="GND_14" pad="M11"/>
<connect gate="D" pin="GND_15" pad="N13"/>
<connect gate="D" pin="GND_16" pad="K19"/>
<connect gate="D" pin="GND_17" pad="M12"/>
<connect gate="D" pin="GND_18" pad="K13"/>
<connect gate="D" pin="GND_19" pad="M13"/>
<connect gate="D" pin="GND_2" pad="K10"/>
<connect gate="D" pin="GND_20" pad="N10"/>
<connect gate="D" pin="GND_21" pad="H20"/>
<connect gate="D" pin="GND_22" pad="K16"/>
<connect gate="D" pin="GND_23" pad="N19"/>
<connect gate="D" pin="GND_24" pad="R13"/>
<connect gate="D" pin="GND_3" pad="L10"/>
<connect gate="D" pin="GND_4" pad="K11"/>
<connect gate="D" pin="GND_5" pad="L11"/>
<connect gate="D" pin="GND_6" pad="K12"/>
<connect gate="D" pin="GND_7" pad="L12"/>
<connect gate="D" pin="GND_8" pad="K15"/>
<connect gate="D" pin="GND_9" pad="L15"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J18"/>
<connect gate="D" pin="IO_11" pad="H19"/>
<connect gate="D" pin="IO_12" pad="J19"/>
<connect gate="D" pin="IO_13" pad="K17"/>
<connect gate="D" pin="IO_14" pad="J20"/>
<connect gate="D" pin="IO_15" pad="K18"/>
<connect gate="D" pin="IO_16" pad="L17"/>
<connect gate="D" pin="IO_17" pad="H21"/>
<connect gate="D" pin="IO_18" pad="L18"/>
<connect gate="D" pin="IO_19" pad="J21"/>
<connect gate="D" pin="IO_2" pad="H14"/>
<connect gate="D" pin="IO_20" pad="L19"/>
<connect gate="D" pin="IO_21" pad="K20"/>
<connect gate="D" pin="IO_22" pad="H22"/>
<connect gate="D" pin="IO_23" pad="K21"/>
<connect gate="D" pin="IO_24" pad="J22"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="M15"/>
<connect gate="D" pin="IO_27" pad="M16"/>
<connect gate="D" pin="IO_28" pad="M18"/>
<connect gate="D" pin="IO_29" pad="M19"/>
<connect gate="D" pin="IO_3" pad="H15"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N21"/>
<connect gate="D" pin="IO_32" pad="N22"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P17"/>
<connect gate="D" pin="IO_35" pad="P18"/>
<connect gate="D" pin="IO_36" pad="P19"/>
<connect gate="D" pin="IO_37" pad="P20"/>
<connect gate="D" pin="IO_38" pad="P21"/>
<connect gate="D" pin="IO_39" pad="P22"/>
<connect gate="D" pin="IO_4" pad="J14"/>
<connect gate="D" pin="IO_40" pad="R11"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H16"/>
<connect gate="D" pin="IO_6" pad="J17"/>
<connect gate="D" pin="IO_7" pad="H17"/>
<connect gate="D" pin="IO_8" pad="J15"/>
<connect gate="D" pin="IO_9" pad="H18"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="L14"/>
<connect gate="D" pin="VCCINT_10" pad="J13"/>
<connect gate="D" pin="VCCINT_11" pad="L16"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="R10"/>
<connect gate="D" pin="VCCINT_14" pad="H12"/>
<connect gate="D" pin="VCCINT_15" pad="N14"/>
<connect gate="D" pin="VCCINT_16" pad="R12"/>
<connect gate="D" pin="VCCINT_17" pad="H13"/>
<connect gate="D" pin="VCCINT_18" pad="K14"/>
<connect gate="D" pin="VCCINT_2" pad="P10"/>
<connect gate="D" pin="VCCINT_3" pad="P11"/>
<connect gate="D" pin="VCCINT_4" pad="J10"/>
<connect gate="D" pin="VCCINT_5" pad="P12"/>
<connect gate="D" pin="VCCINT_6" pad="J11"/>
<connect gate="D" pin="VCCINT_7" pad="P13"/>
<connect gate="D" pin="VCCINT_8" pad="J12"/>
<connect gate="D" pin="VCCINT_9" pad="P14"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="P16"/>
<connect gate="D" pin="VCCIO6_2" pad="M20"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="T10"/>
<connect gate="E" pin="GND_2" pad="T20"/>
<connect gate="E" pin="GND_3" pad="W10"/>
<connect gate="E" pin="GND_4" pad="Y15"/>
<connect gate="E" pin="GND_5" pad="AA21"/>
<connect gate="E" pin="GND_6" pad="T13"/>
<connect gate="E" pin="GND_7" pad="V17"/>
<connect gate="E" pin="GND_8" pad="W19"/>
<connect gate="E" pin="GND_9" pad="W13"/>
<connect gate="E" pin="GND_PLL4" pad="T17"/>
<connect gate="E" pin="GND_PLL4_2" pad="V18"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="T21"/>
<connect gate="E" pin="IO_11" pad="T22"/>
<connect gate="E" pin="IO_12" pad="U10"/>
<connect gate="E" pin="IO_13" pad="U18"/>
<connect gate="E" pin="IO_14" pad="V14"/>
<connect gate="E" pin="IO_15" pad="U19"/>
<connect gate="E" pin="IO_16" pad="V15"/>
<connect gate="E" pin="IO_17" pad="U20"/>
<connect gate="E" pin="IO_18" pad="U13"/>
<connect gate="E" pin="IO_19" pad="U21"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="V20"/>
<connect gate="E" pin="IO_21" pad="U14"/>
<connect gate="E" pin="IO_22" pad="V21"/>
<connect gate="E" pin="IO_23" pad="U22"/>
<connect gate="E" pin="IO_24" pad="V19"/>
<connect gate="E" pin="IO_25" pad="V22"/>
<connect gate="E" pin="IO_26" pad="U15"/>
<connect gate="E" pin="IO_27" pad="V11"/>
<connect gate="E" pin="IO_28" pad="W11"/>
<connect gate="E" pin="IO_29" pad="W14"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="W15"/>
<connect gate="E" pin="IO_31" pad="W16"/>
<connect gate="E" pin="IO_32" pad="W18"/>
<connect gate="E" pin="IO_33" pad="W20"/>
<connect gate="E" pin="IO_34" pad="W21"/>
<connect gate="E" pin="IO_35" pad="W22"/>
<connect gate="E" pin="IO_36" pad="Y10"/>
<connect gate="E" pin="IO_37" pad="Y13"/>
<connect gate="E" pin="IO_38" pad="Y14"/>
<connect gate="E" pin="IO_39" pad="Y16"/>
<connect gate="E" pin="IO_4" pad="T16"/>
<connect gate="E" pin="IO_40" pad="Y17"/>
<connect gate="E" pin="IO_41" pad="Y18"/>
<connect gate="E" pin="IO_42" pad="Y19"/>
<connect gate="E" pin="IO_43" pad="Y20"/>
<connect gate="E" pin="IO_44" pad="Y21"/>
<connect gate="E" pin="IO_45" pad="Y22"/>
<connect gate="E" pin="IO_46" pad="AA10"/>
<connect gate="E" pin="IO_47" pad="AA11"/>
<connect gate="E" pin="IO_48" pad="AA12"/>
<connect gate="E" pin="IO_49" pad="AA13"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="AA14"/>
<connect gate="E" pin="IO_51" pad="AA15"/>
<connect gate="E" pin="IO_52" pad="AA16"/>
<connect gate="E" pin="IO_53" pad="AA17"/>
<connect gate="E" pin="IO_54" pad="AA18"/>
<connect gate="E" pin="IO_55" pad="AA19"/>
<connect gate="E" pin="IO_56" pad="AA20"/>
<connect gate="E" pin="IO_57" pad="AB10"/>
<connect gate="E" pin="IO_58" pad="AB11"/>
<connect gate="E" pin="IO_59" pad="AB12"/>
<connect gate="E" pin="IO_6" pad="R20"/>
<connect gate="E" pin="IO_60" pad="AB13"/>
<connect gate="E" pin="IO_61" pad="AB14"/>
<connect gate="E" pin="IO_62" pad="AB15"/>
<connect gate="E" pin="IO_63" pad="AB16"/>
<connect gate="E" pin="IO_64" pad="AB17"/>
<connect gate="E" pin="IO_65" pad="AB18"/>
<connect gate="E" pin="IO_66" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="T18"/>
<connect gate="E" pin="IO_8" pad="R21"/>
<connect gate="E" pin="IO_9" pad="T11"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="AA22"/>
<connect gate="E" pin="VCCIO6_2" pad="T19"/>
<connect gate="E" pin="VCCIO7" pad="AB21"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="W17"/>
<connect gate="E" pin="VCCIO7_4" pad="Y12"/>
<connect gate="E" pin="VCCIO7_5" pad="V13"/>
<connect gate="E" pin="VCCIO8" pad="V10"/>
<connect gate="E" pin="VCCIO8_2" pad="Y11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C35F484C8N"/>
<attribute name="OC_FARNELL" value="1635084"/>
<attribute name="OC_NEWARK" value="51R0563"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C35F484I8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C35F484I8N_A"/>
<gate name="B" symbol="EP2C35F484I8N_B"/>
<gate name="C" symbol="EP2C35F484I8N_C"/>
<gate name="D" symbol="EP2C35F484I8N_D"/>
<gate name="E" symbol="EP2C35F484I8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K7"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="J9"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="C5"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="GND_6" pad="G4"/>
<connect gate="A" pin="GND_7" pad="K3"/>
<connect gate="A" pin="GND_8" pad="H9"/>
<connect gate="A" pin="GND_9" pad="J8"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="C9"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="D1"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="A5"/>
<connect gate="A" pin="IO_16" pad="D3"/>
<connect gate="A" pin="IO_17" pad="B9"/>
<connect gate="A" pin="IO_18" pad="D4"/>
<connect gate="A" pin="IO_19" pad="A6"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="D5"/>
<connect gate="A" pin="IO_21" pad="C1"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="A7"/>
<connect gate="A" pin="IO_24" pad="D7"/>
<connect gate="A" pin="IO_25" pad="C2"/>
<connect gate="A" pin="IO_26" pad="D8"/>
<connect gate="A" pin="IO_27" pad="A8"/>
<connect gate="A" pin="IO_28" pad="D9"/>
<connect gate="A" pin="IO_29" pad="C3"/>
<connect gate="A" pin="IO_3" pad="C4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E7"/>
<connect gate="A" pin="IO_34" pad="E3"/>
<connect gate="A" pin="IO_35" pad="E8"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="B4"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="G7"/>
<connect gate="A" pin="IO_5" pad="B5"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="J1"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_60" pad="J4"/>
<connect gate="A" pin="IO_61" pad="J5"/>
<connect gate="A" pin="IO_62" pad="L7"/>
<connect gate="A" pin="IO_7" pad="C7"/>
<connect gate="A" pin="IO_8" pad="A3"/>
<connect gate="A" pin="IO_9" pad="B7"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="G8"/>
<connect gate="A" pin="VCCINT_3" pad="K8"/>
<connect gate="A" pin="VCCINT_4" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="J7"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="L3"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="R3"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V6"/>
<connect gate="B" pin="GND_11" pad="V3"/>
<connect gate="B" pin="GND_2" pad="M4"/>
<connect gate="B" pin="GND_3" pad="Y8"/>
<connect gate="B" pin="GND_4" pad="P8"/>
<connect gate="B" pin="GND_5" pad="R9"/>
<connect gate="B" pin="GND_6" pad="N7"/>
<connect gate="B" pin="GND_7" pad="A22"/>
<connect gate="B" pin="GND_8" pad="P9"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GND_PLL1" pad="U5"/>
<connect gate="B" pin="GND_PLL1_2" pad="V5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="R5"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="R6"/>
<connect gate="B" pin="IO_13" pad="N4"/>
<connect gate="B" pin="IO_14" pad="R7"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="R8"/>
<connect gate="B" pin="IO_17" pad="U1"/>
<connect gate="B" pin="IO_18" pad="N6"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="M5"/>
<connect gate="B" pin="IO_20" pad="P1"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="P2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="P3"/>
<connect gate="B" pin="IO_25" pad="P4"/>
<connect gate="B" pin="IO_26" pad="P5"/>
<connect gate="B" pin="IO_27" pad="P6"/>
<connect gate="B" pin="IO_28" pad="T5"/>
<connect gate="B" pin="IO_29" pad="T6"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="T7"/>
<connect gate="B" pin="IO_31" pad="R1"/>
<connect gate="B" pin="IO_32" pad="T8"/>
<connect gate="B" pin="IO_33" pad="R2"/>
<connect gate="B" pin="IO_34" pad="U2"/>
<connect gate="B" pin="IO_35" pad="U3"/>
<connect gate="B" pin="IO_36" pad="U4"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V8"/>
<connect gate="B" pin="IO_43" pad="V9"/>
<connect gate="B" pin="IO_44" pad="W1"/>
<connect gate="B" pin="IO_45" pad="W2"/>
<connect gate="B" pin="IO_46" pad="W3"/>
<connect gate="B" pin="IO_47" pad="W4"/>
<connect gate="B" pin="IO_48" pad="W5"/>
<connect gate="B" pin="IO_49" pad="W7"/>
<connect gate="B" pin="IO_5" pad="M7"/>
<connect gate="B" pin="IO_50" pad="W8"/>
<connect gate="B" pin="IO_51" pad="W9"/>
<connect gate="B" pin="IO_52" pad="Y1"/>
<connect gate="B" pin="IO_53" pad="Y2"/>
<connect gate="B" pin="IO_54" pad="Y3"/>
<connect gate="B" pin="IO_55" pad="Y4"/>
<connect gate="B" pin="IO_56" pad="Y5"/>
<connect gate="B" pin="IO_57" pad="Y6"/>
<connect gate="B" pin="IO_58" pad="Y7"/>
<connect gate="B" pin="IO_59" pad="Y9"/>
<connect gate="B" pin="IO_6" pad="M8"/>
<connect gate="B" pin="IO_60" pad="A10"/>
<connect gate="B" pin="IO_61" pad="A11"/>
<connect gate="B" pin="IO_62" pad="A13"/>
<connect gate="B" pin="IO_63" pad="A14"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_68" pad="A19"/>
<connect gate="B" pin="IO_7" pad="N1"/>
<connect gate="B" pin="IO_8" pad="R4"/>
<connect gate="B" pin="IO_9" pad="N2"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="N9"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="M9"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="P7"/>
<connect gate="B" pin="VCCIO1_3" pad="T4"/>
<connect gate="B" pin="VCCIO1_4" pad="M3"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="T9"/>
<connect gate="B" pin="VCCIO8_2" pad="W6"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="H10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="C15"/>
<connect gate="C" pin="GND_11" pad="G15"/>
<connect gate="C" pin="GND_12" pad="G13"/>
<connect gate="C" pin="GND_2" pad="AB1"/>
<connect gate="C" pin="GND_3" pad="D10"/>
<connect gate="C" pin="GND_4" pad="D18"/>
<connect gate="C" pin="GND_5" pad="D13"/>
<connect gate="C" pin="GND_6" pad="F19"/>
<connect gate="C" pin="GND_7" pad="AA2"/>
<connect gate="C" pin="GND_8" pad="G10"/>
<connect gate="C" pin="GND_9" pad="B21"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="C13"/>
<connect gate="C" pin="IO_11" pad="AA3"/>
<connect gate="C" pin="IO_12" pad="AB9"/>
<connect gate="C" pin="IO_13" pad="AA4"/>
<connect gate="C" pin="IO_14" pad="B10"/>
<connect gate="C" pin="IO_15" pad="AA5"/>
<connect gate="C" pin="IO_16" pad="B11"/>
<connect gate="C" pin="IO_17" pad="AA6"/>
<connect gate="C" pin="IO_18" pad="AA7"/>
<connect gate="C" pin="IO_19" pad="B13"/>
<connect gate="C" pin="IO_2" pad="AB3"/>
<connect gate="C" pin="IO_20" pad="AA8"/>
<connect gate="C" pin="IO_21" pad="B14"/>
<connect gate="C" pin="IO_22" pad="C14"/>
<connect gate="C" pin="IO_23" pad="AA9"/>
<connect gate="C" pin="IO_24" pad="B15"/>
<connect gate="C" pin="IO_25" pad="C16"/>
<connect gate="C" pin="IO_26" pad="B16"/>
<connect gate="C" pin="IO_27" pad="C17"/>
<connect gate="C" pin="IO_28" pad="B17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="D14"/>
<connect gate="C" pin="IO_30" pad="B18"/>
<connect gate="C" pin="IO_31" pad="C19"/>
<connect gate="C" pin="IO_32" pad="B19"/>
<connect gate="C" pin="IO_33" pad="C20"/>
<connect gate="C" pin="IO_34" pad="B20"/>
<connect gate="C" pin="IO_35" pad="C10"/>
<connect gate="C" pin="IO_36" pad="C21"/>
<connect gate="C" pin="IO_37" pad="C22"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AB4"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="D11"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AB5"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G11"/>
<connect gate="C" pin="IO_62" pad="G16"/>
<connect gate="C" pin="IO_63" pad="G17"/>
<connect gate="C" pin="IO_64" pad="G18"/>
<connect gate="C" pin="IO_65" pad="G20"/>
<connect gate="C" pin="IO_66" pad="G21"/>
<connect gate="C" pin="IO_67" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AB6"/>
<connect gate="C" pin="IO_8" pad="AB7"/>
<connect gate="C" pin="IO_9" pad="AB8"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="G14"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="D17"/>
<connect gate="C" pin="VCCIO5" pad="B22"/>
<connect gate="C" pin="VCCIO5_2" pad="G19"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="N16"/>
<connect gate="D" pin="GND_10" pad="M10"/>
<connect gate="D" pin="GND_11" pad="N11"/>
<connect gate="D" pin="GND_12" pad="L13"/>
<connect gate="D" pin="GND_13" pad="N12"/>
<connect gate="D" pin="GND_14" pad="M11"/>
<connect gate="D" pin="GND_15" pad="N13"/>
<connect gate="D" pin="GND_16" pad="K19"/>
<connect gate="D" pin="GND_17" pad="M12"/>
<connect gate="D" pin="GND_18" pad="K13"/>
<connect gate="D" pin="GND_19" pad="M13"/>
<connect gate="D" pin="GND_2" pad="K10"/>
<connect gate="D" pin="GND_20" pad="N10"/>
<connect gate="D" pin="GND_21" pad="H20"/>
<connect gate="D" pin="GND_22" pad="K16"/>
<connect gate="D" pin="GND_23" pad="N19"/>
<connect gate="D" pin="GND_24" pad="R13"/>
<connect gate="D" pin="GND_3" pad="L10"/>
<connect gate="D" pin="GND_4" pad="K11"/>
<connect gate="D" pin="GND_5" pad="L11"/>
<connect gate="D" pin="GND_6" pad="K12"/>
<connect gate="D" pin="GND_7" pad="L12"/>
<connect gate="D" pin="GND_8" pad="K15"/>
<connect gate="D" pin="GND_9" pad="L15"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J18"/>
<connect gate="D" pin="IO_11" pad="H19"/>
<connect gate="D" pin="IO_12" pad="J19"/>
<connect gate="D" pin="IO_13" pad="K17"/>
<connect gate="D" pin="IO_14" pad="J20"/>
<connect gate="D" pin="IO_15" pad="K18"/>
<connect gate="D" pin="IO_16" pad="L17"/>
<connect gate="D" pin="IO_17" pad="H21"/>
<connect gate="D" pin="IO_18" pad="L18"/>
<connect gate="D" pin="IO_19" pad="J21"/>
<connect gate="D" pin="IO_2" pad="H14"/>
<connect gate="D" pin="IO_20" pad="L19"/>
<connect gate="D" pin="IO_21" pad="K20"/>
<connect gate="D" pin="IO_22" pad="H22"/>
<connect gate="D" pin="IO_23" pad="K21"/>
<connect gate="D" pin="IO_24" pad="J22"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="M15"/>
<connect gate="D" pin="IO_27" pad="M16"/>
<connect gate="D" pin="IO_28" pad="M18"/>
<connect gate="D" pin="IO_29" pad="M19"/>
<connect gate="D" pin="IO_3" pad="H15"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N21"/>
<connect gate="D" pin="IO_32" pad="N22"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P17"/>
<connect gate="D" pin="IO_35" pad="P18"/>
<connect gate="D" pin="IO_36" pad="P19"/>
<connect gate="D" pin="IO_37" pad="P20"/>
<connect gate="D" pin="IO_38" pad="P21"/>
<connect gate="D" pin="IO_39" pad="P22"/>
<connect gate="D" pin="IO_4" pad="J14"/>
<connect gate="D" pin="IO_40" pad="R11"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H16"/>
<connect gate="D" pin="IO_6" pad="J17"/>
<connect gate="D" pin="IO_7" pad="H17"/>
<connect gate="D" pin="IO_8" pad="J15"/>
<connect gate="D" pin="IO_9" pad="H18"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="L14"/>
<connect gate="D" pin="VCCINT_10" pad="J13"/>
<connect gate="D" pin="VCCINT_11" pad="L16"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="R10"/>
<connect gate="D" pin="VCCINT_14" pad="H12"/>
<connect gate="D" pin="VCCINT_15" pad="N14"/>
<connect gate="D" pin="VCCINT_16" pad="R12"/>
<connect gate="D" pin="VCCINT_17" pad="H13"/>
<connect gate="D" pin="VCCINT_18" pad="K14"/>
<connect gate="D" pin="VCCINT_2" pad="P10"/>
<connect gate="D" pin="VCCINT_3" pad="P11"/>
<connect gate="D" pin="VCCINT_4" pad="J10"/>
<connect gate="D" pin="VCCINT_5" pad="P12"/>
<connect gate="D" pin="VCCINT_6" pad="J11"/>
<connect gate="D" pin="VCCINT_7" pad="P13"/>
<connect gate="D" pin="VCCINT_8" pad="J12"/>
<connect gate="D" pin="VCCINT_9" pad="P14"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="P16"/>
<connect gate="D" pin="VCCIO6_2" pad="M20"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="T10"/>
<connect gate="E" pin="GND_2" pad="T20"/>
<connect gate="E" pin="GND_3" pad="W10"/>
<connect gate="E" pin="GND_4" pad="Y15"/>
<connect gate="E" pin="GND_5" pad="AA21"/>
<connect gate="E" pin="GND_6" pad="T13"/>
<connect gate="E" pin="GND_7" pad="V17"/>
<connect gate="E" pin="GND_8" pad="W19"/>
<connect gate="E" pin="GND_9" pad="W13"/>
<connect gate="E" pin="GND_PLL4" pad="T17"/>
<connect gate="E" pin="GND_PLL4_2" pad="V18"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="T21"/>
<connect gate="E" pin="IO_11" pad="T22"/>
<connect gate="E" pin="IO_12" pad="U10"/>
<connect gate="E" pin="IO_13" pad="U18"/>
<connect gate="E" pin="IO_14" pad="V14"/>
<connect gate="E" pin="IO_15" pad="U19"/>
<connect gate="E" pin="IO_16" pad="V15"/>
<connect gate="E" pin="IO_17" pad="U20"/>
<connect gate="E" pin="IO_18" pad="U13"/>
<connect gate="E" pin="IO_19" pad="U21"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="V20"/>
<connect gate="E" pin="IO_21" pad="U14"/>
<connect gate="E" pin="IO_22" pad="V21"/>
<connect gate="E" pin="IO_23" pad="U22"/>
<connect gate="E" pin="IO_24" pad="V19"/>
<connect gate="E" pin="IO_25" pad="V22"/>
<connect gate="E" pin="IO_26" pad="U15"/>
<connect gate="E" pin="IO_27" pad="V11"/>
<connect gate="E" pin="IO_28" pad="W11"/>
<connect gate="E" pin="IO_29" pad="W14"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="W15"/>
<connect gate="E" pin="IO_31" pad="W16"/>
<connect gate="E" pin="IO_32" pad="W18"/>
<connect gate="E" pin="IO_33" pad="W20"/>
<connect gate="E" pin="IO_34" pad="W21"/>
<connect gate="E" pin="IO_35" pad="W22"/>
<connect gate="E" pin="IO_36" pad="Y10"/>
<connect gate="E" pin="IO_37" pad="Y13"/>
<connect gate="E" pin="IO_38" pad="Y14"/>
<connect gate="E" pin="IO_39" pad="Y16"/>
<connect gate="E" pin="IO_4" pad="T16"/>
<connect gate="E" pin="IO_40" pad="Y17"/>
<connect gate="E" pin="IO_41" pad="Y18"/>
<connect gate="E" pin="IO_42" pad="Y19"/>
<connect gate="E" pin="IO_43" pad="Y20"/>
<connect gate="E" pin="IO_44" pad="Y21"/>
<connect gate="E" pin="IO_45" pad="Y22"/>
<connect gate="E" pin="IO_46" pad="AA10"/>
<connect gate="E" pin="IO_47" pad="AA11"/>
<connect gate="E" pin="IO_48" pad="AA12"/>
<connect gate="E" pin="IO_49" pad="AA13"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="AA14"/>
<connect gate="E" pin="IO_51" pad="AA15"/>
<connect gate="E" pin="IO_52" pad="AA16"/>
<connect gate="E" pin="IO_53" pad="AA17"/>
<connect gate="E" pin="IO_54" pad="AA18"/>
<connect gate="E" pin="IO_55" pad="AA19"/>
<connect gate="E" pin="IO_56" pad="AA20"/>
<connect gate="E" pin="IO_57" pad="AB10"/>
<connect gate="E" pin="IO_58" pad="AB11"/>
<connect gate="E" pin="IO_59" pad="AB12"/>
<connect gate="E" pin="IO_6" pad="R20"/>
<connect gate="E" pin="IO_60" pad="AB13"/>
<connect gate="E" pin="IO_61" pad="AB14"/>
<connect gate="E" pin="IO_62" pad="AB15"/>
<connect gate="E" pin="IO_63" pad="AB16"/>
<connect gate="E" pin="IO_64" pad="AB17"/>
<connect gate="E" pin="IO_65" pad="AB18"/>
<connect gate="E" pin="IO_66" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="T18"/>
<connect gate="E" pin="IO_8" pad="R21"/>
<connect gate="E" pin="IO_9" pad="T11"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="AA22"/>
<connect gate="E" pin="VCCIO6_2" pad="T19"/>
<connect gate="E" pin="VCCIO7" pad="AB21"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="W17"/>
<connect gate="E" pin="VCCIO7_4" pad="Y12"/>
<connect gate="E" pin="VCCIO7_5" pad="V13"/>
<connect gate="E" pin="VCCIO8" pad="V10"/>
<connect gate="E" pin="VCCIO8_2" pad="Y11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C35F484I8N"/>
<attribute name="OC_FARNELL" value="1453466"/>
<attribute name="OC_NEWARK" value="52R0522"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C35F672I8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C35F672I8N_A"/>
<gate name="B" symbol="EP2C35F672I8N_B"/>
<gate name="C" symbol="EP2C35F672I8N_C"/>
<gate name="D" symbol="EP2C35F672I8N_D"/>
<gate name="E" symbol="EP2C35F672I8N_E"/>
<gate name="F" symbol="EP2C35F672I8N_F"/>
<gate name="G" symbol="EP2C35F672I8N_G"/>
</gates>
<devices>
<device name="" package="BGA672C100P26X26_2700X2700X350">
<connects>
<connect gate="A" pin="GND" pad="A2"/>
<connect gate="A" pin="GNDA_PLL3" pad="F8"/>
<connect gate="A" pin="GND_2" pad="B1"/>
<connect gate="A" pin="GND_3" pad="D4"/>
<connect gate="A" pin="GND_4" pad="E7"/>
<connect gate="A" pin="GND_5" pad="H5"/>
<connect gate="A" pin="GND_6" pad="L5"/>
<connect gate="A" pin="GND_PLL3" pad="G7"/>
<connect gate="A" pin="GND_PLL3_2" pad="E4"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B4"/>
<connect gate="A" pin="IO_11" pad="B5"/>
<connect gate="A" pin="IO_12" pad="B6"/>
<connect gate="A" pin="IO_13" pad="B7"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="C2"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="C4"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="C7"/>
<connect gate="A" pin="IO_22" pad="C8"/>
<connect gate="A" pin="IO_23" pad="C9"/>
<connect gate="A" pin="IO_24" pad="F1"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="F2"/>
<connect gate="A" pin="IO_28" pad="D3"/>
<connect gate="A" pin="IO_29" pad="F3"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="F4"/>
<connect gate="A" pin="IO_31" pad="D5"/>
<connect gate="A" pin="IO_32" pad="D6"/>
<connect gate="A" pin="IO_33" pad="D7"/>
<connect gate="A" pin="IO_34" pad="D8"/>
<connect gate="A" pin="IO_35" pad="D9"/>
<connect gate="A" pin="IO_36" pad="E1"/>
<connect gate="A" pin="IO_37" pad="E2"/>
<connect gate="A" pin="IO_38" pad="E3"/>
<connect gate="A" pin="IO_39" pad="E8"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="E5"/>
<connect gate="A" pin="IO_41" pad="F6"/>
<connect gate="A" pin="IO_42" pad="F7"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G4"/>
<connect gate="A" pin="IO_48" pad="G5"/>
<connect gate="A" pin="IO_49" pad="G6"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="G9"/>
<connect gate="A" pin="IO_51" pad="H1"/>
<connect gate="A" pin="IO_52" pad="H2"/>
<connect gate="A" pin="IO_53" pad="H3"/>
<connect gate="A" pin="IO_54" pad="H4"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H8"/>
<connect gate="A" pin="IO_57" pad="J1"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_60" pad="J4"/>
<connect gate="A" pin="IO_61" pad="J5"/>
<connect gate="A" pin="IO_62" pad="J6"/>
<connect gate="A" pin="IO_63" pad="J7"/>
<connect gate="A" pin="IO_64" pad="J8"/>
<connect gate="A" pin="IO_65" pad="J9"/>
<connect gate="A" pin="IO_66" pad="K1"/>
<connect gate="A" pin="IO_67" pad="K2"/>
<connect gate="A" pin="IO_68" pad="K3"/>
<connect gate="A" pin="IO_69" pad="K4"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_70" pad="K5"/>
<connect gate="A" pin="IO_71" pad="K6"/>
<connect gate="A" pin="IO_72" pad="K7"/>
<connect gate="A" pin="IO_73" pad="K8"/>
<connect gate="A" pin="IO_74" pad="K9"/>
<connect gate="A" pin="IO_75" pad="L2"/>
<connect gate="A" pin="IO_76" pad="L3"/>
<connect gate="A" pin="IO_77" pad="L4"/>
<connect gate="A" pin="IO_78" pad="L6"/>
<connect gate="A" pin="IO_8" pad="B2"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="VCCA_PLL3" pad="G8"/>
<connect gate="A" pin="VCCD_PLL3" pad="H7"/>
<connect gate="A" pin="VCCIO2" pad="L1"/>
<connect gate="A" pin="VCCIO2_2" pad="F5"/>
<connect gate="A" pin="VCCIO2_3" pad="C1"/>
<connect gate="A" pin="VCCIO3" pad="E9"/>
<connect gate="A" pin="VCCIO3_2" pad="H9"/>
<connect gate="A" pin="VCCIO3_3" pad="A3"/>
<connect gate="A" pin="VCCIO3_4" pad="E6"/>
<connect gate="B" pin="CLK0" pad="N2"/>
<connect gate="B" pin="CLK1" pad="N1"/>
<connect gate="B" pin="CLK2" pad="P2"/>
<connect gate="B" pin="CLK3" pad="P1"/>
<connect gate="B" pin="CLK9" pad="A13"/>
<connect gate="B" pin="DATA0" pad="N3"/>
<connect gate="B" pin="DCLK" pad="N6"/>
<connect gate="B" pin="GND" pad="U8"/>
<connect gate="B" pin="GNDA_PLL1" pad="Y8"/>
<connect gate="B" pin="GND_10" pad="N8"/>
<connect gate="B" pin="GND_2" pad="M1"/>
<connect gate="B" pin="GND_3" pad="W5"/>
<connect gate="B" pin="GND_4" pad="R1"/>
<connect gate="B" pin="GND_5" pad="P8"/>
<connect gate="B" pin="GND_6" pad="T5"/>
<connect gate="B" pin="GND_7" pad="Y9"/>
<connect gate="B" pin="GND_8" pad="A12"/>
<connect gate="B" pin="GND_9" pad="A15"/>
<connect gate="B" pin="GND_PLL1" pad="W7"/>
<connect gate="B" pin="GND_PLL1_2" pad="Y6"/>
<connect gate="B" pin="IO" pad="A22"/>
<connect gate="B" pin="IO_10" pad="T2"/>
<connect gate="B" pin="IO_11" pad="P7"/>
<connect gate="B" pin="IO_12" pad="T3"/>
<connect gate="B" pin="IO_13" pad="T4"/>
<connect gate="B" pin="IO_14" pad="P9"/>
<connect gate="B" pin="IO_15" pad="N9"/>
<connect gate="B" pin="IO_16" pad="R2"/>
<connect gate="B" pin="IO_17" pad="R3"/>
<connect gate="B" pin="IO_18" pad="R4"/>
<connect gate="B" pin="IO_19" pad="T6"/>
<connect gate="B" pin="IO_2" pad="P3"/>
<connect gate="B" pin="IO_20" pad="R5"/>
<connect gate="B" pin="IO_21" pad="T7"/>
<connect gate="B" pin="IO_22" pad="R6"/>
<connect gate="B" pin="IO_23" pad="T8"/>
<connect gate="B" pin="IO_24" pad="R7"/>
<connect gate="B" pin="IO_25" pad="T9"/>
<connect gate="B" pin="IO_26" pad="R8"/>
<connect gate="B" pin="IO_27" pad="U1"/>
<connect gate="B" pin="IO_28" pad="U2"/>
<connect gate="B" pin="IO_29" pad="U3"/>
<connect gate="B" pin="IO_3" pad="M2"/>
<connect gate="B" pin="IO_30" pad="U4"/>
<connect gate="B" pin="IO_31" pad="U5"/>
<connect gate="B" pin="IO_32" pad="U6"/>
<connect gate="B" pin="IO_33" pad="U7"/>
<connect gate="B" pin="IO_34" pad="U9"/>
<connect gate="B" pin="IO_35" pad="V1"/>
<connect gate="B" pin="IO_36" pad="V2"/>
<connect gate="B" pin="IO_37" pad="V3"/>
<connect gate="B" pin="IO_38" pad="V4"/>
<connect gate="B" pin="IO_39" pad="V5"/>
<connect gate="B" pin="IO_4" pad="P4"/>
<connect gate="B" pin="IO_40" pad="V6"/>
<connect gate="B" pin="IO_41" pad="V7"/>
<connect gate="B" pin="IO_42" pad="V9"/>
<connect gate="B" pin="IO_43" pad="W1"/>
<connect gate="B" pin="IO_44" pad="W2"/>
<connect gate="B" pin="IO_45" pad="W3"/>
<connect gate="B" pin="IO_46" pad="W4"/>
<connect gate="B" pin="IO_47" pad="W6"/>
<connect gate="B" pin="IO_48" pad="W8"/>
<connect gate="B" pin="IO_49" pad="Y1"/>
<connect gate="B" pin="IO_5" pad="M3"/>
<connect gate="B" pin="IO_50" pad="Y3"/>
<connect gate="B" pin="IO_51" pad="Y4"/>
<connect gate="B" pin="IO_52" pad="Y5"/>
<connect gate="B" pin="IO_53" pad="A10"/>
<connect gate="B" pin="IO_54" pad="A14"/>
<connect gate="B" pin="IO_55" pad="A17"/>
<connect gate="B" pin="IO_56" pad="A18"/>
<connect gate="B" pin="IO_57" pad="A19"/>
<connect gate="B" pin="IO_58" pad="A20"/>
<connect gate="B" pin="IO_59" pad="A21"/>
<connect gate="B" pin="IO_6" pad="M5"/>
<connect gate="B" pin="IO_7" pad="L9"/>
<connect gate="B" pin="IO_8" pad="M4"/>
<connect gate="B" pin="IO_9" pad="P6"/>
<connect gate="B" pin="NC" pad="Y2"/>
<connect gate="B" pin="NCE" pad="N4"/>
<connect gate="B" pin="NCONFIG" pad="N7"/>
<connect gate="B" pin="TCK" pad="M6"/>
<connect gate="B" pin="TDI" pad="M8"/>
<connect gate="B" pin="TDO" pad="M7"/>
<connect gate="B" pin="TMS" pad="L8"/>
<connect gate="B" pin="VCCD_PLL1" pad="Y7"/>
<connect gate="B" pin="VCCIO1" pad="V8"/>
<connect gate="B" pin="VCCIO1_2" pad="P5"/>
<connect gate="B" pin="VCCIO1_3" pad="R9"/>
<connect gate="B" pin="VCCIO1_4" pad="T1"/>
<connect gate="B" pin="VCCIO2" pad="N5"/>
<connect gate="B" pin="VCCIO2_2" pad="M9"/>
<connect gate="B" pin="VCCIO3" pad="A11"/>
<connect gate="B" pin="VCCIO4" pad="A16"/>
<connect gate="B" pin="VCCIO8" pad="W9"/>
<connect gate="C" pin="CLK10" pad="C13"/>
<connect gate="C" pin="CLK11" pad="D13"/>
<connect gate="C" pin="CLK8" pad="B13"/>
<connect gate="C" pin="GND" pad="AC4"/>
<connect gate="C" pin="GND_2" pad="AB7"/>
<connect gate="C" pin="GND_3" pad="AD9"/>
<connect gate="C" pin="GND_4" pad="B26"/>
<connect gate="C" pin="GND_5" pad="A25"/>
<connect gate="C" pin="GND_6" pad="AE1"/>
<connect gate="C" pin="GND_7" pad="C14"/>
<connect gate="C" pin="GND_8" pad="AF2"/>
<connect gate="C" pin="GND_9" pad="C18"/>
<connect gate="C" pin="IO" pad="D15"/>
<connect gate="C" pin="IO_10" pad="AB8"/>
<connect gate="C" pin="IO_11" pad="AA9"/>
<connect gate="C" pin="IO_12" pad="AB1"/>
<connect gate="C" pin="IO_13" pad="AB2"/>
<connect gate="C" pin="IO_14" pad="AB3"/>
<connect gate="C" pin="IO_15" pad="AB4"/>
<connect gate="C" pin="IO_16" pad="AC5"/>
<connect gate="C" pin="IO_17" pad="AC6"/>
<connect gate="C" pin="IO_18" pad="AC7"/>
<connect gate="C" pin="IO_19" pad="AC8"/>
<connect gate="C" pin="IO_2" pad="A23"/>
<connect gate="C" pin="IO_20" pad="AC1"/>
<connect gate="C" pin="IO_21" pad="AC9"/>
<connect gate="C" pin="IO_22" pad="AC2"/>
<connect gate="C" pin="IO_23" pad="AC3"/>
<connect gate="C" pin="IO_24" pad="AD2"/>
<connect gate="C" pin="IO_25" pad="AD3"/>
<connect gate="C" pin="IO_26" pad="AD4"/>
<connect gate="C" pin="IO_27" pad="AD5"/>
<connect gate="C" pin="IO_28" pad="AD6"/>
<connect gate="C" pin="IO_29" pad="AD7"/>
<connect gate="C" pin="IO_3" pad="AA1"/>
<connect gate="C" pin="IO_30" pad="AE2"/>
<connect gate="C" pin="IO_31" pad="AD8"/>
<connect gate="C" pin="IO_32" pad="AE3"/>
<connect gate="C" pin="IO_33" pad="AE4"/>
<connect gate="C" pin="IO_34" pad="AE5"/>
<connect gate="C" pin="IO_35" pad="AE6"/>
<connect gate="C" pin="IO_36" pad="AE7"/>
<connect gate="C" pin="IO_37" pad="AE8"/>
<connect gate="C" pin="IO_38" pad="AE9"/>
<connect gate="C" pin="IO_39" pad="AF4"/>
<connect gate="C" pin="IO_4" pad="AA2"/>
<connect gate="C" pin="IO_40" pad="AF5"/>
<connect gate="C" pin="IO_41" pad="AF6"/>
<connect gate="C" pin="IO_42" pad="AF7"/>
<connect gate="C" pin="IO_43" pad="AF8"/>
<connect gate="C" pin="IO_44" pad="AF9"/>
<connect gate="C" pin="IO_45" pad="B10"/>
<connect gate="C" pin="IO_46" pad="B11"/>
<connect gate="C" pin="IO_47" pad="B12"/>
<connect gate="C" pin="IO_48" pad="B14"/>
<connect gate="C" pin="IO_49" pad="B15"/>
<connect gate="C" pin="IO_5" pad="AA3"/>
<connect gate="C" pin="IO_50" pad="B16"/>
<connect gate="C" pin="IO_51" pad="B17"/>
<connect gate="C" pin="IO_52" pad="B18"/>
<connect gate="C" pin="IO_53" pad="B19"/>
<connect gate="C" pin="IO_54" pad="B20"/>
<connect gate="C" pin="IO_55" pad="B21"/>
<connect gate="C" pin="IO_56" pad="B22"/>
<connect gate="C" pin="IO_57" pad="B23"/>
<connect gate="C" pin="IO_58" pad="B24"/>
<connect gate="C" pin="IO_59" pad="B25"/>
<connect gate="C" pin="IO_6" pad="AA4"/>
<connect gate="C" pin="IO_60" pad="C10"/>
<connect gate="C" pin="IO_61" pad="C11"/>
<connect gate="C" pin="IO_62" pad="C12"/>
<connect gate="C" pin="IO_63" pad="C15"/>
<connect gate="C" pin="IO_64" pad="C16"/>
<connect gate="C" pin="IO_65" pad="C17"/>
<connect gate="C" pin="IO_66" pad="C19"/>
<connect gate="C" pin="IO_67" pad="C21"/>
<connect gate="C" pin="IO_68" pad="C22"/>
<connect gate="C" pin="IO_69" pad="C23"/>
<connect gate="C" pin="IO_7" pad="AA5"/>
<connect gate="C" pin="IO_70" pad="C24"/>
<connect gate="C" pin="IO_71" pad="C25"/>
<connect gate="C" pin="IO_72" pad="D10"/>
<connect gate="C" pin="IO_73" pad="D11"/>
<connect gate="C" pin="IO_74" pad="D12"/>
<connect gate="C" pin="IO_75" pad="D14"/>
<connect gate="C" pin="IO_8" pad="AA6"/>
<connect gate="C" pin="IO_9" pad="AA7"/>
<connect gate="C" pin="VCCA_PLL1" pad="AA8"/>
<connect gate="C" pin="VCCIO1" pad="AD1"/>
<connect gate="C" pin="VCCIO1_2" pad="AB5"/>
<connect gate="C" pin="VCCIO4" pad="C20"/>
<connect gate="C" pin="VCCIO4_2" pad="A24"/>
<connect gate="C" pin="VCCIO5" pad="C26"/>
<connect gate="C" pin="VCCIO8" pad="AF3"/>
<connect gate="C" pin="VCCIO8_2" pad="AB6"/>
<connect gate="C" pin="VCCIO8_3" pad="AB9"/>
<connect gate="D" pin="GND" pad="H14"/>
<connect gate="D" pin="GNDA_PLL2" pad="F19"/>
<connect gate="D" pin="GND_2" pad="D24"/>
<connect gate="D" pin="GND_3" pad="E16"/>
<connect gate="D" pin="GND_4" pad="H22"/>
<connect gate="D" pin="GND_5" pad="E19"/>
<connect gate="D" pin="GND_6" pad="H13"/>
<connect gate="D" pin="GND_7" pad="E11"/>
<connect gate="D" pin="GND_PLL2" pad="G20"/>
<connect gate="D" pin="GND_PLL2_2" pad="E21"/>
<connect gate="D" pin="IO" pad="J26"/>
<connect gate="D" pin="IO_10" pad="E15"/>
<connect gate="D" pin="IO_11" pad="D25"/>
<connect gate="D" pin="IO_12" pad="D26"/>
<connect gate="D" pin="IO_13" pad="E10"/>
<connect gate="D" pin="IO_14" pad="E18"/>
<connect gate="D" pin="IO_15" pad="F20"/>
<connect gate="D" pin="IO_16" pad="F21"/>
<connect gate="D" pin="IO_17" pad="F23"/>
<connect gate="D" pin="IO_18" pad="F24"/>
<connect gate="D" pin="IO_19" pad="F25"/>
<connect gate="D" pin="IO_2" pad="D16"/>
<connect gate="D" pin="IO_20" pad="E20"/>
<connect gate="D" pin="IO_21" pad="F26"/>
<connect gate="D" pin="IO_22" pad="G10"/>
<connect gate="D" pin="IO_23" pad="E22"/>
<connect gate="D" pin="IO_24" pad="G11"/>
<connect gate="D" pin="IO_25" pad="E23"/>
<connect gate="D" pin="IO_26" pad="G12"/>
<connect gate="D" pin="IO_27" pad="E24"/>
<connect gate="D" pin="IO_28" pad="E25"/>
<connect gate="D" pin="IO_29" pad="E26"/>
<connect gate="D" pin="IO_3" pad="D17"/>
<connect gate="D" pin="IO_30" pad="F10"/>
<connect gate="D" pin="IO_31" pad="F11"/>
<connect gate="D" pin="IO_32" pad="F12"/>
<connect gate="D" pin="IO_33" pad="F13"/>
<connect gate="D" pin="IO_34" pad="F14"/>
<connect gate="D" pin="IO_35" pad="F15"/>
<connect gate="D" pin="IO_36" pad="F16"/>
<connect gate="D" pin="IO_37" pad="F17"/>
<connect gate="D" pin="IO_38" pad="F18"/>
<connect gate="D" pin="IO_39" pad="G13"/>
<connect gate="D" pin="IO_4" pad="D18"/>
<connect gate="D" pin="IO_40" pad="G14"/>
<connect gate="D" pin="IO_41" pad="G15"/>
<connect gate="D" pin="IO_42" pad="G16"/>
<connect gate="D" pin="IO_43" pad="G17"/>
<connect gate="D" pin="IO_44" pad="G18"/>
<connect gate="D" pin="IO_45" pad="G21"/>
<connect gate="D" pin="IO_46" pad="G22"/>
<connect gate="D" pin="IO_47" pad="G23"/>
<connect gate="D" pin="IO_48" pad="G24"/>
<connect gate="D" pin="IO_49" pad="G25"/>
<connect gate="D" pin="IO_5" pad="D19"/>
<connect gate="D" pin="IO_50" pad="G26"/>
<connect gate="D" pin="IO_51" pad="H10"/>
<connect gate="D" pin="IO_52" pad="H11"/>
<connect gate="D" pin="IO_53" pad="H12"/>
<connect gate="D" pin="IO_54" pad="H15"/>
<connect gate="D" pin="IO_55" pad="H16"/>
<connect gate="D" pin="IO_56" pad="H17"/>
<connect gate="D" pin="IO_57" pad="H19"/>
<connect gate="D" pin="IO_58" pad="H21"/>
<connect gate="D" pin="IO_59" pad="H23"/>
<connect gate="D" pin="IO_6" pad="D20"/>
<connect gate="D" pin="IO_60" pad="H24"/>
<connect gate="D" pin="IO_61" pad="H25"/>
<connect gate="D" pin="IO_62" pad="H26"/>
<connect gate="D" pin="IO_63" pad="J10"/>
<connect gate="D" pin="IO_64" pad="J11"/>
<connect gate="D" pin="IO_65" pad="J13"/>
<connect gate="D" pin="IO_66" pad="J14"/>
<connect gate="D" pin="IO_67" pad="J16"/>
<connect gate="D" pin="IO_68" pad="J17"/>
<connect gate="D" pin="IO_69" pad="J18"/>
<connect gate="D" pin="IO_7" pad="E12"/>
<connect gate="D" pin="IO_70" pad="J20"/>
<connect gate="D" pin="IO_71" pad="J21"/>
<connect gate="D" pin="IO_72" pad="J22"/>
<connect gate="D" pin="IO_73" pad="J23"/>
<connect gate="D" pin="IO_74" pad="J24"/>
<connect gate="D" pin="IO_75" pad="J25"/>
<connect gate="D" pin="IO_8" pad="D21"/>
<connect gate="D" pin="IO_9" pad="D23"/>
<connect gate="D" pin="VCCA_PLL2" pad="G19"/>
<connect gate="D" pin="VCCD_PLL2" pad="H20"/>
<connect gate="D" pin="VCCIO3" pad="E13"/>
<connect gate="D" pin="VCCIO3_2" pad="J12"/>
<connect gate="D" pin="VCCIO4" pad="H18"/>
<connect gate="D" pin="VCCIO4_2" pad="E17"/>
<connect gate="D" pin="VCCIO4_3" pad="D22"/>
<connect gate="D" pin="VCCIO4_4" pad="J15"/>
<connect gate="D" pin="VCCIO4_5" pad="E14"/>
<connect gate="D" pin="VCCIO5" pad="F22"/>
<connect gate="D" pin="VCCIO5_2" pad="J19"/>
<connect gate="E" pin="CLK4" pad="N25"/>
<connect gate="E" pin="CLK5" pad="N26"/>
<connect gate="E" pin="CLK6" pad="P25"/>
<connect gate="E" pin="CLK7" pad="P26"/>
<connect gate="E" pin="GND" pad="P19"/>
<connect gate="E" pin="GND_10" pad="M13"/>
<connect gate="E" pin="GND_11" pad="N12"/>
<connect gate="E" pin="GND_12" pad="M26"/>
<connect gate="E" pin="GND_13" pad="N13"/>
<connect gate="E" pin="GND_14" pad="M14"/>
<connect gate="E" pin="GND_15" pad="P11"/>
<connect gate="E" pin="GND_16" pad="N19"/>
<connect gate="E" pin="GND_17" pad="P12"/>
<connect gate="E" pin="GND_18" pad="N14"/>
<connect gate="E" pin="GND_19" pad="R12"/>
<connect gate="E" pin="GND_2" pad="M12"/>
<connect gate="E" pin="GND_20" pad="P13"/>
<connect gate="E" pin="GND_21" pad="R13"/>
<connect gate="E" pin="GND_22" pad="M15"/>
<connect gate="E" pin="GND_23" pad="R14"/>
<connect gate="E" pin="GND_24" pad="P14"/>
<connect gate="E" pin="GND_25" pad="R15"/>
<connect gate="E" pin="GND_26" pad="N15"/>
<connect gate="E" pin="GND_27" pad="P15"/>
<connect gate="E" pin="GND_28" pad="N16"/>
<connect gate="E" pin="GND_29" pad="P16"/>
<connect gate="E" pin="GND_3" pad="L12"/>
<connect gate="E" pin="GND_4" pad="L22"/>
<connect gate="E" pin="GND_5" pad="L13"/>
<connect gate="E" pin="GND_6" pad="N11"/>
<connect gate="E" pin="GND_7" pad="K20"/>
<connect gate="E" pin="GND_8" pad="L14"/>
<connect gate="E" pin="GND_9" pad="L15"/>
<connect gate="E" pin="IO" pad="R20"/>
<connect gate="E" pin="IO_10" pad="K18"/>
<connect gate="E" pin="IO_11" pad="L21"/>
<connect gate="E" pin="IO_12" pad="K25"/>
<connect gate="E" pin="IO_13" pad="M19"/>
<connect gate="E" pin="IO_14" pad="K19"/>
<connect gate="E" pin="IO_15" pad="M20"/>
<connect gate="E" pin="IO_16" pad="K26"/>
<connect gate="E" pin="IO_17" pad="L23"/>
<connect gate="E" pin="IO_18" pad="L10"/>
<connect gate="E" pin="IO_19" pad="M21"/>
<connect gate="E" pin="IO_2" pad="K21"/>
<connect gate="E" pin="IO_20" pad="L24"/>
<connect gate="E" pin="IO_21" pad="M22"/>
<connect gate="E" pin="IO_22" pad="L25"/>
<connect gate="E" pin="IO_23" pad="M23"/>
<connect gate="E" pin="IO_24" pad="M24"/>
<connect gate="E" pin="IO_25" pad="M25"/>
<connect gate="E" pin="IO_26" pad="N18"/>
<connect gate="E" pin="IO_27" pad="N20"/>
<connect gate="E" pin="IO_28" pad="N23"/>
<connect gate="E" pin="IO_29" pad="N24"/>
<connect gate="E" pin="IO_3" pad="K22"/>
<connect gate="E" pin="IO_30" pad="P17"/>
<connect gate="E" pin="IO_31" pad="P18"/>
<connect gate="E" pin="IO_32" pad="P23"/>
<connect gate="E" pin="IO_33" pad="P24"/>
<connect gate="E" pin="IO_34" pad="R17"/>
<connect gate="E" pin="IO_35" pad="R19"/>
<connect gate="E" pin="IO_4" pad="K16"/>
<connect gate="E" pin="IO_5" pad="K23"/>
<connect gate="E" pin="IO_6" pad="L19"/>
<connect gate="E" pin="IO_7" pad="K17"/>
<connect gate="E" pin="IO_8" pad="K24"/>
<connect gate="E" pin="IO_9" pad="L20"/>
<connect gate="E" pin="MSEL0" pad="P20"/>
<connect gate="E" pin="MSEL1" pad="P21"/>
<connect gate="E" pin="NC" pad="N21"/>
<connect gate="E" pin="VCCINT" pad="R16"/>
<connect gate="E" pin="VCCINT_10" pad="M17"/>
<connect gate="E" pin="VCCINT_11" pad="N10"/>
<connect gate="E" pin="VCCINT_12" pad="L11"/>
<connect gate="E" pin="VCCINT_13" pad="R10"/>
<connect gate="E" pin="VCCINT_14" pad="L16"/>
<connect gate="E" pin="VCCINT_15" pad="R11"/>
<connect gate="E" pin="VCCINT_16" pad="L17"/>
<connect gate="E" pin="VCCINT_17" pad="L18"/>
<connect gate="E" pin="VCCINT_18" pad="P10"/>
<connect gate="E" pin="VCCINT_19" pad="M10"/>
<connect gate="E" pin="VCCINT_2" pad="K10"/>
<connect gate="E" pin="VCCINT_20" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="K11"/>
<connect gate="E" pin="VCCINT_4" pad="K12"/>
<connect gate="E" pin="VCCINT_5" pad="K13"/>
<connect gate="E" pin="VCCINT_6" pad="K14"/>
<connect gate="E" pin="VCCINT_7" pad="K15"/>
<connect gate="E" pin="VCCINT_8" pad="M16"/>
<connect gate="E" pin="VCCINT_9" pad="N17"/>
<connect gate="E" pin="VCCIO5" pad="N22"/>
<connect gate="E" pin="VCCIO5_2" pad="M18"/>
<connect gate="E" pin="VCCIO5_3" pad="L26"/>
<connect gate="E" pin="VCCIO6" pad="R18"/>
<connect gate="E" pin="VCCIO6_2" pad="P22"/>
<connect gate="F" pin="CONF_DONE" pad="R23"/>
<connect gate="F" pin="GND" pad="Y17"/>
<connect gate="F" pin="GNDA_PLL4" pad="Y19"/>
<connect gate="F" pin="GND_10" pad="T15"/>
<connect gate="F" pin="GND_11" pad="W14"/>
<connect gate="F" pin="GND_2" pad="W13"/>
<connect gate="F" pin="GND_3" pad="T12"/>
<connect gate="F" pin="GND_4" pad="U19"/>
<connect gate="F" pin="GND_5" pad="R21"/>
<connect gate="F" pin="GND_6" pad="T13"/>
<connect gate="F" pin="GND_7" pad="T14"/>
<connect gate="F" pin="GND_8" pad="W22"/>
<connect gate="F" pin="GND_9" pad="R26"/>
<connect gate="F" pin="GND_PLL4" pad="W20"/>
<connect gate="F" pin="IO" pad="AA14"/>
<connect gate="F" pin="IO_10" pad="T25"/>
<connect gate="F" pin="IO_11" pad="U10"/>
<connect gate="F" pin="IO_12" pad="R24"/>
<connect gate="F" pin="IO_13" pad="R25"/>
<connect gate="F" pin="IO_14" pad="U12"/>
<connect gate="F" pin="IO_15" pad="U17"/>
<connect gate="F" pin="IO_16" pad="U18"/>
<connect gate="F" pin="IO_17" pad="T10"/>
<connect gate="F" pin="IO_18" pad="U20"/>
<connect gate="F" pin="IO_19" pad="U21"/>
<connect gate="F" pin="IO_2" pad="T17"/>
<connect gate="F" pin="IO_20" pad="U22"/>
<connect gate="F" pin="IO_21" pad="U23"/>
<connect gate="F" pin="IO_22" pad="U24"/>
<connect gate="F" pin="IO_23" pad="U25"/>
<connect gate="F" pin="IO_24" pad="U26"/>
<connect gate="F" pin="IO_25" pad="V10"/>
<connect gate="F" pin="IO_26" pad="V11"/>
<connect gate="F" pin="IO_27" pad="V17"/>
<connect gate="F" pin="IO_28" pad="V13"/>
<connect gate="F" pin="IO_29" pad="V14"/>
<connect gate="F" pin="IO_3" pad="T18"/>
<connect gate="F" pin="IO_30" pad="V18"/>
<connect gate="F" pin="IO_31" pad="V20"/>
<connect gate="F" pin="IO_32" pad="V21"/>
<connect gate="F" pin="IO_33" pad="V22"/>
<connect gate="F" pin="IO_34" pad="V23"/>
<connect gate="F" pin="IO_35" pad="V24"/>
<connect gate="F" pin="IO_36" pad="V25"/>
<connect gate="F" pin="IO_37" pad="V26"/>
<connect gate="F" pin="IO_38" pad="W10"/>
<connect gate="F" pin="IO_39" pad="W11"/>
<connect gate="F" pin="IO_4" pad="T19"/>
<connect gate="F" pin="IO_40" pad="W12"/>
<connect gate="F" pin="IO_41" pad="W15"/>
<connect gate="F" pin="IO_42" pad="W16"/>
<connect gate="F" pin="IO_43" pad="W17"/>
<connect gate="F" pin="IO_44" pad="W19"/>
<connect gate="F" pin="IO_45" pad="W21"/>
<connect gate="F" pin="IO_46" pad="W23"/>
<connect gate="F" pin="IO_47" pad="W24"/>
<connect gate="F" pin="IO_48" pad="W25"/>
<connect gate="F" pin="IO_49" pad="W26"/>
<connect gate="F" pin="IO_5" pad="T20"/>
<connect gate="F" pin="IO_50" pad="Y10"/>
<connect gate="F" pin="IO_51" pad="Y11"/>
<connect gate="F" pin="IO_52" pad="Y12"/>
<connect gate="F" pin="IO_53" pad="Y13"/>
<connect gate="F" pin="IO_54" pad="Y14"/>
<connect gate="F" pin="IO_55" pad="Y15"/>
<connect gate="F" pin="IO_56" pad="Y16"/>
<connect gate="F" pin="IO_57" pad="Y18"/>
<connect gate="F" pin="IO_58" pad="Y21"/>
<connect gate="F" pin="IO_59" pad="Y22"/>
<connect gate="F" pin="IO_6" pad="T21"/>
<connect gate="F" pin="IO_60" pad="Y23"/>
<connect gate="F" pin="IO_61" pad="Y24"/>
<connect gate="F" pin="IO_62" pad="Y25"/>
<connect gate="F" pin="IO_63" pad="Y26"/>
<connect gate="F" pin="IO_64" pad="AA10"/>
<connect gate="F" pin="IO_65" pad="AA11"/>
<connect gate="F" pin="IO_66" pad="AA12"/>
<connect gate="F" pin="IO_67" pad="AA13"/>
<connect gate="F" pin="IO_7" pad="T22"/>
<connect gate="F" pin="IO_8" pad="T23"/>
<connect gate="F" pin="IO_9" pad="T24"/>
<connect gate="F" pin="NSTATUS" pad="R22"/>
<connect gate="F" pin="VCCD_PLL4" pad="Y20"/>
<connect gate="F" pin="VCCINT" pad="U16"/>
<connect gate="F" pin="VCCINT_2" pad="U11"/>
<connect gate="F" pin="VCCINT_3" pad="U13"/>
<connect gate="F" pin="VCCINT_4" pad="V16"/>
<connect gate="F" pin="VCCINT_5" pad="T11"/>
<connect gate="F" pin="VCCINT_6" pad="U14"/>
<connect gate="F" pin="VCCINT_7" pad="T16"/>
<connect gate="F" pin="VCCINT_8" pad="U15"/>
<connect gate="F" pin="VCCIO6" pad="V19"/>
<connect gate="F" pin="VCCIO6_2" pad="T26"/>
<connect gate="F" pin="VCCIO7" pad="W18"/>
<connect gate="F" pin="VCCIO7_2" pad="V15"/>
<connect gate="F" pin="VCCIO8" pad="V12"/>
<connect gate="G" pin="CLK12" pad="AE14"/>
<connect gate="G" pin="CLK13" pad="AF14"/>
<connect gate="G" pin="CLK14" pad="AD13"/>
<connect gate="G" pin="CLK15" pad="AC13"/>
<connect gate="G" pin="GND" pad="AB19"/>
<connect gate="G" pin="GND_2" pad="AD14"/>
<connect gate="G" pin="GND_3" pad="AD18"/>
<connect gate="G" pin="GND_4" pad="AF15"/>
<connect gate="G" pin="GND_5" pad="AB11"/>
<connect gate="G" pin="GND_6" pad="AB16"/>
<connect gate="G" pin="GND_7" pad="AF25"/>
<connect gate="G" pin="GND_8" pad="AF12"/>
<connect gate="G" pin="GND_9" pad="AE26"/>
<connect gate="G" pin="GND_PLL4" pad="AA21"/>
<connect gate="G" pin="IO" pad="AF23"/>
<connect gate="G" pin="IO_10" pad="AB25"/>
<connect gate="G" pin="IO_11" pad="AA25"/>
<connect gate="G" pin="IO_12" pad="AB26"/>
<connect gate="G" pin="IO_13" pad="AA16"/>
<connect gate="G" pin="IO_14" pad="AC10"/>
<connect gate="G" pin="IO_15" pad="AA26"/>
<connect gate="G" pin="IO_16" pad="AC11"/>
<connect gate="G" pin="IO_17" pad="AA17"/>
<connect gate="G" pin="IO_18" pad="AC12"/>
<connect gate="G" pin="IO_19" pad="AB10"/>
<connect gate="G" pin="IO_2" pad="AB18"/>
<connect gate="G" pin="IO_20" pad="AA20"/>
<connect gate="G" pin="IO_21" pad="AC14"/>
<connect gate="G" pin="IO_22" pad="AA18"/>
<connect gate="G" pin="IO_23" pad="AC15"/>
<connect gate="G" pin="IO_24" pad="AB12"/>
<connect gate="G" pin="IO_25" pad="AC16"/>
<connect gate="G" pin="IO_26" pad="AB15"/>
<connect gate="G" pin="IO_27" pad="AC17"/>
<connect gate="G" pin="IO_28" pad="AC18"/>
<connect gate="G" pin="IO_29" pad="AC19"/>
<connect gate="G" pin="IO_3" pad="AB20"/>
<connect gate="G" pin="IO_30" pad="AC20"/>
<connect gate="G" pin="IO_31" pad="AC21"/>
<connect gate="G" pin="IO_32" pad="AC22"/>
<connect gate="G" pin="IO_33" pad="AC23"/>
<connect gate="G" pin="IO_34" pad="AC25"/>
<connect gate="G" pin="IO_35" pad="AC26"/>
<connect gate="G" pin="IO_36" pad="AD10"/>
<connect gate="G" pin="IO_37" pad="AD11"/>
<connect gate="G" pin="IO_38" pad="AD12"/>
<connect gate="G" pin="IO_39" pad="AD15"/>
<connect gate="G" pin="IO_4" pad="AA23"/>
<connect gate="G" pin="IO_40" pad="AD16"/>
<connect gate="G" pin="IO_41" pad="AD17"/>
<connect gate="G" pin="IO_42" pad="AD19"/>
<connect gate="G" pin="IO_43" pad="AD21"/>
<connect gate="G" pin="IO_44" pad="AD22"/>
<connect gate="G" pin="IO_45" pad="AD23"/>
<connect gate="G" pin="IO_46" pad="AD24"/>
<connect gate="G" pin="IO_47" pad="AD25"/>
<connect gate="G" pin="IO_48" pad="AE10"/>
<connect gate="G" pin="IO_49" pad="AE11"/>
<connect gate="G" pin="IO_5" pad="AB21"/>
<connect gate="G" pin="IO_50" pad="AE12"/>
<connect gate="G" pin="IO_51" pad="AE13"/>
<connect gate="G" pin="IO_52" pad="AE15"/>
<connect gate="G" pin="IO_53" pad="AE16"/>
<connect gate="G" pin="IO_54" pad="AE17"/>
<connect gate="G" pin="IO_55" pad="AE18"/>
<connect gate="G" pin="IO_56" pad="AE19"/>
<connect gate="G" pin="IO_57" pad="AE20"/>
<connect gate="G" pin="IO_58" pad="AE21"/>
<connect gate="G" pin="IO_59" pad="AE22"/>
<connect gate="G" pin="IO_6" pad="AB23"/>
<connect gate="G" pin="IO_60" pad="AE23"/>
<connect gate="G" pin="IO_61" pad="AE24"/>
<connect gate="G" pin="IO_62" pad="AE25"/>
<connect gate="G" pin="IO_63" pad="AF10"/>
<connect gate="G" pin="IO_64" pad="AF13"/>
<connect gate="G" pin="IO_65" pad="AF17"/>
<connect gate="G" pin="IO_66" pad="AF18"/>
<connect gate="G" pin="IO_67" pad="AF19"/>
<connect gate="G" pin="IO_68" pad="AF20"/>
<connect gate="G" pin="IO_69" pad="AF21"/>
<connect gate="G" pin="IO_7" pad="AA24"/>
<connect gate="G" pin="IO_70" pad="AF22"/>
<connect gate="G" pin="IO_8" pad="AB24"/>
<connect gate="G" pin="IO_9" pad="AA15"/>
<connect gate="G" pin="NC" pad="AC24"/>
<connect gate="G" pin="VCCA_PLL4" pad="AA19"/>
<connect gate="G" pin="VCCIO6" pad="AD26"/>
<connect gate="G" pin="VCCIO6_2" pad="AA22"/>
<connect gate="G" pin="VCCIO7" pad="AF24"/>
<connect gate="G" pin="VCCIO7_2" pad="AF16"/>
<connect gate="G" pin="VCCIO7_3" pad="AB17"/>
<connect gate="G" pin="VCCIO7_4" pad="AB22"/>
<connect gate="G" pin="VCCIO7_5" pad="AD20"/>
<connect gate="G" pin="VCCIO7_6" pad="AB14"/>
<connect gate="G" pin="VCCIO8" pad="AF11"/>
<connect gate="G" pin="VCCIO8_2" pad="AB13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C35F672I8N"/>
<attribute name="OC_FARNELL" value="1663199"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="BGA-672"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C35U484C8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C35U484C8N_A"/>
<gate name="B" symbol="EP2C35U484C8N_B"/>
<gate name="C" symbol="EP2C35U484C8N_C"/>
<gate name="D" symbol="EP2C35U484C8N_D"/>
<gate name="E" symbol="EP2C35U484C8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C80P22X22_1900X1900X220">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K7"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="J9"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="C5"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="GND_6" pad="G4"/>
<connect gate="A" pin="GND_7" pad="K3"/>
<connect gate="A" pin="GND_8" pad="H9"/>
<connect gate="A" pin="GND_9" pad="J8"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="C9"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="D1"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="A5"/>
<connect gate="A" pin="IO_16" pad="D3"/>
<connect gate="A" pin="IO_17" pad="B9"/>
<connect gate="A" pin="IO_18" pad="D4"/>
<connect gate="A" pin="IO_19" pad="A6"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="D5"/>
<connect gate="A" pin="IO_21" pad="C1"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="A7"/>
<connect gate="A" pin="IO_24" pad="D7"/>
<connect gate="A" pin="IO_25" pad="C2"/>
<connect gate="A" pin="IO_26" pad="D8"/>
<connect gate="A" pin="IO_27" pad="A8"/>
<connect gate="A" pin="IO_28" pad="D9"/>
<connect gate="A" pin="IO_29" pad="C3"/>
<connect gate="A" pin="IO_3" pad="C4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E7"/>
<connect gate="A" pin="IO_34" pad="E3"/>
<connect gate="A" pin="IO_35" pad="E8"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="B4"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="G7"/>
<connect gate="A" pin="IO_5" pad="B5"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="J1"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_60" pad="J4"/>
<connect gate="A" pin="IO_61" pad="J5"/>
<connect gate="A" pin="IO_62" pad="L7"/>
<connect gate="A" pin="IO_7" pad="C7"/>
<connect gate="A" pin="IO_8" pad="A3"/>
<connect gate="A" pin="IO_9" pad="B7"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="G8"/>
<connect gate="A" pin="VCCINT_3" pad="K8"/>
<connect gate="A" pin="VCCINT_4" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="J7"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="L3"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="R3"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V6"/>
<connect gate="B" pin="GND_11" pad="V3"/>
<connect gate="B" pin="GND_2" pad="M4"/>
<connect gate="B" pin="GND_3" pad="Y8"/>
<connect gate="B" pin="GND_4" pad="P8"/>
<connect gate="B" pin="GND_5" pad="R9"/>
<connect gate="B" pin="GND_6" pad="N7"/>
<connect gate="B" pin="GND_7" pad="A22"/>
<connect gate="B" pin="GND_8" pad="P9"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GND_PLL1" pad="U5"/>
<connect gate="B" pin="GND_PLL1_2" pad="V5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="R5"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="R6"/>
<connect gate="B" pin="IO_13" pad="N4"/>
<connect gate="B" pin="IO_14" pad="R7"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="R8"/>
<connect gate="B" pin="IO_17" pad="U1"/>
<connect gate="B" pin="IO_18" pad="N6"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="M5"/>
<connect gate="B" pin="IO_20" pad="P1"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="P2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="P3"/>
<connect gate="B" pin="IO_25" pad="P4"/>
<connect gate="B" pin="IO_26" pad="P5"/>
<connect gate="B" pin="IO_27" pad="P6"/>
<connect gate="B" pin="IO_28" pad="T5"/>
<connect gate="B" pin="IO_29" pad="T6"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="T7"/>
<connect gate="B" pin="IO_31" pad="R1"/>
<connect gate="B" pin="IO_32" pad="T8"/>
<connect gate="B" pin="IO_33" pad="R2"/>
<connect gate="B" pin="IO_34" pad="U2"/>
<connect gate="B" pin="IO_35" pad="U3"/>
<connect gate="B" pin="IO_36" pad="U4"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V8"/>
<connect gate="B" pin="IO_43" pad="V9"/>
<connect gate="B" pin="IO_44" pad="W1"/>
<connect gate="B" pin="IO_45" pad="W2"/>
<connect gate="B" pin="IO_46" pad="W3"/>
<connect gate="B" pin="IO_47" pad="W4"/>
<connect gate="B" pin="IO_48" pad="W5"/>
<connect gate="B" pin="IO_49" pad="W7"/>
<connect gate="B" pin="IO_5" pad="M7"/>
<connect gate="B" pin="IO_50" pad="W8"/>
<connect gate="B" pin="IO_51" pad="W9"/>
<connect gate="B" pin="IO_52" pad="Y1"/>
<connect gate="B" pin="IO_53" pad="Y2"/>
<connect gate="B" pin="IO_54" pad="Y3"/>
<connect gate="B" pin="IO_55" pad="Y4"/>
<connect gate="B" pin="IO_56" pad="Y5"/>
<connect gate="B" pin="IO_57" pad="Y6"/>
<connect gate="B" pin="IO_58" pad="Y7"/>
<connect gate="B" pin="IO_59" pad="Y9"/>
<connect gate="B" pin="IO_6" pad="M8"/>
<connect gate="B" pin="IO_60" pad="A10"/>
<connect gate="B" pin="IO_61" pad="A11"/>
<connect gate="B" pin="IO_62" pad="A13"/>
<connect gate="B" pin="IO_63" pad="A14"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_68" pad="A19"/>
<connect gate="B" pin="IO_7" pad="N1"/>
<connect gate="B" pin="IO_8" pad="R4"/>
<connect gate="B" pin="IO_9" pad="N2"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="N9"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="M9"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="P7"/>
<connect gate="B" pin="VCCIO1_3" pad="T4"/>
<connect gate="B" pin="VCCIO1_4" pad="M3"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="T9"/>
<connect gate="B" pin="VCCIO8_2" pad="W6"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="H10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="C15"/>
<connect gate="C" pin="GND_11" pad="G15"/>
<connect gate="C" pin="GND_12" pad="G13"/>
<connect gate="C" pin="GND_2" pad="AB1"/>
<connect gate="C" pin="GND_3" pad="D10"/>
<connect gate="C" pin="GND_4" pad="D18"/>
<connect gate="C" pin="GND_5" pad="D13"/>
<connect gate="C" pin="GND_6" pad="F19"/>
<connect gate="C" pin="GND_7" pad="AA2"/>
<connect gate="C" pin="GND_8" pad="G10"/>
<connect gate="C" pin="GND_9" pad="B21"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="C13"/>
<connect gate="C" pin="IO_11" pad="AA3"/>
<connect gate="C" pin="IO_12" pad="AB9"/>
<connect gate="C" pin="IO_13" pad="AA4"/>
<connect gate="C" pin="IO_14" pad="B10"/>
<connect gate="C" pin="IO_15" pad="AA5"/>
<connect gate="C" pin="IO_16" pad="B11"/>
<connect gate="C" pin="IO_17" pad="AA6"/>
<connect gate="C" pin="IO_18" pad="AA7"/>
<connect gate="C" pin="IO_19" pad="B13"/>
<connect gate="C" pin="IO_2" pad="AB3"/>
<connect gate="C" pin="IO_20" pad="AA8"/>
<connect gate="C" pin="IO_21" pad="B14"/>
<connect gate="C" pin="IO_22" pad="C14"/>
<connect gate="C" pin="IO_23" pad="AA9"/>
<connect gate="C" pin="IO_24" pad="B15"/>
<connect gate="C" pin="IO_25" pad="C16"/>
<connect gate="C" pin="IO_26" pad="B16"/>
<connect gate="C" pin="IO_27" pad="C17"/>
<connect gate="C" pin="IO_28" pad="B17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="D14"/>
<connect gate="C" pin="IO_30" pad="B18"/>
<connect gate="C" pin="IO_31" pad="C19"/>
<connect gate="C" pin="IO_32" pad="B19"/>
<connect gate="C" pin="IO_33" pad="C20"/>
<connect gate="C" pin="IO_34" pad="B20"/>
<connect gate="C" pin="IO_35" pad="C10"/>
<connect gate="C" pin="IO_36" pad="C21"/>
<connect gate="C" pin="IO_37" pad="C22"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AB4"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="D11"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AB5"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G11"/>
<connect gate="C" pin="IO_62" pad="G16"/>
<connect gate="C" pin="IO_63" pad="G17"/>
<connect gate="C" pin="IO_64" pad="G18"/>
<connect gate="C" pin="IO_65" pad="G20"/>
<connect gate="C" pin="IO_66" pad="G21"/>
<connect gate="C" pin="IO_67" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AB6"/>
<connect gate="C" pin="IO_8" pad="AB7"/>
<connect gate="C" pin="IO_9" pad="AB8"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="G14"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="D17"/>
<connect gate="C" pin="VCCIO5" pad="B22"/>
<connect gate="C" pin="VCCIO5_2" pad="G19"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="N16"/>
<connect gate="D" pin="GND_10" pad="M10"/>
<connect gate="D" pin="GND_11" pad="N11"/>
<connect gate="D" pin="GND_12" pad="L13"/>
<connect gate="D" pin="GND_13" pad="N12"/>
<connect gate="D" pin="GND_14" pad="M11"/>
<connect gate="D" pin="GND_15" pad="N13"/>
<connect gate="D" pin="GND_16" pad="K19"/>
<connect gate="D" pin="GND_17" pad="M12"/>
<connect gate="D" pin="GND_18" pad="K13"/>
<connect gate="D" pin="GND_19" pad="M13"/>
<connect gate="D" pin="GND_2" pad="K10"/>
<connect gate="D" pin="GND_20" pad="N10"/>
<connect gate="D" pin="GND_21" pad="H20"/>
<connect gate="D" pin="GND_22" pad="K16"/>
<connect gate="D" pin="GND_23" pad="N19"/>
<connect gate="D" pin="GND_24" pad="R13"/>
<connect gate="D" pin="GND_3" pad="L10"/>
<connect gate="D" pin="GND_4" pad="K11"/>
<connect gate="D" pin="GND_5" pad="L11"/>
<connect gate="D" pin="GND_6" pad="K12"/>
<connect gate="D" pin="GND_7" pad="L12"/>
<connect gate="D" pin="GND_8" pad="K15"/>
<connect gate="D" pin="GND_9" pad="L15"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J18"/>
<connect gate="D" pin="IO_11" pad="H19"/>
<connect gate="D" pin="IO_12" pad="J19"/>
<connect gate="D" pin="IO_13" pad="K17"/>
<connect gate="D" pin="IO_14" pad="J20"/>
<connect gate="D" pin="IO_15" pad="K18"/>
<connect gate="D" pin="IO_16" pad="L17"/>
<connect gate="D" pin="IO_17" pad="H21"/>
<connect gate="D" pin="IO_18" pad="L18"/>
<connect gate="D" pin="IO_19" pad="J21"/>
<connect gate="D" pin="IO_2" pad="H14"/>
<connect gate="D" pin="IO_20" pad="L19"/>
<connect gate="D" pin="IO_21" pad="K20"/>
<connect gate="D" pin="IO_22" pad="H22"/>
<connect gate="D" pin="IO_23" pad="K21"/>
<connect gate="D" pin="IO_24" pad="J22"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="M15"/>
<connect gate="D" pin="IO_27" pad="M16"/>
<connect gate="D" pin="IO_28" pad="M18"/>
<connect gate="D" pin="IO_29" pad="M19"/>
<connect gate="D" pin="IO_3" pad="H15"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N21"/>
<connect gate="D" pin="IO_32" pad="N22"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P17"/>
<connect gate="D" pin="IO_35" pad="P18"/>
<connect gate="D" pin="IO_36" pad="P19"/>
<connect gate="D" pin="IO_37" pad="P20"/>
<connect gate="D" pin="IO_38" pad="P21"/>
<connect gate="D" pin="IO_39" pad="P22"/>
<connect gate="D" pin="IO_4" pad="J14"/>
<connect gate="D" pin="IO_40" pad="R11"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H16"/>
<connect gate="D" pin="IO_6" pad="J17"/>
<connect gate="D" pin="IO_7" pad="H17"/>
<connect gate="D" pin="IO_8" pad="J15"/>
<connect gate="D" pin="IO_9" pad="H18"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="L14"/>
<connect gate="D" pin="VCCINT_10" pad="J13"/>
<connect gate="D" pin="VCCINT_11" pad="L16"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="R10"/>
<connect gate="D" pin="VCCINT_14" pad="H12"/>
<connect gate="D" pin="VCCINT_15" pad="N14"/>
<connect gate="D" pin="VCCINT_16" pad="R12"/>
<connect gate="D" pin="VCCINT_17" pad="H13"/>
<connect gate="D" pin="VCCINT_18" pad="K14"/>
<connect gate="D" pin="VCCINT_2" pad="P10"/>
<connect gate="D" pin="VCCINT_3" pad="P11"/>
<connect gate="D" pin="VCCINT_4" pad="J10"/>
<connect gate="D" pin="VCCINT_5" pad="P12"/>
<connect gate="D" pin="VCCINT_6" pad="J11"/>
<connect gate="D" pin="VCCINT_7" pad="P13"/>
<connect gate="D" pin="VCCINT_8" pad="J12"/>
<connect gate="D" pin="VCCINT_9" pad="P14"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="P16"/>
<connect gate="D" pin="VCCIO6_2" pad="M20"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="T10"/>
<connect gate="E" pin="GND_2" pad="T20"/>
<connect gate="E" pin="GND_3" pad="W10"/>
<connect gate="E" pin="GND_4" pad="Y15"/>
<connect gate="E" pin="GND_5" pad="AA21"/>
<connect gate="E" pin="GND_6" pad="T13"/>
<connect gate="E" pin="GND_7" pad="V17"/>
<connect gate="E" pin="GND_8" pad="W19"/>
<connect gate="E" pin="GND_9" pad="W13"/>
<connect gate="E" pin="GND_PLL4" pad="T17"/>
<connect gate="E" pin="GND_PLL4_2" pad="V18"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="T21"/>
<connect gate="E" pin="IO_11" pad="T22"/>
<connect gate="E" pin="IO_12" pad="U10"/>
<connect gate="E" pin="IO_13" pad="U18"/>
<connect gate="E" pin="IO_14" pad="V14"/>
<connect gate="E" pin="IO_15" pad="U19"/>
<connect gate="E" pin="IO_16" pad="V15"/>
<connect gate="E" pin="IO_17" pad="U20"/>
<connect gate="E" pin="IO_18" pad="U13"/>
<connect gate="E" pin="IO_19" pad="U21"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="V20"/>
<connect gate="E" pin="IO_21" pad="U14"/>
<connect gate="E" pin="IO_22" pad="V21"/>
<connect gate="E" pin="IO_23" pad="U22"/>
<connect gate="E" pin="IO_24" pad="V19"/>
<connect gate="E" pin="IO_25" pad="V22"/>
<connect gate="E" pin="IO_26" pad="U15"/>
<connect gate="E" pin="IO_27" pad="V11"/>
<connect gate="E" pin="IO_28" pad="W11"/>
<connect gate="E" pin="IO_29" pad="W14"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="W15"/>
<connect gate="E" pin="IO_31" pad="W16"/>
<connect gate="E" pin="IO_32" pad="W18"/>
<connect gate="E" pin="IO_33" pad="W20"/>
<connect gate="E" pin="IO_34" pad="W21"/>
<connect gate="E" pin="IO_35" pad="W22"/>
<connect gate="E" pin="IO_36" pad="Y10"/>
<connect gate="E" pin="IO_37" pad="Y13"/>
<connect gate="E" pin="IO_38" pad="Y14"/>
<connect gate="E" pin="IO_39" pad="Y16"/>
<connect gate="E" pin="IO_4" pad="T16"/>
<connect gate="E" pin="IO_40" pad="Y17"/>
<connect gate="E" pin="IO_41" pad="Y18"/>
<connect gate="E" pin="IO_42" pad="Y19"/>
<connect gate="E" pin="IO_43" pad="Y20"/>
<connect gate="E" pin="IO_44" pad="Y21"/>
<connect gate="E" pin="IO_45" pad="Y22"/>
<connect gate="E" pin="IO_46" pad="AA10"/>
<connect gate="E" pin="IO_47" pad="AA11"/>
<connect gate="E" pin="IO_48" pad="AA12"/>
<connect gate="E" pin="IO_49" pad="AA13"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="AA14"/>
<connect gate="E" pin="IO_51" pad="AA15"/>
<connect gate="E" pin="IO_52" pad="AA16"/>
<connect gate="E" pin="IO_53" pad="AA17"/>
<connect gate="E" pin="IO_54" pad="AA18"/>
<connect gate="E" pin="IO_55" pad="AA19"/>
<connect gate="E" pin="IO_56" pad="AA20"/>
<connect gate="E" pin="IO_57" pad="AB10"/>
<connect gate="E" pin="IO_58" pad="AB11"/>
<connect gate="E" pin="IO_59" pad="AB12"/>
<connect gate="E" pin="IO_6" pad="R20"/>
<connect gate="E" pin="IO_60" pad="AB13"/>
<connect gate="E" pin="IO_61" pad="AB14"/>
<connect gate="E" pin="IO_62" pad="AB15"/>
<connect gate="E" pin="IO_63" pad="AB16"/>
<connect gate="E" pin="IO_64" pad="AB17"/>
<connect gate="E" pin="IO_65" pad="AB18"/>
<connect gate="E" pin="IO_66" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="T18"/>
<connect gate="E" pin="IO_8" pad="R21"/>
<connect gate="E" pin="IO_9" pad="T11"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="AA22"/>
<connect gate="E" pin="VCCIO6_2" pad="T19"/>
<connect gate="E" pin="VCCIO7" pad="AB21"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="W17"/>
<connect gate="E" pin="VCCIO7_4" pad="Y12"/>
<connect gate="E" pin="VCCIO7_5" pad="V13"/>
<connect gate="E" pin="VCCIO8" pad="V10"/>
<connect gate="E" pin="VCCIO8_2" pad="Y11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C35U484C8N"/>
<attribute name="OC_FARNELL" value="1635085"/>
<attribute name="OC_NEWARK" value="51R0565"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C35U484I8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C35U484I8N_A"/>
<gate name="B" symbol="EP2C35U484I8N_B"/>
<gate name="C" symbol="EP2C35U484I8N_C"/>
<gate name="D" symbol="EP2C35U484I8N_D"/>
<gate name="E" symbol="EP2C35U484I8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C80P22X22_1900X1900X220">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K7"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="J9"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="C5"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="GND_6" pad="G4"/>
<connect gate="A" pin="GND_7" pad="K3"/>
<connect gate="A" pin="GND_8" pad="H9"/>
<connect gate="A" pin="GND_9" pad="J8"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="C9"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="D1"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="D2"/>
<connect gate="A" pin="IO_15" pad="A5"/>
<connect gate="A" pin="IO_16" pad="D3"/>
<connect gate="A" pin="IO_17" pad="B9"/>
<connect gate="A" pin="IO_18" pad="D4"/>
<connect gate="A" pin="IO_19" pad="A6"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="D5"/>
<connect gate="A" pin="IO_21" pad="C1"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="A7"/>
<connect gate="A" pin="IO_24" pad="D7"/>
<connect gate="A" pin="IO_25" pad="C2"/>
<connect gate="A" pin="IO_26" pad="D8"/>
<connect gate="A" pin="IO_27" pad="A8"/>
<connect gate="A" pin="IO_28" pad="D9"/>
<connect gate="A" pin="IO_29" pad="C3"/>
<connect gate="A" pin="IO_3" pad="C4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E7"/>
<connect gate="A" pin="IO_34" pad="E3"/>
<connect gate="A" pin="IO_35" pad="E8"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="B4"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="G7"/>
<connect gate="A" pin="IO_5" pad="B5"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="J1"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_60" pad="J4"/>
<connect gate="A" pin="IO_61" pad="J5"/>
<connect gate="A" pin="IO_62" pad="L7"/>
<connect gate="A" pin="IO_7" pad="C7"/>
<connect gate="A" pin="IO_8" pad="A3"/>
<connect gate="A" pin="IO_9" pad="B7"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="G8"/>
<connect gate="A" pin="VCCINT_3" pad="K8"/>
<connect gate="A" pin="VCCINT_4" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="J7"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="L3"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="R3"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V6"/>
<connect gate="B" pin="GND_11" pad="V3"/>
<connect gate="B" pin="GND_2" pad="M4"/>
<connect gate="B" pin="GND_3" pad="Y8"/>
<connect gate="B" pin="GND_4" pad="P8"/>
<connect gate="B" pin="GND_5" pad="R9"/>
<connect gate="B" pin="GND_6" pad="N7"/>
<connect gate="B" pin="GND_7" pad="A22"/>
<connect gate="B" pin="GND_8" pad="P9"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GND_PLL1" pad="U5"/>
<connect gate="B" pin="GND_PLL1_2" pad="V5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="R5"/>
<connect gate="B" pin="IO_11" pad="N3"/>
<connect gate="B" pin="IO_12" pad="R6"/>
<connect gate="B" pin="IO_13" pad="N4"/>
<connect gate="B" pin="IO_14" pad="R7"/>
<connect gate="B" pin="IO_15" pad="N5"/>
<connect gate="B" pin="IO_16" pad="R8"/>
<connect gate="B" pin="IO_17" pad="U1"/>
<connect gate="B" pin="IO_18" pad="N6"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="M5"/>
<connect gate="B" pin="IO_20" pad="P1"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="P2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="P3"/>
<connect gate="B" pin="IO_25" pad="P4"/>
<connect gate="B" pin="IO_26" pad="P5"/>
<connect gate="B" pin="IO_27" pad="P6"/>
<connect gate="B" pin="IO_28" pad="T5"/>
<connect gate="B" pin="IO_29" pad="T6"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="T7"/>
<connect gate="B" pin="IO_31" pad="R1"/>
<connect gate="B" pin="IO_32" pad="T8"/>
<connect gate="B" pin="IO_33" pad="R2"/>
<connect gate="B" pin="IO_34" pad="U2"/>
<connect gate="B" pin="IO_35" pad="U3"/>
<connect gate="B" pin="IO_36" pad="U4"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="L8"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V8"/>
<connect gate="B" pin="IO_43" pad="V9"/>
<connect gate="B" pin="IO_44" pad="W1"/>
<connect gate="B" pin="IO_45" pad="W2"/>
<connect gate="B" pin="IO_46" pad="W3"/>
<connect gate="B" pin="IO_47" pad="W4"/>
<connect gate="B" pin="IO_48" pad="W5"/>
<connect gate="B" pin="IO_49" pad="W7"/>
<connect gate="B" pin="IO_5" pad="M7"/>
<connect gate="B" pin="IO_50" pad="W8"/>
<connect gate="B" pin="IO_51" pad="W9"/>
<connect gate="B" pin="IO_52" pad="Y1"/>
<connect gate="B" pin="IO_53" pad="Y2"/>
<connect gate="B" pin="IO_54" pad="Y3"/>
<connect gate="B" pin="IO_55" pad="Y4"/>
<connect gate="B" pin="IO_56" pad="Y5"/>
<connect gate="B" pin="IO_57" pad="Y6"/>
<connect gate="B" pin="IO_58" pad="Y7"/>
<connect gate="B" pin="IO_59" pad="Y9"/>
<connect gate="B" pin="IO_6" pad="M8"/>
<connect gate="B" pin="IO_60" pad="A10"/>
<connect gate="B" pin="IO_61" pad="A11"/>
<connect gate="B" pin="IO_62" pad="A13"/>
<connect gate="B" pin="IO_63" pad="A14"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_68" pad="A19"/>
<connect gate="B" pin="IO_7" pad="N1"/>
<connect gate="B" pin="IO_8" pad="R4"/>
<connect gate="B" pin="IO_9" pad="N2"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="N9"/>
<connect gate="B" pin="VCCINT_2" pad="L9"/>
<connect gate="B" pin="VCCINT_3" pad="M9"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="P7"/>
<connect gate="B" pin="VCCIO1_3" pad="T4"/>
<connect gate="B" pin="VCCIO1_4" pad="M3"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="T9"/>
<connect gate="B" pin="VCCIO8_2" pad="W6"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="H10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="C15"/>
<connect gate="C" pin="GND_11" pad="G15"/>
<connect gate="C" pin="GND_12" pad="G13"/>
<connect gate="C" pin="GND_2" pad="AB1"/>
<connect gate="C" pin="GND_3" pad="D10"/>
<connect gate="C" pin="GND_4" pad="D18"/>
<connect gate="C" pin="GND_5" pad="D13"/>
<connect gate="C" pin="GND_6" pad="F19"/>
<connect gate="C" pin="GND_7" pad="AA2"/>
<connect gate="C" pin="GND_8" pad="G10"/>
<connect gate="C" pin="GND_9" pad="B21"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="C13"/>
<connect gate="C" pin="IO_11" pad="AA3"/>
<connect gate="C" pin="IO_12" pad="AB9"/>
<connect gate="C" pin="IO_13" pad="AA4"/>
<connect gate="C" pin="IO_14" pad="B10"/>
<connect gate="C" pin="IO_15" pad="AA5"/>
<connect gate="C" pin="IO_16" pad="B11"/>
<connect gate="C" pin="IO_17" pad="AA6"/>
<connect gate="C" pin="IO_18" pad="AA7"/>
<connect gate="C" pin="IO_19" pad="B13"/>
<connect gate="C" pin="IO_2" pad="AB3"/>
<connect gate="C" pin="IO_20" pad="AA8"/>
<connect gate="C" pin="IO_21" pad="B14"/>
<connect gate="C" pin="IO_22" pad="C14"/>
<connect gate="C" pin="IO_23" pad="AA9"/>
<connect gate="C" pin="IO_24" pad="B15"/>
<connect gate="C" pin="IO_25" pad="C16"/>
<connect gate="C" pin="IO_26" pad="B16"/>
<connect gate="C" pin="IO_27" pad="C17"/>
<connect gate="C" pin="IO_28" pad="B17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="D14"/>
<connect gate="C" pin="IO_30" pad="B18"/>
<connect gate="C" pin="IO_31" pad="C19"/>
<connect gate="C" pin="IO_32" pad="B19"/>
<connect gate="C" pin="IO_33" pad="C20"/>
<connect gate="C" pin="IO_34" pad="B20"/>
<connect gate="C" pin="IO_35" pad="C10"/>
<connect gate="C" pin="IO_36" pad="C21"/>
<connect gate="C" pin="IO_37" pad="C22"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AB4"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="D11"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AB5"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G11"/>
<connect gate="C" pin="IO_62" pad="G16"/>
<connect gate="C" pin="IO_63" pad="G17"/>
<connect gate="C" pin="IO_64" pad="G18"/>
<connect gate="C" pin="IO_65" pad="G20"/>
<connect gate="C" pin="IO_66" pad="G21"/>
<connect gate="C" pin="IO_67" pad="G22"/>
<connect gate="C" pin="IO_7" pad="AB6"/>
<connect gate="C" pin="IO_8" pad="AB7"/>
<connect gate="C" pin="IO_9" pad="AB8"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="G14"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="D17"/>
<connect gate="C" pin="VCCIO5" pad="B22"/>
<connect gate="C" pin="VCCIO5_2" pad="G19"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="N16"/>
<connect gate="D" pin="GND_10" pad="M10"/>
<connect gate="D" pin="GND_11" pad="N11"/>
<connect gate="D" pin="GND_12" pad="L13"/>
<connect gate="D" pin="GND_13" pad="N12"/>
<connect gate="D" pin="GND_14" pad="M11"/>
<connect gate="D" pin="GND_15" pad="N13"/>
<connect gate="D" pin="GND_16" pad="K19"/>
<connect gate="D" pin="GND_17" pad="M12"/>
<connect gate="D" pin="GND_18" pad="K13"/>
<connect gate="D" pin="GND_19" pad="M13"/>
<connect gate="D" pin="GND_2" pad="K10"/>
<connect gate="D" pin="GND_20" pad="N10"/>
<connect gate="D" pin="GND_21" pad="H20"/>
<connect gate="D" pin="GND_22" pad="K16"/>
<connect gate="D" pin="GND_23" pad="N19"/>
<connect gate="D" pin="GND_24" pad="R13"/>
<connect gate="D" pin="GND_3" pad="L10"/>
<connect gate="D" pin="GND_4" pad="K11"/>
<connect gate="D" pin="GND_5" pad="L11"/>
<connect gate="D" pin="GND_6" pad="K12"/>
<connect gate="D" pin="GND_7" pad="L12"/>
<connect gate="D" pin="GND_8" pad="K15"/>
<connect gate="D" pin="GND_9" pad="L15"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J18"/>
<connect gate="D" pin="IO_11" pad="H19"/>
<connect gate="D" pin="IO_12" pad="J19"/>
<connect gate="D" pin="IO_13" pad="K17"/>
<connect gate="D" pin="IO_14" pad="J20"/>
<connect gate="D" pin="IO_15" pad="K18"/>
<connect gate="D" pin="IO_16" pad="L17"/>
<connect gate="D" pin="IO_17" pad="H21"/>
<connect gate="D" pin="IO_18" pad="L18"/>
<connect gate="D" pin="IO_19" pad="J21"/>
<connect gate="D" pin="IO_2" pad="H14"/>
<connect gate="D" pin="IO_20" pad="L19"/>
<connect gate="D" pin="IO_21" pad="K20"/>
<connect gate="D" pin="IO_22" pad="H22"/>
<connect gate="D" pin="IO_23" pad="K21"/>
<connect gate="D" pin="IO_24" pad="J22"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="M15"/>
<connect gate="D" pin="IO_27" pad="M16"/>
<connect gate="D" pin="IO_28" pad="M18"/>
<connect gate="D" pin="IO_29" pad="M19"/>
<connect gate="D" pin="IO_3" pad="H15"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N21"/>
<connect gate="D" pin="IO_32" pad="N22"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P17"/>
<connect gate="D" pin="IO_35" pad="P18"/>
<connect gate="D" pin="IO_36" pad="P19"/>
<connect gate="D" pin="IO_37" pad="P20"/>
<connect gate="D" pin="IO_38" pad="P21"/>
<connect gate="D" pin="IO_39" pad="P22"/>
<connect gate="D" pin="IO_4" pad="J14"/>
<connect gate="D" pin="IO_40" pad="R11"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H16"/>
<connect gate="D" pin="IO_6" pad="J17"/>
<connect gate="D" pin="IO_7" pad="H17"/>
<connect gate="D" pin="IO_8" pad="J15"/>
<connect gate="D" pin="IO_9" pad="H18"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="L14"/>
<connect gate="D" pin="VCCINT_10" pad="J13"/>
<connect gate="D" pin="VCCINT_11" pad="L16"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="R10"/>
<connect gate="D" pin="VCCINT_14" pad="H12"/>
<connect gate="D" pin="VCCINT_15" pad="N14"/>
<connect gate="D" pin="VCCINT_16" pad="R12"/>
<connect gate="D" pin="VCCINT_17" pad="H13"/>
<connect gate="D" pin="VCCINT_18" pad="K14"/>
<connect gate="D" pin="VCCINT_2" pad="P10"/>
<connect gate="D" pin="VCCINT_3" pad="P11"/>
<connect gate="D" pin="VCCINT_4" pad="J10"/>
<connect gate="D" pin="VCCINT_5" pad="P12"/>
<connect gate="D" pin="VCCINT_6" pad="J11"/>
<connect gate="D" pin="VCCINT_7" pad="P13"/>
<connect gate="D" pin="VCCINT_8" pad="J12"/>
<connect gate="D" pin="VCCINT_9" pad="P14"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="P16"/>
<connect gate="D" pin="VCCIO6_2" pad="M20"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="T10"/>
<connect gate="E" pin="GND_2" pad="T20"/>
<connect gate="E" pin="GND_3" pad="W10"/>
<connect gate="E" pin="GND_4" pad="Y15"/>
<connect gate="E" pin="GND_5" pad="AA21"/>
<connect gate="E" pin="GND_6" pad="T13"/>
<connect gate="E" pin="GND_7" pad="V17"/>
<connect gate="E" pin="GND_8" pad="W19"/>
<connect gate="E" pin="GND_9" pad="W13"/>
<connect gate="E" pin="GND_PLL4" pad="T17"/>
<connect gate="E" pin="GND_PLL4_2" pad="V18"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="T21"/>
<connect gate="E" pin="IO_11" pad="T22"/>
<connect gate="E" pin="IO_12" pad="U10"/>
<connect gate="E" pin="IO_13" pad="U18"/>
<connect gate="E" pin="IO_14" pad="V14"/>
<connect gate="E" pin="IO_15" pad="U19"/>
<connect gate="E" pin="IO_16" pad="V15"/>
<connect gate="E" pin="IO_17" pad="U20"/>
<connect gate="E" pin="IO_18" pad="U13"/>
<connect gate="E" pin="IO_19" pad="U21"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="V20"/>
<connect gate="E" pin="IO_21" pad="U14"/>
<connect gate="E" pin="IO_22" pad="V21"/>
<connect gate="E" pin="IO_23" pad="U22"/>
<connect gate="E" pin="IO_24" pad="V19"/>
<connect gate="E" pin="IO_25" pad="V22"/>
<connect gate="E" pin="IO_26" pad="U15"/>
<connect gate="E" pin="IO_27" pad="V11"/>
<connect gate="E" pin="IO_28" pad="W11"/>
<connect gate="E" pin="IO_29" pad="W14"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="W15"/>
<connect gate="E" pin="IO_31" pad="W16"/>
<connect gate="E" pin="IO_32" pad="W18"/>
<connect gate="E" pin="IO_33" pad="W20"/>
<connect gate="E" pin="IO_34" pad="W21"/>
<connect gate="E" pin="IO_35" pad="W22"/>
<connect gate="E" pin="IO_36" pad="Y10"/>
<connect gate="E" pin="IO_37" pad="Y13"/>
<connect gate="E" pin="IO_38" pad="Y14"/>
<connect gate="E" pin="IO_39" pad="Y16"/>
<connect gate="E" pin="IO_4" pad="T16"/>
<connect gate="E" pin="IO_40" pad="Y17"/>
<connect gate="E" pin="IO_41" pad="Y18"/>
<connect gate="E" pin="IO_42" pad="Y19"/>
<connect gate="E" pin="IO_43" pad="Y20"/>
<connect gate="E" pin="IO_44" pad="Y21"/>
<connect gate="E" pin="IO_45" pad="Y22"/>
<connect gate="E" pin="IO_46" pad="AA10"/>
<connect gate="E" pin="IO_47" pad="AA11"/>
<connect gate="E" pin="IO_48" pad="AA12"/>
<connect gate="E" pin="IO_49" pad="AA13"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="AA14"/>
<connect gate="E" pin="IO_51" pad="AA15"/>
<connect gate="E" pin="IO_52" pad="AA16"/>
<connect gate="E" pin="IO_53" pad="AA17"/>
<connect gate="E" pin="IO_54" pad="AA18"/>
<connect gate="E" pin="IO_55" pad="AA19"/>
<connect gate="E" pin="IO_56" pad="AA20"/>
<connect gate="E" pin="IO_57" pad="AB10"/>
<connect gate="E" pin="IO_58" pad="AB11"/>
<connect gate="E" pin="IO_59" pad="AB12"/>
<connect gate="E" pin="IO_6" pad="R20"/>
<connect gate="E" pin="IO_60" pad="AB13"/>
<connect gate="E" pin="IO_61" pad="AB14"/>
<connect gate="E" pin="IO_62" pad="AB15"/>
<connect gate="E" pin="IO_63" pad="AB16"/>
<connect gate="E" pin="IO_64" pad="AB17"/>
<connect gate="E" pin="IO_65" pad="AB18"/>
<connect gate="E" pin="IO_66" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="T18"/>
<connect gate="E" pin="IO_8" pad="R21"/>
<connect gate="E" pin="IO_9" pad="T11"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="AA22"/>
<connect gate="E" pin="VCCIO6_2" pad="T19"/>
<connect gate="E" pin="VCCIO7" pad="AB21"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="W17"/>
<connect gate="E" pin="VCCIO7_4" pad="Y12"/>
<connect gate="E" pin="VCCIO7_5" pad="V13"/>
<connect gate="E" pin="VCCIO8" pad="V10"/>
<connect gate="E" pin="VCCIO8_2" pad="Y11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C35U484I8N"/>
<attribute name="OC_FARNELL" value="1549357"/>
<attribute name="OC_NEWARK" value="52R0536"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C50F484C8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C50F484C8N_A"/>
<gate name="B" symbol="EP2C50F484C8N_B"/>
<gate name="C" symbol="EP2C50F484C8N_C"/>
<gate name="D" symbol="EP2C50F484C8N_D"/>
<gate name="E" symbol="EP2C50F484C8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K3"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="C5"/>
<connect gate="A" pin="GND_2" pad="J8"/>
<connect gate="A" pin="GND_3" pad="A1"/>
<connect gate="A" pin="GND_4" pad="G4"/>
<connect gate="A" pin="GND_5" pad="J9"/>
<connect gate="A" pin="GND_6" pad="B2"/>
<connect gate="A" pin="GND_7" pad="C8"/>
<connect gate="A" pin="GND_8" pad="K7"/>
<connect gate="A" pin="GND_9" pad="H9"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="C7"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="C9"/>
<connect gate="A" pin="IO_15" pad="B7"/>
<connect gate="A" pin="IO_16" pad="D1"/>
<connect gate="A" pin="IO_17" pad="B8"/>
<connect gate="A" pin="IO_18" pad="D2"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="D3"/>
<connect gate="A" pin="IO_21" pad="C1"/>
<connect gate="A" pin="IO_22" pad="D4"/>
<connect gate="A" pin="IO_23" pad="C2"/>
<connect gate="A" pin="IO_24" pad="D5"/>
<connect gate="A" pin="IO_25" pad="C3"/>
<connect gate="A" pin="IO_26" pad="D6"/>
<connect gate="A" pin="IO_27" pad="C4"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A3"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E1"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E7"/>
<connect gate="A" pin="IO_34" pad="E3"/>
<connect gate="A" pin="IO_35" pad="E8"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="H1"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="H2"/>
<connect gate="A" pin="IO_51" pad="H3"/>
<connect gate="A" pin="IO_52" pad="H4"/>
<connect gate="A" pin="IO_53" pad="H5"/>
<connect gate="A" pin="IO_54" pad="H6"/>
<connect gate="A" pin="IO_55" pad="J1"/>
<connect gate="A" pin="IO_56" pad="J2"/>
<connect gate="A" pin="IO_57" pad="J3"/>
<connect gate="A" pin="IO_58" pad="J4"/>
<connect gate="A" pin="IO_59" pad="J5"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="G7"/>
<connect gate="A" pin="VCCINT_3" pad="G8"/>
<connect gate="A" pin="VCCINT_4" pad="L7"/>
<connect gate="A" pin="VCCINT_5" pad="H7"/>
<connect gate="A" pin="VCCINT_6" pad="K8"/>
<connect gate="A" pin="VCCINT_7" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="J7"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="L3"/>
<connect gate="A" pin="VCCIO3" pad="A2"/>
<connect gate="A" pin="VCCIO3_2" pad="G9"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="N8"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V3"/>
<connect gate="B" pin="GND_11" pad="Y8"/>
<connect gate="B" pin="GND_12" pad="M7"/>
<connect gate="B" pin="GND_13" pad="N7"/>
<connect gate="B" pin="GND_2" pad="P9"/>
<connect gate="B" pin="GND_3" pad="P8"/>
<connect gate="B" pin="GND_4" pad="R9"/>
<connect gate="B" pin="GND_5" pad="A22"/>
<connect gate="B" pin="GND_6" pad="M4"/>
<connect gate="B" pin="GND_7" pad="R3"/>
<connect gate="B" pin="GND_8" pad="V6"/>
<connect gate="B" pin="GND_9" pad="M8"/>
<connect gate="B" pin="GND_PLL1" pad="V5"/>
<connect gate="B" pin="GND_PLL1_2" pad="U5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="N4"/>
<connect gate="B" pin="IO_11" pad="N5"/>
<connect gate="B" pin="IO_12" pad="R2"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="R4"/>
<connect gate="B" pin="IO_15" pad="R5"/>
<connect gate="B" pin="IO_16" pad="R6"/>
<connect gate="B" pin="IO_17" pad="P1"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="U1"/>
<connect gate="B" pin="IO_20" pad="R1"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="P3"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="P4"/>
<connect gate="B" pin="IO_25" pad="P5"/>
<connect gate="B" pin="IO_26" pad="P6"/>
<connect gate="B" pin="IO_27" pad="U2"/>
<connect gate="B" pin="IO_28" pad="U3"/>
<connect gate="B" pin="IO_29" pad="U4"/>
<connect gate="B" pin="IO_3" pad="M5"/>
<connect gate="B" pin="IO_30" pad="U8"/>
<connect gate="B" pin="IO_31" pad="U9"/>
<connect gate="B" pin="IO_32" pad="V1"/>
<connect gate="B" pin="IO_33" pad="V2"/>
<connect gate="B" pin="IO_34" pad="V4"/>
<connect gate="B" pin="IO_35" pad="V8"/>
<connect gate="B" pin="IO_36" pad="V9"/>
<connect gate="B" pin="IO_37" pad="W1"/>
<connect gate="B" pin="IO_38" pad="W2"/>
<connect gate="B" pin="IO_39" pad="W3"/>
<connect gate="B" pin="IO_4" pad="M6"/>
<connect gate="B" pin="IO_40" pad="W4"/>
<connect gate="B" pin="IO_41" pad="W5"/>
<connect gate="B" pin="IO_42" pad="W7"/>
<connect gate="B" pin="IO_43" pad="W8"/>
<connect gate="B" pin="IO_44" pad="W9"/>
<connect gate="B" pin="IO_45" pad="Y1"/>
<connect gate="B" pin="IO_46" pad="Y2"/>
<connect gate="B" pin="IO_47" pad="Y3"/>
<connect gate="B" pin="IO_48" pad="Y4"/>
<connect gate="B" pin="IO_49" pad="Y5"/>
<connect gate="B" pin="IO_5" pad="T5"/>
<connect gate="B" pin="IO_50" pad="Y6"/>
<connect gate="B" pin="IO_51" pad="Y7"/>
<connect gate="B" pin="IO_52" pad="Y9"/>
<connect gate="B" pin="IO_53" pad="A10"/>
<connect gate="B" pin="IO_54" pad="A11"/>
<connect gate="B" pin="IO_55" pad="A13"/>
<connect gate="B" pin="IO_56" pad="A14"/>
<connect gate="B" pin="IO_57" pad="A15"/>
<connect gate="B" pin="IO_58" pad="A16"/>
<connect gate="B" pin="IO_59" pad="A17"/>
<connect gate="B" pin="IO_6" pad="N1"/>
<connect gate="B" pin="IO_60" pad="A18"/>
<connect gate="B" pin="IO_61" pad="A19"/>
<connect gate="B" pin="IO_7" pad="T6"/>
<connect gate="B" pin="IO_8" pad="N2"/>
<connect gate="B" pin="IO_9" pad="N3"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="L9"/>
<connect gate="B" pin="VCCINT_2" pad="M9"/>
<connect gate="B" pin="VCCINT_3" pad="L8"/>
<connect gate="B" pin="VCCINT_4" pad="T7"/>
<connect gate="B" pin="VCCINT_5" pad="N9"/>
<connect gate="B" pin="VCCINT_6" pad="R7"/>
<connect gate="B" pin="VCCINT_7" pad="R8"/>
<connect gate="B" pin="VCCINT_8" pad="T8"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="M3"/>
<connect gate="B" pin="VCCIO1_3" pad="P7"/>
<connect gate="B" pin="VCCIO1_4" pad="T4"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="W6"/>
<connect gate="B" pin="VCCIO8_2" pad="T9"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="D10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="G13"/>
<connect gate="C" pin="GND_11" pad="AA2"/>
<connect gate="C" pin="GND_12" pad="C15"/>
<connect gate="C" pin="GND_13" pad="AB1"/>
<connect gate="C" pin="GND_14" pad="D18"/>
<connect gate="C" pin="GND_2" pad="F19"/>
<connect gate="C" pin="GND_3" pad="B21"/>
<connect gate="C" pin="GND_4" pad="G15"/>
<connect gate="C" pin="GND_5" pad="G10"/>
<connect gate="C" pin="GND_6" pad="H10"/>
<connect gate="C" pin="GND_7" pad="D13"/>
<connect gate="C" pin="GND_8" pad="H11"/>
<connect gate="C" pin="GND_9" pad="G11"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="G22"/>
<connect gate="C" pin="IO_10" pad="B20"/>
<connect gate="C" pin="IO_11" pad="D11"/>
<connect gate="C" pin="IO_12" pad="C13"/>
<connect gate="C" pin="IO_13" pad="AB3"/>
<connect gate="C" pin="IO_14" pad="C10"/>
<connect gate="C" pin="IO_15" pad="AB4"/>
<connect gate="C" pin="IO_16" pad="C14"/>
<connect gate="C" pin="IO_17" pad="D14"/>
<connect gate="C" pin="IO_18" pad="AB5"/>
<connect gate="C" pin="IO_19" pad="AB6"/>
<connect gate="C" pin="IO_2" pad="AA3"/>
<connect gate="C" pin="IO_20" pad="AB7"/>
<connect gate="C" pin="IO_21" pad="AB8"/>
<connect gate="C" pin="IO_22" pad="AB9"/>
<connect gate="C" pin="IO_23" pad="B10"/>
<connect gate="C" pin="IO_24" pad="B11"/>
<connect gate="C" pin="IO_25" pad="C16"/>
<connect gate="C" pin="IO_26" pad="C17"/>
<connect gate="C" pin="IO_27" pad="B13"/>
<connect gate="C" pin="IO_28" pad="C18"/>
<connect gate="C" pin="IO_29" pad="B14"/>
<connect gate="C" pin="IO_3" pad="AA4"/>
<connect gate="C" pin="IO_30" pad="C19"/>
<connect gate="C" pin="IO_31" pad="B15"/>
<connect gate="C" pin="IO_32" pad="C20"/>
<connect gate="C" pin="IO_33" pad="B16"/>
<connect gate="C" pin="IO_34" pad="C21"/>
<connect gate="C" pin="IO_35" pad="B17"/>
<connect gate="C" pin="IO_36" pad="B18"/>
<connect gate="C" pin="IO_37" pad="B19"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AA5"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="AA6"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AA7"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G17"/>
<connect gate="C" pin="IO_62" pad="G18"/>
<connect gate="C" pin="IO_63" pad="G20"/>
<connect gate="C" pin="IO_64" pad="G21"/>
<connect gate="C" pin="IO_7" pad="AA8"/>
<connect gate="C" pin="IO_8" pad="C22"/>
<connect gate="C" pin="IO_9" pad="AA9"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G16"/>
<connect gate="C" pin="VCCINT_2" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="G14"/>
<connect gate="C" pin="VCCIO4_2" pad="D17"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="E13"/>
<connect gate="C" pin="VCCIO5" pad="G19"/>
<connect gate="C" pin="VCCIO5_2" pad="B22"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="H15"/>
<connect gate="D" pin="GND_10" pad="K16"/>
<connect gate="D" pin="GND_11" pad="L15"/>
<connect gate="D" pin="GND_12" pad="N10"/>
<connect gate="D" pin="GND_13" pad="K12"/>
<connect gate="D" pin="GND_14" pad="M13"/>
<connect gate="D" pin="GND_15" pad="K13"/>
<connect gate="D" pin="GND_16" pad="N11"/>
<connect gate="D" pin="GND_17" pad="J14"/>
<connect gate="D" pin="GND_18" pad="L10"/>
<connect gate="D" pin="GND_19" pad="L11"/>
<connect gate="D" pin="GND_2" pad="K19"/>
<connect gate="D" pin="GND_20" pad="N12"/>
<connect gate="D" pin="GND_21" pad="J15"/>
<connect gate="D" pin="GND_22" pad="L12"/>
<connect gate="D" pin="GND_23" pad="L13"/>
<connect gate="D" pin="GND_24" pad="N13"/>
<connect gate="D" pin="GND_25" pad="N19"/>
<connect gate="D" pin="GND_26" pad="N16"/>
<connect gate="D" pin="GND_27" pad="P15"/>
<connect gate="D" pin="GND_28" pad="R11"/>
<connect gate="D" pin="GND_29" pad="R13"/>
<connect gate="D" pin="GND_3" pad="M10"/>
<connect gate="D" pin="GND_30" pad="H14"/>
<connect gate="D" pin="GND_31" pad="R14"/>
<connect gate="D" pin="GND_32" pad="H20"/>
<connect gate="D" pin="GND_4" pad="M11"/>
<connect gate="D" pin="GND_5" pad="K10"/>
<connect gate="D" pin="GND_6" pad="M16"/>
<connect gate="D" pin="GND_7" pad="M12"/>
<connect gate="D" pin="GND_8" pad="K11"/>
<connect gate="D" pin="GND_9" pad="K15"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="K17"/>
<connect gate="D" pin="IO_11" pad="H22"/>
<connect gate="D" pin="IO_12" pad="K18"/>
<connect gate="D" pin="IO_13" pad="J21"/>
<connect gate="D" pin="IO_14" pad="J22"/>
<connect gate="D" pin="IO_15" pad="L17"/>
<connect gate="D" pin="IO_16" pad="K20"/>
<connect gate="D" pin="IO_17" pad="L18"/>
<connect gate="D" pin="IO_18" pad="K21"/>
<connect gate="D" pin="IO_19" pad="L19"/>
<connect gate="D" pin="IO_2" pad="H17"/>
<connect gate="D" pin="IO_20" pad="K22"/>
<connect gate="D" pin="IO_21" pad="M18"/>
<connect gate="D" pin="IO_22" pad="M19"/>
<connect gate="D" pin="IO_23" pad="N21"/>
<connect gate="D" pin="IO_24" pad="N22"/>
<connect gate="D" pin="IO_25" pad="P17"/>
<connect gate="D" pin="IO_26" pad="P18"/>
<connect gate="D" pin="IO_27" pad="P19"/>
<connect gate="D" pin="IO_28" pad="P20"/>
<connect gate="D" pin="IO_29" pad="P21"/>
<connect gate="D" pin="IO_3" pad="H18"/>
<connect gate="D" pin="IO_30" pad="P22"/>
<connect gate="D" pin="IO_4" pad="J17"/>
<connect gate="D" pin="IO_5" pad="H19"/>
<connect gate="D" pin="IO_6" pad="J18"/>
<connect gate="D" pin="IO_7" pad="J19"/>
<connect gate="D" pin="IO_8" pad="H21"/>
<connect gate="D" pin="IO_9" pad="J20"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="N15"/>
<connect gate="D" pin="VCCINT_10" pad="P11"/>
<connect gate="D" pin="VCCINT_11" pad="J13"/>
<connect gate="D" pin="VCCINT_12" pad="P12"/>
<connect gate="D" pin="VCCINT_13" pad="R10"/>
<connect gate="D" pin="VCCINT_14" pad="P13"/>
<connect gate="D" pin="VCCINT_15" pad="R12"/>
<connect gate="D" pin="VCCINT_16" pad="L14"/>
<connect gate="D" pin="VCCINT_17" pad="K14"/>
<connect gate="D" pin="VCCINT_18" pad="L16"/>
<connect gate="D" pin="VCCINT_19" pad="P14"/>
<connect gate="D" pin="VCCINT_2" pad="H16"/>
<connect gate="D" pin="VCCINT_20" pad="M14"/>
<connect gate="D" pin="VCCINT_21" pad="R16"/>
<connect gate="D" pin="VCCINT_22" pad="M15"/>
<connect gate="D" pin="VCCINT_23" pad="N14"/>
<connect gate="D" pin="VCCINT_3" pad="H12"/>
<connect gate="D" pin="VCCINT_4" pad="P10"/>
<connect gate="D" pin="VCCINT_5" pad="J10"/>
<connect gate="D" pin="VCCINT_6" pad="R15"/>
<connect gate="D" pin="VCCINT_7" pad="H13"/>
<connect gate="D" pin="VCCINT_8" pad="J11"/>
<connect gate="D" pin="VCCINT_9" pad="J12"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="M20"/>
<connect gate="D" pin="VCCIO6_2" pad="P16"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="W19"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="T11"/>
<connect gate="E" pin="GND_11" pad="V17"/>
<connect gate="E" pin="GND_12" pad="T16"/>
<connect gate="E" pin="GND_2" pad="Y15"/>
<connect gate="E" pin="GND_3" pad="AA21"/>
<connect gate="E" pin="GND_4" pad="T20"/>
<connect gate="E" pin="GND_5" pad="AB22"/>
<connect gate="E" pin="GND_6" pad="T10"/>
<connect gate="E" pin="GND_7" pad="W13"/>
<connect gate="E" pin="GND_8" pad="T13"/>
<connect gate="E" pin="GND_9" pad="W10"/>
<connect gate="E" pin="GND_PLL4" pad="T17"/>
<connect gate="E" pin="GND_PLL4_2" pad="V18"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="U22"/>
<connect gate="E" pin="IO_11" pad="R21"/>
<connect gate="E" pin="IO_12" pad="U14"/>
<connect gate="E" pin="IO_13" pad="T21"/>
<connect gate="E" pin="IO_14" pad="V14"/>
<connect gate="E" pin="IO_15" pad="V11"/>
<connect gate="E" pin="IO_16" pad="V15"/>
<connect gate="E" pin="IO_17" pad="U15"/>
<connect gate="E" pin="IO_18" pad="R22"/>
<connect gate="E" pin="IO_19" pad="T22"/>
<connect gate="E" pin="IO_2" pad="U18"/>
<connect gate="E" pin="IO_20" pad="V19"/>
<connect gate="E" pin="IO_21" pad="T18"/>
<connect gate="E" pin="IO_22" pad="V20"/>
<connect gate="E" pin="IO_23" pad="U10"/>
<connect gate="E" pin="IO_24" pad="V21"/>
<connect gate="E" pin="IO_25" pad="W11"/>
<connect gate="E" pin="IO_26" pad="V22"/>
<connect gate="E" pin="IO_27" pad="W14"/>
<connect gate="E" pin="IO_28" pad="W15"/>
<connect gate="E" pin="IO_29" pad="W16"/>
<connect gate="E" pin="IO_3" pad="R18"/>
<connect gate="E" pin="IO_30" pad="W18"/>
<connect gate="E" pin="IO_31" pad="W20"/>
<connect gate="E" pin="IO_32" pad="W21"/>
<connect gate="E" pin="IO_33" pad="W22"/>
<connect gate="E" pin="IO_34" pad="Y10"/>
<connect gate="E" pin="IO_35" pad="Y13"/>
<connect gate="E" pin="IO_36" pad="Y14"/>
<connect gate="E" pin="IO_37" pad="Y16"/>
<connect gate="E" pin="IO_38" pad="Y17"/>
<connect gate="E" pin="IO_39" pad="Y18"/>
<connect gate="E" pin="IO_4" pad="U19"/>
<connect gate="E" pin="IO_40" pad="Y19"/>
<connect gate="E" pin="IO_41" pad="Y20"/>
<connect gate="E" pin="IO_42" pad="Y21"/>
<connect gate="E" pin="IO_43" pad="Y22"/>
<connect gate="E" pin="IO_44" pad="AA10"/>
<connect gate="E" pin="IO_45" pad="AA11"/>
<connect gate="E" pin="IO_46" pad="AA12"/>
<connect gate="E" pin="IO_47" pad="AA13"/>
<connect gate="E" pin="IO_48" pad="AA14"/>
<connect gate="E" pin="IO_49" pad="AA15"/>
<connect gate="E" pin="IO_5" pad="R19"/>
<connect gate="E" pin="IO_50" pad="AA16"/>
<connect gate="E" pin="IO_51" pad="AA17"/>
<connect gate="E" pin="IO_52" pad="AA18"/>
<connect gate="E" pin="IO_53" pad="AA19"/>
<connect gate="E" pin="IO_54" pad="AA20"/>
<connect gate="E" pin="IO_55" pad="AB10"/>
<connect gate="E" pin="IO_56" pad="AB11"/>
<connect gate="E" pin="IO_57" pad="AB12"/>
<connect gate="E" pin="IO_58" pad="AB13"/>
<connect gate="E" pin="IO_59" pad="AB14"/>
<connect gate="E" pin="IO_6" pad="U20"/>
<connect gate="E" pin="IO_60" pad="AB15"/>
<connect gate="E" pin="IO_61" pad="AB16"/>
<connect gate="E" pin="IO_62" pad="AB17"/>
<connect gate="E" pin="IO_63" pad="AB18"/>
<connect gate="E" pin="IO_64" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="R20"/>
<connect gate="E" pin="IO_8" pad="U21"/>
<connect gate="E" pin="IO_9" pad="U13"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="T19"/>
<connect gate="E" pin="VCCIO6_2" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="W17"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="V13"/>
<connect gate="E" pin="VCCIO7_4" pad="Y12"/>
<connect gate="E" pin="VCCIO7_5" pad="AB21"/>
<connect gate="E" pin="VCCIO8" pad="Y11"/>
<connect gate="E" pin="VCCIO8_2" pad="V10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C50F484C8N"/>
<attribute name="OC_FARNELL" value="1635088"/>
<attribute name="OC_NEWARK" value="51R0569"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C50F484I8N">
<description>FPGA, CYCLONE II</description>
<gates>
<gate name="A" symbol="EP2C50F484I8N_A"/>
<gate name="B" symbol="EP2C50F484I8N_B"/>
<gate name="C" symbol="EP2C50F484I8N_C"/>
<gate name="D" symbol="EP2C50F484I8N_D"/>
<gate name="E" symbol="EP2C50F484I8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22_2300X2300X350">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="K3"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="C5"/>
<connect gate="A" pin="GND_2" pad="J8"/>
<connect gate="A" pin="GND_3" pad="A1"/>
<connect gate="A" pin="GND_4" pad="G4"/>
<connect gate="A" pin="GND_5" pad="J9"/>
<connect gate="A" pin="GND_6" pad="B2"/>
<connect gate="A" pin="GND_7" pad="C8"/>
<connect gate="A" pin="GND_8" pad="K7"/>
<connect gate="A" pin="GND_9" pad="H9"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="C7"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="C9"/>
<connect gate="A" pin="IO_15" pad="B7"/>
<connect gate="A" pin="IO_16" pad="D1"/>
<connect gate="A" pin="IO_17" pad="B8"/>
<connect gate="A" pin="IO_18" pad="D2"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="D3"/>
<connect gate="A" pin="IO_21" pad="C1"/>
<connect gate="A" pin="IO_22" pad="D4"/>
<connect gate="A" pin="IO_23" pad="C2"/>
<connect gate="A" pin="IO_24" pad="D5"/>
<connect gate="A" pin="IO_25" pad="C3"/>
<connect gate="A" pin="IO_26" pad="D6"/>
<connect gate="A" pin="IO_27" pad="C4"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A3"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E1"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E7"/>
<connect gate="A" pin="IO_34" pad="E3"/>
<connect gate="A" pin="IO_35" pad="E8"/>
<connect gate="A" pin="IO_36" pad="E4"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="H1"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="H2"/>
<connect gate="A" pin="IO_51" pad="H3"/>
<connect gate="A" pin="IO_52" pad="H4"/>
<connect gate="A" pin="IO_53" pad="H5"/>
<connect gate="A" pin="IO_54" pad="H6"/>
<connect gate="A" pin="IO_55" pad="J1"/>
<connect gate="A" pin="IO_56" pad="J2"/>
<connect gate="A" pin="IO_57" pad="J3"/>
<connect gate="A" pin="IO_58" pad="J4"/>
<connect gate="A" pin="IO_59" pad="J5"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="G7"/>
<connect gate="A" pin="VCCINT_3" pad="G8"/>
<connect gate="A" pin="VCCINT_4" pad="L7"/>
<connect gate="A" pin="VCCINT_5" pad="H7"/>
<connect gate="A" pin="VCCINT_6" pad="K8"/>
<connect gate="A" pin="VCCINT_7" pad="K9"/>
<connect gate="A" pin="VCCIO2" pad="J7"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="L3"/>
<connect gate="A" pin="VCCIO3" pad="A2"/>
<connect gate="A" pin="VCCIO3_2" pad="G9"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="N8"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V3"/>
<connect gate="B" pin="GND_11" pad="Y8"/>
<connect gate="B" pin="GND_12" pad="M7"/>
<connect gate="B" pin="GND_13" pad="N7"/>
<connect gate="B" pin="GND_2" pad="P9"/>
<connect gate="B" pin="GND_3" pad="P8"/>
<connect gate="B" pin="GND_4" pad="R9"/>
<connect gate="B" pin="GND_5" pad="A22"/>
<connect gate="B" pin="GND_6" pad="M4"/>
<connect gate="B" pin="GND_7" pad="R3"/>
<connect gate="B" pin="GND_8" pad="V6"/>
<connect gate="B" pin="GND_9" pad="M8"/>
<connect gate="B" pin="GND_PLL1" pad="V5"/>
<connect gate="B" pin="GND_PLL1_2" pad="U5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="N4"/>
<connect gate="B" pin="IO_11" pad="N5"/>
<connect gate="B" pin="IO_12" pad="R2"/>
<connect gate="B" pin="IO_13" pad="N6"/>
<connect gate="B" pin="IO_14" pad="R4"/>
<connect gate="B" pin="IO_15" pad="R5"/>
<connect gate="B" pin="IO_16" pad="R6"/>
<connect gate="B" pin="IO_17" pad="P1"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="T1"/>
<connect gate="B" pin="IO_2" pad="U1"/>
<connect gate="B" pin="IO_20" pad="R1"/>
<connect gate="B" pin="IO_21" pad="T2"/>
<connect gate="B" pin="IO_22" pad="P3"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="P4"/>
<connect gate="B" pin="IO_25" pad="P5"/>
<connect gate="B" pin="IO_26" pad="P6"/>
<connect gate="B" pin="IO_27" pad="U2"/>
<connect gate="B" pin="IO_28" pad="U3"/>
<connect gate="B" pin="IO_29" pad="U4"/>
<connect gate="B" pin="IO_3" pad="M5"/>
<connect gate="B" pin="IO_30" pad="U8"/>
<connect gate="B" pin="IO_31" pad="U9"/>
<connect gate="B" pin="IO_32" pad="V1"/>
<connect gate="B" pin="IO_33" pad="V2"/>
<connect gate="B" pin="IO_34" pad="V4"/>
<connect gate="B" pin="IO_35" pad="V8"/>
<connect gate="B" pin="IO_36" pad="V9"/>
<connect gate="B" pin="IO_37" pad="W1"/>
<connect gate="B" pin="IO_38" pad="W2"/>
<connect gate="B" pin="IO_39" pad="W3"/>
<connect gate="B" pin="IO_4" pad="M6"/>
<connect gate="B" pin="IO_40" pad="W4"/>
<connect gate="B" pin="IO_41" pad="W5"/>
<connect gate="B" pin="IO_42" pad="W7"/>
<connect gate="B" pin="IO_43" pad="W8"/>
<connect gate="B" pin="IO_44" pad="W9"/>
<connect gate="B" pin="IO_45" pad="Y1"/>
<connect gate="B" pin="IO_46" pad="Y2"/>
<connect gate="B" pin="IO_47" pad="Y3"/>
<connect gate="B" pin="IO_48" pad="Y4"/>
<connect gate="B" pin="IO_49" pad="Y5"/>
<connect gate="B" pin="IO_5" pad="T5"/>
<connect gate="B" pin="IO_50" pad="Y6"/>
<connect gate="B" pin="IO_51" pad="Y7"/>
<connect gate="B" pin="IO_52" pad="Y9"/>
<connect gate="B" pin="IO_53" pad="A10"/>
<connect gate="B" pin="IO_54" pad="A11"/>
<connect gate="B" pin="IO_55" pad="A13"/>
<connect gate="B" pin="IO_56" pad="A14"/>
<connect gate="B" pin="IO_57" pad="A15"/>
<connect gate="B" pin="IO_58" pad="A16"/>
<connect gate="B" pin="IO_59" pad="A17"/>
<connect gate="B" pin="IO_6" pad="N1"/>
<connect gate="B" pin="IO_60" pad="A18"/>
<connect gate="B" pin="IO_61" pad="A19"/>
<connect gate="B" pin="IO_7" pad="T6"/>
<connect gate="B" pin="IO_8" pad="N2"/>
<connect gate="B" pin="IO_9" pad="N3"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="L9"/>
<connect gate="B" pin="VCCINT_2" pad="M9"/>
<connect gate="B" pin="VCCINT_3" pad="L8"/>
<connect gate="B" pin="VCCINT_4" pad="T7"/>
<connect gate="B" pin="VCCINT_5" pad="N9"/>
<connect gate="B" pin="VCCINT_6" pad="R7"/>
<connect gate="B" pin="VCCINT_7" pad="R8"/>
<connect gate="B" pin="VCCINT_8" pad="T8"/>
<connect gate="B" pin="VCCIO1" pad="AA1"/>
<connect gate="B" pin="VCCIO1_2" pad="M3"/>
<connect gate="B" pin="VCCIO1_3" pad="P7"/>
<connect gate="B" pin="VCCIO1_4" pad="T4"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="W6"/>
<connect gate="B" pin="VCCIO8_2" pad="T9"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="D10"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="G13"/>
<connect gate="C" pin="GND_11" pad="AA2"/>
<connect gate="C" pin="GND_12" pad="C15"/>
<connect gate="C" pin="GND_13" pad="AB1"/>
<connect gate="C" pin="GND_14" pad="D18"/>
<connect gate="C" pin="GND_2" pad="F19"/>
<connect gate="C" pin="GND_3" pad="B21"/>
<connect gate="C" pin="GND_4" pad="G15"/>
<connect gate="C" pin="GND_5" pad="G10"/>
<connect gate="C" pin="GND_6" pad="H10"/>
<connect gate="C" pin="GND_7" pad="D13"/>
<connect gate="C" pin="GND_8" pad="H11"/>
<connect gate="C" pin="GND_9" pad="G11"/>
<connect gate="C" pin="GND_PLL2" pad="F18"/>
<connect gate="C" pin="GND_PLL2_2" pad="E17"/>
<connect gate="C" pin="IO" pad="G22"/>
<connect gate="C" pin="IO_10" pad="B20"/>
<connect gate="C" pin="IO_11" pad="D11"/>
<connect gate="C" pin="IO_12" pad="C13"/>
<connect gate="C" pin="IO_13" pad="AB3"/>
<connect gate="C" pin="IO_14" pad="C10"/>
<connect gate="C" pin="IO_15" pad="AB4"/>
<connect gate="C" pin="IO_16" pad="C14"/>
<connect gate="C" pin="IO_17" pad="D14"/>
<connect gate="C" pin="IO_18" pad="AB5"/>
<connect gate="C" pin="IO_19" pad="AB6"/>
<connect gate="C" pin="IO_2" pad="AA3"/>
<connect gate="C" pin="IO_20" pad="AB7"/>
<connect gate="C" pin="IO_21" pad="AB8"/>
<connect gate="C" pin="IO_22" pad="AB9"/>
<connect gate="C" pin="IO_23" pad="B10"/>
<connect gate="C" pin="IO_24" pad="B11"/>
<connect gate="C" pin="IO_25" pad="C16"/>
<connect gate="C" pin="IO_26" pad="C17"/>
<connect gate="C" pin="IO_27" pad="B13"/>
<connect gate="C" pin="IO_28" pad="C18"/>
<connect gate="C" pin="IO_29" pad="B14"/>
<connect gate="C" pin="IO_3" pad="AA4"/>
<connect gate="C" pin="IO_30" pad="C19"/>
<connect gate="C" pin="IO_31" pad="B15"/>
<connect gate="C" pin="IO_32" pad="C20"/>
<connect gate="C" pin="IO_33" pad="B16"/>
<connect gate="C" pin="IO_34" pad="C21"/>
<connect gate="C" pin="IO_35" pad="B17"/>
<connect gate="C" pin="IO_36" pad="B18"/>
<connect gate="C" pin="IO_37" pad="B19"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AA5"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="AA6"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AA7"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G17"/>
<connect gate="C" pin="IO_62" pad="G18"/>
<connect gate="C" pin="IO_63" pad="G20"/>
<connect gate="C" pin="IO_64" pad="G21"/>
<connect gate="C" pin="IO_7" pad="AA8"/>
<connect gate="C" pin="IO_8" pad="C22"/>
<connect gate="C" pin="IO_9" pad="AA9"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G16"/>
<connect gate="C" pin="VCCINT_2" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="G14"/>
<connect gate="C" pin="VCCIO4_2" pad="D17"/>
<connect gate="C" pin="VCCIO4_3" pad="C12"/>
<connect gate="C" pin="VCCIO4_4" pad="E13"/>
<connect gate="C" pin="VCCIO5" pad="G19"/>
<connect gate="C" pin="VCCIO5_2" pad="B22"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="H15"/>
<connect gate="D" pin="GND_10" pad="K16"/>
<connect gate="D" pin="GND_11" pad="L15"/>
<connect gate="D" pin="GND_12" pad="N10"/>
<connect gate="D" pin="GND_13" pad="K12"/>
<connect gate="D" pin="GND_14" pad="M13"/>
<connect gate="D" pin="GND_15" pad="K13"/>
<connect gate="D" pin="GND_16" pad="N11"/>
<connect gate="D" pin="GND_17" pad="J14"/>
<connect gate="D" pin="GND_18" pad="L10"/>
<connect gate="D" pin="GND_19" pad="L11"/>
<connect gate="D" pin="GND_2" pad="K19"/>
<connect gate="D" pin="GND_20" pad="N12"/>
<connect gate="D" pin="GND_21" pad="J15"/>
<connect gate="D" pin="GND_22" pad="L12"/>
<connect gate="D" pin="GND_23" pad="L13"/>
<connect gate="D" pin="GND_24" pad="N13"/>
<connect gate="D" pin="GND_25" pad="N19"/>
<connect gate="D" pin="GND_26" pad="N16"/>
<connect gate="D" pin="GND_27" pad="P15"/>
<connect gate="D" pin="GND_28" pad="R11"/>
<connect gate="D" pin="GND_29" pad="R13"/>
<connect gate="D" pin="GND_3" pad="M10"/>
<connect gate="D" pin="GND_30" pad="H14"/>
<connect gate="D" pin="GND_31" pad="R14"/>
<connect gate="D" pin="GND_32" pad="H20"/>
<connect gate="D" pin="GND_4" pad="M11"/>
<connect gate="D" pin="GND_5" pad="K10"/>
<connect gate="D" pin="GND_6" pad="M16"/>
<connect gate="D" pin="GND_7" pad="M12"/>
<connect gate="D" pin="GND_8" pad="K11"/>
<connect gate="D" pin="GND_9" pad="K15"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="K17"/>
<connect gate="D" pin="IO_11" pad="H22"/>
<connect gate="D" pin="IO_12" pad="K18"/>
<connect gate="D" pin="IO_13" pad="J21"/>
<connect gate="D" pin="IO_14" pad="J22"/>
<connect gate="D" pin="IO_15" pad="L17"/>
<connect gate="D" pin="IO_16" pad="K20"/>
<connect gate="D" pin="IO_17" pad="L18"/>
<connect gate="D" pin="IO_18" pad="K21"/>
<connect gate="D" pin="IO_19" pad="L19"/>
<connect gate="D" pin="IO_2" pad="H17"/>
<connect gate="D" pin="IO_20" pad="K22"/>
<connect gate="D" pin="IO_21" pad="M18"/>
<connect gate="D" pin="IO_22" pad="M19"/>
<connect gate="D" pin="IO_23" pad="N21"/>
<connect gate="D" pin="IO_24" pad="N22"/>
<connect gate="D" pin="IO_25" pad="P17"/>
<connect gate="D" pin="IO_26" pad="P18"/>
<connect gate="D" pin="IO_27" pad="P19"/>
<connect gate="D" pin="IO_28" pad="P20"/>
<connect gate="D" pin="IO_29" pad="P21"/>
<connect gate="D" pin="IO_3" pad="H18"/>
<connect gate="D" pin="IO_30" pad="P22"/>
<connect gate="D" pin="IO_4" pad="J17"/>
<connect gate="D" pin="IO_5" pad="H19"/>
<connect gate="D" pin="IO_6" pad="J18"/>
<connect gate="D" pin="IO_7" pad="J19"/>
<connect gate="D" pin="IO_8" pad="H21"/>
<connect gate="D" pin="IO_9" pad="J20"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="N15"/>
<connect gate="D" pin="VCCINT_10" pad="P11"/>
<connect gate="D" pin="VCCINT_11" pad="J13"/>
<connect gate="D" pin="VCCINT_12" pad="P12"/>
<connect gate="D" pin="VCCINT_13" pad="R10"/>
<connect gate="D" pin="VCCINT_14" pad="P13"/>
<connect gate="D" pin="VCCINT_15" pad="R12"/>
<connect gate="D" pin="VCCINT_16" pad="L14"/>
<connect gate="D" pin="VCCINT_17" pad="K14"/>
<connect gate="D" pin="VCCINT_18" pad="L16"/>
<connect gate="D" pin="VCCINT_19" pad="P14"/>
<connect gate="D" pin="VCCINT_2" pad="H16"/>
<connect gate="D" pin="VCCINT_20" pad="M14"/>
<connect gate="D" pin="VCCINT_21" pad="R16"/>
<connect gate="D" pin="VCCINT_22" pad="M15"/>
<connect gate="D" pin="VCCINT_23" pad="N14"/>
<connect gate="D" pin="VCCINT_3" pad="H12"/>
<connect gate="D" pin="VCCINT_4" pad="P10"/>
<connect gate="D" pin="VCCINT_5" pad="J10"/>
<connect gate="D" pin="VCCINT_6" pad="R15"/>
<connect gate="D" pin="VCCINT_7" pad="H13"/>
<connect gate="D" pin="VCCINT_8" pad="J11"/>
<connect gate="D" pin="VCCINT_9" pad="J12"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="M20"/>
<connect gate="D" pin="VCCIO6_2" pad="P16"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="W19"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="T11"/>
<connect gate="E" pin="GND_11" pad="V17"/>
<connect gate="E" pin="GND_12" pad="T16"/>
<connect gate="E" pin="GND_2" pad="Y15"/>
<connect gate="E" pin="GND_3" pad="AA21"/>
<connect gate="E" pin="GND_4" pad="T20"/>
<connect gate="E" pin="GND_5" pad="AB22"/>
<connect gate="E" pin="GND_6" pad="T10"/>
<connect gate="E" pin="GND_7" pad="W13"/>
<connect gate="E" pin="GND_8" pad="T13"/>
<connect gate="E" pin="GND_9" pad="W10"/>
<connect gate="E" pin="GND_PLL4" pad="T17"/>
<connect gate="E" pin="GND_PLL4_2" pad="V18"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="U22"/>
<connect gate="E" pin="IO_11" pad="R21"/>
<connect gate="E" pin="IO_12" pad="U14"/>
<connect gate="E" pin="IO_13" pad="T21"/>
<connect gate="E" pin="IO_14" pad="V14"/>
<connect gate="E" pin="IO_15" pad="V11"/>
<connect gate="E" pin="IO_16" pad="V15"/>
<connect gate="E" pin="IO_17" pad="U15"/>
<connect gate="E" pin="IO_18" pad="R22"/>
<connect gate="E" pin="IO_19" pad="T22"/>
<connect gate="E" pin="IO_2" pad="U18"/>
<connect gate="E" pin="IO_20" pad="V19"/>
<connect gate="E" pin="IO_21" pad="T18"/>
<connect gate="E" pin="IO_22" pad="V20"/>
<connect gate="E" pin="IO_23" pad="U10"/>
<connect gate="E" pin="IO_24" pad="V21"/>
<connect gate="E" pin="IO_25" pad="W11"/>
<connect gate="E" pin="IO_26" pad="V22"/>
<connect gate="E" pin="IO_27" pad="W14"/>
<connect gate="E" pin="IO_28" pad="W15"/>
<connect gate="E" pin="IO_29" pad="W16"/>
<connect gate="E" pin="IO_3" pad="R18"/>
<connect gate="E" pin="IO_30" pad="W18"/>
<connect gate="E" pin="IO_31" pad="W20"/>
<connect gate="E" pin="IO_32" pad="W21"/>
<connect gate="E" pin="IO_33" pad="W22"/>
<connect gate="E" pin="IO_34" pad="Y10"/>
<connect gate="E" pin="IO_35" pad="Y13"/>
<connect gate="E" pin="IO_36" pad="Y14"/>
<connect gate="E" pin="IO_37" pad="Y16"/>
<connect gate="E" pin="IO_38" pad="Y17"/>
<connect gate="E" pin="IO_39" pad="Y18"/>
<connect gate="E" pin="IO_4" pad="U19"/>
<connect gate="E" pin="IO_40" pad="Y19"/>
<connect gate="E" pin="IO_41" pad="Y20"/>
<connect gate="E" pin="IO_42" pad="Y21"/>
<connect gate="E" pin="IO_43" pad="Y22"/>
<connect gate="E" pin="IO_44" pad="AA10"/>
<connect gate="E" pin="IO_45" pad="AA11"/>
<connect gate="E" pin="IO_46" pad="AA12"/>
<connect gate="E" pin="IO_47" pad="AA13"/>
<connect gate="E" pin="IO_48" pad="AA14"/>
<connect gate="E" pin="IO_49" pad="AA15"/>
<connect gate="E" pin="IO_5" pad="R19"/>
<connect gate="E" pin="IO_50" pad="AA16"/>
<connect gate="E" pin="IO_51" pad="AA17"/>
<connect gate="E" pin="IO_52" pad="AA18"/>
<connect gate="E" pin="IO_53" pad="AA19"/>
<connect gate="E" pin="IO_54" pad="AA20"/>
<connect gate="E" pin="IO_55" pad="AB10"/>
<connect gate="E" pin="IO_56" pad="AB11"/>
<connect gate="E" pin="IO_57" pad="AB12"/>
<connect gate="E" pin="IO_58" pad="AB13"/>
<connect gate="E" pin="IO_59" pad="AB14"/>
<connect gate="E" pin="IO_6" pad="U20"/>
<connect gate="E" pin="IO_60" pad="AB15"/>
<connect gate="E" pin="IO_61" pad="AB16"/>
<connect gate="E" pin="IO_62" pad="AB17"/>
<connect gate="E" pin="IO_63" pad="AB18"/>
<connect gate="E" pin="IO_64" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="R20"/>
<connect gate="E" pin="IO_8" pad="U21"/>
<connect gate="E" pin="IO_9" pad="U13"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="T19"/>
<connect gate="E" pin="VCCIO6_2" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="W17"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="V13"/>
<connect gate="E" pin="VCCIO7_4" pad="Y12"/>
<connect gate="E" pin="VCCIO7_5" pad="AB21"/>
<connect gate="E" pin="VCCIO8" pad="Y11"/>
<connect gate="E" pin="VCCIO8_2" pad="V10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C50F484I8N"/>
<attribute name="OC_FARNELL" value="1663198"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="BGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C50U484C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP2C50U484C8N_A"/>
<gate name="B" symbol="EP2C50U484C8N_B"/>
<gate name="C" symbol="EP2C50U484C8N_C"/>
<gate name="D" symbol="EP2C50U484C8N_D"/>
<gate name="E" symbol="EP2C50U484C8N_E"/>
</gates>
<devices>
<device name="" package="BGA484C22X22X80P_1900X1900X220">
<connects>
<connect gate="A" pin="CLK0" pad="L1"/>
<connect gate="A" pin="CLK1" pad="L2"/>
<connect gate="A" pin="DATA0" pad="K4"/>
<connect gate="A" pin="DCLK" pad="L6"/>
<connect gate="A" pin="GND" pad="C5"/>
<connect gate="A" pin="GNDA_PLL3" pad="F7"/>
<connect gate="A" pin="GND_10" pad="C8"/>
<connect gate="A" pin="GND_2" pad="H9"/>
<connect gate="A" pin="GND_3" pad="K3"/>
<connect gate="A" pin="GND_4" pad="K7"/>
<connect gate="A" pin="GND_5" pad="J8"/>
<connect gate="A" pin="GND_6" pad="J9"/>
<connect gate="A" pin="GND_7" pad="B2"/>
<connect gate="A" pin="GND_8" pad="G4"/>
<connect gate="A" pin="GND_9" pad="A1"/>
<connect gate="A" pin="GND_PLL3" pad="F6"/>
<connect gate="A" pin="GND_PLL3_2" pad="F5"/>
<connect gate="A" pin="IO" pad="J6"/>
<connect gate="A" pin="IO_10" pad="B4"/>
<connect gate="A" pin="IO_11" pad="B5"/>
<connect gate="A" pin="IO_12" pad="B6"/>
<connect gate="A" pin="IO_13" pad="B7"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="B9"/>
<connect gate="A" pin="IO_16" pad="C1"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C7"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D1"/>
<connect gate="A" pin="IO_23" pad="D2"/>
<connect gate="A" pin="IO_24" pad="D3"/>
<connect gate="A" pin="IO_25" pad="D4"/>
<connect gate="A" pin="IO_26" pad="D5"/>
<connect gate="A" pin="IO_27" pad="D6"/>
<connect gate="A" pin="IO_28" pad="D7"/>
<connect gate="A" pin="IO_29" pad="D8"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D9"/>
<connect gate="A" pin="IO_31" pad="E1"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E3"/>
<connect gate="A" pin="IO_34" pad="E4"/>
<connect gate="A" pin="IO_35" pad="E7"/>
<connect gate="A" pin="IO_36" pad="E8"/>
<connect gate="A" pin="IO_37" pad="E9"/>
<connect gate="A" pin="IO_38" pad="F1"/>
<connect gate="A" pin="IO_39" pad="F2"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="F3"/>
<connect gate="A" pin="IO_41" pad="F4"/>
<connect gate="A" pin="IO_42" pad="F8"/>
<connect gate="A" pin="IO_43" pad="F9"/>
<connect gate="A" pin="IO_44" pad="G1"/>
<connect gate="A" pin="IO_45" pad="G2"/>
<connect gate="A" pin="IO_46" pad="G3"/>
<connect gate="A" pin="IO_47" pad="G5"/>
<connect gate="A" pin="IO_48" pad="G6"/>
<connect gate="A" pin="IO_49" pad="H1"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="H2"/>
<connect gate="A" pin="IO_51" pad="H3"/>
<connect gate="A" pin="IO_52" pad="H4"/>
<connect gate="A" pin="IO_53" pad="H5"/>
<connect gate="A" pin="IO_54" pad="H6"/>
<connect gate="A" pin="IO_55" pad="J1"/>
<connect gate="A" pin="IO_56" pad="J2"/>
<connect gate="A" pin="IO_57" pad="J3"/>
<connect gate="A" pin="IO_58" pad="J4"/>
<connect gate="A" pin="IO_59" pad="J5"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="NCE" pad="K1"/>
<connect gate="A" pin="NCONFIG" pad="L4"/>
<connect gate="A" pin="TCK" pad="K2"/>
<connect gate="A" pin="TDI" pad="K5"/>
<connect gate="A" pin="TDO" pad="L5"/>
<connect gate="A" pin="TMS" pad="K6"/>
<connect gate="A" pin="VCCA_PLL3" pad="E6"/>
<connect gate="A" pin="VCCD_PLL3" pad="E5"/>
<connect gate="A" pin="VCCINT" pad="L7"/>
<connect gate="A" pin="VCCINT_2" pad="H7"/>
<connect gate="A" pin="VCCINT_3" pad="H8"/>
<connect gate="A" pin="VCCINT_4" pad="K8"/>
<connect gate="A" pin="VCCINT_5" pad="G7"/>
<connect gate="A" pin="VCCINT_6" pad="K9"/>
<connect gate="A" pin="VCCINT_7" pad="G8"/>
<connect gate="A" pin="VCCIO2" pad="L3"/>
<connect gate="A" pin="VCCIO2_2" pad="B1"/>
<connect gate="A" pin="VCCIO2_3" pad="J7"/>
<connect gate="A" pin="VCCIO3" pad="G9"/>
<connect gate="A" pin="VCCIO3_2" pad="A2"/>
<connect gate="A" pin="VCCIO3_3" pad="C6"/>
<connect gate="B" pin="CLK2" pad="M1"/>
<connect gate="B" pin="CLK3" pad="M2"/>
<connect gate="B" pin="CLK9" pad="A12"/>
<connect gate="B" pin="GND" pad="R9"/>
<connect gate="B" pin="GNDA_PLL1" pad="V7"/>
<connect gate="B" pin="GND_10" pad="V6"/>
<connect gate="B" pin="GND_11" pad="M8"/>
<connect gate="B" pin="GND_12" pad="Y8"/>
<connect gate="B" pin="GND_13" pad="N8"/>
<connect gate="B" pin="GND_2" pad="V3"/>
<connect gate="B" pin="GND_3" pad="M4"/>
<connect gate="B" pin="GND_4" pad="M7"/>
<connect gate="B" pin="GND_5" pad="P8"/>
<connect gate="B" pin="GND_6" pad="N7"/>
<connect gate="B" pin="GND_7" pad="P9"/>
<connect gate="B" pin="GND_8" pad="R3"/>
<connect gate="B" pin="GND_9" pad="A22"/>
<connect gate="B" pin="GND_PLL1" pad="V5"/>
<connect gate="B" pin="GND_PLL1_2" pad="U5"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="P1"/>
<connect gate="B" pin="IO_11" pad="P2"/>
<connect gate="B" pin="IO_12" pad="P3"/>
<connect gate="B" pin="IO_13" pad="P4"/>
<connect gate="B" pin="IO_14" pad="P5"/>
<connect gate="B" pin="IO_15" pad="P6"/>
<connect gate="B" pin="IO_16" pad="R1"/>
<connect gate="B" pin="IO_17" pad="R2"/>
<connect gate="B" pin="IO_18" pad="R4"/>
<connect gate="B" pin="IO_19" pad="R5"/>
<connect gate="B" pin="IO_2" pad="M5"/>
<connect gate="B" pin="IO_20" pad="R6"/>
<connect gate="B" pin="IO_21" pad="T1"/>
<connect gate="B" pin="IO_22" pad="T2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="T5"/>
<connect gate="B" pin="IO_25" pad="T6"/>
<connect gate="B" pin="IO_26" pad="U1"/>
<connect gate="B" pin="IO_27" pad="U2"/>
<connect gate="B" pin="IO_28" pad="U3"/>
<connect gate="B" pin="IO_29" pad="U4"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="U8"/>
<connect gate="B" pin="IO_31" pad="U9"/>
<connect gate="B" pin="IO_32" pad="V1"/>
<connect gate="B" pin="IO_33" pad="V2"/>
<connect gate="B" pin="IO_34" pad="V4"/>
<connect gate="B" pin="IO_35" pad="V8"/>
<connect gate="B" pin="IO_36" pad="V9"/>
<connect gate="B" pin="IO_37" pad="W1"/>
<connect gate="B" pin="IO_38" pad="W2"/>
<connect gate="B" pin="IO_39" pad="W3"/>
<connect gate="B" pin="IO_4" pad="N1"/>
<connect gate="B" pin="IO_40" pad="W4"/>
<connect gate="B" pin="IO_41" pad="W5"/>
<connect gate="B" pin="IO_42" pad="W7"/>
<connect gate="B" pin="IO_43" pad="W8"/>
<connect gate="B" pin="IO_44" pad="W9"/>
<connect gate="B" pin="IO_45" pad="Y1"/>
<connect gate="B" pin="IO_46" pad="Y2"/>
<connect gate="B" pin="IO_47" pad="Y3"/>
<connect gate="B" pin="IO_48" pad="Y4"/>
<connect gate="B" pin="IO_49" pad="Y5"/>
<connect gate="B" pin="IO_5" pad="N2"/>
<connect gate="B" pin="IO_50" pad="Y6"/>
<connect gate="B" pin="IO_51" pad="Y7"/>
<connect gate="B" pin="IO_52" pad="Y9"/>
<connect gate="B" pin="IO_53" pad="A10"/>
<connect gate="B" pin="IO_54" pad="A11"/>
<connect gate="B" pin="IO_55" pad="A13"/>
<connect gate="B" pin="IO_56" pad="A14"/>
<connect gate="B" pin="IO_57" pad="A15"/>
<connect gate="B" pin="IO_58" pad="A16"/>
<connect gate="B" pin="IO_59" pad="A17"/>
<connect gate="B" pin="IO_6" pad="N3"/>
<connect gate="B" pin="IO_60" pad="A18"/>
<connect gate="B" pin="IO_61" pad="A19"/>
<connect gate="B" pin="IO_7" pad="N4"/>
<connect gate="B" pin="IO_8" pad="N5"/>
<connect gate="B" pin="IO_9" pad="N6"/>
<connect gate="B" pin="VCCA_PLL1" pad="U7"/>
<connect gate="B" pin="VCCD_PLL1" pad="U6"/>
<connect gate="B" pin="VCCINT" pad="N9"/>
<connect gate="B" pin="VCCINT_2" pad="T7"/>
<connect gate="B" pin="VCCINT_3" pad="R7"/>
<connect gate="B" pin="VCCINT_4" pad="T8"/>
<connect gate="B" pin="VCCINT_5" pad="L8"/>
<connect gate="B" pin="VCCINT_6" pad="R8"/>
<connect gate="B" pin="VCCINT_7" pad="L9"/>
<connect gate="B" pin="VCCINT_8" pad="M9"/>
<connect gate="B" pin="VCCIO1" pad="T4"/>
<connect gate="B" pin="VCCIO1_2" pad="M3"/>
<connect gate="B" pin="VCCIO1_3" pad="P7"/>
<connect gate="B" pin="VCCIO1_4" pad="AA1"/>
<connect gate="B" pin="VCCIO4" pad="A21"/>
<connect gate="B" pin="VCCIO8" pad="W6"/>
<connect gate="B" pin="VCCIO8_2" pad="T9"/>
<connect gate="C" pin="CLK10" pad="D12"/>
<connect gate="C" pin="CLK11" pad="E12"/>
<connect gate="C" pin="CLK8" pad="B12"/>
<connect gate="C" pin="GND" pad="H11"/>
<connect gate="C" pin="GNDA_PLL2" pad="E16"/>
<connect gate="C" pin="GND_10" pad="H10"/>
<connect gate="C" pin="GND_11" pad="AB1"/>
<connect gate="C" pin="GND_12" pad="B21"/>
<connect gate="C" pin="GND_13" pad="G13"/>
<connect gate="C" pin="GND_14" pad="G15"/>
<connect gate="C" pin="GND_2" pad="D18"/>
<connect gate="C" pin="GND_3" pad="F19"/>
<connect gate="C" pin="GND_4" pad="C15"/>
<connect gate="C" pin="GND_5" pad="G10"/>
<connect gate="C" pin="GND_6" pad="AA2"/>
<connect gate="C" pin="GND_7" pad="D10"/>
<connect gate="C" pin="GND_8" pad="D13"/>
<connect gate="C" pin="GND_9" pad="G11"/>
<connect gate="C" pin="GND_PLL2" pad="E17"/>
<connect gate="C" pin="GND_PLL2_2" pad="F18"/>
<connect gate="C" pin="IO" pad="G22"/>
<connect gate="C" pin="IO_10" pad="AB4"/>
<connect gate="C" pin="IO_11" pad="AB5"/>
<connect gate="C" pin="IO_12" pad="AB6"/>
<connect gate="C" pin="IO_13" pad="AB7"/>
<connect gate="C" pin="IO_14" pad="AB8"/>
<connect gate="C" pin="IO_15" pad="AB9"/>
<connect gate="C" pin="IO_16" pad="B10"/>
<connect gate="C" pin="IO_17" pad="B11"/>
<connect gate="C" pin="IO_18" pad="B13"/>
<connect gate="C" pin="IO_19" pad="B14"/>
<connect gate="C" pin="IO_2" pad="AA3"/>
<connect gate="C" pin="IO_20" pad="B15"/>
<connect gate="C" pin="IO_21" pad="B16"/>
<connect gate="C" pin="IO_22" pad="B17"/>
<connect gate="C" pin="IO_23" pad="B18"/>
<connect gate="C" pin="IO_24" pad="B19"/>
<connect gate="C" pin="IO_25" pad="B20"/>
<connect gate="C" pin="IO_26" pad="C10"/>
<connect gate="C" pin="IO_27" pad="C13"/>
<connect gate="C" pin="IO_28" pad="C14"/>
<connect gate="C" pin="IO_29" pad="C16"/>
<connect gate="C" pin="IO_3" pad="AA4"/>
<connect gate="C" pin="IO_30" pad="C17"/>
<connect gate="C" pin="IO_31" pad="C18"/>
<connect gate="C" pin="IO_32" pad="C19"/>
<connect gate="C" pin="IO_33" pad="C20"/>
<connect gate="C" pin="IO_34" pad="C21"/>
<connect gate="C" pin="IO_35" pad="C22"/>
<connect gate="C" pin="IO_36" pad="D11"/>
<connect gate="C" pin="IO_37" pad="D14"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D16"/>
<connect gate="C" pin="IO_4" pad="AA5"/>
<connect gate="C" pin="IO_40" pad="D19"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E11"/>
<connect gate="C" pin="IO_45" pad="E14"/>
<connect gate="C" pin="IO_46" pad="E15"/>
<connect gate="C" pin="IO_47" pad="E18"/>
<connect gate="C" pin="IO_48" pad="E19"/>
<connect gate="C" pin="IO_49" pad="E20"/>
<connect gate="C" pin="IO_5" pad="AA6"/>
<connect gate="C" pin="IO_50" pad="E21"/>
<connect gate="C" pin="IO_51" pad="E22"/>
<connect gate="C" pin="IO_52" pad="F10"/>
<connect gate="C" pin="IO_53" pad="F11"/>
<connect gate="C" pin="IO_54" pad="F12"/>
<connect gate="C" pin="IO_55" pad="F13"/>
<connect gate="C" pin="IO_56" pad="F14"/>
<connect gate="C" pin="IO_57" pad="F15"/>
<connect gate="C" pin="IO_58" pad="F20"/>
<connect gate="C" pin="IO_59" pad="F21"/>
<connect gate="C" pin="IO_6" pad="AA7"/>
<connect gate="C" pin="IO_60" pad="F22"/>
<connect gate="C" pin="IO_61" pad="G17"/>
<connect gate="C" pin="IO_62" pad="G18"/>
<connect gate="C" pin="IO_63" pad="G20"/>
<connect gate="C" pin="IO_64" pad="G21"/>
<connect gate="C" pin="IO_7" pad="AA8"/>
<connect gate="C" pin="IO_8" pad="AA9"/>
<connect gate="C" pin="IO_9" pad="AB3"/>
<connect gate="C" pin="VCCA_PLL2" pad="F16"/>
<connect gate="C" pin="VCCD_PLL2" pad="F17"/>
<connect gate="C" pin="VCCINT" pad="G16"/>
<connect gate="C" pin="VCCINT_2" pad="G12"/>
<connect gate="C" pin="VCCIO3" pad="E10"/>
<connect gate="C" pin="VCCIO3_2" pad="C11"/>
<connect gate="C" pin="VCCIO4" pad="E13"/>
<connect gate="C" pin="VCCIO4_2" pad="C12"/>
<connect gate="C" pin="VCCIO4_3" pad="D17"/>
<connect gate="C" pin="VCCIO4_4" pad="G14"/>
<connect gate="C" pin="VCCIO5" pad="B22"/>
<connect gate="C" pin="VCCIO5_2" pad="G19"/>
<connect gate="C" pin="VCCIO8" pad="AB2"/>
<connect gate="D" pin="CLK4" pad="L22"/>
<connect gate="D" pin="CLK5" pad="L21"/>
<connect gate="D" pin="CLK6" pad="M22"/>
<connect gate="D" pin="CLK7" pad="M21"/>
<connect gate="D" pin="CONF_DONE" pad="N18"/>
<connect gate="D" pin="GND" pad="R14"/>
<connect gate="D" pin="GND_10" pad="K12"/>
<connect gate="D" pin="GND_11" pad="K13"/>
<connect gate="D" pin="GND_12" pad="K15"/>
<connect gate="D" pin="GND_13" pad="K16"/>
<connect gate="D" pin="GND_14" pad="H14"/>
<connect gate="D" pin="GND_15" pad="K19"/>
<connect gate="D" pin="GND_16" pad="M12"/>
<connect gate="D" pin="GND_17" pad="L10"/>
<connect gate="D" pin="GND_18" pad="M13"/>
<connect gate="D" pin="GND_19" pad="N11"/>
<connect gate="D" pin="GND_2" pad="P15"/>
<connect gate="D" pin="GND_20" pad="L11"/>
<connect gate="D" pin="GND_21" pad="N10"/>
<connect gate="D" pin="GND_22" pad="N12"/>
<connect gate="D" pin="GND_23" pad="H15"/>
<connect gate="D" pin="GND_24" pad="N13"/>
<connect gate="D" pin="GND_25" pad="L12"/>
<connect gate="D" pin="GND_26" pad="L13"/>
<connect gate="D" pin="GND_27" pad="L15"/>
<connect gate="D" pin="GND_28" pad="M10"/>
<connect gate="D" pin="GND_29" pad="M16"/>
<connect gate="D" pin="GND_3" pad="N19"/>
<connect gate="D" pin="GND_30" pad="M11"/>
<connect gate="D" pin="GND_31" pad="R11"/>
<connect gate="D" pin="GND_32" pad="R13"/>
<connect gate="D" pin="GND_4" pad="N16"/>
<connect gate="D" pin="GND_5" pad="J14"/>
<connect gate="D" pin="GND_6" pad="J15"/>
<connect gate="D" pin="GND_7" pad="H20"/>
<connect gate="D" pin="GND_8" pad="K10"/>
<connect gate="D" pin="GND_9" pad="K11"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="J20"/>
<connect gate="D" pin="IO_11" pad="J21"/>
<connect gate="D" pin="IO_12" pad="J22"/>
<connect gate="D" pin="IO_13" pad="K17"/>
<connect gate="D" pin="IO_14" pad="K18"/>
<connect gate="D" pin="IO_15" pad="K20"/>
<connect gate="D" pin="IO_16" pad="K21"/>
<connect gate="D" pin="IO_17" pad="K22"/>
<connect gate="D" pin="IO_18" pad="L17"/>
<connect gate="D" pin="IO_19" pad="L18"/>
<connect gate="D" pin="IO_2" pad="H17"/>
<connect gate="D" pin="IO_20" pad="L19"/>
<connect gate="D" pin="IO_21" pad="M18"/>
<connect gate="D" pin="IO_22" pad="M19"/>
<connect gate="D" pin="IO_23" pad="N21"/>
<connect gate="D" pin="IO_24" pad="N22"/>
<connect gate="D" pin="IO_25" pad="P17"/>
<connect gate="D" pin="IO_26" pad="P18"/>
<connect gate="D" pin="IO_27" pad="P19"/>
<connect gate="D" pin="IO_28" pad="P20"/>
<connect gate="D" pin="IO_29" pad="P21"/>
<connect gate="D" pin="IO_3" pad="H18"/>
<connect gate="D" pin="IO_30" pad="P22"/>
<connect gate="D" pin="IO_4" pad="H19"/>
<connect gate="D" pin="IO_5" pad="H21"/>
<connect gate="D" pin="IO_6" pad="H22"/>
<connect gate="D" pin="IO_7" pad="J17"/>
<connect gate="D" pin="IO_8" pad="J18"/>
<connect gate="D" pin="IO_9" pad="J19"/>
<connect gate="D" pin="MSEL0" pad="M17"/>
<connect gate="D" pin="MSEL1" pad="N17"/>
<connect gate="D" pin="NSTATUS" pad="N20"/>
<connect gate="D" pin="VCCINT" pad="P14"/>
<connect gate="D" pin="VCCINT_10" pad="J11"/>
<connect gate="D" pin="VCCINT_11" pad="H16"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="L16"/>
<connect gate="D" pin="VCCINT_14" pad="N14"/>
<connect gate="D" pin="VCCINT_15" pad="M15"/>
<connect gate="D" pin="VCCINT_16" pad="P10"/>
<connect gate="D" pin="VCCINT_17" pad="N15"/>
<connect gate="D" pin="VCCINT_18" pad="P11"/>
<connect gate="D" pin="VCCINT_19" pad="K14"/>
<connect gate="D" pin="VCCINT_2" pad="R12"/>
<connect gate="D" pin="VCCINT_20" pad="P12"/>
<connect gate="D" pin="VCCINT_21" pad="J12"/>
<connect gate="D" pin="VCCINT_22" pad="P13"/>
<connect gate="D" pin="VCCINT_23" pad="J13"/>
<connect gate="D" pin="VCCINT_3" pad="H12"/>
<connect gate="D" pin="VCCINT_4" pad="R15"/>
<connect gate="D" pin="VCCINT_5" pad="J10"/>
<connect gate="D" pin="VCCINT_6" pad="R10"/>
<connect gate="D" pin="VCCINT_7" pad="H13"/>
<connect gate="D" pin="VCCINT_8" pad="R16"/>
<connect gate="D" pin="VCCINT_9" pad="L14"/>
<connect gate="D" pin="VCCIO5" pad="L20"/>
<connect gate="D" pin="VCCIO5_2" pad="J16"/>
<connect gate="D" pin="VCCIO6" pad="P16"/>
<connect gate="D" pin="VCCIO6_2" pad="M20"/>
<connect gate="E" pin="CLK12" pad="V12"/>
<connect gate="E" pin="CLK13" pad="W12"/>
<connect gate="E" pin="CLK14" pad="U12"/>
<connect gate="E" pin="CLK15" pad="U11"/>
<connect gate="E" pin="GND" pad="AA21"/>
<connect gate="E" pin="GNDA_PLL4" pad="V16"/>
<connect gate="E" pin="GND_10" pad="W13"/>
<connect gate="E" pin="GND_11" pad="W19"/>
<connect gate="E" pin="GND_12" pad="Y15"/>
<connect gate="E" pin="GND_2" pad="T10"/>
<connect gate="E" pin="GND_3" pad="T13"/>
<connect gate="E" pin="GND_4" pad="T16"/>
<connect gate="E" pin="GND_5" pad="V17"/>
<connect gate="E" pin="GND_6" pad="T11"/>
<connect gate="E" pin="GND_7" pad="T20"/>
<connect gate="E" pin="GND_8" pad="W10"/>
<connect gate="E" pin="GND_9" pad="AB22"/>
<connect gate="E" pin="GND_PLL4" pad="V18"/>
<connect gate="E" pin="GND_PLL4_2" pad="T17"/>
<connect gate="E" pin="IO" pad="AB20"/>
<connect gate="E" pin="IO_10" pad="U10"/>
<connect gate="E" pin="IO_11" pad="U13"/>
<connect gate="E" pin="IO_12" pad="U14"/>
<connect gate="E" pin="IO_13" pad="U15"/>
<connect gate="E" pin="IO_14" pad="U18"/>
<connect gate="E" pin="IO_15" pad="U19"/>
<connect gate="E" pin="IO_16" pad="U20"/>
<connect gate="E" pin="IO_17" pad="U21"/>
<connect gate="E" pin="IO_18" pad="U22"/>
<connect gate="E" pin="IO_19" pad="V11"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="V14"/>
<connect gate="E" pin="IO_21" pad="V15"/>
<connect gate="E" pin="IO_22" pad="V19"/>
<connect gate="E" pin="IO_23" pad="V20"/>
<connect gate="E" pin="IO_24" pad="V21"/>
<connect gate="E" pin="IO_25" pad="V22"/>
<connect gate="E" pin="IO_26" pad="W11"/>
<connect gate="E" pin="IO_27" pad="W14"/>
<connect gate="E" pin="IO_28" pad="W15"/>
<connect gate="E" pin="IO_29" pad="W16"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="W18"/>
<connect gate="E" pin="IO_31" pad="W20"/>
<connect gate="E" pin="IO_32" pad="W21"/>
<connect gate="E" pin="IO_33" pad="W22"/>
<connect gate="E" pin="IO_34" pad="Y10"/>
<connect gate="E" pin="IO_35" pad="Y13"/>
<connect gate="E" pin="IO_36" pad="Y14"/>
<connect gate="E" pin="IO_37" pad="Y16"/>
<connect gate="E" pin="IO_38" pad="Y17"/>
<connect gate="E" pin="IO_39" pad="Y18"/>
<connect gate="E" pin="IO_4" pad="R20"/>
<connect gate="E" pin="IO_40" pad="Y19"/>
<connect gate="E" pin="IO_41" pad="Y20"/>
<connect gate="E" pin="IO_42" pad="Y21"/>
<connect gate="E" pin="IO_43" pad="Y22"/>
<connect gate="E" pin="IO_44" pad="AA10"/>
<connect gate="E" pin="IO_45" pad="AA11"/>
<connect gate="E" pin="IO_46" pad="AA12"/>
<connect gate="E" pin="IO_47" pad="AA13"/>
<connect gate="E" pin="IO_48" pad="AA14"/>
<connect gate="E" pin="IO_49" pad="AA15"/>
<connect gate="E" pin="IO_5" pad="R21"/>
<connect gate="E" pin="IO_50" pad="AA16"/>
<connect gate="E" pin="IO_51" pad="AA17"/>
<connect gate="E" pin="IO_52" pad="AA18"/>
<connect gate="E" pin="IO_53" pad="AA19"/>
<connect gate="E" pin="IO_54" pad="AA20"/>
<connect gate="E" pin="IO_55" pad="AB10"/>
<connect gate="E" pin="IO_56" pad="AB11"/>
<connect gate="E" pin="IO_57" pad="AB12"/>
<connect gate="E" pin="IO_58" pad="AB13"/>
<connect gate="E" pin="IO_59" pad="AB14"/>
<connect gate="E" pin="IO_6" pad="R22"/>
<connect gate="E" pin="IO_60" pad="AB15"/>
<connect gate="E" pin="IO_61" pad="AB16"/>
<connect gate="E" pin="IO_62" pad="AB17"/>
<connect gate="E" pin="IO_63" pad="AB18"/>
<connect gate="E" pin="IO_64" pad="AB19"/>
<connect gate="E" pin="IO_7" pad="T18"/>
<connect gate="E" pin="IO_8" pad="T21"/>
<connect gate="E" pin="IO_9" pad="T22"/>
<connect gate="E" pin="VCCA_PLL4" pad="U16"/>
<connect gate="E" pin="VCCD_PLL4" pad="U17"/>
<connect gate="E" pin="VCCINT" pad="T15"/>
<connect gate="E" pin="VCCINT_2" pad="T12"/>
<connect gate="E" pin="VCCIO6" pad="T19"/>
<connect gate="E" pin="VCCIO6_2" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="W17"/>
<connect gate="E" pin="VCCIO7_2" pad="T14"/>
<connect gate="E" pin="VCCIO7_3" pad="V13"/>
<connect gate="E" pin="VCCIO7_4" pad="AB21"/>
<connect gate="E" pin="VCCIO7_5" pad="Y12"/>
<connect gate="E" pin="VCCIO8" pad="Y11"/>
<connect gate="E" pin="VCCIO8_2" pad="V10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C50U484C8N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R0571"/>
<attribute name="PACKAGE" value="484-UBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C5F256C8">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP2C5F256C8_A"/>
<gate name="B" symbol="EP2C5F256C8_B"/>
<gate name="C" symbol="EP2C5F256C8_C"/>
</gates>
<devices>
<device name="" package="BGA256C16X16X100C_1700X1700X22">
<connects>
<connect gate="A" pin="CLK0" pad="H2"/>
<connect gate="A" pin="CLK1" pad="H1"/>
<connect gate="A" pin="CLK2" pad="J2"/>
<connect gate="A" pin="CLK3" pad="J1"/>
<connect gate="A" pin="DATA0" pad="F1"/>
<connect gate="A" pin="DCLK" pad="H4"/>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="GND_10" pad="J9"/>
<connect gate="A" pin="GND_11" pad="C8"/>
<connect gate="A" pin="GND_12" pad="B2"/>
<connect gate="A" pin="GND_13" pad="C9"/>
<connect gate="A" pin="GND_2" pad="G8"/>
<connect gate="A" pin="GND_3" pad="H3"/>
<connect gate="A" pin="GND_4" pad="E8"/>
<connect gate="A" pin="GND_5" pad="J3"/>
<connect gate="A" pin="GND_6" pad="H8"/>
<connect gate="A" pin="GND_7" pad="H9"/>
<connect gate="A" pin="GND_8" pad="J8"/>
<connect gate="A" pin="GND_9" pad="E9"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO_10" pad="B4"/>
<connect gate="A" pin="IO_11" pad="B5"/>
<connect gate="A" pin="IO_12" pad="B6"/>
<connect gate="A" pin="IO_13" pad="B7"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="C1"/>
<connect gate="A" pin="IO_16" pad="C2"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="C4"/>
<connect gate="A" pin="IO_19" pad="C5"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C6"/>
<connect gate="A" pin="IO_21" pad="D3"/>
<connect gate="A" pin="IO_22" pad="D4"/>
<connect gate="A" pin="IO_23" pad="D5"/>
<connect gate="A" pin="IO_24" pad="D6"/>
<connect gate="A" pin="IO_25" pad="D8"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="E2"/>
<connect gate="A" pin="IO_28" pad="E3"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="E5"/>
<connect gate="A" pin="IO_31" pad="E6"/>
<connect gate="A" pin="IO_32" pad="F3"/>
<connect gate="A" pin="IO_33" pad="F4"/>
<connect gate="A" pin="IO_34" pad="F6"/>
<connect gate="A" pin="IO_35" pad="F7"/>
<connect gate="A" pin="IO_36" pad="F8"/>
<connect gate="A" pin="IO_37" pad="F9"/>
<connect gate="A" pin="IO_38" pad="G6"/>
<connect gate="A" pin="IO_39" pad="G7"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="J4"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_43" pad="K4"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B3"/>
<connect gate="A" pin="NC" pad="H6"/>
<connect gate="A" pin="NCE" pad="G5"/>
<connect gate="A" pin="NCONFIG" pad="J5"/>
<connect gate="A" pin="NC_2" pad="B8"/>
<connect gate="A" pin="NC_3" pad="J6"/>
<connect gate="A" pin="NC_4" pad="D1"/>
<connect gate="A" pin="NC_5" pad="D2"/>
<connect gate="A" pin="NC_6" pad="D7"/>
<connect gate="A" pin="NC_7" pad="G4"/>
<connect gate="A" pin="NC_8" pad="D9"/>
<connect gate="A" pin="NC_9" pad="F5"/>
<connect gate="A" pin="TCK" pad="F2"/>
<connect gate="A" pin="TDI" pad="H5"/>
<connect gate="A" pin="TDO" pad="G2"/>
<connect gate="A" pin="TMS" pad="G1"/>
<connect gate="A" pin="VCCINT" pad="H7"/>
<connect gate="A" pin="VCCINT_2" pad="G9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="B1"/>
<connect gate="A" pin="VCCIO1_2" pad="G3"/>
<connect gate="A" pin="VCCIO1_3" pad="K3"/>
<connect gate="A" pin="VCCIO2" pad="E7"/>
<connect gate="A" pin="VCCIO2_2" pad="A2"/>
<connect gate="A" pin="VCCIO2_3" pad="C7"/>
<connect gate="B" pin="GND" pad="B15"/>
<connect gate="B" pin="GNDA_PLL1" pad="M6"/>
<connect gate="B" pin="GND_2" pad="P8"/>
<connect gate="B" pin="GND_3" pad="P9"/>
<connect gate="B" pin="GND_4" pad="K9"/>
<connect gate="B" pin="GND_5" pad="M8"/>
<connect gate="B" pin="GND_6" pad="R2"/>
<connect gate="B" pin="GND_7" pad="M9"/>
<connect gate="B" pin="GND_8" pad="A16"/>
<connect gate="B" pin="GND_9" pad="T1"/>
<connect gate="B" pin="GND_PLL1" pad="N5"/>
<connect gate="B" pin="GND_PLL1_2" pad="L5"/>
<connect gate="B" pin="GND_PLL2" pad="D12"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO_10" pad="M2"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="M4"/>
<connect gate="B" pin="IO_13" pad="N1"/>
<connect gate="B" pin="IO_14" pad="N2"/>
<connect gate="B" pin="IO_15" pad="N8"/>
<connect gate="B" pin="IO_16" pad="N9"/>
<connect gate="B" pin="IO_17" pad="P1"/>
<connect gate="B" pin="IO_18" pad="P2"/>
<connect gate="B" pin="IO_19" pad="P3"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="P4"/>
<connect gate="B" pin="IO_21" pad="P5"/>
<connect gate="B" pin="IO_22" pad="R3"/>
<connect gate="B" pin="IO_23" pad="R4"/>
<connect gate="B" pin="IO_24" pad="R5"/>
<connect gate="B" pin="IO_25" pad="R7"/>
<connect gate="B" pin="IO_26" pad="R8"/>
<connect gate="B" pin="IO_27" pad="R9"/>
<connect gate="B" pin="IO_28" pad="T3"/>
<connect gate="B" pin="IO_29" pad="T4"/>
<connect gate="B" pin="IO_3" pad="L2"/>
<connect gate="B" pin="IO_30" pad="T5"/>
<connect gate="B" pin="IO_31" pad="T6"/>
<connect gate="B" pin="IO_32" pad="T7"/>
<connect gate="B" pin="IO_33" pad="T8"/>
<connect gate="B" pin="IO_34" pad="T9"/>
<connect gate="B" pin="IO_35" pad="A10"/>
<connect gate="B" pin="IO_36" pad="A11"/>
<connect gate="B" pin="IO_37" pad="A12"/>
<connect gate="B" pin="IO_38" pad="A13"/>
<connect gate="B" pin="IO_39" pad="A14"/>
<connect gate="B" pin="IO_4" pad="L3"/>
<connect gate="B" pin="IO_40" pad="B10"/>
<connect gate="B" pin="IO_41" pad="B11"/>
<connect gate="B" pin="IO_42" pad="B12"/>
<connect gate="B" pin="IO_43" pad="B13"/>
<connect gate="B" pin="IO_44" pad="B14"/>
<connect gate="B" pin="IO_45" pad="C11"/>
<connect gate="B" pin="IO_46" pad="C12"/>
<connect gate="B" pin="IO_47" pad="C13"/>
<connect gate="B" pin="IO_48" pad="C14"/>
<connect gate="B" pin="IO_49" pad="D10"/>
<connect gate="B" pin="IO_5" pad="L4"/>
<connect gate="B" pin="IO_50" pad="D11"/>
<connect gate="B" pin="IO_51" pad="D13"/>
<connect gate="B" pin="IO_52" pad="D14"/>
<connect gate="B" pin="IO_53" pad="D15"/>
<connect gate="B" pin="IO_6" pad="L7"/>
<connect gate="B" pin="IO_7" pad="L8"/>
<connect gate="B" pin="IO_8" pad="L9"/>
<connect gate="B" pin="IO_9" pad="M1"/>
<connect gate="B" pin="NC" pad="C16"/>
<connect gate="B" pin="NC_10" pad="C15"/>
<connect gate="B" pin="NC_11" pad="P6"/>
<connect gate="B" pin="NC_2" pad="N3"/>
<connect gate="B" pin="NC_3" pad="N4"/>
<connect gate="B" pin="NC_4" pad="K6"/>
<connect gate="B" pin="NC_5" pad="K7"/>
<connect gate="B" pin="NC_6" pad="N6"/>
<connect gate="B" pin="NC_7" pad="K8"/>
<connect gate="B" pin="NC_8" pad="N7"/>
<connect gate="B" pin="NC_9" pad="R6"/>
<connect gate="B" pin="VCCA_PLL1" pad="M5"/>
<connect gate="B" pin="VCCD_PLL1" pad="L6"/>
<connect gate="B" pin="VCCIO1" pad="R1"/>
<connect gate="B" pin="VCCIO2" pad="C10"/>
<connect gate="B" pin="VCCIO2_2" pad="A15"/>
<connect gate="B" pin="VCCIO3" pad="B16"/>
<connect gate="B" pin="VCCIO4" pad="T2"/>
<connect gate="B" pin="VCCIO4_2" pad="P7"/>
<connect gate="B" pin="VCCIO4_3" pad="M7"/>
<connect gate="C" pin="CLK4" pad="H16"/>
<connect gate="C" pin="CLK5" pad="H15"/>
<connect gate="C" pin="CLK6" pad="J15"/>
<connect gate="C" pin="CLK7" pad="J16"/>
<connect gate="C" pin="CONF_DONE" pad="L13"/>
<connect gate="C" pin="GND" pad="T16"/>
<connect gate="C" pin="GNDA_PLL2" pad="E11"/>
<connect gate="C" pin="GND_2" pad="H14"/>
<connect gate="C" pin="GND_3" pad="J14"/>
<connect gate="C" pin="GND_4" pad="R15"/>
<connect gate="C" pin="GND_PLL2" pad="F12"/>
<connect gate="C" pin="IO" pad="T14"/>
<connect gate="C" pin="IO_10" pad="G13"/>
<connect gate="C" pin="IO_11" pad="G15"/>
<connect gate="C" pin="IO_12" pad="G16"/>
<connect gate="C" pin="IO_13" pad="H11"/>
<connect gate="C" pin="IO_14" pad="H12"/>
<connect gate="C" pin="IO_15" pad="H13"/>
<connect gate="C" pin="IO_16" pad="J11"/>
<connect gate="C" pin="IO_17" pad="J12"/>
<connect gate="C" pin="IO_18" pad="K10"/>
<connect gate="C" pin="IO_19" pad="K11"/>
<connect gate="C" pin="IO_2" pad="E14"/>
<connect gate="C" pin="IO_20" pad="K15"/>
<connect gate="C" pin="IO_21" pad="K16"/>
<connect gate="C" pin="IO_22" pad="L10"/>
<connect gate="C" pin="IO_23" pad="L11"/>
<connect gate="C" pin="IO_24" pad="L12"/>
<connect gate="C" pin="IO_25" pad="L14"/>
<connect gate="C" pin="IO_26" pad="L15"/>
<connect gate="C" pin="IO_27" pad="L16"/>
<connect gate="C" pin="IO_28" pad="M11"/>
<connect gate="C" pin="IO_29" pad="M12"/>
<connect gate="C" pin="IO_3" pad="E16"/>
<connect gate="C" pin="IO_30" pad="M14"/>
<connect gate="C" pin="IO_31" pad="M15"/>
<connect gate="C" pin="IO_32" pad="M16"/>
<connect gate="C" pin="IO_33" pad="N10"/>
<connect gate="C" pin="IO_34" pad="N11"/>
<connect gate="C" pin="IO_35" pad="N12"/>
<connect gate="C" pin="IO_36" pad="N13"/>
<connect gate="C" pin="IO_37" pad="N14"/>
<connect gate="C" pin="IO_38" pad="N15"/>
<connect gate="C" pin="IO_39" pad="N16"/>
<connect gate="C" pin="IO_4" pad="F10"/>
<connect gate="C" pin="IO_40" pad="P11"/>
<connect gate="C" pin="IO_41" pad="P12"/>
<connect gate="C" pin="IO_42" pad="P13"/>
<connect gate="C" pin="IO_43" pad="P14"/>
<connect gate="C" pin="IO_44" pad="P15"/>
<connect gate="C" pin="IO_45" pad="P16"/>
<connect gate="C" pin="IO_46" pad="R10"/>
<connect gate="C" pin="IO_47" pad="R11"/>
<connect gate="C" pin="IO_48" pad="R12"/>
<connect gate="C" pin="IO_49" pad="R13"/>
<connect gate="C" pin="IO_5" pad="F15"/>
<connect gate="C" pin="IO_50" pad="R14"/>
<connect gate="C" pin="IO_51" pad="T10"/>
<connect gate="C" pin="IO_52" pad="T11"/>
<connect gate="C" pin="IO_53" pad="T12"/>
<connect gate="C" pin="IO_54" pad="T13"/>
<connect gate="C" pin="IO_6" pad="F16"/>
<connect gate="C" pin="IO_7" pad="G10"/>
<connect gate="C" pin="IO_8" pad="G11"/>
<connect gate="C" pin="IO_9" pad="G12"/>
<connect gate="C" pin="MSEL0" pad="J13"/>
<connect gate="C" pin="MSEL1" pad="K12"/>
<connect gate="C" pin="NC" pad="J10"/>
<connect gate="C" pin="NC_2" pad="F13"/>
<connect gate="C" pin="NC_3" pad="K13"/>
<connect gate="C" pin="NC_4" pad="E13"/>
<connect gate="C" pin="NC_5" pad="F14"/>
<connect gate="C" pin="NC_6" pad="E15"/>
<connect gate="C" pin="NSTATUS" pad="M13"/>
<connect gate="C" pin="VCCA_PLL2" pad="E12"/>
<connect gate="C" pin="VCCD_PLL2" pad="F11"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO2" pad="E10"/>
<connect gate="C" pin="VCCIO3" pad="R16"/>
<connect gate="C" pin="VCCIO3_2" pad="G14"/>
<connect gate="C" pin="VCCIO3_3" pad="K14"/>
<connect gate="C" pin="VCCIO4" pad="M10"/>
<connect gate="C" pin="VCCIO4_2" pad="P10"/>
<connect gate="C" pin="VCCIO4_3" pad="T15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C5F256C8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0544"/>
<attribute name="PACKAGE" value="FBGA-256"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C5Q208C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP2C5Q208C8N_A"/>
<gate name="B" symbol="EP2C5Q208C8N_B"/>
<gate name="C" symbol="EP2C5Q208C8N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CLK0" pad="23"/>
<connect gate="A" pin="CLK1" pad="24"/>
<connect gate="A" pin="CLK2" pad="27"/>
<connect gate="A" pin="CLK3" pad="28"/>
<connect gate="A" pin="DATA0" pad="20"/>
<connect gate="A" pin="DCLK" pad="21"/>
<connect gate="A" pin="GND" pad="65"/>
<connect gate="A" pin="GNDA_PLL1" pad="54"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="38"/>
<connect gate="A" pin="GND_4" pad="25"/>
<connect gate="A" pin="GND_5" pad="49"/>
<connect gate="A" pin="GND_6" pad="55"/>
<connect gate="A" pin="GND_PLL1" pad="52"/>
<connect gate="A" pin="GND_PLL1_2" pad="50"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="30"/>
<connect gate="A" pin="IO_16" pad="31"/>
<connect gate="A" pin="IO_17" pad="32"/>
<connect gate="A" pin="IO_18" pad="33"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_27" pad="44"/>
<connect gate="A" pin="IO_28" pad="45"/>
<connect gate="A" pin="IO_29" pad="46"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="47"/>
<connect gate="A" pin="IO_31" pad="48"/>
<connect gate="A" pin="IO_32" pad="56"/>
<connect gate="A" pin="IO_33" pad="57"/>
<connect gate="A" pin="IO_34" pad="58"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="8"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="NCE" pad="22"/>
<connect gate="A" pin="NCONFIG" pad="26"/>
<connect gate="A" pin="TCK" pad="18"/>
<connect gate="A" pin="TDI" pad="19"/>
<connect gate="A" pin="TDO" pad="16"/>
<connect gate="A" pin="TMS" pad="17"/>
<connect gate="A" pin="VCCA_PLL1" pad="53"/>
<connect gate="A" pin="VCCD_PLL1" pad="51"/>
<connect gate="A" pin="VCCINT" pad="66"/>
<connect gate="A" pin="VCCIO1" pad="42"/>
<connect gate="A" pin="VCCIO1_2" pad="7"/>
<connect gate="A" pin="VCCIO1_3" pad="29"/>
<connect gate="A" pin="VCCIO4" pad="62"/>
<connect gate="B" pin="CLK4" pad="132"/>
<connect gate="B" pin="CLK5" pad="131"/>
<connect gate="B" pin="CLK6" pad="130"/>
<connect gate="B" pin="CLK7" pad="129"/>
<connect gate="B" pin="CONF_DONE" pad="123"/>
<connect gate="B" pin="GND" pad="100"/>
<connect gate="B" pin="GND_2" pad="140"/>
<connect gate="B" pin="GND_3" pad="73"/>
<connect gate="B" pin="GND_4" pad="124"/>
<connect gate="B" pin="GND_5" pad="78"/>
<connect gate="B" pin="GND_6" pad="93"/>
<connect gate="B" pin="GND_7" pad="111"/>
<connect gate="B" pin="GND_8" pad="85"/>
<connect gate="B" pin="IO" pad="139"/>
<connect gate="B" pin="IO_10" pad="84"/>
<connect gate="B" pin="IO_11" pad="86"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="88"/>
<connect gate="B" pin="IO_14" pad="89"/>
<connect gate="B" pin="IO_15" pad="90"/>
<connect gate="B" pin="IO_16" pad="92"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="72"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="99"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="110"/>
<connect gate="B" pin="IO_31" pad="112"/>
<connect gate="B" pin="IO_32" pad="113"/>
<connect gate="B" pin="IO_33" pad="114"/>
<connect gate="B" pin="IO_34" pad="115"/>
<connect gate="B" pin="IO_35" pad="116"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="133"/>
<connect gate="B" pin="IO_43" pad="134"/>
<connect gate="B" pin="IO_44" pad="135"/>
<connect gate="B" pin="IO_45" pad="137"/>
<connect gate="B" pin="IO_46" pad="138"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_6" pad="77"/>
<connect gate="B" pin="IO_7" pad="80"/>
<connect gate="B" pin="IO_8" pad="81"/>
<connect gate="B" pin="IO_9" pad="82"/>
<connect gate="B" pin="MSEL0" pad="126"/>
<connect gate="B" pin="MSEL1" pad="125"/>
<connect gate="B" pin="NSTATUS" pad="121"/>
<connect gate="B" pin="VCCINT" pad="79"/>
<connect gate="B" pin="VCCIO3" pad="122"/>
<connect gate="B" pin="VCCIO3_2" pad="109"/>
<connect gate="B" pin="VCCIO3_3" pad="136"/>
<connect gate="B" pin="VCCIO4" pad="98"/>
<connect gate="B" pin="VCCIO4_2" pad="71"/>
<connect gate="B" pin="VCCIO4_3" pad="83"/>
<connect gate="B" pin="VCCIO4_4" pad="91"/>
<connect gate="C" pin="GND" pad="196"/>
<connect gate="C" pin="GNDA_PLL2" pad="158"/>
<connect gate="C" pin="GND_2" pad="159"/>
<connect gate="C" pin="GND_3" pad="167"/>
<connect gate="C" pin="GND_4" pad="174"/>
<connect gate="C" pin="GND_5" pad="177"/>
<connect gate="C" pin="GND_6" pad="204"/>
<connect gate="C" pin="GND_7" pad="184"/>
<connect gate="C" pin="GND_8" pad="153"/>
<connect gate="C" pin="GND_9" pad="186"/>
<connect gate="C" pin="GND_PLL2" pad="156"/>
<connect gate="C" pin="GND_PLL2_2" pad="154"/>
<connect gate="C" pin="IO" pad="208"/>
<connect gate="C" pin="IO_10" pad="150"/>
<connect gate="C" pin="IO_11" pad="151"/>
<connect gate="C" pin="IO_12" pad="152"/>
<connect gate="C" pin="IO_13" pad="160"/>
<connect gate="C" pin="IO_14" pad="161"/>
<connect gate="C" pin="IO_15" pad="162"/>
<connect gate="C" pin="IO_16" pad="163"/>
<connect gate="C" pin="IO_17" pad="164"/>
<connect gate="C" pin="IO_18" pad="165"/>
<connect gate="C" pin="IO_19" pad="168"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="169"/>
<connect gate="C" pin="IO_21" pad="170"/>
<connect gate="C" pin="IO_22" pad="171"/>
<connect gate="C" pin="IO_23" pad="173"/>
<connect gate="C" pin="IO_24" pad="175"/>
<connect gate="C" pin="IO_25" pad="176"/>
<connect gate="C" pin="IO_26" pad="179"/>
<connect gate="C" pin="IO_27" pad="180"/>
<connect gate="C" pin="IO_28" pad="181"/>
<connect gate="C" pin="IO_29" pad="182"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="185"/>
<connect gate="C" pin="IO_31" pad="187"/>
<connect gate="C" pin="IO_32" pad="188"/>
<connect gate="C" pin="IO_33" pad="189"/>
<connect gate="C" pin="IO_34" pad="191"/>
<connect gate="C" pin="IO_35" pad="192"/>
<connect gate="C" pin="IO_36" pad="193"/>
<connect gate="C" pin="IO_37" pad="195"/>
<connect gate="C" pin="IO_38" pad="197"/>
<connect gate="C" pin="IO_39" pad="198"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_40" pad="199"/>
<connect gate="C" pin="IO_41" pad="200"/>
<connect gate="C" pin="IO_42" pad="201"/>
<connect gate="C" pin="IO_43" pad="203"/>
<connect gate="C" pin="IO_44" pad="205"/>
<connect gate="C" pin="IO_45" pad="206"/>
<connect gate="C" pin="IO_46" pad="207"/>
<connect gate="C" pin="IO_5" pad="144"/>
<connect gate="C" pin="IO_6" pad="145"/>
<connect gate="C" pin="IO_7" pad="146"/>
<connect gate="C" pin="IO_8" pad="147"/>
<connect gate="C" pin="IO_9" pad="149"/>
<connect gate="C" pin="VCCA_PLL2" pad="157"/>
<connect gate="C" pin="VCCD_PLL2" pad="155"/>
<connect gate="C" pin="VCCINT" pad="190"/>
<connect gate="C" pin="VCCINT_2" pad="178"/>
<connect gate="C" pin="VCCIO2" pad="202"/>
<connect gate="C" pin="VCCIO2_2" pad="183"/>
<connect gate="C" pin="VCCIO2_3" pad="166"/>
<connect gate="C" pin="VCCIO2_4" pad="172"/>
<connect gate="C" pin="VCCIO2_5" pad="194"/>
<connect gate="C" pin="VCCIO3" pad="148"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C5Q208C8N"/>
<attribute name="OC_FARNELL" value="1635081"/>
<attribute name="OC_NEWARK" value="51R0567"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C5Q208I8">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP2C5Q208I8_A"/>
<gate name="B" symbol="EP2C5Q208I8_B"/>
<gate name="C" symbol="EP2C5Q208I8_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CLK0" pad="23"/>
<connect gate="A" pin="CLK1" pad="24"/>
<connect gate="A" pin="CLK2" pad="27"/>
<connect gate="A" pin="CLK3" pad="28"/>
<connect gate="A" pin="DATA0" pad="20"/>
<connect gate="A" pin="DCLK" pad="21"/>
<connect gate="A" pin="GND" pad="65"/>
<connect gate="A" pin="GNDA_PLL1" pad="54"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="25"/>
<connect gate="A" pin="GND_4" pad="55"/>
<connect gate="A" pin="GND_5" pad="49"/>
<connect gate="A" pin="GND_6" pad="38"/>
<connect gate="A" pin="GND_PLL1" pad="52"/>
<connect gate="A" pin="GND_PLL1_2" pad="50"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="30"/>
<connect gate="A" pin="IO_16" pad="31"/>
<connect gate="A" pin="IO_17" pad="32"/>
<connect gate="A" pin="IO_18" pad="33"/>
<connect gate="A" pin="IO_19" pad="34"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="35"/>
<connect gate="A" pin="IO_21" pad="36"/>
<connect gate="A" pin="IO_22" pad="37"/>
<connect gate="A" pin="IO_23" pad="39"/>
<connect gate="A" pin="IO_24" pad="40"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_27" pad="44"/>
<connect gate="A" pin="IO_28" pad="45"/>
<connect gate="A" pin="IO_29" pad="46"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="47"/>
<connect gate="A" pin="IO_31" pad="48"/>
<connect gate="A" pin="IO_32" pad="56"/>
<connect gate="A" pin="IO_33" pad="57"/>
<connect gate="A" pin="IO_34" pad="58"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="8"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="NCE" pad="22"/>
<connect gate="A" pin="NCONFIG" pad="26"/>
<connect gate="A" pin="TCK" pad="18"/>
<connect gate="A" pin="TDI" pad="19"/>
<connect gate="A" pin="TDO" pad="16"/>
<connect gate="A" pin="TMS" pad="17"/>
<connect gate="A" pin="VCCA_PLL1" pad="53"/>
<connect gate="A" pin="VCCD_PLL1" pad="51"/>
<connect gate="A" pin="VCCINT" pad="66"/>
<connect gate="A" pin="VCCIO1" pad="42"/>
<connect gate="A" pin="VCCIO1_2" pad="29"/>
<connect gate="A" pin="VCCIO1_3" pad="7"/>
<connect gate="A" pin="VCCIO4" pad="62"/>
<connect gate="B" pin="CLK4" pad="132"/>
<connect gate="B" pin="CLK5" pad="131"/>
<connect gate="B" pin="CLK6" pad="130"/>
<connect gate="B" pin="CLK7" pad="129"/>
<connect gate="B" pin="CONF_DONE" pad="123"/>
<connect gate="B" pin="GND" pad="78"/>
<connect gate="B" pin="GND_2" pad="140"/>
<connect gate="B" pin="GND_3" pad="85"/>
<connect gate="B" pin="GND_4" pad="100"/>
<connect gate="B" pin="GND_5" pad="111"/>
<connect gate="B" pin="GND_6" pad="124"/>
<connect gate="B" pin="GND_7" pad="73"/>
<connect gate="B" pin="GND_8" pad="93"/>
<connect gate="B" pin="IO" pad="139"/>
<connect gate="B" pin="IO_10" pad="84"/>
<connect gate="B" pin="IO_11" pad="86"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="88"/>
<connect gate="B" pin="IO_14" pad="89"/>
<connect gate="B" pin="IO_15" pad="90"/>
<connect gate="B" pin="IO_16" pad="92"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="72"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="99"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="110"/>
<connect gate="B" pin="IO_31" pad="112"/>
<connect gate="B" pin="IO_32" pad="113"/>
<connect gate="B" pin="IO_33" pad="114"/>
<connect gate="B" pin="IO_34" pad="115"/>
<connect gate="B" pin="IO_35" pad="116"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="127"/>
<connect gate="B" pin="IO_41" pad="128"/>
<connect gate="B" pin="IO_42" pad="133"/>
<connect gate="B" pin="IO_43" pad="134"/>
<connect gate="B" pin="IO_44" pad="135"/>
<connect gate="B" pin="IO_45" pad="137"/>
<connect gate="B" pin="IO_46" pad="138"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_6" pad="77"/>
<connect gate="B" pin="IO_7" pad="80"/>
<connect gate="B" pin="IO_8" pad="81"/>
<connect gate="B" pin="IO_9" pad="82"/>
<connect gate="B" pin="MSEL0" pad="126"/>
<connect gate="B" pin="MSEL1" pad="125"/>
<connect gate="B" pin="NSTATUS" pad="121"/>
<connect gate="B" pin="VCCINT" pad="79"/>
<connect gate="B" pin="VCCIO3" pad="136"/>
<connect gate="B" pin="VCCIO3_2" pad="109"/>
<connect gate="B" pin="VCCIO3_3" pad="122"/>
<connect gate="B" pin="VCCIO4" pad="98"/>
<connect gate="B" pin="VCCIO4_2" pad="71"/>
<connect gate="B" pin="VCCIO4_3" pad="83"/>
<connect gate="B" pin="VCCIO4_4" pad="91"/>
<connect gate="C" pin="GND" pad="159"/>
<connect gate="C" pin="GNDA_PLL2" pad="158"/>
<connect gate="C" pin="GND_2" pad="204"/>
<connect gate="C" pin="GND_3" pad="153"/>
<connect gate="C" pin="GND_4" pad="196"/>
<connect gate="C" pin="GND_5" pad="184"/>
<connect gate="C" pin="GND_6" pad="174"/>
<connect gate="C" pin="GND_7" pad="186"/>
<connect gate="C" pin="GND_8" pad="177"/>
<connect gate="C" pin="GND_9" pad="167"/>
<connect gate="C" pin="GND_PLL2" pad="154"/>
<connect gate="C" pin="GND_PLL2_2" pad="156"/>
<connect gate="C" pin="IO" pad="208"/>
<connect gate="C" pin="IO_10" pad="150"/>
<connect gate="C" pin="IO_11" pad="151"/>
<connect gate="C" pin="IO_12" pad="152"/>
<connect gate="C" pin="IO_13" pad="160"/>
<connect gate="C" pin="IO_14" pad="161"/>
<connect gate="C" pin="IO_15" pad="162"/>
<connect gate="C" pin="IO_16" pad="163"/>
<connect gate="C" pin="IO_17" pad="164"/>
<connect gate="C" pin="IO_18" pad="165"/>
<connect gate="C" pin="IO_19" pad="168"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="169"/>
<connect gate="C" pin="IO_21" pad="170"/>
<connect gate="C" pin="IO_22" pad="171"/>
<connect gate="C" pin="IO_23" pad="173"/>
<connect gate="C" pin="IO_24" pad="175"/>
<connect gate="C" pin="IO_25" pad="176"/>
<connect gate="C" pin="IO_26" pad="179"/>
<connect gate="C" pin="IO_27" pad="180"/>
<connect gate="C" pin="IO_28" pad="181"/>
<connect gate="C" pin="IO_29" pad="182"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="185"/>
<connect gate="C" pin="IO_31" pad="187"/>
<connect gate="C" pin="IO_32" pad="188"/>
<connect gate="C" pin="IO_33" pad="189"/>
<connect gate="C" pin="IO_34" pad="191"/>
<connect gate="C" pin="IO_35" pad="192"/>
<connect gate="C" pin="IO_36" pad="193"/>
<connect gate="C" pin="IO_37" pad="195"/>
<connect gate="C" pin="IO_38" pad="197"/>
<connect gate="C" pin="IO_39" pad="198"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_40" pad="199"/>
<connect gate="C" pin="IO_41" pad="200"/>
<connect gate="C" pin="IO_42" pad="201"/>
<connect gate="C" pin="IO_43" pad="203"/>
<connect gate="C" pin="IO_44" pad="205"/>
<connect gate="C" pin="IO_45" pad="206"/>
<connect gate="C" pin="IO_46" pad="207"/>
<connect gate="C" pin="IO_5" pad="144"/>
<connect gate="C" pin="IO_6" pad="145"/>
<connect gate="C" pin="IO_7" pad="146"/>
<connect gate="C" pin="IO_8" pad="147"/>
<connect gate="C" pin="IO_9" pad="149"/>
<connect gate="C" pin="VCCA_PLL2" pad="157"/>
<connect gate="C" pin="VCCD_PLL2" pad="155"/>
<connect gate="C" pin="VCCINT" pad="178"/>
<connect gate="C" pin="VCCINT_2" pad="190"/>
<connect gate="C" pin="VCCIO2" pad="202"/>
<connect gate="C" pin="VCCIO2_2" pad="166"/>
<connect gate="C" pin="VCCIO2_3" pad="183"/>
<connect gate="C" pin="VCCIO2_4" pad="194"/>
<connect gate="C" pin="VCCIO2_5" pad="172"/>
<connect gate="C" pin="VCCIO3" pad="148"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C5Q208I8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R0550"/>
<attribute name="PACKAGE" value="QFP-208"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C5T144C8N">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP2C5T144C8N_A"/>
<gate name="B" symbol="EP2C5T144C8N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLK0" pad="17"/>
<connect gate="A" pin="CLK1" pad="18"/>
<connect gate="A" pin="CLK2" pad="21"/>
<connect gate="A" pin="CLK3" pad="22"/>
<connect gate="A" pin="DATA0" pad="14"/>
<connect gate="A" pin="DCLK" pad="15"/>
<connect gate="A" pin="GND" pad="33"/>
<connect gate="A" pin="GNDA_PLL1" pad="38"/>
<connect gate="A" pin="GND_2" pad="19"/>
<connect gate="A" pin="GND_3" pad="68"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="GND_5" pad="49"/>
<connect gate="A" pin="GND_6" pad="39"/>
<connect gate="A" pin="GND_7" pad="56"/>
<connect gate="A" pin="GND_8" pad="61"/>
<connect gate="A" pin="GND_PLL1" pad="36"/>
<connect gate="A" pin="GND_PLL1_2" pad="34"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="25"/>
<connect gate="A" pin="IO_11" pad="26"/>
<connect gate="A" pin="IO_12" pad="27"/>
<connect gate="A" pin="IO_13" pad="28"/>
<connect gate="A" pin="IO_14" pad="30"/>
<connect gate="A" pin="IO_15" pad="31"/>
<connect gate="A" pin="IO_16" pad="32"/>
<connect gate="A" pin="IO_17" pad="40"/>
<connect gate="A" pin="IO_18" pad="41"/>
<connect gate="A" pin="IO_19" pad="42"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="43"/>
<connect gate="A" pin="IO_21" pad="44"/>
<connect gate="A" pin="IO_22" pad="45"/>
<connect gate="A" pin="IO_23" pad="47"/>
<connect gate="A" pin="IO_24" pad="48"/>
<connect gate="A" pin="IO_25" pad="51"/>
<connect gate="A" pin="IO_26" pad="52"/>
<connect gate="A" pin="IO_27" pad="53"/>
<connect gate="A" pin="IO_28" pad="55"/>
<connect gate="A" pin="IO_29" pad="57"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="58"/>
<connect gate="A" pin="IO_31" pad="59"/>
<connect gate="A" pin="IO_32" pad="60"/>
<connect gate="A" pin="IO_33" pad="63"/>
<connect gate="A" pin="IO_34" pad="64"/>
<connect gate="A" pin="IO_35" pad="65"/>
<connect gate="A" pin="IO_36" pad="67"/>
<connect gate="A" pin="IO_37" pad="69"/>
<connect gate="A" pin="IO_38" pad="70"/>
<connect gate="A" pin="IO_39" pad="71"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="24"/>
<connect gate="A" pin="NCE" pad="16"/>
<connect gate="A" pin="NCONFIG" pad="20"/>
<connect gate="A" pin="TCK" pad="12"/>
<connect gate="A" pin="TDI" pad="13"/>
<connect gate="A" pin="TDO" pad="10"/>
<connect gate="A" pin="TMS" pad="11"/>
<connect gate="A" pin="VCCA_PLL1" pad="37"/>
<connect gate="A" pin="VCCD_PLL1" pad="35"/>
<connect gate="A" pin="VCCINT" pad="50"/>
<connect gate="A" pin="VCCINT_2" pad="62"/>
<connect gate="A" pin="VCCIO1" pad="29"/>
<connect gate="A" pin="VCCIO1_2" pad="23"/>
<connect gate="A" pin="VCCIO1_3" pad="5"/>
<connect gate="A" pin="VCCIO4" pad="46"/>
<connect gate="A" pin="VCCIO4_2" pad="54"/>
<connect gate="A" pin="VCCIO4_3" pad="66"/>
<connect gate="B" pin="CLK4" pad="91"/>
<connect gate="B" pin="CLK5" pad="90"/>
<connect gate="B" pin="CLK6" pad="89"/>
<connect gate="B" pin="CLK7" pad="88"/>
<connect gate="B" pin="CONF_DONE" pad="83"/>
<connect gate="B" pin="GND" pad="123"/>
<connect gate="B" pin="GNDA_PLL2" pad="110"/>
<connect gate="B" pin="GND_2" pad="128"/>
<connect gate="B" pin="GND_3" pad="140"/>
<connect gate="B" pin="GND_4" pad="98"/>
<connect gate="B" pin="GND_5" pad="78"/>
<connect gate="B" pin="GND_6" pad="105"/>
<connect gate="B" pin="GND_7" pad="117"/>
<connect gate="B" pin="GND_8" pad="130"/>
<connect gate="B" pin="GND_9" pad="111"/>
<connect gate="B" pin="GND_PLL2" pad="106"/>
<connect gate="B" pin="GND_PLL2_2" pad="108"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="92"/>
<connect gate="B" pin="IO_12" pad="93"/>
<connect gate="B" pin="IO_13" pad="94"/>
<connect gate="B" pin="IO_14" pad="96"/>
<connect gate="B" pin="IO_15" pad="97"/>
<connect gate="B" pin="IO_16" pad="99"/>
<connect gate="B" pin="IO_17" pad="100"/>
<connect gate="B" pin="IO_18" pad="101"/>
<connect gate="B" pin="IO_19" pad="103"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="104"/>
<connect gate="B" pin="IO_21" pad="112"/>
<connect gate="B" pin="IO_22" pad="113"/>
<connect gate="B" pin="IO_23" pad="114"/>
<connect gate="B" pin="IO_24" pad="115"/>
<connect gate="B" pin="IO_25" pad="118"/>
<connect gate="B" pin="IO_26" pad="119"/>
<connect gate="B" pin="IO_27" pad="120"/>
<connect gate="B" pin="IO_28" pad="121"/>
<connect gate="B" pin="IO_29" pad="122"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="125"/>
<connect gate="B" pin="IO_31" pad="126"/>
<connect gate="B" pin="IO_32" pad="129"/>
<connect gate="B" pin="IO_33" pad="132"/>
<connect gate="B" pin="IO_34" pad="133"/>
<connect gate="B" pin="IO_35" pad="134"/>
<connect gate="B" pin="IO_36" pad="135"/>
<connect gate="B" pin="IO_37" pad="136"/>
<connect gate="B" pin="IO_38" pad="137"/>
<connect gate="B" pin="IO_39" pad="139"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="141"/>
<connect gate="B" pin="IO_41" pad="142"/>
<connect gate="B" pin="IO_42" pad="143"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_6" pad="79"/>
<connect gate="B" pin="IO_7" pad="80"/>
<connect gate="B" pin="IO_8" pad="81"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="85"/>
<connect gate="B" pin="MSEL1" pad="84"/>
<connect gate="B" pin="NSTATUS" pad="82"/>
<connect gate="B" pin="VCCA_PLL2" pad="109"/>
<connect gate="B" pin="VCCD_PLL2" pad="107"/>
<connect gate="B" pin="VCCINT" pad="131"/>
<connect gate="B" pin="VCCINT_2" pad="124"/>
<connect gate="B" pin="VCCIO2" pad="116"/>
<connect gate="B" pin="VCCIO2_2" pad="127"/>
<connect gate="B" pin="VCCIO2_3" pad="138"/>
<connect gate="B" pin="VCCIO3" pad="102"/>
<connect gate="B" pin="VCCIO3_2" pad="77"/>
<connect gate="B" pin="VCCIO3_3" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C5T144C8N"/>
<attribute name="OC_FARNELL" value="1662263"/>
<attribute name="OC_NEWARK" value="51R0568"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C8Q208C8N">
<description>CYCLONE II FPGA</description>
<gates>
<gate name="A" symbol="EP2C8Q208C8N_A"/>
<gate name="B" symbol="EP2C8Q208C8N_B"/>
<gate name="C" symbol="EP2C8Q208C8N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CLK0" pad="23"/>
<connect gate="A" pin="CLK1" pad="24"/>
<connect gate="A" pin="CLK2" pad="27"/>
<connect gate="A" pin="CLK3" pad="28"/>
<connect gate="A" pin="DATA0" pad="20"/>
<connect gate="A" pin="DCLK" pad="21"/>
<connect gate="A" pin="GND" pad="65"/>
<connect gate="A" pin="GNDA_PLL1" pad="54"/>
<connect gate="A" pin="GND_2" pad="25"/>
<connect gate="A" pin="GND_3" pad="36"/>
<connect gate="A" pin="GND_4" pad="38"/>
<connect gate="A" pin="GND_5" pad="49"/>
<connect gate="A" pin="GND_6" pad="9"/>
<connect gate="A" pin="GND_7" pad="55"/>
<connect gate="A" pin="GND_PLL1" pad="50"/>
<connect gate="A" pin="GND_PLL1_2" pad="52"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="34"/>
<connect gate="A" pin="IO_12" pad="11"/>
<connect gate="A" pin="IO_13" pad="35"/>
<connect gate="A" pin="IO_14" pad="12"/>
<connect gate="A" pin="IO_15" pad="13"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="30"/>
<connect gate="A" pin="IO_18" pad="15"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="37"/>
<connect gate="A" pin="IO_21" pad="39"/>
<connect gate="A" pin="IO_22" pad="40"/>
<connect gate="A" pin="IO_23" pad="41"/>
<connect gate="A" pin="IO_24" pad="43"/>
<connect gate="A" pin="IO_25" pad="44"/>
<connect gate="A" pin="IO_26" pad="45"/>
<connect gate="A" pin="IO_27" pad="46"/>
<connect gate="A" pin="IO_28" pad="47"/>
<connect gate="A" pin="IO_29" pad="48"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="56"/>
<connect gate="A" pin="IO_31" pad="57"/>
<connect gate="A" pin="IO_32" pad="58"/>
<connect gate="A" pin="IO_33" pad="59"/>
<connect gate="A" pin="IO_34" pad="60"/>
<connect gate="A" pin="IO_35" pad="61"/>
<connect gate="A" pin="IO_36" pad="63"/>
<connect gate="A" pin="IO_37" pad="64"/>
<connect gate="A" pin="IO_38" pad="67"/>
<connect gate="A" pin="IO_39" pad="68"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="69"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="8"/>
<connect gate="A" pin="IO_9" pad="33"/>
<connect gate="A" pin="NCE" pad="22"/>
<connect gate="A" pin="NCONFIG" pad="26"/>
<connect gate="A" pin="TCK" pad="18"/>
<connect gate="A" pin="TDI" pad="19"/>
<connect gate="A" pin="TDO" pad="16"/>
<connect gate="A" pin="TMS" pad="17"/>
<connect gate="A" pin="VCCA_PLL1" pad="53"/>
<connect gate="A" pin="VCCD_PLL1" pad="51"/>
<connect gate="A" pin="VCCINT" pad="66"/>
<connect gate="A" pin="VCCINT_2" pad="32"/>
<connect gate="A" pin="VCCIO1" pad="29"/>
<connect gate="A" pin="VCCIO1_2" pad="42"/>
<connect gate="A" pin="VCCIO1_3" pad="7"/>
<connect gate="A" pin="VCCIO4" pad="62"/>
<connect gate="B" pin="CLK4" pad="132"/>
<connect gate="B" pin="CLK5" pad="131"/>
<connect gate="B" pin="CLK6" pad="130"/>
<connect gate="B" pin="CLK7" pad="129"/>
<connect gate="B" pin="CONF_DONE" pad="123"/>
<connect gate="B" pin="GND" pad="78"/>
<connect gate="B" pin="GND_2" pad="93"/>
<connect gate="B" pin="GND_3" pad="85"/>
<connect gate="B" pin="GND_4" pad="140"/>
<connect gate="B" pin="GND_5" pad="73"/>
<connect gate="B" pin="GND_6" pad="124"/>
<connect gate="B" pin="GND_7" pad="111"/>
<connect gate="B" pin="GND_8" pad="100"/>
<connect gate="B" pin="GND_9" pad="119"/>
<connect gate="B" pin="IO" pad="139"/>
<connect gate="B" pin="IO_10" pad="81"/>
<connect gate="B" pin="IO_11" pad="86"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="88"/>
<connect gate="B" pin="IO_14" pad="89"/>
<connect gate="B" pin="IO_15" pad="90"/>
<connect gate="B" pin="IO_16" pad="99"/>
<connect gate="B" pin="IO_17" pad="92"/>
<connect gate="B" pin="IO_18" pad="101"/>
<connect gate="B" pin="IO_19" pad="94"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="102"/>
<connect gate="B" pin="IO_21" pad="95"/>
<connect gate="B" pin="IO_22" pad="103"/>
<connect gate="B" pin="IO_23" pad="96"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="97"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="75"/>
<connect gate="B" pin="IO_30" pad="110"/>
<connect gate="B" pin="IO_31" pad="112"/>
<connect gate="B" pin="IO_32" pad="113"/>
<connect gate="B" pin="IO_33" pad="114"/>
<connect gate="B" pin="IO_34" pad="115"/>
<connect gate="B" pin="IO_35" pad="116"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="127"/>
<connect gate="B" pin="IO_39" pad="128"/>
<connect gate="B" pin="IO_4" pad="76"/>
<connect gate="B" pin="IO_40" pad="133"/>
<connect gate="B" pin="IO_41" pad="134"/>
<connect gate="B" pin="IO_42" pad="135"/>
<connect gate="B" pin="IO_43" pad="137"/>
<connect gate="B" pin="IO_44" pad="138"/>
<connect gate="B" pin="IO_5" pad="77"/>
<connect gate="B" pin="IO_6" pad="82"/>
<connect gate="B" pin="IO_7" pad="72"/>
<connect gate="B" pin="IO_8" pad="80"/>
<connect gate="B" pin="IO_9" pad="84"/>
<connect gate="B" pin="MSEL0" pad="126"/>
<connect gate="B" pin="MSEL1" pad="125"/>
<connect gate="B" pin="NSTATUS" pad="121"/>
<connect gate="B" pin="VCCINT" pad="79"/>
<connect gate="B" pin="VCCINT_2" pad="120"/>
<connect gate="B" pin="VCCIO3" pad="122"/>
<connect gate="B" pin="VCCIO3_2" pad="109"/>
<connect gate="B" pin="VCCIO3_3" pad="136"/>
<connect gate="B" pin="VCCIO4" pad="71"/>
<connect gate="B" pin="VCCIO4_2" pad="98"/>
<connect gate="B" pin="VCCIO4_3" pad="91"/>
<connect gate="B" pin="VCCIO4_4" pad="83"/>
<connect gate="C" pin="GND" pad="196"/>
<connect gate="C" pin="GNDA_PLL2" pad="158"/>
<connect gate="C" pin="GND_2" pad="177"/>
<connect gate="C" pin="GND_3" pad="174"/>
<connect gate="C" pin="GND_4" pad="167"/>
<connect gate="C" pin="GND_5" pad="184"/>
<connect gate="C" pin="GND_6" pad="186"/>
<connect gate="C" pin="GND_7" pad="204"/>
<connect gate="C" pin="GND_8" pad="153"/>
<connect gate="C" pin="GND_9" pad="159"/>
<connect gate="C" pin="GND_PLL2" pad="154"/>
<connect gate="C" pin="GND_PLL2_2" pad="156"/>
<connect gate="C" pin="IO" pad="208"/>
<connect gate="C" pin="IO_10" pad="150"/>
<connect gate="C" pin="IO_11" pad="151"/>
<connect gate="C" pin="IO_12" pad="152"/>
<connect gate="C" pin="IO_13" pad="160"/>
<connect gate="C" pin="IO_14" pad="161"/>
<connect gate="C" pin="IO_15" pad="162"/>
<connect gate="C" pin="IO_16" pad="163"/>
<connect gate="C" pin="IO_17" pad="168"/>
<connect gate="C" pin="IO_18" pad="164"/>
<connect gate="C" pin="IO_19" pad="169"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="170"/>
<connect gate="C" pin="IO_21" pad="173"/>
<connect gate="C" pin="IO_22" pad="165"/>
<connect gate="C" pin="IO_23" pad="171"/>
<connect gate="C" pin="IO_24" pad="175"/>
<connect gate="C" pin="IO_25" pad="176"/>
<connect gate="C" pin="IO_26" pad="179"/>
<connect gate="C" pin="IO_27" pad="180"/>
<connect gate="C" pin="IO_28" pad="181"/>
<connect gate="C" pin="IO_29" pad="182"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="185"/>
<connect gate="C" pin="IO_31" pad="187"/>
<connect gate="C" pin="IO_32" pad="188"/>
<connect gate="C" pin="IO_33" pad="189"/>
<connect gate="C" pin="IO_34" pad="191"/>
<connect gate="C" pin="IO_35" pad="192"/>
<connect gate="C" pin="IO_36" pad="193"/>
<connect gate="C" pin="IO_37" pad="195"/>
<connect gate="C" pin="IO_38" pad="197"/>
<connect gate="C" pin="IO_39" pad="198"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_40" pad="199"/>
<connect gate="C" pin="IO_41" pad="200"/>
<connect gate="C" pin="IO_42" pad="201"/>
<connect gate="C" pin="IO_43" pad="203"/>
<connect gate="C" pin="IO_44" pad="205"/>
<connect gate="C" pin="IO_45" pad="206"/>
<connect gate="C" pin="IO_46" pad="207"/>
<connect gate="C" pin="IO_5" pad="144"/>
<connect gate="C" pin="IO_6" pad="145"/>
<connect gate="C" pin="IO_7" pad="146"/>
<connect gate="C" pin="IO_8" pad="147"/>
<connect gate="C" pin="IO_9" pad="149"/>
<connect gate="C" pin="VCCA_PLL2" pad="157"/>
<connect gate="C" pin="VCCD_PLL2" pad="155"/>
<connect gate="C" pin="VCCINT" pad="190"/>
<connect gate="C" pin="VCCINT_2" pad="178"/>
<connect gate="C" pin="VCCIO2" pad="202"/>
<connect gate="C" pin="VCCIO2_2" pad="183"/>
<connect gate="C" pin="VCCIO2_3" pad="172"/>
<connect gate="C" pin="VCCIO2_4" pad="166"/>
<connect gate="C" pin="VCCIO2_5" pad="194"/>
<connect gate="C" pin="VCCIO3" pad="148"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C8Q208C8N"/>
<attribute name="OC_FARNELL" value="1453484"/>
<attribute name="OC_NEWARK" value="51R0575"/>
<attribute name="PACKAGE" value="QFP-208"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C8T144C8N">
<description>CYCLONE II FPGA</description>
<gates>
<gate name="A" symbol="EP2C8T144C8N_A"/>
<gate name="B" symbol="EP2C8T144C8N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLK0" pad="17"/>
<connect gate="A" pin="CLK1" pad="18"/>
<connect gate="A" pin="CLK2" pad="21"/>
<connect gate="A" pin="CLK3" pad="22"/>
<connect gate="A" pin="DATA0" pad="14"/>
<connect gate="A" pin="DCLK" pad="15"/>
<connect gate="A" pin="GND" pad="61"/>
<connect gate="A" pin="GNDA_PLL1" pad="38"/>
<connect gate="A" pin="GND_2" pad="39"/>
<connect gate="A" pin="GND_3" pad="27"/>
<connect gate="A" pin="GND_4" pad="68"/>
<connect gate="A" pin="GND_5" pad="6"/>
<connect gate="A" pin="GND_6" pad="33"/>
<connect gate="A" pin="GND_7" pad="56"/>
<connect gate="A" pin="GND_8" pad="19"/>
<connect gate="A" pin="GND_9" pad="49"/>
<connect gate="A" pin="GND_PLL1" pad="36"/>
<connect gate="A" pin="GND_PLL1_2" pad="34"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="25"/>
<connect gate="A" pin="IO_11" pad="4"/>
<connect gate="A" pin="IO_12" pad="7"/>
<connect gate="A" pin="IO_13" pad="8"/>
<connect gate="A" pin="IO_14" pad="9"/>
<connect gate="A" pin="IO_15" pad="40"/>
<connect gate="A" pin="IO_16" pad="41"/>
<connect gate="A" pin="IO_17" pad="42"/>
<connect gate="A" pin="IO_18" pad="43"/>
<connect gate="A" pin="IO_19" pad="44"/>
<connect gate="A" pin="IO_2" pad="31"/>
<connect gate="A" pin="IO_20" pad="45"/>
<connect gate="A" pin="IO_21" pad="47"/>
<connect gate="A" pin="IO_22" pad="48"/>
<connect gate="A" pin="IO_23" pad="51"/>
<connect gate="A" pin="IO_24" pad="52"/>
<connect gate="A" pin="IO_25" pad="53"/>
<connect gate="A" pin="IO_26" pad="55"/>
<connect gate="A" pin="IO_27" pad="57"/>
<connect gate="A" pin="IO_28" pad="58"/>
<connect gate="A" pin="IO_29" pad="59"/>
<connect gate="A" pin="IO_3" pad="1"/>
<connect gate="A" pin="IO_30" pad="60"/>
<connect gate="A" pin="IO_31" pad="63"/>
<connect gate="A" pin="IO_32" pad="64"/>
<connect gate="A" pin="IO_33" pad="65"/>
<connect gate="A" pin="IO_34" pad="67"/>
<connect gate="A" pin="IO_35" pad="69"/>
<connect gate="A" pin="IO_36" pad="70"/>
<connect gate="A" pin="IO_37" pad="71"/>
<connect gate="A" pin="IO_4" pad="28"/>
<connect gate="A" pin="IO_5" pad="32"/>
<connect gate="A" pin="IO_6" pad="2"/>
<connect gate="A" pin="IO_7" pad="24"/>
<connect gate="A" pin="IO_8" pad="30"/>
<connect gate="A" pin="IO_9" pad="3"/>
<connect gate="A" pin="NCE" pad="16"/>
<connect gate="A" pin="NCONFIG" pad="20"/>
<connect gate="A" pin="TCK" pad="12"/>
<connect gate="A" pin="TDI" pad="13"/>
<connect gate="A" pin="TDO" pad="10"/>
<connect gate="A" pin="TMS" pad="11"/>
<connect gate="A" pin="VCCA_PLL1" pad="37"/>
<connect gate="A" pin="VCCD_PLL1" pad="35"/>
<connect gate="A" pin="VCCINT" pad="26"/>
<connect gate="A" pin="VCCINT_2" pad="50"/>
<connect gate="A" pin="VCCINT_3" pad="62"/>
<connect gate="A" pin="VCCIO1" pad="23"/>
<connect gate="A" pin="VCCIO1_2" pad="5"/>
<connect gate="A" pin="VCCIO1_3" pad="29"/>
<connect gate="A" pin="VCCIO4" pad="66"/>
<connect gate="A" pin="VCCIO4_2" pad="54"/>
<connect gate="A" pin="VCCIO4_3" pad="46"/>
<connect gate="B" pin="CLK4" pad="91"/>
<connect gate="B" pin="CLK5" pad="90"/>
<connect gate="B" pin="CLK6" pad="89"/>
<connect gate="B" pin="CLK7" pad="88"/>
<connect gate="B" pin="CONF_DONE" pad="83"/>
<connect gate="B" pin="GND" pad="78"/>
<connect gate="B" pin="GNDA_PLL2" pad="110"/>
<connect gate="B" pin="GND_10" pad="140"/>
<connect gate="B" pin="GND_2" pad="111"/>
<connect gate="B" pin="GND_3" pad="128"/>
<connect gate="B" pin="GND_4" pad="130"/>
<connect gate="B" pin="GND_5" pad="98"/>
<connect gate="B" pin="GND_6" pad="117"/>
<connect gate="B" pin="GND_7" pad="123"/>
<connect gate="B" pin="GND_8" pad="80"/>
<connect gate="B" pin="GND_9" pad="105"/>
<connect gate="B" pin="GND_PLL2" pad="106"/>
<connect gate="B" pin="GND_PLL2_2" pad="108"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="79"/>
<connect gate="B" pin="IO_11" pad="99"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="100"/>
<connect gate="B" pin="IO_14" pad="75"/>
<connect gate="B" pin="IO_15" pad="101"/>
<connect gate="B" pin="IO_16" pad="76"/>
<connect gate="B" pin="IO_17" pad="103"/>
<connect gate="B" pin="IO_18" pad="104"/>
<connect gate="B" pin="IO_19" pad="112"/>
<connect gate="B" pin="IO_2" pad="92"/>
<connect gate="B" pin="IO_20" pad="113"/>
<connect gate="B" pin="IO_21" pad="114"/>
<connect gate="B" pin="IO_22" pad="115"/>
<connect gate="B" pin="IO_23" pad="118"/>
<connect gate="B" pin="IO_24" pad="119"/>
<connect gate="B" pin="IO_25" pad="120"/>
<connect gate="B" pin="IO_26" pad="121"/>
<connect gate="B" pin="IO_27" pad="122"/>
<connect gate="B" pin="IO_28" pad="125"/>
<connect gate="B" pin="IO_29" pad="126"/>
<connect gate="B" pin="IO_3" pad="93"/>
<connect gate="B" pin="IO_30" pad="129"/>
<connect gate="B" pin="IO_31" pad="132"/>
<connect gate="B" pin="IO_32" pad="133"/>
<connect gate="B" pin="IO_33" pad="134"/>
<connect gate="B" pin="IO_34" pad="135"/>
<connect gate="B" pin="IO_35" pad="136"/>
<connect gate="B" pin="IO_36" pad="137"/>
<connect gate="B" pin="IO_37" pad="139"/>
<connect gate="B" pin="IO_38" pad="141"/>
<connect gate="B" pin="IO_39" pad="142"/>
<connect gate="B" pin="IO_4" pad="73"/>
<connect gate="B" pin="IO_40" pad="143"/>
<connect gate="B" pin="IO_5" pad="94"/>
<connect gate="B" pin="IO_6" pad="96"/>
<connect gate="B" pin="IO_7" pad="74"/>
<connect gate="B" pin="IO_8" pad="97"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="85"/>
<connect gate="B" pin="MSEL1" pad="84"/>
<connect gate="B" pin="NSTATUS" pad="82"/>
<connect gate="B" pin="VCCA_PLL2" pad="109"/>
<connect gate="B" pin="VCCD_PLL2" pad="107"/>
<connect gate="B" pin="VCCINT" pad="124"/>
<connect gate="B" pin="VCCINT_2" pad="81"/>
<connect gate="B" pin="VCCINT_3" pad="131"/>
<connect gate="B" pin="VCCIO2" pad="127"/>
<connect gate="B" pin="VCCIO2_2" pad="116"/>
<connect gate="B" pin="VCCIO2_3" pad="138"/>
<connect gate="B" pin="VCCIO3" pad="102"/>
<connect gate="B" pin="VCCIO3_2" pad="77"/>
<connect gate="B" pin="VCCIO3_3" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2C8T144C8N"/>
<attribute name="OC_FARNELL" value="1453487"/>
<attribute name="OC_NEWARK" value="51R0576"/>
<attribute name="PACKAGE" value="Altera"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S15F484C3N">
<description>FPGA, STRATIX II</description>
<gates>
<gate name="A" symbol="EP2S15F484C3N_A"/>
<gate name="B" symbol="EP2S15F484C3N_B"/>
<gate name="C" symbol="EP2S15F484C3N_C"/>
<gate name="D" symbol="EP2S15F484C3N_D"/>
<gate name="E" symbol="EP2S15F484C3N_E"/>
</gates>
<devices>
<device name="" package="BGA484C100P22X22-2300X2300X350">
<connects>
<connect gate="A" pin="GND" pad="K9"/>
<connect gate="A" pin="GNDA_PLL4" pad="L5"/>
<connect gate="A" pin="GNDA_PLL4_2" pad="L4"/>
<connect gate="A" pin="GND_2" pad="A9"/>
<connect gate="A" pin="GND_3" pad="B2"/>
<connect gate="A" pin="GND_4" pad="A1"/>
<connect gate="A" pin="GND_5" pad="J1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="A8"/>
<connect gate="A" pin="IO_11" pad="C1"/>
<connect gate="A" pin="IO_12" pad="C4"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="C5"/>
<connect gate="A" pin="IO_15" pad="C6"/>
<connect gate="A" pin="IO_16" pad="C7"/>
<connect gate="A" pin="IO_17" pad="C8"/>
<connect gate="A" pin="IO_18" pad="C9"/>
<connect gate="A" pin="IO_19" pad="D1"/>
<connect gate="A" pin="IO_2" pad="B5"/>
<connect gate="A" pin="IO_20" pad="D2"/>
<connect gate="A" pin="IO_21" pad="D3"/>
<connect gate="A" pin="IO_22" pad="E6"/>
<connect gate="A" pin="IO_23" pad="D5"/>
<connect gate="A" pin="IO_24" pad="E7"/>
<connect gate="A" pin="IO_25" pad="D6"/>
<connect gate="A" pin="IO_26" pad="E8"/>
<connect gate="A" pin="IO_27" pad="E9"/>
<connect gate="A" pin="IO_28" pad="D8"/>
<connect gate="A" pin="IO_29" pad="F1"/>
<connect gate="A" pin="IO_3" pad="B6"/>
<connect gate="A" pin="IO_30" pad="F2"/>
<connect gate="A" pin="IO_31" pad="E1"/>
<connect gate="A" pin="IO_32" pad="E2"/>
<connect gate="A" pin="IO_33" pad="E3"/>
<connect gate="A" pin="IO_34" pad="E4"/>
<connect gate="A" pin="IO_35" pad="F4"/>
<connect gate="A" pin="IO_36" pad="F5"/>
<connect gate="A" pin="IO_37" pad="F6"/>
<connect gate="A" pin="IO_38" pad="F7"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="G9"/>
<connect gate="A" pin="IO_5" pad="B7"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="A6"/>
<connect gate="A" pin="IO_60" pad="J5"/>
<connect gate="A" pin="IO_61" pad="J6"/>
<connect gate="A" pin="IO_62" pad="J7"/>
<connect gate="A" pin="IO_63" pad="J8"/>
<connect gate="A" pin="IO_64" pad="K1"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_66" pad="K3"/>
<connect gate="A" pin="IO_67" pad="K4"/>
<connect gate="A" pin="IO_68" pad="K5"/>
<connect gate="A" pin="IO_69" pad="K6"/>
<connect gate="A" pin="IO_7" pad="B8"/>
<connect gate="A" pin="IO_70" pad="K7"/>
<connect gate="A" pin="IO_71" pad="K8"/>
<connect gate="A" pin="IO_72" pad="L2"/>
<connect gate="A" pin="IO_73" pad="L3"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="B9"/>
<connect gate="A" pin="MSEL0" pad="E5"/>
<connect gate="A" pin="MSEL1" pad="D4"/>
<connect gate="A" pin="MSEL2" pad="B4"/>
<connect gate="A" pin="MSEL3" pad="A4"/>
<connect gate="A" pin="TDO" pad="B3"/>
<connect gate="A" pin="TEMPDIODEN" pad="C3"/>
<connect gate="A" pin="TEMPDIODEP" pad="A2"/>
<connect gate="A" pin="VCCD_PLL4" pad="L6"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="B1"/>
<connect gate="A" pin="VREFB4N0" pad="D7"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N0" pad="J4"/>
<connect gate="A" pin="VREFB5N1" pad="F3"/>
<connect gate="B" pin="CLK11N" pad="M3"/>
<connect gate="B" pin="CLK11P" pad="M2"/>
<connect gate="B" pin="CLK9N" pad="N4"/>
<connect gate="B" pin="CLK9P" pad="N3"/>
<connect gate="B" pin="GND" pad="A22"/>
<connect gate="B" pin="GNDA_PLL3" pad="N6"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="N5"/>
<connect gate="B" pin="GND_2" pad="M7"/>
<connect gate="B" pin="GND_3" pad="A14"/>
<connect gate="B" pin="GND_4" pad="M9"/>
<connect gate="B" pin="GND_5" pad="P1"/>
<connect gate="B" pin="IO" pad="A19"/>
<connect gate="B" pin="IO_10" pad="P7"/>
<connect gate="B" pin="IO_11" pad="N2"/>
<connect gate="B" pin="IO_12" pad="P8"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="R2"/>
<connect gate="B" pin="IO_15" pad="R3"/>
<connect gate="B" pin="IO_16" pad="R4"/>
<connect gate="B" pin="IO_17" pad="R5"/>
<connect gate="B" pin="IO_18" pad="R6"/>
<connect gate="B" pin="IO_19" pad="R7"/>
<connect gate="B" pin="IO_2" pad="P2"/>
<connect gate="B" pin="IO_20" pad="R8"/>
<connect gate="B" pin="IO_21" pad="R9"/>
<connect gate="B" pin="IO_22" pad="T1"/>
<connect gate="B" pin="IO_23" pad="T2"/>
<connect gate="B" pin="IO_24" pad="T3"/>
<connect gate="B" pin="IO_25" pad="T4"/>
<connect gate="B" pin="IO_26" pad="T5"/>
<connect gate="B" pin="IO_27" pad="T6"/>
<connect gate="B" pin="IO_28" pad="T7"/>
<connect gate="B" pin="IO_29" pad="T8"/>
<connect gate="B" pin="IO_3" pad="P3"/>
<connect gate="B" pin="IO_30" pad="T9"/>
<connect gate="B" pin="IO_31" pad="U1"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="N1"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V3"/>
<connect gate="B" pin="IO_42" pad="V4"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="V9"/>
<connect gate="B" pin="IO_47" pad="W1"/>
<connect gate="B" pin="IO_48" pad="W2"/>
<connect gate="B" pin="IO_49" pad="W3"/>
<connect gate="B" pin="IO_5" pad="N7"/>
<connect gate="B" pin="IO_50" pad="W4"/>
<connect gate="B" pin="IO_51" pad="W5"/>
<connect gate="B" pin="IO_52" pad="W7"/>
<connect gate="B" pin="IO_53" pad="W9"/>
<connect gate="B" pin="IO_54" pad="Y1"/>
<connect gate="B" pin="IO_55" pad="Y2"/>
<connect gate="B" pin="IO_56" pad="Y3"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="P5"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A13"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_7" pad="L8"/>
<connect gate="B" pin="IO_8" pad="P6"/>
<connect gate="B" pin="IO_9" pad="N8"/>
<connect gate="B" pin="NCE" pad="A21"/>
<connect gate="B" pin="PLL_ENA" pad="Y4"/>
<connect gate="B" pin="PORSEL" pad="V5"/>
<connect gate="B" pin="VCCA_PLL3" pad="M4"/>
<connect gate="B" pin="VCCA_PLL4" pad="M6"/>
<connect gate="B" pin="VCCD_PLL3" pad="M5"/>
<connect gate="B" pin="VCCINT" pad="P9"/>
<connect gate="B" pin="VCCINT_2" pad="M8"/>
<connect gate="B" pin="VCCIO3" pad="A12"/>
<connect gate="B" pin="VCCIO3_2" pad="A20"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="M1"/>
<connect gate="B" pin="VCCIO6_2" pad="AA1"/>
<connect gate="B" pin="VCCPD5" pad="L9"/>
<connect gate="B" pin="VCCPD6" pad="N9"/>
<connect gate="B" pin="VREFB6N0" pad="U3"/>
<connect gate="B" pin="VREFB6N1" pad="P4"/>
<connect gate="B" pin="VREFB7N0" pad="W8"/>
<connect gate="B" pin="VREFB7N1" pad="W6"/>
<connect gate="C" pin="CONF_DONE" pad="C20"/>
<connect gate="C" pin="DCLK" pad="D19"/>
<connect gate="C" pin="GND" pad="B21"/>
<connect gate="C" pin="GNDA_PLL5" pad="F11"/>
<connect gate="C" pin="GNDA_PLL5_2" pad="F10"/>
<connect gate="C" pin="GND_2" pad="AA2"/>
<connect gate="C" pin="GND_3" pad="AB1"/>
<connect gate="C" pin="GND_4" pad="AB4"/>
<connect gate="C" pin="GND_5" pad="AB9"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="C15"/>
<connect gate="C" pin="IO_11" pad="AA7"/>
<connect gate="C" pin="IO_12" pad="C16"/>
<connect gate="C" pin="IO_13" pad="AA8"/>
<connect gate="C" pin="IO_14" pad="C17"/>
<connect gate="C" pin="IO_15" pad="AB6"/>
<connect gate="C" pin="IO_16" pad="C18"/>
<connect gate="C" pin="IO_17" pad="AA9"/>
<connect gate="C" pin="IO_18" pad="C19"/>
<connect gate="C" pin="IO_19" pad="AB7"/>
<connect gate="C" pin="IO_2" pad="C10"/>
<connect gate="C" pin="IO_20" pad="AB5"/>
<connect gate="C" pin="IO_21" pad="C21"/>
<connect gate="C" pin="IO_22" pad="AB8"/>
<connect gate="C" pin="IO_23" pad="C22"/>
<connect gate="C" pin="IO_24" pad="B10"/>
<connect gate="C" pin="IO_25" pad="D10"/>
<connect gate="C" pin="IO_26" pad="B11"/>
<connect gate="C" pin="IO_27" pad="D11"/>
<connect gate="C" pin="IO_28" pad="B12"/>
<connect gate="C" pin="IO_29" pad="D12"/>
<connect gate="C" pin="IO_3" pad="C11"/>
<connect gate="C" pin="IO_30" pad="B13"/>
<connect gate="C" pin="IO_31" pad="D13"/>
<connect gate="C" pin="IO_32" pad="D14"/>
<connect gate="C" pin="IO_33" pad="B15"/>
<connect gate="C" pin="IO_34" pad="B16"/>
<connect gate="C" pin="IO_35" pad="B17"/>
<connect gate="C" pin="IO_36" pad="B18"/>
<connect gate="C" pin="IO_37" pad="B19"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D17"/>
<connect gate="C" pin="IO_4" pad="C12"/>
<connect gate="C" pin="IO_40" pad="D18"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E10"/>
<connect gate="C" pin="IO_45" pad="E11"/>
<connect gate="C" pin="IO_46" pad="E12"/>
<connect gate="C" pin="IO_47" pad="E13"/>
<connect gate="C" pin="IO_48" pad="E14"/>
<connect gate="C" pin="IO_49" pad="E15"/>
<connect gate="C" pin="IO_5" pad="AA4"/>
<connect gate="C" pin="IO_50" pad="E16"/>
<connect gate="C" pin="IO_51" pad="E17"/>
<connect gate="C" pin="IO_52" pad="E18"/>
<connect gate="C" pin="IO_53" pad="E19"/>
<connect gate="C" pin="IO_54" pad="E20"/>
<connect gate="C" pin="IO_55" pad="E21"/>
<connect gate="C" pin="IO_56" pad="E22"/>
<connect gate="C" pin="IO_57" pad="F13"/>
<connect gate="C" pin="IO_58" pad="F14"/>
<connect gate="C" pin="IO_59" pad="F15"/>
<connect gate="C" pin="IO_6" pad="C13"/>
<connect gate="C" pin="IO_60" pad="F16"/>
<connect gate="C" pin="IO_61" pad="F17"/>
<connect gate="C" pin="IO_62" pad="F19"/>
<connect gate="C" pin="IO_63" pad="F20"/>
<connect gate="C" pin="IO_64" pad="F21"/>
<connect gate="C" pin="IO_65" pad="F22"/>
<connect gate="C" pin="IO_66" pad="G12"/>
<connect gate="C" pin="IO_67" pad="G13"/>
<connect gate="C" pin="IO_68" pad="G14"/>
<connect gate="C" pin="IO_69" pad="G15"/>
<connect gate="C" pin="IO_7" pad="AA5"/>
<connect gate="C" pin="IO_70" pad="G16"/>
<connect gate="C" pin="IO_71" pad="G17"/>
<connect gate="C" pin="IO_72" pad="G18"/>
<connect gate="C" pin="IO_73" pad="G19"/>
<connect gate="C" pin="IO_74" pad="G20"/>
<connect gate="C" pin="IO_75" pad="G21"/>
<connect gate="C" pin="IO_76" pad="G22"/>
<connect gate="C" pin="IO_8" pad="C14"/>
<connect gate="C" pin="IO_9" pad="AA6"/>
<connect gate="C" pin="NCEO" pad="AA3"/>
<connect gate="C" pin="NIO_PULLUP" pad="AB2"/>
<connect gate="C" pin="NSTATUS" pad="B20"/>
<connect gate="C" pin="VCCA_PLL5" pad="F12"/>
<connect gate="C" pin="VCCD_PLL5" pad="G11"/>
<connect gate="C" pin="VCCIO2" pad="B22"/>
<connect gate="C" pin="VCCIO7" pad="AB3"/>
<connect gate="C" pin="VCCPD4" pad="H10"/>
<connect gate="C" pin="VCC_PLL5_OUT" pad="G10"/>
<connect gate="C" pin="VREFB2N0" pad="F18"/>
<connect gate="C" pin="VREFB3N0" pad="B14"/>
<connect gate="C" pin="VREFB3N1" pad="D16"/>
<connect gate="D" pin="CLK1N" pad="M20"/>
<connect gate="D" pin="CLK1P" pad="M21"/>
<connect gate="D" pin="CLK3N" pad="N19"/>
<connect gate="D" pin="CLK3P" pad="N20"/>
<connect gate="D" pin="GND" pad="N12"/>
<connect gate="D" pin="GNDA_PLL1" pad="L18"/>
<connect gate="D" pin="GNDA_PLL1_2" pad="L17"/>
<connect gate="D" pin="GNDA_PLL2" pad="N18"/>
<connect gate="D" pin="GNDA_PLL2_2" pad="N17"/>
<connect gate="D" pin="GND_10" pad="K13"/>
<connect gate="D" pin="GND_11" pad="M15"/>
<connect gate="D" pin="GND_12" pad="M13"/>
<connect gate="D" pin="GND_13" pad="N10"/>
<connect gate="D" pin="GND_14" pad="P22"/>
<connect gate="D" pin="GND_15" pad="P13"/>
<connect gate="D" pin="GND_16" pad="R10"/>
<connect gate="D" pin="GND_17" pad="M11"/>
<connect gate="D" pin="GND_18" pad="P11"/>
<connect gate="D" pin="GND_19" pad="N14"/>
<connect gate="D" pin="GND_2" pad="H15"/>
<connect gate="D" pin="GND_20" pad="L12"/>
<connect gate="D" pin="GND_3" pad="J10"/>
<connect gate="D" pin="GND_4" pad="J12"/>
<connect gate="D" pin="GND_5" pad="J22"/>
<connect gate="D" pin="GND_6" pad="J14"/>
<connect gate="D" pin="GND_7" pad="L14"/>
<connect gate="D" pin="GND_8" pad="L10"/>
<connect gate="D" pin="GND_9" pad="K11"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="H12"/>
<connect gate="D" pin="IO_11" pad="J17"/>
<connect gate="D" pin="IO_12" pad="K15"/>
<connect gate="D" pin="IO_13" pad="H21"/>
<connect gate="D" pin="IO_14" pad="K16"/>
<connect gate="D" pin="IO_15" pad="L15"/>
<connect gate="D" pin="IO_16" pad="J18"/>
<connect gate="D" pin="IO_17" pad="L16"/>
<connect gate="D" pin="IO_18" pad="K17"/>
<connect gate="D" pin="IO_19" pad="H22"/>
<connect gate="D" pin="IO_2" pad="H16"/>
<connect gate="D" pin="IO_20" pad="K18"/>
<connect gate="D" pin="IO_21" pad="J19"/>
<connect gate="D" pin="IO_22" pad="L20"/>
<connect gate="D" pin="IO_23" pad="K19"/>
<connect gate="D" pin="IO_24" pad="J20"/>
<connect gate="D" pin="IO_25" pad="K20"/>
<connect gate="D" pin="IO_26" pad="J21"/>
<connect gate="D" pin="IO_27" pad="K21"/>
<connect gate="D" pin="IO_28" pad="K22"/>
<connect gate="D" pin="IO_29" pad="L21"/>
<connect gate="D" pin="IO_3" pad="H17"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N16"/>
<connect gate="D" pin="IO_32" pad="N21"/>
<connect gate="D" pin="IO_33" pad="N22"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="P19"/>
<connect gate="D" pin="IO_38" pad="P20"/>
<connect gate="D" pin="IO_39" pad="P21"/>
<connect gate="D" pin="IO_4" pad="H18"/>
<connect gate="D" pin="IO_40" pad="R14"/>
<connect gate="D" pin="IO_41" pad="R15"/>
<connect gate="D" pin="IO_42" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H14"/>
<connect gate="D" pin="IO_6" pad="H19"/>
<connect gate="D" pin="IO_7" pad="J15"/>
<connect gate="D" pin="IO_8" pad="H20"/>
<connect gate="D" pin="IO_9" pad="J16"/>
<connect gate="D" pin="VCCA_PLL1" pad="M17"/>
<connect gate="D" pin="VCCA_PLL2" pad="M19"/>
<connect gate="D" pin="VCCA_PLL6" pad="R12"/>
<connect gate="D" pin="VCCD_PLL1" pad="M16"/>
<connect gate="D" pin="VCCD_PLL2" pad="M18"/>
<connect gate="D" pin="VCCINT" pad="N13"/>
<connect gate="D" pin="VCCINT_10" pad="N11"/>
<connect gate="D" pin="VCCINT_11" pad="M10"/>
<connect gate="D" pin="VCCINT_12" pad="M12"/>
<connect gate="D" pin="VCCINT_13" pad="P12"/>
<connect gate="D" pin="VCCINT_2" pad="P14"/>
<connect gate="D" pin="VCCINT_3" pad="J11"/>
<connect gate="D" pin="VCCINT_4" pad="K10"/>
<connect gate="D" pin="VCCINT_5" pad="J13"/>
<connect gate="D" pin="VCCINT_6" pad="L13"/>
<connect gate="D" pin="VCCINT_7" pad="K12"/>
<connect gate="D" pin="VCCINT_8" pad="L11"/>
<connect gate="D" pin="VCCINT_9" pad="M14"/>
<connect gate="D" pin="VCCIO1" pad="M22"/>
<connect gate="D" pin="VCCIO2" pad="L22"/>
<connect gate="D" pin="VCCPD1" pad="P15"/>
<connect gate="D" pin="VCCPD2" pad="K14"/>
<connect gate="D" pin="VCCPD3" pad="H13"/>
<connect gate="D" pin="VCCPD7" pad="P10"/>
<connect gate="D" pin="VCCPD8" pad="R13"/>
<connect gate="D" pin="VCC_PLL6_OUT" pad="R11"/>
<connect gate="D" pin="VREFB2N1" pad="L19"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL6" pad="T12"/>
<connect gate="E" pin="GNDA_PLL6_2" pad="T11"/>
<connect gate="E" pin="GND_2" pad="AA21"/>
<connect gate="E" pin="GND_3" pad="AB14"/>
<connect gate="E" pin="IO" pad="AB18"/>
<connect gate="E" pin="IO_10" pad="T16"/>
<connect gate="E" pin="IO_11" pad="T17"/>
<connect gate="E" pin="IO_12" pad="T18"/>
<connect gate="E" pin="IO_13" pad="T19"/>
<connect gate="E" pin="IO_14" pad="T20"/>
<connect gate="E" pin="IO_15" pad="T21"/>
<connect gate="E" pin="IO_16" pad="T22"/>
<connect gate="E" pin="IO_17" pad="U10"/>
<connect gate="E" pin="IO_18" pad="V18"/>
<connect gate="E" pin="IO_19" pad="V19"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="U12"/>
<connect gate="E" pin="IO_21" pad="U13"/>
<connect gate="E" pin="IO_22" pad="U14"/>
<connect gate="E" pin="IO_23" pad="U15"/>
<connect gate="E" pin="IO_24" pad="U16"/>
<connect gate="E" pin="IO_25" pad="U17"/>
<connect gate="E" pin="IO_26" pad="U18"/>
<connect gate="E" pin="IO_27" pad="U19"/>
<connect gate="E" pin="IO_28" pad="U20"/>
<connect gate="E" pin="IO_29" pad="U21"/>
<connect gate="E" pin="IO_3" pad="R21"/>
<connect gate="E" pin="IO_30" pad="U22"/>
<connect gate="E" pin="IO_31" pad="V10"/>
<connect gate="E" pin="IO_32" pad="V11"/>
<connect gate="E" pin="IO_33" pad="V12"/>
<connect gate="E" pin="IO_34" pad="V13"/>
<connect gate="E" pin="IO_35" pad="V14"/>
<connect gate="E" pin="IO_36" pad="V15"/>
<connect gate="E" pin="IO_37" pad="V21"/>
<connect gate="E" pin="IO_38" pad="V16"/>
<connect gate="E" pin="IO_39" pad="V22"/>
<connect gate="E" pin="IO_4" pad="R19"/>
<connect gate="E" pin="IO_40" pad="W10"/>
<connect gate="E" pin="IO_41" pad="W11"/>
<connect gate="E" pin="IO_42" pad="W12"/>
<connect gate="E" pin="IO_43" pad="W13"/>
<connect gate="E" pin="IO_44" pad="W14"/>
<connect gate="E" pin="IO_45" pad="W15"/>
<connect gate="E" pin="IO_46" pad="W16"/>
<connect gate="E" pin="IO_47" pad="W17"/>
<connect gate="E" pin="IO_48" pad="W19"/>
<connect gate="E" pin="IO_49" pad="W20"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="W21"/>
<connect gate="E" pin="IO_51" pad="W22"/>
<connect gate="E" pin="IO_52" pad="Y10"/>
<connect gate="E" pin="IO_53" pad="Y11"/>
<connect gate="E" pin="IO_54" pad="Y12"/>
<connect gate="E" pin="IO_55" pad="Y13"/>
<connect gate="E" pin="IO_56" pad="Y14"/>
<connect gate="E" pin="IO_57" pad="Y15"/>
<connect gate="E" pin="IO_58" pad="Y16"/>
<connect gate="E" pin="IO_59" pad="Y17"/>
<connect gate="E" pin="IO_6" pad="T13"/>
<connect gate="E" pin="IO_60" pad="Y18"/>
<connect gate="E" pin="IO_61" pad="Y20"/>
<connect gate="E" pin="IO_62" pad="Y21"/>
<connect gate="E" pin="IO_63" pad="Y22"/>
<connect gate="E" pin="IO_64" pad="AA10"/>
<connect gate="E" pin="IO_65" pad="AA11"/>
<connect gate="E" pin="IO_66" pad="AA12"/>
<connect gate="E" pin="IO_67" pad="AA13"/>
<connect gate="E" pin="IO_68" pad="AA15"/>
<connect gate="E" pin="IO_69" pad="AA16"/>
<connect gate="E" pin="IO_7" pad="T10"/>
<connect gate="E" pin="IO_70" pad="AA17"/>
<connect gate="E" pin="IO_71" pad="AA18"/>
<connect gate="E" pin="IO_72" pad="AB10"/>
<connect gate="E" pin="IO_73" pad="AB13"/>
<connect gate="E" pin="IO_74" pad="AB15"/>
<connect gate="E" pin="IO_75" pad="AB16"/>
<connect gate="E" pin="IO_76" pad="AB17"/>
<connect gate="E" pin="IO_8" pad="T14"/>
<connect gate="E" pin="IO_9" pad="T15"/>
<connect gate="E" pin="NCONFIG" pad="W18"/>
<connect gate="E" pin="TCK" pad="AA19"/>
<connect gate="E" pin="TDI" pad="AB21"/>
<connect gate="E" pin="TMS" pad="AA20"/>
<connect gate="E" pin="TRST" pad="AB19"/>
<connect gate="E" pin="VCCD_PLL6" pad="U11"/>
<connect gate="E" pin="VCCIO1" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="AB11"/>
<connect gate="E" pin="VCCIO8" pad="AB20"/>
<connect gate="E" pin="VCCIO8_2" pad="AB12"/>
<connect gate="E" pin="VCCSEL" pad="V17"/>
<connect gate="E" pin="VREFB1N0" pad="R20"/>
<connect gate="E" pin="VREFB1N1" pad="V20"/>
<connect gate="E" pin="VREFB8N0" pad="Y19"/>
<connect gate="E" pin="VREFB8N1" pad="AA14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S15F484C3N"/>
<attribute name="OC_FARNELL" value="1637232"/>
<attribute name="OC_NEWARK" value="51R0581"/>
<attribute name="PACKAGE" value="FBGA-484"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S15F484C5N">
<description>Stratix II Devices</description>
<gates>
<gate name="A" symbol="EP2S15F484C5N_A"/>
<gate name="B" symbol="EP2S15F484C5N_B"/>
<gate name="C" symbol="EP2S15F484C5N_C"/>
<gate name="D" symbol="EP2S15F484C5N_D"/>
<gate name="E" symbol="EP2S15F484C5N_E"/>
</gates>
<devices>
<device name="" package="BGA484C22X22X100P_2300X2300X35">
<connects>
<connect gate="A" pin="GND" pad="K9"/>
<connect gate="A" pin="GNDA_PLL4" pad="L5"/>
<connect gate="A" pin="GNDA_PLL4_2" pad="L4"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="A9"/>
<connect gate="A" pin="GND_4" pad="J1"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B9"/>
<connect gate="A" pin="IO_11" pad="C1"/>
<connect gate="A" pin="IO_12" pad="C2"/>
<connect gate="A" pin="IO_13" pad="C4"/>
<connect gate="A" pin="IO_14" pad="C5"/>
<connect gate="A" pin="IO_15" pad="C6"/>
<connect gate="A" pin="IO_16" pad="C7"/>
<connect gate="A" pin="IO_17" pad="C8"/>
<connect gate="A" pin="IO_18" pad="C9"/>
<connect gate="A" pin="IO_19" pad="D1"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="D2"/>
<connect gate="A" pin="IO_21" pad="D3"/>
<connect gate="A" pin="IO_22" pad="D5"/>
<connect gate="A" pin="IO_23" pad="D6"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="E1"/>
<connect gate="A" pin="IO_26" pad="E2"/>
<connect gate="A" pin="IO_27" pad="E3"/>
<connect gate="A" pin="IO_28" pad="E4"/>
<connect gate="A" pin="IO_29" pad="E6"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="E7"/>
<connect gate="A" pin="IO_31" pad="E8"/>
<connect gate="A" pin="IO_32" pad="E9"/>
<connect gate="A" pin="IO_33" pad="F1"/>
<connect gate="A" pin="IO_34" pad="F2"/>
<connect gate="A" pin="IO_35" pad="F4"/>
<connect gate="A" pin="IO_36" pad="F5"/>
<connect gate="A" pin="IO_37" pad="F6"/>
<connect gate="A" pin="IO_38" pad="F7"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="G9"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B5"/>
<connect gate="A" pin="IO_60" pad="J5"/>
<connect gate="A" pin="IO_61" pad="J6"/>
<connect gate="A" pin="IO_62" pad="J7"/>
<connect gate="A" pin="IO_63" pad="J8"/>
<connect gate="A" pin="IO_64" pad="K1"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_66" pad="K3"/>
<connect gate="A" pin="IO_67" pad="K4"/>
<connect gate="A" pin="IO_68" pad="K5"/>
<connect gate="A" pin="IO_69" pad="K6"/>
<connect gate="A" pin="IO_7" pad="B6"/>
<connect gate="A" pin="IO_70" pad="K7"/>
<connect gate="A" pin="IO_71" pad="K8"/>
<connect gate="A" pin="IO_72" pad="L2"/>
<connect gate="A" pin="IO_73" pad="L3"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="B8"/>
<connect gate="A" pin="MSEL0" pad="E5"/>
<connect gate="A" pin="MSEL1" pad="D4"/>
<connect gate="A" pin="MSEL2" pad="B4"/>
<connect gate="A" pin="MSEL3" pad="A4"/>
<connect gate="A" pin="TDO" pad="B3"/>
<connect gate="A" pin="TEMPDIODEN" pad="C3"/>
<connect gate="A" pin="TEMPDIODEP" pad="A2"/>
<connect gate="A" pin="VCCD_PLL4" pad="L6"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="H8"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="B1"/>
<connect gate="A" pin="VREFB4N0" pad="D7"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N0" pad="J4"/>
<connect gate="A" pin="VREFB5N1" pad="F3"/>
<connect gate="B" pin="CLK11N" pad="M3"/>
<connect gate="B" pin="CLK11P" pad="M2"/>
<connect gate="B" pin="CLK9N" pad="N4"/>
<connect gate="B" pin="CLK9P" pad="N3"/>
<connect gate="B" pin="GND" pad="M7"/>
<connect gate="B" pin="GNDA_PLL3" pad="N6"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="N5"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="M9"/>
<connect gate="B" pin="GND_4" pad="A14"/>
<connect gate="B" pin="GND_5" pad="A22"/>
<connect gate="B" pin="IO" pad="A19"/>
<connect gate="B" pin="IO_10" pad="P6"/>
<connect gate="B" pin="IO_11" pad="P7"/>
<connect gate="B" pin="IO_12" pad="P8"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="R2"/>
<connect gate="B" pin="IO_15" pad="R3"/>
<connect gate="B" pin="IO_16" pad="R4"/>
<connect gate="B" pin="IO_17" pad="R5"/>
<connect gate="B" pin="IO_18" pad="R6"/>
<connect gate="B" pin="IO_19" pad="R7"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R8"/>
<connect gate="B" pin="IO_21" pad="R9"/>
<connect gate="B" pin="IO_22" pad="T1"/>
<connect gate="B" pin="IO_23" pad="T2"/>
<connect gate="B" pin="IO_24" pad="T3"/>
<connect gate="B" pin="IO_25" pad="T4"/>
<connect gate="B" pin="IO_26" pad="T5"/>
<connect gate="B" pin="IO_27" pad="T6"/>
<connect gate="B" pin="IO_28" pad="T7"/>
<connect gate="B" pin="IO_29" pad="T8"/>
<connect gate="B" pin="IO_3" pad="N1"/>
<connect gate="B" pin="IO_30" pad="T9"/>
<connect gate="B" pin="IO_31" pad="U1"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V3"/>
<connect gate="B" pin="IO_42" pad="V4"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="V9"/>
<connect gate="B" pin="IO_47" pad="W1"/>
<connect gate="B" pin="IO_48" pad="W2"/>
<connect gate="B" pin="IO_49" pad="W3"/>
<connect gate="B" pin="IO_5" pad="N7"/>
<connect gate="B" pin="IO_50" pad="W4"/>
<connect gate="B" pin="IO_51" pad="W5"/>
<connect gate="B" pin="IO_52" pad="W7"/>
<connect gate="B" pin="IO_53" pad="W9"/>
<connect gate="B" pin="IO_54" pad="Y1"/>
<connect gate="B" pin="IO_55" pad="Y2"/>
<connect gate="B" pin="IO_56" pad="Y3"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="N8"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A13"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_7" pad="P2"/>
<connect gate="B" pin="IO_8" pad="P3"/>
<connect gate="B" pin="IO_9" pad="P5"/>
<connect gate="B" pin="NCE" pad="A21"/>
<connect gate="B" pin="PLL_ENA" pad="Y4"/>
<connect gate="B" pin="PORSEL" pad="V5"/>
<connect gate="B" pin="VCCA_PLL3" pad="M4"/>
<connect gate="B" pin="VCCA_PLL4" pad="M6"/>
<connect gate="B" pin="VCCD_PLL3" pad="M5"/>
<connect gate="B" pin="VCCINT" pad="P9"/>
<connect gate="B" pin="VCCINT_2" pad="M8"/>
<connect gate="B" pin="VCCIO3" pad="A20"/>
<connect gate="B" pin="VCCIO3_2" pad="A12"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="AA1"/>
<connect gate="B" pin="VCCIO6_2" pad="M1"/>
<connect gate="B" pin="VCCPD5" pad="L9"/>
<connect gate="B" pin="VCCPD6" pad="N9"/>
<connect gate="B" pin="VREFB6N0" pad="U3"/>
<connect gate="B" pin="VREFB6N1" pad="P4"/>
<connect gate="B" pin="VREFB7N0" pad="W8"/>
<connect gate="B" pin="VREFB7N1" pad="W6"/>
<connect gate="C" pin="CONF_DONE" pad="C20"/>
<connect gate="C" pin="DCLK" pad="D19"/>
<connect gate="C" pin="GND" pad="B21"/>
<connect gate="C" pin="GNDA_PLL5" pad="F11"/>
<connect gate="C" pin="GNDA_PLL5_2" pad="F10"/>
<connect gate="C" pin="GND_2" pad="AA2"/>
<connect gate="C" pin="GND_3" pad="AB1"/>
<connect gate="C" pin="GND_4" pad="AB4"/>
<connect gate="C" pin="GND_5" pad="AB9"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="AB7"/>
<connect gate="C" pin="IO_11" pad="AB8"/>
<connect gate="C" pin="IO_12" pad="B10"/>
<connect gate="C" pin="IO_13" pad="B11"/>
<connect gate="C" pin="IO_14" pad="B12"/>
<connect gate="C" pin="IO_15" pad="B13"/>
<connect gate="C" pin="IO_16" pad="B15"/>
<connect gate="C" pin="IO_17" pad="B16"/>
<connect gate="C" pin="IO_18" pad="B17"/>
<connect gate="C" pin="IO_19" pad="B18"/>
<connect gate="C" pin="IO_2" pad="AA4"/>
<connect gate="C" pin="IO_20" pad="B19"/>
<connect gate="C" pin="IO_21" pad="C10"/>
<connect gate="C" pin="IO_22" pad="C11"/>
<connect gate="C" pin="IO_23" pad="C12"/>
<connect gate="C" pin="IO_24" pad="C13"/>
<connect gate="C" pin="IO_25" pad="C14"/>
<connect gate="C" pin="IO_26" pad="C15"/>
<connect gate="C" pin="IO_27" pad="C16"/>
<connect gate="C" pin="IO_28" pad="C17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="AA5"/>
<connect gate="C" pin="IO_30" pad="C19"/>
<connect gate="C" pin="IO_31" pad="C21"/>
<connect gate="C" pin="IO_32" pad="C22"/>
<connect gate="C" pin="IO_33" pad="D10"/>
<connect gate="C" pin="IO_34" pad="D11"/>
<connect gate="C" pin="IO_35" pad="D12"/>
<connect gate="C" pin="IO_36" pad="D13"/>
<connect gate="C" pin="IO_37" pad="D14"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D17"/>
<connect gate="C" pin="IO_4" pad="AA6"/>
<connect gate="C" pin="IO_40" pad="D18"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E10"/>
<connect gate="C" pin="IO_45" pad="E11"/>
<connect gate="C" pin="IO_46" pad="E12"/>
<connect gate="C" pin="IO_47" pad="E13"/>
<connect gate="C" pin="IO_48" pad="E14"/>
<connect gate="C" pin="IO_49" pad="E15"/>
<connect gate="C" pin="IO_5" pad="AA7"/>
<connect gate="C" pin="IO_50" pad="E16"/>
<connect gate="C" pin="IO_51" pad="E17"/>
<connect gate="C" pin="IO_52" pad="E18"/>
<connect gate="C" pin="IO_53" pad="E19"/>
<connect gate="C" pin="IO_54" pad="E20"/>
<connect gate="C" pin="IO_55" pad="E21"/>
<connect gate="C" pin="IO_56" pad="E22"/>
<connect gate="C" pin="IO_57" pad="F13"/>
<connect gate="C" pin="IO_58" pad="F14"/>
<connect gate="C" pin="IO_59" pad="F15"/>
<connect gate="C" pin="IO_6" pad="AA8"/>
<connect gate="C" pin="IO_60" pad="F16"/>
<connect gate="C" pin="IO_61" pad="F17"/>
<connect gate="C" pin="IO_62" pad="F19"/>
<connect gate="C" pin="IO_63" pad="F20"/>
<connect gate="C" pin="IO_64" pad="F21"/>
<connect gate="C" pin="IO_65" pad="F22"/>
<connect gate="C" pin="IO_66" pad="G12"/>
<connect gate="C" pin="IO_67" pad="G13"/>
<connect gate="C" pin="IO_68" pad="G14"/>
<connect gate="C" pin="IO_69" pad="G15"/>
<connect gate="C" pin="IO_7" pad="AA9"/>
<connect gate="C" pin="IO_70" pad="G16"/>
<connect gate="C" pin="IO_71" pad="G17"/>
<connect gate="C" pin="IO_72" pad="G18"/>
<connect gate="C" pin="IO_73" pad="G19"/>
<connect gate="C" pin="IO_74" pad="G20"/>
<connect gate="C" pin="IO_75" pad="G21"/>
<connect gate="C" pin="IO_76" pad="G22"/>
<connect gate="C" pin="IO_8" pad="AB5"/>
<connect gate="C" pin="IO_9" pad="AB6"/>
<connect gate="C" pin="NCEO" pad="AA3"/>
<connect gate="C" pin="NIO_PULLUP" pad="AB2"/>
<connect gate="C" pin="NSTATUS" pad="B20"/>
<connect gate="C" pin="VCCA_PLL5" pad="F12"/>
<connect gate="C" pin="VCCD_PLL5" pad="G11"/>
<connect gate="C" pin="VCCIO2" pad="B22"/>
<connect gate="C" pin="VCCIO7" pad="AB3"/>
<connect gate="C" pin="VCCPD4" pad="H10"/>
<connect gate="C" pin="VCC_PLL5_OUT" pad="G10"/>
<connect gate="C" pin="VREFB2N0" pad="F18"/>
<connect gate="C" pin="VREFB3N0" pad="B14"/>
<connect gate="C" pin="VREFB3N1" pad="D16"/>
<connect gate="D" pin="CLK1N" pad="M20"/>
<connect gate="D" pin="CLK1P" pad="M21"/>
<connect gate="D" pin="CLK3N" pad="N19"/>
<connect gate="D" pin="CLK3P" pad="N20"/>
<connect gate="D" pin="GND" pad="R10"/>
<connect gate="D" pin="GNDA_PLL1" pad="L18"/>
<connect gate="D" pin="GNDA_PLL1_2" pad="L17"/>
<connect gate="D" pin="GNDA_PLL2" pad="N18"/>
<connect gate="D" pin="GNDA_PLL2_2" pad="N17"/>
<connect gate="D" pin="GND_10" pad="M11"/>
<connect gate="D" pin="GND_11" pad="L14"/>
<connect gate="D" pin="GND_12" pad="N12"/>
<connect gate="D" pin="GND_13" pad="L10"/>
<connect gate="D" pin="GND_14" pad="P13"/>
<connect gate="D" pin="GND_15" pad="L12"/>
<connect gate="D" pin="GND_16" pad="N14"/>
<connect gate="D" pin="GND_17" pad="N10"/>
<connect gate="D" pin="GND_18" pad="P22"/>
<connect gate="D" pin="GND_19" pad="J10"/>
<connect gate="D" pin="GND_2" pad="K11"/>
<connect gate="D" pin="GND_20" pad="P11"/>
<connect gate="D" pin="GND_3" pad="H15"/>
<connect gate="D" pin="GND_4" pad="J12"/>
<connect gate="D" pin="GND_5" pad="K13"/>
<connect gate="D" pin="GND_6" pad="M13"/>
<connect gate="D" pin="GND_7" pad="J14"/>
<connect gate="D" pin="GND_8" pad="M15"/>
<connect gate="D" pin="GND_9" pad="J22"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="H22"/>
<connect gate="D" pin="IO_11" pad="J15"/>
<connect gate="D" pin="IO_12" pad="J16"/>
<connect gate="D" pin="IO_13" pad="J17"/>
<connect gate="D" pin="IO_14" pad="J18"/>
<connect gate="D" pin="IO_15" pad="J19"/>
<connect gate="D" pin="IO_16" pad="J20"/>
<connect gate="D" pin="IO_17" pad="J21"/>
<connect gate="D" pin="IO_18" pad="K15"/>
<connect gate="D" pin="IO_19" pad="K16"/>
<connect gate="D" pin="IO_2" pad="H12"/>
<connect gate="D" pin="IO_20" pad="K17"/>
<connect gate="D" pin="IO_21" pad="K18"/>
<connect gate="D" pin="IO_22" pad="K19"/>
<connect gate="D" pin="IO_23" pad="K20"/>
<connect gate="D" pin="IO_24" pad="K21"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="L15"/>
<connect gate="D" pin="IO_27" pad="L16"/>
<connect gate="D" pin="IO_28" pad="L20"/>
<connect gate="D" pin="IO_29" pad="L21"/>
<connect gate="D" pin="IO_3" pad="H14"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N16"/>
<connect gate="D" pin="IO_32" pad="N21"/>
<connect gate="D" pin="IO_33" pad="N22"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="P19"/>
<connect gate="D" pin="IO_38" pad="P20"/>
<connect gate="D" pin="IO_39" pad="P21"/>
<connect gate="D" pin="IO_4" pad="H16"/>
<connect gate="D" pin="IO_40" pad="R14"/>
<connect gate="D" pin="IO_41" pad="R15"/>
<connect gate="D" pin="IO_42" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H17"/>
<connect gate="D" pin="IO_6" pad="H18"/>
<connect gate="D" pin="IO_7" pad="H19"/>
<connect gate="D" pin="IO_8" pad="H20"/>
<connect gate="D" pin="IO_9" pad="H21"/>
<connect gate="D" pin="VCCA_PLL1" pad="M17"/>
<connect gate="D" pin="VCCA_PLL2" pad="M19"/>
<connect gate="D" pin="VCCA_PLL6" pad="R12"/>
<connect gate="D" pin="VCCD_PLL1" pad="M16"/>
<connect gate="D" pin="VCCD_PLL2" pad="M18"/>
<connect gate="D" pin="VCCINT" pad="P14"/>
<connect gate="D" pin="VCCINT_10" pad="M12"/>
<connect gate="D" pin="VCCINT_11" pad="N13"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="P12"/>
<connect gate="D" pin="VCCINT_2" pad="L11"/>
<connect gate="D" pin="VCCINT_3" pad="K12"/>
<connect gate="D" pin="VCCINT_4" pad="J11"/>
<connect gate="D" pin="VCCINT_5" pad="J13"/>
<connect gate="D" pin="VCCINT_6" pad="K10"/>
<connect gate="D" pin="VCCINT_7" pad="L13"/>
<connect gate="D" pin="VCCINT_8" pad="M10"/>
<connect gate="D" pin="VCCINT_9" pad="N11"/>
<connect gate="D" pin="VCCIO1" pad="M22"/>
<connect gate="D" pin="VCCIO2" pad="L22"/>
<connect gate="D" pin="VCCPD1" pad="P15"/>
<connect gate="D" pin="VCCPD2" pad="K14"/>
<connect gate="D" pin="VCCPD3" pad="H13"/>
<connect gate="D" pin="VCCPD7" pad="P10"/>
<connect gate="D" pin="VCCPD8" pad="R13"/>
<connect gate="D" pin="VCC_PLL6_OUT" pad="R11"/>
<connect gate="D" pin="VREFB2N1" pad="L19"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL6" pad="T12"/>
<connect gate="E" pin="GNDA_PLL6_2" pad="T11"/>
<connect gate="E" pin="GND_2" pad="AA21"/>
<connect gate="E" pin="GND_3" pad="AB14"/>
<connect gate="E" pin="IO" pad="AB18"/>
<connect gate="E" pin="IO_10" pad="T16"/>
<connect gate="E" pin="IO_11" pad="T17"/>
<connect gate="E" pin="IO_12" pad="T18"/>
<connect gate="E" pin="IO_13" pad="T19"/>
<connect gate="E" pin="IO_14" pad="T20"/>
<connect gate="E" pin="IO_15" pad="T21"/>
<connect gate="E" pin="IO_16" pad="T22"/>
<connect gate="E" pin="IO_17" pad="U10"/>
<connect gate="E" pin="IO_18" pad="U12"/>
<connect gate="E" pin="IO_19" pad="U13"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="U14"/>
<connect gate="E" pin="IO_21" pad="U15"/>
<connect gate="E" pin="IO_22" pad="U16"/>
<connect gate="E" pin="IO_23" pad="U17"/>
<connect gate="E" pin="IO_24" pad="U18"/>
<connect gate="E" pin="IO_25" pad="U19"/>
<connect gate="E" pin="IO_26" pad="U20"/>
<connect gate="E" pin="IO_27" pad="U21"/>
<connect gate="E" pin="IO_28" pad="U22"/>
<connect gate="E" pin="IO_29" pad="V10"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="V11"/>
<connect gate="E" pin="IO_31" pad="V12"/>
<connect gate="E" pin="IO_32" pad="V13"/>
<connect gate="E" pin="IO_33" pad="V14"/>
<connect gate="E" pin="IO_34" pad="V15"/>
<connect gate="E" pin="IO_35" pad="V16"/>
<connect gate="E" pin="IO_36" pad="V18"/>
<connect gate="E" pin="IO_37" pad="V19"/>
<connect gate="E" pin="IO_38" pad="V21"/>
<connect gate="E" pin="IO_39" pad="V22"/>
<connect gate="E" pin="IO_4" pad="R21"/>
<connect gate="E" pin="IO_40" pad="W10"/>
<connect gate="E" pin="IO_41" pad="W11"/>
<connect gate="E" pin="IO_42" pad="W12"/>
<connect gate="E" pin="IO_43" pad="W13"/>
<connect gate="E" pin="IO_44" pad="W14"/>
<connect gate="E" pin="IO_45" pad="W15"/>
<connect gate="E" pin="IO_46" pad="W16"/>
<connect gate="E" pin="IO_47" pad="W17"/>
<connect gate="E" pin="IO_48" pad="W19"/>
<connect gate="E" pin="IO_49" pad="W20"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="W21"/>
<connect gate="E" pin="IO_51" pad="W22"/>
<connect gate="E" pin="IO_52" pad="Y10"/>
<connect gate="E" pin="IO_53" pad="Y11"/>
<connect gate="E" pin="IO_54" pad="Y12"/>
<connect gate="E" pin="IO_55" pad="Y13"/>
<connect gate="E" pin="IO_56" pad="Y14"/>
<connect gate="E" pin="IO_57" pad="Y15"/>
<connect gate="E" pin="IO_58" pad="Y16"/>
<connect gate="E" pin="IO_59" pad="Y17"/>
<connect gate="E" pin="IO_6" pad="T10"/>
<connect gate="E" pin="IO_60" pad="Y18"/>
<connect gate="E" pin="IO_61" pad="Y20"/>
<connect gate="E" pin="IO_62" pad="Y21"/>
<connect gate="E" pin="IO_63" pad="Y22"/>
<connect gate="E" pin="IO_64" pad="AA10"/>
<connect gate="E" pin="IO_65" pad="AA11"/>
<connect gate="E" pin="IO_66" pad="AA12"/>
<connect gate="E" pin="IO_67" pad="AA13"/>
<connect gate="E" pin="IO_68" pad="AA15"/>
<connect gate="E" pin="IO_69" pad="AA16"/>
<connect gate="E" pin="IO_7" pad="T13"/>
<connect gate="E" pin="IO_70" pad="AA17"/>
<connect gate="E" pin="IO_71" pad="AA18"/>
<connect gate="E" pin="IO_72" pad="AB10"/>
<connect gate="E" pin="IO_73" pad="AB13"/>
<connect gate="E" pin="IO_74" pad="AB15"/>
<connect gate="E" pin="IO_75" pad="AB16"/>
<connect gate="E" pin="IO_76" pad="AB17"/>
<connect gate="E" pin="IO_8" pad="T14"/>
<connect gate="E" pin="IO_9" pad="T15"/>
<connect gate="E" pin="NCONFIG" pad="W18"/>
<connect gate="E" pin="TCK" pad="AA19"/>
<connect gate="E" pin="TDI" pad="AB21"/>
<connect gate="E" pin="TMS" pad="AA20"/>
<connect gate="E" pin="TRST" pad="AB19"/>
<connect gate="E" pin="VCCD_PLL6" pad="U11"/>
<connect gate="E" pin="VCCIO1" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="AB11"/>
<connect gate="E" pin="VCCIO8" pad="AB20"/>
<connect gate="E" pin="VCCIO8_2" pad="AB12"/>
<connect gate="E" pin="VCCSEL" pad="V17"/>
<connect gate="E" pin="VREFB1N0" pad="R20"/>
<connect gate="E" pin="VREFB1N1" pad="V20"/>
<connect gate="E" pin="VREFB8N0" pad="Y19"/>
<connect gate="E" pin="VREFB8N1" pad="AA14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S15F484C5N"/>
<attribute name="OC_FARNELL" value="1637233"/>
<attribute name="OC_NEWARK" value="51R0582"/>
<attribute name="PACKAGE" value="484-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S15F672C3N">
<description>Stratix II Devices</description>
<gates>
<gate name="A" symbol="EP2S15F672C3N_A"/>
<gate name="B" symbol="EP2S15F672C3N_B"/>
<gate name="C" symbol="EP2S15F672C3N_C"/>
<gate name="D" symbol="EP2S15F672C3N_D"/>
<gate name="E" symbol="EP2S15F672C3N_E"/>
<gate name="F" symbol="EP2S15F672C3N_F"/>
<gate name="G" symbol="EP2S15F672C3N_G"/>
</gates>
<devices>
<device name="" package="BGA672C26X26X100P_2700X2700X35">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="D7"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D9"/>
<connect gate="A" pin="IO_26" pad="E7"/>
<connect gate="A" pin="IO_27" pad="E8"/>
<connect gate="A" pin="IO_28" pad="E9"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G3"/>
<connect gate="A" pin="IO_32" pad="G4"/>
<connect gate="A" pin="IO_33" pad="H1"/>
<connect gate="A" pin="IO_34" pad="H2"/>
<connect gate="A" pin="IO_35" pad="H3"/>
<connect gate="A" pin="IO_36" pad="H4"/>
<connect gate="A" pin="IO_37" pad="J1"/>
<connect gate="A" pin="IO_38" pad="J2"/>
<connect gate="A" pin="IO_39" pad="J3"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="J4"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_43" pad="K3"/>
<connect gate="A" pin="IO_44" pad="K4"/>
<connect gate="A" pin="IO_45" pad="K8"/>
<connect gate="A" pin="IO_46" pad="K9"/>
<connect gate="A" pin="IO_47" pad="L2"/>
<connect gate="A" pin="IO_48" pad="L3"/>
<connect gate="A" pin="IO_49" pad="L4"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="L5"/>
<connect gate="A" pin="IO_51" pad="L6"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="G8"/>
<connect gate="A" pin="MSEL1" pad="B2"/>
<connect gate="A" pin="MSEL2" pad="E6"/>
<connect gate="A" pin="MSEL3" pad="F7"/>
<connect gate="A" pin="NC" pad="K7"/>
<connect gate="A" pin="NC_10" pad="H8"/>
<connect gate="A" pin="NC_11" pad="D4"/>
<connect gate="A" pin="NC_12" pad="F8"/>
<connect gate="A" pin="NC_13" pad="F1"/>
<connect gate="A" pin="NC_14" pad="F9"/>
<connect gate="A" pin="NC_15" pad="E1"/>
<connect gate="A" pin="NC_16" pad="F2"/>
<connect gate="A" pin="NC_17" pad="F3"/>
<connect gate="A" pin="NC_18" pad="H9"/>
<connect gate="A" pin="NC_19" pad="C1"/>
<connect gate="A" pin="NC_2" pad="G9"/>
<connect gate="A" pin="NC_20" pad="F4"/>
<connect gate="A" pin="NC_21" pad="E2"/>
<connect gate="A" pin="NC_22" pad="E3"/>
<connect gate="A" pin="NC_23" pad="J5"/>
<connect gate="A" pin="NC_24" pad="C2"/>
<connect gate="A" pin="NC_25" pad="E4"/>
<connect gate="A" pin="NC_26" pad="J6"/>
<connect gate="A" pin="NC_27" pad="J7"/>
<connect gate="A" pin="NC_28" pad="J8"/>
<connect gate="A" pin="NC_29" pad="J9"/>
<connect gate="A" pin="NC_3" pad="H5"/>
<connect gate="A" pin="NC_30" pad="K6"/>
<connect gate="A" pin="NC_4" pad="H6"/>
<connect gate="A" pin="NC_5" pad="D2"/>
<connect gate="A" pin="NC_6" pad="H7"/>
<connect gate="A" pin="NC_7" pad="D3"/>
<connect gate="A" pin="NC_8" pad="G6"/>
<connect gate="A" pin="NC_9" pad="G7"/>
<connect gate="A" pin="TDO" pad="F6"/>
<connect gate="A" pin="TEMPDIODEN" pad="F5"/>
<connect gate="A" pin="TEMPDIODEP" pad="E5"/>
<connect gate="A" pin="VCCIO4" pad="A4"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="D1"/>
<connect gate="A" pin="VREFB4N0" pad="D5"/>
<connect gate="A" pin="VREFB5N0" pad="K5"/>
<connect gate="A" pin="VREFB5N1" pad="G5"/>
<connect gate="B" pin="CLK11N" pad="N3"/>
<connect gate="B" pin="CLK11P" pad="N2"/>
<connect gate="B" pin="CLK9N" pad="R4"/>
<connect gate="B" pin="CLK9P" pad="R3"/>
<connect gate="B" pin="GND" pad="A14"/>
<connect gate="B" pin="GNDA_PLL3" pad="R8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="R7"/>
<connect gate="B" pin="GNDA_PLL4" pad="N9"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="N8"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="A13"/>
<connect gate="B" pin="GND_4" pad="N1"/>
<connect gate="B" pin="GND_5" pad="P6"/>
<connect gate="B" pin="GND_6" pad="U9"/>
<connect gate="B" pin="IO" pad="A22"/>
<connect gate="B" pin="IO_10" pad="M7"/>
<connect gate="B" pin="IO_11" pad="M8"/>
<connect gate="B" pin="IO_12" pad="N4"/>
<connect gate="B" pin="IO_13" pad="N5"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="P2"/>
<connect gate="B" pin="IO_17" pad="P3"/>
<connect gate="B" pin="IO_18" pad="P4"/>
<connect gate="B" pin="IO_19" pad="P5"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R1"/>
<connect gate="B" pin="IO_21" pad="R2"/>
<connect gate="B" pin="IO_22" pad="T2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="T4"/>
<connect gate="B" pin="IO_25" pad="T5"/>
<connect gate="B" pin="IO_26" pad="T6"/>
<connect gate="B" pin="IO_27" pad="T7"/>
<connect gate="B" pin="IO_28" pad="T8"/>
<connect gate="B" pin="IO_29" pad="T9"/>
<connect gate="B" pin="IO_3" pad="L9"/>
<connect gate="B" pin="IO_30" pad="U1"/>
<connect gate="B" pin="IO_31" pad="U2"/>
<connect gate="B" pin="IO_32" pad="U3"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="V1"/>
<connect gate="B" pin="IO_39" pad="V2"/>
<connect gate="B" pin="IO_4" pad="M1"/>
<connect gate="B" pin="IO_40" pad="V3"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V5"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="W1"/>
<connect gate="B" pin="IO_47" pad="W2"/>
<connect gate="B" pin="IO_48" pad="W3"/>
<connect gate="B" pin="IO_49" pad="W4"/>
<connect gate="B" pin="IO_5" pad="M2"/>
<connect gate="B" pin="IO_50" pad="Y1"/>
<connect gate="B" pin="IO_51" pad="Y2"/>
<connect gate="B" pin="IO_52" pad="Y3"/>
<connect gate="B" pin="IO_53" pad="Y4"/>
<connect gate="B" pin="IO_54" pad="A10"/>
<connect gate="B" pin="IO_55" pad="A12"/>
<connect gate="B" pin="IO_56" pad="A15"/>
<connect gate="B" pin="IO_57" pad="A17"/>
<connect gate="B" pin="IO_58" pad="A18"/>
<connect gate="B" pin="IO_59" pad="A19"/>
<connect gate="B" pin="IO_6" pad="M3"/>
<connect gate="B" pin="IO_60" pad="A20"/>
<connect gate="B" pin="IO_61" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M4"/>
<connect gate="B" pin="IO_8" pad="M5"/>
<connect gate="B" pin="IO_9" pad="M6"/>
<connect gate="B" pin="NC" pad="W9"/>
<connect gate="B" pin="NC_2" pad="Y6"/>
<connect gate="B" pin="NC_3" pad="W5"/>
<connect gate="B" pin="NC_4" pad="Y9"/>
<connect gate="B" pin="NC_5" pad="W6"/>
<connect gate="B" pin="NC_6" pad="Y7"/>
<connect gate="B" pin="NC_7" pad="W7"/>
<connect gate="B" pin="NC_8" pad="W8"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA_PLL3" pad="R6"/>
<connect gate="B" pin="VCCA_PLL4" pad="P8"/>
<connect gate="B" pin="VCCD_PLL3" pad="P7"/>
<connect gate="B" pin="VCCD_PLL4" pad="P9"/>
<connect gate="B" pin="VCCINT" pad="V9"/>
<connect gate="B" pin="VCCIO3" pad="A16"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="T1"/>
<connect gate="B" pin="VCCPD5" pad="M9"/>
<connect gate="B" pin="VCCPD6" pad="R9"/>
<connect gate="B" pin="VREFB6N0" pad="Y5"/>
<connect gate="B" pin="VREFB6N1" pad="R5"/>
<connect gate="C" pin="CONF_DONE" pad="B25"/>
<connect gate="C" pin="DCLK" pad="C24"/>
<connect gate="C" pin="GND" pad="B26"/>
<connect gate="C" pin="GND_2" pad="AE1"/>
<connect gate="C" pin="GND_3" pad="A25"/>
<connect gate="C" pin="GND_4" pad="AF2"/>
<connect gate="C" pin="GND_5" pad="AA7"/>
<connect gate="C" pin="IO" pad="D15"/>
<connect gate="C" pin="IO_10" pad="AC8"/>
<connect gate="C" pin="IO_11" pad="AC9"/>
<connect gate="C" pin="IO_12" pad="AD3"/>
<connect gate="C" pin="IO_13" pad="AD4"/>
<connect gate="C" pin="IO_14" pad="AD5"/>
<connect gate="C" pin="IO_15" pad="AD6"/>
<connect gate="C" pin="IO_16" pad="AD7"/>
<connect gate="C" pin="IO_17" pad="AD8"/>
<connect gate="C" pin="IO_18" pad="AD9"/>
<connect gate="C" pin="IO_19" pad="AE3"/>
<connect gate="C" pin="IO_2" pad="A24"/>
<connect gate="C" pin="IO_20" pad="AE4"/>
<connect gate="C" pin="IO_21" pad="AE5"/>
<connect gate="C" pin="IO_22" pad="AE6"/>
<connect gate="C" pin="IO_23" pad="AE7"/>
<connect gate="C" pin="IO_24" pad="AE8"/>
<connect gate="C" pin="IO_25" pad="AE9"/>
<connect gate="C" pin="IO_26" pad="AF3"/>
<connect gate="C" pin="IO_27" pad="AF5"/>
<connect gate="C" pin="IO_28" pad="AF6"/>
<connect gate="C" pin="IO_29" pad="AF7"/>
<connect gate="C" pin="IO_3" pad="AA1"/>
<connect gate="C" pin="IO_30" pad="AF8"/>
<connect gate="C" pin="IO_31" pad="AF9"/>
<connect gate="C" pin="IO_32" pad="B10"/>
<connect gate="C" pin="IO_33" pad="B11"/>
<connect gate="C" pin="IO_34" pad="B12"/>
<connect gate="C" pin="IO_35" pad="B13"/>
<connect gate="C" pin="IO_36" pad="B14"/>
<connect gate="C" pin="IO_37" pad="B15"/>
<connect gate="C" pin="IO_38" pad="B16"/>
<connect gate="C" pin="IO_39" pad="B17"/>
<connect gate="C" pin="IO_4" pad="AA2"/>
<connect gate="C" pin="IO_40" pad="B18"/>
<connect gate="C" pin="IO_41" pad="B19"/>
<connect gate="C" pin="IO_42" pad="B20"/>
<connect gate="C" pin="IO_43" pad="B21"/>
<connect gate="C" pin="IO_44" pad="B22"/>
<connect gate="C" pin="IO_45" pad="B23"/>
<connect gate="C" pin="IO_46" pad="B24"/>
<connect gate="C" pin="IO_47" pad="C10"/>
<connect gate="C" pin="IO_48" pad="C11"/>
<connect gate="C" pin="IO_49" pad="C12"/>
<connect gate="C" pin="IO_5" pad="AB1"/>
<connect gate="C" pin="IO_50" pad="C13"/>
<connect gate="C" pin="IO_51" pad="C14"/>
<connect gate="C" pin="IO_52" pad="C15"/>
<connect gate="C" pin="IO_53" pad="C16"/>
<connect gate="C" pin="IO_54" pad="C17"/>
<connect gate="C" pin="IO_55" pad="C18"/>
<connect gate="C" pin="IO_56" pad="C19"/>
<connect gate="C" pin="IO_57" pad="C20"/>
<connect gate="C" pin="IO_58" pad="C21"/>
<connect gate="C" pin="IO_59" pad="C22"/>
<connect gate="C" pin="IO_6" pad="AB2"/>
<connect gate="C" pin="IO_60" pad="C23"/>
<connect gate="C" pin="IO_61" pad="D10"/>
<connect gate="C" pin="IO_62" pad="D12"/>
<connect gate="C" pin="IO_63" pad="D13"/>
<connect gate="C" pin="IO_7" pad="AB9"/>
<connect gate="C" pin="IO_8" pad="AC6"/>
<connect gate="C" pin="IO_9" pad="AC7"/>
<connect gate="C" pin="NC" pad="AC4"/>
<connect gate="C" pin="NCEO" pad="AB5"/>
<connect gate="C" pin="NC_10" pad="AB7"/>
<connect gate="C" pin="NC_11" pad="AB8"/>
<connect gate="C" pin="NC_12" pad="D14"/>
<connect gate="C" pin="NC_13" pad="C25"/>
<connect gate="C" pin="NC_14" pad="AD1"/>
<connect gate="C" pin="NC_15" pad="AC2"/>
<connect gate="C" pin="NC_16" pad="C26"/>
<connect gate="C" pin="NC_17" pad="AC3"/>
<connect gate="C" pin="NC_18" pad="AD2"/>
<connect gate="C" pin="NC_2" pad="AA3"/>
<connect gate="C" pin="NC_3" pad="AA8"/>
<connect gate="C" pin="NC_4" pad="AA4"/>
<connect gate="C" pin="NC_5" pad="AA9"/>
<connect gate="C" pin="NC_6" pad="AA5"/>
<connect gate="C" pin="NC_7" pad="AB3"/>
<connect gate="C" pin="NC_8" pad="AA6"/>
<connect gate="C" pin="NC_9" pad="AB4"/>
<connect gate="C" pin="NIO_PULLUP" pad="AE2"/>
<connect gate="C" pin="PLL_ENA" pad="AB6"/>
<connect gate="C" pin="VCCIO3" pad="A23"/>
<connect gate="C" pin="VCCIO6" pad="AC1"/>
<connect gate="C" pin="VCCIO7" pad="AF4"/>
<connect gate="C" pin="VREFB4N1" pad="D11"/>
<connect gate="C" pin="VREFB7N1" pad="AC5"/>
<connect gate="D" pin="GND" pad="G13"/>
<connect gate="D" pin="GNDA_PLL5" pad="H13"/>
<connect gate="D" pin="GNDA_PLL5_2" pad="J13"/>
<connect gate="D" pin="IO" pad="J26"/>
<connect gate="D" pin="IO_10" pad="E13"/>
<connect gate="D" pin="IO_11" pad="E14"/>
<connect gate="D" pin="IO_12" pad="E15"/>
<connect gate="D" pin="IO_13" pad="E16"/>
<connect gate="D" pin="IO_14" pad="E17"/>
<connect gate="D" pin="IO_15" pad="E18"/>
<connect gate="D" pin="IO_16" pad="E19"/>
<connect gate="D" pin="IO_17" pad="E20"/>
<connect gate="D" pin="IO_18" pad="F10"/>
<connect gate="D" pin="IO_19" pad="F11"/>
<connect gate="D" pin="IO_2" pad="D17"/>
<connect gate="D" pin="IO_20" pad="F14"/>
<connect gate="D" pin="IO_21" pad="F15"/>
<connect gate="D" pin="IO_22" pad="F16"/>
<connect gate="D" pin="IO_23" pad="F17"/>
<connect gate="D" pin="IO_24" pad="F19"/>
<connect gate="D" pin="IO_25" pad="F20"/>
<connect gate="D" pin="IO_26" pad="G14"/>
<connect gate="D" pin="IO_27" pad="G15"/>
<connect gate="D" pin="IO_28" pad="G16"/>
<connect gate="D" pin="IO_29" pad="G17"/>
<connect gate="D" pin="IO_3" pad="D18"/>
<connect gate="D" pin="IO_30" pad="G18"/>
<connect gate="D" pin="IO_31" pad="G19"/>
<connect gate="D" pin="IO_32" pad="G23"/>
<connect gate="D" pin="IO_33" pad="G24"/>
<connect gate="D" pin="IO_34" pad="G25"/>
<connect gate="D" pin="IO_35" pad="G26"/>
<connect gate="D" pin="IO_36" pad="H23"/>
<connect gate="D" pin="IO_37" pad="H24"/>
<connect gate="D" pin="IO_38" pad="H25"/>
<connect gate="D" pin="IO_39" pad="H26"/>
<connect gate="D" pin="IO_4" pad="D19"/>
<connect gate="D" pin="IO_40" pad="J23"/>
<connect gate="D" pin="IO_41" pad="J24"/>
<connect gate="D" pin="IO_42" pad="J25"/>
<connect gate="D" pin="IO_5" pad="D20"/>
<connect gate="D" pin="IO_6" pad="D21"/>
<connect gate="D" pin="IO_7" pad="E10"/>
<connect gate="D" pin="IO_8" pad="E11"/>
<connect gate="D" pin="IO_9" pad="E12"/>
<connect gate="D" pin="NC" pad="G11"/>
<connect gate="D" pin="NCE" pad="E22"/>
<connect gate="D" pin="NC_10" pad="J18"/>
<connect gate="D" pin="NC_11" pad="F13"/>
<connect gate="D" pin="NC_12" pad="H17"/>
<connect gate="D" pin="NC_13" pad="F18"/>
<connect gate="D" pin="NC_14" pad="J14"/>
<connect gate="D" pin="NC_15" pad="D23"/>
<connect gate="D" pin="NC_16" pad="H18"/>
<connect gate="D" pin="NC_17" pad="F21"/>
<connect gate="D" pin="NC_18" pad="J19"/>
<connect gate="D" pin="NC_19" pad="D24"/>
<connect gate="D" pin="NC_2" pad="E23"/>
<connect gate="D" pin="NC_20" pad="H19"/>
<connect gate="D" pin="NC_21" pad="F22"/>
<connect gate="D" pin="NC_22" pad="J15"/>
<connect gate="D" pin="NC_23" pad="H10"/>
<connect gate="D" pin="NC_24" pad="H20"/>
<connect gate="D" pin="NC_25" pad="D25"/>
<connect gate="D" pin="NC_26" pad="J20"/>
<connect gate="D" pin="NC_27" pad="H11"/>
<connect gate="D" pin="NC_28" pad="H21"/>
<connect gate="D" pin="NC_29" pad="F23"/>
<connect gate="D" pin="NC_3" pad="E24"/>
<connect gate="D" pin="NC_30" pad="J21"/>
<connect gate="D" pin="NC_31" pad="G20"/>
<connect gate="D" pin="NC_32" pad="H22"/>
<connect gate="D" pin="NC_33" pad="F24"/>
<connect gate="D" pin="NC_34" pad="J22"/>
<connect gate="D" pin="NC_35" pad="G21"/>
<connect gate="D" pin="NC_36" pad="J10"/>
<connect gate="D" pin="NC_37" pad="F25"/>
<connect gate="D" pin="NC_38" pad="J11"/>
<connect gate="D" pin="NC_39" pad="F26"/>
<connect gate="D" pin="NC_4" pad="H15"/>
<connect gate="D" pin="NC_40" pad="G10"/>
<connect gate="D" pin="NC_5" pad="E25"/>
<connect gate="D" pin="NC_6" pad="J17"/>
<connect gate="D" pin="NC_7" pad="E26"/>
<connect gate="D" pin="NC_8" pad="H16"/>
<connect gate="D" pin="NC_9" pad="F12"/>
<connect gate="D" pin="NSTATUS" pad="E21"/>
<connect gate="D" pin="VCCA_PLL5" pad="G12"/>
<connect gate="D" pin="VCCD_PLL5" pad="H14"/>
<connect gate="D" pin="VCCIO2" pad="D26"/>
<connect gate="D" pin="VCCPD3" pad="J16"/>
<connect gate="D" pin="VCCPD4" pad="J12"/>
<connect gate="D" pin="VCC_PLL5_OUT" pad="H12"/>
<connect gate="D" pin="VREFB2N0" pad="G22"/>
<connect gate="D" pin="VREFB3N0" pad="D16"/>
<connect gate="D" pin="VREFB3N1" pad="D22"/>
<connect gate="E" pin="CLK1N" pad="N24"/>
<connect gate="E" pin="CLK1P" pad="N25"/>
<connect gate="E" pin="CLK3N" pad="P22"/>
<connect gate="E" pin="CLK3P" pad="P23"/>
<connect gate="E" pin="GND" pad="L13"/>
<connect gate="E" pin="GNDA_PLL1" pad="P18"/>
<connect gate="E" pin="GNDA_PLL1_2" pad="N18"/>
<connect gate="E" pin="GNDA_PLL2" pad="R20"/>
<connect gate="E" pin="GNDA_PLL2_2" pad="R19"/>
<connect gate="E" pin="GND_10" pad="N11"/>
<connect gate="E" pin="GND_11" pad="P10"/>
<connect gate="E" pin="GND_12" pad="M12"/>
<connect gate="E" pin="GND_13" pad="M14"/>
<connect gate="E" pin="GND_14" pad="N15"/>
<connect gate="E" pin="GND_15" pad="L17"/>
<connect gate="E" pin="GND_16" pad="N17"/>
<connect gate="E" pin="GND_17" pad="R11"/>
<connect gate="E" pin="GND_18" pad="R15"/>
<connect gate="E" pin="GND_19" pad="N13"/>
<connect gate="E" pin="GND_2" pad="K12"/>
<connect gate="E" pin="GND_20" pad="P16"/>
<connect gate="E" pin="GND_21" pad="P14"/>
<connect gate="E" pin="GND_22" pad="P26"/>
<connect gate="E" pin="GND_23" pad="R13"/>
<connect gate="E" pin="GND_24" pad="R17"/>
<connect gate="E" pin="GND_3" pad="K14"/>
<connect gate="E" pin="GND_4" pad="L15"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="M10"/>
<connect gate="E" pin="GND_7" pad="M16"/>
<connect gate="E" pin="GND_8" pad="P12"/>
<connect gate="E" pin="GND_9" pad="N26"/>
<connect gate="E" pin="IO" pad="P25"/>
<connect gate="E" pin="IO_10" pad="L18"/>
<connect gate="E" pin="IO_11" pad="L19"/>
<connect gate="E" pin="IO_12" pad="L20"/>
<connect gate="E" pin="IO_13" pad="L21"/>
<connect gate="E" pin="IO_14" pad="L22"/>
<connect gate="E" pin="IO_15" pad="L23"/>
<connect gate="E" pin="IO_16" pad="L24"/>
<connect gate="E" pin="IO_17" pad="L25"/>
<connect gate="E" pin="IO_18" pad="M19"/>
<connect gate="E" pin="IO_19" pad="M20"/>
<connect gate="E" pin="IO_2" pad="K19"/>
<connect gate="E" pin="IO_20" pad="M21"/>
<connect gate="E" pin="IO_21" pad="M22"/>
<connect gate="E" pin="IO_22" pad="M23"/>
<connect gate="E" pin="IO_23" pad="M24"/>
<connect gate="E" pin="IO_24" pad="M25"/>
<connect gate="E" pin="IO_25" pad="M26"/>
<connect gate="E" pin="IO_26" pad="N19"/>
<connect gate="E" pin="IO_27" pad="N20"/>
<connect gate="E" pin="IO_28" pad="N21"/>
<connect gate="E" pin="IO_29" pad="N22"/>
<connect gate="E" pin="IO_3" pad="K20"/>
<connect gate="E" pin="IO_30" pad="P24"/>
<connect gate="E" pin="IO_4" pad="K21"/>
<connect gate="E" pin="IO_5" pad="K22"/>
<connect gate="E" pin="IO_6" pad="K23"/>
<connect gate="E" pin="IO_7" pad="K24"/>
<connect gate="E" pin="IO_8" pad="K25"/>
<connect gate="E" pin="IO_9" pad="K26"/>
<connect gate="E" pin="NC" pad="K11"/>
<connect gate="E" pin="NC_2" pad="K16"/>
<connect gate="E" pin="NC_3" pad="K17"/>
<connect gate="E" pin="NC_4" pad="K10"/>
<connect gate="E" pin="NC_5" pad="K18"/>
<connect gate="E" pin="VCCA_PLL1" pad="P21"/>
<connect gate="E" pin="VCCD_PLL1" pad="P19"/>
<connect gate="E" pin="VCCD_PLL2" pad="P20"/>
<connect gate="E" pin="VCCINT" pad="L16"/>
<connect gate="E" pin="VCCINT_10" pad="N12"/>
<connect gate="E" pin="VCCINT_11" pad="L12"/>
<connect gate="E" pin="VCCINT_12" pad="P13"/>
<connect gate="E" pin="VCCINT_13" pad="N14"/>
<connect gate="E" pin="VCCINT_14" pad="L14"/>
<connect gate="E" pin="VCCINT_15" pad="P15"/>
<connect gate="E" pin="VCCINT_16" pad="N16"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="R12"/>
<connect gate="E" pin="VCCINT_4" pad="M13"/>
<connect gate="E" pin="VCCINT_5" pad="R16"/>
<connect gate="E" pin="VCCINT_6" pad="M15"/>
<connect gate="E" pin="VCCINT_7" pad="R14"/>
<connect gate="E" pin="VCCINT_8" pad="L10"/>
<connect gate="E" pin="VCCINT_9" pad="P11"/>
<connect gate="E" pin="VCCIO1" pad="P17"/>
<connect gate="E" pin="VCCIO2" pad="M17"/>
<connect gate="E" pin="VCCIO2_2" pad="L26"/>
<connect gate="E" pin="VCCIO3" pad="K15"/>
<connect gate="E" pin="VCCIO4" pad="K13"/>
<connect gate="E" pin="VCCIO5" pad="N10"/>
<connect gate="E" pin="VCCIO6" pad="R10"/>
<connect gate="E" pin="VCCPD1" pad="R18"/>
<connect gate="E" pin="VCCPD2" pad="M18"/>
<connect gate="E" pin="VREFB2N1" pad="N23"/>
<connect gate="F" pin="GND" pad="U11"/>
<connect gate="F" pin="GNDA_PLL6" pad="W14"/>
<connect gate="F" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="F" pin="GND_10" pad="U17"/>
<connect gate="F" pin="GND_11" pad="AA13"/>
<connect gate="F" pin="GND_2" pad="R22"/>
<connect gate="F" pin="GND_3" pad="T12"/>
<connect gate="F" pin="GND_4" pad="T10"/>
<connect gate="F" pin="GND_5" pad="U15"/>
<connect gate="F" pin="GND_6" pad="T14"/>
<connect gate="F" pin="GND_7" pad="T16"/>
<connect gate="F" pin="GND_8" pad="U13"/>
<connect gate="F" pin="GND_9" pad="T18"/>
<connect gate="F" pin="IO" pad="AA14"/>
<connect gate="F" pin="IO_10" pad="T24"/>
<connect gate="F" pin="IO_11" pad="T25"/>
<connect gate="F" pin="IO_12" pad="U19"/>
<connect gate="F" pin="IO_13" pad="U20"/>
<connect gate="F" pin="IO_14" pad="U21"/>
<connect gate="F" pin="IO_15" pad="U22"/>
<connect gate="F" pin="IO_16" pad="U23"/>
<connect gate="F" pin="IO_17" pad="U24"/>
<connect gate="F" pin="IO_18" pad="U25"/>
<connect gate="F" pin="IO_19" pad="U26"/>
<connect gate="F" pin="IO_2" pad="R23"/>
<connect gate="F" pin="IO_20" pad="V21"/>
<connect gate="F" pin="IO_21" pad="V22"/>
<connect gate="F" pin="IO_22" pad="V23"/>
<connect gate="F" pin="IO_23" pad="V24"/>
<connect gate="F" pin="IO_24" pad="V25"/>
<connect gate="F" pin="IO_25" pad="V26"/>
<connect gate="F" pin="IO_26" pad="W17"/>
<connect gate="F" pin="IO_27" pad="W18"/>
<connect gate="F" pin="IO_28" pad="W21"/>
<connect gate="F" pin="IO_29" pad="W22"/>
<connect gate="F" pin="IO_3" pad="R24"/>
<connect gate="F" pin="IO_30" pad="W23"/>
<connect gate="F" pin="IO_31" pad="W24"/>
<connect gate="F" pin="IO_32" pad="W25"/>
<connect gate="F" pin="IO_33" pad="W26"/>
<connect gate="F" pin="IO_34" pad="Y10"/>
<connect gate="F" pin="IO_35" pad="Y15"/>
<connect gate="F" pin="IO_36" pad="Y16"/>
<connect gate="F" pin="IO_37" pad="Y17"/>
<connect gate="F" pin="IO_38" pad="Y18"/>
<connect gate="F" pin="IO_39" pad="Y23"/>
<connect gate="F" pin="IO_4" pad="R25"/>
<connect gate="F" pin="IO_40" pad="Y24"/>
<connect gate="F" pin="IO_41" pad="Y25"/>
<connect gate="F" pin="IO_42" pad="Y26"/>
<connect gate="F" pin="IO_43" pad="AA10"/>
<connect gate="F" pin="IO_44" pad="AA11"/>
<connect gate="F" pin="IO_45" pad="AA12"/>
<connect gate="F" pin="IO_5" pad="R26"/>
<connect gate="F" pin="IO_6" pad="T19"/>
<connect gate="F" pin="IO_7" pad="T20"/>
<connect gate="F" pin="IO_8" pad="T21"/>
<connect gate="F" pin="IO_9" pad="T22"/>
<connect gate="F" pin="NC" pad="Y12"/>
<connect gate="F" pin="NC_10" pad="W10"/>
<connect gate="F" pin="NC_11" pad="W11"/>
<connect gate="F" pin="NC_12" pad="W12"/>
<connect gate="F" pin="NC_13" pad="W15"/>
<connect gate="F" pin="NC_14" pad="W16"/>
<connect gate="F" pin="NC_15" pad="Y20"/>
<connect gate="F" pin="NC_16" pad="W19"/>
<connect gate="F" pin="NC_17" pad="Y21"/>
<connect gate="F" pin="NC_18" pad="W20"/>
<connect gate="F" pin="NC_19" pad="Y11"/>
<connect gate="F" pin="NC_2" pad="V10"/>
<connect gate="F" pin="NC_3" pad="V12"/>
<connect gate="F" pin="NC_4" pad="V14"/>
<connect gate="F" pin="NC_5" pad="V16"/>
<connect gate="F" pin="NC_6" pad="V17"/>
<connect gate="F" pin="NC_7" pad="V18"/>
<connect gate="F" pin="NC_8" pad="V19"/>
<connect gate="F" pin="NC_9" pad="V20"/>
<connect gate="F" pin="VCCA_PLL2" pad="R21"/>
<connect gate="F" pin="VCCA_PLL6" pad="Y13"/>
<connect gate="F" pin="VCCD_PLL6" pad="Y14"/>
<connect gate="F" pin="VCCINT" pad="U10"/>
<connect gate="F" pin="VCCINT_2" pad="T13"/>
<connect gate="F" pin="VCCINT_3" pad="T17"/>
<connect gate="F" pin="VCCINT_4" pad="T15"/>
<connect gate="F" pin="VCCINT_5" pad="T11"/>
<connect gate="F" pin="VCCINT_6" pad="U18"/>
<connect gate="F" pin="VCCINT_7" pad="U16"/>
<connect gate="F" pin="VCCIO1" pad="T26"/>
<connect gate="F" pin="VCCIO7" pad="U12"/>
<connect gate="F" pin="VCCIO8" pad="U14"/>
<connect gate="F" pin="VCCPD7" pad="V11"/>
<connect gate="F" pin="VCCPD8" pad="V15"/>
<connect gate="F" pin="VCCSEL" pad="Y19"/>
<connect gate="F" pin="VCC_PLL6_OUT" pad="V13"/>
<connect gate="F" pin="VREFB1N0" pad="T23"/>
<connect gate="F" pin="VREFB1N1" pad="Y22"/>
<connect gate="G" pin="GND" pad="AF14"/>
<connect gate="G" pin="GND_2" pad="AE26"/>
<connect gate="G" pin="GND_3" pad="AF25"/>
<connect gate="G" pin="GND_4" pad="AF13"/>
<connect gate="G" pin="IO" pad="AF24"/>
<connect gate="G" pin="IO_10" pad="AB10"/>
<connect gate="G" pin="IO_11" pad="AB11"/>
<connect gate="G" pin="IO_12" pad="AB12"/>
<connect gate="G" pin="IO_13" pad="AB13"/>
<connect gate="G" pin="IO_14" pad="AB14"/>
<connect gate="G" pin="IO_15" pad="AB15"/>
<connect gate="G" pin="IO_16" pad="AB16"/>
<connect gate="G" pin="IO_17" pad="AB17"/>
<connect gate="G" pin="IO_18" pad="AB18"/>
<connect gate="G" pin="IO_19" pad="AB19"/>
<connect gate="G" pin="IO_2" pad="AA15"/>
<connect gate="G" pin="IO_20" pad="AB20"/>
<connect gate="G" pin="IO_21" pad="AC10"/>
<connect gate="G" pin="IO_22" pad="AC12"/>
<connect gate="G" pin="IO_23" pad="AC13"/>
<connect gate="G" pin="IO_24" pad="AC14"/>
<connect gate="G" pin="IO_25" pad="AC17"/>
<connect gate="G" pin="IO_26" pad="AC18"/>
<connect gate="G" pin="IO_27" pad="AC19"/>
<connect gate="G" pin="IO_28" pad="AC20"/>
<connect gate="G" pin="IO_29" pad="AC21"/>
<connect gate="G" pin="IO_3" pad="AA16"/>
<connect gate="G" pin="IO_30" pad="AD10"/>
<connect gate="G" pin="IO_31" pad="AD11"/>
<connect gate="G" pin="IO_32" pad="AD12"/>
<connect gate="G" pin="IO_33" pad="AD13"/>
<connect gate="G" pin="IO_34" pad="AD14"/>
<connect gate="G" pin="IO_35" pad="AD16"/>
<connect gate="G" pin="IO_36" pad="AD17"/>
<connect gate="G" pin="IO_37" pad="AD18"/>
<connect gate="G" pin="IO_38" pad="AD19"/>
<connect gate="G" pin="IO_39" pad="AD20"/>
<connect gate="G" pin="IO_4" pad="AA17"/>
<connect gate="G" pin="IO_40" pad="AD21"/>
<connect gate="G" pin="IO_41" pad="AD22"/>
<connect gate="G" pin="IO_42" pad="AD23"/>
<connect gate="G" pin="IO_43" pad="AE10"/>
<connect gate="G" pin="IO_44" pad="AE11"/>
<connect gate="G" pin="IO_45" pad="AE12"/>
<connect gate="G" pin="IO_46" pad="AE13"/>
<connect gate="G" pin="IO_47" pad="AE14"/>
<connect gate="G" pin="IO_48" pad="AE15"/>
<connect gate="G" pin="IO_49" pad="AE16"/>
<connect gate="G" pin="IO_5" pad="AA19"/>
<connect gate="G" pin="IO_50" pad="AE17"/>
<connect gate="G" pin="IO_51" pad="AE18"/>
<connect gate="G" pin="IO_52" pad="AE19"/>
<connect gate="G" pin="IO_53" pad="AE20"/>
<connect gate="G" pin="IO_54" pad="AE21"/>
<connect gate="G" pin="IO_55" pad="AE22"/>
<connect gate="G" pin="IO_56" pad="AE23"/>
<connect gate="G" pin="IO_57" pad="AE24"/>
<connect gate="G" pin="IO_58" pad="AF10"/>
<connect gate="G" pin="IO_59" pad="AF12"/>
<connect gate="G" pin="IO_6" pad="AA23"/>
<connect gate="G" pin="IO_60" pad="AF15"/>
<connect gate="G" pin="IO_61" pad="AF17"/>
<connect gate="G" pin="IO_62" pad="AF18"/>
<connect gate="G" pin="IO_63" pad="AF19"/>
<connect gate="G" pin="IO_64" pad="AF20"/>
<connect gate="G" pin="IO_65" pad="AF21"/>
<connect gate="G" pin="IO_66" pad="AF22"/>
<connect gate="G" pin="IO_7" pad="AA24"/>
<connect gate="G" pin="IO_8" pad="AA25"/>
<connect gate="G" pin="IO_9" pad="AA26"/>
<connect gate="G" pin="NC" pad="AC25"/>
<connect gate="G" pin="NCONFIG" pad="AA20"/>
<connect gate="G" pin="NC_10" pad="AC24"/>
<connect gate="G" pin="NC_11" pad="AD15"/>
<connect gate="G" pin="NC_12" pad="AD25"/>
<connect gate="G" pin="NC_13" pad="AB26"/>
<connect gate="G" pin="NC_14" pad="AD26"/>
<connect gate="G" pin="NC_2" pad="AA21"/>
<connect gate="G" pin="NC_3" pad="AA18"/>
<connect gate="G" pin="NC_4" pad="AA22"/>
<connect gate="G" pin="NC_5" pad="AC15"/>
<connect gate="G" pin="NC_6" pad="AB23"/>
<connect gate="G" pin="NC_7" pad="AB24"/>
<connect gate="G" pin="NC_8" pad="AC23"/>
<connect gate="G" pin="NC_9" pad="AB25"/>
<connect gate="G" pin="TCK" pad="AB22"/>
<connect gate="G" pin="TDI" pad="AE25"/>
<connect gate="G" pin="TMS" pad="AD24"/>
<connect gate="G" pin="TRST" pad="AB21"/>
<connect gate="G" pin="VCCIO1" pad="AC26"/>
<connect gate="G" pin="VCCIO7" pad="AF11"/>
<connect gate="G" pin="VCCIO8" pad="AF23"/>
<connect gate="G" pin="VCCIO8_2" pad="AF16"/>
<connect gate="G" pin="VREFB7N0" pad="AC11"/>
<connect gate="G" pin="VREFB8N0" pad="AC22"/>
<connect gate="G" pin="VREFB8N1" pad="AC16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S15F672C3N"/>
<attribute name="OC_FARNELL" value="1549486"/>
<attribute name="OC_NEWARK" value="52R0700"/>
<attribute name="PACKAGE" value="672-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S180F1020C3N">
<description>FPGA, STRATIX II</description>
<gates>
<gate name="A" symbol="EP2S180F1020C3N_A"/>
<gate name="B" symbol="EP2S180F1020C3N_B"/>
<gate name="C" symbol="EP2S180F1020C3N_C"/>
<gate name="D" symbol="EP2S180F1020C3N_D"/>
<gate name="E" symbol="EP2S180F1020C3N_E"/>
<gate name="F" symbol="EP2S180F1020C3N_F"/>
<gate name="G" symbol="EP2S180F1020C3N_G"/>
<gate name="H" symbol="EP2S180F1020C3N_H"/>
<gate name="I" symbol="EP2S180F1020C3N_I"/>
<gate name="J" symbol="EP2S180F1020C3N_J"/>
<gate name="K" symbol="EP2S180F1020C3N_K"/>
</gates>
<devices>
<device name="" package="BGA1020C100P32X32_3300X3300X35">
<connects>
<connect gate="A" pin="FPLL10CLKN" pad="D4"/>
<connect gate="A" pin="FPLL10CLKP" pad="D3"/>
<connect gate="A" pin="GND" pad="F7"/>
<connect gate="A" pin="GNDA_PLL10" pad="G8"/>
<connect gate="A" pin="GNDA_PLL10_2" pad="G7"/>
<connect gate="A" pin="GND_2" pad="K5"/>
<connect gate="A" pin="GND_3" pad="A2"/>
<connect gate="A" pin="GND_4" pad="B1"/>
<connect gate="A" pin="IO" pad="L4"/>
<connect gate="A" pin="IO_10" pad="D1"/>
<connect gate="A" pin="IO_11" pad="D2"/>
<connect gate="A" pin="IO_12" pad="B4"/>
<connect gate="A" pin="IO_13" pad="B5"/>
<connect gate="A" pin="IO_14" pad="B6"/>
<connect gate="A" pin="IO_15" pad="D5"/>
<connect gate="A" pin="IO_16" pad="B7"/>
<connect gate="A" pin="IO_17" pad="D6"/>
<connect gate="A" pin="IO_18" pad="A4"/>
<connect gate="A" pin="IO_19" pad="D7"/>
<connect gate="A" pin="IO_2" pad="A8"/>
<connect gate="A" pin="IO_20" pad="B8"/>
<connect gate="A" pin="IO_21" pad="D8"/>
<connect gate="A" pin="IO_22" pad="A5"/>
<connect gate="A" pin="IO_23" pad="B9"/>
<connect gate="A" pin="IO_24" pad="E1"/>
<connect gate="A" pin="IO_25" pad="A6"/>
<connect gate="A" pin="IO_26" pad="E2"/>
<connect gate="A" pin="IO_27" pad="A7"/>
<connect gate="A" pin="IO_28" pad="E3"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="C4"/>
<connect gate="A" pin="IO_30" pad="E5"/>
<connect gate="A" pin="IO_31" pad="E6"/>
<connect gate="A" pin="IO_32" pad="E7"/>
<connect gate="A" pin="IO_33" pad="E8"/>
<connect gate="A" pin="IO_34" pad="E9"/>
<connect gate="A" pin="IO_35" pad="F1"/>
<connect gate="A" pin="IO_36" pad="F2"/>
<connect gate="A" pin="IO_37" pad="F3"/>
<connect gate="A" pin="IO_38" pad="F4"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="H1"/>
<connect gate="A" pin="IO_48" pad="H2"/>
<connect gate="A" pin="IO_49" pad="H3"/>
<connect gate="A" pin="IO_5" pad="C5"/>
<connect gate="A" pin="IO_50" pad="H4"/>
<connect gate="A" pin="IO_51" pad="J1"/>
<connect gate="A" pin="IO_52" pad="J2"/>
<connect gate="A" pin="IO_53" pad="J3"/>
<connect gate="A" pin="IO_54" pad="J4"/>
<connect gate="A" pin="IO_55" pad="J6"/>
<connect gate="A" pin="IO_56" pad="J7"/>
<connect gate="A" pin="IO_57" pad="J8"/>
<connect gate="A" pin="IO_58" pad="J9"/>
<connect gate="A" pin="IO_59" pad="K1"/>
<connect gate="A" pin="IO_6" pad="C6"/>
<connect gate="A" pin="IO_60" pad="K2"/>
<connect gate="A" pin="IO_61" pad="K3"/>
<connect gate="A" pin="IO_62" pad="K4"/>
<connect gate="A" pin="IO_63" pad="K6"/>
<connect gate="A" pin="IO_64" pad="K7"/>
<connect gate="A" pin="IO_65" pad="K8"/>
<connect gate="A" pin="IO_66" pad="K9"/>
<connect gate="A" pin="IO_67" pad="L1"/>
<connect gate="A" pin="IO_68" pad="L2"/>
<connect gate="A" pin="IO_69" pad="L3"/>
<connect gate="A" pin="IO_7" pad="C7"/>
<connect gate="A" pin="IO_8" pad="C8"/>
<connect gate="A" pin="IO_9" pad="C9"/>
<connect gate="A" pin="MSEL0" pad="B2"/>
<connect gate="A" pin="MSEL1" pad="F6"/>
<connect gate="A" pin="TDO" pad="C3"/>
<connect gate="A" pin="TEMPDIODEN" pad="B3"/>
<connect gate="A" pin="TEMPDIODEP" pad="G9"/>
<connect gate="A" pin="VCCA_PLL10" pad="H8"/>
<connect gate="A" pin="VCCD_PLL10" pad="H7"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="C1"/>
<connect gate="A" pin="VREFB4N0" pad="C2"/>
<connect gate="A" pin="VREFB4N1" pad="H9"/>
<connect gate="A" pin="VREFB4N2" pad="D9"/>
<connect gate="A" pin="VREFB5N1" pad="J5"/>
<connect gate="A" pin="VREFB5N2" pad="H5"/>
<connect gate="A" pin="VREFB5N3" pad="H6"/>
<connect gate="A" pin="VREFB5N4" pad="F5"/>
<connect gate="B" pin="CLK11N" pad="T4"/>
<connect gate="B" pin="CLK11P" pad="T3"/>
<connect gate="B" pin="CLK9N" pad="U4"/>
<connect gate="B" pin="CLK9P" pad="U3"/>
<connect gate="B" pin="GND" pad="T7"/>
<connect gate="B" pin="GNDA_PLL3" pad="U8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="V8"/>
<connect gate="B" pin="GNDA_PLL4" pad="R8"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="T8"/>
<connect gate="B" pin="GND_2" pad="Y1"/>
<connect gate="B" pin="GND_3" pad="N1"/>
<connect gate="B" pin="GND_4" pad="A13"/>
<connect gate="B" pin="IO" pad="A16"/>
<connect gate="B" pin="IO_10" pad="L9"/>
<connect gate="B" pin="IO_11" pad="M1"/>
<connect gate="B" pin="IO_12" pad="N2"/>
<connect gate="B" pin="IO_13" pad="M2"/>
<connect gate="B" pin="IO_14" pad="N3"/>
<connect gate="B" pin="IO_15" pad="M3"/>
<connect gate="B" pin="IO_16" pad="N4"/>
<connect gate="B" pin="IO_17" pad="M4"/>
<connect gate="B" pin="IO_18" pad="N5"/>
<connect gate="B" pin="IO_19" pad="N6"/>
<connect gate="B" pin="IO_2" pad="L5"/>
<connect gate="B" pin="IO_20" pad="P6"/>
<connect gate="B" pin="IO_21" pad="N7"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="N8"/>
<connect gate="B" pin="IO_24" pad="P8"/>
<connect gate="B" pin="IO_25" pad="N9"/>
<connect gate="B" pin="IO_26" pad="P9"/>
<connect gate="B" pin="IO_27" pad="P1"/>
<connect gate="B" pin="IO_28" pad="P2"/>
<connect gate="B" pin="IO_29" pad="R2"/>
<connect gate="B" pin="IO_3" pad="M6"/>
<connect gate="B" pin="IO_30" pad="R3"/>
<connect gate="B" pin="IO_31" pad="P4"/>
<connect gate="B" pin="IO_32" pad="R4"/>
<connect gate="B" pin="IO_33" pad="T1"/>
<connect gate="B" pin="IO_34" pad="P5"/>
<connect gate="B" pin="IO_35" pad="T2"/>
<connect gate="B" pin="IO_36" pad="R5"/>
<connect gate="B" pin="IO_37" pad="R6"/>
<connect gate="B" pin="IO_38" pad="R7"/>
<connect gate="B" pin="IO_39" pad="T5"/>
<connect gate="B" pin="IO_4" pad="L6"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="U1"/>
<connect gate="B" pin="IO_42" pad="U2"/>
<connect gate="B" pin="IO_43" pad="U5"/>
<connect gate="B" pin="IO_44" pad="U6"/>
<connect gate="B" pin="IO_45" pad="V2"/>
<connect gate="B" pin="IO_46" pad="V3"/>
<connect gate="B" pin="IO_47" pad="V4"/>
<connect gate="B" pin="IO_48" pad="V5"/>
<connect gate="B" pin="IO_49" pad="V6"/>
<connect gate="B" pin="IO_5" pad="M7"/>
<connect gate="B" pin="IO_50" pad="V7"/>
<connect gate="B" pin="IO_51" pad="V9"/>
<connect gate="B" pin="IO_52" pad="W1"/>
<connect gate="B" pin="IO_53" pad="W2"/>
<connect gate="B" pin="IO_54" pad="W4"/>
<connect gate="B" pin="IO_55" pad="W5"/>
<connect gate="B" pin="IO_56" pad="W6"/>
<connect gate="B" pin="IO_57" pad="W7"/>
<connect gate="B" pin="IO_58" pad="W8"/>
<connect gate="B" pin="IO_59" pad="W9"/>
<connect gate="B" pin="IO_6" pad="L7"/>
<connect gate="B" pin="IO_60" pad="Y2"/>
<connect gate="B" pin="IO_61" pad="Y3"/>
<connect gate="B" pin="IO_62" pad="Y4"/>
<connect gate="B" pin="IO_63" pad="Y5"/>
<connect gate="B" pin="IO_64" pad="Y6"/>
<connect gate="B" pin="IO_65" pad="Y7"/>
<connect gate="B" pin="IO_66" pad="Y8"/>
<connect gate="B" pin="IO_67" pad="Y9"/>
<connect gate="B" pin="IO_68" pad="A10"/>
<connect gate="B" pin="IO_69" pad="A11"/>
<connect gate="B" pin="IO_7" pad="M8"/>
<connect gate="B" pin="IO_70" pad="A12"/>
<connect gate="B" pin="IO_71" pad="A14"/>
<connect gate="B" pin="IO_8" pad="L8"/>
<connect gate="B" pin="IO_9" pad="M9"/>
<connect gate="B" pin="VCCA_PLL3" pad="U9"/>
<connect gate="B" pin="VCCA_PLL4" pad="R9"/>
<connect gate="B" pin="VCCD_PLL3" pad="U7"/>
<connect gate="B" pin="VCCD_PLL4" pad="T9"/>
<connect gate="B" pin="VCCIO4" pad="A15"/>
<connect gate="B" pin="VCCIO5" pad="R1"/>
<connect gate="B" pin="VCCIO5_2" pad="M5"/>
<connect gate="B" pin="VCCIO6" pad="V1"/>
<connect gate="B" pin="VREFB5N0" pad="P3"/>
<connect gate="B" pin="VREFB6N4" pad="W3"/>
<connect gate="C" pin="FPLL9CLKN" pad="AJ4"/>
<connect gate="C" pin="FPLL9CLKP" pad="AJ3"/>
<connect gate="C" pin="GND" pad="AF9"/>
<connect gate="C" pin="GNDA_PLL9" pad="AG7"/>
<connect gate="C" pin="GNDA_PLL9_2" pad="AF7"/>
<connect gate="C" pin="GND_2" pad="AC5"/>
<connect gate="C" pin="GND_3" pad="A20"/>
<connect gate="C" pin="GND_4" pad="AG6"/>
<connect gate="C" pin="GND_5" pad="A31"/>
<connect gate="C" pin="IO" pad="AJ6"/>
<connect gate="C" pin="IO_10" pad="AB1"/>
<connect gate="C" pin="IO_11" pad="A25"/>
<connect gate="C" pin="IO_12" pad="AB2"/>
<connect gate="C" pin="IO_13" pad="A26"/>
<connect gate="C" pin="IO_14" pad="AB3"/>
<connect gate="C" pin="IO_15" pad="A27"/>
<connect gate="C" pin="IO_16" pad="AB4"/>
<connect gate="C" pin="IO_17" pad="A28"/>
<connect gate="C" pin="IO_18" pad="AB5"/>
<connect gate="C" pin="IO_19" pad="A17"/>
<connect gate="C" pin="IO_2" pad="AA6"/>
<connect gate="C" pin="IO_20" pad="AB6"/>
<connect gate="C" pin="IO_21" pad="A29"/>
<connect gate="C" pin="IO_22" pad="AB7"/>
<connect gate="C" pin="IO_23" pad="AB8"/>
<connect gate="C" pin="IO_24" pad="A19"/>
<connect gate="C" pin="IO_25" pad="AB9"/>
<connect gate="C" pin="IO_26" pad="AC1"/>
<connect gate="C" pin="IO_27" pad="AA1"/>
<connect gate="C" pin="IO_28" pad="AC2"/>
<connect gate="C" pin="IO_29" pad="AA2"/>
<connect gate="C" pin="IO_3" pad="A21"/>
<connect gate="C" pin="IO_30" pad="AC3"/>
<connect gate="C" pin="IO_31" pad="AA3"/>
<connect gate="C" pin="IO_32" pad="AC4"/>
<connect gate="C" pin="IO_33" pad="AA4"/>
<connect gate="C" pin="IO_34" pad="AC6"/>
<connect gate="C" pin="IO_35" pad="AC7"/>
<connect gate="C" pin="IO_36" pad="AC8"/>
<connect gate="C" pin="IO_37" pad="AC9"/>
<connect gate="C" pin="IO_38" pad="AD1"/>
<connect gate="C" pin="IO_39" pad="AD2"/>
<connect gate="C" pin="IO_4" pad="AA7"/>
<connect gate="C" pin="IO_40" pad="AD3"/>
<connect gate="C" pin="IO_41" pad="AD4"/>
<connect gate="C" pin="IO_42" pad="AD6"/>
<connect gate="C" pin="IO_43" pad="AD7"/>
<connect gate="C" pin="IO_44" pad="AD8"/>
<connect gate="C" pin="IO_45" pad="AD9"/>
<connect gate="C" pin="IO_46" pad="AE1"/>
<connect gate="C" pin="IO_47" pad="AE2"/>
<connect gate="C" pin="IO_48" pad="AE3"/>
<connect gate="C" pin="IO_49" pad="AE4"/>
<connect gate="C" pin="IO_5" pad="A22"/>
<connect gate="C" pin="IO_50" pad="AE5"/>
<connect gate="C" pin="IO_51" pad="AE6"/>
<connect gate="C" pin="IO_52" pad="AF1"/>
<connect gate="C" pin="IO_53" pad="AF2"/>
<connect gate="C" pin="IO_54" pad="AF3"/>
<connect gate="C" pin="IO_55" pad="AF4"/>
<connect gate="C" pin="IO_56" pad="AG1"/>
<connect gate="C" pin="IO_57" pad="AG2"/>
<connect gate="C" pin="IO_58" pad="AG3"/>
<connect gate="C" pin="IO_59" pad="AG4"/>
<connect gate="C" pin="IO_6" pad="AA8"/>
<connect gate="C" pin="IO_60" pad="AG8"/>
<connect gate="C" pin="IO_61" pad="AG9"/>
<connect gate="C" pin="IO_62" pad="AH1"/>
<connect gate="C" pin="IO_63" pad="AH2"/>
<connect gate="C" pin="IO_64" pad="AH3"/>
<connect gate="C" pin="IO_65" pad="AH4"/>
<connect gate="C" pin="IO_66" pad="AH5"/>
<connect gate="C" pin="IO_67" pad="AH6"/>
<connect gate="C" pin="IO_68" pad="AH7"/>
<connect gate="C" pin="IO_69" pad="AH8"/>
<connect gate="C" pin="IO_7" pad="A23"/>
<connect gate="C" pin="IO_70" pad="AH9"/>
<connect gate="C" pin="IO_71" pad="AJ1"/>
<connect gate="C" pin="IO_72" pad="AJ2"/>
<connect gate="C" pin="IO_73" pad="AJ5"/>
<connect gate="C" pin="IO_8" pad="AA9"/>
<connect gate="C" pin="IO_9" pad="A24"/>
<connect gate="C" pin="PLL_ENA" pad="AF8"/>
<connect gate="C" pin="VCCA_PLL9" pad="AE7"/>
<connect gate="C" pin="VCCD_PLL9" pad="AE8"/>
<connect gate="C" pin="VCCIO3" pad="A18"/>
<connect gate="C" pin="VCCIO3_2" pad="A30"/>
<connect gate="C" pin="VCCIO6" pad="AA5"/>
<connect gate="C" pin="VREFB6N0" pad="AG5"/>
<connect gate="C" pin="VREFB6N1" pad="AF6"/>
<connect gate="C" pin="VREFB6N2" pad="AF5"/>
<connect gate="C" pin="VREFB6N3" pad="AD5"/>
<connect gate="C" pin="VREFB7N3" pad="AE9"/>
<connect gate="D" pin="DCLK" pad="B31"/>
<connect gate="D" pin="GND" pad="B32"/>
<connect gate="D" pin="GND_2" pad="AM2"/>
<connect gate="D" pin="GND_3" pad="AL1"/>
<connect gate="D" pin="IO" pad="D27"/>
<connect gate="D" pin="IO_10" pad="AM5"/>
<connect gate="D" pin="IO_11" pad="AK9"/>
<connect gate="D" pin="IO_12" pad="AM6"/>
<connect gate="D" pin="IO_13" pad="AL5"/>
<connect gate="D" pin="IO_14" pad="AM7"/>
<connect gate="D" pin="IO_15" pad="AL6"/>
<connect gate="D" pin="IO_16" pad="AM8"/>
<connect gate="D" pin="IO_17" pad="AL7"/>
<connect gate="D" pin="IO_18" pad="AM9"/>
<connect gate="D" pin="IO_19" pad="AL4"/>
<connect gate="D" pin="IO_2" pad="AK4"/>
<connect gate="D" pin="IO_20" pad="B10"/>
<connect gate="D" pin="IO_21" pad="AL8"/>
<connect gate="D" pin="IO_22" pad="B11"/>
<connect gate="D" pin="IO_23" pad="AL9"/>
<connect gate="D" pin="IO_24" pad="B12"/>
<connect gate="D" pin="IO_25" pad="B13"/>
<connect gate="D" pin="IO_26" pad="B14"/>
<connect gate="D" pin="IO_27" pad="B15"/>
<connect gate="D" pin="IO_28" pad="B16"/>
<connect gate="D" pin="IO_29" pad="B17"/>
<connect gate="D" pin="IO_3" pad="AK5"/>
<connect gate="D" pin="IO_30" pad="B18"/>
<connect gate="D" pin="IO_31" pad="B19"/>
<connect gate="D" pin="IO_32" pad="B20"/>
<connect gate="D" pin="IO_33" pad="B21"/>
<connect gate="D" pin="IO_34" pad="B22"/>
<connect gate="D" pin="IO_35" pad="B23"/>
<connect gate="D" pin="IO_36" pad="B24"/>
<connect gate="D" pin="IO_37" pad="B25"/>
<connect gate="D" pin="IO_38" pad="B26"/>
<connect gate="D" pin="IO_39" pad="B27"/>
<connect gate="D" pin="IO_4" pad="AJ7"/>
<connect gate="D" pin="IO_40" pad="B28"/>
<connect gate="D" pin="IO_41" pad="B29"/>
<connect gate="D" pin="IO_42" pad="C10"/>
<connect gate="D" pin="IO_43" pad="C11"/>
<connect gate="D" pin="IO_44" pad="C12"/>
<connect gate="D" pin="IO_45" pad="C13"/>
<connect gate="D" pin="IO_46" pad="C15"/>
<connect gate="D" pin="IO_47" pad="C16"/>
<connect gate="D" pin="IO_48" pad="C17"/>
<connect gate="D" pin="IO_49" pad="C18"/>
<connect gate="D" pin="IO_5" pad="AK6"/>
<connect gate="D" pin="IO_50" pad="C20"/>
<connect gate="D" pin="IO_51" pad="C21"/>
<connect gate="D" pin="IO_52" pad="C22"/>
<connect gate="D" pin="IO_53" pad="C23"/>
<connect gate="D" pin="IO_54" pad="C24"/>
<connect gate="D" pin="IO_55" pad="C25"/>
<connect gate="D" pin="IO_56" pad="C26"/>
<connect gate="D" pin="IO_57" pad="C27"/>
<connect gate="D" pin="IO_58" pad="C28"/>
<connect gate="D" pin="IO_59" pad="C29"/>
<connect gate="D" pin="IO_6" pad="AJ8"/>
<connect gate="D" pin="IO_60" pad="D10"/>
<connect gate="D" pin="IO_61" pad="D11"/>
<connect gate="D" pin="IO_62" pad="D12"/>
<connect gate="D" pin="IO_63" pad="D13"/>
<connect gate="D" pin="IO_64" pad="D14"/>
<connect gate="D" pin="IO_65" pad="D15"/>
<connect gate="D" pin="IO_66" pad="D16"/>
<connect gate="D" pin="IO_67" pad="D17"/>
<connect gate="D" pin="IO_68" pad="D18"/>
<connect gate="D" pin="IO_69" pad="D19"/>
<connect gate="D" pin="IO_7" pad="AK7"/>
<connect gate="D" pin="IO_70" pad="D20"/>
<connect gate="D" pin="IO_71" pad="D21"/>
<connect gate="D" pin="IO_72" pad="D22"/>
<connect gate="D" pin="IO_73" pad="D23"/>
<connect gate="D" pin="IO_74" pad="D25"/>
<connect gate="D" pin="IO_75" pad="D26"/>
<connect gate="D" pin="IO_8" pad="AM4"/>
<connect gate="D" pin="IO_9" pad="AK8"/>
<connect gate="D" pin="NCE" pad="C30"/>
<connect gate="D" pin="NCEO" pad="AL3"/>
<connect gate="D" pin="NIO_PULLUP" pad="AK3"/>
<connect gate="D" pin="NSTATUS" pad="B30"/>
<connect gate="D" pin="PORSEL" pad="AL2"/>
<connect gate="D" pin="VCCIO2" pad="C32"/>
<connect gate="D" pin="VCCIO6" pad="AK1"/>
<connect gate="D" pin="VCCIO7" pad="AM3"/>
<connect gate="D" pin="VREFB3N0" pad="C19"/>
<connect gate="D" pin="VREFB3N2" pad="D24"/>
<connect gate="D" pin="VREFB3N4" pad="C31"/>
<connect gate="D" pin="VREFB4N4" pad="C14"/>
<connect gate="D" pin="VREFB7N2" pad="AJ9"/>
<connect gate="D" pin="VREFB7N4" pad="AK2"/>
<connect gate="E" pin="FPLL7CLKN" pad="D29"/>
<connect gate="E" pin="FPLL7CLKP" pad="D30"/>
<connect gate="E" pin="GND" pad="G17"/>
<connect gate="E" pin="GNDA_PLL11" pad="H18"/>
<connect gate="E" pin="GNDA_PLL11_2" pad="G18"/>
<connect gate="E" pin="GNDA_PLL5" pad="H16"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="G16"/>
<connect gate="E" pin="GNDA_PLL7" pad="G26"/>
<connect gate="E" pin="GNDA_PLL7_2" pad="F26"/>
<connect gate="E" pin="GND_2" pad="E10"/>
<connect gate="E" pin="GND_3" pad="E23"/>
<connect gate="E" pin="GND_4" pad="F27"/>
<connect gate="E" pin="IO" pad="H28"/>
<connect gate="E" pin="IO_10" pad="E16"/>
<connect gate="E" pin="IO_11" pad="E22"/>
<connect gate="E" pin="IO_12" pad="E17"/>
<connect gate="E" pin="IO_13" pad="E18"/>
<connect gate="E" pin="IO_14" pad="E24"/>
<connect gate="E" pin="IO_15" pad="E19"/>
<connect gate="E" pin="IO_16" pad="E25"/>
<connect gate="E" pin="IO_17" pad="E26"/>
<connect gate="E" pin="IO_18" pad="E27"/>
<connect gate="E" pin="IO_19" pad="E28"/>
<connect gate="E" pin="IO_2" pad="E11"/>
<connect gate="E" pin="IO_20" pad="E29"/>
<connect gate="E" pin="IO_21" pad="E30"/>
<connect gate="E" pin="IO_22" pad="E31"/>
<connect gate="E" pin="IO_23" pad="E32"/>
<connect gate="E" pin="IO_24" pad="F10"/>
<connect gate="E" pin="IO_25" pad="F11"/>
<connect gate="E" pin="IO_26" pad="F12"/>
<connect gate="E" pin="IO_27" pad="F13"/>
<connect gate="E" pin="IO_28" pad="F22"/>
<connect gate="E" pin="IO_29" pad="F14"/>
<connect gate="E" pin="IO_3" pad="D28"/>
<connect gate="E" pin="IO_30" pad="F23"/>
<connect gate="E" pin="IO_31" pad="F15"/>
<connect gate="E" pin="IO_32" pad="F24"/>
<connect gate="E" pin="IO_33" pad="F16"/>
<connect gate="E" pin="IO_34" pad="F17"/>
<connect gate="E" pin="IO_35" pad="F18"/>
<connect gate="E" pin="IO_36" pad="F19"/>
<connect gate="E" pin="IO_37" pad="F20"/>
<connect gate="E" pin="IO_38" pad="F29"/>
<connect gate="E" pin="IO_39" pad="F30"/>
<connect gate="E" pin="IO_4" pad="D31"/>
<connect gate="E" pin="IO_40" pad="F31"/>
<connect gate="E" pin="IO_41" pad="F32"/>
<connect gate="E" pin="IO_42" pad="G10"/>
<connect gate="E" pin="IO_43" pad="G11"/>
<connect gate="E" pin="IO_44" pad="G12"/>
<connect gate="E" pin="IO_45" pad="G13"/>
<connect gate="E" pin="IO_46" pad="G19"/>
<connect gate="E" pin="IO_47" pad="G20"/>
<connect gate="E" pin="IO_48" pad="G21"/>
<connect gate="E" pin="IO_49" pad="G22"/>
<connect gate="E" pin="IO_5" pad="E13"/>
<connect gate="E" pin="IO_50" pad="G23"/>
<connect gate="E" pin="IO_51" pad="G24"/>
<connect gate="E" pin="IO_52" pad="G25"/>
<connect gate="E" pin="IO_53" pad="G27"/>
<connect gate="E" pin="IO_54" pad="G28"/>
<connect gate="E" pin="IO_55" pad="G29"/>
<connect gate="E" pin="IO_56" pad="G30"/>
<connect gate="E" pin="IO_57" pad="G31"/>
<connect gate="E" pin="IO_58" pad="G32"/>
<connect gate="E" pin="IO_59" pad="H11"/>
<connect gate="E" pin="IO_6" pad="D32"/>
<connect gate="E" pin="IO_60" pad="H12"/>
<connect gate="E" pin="IO_61" pad="H13"/>
<connect gate="E" pin="IO_62" pad="H14"/>
<connect gate="E" pin="IO_63" pad="H19"/>
<connect gate="E" pin="IO_64" pad="H20"/>
<connect gate="E" pin="IO_65" pad="H21"/>
<connect gate="E" pin="IO_66" pad="H22"/>
<connect gate="E" pin="IO_67" pad="H23"/>
<connect gate="E" pin="IO_68" pad="H24"/>
<connect gate="E" pin="IO_69" pad="H27"/>
<connect gate="E" pin="IO_7" pad="E14"/>
<connect gate="E" pin="IO_8" pad="E20"/>
<connect gate="E" pin="IO_9" pad="E15"/>
<connect gate="E" pin="MSEL3" pad="H10"/>
<connect gate="E" pin="VCCA_PLL11" pad="H17"/>
<connect gate="E" pin="VCCA_PLL5" pad="G15"/>
<connect gate="E" pin="VCCA_PLL7" pad="H26"/>
<connect gate="E" pin="VCCD_PLL5" pad="H15"/>
<connect gate="E" pin="VCCD_PLL7" pad="H25"/>
<connect gate="E" pin="VCCIO3" pad="E21"/>
<connect gate="E" pin="VCCIO4" pad="E12"/>
<connect gate="E" pin="VREFB2N1" pad="F28"/>
<connect gate="E" pin="VREFB3N1" pad="F21"/>
<connect gate="E" pin="VREFB3N3" pad="F25"/>
<connect gate="E" pin="VREFB4N3" pad="G14"/>
<connect gate="F" pin="CONF_DONE" pad="J25"/>
<connect gate="F" pin="GND" pad="M12"/>
<connect gate="F" pin="GND_2" pad="J24"/>
<connect gate="F" pin="GND_3" pad="K28"/>
<connect gate="F" pin="GND_4" pad="L11"/>
<connect gate="F" pin="GND_5" pad="M19"/>
<connect gate="F" pin="GND_6" pad="M14"/>
<connect gate="F" pin="IO" pad="M29"/>
<connect gate="F" pin="IO_10" pad="J15"/>
<connect gate="F" pin="IO_11" pad="J31"/>
<connect gate="F" pin="IO_12" pad="H31"/>
<connect gate="F" pin="IO_13" pad="J32"/>
<connect gate="F" pin="IO_14" pad="H32"/>
<connect gate="F" pin="IO_15" pad="J26"/>
<connect gate="F" pin="IO_16" pad="K11"/>
<connect gate="F" pin="IO_17" pad="J19"/>
<connect gate="F" pin="IO_18" pad="K12"/>
<connect gate="F" pin="IO_19" pad="J27"/>
<connect gate="F" pin="IO_2" pad="J11"/>
<connect gate="F" pin="IO_20" pad="K13"/>
<connect gate="F" pin="IO_21" pad="J20"/>
<connect gate="F" pin="IO_22" pad="K14"/>
<connect gate="F" pin="IO_23" pad="J21"/>
<connect gate="F" pin="IO_24" pad="K15"/>
<connect gate="F" pin="IO_25" pad="J22"/>
<connect gate="F" pin="IO_26" pad="K16"/>
<connect gate="F" pin="IO_27" pad="J23"/>
<connect gate="F" pin="IO_28" pad="K17"/>
<connect gate="F" pin="IO_29" pad="K18"/>
<connect gate="F" pin="IO_3" pad="J12"/>
<connect gate="F" pin="IO_30" pad="K19"/>
<connect gate="F" pin="IO_31" pad="K20"/>
<connect gate="F" pin="IO_32" pad="K21"/>
<connect gate="F" pin="IO_33" pad="K24"/>
<connect gate="F" pin="IO_34" pad="K22"/>
<connect gate="F" pin="IO_35" pad="K25"/>
<connect gate="F" pin="IO_36" pad="K26"/>
<connect gate="F" pin="IO_37" pad="K27"/>
<connect gate="F" pin="IO_38" pad="K29"/>
<connect gate="F" pin="IO_39" pad="K30"/>
<connect gate="F" pin="IO_4" pad="J13"/>
<connect gate="F" pin="IO_40" pad="K31"/>
<connect gate="F" pin="IO_41" pad="K32"/>
<connect gate="F" pin="IO_42" pad="L10"/>
<connect gate="F" pin="IO_43" pad="L12"/>
<connect gate="F" pin="IO_44" pad="L13"/>
<connect gate="F" pin="IO_45" pad="L14"/>
<connect gate="F" pin="IO_46" pad="L15"/>
<connect gate="F" pin="IO_47" pad="L16"/>
<connect gate="F" pin="IO_48" pad="L17"/>
<connect gate="F" pin="IO_49" pad="L18"/>
<connect gate="F" pin="IO_5" pad="H29"/>
<connect gate="F" pin="IO_50" pad="L19"/>
<connect gate="F" pin="IO_51" pad="L20"/>
<connect gate="F" pin="IO_52" pad="L21"/>
<connect gate="F" pin="IO_53" pad="L22"/>
<connect gate="F" pin="IO_54" pad="L23"/>
<connect gate="F" pin="IO_55" pad="L24"/>
<connect gate="F" pin="IO_56" pad="L25"/>
<connect gate="F" pin="IO_57" pad="L26"/>
<connect gate="F" pin="IO_58" pad="L29"/>
<connect gate="F" pin="IO_59" pad="L30"/>
<connect gate="F" pin="IO_6" pad="J14"/>
<connect gate="F" pin="IO_60" pad="L31"/>
<connect gate="F" pin="IO_61" pad="L32"/>
<connect gate="F" pin="IO_62" pad="M10"/>
<connect gate="F" pin="IO_63" pad="M11"/>
<connect gate="F" pin="IO_64" pad="M22"/>
<connect gate="F" pin="IO_65" pad="M23"/>
<connect gate="F" pin="IO_66" pad="M24"/>
<connect gate="F" pin="IO_67" pad="M25"/>
<connect gate="F" pin="IO_68" pad="M26"/>
<connect gate="F" pin="IO_69" pad="M27"/>
<connect gate="F" pin="IO_7" pad="J29"/>
<connect gate="F" pin="IO_8" pad="H30"/>
<connect gate="F" pin="IO_9" pad="J30"/>
<connect gate="F" pin="MSEL2" pad="J10"/>
<connect gate="F" pin="VCCD_PLL11" pad="J18"/>
<connect gate="F" pin="VCCINT" pad="M21"/>
<connect gate="F" pin="VCCINT_2" pad="K23"/>
<connect gate="F" pin="VCCINT_3" pad="K10"/>
<connect gate="F" pin="VCCIO2" pad="M28"/>
<connect gate="F" pin="VCCIO3" pad="M17"/>
<connect gate="F" pin="VCCIO4" pad="M16"/>
<connect gate="F" pin="VCCPD3" pad="M18"/>
<connect gate="F" pin="VCCPD3_2" pad="M20"/>
<connect gate="F" pin="VCCPD4" pad="M13"/>
<connect gate="F" pin="VCCPD4_2" pad="M15"/>
<connect gate="F" pin="VCC_PLL11_OUT" pad="J17"/>
<connect gate="F" pin="VCC_PLL5_OUT" pad="J16"/>
<connect gate="F" pin="VREFB2N1" pad="J28"/>
<connect gate="F" pin="VREFB2N2" pad="L27"/>
<connect gate="F" pin="VREFB2N3" pad="L28"/>
<connect gate="G" pin="CLK1N" pad="T29"/>
<connect gate="G" pin="CLK1P" pad="T30"/>
<connect gate="G" pin="GND" pad="T15"/>
<connect gate="G" pin="GNDA_PLL1" pad="T26"/>
<connect gate="G" pin="GNDA_PLL1_2" pad="T25"/>
<connect gate="G" pin="GND_10" pad="P17"/>
<connect gate="G" pin="GND_11" pad="P19"/>
<connect gate="G" pin="GND_12" pad="T19"/>
<connect gate="G" pin="GND_13" pad="P21"/>
<connect gate="G" pin="GND_14" pad="R16"/>
<connect gate="G" pin="GND_15" pad="R14"/>
<connect gate="G" pin="GND_16" pad="R20"/>
<connect gate="G" pin="GND_17" pad="T13"/>
<connect gate="G" pin="GND_18" pad="T17"/>
<connect gate="G" pin="GND_19" pad="R18"/>
<connect gate="G" pin="GND_2" pad="N14"/>
<connect gate="G" pin="GND_3" pad="N18"/>
<connect gate="G" pin="GND_4" pad="P12"/>
<connect gate="G" pin="GND_5" pad="N20"/>
<connect gate="G" pin="GND_6" pad="P13"/>
<connect gate="G" pin="GND_7" pad="N16"/>
<connect gate="G" pin="GND_8" pad="P15"/>
<connect gate="G" pin="GND_9" pad="N32"/>
<connect gate="G" pin="IO" pad="T28"/>
<connect gate="G" pin="IO_10" pad="M31"/>
<connect gate="G" pin="IO_11" pad="N24"/>
<connect gate="G" pin="IO_12" pad="M32"/>
<connect gate="G" pin="IO_13" pad="N25"/>
<connect gate="G" pin="IO_14" pad="N10"/>
<connect gate="G" pin="IO_15" pad="P10"/>
<connect gate="G" pin="IO_16" pad="N11"/>
<connect gate="G" pin="IO_17" pad="N26"/>
<connect gate="G" pin="IO_18" pad="P22"/>
<connect gate="G" pin="IO_19" pad="P11"/>
<connect gate="G" pin="IO_2" pad="N27"/>
<connect gate="G" pin="IO_20" pad="P23"/>
<connect gate="G" pin="IO_21" pad="P24"/>
<connect gate="G" pin="IO_22" pad="P25"/>
<connect gate="G" pin="IO_23" pad="P26"/>
<connect gate="G" pin="IO_24" pad="P27"/>
<connect gate="G" pin="IO_25" pad="P28"/>
<connect gate="G" pin="IO_26" pad="P29"/>
<connect gate="G" pin="IO_27" pad="P31"/>
<connect gate="G" pin="IO_28" pad="P32"/>
<connect gate="G" pin="IO_29" pad="R10"/>
<connect gate="G" pin="IO_3" pad="N28"/>
<connect gate="G" pin="IO_30" pad="R11"/>
<connect gate="G" pin="IO_31" pad="R22"/>
<connect gate="G" pin="IO_32" pad="R23"/>
<connect gate="G" pin="IO_33" pad="R24"/>
<connect gate="G" pin="IO_34" pad="R25"/>
<connect gate="G" pin="IO_35" pad="R26"/>
<connect gate="G" pin="IO_36" pad="R27"/>
<connect gate="G" pin="IO_37" pad="R28"/>
<connect gate="G" pin="IO_38" pad="R29"/>
<connect gate="G" pin="IO_39" pad="R30"/>
<connect gate="G" pin="IO_4" pad="N29"/>
<connect gate="G" pin="IO_40" pad="R31"/>
<connect gate="G" pin="IO_41" pad="T10"/>
<connect gate="G" pin="IO_42" pad="T11"/>
<connect gate="G" pin="IO_43" pad="T22"/>
<connect gate="G" pin="IO_44" pad="T23"/>
<connect gate="G" pin="IO_45" pad="T27"/>
<connect gate="G" pin="IO_5" pad="N22"/>
<connect gate="G" pin="IO_6" pad="N30"/>
<connect gate="G" pin="IO_7" pad="N23"/>
<connect gate="G" pin="IO_8" pad="M30"/>
<connect gate="G" pin="IO_9" pad="N31"/>
<connect gate="G" pin="VCCA_PLL1" pad="T24"/>
<connect gate="G" pin="VCCINT" pad="N19"/>
<connect gate="G" pin="VCCINT_10" pad="T16"/>
<connect gate="G" pin="VCCINT_11" pad="R15"/>
<connect gate="G" pin="VCCINT_12" pad="T20"/>
<connect gate="G" pin="VCCINT_13" pad="T18"/>
<connect gate="G" pin="VCCINT_14" pad="N15"/>
<connect gate="G" pin="VCCINT_15" pad="N13"/>
<connect gate="G" pin="VCCINT_16" pad="N17"/>
<connect gate="G" pin="VCCINT_2" pad="P14"/>
<connect gate="G" pin="VCCINT_3" pad="R13"/>
<connect gate="G" pin="VCCINT_4" pad="P16"/>
<connect gate="G" pin="VCCINT_5" pad="P18"/>
<connect gate="G" pin="VCCINT_6" pad="R19"/>
<connect gate="G" pin="VCCINT_7" pad="T14"/>
<connect gate="G" pin="VCCINT_8" pad="R17"/>
<connect gate="G" pin="VCCINT_9" pad="P20"/>
<connect gate="G" pin="VCCIO2" pad="R32"/>
<connect gate="G" pin="VCCIO2_2" pad="T21"/>
<connect gate="G" pin="VCCIO5" pad="T12"/>
<connect gate="G" pin="VCCPD2" pad="R21"/>
<connect gate="G" pin="VCCPD2_2" pad="N21"/>
<connect gate="G" pin="VCCPD5" pad="R12"/>
<connect gate="G" pin="VCCPD5_2" pad="N12"/>
<connect gate="G" pin="VREFB2N4" pad="P30"/>
<connect gate="H" pin="CLK3N" pad="U29"/>
<connect gate="H" pin="CLK3P" pad="U30"/>
<connect gate="H" pin="GND" pad="Y19"/>
<connect gate="H" pin="GNDA_PLL2" pad="U26"/>
<connect gate="H" pin="GNDA_PLL2_2" pad="U25"/>
<connect gate="H" pin="GND_10" pad="V11"/>
<connect gate="H" pin="GND_11" pad="V22"/>
<connect gate="H" pin="GND_12" pad="W20"/>
<connect gate="H" pin="GND_13" pad="V27"/>
<connect gate="H" pin="GND_14" pad="U14"/>
<connect gate="H" pin="GND_15" pad="Y13"/>
<connect gate="H" pin="GND_16" pad="U16"/>
<connect gate="H" pin="GND_17" pad="Y15"/>
<connect gate="H" pin="GND_18" pad="U18"/>
<connect gate="H" pin="GND_19" pad="Y17"/>
<connect gate="H" pin="GND_2" pad="W12"/>
<connect gate="H" pin="GND_20" pad="U20"/>
<connect gate="H" pin="GND_3" pad="V17"/>
<connect gate="H" pin="GND_4" pad="V15"/>
<connect gate="H" pin="GND_5" pad="W16"/>
<connect gate="H" pin="GND_6" pad="V13"/>
<connect gate="H" pin="GND_7" pad="W14"/>
<connect gate="H" pin="GND_8" pad="V19"/>
<connect gate="H" pin="GND_9" pad="W18"/>
<connect gate="H" pin="IO" pad="Y31"/>
<connect gate="H" pin="IO_10" pad="V28"/>
<connect gate="H" pin="IO_11" pad="U32"/>
<connect gate="H" pin="IO_12" pad="V29"/>
<connect gate="H" pin="IO_13" pad="V24"/>
<connect gate="H" pin="IO_14" pad="V30"/>
<connect gate="H" pin="IO_15" pad="U10"/>
<connect gate="H" pin="IO_16" pad="V10"/>
<connect gate="H" pin="IO_17" pad="U11"/>
<connect gate="H" pin="IO_18" pad="V31"/>
<connect gate="H" pin="IO_19" pad="W10"/>
<connect gate="H" pin="IO_2" pad="U27"/>
<connect gate="H" pin="IO_20" pad="W11"/>
<connect gate="H" pin="IO_21" pad="W22"/>
<connect gate="H" pin="IO_22" pad="W23"/>
<connect gate="H" pin="IO_23" pad="W24"/>
<connect gate="H" pin="IO_24" pad="W25"/>
<connect gate="H" pin="IO_25" pad="W26"/>
<connect gate="H" pin="IO_26" pad="W27"/>
<connect gate="H" pin="IO_27" pad="W28"/>
<connect gate="H" pin="IO_28" pad="W29"/>
<connect gate="H" pin="IO_29" pad="W31"/>
<connect gate="H" pin="IO_3" pad="U28"/>
<connect gate="H" pin="IO_30" pad="W32"/>
<connect gate="H" pin="IO_31" pad="Y10"/>
<connect gate="H" pin="IO_32" pad="Y11"/>
<connect gate="H" pin="IO_33" pad="Y22"/>
<connect gate="H" pin="IO_34" pad="Y23"/>
<connect gate="H" pin="IO_35" pad="Y24"/>
<connect gate="H" pin="IO_36" pad="Y25"/>
<connect gate="H" pin="IO_37" pad="Y26"/>
<connect gate="H" pin="IO_38" pad="Y27"/>
<connect gate="H" pin="IO_39" pad="Y28"/>
<connect gate="H" pin="IO_4" pad="U22"/>
<connect gate="H" pin="IO_40" pad="Y29"/>
<connect gate="H" pin="IO_41" pad="Y30"/>
<connect gate="H" pin="IO_5" pad="U23"/>
<connect gate="H" pin="IO_6" pad="T31"/>
<connect gate="H" pin="IO_7" pad="U31"/>
<connect gate="H" pin="IO_8" pad="T32"/>
<connect gate="H" pin="IO_9" pad="V23"/>
<connect gate="H" pin="VCCA_PLL2" pad="V26"/>
<connect gate="H" pin="VCCD_PLL1" pad="U24"/>
<connect gate="H" pin="VCCD_PLL2" pad="V25"/>
<connect gate="H" pin="VCCINT" pad="W19"/>
<connect gate="H" pin="VCCINT_10" pad="V18"/>
<connect gate="H" pin="VCCINT_11" pad="Y14"/>
<connect gate="H" pin="VCCINT_12" pad="U13"/>
<connect gate="H" pin="VCCINT_13" pad="V20"/>
<connect gate="H" pin="VCCINT_14" pad="U17"/>
<connect gate="H" pin="VCCINT_15" pad="U19"/>
<connect gate="H" pin="VCCINT_16" pad="W17"/>
<connect gate="H" pin="VCCINT_17" pad="Y20"/>
<connect gate="H" pin="VCCINT_2" pad="W13"/>
<connect gate="H" pin="VCCINT_3" pad="W15"/>
<connect gate="H" pin="VCCINT_4" pad="Y18"/>
<connect gate="H" pin="VCCINT_5" pad="W21"/>
<connect gate="H" pin="VCCINT_6" pad="V16"/>
<connect gate="H" pin="VCCINT_7" pad="Y16"/>
<connect gate="H" pin="VCCINT_8" pad="U15"/>
<connect gate="H" pin="VCCINT_9" pad="V14"/>
<connect gate="H" pin="VCCIO1" pad="V32"/>
<connect gate="H" pin="VCCIO1_2" pad="U21"/>
<connect gate="H" pin="VCCIO6" pad="U12"/>
<connect gate="H" pin="VCCPD1" pad="Y21"/>
<connect gate="H" pin="VCCPD1_2" pad="V21"/>
<connect gate="H" pin="VCCPD6" pad="Y12"/>
<connect gate="H" pin="VCCPD6_2" pad="V12"/>
<connect gate="H" pin="VREFB1N0" pad="W30"/>
<connect gate="I" pin="GND" pad="AA21"/>
<connect gate="I" pin="GNDA_PLL12" pad="AD17"/>
<connect gate="I" pin="GNDA_PLL6" pad="AD16"/>
<connect gate="I" pin="GND_2" pad="AA19"/>
<connect gate="I" pin="GND_3" pad="AC28"/>
<connect gate="I" pin="GND_4" pad="Y32"/>
<connect gate="I" pin="GND_5" pad="AB22"/>
<connect gate="I" pin="GND_6" pad="AA14"/>
<connect gate="I" pin="IO" pad="AD32"/>
<connect gate="I" pin="IO_10" pad="AB12"/>
<connect gate="I" pin="IO_11" pad="AB13"/>
<connect gate="I" pin="IO_12" pad="AB14"/>
<connect gate="I" pin="IO_13" pad="AB15"/>
<connect gate="I" pin="IO_14" pad="AB16"/>
<connect gate="I" pin="IO_15" pad="AB17"/>
<connect gate="I" pin="IO_16" pad="AB18"/>
<connect gate="I" pin="IO_17" pad="AB19"/>
<connect gate="I" pin="IO_18" pad="AA22"/>
<connect gate="I" pin="IO_19" pad="AB20"/>
<connect gate="I" pin="IO_2" pad="AA10"/>
<connect gate="I" pin="IO_20" pad="AA23"/>
<connect gate="I" pin="IO_21" pad="AB21"/>
<connect gate="I" pin="IO_22" pad="AA24"/>
<connect gate="I" pin="IO_23" pad="AA25"/>
<connect gate="I" pin="IO_24" pad="AB23"/>
<connect gate="I" pin="IO_25" pad="AA26"/>
<connect gate="I" pin="IO_26" pad="AB24"/>
<connect gate="I" pin="IO_27" pad="AA27"/>
<connect gate="I" pin="IO_28" pad="AB25"/>
<connect gate="I" pin="IO_29" pad="AB26"/>
<connect gate="I" pin="IO_3" pad="AA29"/>
<connect gate="I" pin="IO_30" pad="AB27"/>
<connect gate="I" pin="IO_31" pad="AB28"/>
<connect gate="I" pin="IO_32" pad="AB29"/>
<connect gate="I" pin="IO_33" pad="AB30"/>
<connect gate="I" pin="IO_34" pad="AB31"/>
<connect gate="I" pin="IO_35" pad="AB32"/>
<connect gate="I" pin="IO_36" pad="AC11"/>
<connect gate="I" pin="IO_37" pad="AC12"/>
<connect gate="I" pin="IO_38" pad="AC13"/>
<connect gate="I" pin="IO_39" pad="AC14"/>
<connect gate="I" pin="IO_4" pad="AA11"/>
<connect gate="I" pin="IO_40" pad="AC15"/>
<connect gate="I" pin="IO_41" pad="AC16"/>
<connect gate="I" pin="IO_42" pad="AC17"/>
<connect gate="I" pin="IO_43" pad="AC18"/>
<connect gate="I" pin="IO_44" pad="AC19"/>
<connect gate="I" pin="IO_45" pad="AC20"/>
<connect gate="I" pin="IO_46" pad="AC21"/>
<connect gate="I" pin="IO_47" pad="AC22"/>
<connect gate="I" pin="IO_48" pad="AC24"/>
<connect gate="I" pin="IO_49" pad="AC25"/>
<connect gate="I" pin="IO_5" pad="AA30"/>
<connect gate="I" pin="IO_50" pad="AC26"/>
<connect gate="I" pin="IO_51" pad="AC27"/>
<connect gate="I" pin="IO_52" pad="AC29"/>
<connect gate="I" pin="IO_53" pad="AC30"/>
<connect gate="I" pin="IO_54" pad="AC31"/>
<connect gate="I" pin="IO_55" pad="AC32"/>
<connect gate="I" pin="IO_56" pad="AD10"/>
<connect gate="I" pin="IO_57" pad="AD11"/>
<connect gate="I" pin="IO_58" pad="AD12"/>
<connect gate="I" pin="IO_59" pad="AD13"/>
<connect gate="I" pin="IO_6" pad="AA31"/>
<connect gate="I" pin="IO_60" pad="AD14"/>
<connect gate="I" pin="IO_61" pad="AD18"/>
<connect gate="I" pin="IO_62" pad="AD19"/>
<connect gate="I" pin="IO_63" pad="AD20"/>
<connect gate="I" pin="IO_64" pad="AD21"/>
<connect gate="I" pin="IO_65" pad="AD22"/>
<connect gate="I" pin="IO_66" pad="AD23"/>
<connect gate="I" pin="IO_67" pad="AD24"/>
<connect gate="I" pin="IO_68" pad="AD25"/>
<connect gate="I" pin="IO_69" pad="AD26"/>
<connect gate="I" pin="IO_7" pad="AA32"/>
<connect gate="I" pin="IO_70" pad="AD27"/>
<connect gate="I" pin="IO_71" pad="AD29"/>
<connect gate="I" pin="IO_72" pad="AD30"/>
<connect gate="I" pin="IO_73" pad="AD31"/>
<connect gate="I" pin="IO_8" pad="AB10"/>
<connect gate="I" pin="IO_9" pad="AB11"/>
<connect gate="I" pin="VCCD_PLL6" pad="AD15"/>
<connect gate="I" pin="VCCINT" pad="AC10"/>
<connect gate="I" pin="VCCINT_2" pad="AA12"/>
<connect gate="I" pin="VCCIO1" pad="AA28"/>
<connect gate="I" pin="VCCIO7" pad="AA16"/>
<connect gate="I" pin="VCCIO8" pad="AA17"/>
<connect gate="I" pin="VCCPD7" pad="AA15"/>
<connect gate="I" pin="VCCPD7_2" pad="AA13"/>
<connect gate="I" pin="VCCPD8" pad="AA18"/>
<connect gate="I" pin="VCCPD8_2" pad="AA20"/>
<connect gate="I" pin="VCCSEL" pad="AC23"/>
<connect gate="I" pin="VREFB1N1" pad="AD28"/>
<connect gate="J" pin="GND" pad="AH27"/>
<connect gate="J" pin="GNDA_PLL12" pad="AE17"/>
<connect gate="J" pin="GNDA_PLL6" pad="AE16"/>
<connect gate="J" pin="GNDA_PLL8" pad="AG27"/>
<connect gate="J" pin="GNDA_PLL8_2" pad="AG26"/>
<connect gate="J" pin="GND_2" pad="AF17"/>
<connect gate="J" pin="GND_3" pad="AH10"/>
<connect gate="J" pin="GND_4" pad="AH23"/>
<connect gate="J" pin="IO" pad="AJ10"/>
<connect gate="J" pin="IO_10" pad="AE26"/>
<connect gate="J" pin="IO_11" pad="AE14"/>
<connect gate="J" pin="IO_12" pad="AE27"/>
<connect gate="J" pin="IO_13" pad="AE22"/>
<connect gate="J" pin="IO_14" pad="AE28"/>
<connect gate="J" pin="IO_15" pad="AE23"/>
<connect gate="J" pin="IO_16" pad="AE29"/>
<connect gate="J" pin="IO_17" pad="AE30"/>
<connect gate="J" pin="IO_18" pad="AE31"/>
<connect gate="J" pin="IO_19" pad="AE32"/>
<connect gate="J" pin="IO_2" pad="AE10"/>
<connect gate="J" pin="IO_20" pad="AF19"/>
<connect gate="J" pin="IO_21" pad="AF10"/>
<connect gate="J" pin="IO_22" pad="AF20"/>
<connect gate="J" pin="IO_23" pad="AF11"/>
<connect gate="J" pin="IO_24" pad="AF21"/>
<connect gate="J" pin="IO_25" pad="AF29"/>
<connect gate="J" pin="IO_26" pad="AF12"/>
<connect gate="J" pin="IO_27" pad="AF30"/>
<connect gate="J" pin="IO_28" pad="AF22"/>
<connect gate="J" pin="IO_29" pad="AF31"/>
<connect gate="J" pin="IO_3" pad="AE11"/>
<connect gate="J" pin="IO_30" pad="AF13"/>
<connect gate="J" pin="IO_31" pad="AF32"/>
<connect gate="J" pin="IO_32" pad="AF23"/>
<connect gate="J" pin="IO_33" pad="AG10"/>
<connect gate="J" pin="IO_34" pad="AG11"/>
<connect gate="J" pin="IO_35" pad="AG12"/>
<connect gate="J" pin="IO_36" pad="AG13"/>
<connect gate="J" pin="IO_37" pad="AG14"/>
<connect gate="J" pin="IO_38" pad="AG15"/>
<connect gate="J" pin="IO_39" pad="AG16"/>
<connect gate="J" pin="IO_4" pad="AE19"/>
<connect gate="J" pin="IO_40" pad="AG17"/>
<connect gate="J" pin="IO_41" pad="AG18"/>
<connect gate="J" pin="IO_42" pad="AG19"/>
<connect gate="J" pin="IO_43" pad="AG20"/>
<connect gate="J" pin="IO_44" pad="AG22"/>
<connect gate="J" pin="IO_45" pad="AG23"/>
<connect gate="J" pin="IO_46" pad="AG24"/>
<connect gate="J" pin="IO_47" pad="AG29"/>
<connect gate="J" pin="IO_48" pad="AG30"/>
<connect gate="J" pin="IO_49" pad="AG31"/>
<connect gate="J" pin="IO_5" pad="AE12"/>
<connect gate="J" pin="IO_50" pad="AG32"/>
<connect gate="J" pin="IO_51" pad="AH11"/>
<connect gate="J" pin="IO_52" pad="AH13"/>
<connect gate="J" pin="IO_53" pad="AH14"/>
<connect gate="J" pin="IO_54" pad="AH15"/>
<connect gate="J" pin="IO_55" pad="AH16"/>
<connect gate="J" pin="IO_56" pad="AH17"/>
<connect gate="J" pin="IO_57" pad="AH18"/>
<connect gate="J" pin="IO_58" pad="AH19"/>
<connect gate="J" pin="IO_59" pad="AH20"/>
<connect gate="J" pin="IO_6" pad="AE20"/>
<connect gate="J" pin="IO_60" pad="AH22"/>
<connect gate="J" pin="IO_61" pad="AH24"/>
<connect gate="J" pin="IO_62" pad="AH25"/>
<connect gate="J" pin="IO_63" pad="AH26"/>
<connect gate="J" pin="IO_64" pad="AH28"/>
<connect gate="J" pin="IO_65" pad="AH29"/>
<connect gate="J" pin="IO_66" pad="AH30"/>
<connect gate="J" pin="IO_67" pad="AH31"/>
<connect gate="J" pin="IO_68" pad="AH32"/>
<connect gate="J" pin="IO_7" pad="AE13"/>
<connect gate="J" pin="IO_8" pad="AE25"/>
<connect gate="J" pin="IO_9" pad="AE21"/>
<connect gate="J" pin="TCK" pad="AF24"/>
<connect gate="J" pin="TMS" pad="AE24"/>
<connect gate="J" pin="VCCA_PLL12" pad="AF18"/>
<connect gate="J" pin="VCCA_PLL6" pad="AE15"/>
<connect gate="J" pin="VCCA_PLL8" pad="AF26"/>
<connect gate="J" pin="VCCD_PLL12" pad="AE18"/>
<connect gate="J" pin="VCCD_PLL8" pad="AF25"/>
<connect gate="J" pin="VCCIO7" pad="AH12"/>
<connect gate="J" pin="VCCIO8" pad="AH21"/>
<connect gate="J" pin="VCC_PLL12_OUT" pad="AF16"/>
<connect gate="J" pin="VCC_PLL6_OUT" pad="AF15"/>
<connect gate="J" pin="VREFB1N2" pad="AF28"/>
<connect gate="J" pin="VREFB1N3" pad="AF27"/>
<connect gate="J" pin="VREFB1N4" pad="AG28"/>
<connect gate="J" pin="VREFB7N1" pad="AF14"/>
<connect gate="J" pin="VREFB8N1" pad="AG25"/>
<connect gate="J" pin="VREFB8N2" pad="AG21"/>
<connect gate="K" pin="FPLL8CLKN" pad="AJ29"/>
<connect gate="K" pin="FPLL8CLKP" pad="AJ30"/>
<connect gate="K" pin="GND" pad="AM31"/>
<connect gate="K" pin="GND_2" pad="AM20"/>
<connect gate="K" pin="GND_3" pad="AL32"/>
<connect gate="K" pin="GND_4" pad="AM13"/>
<connect gate="K" pin="IO" pad="AM29"/>
<connect gate="K" pin="IO_10" pad="AJ19"/>
<connect gate="K" pin="IO_11" pad="AJ20"/>
<connect gate="K" pin="IO_12" pad="AJ21"/>
<connect gate="K" pin="IO_13" pad="AJ25"/>
<connect gate="K" pin="IO_14" pad="AJ22"/>
<connect gate="K" pin="IO_15" pad="AJ26"/>
<connect gate="K" pin="IO_16" pad="AJ23"/>
<connect gate="K" pin="IO_17" pad="AJ27"/>
<connect gate="K" pin="IO_18" pad="AJ31"/>
<connect gate="K" pin="IO_19" pad="AJ28"/>
<connect gate="K" pin="IO_2" pad="AJ11"/>
<connect gate="K" pin="IO_20" pad="AJ32"/>
<connect gate="K" pin="IO_21" pad="AK10"/>
<connect gate="K" pin="IO_22" pad="AK11"/>
<connect gate="K" pin="IO_23" pad="AK12"/>
<connect gate="K" pin="IO_24" pad="AK15"/>
<connect gate="K" pin="IO_25" pad="AK13"/>
<connect gate="K" pin="IO_26" pad="AK16"/>
<connect gate="K" pin="IO_27" pad="AK17"/>
<connect gate="K" pin="IO_28" pad="AK18"/>
<connect gate="K" pin="IO_29" pad="AK20"/>
<connect gate="K" pin="IO_3" pad="AJ12"/>
<connect gate="K" pin="IO_30" pad="AK21"/>
<connect gate="K" pin="IO_31" pad="AK22"/>
<connect gate="K" pin="IO_32" pad="AK23"/>
<connect gate="K" pin="IO_33" pad="AK24"/>
<connect gate="K" pin="IO_34" pad="AK25"/>
<connect gate="K" pin="IO_35" pad="AK26"/>
<connect gate="K" pin="IO_36" pad="AK27"/>
<connect gate="K" pin="IO_37" pad="AK28"/>
<connect gate="K" pin="IO_38" pad="AK29"/>
<connect gate="K" pin="IO_39" pad="AL10"/>
<connect gate="K" pin="IO_4" pad="AJ13"/>
<connect gate="K" pin="IO_40" pad="AL11"/>
<connect gate="K" pin="IO_41" pad="AL12"/>
<connect gate="K" pin="IO_42" pad="AL13"/>
<connect gate="K" pin="IO_43" pad="AL14"/>
<connect gate="K" pin="IO_44" pad="AL15"/>
<connect gate="K" pin="IO_45" pad="AL16"/>
<connect gate="K" pin="IO_46" pad="AL17"/>
<connect gate="K" pin="IO_47" pad="AL18"/>
<connect gate="K" pin="IO_48" pad="AL19"/>
<connect gate="K" pin="IO_49" pad="AL20"/>
<connect gate="K" pin="IO_5" pad="AJ14"/>
<connect gate="K" pin="IO_50" pad="AL21"/>
<connect gate="K" pin="IO_51" pad="AL22"/>
<connect gate="K" pin="IO_52" pad="AL23"/>
<connect gate="K" pin="IO_53" pad="AL24"/>
<connect gate="K" pin="IO_54" pad="AL25"/>
<connect gate="K" pin="IO_55" pad="AL26"/>
<connect gate="K" pin="IO_56" pad="AL27"/>
<connect gate="K" pin="IO_57" pad="AL28"/>
<connect gate="K" pin="IO_58" pad="AL29"/>
<connect gate="K" pin="IO_59" pad="AM10"/>
<connect gate="K" pin="IO_6" pad="AJ15"/>
<connect gate="K" pin="IO_60" pad="AM11"/>
<connect gate="K" pin="IO_61" pad="AM12"/>
<connect gate="K" pin="IO_62" pad="AM14"/>
<connect gate="K" pin="IO_63" pad="AM16"/>
<connect gate="K" pin="IO_64" pad="AM17"/>
<connect gate="K" pin="IO_65" pad="AM19"/>
<connect gate="K" pin="IO_66" pad="AM21"/>
<connect gate="K" pin="IO_67" pad="AM22"/>
<connect gate="K" pin="IO_68" pad="AM23"/>
<connect gate="K" pin="IO_69" pad="AM24"/>
<connect gate="K" pin="IO_7" pad="AJ16"/>
<connect gate="K" pin="IO_70" pad="AM25"/>
<connect gate="K" pin="IO_71" pad="AM26"/>
<connect gate="K" pin="IO_72" pad="AM27"/>
<connect gate="K" pin="IO_73" pad="AM28"/>
<connect gate="K" pin="IO_8" pad="AJ17"/>
<connect gate="K" pin="IO_9" pad="AJ18"/>
<connect gate="K" pin="NCONFIG" pad="AL30"/>
<connect gate="K" pin="TDI" pad="AL31"/>
<connect gate="K" pin="TRST" pad="AK30"/>
<connect gate="K" pin="VCCIO1" pad="AK32"/>
<connect gate="K" pin="VCCIO7" pad="AM15"/>
<connect gate="K" pin="VCCIO8" pad="AM18"/>
<connect gate="K" pin="VCCIO8_2" pad="AM30"/>
<connect gate="K" pin="VREFB7N0" pad="AK14"/>
<connect gate="K" pin="VREFB8N0" pad="AK31"/>
<connect gate="K" pin="VREFB8N3" pad="AJ24"/>
<connect gate="K" pin="VREFB8N4" pad="AK19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S180F1020C3N"/>
<attribute name="OC_FARNELL" value="1637234"/>
<attribute name="OC_NEWARK" value="51R0583"/>
<attribute name="PACKAGE" value="BGA-1020"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S30F484C3N">
<description>Stratix II Devices</description>
<gates>
<gate name="A" symbol="EP2S30F484C3N_A"/>
<gate name="B" symbol="EP2S30F484C3N_B"/>
<gate name="C" symbol="EP2S30F484C3N_C"/>
<gate name="D" symbol="EP2S30F484C3N_D"/>
<gate name="E" symbol="EP2S30F484C3N_E"/>
</gates>
<devices>
<device name="" package="BGA484C22X22X100P_2300X2300X35">
<connects>
<connect gate="A" pin="GND" pad="K9"/>
<connect gate="A" pin="GNDA_PLL4" pad="L5"/>
<connect gate="A" pin="GNDA_PLL4_2" pad="L4"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="A9"/>
<connect gate="A" pin="GND_4" pad="J1"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B9"/>
<connect gate="A" pin="IO_11" pad="C1"/>
<connect gate="A" pin="IO_12" pad="C2"/>
<connect gate="A" pin="IO_13" pad="C4"/>
<connect gate="A" pin="IO_14" pad="C5"/>
<connect gate="A" pin="IO_15" pad="C6"/>
<connect gate="A" pin="IO_16" pad="C7"/>
<connect gate="A" pin="IO_17" pad="C8"/>
<connect gate="A" pin="IO_18" pad="C9"/>
<connect gate="A" pin="IO_19" pad="D1"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="D2"/>
<connect gate="A" pin="IO_21" pad="D3"/>
<connect gate="A" pin="IO_22" pad="D5"/>
<connect gate="A" pin="IO_23" pad="D6"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="E1"/>
<connect gate="A" pin="IO_26" pad="E2"/>
<connect gate="A" pin="IO_27" pad="E3"/>
<connect gate="A" pin="IO_28" pad="E4"/>
<connect gate="A" pin="IO_29" pad="E6"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="E7"/>
<connect gate="A" pin="IO_31" pad="E8"/>
<connect gate="A" pin="IO_32" pad="E9"/>
<connect gate="A" pin="IO_33" pad="F1"/>
<connect gate="A" pin="IO_34" pad="F2"/>
<connect gate="A" pin="IO_35" pad="F4"/>
<connect gate="A" pin="IO_36" pad="F5"/>
<connect gate="A" pin="IO_37" pad="F6"/>
<connect gate="A" pin="IO_38" pad="F7"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="G9"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B5"/>
<connect gate="A" pin="IO_60" pad="J5"/>
<connect gate="A" pin="IO_61" pad="J6"/>
<connect gate="A" pin="IO_62" pad="J7"/>
<connect gate="A" pin="IO_63" pad="J8"/>
<connect gate="A" pin="IO_64" pad="K1"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_66" pad="K3"/>
<connect gate="A" pin="IO_67" pad="K4"/>
<connect gate="A" pin="IO_68" pad="K5"/>
<connect gate="A" pin="IO_69" pad="K6"/>
<connect gate="A" pin="IO_7" pad="B6"/>
<connect gate="A" pin="IO_70" pad="K7"/>
<connect gate="A" pin="IO_71" pad="K8"/>
<connect gate="A" pin="IO_72" pad="L2"/>
<connect gate="A" pin="IO_73" pad="L3"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="B8"/>
<connect gate="A" pin="MSEL0" pad="E5"/>
<connect gate="A" pin="MSEL1" pad="D4"/>
<connect gate="A" pin="MSEL2" pad="B4"/>
<connect gate="A" pin="MSEL3" pad="A4"/>
<connect gate="A" pin="TDO" pad="B3"/>
<connect gate="A" pin="TEMPDIODEN" pad="C3"/>
<connect gate="A" pin="TEMPDIODEP" pad="A2"/>
<connect gate="A" pin="VCCD_PLL4" pad="L6"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="H8"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="B1"/>
<connect gate="A" pin="VREFB4N0" pad="D7"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N0" pad="J4"/>
<connect gate="A" pin="VREFB5N1" pad="F3"/>
<connect gate="B" pin="CLK11N" pad="M3"/>
<connect gate="B" pin="CLK11P" pad="M2"/>
<connect gate="B" pin="CLK9N" pad="N4"/>
<connect gate="B" pin="CLK9P" pad="N3"/>
<connect gate="B" pin="GND" pad="M7"/>
<connect gate="B" pin="GNDA_PLL3" pad="N6"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="N5"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="M9"/>
<connect gate="B" pin="GND_4" pad="A14"/>
<connect gate="B" pin="GND_5" pad="A22"/>
<connect gate="B" pin="IO" pad="A19"/>
<connect gate="B" pin="IO_10" pad="P6"/>
<connect gate="B" pin="IO_11" pad="P7"/>
<connect gate="B" pin="IO_12" pad="P8"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="R2"/>
<connect gate="B" pin="IO_15" pad="R3"/>
<connect gate="B" pin="IO_16" pad="R4"/>
<connect gate="B" pin="IO_17" pad="R5"/>
<connect gate="B" pin="IO_18" pad="R6"/>
<connect gate="B" pin="IO_19" pad="R7"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R8"/>
<connect gate="B" pin="IO_21" pad="R9"/>
<connect gate="B" pin="IO_22" pad="T1"/>
<connect gate="B" pin="IO_23" pad="T2"/>
<connect gate="B" pin="IO_24" pad="T3"/>
<connect gate="B" pin="IO_25" pad="T4"/>
<connect gate="B" pin="IO_26" pad="T5"/>
<connect gate="B" pin="IO_27" pad="T6"/>
<connect gate="B" pin="IO_28" pad="T7"/>
<connect gate="B" pin="IO_29" pad="T8"/>
<connect gate="B" pin="IO_3" pad="N1"/>
<connect gate="B" pin="IO_30" pad="T9"/>
<connect gate="B" pin="IO_31" pad="U1"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V3"/>
<connect gate="B" pin="IO_42" pad="V4"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="V9"/>
<connect gate="B" pin="IO_47" pad="W1"/>
<connect gate="B" pin="IO_48" pad="W2"/>
<connect gate="B" pin="IO_49" pad="W3"/>
<connect gate="B" pin="IO_5" pad="N7"/>
<connect gate="B" pin="IO_50" pad="W4"/>
<connect gate="B" pin="IO_51" pad="W5"/>
<connect gate="B" pin="IO_52" pad="W7"/>
<connect gate="B" pin="IO_53" pad="W9"/>
<connect gate="B" pin="IO_54" pad="Y1"/>
<connect gate="B" pin="IO_55" pad="Y2"/>
<connect gate="B" pin="IO_56" pad="Y3"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="N8"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A13"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_7" pad="P2"/>
<connect gate="B" pin="IO_8" pad="P3"/>
<connect gate="B" pin="IO_9" pad="P5"/>
<connect gate="B" pin="NCE" pad="A21"/>
<connect gate="B" pin="PLL_ENA" pad="Y4"/>
<connect gate="B" pin="PORSEL" pad="V5"/>
<connect gate="B" pin="VCCA_PLL3" pad="M4"/>
<connect gate="B" pin="VCCA_PLL4" pad="M6"/>
<connect gate="B" pin="VCCD_PLL3" pad="M5"/>
<connect gate="B" pin="VCCINT" pad="P9"/>
<connect gate="B" pin="VCCINT_2" pad="M8"/>
<connect gate="B" pin="VCCIO3" pad="A20"/>
<connect gate="B" pin="VCCIO3_2" pad="A12"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="AA1"/>
<connect gate="B" pin="VCCIO6_2" pad="M1"/>
<connect gate="B" pin="VCCPD5" pad="L9"/>
<connect gate="B" pin="VCCPD6" pad="N9"/>
<connect gate="B" pin="VREFB6N0" pad="U3"/>
<connect gate="B" pin="VREFB6N1" pad="P4"/>
<connect gate="B" pin="VREFB7N0" pad="W8"/>
<connect gate="B" pin="VREFB7N1" pad="W6"/>
<connect gate="C" pin="CONF_DONE" pad="C20"/>
<connect gate="C" pin="DCLK" pad="D19"/>
<connect gate="C" pin="GND" pad="B21"/>
<connect gate="C" pin="GNDA_PLL5" pad="F11"/>
<connect gate="C" pin="GNDA_PLL5_2" pad="F10"/>
<connect gate="C" pin="GND_2" pad="AA2"/>
<connect gate="C" pin="GND_3" pad="AB1"/>
<connect gate="C" pin="GND_4" pad="AB4"/>
<connect gate="C" pin="GND_5" pad="AB9"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="AB7"/>
<connect gate="C" pin="IO_11" pad="AB8"/>
<connect gate="C" pin="IO_12" pad="B10"/>
<connect gate="C" pin="IO_13" pad="B11"/>
<connect gate="C" pin="IO_14" pad="B12"/>
<connect gate="C" pin="IO_15" pad="B13"/>
<connect gate="C" pin="IO_16" pad="B15"/>
<connect gate="C" pin="IO_17" pad="B16"/>
<connect gate="C" pin="IO_18" pad="B17"/>
<connect gate="C" pin="IO_19" pad="B18"/>
<connect gate="C" pin="IO_2" pad="AA4"/>
<connect gate="C" pin="IO_20" pad="B19"/>
<connect gate="C" pin="IO_21" pad="C10"/>
<connect gate="C" pin="IO_22" pad="C11"/>
<connect gate="C" pin="IO_23" pad="C12"/>
<connect gate="C" pin="IO_24" pad="C13"/>
<connect gate="C" pin="IO_25" pad="C14"/>
<connect gate="C" pin="IO_26" pad="C15"/>
<connect gate="C" pin="IO_27" pad="C16"/>
<connect gate="C" pin="IO_28" pad="C17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="AA5"/>
<connect gate="C" pin="IO_30" pad="C19"/>
<connect gate="C" pin="IO_31" pad="C21"/>
<connect gate="C" pin="IO_32" pad="C22"/>
<connect gate="C" pin="IO_33" pad="D10"/>
<connect gate="C" pin="IO_34" pad="D11"/>
<connect gate="C" pin="IO_35" pad="D12"/>
<connect gate="C" pin="IO_36" pad="D13"/>
<connect gate="C" pin="IO_37" pad="D14"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D17"/>
<connect gate="C" pin="IO_4" pad="AA6"/>
<connect gate="C" pin="IO_40" pad="D18"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E10"/>
<connect gate="C" pin="IO_45" pad="E11"/>
<connect gate="C" pin="IO_46" pad="E12"/>
<connect gate="C" pin="IO_47" pad="E13"/>
<connect gate="C" pin="IO_48" pad="E14"/>
<connect gate="C" pin="IO_49" pad="E15"/>
<connect gate="C" pin="IO_5" pad="AA7"/>
<connect gate="C" pin="IO_50" pad="E16"/>
<connect gate="C" pin="IO_51" pad="E17"/>
<connect gate="C" pin="IO_52" pad="E18"/>
<connect gate="C" pin="IO_53" pad="E19"/>
<connect gate="C" pin="IO_54" pad="E20"/>
<connect gate="C" pin="IO_55" pad="E21"/>
<connect gate="C" pin="IO_56" pad="E22"/>
<connect gate="C" pin="IO_57" pad="F13"/>
<connect gate="C" pin="IO_58" pad="F14"/>
<connect gate="C" pin="IO_59" pad="F15"/>
<connect gate="C" pin="IO_6" pad="AA8"/>
<connect gate="C" pin="IO_60" pad="F16"/>
<connect gate="C" pin="IO_61" pad="F17"/>
<connect gate="C" pin="IO_62" pad="F19"/>
<connect gate="C" pin="IO_63" pad="F20"/>
<connect gate="C" pin="IO_64" pad="F21"/>
<connect gate="C" pin="IO_65" pad="F22"/>
<connect gate="C" pin="IO_66" pad="G12"/>
<connect gate="C" pin="IO_67" pad="G13"/>
<connect gate="C" pin="IO_68" pad="G14"/>
<connect gate="C" pin="IO_69" pad="G15"/>
<connect gate="C" pin="IO_7" pad="AA9"/>
<connect gate="C" pin="IO_70" pad="G16"/>
<connect gate="C" pin="IO_71" pad="G17"/>
<connect gate="C" pin="IO_72" pad="G18"/>
<connect gate="C" pin="IO_73" pad="G19"/>
<connect gate="C" pin="IO_74" pad="G20"/>
<connect gate="C" pin="IO_75" pad="G21"/>
<connect gate="C" pin="IO_76" pad="G22"/>
<connect gate="C" pin="IO_8" pad="AB5"/>
<connect gate="C" pin="IO_9" pad="AB6"/>
<connect gate="C" pin="NCEO" pad="AA3"/>
<connect gate="C" pin="NIO_PULLUP" pad="AB2"/>
<connect gate="C" pin="NSTATUS" pad="B20"/>
<connect gate="C" pin="VCCA_PLL5" pad="F12"/>
<connect gate="C" pin="VCCD_PLL5" pad="G11"/>
<connect gate="C" pin="VCCIO2" pad="B22"/>
<connect gate="C" pin="VCCIO7" pad="AB3"/>
<connect gate="C" pin="VCCPD4" pad="H10"/>
<connect gate="C" pin="VCC_PLL5_OUT" pad="G10"/>
<connect gate="C" pin="VREFB2N0" pad="F18"/>
<connect gate="C" pin="VREFB3N0" pad="B14"/>
<connect gate="C" pin="VREFB3N1" pad="D16"/>
<connect gate="D" pin="CLK1N" pad="M20"/>
<connect gate="D" pin="CLK1P" pad="M21"/>
<connect gate="D" pin="CLK3N" pad="N19"/>
<connect gate="D" pin="CLK3P" pad="N20"/>
<connect gate="D" pin="GND" pad="R10"/>
<connect gate="D" pin="GNDA_PLL1" pad="L18"/>
<connect gate="D" pin="GNDA_PLL1_2" pad="L17"/>
<connect gate="D" pin="GNDA_PLL2" pad="N18"/>
<connect gate="D" pin="GNDA_PLL2_2" pad="N17"/>
<connect gate="D" pin="GND_10" pad="M11"/>
<connect gate="D" pin="GND_11" pad="L14"/>
<connect gate="D" pin="GND_12" pad="N12"/>
<connect gate="D" pin="GND_13" pad="L10"/>
<connect gate="D" pin="GND_14" pad="P13"/>
<connect gate="D" pin="GND_15" pad="L12"/>
<connect gate="D" pin="GND_16" pad="N14"/>
<connect gate="D" pin="GND_17" pad="N10"/>
<connect gate="D" pin="GND_18" pad="P22"/>
<connect gate="D" pin="GND_19" pad="J10"/>
<connect gate="D" pin="GND_2" pad="K11"/>
<connect gate="D" pin="GND_20" pad="P11"/>
<connect gate="D" pin="GND_3" pad="H15"/>
<connect gate="D" pin="GND_4" pad="J12"/>
<connect gate="D" pin="GND_5" pad="K13"/>
<connect gate="D" pin="GND_6" pad="M13"/>
<connect gate="D" pin="GND_7" pad="J14"/>
<connect gate="D" pin="GND_8" pad="M15"/>
<connect gate="D" pin="GND_9" pad="J22"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="H22"/>
<connect gate="D" pin="IO_11" pad="J15"/>
<connect gate="D" pin="IO_12" pad="J16"/>
<connect gate="D" pin="IO_13" pad="J17"/>
<connect gate="D" pin="IO_14" pad="J18"/>
<connect gate="D" pin="IO_15" pad="J19"/>
<connect gate="D" pin="IO_16" pad="J20"/>
<connect gate="D" pin="IO_17" pad="J21"/>
<connect gate="D" pin="IO_18" pad="K15"/>
<connect gate="D" pin="IO_19" pad="K16"/>
<connect gate="D" pin="IO_2" pad="H12"/>
<connect gate="D" pin="IO_20" pad="K17"/>
<connect gate="D" pin="IO_21" pad="K18"/>
<connect gate="D" pin="IO_22" pad="K19"/>
<connect gate="D" pin="IO_23" pad="K20"/>
<connect gate="D" pin="IO_24" pad="K21"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="L15"/>
<connect gate="D" pin="IO_27" pad="L16"/>
<connect gate="D" pin="IO_28" pad="L20"/>
<connect gate="D" pin="IO_29" pad="L21"/>
<connect gate="D" pin="IO_3" pad="H14"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N16"/>
<connect gate="D" pin="IO_32" pad="N21"/>
<connect gate="D" pin="IO_33" pad="N22"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="P19"/>
<connect gate="D" pin="IO_38" pad="P20"/>
<connect gate="D" pin="IO_39" pad="P21"/>
<connect gate="D" pin="IO_4" pad="H16"/>
<connect gate="D" pin="IO_40" pad="R14"/>
<connect gate="D" pin="IO_41" pad="R15"/>
<connect gate="D" pin="IO_42" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H17"/>
<connect gate="D" pin="IO_6" pad="H18"/>
<connect gate="D" pin="IO_7" pad="H19"/>
<connect gate="D" pin="IO_8" pad="H20"/>
<connect gate="D" pin="IO_9" pad="H21"/>
<connect gate="D" pin="VCCA_PLL1" pad="M17"/>
<connect gate="D" pin="VCCA_PLL2" pad="M19"/>
<connect gate="D" pin="VCCA_PLL6" pad="R12"/>
<connect gate="D" pin="VCCD_PLL1" pad="M16"/>
<connect gate="D" pin="VCCD_PLL2" pad="M18"/>
<connect gate="D" pin="VCCINT" pad="P14"/>
<connect gate="D" pin="VCCINT_10" pad="M12"/>
<connect gate="D" pin="VCCINT_11" pad="N13"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="P12"/>
<connect gate="D" pin="VCCINT_2" pad="L11"/>
<connect gate="D" pin="VCCINT_3" pad="K12"/>
<connect gate="D" pin="VCCINT_4" pad="J11"/>
<connect gate="D" pin="VCCINT_5" pad="J13"/>
<connect gate="D" pin="VCCINT_6" pad="K10"/>
<connect gate="D" pin="VCCINT_7" pad="L13"/>
<connect gate="D" pin="VCCINT_8" pad="M10"/>
<connect gate="D" pin="VCCINT_9" pad="N11"/>
<connect gate="D" pin="VCCIO1" pad="M22"/>
<connect gate="D" pin="VCCIO2" pad="L22"/>
<connect gate="D" pin="VCCPD1" pad="P15"/>
<connect gate="D" pin="VCCPD2" pad="K14"/>
<connect gate="D" pin="VCCPD3" pad="H13"/>
<connect gate="D" pin="VCCPD7" pad="P10"/>
<connect gate="D" pin="VCCPD8" pad="R13"/>
<connect gate="D" pin="VCC_PLL6_OUT" pad="R11"/>
<connect gate="D" pin="VREFB2N1" pad="L19"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL6" pad="T12"/>
<connect gate="E" pin="GNDA_PLL6_2" pad="T11"/>
<connect gate="E" pin="GND_2" pad="AA21"/>
<connect gate="E" pin="GND_3" pad="AB14"/>
<connect gate="E" pin="IO" pad="AB18"/>
<connect gate="E" pin="IO_10" pad="T16"/>
<connect gate="E" pin="IO_11" pad="T17"/>
<connect gate="E" pin="IO_12" pad="T18"/>
<connect gate="E" pin="IO_13" pad="T19"/>
<connect gate="E" pin="IO_14" pad="T20"/>
<connect gate="E" pin="IO_15" pad="T21"/>
<connect gate="E" pin="IO_16" pad="T22"/>
<connect gate="E" pin="IO_17" pad="U10"/>
<connect gate="E" pin="IO_18" pad="U12"/>
<connect gate="E" pin="IO_19" pad="U13"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="U14"/>
<connect gate="E" pin="IO_21" pad="U15"/>
<connect gate="E" pin="IO_22" pad="U16"/>
<connect gate="E" pin="IO_23" pad="U17"/>
<connect gate="E" pin="IO_24" pad="U18"/>
<connect gate="E" pin="IO_25" pad="U19"/>
<connect gate="E" pin="IO_26" pad="U20"/>
<connect gate="E" pin="IO_27" pad="U21"/>
<connect gate="E" pin="IO_28" pad="U22"/>
<connect gate="E" pin="IO_29" pad="V10"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="V11"/>
<connect gate="E" pin="IO_31" pad="V12"/>
<connect gate="E" pin="IO_32" pad="V13"/>
<connect gate="E" pin="IO_33" pad="V14"/>
<connect gate="E" pin="IO_34" pad="V15"/>
<connect gate="E" pin="IO_35" pad="V16"/>
<connect gate="E" pin="IO_36" pad="V18"/>
<connect gate="E" pin="IO_37" pad="V19"/>
<connect gate="E" pin="IO_38" pad="V21"/>
<connect gate="E" pin="IO_39" pad="V22"/>
<connect gate="E" pin="IO_4" pad="R21"/>
<connect gate="E" pin="IO_40" pad="W10"/>
<connect gate="E" pin="IO_41" pad="W11"/>
<connect gate="E" pin="IO_42" pad="W12"/>
<connect gate="E" pin="IO_43" pad="W13"/>
<connect gate="E" pin="IO_44" pad="W14"/>
<connect gate="E" pin="IO_45" pad="W15"/>
<connect gate="E" pin="IO_46" pad="W16"/>
<connect gate="E" pin="IO_47" pad="W17"/>
<connect gate="E" pin="IO_48" pad="W19"/>
<connect gate="E" pin="IO_49" pad="W20"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="W21"/>
<connect gate="E" pin="IO_51" pad="W22"/>
<connect gate="E" pin="IO_52" pad="Y10"/>
<connect gate="E" pin="IO_53" pad="Y11"/>
<connect gate="E" pin="IO_54" pad="Y12"/>
<connect gate="E" pin="IO_55" pad="Y13"/>
<connect gate="E" pin="IO_56" pad="Y14"/>
<connect gate="E" pin="IO_57" pad="Y15"/>
<connect gate="E" pin="IO_58" pad="Y16"/>
<connect gate="E" pin="IO_59" pad="Y17"/>
<connect gate="E" pin="IO_6" pad="T10"/>
<connect gate="E" pin="IO_60" pad="Y18"/>
<connect gate="E" pin="IO_61" pad="Y20"/>
<connect gate="E" pin="IO_62" pad="Y21"/>
<connect gate="E" pin="IO_63" pad="Y22"/>
<connect gate="E" pin="IO_64" pad="AA10"/>
<connect gate="E" pin="IO_65" pad="AA11"/>
<connect gate="E" pin="IO_66" pad="AA12"/>
<connect gate="E" pin="IO_67" pad="AA13"/>
<connect gate="E" pin="IO_68" pad="AA15"/>
<connect gate="E" pin="IO_69" pad="AA16"/>
<connect gate="E" pin="IO_7" pad="T13"/>
<connect gate="E" pin="IO_70" pad="AA17"/>
<connect gate="E" pin="IO_71" pad="AA18"/>
<connect gate="E" pin="IO_72" pad="AB10"/>
<connect gate="E" pin="IO_73" pad="AB13"/>
<connect gate="E" pin="IO_74" pad="AB15"/>
<connect gate="E" pin="IO_75" pad="AB16"/>
<connect gate="E" pin="IO_76" pad="AB17"/>
<connect gate="E" pin="IO_8" pad="T14"/>
<connect gate="E" pin="IO_9" pad="T15"/>
<connect gate="E" pin="NCONFIG" pad="W18"/>
<connect gate="E" pin="TCK" pad="AA19"/>
<connect gate="E" pin="TDI" pad="AB21"/>
<connect gate="E" pin="TMS" pad="AA20"/>
<connect gate="E" pin="TRST" pad="AB19"/>
<connect gate="E" pin="VCCD_PLL6" pad="U11"/>
<connect gate="E" pin="VCCIO1" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="AB11"/>
<connect gate="E" pin="VCCIO8" pad="AB20"/>
<connect gate="E" pin="VCCIO8_2" pad="AB12"/>
<connect gate="E" pin="VCCSEL" pad="V17"/>
<connect gate="E" pin="VREFB1N0" pad="R20"/>
<connect gate="E" pin="VREFB1N1" pad="V20"/>
<connect gate="E" pin="VREFB8N0" pad="Y19"/>
<connect gate="E" pin="VREFB8N1" pad="AA14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S30F484C3N"/>
<attribute name="OC_FARNELL" value="1549485"/>
<attribute name="OC_NEWARK" value="52R0722"/>
<attribute name="PACKAGE" value="484-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S30F484C5N">
<description>Stratix II Devices</description>
<gates>
<gate name="A" symbol="EP2S30F484C5N_A"/>
<gate name="B" symbol="EP2S30F484C5N_B"/>
<gate name="C" symbol="EP2S30F484C5N_C"/>
<gate name="D" symbol="EP2S30F484C5N_D"/>
<gate name="E" symbol="EP2S30F484C5N_E"/>
</gates>
<devices>
<device name="" package="BGA484C22X22X100P_2300X2300X35">
<connects>
<connect gate="A" pin="GND" pad="K9"/>
<connect gate="A" pin="GNDA_PLL4" pad="L5"/>
<connect gate="A" pin="GNDA_PLL4_2" pad="L4"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="A9"/>
<connect gate="A" pin="GND_4" pad="J1"/>
<connect gate="A" pin="GND_5" pad="A1"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B9"/>
<connect gate="A" pin="IO_11" pad="C1"/>
<connect gate="A" pin="IO_12" pad="C2"/>
<connect gate="A" pin="IO_13" pad="C4"/>
<connect gate="A" pin="IO_14" pad="C5"/>
<connect gate="A" pin="IO_15" pad="C6"/>
<connect gate="A" pin="IO_16" pad="C7"/>
<connect gate="A" pin="IO_17" pad="C8"/>
<connect gate="A" pin="IO_18" pad="C9"/>
<connect gate="A" pin="IO_19" pad="D1"/>
<connect gate="A" pin="IO_2" pad="A5"/>
<connect gate="A" pin="IO_20" pad="D2"/>
<connect gate="A" pin="IO_21" pad="D3"/>
<connect gate="A" pin="IO_22" pad="D5"/>
<connect gate="A" pin="IO_23" pad="D6"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="E1"/>
<connect gate="A" pin="IO_26" pad="E2"/>
<connect gate="A" pin="IO_27" pad="E3"/>
<connect gate="A" pin="IO_28" pad="E4"/>
<connect gate="A" pin="IO_29" pad="E6"/>
<connect gate="A" pin="IO_3" pad="A6"/>
<connect gate="A" pin="IO_30" pad="E7"/>
<connect gate="A" pin="IO_31" pad="E8"/>
<connect gate="A" pin="IO_32" pad="E9"/>
<connect gate="A" pin="IO_33" pad="F1"/>
<connect gate="A" pin="IO_34" pad="F2"/>
<connect gate="A" pin="IO_35" pad="F4"/>
<connect gate="A" pin="IO_36" pad="F5"/>
<connect gate="A" pin="IO_37" pad="F6"/>
<connect gate="A" pin="IO_38" pad="F7"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A7"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="G7"/>
<connect gate="A" pin="IO_48" pad="G8"/>
<connect gate="A" pin="IO_49" pad="G9"/>
<connect gate="A" pin="IO_5" pad="A8"/>
<connect gate="A" pin="IO_50" pad="H1"/>
<connect gate="A" pin="IO_51" pad="H2"/>
<connect gate="A" pin="IO_52" pad="H3"/>
<connect gate="A" pin="IO_53" pad="H4"/>
<connect gate="A" pin="IO_54" pad="H5"/>
<connect gate="A" pin="IO_55" pad="H6"/>
<connect gate="A" pin="IO_56" pad="H7"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J2"/>
<connect gate="A" pin="IO_59" pad="J3"/>
<connect gate="A" pin="IO_6" pad="B5"/>
<connect gate="A" pin="IO_60" pad="J5"/>
<connect gate="A" pin="IO_61" pad="J6"/>
<connect gate="A" pin="IO_62" pad="J7"/>
<connect gate="A" pin="IO_63" pad="J8"/>
<connect gate="A" pin="IO_64" pad="K1"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_66" pad="K3"/>
<connect gate="A" pin="IO_67" pad="K4"/>
<connect gate="A" pin="IO_68" pad="K5"/>
<connect gate="A" pin="IO_69" pad="K6"/>
<connect gate="A" pin="IO_7" pad="B6"/>
<connect gate="A" pin="IO_70" pad="K7"/>
<connect gate="A" pin="IO_71" pad="K8"/>
<connect gate="A" pin="IO_72" pad="L2"/>
<connect gate="A" pin="IO_73" pad="L3"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="B8"/>
<connect gate="A" pin="MSEL0" pad="E5"/>
<connect gate="A" pin="MSEL1" pad="D4"/>
<connect gate="A" pin="MSEL2" pad="B4"/>
<connect gate="A" pin="MSEL3" pad="A4"/>
<connect gate="A" pin="TDO" pad="B3"/>
<connect gate="A" pin="TEMPDIODEN" pad="C3"/>
<connect gate="A" pin="TEMPDIODEP" pad="A2"/>
<connect gate="A" pin="VCCD_PLL4" pad="L6"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="H8"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="B1"/>
<connect gate="A" pin="VREFB4N0" pad="D7"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N0" pad="J4"/>
<connect gate="A" pin="VREFB5N1" pad="F3"/>
<connect gate="B" pin="CLK11N" pad="M3"/>
<connect gate="B" pin="CLK11P" pad="M2"/>
<connect gate="B" pin="CLK9N" pad="N4"/>
<connect gate="B" pin="CLK9P" pad="N3"/>
<connect gate="B" pin="GND" pad="M7"/>
<connect gate="B" pin="GNDA_PLL3" pad="N6"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="N5"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="M9"/>
<connect gate="B" pin="GND_4" pad="A14"/>
<connect gate="B" pin="GND_5" pad="A22"/>
<connect gate="B" pin="IO" pad="A19"/>
<connect gate="B" pin="IO_10" pad="P6"/>
<connect gate="B" pin="IO_11" pad="P7"/>
<connect gate="B" pin="IO_12" pad="P8"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="R2"/>
<connect gate="B" pin="IO_15" pad="R3"/>
<connect gate="B" pin="IO_16" pad="R4"/>
<connect gate="B" pin="IO_17" pad="R5"/>
<connect gate="B" pin="IO_18" pad="R6"/>
<connect gate="B" pin="IO_19" pad="R7"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R8"/>
<connect gate="B" pin="IO_21" pad="R9"/>
<connect gate="B" pin="IO_22" pad="T1"/>
<connect gate="B" pin="IO_23" pad="T2"/>
<connect gate="B" pin="IO_24" pad="T3"/>
<connect gate="B" pin="IO_25" pad="T4"/>
<connect gate="B" pin="IO_26" pad="T5"/>
<connect gate="B" pin="IO_27" pad="T6"/>
<connect gate="B" pin="IO_28" pad="T7"/>
<connect gate="B" pin="IO_29" pad="T8"/>
<connect gate="B" pin="IO_3" pad="N1"/>
<connect gate="B" pin="IO_30" pad="T9"/>
<connect gate="B" pin="IO_31" pad="U1"/>
<connect gate="B" pin="IO_32" pad="U2"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="U9"/>
<connect gate="B" pin="IO_39" pad="V1"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="V2"/>
<connect gate="B" pin="IO_41" pad="V3"/>
<connect gate="B" pin="IO_42" pad="V4"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="V9"/>
<connect gate="B" pin="IO_47" pad="W1"/>
<connect gate="B" pin="IO_48" pad="W2"/>
<connect gate="B" pin="IO_49" pad="W3"/>
<connect gate="B" pin="IO_5" pad="N7"/>
<connect gate="B" pin="IO_50" pad="W4"/>
<connect gate="B" pin="IO_51" pad="W5"/>
<connect gate="B" pin="IO_52" pad="W7"/>
<connect gate="B" pin="IO_53" pad="W9"/>
<connect gate="B" pin="IO_54" pad="Y1"/>
<connect gate="B" pin="IO_55" pad="Y2"/>
<connect gate="B" pin="IO_56" pad="Y3"/>
<connect gate="B" pin="IO_57" pad="Y5"/>
<connect gate="B" pin="IO_58" pad="Y6"/>
<connect gate="B" pin="IO_59" pad="Y7"/>
<connect gate="B" pin="IO_6" pad="N8"/>
<connect gate="B" pin="IO_60" pad="Y8"/>
<connect gate="B" pin="IO_61" pad="Y9"/>
<connect gate="B" pin="IO_62" pad="A10"/>
<connect gate="B" pin="IO_63" pad="A13"/>
<connect gate="B" pin="IO_64" pad="A15"/>
<connect gate="B" pin="IO_65" pad="A16"/>
<connect gate="B" pin="IO_66" pad="A17"/>
<connect gate="B" pin="IO_67" pad="A18"/>
<connect gate="B" pin="IO_7" pad="P2"/>
<connect gate="B" pin="IO_8" pad="P3"/>
<connect gate="B" pin="IO_9" pad="P5"/>
<connect gate="B" pin="NCE" pad="A21"/>
<connect gate="B" pin="PLL_ENA" pad="Y4"/>
<connect gate="B" pin="PORSEL" pad="V5"/>
<connect gate="B" pin="VCCA_PLL3" pad="M4"/>
<connect gate="B" pin="VCCA_PLL4" pad="M6"/>
<connect gate="B" pin="VCCD_PLL3" pad="M5"/>
<connect gate="B" pin="VCCINT" pad="P9"/>
<connect gate="B" pin="VCCINT_2" pad="M8"/>
<connect gate="B" pin="VCCIO3" pad="A20"/>
<connect gate="B" pin="VCCIO3_2" pad="A12"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="AA1"/>
<connect gate="B" pin="VCCIO6_2" pad="M1"/>
<connect gate="B" pin="VCCPD5" pad="L9"/>
<connect gate="B" pin="VCCPD6" pad="N9"/>
<connect gate="B" pin="VREFB6N0" pad="U3"/>
<connect gate="B" pin="VREFB6N1" pad="P4"/>
<connect gate="B" pin="VREFB7N0" pad="W8"/>
<connect gate="B" pin="VREFB7N1" pad="W6"/>
<connect gate="C" pin="CONF_DONE" pad="C20"/>
<connect gate="C" pin="DCLK" pad="D19"/>
<connect gate="C" pin="GND" pad="B21"/>
<connect gate="C" pin="GNDA_PLL5" pad="F11"/>
<connect gate="C" pin="GNDA_PLL5_2" pad="F10"/>
<connect gate="C" pin="GND_2" pad="AA2"/>
<connect gate="C" pin="GND_3" pad="AB1"/>
<connect gate="C" pin="GND_4" pad="AB4"/>
<connect gate="C" pin="GND_5" pad="AB9"/>
<connect gate="C" pin="IO" pad="H11"/>
<connect gate="C" pin="IO_10" pad="AB7"/>
<connect gate="C" pin="IO_11" pad="AB8"/>
<connect gate="C" pin="IO_12" pad="B10"/>
<connect gate="C" pin="IO_13" pad="B11"/>
<connect gate="C" pin="IO_14" pad="B12"/>
<connect gate="C" pin="IO_15" pad="B13"/>
<connect gate="C" pin="IO_16" pad="B15"/>
<connect gate="C" pin="IO_17" pad="B16"/>
<connect gate="C" pin="IO_18" pad="B17"/>
<connect gate="C" pin="IO_19" pad="B18"/>
<connect gate="C" pin="IO_2" pad="AA4"/>
<connect gate="C" pin="IO_20" pad="B19"/>
<connect gate="C" pin="IO_21" pad="C10"/>
<connect gate="C" pin="IO_22" pad="C11"/>
<connect gate="C" pin="IO_23" pad="C12"/>
<connect gate="C" pin="IO_24" pad="C13"/>
<connect gate="C" pin="IO_25" pad="C14"/>
<connect gate="C" pin="IO_26" pad="C15"/>
<connect gate="C" pin="IO_27" pad="C16"/>
<connect gate="C" pin="IO_28" pad="C17"/>
<connect gate="C" pin="IO_29" pad="C18"/>
<connect gate="C" pin="IO_3" pad="AA5"/>
<connect gate="C" pin="IO_30" pad="C19"/>
<connect gate="C" pin="IO_31" pad="C21"/>
<connect gate="C" pin="IO_32" pad="C22"/>
<connect gate="C" pin="IO_33" pad="D10"/>
<connect gate="C" pin="IO_34" pad="D11"/>
<connect gate="C" pin="IO_35" pad="D12"/>
<connect gate="C" pin="IO_36" pad="D13"/>
<connect gate="C" pin="IO_37" pad="D14"/>
<connect gate="C" pin="IO_38" pad="D15"/>
<connect gate="C" pin="IO_39" pad="D17"/>
<connect gate="C" pin="IO_4" pad="AA6"/>
<connect gate="C" pin="IO_40" pad="D18"/>
<connect gate="C" pin="IO_41" pad="D20"/>
<connect gate="C" pin="IO_42" pad="D21"/>
<connect gate="C" pin="IO_43" pad="D22"/>
<connect gate="C" pin="IO_44" pad="E10"/>
<connect gate="C" pin="IO_45" pad="E11"/>
<connect gate="C" pin="IO_46" pad="E12"/>
<connect gate="C" pin="IO_47" pad="E13"/>
<connect gate="C" pin="IO_48" pad="E14"/>
<connect gate="C" pin="IO_49" pad="E15"/>
<connect gate="C" pin="IO_5" pad="AA7"/>
<connect gate="C" pin="IO_50" pad="E16"/>
<connect gate="C" pin="IO_51" pad="E17"/>
<connect gate="C" pin="IO_52" pad="E18"/>
<connect gate="C" pin="IO_53" pad="E19"/>
<connect gate="C" pin="IO_54" pad="E20"/>
<connect gate="C" pin="IO_55" pad="E21"/>
<connect gate="C" pin="IO_56" pad="E22"/>
<connect gate="C" pin="IO_57" pad="F13"/>
<connect gate="C" pin="IO_58" pad="F14"/>
<connect gate="C" pin="IO_59" pad="F15"/>
<connect gate="C" pin="IO_6" pad="AA8"/>
<connect gate="C" pin="IO_60" pad="F16"/>
<connect gate="C" pin="IO_61" pad="F17"/>
<connect gate="C" pin="IO_62" pad="F19"/>
<connect gate="C" pin="IO_63" pad="F20"/>
<connect gate="C" pin="IO_64" pad="F21"/>
<connect gate="C" pin="IO_65" pad="F22"/>
<connect gate="C" pin="IO_66" pad="G12"/>
<connect gate="C" pin="IO_67" pad="G13"/>
<connect gate="C" pin="IO_68" pad="G14"/>
<connect gate="C" pin="IO_69" pad="G15"/>
<connect gate="C" pin="IO_7" pad="AA9"/>
<connect gate="C" pin="IO_70" pad="G16"/>
<connect gate="C" pin="IO_71" pad="G17"/>
<connect gate="C" pin="IO_72" pad="G18"/>
<connect gate="C" pin="IO_73" pad="G19"/>
<connect gate="C" pin="IO_74" pad="G20"/>
<connect gate="C" pin="IO_75" pad="G21"/>
<connect gate="C" pin="IO_76" pad="G22"/>
<connect gate="C" pin="IO_8" pad="AB5"/>
<connect gate="C" pin="IO_9" pad="AB6"/>
<connect gate="C" pin="NCEO" pad="AA3"/>
<connect gate="C" pin="NIO_PULLUP" pad="AB2"/>
<connect gate="C" pin="NSTATUS" pad="B20"/>
<connect gate="C" pin="VCCA_PLL5" pad="F12"/>
<connect gate="C" pin="VCCD_PLL5" pad="G11"/>
<connect gate="C" pin="VCCIO2" pad="B22"/>
<connect gate="C" pin="VCCIO7" pad="AB3"/>
<connect gate="C" pin="VCCPD4" pad="H10"/>
<connect gate="C" pin="VCC_PLL5_OUT" pad="G10"/>
<connect gate="C" pin="VREFB2N0" pad="F18"/>
<connect gate="C" pin="VREFB3N0" pad="B14"/>
<connect gate="C" pin="VREFB3N1" pad="D16"/>
<connect gate="D" pin="CLK1N" pad="M20"/>
<connect gate="D" pin="CLK1P" pad="M21"/>
<connect gate="D" pin="CLK3N" pad="N19"/>
<connect gate="D" pin="CLK3P" pad="N20"/>
<connect gate="D" pin="GND" pad="R10"/>
<connect gate="D" pin="GNDA_PLL1" pad="L18"/>
<connect gate="D" pin="GNDA_PLL1_2" pad="L17"/>
<connect gate="D" pin="GNDA_PLL2" pad="N18"/>
<connect gate="D" pin="GNDA_PLL2_2" pad="N17"/>
<connect gate="D" pin="GND_10" pad="M11"/>
<connect gate="D" pin="GND_11" pad="L14"/>
<connect gate="D" pin="GND_12" pad="N12"/>
<connect gate="D" pin="GND_13" pad="L10"/>
<connect gate="D" pin="GND_14" pad="P13"/>
<connect gate="D" pin="GND_15" pad="L12"/>
<connect gate="D" pin="GND_16" pad="N14"/>
<connect gate="D" pin="GND_17" pad="N10"/>
<connect gate="D" pin="GND_18" pad="P22"/>
<connect gate="D" pin="GND_19" pad="J10"/>
<connect gate="D" pin="GND_2" pad="K11"/>
<connect gate="D" pin="GND_20" pad="P11"/>
<connect gate="D" pin="GND_3" pad="H15"/>
<connect gate="D" pin="GND_4" pad="J12"/>
<connect gate="D" pin="GND_5" pad="K13"/>
<connect gate="D" pin="GND_6" pad="M13"/>
<connect gate="D" pin="GND_7" pad="J14"/>
<connect gate="D" pin="GND_8" pad="M15"/>
<connect gate="D" pin="GND_9" pad="J22"/>
<connect gate="D" pin="IO" pad="R17"/>
<connect gate="D" pin="IO_10" pad="H22"/>
<connect gate="D" pin="IO_11" pad="J15"/>
<connect gate="D" pin="IO_12" pad="J16"/>
<connect gate="D" pin="IO_13" pad="J17"/>
<connect gate="D" pin="IO_14" pad="J18"/>
<connect gate="D" pin="IO_15" pad="J19"/>
<connect gate="D" pin="IO_16" pad="J20"/>
<connect gate="D" pin="IO_17" pad="J21"/>
<connect gate="D" pin="IO_18" pad="K15"/>
<connect gate="D" pin="IO_19" pad="K16"/>
<connect gate="D" pin="IO_2" pad="H12"/>
<connect gate="D" pin="IO_20" pad="K17"/>
<connect gate="D" pin="IO_21" pad="K18"/>
<connect gate="D" pin="IO_22" pad="K19"/>
<connect gate="D" pin="IO_23" pad="K20"/>
<connect gate="D" pin="IO_24" pad="K21"/>
<connect gate="D" pin="IO_25" pad="K22"/>
<connect gate="D" pin="IO_26" pad="L15"/>
<connect gate="D" pin="IO_27" pad="L16"/>
<connect gate="D" pin="IO_28" pad="L20"/>
<connect gate="D" pin="IO_29" pad="L21"/>
<connect gate="D" pin="IO_3" pad="H14"/>
<connect gate="D" pin="IO_30" pad="N15"/>
<connect gate="D" pin="IO_31" pad="N16"/>
<connect gate="D" pin="IO_32" pad="N21"/>
<connect gate="D" pin="IO_33" pad="N22"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="P19"/>
<connect gate="D" pin="IO_38" pad="P20"/>
<connect gate="D" pin="IO_39" pad="P21"/>
<connect gate="D" pin="IO_4" pad="H16"/>
<connect gate="D" pin="IO_40" pad="R14"/>
<connect gate="D" pin="IO_41" pad="R15"/>
<connect gate="D" pin="IO_42" pad="R16"/>
<connect gate="D" pin="IO_5" pad="H17"/>
<connect gate="D" pin="IO_6" pad="H18"/>
<connect gate="D" pin="IO_7" pad="H19"/>
<connect gate="D" pin="IO_8" pad="H20"/>
<connect gate="D" pin="IO_9" pad="H21"/>
<connect gate="D" pin="VCCA_PLL1" pad="M17"/>
<connect gate="D" pin="VCCA_PLL2" pad="M19"/>
<connect gate="D" pin="VCCA_PLL6" pad="R12"/>
<connect gate="D" pin="VCCD_PLL1" pad="M16"/>
<connect gate="D" pin="VCCD_PLL2" pad="M18"/>
<connect gate="D" pin="VCCINT" pad="P14"/>
<connect gate="D" pin="VCCINT_10" pad="M12"/>
<connect gate="D" pin="VCCINT_11" pad="N13"/>
<connect gate="D" pin="VCCINT_12" pad="M14"/>
<connect gate="D" pin="VCCINT_13" pad="P12"/>
<connect gate="D" pin="VCCINT_2" pad="L11"/>
<connect gate="D" pin="VCCINT_3" pad="K12"/>
<connect gate="D" pin="VCCINT_4" pad="J11"/>
<connect gate="D" pin="VCCINT_5" pad="J13"/>
<connect gate="D" pin="VCCINT_6" pad="K10"/>
<connect gate="D" pin="VCCINT_7" pad="L13"/>
<connect gate="D" pin="VCCINT_8" pad="M10"/>
<connect gate="D" pin="VCCINT_9" pad="N11"/>
<connect gate="D" pin="VCCIO1" pad="M22"/>
<connect gate="D" pin="VCCIO2" pad="L22"/>
<connect gate="D" pin="VCCPD1" pad="P15"/>
<connect gate="D" pin="VCCPD2" pad="K14"/>
<connect gate="D" pin="VCCPD3" pad="H13"/>
<connect gate="D" pin="VCCPD7" pad="P10"/>
<connect gate="D" pin="VCCPD8" pad="R13"/>
<connect gate="D" pin="VCC_PLL6_OUT" pad="R11"/>
<connect gate="D" pin="VREFB2N1" pad="L19"/>
<connect gate="E" pin="GND" pad="AB22"/>
<connect gate="E" pin="GNDA_PLL6" pad="T12"/>
<connect gate="E" pin="GNDA_PLL6_2" pad="T11"/>
<connect gate="E" pin="GND_2" pad="AA21"/>
<connect gate="E" pin="GND_3" pad="AB14"/>
<connect gate="E" pin="IO" pad="AB18"/>
<connect gate="E" pin="IO_10" pad="T16"/>
<connect gate="E" pin="IO_11" pad="T17"/>
<connect gate="E" pin="IO_12" pad="T18"/>
<connect gate="E" pin="IO_13" pad="T19"/>
<connect gate="E" pin="IO_14" pad="T20"/>
<connect gate="E" pin="IO_15" pad="T21"/>
<connect gate="E" pin="IO_16" pad="T22"/>
<connect gate="E" pin="IO_17" pad="U10"/>
<connect gate="E" pin="IO_18" pad="U12"/>
<connect gate="E" pin="IO_19" pad="U13"/>
<connect gate="E" pin="IO_2" pad="R18"/>
<connect gate="E" pin="IO_20" pad="U14"/>
<connect gate="E" pin="IO_21" pad="U15"/>
<connect gate="E" pin="IO_22" pad="U16"/>
<connect gate="E" pin="IO_23" pad="U17"/>
<connect gate="E" pin="IO_24" pad="U18"/>
<connect gate="E" pin="IO_25" pad="U19"/>
<connect gate="E" pin="IO_26" pad="U20"/>
<connect gate="E" pin="IO_27" pad="U21"/>
<connect gate="E" pin="IO_28" pad="U22"/>
<connect gate="E" pin="IO_29" pad="V10"/>
<connect gate="E" pin="IO_3" pad="R19"/>
<connect gate="E" pin="IO_30" pad="V11"/>
<connect gate="E" pin="IO_31" pad="V12"/>
<connect gate="E" pin="IO_32" pad="V13"/>
<connect gate="E" pin="IO_33" pad="V14"/>
<connect gate="E" pin="IO_34" pad="V15"/>
<connect gate="E" pin="IO_35" pad="V16"/>
<connect gate="E" pin="IO_36" pad="V18"/>
<connect gate="E" pin="IO_37" pad="V19"/>
<connect gate="E" pin="IO_38" pad="V21"/>
<connect gate="E" pin="IO_39" pad="V22"/>
<connect gate="E" pin="IO_4" pad="R21"/>
<connect gate="E" pin="IO_40" pad="W10"/>
<connect gate="E" pin="IO_41" pad="W11"/>
<connect gate="E" pin="IO_42" pad="W12"/>
<connect gate="E" pin="IO_43" pad="W13"/>
<connect gate="E" pin="IO_44" pad="W14"/>
<connect gate="E" pin="IO_45" pad="W15"/>
<connect gate="E" pin="IO_46" pad="W16"/>
<connect gate="E" pin="IO_47" pad="W17"/>
<connect gate="E" pin="IO_48" pad="W19"/>
<connect gate="E" pin="IO_49" pad="W20"/>
<connect gate="E" pin="IO_5" pad="R22"/>
<connect gate="E" pin="IO_50" pad="W21"/>
<connect gate="E" pin="IO_51" pad="W22"/>
<connect gate="E" pin="IO_52" pad="Y10"/>
<connect gate="E" pin="IO_53" pad="Y11"/>
<connect gate="E" pin="IO_54" pad="Y12"/>
<connect gate="E" pin="IO_55" pad="Y13"/>
<connect gate="E" pin="IO_56" pad="Y14"/>
<connect gate="E" pin="IO_57" pad="Y15"/>
<connect gate="E" pin="IO_58" pad="Y16"/>
<connect gate="E" pin="IO_59" pad="Y17"/>
<connect gate="E" pin="IO_6" pad="T10"/>
<connect gate="E" pin="IO_60" pad="Y18"/>
<connect gate="E" pin="IO_61" pad="Y20"/>
<connect gate="E" pin="IO_62" pad="Y21"/>
<connect gate="E" pin="IO_63" pad="Y22"/>
<connect gate="E" pin="IO_64" pad="AA10"/>
<connect gate="E" pin="IO_65" pad="AA11"/>
<connect gate="E" pin="IO_66" pad="AA12"/>
<connect gate="E" pin="IO_67" pad="AA13"/>
<connect gate="E" pin="IO_68" pad="AA15"/>
<connect gate="E" pin="IO_69" pad="AA16"/>
<connect gate="E" pin="IO_7" pad="T13"/>
<connect gate="E" pin="IO_70" pad="AA17"/>
<connect gate="E" pin="IO_71" pad="AA18"/>
<connect gate="E" pin="IO_72" pad="AB10"/>
<connect gate="E" pin="IO_73" pad="AB13"/>
<connect gate="E" pin="IO_74" pad="AB15"/>
<connect gate="E" pin="IO_75" pad="AB16"/>
<connect gate="E" pin="IO_76" pad="AB17"/>
<connect gate="E" pin="IO_8" pad="T14"/>
<connect gate="E" pin="IO_9" pad="T15"/>
<connect gate="E" pin="NCONFIG" pad="W18"/>
<connect gate="E" pin="TCK" pad="AA19"/>
<connect gate="E" pin="TDI" pad="AB21"/>
<connect gate="E" pin="TMS" pad="AA20"/>
<connect gate="E" pin="TRST" pad="AB19"/>
<connect gate="E" pin="VCCD_PLL6" pad="U11"/>
<connect gate="E" pin="VCCIO1" pad="AA22"/>
<connect gate="E" pin="VCCIO7" pad="AB11"/>
<connect gate="E" pin="VCCIO8" pad="AB20"/>
<connect gate="E" pin="VCCIO8_2" pad="AB12"/>
<connect gate="E" pin="VCCSEL" pad="V17"/>
<connect gate="E" pin="VREFB1N0" pad="R20"/>
<connect gate="E" pin="VREFB1N1" pad="V20"/>
<connect gate="E" pin="VREFB8N0" pad="Y19"/>
<connect gate="E" pin="VREFB8N1" pad="AA14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S30F484C5N"/>
<attribute name="OC_FARNELL" value="1637236"/>
<attribute name="OC_NEWARK" value="51R0585"/>
<attribute name="PACKAGE" value="484-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S30F672C3N">
<description>Stratix II Devices</description>
<gates>
<gate name="A" symbol="EP2S30F672C3N_A"/>
<gate name="B" symbol="EP2S30F672C3N_B"/>
<gate name="C" symbol="EP2S30F672C3N_C"/>
<gate name="D" symbol="EP2S30F672C3N_D"/>
<gate name="E" symbol="EP2S30F672C3N_E"/>
<gate name="F" symbol="EP2S30F672C3N_F"/>
<gate name="G" symbol="EP2S30F672C3N_G"/>
</gates>
<devices>
<device name="" package="BGA672C26X26X100P_2700X2700X35">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="D7"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D9"/>
<connect gate="A" pin="IO_26" pad="E7"/>
<connect gate="A" pin="IO_27" pad="E8"/>
<connect gate="A" pin="IO_28" pad="E9"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G3"/>
<connect gate="A" pin="IO_32" pad="G4"/>
<connect gate="A" pin="IO_33" pad="H1"/>
<connect gate="A" pin="IO_34" pad="H2"/>
<connect gate="A" pin="IO_35" pad="H3"/>
<connect gate="A" pin="IO_36" pad="H4"/>
<connect gate="A" pin="IO_37" pad="J1"/>
<connect gate="A" pin="IO_38" pad="J2"/>
<connect gate="A" pin="IO_39" pad="J3"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="J4"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_43" pad="K3"/>
<connect gate="A" pin="IO_44" pad="K4"/>
<connect gate="A" pin="IO_45" pad="K8"/>
<connect gate="A" pin="IO_46" pad="K9"/>
<connect gate="A" pin="IO_47" pad="L2"/>
<connect gate="A" pin="IO_48" pad="L3"/>
<connect gate="A" pin="IO_49" pad="L4"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="L5"/>
<connect gate="A" pin="IO_51" pad="L6"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="G8"/>
<connect gate="A" pin="MSEL1" pad="B2"/>
<connect gate="A" pin="MSEL2" pad="E6"/>
<connect gate="A" pin="MSEL3" pad="F7"/>
<connect gate="A" pin="NC" pad="K7"/>
<connect gate="A" pin="NC_10" pad="H8"/>
<connect gate="A" pin="NC_11" pad="D4"/>
<connect gate="A" pin="NC_12" pad="F8"/>
<connect gate="A" pin="NC_13" pad="F1"/>
<connect gate="A" pin="NC_14" pad="F9"/>
<connect gate="A" pin="NC_15" pad="E1"/>
<connect gate="A" pin="NC_16" pad="F2"/>
<connect gate="A" pin="NC_17" pad="F3"/>
<connect gate="A" pin="NC_18" pad="H9"/>
<connect gate="A" pin="NC_19" pad="C1"/>
<connect gate="A" pin="NC_2" pad="G9"/>
<connect gate="A" pin="NC_20" pad="F4"/>
<connect gate="A" pin="NC_21" pad="E2"/>
<connect gate="A" pin="NC_22" pad="E3"/>
<connect gate="A" pin="NC_23" pad="J5"/>
<connect gate="A" pin="NC_24" pad="C2"/>
<connect gate="A" pin="NC_25" pad="E4"/>
<connect gate="A" pin="NC_26" pad="J6"/>
<connect gate="A" pin="NC_27" pad="J7"/>
<connect gate="A" pin="NC_28" pad="J8"/>
<connect gate="A" pin="NC_29" pad="J9"/>
<connect gate="A" pin="NC_3" pad="H5"/>
<connect gate="A" pin="NC_30" pad="K6"/>
<connect gate="A" pin="NC_4" pad="H6"/>
<connect gate="A" pin="NC_5" pad="D2"/>
<connect gate="A" pin="NC_6" pad="H7"/>
<connect gate="A" pin="NC_7" pad="D3"/>
<connect gate="A" pin="NC_8" pad="G6"/>
<connect gate="A" pin="NC_9" pad="G7"/>
<connect gate="A" pin="TDO" pad="F6"/>
<connect gate="A" pin="TEMPDIODEN" pad="F5"/>
<connect gate="A" pin="TEMPDIODEP" pad="E5"/>
<connect gate="A" pin="VCCIO4" pad="A4"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="D1"/>
<connect gate="A" pin="VREFB4N0" pad="D5"/>
<connect gate="A" pin="VREFB5N0" pad="K5"/>
<connect gate="A" pin="VREFB5N1" pad="G5"/>
<connect gate="B" pin="CLK11N" pad="N3"/>
<connect gate="B" pin="CLK11P" pad="N2"/>
<connect gate="B" pin="CLK9N" pad="R4"/>
<connect gate="B" pin="CLK9P" pad="R3"/>
<connect gate="B" pin="GND" pad="A14"/>
<connect gate="B" pin="GNDA_PLL3" pad="R8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="R7"/>
<connect gate="B" pin="GNDA_PLL4" pad="N9"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="N8"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="A13"/>
<connect gate="B" pin="GND_4" pad="N1"/>
<connect gate="B" pin="GND_5" pad="P6"/>
<connect gate="B" pin="GND_6" pad="U9"/>
<connect gate="B" pin="IO" pad="A22"/>
<connect gate="B" pin="IO_10" pad="M7"/>
<connect gate="B" pin="IO_11" pad="M8"/>
<connect gate="B" pin="IO_12" pad="N4"/>
<connect gate="B" pin="IO_13" pad="N5"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="P2"/>
<connect gate="B" pin="IO_17" pad="P3"/>
<connect gate="B" pin="IO_18" pad="P4"/>
<connect gate="B" pin="IO_19" pad="P5"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R1"/>
<connect gate="B" pin="IO_21" pad="R2"/>
<connect gate="B" pin="IO_22" pad="T2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="T4"/>
<connect gate="B" pin="IO_25" pad="T5"/>
<connect gate="B" pin="IO_26" pad="T6"/>
<connect gate="B" pin="IO_27" pad="T7"/>
<connect gate="B" pin="IO_28" pad="T8"/>
<connect gate="B" pin="IO_29" pad="T9"/>
<connect gate="B" pin="IO_3" pad="L9"/>
<connect gate="B" pin="IO_30" pad="U1"/>
<connect gate="B" pin="IO_31" pad="U2"/>
<connect gate="B" pin="IO_32" pad="U3"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="V1"/>
<connect gate="B" pin="IO_39" pad="V2"/>
<connect gate="B" pin="IO_4" pad="M1"/>
<connect gate="B" pin="IO_40" pad="V3"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V5"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="W1"/>
<connect gate="B" pin="IO_47" pad="W2"/>
<connect gate="B" pin="IO_48" pad="W3"/>
<connect gate="B" pin="IO_49" pad="W4"/>
<connect gate="B" pin="IO_5" pad="M2"/>
<connect gate="B" pin="IO_50" pad="Y1"/>
<connect gate="B" pin="IO_51" pad="Y2"/>
<connect gate="B" pin="IO_52" pad="Y3"/>
<connect gate="B" pin="IO_53" pad="Y4"/>
<connect gate="B" pin="IO_54" pad="A10"/>
<connect gate="B" pin="IO_55" pad="A12"/>
<connect gate="B" pin="IO_56" pad="A15"/>
<connect gate="B" pin="IO_57" pad="A17"/>
<connect gate="B" pin="IO_58" pad="A18"/>
<connect gate="B" pin="IO_59" pad="A19"/>
<connect gate="B" pin="IO_6" pad="M3"/>
<connect gate="B" pin="IO_60" pad="A20"/>
<connect gate="B" pin="IO_61" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M4"/>
<connect gate="B" pin="IO_8" pad="M5"/>
<connect gate="B" pin="IO_9" pad="M6"/>
<connect gate="B" pin="NC" pad="W9"/>
<connect gate="B" pin="NC_2" pad="Y6"/>
<connect gate="B" pin="NC_3" pad="W5"/>
<connect gate="B" pin="NC_4" pad="Y9"/>
<connect gate="B" pin="NC_5" pad="W6"/>
<connect gate="B" pin="NC_6" pad="Y7"/>
<connect gate="B" pin="NC_7" pad="W7"/>
<connect gate="B" pin="NC_8" pad="W8"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA_PLL3" pad="R6"/>
<connect gate="B" pin="VCCA_PLL4" pad="P8"/>
<connect gate="B" pin="VCCD_PLL3" pad="P7"/>
<connect gate="B" pin="VCCD_PLL4" pad="P9"/>
<connect gate="B" pin="VCCINT" pad="V9"/>
<connect gate="B" pin="VCCIO3" pad="A16"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="T1"/>
<connect gate="B" pin="VCCPD5" pad="M9"/>
<connect gate="B" pin="VCCPD6" pad="R9"/>
<connect gate="B" pin="VREFB6N0" pad="Y5"/>
<connect gate="B" pin="VREFB6N1" pad="R5"/>
<connect gate="C" pin="CONF_DONE" pad="B25"/>
<connect gate="C" pin="DCLK" pad="C24"/>
<connect gate="C" pin="GND" pad="B26"/>
<connect gate="C" pin="GND_2" pad="AE1"/>
<connect gate="C" pin="GND_3" pad="A25"/>
<connect gate="C" pin="GND_4" pad="AF2"/>
<connect gate="C" pin="GND_5" pad="AA7"/>
<connect gate="C" pin="IO" pad="D15"/>
<connect gate="C" pin="IO_10" pad="AC8"/>
<connect gate="C" pin="IO_11" pad="AC9"/>
<connect gate="C" pin="IO_12" pad="AD3"/>
<connect gate="C" pin="IO_13" pad="AD4"/>
<connect gate="C" pin="IO_14" pad="AD5"/>
<connect gate="C" pin="IO_15" pad="AD6"/>
<connect gate="C" pin="IO_16" pad="AD7"/>
<connect gate="C" pin="IO_17" pad="AD8"/>
<connect gate="C" pin="IO_18" pad="AD9"/>
<connect gate="C" pin="IO_19" pad="AE3"/>
<connect gate="C" pin="IO_2" pad="A24"/>
<connect gate="C" pin="IO_20" pad="AE4"/>
<connect gate="C" pin="IO_21" pad="AE5"/>
<connect gate="C" pin="IO_22" pad="AE6"/>
<connect gate="C" pin="IO_23" pad="AE7"/>
<connect gate="C" pin="IO_24" pad="AE8"/>
<connect gate="C" pin="IO_25" pad="AE9"/>
<connect gate="C" pin="IO_26" pad="AF3"/>
<connect gate="C" pin="IO_27" pad="AF5"/>
<connect gate="C" pin="IO_28" pad="AF6"/>
<connect gate="C" pin="IO_29" pad="AF7"/>
<connect gate="C" pin="IO_3" pad="AA1"/>
<connect gate="C" pin="IO_30" pad="AF8"/>
<connect gate="C" pin="IO_31" pad="AF9"/>
<connect gate="C" pin="IO_32" pad="B10"/>
<connect gate="C" pin="IO_33" pad="B11"/>
<connect gate="C" pin="IO_34" pad="B12"/>
<connect gate="C" pin="IO_35" pad="B13"/>
<connect gate="C" pin="IO_36" pad="B14"/>
<connect gate="C" pin="IO_37" pad="B15"/>
<connect gate="C" pin="IO_38" pad="B16"/>
<connect gate="C" pin="IO_39" pad="B17"/>
<connect gate="C" pin="IO_4" pad="AA2"/>
<connect gate="C" pin="IO_40" pad="B18"/>
<connect gate="C" pin="IO_41" pad="B19"/>
<connect gate="C" pin="IO_42" pad="B20"/>
<connect gate="C" pin="IO_43" pad="B21"/>
<connect gate="C" pin="IO_44" pad="B22"/>
<connect gate="C" pin="IO_45" pad="B23"/>
<connect gate="C" pin="IO_46" pad="B24"/>
<connect gate="C" pin="IO_47" pad="C10"/>
<connect gate="C" pin="IO_48" pad="C11"/>
<connect gate="C" pin="IO_49" pad="C12"/>
<connect gate="C" pin="IO_5" pad="AB1"/>
<connect gate="C" pin="IO_50" pad="C13"/>
<connect gate="C" pin="IO_51" pad="C14"/>
<connect gate="C" pin="IO_52" pad="C15"/>
<connect gate="C" pin="IO_53" pad="C16"/>
<connect gate="C" pin="IO_54" pad="C17"/>
<connect gate="C" pin="IO_55" pad="C18"/>
<connect gate="C" pin="IO_56" pad="C19"/>
<connect gate="C" pin="IO_57" pad="C20"/>
<connect gate="C" pin="IO_58" pad="C21"/>
<connect gate="C" pin="IO_59" pad="C22"/>
<connect gate="C" pin="IO_6" pad="AB2"/>
<connect gate="C" pin="IO_60" pad="C23"/>
<connect gate="C" pin="IO_61" pad="D10"/>
<connect gate="C" pin="IO_62" pad="D12"/>
<connect gate="C" pin="IO_63" pad="D13"/>
<connect gate="C" pin="IO_7" pad="AB9"/>
<connect gate="C" pin="IO_8" pad="AC6"/>
<connect gate="C" pin="IO_9" pad="AC7"/>
<connect gate="C" pin="NC" pad="AC4"/>
<connect gate="C" pin="NCEO" pad="AB5"/>
<connect gate="C" pin="NC_10" pad="AB7"/>
<connect gate="C" pin="NC_11" pad="AB8"/>
<connect gate="C" pin="NC_12" pad="D14"/>
<connect gate="C" pin="NC_13" pad="C25"/>
<connect gate="C" pin="NC_14" pad="AD1"/>
<connect gate="C" pin="NC_15" pad="AC2"/>
<connect gate="C" pin="NC_16" pad="C26"/>
<connect gate="C" pin="NC_17" pad="AC3"/>
<connect gate="C" pin="NC_18" pad="AD2"/>
<connect gate="C" pin="NC_2" pad="AA3"/>
<connect gate="C" pin="NC_3" pad="AA8"/>
<connect gate="C" pin="NC_4" pad="AA4"/>
<connect gate="C" pin="NC_5" pad="AA9"/>
<connect gate="C" pin="NC_6" pad="AA5"/>
<connect gate="C" pin="NC_7" pad="AB3"/>
<connect gate="C" pin="NC_8" pad="AA6"/>
<connect gate="C" pin="NC_9" pad="AB4"/>
<connect gate="C" pin="NIO_PULLUP" pad="AE2"/>
<connect gate="C" pin="PLL_ENA" pad="AB6"/>
<connect gate="C" pin="VCCIO3" pad="A23"/>
<connect gate="C" pin="VCCIO6" pad="AC1"/>
<connect gate="C" pin="VCCIO7" pad="AF4"/>
<connect gate="C" pin="VREFB4N1" pad="D11"/>
<connect gate="C" pin="VREFB7N1" pad="AC5"/>
<connect gate="D" pin="GND" pad="G13"/>
<connect gate="D" pin="GNDA_PLL5" pad="H13"/>
<connect gate="D" pin="GNDA_PLL5_2" pad="J13"/>
<connect gate="D" pin="IO" pad="J26"/>
<connect gate="D" pin="IO_10" pad="E13"/>
<connect gate="D" pin="IO_11" pad="E14"/>
<connect gate="D" pin="IO_12" pad="E15"/>
<connect gate="D" pin="IO_13" pad="E16"/>
<connect gate="D" pin="IO_14" pad="E17"/>
<connect gate="D" pin="IO_15" pad="E18"/>
<connect gate="D" pin="IO_16" pad="E19"/>
<connect gate="D" pin="IO_17" pad="E20"/>
<connect gate="D" pin="IO_18" pad="F10"/>
<connect gate="D" pin="IO_19" pad="F11"/>
<connect gate="D" pin="IO_2" pad="D17"/>
<connect gate="D" pin="IO_20" pad="F14"/>
<connect gate="D" pin="IO_21" pad="F15"/>
<connect gate="D" pin="IO_22" pad="F16"/>
<connect gate="D" pin="IO_23" pad="F17"/>
<connect gate="D" pin="IO_24" pad="F19"/>
<connect gate="D" pin="IO_25" pad="F20"/>
<connect gate="D" pin="IO_26" pad="G14"/>
<connect gate="D" pin="IO_27" pad="G15"/>
<connect gate="D" pin="IO_28" pad="G16"/>
<connect gate="D" pin="IO_29" pad="G17"/>
<connect gate="D" pin="IO_3" pad="D18"/>
<connect gate="D" pin="IO_30" pad="G18"/>
<connect gate="D" pin="IO_31" pad="G19"/>
<connect gate="D" pin="IO_32" pad="G23"/>
<connect gate="D" pin="IO_33" pad="G24"/>
<connect gate="D" pin="IO_34" pad="G25"/>
<connect gate="D" pin="IO_35" pad="G26"/>
<connect gate="D" pin="IO_36" pad="H23"/>
<connect gate="D" pin="IO_37" pad="H24"/>
<connect gate="D" pin="IO_38" pad="H25"/>
<connect gate="D" pin="IO_39" pad="H26"/>
<connect gate="D" pin="IO_4" pad="D19"/>
<connect gate="D" pin="IO_40" pad="J23"/>
<connect gate="D" pin="IO_41" pad="J24"/>
<connect gate="D" pin="IO_42" pad="J25"/>
<connect gate="D" pin="IO_5" pad="D20"/>
<connect gate="D" pin="IO_6" pad="D21"/>
<connect gate="D" pin="IO_7" pad="E10"/>
<connect gate="D" pin="IO_8" pad="E11"/>
<connect gate="D" pin="IO_9" pad="E12"/>
<connect gate="D" pin="NC" pad="G11"/>
<connect gate="D" pin="NCE" pad="E22"/>
<connect gate="D" pin="NC_10" pad="J18"/>
<connect gate="D" pin="NC_11" pad="F13"/>
<connect gate="D" pin="NC_12" pad="H17"/>
<connect gate="D" pin="NC_13" pad="F18"/>
<connect gate="D" pin="NC_14" pad="J14"/>
<connect gate="D" pin="NC_15" pad="D23"/>
<connect gate="D" pin="NC_16" pad="H18"/>
<connect gate="D" pin="NC_17" pad="F21"/>
<connect gate="D" pin="NC_18" pad="J19"/>
<connect gate="D" pin="NC_19" pad="D24"/>
<connect gate="D" pin="NC_2" pad="E23"/>
<connect gate="D" pin="NC_20" pad="H19"/>
<connect gate="D" pin="NC_21" pad="F22"/>
<connect gate="D" pin="NC_22" pad="J15"/>
<connect gate="D" pin="NC_23" pad="H10"/>
<connect gate="D" pin="NC_24" pad="H20"/>
<connect gate="D" pin="NC_25" pad="D25"/>
<connect gate="D" pin="NC_26" pad="J20"/>
<connect gate="D" pin="NC_27" pad="H11"/>
<connect gate="D" pin="NC_28" pad="H21"/>
<connect gate="D" pin="NC_29" pad="F23"/>
<connect gate="D" pin="NC_3" pad="E24"/>
<connect gate="D" pin="NC_30" pad="J21"/>
<connect gate="D" pin="NC_31" pad="G20"/>
<connect gate="D" pin="NC_32" pad="H22"/>
<connect gate="D" pin="NC_33" pad="F24"/>
<connect gate="D" pin="NC_34" pad="J22"/>
<connect gate="D" pin="NC_35" pad="G21"/>
<connect gate="D" pin="NC_36" pad="J10"/>
<connect gate="D" pin="NC_37" pad="F25"/>
<connect gate="D" pin="NC_38" pad="J11"/>
<connect gate="D" pin="NC_39" pad="F26"/>
<connect gate="D" pin="NC_4" pad="H15"/>
<connect gate="D" pin="NC_40" pad="G10"/>
<connect gate="D" pin="NC_5" pad="E25"/>
<connect gate="D" pin="NC_6" pad="J17"/>
<connect gate="D" pin="NC_7" pad="E26"/>
<connect gate="D" pin="NC_8" pad="H16"/>
<connect gate="D" pin="NC_9" pad="F12"/>
<connect gate="D" pin="NSTATUS" pad="E21"/>
<connect gate="D" pin="VCCA_PLL5" pad="G12"/>
<connect gate="D" pin="VCCD_PLL5" pad="H14"/>
<connect gate="D" pin="VCCIO2" pad="D26"/>
<connect gate="D" pin="VCCPD3" pad="J16"/>
<connect gate="D" pin="VCCPD4" pad="J12"/>
<connect gate="D" pin="VCC_PLL5_OUT" pad="H12"/>
<connect gate="D" pin="VREFB2N0" pad="G22"/>
<connect gate="D" pin="VREFB3N0" pad="D16"/>
<connect gate="D" pin="VREFB3N1" pad="D22"/>
<connect gate="E" pin="CLK1N" pad="N24"/>
<connect gate="E" pin="CLK1P" pad="N25"/>
<connect gate="E" pin="CLK3N" pad="P22"/>
<connect gate="E" pin="CLK3P" pad="P23"/>
<connect gate="E" pin="GND" pad="L13"/>
<connect gate="E" pin="GNDA_PLL1" pad="P18"/>
<connect gate="E" pin="GNDA_PLL1_2" pad="N18"/>
<connect gate="E" pin="GNDA_PLL2" pad="R20"/>
<connect gate="E" pin="GNDA_PLL2_2" pad="R19"/>
<connect gate="E" pin="GND_10" pad="N11"/>
<connect gate="E" pin="GND_11" pad="P10"/>
<connect gate="E" pin="GND_12" pad="M12"/>
<connect gate="E" pin="GND_13" pad="M14"/>
<connect gate="E" pin="GND_14" pad="N15"/>
<connect gate="E" pin="GND_15" pad="L17"/>
<connect gate="E" pin="GND_16" pad="N17"/>
<connect gate="E" pin="GND_17" pad="R11"/>
<connect gate="E" pin="GND_18" pad="R15"/>
<connect gate="E" pin="GND_19" pad="N13"/>
<connect gate="E" pin="GND_2" pad="K12"/>
<connect gate="E" pin="GND_20" pad="P16"/>
<connect gate="E" pin="GND_21" pad="P14"/>
<connect gate="E" pin="GND_22" pad="P26"/>
<connect gate="E" pin="GND_23" pad="R13"/>
<connect gate="E" pin="GND_24" pad="R17"/>
<connect gate="E" pin="GND_3" pad="K14"/>
<connect gate="E" pin="GND_4" pad="L15"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="M10"/>
<connect gate="E" pin="GND_7" pad="M16"/>
<connect gate="E" pin="GND_8" pad="P12"/>
<connect gate="E" pin="GND_9" pad="N26"/>
<connect gate="E" pin="IO" pad="P25"/>
<connect gate="E" pin="IO_10" pad="L18"/>
<connect gate="E" pin="IO_11" pad="L19"/>
<connect gate="E" pin="IO_12" pad="L20"/>
<connect gate="E" pin="IO_13" pad="L21"/>
<connect gate="E" pin="IO_14" pad="L22"/>
<connect gate="E" pin="IO_15" pad="L23"/>
<connect gate="E" pin="IO_16" pad="L24"/>
<connect gate="E" pin="IO_17" pad="L25"/>
<connect gate="E" pin="IO_18" pad="M19"/>
<connect gate="E" pin="IO_19" pad="M20"/>
<connect gate="E" pin="IO_2" pad="K19"/>
<connect gate="E" pin="IO_20" pad="M21"/>
<connect gate="E" pin="IO_21" pad="M22"/>
<connect gate="E" pin="IO_22" pad="M23"/>
<connect gate="E" pin="IO_23" pad="M24"/>
<connect gate="E" pin="IO_24" pad="M25"/>
<connect gate="E" pin="IO_25" pad="M26"/>
<connect gate="E" pin="IO_26" pad="N19"/>
<connect gate="E" pin="IO_27" pad="N20"/>
<connect gate="E" pin="IO_28" pad="N21"/>
<connect gate="E" pin="IO_29" pad="N22"/>
<connect gate="E" pin="IO_3" pad="K20"/>
<connect gate="E" pin="IO_30" pad="P24"/>
<connect gate="E" pin="IO_4" pad="K21"/>
<connect gate="E" pin="IO_5" pad="K22"/>
<connect gate="E" pin="IO_6" pad="K23"/>
<connect gate="E" pin="IO_7" pad="K24"/>
<connect gate="E" pin="IO_8" pad="K25"/>
<connect gate="E" pin="IO_9" pad="K26"/>
<connect gate="E" pin="NC" pad="K11"/>
<connect gate="E" pin="NC_2" pad="K16"/>
<connect gate="E" pin="NC_3" pad="K17"/>
<connect gate="E" pin="NC_4" pad="K10"/>
<connect gate="E" pin="NC_5" pad="K18"/>
<connect gate="E" pin="VCCA_PLL1" pad="P21"/>
<connect gate="E" pin="VCCD_PLL1" pad="P19"/>
<connect gate="E" pin="VCCD_PLL2" pad="P20"/>
<connect gate="E" pin="VCCINT" pad="L16"/>
<connect gate="E" pin="VCCINT_10" pad="N12"/>
<connect gate="E" pin="VCCINT_11" pad="L12"/>
<connect gate="E" pin="VCCINT_12" pad="P13"/>
<connect gate="E" pin="VCCINT_13" pad="N14"/>
<connect gate="E" pin="VCCINT_14" pad="L14"/>
<connect gate="E" pin="VCCINT_15" pad="P15"/>
<connect gate="E" pin="VCCINT_16" pad="N16"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="R12"/>
<connect gate="E" pin="VCCINT_4" pad="M13"/>
<connect gate="E" pin="VCCINT_5" pad="R16"/>
<connect gate="E" pin="VCCINT_6" pad="M15"/>
<connect gate="E" pin="VCCINT_7" pad="R14"/>
<connect gate="E" pin="VCCINT_8" pad="L10"/>
<connect gate="E" pin="VCCINT_9" pad="P11"/>
<connect gate="E" pin="VCCIO1" pad="P17"/>
<connect gate="E" pin="VCCIO2" pad="M17"/>
<connect gate="E" pin="VCCIO2_2" pad="L26"/>
<connect gate="E" pin="VCCIO3" pad="K15"/>
<connect gate="E" pin="VCCIO4" pad="K13"/>
<connect gate="E" pin="VCCIO5" pad="N10"/>
<connect gate="E" pin="VCCIO6" pad="R10"/>
<connect gate="E" pin="VCCPD1" pad="R18"/>
<connect gate="E" pin="VCCPD2" pad="M18"/>
<connect gate="E" pin="VREFB2N1" pad="N23"/>
<connect gate="F" pin="GND" pad="U11"/>
<connect gate="F" pin="GNDA_PLL6" pad="W14"/>
<connect gate="F" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="F" pin="GND_10" pad="U17"/>
<connect gate="F" pin="GND_11" pad="AA13"/>
<connect gate="F" pin="GND_2" pad="R22"/>
<connect gate="F" pin="GND_3" pad="T12"/>
<connect gate="F" pin="GND_4" pad="T10"/>
<connect gate="F" pin="GND_5" pad="U15"/>
<connect gate="F" pin="GND_6" pad="T14"/>
<connect gate="F" pin="GND_7" pad="T16"/>
<connect gate="F" pin="GND_8" pad="U13"/>
<connect gate="F" pin="GND_9" pad="T18"/>
<connect gate="F" pin="IO" pad="AA14"/>
<connect gate="F" pin="IO_10" pad="T24"/>
<connect gate="F" pin="IO_11" pad="T25"/>
<connect gate="F" pin="IO_12" pad="U19"/>
<connect gate="F" pin="IO_13" pad="U20"/>
<connect gate="F" pin="IO_14" pad="U21"/>
<connect gate="F" pin="IO_15" pad="U22"/>
<connect gate="F" pin="IO_16" pad="U23"/>
<connect gate="F" pin="IO_17" pad="U24"/>
<connect gate="F" pin="IO_18" pad="U25"/>
<connect gate="F" pin="IO_19" pad="U26"/>
<connect gate="F" pin="IO_2" pad="R23"/>
<connect gate="F" pin="IO_20" pad="V21"/>
<connect gate="F" pin="IO_21" pad="V22"/>
<connect gate="F" pin="IO_22" pad="V23"/>
<connect gate="F" pin="IO_23" pad="V24"/>
<connect gate="F" pin="IO_24" pad="V25"/>
<connect gate="F" pin="IO_25" pad="V26"/>
<connect gate="F" pin="IO_26" pad="W17"/>
<connect gate="F" pin="IO_27" pad="W18"/>
<connect gate="F" pin="IO_28" pad="W21"/>
<connect gate="F" pin="IO_29" pad="W22"/>
<connect gate="F" pin="IO_3" pad="R24"/>
<connect gate="F" pin="IO_30" pad="W23"/>
<connect gate="F" pin="IO_31" pad="W24"/>
<connect gate="F" pin="IO_32" pad="W25"/>
<connect gate="F" pin="IO_33" pad="W26"/>
<connect gate="F" pin="IO_34" pad="Y10"/>
<connect gate="F" pin="IO_35" pad="Y15"/>
<connect gate="F" pin="IO_36" pad="Y16"/>
<connect gate="F" pin="IO_37" pad="Y17"/>
<connect gate="F" pin="IO_38" pad="Y18"/>
<connect gate="F" pin="IO_39" pad="Y23"/>
<connect gate="F" pin="IO_4" pad="R25"/>
<connect gate="F" pin="IO_40" pad="Y24"/>
<connect gate="F" pin="IO_41" pad="Y25"/>
<connect gate="F" pin="IO_42" pad="Y26"/>
<connect gate="F" pin="IO_43" pad="AA10"/>
<connect gate="F" pin="IO_44" pad="AA11"/>
<connect gate="F" pin="IO_45" pad="AA12"/>
<connect gate="F" pin="IO_5" pad="R26"/>
<connect gate="F" pin="IO_6" pad="T19"/>
<connect gate="F" pin="IO_7" pad="T20"/>
<connect gate="F" pin="IO_8" pad="T21"/>
<connect gate="F" pin="IO_9" pad="T22"/>
<connect gate="F" pin="NC" pad="Y12"/>
<connect gate="F" pin="NC_10" pad="W10"/>
<connect gate="F" pin="NC_11" pad="W11"/>
<connect gate="F" pin="NC_12" pad="W12"/>
<connect gate="F" pin="NC_13" pad="W15"/>
<connect gate="F" pin="NC_14" pad="W16"/>
<connect gate="F" pin="NC_15" pad="Y20"/>
<connect gate="F" pin="NC_16" pad="W19"/>
<connect gate="F" pin="NC_17" pad="Y21"/>
<connect gate="F" pin="NC_18" pad="W20"/>
<connect gate="F" pin="NC_19" pad="Y11"/>
<connect gate="F" pin="NC_2" pad="V10"/>
<connect gate="F" pin="NC_3" pad="V12"/>
<connect gate="F" pin="NC_4" pad="V14"/>
<connect gate="F" pin="NC_5" pad="V16"/>
<connect gate="F" pin="NC_6" pad="V17"/>
<connect gate="F" pin="NC_7" pad="V18"/>
<connect gate="F" pin="NC_8" pad="V19"/>
<connect gate="F" pin="NC_9" pad="V20"/>
<connect gate="F" pin="VCCA_PLL2" pad="R21"/>
<connect gate="F" pin="VCCA_PLL6" pad="Y13"/>
<connect gate="F" pin="VCCD_PLL6" pad="Y14"/>
<connect gate="F" pin="VCCINT" pad="U10"/>
<connect gate="F" pin="VCCINT_2" pad="T13"/>
<connect gate="F" pin="VCCINT_3" pad="T17"/>
<connect gate="F" pin="VCCINT_4" pad="T15"/>
<connect gate="F" pin="VCCINT_5" pad="T11"/>
<connect gate="F" pin="VCCINT_6" pad="U18"/>
<connect gate="F" pin="VCCINT_7" pad="U16"/>
<connect gate="F" pin="VCCIO1" pad="T26"/>
<connect gate="F" pin="VCCIO7" pad="U12"/>
<connect gate="F" pin="VCCIO8" pad="U14"/>
<connect gate="F" pin="VCCPD7" pad="V11"/>
<connect gate="F" pin="VCCPD8" pad="V15"/>
<connect gate="F" pin="VCCSEL" pad="Y19"/>
<connect gate="F" pin="VCC_PLL6_OUT" pad="V13"/>
<connect gate="F" pin="VREFB1N0" pad="T23"/>
<connect gate="F" pin="VREFB1N1" pad="Y22"/>
<connect gate="G" pin="GND" pad="AF14"/>
<connect gate="G" pin="GND_2" pad="AE26"/>
<connect gate="G" pin="GND_3" pad="AF25"/>
<connect gate="G" pin="GND_4" pad="AF13"/>
<connect gate="G" pin="IO" pad="AF24"/>
<connect gate="G" pin="IO_10" pad="AB10"/>
<connect gate="G" pin="IO_11" pad="AB11"/>
<connect gate="G" pin="IO_12" pad="AB12"/>
<connect gate="G" pin="IO_13" pad="AB13"/>
<connect gate="G" pin="IO_14" pad="AB14"/>
<connect gate="G" pin="IO_15" pad="AB15"/>
<connect gate="G" pin="IO_16" pad="AB16"/>
<connect gate="G" pin="IO_17" pad="AB17"/>
<connect gate="G" pin="IO_18" pad="AB18"/>
<connect gate="G" pin="IO_19" pad="AB19"/>
<connect gate="G" pin="IO_2" pad="AA15"/>
<connect gate="G" pin="IO_20" pad="AB20"/>
<connect gate="G" pin="IO_21" pad="AC10"/>
<connect gate="G" pin="IO_22" pad="AC12"/>
<connect gate="G" pin="IO_23" pad="AC13"/>
<connect gate="G" pin="IO_24" pad="AC14"/>
<connect gate="G" pin="IO_25" pad="AC17"/>
<connect gate="G" pin="IO_26" pad="AC18"/>
<connect gate="G" pin="IO_27" pad="AC19"/>
<connect gate="G" pin="IO_28" pad="AC20"/>
<connect gate="G" pin="IO_29" pad="AC21"/>
<connect gate="G" pin="IO_3" pad="AA16"/>
<connect gate="G" pin="IO_30" pad="AD10"/>
<connect gate="G" pin="IO_31" pad="AD11"/>
<connect gate="G" pin="IO_32" pad="AD12"/>
<connect gate="G" pin="IO_33" pad="AD13"/>
<connect gate="G" pin="IO_34" pad="AD14"/>
<connect gate="G" pin="IO_35" pad="AD16"/>
<connect gate="G" pin="IO_36" pad="AD17"/>
<connect gate="G" pin="IO_37" pad="AD18"/>
<connect gate="G" pin="IO_38" pad="AD19"/>
<connect gate="G" pin="IO_39" pad="AD20"/>
<connect gate="G" pin="IO_4" pad="AA17"/>
<connect gate="G" pin="IO_40" pad="AD21"/>
<connect gate="G" pin="IO_41" pad="AD22"/>
<connect gate="G" pin="IO_42" pad="AD23"/>
<connect gate="G" pin="IO_43" pad="AE10"/>
<connect gate="G" pin="IO_44" pad="AE11"/>
<connect gate="G" pin="IO_45" pad="AE12"/>
<connect gate="G" pin="IO_46" pad="AE13"/>
<connect gate="G" pin="IO_47" pad="AE14"/>
<connect gate="G" pin="IO_48" pad="AE15"/>
<connect gate="G" pin="IO_49" pad="AE16"/>
<connect gate="G" pin="IO_5" pad="AA19"/>
<connect gate="G" pin="IO_50" pad="AE17"/>
<connect gate="G" pin="IO_51" pad="AE18"/>
<connect gate="G" pin="IO_52" pad="AE19"/>
<connect gate="G" pin="IO_53" pad="AE20"/>
<connect gate="G" pin="IO_54" pad="AE21"/>
<connect gate="G" pin="IO_55" pad="AE22"/>
<connect gate="G" pin="IO_56" pad="AE23"/>
<connect gate="G" pin="IO_57" pad="AE24"/>
<connect gate="G" pin="IO_58" pad="AF10"/>
<connect gate="G" pin="IO_59" pad="AF12"/>
<connect gate="G" pin="IO_6" pad="AA23"/>
<connect gate="G" pin="IO_60" pad="AF15"/>
<connect gate="G" pin="IO_61" pad="AF17"/>
<connect gate="G" pin="IO_62" pad="AF18"/>
<connect gate="G" pin="IO_63" pad="AF19"/>
<connect gate="G" pin="IO_64" pad="AF20"/>
<connect gate="G" pin="IO_65" pad="AF21"/>
<connect gate="G" pin="IO_66" pad="AF22"/>
<connect gate="G" pin="IO_7" pad="AA24"/>
<connect gate="G" pin="IO_8" pad="AA25"/>
<connect gate="G" pin="IO_9" pad="AA26"/>
<connect gate="G" pin="NC" pad="AC25"/>
<connect gate="G" pin="NCONFIG" pad="AA20"/>
<connect gate="G" pin="NC_10" pad="AC24"/>
<connect gate="G" pin="NC_11" pad="AD15"/>
<connect gate="G" pin="NC_12" pad="AD25"/>
<connect gate="G" pin="NC_13" pad="AB26"/>
<connect gate="G" pin="NC_14" pad="AD26"/>
<connect gate="G" pin="NC_2" pad="AA21"/>
<connect gate="G" pin="NC_3" pad="AA18"/>
<connect gate="G" pin="NC_4" pad="AA22"/>
<connect gate="G" pin="NC_5" pad="AC15"/>
<connect gate="G" pin="NC_6" pad="AB23"/>
<connect gate="G" pin="NC_7" pad="AB24"/>
<connect gate="G" pin="NC_8" pad="AC23"/>
<connect gate="G" pin="NC_9" pad="AB25"/>
<connect gate="G" pin="TCK" pad="AB22"/>
<connect gate="G" pin="TDI" pad="AE25"/>
<connect gate="G" pin="TMS" pad="AD24"/>
<connect gate="G" pin="TRST" pad="AB21"/>
<connect gate="G" pin="VCCIO1" pad="AC26"/>
<connect gate="G" pin="VCCIO7" pad="AF11"/>
<connect gate="G" pin="VCCIO8" pad="AF23"/>
<connect gate="G" pin="VCCIO8_2" pad="AF16"/>
<connect gate="G" pin="VREFB7N0" pad="AC11"/>
<connect gate="G" pin="VREFB8N0" pad="AC22"/>
<connect gate="G" pin="VREFB8N1" pad="AC16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S30F672C3N"/>
<attribute name="OC_FARNELL" value="1549487"/>
<attribute name="OC_NEWARK" value="52R0729"/>
<attribute name="PACKAGE" value="672-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S30F672C5N">
<description>Stratix II Devices</description>
<gates>
<gate name="A" symbol="EP2S30F672C5N_A"/>
<gate name="B" symbol="EP2S30F672C5N_B"/>
<gate name="C" symbol="EP2S30F672C5N_C"/>
<gate name="D" symbol="EP2S30F672C5N_D"/>
<gate name="E" symbol="EP2S30F672C5N_E"/>
<gate name="F" symbol="EP2S30F672C5N_F"/>
<gate name="G" symbol="EP2S30F672C5N_G"/>
</gates>
<devices>
<device name="" package="BGA672C26X26X100P_2700X2700X35">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="B6"/>
<connect gate="A" pin="IO_12" pad="B7"/>
<connect gate="A" pin="IO_13" pad="B8"/>
<connect gate="A" pin="IO_14" pad="B9"/>
<connect gate="A" pin="IO_15" pad="C3"/>
<connect gate="A" pin="IO_16" pad="C4"/>
<connect gate="A" pin="IO_17" pad="C5"/>
<connect gate="A" pin="IO_18" pad="C6"/>
<connect gate="A" pin="IO_19" pad="C7"/>
<connect gate="A" pin="IO_2" pad="A3"/>
<connect gate="A" pin="IO_20" pad="C8"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D6"/>
<connect gate="A" pin="IO_23" pad="D7"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D9"/>
<connect gate="A" pin="IO_26" pad="E7"/>
<connect gate="A" pin="IO_27" pad="E8"/>
<connect gate="A" pin="IO_28" pad="E9"/>
<connect gate="A" pin="IO_29" pad="G1"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="G2"/>
<connect gate="A" pin="IO_31" pad="G3"/>
<connect gate="A" pin="IO_32" pad="G4"/>
<connect gate="A" pin="IO_33" pad="H1"/>
<connect gate="A" pin="IO_34" pad="H2"/>
<connect gate="A" pin="IO_35" pad="H3"/>
<connect gate="A" pin="IO_36" pad="H4"/>
<connect gate="A" pin="IO_37" pad="J1"/>
<connect gate="A" pin="IO_38" pad="J2"/>
<connect gate="A" pin="IO_39" pad="J3"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="J4"/>
<connect gate="A" pin="IO_41" pad="K1"/>
<connect gate="A" pin="IO_42" pad="K2"/>
<connect gate="A" pin="IO_43" pad="K3"/>
<connect gate="A" pin="IO_44" pad="K4"/>
<connect gate="A" pin="IO_45" pad="K8"/>
<connect gate="A" pin="IO_46" pad="K9"/>
<connect gate="A" pin="IO_47" pad="L2"/>
<connect gate="A" pin="IO_48" pad="L3"/>
<connect gate="A" pin="IO_49" pad="L4"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="L5"/>
<connect gate="A" pin="IO_51" pad="L6"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_8" pad="B3"/>
<connect gate="A" pin="IO_9" pad="B4"/>
<connect gate="A" pin="MSEL0" pad="G8"/>
<connect gate="A" pin="MSEL1" pad="B2"/>
<connect gate="A" pin="MSEL2" pad="E6"/>
<connect gate="A" pin="MSEL3" pad="F7"/>
<connect gate="A" pin="NC" pad="K7"/>
<connect gate="A" pin="NC_10" pad="H8"/>
<connect gate="A" pin="NC_11" pad="D4"/>
<connect gate="A" pin="NC_12" pad="F8"/>
<connect gate="A" pin="NC_13" pad="F1"/>
<connect gate="A" pin="NC_14" pad="F9"/>
<connect gate="A" pin="NC_15" pad="E1"/>
<connect gate="A" pin="NC_16" pad="F2"/>
<connect gate="A" pin="NC_17" pad="F3"/>
<connect gate="A" pin="NC_18" pad="H9"/>
<connect gate="A" pin="NC_19" pad="C1"/>
<connect gate="A" pin="NC_2" pad="G9"/>
<connect gate="A" pin="NC_20" pad="F4"/>
<connect gate="A" pin="NC_21" pad="E2"/>
<connect gate="A" pin="NC_22" pad="E3"/>
<connect gate="A" pin="NC_23" pad="J5"/>
<connect gate="A" pin="NC_24" pad="C2"/>
<connect gate="A" pin="NC_25" pad="E4"/>
<connect gate="A" pin="NC_26" pad="J6"/>
<connect gate="A" pin="NC_27" pad="J7"/>
<connect gate="A" pin="NC_28" pad="J8"/>
<connect gate="A" pin="NC_29" pad="J9"/>
<connect gate="A" pin="NC_3" pad="H5"/>
<connect gate="A" pin="NC_30" pad="K6"/>
<connect gate="A" pin="NC_4" pad="H6"/>
<connect gate="A" pin="NC_5" pad="D2"/>
<connect gate="A" pin="NC_6" pad="H7"/>
<connect gate="A" pin="NC_7" pad="D3"/>
<connect gate="A" pin="NC_8" pad="G6"/>
<connect gate="A" pin="NC_9" pad="G7"/>
<connect gate="A" pin="TDO" pad="F6"/>
<connect gate="A" pin="TEMPDIODEN" pad="F5"/>
<connect gate="A" pin="TEMPDIODEP" pad="E5"/>
<connect gate="A" pin="VCCIO4" pad="A4"/>
<connect gate="A" pin="VCCIO5" pad="L1"/>
<connect gate="A" pin="VCCIO5_2" pad="D1"/>
<connect gate="A" pin="VREFB4N0" pad="D5"/>
<connect gate="A" pin="VREFB5N0" pad="K5"/>
<connect gate="A" pin="VREFB5N1" pad="G5"/>
<connect gate="B" pin="CLK11N" pad="N3"/>
<connect gate="B" pin="CLK11P" pad="N2"/>
<connect gate="B" pin="CLK9N" pad="R4"/>
<connect gate="B" pin="CLK9P" pad="R3"/>
<connect gate="B" pin="GND" pad="A14"/>
<connect gate="B" pin="GNDA_PLL3" pad="R8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="R7"/>
<connect gate="B" pin="GNDA_PLL4" pad="N9"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="N8"/>
<connect gate="B" pin="GND_2" pad="P1"/>
<connect gate="B" pin="GND_3" pad="A13"/>
<connect gate="B" pin="GND_4" pad="N1"/>
<connect gate="B" pin="GND_5" pad="P6"/>
<connect gate="B" pin="GND_6" pad="U9"/>
<connect gate="B" pin="IO" pad="A22"/>
<connect gate="B" pin="IO_10" pad="M7"/>
<connect gate="B" pin="IO_11" pad="M8"/>
<connect gate="B" pin="IO_12" pad="N4"/>
<connect gate="B" pin="IO_13" pad="N5"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="N7"/>
<connect gate="B" pin="IO_16" pad="P2"/>
<connect gate="B" pin="IO_17" pad="P3"/>
<connect gate="B" pin="IO_18" pad="P4"/>
<connect gate="B" pin="IO_19" pad="P5"/>
<connect gate="B" pin="IO_2" pad="L8"/>
<connect gate="B" pin="IO_20" pad="R1"/>
<connect gate="B" pin="IO_21" pad="R2"/>
<connect gate="B" pin="IO_22" pad="T2"/>
<connect gate="B" pin="IO_23" pad="T3"/>
<connect gate="B" pin="IO_24" pad="T4"/>
<connect gate="B" pin="IO_25" pad="T5"/>
<connect gate="B" pin="IO_26" pad="T6"/>
<connect gate="B" pin="IO_27" pad="T7"/>
<connect gate="B" pin="IO_28" pad="T8"/>
<connect gate="B" pin="IO_29" pad="T9"/>
<connect gate="B" pin="IO_3" pad="L9"/>
<connect gate="B" pin="IO_30" pad="U1"/>
<connect gate="B" pin="IO_31" pad="U2"/>
<connect gate="B" pin="IO_32" pad="U3"/>
<connect gate="B" pin="IO_33" pad="U4"/>
<connect gate="B" pin="IO_34" pad="U5"/>
<connect gate="B" pin="IO_35" pad="U6"/>
<connect gate="B" pin="IO_36" pad="U7"/>
<connect gate="B" pin="IO_37" pad="U8"/>
<connect gate="B" pin="IO_38" pad="V1"/>
<connect gate="B" pin="IO_39" pad="V2"/>
<connect gate="B" pin="IO_4" pad="M1"/>
<connect gate="B" pin="IO_40" pad="V3"/>
<connect gate="B" pin="IO_41" pad="V4"/>
<connect gate="B" pin="IO_42" pad="V5"/>
<connect gate="B" pin="IO_43" pad="V6"/>
<connect gate="B" pin="IO_44" pad="V7"/>
<connect gate="B" pin="IO_45" pad="V8"/>
<connect gate="B" pin="IO_46" pad="W1"/>
<connect gate="B" pin="IO_47" pad="W2"/>
<connect gate="B" pin="IO_48" pad="W3"/>
<connect gate="B" pin="IO_49" pad="W4"/>
<connect gate="B" pin="IO_5" pad="M2"/>
<connect gate="B" pin="IO_50" pad="Y1"/>
<connect gate="B" pin="IO_51" pad="Y2"/>
<connect gate="B" pin="IO_52" pad="Y3"/>
<connect gate="B" pin="IO_53" pad="Y4"/>
<connect gate="B" pin="IO_54" pad="A10"/>
<connect gate="B" pin="IO_55" pad="A12"/>
<connect gate="B" pin="IO_56" pad="A15"/>
<connect gate="B" pin="IO_57" pad="A17"/>
<connect gate="B" pin="IO_58" pad="A18"/>
<connect gate="B" pin="IO_59" pad="A19"/>
<connect gate="B" pin="IO_6" pad="M3"/>
<connect gate="B" pin="IO_60" pad="A20"/>
<connect gate="B" pin="IO_61" pad="A21"/>
<connect gate="B" pin="IO_7" pad="M4"/>
<connect gate="B" pin="IO_8" pad="M5"/>
<connect gate="B" pin="IO_9" pad="M6"/>
<connect gate="B" pin="NC" pad="W9"/>
<connect gate="B" pin="NC_2" pad="Y6"/>
<connect gate="B" pin="NC_3" pad="W5"/>
<connect gate="B" pin="NC_4" pad="Y9"/>
<connect gate="B" pin="NC_5" pad="W6"/>
<connect gate="B" pin="NC_6" pad="Y7"/>
<connect gate="B" pin="NC_7" pad="W7"/>
<connect gate="B" pin="NC_8" pad="W8"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA_PLL3" pad="R6"/>
<connect gate="B" pin="VCCA_PLL4" pad="P8"/>
<connect gate="B" pin="VCCD_PLL3" pad="P7"/>
<connect gate="B" pin="VCCD_PLL4" pad="P9"/>
<connect gate="B" pin="VCCINT" pad="V9"/>
<connect gate="B" pin="VCCIO3" pad="A16"/>
<connect gate="B" pin="VCCIO4" pad="A11"/>
<connect gate="B" pin="VCCIO6" pad="T1"/>
<connect gate="B" pin="VCCPD5" pad="M9"/>
<connect gate="B" pin="VCCPD6" pad="R9"/>
<connect gate="B" pin="VREFB6N0" pad="Y5"/>
<connect gate="B" pin="VREFB6N1" pad="R5"/>
<connect gate="C" pin="CONF_DONE" pad="B25"/>
<connect gate="C" pin="DCLK" pad="C24"/>
<connect gate="C" pin="GND" pad="B26"/>
<connect gate="C" pin="GND_2" pad="AE1"/>
<connect gate="C" pin="GND_3" pad="A25"/>
<connect gate="C" pin="GND_4" pad="AF2"/>
<connect gate="C" pin="GND_5" pad="AA7"/>
<connect gate="C" pin="IO" pad="D15"/>
<connect gate="C" pin="IO_10" pad="AC8"/>
<connect gate="C" pin="IO_11" pad="AC9"/>
<connect gate="C" pin="IO_12" pad="AD3"/>
<connect gate="C" pin="IO_13" pad="AD4"/>
<connect gate="C" pin="IO_14" pad="AD5"/>
<connect gate="C" pin="IO_15" pad="AD6"/>
<connect gate="C" pin="IO_16" pad="AD7"/>
<connect gate="C" pin="IO_17" pad="AD8"/>
<connect gate="C" pin="IO_18" pad="AD9"/>
<connect gate="C" pin="IO_19" pad="AE3"/>
<connect gate="C" pin="IO_2" pad="A24"/>
<connect gate="C" pin="IO_20" pad="AE4"/>
<connect gate="C" pin="IO_21" pad="AE5"/>
<connect gate="C" pin="IO_22" pad="AE6"/>
<connect gate="C" pin="IO_23" pad="AE7"/>
<connect gate="C" pin="IO_24" pad="AE8"/>
<connect gate="C" pin="IO_25" pad="AE9"/>
<connect gate="C" pin="IO_26" pad="AF3"/>
<connect gate="C" pin="IO_27" pad="AF5"/>
<connect gate="C" pin="IO_28" pad="AF6"/>
<connect gate="C" pin="IO_29" pad="AF7"/>
<connect gate="C" pin="IO_3" pad="AA1"/>
<connect gate="C" pin="IO_30" pad="AF8"/>
<connect gate="C" pin="IO_31" pad="AF9"/>
<connect gate="C" pin="IO_32" pad="B10"/>
<connect gate="C" pin="IO_33" pad="B11"/>
<connect gate="C" pin="IO_34" pad="B12"/>
<connect gate="C" pin="IO_35" pad="B13"/>
<connect gate="C" pin="IO_36" pad="B14"/>
<connect gate="C" pin="IO_37" pad="B15"/>
<connect gate="C" pin="IO_38" pad="B16"/>
<connect gate="C" pin="IO_39" pad="B17"/>
<connect gate="C" pin="IO_4" pad="AA2"/>
<connect gate="C" pin="IO_40" pad="B18"/>
<connect gate="C" pin="IO_41" pad="B19"/>
<connect gate="C" pin="IO_42" pad="B20"/>
<connect gate="C" pin="IO_43" pad="B21"/>
<connect gate="C" pin="IO_44" pad="B22"/>
<connect gate="C" pin="IO_45" pad="B23"/>
<connect gate="C" pin="IO_46" pad="B24"/>
<connect gate="C" pin="IO_47" pad="C10"/>
<connect gate="C" pin="IO_48" pad="C11"/>
<connect gate="C" pin="IO_49" pad="C12"/>
<connect gate="C" pin="IO_5" pad="AB1"/>
<connect gate="C" pin="IO_50" pad="C13"/>
<connect gate="C" pin="IO_51" pad="C14"/>
<connect gate="C" pin="IO_52" pad="C15"/>
<connect gate="C" pin="IO_53" pad="C16"/>
<connect gate="C" pin="IO_54" pad="C17"/>
<connect gate="C" pin="IO_55" pad="C18"/>
<connect gate="C" pin="IO_56" pad="C19"/>
<connect gate="C" pin="IO_57" pad="C20"/>
<connect gate="C" pin="IO_58" pad="C21"/>
<connect gate="C" pin="IO_59" pad="C22"/>
<connect gate="C" pin="IO_6" pad="AB2"/>
<connect gate="C" pin="IO_60" pad="C23"/>
<connect gate="C" pin="IO_61" pad="D10"/>
<connect gate="C" pin="IO_62" pad="D12"/>
<connect gate="C" pin="IO_63" pad="D13"/>
<connect gate="C" pin="IO_7" pad="AB9"/>
<connect gate="C" pin="IO_8" pad="AC6"/>
<connect gate="C" pin="IO_9" pad="AC7"/>
<connect gate="C" pin="NC" pad="AC4"/>
<connect gate="C" pin="NCEO" pad="AB5"/>
<connect gate="C" pin="NC_10" pad="AB7"/>
<connect gate="C" pin="NC_11" pad="AB8"/>
<connect gate="C" pin="NC_12" pad="D14"/>
<connect gate="C" pin="NC_13" pad="C25"/>
<connect gate="C" pin="NC_14" pad="AD1"/>
<connect gate="C" pin="NC_15" pad="AC2"/>
<connect gate="C" pin="NC_16" pad="C26"/>
<connect gate="C" pin="NC_17" pad="AC3"/>
<connect gate="C" pin="NC_18" pad="AD2"/>
<connect gate="C" pin="NC_2" pad="AA3"/>
<connect gate="C" pin="NC_3" pad="AA8"/>
<connect gate="C" pin="NC_4" pad="AA4"/>
<connect gate="C" pin="NC_5" pad="AA9"/>
<connect gate="C" pin="NC_6" pad="AA5"/>
<connect gate="C" pin="NC_7" pad="AB3"/>
<connect gate="C" pin="NC_8" pad="AA6"/>
<connect gate="C" pin="NC_9" pad="AB4"/>
<connect gate="C" pin="NIO_PULLUP" pad="AE2"/>
<connect gate="C" pin="PLL_ENA" pad="AB6"/>
<connect gate="C" pin="VCCIO3" pad="A23"/>
<connect gate="C" pin="VCCIO6" pad="AC1"/>
<connect gate="C" pin="VCCIO7" pad="AF4"/>
<connect gate="C" pin="VREFB4N1" pad="D11"/>
<connect gate="C" pin="VREFB7N1" pad="AC5"/>
<connect gate="D" pin="GND" pad="G13"/>
<connect gate="D" pin="GNDA_PLL5" pad="H13"/>
<connect gate="D" pin="GNDA_PLL5_2" pad="J13"/>
<connect gate="D" pin="IO" pad="J26"/>
<connect gate="D" pin="IO_10" pad="E13"/>
<connect gate="D" pin="IO_11" pad="E14"/>
<connect gate="D" pin="IO_12" pad="E15"/>
<connect gate="D" pin="IO_13" pad="E16"/>
<connect gate="D" pin="IO_14" pad="E17"/>
<connect gate="D" pin="IO_15" pad="E18"/>
<connect gate="D" pin="IO_16" pad="E19"/>
<connect gate="D" pin="IO_17" pad="E20"/>
<connect gate="D" pin="IO_18" pad="F10"/>
<connect gate="D" pin="IO_19" pad="F11"/>
<connect gate="D" pin="IO_2" pad="D17"/>
<connect gate="D" pin="IO_20" pad="F14"/>
<connect gate="D" pin="IO_21" pad="F15"/>
<connect gate="D" pin="IO_22" pad="F16"/>
<connect gate="D" pin="IO_23" pad="F17"/>
<connect gate="D" pin="IO_24" pad="F19"/>
<connect gate="D" pin="IO_25" pad="F20"/>
<connect gate="D" pin="IO_26" pad="G14"/>
<connect gate="D" pin="IO_27" pad="G15"/>
<connect gate="D" pin="IO_28" pad="G16"/>
<connect gate="D" pin="IO_29" pad="G17"/>
<connect gate="D" pin="IO_3" pad="D18"/>
<connect gate="D" pin="IO_30" pad="G18"/>
<connect gate="D" pin="IO_31" pad="G19"/>
<connect gate="D" pin="IO_32" pad="G23"/>
<connect gate="D" pin="IO_33" pad="G24"/>
<connect gate="D" pin="IO_34" pad="G25"/>
<connect gate="D" pin="IO_35" pad="G26"/>
<connect gate="D" pin="IO_36" pad="H23"/>
<connect gate="D" pin="IO_37" pad="H24"/>
<connect gate="D" pin="IO_38" pad="H25"/>
<connect gate="D" pin="IO_39" pad="H26"/>
<connect gate="D" pin="IO_4" pad="D19"/>
<connect gate="D" pin="IO_40" pad="J23"/>
<connect gate="D" pin="IO_41" pad="J24"/>
<connect gate="D" pin="IO_42" pad="J25"/>
<connect gate="D" pin="IO_5" pad="D20"/>
<connect gate="D" pin="IO_6" pad="D21"/>
<connect gate="D" pin="IO_7" pad="E10"/>
<connect gate="D" pin="IO_8" pad="E11"/>
<connect gate="D" pin="IO_9" pad="E12"/>
<connect gate="D" pin="NC" pad="G11"/>
<connect gate="D" pin="NCE" pad="E22"/>
<connect gate="D" pin="NC_10" pad="J18"/>
<connect gate="D" pin="NC_11" pad="F13"/>
<connect gate="D" pin="NC_12" pad="H17"/>
<connect gate="D" pin="NC_13" pad="F18"/>
<connect gate="D" pin="NC_14" pad="J14"/>
<connect gate="D" pin="NC_15" pad="D23"/>
<connect gate="D" pin="NC_16" pad="H18"/>
<connect gate="D" pin="NC_17" pad="F21"/>
<connect gate="D" pin="NC_18" pad="J19"/>
<connect gate="D" pin="NC_19" pad="D24"/>
<connect gate="D" pin="NC_2" pad="E23"/>
<connect gate="D" pin="NC_20" pad="H19"/>
<connect gate="D" pin="NC_21" pad="F22"/>
<connect gate="D" pin="NC_22" pad="J15"/>
<connect gate="D" pin="NC_23" pad="H10"/>
<connect gate="D" pin="NC_24" pad="H20"/>
<connect gate="D" pin="NC_25" pad="D25"/>
<connect gate="D" pin="NC_26" pad="J20"/>
<connect gate="D" pin="NC_27" pad="H11"/>
<connect gate="D" pin="NC_28" pad="H21"/>
<connect gate="D" pin="NC_29" pad="F23"/>
<connect gate="D" pin="NC_3" pad="E24"/>
<connect gate="D" pin="NC_30" pad="J21"/>
<connect gate="D" pin="NC_31" pad="G20"/>
<connect gate="D" pin="NC_32" pad="H22"/>
<connect gate="D" pin="NC_33" pad="F24"/>
<connect gate="D" pin="NC_34" pad="J22"/>
<connect gate="D" pin="NC_35" pad="G21"/>
<connect gate="D" pin="NC_36" pad="J10"/>
<connect gate="D" pin="NC_37" pad="F25"/>
<connect gate="D" pin="NC_38" pad="J11"/>
<connect gate="D" pin="NC_39" pad="F26"/>
<connect gate="D" pin="NC_4" pad="H15"/>
<connect gate="D" pin="NC_40" pad="G10"/>
<connect gate="D" pin="NC_5" pad="E25"/>
<connect gate="D" pin="NC_6" pad="J17"/>
<connect gate="D" pin="NC_7" pad="E26"/>
<connect gate="D" pin="NC_8" pad="H16"/>
<connect gate="D" pin="NC_9" pad="F12"/>
<connect gate="D" pin="NSTATUS" pad="E21"/>
<connect gate="D" pin="VCCA_PLL5" pad="G12"/>
<connect gate="D" pin="VCCD_PLL5" pad="H14"/>
<connect gate="D" pin="VCCIO2" pad="D26"/>
<connect gate="D" pin="VCCPD3" pad="J16"/>
<connect gate="D" pin="VCCPD4" pad="J12"/>
<connect gate="D" pin="VCC_PLL5_OUT" pad="H12"/>
<connect gate="D" pin="VREFB2N0" pad="G22"/>
<connect gate="D" pin="VREFB3N0" pad="D16"/>
<connect gate="D" pin="VREFB3N1" pad="D22"/>
<connect gate="E" pin="CLK1N" pad="N24"/>
<connect gate="E" pin="CLK1P" pad="N25"/>
<connect gate="E" pin="CLK3N" pad="P22"/>
<connect gate="E" pin="CLK3P" pad="P23"/>
<connect gate="E" pin="GND" pad="L13"/>
<connect gate="E" pin="GNDA_PLL1" pad="P18"/>
<connect gate="E" pin="GNDA_PLL1_2" pad="N18"/>
<connect gate="E" pin="GNDA_PLL2" pad="R20"/>
<connect gate="E" pin="GNDA_PLL2_2" pad="R19"/>
<connect gate="E" pin="GND_10" pad="N11"/>
<connect gate="E" pin="GND_11" pad="P10"/>
<connect gate="E" pin="GND_12" pad="M12"/>
<connect gate="E" pin="GND_13" pad="M14"/>
<connect gate="E" pin="GND_14" pad="N15"/>
<connect gate="E" pin="GND_15" pad="L17"/>
<connect gate="E" pin="GND_16" pad="N17"/>
<connect gate="E" pin="GND_17" pad="R11"/>
<connect gate="E" pin="GND_18" pad="R15"/>
<connect gate="E" pin="GND_19" pad="N13"/>
<connect gate="E" pin="GND_2" pad="K12"/>
<connect gate="E" pin="GND_20" pad="P16"/>
<connect gate="E" pin="GND_21" pad="P14"/>
<connect gate="E" pin="GND_22" pad="P26"/>
<connect gate="E" pin="GND_23" pad="R13"/>
<connect gate="E" pin="GND_24" pad="R17"/>
<connect gate="E" pin="GND_3" pad="K14"/>
<connect gate="E" pin="GND_4" pad="L15"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="M10"/>
<connect gate="E" pin="GND_7" pad="M16"/>
<connect gate="E" pin="GND_8" pad="P12"/>
<connect gate="E" pin="GND_9" pad="N26"/>
<connect gate="E" pin="IO" pad="P25"/>
<connect gate="E" pin="IO_10" pad="L18"/>
<connect gate="E" pin="IO_11" pad="L19"/>
<connect gate="E" pin="IO_12" pad="L20"/>
<connect gate="E" pin="IO_13" pad="L21"/>
<connect gate="E" pin="IO_14" pad="L22"/>
<connect gate="E" pin="IO_15" pad="L23"/>
<connect gate="E" pin="IO_16" pad="L24"/>
<connect gate="E" pin="IO_17" pad="L25"/>
<connect gate="E" pin="IO_18" pad="M19"/>
<connect gate="E" pin="IO_19" pad="M20"/>
<connect gate="E" pin="IO_2" pad="K19"/>
<connect gate="E" pin="IO_20" pad="M21"/>
<connect gate="E" pin="IO_21" pad="M22"/>
<connect gate="E" pin="IO_22" pad="M23"/>
<connect gate="E" pin="IO_23" pad="M24"/>
<connect gate="E" pin="IO_24" pad="M25"/>
<connect gate="E" pin="IO_25" pad="M26"/>
<connect gate="E" pin="IO_26" pad="N19"/>
<connect gate="E" pin="IO_27" pad="N20"/>
<connect gate="E" pin="IO_28" pad="N21"/>
<connect gate="E" pin="IO_29" pad="N22"/>
<connect gate="E" pin="IO_3" pad="K20"/>
<connect gate="E" pin="IO_30" pad="P24"/>
<connect gate="E" pin="IO_4" pad="K21"/>
<connect gate="E" pin="IO_5" pad="K22"/>
<connect gate="E" pin="IO_6" pad="K23"/>
<connect gate="E" pin="IO_7" pad="K24"/>
<connect gate="E" pin="IO_8" pad="K25"/>
<connect gate="E" pin="IO_9" pad="K26"/>
<connect gate="E" pin="NC" pad="K11"/>
<connect gate="E" pin="NC_2" pad="K16"/>
<connect gate="E" pin="NC_3" pad="K17"/>
<connect gate="E" pin="NC_4" pad="K10"/>
<connect gate="E" pin="NC_5" pad="K18"/>
<connect gate="E" pin="VCCA_PLL1" pad="P21"/>
<connect gate="E" pin="VCCD_PLL1" pad="P19"/>
<connect gate="E" pin="VCCD_PLL2" pad="P20"/>
<connect gate="E" pin="VCCINT" pad="L16"/>
<connect gate="E" pin="VCCINT_10" pad="N12"/>
<connect gate="E" pin="VCCINT_11" pad="L12"/>
<connect gate="E" pin="VCCINT_12" pad="P13"/>
<connect gate="E" pin="VCCINT_13" pad="N14"/>
<connect gate="E" pin="VCCINT_14" pad="L14"/>
<connect gate="E" pin="VCCINT_15" pad="P15"/>
<connect gate="E" pin="VCCINT_16" pad="N16"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="R12"/>
<connect gate="E" pin="VCCINT_4" pad="M13"/>
<connect gate="E" pin="VCCINT_5" pad="R16"/>
<connect gate="E" pin="VCCINT_6" pad="M15"/>
<connect gate="E" pin="VCCINT_7" pad="R14"/>
<connect gate="E" pin="VCCINT_8" pad="L10"/>
<connect gate="E" pin="VCCINT_9" pad="P11"/>
<connect gate="E" pin="VCCIO1" pad="P17"/>
<connect gate="E" pin="VCCIO2" pad="M17"/>
<connect gate="E" pin="VCCIO2_2" pad="L26"/>
<connect gate="E" pin="VCCIO3" pad="K15"/>
<connect gate="E" pin="VCCIO4" pad="K13"/>
<connect gate="E" pin="VCCIO5" pad="N10"/>
<connect gate="E" pin="VCCIO6" pad="R10"/>
<connect gate="E" pin="VCCPD1" pad="R18"/>
<connect gate="E" pin="VCCPD2" pad="M18"/>
<connect gate="E" pin="VREFB2N1" pad="N23"/>
<connect gate="F" pin="GND" pad="U11"/>
<connect gate="F" pin="GNDA_PLL6" pad="W14"/>
<connect gate="F" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="F" pin="GND_10" pad="U17"/>
<connect gate="F" pin="GND_11" pad="AA13"/>
<connect gate="F" pin="GND_2" pad="R22"/>
<connect gate="F" pin="GND_3" pad="T12"/>
<connect gate="F" pin="GND_4" pad="T10"/>
<connect gate="F" pin="GND_5" pad="U15"/>
<connect gate="F" pin="GND_6" pad="T14"/>
<connect gate="F" pin="GND_7" pad="T16"/>
<connect gate="F" pin="GND_8" pad="U13"/>
<connect gate="F" pin="GND_9" pad="T18"/>
<connect gate="F" pin="IO" pad="AA14"/>
<connect gate="F" pin="IO_10" pad="T24"/>
<connect gate="F" pin="IO_11" pad="T25"/>
<connect gate="F" pin="IO_12" pad="U19"/>
<connect gate="F" pin="IO_13" pad="U20"/>
<connect gate="F" pin="IO_14" pad="U21"/>
<connect gate="F" pin="IO_15" pad="U22"/>
<connect gate="F" pin="IO_16" pad="U23"/>
<connect gate="F" pin="IO_17" pad="U24"/>
<connect gate="F" pin="IO_18" pad="U25"/>
<connect gate="F" pin="IO_19" pad="U26"/>
<connect gate="F" pin="IO_2" pad="R23"/>
<connect gate="F" pin="IO_20" pad="V21"/>
<connect gate="F" pin="IO_21" pad="V22"/>
<connect gate="F" pin="IO_22" pad="V23"/>
<connect gate="F" pin="IO_23" pad="V24"/>
<connect gate="F" pin="IO_24" pad="V25"/>
<connect gate="F" pin="IO_25" pad="V26"/>
<connect gate="F" pin="IO_26" pad="W17"/>
<connect gate="F" pin="IO_27" pad="W18"/>
<connect gate="F" pin="IO_28" pad="W21"/>
<connect gate="F" pin="IO_29" pad="W22"/>
<connect gate="F" pin="IO_3" pad="R24"/>
<connect gate="F" pin="IO_30" pad="W23"/>
<connect gate="F" pin="IO_31" pad="W24"/>
<connect gate="F" pin="IO_32" pad="W25"/>
<connect gate="F" pin="IO_33" pad="W26"/>
<connect gate="F" pin="IO_34" pad="Y10"/>
<connect gate="F" pin="IO_35" pad="Y15"/>
<connect gate="F" pin="IO_36" pad="Y16"/>
<connect gate="F" pin="IO_37" pad="Y17"/>
<connect gate="F" pin="IO_38" pad="Y18"/>
<connect gate="F" pin="IO_39" pad="Y23"/>
<connect gate="F" pin="IO_4" pad="R25"/>
<connect gate="F" pin="IO_40" pad="Y24"/>
<connect gate="F" pin="IO_41" pad="Y25"/>
<connect gate="F" pin="IO_42" pad="Y26"/>
<connect gate="F" pin="IO_43" pad="AA10"/>
<connect gate="F" pin="IO_44" pad="AA11"/>
<connect gate="F" pin="IO_45" pad="AA12"/>
<connect gate="F" pin="IO_5" pad="R26"/>
<connect gate="F" pin="IO_6" pad="T19"/>
<connect gate="F" pin="IO_7" pad="T20"/>
<connect gate="F" pin="IO_8" pad="T21"/>
<connect gate="F" pin="IO_9" pad="T22"/>
<connect gate="F" pin="NC" pad="Y12"/>
<connect gate="F" pin="NC_10" pad="W10"/>
<connect gate="F" pin="NC_11" pad="W11"/>
<connect gate="F" pin="NC_12" pad="W12"/>
<connect gate="F" pin="NC_13" pad="W15"/>
<connect gate="F" pin="NC_14" pad="W16"/>
<connect gate="F" pin="NC_15" pad="Y20"/>
<connect gate="F" pin="NC_16" pad="W19"/>
<connect gate="F" pin="NC_17" pad="Y21"/>
<connect gate="F" pin="NC_18" pad="W20"/>
<connect gate="F" pin="NC_19" pad="Y11"/>
<connect gate="F" pin="NC_2" pad="V10"/>
<connect gate="F" pin="NC_3" pad="V12"/>
<connect gate="F" pin="NC_4" pad="V14"/>
<connect gate="F" pin="NC_5" pad="V16"/>
<connect gate="F" pin="NC_6" pad="V17"/>
<connect gate="F" pin="NC_7" pad="V18"/>
<connect gate="F" pin="NC_8" pad="V19"/>
<connect gate="F" pin="NC_9" pad="V20"/>
<connect gate="F" pin="VCCA_PLL2" pad="R21"/>
<connect gate="F" pin="VCCA_PLL6" pad="Y13"/>
<connect gate="F" pin="VCCD_PLL6" pad="Y14"/>
<connect gate="F" pin="VCCINT" pad="U10"/>
<connect gate="F" pin="VCCINT_2" pad="T13"/>
<connect gate="F" pin="VCCINT_3" pad="T17"/>
<connect gate="F" pin="VCCINT_4" pad="T15"/>
<connect gate="F" pin="VCCINT_5" pad="T11"/>
<connect gate="F" pin="VCCINT_6" pad="U18"/>
<connect gate="F" pin="VCCINT_7" pad="U16"/>
<connect gate="F" pin="VCCIO1" pad="T26"/>
<connect gate="F" pin="VCCIO7" pad="U12"/>
<connect gate="F" pin="VCCIO8" pad="U14"/>
<connect gate="F" pin="VCCPD7" pad="V11"/>
<connect gate="F" pin="VCCPD8" pad="V15"/>
<connect gate="F" pin="VCCSEL" pad="Y19"/>
<connect gate="F" pin="VCC_PLL6_OUT" pad="V13"/>
<connect gate="F" pin="VREFB1N0" pad="T23"/>
<connect gate="F" pin="VREFB1N1" pad="Y22"/>
<connect gate="G" pin="GND" pad="AF14"/>
<connect gate="G" pin="GND_2" pad="AE26"/>
<connect gate="G" pin="GND_3" pad="AF25"/>
<connect gate="G" pin="GND_4" pad="AF13"/>
<connect gate="G" pin="IO" pad="AF24"/>
<connect gate="G" pin="IO_10" pad="AB10"/>
<connect gate="G" pin="IO_11" pad="AB11"/>
<connect gate="G" pin="IO_12" pad="AB12"/>
<connect gate="G" pin="IO_13" pad="AB13"/>
<connect gate="G" pin="IO_14" pad="AB14"/>
<connect gate="G" pin="IO_15" pad="AB15"/>
<connect gate="G" pin="IO_16" pad="AB16"/>
<connect gate="G" pin="IO_17" pad="AB17"/>
<connect gate="G" pin="IO_18" pad="AB18"/>
<connect gate="G" pin="IO_19" pad="AB19"/>
<connect gate="G" pin="IO_2" pad="AA15"/>
<connect gate="G" pin="IO_20" pad="AB20"/>
<connect gate="G" pin="IO_21" pad="AC10"/>
<connect gate="G" pin="IO_22" pad="AC12"/>
<connect gate="G" pin="IO_23" pad="AC13"/>
<connect gate="G" pin="IO_24" pad="AC14"/>
<connect gate="G" pin="IO_25" pad="AC17"/>
<connect gate="G" pin="IO_26" pad="AC18"/>
<connect gate="G" pin="IO_27" pad="AC19"/>
<connect gate="G" pin="IO_28" pad="AC20"/>
<connect gate="G" pin="IO_29" pad="AC21"/>
<connect gate="G" pin="IO_3" pad="AA16"/>
<connect gate="G" pin="IO_30" pad="AD10"/>
<connect gate="G" pin="IO_31" pad="AD11"/>
<connect gate="G" pin="IO_32" pad="AD12"/>
<connect gate="G" pin="IO_33" pad="AD13"/>
<connect gate="G" pin="IO_34" pad="AD14"/>
<connect gate="G" pin="IO_35" pad="AD16"/>
<connect gate="G" pin="IO_36" pad="AD17"/>
<connect gate="G" pin="IO_37" pad="AD18"/>
<connect gate="G" pin="IO_38" pad="AD19"/>
<connect gate="G" pin="IO_39" pad="AD20"/>
<connect gate="G" pin="IO_4" pad="AA17"/>
<connect gate="G" pin="IO_40" pad="AD21"/>
<connect gate="G" pin="IO_41" pad="AD22"/>
<connect gate="G" pin="IO_42" pad="AD23"/>
<connect gate="G" pin="IO_43" pad="AE10"/>
<connect gate="G" pin="IO_44" pad="AE11"/>
<connect gate="G" pin="IO_45" pad="AE12"/>
<connect gate="G" pin="IO_46" pad="AE13"/>
<connect gate="G" pin="IO_47" pad="AE14"/>
<connect gate="G" pin="IO_48" pad="AE15"/>
<connect gate="G" pin="IO_49" pad="AE16"/>
<connect gate="G" pin="IO_5" pad="AA19"/>
<connect gate="G" pin="IO_50" pad="AE17"/>
<connect gate="G" pin="IO_51" pad="AE18"/>
<connect gate="G" pin="IO_52" pad="AE19"/>
<connect gate="G" pin="IO_53" pad="AE20"/>
<connect gate="G" pin="IO_54" pad="AE21"/>
<connect gate="G" pin="IO_55" pad="AE22"/>
<connect gate="G" pin="IO_56" pad="AE23"/>
<connect gate="G" pin="IO_57" pad="AE24"/>
<connect gate="G" pin="IO_58" pad="AF10"/>
<connect gate="G" pin="IO_59" pad="AF12"/>
<connect gate="G" pin="IO_6" pad="AA23"/>
<connect gate="G" pin="IO_60" pad="AF15"/>
<connect gate="G" pin="IO_61" pad="AF17"/>
<connect gate="G" pin="IO_62" pad="AF18"/>
<connect gate="G" pin="IO_63" pad="AF19"/>
<connect gate="G" pin="IO_64" pad="AF20"/>
<connect gate="G" pin="IO_65" pad="AF21"/>
<connect gate="G" pin="IO_66" pad="AF22"/>
<connect gate="G" pin="IO_7" pad="AA24"/>
<connect gate="G" pin="IO_8" pad="AA25"/>
<connect gate="G" pin="IO_9" pad="AA26"/>
<connect gate="G" pin="NC" pad="AC25"/>
<connect gate="G" pin="NCONFIG" pad="AA20"/>
<connect gate="G" pin="NC_10" pad="AC24"/>
<connect gate="G" pin="NC_11" pad="AD15"/>
<connect gate="G" pin="NC_12" pad="AD25"/>
<connect gate="G" pin="NC_13" pad="AB26"/>
<connect gate="G" pin="NC_14" pad="AD26"/>
<connect gate="G" pin="NC_2" pad="AA21"/>
<connect gate="G" pin="NC_3" pad="AA18"/>
<connect gate="G" pin="NC_4" pad="AA22"/>
<connect gate="G" pin="NC_5" pad="AC15"/>
<connect gate="G" pin="NC_6" pad="AB23"/>
<connect gate="G" pin="NC_7" pad="AB24"/>
<connect gate="G" pin="NC_8" pad="AC23"/>
<connect gate="G" pin="NC_9" pad="AB25"/>
<connect gate="G" pin="TCK" pad="AB22"/>
<connect gate="G" pin="TDI" pad="AE25"/>
<connect gate="G" pin="TMS" pad="AD24"/>
<connect gate="G" pin="TRST" pad="AB21"/>
<connect gate="G" pin="VCCIO1" pad="AC26"/>
<connect gate="G" pin="VCCIO7" pad="AF11"/>
<connect gate="G" pin="VCCIO8" pad="AF23"/>
<connect gate="G" pin="VCCIO8_2" pad="AF16"/>
<connect gate="G" pin="VREFB7N0" pad="AC11"/>
<connect gate="G" pin="VREFB8N0" pad="AC22"/>
<connect gate="G" pin="VREFB8N1" pad="AC16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S30F672C5N"/>
<attribute name="OC_FARNELL" value="1549489"/>
<attribute name="OC_NEWARK" value="51R0586"/>
<attribute name="PACKAGE" value="672-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S60F1020C3N">
<description>FPGA, STRATIX II</description>
<gates>
<gate name="A" symbol="EP2S60F1020C3N_A"/>
<gate name="B" symbol="EP2S60F1020C3N_B"/>
<gate name="C" symbol="EP2S60F1020C3N_C"/>
<gate name="D" symbol="EP2S60F1020C3N_D"/>
<gate name="E" symbol="EP2S60F1020C3N_E"/>
<gate name="F" symbol="EP2S60F1020C3N_F"/>
<gate name="G" symbol="EP2S60F1020C3N_G"/>
<gate name="H" symbol="EP2S60F1020C3N_H"/>
<gate name="I" symbol="EP2S60F1020C3N_I"/>
<gate name="J" symbol="EP2S60F1020C3N_J"/>
<gate name="K" symbol="EP2S60F1020C3N_K"/>
</gates>
<devices>
<device name="" package="BGA1020C100P32X32_3300X3300X35">
<connects>
<connect gate="A" pin="FPLL10CLKN" pad="D4"/>
<connect gate="A" pin="FPLL10CLKP" pad="D3"/>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GNDA_PLL10" pad="G8"/>
<connect gate="A" pin="GNDA_PLL10_2" pad="G7"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_3" pad="F7"/>
<connect gate="A" pin="GND_4" pad="K5"/>
<connect gate="A" pin="IO" pad="L4"/>
<connect gate="A" pin="IO_10" pad="A6"/>
<connect gate="A" pin="IO_11" pad="A7"/>
<connect gate="A" pin="IO_12" pad="A8"/>
<connect gate="A" pin="IO_13" pad="C4"/>
<connect gate="A" pin="IO_14" pad="A9"/>
<connect gate="A" pin="IO_15" pad="C5"/>
<connect gate="A" pin="IO_16" pad="C6"/>
<connect gate="A" pin="IO_17" pad="C7"/>
<connect gate="A" pin="IO_18" pad="D5"/>
<connect gate="A" pin="IO_19" pad="C8"/>
<connect gate="A" pin="IO_2" pad="B4"/>
<connect gate="A" pin="IO_20" pad="D6"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D7"/>
<connect gate="A" pin="IO_23" pad="D1"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="E2"/>
<connect gate="A" pin="IO_28" pad="E3"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="B5"/>
<connect gate="A" pin="IO_30" pad="E5"/>
<connect gate="A" pin="IO_31" pad="E6"/>
<connect gate="A" pin="IO_32" pad="E7"/>
<connect gate="A" pin="IO_33" pad="E8"/>
<connect gate="A" pin="IO_34" pad="E9"/>
<connect gate="A" pin="IO_35" pad="F1"/>
<connect gate="A" pin="IO_36" pad="F2"/>
<connect gate="A" pin="IO_37" pad="F3"/>
<connect gate="A" pin="IO_38" pad="F4"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="H1"/>
<connect gate="A" pin="IO_46" pad="H2"/>
<connect gate="A" pin="IO_47" pad="J1"/>
<connect gate="A" pin="IO_48" pad="J2"/>
<connect gate="A" pin="IO_49" pad="J3"/>
<connect gate="A" pin="IO_5" pad="B7"/>
<connect gate="A" pin="IO_50" pad="J4"/>
<connect gate="A" pin="IO_51" pad="J6"/>
<connect gate="A" pin="IO_52" pad="J7"/>
<connect gate="A" pin="IO_53" pad="J8"/>
<connect gate="A" pin="IO_54" pad="J9"/>
<connect gate="A" pin="IO_55" pad="K1"/>
<connect gate="A" pin="IO_56" pad="K2"/>
<connect gate="A" pin="IO_57" pad="K3"/>
<connect gate="A" pin="IO_58" pad="K4"/>
<connect gate="A" pin="IO_59" pad="K6"/>
<connect gate="A" pin="IO_6" pad="A4"/>
<connect gate="A" pin="IO_60" pad="K7"/>
<connect gate="A" pin="IO_61" pad="K8"/>
<connect gate="A" pin="IO_62" pad="K9"/>
<connect gate="A" pin="IO_63" pad="L1"/>
<connect gate="A" pin="IO_64" pad="L2"/>
<connect gate="A" pin="IO_65" pad="L3"/>
<connect gate="A" pin="IO_7" pad="B8"/>
<connect gate="A" pin="IO_8" pad="A5"/>
<connect gate="A" pin="IO_9" pad="B9"/>
<connect gate="A" pin="MSEL0" pad="B2"/>
<connect gate="A" pin="MSEL1" pad="F6"/>
<connect gate="A" pin="NC" pad="H6"/>
<connect gate="A" pin="NC_2" pad="G6"/>
<connect gate="A" pin="NC_3" pad="H3"/>
<connect gate="A" pin="NC_4" pad="H4"/>
<connect gate="A" pin="NC_5" pad="H5"/>
<connect gate="A" pin="NC_6" pad="H9"/>
<connect gate="A" pin="NC_7" pad="G5"/>
<connect gate="A" pin="TDO" pad="C3"/>
<connect gate="A" pin="TEMPDIODEN" pad="B3"/>
<connect gate="A" pin="TEMPDIODEP" pad="G9"/>
<connect gate="A" pin="VCCA_PLL10" pad="H8"/>
<connect gate="A" pin="VCCD_PLL10" pad="H7"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="C1"/>
<connect gate="A" pin="VREFB4N0" pad="C2"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N1" pad="J5"/>
<connect gate="A" pin="VREFB5N2" pad="F5"/>
<connect gate="B" pin="CLK11N" pad="T4"/>
<connect gate="B" pin="CLK11P" pad="T3"/>
<connect gate="B" pin="CLK9N" pad="U4"/>
<connect gate="B" pin="CLK9P" pad="U3"/>
<connect gate="B" pin="GND" pad="A13"/>
<connect gate="B" pin="GNDA_PLL3" pad="V8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="U8"/>
<connect gate="B" pin="GNDA_PLL4" pad="T8"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="R8"/>
<connect gate="B" pin="GND_2" pad="T7"/>
<connect gate="B" pin="GND_3" pad="N1"/>
<connect gate="B" pin="GND_4" pad="Y1"/>
<connect gate="B" pin="IO" pad="A16"/>
<connect gate="B" pin="IO_10" pad="M4"/>
<connect gate="B" pin="IO_11" pad="N4"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="M6"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="M7"/>
<connect gate="B" pin="IO_16" pad="N7"/>
<connect gate="B" pin="IO_17" pad="M8"/>
<connect gate="B" pin="IO_18" pad="N8"/>
<connect gate="B" pin="IO_19" pad="M9"/>
<connect gate="B" pin="IO_2" pad="L5"/>
<connect gate="B" pin="IO_20" pad="N9"/>
<connect gate="B" pin="IO_21" pad="P1"/>
<connect gate="B" pin="IO_22" pad="N2"/>
<connect gate="B" pin="IO_23" pad="P2"/>
<connect gate="B" pin="IO_24" pad="N3"/>
<connect gate="B" pin="IO_25" pad="T1"/>
<connect gate="B" pin="IO_26" pad="P4"/>
<connect gate="B" pin="IO_27" pad="T2"/>
<connect gate="B" pin="IO_28" pad="P5"/>
<connect gate="B" pin="IO_29" pad="P6"/>
<connect gate="B" pin="IO_3" pad="L6"/>
<connect gate="B" pin="IO_30" pad="P7"/>
<connect gate="B" pin="IO_31" pad="P8"/>
<connect gate="B" pin="IO_32" pad="P9"/>
<connect gate="B" pin="IO_33" pad="T5"/>
<connect gate="B" pin="IO_34" pad="R2"/>
<connect gate="B" pin="IO_35" pad="R3"/>
<connect gate="B" pin="IO_36" pad="R4"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="L7"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="U1"/>
<connect gate="B" pin="IO_42" pad="U2"/>
<connect gate="B" pin="IO_43" pad="U5"/>
<connect gate="B" pin="IO_44" pad="U6"/>
<connect gate="B" pin="IO_45" pad="V2"/>
<connect gate="B" pin="IO_46" pad="V3"/>
<connect gate="B" pin="IO_47" pad="V4"/>
<connect gate="B" pin="IO_48" pad="V5"/>
<connect gate="B" pin="IO_49" pad="V6"/>
<connect gate="B" pin="IO_5" pad="L8"/>
<connect gate="B" pin="IO_50" pad="V7"/>
<connect gate="B" pin="IO_51" pad="V9"/>
<connect gate="B" pin="IO_52" pad="W1"/>
<connect gate="B" pin="IO_53" pad="W2"/>
<connect gate="B" pin="IO_54" pad="W4"/>
<connect gate="B" pin="IO_55" pad="W5"/>
<connect gate="B" pin="IO_56" pad="W6"/>
<connect gate="B" pin="IO_57" pad="W7"/>
<connect gate="B" pin="IO_58" pad="W8"/>
<connect gate="B" pin="IO_59" pad="W9"/>
<connect gate="B" pin="IO_6" pad="L9"/>
<connect gate="B" pin="IO_60" pad="Y2"/>
<connect gate="B" pin="IO_61" pad="Y3"/>
<connect gate="B" pin="IO_62" pad="Y4"/>
<connect gate="B" pin="IO_63" pad="Y5"/>
<connect gate="B" pin="IO_64" pad="Y6"/>
<connect gate="B" pin="IO_65" pad="Y7"/>
<connect gate="B" pin="IO_66" pad="Y8"/>
<connect gate="B" pin="IO_67" pad="Y9"/>
<connect gate="B" pin="IO_68" pad="A10"/>
<connect gate="B" pin="IO_69" pad="A11"/>
<connect gate="B" pin="IO_7" pad="M1"/>
<connect gate="B" pin="IO_70" pad="A12"/>
<connect gate="B" pin="IO_71" pad="A14"/>
<connect gate="B" pin="IO_8" pad="M2"/>
<connect gate="B" pin="IO_9" pad="M3"/>
<connect gate="B" pin="VCCA_PLL3" pad="U9"/>
<connect gate="B" pin="VCCA_PLL4" pad="R9"/>
<connect gate="B" pin="VCCD_PLL3" pad="U7"/>
<connect gate="B" pin="VCCD_PLL4" pad="T9"/>
<connect gate="B" pin="VCCIO4" pad="A15"/>
<connect gate="B" pin="VCCIO5" pad="R1"/>
<connect gate="B" pin="VCCIO5_2" pad="M5"/>
<connect gate="B" pin="VCCIO6" pad="V1"/>
<connect gate="B" pin="VREFB5N0" pad="P3"/>
<connect gate="B" pin="VREFB6N2" pad="W3"/>
<connect gate="C" pin="FPLL9CLKN" pad="AJ4"/>
<connect gate="C" pin="FPLL9CLKP" pad="AJ3"/>
<connect gate="C" pin="GND" pad="AC5"/>
<connect gate="C" pin="GNDA_PLL9" pad="AF7"/>
<connect gate="C" pin="GNDA_PLL9_2" pad="AG7"/>
<connect gate="C" pin="GND_2" pad="AF9"/>
<connect gate="C" pin="GND_3" pad="A20"/>
<connect gate="C" pin="GND_4" pad="A31"/>
<connect gate="C" pin="GND_5" pad="AG6"/>
<connect gate="C" pin="IO" pad="AJ6"/>
<connect gate="C" pin="IO_10" pad="AA6"/>
<connect gate="C" pin="IO_11" pad="A19"/>
<connect gate="C" pin="IO_12" pad="AA7"/>
<connect gate="C" pin="IO_13" pad="A24"/>
<connect gate="C" pin="IO_14" pad="AA8"/>
<connect gate="C" pin="IO_15" pad="A25"/>
<connect gate="C" pin="IO_16" pad="AA9"/>
<connect gate="C" pin="IO_17" pad="A26"/>
<connect gate="C" pin="IO_18" pad="AB1"/>
<connect gate="C" pin="IO_19" pad="A27"/>
<connect gate="C" pin="IO_2" pad="AA1"/>
<connect gate="C" pin="IO_20" pad="AB2"/>
<connect gate="C" pin="IO_21" pad="A28"/>
<connect gate="C" pin="IO_22" pad="AB3"/>
<connect gate="C" pin="IO_23" pad="A29"/>
<connect gate="C" pin="IO_24" pad="AB4"/>
<connect gate="C" pin="IO_25" pad="AB5"/>
<connect gate="C" pin="IO_26" pad="AB6"/>
<connect gate="C" pin="IO_27" pad="AB7"/>
<connect gate="C" pin="IO_28" pad="AB8"/>
<connect gate="C" pin="IO_29" pad="AB9"/>
<connect gate="C" pin="IO_3" pad="AA2"/>
<connect gate="C" pin="IO_30" pad="AC1"/>
<connect gate="C" pin="IO_31" pad="AC2"/>
<connect gate="C" pin="IO_32" pad="AC3"/>
<connect gate="C" pin="IO_33" pad="AC4"/>
<connect gate="C" pin="IO_34" pad="AC6"/>
<connect gate="C" pin="IO_35" pad="AC7"/>
<connect gate="C" pin="IO_36" pad="AC8"/>
<connect gate="C" pin="IO_37" pad="AC9"/>
<connect gate="C" pin="IO_38" pad="AD1"/>
<connect gate="C" pin="IO_39" pad="AD2"/>
<connect gate="C" pin="IO_4" pad="A21"/>
<connect gate="C" pin="IO_40" pad="AD6"/>
<connect gate="C" pin="IO_41" pad="AD7"/>
<connect gate="C" pin="IO_42" pad="AD8"/>
<connect gate="C" pin="IO_43" pad="AD9"/>
<connect gate="C" pin="IO_44" pad="AE1"/>
<connect gate="C" pin="IO_45" pad="AE2"/>
<connect gate="C" pin="IO_46" pad="AE3"/>
<connect gate="C" pin="IO_47" pad="AE4"/>
<connect gate="C" pin="IO_48" pad="AF1"/>
<connect gate="C" pin="IO_49" pad="AF2"/>
<connect gate="C" pin="IO_5" pad="AA3"/>
<connect gate="C" pin="IO_50" pad="AF3"/>
<connect gate="C" pin="IO_51" pad="AF4"/>
<connect gate="C" pin="IO_52" pad="AG1"/>
<connect gate="C" pin="IO_53" pad="AG2"/>
<connect gate="C" pin="IO_54" pad="AG3"/>
<connect gate="C" pin="IO_55" pad="AG4"/>
<connect gate="C" pin="IO_56" pad="AG8"/>
<connect gate="C" pin="IO_57" pad="AG9"/>
<connect gate="C" pin="IO_58" pad="AH1"/>
<connect gate="C" pin="IO_59" pad="AH2"/>
<connect gate="C" pin="IO_6" pad="A22"/>
<connect gate="C" pin="IO_60" pad="AH3"/>
<connect gate="C" pin="IO_61" pad="AH4"/>
<connect gate="C" pin="IO_62" pad="AH5"/>
<connect gate="C" pin="IO_63" pad="AH6"/>
<connect gate="C" pin="IO_64" pad="AH7"/>
<connect gate="C" pin="IO_65" pad="AH8"/>
<connect gate="C" pin="IO_66" pad="AH9"/>
<connect gate="C" pin="IO_67" pad="AJ1"/>
<connect gate="C" pin="IO_68" pad="AJ2"/>
<connect gate="C" pin="IO_69" pad="AJ5"/>
<connect gate="C" pin="IO_7" pad="AA4"/>
<connect gate="C" pin="IO_8" pad="A23"/>
<connect gate="C" pin="IO_9" pad="A17"/>
<connect gate="C" pin="NC" pad="AF6"/>
<connect gate="C" pin="NC_2" pad="AE9"/>
<connect gate="C" pin="NC_3" pad="AE5"/>
<connect gate="C" pin="NC_4" pad="AD3"/>
<connect gate="C" pin="NC_5" pad="AF5"/>
<connect gate="C" pin="NC_6" pad="AD4"/>
<connect gate="C" pin="NC_7" pad="AE6"/>
<connect gate="C" pin="PLL_ENA" pad="AF8"/>
<connect gate="C" pin="VCCA_PLL9" pad="AE7"/>
<connect gate="C" pin="VCCD_PLL9" pad="AE8"/>
<connect gate="C" pin="VCCIO3" pad="A30"/>
<connect gate="C" pin="VCCIO3_2" pad="A18"/>
<connect gate="C" pin="VCCIO6" pad="AA5"/>
<connect gate="C" pin="VREFB6N0" pad="AG5"/>
<connect gate="C" pin="VREFB6N1" pad="AD5"/>
<connect gate="D" pin="DCLK" pad="B31"/>
<connect gate="D" pin="GND" pad="AM2"/>
<connect gate="D" pin="GND_2" pad="AL1"/>
<connect gate="D" pin="GND_3" pad="B32"/>
<connect gate="D" pin="IO" pad="D27"/>
<connect gate="D" pin="IO_10" pad="AL8"/>
<connect gate="D" pin="IO_11" pad="AK8"/>
<connect gate="D" pin="IO_12" pad="AL9"/>
<connect gate="D" pin="IO_13" pad="AJ7"/>
<connect gate="D" pin="IO_14" pad="AK9"/>
<connect gate="D" pin="IO_15" pad="AM4"/>
<connect gate="D" pin="IO_16" pad="AJ8"/>
<connect gate="D" pin="IO_17" pad="AM5"/>
<connect gate="D" pin="IO_18" pad="AM6"/>
<connect gate="D" pin="IO_19" pad="AM7"/>
<connect gate="D" pin="IO_2" pad="AL4"/>
<connect gate="D" pin="IO_20" pad="AM8"/>
<connect gate="D" pin="IO_21" pad="AM9"/>
<connect gate="D" pin="IO_22" pad="B10"/>
<connect gate="D" pin="IO_23" pad="B11"/>
<connect gate="D" pin="IO_24" pad="B12"/>
<connect gate="D" pin="IO_25" pad="B13"/>
<connect gate="D" pin="IO_26" pad="B14"/>
<connect gate="D" pin="IO_27" pad="B15"/>
<connect gate="D" pin="IO_28" pad="B16"/>
<connect gate="D" pin="IO_29" pad="B17"/>
<connect gate="D" pin="IO_3" pad="AK4"/>
<connect gate="D" pin="IO_30" pad="B18"/>
<connect gate="D" pin="IO_31" pad="B19"/>
<connect gate="D" pin="IO_32" pad="B20"/>
<connect gate="D" pin="IO_33" pad="B21"/>
<connect gate="D" pin="IO_34" pad="B22"/>
<connect gate="D" pin="IO_35" pad="B23"/>
<connect gate="D" pin="IO_36" pad="B24"/>
<connect gate="D" pin="IO_37" pad="B25"/>
<connect gate="D" pin="IO_38" pad="B26"/>
<connect gate="D" pin="IO_39" pad="B27"/>
<connect gate="D" pin="IO_4" pad="AL5"/>
<connect gate="D" pin="IO_40" pad="B28"/>
<connect gate="D" pin="IO_41" pad="B29"/>
<connect gate="D" pin="IO_42" pad="C10"/>
<connect gate="D" pin="IO_43" pad="C11"/>
<connect gate="D" pin="IO_44" pad="C12"/>
<connect gate="D" pin="IO_45" pad="C13"/>
<connect gate="D" pin="IO_46" pad="C15"/>
<connect gate="D" pin="IO_47" pad="C16"/>
<connect gate="D" pin="IO_48" pad="C17"/>
<connect gate="D" pin="IO_49" pad="C18"/>
<connect gate="D" pin="IO_5" pad="AK5"/>
<connect gate="D" pin="IO_50" pad="C20"/>
<connect gate="D" pin="IO_51" pad="C21"/>
<connect gate="D" pin="IO_52" pad="C22"/>
<connect gate="D" pin="IO_53" pad="C23"/>
<connect gate="D" pin="IO_54" pad="C24"/>
<connect gate="D" pin="IO_55" pad="C25"/>
<connect gate="D" pin="IO_56" pad="C26"/>
<connect gate="D" pin="IO_57" pad="C27"/>
<connect gate="D" pin="IO_58" pad="C28"/>
<connect gate="D" pin="IO_59" pad="C29"/>
<connect gate="D" pin="IO_6" pad="AL6"/>
<connect gate="D" pin="IO_60" pad="D10"/>
<connect gate="D" pin="IO_61" pad="D11"/>
<connect gate="D" pin="IO_62" pad="D12"/>
<connect gate="D" pin="IO_63" pad="D13"/>
<connect gate="D" pin="IO_64" pad="D14"/>
<connect gate="D" pin="IO_65" pad="D15"/>
<connect gate="D" pin="IO_66" pad="D16"/>
<connect gate="D" pin="IO_67" pad="D17"/>
<connect gate="D" pin="IO_68" pad="D18"/>
<connect gate="D" pin="IO_69" pad="D19"/>
<connect gate="D" pin="IO_7" pad="AK6"/>
<connect gate="D" pin="IO_70" pad="D20"/>
<connect gate="D" pin="IO_71" pad="D21"/>
<connect gate="D" pin="IO_72" pad="D22"/>
<connect gate="D" pin="IO_73" pad="D23"/>
<connect gate="D" pin="IO_74" pad="D25"/>
<connect gate="D" pin="IO_75" pad="D26"/>
<connect gate="D" pin="IO_8" pad="AL7"/>
<connect gate="D" pin="IO_9" pad="AK7"/>
<connect gate="D" pin="NCE" pad="C30"/>
<connect gate="D" pin="NCEO" pad="AL3"/>
<connect gate="D" pin="NIO_PULLUP" pad="AK3"/>
<connect gate="D" pin="NSTATUS" pad="B30"/>
<connect gate="D" pin="PORSEL" pad="AL2"/>
<connect gate="D" pin="VCCIO2" pad="C32"/>
<connect gate="D" pin="VCCIO6" pad="AK1"/>
<connect gate="D" pin="VCCIO7" pad="AM3"/>
<connect gate="D" pin="VREFB3N0" pad="C19"/>
<connect gate="D" pin="VREFB3N1" pad="D24"/>
<connect gate="D" pin="VREFB3N2" pad="C31"/>
<connect gate="D" pin="VREFB4N2" pad="C14"/>
<connect gate="D" pin="VREFB7N1" pad="AJ9"/>
<connect gate="D" pin="VREFB7N2" pad="AK2"/>
<connect gate="E" pin="FPLL7CLKN" pad="D29"/>
<connect gate="E" pin="FPLL7CLKP" pad="D30"/>
<connect gate="E" pin="GND" pad="E23"/>
<connect gate="E" pin="GNDA_PLL11" pad="H18"/>
<connect gate="E" pin="GNDA_PLL11_2" pad="G18"/>
<connect gate="E" pin="GNDA_PLL5" pad="H16"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="G16"/>
<connect gate="E" pin="GNDA_PLL7" pad="G26"/>
<connect gate="E" pin="GNDA_PLL7_2" pad="F26"/>
<connect gate="E" pin="GND_2" pad="E10"/>
<connect gate="E" pin="GND_3" pad="F27"/>
<connect gate="E" pin="GND_4" pad="G17"/>
<connect gate="E" pin="IO" pad="H28"/>
<connect gate="E" pin="IO_10" pad="E17"/>
<connect gate="E" pin="IO_11" pad="E18"/>
<connect gate="E" pin="IO_12" pad="E24"/>
<connect gate="E" pin="IO_13" pad="E19"/>
<connect gate="E" pin="IO_14" pad="E25"/>
<connect gate="E" pin="IO_15" pad="E20"/>
<connect gate="E" pin="IO_16" pad="E26"/>
<connect gate="E" pin="IO_17" pad="E27"/>
<connect gate="E" pin="IO_18" pad="E22"/>
<connect gate="E" pin="IO_19" pad="E28"/>
<connect gate="E" pin="IO_2" pad="D28"/>
<connect gate="E" pin="IO_20" pad="E29"/>
<connect gate="E" pin="IO_21" pad="E30"/>
<connect gate="E" pin="IO_22" pad="E31"/>
<connect gate="E" pin="IO_23" pad="E32"/>
<connect gate="E" pin="IO_24" pad="F10"/>
<connect gate="E" pin="IO_25" pad="F11"/>
<connect gate="E" pin="IO_26" pad="F12"/>
<connect gate="E" pin="IO_27" pad="F13"/>
<connect gate="E" pin="IO_28" pad="F14"/>
<connect gate="E" pin="IO_29" pad="F15"/>
<connect gate="E" pin="IO_3" pad="E13"/>
<connect gate="E" pin="IO_30" pad="F16"/>
<connect gate="E" pin="IO_31" pad="F17"/>
<connect gate="E" pin="IO_32" pad="F18"/>
<connect gate="E" pin="IO_33" pad="F19"/>
<connect gate="E" pin="IO_34" pad="F20"/>
<connect gate="E" pin="IO_35" pad="F22"/>
<connect gate="E" pin="IO_36" pad="F23"/>
<connect gate="E" pin="IO_37" pad="F24"/>
<connect gate="E" pin="IO_38" pad="F29"/>
<connect gate="E" pin="IO_39" pad="F30"/>
<connect gate="E" pin="IO_4" pad="D31"/>
<connect gate="E" pin="IO_40" pad="F31"/>
<connect gate="E" pin="IO_41" pad="F32"/>
<connect gate="E" pin="IO_42" pad="G10"/>
<connect gate="E" pin="IO_43" pad="G11"/>
<connect gate="E" pin="IO_44" pad="G12"/>
<connect gate="E" pin="IO_45" pad="G13"/>
<connect gate="E" pin="IO_46" pad="G19"/>
<connect gate="E" pin="IO_47" pad="G20"/>
<connect gate="E" pin="IO_48" pad="G21"/>
<connect gate="E" pin="IO_49" pad="G22"/>
<connect gate="E" pin="IO_5" pad="E14"/>
<connect gate="E" pin="IO_50" pad="G23"/>
<connect gate="E" pin="IO_51" pad="G24"/>
<connect gate="E" pin="IO_52" pad="G25"/>
<connect gate="E" pin="IO_53" pad="G29"/>
<connect gate="E" pin="IO_54" pad="G30"/>
<connect gate="E" pin="IO_55" pad="G31"/>
<connect gate="E" pin="IO_56" pad="G32"/>
<connect gate="E" pin="IO_57" pad="H11"/>
<connect gate="E" pin="IO_58" pad="H12"/>
<connect gate="E" pin="IO_59" pad="H13"/>
<connect gate="E" pin="IO_6" pad="D32"/>
<connect gate="E" pin="IO_60" pad="H14"/>
<connect gate="E" pin="IO_61" pad="H19"/>
<connect gate="E" pin="IO_62" pad="H20"/>
<connect gate="E" pin="IO_63" pad="H21"/>
<connect gate="E" pin="IO_64" pad="H22"/>
<connect gate="E" pin="IO_65" pad="H23"/>
<connect gate="E" pin="IO_66" pad="H24"/>
<connect gate="E" pin="IO_67" pad="H27"/>
<connect gate="E" pin="IO_7" pad="E15"/>
<connect gate="E" pin="IO_8" pad="E16"/>
<connect gate="E" pin="IO_9" pad="E11"/>
<connect gate="E" pin="MSEL3" pad="H10"/>
<connect gate="E" pin="NC" pad="G28"/>
<connect gate="E" pin="NC_2" pad="F21"/>
<connect gate="E" pin="NC_3" pad="F25"/>
<connect gate="E" pin="NC_4" pad="G14"/>
<connect gate="E" pin="NC_5" pad="G27"/>
<connect gate="E" pin="VCCA_PLL11" pad="H17"/>
<connect gate="E" pin="VCCA_PLL5" pad="G15"/>
<connect gate="E" pin="VCCA_PLL7" pad="H26"/>
<connect gate="E" pin="VCCD_PLL5" pad="H15"/>
<connect gate="E" pin="VCCD_PLL7" pad="H25"/>
<connect gate="E" pin="VCCIO3" pad="E21"/>
<connect gate="E" pin="VCCIO4" pad="E12"/>
<connect gate="E" pin="VREFB2N0" pad="F28"/>
<connect gate="F" pin="CONF_DONE" pad="J25"/>
<connect gate="F" pin="GND" pad="M19"/>
<connect gate="F" pin="GND_2" pad="J24"/>
<connect gate="F" pin="GND_3" pad="K28"/>
<connect gate="F" pin="GND_4" pad="M14"/>
<connect gate="F" pin="GND_5" pad="L11"/>
<connect gate="F" pin="GND_6" pad="M12"/>
<connect gate="F" pin="IO" pad="M29"/>
<connect gate="F" pin="IO_10" pad="J19"/>
<connect gate="F" pin="IO_11" pad="J15"/>
<connect gate="F" pin="IO_12" pad="J26"/>
<connect gate="F" pin="IO_13" pad="J20"/>
<connect gate="F" pin="IO_14" pad="J27"/>
<connect gate="F" pin="IO_15" pad="J21"/>
<connect gate="F" pin="IO_16" pad="K11"/>
<connect gate="F" pin="IO_17" pad="J22"/>
<connect gate="F" pin="IO_18" pad="K12"/>
<connect gate="F" pin="IO_19" pad="J23"/>
<connect gate="F" pin="IO_2" pad="H29"/>
<connect gate="F" pin="IO_20" pad="K13"/>
<connect gate="F" pin="IO_21" pad="J31"/>
<connect gate="F" pin="IO_22" pad="K14"/>
<connect gate="F" pin="IO_23" pad="J32"/>
<connect gate="F" pin="IO_24" pad="K15"/>
<connect gate="F" pin="IO_25" pad="K16"/>
<connect gate="F" pin="IO_26" pad="K17"/>
<connect gate="F" pin="IO_27" pad="K18"/>
<connect gate="F" pin="IO_28" pad="K19"/>
<connect gate="F" pin="IO_29" pad="K20"/>
<connect gate="F" pin="IO_3" pad="H30"/>
<connect gate="F" pin="IO_30" pad="K24"/>
<connect gate="F" pin="IO_31" pad="K21"/>
<connect gate="F" pin="IO_32" pad="K25"/>
<connect gate="F" pin="IO_33" pad="K22"/>
<connect gate="F" pin="IO_34" pad="K26"/>
<connect gate="F" pin="IO_35" pad="K27"/>
<connect gate="F" pin="IO_36" pad="K29"/>
<connect gate="F" pin="IO_37" pad="K30"/>
<connect gate="F" pin="IO_38" pad="K31"/>
<connect gate="F" pin="IO_39" pad="K32"/>
<connect gate="F" pin="IO_4" pad="J11"/>
<connect gate="F" pin="IO_40" pad="L10"/>
<connect gate="F" pin="IO_41" pad="L12"/>
<connect gate="F" pin="IO_42" pad="L13"/>
<connect gate="F" pin="IO_43" pad="L14"/>
<connect gate="F" pin="IO_44" pad="L15"/>
<connect gate="F" pin="IO_45" pad="L16"/>
<connect gate="F" pin="IO_46" pad="L17"/>
<connect gate="F" pin="IO_47" pad="L18"/>
<connect gate="F" pin="IO_48" pad="L19"/>
<connect gate="F" pin="IO_49" pad="L20"/>
<connect gate="F" pin="IO_5" pad="H31"/>
<connect gate="F" pin="IO_50" pad="L21"/>
<connect gate="F" pin="IO_51" pad="L22"/>
<connect gate="F" pin="IO_52" pad="L23"/>
<connect gate="F" pin="IO_53" pad="L24"/>
<connect gate="F" pin="IO_54" pad="L25"/>
<connect gate="F" pin="IO_55" pad="L26"/>
<connect gate="F" pin="IO_56" pad="L29"/>
<connect gate="F" pin="IO_57" pad="L30"/>
<connect gate="F" pin="IO_58" pad="L31"/>
<connect gate="F" pin="IO_59" pad="L32"/>
<connect gate="F" pin="IO_6" pad="J12"/>
<connect gate="F" pin="IO_60" pad="M10"/>
<connect gate="F" pin="IO_61" pad="M11"/>
<connect gate="F" pin="IO_62" pad="M22"/>
<connect gate="F" pin="IO_63" pad="M23"/>
<connect gate="F" pin="IO_64" pad="M24"/>
<connect gate="F" pin="IO_65" pad="M25"/>
<connect gate="F" pin="IO_66" pad="M26"/>
<connect gate="F" pin="IO_67" pad="M27"/>
<connect gate="F" pin="IO_7" pad="H32"/>
<connect gate="F" pin="IO_8" pad="J13"/>
<connect gate="F" pin="IO_9" pad="J14"/>
<connect gate="F" pin="MSEL2" pad="J10"/>
<connect gate="F" pin="NC" pad="J30"/>
<connect gate="F" pin="NC_2" pad="L27"/>
<connect gate="F" pin="NC_3" pad="J29"/>
<connect gate="F" pin="NC_4" pad="L28"/>
<connect gate="F" pin="VCCD_PLL11" pad="J18"/>
<connect gate="F" pin="VCCINT" pad="K23"/>
<connect gate="F" pin="VCCINT_2" pad="M21"/>
<connect gate="F" pin="VCCINT_3" pad="K10"/>
<connect gate="F" pin="VCCIO2" pad="M28"/>
<connect gate="F" pin="VCCIO3" pad="M17"/>
<connect gate="F" pin="VCCIO4" pad="M16"/>
<connect gate="F" pin="VCCPD3" pad="M20"/>
<connect gate="F" pin="VCCPD3_2" pad="M18"/>
<connect gate="F" pin="VCCPD4" pad="M13"/>
<connect gate="F" pin="VCCPD4_2" pad="M15"/>
<connect gate="F" pin="VCC_PLL11_OUT" pad="J17"/>
<connect gate="F" pin="VCC_PLL5_OUT" pad="J16"/>
<connect gate="F" pin="VREFB2N1" pad="J28"/>
<connect gate="G" pin="CLK1N" pad="T29"/>
<connect gate="G" pin="CLK1P" pad="T30"/>
<connect gate="G" pin="GND" pad="N20"/>
<connect gate="G" pin="GNDA_PLL1" pad="T26"/>
<connect gate="G" pin="GNDA_PLL1_2" pad="T25"/>
<connect gate="G" pin="GND_10" pad="R14"/>
<connect gate="G" pin="GND_11" pad="P13"/>
<connect gate="G" pin="GND_12" pad="T19"/>
<connect gate="G" pin="GND_13" pad="P21"/>
<connect gate="G" pin="GND_14" pad="T13"/>
<connect gate="G" pin="GND_15" pad="P15"/>
<connect gate="G" pin="GND_16" pad="T17"/>
<connect gate="G" pin="GND_17" pad="P17"/>
<connect gate="G" pin="GND_18" pad="R16"/>
<connect gate="G" pin="GND_19" pad="P19"/>
<connect gate="G" pin="GND_2" pad="N16"/>
<connect gate="G" pin="GND_3" pad="N14"/>
<connect gate="G" pin="GND_4" pad="R20"/>
<connect gate="G" pin="GND_5" pad="N18"/>
<connect gate="G" pin="GND_6" pad="R18"/>
<connect gate="G" pin="GND_7" pad="P12"/>
<connect gate="G" pin="GND_8" pad="T15"/>
<connect gate="G" pin="GND_9" pad="N32"/>
<connect gate="G" pin="IO" pad="T28"/>
<connect gate="G" pin="IO_10" pad="N28"/>
<connect gate="G" pin="IO_11" pad="M32"/>
<connect gate="G" pin="IO_12" pad="P24"/>
<connect gate="G" pin="IO_13" pad="N29"/>
<connect gate="G" pin="IO_14" pad="P25"/>
<connect gate="G" pin="IO_15" pad="N30"/>
<connect gate="G" pin="IO_16" pad="P26"/>
<connect gate="G" pin="IO_17" pad="N31"/>
<connect gate="G" pin="IO_18" pad="P27"/>
<connect gate="G" pin="IO_19" pad="P28"/>
<connect gate="G" pin="IO_2" pad="N22"/>
<connect gate="G" pin="IO_20" pad="P10"/>
<connect gate="G" pin="IO_21" pad="P29"/>
<connect gate="G" pin="IO_22" pad="P11"/>
<connect gate="G" pin="IO_23" pad="P31"/>
<connect gate="G" pin="IO_24" pad="P32"/>
<connect gate="G" pin="IO_25" pad="R10"/>
<connect gate="G" pin="IO_26" pad="R11"/>
<connect gate="G" pin="IO_27" pad="R22"/>
<connect gate="G" pin="IO_28" pad="R23"/>
<connect gate="G" pin="IO_29" pad="R24"/>
<connect gate="G" pin="IO_3" pad="N23"/>
<connect gate="G" pin="IO_30" pad="R25"/>
<connect gate="G" pin="IO_31" pad="R26"/>
<connect gate="G" pin="IO_32" pad="R27"/>
<connect gate="G" pin="IO_33" pad="R28"/>
<connect gate="G" pin="IO_34" pad="R29"/>
<connect gate="G" pin="IO_35" pad="R30"/>
<connect gate="G" pin="IO_36" pad="R31"/>
<connect gate="G" pin="IO_37" pad="T10"/>
<connect gate="G" pin="IO_38" pad="T11"/>
<connect gate="G" pin="IO_39" pad="T22"/>
<connect gate="G" pin="IO_4" pad="N24"/>
<connect gate="G" pin="IO_40" pad="T23"/>
<connect gate="G" pin="IO_41" pad="T27"/>
<connect gate="G" pin="IO_5" pad="N25"/>
<connect gate="G" pin="IO_6" pad="N26"/>
<connect gate="G" pin="IO_7" pad="M30"/>
<connect gate="G" pin="IO_8" pad="N27"/>
<connect gate="G" pin="IO_9" pad="M31"/>
<connect gate="G" pin="NC" pad="P23"/>
<connect gate="G" pin="NC_2" pad="N10"/>
<connect gate="G" pin="NC_3" pad="P22"/>
<connect gate="G" pin="NC_4" pad="N11"/>
<connect gate="G" pin="VCCA_PLL1" pad="T24"/>
<connect gate="G" pin="VCCINT" pad="T20"/>
<connect gate="G" pin="VCCINT_10" pad="R15"/>
<connect gate="G" pin="VCCINT_11" pad="T14"/>
<connect gate="G" pin="VCCINT_12" pad="R13"/>
<connect gate="G" pin="VCCINT_13" pad="R17"/>
<connect gate="G" pin="VCCINT_14" pad="T16"/>
<connect gate="G" pin="VCCINT_15" pad="R19"/>
<connect gate="G" pin="VCCINT_16" pad="T18"/>
<connect gate="G" pin="VCCINT_2" pad="N17"/>
<connect gate="G" pin="VCCINT_3" pad="N15"/>
<connect gate="G" pin="VCCINT_4" pad="N19"/>
<connect gate="G" pin="VCCINT_5" pad="N13"/>
<connect gate="G" pin="VCCINT_6" pad="P14"/>
<connect gate="G" pin="VCCINT_7" pad="P16"/>
<connect gate="G" pin="VCCINT_8" pad="P18"/>
<connect gate="G" pin="VCCINT_9" pad="P20"/>
<connect gate="G" pin="VCCIO2" pad="T21"/>
<connect gate="G" pin="VCCIO2_2" pad="R32"/>
<connect gate="G" pin="VCCIO5" pad="T12"/>
<connect gate="G" pin="VCCPD2" pad="R21"/>
<connect gate="G" pin="VCCPD2_2" pad="N21"/>
<connect gate="G" pin="VCCPD5" pad="R12"/>
<connect gate="G" pin="VCCPD5_2" pad="N12"/>
<connect gate="G" pin="VREFB2N2" pad="P30"/>
<connect gate="H" pin="CLK3N" pad="U29"/>
<connect gate="H" pin="CLK3P" pad="U30"/>
<connect gate="H" pin="GND" pad="Y19"/>
<connect gate="H" pin="GNDA_PLL2" pad="U26"/>
<connect gate="H" pin="GNDA_PLL2_2" pad="U25"/>
<connect gate="H" pin="GND_10" pad="U20"/>
<connect gate="H" pin="GND_11" pad="W16"/>
<connect gate="H" pin="GND_12" pad="V13"/>
<connect gate="H" pin="GND_13" pad="W20"/>
<connect gate="H" pin="GND_14" pad="Y13"/>
<connect gate="H" pin="GND_15" pad="W18"/>
<connect gate="H" pin="GND_16" pad="V27"/>
<connect gate="H" pin="GND_17" pad="W12"/>
<connect gate="H" pin="GND_18" pad="Y17"/>
<connect gate="H" pin="GND_19" pad="Y15"/>
<connect gate="H" pin="GND_2" pad="U18"/>
<connect gate="H" pin="GND_20" pad="V19"/>
<connect gate="H" pin="GND_3" pad="V11"/>
<connect gate="H" pin="GND_4" pad="V17"/>
<connect gate="H" pin="GND_5" pad="V22"/>
<connect gate="H" pin="GND_6" pad="U16"/>
<connect gate="H" pin="GND_7" pad="V15"/>
<connect gate="H" pin="GND_8" pad="U14"/>
<connect gate="H" pin="GND_9" pad="W14"/>
<connect gate="H" pin="IO" pad="Y31"/>
<connect gate="H" pin="IO_10" pad="U10"/>
<connect gate="H" pin="IO_11" pad="U23"/>
<connect gate="H" pin="IO_12" pad="U31"/>
<connect gate="H" pin="IO_13" pad="V29"/>
<connect gate="H" pin="IO_14" pad="U11"/>
<connect gate="H" pin="IO_15" pad="U32"/>
<connect gate="H" pin="IO_16" pad="V10"/>
<connect gate="H" pin="IO_17" pad="V30"/>
<connect gate="H" pin="IO_18" pad="V31"/>
<connect gate="H" pin="IO_19" pad="W24"/>
<connect gate="H" pin="IO_2" pad="V23"/>
<connect gate="H" pin="IO_20" pad="W25"/>
<connect gate="H" pin="IO_21" pad="W26"/>
<connect gate="H" pin="IO_22" pad="W27"/>
<connect gate="H" pin="IO_23" pad="W28"/>
<connect gate="H" pin="IO_24" pad="W29"/>
<connect gate="H" pin="IO_25" pad="W31"/>
<connect gate="H" pin="IO_26" pad="W32"/>
<connect gate="H" pin="IO_27" pad="Y10"/>
<connect gate="H" pin="IO_28" pad="Y11"/>
<connect gate="H" pin="IO_29" pad="Y22"/>
<connect gate="H" pin="IO_3" pad="T31"/>
<connect gate="H" pin="IO_30" pad="Y23"/>
<connect gate="H" pin="IO_31" pad="Y24"/>
<connect gate="H" pin="IO_32" pad="Y25"/>
<connect gate="H" pin="IO_33" pad="Y26"/>
<connect gate="H" pin="IO_34" pad="Y27"/>
<connect gate="H" pin="IO_35" pad="Y28"/>
<connect gate="H" pin="IO_36" pad="Y29"/>
<connect gate="H" pin="IO_37" pad="Y30"/>
<connect gate="H" pin="IO_4" pad="U27"/>
<connect gate="H" pin="IO_5" pad="V24"/>
<connect gate="H" pin="IO_6" pad="T32"/>
<connect gate="H" pin="IO_7" pad="U28"/>
<connect gate="H" pin="IO_8" pad="U22"/>
<connect gate="H" pin="IO_9" pad="V28"/>
<connect gate="H" pin="NC" pad="W11"/>
<connect gate="H" pin="NC_2" pad="W22"/>
<connect gate="H" pin="NC_3" pad="W23"/>
<connect gate="H" pin="NC_4" pad="W10"/>
<connect gate="H" pin="VCCA_PLL2" pad="V26"/>
<connect gate="H" pin="VCCD_PLL1" pad="U24"/>
<connect gate="H" pin="VCCD_PLL2" pad="V25"/>
<connect gate="H" pin="VCCINT" pad="U13"/>
<connect gate="H" pin="VCCINT_10" pad="W13"/>
<connect gate="H" pin="VCCINT_11" pad="Y20"/>
<connect gate="H" pin="VCCINT_12" pad="W15"/>
<connect gate="H" pin="VCCINT_13" pad="W19"/>
<connect gate="H" pin="VCCINT_14" pad="V20"/>
<connect gate="H" pin="VCCINT_15" pad="Y14"/>
<connect gate="H" pin="VCCINT_16" pad="U15"/>
<connect gate="H" pin="VCCINT_17" pad="W17"/>
<connect gate="H" pin="VCCINT_2" pad="U19"/>
<connect gate="H" pin="VCCINT_3" pad="V14"/>
<connect gate="H" pin="VCCINT_4" pad="U17"/>
<connect gate="H" pin="VCCINT_5" pad="V18"/>
<connect gate="H" pin="VCCINT_6" pad="W21"/>
<connect gate="H" pin="VCCINT_7" pad="Y16"/>
<connect gate="H" pin="VCCINT_8" pad="V16"/>
<connect gate="H" pin="VCCINT_9" pad="Y18"/>
<connect gate="H" pin="VCCIO1" pad="U21"/>
<connect gate="H" pin="VCCIO1_2" pad="V32"/>
<connect gate="H" pin="VCCIO6" pad="U12"/>
<connect gate="H" pin="VCCPD1" pad="Y21"/>
<connect gate="H" pin="VCCPD1_2" pad="V21"/>
<connect gate="H" pin="VCCPD6" pad="V12"/>
<connect gate="H" pin="VCCPD6_2" pad="Y12"/>
<connect gate="H" pin="VREFB1N0" pad="W30"/>
<connect gate="I" pin="GND" pad="AC28"/>
<connect gate="I" pin="GNDA_PLL12" pad="AD17"/>
<connect gate="I" pin="GNDA_PLL6" pad="AD16"/>
<connect gate="I" pin="GND_2" pad="AA14"/>
<connect gate="I" pin="GND_3" pad="AA21"/>
<connect gate="I" pin="GND_4" pad="Y32"/>
<connect gate="I" pin="GND_5" pad="AB22"/>
<connect gate="I" pin="GND_6" pad="AA19"/>
<connect gate="I" pin="IO" pad="AD32"/>
<connect gate="I" pin="IO_10" pad="AA29"/>
<connect gate="I" pin="IO_11" pad="AA30"/>
<connect gate="I" pin="IO_12" pad="AA31"/>
<connect gate="I" pin="IO_13" pad="AA32"/>
<connect gate="I" pin="IO_14" pad="AB10"/>
<connect gate="I" pin="IO_15" pad="AB11"/>
<connect gate="I" pin="IO_16" pad="AB12"/>
<connect gate="I" pin="IO_17" pad="AB13"/>
<connect gate="I" pin="IO_18" pad="AB14"/>
<connect gate="I" pin="IO_19" pad="AB15"/>
<connect gate="I" pin="IO_2" pad="AA22"/>
<connect gate="I" pin="IO_20" pad="AB16"/>
<connect gate="I" pin="IO_21" pad="AB17"/>
<connect gate="I" pin="IO_22" pad="AB18"/>
<connect gate="I" pin="IO_23" pad="AB19"/>
<connect gate="I" pin="IO_24" pad="AB20"/>
<connect gate="I" pin="IO_25" pad="AB23"/>
<connect gate="I" pin="IO_26" pad="AB21"/>
<connect gate="I" pin="IO_27" pad="AB24"/>
<connect gate="I" pin="IO_28" pad="AB25"/>
<connect gate="I" pin="IO_29" pad="AB26"/>
<connect gate="I" pin="IO_3" pad="AA23"/>
<connect gate="I" pin="IO_30" pad="AB27"/>
<connect gate="I" pin="IO_31" pad="AB28"/>
<connect gate="I" pin="IO_32" pad="AB29"/>
<connect gate="I" pin="IO_33" pad="AB30"/>
<connect gate="I" pin="IO_34" pad="AB31"/>
<connect gate="I" pin="IO_35" pad="AB32"/>
<connect gate="I" pin="IO_36" pad="AC11"/>
<connect gate="I" pin="IO_37" pad="AC12"/>
<connect gate="I" pin="IO_38" pad="AC13"/>
<connect gate="I" pin="IO_39" pad="AC14"/>
<connect gate="I" pin="IO_4" pad="AA24"/>
<connect gate="I" pin="IO_40" pad="AC15"/>
<connect gate="I" pin="IO_41" pad="AC16"/>
<connect gate="I" pin="IO_42" pad="AC17"/>
<connect gate="I" pin="IO_43" pad="AC18"/>
<connect gate="I" pin="IO_44" pad="AC19"/>
<connect gate="I" pin="IO_45" pad="AC20"/>
<connect gate="I" pin="IO_46" pad="AC21"/>
<connect gate="I" pin="IO_47" pad="AC22"/>
<connect gate="I" pin="IO_48" pad="AC24"/>
<connect gate="I" pin="IO_49" pad="AC25"/>
<connect gate="I" pin="IO_5" pad="AA25"/>
<connect gate="I" pin="IO_50" pad="AC26"/>
<connect gate="I" pin="IO_51" pad="AC27"/>
<connect gate="I" pin="IO_52" pad="AC31"/>
<connect gate="I" pin="IO_53" pad="AC32"/>
<connect gate="I" pin="IO_54" pad="AD10"/>
<connect gate="I" pin="IO_55" pad="AD11"/>
<connect gate="I" pin="IO_56" pad="AD12"/>
<connect gate="I" pin="IO_57" pad="AD13"/>
<connect gate="I" pin="IO_58" pad="AD14"/>
<connect gate="I" pin="IO_59" pad="AD18"/>
<connect gate="I" pin="IO_6" pad="AA26"/>
<connect gate="I" pin="IO_60" pad="AD19"/>
<connect gate="I" pin="IO_61" pad="AD20"/>
<connect gate="I" pin="IO_62" pad="AD21"/>
<connect gate="I" pin="IO_63" pad="AD22"/>
<connect gate="I" pin="IO_64" pad="AD23"/>
<connect gate="I" pin="IO_65" pad="AD24"/>
<connect gate="I" pin="IO_66" pad="AD25"/>
<connect gate="I" pin="IO_67" pad="AD26"/>
<connect gate="I" pin="IO_68" pad="AD27"/>
<connect gate="I" pin="IO_69" pad="AD31"/>
<connect gate="I" pin="IO_7" pad="AA27"/>
<connect gate="I" pin="IO_8" pad="AA10"/>
<connect gate="I" pin="IO_9" pad="AA11"/>
<connect gate="I" pin="NC" pad="AD30"/>
<connect gate="I" pin="NC_2" pad="AC29"/>
<connect gate="I" pin="NC_3" pad="AC30"/>
<connect gate="I" pin="NC_4" pad="AD29"/>
<connect gate="I" pin="VCCD_PLL6" pad="AD15"/>
<connect gate="I" pin="VCCINT" pad="AA12"/>
<connect gate="I" pin="VCCINT_2" pad="AC10"/>
<connect gate="I" pin="VCCIO1" pad="AA28"/>
<connect gate="I" pin="VCCIO7" pad="AA16"/>
<connect gate="I" pin="VCCIO8" pad="AA17"/>
<connect gate="I" pin="VCCPD7" pad="AA13"/>
<connect gate="I" pin="VCCPD7_2" pad="AA15"/>
<connect gate="I" pin="VCCPD8" pad="AA18"/>
<connect gate="I" pin="VCCPD8_2" pad="AA20"/>
<connect gate="I" pin="VCCSEL" pad="AC23"/>
<connect gate="I" pin="VREFB1N1" pad="AD28"/>
<connect gate="J" pin="GND" pad="AH27"/>
<connect gate="J" pin="GNDA_PLL12" pad="AE17"/>
<connect gate="J" pin="GNDA_PLL6" pad="AE16"/>
<connect gate="J" pin="GNDA_PLL8" pad="AG26"/>
<connect gate="J" pin="GNDA_PLL8_2" pad="AG27"/>
<connect gate="J" pin="GND_2" pad="AH10"/>
<connect gate="J" pin="GND_3" pad="AF17"/>
<connect gate="J" pin="GND_4" pad="AH23"/>
<connect gate="J" pin="IO" pad="AJ10"/>
<connect gate="J" pin="IO_10" pad="AE25"/>
<connect gate="J" pin="IO_11" pad="AE13"/>
<connect gate="J" pin="IO_12" pad="AE26"/>
<connect gate="J" pin="IO_13" pad="AE14"/>
<connect gate="J" pin="IO_14" pad="AE27"/>
<connect gate="J" pin="IO_15" pad="AE28"/>
<connect gate="J" pin="IO_16" pad="AE29"/>
<connect gate="J" pin="IO_17" pad="AE30"/>
<connect gate="J" pin="IO_18" pad="AE31"/>
<connect gate="J" pin="IO_19" pad="AF19"/>
<connect gate="J" pin="IO_2" pad="AE19"/>
<connect gate="J" pin="IO_20" pad="AE32"/>
<connect gate="J" pin="IO_21" pad="AF20"/>
<connect gate="J" pin="IO_22" pad="AF10"/>
<connect gate="J" pin="IO_23" pad="AF21"/>
<connect gate="J" pin="IO_24" pad="AF11"/>
<connect gate="J" pin="IO_25" pad="AF22"/>
<connect gate="J" pin="IO_26" pad="AF12"/>
<connect gate="J" pin="IO_27" pad="AF23"/>
<connect gate="J" pin="IO_28" pad="AF13"/>
<connect gate="J" pin="IO_29" pad="AF29"/>
<connect gate="J" pin="IO_3" pad="AE20"/>
<connect gate="J" pin="IO_30" pad="AF30"/>
<connect gate="J" pin="IO_31" pad="AF31"/>
<connect gate="J" pin="IO_32" pad="AF32"/>
<connect gate="J" pin="IO_33" pad="AG10"/>
<connect gate="J" pin="IO_34" pad="AG11"/>
<connect gate="J" pin="IO_35" pad="AG12"/>
<connect gate="J" pin="IO_36" pad="AG13"/>
<connect gate="J" pin="IO_37" pad="AG14"/>
<connect gate="J" pin="IO_38" pad="AG15"/>
<connect gate="J" pin="IO_39" pad="AG16"/>
<connect gate="J" pin="IO_4" pad="AE21"/>
<connect gate="J" pin="IO_40" pad="AG17"/>
<connect gate="J" pin="IO_41" pad="AG18"/>
<connect gate="J" pin="IO_42" pad="AG19"/>
<connect gate="J" pin="IO_43" pad="AG20"/>
<connect gate="J" pin="IO_44" pad="AG22"/>
<connect gate="J" pin="IO_45" pad="AG23"/>
<connect gate="J" pin="IO_46" pad="AG24"/>
<connect gate="J" pin="IO_47" pad="AG29"/>
<connect gate="J" pin="IO_48" pad="AG30"/>
<connect gate="J" pin="IO_49" pad="AG31"/>
<connect gate="J" pin="IO_5" pad="AE22"/>
<connect gate="J" pin="IO_50" pad="AG32"/>
<connect gate="J" pin="IO_51" pad="AH11"/>
<connect gate="J" pin="IO_52" pad="AH13"/>
<connect gate="J" pin="IO_53" pad="AH14"/>
<connect gate="J" pin="IO_54" pad="AH15"/>
<connect gate="J" pin="IO_55" pad="AH16"/>
<connect gate="J" pin="IO_56" pad="AH17"/>
<connect gate="J" pin="IO_57" pad="AH18"/>
<connect gate="J" pin="IO_58" pad="AH19"/>
<connect gate="J" pin="IO_59" pad="AH20"/>
<connect gate="J" pin="IO_6" pad="AE10"/>
<connect gate="J" pin="IO_60" pad="AH22"/>
<connect gate="J" pin="IO_61" pad="AH24"/>
<connect gate="J" pin="IO_62" pad="AH25"/>
<connect gate="J" pin="IO_63" pad="AH26"/>
<connect gate="J" pin="IO_64" pad="AH28"/>
<connect gate="J" pin="IO_65" pad="AH29"/>
<connect gate="J" pin="IO_66" pad="AH30"/>
<connect gate="J" pin="IO_67" pad="AH31"/>
<connect gate="J" pin="IO_68" pad="AH32"/>
<connect gate="J" pin="IO_7" pad="AE23"/>
<connect gate="J" pin="IO_8" pad="AE11"/>
<connect gate="J" pin="IO_9" pad="AE12"/>
<connect gate="J" pin="NC" pad="AF28"/>
<connect gate="J" pin="NC_2" pad="AG21"/>
<connect gate="J" pin="NC_3" pad="AG25"/>
<connect gate="J" pin="NC_4" pad="AF27"/>
<connect gate="J" pin="NC_5" pad="AF14"/>
<connect gate="J" pin="TCK" pad="AF24"/>
<connect gate="J" pin="TMS" pad="AE24"/>
<connect gate="J" pin="VCCA_PLL12" pad="AF18"/>
<connect gate="J" pin="VCCA_PLL6" pad="AE15"/>
<connect gate="J" pin="VCCA_PLL8" pad="AF26"/>
<connect gate="J" pin="VCCD_PLL12" pad="AE18"/>
<connect gate="J" pin="VCCD_PLL8" pad="AF25"/>
<connect gate="J" pin="VCCIO7" pad="AH12"/>
<connect gate="J" pin="VCCIO8" pad="AH21"/>
<connect gate="J" pin="VCC_PLL12_OUT" pad="AF16"/>
<connect gate="J" pin="VCC_PLL6_OUT" pad="AF15"/>
<connect gate="J" pin="VREFB1N2" pad="AG28"/>
<connect gate="K" pin="FPLL8CLKN" pad="AJ29"/>
<connect gate="K" pin="FPLL8CLKP" pad="AJ30"/>
<connect gate="K" pin="GND" pad="AM31"/>
<connect gate="K" pin="GND_2" pad="AM20"/>
<connect gate="K" pin="GND_3" pad="AL32"/>
<connect gate="K" pin="GND_4" pad="AM13"/>
<connect gate="K" pin="IO" pad="AM29"/>
<connect gate="K" pin="IO_10" pad="AK26"/>
<connect gate="K" pin="IO_11" pad="AJ12"/>
<connect gate="K" pin="IO_12" pad="AK27"/>
<connect gate="K" pin="IO_13" pad="AJ13"/>
<connect gate="K" pin="IO_14" pad="AK28"/>
<connect gate="K" pin="IO_15" pad="AJ14"/>
<connect gate="K" pin="IO_16" pad="AK29"/>
<connect gate="K" pin="IO_17" pad="AJ25"/>
<connect gate="K" pin="IO_18" pad="AJ15"/>
<connect gate="K" pin="IO_19" pad="AJ26"/>
<connect gate="K" pin="IO_2" pad="AK20"/>
<connect gate="K" pin="IO_20" pad="AJ16"/>
<connect gate="K" pin="IO_21" pad="AJ22"/>
<connect gate="K" pin="IO_22" pad="AJ27"/>
<connect gate="K" pin="IO_23" pad="AJ17"/>
<connect gate="K" pin="IO_24" pad="AK10"/>
<connect gate="K" pin="IO_25" pad="AJ23"/>
<connect gate="K" pin="IO_26" pad="AJ28"/>
<connect gate="K" pin="IO_27" pad="AJ18"/>
<connect gate="K" pin="IO_28" pad="AK11"/>
<connect gate="K" pin="IO_29" pad="AJ19"/>
<connect gate="K" pin="IO_3" pad="AK21"/>
<connect gate="K" pin="IO_30" pad="AK12"/>
<connect gate="K" pin="IO_31" pad="AJ20"/>
<connect gate="K" pin="IO_32" pad="AK13"/>
<connect gate="K" pin="IO_33" pad="AJ31"/>
<connect gate="K" pin="IO_34" pad="AJ21"/>
<connect gate="K" pin="IO_35" pad="AK15"/>
<connect gate="K" pin="IO_36" pad="AJ32"/>
<connect gate="K" pin="IO_37" pad="AK16"/>
<connect gate="K" pin="IO_38" pad="AK17"/>
<connect gate="K" pin="IO_39" pad="AK18"/>
<connect gate="K" pin="IO_4" pad="AK22"/>
<connect gate="K" pin="IO_40" pad="AL11"/>
<connect gate="K" pin="IO_41" pad="AL12"/>
<connect gate="K" pin="IO_42" pad="AL13"/>
<connect gate="K" pin="IO_43" pad="AL14"/>
<connect gate="K" pin="IO_44" pad="AL15"/>
<connect gate="K" pin="IO_45" pad="AL16"/>
<connect gate="K" pin="IO_46" pad="AL17"/>
<connect gate="K" pin="IO_47" pad="AL18"/>
<connect gate="K" pin="IO_48" pad="AL19"/>
<connect gate="K" pin="IO_49" pad="AL20"/>
<connect gate="K" pin="IO_5" pad="AK23"/>
<connect gate="K" pin="IO_50" pad="AL21"/>
<connect gate="K" pin="IO_51" pad="AL22"/>
<connect gate="K" pin="IO_52" pad="AL23"/>
<connect gate="K" pin="IO_53" pad="AL24"/>
<connect gate="K" pin="IO_54" pad="AL25"/>
<connect gate="K" pin="IO_55" pad="AL26"/>
<connect gate="K" pin="IO_56" pad="AL27"/>
<connect gate="K" pin="IO_57" pad="AL28"/>
<connect gate="K" pin="IO_58" pad="AL29"/>
<connect gate="K" pin="IO_59" pad="AM10"/>
<connect gate="K" pin="IO_6" pad="AK24"/>
<connect gate="K" pin="IO_60" pad="AM11"/>
<connect gate="K" pin="IO_61" pad="AM12"/>
<connect gate="K" pin="IO_62" pad="AM14"/>
<connect gate="K" pin="IO_63" pad="AM16"/>
<connect gate="K" pin="IO_64" pad="AM17"/>
<connect gate="K" pin="IO_65" pad="AM19"/>
<connect gate="K" pin="IO_66" pad="AM21"/>
<connect gate="K" pin="IO_67" pad="AM22"/>
<connect gate="K" pin="IO_68" pad="AM23"/>
<connect gate="K" pin="IO_69" pad="AM24"/>
<connect gate="K" pin="IO_7" pad="AK25"/>
<connect gate="K" pin="IO_70" pad="AM25"/>
<connect gate="K" pin="IO_71" pad="AM26"/>
<connect gate="K" pin="IO_72" pad="AM27"/>
<connect gate="K" pin="IO_73" pad="AM28"/>
<connect gate="K" pin="IO_8" pad="AL10"/>
<connect gate="K" pin="IO_9" pad="AJ11"/>
<connect gate="K" pin="NCONFIG" pad="AL30"/>
<connect gate="K" pin="TDI" pad="AL31"/>
<connect gate="K" pin="TRST" pad="AK30"/>
<connect gate="K" pin="VCCIO1" pad="AK32"/>
<connect gate="K" pin="VCCIO7" pad="AM15"/>
<connect gate="K" pin="VCCIO8" pad="AM30"/>
<connect gate="K" pin="VCCIO8_2" pad="AM18"/>
<connect gate="K" pin="VREFB7N0" pad="AK14"/>
<connect gate="K" pin="VREFB8N0" pad="AK31"/>
<connect gate="K" pin="VREFB8N1" pad="AJ24"/>
<connect gate="K" pin="VREFB8N2" pad="AK19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S60F1020C3N"/>
<attribute name="OC_FARNELL" value="1637237"/>
<attribute name="OC_NEWARK" value="51R0587"/>
<attribute name="PACKAGE" value="BGA-1020"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S60F1020C5N">
<description>FPGA, STRATIX II</description>
<gates>
<gate name="A" symbol="EP2S60F1020C5N_A"/>
<gate name="B" symbol="EP2S60F1020C5N_B"/>
<gate name="C" symbol="EP2S60F1020C5N_C"/>
<gate name="D" symbol="EP2S60F1020C5N_D"/>
<gate name="E" symbol="EP2S60F1020C5N_E"/>
<gate name="F" symbol="EP2S60F1020C5N_F"/>
<gate name="G" symbol="EP2S60F1020C5N_G"/>
<gate name="H" symbol="EP2S60F1020C5N_H"/>
<gate name="I" symbol="EP2S60F1020C5N_I"/>
<gate name="J" symbol="EP2S60F1020C5N_J"/>
<gate name="K" symbol="EP2S60F1020C5N_K"/>
</gates>
<devices>
<device name="" package="BGA1020C100P32X32_3300X3300X35">
<connects>
<connect gate="A" pin="FPLL10CLKN" pad="D4"/>
<connect gate="A" pin="FPLL10CLKP" pad="D3"/>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="GNDA_PLL10" pad="G8"/>
<connect gate="A" pin="GNDA_PLL10_2" pad="G7"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_3" pad="F7"/>
<connect gate="A" pin="GND_4" pad="K5"/>
<connect gate="A" pin="IO" pad="L4"/>
<connect gate="A" pin="IO_10" pad="A6"/>
<connect gate="A" pin="IO_11" pad="A7"/>
<connect gate="A" pin="IO_12" pad="A8"/>
<connect gate="A" pin="IO_13" pad="C4"/>
<connect gate="A" pin="IO_14" pad="A9"/>
<connect gate="A" pin="IO_15" pad="C5"/>
<connect gate="A" pin="IO_16" pad="C6"/>
<connect gate="A" pin="IO_17" pad="C7"/>
<connect gate="A" pin="IO_18" pad="D5"/>
<connect gate="A" pin="IO_19" pad="C8"/>
<connect gate="A" pin="IO_2" pad="B4"/>
<connect gate="A" pin="IO_20" pad="D6"/>
<connect gate="A" pin="IO_21" pad="C9"/>
<connect gate="A" pin="IO_22" pad="D7"/>
<connect gate="A" pin="IO_23" pad="D1"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D2"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="E2"/>
<connect gate="A" pin="IO_28" pad="E3"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="B5"/>
<connect gate="A" pin="IO_30" pad="E5"/>
<connect gate="A" pin="IO_31" pad="E6"/>
<connect gate="A" pin="IO_32" pad="E7"/>
<connect gate="A" pin="IO_33" pad="E8"/>
<connect gate="A" pin="IO_34" pad="E9"/>
<connect gate="A" pin="IO_35" pad="F1"/>
<connect gate="A" pin="IO_36" pad="F2"/>
<connect gate="A" pin="IO_37" pad="F3"/>
<connect gate="A" pin="IO_38" pad="F4"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="H1"/>
<connect gate="A" pin="IO_46" pad="H2"/>
<connect gate="A" pin="IO_47" pad="J1"/>
<connect gate="A" pin="IO_48" pad="J2"/>
<connect gate="A" pin="IO_49" pad="J3"/>
<connect gate="A" pin="IO_5" pad="B7"/>
<connect gate="A" pin="IO_50" pad="J4"/>
<connect gate="A" pin="IO_51" pad="J6"/>
<connect gate="A" pin="IO_52" pad="J7"/>
<connect gate="A" pin="IO_53" pad="J8"/>
<connect gate="A" pin="IO_54" pad="J9"/>
<connect gate="A" pin="IO_55" pad="K1"/>
<connect gate="A" pin="IO_56" pad="K2"/>
<connect gate="A" pin="IO_57" pad="K3"/>
<connect gate="A" pin="IO_58" pad="K4"/>
<connect gate="A" pin="IO_59" pad="K6"/>
<connect gate="A" pin="IO_6" pad="A4"/>
<connect gate="A" pin="IO_60" pad="K7"/>
<connect gate="A" pin="IO_61" pad="K8"/>
<connect gate="A" pin="IO_62" pad="K9"/>
<connect gate="A" pin="IO_63" pad="L1"/>
<connect gate="A" pin="IO_64" pad="L2"/>
<connect gate="A" pin="IO_65" pad="L3"/>
<connect gate="A" pin="IO_7" pad="B8"/>
<connect gate="A" pin="IO_8" pad="A5"/>
<connect gate="A" pin="IO_9" pad="B9"/>
<connect gate="A" pin="MSEL0" pad="B2"/>
<connect gate="A" pin="MSEL1" pad="F6"/>
<connect gate="A" pin="NC" pad="H6"/>
<connect gate="A" pin="NC_2" pad="G6"/>
<connect gate="A" pin="NC_3" pad="H3"/>
<connect gate="A" pin="NC_4" pad="H4"/>
<connect gate="A" pin="NC_5" pad="H5"/>
<connect gate="A" pin="NC_6" pad="H9"/>
<connect gate="A" pin="NC_7" pad="G5"/>
<connect gate="A" pin="TDO" pad="C3"/>
<connect gate="A" pin="TEMPDIODEN" pad="B3"/>
<connect gate="A" pin="TEMPDIODEP" pad="G9"/>
<connect gate="A" pin="VCCA_PLL10" pad="H8"/>
<connect gate="A" pin="VCCD_PLL10" pad="H7"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="C1"/>
<connect gate="A" pin="VREFB4N0" pad="C2"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N1" pad="J5"/>
<connect gate="A" pin="VREFB5N2" pad="F5"/>
<connect gate="B" pin="CLK11N" pad="T4"/>
<connect gate="B" pin="CLK11P" pad="T3"/>
<connect gate="B" pin="CLK9N" pad="U4"/>
<connect gate="B" pin="CLK9P" pad="U3"/>
<connect gate="B" pin="GND" pad="A13"/>
<connect gate="B" pin="GNDA_PLL3" pad="V8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="U8"/>
<connect gate="B" pin="GNDA_PLL4" pad="T8"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="R8"/>
<connect gate="B" pin="GND_2" pad="T7"/>
<connect gate="B" pin="GND_3" pad="N1"/>
<connect gate="B" pin="GND_4" pad="Y1"/>
<connect gate="B" pin="IO" pad="A16"/>
<connect gate="B" pin="IO_10" pad="M4"/>
<connect gate="B" pin="IO_11" pad="N4"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="M6"/>
<connect gate="B" pin="IO_14" pad="N6"/>
<connect gate="B" pin="IO_15" pad="M7"/>
<connect gate="B" pin="IO_16" pad="N7"/>
<connect gate="B" pin="IO_17" pad="M8"/>
<connect gate="B" pin="IO_18" pad="N8"/>
<connect gate="B" pin="IO_19" pad="M9"/>
<connect gate="B" pin="IO_2" pad="L5"/>
<connect gate="B" pin="IO_20" pad="N9"/>
<connect gate="B" pin="IO_21" pad="P1"/>
<connect gate="B" pin="IO_22" pad="N2"/>
<connect gate="B" pin="IO_23" pad="P2"/>
<connect gate="B" pin="IO_24" pad="N3"/>
<connect gate="B" pin="IO_25" pad="T1"/>
<connect gate="B" pin="IO_26" pad="P4"/>
<connect gate="B" pin="IO_27" pad="T2"/>
<connect gate="B" pin="IO_28" pad="P5"/>
<connect gate="B" pin="IO_29" pad="P6"/>
<connect gate="B" pin="IO_3" pad="L6"/>
<connect gate="B" pin="IO_30" pad="P7"/>
<connect gate="B" pin="IO_31" pad="P8"/>
<connect gate="B" pin="IO_32" pad="P9"/>
<connect gate="B" pin="IO_33" pad="T5"/>
<connect gate="B" pin="IO_34" pad="R2"/>
<connect gate="B" pin="IO_35" pad="R3"/>
<connect gate="B" pin="IO_36" pad="R4"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="L7"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="U1"/>
<connect gate="B" pin="IO_42" pad="U2"/>
<connect gate="B" pin="IO_43" pad="U5"/>
<connect gate="B" pin="IO_44" pad="U6"/>
<connect gate="B" pin="IO_45" pad="V2"/>
<connect gate="B" pin="IO_46" pad="V3"/>
<connect gate="B" pin="IO_47" pad="V4"/>
<connect gate="B" pin="IO_48" pad="V5"/>
<connect gate="B" pin="IO_49" pad="V6"/>
<connect gate="B" pin="IO_5" pad="L8"/>
<connect gate="B" pin="IO_50" pad="V7"/>
<connect gate="B" pin="IO_51" pad="V9"/>
<connect gate="B" pin="IO_52" pad="W1"/>
<connect gate="B" pin="IO_53" pad="W2"/>
<connect gate="B" pin="IO_54" pad="W4"/>
<connect gate="B" pin="IO_55" pad="W5"/>
<connect gate="B" pin="IO_56" pad="W6"/>
<connect gate="B" pin="IO_57" pad="W7"/>
<connect gate="B" pin="IO_58" pad="W8"/>
<connect gate="B" pin="IO_59" pad="W9"/>
<connect gate="B" pin="IO_6" pad="L9"/>
<connect gate="B" pin="IO_60" pad="Y2"/>
<connect gate="B" pin="IO_61" pad="Y3"/>
<connect gate="B" pin="IO_62" pad="Y4"/>
<connect gate="B" pin="IO_63" pad="Y5"/>
<connect gate="B" pin="IO_64" pad="Y6"/>
<connect gate="B" pin="IO_65" pad="Y7"/>
<connect gate="B" pin="IO_66" pad="Y8"/>
<connect gate="B" pin="IO_67" pad="Y9"/>
<connect gate="B" pin="IO_68" pad="A10"/>
<connect gate="B" pin="IO_69" pad="A11"/>
<connect gate="B" pin="IO_7" pad="M1"/>
<connect gate="B" pin="IO_70" pad="A12"/>
<connect gate="B" pin="IO_71" pad="A14"/>
<connect gate="B" pin="IO_8" pad="M2"/>
<connect gate="B" pin="IO_9" pad="M3"/>
<connect gate="B" pin="VCCA_PLL3" pad="U9"/>
<connect gate="B" pin="VCCA_PLL4" pad="R9"/>
<connect gate="B" pin="VCCD_PLL3" pad="U7"/>
<connect gate="B" pin="VCCD_PLL4" pad="T9"/>
<connect gate="B" pin="VCCIO4" pad="A15"/>
<connect gate="B" pin="VCCIO5" pad="R1"/>
<connect gate="B" pin="VCCIO5_2" pad="M5"/>
<connect gate="B" pin="VCCIO6" pad="V1"/>
<connect gate="B" pin="VREFB5N0" pad="P3"/>
<connect gate="B" pin="VREFB6N2" pad="W3"/>
<connect gate="C" pin="FPLL9CLKN" pad="AJ4"/>
<connect gate="C" pin="FPLL9CLKP" pad="AJ3"/>
<connect gate="C" pin="GND" pad="AC5"/>
<connect gate="C" pin="GNDA_PLL9" pad="AF7"/>
<connect gate="C" pin="GNDA_PLL9_2" pad="AG7"/>
<connect gate="C" pin="GND_2" pad="AF9"/>
<connect gate="C" pin="GND_3" pad="A20"/>
<connect gate="C" pin="GND_4" pad="A31"/>
<connect gate="C" pin="GND_5" pad="AG6"/>
<connect gate="C" pin="IO" pad="AJ6"/>
<connect gate="C" pin="IO_10" pad="AA6"/>
<connect gate="C" pin="IO_11" pad="A19"/>
<connect gate="C" pin="IO_12" pad="AA7"/>
<connect gate="C" pin="IO_13" pad="A24"/>
<connect gate="C" pin="IO_14" pad="AA8"/>
<connect gate="C" pin="IO_15" pad="A25"/>
<connect gate="C" pin="IO_16" pad="AA9"/>
<connect gate="C" pin="IO_17" pad="A26"/>
<connect gate="C" pin="IO_18" pad="AB1"/>
<connect gate="C" pin="IO_19" pad="A27"/>
<connect gate="C" pin="IO_2" pad="AA1"/>
<connect gate="C" pin="IO_20" pad="AB2"/>
<connect gate="C" pin="IO_21" pad="A28"/>
<connect gate="C" pin="IO_22" pad="AB3"/>
<connect gate="C" pin="IO_23" pad="A29"/>
<connect gate="C" pin="IO_24" pad="AB4"/>
<connect gate="C" pin="IO_25" pad="AB5"/>
<connect gate="C" pin="IO_26" pad="AB6"/>
<connect gate="C" pin="IO_27" pad="AB7"/>
<connect gate="C" pin="IO_28" pad="AB8"/>
<connect gate="C" pin="IO_29" pad="AB9"/>
<connect gate="C" pin="IO_3" pad="AA2"/>
<connect gate="C" pin="IO_30" pad="AC1"/>
<connect gate="C" pin="IO_31" pad="AC2"/>
<connect gate="C" pin="IO_32" pad="AC3"/>
<connect gate="C" pin="IO_33" pad="AC4"/>
<connect gate="C" pin="IO_34" pad="AC6"/>
<connect gate="C" pin="IO_35" pad="AC7"/>
<connect gate="C" pin="IO_36" pad="AC8"/>
<connect gate="C" pin="IO_37" pad="AC9"/>
<connect gate="C" pin="IO_38" pad="AD1"/>
<connect gate="C" pin="IO_39" pad="AD2"/>
<connect gate="C" pin="IO_4" pad="A21"/>
<connect gate="C" pin="IO_40" pad="AD6"/>
<connect gate="C" pin="IO_41" pad="AD7"/>
<connect gate="C" pin="IO_42" pad="AD8"/>
<connect gate="C" pin="IO_43" pad="AD9"/>
<connect gate="C" pin="IO_44" pad="AE1"/>
<connect gate="C" pin="IO_45" pad="AE2"/>
<connect gate="C" pin="IO_46" pad="AE3"/>
<connect gate="C" pin="IO_47" pad="AE4"/>
<connect gate="C" pin="IO_48" pad="AF1"/>
<connect gate="C" pin="IO_49" pad="AF2"/>
<connect gate="C" pin="IO_5" pad="AA3"/>
<connect gate="C" pin="IO_50" pad="AF3"/>
<connect gate="C" pin="IO_51" pad="AF4"/>
<connect gate="C" pin="IO_52" pad="AG1"/>
<connect gate="C" pin="IO_53" pad="AG2"/>
<connect gate="C" pin="IO_54" pad="AG3"/>
<connect gate="C" pin="IO_55" pad="AG4"/>
<connect gate="C" pin="IO_56" pad="AG8"/>
<connect gate="C" pin="IO_57" pad="AG9"/>
<connect gate="C" pin="IO_58" pad="AH1"/>
<connect gate="C" pin="IO_59" pad="AH2"/>
<connect gate="C" pin="IO_6" pad="A22"/>
<connect gate="C" pin="IO_60" pad="AH3"/>
<connect gate="C" pin="IO_61" pad="AH4"/>
<connect gate="C" pin="IO_62" pad="AH5"/>
<connect gate="C" pin="IO_63" pad="AH6"/>
<connect gate="C" pin="IO_64" pad="AH7"/>
<connect gate="C" pin="IO_65" pad="AH8"/>
<connect gate="C" pin="IO_66" pad="AH9"/>
<connect gate="C" pin="IO_67" pad="AJ1"/>
<connect gate="C" pin="IO_68" pad="AJ2"/>
<connect gate="C" pin="IO_69" pad="AJ5"/>
<connect gate="C" pin="IO_7" pad="AA4"/>
<connect gate="C" pin="IO_8" pad="A23"/>
<connect gate="C" pin="IO_9" pad="A17"/>
<connect gate="C" pin="NC" pad="AF6"/>
<connect gate="C" pin="NC_2" pad="AE9"/>
<connect gate="C" pin="NC_3" pad="AE5"/>
<connect gate="C" pin="NC_4" pad="AD3"/>
<connect gate="C" pin="NC_5" pad="AF5"/>
<connect gate="C" pin="NC_6" pad="AD4"/>
<connect gate="C" pin="NC_7" pad="AE6"/>
<connect gate="C" pin="PLL_ENA" pad="AF8"/>
<connect gate="C" pin="VCCA_PLL9" pad="AE7"/>
<connect gate="C" pin="VCCD_PLL9" pad="AE8"/>
<connect gate="C" pin="VCCIO3" pad="A30"/>
<connect gate="C" pin="VCCIO3_2" pad="A18"/>
<connect gate="C" pin="VCCIO6" pad="AA5"/>
<connect gate="C" pin="VREFB6N0" pad="AG5"/>
<connect gate="C" pin="VREFB6N1" pad="AD5"/>
<connect gate="D" pin="DCLK" pad="B31"/>
<connect gate="D" pin="GND" pad="AM2"/>
<connect gate="D" pin="GND_2" pad="AL1"/>
<connect gate="D" pin="GND_3" pad="B32"/>
<connect gate="D" pin="IO" pad="D27"/>
<connect gate="D" pin="IO_10" pad="AL8"/>
<connect gate="D" pin="IO_11" pad="AK8"/>
<connect gate="D" pin="IO_12" pad="AL9"/>
<connect gate="D" pin="IO_13" pad="AJ7"/>
<connect gate="D" pin="IO_14" pad="AK9"/>
<connect gate="D" pin="IO_15" pad="AM4"/>
<connect gate="D" pin="IO_16" pad="AJ8"/>
<connect gate="D" pin="IO_17" pad="AM5"/>
<connect gate="D" pin="IO_18" pad="AM6"/>
<connect gate="D" pin="IO_19" pad="AM7"/>
<connect gate="D" pin="IO_2" pad="AL4"/>
<connect gate="D" pin="IO_20" pad="AM8"/>
<connect gate="D" pin="IO_21" pad="AM9"/>
<connect gate="D" pin="IO_22" pad="B10"/>
<connect gate="D" pin="IO_23" pad="B11"/>
<connect gate="D" pin="IO_24" pad="B12"/>
<connect gate="D" pin="IO_25" pad="B13"/>
<connect gate="D" pin="IO_26" pad="B14"/>
<connect gate="D" pin="IO_27" pad="B15"/>
<connect gate="D" pin="IO_28" pad="B16"/>
<connect gate="D" pin="IO_29" pad="B17"/>
<connect gate="D" pin="IO_3" pad="AK4"/>
<connect gate="D" pin="IO_30" pad="B18"/>
<connect gate="D" pin="IO_31" pad="B19"/>
<connect gate="D" pin="IO_32" pad="B20"/>
<connect gate="D" pin="IO_33" pad="B21"/>
<connect gate="D" pin="IO_34" pad="B22"/>
<connect gate="D" pin="IO_35" pad="B23"/>
<connect gate="D" pin="IO_36" pad="B24"/>
<connect gate="D" pin="IO_37" pad="B25"/>
<connect gate="D" pin="IO_38" pad="B26"/>
<connect gate="D" pin="IO_39" pad="B27"/>
<connect gate="D" pin="IO_4" pad="AL5"/>
<connect gate="D" pin="IO_40" pad="B28"/>
<connect gate="D" pin="IO_41" pad="B29"/>
<connect gate="D" pin="IO_42" pad="C10"/>
<connect gate="D" pin="IO_43" pad="C11"/>
<connect gate="D" pin="IO_44" pad="C12"/>
<connect gate="D" pin="IO_45" pad="C13"/>
<connect gate="D" pin="IO_46" pad="C15"/>
<connect gate="D" pin="IO_47" pad="C16"/>
<connect gate="D" pin="IO_48" pad="C17"/>
<connect gate="D" pin="IO_49" pad="C18"/>
<connect gate="D" pin="IO_5" pad="AK5"/>
<connect gate="D" pin="IO_50" pad="C20"/>
<connect gate="D" pin="IO_51" pad="C21"/>
<connect gate="D" pin="IO_52" pad="C22"/>
<connect gate="D" pin="IO_53" pad="C23"/>
<connect gate="D" pin="IO_54" pad="C24"/>
<connect gate="D" pin="IO_55" pad="C25"/>
<connect gate="D" pin="IO_56" pad="C26"/>
<connect gate="D" pin="IO_57" pad="C27"/>
<connect gate="D" pin="IO_58" pad="C28"/>
<connect gate="D" pin="IO_59" pad="C29"/>
<connect gate="D" pin="IO_6" pad="AL6"/>
<connect gate="D" pin="IO_60" pad="D10"/>
<connect gate="D" pin="IO_61" pad="D11"/>
<connect gate="D" pin="IO_62" pad="D12"/>
<connect gate="D" pin="IO_63" pad="D13"/>
<connect gate="D" pin="IO_64" pad="D14"/>
<connect gate="D" pin="IO_65" pad="D15"/>
<connect gate="D" pin="IO_66" pad="D16"/>
<connect gate="D" pin="IO_67" pad="D17"/>
<connect gate="D" pin="IO_68" pad="D18"/>
<connect gate="D" pin="IO_69" pad="D19"/>
<connect gate="D" pin="IO_7" pad="AK6"/>
<connect gate="D" pin="IO_70" pad="D20"/>
<connect gate="D" pin="IO_71" pad="D21"/>
<connect gate="D" pin="IO_72" pad="D22"/>
<connect gate="D" pin="IO_73" pad="D23"/>
<connect gate="D" pin="IO_74" pad="D25"/>
<connect gate="D" pin="IO_75" pad="D26"/>
<connect gate="D" pin="IO_8" pad="AL7"/>
<connect gate="D" pin="IO_9" pad="AK7"/>
<connect gate="D" pin="NCE" pad="C30"/>
<connect gate="D" pin="NCEO" pad="AL3"/>
<connect gate="D" pin="NIO_PULLUP" pad="AK3"/>
<connect gate="D" pin="NSTATUS" pad="B30"/>
<connect gate="D" pin="PORSEL" pad="AL2"/>
<connect gate="D" pin="VCCIO2" pad="C32"/>
<connect gate="D" pin="VCCIO6" pad="AK1"/>
<connect gate="D" pin="VCCIO7" pad="AM3"/>
<connect gate="D" pin="VREFB3N0" pad="C19"/>
<connect gate="D" pin="VREFB3N1" pad="D24"/>
<connect gate="D" pin="VREFB3N2" pad="C31"/>
<connect gate="D" pin="VREFB4N2" pad="C14"/>
<connect gate="D" pin="VREFB7N1" pad="AJ9"/>
<connect gate="D" pin="VREFB7N2" pad="AK2"/>
<connect gate="E" pin="FPLL7CLKN" pad="D29"/>
<connect gate="E" pin="FPLL7CLKP" pad="D30"/>
<connect gate="E" pin="GND" pad="E23"/>
<connect gate="E" pin="GNDA_PLL11" pad="H18"/>
<connect gate="E" pin="GNDA_PLL11_2" pad="G18"/>
<connect gate="E" pin="GNDA_PLL5" pad="H16"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="G16"/>
<connect gate="E" pin="GNDA_PLL7" pad="G26"/>
<connect gate="E" pin="GNDA_PLL7_2" pad="F26"/>
<connect gate="E" pin="GND_2" pad="E10"/>
<connect gate="E" pin="GND_3" pad="F27"/>
<connect gate="E" pin="GND_4" pad="G17"/>
<connect gate="E" pin="IO" pad="H28"/>
<connect gate="E" pin="IO_10" pad="E17"/>
<connect gate="E" pin="IO_11" pad="E18"/>
<connect gate="E" pin="IO_12" pad="E24"/>
<connect gate="E" pin="IO_13" pad="E19"/>
<connect gate="E" pin="IO_14" pad="E25"/>
<connect gate="E" pin="IO_15" pad="E20"/>
<connect gate="E" pin="IO_16" pad="E26"/>
<connect gate="E" pin="IO_17" pad="E27"/>
<connect gate="E" pin="IO_18" pad="E22"/>
<connect gate="E" pin="IO_19" pad="E28"/>
<connect gate="E" pin="IO_2" pad="D28"/>
<connect gate="E" pin="IO_20" pad="E29"/>
<connect gate="E" pin="IO_21" pad="E30"/>
<connect gate="E" pin="IO_22" pad="E31"/>
<connect gate="E" pin="IO_23" pad="E32"/>
<connect gate="E" pin="IO_24" pad="F10"/>
<connect gate="E" pin="IO_25" pad="F11"/>
<connect gate="E" pin="IO_26" pad="F12"/>
<connect gate="E" pin="IO_27" pad="F13"/>
<connect gate="E" pin="IO_28" pad="F14"/>
<connect gate="E" pin="IO_29" pad="F15"/>
<connect gate="E" pin="IO_3" pad="E13"/>
<connect gate="E" pin="IO_30" pad="F16"/>
<connect gate="E" pin="IO_31" pad="F17"/>
<connect gate="E" pin="IO_32" pad="F18"/>
<connect gate="E" pin="IO_33" pad="F19"/>
<connect gate="E" pin="IO_34" pad="F20"/>
<connect gate="E" pin="IO_35" pad="F22"/>
<connect gate="E" pin="IO_36" pad="F23"/>
<connect gate="E" pin="IO_37" pad="F24"/>
<connect gate="E" pin="IO_38" pad="F29"/>
<connect gate="E" pin="IO_39" pad="F30"/>
<connect gate="E" pin="IO_4" pad="D31"/>
<connect gate="E" pin="IO_40" pad="F31"/>
<connect gate="E" pin="IO_41" pad="F32"/>
<connect gate="E" pin="IO_42" pad="G10"/>
<connect gate="E" pin="IO_43" pad="G11"/>
<connect gate="E" pin="IO_44" pad="G12"/>
<connect gate="E" pin="IO_45" pad="G13"/>
<connect gate="E" pin="IO_46" pad="G19"/>
<connect gate="E" pin="IO_47" pad="G20"/>
<connect gate="E" pin="IO_48" pad="G21"/>
<connect gate="E" pin="IO_49" pad="G22"/>
<connect gate="E" pin="IO_5" pad="E14"/>
<connect gate="E" pin="IO_50" pad="G23"/>
<connect gate="E" pin="IO_51" pad="G24"/>
<connect gate="E" pin="IO_52" pad="G25"/>
<connect gate="E" pin="IO_53" pad="G29"/>
<connect gate="E" pin="IO_54" pad="G30"/>
<connect gate="E" pin="IO_55" pad="G31"/>
<connect gate="E" pin="IO_56" pad="G32"/>
<connect gate="E" pin="IO_57" pad="H11"/>
<connect gate="E" pin="IO_58" pad="H12"/>
<connect gate="E" pin="IO_59" pad="H13"/>
<connect gate="E" pin="IO_6" pad="D32"/>
<connect gate="E" pin="IO_60" pad="H14"/>
<connect gate="E" pin="IO_61" pad="H19"/>
<connect gate="E" pin="IO_62" pad="H20"/>
<connect gate="E" pin="IO_63" pad="H21"/>
<connect gate="E" pin="IO_64" pad="H22"/>
<connect gate="E" pin="IO_65" pad="H23"/>
<connect gate="E" pin="IO_66" pad="H24"/>
<connect gate="E" pin="IO_67" pad="H27"/>
<connect gate="E" pin="IO_7" pad="E15"/>
<connect gate="E" pin="IO_8" pad="E16"/>
<connect gate="E" pin="IO_9" pad="E11"/>
<connect gate="E" pin="MSEL3" pad="H10"/>
<connect gate="E" pin="NC" pad="G28"/>
<connect gate="E" pin="NC_2" pad="F21"/>
<connect gate="E" pin="NC_3" pad="F25"/>
<connect gate="E" pin="NC_4" pad="G14"/>
<connect gate="E" pin="NC_5" pad="G27"/>
<connect gate="E" pin="VCCA_PLL11" pad="H17"/>
<connect gate="E" pin="VCCA_PLL5" pad="G15"/>
<connect gate="E" pin="VCCA_PLL7" pad="H26"/>
<connect gate="E" pin="VCCD_PLL5" pad="H15"/>
<connect gate="E" pin="VCCD_PLL7" pad="H25"/>
<connect gate="E" pin="VCCIO3" pad="E21"/>
<connect gate="E" pin="VCCIO4" pad="E12"/>
<connect gate="E" pin="VREFB2N0" pad="F28"/>
<connect gate="F" pin="CONF_DONE" pad="J25"/>
<connect gate="F" pin="GND" pad="M19"/>
<connect gate="F" pin="GND_2" pad="J24"/>
<connect gate="F" pin="GND_3" pad="K28"/>
<connect gate="F" pin="GND_4" pad="M14"/>
<connect gate="F" pin="GND_5" pad="L11"/>
<connect gate="F" pin="GND_6" pad="M12"/>
<connect gate="F" pin="IO" pad="M29"/>
<connect gate="F" pin="IO_10" pad="J19"/>
<connect gate="F" pin="IO_11" pad="J15"/>
<connect gate="F" pin="IO_12" pad="J26"/>
<connect gate="F" pin="IO_13" pad="J20"/>
<connect gate="F" pin="IO_14" pad="J27"/>
<connect gate="F" pin="IO_15" pad="J21"/>
<connect gate="F" pin="IO_16" pad="K11"/>
<connect gate="F" pin="IO_17" pad="J22"/>
<connect gate="F" pin="IO_18" pad="K12"/>
<connect gate="F" pin="IO_19" pad="J23"/>
<connect gate="F" pin="IO_2" pad="H29"/>
<connect gate="F" pin="IO_20" pad="K13"/>
<connect gate="F" pin="IO_21" pad="J31"/>
<connect gate="F" pin="IO_22" pad="K14"/>
<connect gate="F" pin="IO_23" pad="J32"/>
<connect gate="F" pin="IO_24" pad="K15"/>
<connect gate="F" pin="IO_25" pad="K16"/>
<connect gate="F" pin="IO_26" pad="K17"/>
<connect gate="F" pin="IO_27" pad="K18"/>
<connect gate="F" pin="IO_28" pad="K19"/>
<connect gate="F" pin="IO_29" pad="K20"/>
<connect gate="F" pin="IO_3" pad="H30"/>
<connect gate="F" pin="IO_30" pad="K24"/>
<connect gate="F" pin="IO_31" pad="K21"/>
<connect gate="F" pin="IO_32" pad="K25"/>
<connect gate="F" pin="IO_33" pad="K22"/>
<connect gate="F" pin="IO_34" pad="K26"/>
<connect gate="F" pin="IO_35" pad="K27"/>
<connect gate="F" pin="IO_36" pad="K29"/>
<connect gate="F" pin="IO_37" pad="K30"/>
<connect gate="F" pin="IO_38" pad="K31"/>
<connect gate="F" pin="IO_39" pad="K32"/>
<connect gate="F" pin="IO_4" pad="J11"/>
<connect gate="F" pin="IO_40" pad="L10"/>
<connect gate="F" pin="IO_41" pad="L12"/>
<connect gate="F" pin="IO_42" pad="L13"/>
<connect gate="F" pin="IO_43" pad="L14"/>
<connect gate="F" pin="IO_44" pad="L15"/>
<connect gate="F" pin="IO_45" pad="L16"/>
<connect gate="F" pin="IO_46" pad="L17"/>
<connect gate="F" pin="IO_47" pad="L18"/>
<connect gate="F" pin="IO_48" pad="L19"/>
<connect gate="F" pin="IO_49" pad="L20"/>
<connect gate="F" pin="IO_5" pad="H31"/>
<connect gate="F" pin="IO_50" pad="L21"/>
<connect gate="F" pin="IO_51" pad="L22"/>
<connect gate="F" pin="IO_52" pad="L23"/>
<connect gate="F" pin="IO_53" pad="L24"/>
<connect gate="F" pin="IO_54" pad="L25"/>
<connect gate="F" pin="IO_55" pad="L26"/>
<connect gate="F" pin="IO_56" pad="L29"/>
<connect gate="F" pin="IO_57" pad="L30"/>
<connect gate="F" pin="IO_58" pad="L31"/>
<connect gate="F" pin="IO_59" pad="L32"/>
<connect gate="F" pin="IO_6" pad="J12"/>
<connect gate="F" pin="IO_60" pad="M10"/>
<connect gate="F" pin="IO_61" pad="M11"/>
<connect gate="F" pin="IO_62" pad="M22"/>
<connect gate="F" pin="IO_63" pad="M23"/>
<connect gate="F" pin="IO_64" pad="M24"/>
<connect gate="F" pin="IO_65" pad="M25"/>
<connect gate="F" pin="IO_66" pad="M26"/>
<connect gate="F" pin="IO_67" pad="M27"/>
<connect gate="F" pin="IO_7" pad="H32"/>
<connect gate="F" pin="IO_8" pad="J13"/>
<connect gate="F" pin="IO_9" pad="J14"/>
<connect gate="F" pin="MSEL2" pad="J10"/>
<connect gate="F" pin="NC" pad="J30"/>
<connect gate="F" pin="NC_2" pad="L27"/>
<connect gate="F" pin="NC_3" pad="J29"/>
<connect gate="F" pin="NC_4" pad="L28"/>
<connect gate="F" pin="VCCD_PLL11" pad="J18"/>
<connect gate="F" pin="VCCINT" pad="K23"/>
<connect gate="F" pin="VCCINT_2" pad="M21"/>
<connect gate="F" pin="VCCINT_3" pad="K10"/>
<connect gate="F" pin="VCCIO2" pad="M28"/>
<connect gate="F" pin="VCCIO3" pad="M17"/>
<connect gate="F" pin="VCCIO4" pad="M16"/>
<connect gate="F" pin="VCCPD3" pad="M20"/>
<connect gate="F" pin="VCCPD3_2" pad="M18"/>
<connect gate="F" pin="VCCPD4" pad="M13"/>
<connect gate="F" pin="VCCPD4_2" pad="M15"/>
<connect gate="F" pin="VCC_PLL11_OUT" pad="J17"/>
<connect gate="F" pin="VCC_PLL5_OUT" pad="J16"/>
<connect gate="F" pin="VREFB2N1" pad="J28"/>
<connect gate="G" pin="CLK1N" pad="T29"/>
<connect gate="G" pin="CLK1P" pad="T30"/>
<connect gate="G" pin="GND" pad="N20"/>
<connect gate="G" pin="GNDA_PLL1" pad="T26"/>
<connect gate="G" pin="GNDA_PLL1_2" pad="T25"/>
<connect gate="G" pin="GND_10" pad="R14"/>
<connect gate="G" pin="GND_11" pad="P13"/>
<connect gate="G" pin="GND_12" pad="T19"/>
<connect gate="G" pin="GND_13" pad="P21"/>
<connect gate="G" pin="GND_14" pad="T13"/>
<connect gate="G" pin="GND_15" pad="P15"/>
<connect gate="G" pin="GND_16" pad="T17"/>
<connect gate="G" pin="GND_17" pad="P17"/>
<connect gate="G" pin="GND_18" pad="R16"/>
<connect gate="G" pin="GND_19" pad="P19"/>
<connect gate="G" pin="GND_2" pad="N16"/>
<connect gate="G" pin="GND_3" pad="N14"/>
<connect gate="G" pin="GND_4" pad="R20"/>
<connect gate="G" pin="GND_5" pad="N18"/>
<connect gate="G" pin="GND_6" pad="R18"/>
<connect gate="G" pin="GND_7" pad="P12"/>
<connect gate="G" pin="GND_8" pad="T15"/>
<connect gate="G" pin="GND_9" pad="N32"/>
<connect gate="G" pin="IO" pad="T28"/>
<connect gate="G" pin="IO_10" pad="N28"/>
<connect gate="G" pin="IO_11" pad="M32"/>
<connect gate="G" pin="IO_12" pad="P24"/>
<connect gate="G" pin="IO_13" pad="N29"/>
<connect gate="G" pin="IO_14" pad="P25"/>
<connect gate="G" pin="IO_15" pad="N30"/>
<connect gate="G" pin="IO_16" pad="P26"/>
<connect gate="G" pin="IO_17" pad="N31"/>
<connect gate="G" pin="IO_18" pad="P27"/>
<connect gate="G" pin="IO_19" pad="P28"/>
<connect gate="G" pin="IO_2" pad="N22"/>
<connect gate="G" pin="IO_20" pad="P10"/>
<connect gate="G" pin="IO_21" pad="P29"/>
<connect gate="G" pin="IO_22" pad="P11"/>
<connect gate="G" pin="IO_23" pad="P31"/>
<connect gate="G" pin="IO_24" pad="P32"/>
<connect gate="G" pin="IO_25" pad="R10"/>
<connect gate="G" pin="IO_26" pad="R11"/>
<connect gate="G" pin="IO_27" pad="R22"/>
<connect gate="G" pin="IO_28" pad="R23"/>
<connect gate="G" pin="IO_29" pad="R24"/>
<connect gate="G" pin="IO_3" pad="N23"/>
<connect gate="G" pin="IO_30" pad="R25"/>
<connect gate="G" pin="IO_31" pad="R26"/>
<connect gate="G" pin="IO_32" pad="R27"/>
<connect gate="G" pin="IO_33" pad="R28"/>
<connect gate="G" pin="IO_34" pad="R29"/>
<connect gate="G" pin="IO_35" pad="R30"/>
<connect gate="G" pin="IO_36" pad="R31"/>
<connect gate="G" pin="IO_37" pad="T10"/>
<connect gate="G" pin="IO_38" pad="T11"/>
<connect gate="G" pin="IO_39" pad="T22"/>
<connect gate="G" pin="IO_4" pad="N24"/>
<connect gate="G" pin="IO_40" pad="T23"/>
<connect gate="G" pin="IO_41" pad="T27"/>
<connect gate="G" pin="IO_5" pad="N25"/>
<connect gate="G" pin="IO_6" pad="N26"/>
<connect gate="G" pin="IO_7" pad="M30"/>
<connect gate="G" pin="IO_8" pad="N27"/>
<connect gate="G" pin="IO_9" pad="M31"/>
<connect gate="G" pin="NC" pad="P23"/>
<connect gate="G" pin="NC_2" pad="N10"/>
<connect gate="G" pin="NC_3" pad="P22"/>
<connect gate="G" pin="NC_4" pad="N11"/>
<connect gate="G" pin="VCCA_PLL1" pad="T24"/>
<connect gate="G" pin="VCCINT" pad="T20"/>
<connect gate="G" pin="VCCINT_10" pad="R15"/>
<connect gate="G" pin="VCCINT_11" pad="T14"/>
<connect gate="G" pin="VCCINT_12" pad="R13"/>
<connect gate="G" pin="VCCINT_13" pad="R17"/>
<connect gate="G" pin="VCCINT_14" pad="T16"/>
<connect gate="G" pin="VCCINT_15" pad="R19"/>
<connect gate="G" pin="VCCINT_16" pad="T18"/>
<connect gate="G" pin="VCCINT_2" pad="N17"/>
<connect gate="G" pin="VCCINT_3" pad="N15"/>
<connect gate="G" pin="VCCINT_4" pad="N19"/>
<connect gate="G" pin="VCCINT_5" pad="N13"/>
<connect gate="G" pin="VCCINT_6" pad="P14"/>
<connect gate="G" pin="VCCINT_7" pad="P16"/>
<connect gate="G" pin="VCCINT_8" pad="P18"/>
<connect gate="G" pin="VCCINT_9" pad="P20"/>
<connect gate="G" pin="VCCIO2" pad="T21"/>
<connect gate="G" pin="VCCIO2_2" pad="R32"/>
<connect gate="G" pin="VCCIO5" pad="T12"/>
<connect gate="G" pin="VCCPD2" pad="R21"/>
<connect gate="G" pin="VCCPD2_2" pad="N21"/>
<connect gate="G" pin="VCCPD5" pad="R12"/>
<connect gate="G" pin="VCCPD5_2" pad="N12"/>
<connect gate="G" pin="VREFB2N2" pad="P30"/>
<connect gate="H" pin="CLK3N" pad="U29"/>
<connect gate="H" pin="CLK3P" pad="U30"/>
<connect gate="H" pin="GND" pad="Y19"/>
<connect gate="H" pin="GNDA_PLL2" pad="U26"/>
<connect gate="H" pin="GNDA_PLL2_2" pad="U25"/>
<connect gate="H" pin="GND_10" pad="U20"/>
<connect gate="H" pin="GND_11" pad="W16"/>
<connect gate="H" pin="GND_12" pad="V13"/>
<connect gate="H" pin="GND_13" pad="W20"/>
<connect gate="H" pin="GND_14" pad="Y13"/>
<connect gate="H" pin="GND_15" pad="W18"/>
<connect gate="H" pin="GND_16" pad="V27"/>
<connect gate="H" pin="GND_17" pad="W12"/>
<connect gate="H" pin="GND_18" pad="Y17"/>
<connect gate="H" pin="GND_19" pad="Y15"/>
<connect gate="H" pin="GND_2" pad="U18"/>
<connect gate="H" pin="GND_20" pad="V19"/>
<connect gate="H" pin="GND_3" pad="V11"/>
<connect gate="H" pin="GND_4" pad="V17"/>
<connect gate="H" pin="GND_5" pad="V22"/>
<connect gate="H" pin="GND_6" pad="U16"/>
<connect gate="H" pin="GND_7" pad="V15"/>
<connect gate="H" pin="GND_8" pad="U14"/>
<connect gate="H" pin="GND_9" pad="W14"/>
<connect gate="H" pin="IO" pad="Y31"/>
<connect gate="H" pin="IO_10" pad="U10"/>
<connect gate="H" pin="IO_11" pad="U23"/>
<connect gate="H" pin="IO_12" pad="U31"/>
<connect gate="H" pin="IO_13" pad="V29"/>
<connect gate="H" pin="IO_14" pad="U11"/>
<connect gate="H" pin="IO_15" pad="U32"/>
<connect gate="H" pin="IO_16" pad="V10"/>
<connect gate="H" pin="IO_17" pad="V30"/>
<connect gate="H" pin="IO_18" pad="V31"/>
<connect gate="H" pin="IO_19" pad="W24"/>
<connect gate="H" pin="IO_2" pad="V23"/>
<connect gate="H" pin="IO_20" pad="W25"/>
<connect gate="H" pin="IO_21" pad="W26"/>
<connect gate="H" pin="IO_22" pad="W27"/>
<connect gate="H" pin="IO_23" pad="W28"/>
<connect gate="H" pin="IO_24" pad="W29"/>
<connect gate="H" pin="IO_25" pad="W31"/>
<connect gate="H" pin="IO_26" pad="W32"/>
<connect gate="H" pin="IO_27" pad="Y10"/>
<connect gate="H" pin="IO_28" pad="Y11"/>
<connect gate="H" pin="IO_29" pad="Y22"/>
<connect gate="H" pin="IO_3" pad="T31"/>
<connect gate="H" pin="IO_30" pad="Y23"/>
<connect gate="H" pin="IO_31" pad="Y24"/>
<connect gate="H" pin="IO_32" pad="Y25"/>
<connect gate="H" pin="IO_33" pad="Y26"/>
<connect gate="H" pin="IO_34" pad="Y27"/>
<connect gate="H" pin="IO_35" pad="Y28"/>
<connect gate="H" pin="IO_36" pad="Y29"/>
<connect gate="H" pin="IO_37" pad="Y30"/>
<connect gate="H" pin="IO_4" pad="U27"/>
<connect gate="H" pin="IO_5" pad="V24"/>
<connect gate="H" pin="IO_6" pad="T32"/>
<connect gate="H" pin="IO_7" pad="U28"/>
<connect gate="H" pin="IO_8" pad="U22"/>
<connect gate="H" pin="IO_9" pad="V28"/>
<connect gate="H" pin="NC" pad="W11"/>
<connect gate="H" pin="NC_2" pad="W22"/>
<connect gate="H" pin="NC_3" pad="W23"/>
<connect gate="H" pin="NC_4" pad="W10"/>
<connect gate="H" pin="VCCA_PLL2" pad="V26"/>
<connect gate="H" pin="VCCD_PLL1" pad="U24"/>
<connect gate="H" pin="VCCD_PLL2" pad="V25"/>
<connect gate="H" pin="VCCINT" pad="U13"/>
<connect gate="H" pin="VCCINT_10" pad="W13"/>
<connect gate="H" pin="VCCINT_11" pad="Y20"/>
<connect gate="H" pin="VCCINT_12" pad="W15"/>
<connect gate="H" pin="VCCINT_13" pad="W19"/>
<connect gate="H" pin="VCCINT_14" pad="V20"/>
<connect gate="H" pin="VCCINT_15" pad="Y14"/>
<connect gate="H" pin="VCCINT_16" pad="U15"/>
<connect gate="H" pin="VCCINT_17" pad="W17"/>
<connect gate="H" pin="VCCINT_2" pad="U19"/>
<connect gate="H" pin="VCCINT_3" pad="V14"/>
<connect gate="H" pin="VCCINT_4" pad="U17"/>
<connect gate="H" pin="VCCINT_5" pad="V18"/>
<connect gate="H" pin="VCCINT_6" pad="W21"/>
<connect gate="H" pin="VCCINT_7" pad="Y16"/>
<connect gate="H" pin="VCCINT_8" pad="V16"/>
<connect gate="H" pin="VCCINT_9" pad="Y18"/>
<connect gate="H" pin="VCCIO1" pad="U21"/>
<connect gate="H" pin="VCCIO1_2" pad="V32"/>
<connect gate="H" pin="VCCIO6" pad="U12"/>
<connect gate="H" pin="VCCPD1" pad="Y21"/>
<connect gate="H" pin="VCCPD1_2" pad="V21"/>
<connect gate="H" pin="VCCPD6" pad="V12"/>
<connect gate="H" pin="VCCPD6_2" pad="Y12"/>
<connect gate="H" pin="VREFB1N0" pad="W30"/>
<connect gate="I" pin="GND" pad="AC28"/>
<connect gate="I" pin="GNDA_PLL12" pad="AD17"/>
<connect gate="I" pin="GNDA_PLL6" pad="AD16"/>
<connect gate="I" pin="GND_2" pad="AA14"/>
<connect gate="I" pin="GND_3" pad="AA21"/>
<connect gate="I" pin="GND_4" pad="Y32"/>
<connect gate="I" pin="GND_5" pad="AB22"/>
<connect gate="I" pin="GND_6" pad="AA19"/>
<connect gate="I" pin="IO" pad="AD32"/>
<connect gate="I" pin="IO_10" pad="AA29"/>
<connect gate="I" pin="IO_11" pad="AA30"/>
<connect gate="I" pin="IO_12" pad="AA31"/>
<connect gate="I" pin="IO_13" pad="AA32"/>
<connect gate="I" pin="IO_14" pad="AB10"/>
<connect gate="I" pin="IO_15" pad="AB11"/>
<connect gate="I" pin="IO_16" pad="AB12"/>
<connect gate="I" pin="IO_17" pad="AB13"/>
<connect gate="I" pin="IO_18" pad="AB14"/>
<connect gate="I" pin="IO_19" pad="AB15"/>
<connect gate="I" pin="IO_2" pad="AA22"/>
<connect gate="I" pin="IO_20" pad="AB16"/>
<connect gate="I" pin="IO_21" pad="AB17"/>
<connect gate="I" pin="IO_22" pad="AB18"/>
<connect gate="I" pin="IO_23" pad="AB19"/>
<connect gate="I" pin="IO_24" pad="AB20"/>
<connect gate="I" pin="IO_25" pad="AB23"/>
<connect gate="I" pin="IO_26" pad="AB21"/>
<connect gate="I" pin="IO_27" pad="AB24"/>
<connect gate="I" pin="IO_28" pad="AB25"/>
<connect gate="I" pin="IO_29" pad="AB26"/>
<connect gate="I" pin="IO_3" pad="AA23"/>
<connect gate="I" pin="IO_30" pad="AB27"/>
<connect gate="I" pin="IO_31" pad="AB28"/>
<connect gate="I" pin="IO_32" pad="AB29"/>
<connect gate="I" pin="IO_33" pad="AB30"/>
<connect gate="I" pin="IO_34" pad="AB31"/>
<connect gate="I" pin="IO_35" pad="AB32"/>
<connect gate="I" pin="IO_36" pad="AC11"/>
<connect gate="I" pin="IO_37" pad="AC12"/>
<connect gate="I" pin="IO_38" pad="AC13"/>
<connect gate="I" pin="IO_39" pad="AC14"/>
<connect gate="I" pin="IO_4" pad="AA24"/>
<connect gate="I" pin="IO_40" pad="AC15"/>
<connect gate="I" pin="IO_41" pad="AC16"/>
<connect gate="I" pin="IO_42" pad="AC17"/>
<connect gate="I" pin="IO_43" pad="AC18"/>
<connect gate="I" pin="IO_44" pad="AC19"/>
<connect gate="I" pin="IO_45" pad="AC20"/>
<connect gate="I" pin="IO_46" pad="AC21"/>
<connect gate="I" pin="IO_47" pad="AC22"/>
<connect gate="I" pin="IO_48" pad="AC24"/>
<connect gate="I" pin="IO_49" pad="AC25"/>
<connect gate="I" pin="IO_5" pad="AA25"/>
<connect gate="I" pin="IO_50" pad="AC26"/>
<connect gate="I" pin="IO_51" pad="AC27"/>
<connect gate="I" pin="IO_52" pad="AC31"/>
<connect gate="I" pin="IO_53" pad="AC32"/>
<connect gate="I" pin="IO_54" pad="AD10"/>
<connect gate="I" pin="IO_55" pad="AD11"/>
<connect gate="I" pin="IO_56" pad="AD12"/>
<connect gate="I" pin="IO_57" pad="AD13"/>
<connect gate="I" pin="IO_58" pad="AD14"/>
<connect gate="I" pin="IO_59" pad="AD18"/>
<connect gate="I" pin="IO_6" pad="AA26"/>
<connect gate="I" pin="IO_60" pad="AD19"/>
<connect gate="I" pin="IO_61" pad="AD20"/>
<connect gate="I" pin="IO_62" pad="AD21"/>
<connect gate="I" pin="IO_63" pad="AD22"/>
<connect gate="I" pin="IO_64" pad="AD23"/>
<connect gate="I" pin="IO_65" pad="AD24"/>
<connect gate="I" pin="IO_66" pad="AD25"/>
<connect gate="I" pin="IO_67" pad="AD26"/>
<connect gate="I" pin="IO_68" pad="AD27"/>
<connect gate="I" pin="IO_69" pad="AD31"/>
<connect gate="I" pin="IO_7" pad="AA27"/>
<connect gate="I" pin="IO_8" pad="AA10"/>
<connect gate="I" pin="IO_9" pad="AA11"/>
<connect gate="I" pin="NC" pad="AD30"/>
<connect gate="I" pin="NC_2" pad="AC29"/>
<connect gate="I" pin="NC_3" pad="AC30"/>
<connect gate="I" pin="NC_4" pad="AD29"/>
<connect gate="I" pin="VCCD_PLL6" pad="AD15"/>
<connect gate="I" pin="VCCINT" pad="AA12"/>
<connect gate="I" pin="VCCINT_2" pad="AC10"/>
<connect gate="I" pin="VCCIO1" pad="AA28"/>
<connect gate="I" pin="VCCIO7" pad="AA16"/>
<connect gate="I" pin="VCCIO8" pad="AA17"/>
<connect gate="I" pin="VCCPD7" pad="AA13"/>
<connect gate="I" pin="VCCPD7_2" pad="AA15"/>
<connect gate="I" pin="VCCPD8" pad="AA18"/>
<connect gate="I" pin="VCCPD8_2" pad="AA20"/>
<connect gate="I" pin="VCCSEL" pad="AC23"/>
<connect gate="I" pin="VREFB1N1" pad="AD28"/>
<connect gate="J" pin="GND" pad="AH27"/>
<connect gate="J" pin="GNDA_PLL12" pad="AE17"/>
<connect gate="J" pin="GNDA_PLL6" pad="AE16"/>
<connect gate="J" pin="GNDA_PLL8" pad="AG26"/>
<connect gate="J" pin="GNDA_PLL8_2" pad="AG27"/>
<connect gate="J" pin="GND_2" pad="AH10"/>
<connect gate="J" pin="GND_3" pad="AF17"/>
<connect gate="J" pin="GND_4" pad="AH23"/>
<connect gate="J" pin="IO" pad="AJ10"/>
<connect gate="J" pin="IO_10" pad="AE25"/>
<connect gate="J" pin="IO_11" pad="AE13"/>
<connect gate="J" pin="IO_12" pad="AE26"/>
<connect gate="J" pin="IO_13" pad="AE14"/>
<connect gate="J" pin="IO_14" pad="AE27"/>
<connect gate="J" pin="IO_15" pad="AE28"/>
<connect gate="J" pin="IO_16" pad="AE29"/>
<connect gate="J" pin="IO_17" pad="AE30"/>
<connect gate="J" pin="IO_18" pad="AE31"/>
<connect gate="J" pin="IO_19" pad="AF19"/>
<connect gate="J" pin="IO_2" pad="AE19"/>
<connect gate="J" pin="IO_20" pad="AE32"/>
<connect gate="J" pin="IO_21" pad="AF20"/>
<connect gate="J" pin="IO_22" pad="AF10"/>
<connect gate="J" pin="IO_23" pad="AF21"/>
<connect gate="J" pin="IO_24" pad="AF11"/>
<connect gate="J" pin="IO_25" pad="AF22"/>
<connect gate="J" pin="IO_26" pad="AF12"/>
<connect gate="J" pin="IO_27" pad="AF23"/>
<connect gate="J" pin="IO_28" pad="AF13"/>
<connect gate="J" pin="IO_29" pad="AF29"/>
<connect gate="J" pin="IO_3" pad="AE20"/>
<connect gate="J" pin="IO_30" pad="AF30"/>
<connect gate="J" pin="IO_31" pad="AF31"/>
<connect gate="J" pin="IO_32" pad="AF32"/>
<connect gate="J" pin="IO_33" pad="AG10"/>
<connect gate="J" pin="IO_34" pad="AG11"/>
<connect gate="J" pin="IO_35" pad="AG12"/>
<connect gate="J" pin="IO_36" pad="AG13"/>
<connect gate="J" pin="IO_37" pad="AG14"/>
<connect gate="J" pin="IO_38" pad="AG15"/>
<connect gate="J" pin="IO_39" pad="AG16"/>
<connect gate="J" pin="IO_4" pad="AE21"/>
<connect gate="J" pin="IO_40" pad="AG17"/>
<connect gate="J" pin="IO_41" pad="AG18"/>
<connect gate="J" pin="IO_42" pad="AG19"/>
<connect gate="J" pin="IO_43" pad="AG20"/>
<connect gate="J" pin="IO_44" pad="AG22"/>
<connect gate="J" pin="IO_45" pad="AG23"/>
<connect gate="J" pin="IO_46" pad="AG24"/>
<connect gate="J" pin="IO_47" pad="AG29"/>
<connect gate="J" pin="IO_48" pad="AG30"/>
<connect gate="J" pin="IO_49" pad="AG31"/>
<connect gate="J" pin="IO_5" pad="AE22"/>
<connect gate="J" pin="IO_50" pad="AG32"/>
<connect gate="J" pin="IO_51" pad="AH11"/>
<connect gate="J" pin="IO_52" pad="AH13"/>
<connect gate="J" pin="IO_53" pad="AH14"/>
<connect gate="J" pin="IO_54" pad="AH15"/>
<connect gate="J" pin="IO_55" pad="AH16"/>
<connect gate="J" pin="IO_56" pad="AH17"/>
<connect gate="J" pin="IO_57" pad="AH18"/>
<connect gate="J" pin="IO_58" pad="AH19"/>
<connect gate="J" pin="IO_59" pad="AH20"/>
<connect gate="J" pin="IO_6" pad="AE10"/>
<connect gate="J" pin="IO_60" pad="AH22"/>
<connect gate="J" pin="IO_61" pad="AH24"/>
<connect gate="J" pin="IO_62" pad="AH25"/>
<connect gate="J" pin="IO_63" pad="AH26"/>
<connect gate="J" pin="IO_64" pad="AH28"/>
<connect gate="J" pin="IO_65" pad="AH29"/>
<connect gate="J" pin="IO_66" pad="AH30"/>
<connect gate="J" pin="IO_67" pad="AH31"/>
<connect gate="J" pin="IO_68" pad="AH32"/>
<connect gate="J" pin="IO_7" pad="AE23"/>
<connect gate="J" pin="IO_8" pad="AE11"/>
<connect gate="J" pin="IO_9" pad="AE12"/>
<connect gate="J" pin="NC" pad="AF28"/>
<connect gate="J" pin="NC_2" pad="AG21"/>
<connect gate="J" pin="NC_3" pad="AG25"/>
<connect gate="J" pin="NC_4" pad="AF27"/>
<connect gate="J" pin="NC_5" pad="AF14"/>
<connect gate="J" pin="TCK" pad="AF24"/>
<connect gate="J" pin="TMS" pad="AE24"/>
<connect gate="J" pin="VCCA_PLL12" pad="AF18"/>
<connect gate="J" pin="VCCA_PLL6" pad="AE15"/>
<connect gate="J" pin="VCCA_PLL8" pad="AF26"/>
<connect gate="J" pin="VCCD_PLL12" pad="AE18"/>
<connect gate="J" pin="VCCD_PLL8" pad="AF25"/>
<connect gate="J" pin="VCCIO7" pad="AH12"/>
<connect gate="J" pin="VCCIO8" pad="AH21"/>
<connect gate="J" pin="VCC_PLL12_OUT" pad="AF16"/>
<connect gate="J" pin="VCC_PLL6_OUT" pad="AF15"/>
<connect gate="J" pin="VREFB1N2" pad="AG28"/>
<connect gate="K" pin="FPLL8CLKN" pad="AJ29"/>
<connect gate="K" pin="FPLL8CLKP" pad="AJ30"/>
<connect gate="K" pin="GND" pad="AM31"/>
<connect gate="K" pin="GND_2" pad="AM20"/>
<connect gate="K" pin="GND_3" pad="AL32"/>
<connect gate="K" pin="GND_4" pad="AM13"/>
<connect gate="K" pin="IO" pad="AM29"/>
<connect gate="K" pin="IO_10" pad="AK26"/>
<connect gate="K" pin="IO_11" pad="AJ12"/>
<connect gate="K" pin="IO_12" pad="AK27"/>
<connect gate="K" pin="IO_13" pad="AJ13"/>
<connect gate="K" pin="IO_14" pad="AK28"/>
<connect gate="K" pin="IO_15" pad="AJ14"/>
<connect gate="K" pin="IO_16" pad="AK29"/>
<connect gate="K" pin="IO_17" pad="AJ25"/>
<connect gate="K" pin="IO_18" pad="AJ15"/>
<connect gate="K" pin="IO_19" pad="AJ26"/>
<connect gate="K" pin="IO_2" pad="AK20"/>
<connect gate="K" pin="IO_20" pad="AJ16"/>
<connect gate="K" pin="IO_21" pad="AJ22"/>
<connect gate="K" pin="IO_22" pad="AJ27"/>
<connect gate="K" pin="IO_23" pad="AJ17"/>
<connect gate="K" pin="IO_24" pad="AK10"/>
<connect gate="K" pin="IO_25" pad="AJ23"/>
<connect gate="K" pin="IO_26" pad="AJ28"/>
<connect gate="K" pin="IO_27" pad="AJ18"/>
<connect gate="K" pin="IO_28" pad="AK11"/>
<connect gate="K" pin="IO_29" pad="AJ19"/>
<connect gate="K" pin="IO_3" pad="AK21"/>
<connect gate="K" pin="IO_30" pad="AK12"/>
<connect gate="K" pin="IO_31" pad="AJ20"/>
<connect gate="K" pin="IO_32" pad="AK13"/>
<connect gate="K" pin="IO_33" pad="AJ31"/>
<connect gate="K" pin="IO_34" pad="AJ21"/>
<connect gate="K" pin="IO_35" pad="AK15"/>
<connect gate="K" pin="IO_36" pad="AJ32"/>
<connect gate="K" pin="IO_37" pad="AK16"/>
<connect gate="K" pin="IO_38" pad="AK17"/>
<connect gate="K" pin="IO_39" pad="AK18"/>
<connect gate="K" pin="IO_4" pad="AK22"/>
<connect gate="K" pin="IO_40" pad="AL11"/>
<connect gate="K" pin="IO_41" pad="AL12"/>
<connect gate="K" pin="IO_42" pad="AL13"/>
<connect gate="K" pin="IO_43" pad="AL14"/>
<connect gate="K" pin="IO_44" pad="AL15"/>
<connect gate="K" pin="IO_45" pad="AL16"/>
<connect gate="K" pin="IO_46" pad="AL17"/>
<connect gate="K" pin="IO_47" pad="AL18"/>
<connect gate="K" pin="IO_48" pad="AL19"/>
<connect gate="K" pin="IO_49" pad="AL20"/>
<connect gate="K" pin="IO_5" pad="AK23"/>
<connect gate="K" pin="IO_50" pad="AL21"/>
<connect gate="K" pin="IO_51" pad="AL22"/>
<connect gate="K" pin="IO_52" pad="AL23"/>
<connect gate="K" pin="IO_53" pad="AL24"/>
<connect gate="K" pin="IO_54" pad="AL25"/>
<connect gate="K" pin="IO_55" pad="AL26"/>
<connect gate="K" pin="IO_56" pad="AL27"/>
<connect gate="K" pin="IO_57" pad="AL28"/>
<connect gate="K" pin="IO_58" pad="AL29"/>
<connect gate="K" pin="IO_59" pad="AM10"/>
<connect gate="K" pin="IO_6" pad="AK24"/>
<connect gate="K" pin="IO_60" pad="AM11"/>
<connect gate="K" pin="IO_61" pad="AM12"/>
<connect gate="K" pin="IO_62" pad="AM14"/>
<connect gate="K" pin="IO_63" pad="AM16"/>
<connect gate="K" pin="IO_64" pad="AM17"/>
<connect gate="K" pin="IO_65" pad="AM19"/>
<connect gate="K" pin="IO_66" pad="AM21"/>
<connect gate="K" pin="IO_67" pad="AM22"/>
<connect gate="K" pin="IO_68" pad="AM23"/>
<connect gate="K" pin="IO_69" pad="AM24"/>
<connect gate="K" pin="IO_7" pad="AK25"/>
<connect gate="K" pin="IO_70" pad="AM25"/>
<connect gate="K" pin="IO_71" pad="AM26"/>
<connect gate="K" pin="IO_72" pad="AM27"/>
<connect gate="K" pin="IO_73" pad="AM28"/>
<connect gate="K" pin="IO_8" pad="AL10"/>
<connect gate="K" pin="IO_9" pad="AJ11"/>
<connect gate="K" pin="NCONFIG" pad="AL30"/>
<connect gate="K" pin="TDI" pad="AL31"/>
<connect gate="K" pin="TRST" pad="AK30"/>
<connect gate="K" pin="VCCIO1" pad="AK32"/>
<connect gate="K" pin="VCCIO7" pad="AM15"/>
<connect gate="K" pin="VCCIO8" pad="AM30"/>
<connect gate="K" pin="VCCIO8_2" pad="AM18"/>
<connect gate="K" pin="VREFB7N0" pad="AK14"/>
<connect gate="K" pin="VREFB8N0" pad="AK31"/>
<connect gate="K" pin="VREFB8N1" pad="AJ24"/>
<connect gate="K" pin="VREFB8N2" pad="AK19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S60F1020C5N"/>
<attribute name="OC_FARNELL" value="1637238"/>
<attribute name="OC_NEWARK" value="51R0588"/>
<attribute name="PACKAGE" value="BGA-1020"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2S90F1020C5N">
<description>FPGA, STRATIX II</description>
<gates>
<gate name="A" symbol="EP2S90F1020C5N_A"/>
<gate name="B" symbol="EP2S90F1020C5N_B"/>
<gate name="C" symbol="EP2S90F1020C5N_C"/>
<gate name="D" symbol="EP2S90F1020C5N_D"/>
<gate name="E" symbol="EP2S90F1020C5N_E"/>
<gate name="F" symbol="EP2S90F1020C5N_F"/>
<gate name="G" symbol="EP2S90F1020C5N_G"/>
<gate name="H" symbol="EP2S90F1020C5N_H"/>
<gate name="I" symbol="EP2S90F1020C5N_I"/>
<gate name="J" symbol="EP2S90F1020C5N_J"/>
<gate name="K" symbol="EP2S90F1020C5N_K"/>
</gates>
<devices>
<device name="" package="BGA1020C32X32X100C_3300X3300X3">
<connects>
<connect gate="A" pin="FPLL10CLKN" pad="D4"/>
<connect gate="A" pin="FPLL10CLKP" pad="D3"/>
<connect gate="A" pin="GND" pad="A2"/>
<connect gate="A" pin="GNDA_PLL10" pad="G8"/>
<connect gate="A" pin="GNDA_PLL10_2" pad="G7"/>
<connect gate="A" pin="GND_2" pad="F7"/>
<connect gate="A" pin="GND_3" pad="K5"/>
<connect gate="A" pin="GND_4" pad="B1"/>
<connect gate="A" pin="IO" pad="L4"/>
<connect gate="A" pin="IO_10" pad="B6"/>
<connect gate="A" pin="IO_11" pad="B7"/>
<connect gate="A" pin="IO_12" pad="B8"/>
<connect gate="A" pin="IO_13" pad="B9"/>
<connect gate="A" pin="IO_14" pad="C4"/>
<connect gate="A" pin="IO_15" pad="C5"/>
<connect gate="A" pin="IO_16" pad="C6"/>
<connect gate="A" pin="IO_17" pad="C7"/>
<connect gate="A" pin="IO_18" pad="C8"/>
<connect gate="A" pin="IO_19" pad="C9"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="D1"/>
<connect gate="A" pin="IO_21" pad="D2"/>
<connect gate="A" pin="IO_22" pad="D5"/>
<connect gate="A" pin="IO_23" pad="D6"/>
<connect gate="A" pin="IO_24" pad="D7"/>
<connect gate="A" pin="IO_25" pad="D8"/>
<connect gate="A" pin="IO_26" pad="E1"/>
<connect gate="A" pin="IO_27" pad="E2"/>
<connect gate="A" pin="IO_28" pad="E3"/>
<connect gate="A" pin="IO_29" pad="E4"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="E5"/>
<connect gate="A" pin="IO_31" pad="E6"/>
<connect gate="A" pin="IO_32" pad="E7"/>
<connect gate="A" pin="IO_33" pad="E8"/>
<connect gate="A" pin="IO_34" pad="E9"/>
<connect gate="A" pin="IO_35" pad="F1"/>
<connect gate="A" pin="IO_36" pad="F2"/>
<connect gate="A" pin="IO_37" pad="F3"/>
<connect gate="A" pin="IO_38" pad="F4"/>
<connect gate="A" pin="IO_39" pad="F8"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="F9"/>
<connect gate="A" pin="IO_41" pad="G1"/>
<connect gate="A" pin="IO_42" pad="G2"/>
<connect gate="A" pin="IO_43" pad="G3"/>
<connect gate="A" pin="IO_44" pad="G4"/>
<connect gate="A" pin="IO_45" pad="G5"/>
<connect gate="A" pin="IO_46" pad="G6"/>
<connect gate="A" pin="IO_47" pad="H1"/>
<connect gate="A" pin="IO_48" pad="H2"/>
<connect gate="A" pin="IO_49" pad="H3"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="H4"/>
<connect gate="A" pin="IO_51" pad="H5"/>
<connect gate="A" pin="IO_52" pad="H6"/>
<connect gate="A" pin="IO_53" pad="H9"/>
<connect gate="A" pin="IO_54" pad="J1"/>
<connect gate="A" pin="IO_55" pad="J2"/>
<connect gate="A" pin="IO_56" pad="J3"/>
<connect gate="A" pin="IO_57" pad="J4"/>
<connect gate="A" pin="IO_58" pad="J6"/>
<connect gate="A" pin="IO_59" pad="J7"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_60" pad="J8"/>
<connect gate="A" pin="IO_61" pad="J9"/>
<connect gate="A" pin="IO_62" pad="K1"/>
<connect gate="A" pin="IO_63" pad="K2"/>
<connect gate="A" pin="IO_64" pad="K3"/>
<connect gate="A" pin="IO_65" pad="K4"/>
<connect gate="A" pin="IO_66" pad="K6"/>
<connect gate="A" pin="IO_67" pad="K7"/>
<connect gate="A" pin="IO_68" pad="K8"/>
<connect gate="A" pin="IO_69" pad="K9"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_70" pad="L1"/>
<connect gate="A" pin="IO_71" pad="L2"/>
<connect gate="A" pin="IO_72" pad="L3"/>
<connect gate="A" pin="IO_8" pad="B4"/>
<connect gate="A" pin="IO_9" pad="B5"/>
<connect gate="A" pin="MSEL0" pad="B2"/>
<connect gate="A" pin="MSEL1" pad="F6"/>
<connect gate="A" pin="TDO" pad="C3"/>
<connect gate="A" pin="TEMPDIODEN" pad="B3"/>
<connect gate="A" pin="TEMPDIODEP" pad="G9"/>
<connect gate="A" pin="VCCA_PLL10" pad="H8"/>
<connect gate="A" pin="VCCD_PLL10" pad="H7"/>
<connect gate="A" pin="VCCIO4" pad="A3"/>
<connect gate="A" pin="VCCIO5" pad="C1"/>
<connect gate="A" pin="VREFB4N0" pad="C2"/>
<connect gate="A" pin="VREFB4N1" pad="D9"/>
<connect gate="A" pin="VREFB5N1" pad="J5"/>
<connect gate="A" pin="VREFB5N2" pad="F5"/>
<connect gate="B" pin="CLK11N" pad="T4"/>
<connect gate="B" pin="CLK11P" pad="T3"/>
<connect gate="B" pin="CLK9N" pad="U4"/>
<connect gate="B" pin="CLK9P" pad="U3"/>
<connect gate="B" pin="GND" pad="N1"/>
<connect gate="B" pin="GNDA_PLL3" pad="V8"/>
<connect gate="B" pin="GNDA_PLL3_2" pad="U8"/>
<connect gate="B" pin="GNDA_PLL4" pad="T8"/>
<connect gate="B" pin="GNDA_PLL4_2" pad="R8"/>
<connect gate="B" pin="GND_2" pad="Y1"/>
<connect gate="B" pin="GND_3" pad="A13"/>
<connect gate="B" pin="GND_4" pad="T7"/>
<connect gate="B" pin="IO" pad="A16"/>
<connect gate="B" pin="IO_10" pad="M4"/>
<connect gate="B" pin="IO_11" pad="M6"/>
<connect gate="B" pin="IO_12" pad="M7"/>
<connect gate="B" pin="IO_13" pad="M8"/>
<connect gate="B" pin="IO_14" pad="M9"/>
<connect gate="B" pin="IO_15" pad="N2"/>
<connect gate="B" pin="IO_16" pad="N3"/>
<connect gate="B" pin="IO_17" pad="N4"/>
<connect gate="B" pin="IO_18" pad="N5"/>
<connect gate="B" pin="IO_19" pad="N6"/>
<connect gate="B" pin="IO_2" pad="L5"/>
<connect gate="B" pin="IO_20" pad="N7"/>
<connect gate="B" pin="IO_21" pad="N8"/>
<connect gate="B" pin="IO_22" pad="N9"/>
<connect gate="B" pin="IO_23" pad="P1"/>
<connect gate="B" pin="IO_24" pad="P2"/>
<connect gate="B" pin="IO_25" pad="P4"/>
<connect gate="B" pin="IO_26" pad="P5"/>
<connect gate="B" pin="IO_27" pad="P6"/>
<connect gate="B" pin="IO_28" pad="P7"/>
<connect gate="B" pin="IO_29" pad="P8"/>
<connect gate="B" pin="IO_3" pad="L6"/>
<connect gate="B" pin="IO_30" pad="P9"/>
<connect gate="B" pin="IO_31" pad="R2"/>
<connect gate="B" pin="IO_32" pad="R3"/>
<connect gate="B" pin="IO_33" pad="R4"/>
<connect gate="B" pin="IO_34" pad="R5"/>
<connect gate="B" pin="IO_35" pad="R6"/>
<connect gate="B" pin="IO_36" pad="R7"/>
<connect gate="B" pin="IO_37" pad="T1"/>
<connect gate="B" pin="IO_38" pad="T2"/>
<connect gate="B" pin="IO_39" pad="T5"/>
<connect gate="B" pin="IO_4" pad="L7"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="U1"/>
<connect gate="B" pin="IO_42" pad="U2"/>
<connect gate="B" pin="IO_43" pad="U5"/>
<connect gate="B" pin="IO_44" pad="U6"/>
<connect gate="B" pin="IO_45" pad="V2"/>
<connect gate="B" pin="IO_46" pad="V3"/>
<connect gate="B" pin="IO_47" pad="V4"/>
<connect gate="B" pin="IO_48" pad="V5"/>
<connect gate="B" pin="IO_49" pad="V6"/>
<connect gate="B" pin="IO_5" pad="L8"/>
<connect gate="B" pin="IO_50" pad="V7"/>
<connect gate="B" pin="IO_51" pad="V9"/>
<connect gate="B" pin="IO_52" pad="W1"/>
<connect gate="B" pin="IO_53" pad="W2"/>
<connect gate="B" pin="IO_54" pad="W4"/>
<connect gate="B" pin="IO_55" pad="W5"/>
<connect gate="B" pin="IO_56" pad="W6"/>
<connect gate="B" pin="IO_57" pad="W7"/>
<connect gate="B" pin="IO_58" pad="W8"/>
<connect gate="B" pin="IO_59" pad="W9"/>
<connect gate="B" pin="IO_6" pad="L9"/>
<connect gate="B" pin="IO_60" pad="Y2"/>
<connect gate="B" pin="IO_61" pad="Y3"/>
<connect gate="B" pin="IO_62" pad="Y4"/>
<connect gate="B" pin="IO_63" pad="Y5"/>
<connect gate="B" pin="IO_64" pad="Y6"/>
<connect gate="B" pin="IO_65" pad="Y7"/>
<connect gate="B" pin="IO_66" pad="Y8"/>
<connect gate="B" pin="IO_67" pad="Y9"/>
<connect gate="B" pin="IO_68" pad="A10"/>
<connect gate="B" pin="IO_69" pad="A11"/>
<connect gate="B" pin="IO_7" pad="M1"/>
<connect gate="B" pin="IO_70" pad="A12"/>
<connect gate="B" pin="IO_71" pad="A14"/>
<connect gate="B" pin="IO_8" pad="M2"/>
<connect gate="B" pin="IO_9" pad="M3"/>
<connect gate="B" pin="VCCA_PLL3" pad="U9"/>
<connect gate="B" pin="VCCA_PLL4" pad="R9"/>
<connect gate="B" pin="VCCD_PLL3" pad="U7"/>
<connect gate="B" pin="VCCD_PLL4" pad="T9"/>
<connect gate="B" pin="VCCIO4" pad="A15"/>
<connect gate="B" pin="VCCIO5" pad="R1"/>
<connect gate="B" pin="VCCIO5_2" pad="M5"/>
<connect gate="B" pin="VCCIO6" pad="V1"/>
<connect gate="B" pin="VREFB5N0" pad="P3"/>
<connect gate="B" pin="VREFB6N2" pad="W3"/>
<connect gate="C" pin="FPLL9CLKN" pad="AJ4"/>
<connect gate="C" pin="FPLL9CLKP" pad="AJ3"/>
<connect gate="C" pin="GND" pad="AG6"/>
<connect gate="C" pin="GNDA_PLL9" pad="AG7"/>
<connect gate="C" pin="GNDA_PLL9_2" pad="AF7"/>
<connect gate="C" pin="GND_2" pad="A20"/>
<connect gate="C" pin="GND_3" pad="A31"/>
<connect gate="C" pin="GND_4" pad="AC5"/>
<connect gate="C" pin="GND_5" pad="AF9"/>
<connect gate="C" pin="IO" pad="AJ6"/>
<connect gate="C" pin="IO_10" pad="A27"/>
<connect gate="C" pin="IO_11" pad="A28"/>
<connect gate="C" pin="IO_12" pad="A29"/>
<connect gate="C" pin="IO_13" pad="AA1"/>
<connect gate="C" pin="IO_14" pad="AA2"/>
<connect gate="C" pin="IO_15" pad="AA3"/>
<connect gate="C" pin="IO_16" pad="AA4"/>
<connect gate="C" pin="IO_17" pad="AA6"/>
<connect gate="C" pin="IO_18" pad="AA7"/>
<connect gate="C" pin="IO_19" pad="AA8"/>
<connect gate="C" pin="IO_2" pad="A17"/>
<connect gate="C" pin="IO_20" pad="AA9"/>
<connect gate="C" pin="IO_21" pad="AB1"/>
<connect gate="C" pin="IO_22" pad="AB2"/>
<connect gate="C" pin="IO_23" pad="AB3"/>
<connect gate="C" pin="IO_24" pad="AB4"/>
<connect gate="C" pin="IO_25" pad="AB5"/>
<connect gate="C" pin="IO_26" pad="AB6"/>
<connect gate="C" pin="IO_27" pad="AB7"/>
<connect gate="C" pin="IO_28" pad="AB8"/>
<connect gate="C" pin="IO_29" pad="AB9"/>
<connect gate="C" pin="IO_3" pad="A19"/>
<connect gate="C" pin="IO_30" pad="AC1"/>
<connect gate="C" pin="IO_31" pad="AC2"/>
<connect gate="C" pin="IO_32" pad="AC3"/>
<connect gate="C" pin="IO_33" pad="AC4"/>
<connect gate="C" pin="IO_34" pad="AC6"/>
<connect gate="C" pin="IO_35" pad="AC7"/>
<connect gate="C" pin="IO_36" pad="AC8"/>
<connect gate="C" pin="IO_37" pad="AC9"/>
<connect gate="C" pin="IO_38" pad="AD1"/>
<connect gate="C" pin="IO_39" pad="AD2"/>
<connect gate="C" pin="IO_4" pad="A21"/>
<connect gate="C" pin="IO_40" pad="AD3"/>
<connect gate="C" pin="IO_41" pad="AD4"/>
<connect gate="C" pin="IO_42" pad="AD6"/>
<connect gate="C" pin="IO_43" pad="AD7"/>
<connect gate="C" pin="IO_44" pad="AD8"/>
<connect gate="C" pin="IO_45" pad="AD9"/>
<connect gate="C" pin="IO_46" pad="AE1"/>
<connect gate="C" pin="IO_47" pad="AE2"/>
<connect gate="C" pin="IO_48" pad="AE3"/>
<connect gate="C" pin="IO_49" pad="AE4"/>
<connect gate="C" pin="IO_5" pad="A22"/>
<connect gate="C" pin="IO_50" pad="AE5"/>
<connect gate="C" pin="IO_51" pad="AE6"/>
<connect gate="C" pin="IO_52" pad="AE9"/>
<connect gate="C" pin="IO_53" pad="AF1"/>
<connect gate="C" pin="IO_54" pad="AF2"/>
<connect gate="C" pin="IO_55" pad="AF3"/>
<connect gate="C" pin="IO_56" pad="AF4"/>
<connect gate="C" pin="IO_57" pad="AF5"/>
<connect gate="C" pin="IO_58" pad="AF6"/>
<connect gate="C" pin="IO_59" pad="AG1"/>
<connect gate="C" pin="IO_6" pad="A23"/>
<connect gate="C" pin="IO_60" pad="AG2"/>
<connect gate="C" pin="IO_61" pad="AG3"/>
<connect gate="C" pin="IO_62" pad="AG4"/>
<connect gate="C" pin="IO_63" pad="AG8"/>
<connect gate="C" pin="IO_64" pad="AG9"/>
<connect gate="C" pin="IO_65" pad="AH1"/>
<connect gate="C" pin="IO_66" pad="AH2"/>
<connect gate="C" pin="IO_67" pad="AH3"/>
<connect gate="C" pin="IO_68" pad="AH4"/>
<connect gate="C" pin="IO_69" pad="AH5"/>
<connect gate="C" pin="IO_7" pad="A24"/>
<connect gate="C" pin="IO_70" pad="AH6"/>
<connect gate="C" pin="IO_71" pad="AH7"/>
<connect gate="C" pin="IO_72" pad="AH8"/>
<connect gate="C" pin="IO_73" pad="AH9"/>
<connect gate="C" pin="IO_74" pad="AJ1"/>
<connect gate="C" pin="IO_75" pad="AJ2"/>
<connect gate="C" pin="IO_76" pad="AJ5"/>
<connect gate="C" pin="IO_8" pad="A25"/>
<connect gate="C" pin="IO_9" pad="A26"/>
<connect gate="C" pin="PLL_ENA" pad="AF8"/>
<connect gate="C" pin="VCCA_PLL9" pad="AE7"/>
<connect gate="C" pin="VCCD_PLL9" pad="AE8"/>
<connect gate="C" pin="VCCIO3" pad="A30"/>
<connect gate="C" pin="VCCIO3_2" pad="A18"/>
<connect gate="C" pin="VCCIO6" pad="AA5"/>
<connect gate="C" pin="VREFB6N0" pad="AG5"/>
<connect gate="C" pin="VREFB6N1" pad="AD5"/>
<connect gate="D" pin="DCLK" pad="B31"/>
<connect gate="D" pin="GND" pad="B32"/>
<connect gate="D" pin="GND_2" pad="AL1"/>
<connect gate="D" pin="GND_3" pad="AM2"/>
<connect gate="D" pin="IO" pad="D27"/>
<connect gate="D" pin="IO_10" pad="AL4"/>
<connect gate="D" pin="IO_11" pad="AL5"/>
<connect gate="D" pin="IO_12" pad="AL6"/>
<connect gate="D" pin="IO_13" pad="AL7"/>
<connect gate="D" pin="IO_14" pad="AL8"/>
<connect gate="D" pin="IO_15" pad="AL9"/>
<connect gate="D" pin="IO_16" pad="AM4"/>
<connect gate="D" pin="IO_17" pad="AM5"/>
<connect gate="D" pin="IO_18" pad="AM6"/>
<connect gate="D" pin="IO_19" pad="AM7"/>
<connect gate="D" pin="IO_2" pad="AJ7"/>
<connect gate="D" pin="IO_20" pad="AM8"/>
<connect gate="D" pin="IO_21" pad="AM9"/>
<connect gate="D" pin="IO_22" pad="B10"/>
<connect gate="D" pin="IO_23" pad="B11"/>
<connect gate="D" pin="IO_24" pad="B12"/>
<connect gate="D" pin="IO_25" pad="B13"/>
<connect gate="D" pin="IO_26" pad="B14"/>
<connect gate="D" pin="IO_27" pad="B15"/>
<connect gate="D" pin="IO_28" pad="B16"/>
<connect gate="D" pin="IO_29" pad="B17"/>
<connect gate="D" pin="IO_3" pad="AJ8"/>
<connect gate="D" pin="IO_30" pad="B18"/>
<connect gate="D" pin="IO_31" pad="B19"/>
<connect gate="D" pin="IO_32" pad="B20"/>
<connect gate="D" pin="IO_33" pad="B21"/>
<connect gate="D" pin="IO_34" pad="B22"/>
<connect gate="D" pin="IO_35" pad="B23"/>
<connect gate="D" pin="IO_36" pad="B24"/>
<connect gate="D" pin="IO_37" pad="B25"/>
<connect gate="D" pin="IO_38" pad="B26"/>
<connect gate="D" pin="IO_39" pad="B27"/>
<connect gate="D" pin="IO_4" pad="AK4"/>
<connect gate="D" pin="IO_40" pad="B28"/>
<connect gate="D" pin="IO_41" pad="B29"/>
<connect gate="D" pin="IO_42" pad="C10"/>
<connect gate="D" pin="IO_43" pad="C11"/>
<connect gate="D" pin="IO_44" pad="C12"/>
<connect gate="D" pin="IO_45" pad="C13"/>
<connect gate="D" pin="IO_46" pad="C15"/>
<connect gate="D" pin="IO_47" pad="C16"/>
<connect gate="D" pin="IO_48" pad="C17"/>
<connect gate="D" pin="IO_49" pad="C18"/>
<connect gate="D" pin="IO_5" pad="AK5"/>
<connect gate="D" pin="IO_50" pad="C20"/>
<connect gate="D" pin="IO_51" pad="C21"/>
<connect gate="D" pin="IO_52" pad="C22"/>
<connect gate="D" pin="IO_53" pad="C23"/>
<connect gate="D" pin="IO_54" pad="C24"/>
<connect gate="D" pin="IO_55" pad="C25"/>
<connect gate="D" pin="IO_56" pad="C26"/>
<connect gate="D" pin="IO_57" pad="C27"/>
<connect gate="D" pin="IO_58" pad="C28"/>
<connect gate="D" pin="IO_59" pad="C29"/>
<connect gate="D" pin="IO_6" pad="AK6"/>
<connect gate="D" pin="IO_60" pad="D10"/>
<connect gate="D" pin="IO_61" pad="D11"/>
<connect gate="D" pin="IO_62" pad="D12"/>
<connect gate="D" pin="IO_63" pad="D13"/>
<connect gate="D" pin="IO_64" pad="D14"/>
<connect gate="D" pin="IO_65" pad="D15"/>
<connect gate="D" pin="IO_66" pad="D16"/>
<connect gate="D" pin="IO_67" pad="D17"/>
<connect gate="D" pin="IO_68" pad="D18"/>
<connect gate="D" pin="IO_69" pad="D19"/>
<connect gate="D" pin="IO_7" pad="AK7"/>
<connect gate="D" pin="IO_70" pad="D20"/>
<connect gate="D" pin="IO_71" pad="D21"/>
<connect gate="D" pin="IO_72" pad="D22"/>
<connect gate="D" pin="IO_73" pad="D23"/>
<connect gate="D" pin="IO_74" pad="D25"/>
<connect gate="D" pin="IO_75" pad="D26"/>
<connect gate="D" pin="IO_8" pad="AK8"/>
<connect gate="D" pin="IO_9" pad="AK9"/>
<connect gate="D" pin="NCE" pad="C30"/>
<connect gate="D" pin="NCEO" pad="AL3"/>
<connect gate="D" pin="NIO_PULLUP" pad="AK3"/>
<connect gate="D" pin="NSTATUS" pad="B30"/>
<connect gate="D" pin="PORSEL" pad="AL2"/>
<connect gate="D" pin="VCCIO2" pad="C32"/>
<connect gate="D" pin="VCCIO6" pad="AK1"/>
<connect gate="D" pin="VCCIO7" pad="AM3"/>
<connect gate="D" pin="VREFB3N0" pad="C19"/>
<connect gate="D" pin="VREFB3N1" pad="D24"/>
<connect gate="D" pin="VREFB3N2" pad="C31"/>
<connect gate="D" pin="VREFB4N2" pad="C14"/>
<connect gate="D" pin="VREFB7N1" pad="AJ9"/>
<connect gate="D" pin="VREFB7N2" pad="AK2"/>
<connect gate="E" pin="FPLL7CLKN" pad="D29"/>
<connect gate="E" pin="FPLL7CLKP" pad="D30"/>
<connect gate="E" pin="GND" pad="F27"/>
<connect gate="E" pin="GNDA_PLL11" pad="G18"/>
<connect gate="E" pin="GNDA_PLL11_2" pad="H18"/>
<connect gate="E" pin="GNDA_PLL5" pad="H16"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="G16"/>
<connect gate="E" pin="GNDA_PLL7" pad="G26"/>
<connect gate="E" pin="GNDA_PLL7_2" pad="F26"/>
<connect gate="E" pin="GND_2" pad="E10"/>
<connect gate="E" pin="GND_3" pad="E23"/>
<connect gate="E" pin="GND_4" pad="G17"/>
<connect gate="E" pin="IO" pad="H28"/>
<connect gate="E" pin="IO_10" pad="E17"/>
<connect gate="E" pin="IO_11" pad="E18"/>
<connect gate="E" pin="IO_12" pad="E19"/>
<connect gate="E" pin="IO_13" pad="E20"/>
<connect gate="E" pin="IO_14" pad="E22"/>
<connect gate="E" pin="IO_15" pad="E24"/>
<connect gate="E" pin="IO_16" pad="E25"/>
<connect gate="E" pin="IO_17" pad="E26"/>
<connect gate="E" pin="IO_18" pad="E27"/>
<connect gate="E" pin="IO_19" pad="E28"/>
<connect gate="E" pin="IO_2" pad="D28"/>
<connect gate="E" pin="IO_20" pad="E29"/>
<connect gate="E" pin="IO_21" pad="E30"/>
<connect gate="E" pin="IO_22" pad="E31"/>
<connect gate="E" pin="IO_23" pad="E32"/>
<connect gate="E" pin="IO_24" pad="F10"/>
<connect gate="E" pin="IO_25" pad="F11"/>
<connect gate="E" pin="IO_26" pad="F12"/>
<connect gate="E" pin="IO_27" pad="F13"/>
<connect gate="E" pin="IO_28" pad="F14"/>
<connect gate="E" pin="IO_29" pad="F15"/>
<connect gate="E" pin="IO_3" pad="D31"/>
<connect gate="E" pin="IO_30" pad="F16"/>
<connect gate="E" pin="IO_31" pad="F17"/>
<connect gate="E" pin="IO_32" pad="F18"/>
<connect gate="E" pin="IO_33" pad="F19"/>
<connect gate="E" pin="IO_34" pad="F20"/>
<connect gate="E" pin="IO_35" pad="F21"/>
<connect gate="E" pin="IO_36" pad="F22"/>
<connect gate="E" pin="IO_37" pad="F23"/>
<connect gate="E" pin="IO_38" pad="F24"/>
<connect gate="E" pin="IO_39" pad="F25"/>
<connect gate="E" pin="IO_4" pad="D32"/>
<connect gate="E" pin="IO_40" pad="F29"/>
<connect gate="E" pin="IO_41" pad="F30"/>
<connect gate="E" pin="IO_42" pad="F31"/>
<connect gate="E" pin="IO_43" pad="F32"/>
<connect gate="E" pin="IO_44" pad="G10"/>
<connect gate="E" pin="IO_45" pad="G11"/>
<connect gate="E" pin="IO_46" pad="G12"/>
<connect gate="E" pin="IO_47" pad="G13"/>
<connect gate="E" pin="IO_48" pad="G14"/>
<connect gate="E" pin="IO_49" pad="G19"/>
<connect gate="E" pin="IO_5" pad="E11"/>
<connect gate="E" pin="IO_50" pad="G20"/>
<connect gate="E" pin="IO_51" pad="G21"/>
<connect gate="E" pin="IO_52" pad="G22"/>
<connect gate="E" pin="IO_53" pad="G23"/>
<connect gate="E" pin="IO_54" pad="G24"/>
<connect gate="E" pin="IO_55" pad="G25"/>
<connect gate="E" pin="IO_56" pad="G27"/>
<connect gate="E" pin="IO_57" pad="G28"/>
<connect gate="E" pin="IO_58" pad="G29"/>
<connect gate="E" pin="IO_59" pad="G30"/>
<connect gate="E" pin="IO_6" pad="E13"/>
<connect gate="E" pin="IO_60" pad="G31"/>
<connect gate="E" pin="IO_61" pad="G32"/>
<connect gate="E" pin="IO_62" pad="H11"/>
<connect gate="E" pin="IO_63" pad="H12"/>
<connect gate="E" pin="IO_64" pad="H13"/>
<connect gate="E" pin="IO_65" pad="H14"/>
<connect gate="E" pin="IO_66" pad="H19"/>
<connect gate="E" pin="IO_67" pad="H20"/>
<connect gate="E" pin="IO_68" pad="H21"/>
<connect gate="E" pin="IO_69" pad="H22"/>
<connect gate="E" pin="IO_7" pad="E14"/>
<connect gate="E" pin="IO_70" pad="H23"/>
<connect gate="E" pin="IO_71" pad="H24"/>
<connect gate="E" pin="IO_72" pad="H27"/>
<connect gate="E" pin="IO_8" pad="E15"/>
<connect gate="E" pin="IO_9" pad="E16"/>
<connect gate="E" pin="MSEL3" pad="H10"/>
<connect gate="E" pin="VCCA_PLL11" pad="H17"/>
<connect gate="E" pin="VCCA_PLL5" pad="G15"/>
<connect gate="E" pin="VCCA_PLL7" pad="H26"/>
<connect gate="E" pin="VCCD_PLL5" pad="H15"/>
<connect gate="E" pin="VCCD_PLL7" pad="H25"/>
<connect gate="E" pin="VCCIO3" pad="E21"/>
<connect gate="E" pin="VCCIO4" pad="E12"/>
<connect gate="E" pin="VREFB2N0" pad="F28"/>
<connect gate="F" pin="CONF_DONE" pad="J25"/>
<connect gate="F" pin="GND" pad="M14"/>
<connect gate="F" pin="GND_2" pad="K28"/>
<connect gate="F" pin="GND_3" pad="L11"/>
<connect gate="F" pin="GND_4" pad="M19"/>
<connect gate="F" pin="GND_5" pad="J24"/>
<connect gate="F" pin="GND_6" pad="M12"/>
<connect gate="F" pin="IO" pad="M29"/>
<connect gate="F" pin="IO_10" pad="J15"/>
<connect gate="F" pin="IO_11" pad="J19"/>
<connect gate="F" pin="IO_12" pad="J20"/>
<connect gate="F" pin="IO_13" pad="J21"/>
<connect gate="F" pin="IO_14" pad="J22"/>
<connect gate="F" pin="IO_15" pad="J23"/>
<connect gate="F" pin="IO_16" pad="J26"/>
<connect gate="F" pin="IO_17" pad="J27"/>
<connect gate="F" pin="IO_18" pad="J29"/>
<connect gate="F" pin="IO_19" pad="J30"/>
<connect gate="F" pin="IO_2" pad="H29"/>
<connect gate="F" pin="IO_20" pad="J31"/>
<connect gate="F" pin="IO_21" pad="J32"/>
<connect gate="F" pin="IO_22" pad="K11"/>
<connect gate="F" pin="IO_23" pad="K12"/>
<connect gate="F" pin="IO_24" pad="K13"/>
<connect gate="F" pin="IO_25" pad="K14"/>
<connect gate="F" pin="IO_26" pad="K15"/>
<connect gate="F" pin="IO_27" pad="K16"/>
<connect gate="F" pin="IO_28" pad="K17"/>
<connect gate="F" pin="IO_29" pad="K18"/>
<connect gate="F" pin="IO_3" pad="H30"/>
<connect gate="F" pin="IO_30" pad="K19"/>
<connect gate="F" pin="IO_31" pad="K20"/>
<connect gate="F" pin="IO_32" pad="K21"/>
<connect gate="F" pin="IO_33" pad="K22"/>
<connect gate="F" pin="IO_34" pad="K24"/>
<connect gate="F" pin="IO_35" pad="K25"/>
<connect gate="F" pin="IO_36" pad="K26"/>
<connect gate="F" pin="IO_37" pad="K27"/>
<connect gate="F" pin="IO_38" pad="K29"/>
<connect gate="F" pin="IO_39" pad="K30"/>
<connect gate="F" pin="IO_4" pad="H31"/>
<connect gate="F" pin="IO_40" pad="K31"/>
<connect gate="F" pin="IO_41" pad="K32"/>
<connect gate="F" pin="IO_42" pad="L10"/>
<connect gate="F" pin="IO_43" pad="L12"/>
<connect gate="F" pin="IO_44" pad="L13"/>
<connect gate="F" pin="IO_45" pad="L14"/>
<connect gate="F" pin="IO_46" pad="L15"/>
<connect gate="F" pin="IO_47" pad="L16"/>
<connect gate="F" pin="IO_48" pad="L17"/>
<connect gate="F" pin="IO_49" pad="L18"/>
<connect gate="F" pin="IO_5" pad="H32"/>
<connect gate="F" pin="IO_50" pad="L19"/>
<connect gate="F" pin="IO_51" pad="L20"/>
<connect gate="F" pin="IO_52" pad="L21"/>
<connect gate="F" pin="IO_53" pad="L22"/>
<connect gate="F" pin="IO_54" pad="L23"/>
<connect gate="F" pin="IO_55" pad="L24"/>
<connect gate="F" pin="IO_56" pad="L25"/>
<connect gate="F" pin="IO_57" pad="L26"/>
<connect gate="F" pin="IO_58" pad="L27"/>
<connect gate="F" pin="IO_59" pad="L28"/>
<connect gate="F" pin="IO_6" pad="J11"/>
<connect gate="F" pin="IO_60" pad="L29"/>
<connect gate="F" pin="IO_61" pad="L30"/>
<connect gate="F" pin="IO_62" pad="L31"/>
<connect gate="F" pin="IO_63" pad="L32"/>
<connect gate="F" pin="IO_64" pad="M10"/>
<connect gate="F" pin="IO_65" pad="M11"/>
<connect gate="F" pin="IO_66" pad="M22"/>
<connect gate="F" pin="IO_67" pad="M23"/>
<connect gate="F" pin="IO_68" pad="M24"/>
<connect gate="F" pin="IO_69" pad="M25"/>
<connect gate="F" pin="IO_7" pad="J12"/>
<connect gate="F" pin="IO_70" pad="M26"/>
<connect gate="F" pin="IO_71" pad="M27"/>
<connect gate="F" pin="IO_8" pad="J13"/>
<connect gate="F" pin="IO_9" pad="J14"/>
<connect gate="F" pin="MSEL2" pad="J10"/>
<connect gate="F" pin="VCCD_PLL11" pad="J18"/>
<connect gate="F" pin="VCCINT" pad="K23"/>
<connect gate="F" pin="VCCINT_2" pad="K10"/>
<connect gate="F" pin="VCCINT_3" pad="M21"/>
<connect gate="F" pin="VCCIO2" pad="M28"/>
<connect gate="F" pin="VCCIO3" pad="M17"/>
<connect gate="F" pin="VCCIO4" pad="M16"/>
<connect gate="F" pin="VCCPD3" pad="M20"/>
<connect gate="F" pin="VCCPD3_2" pad="M18"/>
<connect gate="F" pin="VCCPD4" pad="M15"/>
<connect gate="F" pin="VCCPD4_2" pad="M13"/>
<connect gate="F" pin="VCC_PLL11_OUT" pad="J17"/>
<connect gate="F" pin="VCC_PLL5_OUT" pad="J16"/>
<connect gate="F" pin="VREFB2N1" pad="J28"/>
<connect gate="G" pin="CLK1N" pad="T29"/>
<connect gate="G" pin="CLK1P" pad="T30"/>
<connect gate="G" pin="GND" pad="P21"/>
<connect gate="G" pin="GNDA_PLL1" pad="T26"/>
<connect gate="G" pin="GNDA_PLL1_2" pad="T25"/>
<connect gate="G" pin="GND_10" pad="R16"/>
<connect gate="G" pin="GND_11" pad="T17"/>
<connect gate="G" pin="GND_12" pad="P17"/>
<connect gate="G" pin="GND_13" pad="R20"/>
<connect gate="G" pin="GND_14" pad="P12"/>
<connect gate="G" pin="GND_15" pad="T19"/>
<connect gate="G" pin="GND_16" pad="R18"/>
<connect gate="G" pin="GND_17" pad="P13"/>
<connect gate="G" pin="GND_18" pad="T13"/>
<connect gate="G" pin="GND_19" pad="P19"/>
<connect gate="G" pin="GND_2" pad="N16"/>
<connect gate="G" pin="GND_3" pad="N20"/>
<connect gate="G" pin="GND_4" pad="N14"/>
<connect gate="G" pin="GND_5" pad="P15"/>
<connect gate="G" pin="GND_6" pad="R14"/>
<connect gate="G" pin="GND_7" pad="N18"/>
<connect gate="G" pin="GND_8" pad="T15"/>
<connect gate="G" pin="GND_9" pad="N32"/>
<connect gate="G" pin="IO" pad="T28"/>
<connect gate="G" pin="IO_10" pad="N25"/>
<connect gate="G" pin="IO_11" pad="N26"/>
<connect gate="G" pin="IO_12" pad="N27"/>
<connect gate="G" pin="IO_13" pad="N28"/>
<connect gate="G" pin="IO_14" pad="N29"/>
<connect gate="G" pin="IO_15" pad="N30"/>
<connect gate="G" pin="IO_16" pad="N31"/>
<connect gate="G" pin="IO_17" pad="P10"/>
<connect gate="G" pin="IO_18" pad="P11"/>
<connect gate="G" pin="IO_19" pad="P22"/>
<connect gate="G" pin="IO_2" pad="M30"/>
<connect gate="G" pin="IO_20" pad="P23"/>
<connect gate="G" pin="IO_21" pad="P24"/>
<connect gate="G" pin="IO_22" pad="P25"/>
<connect gate="G" pin="IO_23" pad="P26"/>
<connect gate="G" pin="IO_24" pad="P27"/>
<connect gate="G" pin="IO_25" pad="P28"/>
<connect gate="G" pin="IO_26" pad="P29"/>
<connect gate="G" pin="IO_27" pad="P31"/>
<connect gate="G" pin="IO_28" pad="P32"/>
<connect gate="G" pin="IO_29" pad="R10"/>
<connect gate="G" pin="IO_3" pad="M31"/>
<connect gate="G" pin="IO_30" pad="R11"/>
<connect gate="G" pin="IO_31" pad="R22"/>
<connect gate="G" pin="IO_32" pad="R23"/>
<connect gate="G" pin="IO_33" pad="R24"/>
<connect gate="G" pin="IO_34" pad="R25"/>
<connect gate="G" pin="IO_35" pad="R26"/>
<connect gate="G" pin="IO_36" pad="R27"/>
<connect gate="G" pin="IO_37" pad="R28"/>
<connect gate="G" pin="IO_38" pad="R29"/>
<connect gate="G" pin="IO_39" pad="R30"/>
<connect gate="G" pin="IO_4" pad="M32"/>
<connect gate="G" pin="IO_40" pad="R31"/>
<connect gate="G" pin="IO_41" pad="T10"/>
<connect gate="G" pin="IO_42" pad="T11"/>
<connect gate="G" pin="IO_43" pad="T22"/>
<connect gate="G" pin="IO_44" pad="T23"/>
<connect gate="G" pin="IO_45" pad="T27"/>
<connect gate="G" pin="IO_5" pad="N10"/>
<connect gate="G" pin="IO_6" pad="N11"/>
<connect gate="G" pin="IO_7" pad="N22"/>
<connect gate="G" pin="IO_8" pad="N23"/>
<connect gate="G" pin="IO_9" pad="N24"/>
<connect gate="G" pin="VCCA_PLL1" pad="T24"/>
<connect gate="G" pin="VCCINT" pad="N15"/>
<connect gate="G" pin="VCCINT_10" pad="T18"/>
<connect gate="G" pin="VCCINT_11" pad="T16"/>
<connect gate="G" pin="VCCINT_12" pad="T14"/>
<connect gate="G" pin="VCCINT_13" pad="N17"/>
<connect gate="G" pin="VCCINT_14" pad="P20"/>
<connect gate="G" pin="VCCINT_15" pad="T20"/>
<connect gate="G" pin="VCCINT_16" pad="R15"/>
<connect gate="G" pin="VCCINT_2" pad="N13"/>
<connect gate="G" pin="VCCINT_3" pad="P16"/>
<connect gate="G" pin="VCCINT_4" pad="R13"/>
<connect gate="G" pin="VCCINT_5" pad="P18"/>
<connect gate="G" pin="VCCINT_6" pad="N19"/>
<connect gate="G" pin="VCCINT_7" pad="P14"/>
<connect gate="G" pin="VCCINT_8" pad="R17"/>
<connect gate="G" pin="VCCINT_9" pad="R19"/>
<connect gate="G" pin="VCCIO2" pad="R32"/>
<connect gate="G" pin="VCCIO2_2" pad="T21"/>
<connect gate="G" pin="VCCIO5" pad="T12"/>
<connect gate="G" pin="VCCPD2" pad="R21"/>
<connect gate="G" pin="VCCPD2_2" pad="N21"/>
<connect gate="G" pin="VCCPD5" pad="R12"/>
<connect gate="G" pin="VCCPD5_2" pad="N12"/>
<connect gate="G" pin="VREFB2N2" pad="P30"/>
<connect gate="H" pin="CLK3N" pad="U29"/>
<connect gate="H" pin="CLK3P" pad="U30"/>
<connect gate="H" pin="GND" pad="V17"/>
<connect gate="H" pin="GNDA_PLL2" pad="U26"/>
<connect gate="H" pin="GNDA_PLL2_2" pad="U25"/>
<connect gate="H" pin="GND_10" pad="V13"/>
<connect gate="H" pin="GND_11" pad="Y15"/>
<connect gate="H" pin="GND_12" pad="U18"/>
<connect gate="H" pin="GND_13" pad="Y17"/>
<connect gate="H" pin="GND_14" pad="V19"/>
<connect gate="H" pin="GND_15" pad="V22"/>
<connect gate="H" pin="GND_16" pad="U14"/>
<connect gate="H" pin="GND_17" pad="V11"/>
<connect gate="H" pin="GND_18" pad="V27"/>
<connect gate="H" pin="GND_19" pad="V15"/>
<connect gate="H" pin="GND_2" pad="U16"/>
<connect gate="H" pin="GND_20" pad="U20"/>
<connect gate="H" pin="GND_3" pad="W16"/>
<connect gate="H" pin="GND_4" pad="W14"/>
<connect gate="H" pin="GND_5" pad="W18"/>
<connect gate="H" pin="GND_6" pad="W12"/>
<connect gate="H" pin="GND_7" pad="Y13"/>
<connect gate="H" pin="GND_8" pad="W20"/>
<connect gate="H" pin="GND_9" pad="Y19"/>
<connect gate="H" pin="IO" pad="Y31"/>
<connect gate="H" pin="IO_10" pad="U31"/>
<connect gate="H" pin="IO_11" pad="U32"/>
<connect gate="H" pin="IO_12" pad="V10"/>
<connect gate="H" pin="IO_13" pad="V23"/>
<connect gate="H" pin="IO_14" pad="V24"/>
<connect gate="H" pin="IO_15" pad="V28"/>
<connect gate="H" pin="IO_16" pad="V29"/>
<connect gate="H" pin="IO_17" pad="V30"/>
<connect gate="H" pin="IO_18" pad="V31"/>
<connect gate="H" pin="IO_19" pad="W10"/>
<connect gate="H" pin="IO_2" pad="T31"/>
<connect gate="H" pin="IO_20" pad="W11"/>
<connect gate="H" pin="IO_21" pad="W22"/>
<connect gate="H" pin="IO_22" pad="W23"/>
<connect gate="H" pin="IO_23" pad="W24"/>
<connect gate="H" pin="IO_24" pad="W25"/>
<connect gate="H" pin="IO_25" pad="W26"/>
<connect gate="H" pin="IO_26" pad="W27"/>
<connect gate="H" pin="IO_27" pad="W28"/>
<connect gate="H" pin="IO_28" pad="W29"/>
<connect gate="H" pin="IO_29" pad="W31"/>
<connect gate="H" pin="IO_3" pad="T32"/>
<connect gate="H" pin="IO_30" pad="W32"/>
<connect gate="H" pin="IO_31" pad="Y10"/>
<connect gate="H" pin="IO_32" pad="Y11"/>
<connect gate="H" pin="IO_33" pad="Y22"/>
<connect gate="H" pin="IO_34" pad="Y23"/>
<connect gate="H" pin="IO_35" pad="Y24"/>
<connect gate="H" pin="IO_36" pad="Y25"/>
<connect gate="H" pin="IO_37" pad="Y26"/>
<connect gate="H" pin="IO_38" pad="Y27"/>
<connect gate="H" pin="IO_39" pad="Y28"/>
<connect gate="H" pin="IO_4" pad="U10"/>
<connect gate="H" pin="IO_40" pad="Y29"/>
<connect gate="H" pin="IO_41" pad="Y30"/>
<connect gate="H" pin="IO_5" pad="U11"/>
<connect gate="H" pin="IO_6" pad="U22"/>
<connect gate="H" pin="IO_7" pad="U23"/>
<connect gate="H" pin="IO_8" pad="U27"/>
<connect gate="H" pin="IO_9" pad="U28"/>
<connect gate="H" pin="VCCA_PLL2" pad="V26"/>
<connect gate="H" pin="VCCD_PLL1" pad="U24"/>
<connect gate="H" pin="VCCD_PLL2" pad="V25"/>
<connect gate="H" pin="VCCINT" pad="W21"/>
<connect gate="H" pin="VCCINT_10" pad="Y14"/>
<connect gate="H" pin="VCCINT_11" pad="Y16"/>
<connect gate="H" pin="VCCINT_12" pad="Y18"/>
<connect gate="H" pin="VCCINT_13" pad="W19"/>
<connect gate="H" pin="VCCINT_14" pad="V20"/>
<connect gate="H" pin="VCCINT_15" pad="U17"/>
<connect gate="H" pin="VCCINT_16" pad="Y20"/>
<connect gate="H" pin="VCCINT_17" pad="W15"/>
<connect gate="H" pin="VCCINT_2" pad="U13"/>
<connect gate="H" pin="VCCINT_3" pad="U15"/>
<connect gate="H" pin="VCCINT_4" pad="U19"/>
<connect gate="H" pin="VCCINT_5" pad="V14"/>
<connect gate="H" pin="VCCINT_6" pad="W13"/>
<connect gate="H" pin="VCCINT_7" pad="V18"/>
<connect gate="H" pin="VCCINT_8" pad="V16"/>
<connect gate="H" pin="VCCINT_9" pad="W17"/>
<connect gate="H" pin="VCCIO1" pad="V32"/>
<connect gate="H" pin="VCCIO1_2" pad="U21"/>
<connect gate="H" pin="VCCIO6" pad="U12"/>
<connect gate="H" pin="VCCPD1" pad="Y21"/>
<connect gate="H" pin="VCCPD1_2" pad="V21"/>
<connect gate="H" pin="VCCPD6" pad="V12"/>
<connect gate="H" pin="VCCPD6_2" pad="Y12"/>
<connect gate="H" pin="VREFB1N0" pad="W30"/>
<connect gate="I" pin="GND" pad="AB22"/>
<connect gate="I" pin="GNDA_PLL12" pad="AD17"/>
<connect gate="I" pin="GNDA_PLL6" pad="AD16"/>
<connect gate="I" pin="GND_2" pad="AA19"/>
<connect gate="I" pin="GND_3" pad="Y32"/>
<connect gate="I" pin="GND_4" pad="AA14"/>
<connect gate="I" pin="GND_5" pad="AA21"/>
<connect gate="I" pin="GND_6" pad="AC28"/>
<connect gate="I" pin="IO" pad="AD32"/>
<connect gate="I" pin="IO_10" pad="AA29"/>
<connect gate="I" pin="IO_11" pad="AA30"/>
<connect gate="I" pin="IO_12" pad="AA31"/>
<connect gate="I" pin="IO_13" pad="AA32"/>
<connect gate="I" pin="IO_14" pad="AB10"/>
<connect gate="I" pin="IO_15" pad="AB11"/>
<connect gate="I" pin="IO_16" pad="AB12"/>
<connect gate="I" pin="IO_17" pad="AB13"/>
<connect gate="I" pin="IO_18" pad="AB14"/>
<connect gate="I" pin="IO_19" pad="AB15"/>
<connect gate="I" pin="IO_2" pad="AA10"/>
<connect gate="I" pin="IO_20" pad="AB16"/>
<connect gate="I" pin="IO_21" pad="AB17"/>
<connect gate="I" pin="IO_22" pad="AB18"/>
<connect gate="I" pin="IO_23" pad="AB19"/>
<connect gate="I" pin="IO_24" pad="AB20"/>
<connect gate="I" pin="IO_25" pad="AB21"/>
<connect gate="I" pin="IO_26" pad="AB23"/>
<connect gate="I" pin="IO_27" pad="AB24"/>
<connect gate="I" pin="IO_28" pad="AB25"/>
<connect gate="I" pin="IO_29" pad="AB26"/>
<connect gate="I" pin="IO_3" pad="AA11"/>
<connect gate="I" pin="IO_30" pad="AB27"/>
<connect gate="I" pin="IO_31" pad="AB28"/>
<connect gate="I" pin="IO_32" pad="AB29"/>
<connect gate="I" pin="IO_33" pad="AB30"/>
<connect gate="I" pin="IO_34" pad="AB31"/>
<connect gate="I" pin="IO_35" pad="AB32"/>
<connect gate="I" pin="IO_36" pad="AC11"/>
<connect gate="I" pin="IO_37" pad="AC12"/>
<connect gate="I" pin="IO_38" pad="AC13"/>
<connect gate="I" pin="IO_39" pad="AC14"/>
<connect gate="I" pin="IO_4" pad="AA22"/>
<connect gate="I" pin="IO_40" pad="AC15"/>
<connect gate="I" pin="IO_41" pad="AC16"/>
<connect gate="I" pin="IO_42" pad="AC17"/>
<connect gate="I" pin="IO_43" pad="AC18"/>
<connect gate="I" pin="IO_44" pad="AC19"/>
<connect gate="I" pin="IO_45" pad="AC20"/>
<connect gate="I" pin="IO_46" pad="AC21"/>
<connect gate="I" pin="IO_47" pad="AC22"/>
<connect gate="I" pin="IO_48" pad="AC24"/>
<connect gate="I" pin="IO_49" pad="AC25"/>
<connect gate="I" pin="IO_5" pad="AA23"/>
<connect gate="I" pin="IO_50" pad="AC26"/>
<connect gate="I" pin="IO_51" pad="AC27"/>
<connect gate="I" pin="IO_52" pad="AC29"/>
<connect gate="I" pin="IO_53" pad="AC30"/>
<connect gate="I" pin="IO_54" pad="AC31"/>
<connect gate="I" pin="IO_55" pad="AC32"/>
<connect gate="I" pin="IO_56" pad="AD10"/>
<connect gate="I" pin="IO_57" pad="AD11"/>
<connect gate="I" pin="IO_58" pad="AD12"/>
<connect gate="I" pin="IO_59" pad="AD13"/>
<connect gate="I" pin="IO_6" pad="AA24"/>
<connect gate="I" pin="IO_60" pad="AD14"/>
<connect gate="I" pin="IO_61" pad="AD18"/>
<connect gate="I" pin="IO_62" pad="AD19"/>
<connect gate="I" pin="IO_63" pad="AD20"/>
<connect gate="I" pin="IO_64" pad="AD21"/>
<connect gate="I" pin="IO_65" pad="AD22"/>
<connect gate="I" pin="IO_66" pad="AD23"/>
<connect gate="I" pin="IO_67" pad="AD24"/>
<connect gate="I" pin="IO_68" pad="AD25"/>
<connect gate="I" pin="IO_69" pad="AD26"/>
<connect gate="I" pin="IO_7" pad="AA25"/>
<connect gate="I" pin="IO_70" pad="AD27"/>
<connect gate="I" pin="IO_71" pad="AD29"/>
<connect gate="I" pin="IO_72" pad="AD30"/>
<connect gate="I" pin="IO_73" pad="AD31"/>
<connect gate="I" pin="IO_8" pad="AA26"/>
<connect gate="I" pin="IO_9" pad="AA27"/>
<connect gate="I" pin="VCCD_PLL6" pad="AD15"/>
<connect gate="I" pin="VCCINT" pad="AC10"/>
<connect gate="I" pin="VCCINT_2" pad="AA12"/>
<connect gate="I" pin="VCCIO1" pad="AA28"/>
<connect gate="I" pin="VCCIO7" pad="AA16"/>
<connect gate="I" pin="VCCIO8" pad="AA17"/>
<connect gate="I" pin="VCCPD7" pad="AA13"/>
<connect gate="I" pin="VCCPD7_2" pad="AA15"/>
<connect gate="I" pin="VCCPD8" pad="AA20"/>
<connect gate="I" pin="VCCPD8_2" pad="AA18"/>
<connect gate="I" pin="VCCSEL" pad="AC23"/>
<connect gate="I" pin="VREFB1N1" pad="AD28"/>
<connect gate="J" pin="GND" pad="AH27"/>
<connect gate="J" pin="GNDA_PLL12" pad="AE17"/>
<connect gate="J" pin="GNDA_PLL6" pad="AE16"/>
<connect gate="J" pin="GNDA_PLL8" pad="AG27"/>
<connect gate="J" pin="GNDA_PLL8_2" pad="AG26"/>
<connect gate="J" pin="GND_2" pad="AF17"/>
<connect gate="J" pin="GND_3" pad="AH10"/>
<connect gate="J" pin="GND_4" pad="AH23"/>
<connect gate="J" pin="IO" pad="AJ10"/>
<connect gate="J" pin="IO_10" pad="AE22"/>
<connect gate="J" pin="IO_11" pad="AE23"/>
<connect gate="J" pin="IO_12" pad="AE25"/>
<connect gate="J" pin="IO_13" pad="AE26"/>
<connect gate="J" pin="IO_14" pad="AE27"/>
<connect gate="J" pin="IO_15" pad="AE28"/>
<connect gate="J" pin="IO_16" pad="AE29"/>
<connect gate="J" pin="IO_17" pad="AE30"/>
<connect gate="J" pin="IO_18" pad="AE31"/>
<connect gate="J" pin="IO_19" pad="AE32"/>
<connect gate="J" pin="IO_2" pad="AE10"/>
<connect gate="J" pin="IO_20" pad="AF10"/>
<connect gate="J" pin="IO_21" pad="AF11"/>
<connect gate="J" pin="IO_22" pad="AF12"/>
<connect gate="J" pin="IO_23" pad="AF13"/>
<connect gate="J" pin="IO_24" pad="AF14"/>
<connect gate="J" pin="IO_25" pad="AF19"/>
<connect gate="J" pin="IO_26" pad="AF20"/>
<connect gate="J" pin="IO_27" pad="AF21"/>
<connect gate="J" pin="IO_28" pad="AF22"/>
<connect gate="J" pin="IO_29" pad="AF23"/>
<connect gate="J" pin="IO_3" pad="AE11"/>
<connect gate="J" pin="IO_30" pad="AF27"/>
<connect gate="J" pin="IO_31" pad="AF28"/>
<connect gate="J" pin="IO_32" pad="AF29"/>
<connect gate="J" pin="IO_33" pad="AF30"/>
<connect gate="J" pin="IO_34" pad="AF31"/>
<connect gate="J" pin="IO_35" pad="AF32"/>
<connect gate="J" pin="IO_36" pad="AG10"/>
<connect gate="J" pin="IO_37" pad="AG11"/>
<connect gate="J" pin="IO_38" pad="AG12"/>
<connect gate="J" pin="IO_39" pad="AG13"/>
<connect gate="J" pin="IO_4" pad="AE12"/>
<connect gate="J" pin="IO_40" pad="AG14"/>
<connect gate="J" pin="IO_41" pad="AG15"/>
<connect gate="J" pin="IO_42" pad="AG16"/>
<connect gate="J" pin="IO_43" pad="AG17"/>
<connect gate="J" pin="IO_44" pad="AG18"/>
<connect gate="J" pin="IO_45" pad="AG19"/>
<connect gate="J" pin="IO_46" pad="AG20"/>
<connect gate="J" pin="IO_47" pad="AG21"/>
<connect gate="J" pin="IO_48" pad="AG22"/>
<connect gate="J" pin="IO_49" pad="AG23"/>
<connect gate="J" pin="IO_5" pad="AE13"/>
<connect gate="J" pin="IO_50" pad="AG24"/>
<connect gate="J" pin="IO_51" pad="AG25"/>
<connect gate="J" pin="IO_52" pad="AG29"/>
<connect gate="J" pin="IO_53" pad="AG30"/>
<connect gate="J" pin="IO_54" pad="AG31"/>
<connect gate="J" pin="IO_55" pad="AG32"/>
<connect gate="J" pin="IO_56" pad="AH11"/>
<connect gate="J" pin="IO_57" pad="AH13"/>
<connect gate="J" pin="IO_58" pad="AH14"/>
<connect gate="J" pin="IO_59" pad="AH15"/>
<connect gate="J" pin="IO_6" pad="AE14"/>
<connect gate="J" pin="IO_60" pad="AH16"/>
<connect gate="J" pin="IO_61" pad="AH17"/>
<connect gate="J" pin="IO_62" pad="AH18"/>
<connect gate="J" pin="IO_63" pad="AH19"/>
<connect gate="J" pin="IO_64" pad="AH20"/>
<connect gate="J" pin="IO_65" pad="AH22"/>
<connect gate="J" pin="IO_66" pad="AH24"/>
<connect gate="J" pin="IO_67" pad="AH25"/>
<connect gate="J" pin="IO_68" pad="AH26"/>
<connect gate="J" pin="IO_69" pad="AH28"/>
<connect gate="J" pin="IO_7" pad="AE19"/>
<connect gate="J" pin="IO_70" pad="AH29"/>
<connect gate="J" pin="IO_71" pad="AH30"/>
<connect gate="J" pin="IO_72" pad="AH31"/>
<connect gate="J" pin="IO_73" pad="AH32"/>
<connect gate="J" pin="IO_8" pad="AE20"/>
<connect gate="J" pin="IO_9" pad="AE21"/>
<connect gate="J" pin="TCK" pad="AF24"/>
<connect gate="J" pin="TMS" pad="AE24"/>
<connect gate="J" pin="VCCA_PLL12" pad="AF18"/>
<connect gate="J" pin="VCCA_PLL6" pad="AE15"/>
<connect gate="J" pin="VCCA_PLL8" pad="AF26"/>
<connect gate="J" pin="VCCD_PLL12" pad="AE18"/>
<connect gate="J" pin="VCCD_PLL8" pad="AF25"/>
<connect gate="J" pin="VCCIO7" pad="AH12"/>
<connect gate="J" pin="VCCIO8" pad="AH21"/>
<connect gate="J" pin="VCC_PLL12_OUT" pad="AF16"/>
<connect gate="J" pin="VCC_PLL6_OUT" pad="AF15"/>
<connect gate="J" pin="VREFB1N2" pad="AG28"/>
<connect gate="K" pin="FPLL8CLKN" pad="AJ29"/>
<connect gate="K" pin="FPLL8CLKP" pad="AJ30"/>
<connect gate="K" pin="GND" pad="AM13"/>
<connect gate="K" pin="GND_2" pad="AM31"/>
<connect gate="K" pin="GND_3" pad="AM20"/>
<connect gate="K" pin="GND_4" pad="AL32"/>
<connect gate="K" pin="IO" pad="AM29"/>
<connect gate="K" pin="IO_10" pad="AJ19"/>
<connect gate="K" pin="IO_11" pad="AJ20"/>
<connect gate="K" pin="IO_12" pad="AJ21"/>
<connect gate="K" pin="IO_13" pad="AJ22"/>
<connect gate="K" pin="IO_14" pad="AJ23"/>
<connect gate="K" pin="IO_15" pad="AJ25"/>
<connect gate="K" pin="IO_16" pad="AJ26"/>
<connect gate="K" pin="IO_17" pad="AJ27"/>
<connect gate="K" pin="IO_18" pad="AJ28"/>
<connect gate="K" pin="IO_19" pad="AJ31"/>
<connect gate="K" pin="IO_2" pad="AJ11"/>
<connect gate="K" pin="IO_20" pad="AJ32"/>
<connect gate="K" pin="IO_21" pad="AK10"/>
<connect gate="K" pin="IO_22" pad="AK11"/>
<connect gate="K" pin="IO_23" pad="AK12"/>
<connect gate="K" pin="IO_24" pad="AK13"/>
<connect gate="K" pin="IO_25" pad="AK15"/>
<connect gate="K" pin="IO_26" pad="AK16"/>
<connect gate="K" pin="IO_27" pad="AK17"/>
<connect gate="K" pin="IO_28" pad="AK18"/>
<connect gate="K" pin="IO_29" pad="AK20"/>
<connect gate="K" pin="IO_3" pad="AJ12"/>
<connect gate="K" pin="IO_30" pad="AK21"/>
<connect gate="K" pin="IO_31" pad="AK22"/>
<connect gate="K" pin="IO_32" pad="AK23"/>
<connect gate="K" pin="IO_33" pad="AK24"/>
<connect gate="K" pin="IO_34" pad="AK25"/>
<connect gate="K" pin="IO_35" pad="AK26"/>
<connect gate="K" pin="IO_36" pad="AK27"/>
<connect gate="K" pin="IO_37" pad="AK28"/>
<connect gate="K" pin="IO_38" pad="AK29"/>
<connect gate="K" pin="IO_39" pad="AL10"/>
<connect gate="K" pin="IO_4" pad="AJ13"/>
<connect gate="K" pin="IO_40" pad="AL11"/>
<connect gate="K" pin="IO_41" pad="AL12"/>
<connect gate="K" pin="IO_42" pad="AL13"/>
<connect gate="K" pin="IO_43" pad="AL14"/>
<connect gate="K" pin="IO_44" pad="AL15"/>
<connect gate="K" pin="IO_45" pad="AL16"/>
<connect gate="K" pin="IO_46" pad="AL17"/>
<connect gate="K" pin="IO_47" pad="AL18"/>
<connect gate="K" pin="IO_48" pad="AL19"/>
<connect gate="K" pin="IO_49" pad="AL20"/>
<connect gate="K" pin="IO_5" pad="AJ14"/>
<connect gate="K" pin="IO_50" pad="AL21"/>
<connect gate="K" pin="IO_51" pad="AL22"/>
<connect gate="K" pin="IO_52" pad="AL23"/>
<connect gate="K" pin="IO_53" pad="AL24"/>
<connect gate="K" pin="IO_54" pad="AL25"/>
<connect gate="K" pin="IO_55" pad="AL26"/>
<connect gate="K" pin="IO_56" pad="AL27"/>
<connect gate="K" pin="IO_57" pad="AL28"/>
<connect gate="K" pin="IO_58" pad="AL29"/>
<connect gate="K" pin="IO_59" pad="AM10"/>
<connect gate="K" pin="IO_6" pad="AJ15"/>
<connect gate="K" pin="IO_60" pad="AM11"/>
<connect gate="K" pin="IO_61" pad="AM12"/>
<connect gate="K" pin="IO_62" pad="AM14"/>
<connect gate="K" pin="IO_63" pad="AM16"/>
<connect gate="K" pin="IO_64" pad="AM17"/>
<connect gate="K" pin="IO_65" pad="AM19"/>
<connect gate="K" pin="IO_66" pad="AM21"/>
<connect gate="K" pin="IO_67" pad="AM22"/>
<connect gate="K" pin="IO_68" pad="AM23"/>
<connect gate="K" pin="IO_69" pad="AM24"/>
<connect gate="K" pin="IO_7" pad="AJ16"/>
<connect gate="K" pin="IO_70" pad="AM25"/>
<connect gate="K" pin="IO_71" pad="AM26"/>
<connect gate="K" pin="IO_72" pad="AM27"/>
<connect gate="K" pin="IO_73" pad="AM28"/>
<connect gate="K" pin="IO_8" pad="AJ17"/>
<connect gate="K" pin="IO_9" pad="AJ18"/>
<connect gate="K" pin="NCONFIG" pad="AL30"/>
<connect gate="K" pin="TDI" pad="AL31"/>
<connect gate="K" pin="TRST" pad="AK30"/>
<connect gate="K" pin="VCCIO1" pad="AK32"/>
<connect gate="K" pin="VCCIO7" pad="AM15"/>
<connect gate="K" pin="VCCIO8" pad="AM30"/>
<connect gate="K" pin="VCCIO8_2" pad="AM18"/>
<connect gate="K" pin="VREFB7N0" pad="AK14"/>
<connect gate="K" pin="VREFB8N0" pad="AK31"/>
<connect gate="K" pin="VREFB8N1" pad="AJ24"/>
<connect gate="K" pin="VREFB8N2" pad="AK19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2S90F1020C5N"/>
<attribute name="OC_FARNELL" value="1637239"/>
<attribute name="OC_NEWARK" value="51R0589"/>
<attribute name="PACKAGE" value="IC STRATIX II FPGA 90K 1020-FBGA"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2SGX130GF1508C4N">
<description>FPGA, STRATIX II</description>
<gates>
<gate name="A" symbol="EP2SGX130GF1508C4N_A"/>
<gate name="B" symbol="EP2SGX130GF1508C4N_B"/>
<gate name="C" symbol="EP2SGX130GF1508C4N_C"/>
<gate name="D" symbol="EP2SGX130GF1508C4N_D"/>
<gate name="E" symbol="EP2SGX130GF1508C4N_E"/>
<gate name="F" symbol="EP2SGX130GF1508C4N_F"/>
<gate name="G" symbol="EP2SGX130GF1508C4N_G"/>
<gate name="H" symbol="EP2SGX130GF1508C4N_H"/>
<gate name="I" symbol="EP2SGX130GF1508C4N_I"/>
<gate name="J" symbol="EP2SGX130GF1508C4N_J"/>
<gate name="K" symbol="EP2SGX130GF1508C4N_K"/>
<gate name="L" symbol="EP2SGX130GF1508C4N_L"/>
<gate name="M" symbol="EP2SGX130GF1508C4N_M"/>
<gate name="N" symbol="EP2SGX130GF1508C4N_N"/>
<gate name="O" symbol="EP2SGX130GF1508C4N_O"/>
<gate name="P" symbol="EP2SGX130GF1508C4N_P"/>
</gates>
<devices>
<device name="" package="BGA1508C100P39X39_4000X4000X35">
<connects>
<connect gate="A" pin="GND" pad="L3"/>
<connect gate="A" pin="GND_10" pad="B6"/>
<connect gate="A" pin="GND_11" pad="B7"/>
<connect gate="A" pin="GND_12" pad="B8"/>
<connect gate="A" pin="GND_13" pad="H9"/>
<connect gate="A" pin="GND_14" pad="B9"/>
<connect gate="A" pin="GND_15" pad="C6"/>
<connect gate="A" pin="GND_16" pad="C3"/>
<connect gate="A" pin="GND_17" pad="D1"/>
<connect gate="A" pin="GND_18" pad="C7"/>
<connect gate="A" pin="GND_19" pad="J3"/>
<connect gate="A" pin="GND_2" pad="A8"/>
<connect gate="A" pin="GND_20" pad="C8"/>
<connect gate="A" pin="GND_21" pad="D2"/>
<connect gate="A" pin="GND_22" pad="J6"/>
<connect gate="A" pin="GND_23" pad="D3"/>
<connect gate="A" pin="GND_24" pad="G6"/>
<connect gate="A" pin="GND_25" pad="D4"/>
<connect gate="A" pin="GND_26" pad="E6"/>
<connect gate="A" pin="GND_27" pad="D5"/>
<connect gate="A" pin="GND_28" pad="E3"/>
<connect gate="A" pin="GND_29" pad="D6"/>
<connect gate="A" pin="GND_3" pad="B1"/>
<connect gate="A" pin="GND_30" pad="J7"/>
<connect gate="A" pin="GND_31" pad="D7"/>
<connect gate="A" pin="GND_32" pad="E7"/>
<connect gate="A" pin="GND_33" pad="D8"/>
<connect gate="A" pin="GND_34" pad="F9"/>
<connect gate="A" pin="GND_35" pad="E8"/>
<connect gate="A" pin="GND_36" pad="G7"/>
<connect gate="A" pin="GND_37" pad="E9"/>
<connect gate="A" pin="GND_38" pad="G3"/>
<connect gate="A" pin="GND_39" pad="F1"/>
<connect gate="A" pin="GND_4" pad="B2"/>
<connect gate="A" pin="GND_40" pad="F5"/>
<connect gate="A" pin="GND_41" pad="J8"/>
<connect gate="A" pin="GND_42" pad="F2"/>
<connect gate="A" pin="GND_43" pad="K1"/>
<connect gate="A" pin="GND_44" pad="F6"/>
<connect gate="A" pin="GND_45" pad="G8"/>
<connect gate="A" pin="GND_46" pad="F3"/>
<connect gate="A" pin="GND_47" pad="H1"/>
<connect gate="A" pin="GND_48" pad="J9"/>
<connect gate="A" pin="GND_49" pad="K2"/>
<connect gate="A" pin="GND_5" pad="A2"/>
<connect gate="A" pin="GND_50" pad="F4"/>
<connect gate="A" pin="GND_51" pad="H2"/>
<connect gate="A" pin="GND_52" pad="G9"/>
<connect gate="A" pin="GND_53" pad="K3"/>
<connect gate="A" pin="GND_54" pad="H3"/>
<connect gate="A" pin="GND_55" pad="K4"/>
<connect gate="A" pin="GND_56" pad="H4"/>
<connect gate="A" pin="GND_57" pad="K5"/>
<connect gate="A" pin="GND_58" pad="H5"/>
<connect gate="A" pin="GND_59" pad="K6"/>
<connect gate="A" pin="GND_6" pad="B3"/>
<connect gate="A" pin="GND_60" pad="H6"/>
<connect gate="A" pin="GND_61" pad="L6"/>
<connect gate="A" pin="GND_62" pad="K8"/>
<connect gate="A" pin="GND_7" pad="A5"/>
<connect gate="A" pin="GND_8" pad="B4"/>
<connect gate="A" pin="GND_9" pad="B5"/>
<connect gate="A" pin="GXB_RX0N" pad="C2"/>
<connect gate="A" pin="GXB_RX0P" pad="C1"/>
<connect gate="A" pin="GXB_RX1N" pad="A4"/>
<connect gate="A" pin="GXB_RX1P" pad="A3"/>
<connect gate="A" pin="GXB_RX2N" pad="E2"/>
<connect gate="A" pin="GXB_RX2P" pad="E1"/>
<connect gate="A" pin="GXB_RX3N" pad="G2"/>
<connect gate="A" pin="GXB_RX3P" pad="G1"/>
<connect gate="A" pin="GXB_RX4N" pad="L2"/>
<connect gate="A" pin="GXB_RX4P" pad="L1"/>
<connect gate="A" pin="GXB_RX5N" pad="J2"/>
<connect gate="A" pin="GXB_RX5P" pad="J1"/>
<connect gate="A" pin="GXB_TX0N" pad="C5"/>
<connect gate="A" pin="GXB_TX0P" pad="C4"/>
<connect gate="A" pin="GXB_TX1N" pad="A7"/>
<connect gate="A" pin="GXB_TX1P" pad="A6"/>
<connect gate="A" pin="GXB_TX2N" pad="E5"/>
<connect gate="A" pin="GXB_TX2P" pad="E4"/>
<connect gate="A" pin="GXB_TX3N" pad="G5"/>
<connect gate="A" pin="GXB_TX3P" pad="G4"/>
<connect gate="A" pin="GXB_TX4N" pad="L5"/>
<connect gate="A" pin="GXB_TX4P" pad="L4"/>
<connect gate="A" pin="GXB_TX5N" pad="J5"/>
<connect gate="A" pin="GXB_TX5P" pad="J4"/>
<connect gate="A" pin="IO" pad="C9"/>
<connect gate="A" pin="IO_2" pad="A9"/>
<connect gate="A" pin="IO_3" pad="D9"/>
<connect gate="A" pin="REFCLK0_B13N" pad="H8"/>
<connect gate="A" pin="REFCLK0_B13P" pad="H7"/>
<connect gate="A" pin="REFCLK1_B13N" pad="F8"/>
<connect gate="A" pin="REFCLK1_B13P" pad="F7"/>
<connect gate="A" pin="RREFB13" pad="K7"/>
<connect gate="A" pin="VCCA" pad="K9"/>
<connect gate="B" pin="GND" pad="Y6"/>
<connect gate="B" pin="GND_10" pad="N8"/>
<connect gate="B" pin="GND_11" pad="M1"/>
<connect gate="B" pin="GND_12" pad="P5"/>
<connect gate="B" pin="GND_13" pad="N9"/>
<connect gate="B" pin="GND_14" pad="R6"/>
<connect gate="B" pin="GND_15" pad="M2"/>
<connect gate="B" pin="GND_16" pad="P6"/>
<connect gate="B" pin="GND_17" pad="P1"/>
<connect gate="B" pin="GND_18" pad="R7"/>
<connect gate="B" pin="GND_19" pad="M3"/>
<connect gate="B" pin="GND_2" pad="N3"/>
<connect gate="B" pin="GND_20" pad="R3"/>
<connect gate="B" pin="GND_21" pad="P2"/>
<connect gate="B" pin="GND_22" pad="R8"/>
<connect gate="B" pin="GND_23" pad="M4"/>
<connect gate="B" pin="GND_24" pad="T1"/>
<connect gate="B" pin="GND_25" pad="P3"/>
<connect gate="B" pin="GND_26" pad="T2"/>
<connect gate="B" pin="GND_27" pad="T3"/>
<connect gate="B" pin="GND_28" pad="T4"/>
<connect gate="B" pin="GND_29" pad="T5"/>
<connect gate="B" pin="GND_3" pad="L7"/>
<connect gate="B" pin="GND_30" pad="T6"/>
<connect gate="B" pin="GND_31" pad="T8"/>
<connect gate="B" pin="GND_32" pad="U6"/>
<connect gate="B" pin="GND_33" pad="U7"/>
<connect gate="B" pin="GND_34" pad="U8"/>
<connect gate="B" pin="GND_35" pad="U3"/>
<connect gate="B" pin="GND_36" pad="U9"/>
<connect gate="B" pin="GND_37" pad="V1"/>
<connect gate="B" pin="GND_38" pad="V2"/>
<connect gate="B" pin="GND_39" pad="V3"/>
<connect gate="B" pin="GND_4" pad="L8"/>
<connect gate="B" pin="GND_40" pad="V4"/>
<connect gate="B" pin="GND_41" pad="V5"/>
<connect gate="B" pin="GND_42" pad="W7"/>
<connect gate="B" pin="GND_43" pad="V6"/>
<connect gate="B" pin="GND_44" pad="W6"/>
<connect gate="B" pin="GND_45" pad="V9"/>
<connect gate="B" pin="GND_46" pad="Y1"/>
<connect gate="B" pin="GND_47" pad="W3"/>
<connect gate="B" pin="GND_48" pad="Y2"/>
<connect gate="B" pin="GND_49" pad="W8"/>
<connect gate="B" pin="GND_5" pad="M5"/>
<connect gate="B" pin="GND_50" pad="Y3"/>
<connect gate="B" pin="GND_51" pad="Y4"/>
<connect gate="B" pin="GND_52" pad="Y8"/>
<connect gate="B" pin="GND_53" pad="Y5"/>
<connect gate="B" pin="GND_6" pad="N6"/>
<connect gate="B" pin="GND_7" pad="N7"/>
<connect gate="B" pin="GND_8" pad="P4"/>
<connect gate="B" pin="GND_9" pad="M6"/>
<connect gate="B" pin="GXB_RX6N" pad="N2"/>
<connect gate="B" pin="GXB_RX6P" pad="N1"/>
<connect gate="B" pin="GXB_RX7N" pad="R2"/>
<connect gate="B" pin="GXB_RX7P" pad="R1"/>
<connect gate="B" pin="GXB_RX8N" pad="W2"/>
<connect gate="B" pin="GXB_RX8P" pad="W1"/>
<connect gate="B" pin="GXB_RX9N" pad="U2"/>
<connect gate="B" pin="GXB_RX9P" pad="U1"/>
<connect gate="B" pin="GXB_TX6N" pad="N5"/>
<connect gate="B" pin="GXB_TX6P" pad="N4"/>
<connect gate="B" pin="GXB_TX7N" pad="R5"/>
<connect gate="B" pin="GXB_TX7P" pad="R4"/>
<connect gate="B" pin="GXB_TX8N" pad="W5"/>
<connect gate="B" pin="GXB_TX8P" pad="W4"/>
<connect gate="B" pin="GXB_TX9N" pad="U5"/>
<connect gate="B" pin="GXB_TX9P" pad="U4"/>
<connect gate="B" pin="IO" pad="A20"/>
<connect gate="B" pin="IO_10" pad="A18"/>
<connect gate="B" pin="IO_11" pad="A19"/>
<connect gate="B" pin="IO_2" pad="A10"/>
<connect gate="B" pin="IO_3" pad="A11"/>
<connect gate="B" pin="IO_4" pad="A12"/>
<connect gate="B" pin="IO_5" pad="A13"/>
<connect gate="B" pin="IO_6" pad="A14"/>
<connect gate="B" pin="IO_7" pad="A15"/>
<connect gate="B" pin="IO_8" pad="A16"/>
<connect gate="B" pin="IO_9" pad="A17"/>
<connect gate="B" pin="REFCLK0_B14N" pad="P8"/>
<connect gate="B" pin="REFCLK0_B14P" pad="P7"/>
<connect gate="B" pin="REFCLK1_B14N" pad="M8"/>
<connect gate="B" pin="REFCLK1_B14P" pad="M7"/>
<connect gate="B" pin="REFCLK1_B15N" pad="V8"/>
<connect gate="B" pin="REFCLK1_B15P" pad="V7"/>
<connect gate="B" pin="RREFB14" pad="T7"/>
<connect gate="B" pin="RREFB15" pad="Y7"/>
<connect gate="B" pin="VCCA" pad="W9"/>
<connect gate="B" pin="VCCA_2" pad="L9"/>
<connect gate="B" pin="VCCA_3" pad="P9"/>
<connect gate="B" pin="VCCA_4" pad="Y9"/>
<connect gate="B" pin="VCCA_5" pad="R9"/>
<connect gate="B" pin="VCCL_B13" pad="M9"/>
<connect gate="B" pin="VCCL_B14" pad="T9"/>
<connect gate="C" pin="GND" pad="AF9"/>
<connect gate="C" pin="GND_10" pad="AB4"/>
<connect gate="C" pin="GND_11" pad="AC6"/>
<connect gate="C" pin="GND_12" pad="AB9"/>
<connect gate="C" pin="GND_13" pad="AC7"/>
<connect gate="C" pin="GND_14" pad="AB5"/>
<connect gate="C" pin="GND_15" pad="AC8"/>
<connect gate="C" pin="GND_16" pad="AB6"/>
<connect gate="C" pin="GND_17" pad="AE3"/>
<connect gate="C" pin="GND_18" pad="AC3"/>
<connect gate="C" pin="GND_19" pad="AD1"/>
<connect gate="C" pin="GND_2" pad="A38"/>
<connect gate="C" pin="GND_20" pad="AD2"/>
<connect gate="C" pin="GND_21" pad="AE6"/>
<connect gate="C" pin="GND_22" pad="AD3"/>
<connect gate="C" pin="GND_23" pad="AE7"/>
<connect gate="C" pin="GND_24" pad="AD4"/>
<connect gate="C" pin="GND_25" pad="AE8"/>
<connect gate="C" pin="GND_26" pad="AD5"/>
<connect gate="C" pin="GND_27" pad="AD6"/>
<connect gate="C" pin="GND_28" pad="AG3"/>
<connect gate="C" pin="GND_29" pad="AF1"/>
<connect gate="C" pin="GND_3" pad="AA6"/>
<connect gate="C" pin="GND_30" pad="AF2"/>
<connect gate="C" pin="GND_31" pad="AD8"/>
<connect gate="C" pin="GND_32" pad="AG6"/>
<connect gate="C" pin="GND_33" pad="AF3"/>
<connect gate="C" pin="GND_34" pad="AG7"/>
<connect gate="C" pin="GND_35" pad="AF4"/>
<connect gate="C" pin="GND_36" pad="AG8"/>
<connect gate="C" pin="GND_37" pad="AF5"/>
<connect gate="C" pin="GND_38" pad="AF6"/>
<connect gate="C" pin="GND_39" pad="AH3"/>
<connect gate="C" pin="GND_4" pad="AA7"/>
<connect gate="C" pin="GND_40" pad="AH1"/>
<connect gate="C" pin="GND_41" pad="AH4"/>
<connect gate="C" pin="GND_42" pad="AH2"/>
<connect gate="C" pin="GND_43" pad="AH5"/>
<connect gate="C" pin="GND_44" pad="AJ3"/>
<connect gate="C" pin="GND_45" pad="AH6"/>
<connect gate="C" pin="GND_5" pad="AA8"/>
<connect gate="C" pin="GND_6" pad="AA3"/>
<connect gate="C" pin="GND_7" pad="AB1"/>
<connect gate="C" pin="GND_8" pad="AB2"/>
<connect gate="C" pin="GND_9" pad="AB3"/>
<connect gate="C" pin="GXB_RX10N" pad="AA2"/>
<connect gate="C" pin="GXB_RX10P" pad="AA1"/>
<connect gate="C" pin="GXB_RX11N" pad="AC2"/>
<connect gate="C" pin="GXB_RX11P" pad="AC1"/>
<connect gate="C" pin="GXB_RX12N" pad="AG2"/>
<connect gate="C" pin="GXB_RX12P" pad="AG1"/>
<connect gate="C" pin="GXB_RX13N" pad="AE2"/>
<connect gate="C" pin="GXB_RX13P" pad="AE1"/>
<connect gate="C" pin="GXB_RX14N" pad="AJ2"/>
<connect gate="C" pin="GXB_RX14P" pad="AJ1"/>
<connect gate="C" pin="GXB_TX10N" pad="AA5"/>
<connect gate="C" pin="GXB_TX10P" pad="AA4"/>
<connect gate="C" pin="GXB_TX11N" pad="AC5"/>
<connect gate="C" pin="GXB_TX11P" pad="AC4"/>
<connect gate="C" pin="GXB_TX12N" pad="AG5"/>
<connect gate="C" pin="GXB_TX12P" pad="AG4"/>
<connect gate="C" pin="GXB_TX13N" pad="AE5"/>
<connect gate="C" pin="GXB_TX13P" pad="AE4"/>
<connect gate="C" pin="GXB_TX14N" pad="AJ5"/>
<connect gate="C" pin="GXB_TX14P" pad="AJ4"/>
<connect gate="C" pin="IO" pad="A33"/>
<connect gate="C" pin="IO_10" pad="A25"/>
<connect gate="C" pin="IO_11" pad="A26"/>
<connect gate="C" pin="IO_12" pad="A27"/>
<connect gate="C" pin="IO_13" pad="A28"/>
<connect gate="C" pin="IO_14" pad="A29"/>
<connect gate="C" pin="IO_15" pad="A30"/>
<connect gate="C" pin="IO_16" pad="A31"/>
<connect gate="C" pin="IO_17" pad="A32"/>
<connect gate="C" pin="IO_2" pad="A34"/>
<connect gate="C" pin="IO_3" pad="A35"/>
<connect gate="C" pin="IO_4" pad="A36"/>
<connect gate="C" pin="IO_5" pad="A37"/>
<connect gate="C" pin="IO_6" pad="A21"/>
<connect gate="C" pin="IO_7" pad="A22"/>
<connect gate="C" pin="IO_8" pad="A23"/>
<connect gate="C" pin="IO_9" pad="A24"/>
<connect gate="C" pin="REFCLK0_B15N" pad="AB8"/>
<connect gate="C" pin="REFCLK0_B15P" pad="AB7"/>
<connect gate="C" pin="REFCLK0_B16N" pad="AH8"/>
<connect gate="C" pin="REFCLK0_B16P" pad="AH7"/>
<connect gate="C" pin="REFCLK1_B16N" pad="AF8"/>
<connect gate="C" pin="REFCLK1_B16P" pad="AF7"/>
<connect gate="C" pin="RREFB16" pad="AD7"/>
<connect gate="C" pin="VCCA" pad="AD9"/>
<connect gate="C" pin="VCCA_2" pad="AC9"/>
<connect gate="C" pin="VCCA_3" pad="AH9"/>
<connect gate="C" pin="VCCA_4" pad="AG9"/>
<connect gate="C" pin="VCCL_B15" pad="AA9"/>
<connect gate="C" pin="VCCL_B16" pad="AE9"/>
<connect gate="D" pin="GND" pad="B11"/>
<connect gate="D" pin="GND_10" pad="AM2"/>
<connect gate="D" pin="GND_11" pad="AM9"/>
<connect gate="D" pin="GND_12" pad="AK1"/>
<connect gate="D" pin="GND_13" pad="AM3"/>
<connect gate="D" pin="GND_14" pad="AL3"/>
<connect gate="D" pin="GND_15" pad="AM4"/>
<connect gate="D" pin="GND_16" pad="AK2"/>
<connect gate="D" pin="GND_17" pad="AM5"/>
<connect gate="D" pin="GND_18" pad="AJ6"/>
<connect gate="D" pin="GND_19" pad="AK8"/>
<connect gate="D" pin="GND_2" pad="AJ7"/>
<connect gate="D" pin="GND_20" pad="AK3"/>
<connect gate="D" pin="GND_21" pad="AM6"/>
<connect gate="D" pin="GND_22" pad="AK4"/>
<connect gate="D" pin="GND_23" pad="AK5"/>
<connect gate="D" pin="GND_24" pad="AK6"/>
<connect gate="D" pin="GND_25" pad="AN6"/>
<connect gate="D" pin="GND_26" pad="AN7"/>
<connect gate="D" pin="GND_27" pad="AN8"/>
<connect gate="D" pin="GND_28" pad="AN9"/>
<connect gate="D" pin="GND_29" pad="AP1"/>
<connect gate="D" pin="GND_3" pad="AL6"/>
<connect gate="D" pin="GND_30" pad="AP2"/>
<connect gate="D" pin="GND_31" pad="AP3"/>
<connect gate="D" pin="GND_32" pad="AP4"/>
<connect gate="D" pin="GND_33" pad="AP5"/>
<connect gate="D" pin="GND_34" pad="AP6"/>
<connect gate="D" pin="GND_35" pad="AN3"/>
<connect gate="D" pin="GND_36" pad="AR6"/>
<connect gate="D" pin="GND_37" pad="AR7"/>
<connect gate="D" pin="GND_38" pad="AP9"/>
<connect gate="D" pin="GND_39" pad="AR8"/>
<connect gate="D" pin="GND_4" pad="AJ8"/>
<connect gate="D" pin="GND_40" pad="AR9"/>
<connect gate="D" pin="GND_41" pad="AT1"/>
<connect gate="D" pin="GND_42" pad="AR3"/>
<connect gate="D" pin="GND_43" pad="AU6"/>
<connect gate="D" pin="GND_44" pad="AT2"/>
<connect gate="D" pin="GND_45" pad="AU7"/>
<connect gate="D" pin="GND_46" pad="AT3"/>
<connect gate="D" pin="GND_47" pad="AU8"/>
<connect gate="D" pin="GND_48" pad="AT4"/>
<connect gate="D" pin="GND_49" pad="AV1"/>
<connect gate="D" pin="GND_5" pad="AL7"/>
<connect gate="D" pin="GND_50" pad="AT5"/>
<connect gate="D" pin="GND_51" pad="AV2"/>
<connect gate="D" pin="GND_52" pad="AT6"/>
<connect gate="D" pin="GND_53" pad="AV3"/>
<connect gate="D" pin="GND_54" pad="AT7"/>
<connect gate="D" pin="GND_55" pad="AV4"/>
<connect gate="D" pin="GND_56" pad="AT8"/>
<connect gate="D" pin="GND_57" pad="AV5"/>
<connect gate="D" pin="GND_58" pad="AV6"/>
<connect gate="D" pin="GND_59" pad="AV7"/>
<connect gate="D" pin="GND_6" pad="AL8"/>
<connect gate="D" pin="GND_60" pad="AW5"/>
<connect gate="D" pin="GND_61" pad="AU3"/>
<connect gate="D" pin="GND_62" pad="AV8"/>
<connect gate="D" pin="GND_63" pad="AV9"/>
<connect gate="D" pin="GND_64" pad="AW8"/>
<connect gate="D" pin="GND_65" pad="AW2"/>
<connect gate="D" pin="GND_7" pad="AK9"/>
<connect gate="D" pin="GND_8" pad="AL9"/>
<connect gate="D" pin="GND_9" pad="AM1"/>
<connect gate="D" pin="GXB_RX15N" pad="AL2"/>
<connect gate="D" pin="GXB_RX15P" pad="AL1"/>
<connect gate="D" pin="GXB_RX16N" pad="AR2"/>
<connect gate="D" pin="GXB_RX16P" pad="AR1"/>
<connect gate="D" pin="GXB_RX17N" pad="AN2"/>
<connect gate="D" pin="GXB_RX17P" pad="AN1"/>
<connect gate="D" pin="GXB_RX18N" pad="AU2"/>
<connect gate="D" pin="GXB_RX18P" pad="AU1"/>
<connect gate="D" pin="GXB_RX19N" pad="AW4"/>
<connect gate="D" pin="GXB_RX19P" pad="AW3"/>
<connect gate="D" pin="GXB_TX15N" pad="AL5"/>
<connect gate="D" pin="GXB_TX15P" pad="AL4"/>
<connect gate="D" pin="GXB_TX16N" pad="AR5"/>
<connect gate="D" pin="GXB_TX16P" pad="AR4"/>
<connect gate="D" pin="GXB_TX17N" pad="AN5"/>
<connect gate="D" pin="GXB_TX17P" pad="AN4"/>
<connect gate="D" pin="GXB_TX18N" pad="AU5"/>
<connect gate="D" pin="GXB_TX18P" pad="AU4"/>
<connect gate="D" pin="GXB_TX19N" pad="AW7"/>
<connect gate="D" pin="GXB_TX19P" pad="AW6"/>
<connect gate="D" pin="IO" pad="B10"/>
<connect gate="D" pin="IO_2" pad="AT9"/>
<connect gate="D" pin="IO_3" pad="AU9"/>
<connect gate="D" pin="IO_4" pad="AW9"/>
<connect gate="D" pin="REFCLK0_B17N" pad="AP8"/>
<connect gate="D" pin="REFCLK0_B17P" pad="AP7"/>
<connect gate="D" pin="REFCLK1_B17N" pad="AM8"/>
<connect gate="D" pin="REFCLK1_B17P" pad="AM7"/>
<connect gate="D" pin="RREFB17" pad="AK7"/>
<connect gate="D" pin="VCCL_B17" pad="AJ9"/>
<connect gate="E" pin="CONF_DONE" pad="D35"/>
<connect gate="E" pin="DCLK" pad="C35"/>
<connect gate="E" pin="FPLL7CLKN" pad="C38"/>
<connect gate="E" pin="FPLL7CLKP" pad="C39"/>
<connect gate="E" pin="GND" pad="B39"/>
<connect gate="E" pin="GND_10" pad="B23"/>
<connect gate="E" pin="GND_11" pad="B35"/>
<connect gate="E" pin="GND_12" pad="B38"/>
<connect gate="E" pin="GND_2" pad="B14"/>
<connect gate="E" pin="GND_3" pad="B20"/>
<connect gate="E" pin="GND_4" pad="B32"/>
<connect gate="E" pin="GND_5" pad="B29"/>
<connect gate="E" pin="GND_6" pad="B26"/>
<connect gate="E" pin="GND_7" pad="E11"/>
<connect gate="E" pin="GND_8" pad="B17"/>
<connect gate="E" pin="GND_9" pad="E14"/>
<connect gate="E" pin="IO" pad="E15"/>
<connect gate="E" pin="IO_10" pad="B19"/>
<connect gate="E" pin="IO_11" pad="C13"/>
<connect gate="E" pin="IO_12" pad="B21"/>
<connect gate="E" pin="IO_13" pad="C14"/>
<connect gate="E" pin="IO_14" pad="B22"/>
<connect gate="E" pin="IO_15" pad="C15"/>
<connect gate="E" pin="IO_16" pad="B24"/>
<connect gate="E" pin="IO_17" pad="C16"/>
<connect gate="E" pin="IO_18" pad="B25"/>
<connect gate="E" pin="IO_19" pad="C17"/>
<connect gate="E" pin="IO_2" pad="B12"/>
<connect gate="E" pin="IO_20" pad="B27"/>
<connect gate="E" pin="IO_21" pad="C18"/>
<connect gate="E" pin="IO_22" pad="B28"/>
<connect gate="E" pin="IO_23" pad="C19"/>
<connect gate="E" pin="IO_24" pad="B30"/>
<connect gate="E" pin="IO_25" pad="C20"/>
<connect gate="E" pin="IO_26" pad="B31"/>
<connect gate="E" pin="IO_27" pad="C21"/>
<connect gate="E" pin="IO_28" pad="B33"/>
<connect gate="E" pin="IO_29" pad="C22"/>
<connect gate="E" pin="IO_3" pad="B13"/>
<connect gate="E" pin="IO_30" pad="B34"/>
<connect gate="E" pin="IO_31" pad="C23"/>
<connect gate="E" pin="IO_32" pad="B36"/>
<connect gate="E" pin="IO_33" pad="C24"/>
<connect gate="E" pin="IO_34" pad="B37"/>
<connect gate="E" pin="IO_35" pad="C25"/>
<connect gate="E" pin="IO_36" pad="C26"/>
<connect gate="E" pin="IO_37" pad="C27"/>
<connect gate="E" pin="IO_38" pad="C28"/>
<connect gate="E" pin="IO_39" pad="C29"/>
<connect gate="E" pin="IO_4" pad="B15"/>
<connect gate="E" pin="IO_40" pad="C30"/>
<connect gate="E" pin="IO_41" pad="C31"/>
<connect gate="E" pin="IO_42" pad="C32"/>
<connect gate="E" pin="IO_43" pad="C33"/>
<connect gate="E" pin="IO_44" pad="C36"/>
<connect gate="E" pin="IO_45" pad="C37"/>
<connect gate="E" pin="IO_46" pad="D10"/>
<connect gate="E" pin="IO_47" pad="D11"/>
<connect gate="E" pin="IO_48" pad="D12"/>
<connect gate="E" pin="IO_49" pad="D13"/>
<connect gate="E" pin="IO_5" pad="C10"/>
<connect gate="E" pin="IO_50" pad="D14"/>
<connect gate="E" pin="IO_51" pad="D15"/>
<connect gate="E" pin="IO_52" pad="D16"/>
<connect gate="E" pin="IO_53" pad="D17"/>
<connect gate="E" pin="IO_54" pad="D18"/>
<connect gate="E" pin="IO_55" pad="D19"/>
<connect gate="E" pin="IO_56" pad="D20"/>
<connect gate="E" pin="IO_57" pad="D21"/>
<connect gate="E" pin="IO_58" pad="D22"/>
<connect gate="E" pin="IO_59" pad="D23"/>
<connect gate="E" pin="IO_6" pad="B16"/>
<connect gate="E" pin="IO_60" pad="D24"/>
<connect gate="E" pin="IO_61" pad="D25"/>
<connect gate="E" pin="IO_62" pad="D26"/>
<connect gate="E" pin="IO_63" pad="D27"/>
<connect gate="E" pin="IO_64" pad="D28"/>
<connect gate="E" pin="IO_65" pad="D29"/>
<connect gate="E" pin="IO_66" pad="D30"/>
<connect gate="E" pin="IO_67" pad="D31"/>
<connect gate="E" pin="IO_68" pad="D32"/>
<connect gate="E" pin="IO_69" pad="D33"/>
<connect gate="E" pin="IO_7" pad="C11"/>
<connect gate="E" pin="IO_70" pad="D36"/>
<connect gate="E" pin="IO_71" pad="D37"/>
<connect gate="E" pin="IO_72" pad="D38"/>
<connect gate="E" pin="IO_73" pad="D39"/>
<connect gate="E" pin="IO_74" pad="E12"/>
<connect gate="E" pin="IO_8" pad="B18"/>
<connect gate="E" pin="IO_9" pad="C12"/>
<connect gate="E" pin="NCE" pad="D34"/>
<connect gate="E" pin="NSTATUS" pad="C34"/>
<connect gate="E" pin="VREFB4N0" pad="E10"/>
<connect gate="E" pin="VREFB4N2" pad="E13"/>
<connect gate="E" pin="VREFB4N3" pad="E16"/>
<connect gate="F" pin="GND" pad="H20"/>
<connect gate="F" pin="GND_10" pad="H14"/>
<connect gate="F" pin="GND_11" pad="E32"/>
<connect gate="F" pin="GND_12" pad="H17"/>
<connect gate="F" pin="GND_2" pad="E29"/>
<connect gate="F" pin="GND_3" pad="E17"/>
<connect gate="F" pin="GND_4" pad="E38"/>
<connect gate="F" pin="GND_5" pad="E20"/>
<connect gate="F" pin="GND_6" pad="E35"/>
<connect gate="F" pin="GND_7" pad="H11"/>
<connect gate="F" pin="GND_8" pad="E26"/>
<connect gate="F" pin="GND_9" pad="E23"/>
<connect gate="F" pin="IO" pad="H21"/>
<connect gate="F" pin="IO_10" pad="F14"/>
<connect gate="F" pin="IO_11" pad="E25"/>
<connect gate="F" pin="IO_12" pad="E28"/>
<connect gate="F" pin="IO_13" pad="F15"/>
<connect gate="F" pin="IO_14" pad="F16"/>
<connect gate="F" pin="IO_15" pad="E18"/>
<connect gate="F" pin="IO_16" pad="F17"/>
<connect gate="F" pin="IO_17" pad="F18"/>
<connect gate="F" pin="IO_18" pad="F19"/>
<connect gate="F" pin="IO_19" pad="F20"/>
<connect gate="F" pin="IO_2" pad="E33"/>
<connect gate="F" pin="IO_20" pad="E22"/>
<connect gate="F" pin="IO_21" pad="F21"/>
<connect gate="F" pin="IO_22" pad="F22"/>
<connect gate="F" pin="IO_23" pad="F23"/>
<connect gate="F" pin="IO_24" pad="F24"/>
<connect gate="F" pin="IO_25" pad="F25"/>
<connect gate="F" pin="IO_26" pad="F26"/>
<connect gate="F" pin="IO_27" pad="F27"/>
<connect gate="F" pin="IO_28" pad="F28"/>
<connect gate="F" pin="IO_29" pad="F29"/>
<connect gate="F" pin="IO_3" pad="E34"/>
<connect gate="F" pin="IO_30" pad="F30"/>
<connect gate="F" pin="IO_31" pad="F31"/>
<connect gate="F" pin="IO_32" pad="F32"/>
<connect gate="F" pin="IO_33" pad="F33"/>
<connect gate="F" pin="IO_34" pad="F34"/>
<connect gate="F" pin="IO_35" pad="F35"/>
<connect gate="F" pin="IO_36" pad="F36"/>
<connect gate="F" pin="IO_37" pad="F37"/>
<connect gate="F" pin="IO_38" pad="F38"/>
<connect gate="F" pin="IO_39" pad="F39"/>
<connect gate="F" pin="IO_4" pad="E36"/>
<connect gate="F" pin="IO_40" pad="G10"/>
<connect gate="F" pin="IO_41" pad="G11"/>
<connect gate="F" pin="IO_42" pad="G12"/>
<connect gate="F" pin="IO_43" pad="G13"/>
<connect gate="F" pin="IO_44" pad="G14"/>
<connect gate="F" pin="IO_45" pad="G15"/>
<connect gate="F" pin="IO_46" pad="G16"/>
<connect gate="F" pin="IO_47" pad="G17"/>
<connect gate="F" pin="IO_48" pad="G18"/>
<connect gate="F" pin="IO_49" pad="G19"/>
<connect gate="F" pin="IO_5" pad="E37"/>
<connect gate="F" pin="IO_50" pad="G20"/>
<connect gate="F" pin="IO_51" pad="G21"/>
<connect gate="F" pin="IO_52" pad="G22"/>
<connect gate="F" pin="IO_53" pad="G23"/>
<connect gate="F" pin="IO_54" pad="G24"/>
<connect gate="F" pin="IO_55" pad="G25"/>
<connect gate="F" pin="IO_56" pad="G26"/>
<connect gate="F" pin="IO_57" pad="G27"/>
<connect gate="F" pin="IO_58" pad="G28"/>
<connect gate="F" pin="IO_59" pad="G29"/>
<connect gate="F" pin="IO_6" pad="E39"/>
<connect gate="F" pin="IO_60" pad="G30"/>
<connect gate="F" pin="IO_61" pad="G31"/>
<connect gate="F" pin="IO_62" pad="G32"/>
<connect gate="F" pin="IO_63" pad="G33"/>
<connect gate="F" pin="IO_64" pad="G34"/>
<connect gate="F" pin="IO_65" pad="G35"/>
<connect gate="F" pin="IO_66" pad="G37"/>
<connect gate="F" pin="IO_67" pad="G38"/>
<connect gate="F" pin="IO_68" pad="G39"/>
<connect gate="F" pin="IO_69" pad="H16"/>
<connect gate="F" pin="IO_7" pad="F10"/>
<connect gate="F" pin="IO_70" pad="H18"/>
<connect gate="F" pin="IO_71" pad="H15"/>
<connect gate="F" pin="IO_72" pad="H19"/>
<connect gate="F" pin="IO_8" pad="F12"/>
<connect gate="F" pin="IO_9" pad="F13"/>
<connect gate="F" pin="MSEL3" pad="H12"/>
<connect gate="F" pin="TDO" pad="H13"/>
<connect gate="F" pin="TEMPDIODEP" pad="H10"/>
<connect gate="F" pin="VREFB2N4" pad="G36"/>
<connect gate="F" pin="VREFB3N0" pad="E21"/>
<connect gate="F" pin="VREFB3N1" pad="E24"/>
<connect gate="F" pin="VREFB3N2" pad="E27"/>
<connect gate="F" pin="VREFB3N3" pad="E30"/>
<connect gate="F" pin="VREFB3N4" pad="E31"/>
<connect gate="F" pin="VREFB4N1" pad="F11"/>
<connect gate="F" pin="VREFB4N4" pad="E19"/>
<connect gate="G" pin="GND" pad="H38"/>
<connect gate="G" pin="GNDA_PLL11" pad="K22"/>
<connect gate="G" pin="GNDA_PLL11_2" pad="L22"/>
<connect gate="G" pin="GNDA_PLL5" pad="K20"/>
<connect gate="G" pin="GNDA_PLL5_2" pad="K19"/>
<connect gate="G" pin="GNDA_PLL7" pad="K29"/>
<connect gate="G" pin="GNDA_PLL7_2" pad="K28"/>
<connect gate="G" pin="GND_10" pad="H35"/>
<connect gate="G" pin="GND_11" pad="L26"/>
<connect gate="G" pin="GND_2" pad="H23"/>
<connect gate="G" pin="GND_3" pad="L14"/>
<connect gate="G" pin="GND_4" pad="H26"/>
<connect gate="G" pin="GND_5" pad="L17"/>
<connect gate="G" pin="GND_6" pad="H32"/>
<connect gate="G" pin="GND_7" pad="L23"/>
<connect gate="G" pin="GND_8" pad="H29"/>
<connect gate="G" pin="GND_9" pad="L20"/>
<connect gate="G" pin="IO" pad="L25"/>
<connect gate="G" pin="IO_10" pad="J30"/>
<connect gate="G" pin="IO_11" pad="H28"/>
<connect gate="G" pin="IO_12" pad="J31"/>
<connect gate="G" pin="IO_13" pad="J25"/>
<connect gate="G" pin="IO_14" pad="H34"/>
<connect gate="G" pin="IO_15" pad="J32"/>
<connect gate="G" pin="IO_16" pad="J33"/>
<connect gate="G" pin="IO_17" pad="H30"/>
<connect gate="G" pin="IO_18" pad="J34"/>
<connect gate="G" pin="IO_19" pad="J27"/>
<connect gate="G" pin="IO_2" pad="J15"/>
<connect gate="G" pin="IO_20" pad="J36"/>
<connect gate="G" pin="IO_21" pad="H24"/>
<connect gate="G" pin="IO_22" pad="H36"/>
<connect gate="G" pin="IO_23" pad="H25"/>
<connect gate="G" pin="IO_24" pad="J37"/>
<connect gate="G" pin="IO_25" pad="H37"/>
<connect gate="G" pin="IO_26" pad="J28"/>
<connect gate="G" pin="IO_27" pad="J38"/>
<connect gate="G" pin="IO_28" pad="H31"/>
<connect gate="G" pin="IO_29" pad="H39"/>
<connect gate="G" pin="IO_3" pad="J16"/>
<connect gate="G" pin="IO_30" pad="J39"/>
<connect gate="G" pin="IO_31" pad="K15"/>
<connect gate="G" pin="IO_32" pad="K16"/>
<connect gate="G" pin="IO_33" pad="K18"/>
<connect gate="G" pin="IO_34" pad="K24"/>
<connect gate="G" pin="IO_35" pad="K25"/>
<connect gate="G" pin="IO_36" pad="K27"/>
<connect gate="G" pin="IO_37" pad="K30"/>
<connect gate="G" pin="IO_38" pad="K31"/>
<connect gate="G" pin="IO_39" pad="K32"/>
<connect gate="G" pin="IO_4" pad="J18"/>
<connect gate="G" pin="IO_40" pad="K33"/>
<connect gate="G" pin="IO_41" pad="K34"/>
<connect gate="G" pin="IO_42" pad="K35"/>
<connect gate="G" pin="IO_43" pad="K36"/>
<connect gate="G" pin="IO_44" pad="K37"/>
<connect gate="G" pin="IO_45" pad="K38"/>
<connect gate="G" pin="IO_46" pad="K39"/>
<connect gate="G" pin="IO_47" pad="L15"/>
<connect gate="G" pin="IO_48" pad="L16"/>
<connect gate="G" pin="IO_5" pad="J21"/>
<connect gate="G" pin="IO_6" pad="H27"/>
<connect gate="G" pin="IO_7" pad="H33"/>
<connect gate="G" pin="IO_8" pad="H22"/>
<connect gate="G" pin="IO_9" pad="J24"/>
<connect gate="G" pin="MSEL0" pad="J11"/>
<connect gate="G" pin="MSEL1" pad="J12"/>
<connect gate="G" pin="MSEL2" pad="J13"/>
<connect gate="G" pin="TEMPDIODEN" pad="J10"/>
<connect gate="G" pin="VCCA_PLL11" pad="J22"/>
<connect gate="G" pin="VCCA_PLL5" pad="J20"/>
<connect gate="G" pin="VCCA_PLL7" pad="J29"/>
<connect gate="G" pin="VCCD_PLL11" pad="L21"/>
<connect gate="G" pin="VCCD_PLL5" pad="L19"/>
<connect gate="G" pin="VCCH_B13" pad="K12"/>
<connect gate="G" pin="VCCH_B13_2" pad="L12"/>
<connect gate="G" pin="VCCIO3" pad="K21"/>
<connect gate="G" pin="VCCIO3_2" pad="J23"/>
<connect gate="G" pin="VCCIO3_3" pad="J26"/>
<connect gate="G" pin="VCCIO3_4" pad="K23"/>
<connect gate="G" pin="VCCIO3_5" pad="K26"/>
<connect gate="G" pin="VCCIO4" pad="J19"/>
<connect gate="G" pin="VCCIO4_2" pad="J14"/>
<connect gate="G" pin="VCCIO4_3" pad="J17"/>
<connect gate="G" pin="VCCIO4_4" pad="K14"/>
<connect gate="G" pin="VCCIO4_5" pad="K17"/>
<connect gate="G" pin="VCCP" pad="L13"/>
<connect gate="G" pin="VCCP_2" pad="K13"/>
<connect gate="G" pin="VCCR" pad="L10"/>
<connect gate="G" pin="VCCR_2" pad="K10"/>
<connect gate="G" pin="VCCT_B13" pad="K11"/>
<connect gate="G" pin="VCCT_B13_2" pad="L11"/>
<connect gate="G" pin="VCC_PLL11_OUT" pad="L24"/>
<connect gate="G" pin="VCC_PLL5_OUT" pad="L18"/>
<connect gate="G" pin="VREFB2N3" pad="J35"/>
<connect gate="H" pin="GND" pad="P29"/>
<connect gate="H" pin="GND_10" pad="M11"/>
<connect gate="H" pin="GND_11" pad="P20"/>
<connect gate="H" pin="GND_12" pad="M12"/>
<connect gate="H" pin="GND_13" pad="P23"/>
<connect gate="H" pin="GND_14" pad="M13"/>
<connect gate="H" pin="GND_15" pad="P26"/>
<connect gate="H" pin="GND_2" pad="L29"/>
<connect gate="H" pin="GND_3" pad="L32"/>
<connect gate="H" pin="GND_4" pad="N11"/>
<connect gate="H" pin="GND_5" pad="P14"/>
<connect gate="H" pin="GND_6" pad="L35"/>
<connect gate="H" pin="GND_7" pad="M10"/>
<connect gate="H" pin="GND_8" pad="L38"/>
<connect gate="H" pin="GND_9" pad="P17"/>
<connect gate="H" pin="IO" pad="P30"/>
<connect gate="H" pin="IO_10" pad="L27"/>
<connect gate="H" pin="IO_11" pad="M26"/>
<connect gate="H" pin="IO_12" pad="L34"/>
<connect gate="H" pin="IO_13" pad="M27"/>
<connect gate="H" pin="IO_14" pad="L31"/>
<connect gate="H" pin="IO_15" pad="M28"/>
<connect gate="H" pin="IO_16" pad="L36"/>
<connect gate="H" pin="IO_17" pad="M29"/>
<connect gate="H" pin="IO_18" pad="M20"/>
<connect gate="H" pin="IO_19" pad="M30"/>
<connect gate="H" pin="IO_2" pad="M14"/>
<connect gate="H" pin="IO_20" pad="L37"/>
<connect gate="H" pin="IO_21" pad="M31"/>
<connect gate="H" pin="IO_22" pad="L39"/>
<connect gate="H" pin="IO_23" pad="M32"/>
<connect gate="H" pin="IO_24" pad="M33"/>
<connect gate="H" pin="IO_25" pad="M34"/>
<connect gate="H" pin="IO_26" pad="M36"/>
<connect gate="H" pin="IO_27" pad="M37"/>
<connect gate="H" pin="IO_28" pad="M38"/>
<connect gate="H" pin="IO_29" pad="M39"/>
<connect gate="H" pin="IO_3" pad="M15"/>
<connect gate="H" pin="IO_30" pad="N14"/>
<connect gate="H" pin="IO_31" pad="N15"/>
<connect gate="H" pin="IO_32" pad="N16"/>
<connect gate="H" pin="IO_33" pad="N17"/>
<connect gate="H" pin="IO_34" pad="N18"/>
<connect gate="H" pin="IO_35" pad="N19"/>
<connect gate="H" pin="IO_36" pad="N20"/>
<connect gate="H" pin="IO_37" pad="N21"/>
<connect gate="H" pin="IO_38" pad="N22"/>
<connect gate="H" pin="IO_39" pad="N23"/>
<connect gate="H" pin="IO_4" pad="M16"/>
<connect gate="H" pin="IO_40" pad="N24"/>
<connect gate="H" pin="IO_41" pad="N25"/>
<connect gate="H" pin="IO_42" pad="N26"/>
<connect gate="H" pin="IO_43" pad="N27"/>
<connect gate="H" pin="IO_44" pad="N28"/>
<connect gate="H" pin="IO_45" pad="N29"/>
<connect gate="H" pin="IO_46" pad="N30"/>
<connect gate="H" pin="IO_47" pad="N31"/>
<connect gate="H" pin="IO_48" pad="N32"/>
<connect gate="H" pin="IO_49" pad="N33"/>
<connect gate="H" pin="IO_5" pad="N13"/>
<connect gate="H" pin="IO_50" pad="N34"/>
<connect gate="H" pin="IO_51" pad="N35"/>
<connect gate="H" pin="IO_52" pad="N36"/>
<connect gate="H" pin="IO_53" pad="N37"/>
<connect gate="H" pin="IO_54" pad="N38"/>
<connect gate="H" pin="IO_55" pad="N39"/>
<connect gate="H" pin="IO_56" pad="P15"/>
<connect gate="H" pin="IO_57" pad="P16"/>
<connect gate="H" pin="IO_58" pad="P18"/>
<connect gate="H" pin="IO_59" pad="P19"/>
<connect gate="H" pin="IO_6" pad="L30"/>
<connect gate="H" pin="IO_60" pad="P21"/>
<connect gate="H" pin="IO_61" pad="P22"/>
<connect gate="H" pin="IO_62" pad="P24"/>
<connect gate="H" pin="IO_63" pad="P25"/>
<connect gate="H" pin="IO_64" pad="P27"/>
<connect gate="H" pin="IO_65" pad="P28"/>
<connect gate="H" pin="IO_7" pad="M24"/>
<connect gate="H" pin="IO_8" pad="L33"/>
<connect gate="H" pin="IO_9" pad="M25"/>
<connect gate="H" pin="VCCA" pad="N12"/>
<connect gate="H" pin="VCCA_2" pad="N10"/>
<connect gate="H" pin="VCCD_PLL7" pad="L28"/>
<connect gate="H" pin="VCCH_B14" pad="P12"/>
<connect gate="H" pin="VCCIO2" pad="P31"/>
<connect gate="H" pin="VCCP" pad="P13"/>
<connect gate="H" pin="VCCPD3" pad="M23"/>
<connect gate="H" pin="VCCPD3_2" pad="M21"/>
<connect gate="H" pin="VCCPD3_3" pad="M22"/>
<connect gate="H" pin="VCCPD4" pad="M19"/>
<connect gate="H" pin="VCCPD4_2" pad="M17"/>
<connect gate="H" pin="VCCPD4_3" pad="M18"/>
<connect gate="H" pin="VCCR" pad="P10"/>
<connect gate="H" pin="VCCT_B14" pad="P11"/>
<connect gate="H" pin="VREFB2N2" pad="M35"/>
<connect gate="I" pin="GND" pad="T13"/>
<connect gate="I" pin="GND_10" pad="U11"/>
<connect gate="I" pin="GND_11" pad="U16"/>
<connect gate="I" pin="GND_12" pad="U24"/>
<connect gate="I" pin="GND_13" pad="U26"/>
<connect gate="I" pin="GND_14" pad="U32"/>
<connect gate="I" pin="GND_15" pad="U29"/>
<connect gate="I" pin="GND_16" pad="U35"/>
<connect gate="I" pin="GND_17" pad="T10"/>
<connect gate="I" pin="GND_18" pad="T11"/>
<connect gate="I" pin="GND_19" pad="T12"/>
<connect gate="I" pin="GND_2" pad="U13"/>
<connect gate="I" pin="GND_3" pad="U18"/>
<connect gate="I" pin="GND_4" pad="P35"/>
<connect gate="I" pin="GND_5" pad="P38"/>
<connect gate="I" pin="GND_6" pad="P32"/>
<connect gate="I" pin="GND_7" pad="U14"/>
<connect gate="I" pin="GND_8" pad="U20"/>
<connect gate="I" pin="GND_9" pad="U22"/>
<connect gate="I" pin="IO" pad="U36"/>
<connect gate="I" pin="IO_10" pad="R17"/>
<connect gate="I" pin="IO_11" pad="R18"/>
<connect gate="I" pin="IO_12" pad="R19"/>
<connect gate="I" pin="IO_13" pad="R20"/>
<connect gate="I" pin="IO_14" pad="R21"/>
<connect gate="I" pin="IO_15" pad="R22"/>
<connect gate="I" pin="IO_16" pad="R23"/>
<connect gate="I" pin="IO_17" pad="R24"/>
<connect gate="I" pin="IO_18" pad="R25"/>
<connect gate="I" pin="IO_19" pad="R26"/>
<connect gate="I" pin="IO_2" pad="P33"/>
<connect gate="I" pin="IO_20" pad="R27"/>
<connect gate="I" pin="IO_21" pad="R31"/>
<connect gate="I" pin="IO_22" pad="R30"/>
<connect gate="I" pin="IO_23" pad="R32"/>
<connect gate="I" pin="IO_24" pad="R33"/>
<connect gate="I" pin="IO_25" pad="R34"/>
<connect gate="I" pin="IO_26" pad="R35"/>
<connect gate="I" pin="IO_27" pad="R36"/>
<connect gate="I" pin="IO_28" pad="R37"/>
<connect gate="I" pin="IO_29" pad="R38"/>
<connect gate="I" pin="IO_3" pad="P34"/>
<connect gate="I" pin="IO_30" pad="R39"/>
<connect gate="I" pin="IO_31" pad="T24"/>
<connect gate="I" pin="IO_32" pad="T25"/>
<connect gate="I" pin="IO_33" pad="T26"/>
<connect gate="I" pin="IO_34" pad="T27"/>
<connect gate="I" pin="IO_35" pad="T29"/>
<connect gate="I" pin="IO_36" pad="T30"/>
<connect gate="I" pin="IO_37" pad="T31"/>
<connect gate="I" pin="IO_38" pad="T32"/>
<connect gate="I" pin="IO_39" pad="T33"/>
<connect gate="I" pin="IO_4" pad="P36"/>
<connect gate="I" pin="IO_40" pad="T34"/>
<connect gate="I" pin="IO_41" pad="T35"/>
<connect gate="I" pin="IO_42" pad="T37"/>
<connect gate="I" pin="IO_43" pad="T38"/>
<connect gate="I" pin="IO_44" pad="T39"/>
<connect gate="I" pin="IO_45" pad="U25"/>
<connect gate="I" pin="IO_46" pad="U27"/>
<connect gate="I" pin="IO_47" pad="U30"/>
<connect gate="I" pin="IO_48" pad="U33"/>
<connect gate="I" pin="IO_49" pad="U34"/>
<connect gate="I" pin="IO_5" pad="P37"/>
<connect gate="I" pin="IO_6" pad="P39"/>
<connect gate="I" pin="IO_7" pad="R14"/>
<connect gate="I" pin="IO_8" pad="R15"/>
<connect gate="I" pin="IO_9" pad="R16"/>
<connect gate="I" pin="VCCA" pad="U12"/>
<connect gate="I" pin="VCCA_2" pad="U10"/>
<connect gate="I" pin="VCCH_B14" pad="R12"/>
<connect gate="I" pin="VCCINT" pad="T23"/>
<connect gate="I" pin="VCCINT_10" pad="T19"/>
<connect gate="I" pin="VCCINT_11" pad="U23"/>
<connect gate="I" pin="VCCINT_12" pad="U19"/>
<connect gate="I" pin="VCCINT_13" pad="T20"/>
<connect gate="I" pin="VCCINT_14" pad="T21"/>
<connect gate="I" pin="VCCINT_15" pad="T22"/>
<connect gate="I" pin="VCCINT_2" pad="U15"/>
<connect gate="I" pin="VCCINT_3" pad="T14"/>
<connect gate="I" pin="VCCINT_4" pad="T15"/>
<connect gate="I" pin="VCCINT_5" pad="U17"/>
<connect gate="I" pin="VCCINT_6" pad="T16"/>
<connect gate="I" pin="VCCINT_7" pad="U21"/>
<connect gate="I" pin="VCCINT_8" pad="T17"/>
<connect gate="I" pin="VCCINT_9" pad="T18"/>
<connect gate="I" pin="VCCIO2" pad="R29"/>
<connect gate="I" pin="VCCIO2_2" pad="U31"/>
<connect gate="I" pin="VCCP" pad="R13"/>
<connect gate="I" pin="VCCPD2" pad="R28"/>
<connect gate="I" pin="VCCPD2_2" pad="U28"/>
<connect gate="I" pin="VCCPD2_3" pad="T28"/>
<connect gate="I" pin="VCCR" pad="R10"/>
<connect gate="I" pin="VCCT_B14" pad="R11"/>
<connect gate="I" pin="VREFB2N1" pad="T36"/>
<connect gate="J" pin="CLK1N" pad="V36"/>
<connect gate="J" pin="CLK1P" pad="V37"/>
<connect gate="J" pin="CLK3N" pad="W36"/>
<connect gate="J" pin="CLK3P" pad="W37"/>
<connect gate="J" pin="GND" pad="W24"/>
<connect gate="J" pin="GNDA_PLL1" pad="W30"/>
<connect gate="J" pin="GNDA_PLL1_2" pad="W29"/>
<connect gate="J" pin="GNDA_PLL2" pad="Y28"/>
<connect gate="J" pin="GND_10" pad="Y15"/>
<connect gate="J" pin="GND_11" pad="V21"/>
<connect gate="J" pin="GND_12" pad="AA11"/>
<connect gate="J" pin="GND_13" pad="V17"/>
<connect gate="J" pin="GND_14" pad="Y23"/>
<connect gate="J" pin="GND_15" pad="V23"/>
<connect gate="J" pin="GND_16" pad="AA12"/>
<connect gate="J" pin="GND_17" pad="W14"/>
<connect gate="J" pin="GND_18" pad="AA13"/>
<connect gate="J" pin="GND_19" pad="Y29"/>
<connect gate="J" pin="GND_2" pad="Y32"/>
<connect gate="J" pin="GND_20" pad="AA14"/>
<connect gate="J" pin="GND_21" pad="Y26"/>
<connect gate="J" pin="GND_22" pad="W16"/>
<connect gate="J" pin="GND_23" pad="W22"/>
<connect gate="J" pin="GND_24" pad="AA16"/>
<connect gate="J" pin="GND_25" pad="Y17"/>
<connect gate="J" pin="GND_26" pad="W18"/>
<connect gate="J" pin="GND_3" pad="Y35"/>
<connect gate="J" pin="GND_4" pad="Y38"/>
<connect gate="J" pin="GND_5" pad="U38"/>
<connect gate="J" pin="GND_6" pad="V19"/>
<connect gate="J" pin="GND_7" pad="V13"/>
<connect gate="J" pin="GND_8" pad="AA10"/>
<connect gate="J" pin="GND_9" pad="V15"/>
<connect gate="J" pin="IO" pad="Y39"/>
<connect gate="J" pin="IO_10" pad="V33"/>
<connect gate="J" pin="IO_11" pad="V34"/>
<connect gate="J" pin="IO_12" pad="V35"/>
<connect gate="J" pin="IO_13" pad="W25"/>
<connect gate="J" pin="IO_14" pad="W26"/>
<connect gate="J" pin="IO_15" pad="V38"/>
<connect gate="J" pin="IO_16" pad="V39"/>
<connect gate="J" pin="IO_17" pad="W27"/>
<connect gate="J" pin="IO_18" pad="W32"/>
<connect gate="J" pin="IO_19" pad="W33"/>
<connect gate="J" pin="IO_2" pad="U37"/>
<connect gate="J" pin="IO_20" pad="W34"/>
<connect gate="J" pin="IO_21" pad="W38"/>
<connect gate="J" pin="IO_22" pad="W39"/>
<connect gate="J" pin="IO_23" pad="Y25"/>
<connect gate="J" pin="IO_24" pad="Y27"/>
<connect gate="J" pin="IO_25" pad="Y31"/>
<connect gate="J" pin="IO_26" pad="Y33"/>
<connect gate="J" pin="IO_27" pad="Y34"/>
<connect gate="J" pin="IO_28" pad="Y36"/>
<connect gate="J" pin="IO_29" pad="Y37"/>
<connect gate="J" pin="IO_3" pad="U39"/>
<connect gate="J" pin="IO_4" pad="V25"/>
<connect gate="J" pin="IO_5" pad="V26"/>
<connect gate="J" pin="IO_6" pad="V31"/>
<connect gate="J" pin="IO_7" pad="V27"/>
<connect gate="J" pin="IO_8" pad="V32"/>
<connect gate="J" pin="IO_9" pad="V28"/>
<connect gate="J" pin="NC" pad="V11"/>
<connect gate="J" pin="NC_2" pad="V10"/>
<connect gate="J" pin="VCCA" pad="V12"/>
<connect gate="J" pin="VCCA_PLL1" pad="V30"/>
<connect gate="J" pin="VCCA_PLL2" pad="Y30"/>
<connect gate="J" pin="VCCD_PLL1" pad="W28"/>
<connect gate="J" pin="VCCH_B15" pad="Y12"/>
<connect gate="J" pin="VCCH_B15_2" pad="W12"/>
<connect gate="J" pin="VCCINT" pad="V18"/>
<connect gate="J" pin="VCCINT_10" pad="AA15"/>
<connect gate="J" pin="VCCINT_11" pad="V14"/>
<connect gate="J" pin="VCCINT_12" pad="AA17"/>
<connect gate="J" pin="VCCINT_13" pad="V22"/>
<connect gate="J" pin="VCCINT_14" pad="V24"/>
<connect gate="J" pin="VCCINT_15" pad="V20"/>
<connect gate="J" pin="VCCINT_16" pad="V16"/>
<connect gate="J" pin="VCCINT_2" pad="W15"/>
<connect gate="J" pin="VCCINT_3" pad="Y18"/>
<connect gate="J" pin="VCCINT_4" pad="Y16"/>
<connect gate="J" pin="VCCINT_5" pad="Y22"/>
<connect gate="J" pin="VCCINT_6" pad="Y24"/>
<connect gate="J" pin="VCCINT_7" pad="W17"/>
<connect gate="J" pin="VCCINT_8" pad="Y14"/>
<connect gate="J" pin="VCCINT_9" pad="W23"/>
<connect gate="J" pin="VCCIO2" pad="W31"/>
<connect gate="J" pin="VCCIO2_2" pad="V29"/>
<connect gate="J" pin="VCCP" pad="Y13"/>
<connect gate="J" pin="VCCP_2" pad="W13"/>
<connect gate="J" pin="VCCR" pad="Y10"/>
<connect gate="J" pin="VCCR_2" pad="W10"/>
<connect gate="J" pin="VCCT_B15" pad="Y11"/>
<connect gate="J" pin="VCCT_B15_2" pad="W11"/>
<connect gate="J" pin="VREFB2N0" pad="W35"/>
<connect gate="K" pin="GND" pad="AC38"/>
<connect gate="K" pin="GNDA_PLL2" pad="AA29"/>
<connect gate="K" pin="GND_10" pad="AC18"/>
<connect gate="K" pin="GND_11" pad="AA24"/>
<connect gate="K" pin="GND_12" pad="AC16"/>
<connect gate="K" pin="GND_13" pad="AB23"/>
<connect gate="K" pin="GND_14" pad="AC22"/>
<connect gate="K" pin="GND_15" pad="AC14"/>
<connect gate="K" pin="GND_16" pad="AC29"/>
<connect gate="K" pin="GND_17" pad="AC24"/>
<connect gate="K" pin="GND_18" pad="AC20"/>
<connect gate="K" pin="GND_19" pad="AC32"/>
<connect gate="K" pin="GND_2" pad="AB11"/>
<connect gate="K" pin="GND_20" pad="AC26"/>
<connect gate="K" pin="GND_21" pad="AC35"/>
<connect gate="K" pin="GND_3" pad="AB13"/>
<connect gate="K" pin="GND_4" pad="AB15"/>
<connect gate="K" pin="GND_5" pad="AB17"/>
<connect gate="K" pin="GND_6" pad="AA18"/>
<connect gate="K" pin="GND_7" pad="AB19"/>
<connect gate="K" pin="GND_8" pad="AA22"/>
<connect gate="K" pin="GND_9" pad="AB21"/>
<connect gate="K" pin="IO" pad="AD25"/>
<connect gate="K" pin="IO_10" pad="AB25"/>
<connect gate="K" pin="IO_11" pad="AA37"/>
<connect gate="K" pin="IO_12" pad="AB26"/>
<connect gate="K" pin="IO_13" pad="AA38"/>
<connect gate="K" pin="IO_14" pad="AB27"/>
<connect gate="K" pin="IO_15" pad="AA39"/>
<connect gate="K" pin="IO_16" pad="AB29"/>
<connect gate="K" pin="IO_17" pad="AB30"/>
<connect gate="K" pin="IO_18" pad="AB33"/>
<connect gate="K" pin="IO_19" pad="AB31"/>
<connect gate="K" pin="IO_2" pad="AA31"/>
<connect gate="K" pin="IO_20" pad="AB34"/>
<connect gate="K" pin="IO_21" pad="AB32"/>
<connect gate="K" pin="IO_22" pad="AB35"/>
<connect gate="K" pin="IO_23" pad="AB36"/>
<connect gate="K" pin="IO_24" pad="AB37"/>
<connect gate="K" pin="IO_25" pad="AB38"/>
<connect gate="K" pin="IO_26" pad="AB39"/>
<connect gate="K" pin="IO_27" pad="AC25"/>
<connect gate="K" pin="IO_28" pad="AC27"/>
<connect gate="K" pin="IO_29" pad="AC30"/>
<connect gate="K" pin="IO_3" pad="AA32"/>
<connect gate="K" pin="IO_30" pad="AC33"/>
<connect gate="K" pin="IO_31" pad="AC34"/>
<connect gate="K" pin="IO_32" pad="AC36"/>
<connect gate="K" pin="IO_33" pad="AC37"/>
<connect gate="K" pin="IO_34" pad="AC39"/>
<connect gate="K" pin="IO_4" pad="AA33"/>
<connect gate="K" pin="IO_5" pad="AA34"/>
<connect gate="K" pin="IO_6" pad="AA25"/>
<connect gate="K" pin="IO_7" pad="AA35"/>
<connect gate="K" pin="IO_8" pad="AA26"/>
<connect gate="K" pin="IO_9" pad="AA27"/>
<connect gate="K" pin="VCCA" pad="AB10"/>
<connect gate="K" pin="VCCA_2" pad="AB12"/>
<connect gate="K" pin="VCCD_PLL2" pad="AA28"/>
<connect gate="K" pin="VCCH_B16" pad="AC12"/>
<connect gate="K" pin="VCCH_B16_2" pad="AD12"/>
<connect gate="K" pin="VCCINT" pad="AD24"/>
<connect gate="K" pin="VCCINT_10" pad="AC15"/>
<connect gate="K" pin="VCCINT_11" pad="AD15"/>
<connect gate="K" pin="VCCINT_12" pad="AC17"/>
<connect gate="K" pin="VCCINT_13" pad="AD16"/>
<connect gate="K" pin="VCCINT_14" pad="AC19"/>
<connect gate="K" pin="VCCINT_15" pad="AD17"/>
<connect gate="K" pin="VCCINT_16" pad="AC23"/>
<connect gate="K" pin="VCCINT_17" pad="AD18"/>
<connect gate="K" pin="VCCINT_18" pad="AC21"/>
<connect gate="K" pin="VCCINT_19" pad="AD19"/>
<connect gate="K" pin="VCCINT_2" pad="AA23"/>
<connect gate="K" pin="VCCINT_20" pad="AD20"/>
<connect gate="K" pin="VCCINT_21" pad="AD21"/>
<connect gate="K" pin="VCCINT_22" pad="AD22"/>
<connect gate="K" pin="VCCINT_23" pad="AD23"/>
<connect gate="K" pin="VCCINT_3" pad="AB18"/>
<connect gate="K" pin="VCCINT_4" pad="AB16"/>
<connect gate="K" pin="VCCINT_5" pad="AB22"/>
<connect gate="K" pin="VCCINT_6" pad="AB24"/>
<connect gate="K" pin="VCCINT_7" pad="AB20"/>
<connect gate="K" pin="VCCINT_8" pad="AB14"/>
<connect gate="K" pin="VCCINT_9" pad="AD14"/>
<connect gate="K" pin="VCCIO1" pad="AC31"/>
<connect gate="K" pin="VCCIO1_2" pad="AA30"/>
<connect gate="K" pin="VCCP" pad="AD13"/>
<connect gate="K" pin="VCCPD1" pad="AC28"/>
<connect gate="K" pin="VCCPD1_2" pad="AB28"/>
<connect gate="K" pin="VCCP_2" pad="AC13"/>
<connect gate="K" pin="VCCR" pad="AD10"/>
<connect gate="K" pin="VCCR_2" pad="AC10"/>
<connect gate="K" pin="VCCT_B16" pad="AC11"/>
<connect gate="K" pin="VCCT_B16_2" pad="AD11"/>
<connect gate="K" pin="VREFB1N4" pad="AA36"/>
<connect gate="L" pin="GND" pad="AE13"/>
<connect gate="L" pin="GND_10" pad="AF32"/>
<connect gate="L" pin="GND_11" pad="AF35"/>
<connect gate="L" pin="GND_12" pad="AF38"/>
<connect gate="L" pin="GND_13" pad="AE10"/>
<connect gate="L" pin="GND_14" pad="AE11"/>
<connect gate="L" pin="GND_15" pad="AE12"/>
<connect gate="L" pin="GND_2" pad="AF13"/>
<connect gate="L" pin="GND_3" pad="AF11"/>
<connect gate="L" pin="GND_4" pad="AF14"/>
<connect gate="L" pin="GND_5" pad="AF17"/>
<connect gate="L" pin="GND_6" pad="AF20"/>
<connect gate="L" pin="GND_7" pad="AF23"/>
<connect gate="L" pin="GND_8" pad="AF26"/>
<connect gate="L" pin="GND_9" pad="AF29"/>
<connect gate="L" pin="IO" pad="AG30"/>
<connect gate="L" pin="IO_10" pad="AD33"/>
<connect gate="L" pin="IO_11" pad="AE17"/>
<connect gate="L" pin="IO_12" pad="AD34"/>
<connect gate="L" pin="IO_13" pad="AE18"/>
<connect gate="L" pin="IO_14" pad="AD35"/>
<connect gate="L" pin="IO_15" pad="AE19"/>
<connect gate="L" pin="IO_16" pad="AE20"/>
<connect gate="L" pin="IO_17" pad="AD37"/>
<connect gate="L" pin="IO_18" pad="AE21"/>
<connect gate="L" pin="IO_19" pad="AD38"/>
<connect gate="L" pin="IO_2" pad="AD30"/>
<connect gate="L" pin="IO_20" pad="AE22"/>
<connect gate="L" pin="IO_21" pad="AD39"/>
<connect gate="L" pin="IO_22" pad="AE23"/>
<connect gate="L" pin="IO_23" pad="AE24"/>
<connect gate="L" pin="IO_24" pad="AE25"/>
<connect gate="L" pin="IO_25" pad="AE26"/>
<connect gate="L" pin="IO_26" pad="AE27"/>
<connect gate="L" pin="IO_27" pad="AE28"/>
<connect gate="L" pin="IO_28" pad="AE29"/>
<connect gate="L" pin="IO_29" pad="AE30"/>
<connect gate="L" pin="IO_3" pad="AD26"/>
<connect gate="L" pin="IO_30" pad="AE31"/>
<connect gate="L" pin="IO_31" pad="AE32"/>
<connect gate="L" pin="IO_32" pad="AE33"/>
<connect gate="L" pin="IO_33" pad="AE34"/>
<connect gate="L" pin="IO_34" pad="AE35"/>
<connect gate="L" pin="IO_35" pad="AE36"/>
<connect gate="L" pin="IO_36" pad="AE37"/>
<connect gate="L" pin="IO_37" pad="AE38"/>
<connect gate="L" pin="IO_38" pad="AE39"/>
<connect gate="L" pin="IO_39" pad="AF15"/>
<connect gate="L" pin="IO_4" pad="AD31"/>
<connect gate="L" pin="IO_40" pad="AF16"/>
<connect gate="L" pin="IO_41" pad="AF18"/>
<connect gate="L" pin="IO_42" pad="AF19"/>
<connect gate="L" pin="IO_43" pad="AF21"/>
<connect gate="L" pin="IO_44" pad="AF22"/>
<connect gate="L" pin="IO_45" pad="AF24"/>
<connect gate="L" pin="IO_46" pad="AF25"/>
<connect gate="L" pin="IO_47" pad="AF27"/>
<connect gate="L" pin="IO_48" pad="AF28"/>
<connect gate="L" pin="IO_49" pad="AF30"/>
<connect gate="L" pin="IO_5" pad="AE14"/>
<connect gate="L" pin="IO_50" pad="AF33"/>
<connect gate="L" pin="IO_51" pad="AF34"/>
<connect gate="L" pin="IO_52" pad="AF36"/>
<connect gate="L" pin="IO_53" pad="AF37"/>
<connect gate="L" pin="IO_54" pad="AF39"/>
<connect gate="L" pin="IO_55" pad="AG14"/>
<connect gate="L" pin="IO_56" pad="AG15"/>
<connect gate="L" pin="IO_57" pad="AG16"/>
<connect gate="L" pin="IO_58" pad="AG17"/>
<connect gate="L" pin="IO_59" pad="AG18"/>
<connect gate="L" pin="IO_6" pad="AD27"/>
<connect gate="L" pin="IO_60" pad="AG19"/>
<connect gate="L" pin="IO_61" pad="AG20"/>
<connect gate="L" pin="IO_62" pad="AG21"/>
<connect gate="L" pin="IO_63" pad="AG22"/>
<connect gate="L" pin="IO_64" pad="AG23"/>
<connect gate="L" pin="IO_65" pad="AG24"/>
<connect gate="L" pin="IO_66" pad="AG25"/>
<connect gate="L" pin="IO_67" pad="AG26"/>
<connect gate="L" pin="IO_68" pad="AG27"/>
<connect gate="L" pin="IO_69" pad="AG28"/>
<connect gate="L" pin="IO_7" pad="AE15"/>
<connect gate="L" pin="IO_8" pad="AD32"/>
<connect gate="L" pin="IO_9" pad="AE16"/>
<connect gate="L" pin="VCCA" pad="AF12"/>
<connect gate="L" pin="VCCA_2" pad="AF10"/>
<connect gate="L" pin="VCCH_B17" pad="AG12"/>
<connect gate="L" pin="VCCIO1" pad="AG29"/>
<connect gate="L" pin="VCCIO1_2" pad="AD29"/>
<connect gate="L" pin="VCCIO1_3" pad="AF31"/>
<connect gate="L" pin="VCCP" pad="AG13"/>
<connect gate="L" pin="VCCPD1" pad="AD28"/>
<connect gate="L" pin="VCCR" pad="AG10"/>
<connect gate="L" pin="VCCT_B17" pad="AG11"/>
<connect gate="L" pin="VREFB1N3" pad="AD36"/>
<connect gate="M" pin="GND" pad="AJ14"/>
<connect gate="M" pin="GNDA_PLL12" pad="AK22"/>
<connect gate="M" pin="GNDA_PLL12_2" pad="AJ22"/>
<connect gate="M" pin="GNDA_PLL6" pad="AK20"/>
<connect gate="M" pin="GNDA_PLL6_2" pad="AK19"/>
<connect gate="M" pin="GNDA_PLL8" pad="AK29"/>
<connect gate="M" pin="GNDA_PLL8_2" pad="AK28"/>
<connect gate="M" pin="GND_10" pad="AJ26"/>
<connect gate="M" pin="GND_11" pad="AJ38"/>
<connect gate="M" pin="GND_12" pad="AJ12"/>
<connect gate="M" pin="GND_13" pad="AJ17"/>
<connect gate="M" pin="GND_14" pad="AJ13"/>
<connect gate="M" pin="GND_2" pad="AJ29"/>
<connect gate="M" pin="GND_3" pad="AK11"/>
<connect gate="M" pin="GND_4" pad="AJ10"/>
<connect gate="M" pin="GND_5" pad="AJ32"/>
<connect gate="M" pin="GND_6" pad="AJ11"/>
<connect gate="M" pin="GND_7" pad="AJ23"/>
<connect gate="M" pin="GND_8" pad="AJ35"/>
<connect gate="M" pin="GND_9" pad="AJ20"/>
<connect gate="M" pin="IO" pad="AK35"/>
<connect gate="M" pin="IO_10" pad="AG35"/>
<connect gate="M" pin="IO_11" pad="AH24"/>
<connect gate="M" pin="IO_12" pad="AG36"/>
<connect gate="M" pin="IO_13" pad="AH25"/>
<connect gate="M" pin="IO_14" pad="AG37"/>
<connect gate="M" pin="IO_15" pad="AH26"/>
<connect gate="M" pin="IO_16" pad="AG38"/>
<connect gate="M" pin="IO_17" pad="AH27"/>
<connect gate="M" pin="IO_18" pad="AH20"/>
<connect gate="M" pin="IO_19" pad="AH28"/>
<connect gate="M" pin="IO_2" pad="AG31"/>
<connect gate="M" pin="IO_20" pad="AH29"/>
<connect gate="M" pin="IO_21" pad="AH30"/>
<connect gate="M" pin="IO_22" pad="AH31"/>
<connect gate="M" pin="IO_23" pad="AH32"/>
<connect gate="M" pin="IO_24" pad="AH33"/>
<connect gate="M" pin="IO_25" pad="AH34"/>
<connect gate="M" pin="IO_26" pad="AJ15"/>
<connect gate="M" pin="IO_27" pad="AJ16"/>
<connect gate="M" pin="IO_28" pad="AH36"/>
<connect gate="M" pin="IO_29" pad="AH37"/>
<connect gate="M" pin="IO_3" pad="AG32"/>
<connect gate="M" pin="IO_30" pad="AH38"/>
<connect gate="M" pin="IO_31" pad="AH39"/>
<connect gate="M" pin="IO_32" pad="AJ25"/>
<connect gate="M" pin="IO_33" pad="AJ27"/>
<connect gate="M" pin="IO_34" pad="AJ30"/>
<connect gate="M" pin="IO_35" pad="AJ33"/>
<connect gate="M" pin="IO_36" pad="AJ34"/>
<connect gate="M" pin="IO_37" pad="AJ36"/>
<connect gate="M" pin="IO_38" pad="AJ37"/>
<connect gate="M" pin="IO_39" pad="AJ39"/>
<connect gate="M" pin="IO_4" pad="AH14"/>
<connect gate="M" pin="IO_40" pad="AK13"/>
<connect gate="M" pin="IO_41" pad="AK15"/>
<connect gate="M" pin="IO_42" pad="AK16"/>
<connect gate="M" pin="IO_43" pad="AK18"/>
<connect gate="M" pin="IO_44" pad="AK24"/>
<connect gate="M" pin="IO_45" pad="AK25"/>
<connect gate="M" pin="IO_46" pad="AK27"/>
<connect gate="M" pin="IO_47" pad="AK30"/>
<connect gate="M" pin="IO_48" pad="AK31"/>
<connect gate="M" pin="IO_49" pad="AK32"/>
<connect gate="M" pin="IO_5" pad="AG33"/>
<connect gate="M" pin="IO_50" pad="AK33"/>
<connect gate="M" pin="IO_51" pad="AK34"/>
<connect gate="M" pin="IO_6" pad="AG39"/>
<connect gate="M" pin="IO_7" pad="AH15"/>
<connect gate="M" pin="IO_8" pad="AG34"/>
<connect gate="M" pin="IO_9" pad="AH16"/>
<connect gate="M" pin="VCCA" pad="AK12"/>
<connect gate="M" pin="VCCA_2" pad="AK10"/>
<connect gate="M" pin="VCCD_PLL12" pad="AJ21"/>
<connect gate="M" pin="VCCD_PLL6" pad="AJ19"/>
<connect gate="M" pin="VCCD_PLL8" pad="AJ28"/>
<connect gate="M" pin="VCCH_B17" pad="AH12"/>
<connect gate="M" pin="VCCIO1" pad="AJ31"/>
<connect gate="M" pin="VCCIO7" pad="AK17"/>
<connect gate="M" pin="VCCIO7_2" pad="AK14"/>
<connect gate="M" pin="VCCIO8" pad="AK26"/>
<connect gate="M" pin="VCCIO8_2" pad="AK23"/>
<connect gate="M" pin="VCCIO8_3" pad="AK21"/>
<connect gate="M" pin="VCCP" pad="AH13"/>
<connect gate="M" pin="VCCPD7" pad="AH18"/>
<connect gate="M" pin="VCCPD7_2" pad="AH17"/>
<connect gate="M" pin="VCCPD7_3" pad="AH19"/>
<connect gate="M" pin="VCCPD8" pad="AH23"/>
<connect gate="M" pin="VCCPD8_2" pad="AH21"/>
<connect gate="M" pin="VCCPD8_3" pad="AH22"/>
<connect gate="M" pin="VCCR" pad="AH10"/>
<connect gate="M" pin="VCCT_B17" pad="AH11"/>
<connect gate="M" pin="VCC_PLL12_OUT" pad="AJ24"/>
<connect gate="M" pin="VCC_PLL6_OUT" pad="AJ18"/>
<connect gate="M" pin="VREFB1N2" pad="AH35"/>
<connect gate="N" pin="GND" pad="AM12"/>
<connect gate="N" pin="GND_10" pad="AM20"/>
<connect gate="N" pin="GND_11" pad="AM38"/>
<connect gate="N" pin="GND_2" pad="AM23"/>
<connect gate="N" pin="GND_3" pad="AM26"/>
<connect gate="N" pin="GND_4" pad="AM29"/>
<connect gate="N" pin="GND_5" pad="AM32"/>
<connect gate="N" pin="GND_6" pad="AM35"/>
<connect gate="N" pin="GND_7" pad="AM11"/>
<connect gate="N" pin="GND_8" pad="AM17"/>
<connect gate="N" pin="GND_9" pad="AM14"/>
<connect gate="N" pin="IO" pad="AP10"/>
<connect gate="N" pin="IO_10" pad="AL27"/>
<connect gate="N" pin="IO_11" pad="AK38"/>
<connect gate="N" pin="IO_12" pad="AL28"/>
<connect gate="N" pin="IO_13" pad="AL18"/>
<connect gate="N" pin="IO_14" pad="AK39"/>
<connect gate="N" pin="IO_15" pad="AL30"/>
<connect gate="N" pin="IO_16" pad="AL31"/>
<connect gate="N" pin="IO_17" pad="AL32"/>
<connect gate="N" pin="IO_18" pad="AL33"/>
<connect gate="N" pin="IO_19" pad="AM19"/>
<connect gate="N" pin="IO_2" pad="AL13"/>
<connect gate="N" pin="IO_20" pad="AM13"/>
<connect gate="N" pin="IO_21" pad="AM15"/>
<connect gate="N" pin="IO_22" pad="AL34"/>
<connect gate="N" pin="IO_23" pad="AM16"/>
<connect gate="N" pin="IO_24" pad="AM21"/>
<connect gate="N" pin="IO_25" pad="AL36"/>
<connect gate="N" pin="IO_26" pad="AM18"/>
<connect gate="N" pin="IO_27" pad="AL37"/>
<connect gate="N" pin="IO_28" pad="AM22"/>
<connect gate="N" pin="IO_29" pad="AL38"/>
<connect gate="N" pin="IO_3" pad="AL21"/>
<connect gate="N" pin="IO_30" pad="AL39"/>
<connect gate="N" pin="IO_31" pad="AM24"/>
<connect gate="N" pin="IO_32" pad="AM25"/>
<connect gate="N" pin="IO_33" pad="AM27"/>
<connect gate="N" pin="IO_34" pad="AM28"/>
<connect gate="N" pin="IO_35" pad="AM30"/>
<connect gate="N" pin="IO_36" pad="AM31"/>
<connect gate="N" pin="IO_37" pad="AM33"/>
<connect gate="N" pin="IO_38" pad="AM34"/>
<connect gate="N" pin="IO_39" pad="AM36"/>
<connect gate="N" pin="IO_4" pad="AL15"/>
<connect gate="N" pin="IO_40" pad="AM37"/>
<connect gate="N" pin="IO_41" pad="AM39"/>
<connect gate="N" pin="IO_42" pad="AN10"/>
<connect gate="N" pin="IO_43" pad="AN11"/>
<connect gate="N" pin="IO_44" pad="AN12"/>
<connect gate="N" pin="IO_45" pad="AN13"/>
<connect gate="N" pin="IO_46" pad="AN14"/>
<connect gate="N" pin="IO_47" pad="AN15"/>
<connect gate="N" pin="IO_48" pad="AN16"/>
<connect gate="N" pin="IO_49" pad="AN17"/>
<connect gate="N" pin="IO_5" pad="AL24"/>
<connect gate="N" pin="IO_50" pad="AN18"/>
<connect gate="N" pin="IO_51" pad="AN19"/>
<connect gate="N" pin="IO_52" pad="AN20"/>
<connect gate="N" pin="IO_53" pad="AN21"/>
<connect gate="N" pin="IO_54" pad="AN22"/>
<connect gate="N" pin="IO_55" pad="AN23"/>
<connect gate="N" pin="IO_56" pad="AN24"/>
<connect gate="N" pin="IO_57" pad="AN25"/>
<connect gate="N" pin="IO_58" pad="AN26"/>
<connect gate="N" pin="IO_59" pad="AN27"/>
<connect gate="N" pin="IO_6" pad="AK36"/>
<connect gate="N" pin="IO_60" pad="AN28"/>
<connect gate="N" pin="IO_61" pad="AN29"/>
<connect gate="N" pin="IO_62" pad="AN30"/>
<connect gate="N" pin="IO_63" pad="AN31"/>
<connect gate="N" pin="IO_64" pad="AN32"/>
<connect gate="N" pin="IO_65" pad="AN33"/>
<connect gate="N" pin="IO_66" pad="AN34"/>
<connect gate="N" pin="IO_67" pad="AN35"/>
<connect gate="N" pin="IO_68" pad="AN36"/>
<connect gate="N" pin="IO_69" pad="AN37"/>
<connect gate="N" pin="IO_7" pad="AL25"/>
<connect gate="N" pin="IO_70" pad="AN38"/>
<connect gate="N" pin="IO_71" pad="AN39"/>
<connect gate="N" pin="IO_8" pad="AL16"/>
<connect gate="N" pin="IO_9" pad="AK37"/>
<connect gate="N" pin="NCEO" pad="AM10"/>
<connect gate="N" pin="NIO_PULLUP" pad="AL11"/>
<connect gate="N" pin="PLL_ENA" pad="AL12"/>
<connect gate="N" pin="PORSEL" pad="AL10"/>
<connect gate="N" pin="VCCA_PLL12" pad="AL22"/>
<connect gate="N" pin="VCCA_PLL6" pad="AL20"/>
<connect gate="N" pin="VCCA_PLL8" pad="AL29"/>
<connect gate="N" pin="VCCIO7" pad="AL19"/>
<connect gate="N" pin="VCCIO7_2" pad="AL14"/>
<connect gate="N" pin="VCCIO7_3" pad="AL17"/>
<connect gate="N" pin="VCCIO8" pad="AL26"/>
<connect gate="N" pin="VCCIO8_2" pad="AL23"/>
<connect gate="N" pin="VREFB1N1" pad="AL35"/>
<connect gate="O" pin="GND" pad="AR38"/>
<connect gate="O" pin="GND_10" pad="AR35"/>
<connect gate="O" pin="GND_2" pad="AR29"/>
<connect gate="O" pin="GND_3" pad="AR20"/>
<connect gate="O" pin="GND_4" pad="AR14"/>
<connect gate="O" pin="GND_5" pad="AR32"/>
<connect gate="O" pin="GND_6" pad="AR17"/>
<connect gate="O" pin="GND_7" pad="AR11"/>
<connect gate="O" pin="GND_8" pad="AR23"/>
<connect gate="O" pin="GND_9" pad="AR26"/>
<connect gate="O" pin="IO" pad="AU15"/>
<connect gate="O" pin="IO_10" pad="AP20"/>
<connect gate="O" pin="IO_11" pad="AP21"/>
<connect gate="O" pin="IO_12" pad="AP22"/>
<connect gate="O" pin="IO_13" pad="AP23"/>
<connect gate="O" pin="IO_14" pad="AP24"/>
<connect gate="O" pin="IO_15" pad="AP25"/>
<connect gate="O" pin="IO_16" pad="AP26"/>
<connect gate="O" pin="IO_17" pad="AP27"/>
<connect gate="O" pin="IO_18" pad="AP28"/>
<connect gate="O" pin="IO_19" pad="AP29"/>
<connect gate="O" pin="IO_2" pad="AP12"/>
<connect gate="O" pin="IO_20" pad="AP30"/>
<connect gate="O" pin="IO_21" pad="AP36"/>
<connect gate="O" pin="IO_22" pad="AP31"/>
<connect gate="O" pin="IO_23" pad="AP37"/>
<connect gate="O" pin="IO_24" pad="AP38"/>
<connect gate="O" pin="IO_25" pad="AP39"/>
<connect gate="O" pin="IO_26" pad="AR25"/>
<connect gate="O" pin="IO_27" pad="AR18"/>
<connect gate="O" pin="IO_28" pad="AR12"/>
<connect gate="O" pin="IO_29" pad="AR22"/>
<connect gate="O" pin="IO_3" pad="AP13"/>
<connect gate="O" pin="IO_30" pad="AR15"/>
<connect gate="O" pin="IO_31" pad="AR28"/>
<connect gate="O" pin="IO_32" pad="AR33"/>
<connect gate="O" pin="IO_33" pad="AR36"/>
<connect gate="O" pin="IO_34" pad="AR37"/>
<connect gate="O" pin="IO_35" pad="AR39"/>
<connect gate="O" pin="IO_36" pad="AT10"/>
<connect gate="O" pin="IO_37" pad="AT11"/>
<connect gate="O" pin="IO_38" pad="AT12"/>
<connect gate="O" pin="IO_39" pad="AT13"/>
<connect gate="O" pin="IO_4" pad="AP14"/>
<connect gate="O" pin="IO_40" pad="AT14"/>
<connect gate="O" pin="IO_41" pad="AT15"/>
<connect gate="O" pin="IO_42" pad="AT16"/>
<connect gate="O" pin="IO_43" pad="AT17"/>
<connect gate="O" pin="IO_44" pad="AT18"/>
<connect gate="O" pin="IO_45" pad="AT19"/>
<connect gate="O" pin="IO_46" pad="AT20"/>
<connect gate="O" pin="IO_47" pad="AT21"/>
<connect gate="O" pin="IO_48" pad="AT22"/>
<connect gate="O" pin="IO_49" pad="AT23"/>
<connect gate="O" pin="IO_5" pad="AP15"/>
<connect gate="O" pin="IO_50" pad="AT24"/>
<connect gate="O" pin="IO_51" pad="AT25"/>
<connect gate="O" pin="IO_52" pad="AT26"/>
<connect gate="O" pin="IO_53" pad="AT27"/>
<connect gate="O" pin="IO_54" pad="AT28"/>
<connect gate="O" pin="IO_55" pad="AT29"/>
<connect gate="O" pin="IO_56" pad="AT30"/>
<connect gate="O" pin="IO_57" pad="AT31"/>
<connect gate="O" pin="IO_58" pad="AT32"/>
<connect gate="O" pin="IO_59" pad="AT33"/>
<connect gate="O" pin="IO_6" pad="AP16"/>
<connect gate="O" pin="IO_60" pad="AT35"/>
<connect gate="O" pin="IO_61" pad="AT36"/>
<connect gate="O" pin="IO_62" pad="AT37"/>
<connect gate="O" pin="IO_63" pad="AT38"/>
<connect gate="O" pin="IO_64" pad="AT39"/>
<connect gate="O" pin="IO_65" pad="AU10"/>
<connect gate="O" pin="IO_66" pad="AU11"/>
<connect gate="O" pin="IO_67" pad="AU12"/>
<connect gate="O" pin="IO_68" pad="AU13"/>
<connect gate="O" pin="IO_69" pad="AU14"/>
<connect gate="O" pin="IO_7" pad="AP17"/>
<connect gate="O" pin="IO_8" pad="AP18"/>
<connect gate="O" pin="IO_9" pad="AP19"/>
<connect gate="O" pin="NCONFIG" pad="AR34"/>
<connect gate="O" pin="TDI" pad="AP34"/>
<connect gate="O" pin="TMS" pad="AP33"/>
<connect gate="O" pin="TRST" pad="AP32"/>
<connect gate="O" pin="VCCSEL" pad="AT34"/>
<connect gate="O" pin="VREFB1N0" pad="AP35"/>
<connect gate="O" pin="VREFB7N0" pad="AR19"/>
<connect gate="O" pin="VREFB7N1" pad="AR16"/>
<connect gate="O" pin="VREFB7N2" pad="AR13"/>
<connect gate="O" pin="VREFB7N3" pad="AP11"/>
<connect gate="O" pin="VREFB7N4" pad="AR10"/>
<connect gate="O" pin="VREFB8N0" pad="AR31"/>
<connect gate="O" pin="VREFB8N1" pad="AR30"/>
<connect gate="O" pin="VREFB8N2" pad="AR27"/>
<connect gate="O" pin="VREFB8N3" pad="AR24"/>
<connect gate="O" pin="VREFB8N4" pad="AR21"/>
<connect gate="P" pin="FPLL8CLKN" pad="AU38"/>
<connect gate="P" pin="FPLL8CLKP" pad="AU39"/>
<connect gate="P" pin="GND" pad="AW38"/>
<connect gate="P" pin="GND_10" pad="AV29"/>
<connect gate="P" pin="GND_11" pad="AV38"/>
<connect gate="P" pin="GND_12" pad="AV39"/>
<connect gate="P" pin="GND_2" pad="AV32"/>
<connect gate="P" pin="GND_3" pad="AV23"/>
<connect gate="P" pin="GND_4" pad="AV20"/>
<connect gate="P" pin="GND_5" pad="AV35"/>
<connect gate="P" pin="GND_6" pad="AV11"/>
<connect gate="P" pin="GND_7" pad="AV14"/>
<connect gate="P" pin="GND_8" pad="AV17"/>
<connect gate="P" pin="GND_9" pad="AV26"/>
<connect gate="P" pin="IO" pad="AW37"/>
<connect gate="P" pin="IO_10" pad="AU24"/>
<connect gate="P" pin="IO_11" pad="AU25"/>
<connect gate="P" pin="IO_12" pad="AU26"/>
<connect gate="P" pin="IO_13" pad="AU27"/>
<connect gate="P" pin="IO_14" pad="AU28"/>
<connect gate="P" pin="IO_15" pad="AU29"/>
<connect gate="P" pin="IO_16" pad="AU30"/>
<connect gate="P" pin="IO_17" pad="AU31"/>
<connect gate="P" pin="IO_18" pad="AU32"/>
<connect gate="P" pin="IO_19" pad="AU33"/>
<connect gate="P" pin="IO_2" pad="AU16"/>
<connect gate="P" pin="IO_20" pad="AU34"/>
<connect gate="P" pin="IO_21" pad="AV21"/>
<connect gate="P" pin="IO_22" pad="AU36"/>
<connect gate="P" pin="IO_23" pad="AV22"/>
<connect gate="P" pin="IO_24" pad="AU37"/>
<connect gate="P" pin="IO_25" pad="AV24"/>
<connect gate="P" pin="IO_26" pad="AV25"/>
<connect gate="P" pin="IO_27" pad="AV10"/>
<connect gate="P" pin="IO_28" pad="AV12"/>
<connect gate="P" pin="IO_29" pad="AV13"/>
<connect gate="P" pin="IO_3" pad="AU17"/>
<connect gate="P" pin="IO_30" pad="AV27"/>
<connect gate="P" pin="IO_31" pad="AV15"/>
<connect gate="P" pin="IO_32" pad="AV28"/>
<connect gate="P" pin="IO_33" pad="AV16"/>
<connect gate="P" pin="IO_34" pad="AV30"/>
<connect gate="P" pin="IO_35" pad="AV18"/>
<connect gate="P" pin="IO_36" pad="AV31"/>
<connect gate="P" pin="IO_37" pad="AV19"/>
<connect gate="P" pin="IO_38" pad="AV33"/>
<connect gate="P" pin="IO_39" pad="AV34"/>
<connect gate="P" pin="IO_4" pad="AU18"/>
<connect gate="P" pin="IO_40" pad="AV36"/>
<connect gate="P" pin="IO_41" pad="AV37"/>
<connect gate="P" pin="IO_42" pad="AW10"/>
<connect gate="P" pin="IO_43" pad="AW11"/>
<connect gate="P" pin="IO_44" pad="AW12"/>
<connect gate="P" pin="IO_45" pad="AW13"/>
<connect gate="P" pin="IO_46" pad="AW14"/>
<connect gate="P" pin="IO_47" pad="AW15"/>
<connect gate="P" pin="IO_48" pad="AW16"/>
<connect gate="P" pin="IO_49" pad="AW17"/>
<connect gate="P" pin="IO_5" pad="AU19"/>
<connect gate="P" pin="IO_50" pad="AW18"/>
<connect gate="P" pin="IO_51" pad="AW19"/>
<connect gate="P" pin="IO_52" pad="AW20"/>
<connect gate="P" pin="IO_53" pad="AW21"/>
<connect gate="P" pin="IO_54" pad="AW22"/>
<connect gate="P" pin="IO_55" pad="AW23"/>
<connect gate="P" pin="IO_56" pad="AW24"/>
<connect gate="P" pin="IO_57" pad="AW25"/>
<connect gate="P" pin="IO_58" pad="AW26"/>
<connect gate="P" pin="IO_59" pad="AW27"/>
<connect gate="P" pin="IO_6" pad="AU20"/>
<connect gate="P" pin="IO_60" pad="AW28"/>
<connect gate="P" pin="IO_61" pad="AW29"/>
<connect gate="P" pin="IO_62" pad="AW30"/>
<connect gate="P" pin="IO_63" pad="AW31"/>
<connect gate="P" pin="IO_64" pad="AW32"/>
<connect gate="P" pin="IO_65" pad="AW33"/>
<connect gate="P" pin="IO_66" pad="AW34"/>
<connect gate="P" pin="IO_67" pad="AW35"/>
<connect gate="P" pin="IO_68" pad="AW36"/>
<connect gate="P" pin="IO_7" pad="AU21"/>
<connect gate="P" pin="IO_8" pad="AU22"/>
<connect gate="P" pin="IO_9" pad="AU23"/>
<connect gate="P" pin="TCK" pad="AU35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2SGX130GF1508C4N"/>
<attribute name="OC_FARNELL" value="1637240"/>
<attribute name="OC_NEWARK" value="51R0577"/>
<attribute name="PACKAGE" value="FBGA-1508"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2SGX30CF780C5N">
<description>FPGA, STRATIX II GX</description>
<gates>
<gate name="A" symbol="EP2SGX30CF780C5N_A"/>
<gate name="B" symbol="EP2SGX30CF780C5N_B"/>
<gate name="C" symbol="EP2SGX30CF780C5N_C"/>
<gate name="D" symbol="EP2SGX30CF780C5N_D"/>
<gate name="E" symbol="EP2SGX30CF780C5N_E"/>
<gate name="F" symbol="EP2SGX30CF780C5N_F"/>
<gate name="G" symbol="EP2SGX30CF780C5N_G"/>
<gate name="H" symbol="EP2SGX30CF780C5N_H"/>
</gates>
<devices>
<device name="" package="BGA780C100P28X28_2900X2900X350">
<connects>
<connect gate="A" pin="GND" pad="L3"/>
<connect gate="A" pin="GND_10" pad="B4"/>
<connect gate="A" pin="GND_11" pad="B5"/>
<connect gate="A" pin="GND_12" pad="B6"/>
<connect gate="A" pin="GND_13" pad="B7"/>
<connect gate="A" pin="GND_14" pad="B9"/>
<connect gate="A" pin="GND_15" pad="C1"/>
<connect gate="A" pin="GND_16" pad="C2"/>
<connect gate="A" pin="GND_17" pad="C3"/>
<connect gate="A" pin="GND_18" pad="C6"/>
<connect gate="A" pin="GND_19" pad="D1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_20" pad="D2"/>
<connect gate="A" pin="GND_21" pad="D3"/>
<connect gate="A" pin="GND_22" pad="D4"/>
<connect gate="A" pin="GND_23" pad="D5"/>
<connect gate="A" pin="GND_24" pad="D6"/>
<connect gate="A" pin="GND_25" pad="E3"/>
<connect gate="A" pin="GND_26" pad="E6"/>
<connect gate="A" pin="GND_27" pad="E7"/>
<connect gate="A" pin="GND_28" pad="E9"/>
<connect gate="A" pin="GND_29" pad="F1"/>
<connect gate="A" pin="GND_3" pad="A3"/>
<connect gate="A" pin="GND_30" pad="F2"/>
<connect gate="A" pin="GND_31" pad="F3"/>
<connect gate="A" pin="GND_32" pad="F4"/>
<connect gate="A" pin="GND_33" pad="F5"/>
<connect gate="A" pin="GND_34" pad="F6"/>
<connect gate="A" pin="GND_35" pad="G3"/>
<connect gate="A" pin="GND_36" pad="G6"/>
<connect gate="A" pin="GND_37" pad="H1"/>
<connect gate="A" pin="GND_38" pad="H2"/>
<connect gate="A" pin="GND_39" pad="H3"/>
<connect gate="A" pin="GND_4" pad="A4"/>
<connect gate="A" pin="GND_40" pad="H4"/>
<connect gate="A" pin="GND_41" pad="H5"/>
<connect gate="A" pin="GND_42" pad="H6"/>
<connect gate="A" pin="GND_43" pad="H7"/>
<connect gate="A" pin="GND_44" pad="H9"/>
<connect gate="A" pin="GND_45" pad="J3"/>
<connect gate="A" pin="GND_46" pad="J5"/>
<connect gate="A" pin="GND_47" pad="J6"/>
<connect gate="A" pin="GND_48" pad="J7"/>
<connect gate="A" pin="GND_49" pad="K1"/>
<connect gate="A" pin="GND_5" pad="A5"/>
<connect gate="A" pin="GND_50" pad="K2"/>
<connect gate="A" pin="GND_51" pad="K3"/>
<connect gate="A" pin="GND_52" pad="K4"/>
<connect gate="A" pin="GND_53" pad="K5"/>
<connect gate="A" pin="GND_54" pad="K6"/>
<connect gate="A" pin="GND_6" pad="A6"/>
<connect gate="A" pin="GND_7" pad="B1"/>
<connect gate="A" pin="GND_8" pad="B2"/>
<connect gate="A" pin="GND_9" pad="B3"/>
<connect gate="A" pin="GXB_RX0N" pad="G2"/>
<connect gate="A" pin="GXB_RX0P" pad="G1"/>
<connect gate="A" pin="GXB_RX1N" pad="E2"/>
<connect gate="A" pin="GXB_RX1P" pad="E1"/>
<connect gate="A" pin="GXB_RX2N" pad="L2"/>
<connect gate="A" pin="GXB_RX2P" pad="L1"/>
<connect gate="A" pin="GXB_TX0N" pad="E5"/>
<connect gate="A" pin="GXB_TX0P" pad="E4"/>
<connect gate="A" pin="GXB_TX1N" pad="C5"/>
<connect gate="A" pin="GXB_TX1P" pad="C4"/>
<connect gate="A" pin="GXB_TX2N" pad="L5"/>
<connect gate="A" pin="GXB_TX2P" pad="L4"/>
<connect gate="A" pin="IO" pad="G9"/>
<connect gate="A" pin="IO_10" pad="D8"/>
<connect gate="A" pin="IO_11" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A8"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_5" pad="B8"/>
<connect gate="A" pin="IO_6" pad="C7"/>
<connect gate="A" pin="IO_7" pad="C8"/>
<connect gate="A" pin="IO_8" pad="C9"/>
<connect gate="A" pin="IO_9" pad="D7"/>
<connect gate="A" pin="MSEL0" pad="J8"/>
<connect gate="A" pin="MSEL1" pad="E8"/>
<connect gate="A" pin="MSEL2" pad="H8"/>
<connect gate="A" pin="MSEL3" pad="G8"/>
<connect gate="A" pin="NC" pad="K8"/>
<connect gate="A" pin="NC_2" pad="F9"/>
<connect gate="A" pin="NC_3" pad="K7"/>
<connect gate="A" pin="REFCLK0_B13N" pad="J2"/>
<connect gate="A" pin="REFCLK0_B13P" pad="J1"/>
<connect gate="A" pin="REFCLK1_B13N" pad="G5"/>
<connect gate="A" pin="REFCLK1_B13P" pad="G4"/>
<connect gate="A" pin="RREFB13" pad="J4"/>
<connect gate="A" pin="TDO" pad="F8"/>
<connect gate="A" pin="TEMPDIODEN" pad="G7"/>
<connect gate="A" pin="TEMPDIODEP" pad="F7"/>
<connect gate="A" pin="VCCA" pad="L6"/>
<connect gate="A" pin="VCCA_2" pad="K9"/>
<connect gate="A" pin="VCCH_B13" pad="L9"/>
<connect gate="A" pin="VCCIO4" pad="J9"/>
<connect gate="A" pin="VCCR" pad="L7"/>
<connect gate="A" pin="VCCT_B13" pad="L8"/>
<connect gate="B" pin="GND" pad="Y6"/>
<connect gate="B" pin="GND_10" pad="N9"/>
<connect gate="B" pin="GND_11" pad="P1"/>
<connect gate="B" pin="GND_12" pad="P2"/>
<connect gate="B" pin="GND_13" pad="P3"/>
<connect gate="B" pin="GND_14" pad="P4"/>
<connect gate="B" pin="GND_15" pad="P5"/>
<connect gate="B" pin="GND_16" pad="P6"/>
<connect gate="B" pin="GND_17" pad="P8"/>
<connect gate="B" pin="GND_18" pad="R1"/>
<connect gate="B" pin="GND_19" pad="R2"/>
<connect gate="B" pin="GND_2" pad="M1"/>
<connect gate="B" pin="GND_20" pad="R3"/>
<connect gate="B" pin="GND_21" pad="R4"/>
<connect gate="B" pin="GND_22" pad="R5"/>
<connect gate="B" pin="GND_23" pad="T3"/>
<connect gate="B" pin="GND_24" pad="U1"/>
<connect gate="B" pin="GND_25" pad="U2"/>
<connect gate="B" pin="GND_26" pad="U3"/>
<connect gate="B" pin="GND_27" pad="U4"/>
<connect gate="B" pin="GND_28" pad="U5"/>
<connect gate="B" pin="GND_29" pad="U7"/>
<connect gate="B" pin="GND_3" pad="M2"/>
<connect gate="B" pin="GND_30" pad="U8"/>
<connect gate="B" pin="GND_31" pad="U9"/>
<connect gate="B" pin="GND_32" pad="V3"/>
<connect gate="B" pin="GND_33" pad="V6"/>
<connect gate="B" pin="GND_34" pad="V8"/>
<connect gate="B" pin="GND_35" pad="W1"/>
<connect gate="B" pin="GND_36" pad="W2"/>
<connect gate="B" pin="GND_37" pad="W3"/>
<connect gate="B" pin="GND_38" pad="W4"/>
<connect gate="B" pin="GND_39" pad="W5"/>
<connect gate="B" pin="GND_4" pad="M3"/>
<connect gate="B" pin="GND_40" pad="W6"/>
<connect gate="B" pin="GND_41" pad="W7"/>
<connect gate="B" pin="GND_42" pad="W8"/>
<connect gate="B" pin="GND_43" pad="Y3"/>
<connect gate="B" pin="GND_44" pad="Y5"/>
<connect gate="B" pin="GND_5" pad="M4"/>
<connect gate="B" pin="GND_6" pad="M5"/>
<connect gate="B" pin="GND_7" pad="N3"/>
<connect gate="B" pin="GND_8" pad="N7"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GXB_RX3N" pad="N2"/>
<connect gate="B" pin="GXB_RX3P" pad="N1"/>
<connect gate="B" pin="GXB_TX3N" pad="N5"/>
<connect gate="B" pin="GXB_TX3P" pad="N4"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="A17"/>
<connect gate="B" pin="IO_11" pad="A18"/>
<connect gate="B" pin="IO_12" pad="A19"/>
<connect gate="B" pin="IO_13" pad="A20"/>
<connect gate="B" pin="IO_14" pad="A21"/>
<connect gate="B" pin="IO_15" pad="A22"/>
<connect gate="B" pin="IO_16" pad="A23"/>
<connect gate="B" pin="IO_17" pad="A24"/>
<connect gate="B" pin="IO_18" pad="A25"/>
<connect gate="B" pin="IO_2" pad="W9"/>
<connect gate="B" pin="IO_3" pad="A10"/>
<connect gate="B" pin="IO_4" pad="A11"/>
<connect gate="B" pin="IO_5" pad="A12"/>
<connect gate="B" pin="IO_6" pad="A13"/>
<connect gate="B" pin="IO_7" pad="A14"/>
<connect gate="B" pin="IO_8" pad="A15"/>
<connect gate="B" pin="IO_9" pad="A16"/>
<connect gate="B" pin="NC" pad="Y4"/>
<connect gate="B" pin="NC_10" pad="Y1"/>
<connect gate="B" pin="NC_11" pad="Y2"/>
<connect gate="B" pin="NC_2" pad="T1"/>
<connect gate="B" pin="NC_3" pad="T2"/>
<connect gate="B" pin="NC_4" pad="T4"/>
<connect gate="B" pin="NC_5" pad="T5"/>
<connect gate="B" pin="NC_6" pad="V1"/>
<connect gate="B" pin="NC_7" pad="V2"/>
<connect gate="B" pin="NC_8" pad="V4"/>
<connect gate="B" pin="NC_9" pad="V5"/>
<connect gate="B" pin="NIO_PULLUP" pad="Y7"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA" pad="V9"/>
<connect gate="B" pin="VCCA_2" pad="M6"/>
<connect gate="B" pin="VCCA_3" pad="P7"/>
<connect gate="B" pin="VCCA_4" pad="P9"/>
<connect gate="B" pin="VCCA_5" pad="R6"/>
<connect gate="B" pin="VCCA_6" pad="T6"/>
<connect gate="B" pin="VCCA_7" pad="V7"/>
<connect gate="B" pin="VCCH_B13" pad="M9"/>
<connect gate="B" pin="VCCH_B14" pad="T9"/>
<connect gate="B" pin="VCCH_B14_2" pad="R9"/>
<connect gate="B" pin="VCCIO7" pad="Y9"/>
<connect gate="B" pin="VCCL_B13" pad="N6"/>
<connect gate="B" pin="VCCL_B14" pad="U6"/>
<connect gate="B" pin="VCCR" pad="T7"/>
<connect gate="B" pin="VCCR_2" pad="M7"/>
<connect gate="B" pin="VCCR_3" pad="R7"/>
<connect gate="B" pin="VCCT_B13" pad="M8"/>
<connect gate="B" pin="VCCT_B14" pad="T8"/>
<connect gate="B" pin="VCCT_B14_2" pad="R8"/>
<connect gate="C" pin="GND" pad="B28"/>
<connect gate="C" pin="GND_10" pad="AA9"/>
<connect gate="C" pin="GND_11" pad="AB3"/>
<connect gate="C" pin="GND_12" pad="AB6"/>
<connect gate="C" pin="GND_13" pad="AC1"/>
<connect gate="C" pin="GND_14" pad="AC2"/>
<connect gate="C" pin="GND_15" pad="AC3"/>
<connect gate="C" pin="GND_16" pad="AC4"/>
<connect gate="C" pin="GND_17" pad="AC5"/>
<connect gate="C" pin="GND_18" pad="AC6"/>
<connect gate="C" pin="GND_19" pad="AC7"/>
<connect gate="C" pin="GND_2" pad="A27"/>
<connect gate="C" pin="GND_20" pad="AD3"/>
<connect gate="C" pin="GND_21" pad="AD6"/>
<connect gate="C" pin="GND_22" pad="AD7"/>
<connect gate="C" pin="GND_23" pad="AD9"/>
<connect gate="C" pin="GND_24" pad="AE1"/>
<connect gate="C" pin="GND_25" pad="AE2"/>
<connect gate="C" pin="GND_26" pad="AE3"/>
<connect gate="C" pin="GND_27" pad="AE4"/>
<connect gate="C" pin="GND_28" pad="AE5"/>
<connect gate="C" pin="GND_29" pad="AE6"/>
<connect gate="C" pin="GND_3" pad="AA1"/>
<connect gate="C" pin="GND_30" pad="AF1"/>
<connect gate="C" pin="GND_31" pad="AF2"/>
<connect gate="C" pin="GND_32" pad="AF3"/>
<connect gate="C" pin="GND_33" pad="AF6"/>
<connect gate="C" pin="GND_34" pad="AG1"/>
<connect gate="C" pin="GND_35" pad="AG2"/>
<connect gate="C" pin="GND_36" pad="AG3"/>
<connect gate="C" pin="GND_37" pad="AG4"/>
<connect gate="C" pin="GND_38" pad="AG5"/>
<connect gate="C" pin="GND_39" pad="AG6"/>
<connect gate="C" pin="GND_4" pad="AA2"/>
<connect gate="C" pin="GND_40" pad="AG7"/>
<connect gate="C" pin="GND_41" pad="AG9"/>
<connect gate="C" pin="GND_42" pad="AH2"/>
<connect gate="C" pin="GND_43" pad="AH3"/>
<connect gate="C" pin="GND_44" pad="AH4"/>
<connect gate="C" pin="GND_45" pad="AH5"/>
<connect gate="C" pin="GND_46" pad="AH6"/>
<connect gate="C" pin="GND_47" pad="B12"/>
<connect gate="C" pin="GND_48" pad="B15"/>
<connect gate="C" pin="GND_49" pad="B18"/>
<connect gate="C" pin="GND_5" pad="AA3"/>
<connect gate="C" pin="GND_50" pad="B21"/>
<connect gate="C" pin="GND_51" pad="B24"/>
<connect gate="C" pin="GND_52" pad="B27"/>
<connect gate="C" pin="GND_6" pad="AA4"/>
<connect gate="C" pin="GND_7" pad="AA5"/>
<connect gate="C" pin="GND_8" pad="AA6"/>
<connect gate="C" pin="GND_9" pad="AA7"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AF8"/>
<connect gate="C" pin="IO_11" pad="AF9"/>
<connect gate="C" pin="IO_12" pad="AG8"/>
<connect gate="C" pin="IO_13" pad="AH7"/>
<connect gate="C" pin="IO_14" pad="AH8"/>
<connect gate="C" pin="IO_15" pad="AH9"/>
<connect gate="C" pin="IO_16" pad="B10"/>
<connect gate="C" pin="IO_17" pad="B11"/>
<connect gate="C" pin="IO_18" pad="B13"/>
<connect gate="C" pin="IO_19" pad="B14"/>
<connect gate="C" pin="IO_2" pad="AB8"/>
<connect gate="C" pin="IO_20" pad="B16"/>
<connect gate="C" pin="IO_21" pad="B17"/>
<connect gate="C" pin="IO_22" pad="B19"/>
<connect gate="C" pin="IO_23" pad="B20"/>
<connect gate="C" pin="IO_24" pad="B22"/>
<connect gate="C" pin="IO_25" pad="B23"/>
<connect gate="C" pin="IO_26" pad="B25"/>
<connect gate="C" pin="IO_27" pad="B26"/>
<connect gate="C" pin="IO_28" pad="C10"/>
<connect gate="C" pin="IO_29" pad="C11"/>
<connect gate="C" pin="IO_3" pad="AB9"/>
<connect gate="C" pin="IO_30" pad="C12"/>
<connect gate="C" pin="IO_31" pad="C13"/>
<connect gate="C" pin="IO_32" pad="C14"/>
<connect gate="C" pin="IO_33" pad="C15"/>
<connect gate="C" pin="IO_4" pad="AC8"/>
<connect gate="C" pin="IO_5" pad="AC9"/>
<connect gate="C" pin="IO_6" pad="AE7"/>
<connect gate="C" pin="IO_7" pad="AE8"/>
<connect gate="C" pin="IO_8" pad="AE9"/>
<connect gate="C" pin="IO_9" pad="AF7"/>
<connect gate="C" pin="NC" pad="AF5"/>
<connect gate="C" pin="NCEO" pad="AB7"/>
<connect gate="C" pin="NC_10" pad="AB1"/>
<connect gate="C" pin="NC_11" pad="AF4"/>
<connect gate="C" pin="NC_2" pad="AB2"/>
<connect gate="C" pin="NC_3" pad="AB4"/>
<connect gate="C" pin="NC_4" pad="AB5"/>
<connect gate="C" pin="NC_5" pad="AD1"/>
<connect gate="C" pin="NC_6" pad="AD2"/>
<connect gate="C" pin="NC_7" pad="AD4"/>
<connect gate="C" pin="NC_8" pad="AD5"/>
<connect gate="C" pin="NC_9" pad="AD8"/>
<connect gate="C" pin="PLL_ENA" pad="AA8"/>
<connect gate="D" pin="CONF_DONE" pad="D26"/>
<connect gate="D" pin="DCLK" pad="D25"/>
<connect gate="D" pin="GND" pad="H18"/>
<connect gate="D" pin="GND_10" pad="H16"/>
<connect gate="D" pin="GND_2" pad="E12"/>
<connect gate="D" pin="GND_3" pad="E15"/>
<connect gate="D" pin="GND_4" pad="E18"/>
<connect gate="D" pin="GND_5" pad="E21"/>
<connect gate="D" pin="GND_6" pad="E24"/>
<connect gate="D" pin="GND_7" pad="E27"/>
<connect gate="D" pin="GND_8" pad="H12"/>
<connect gate="D" pin="GND_9" pad="H15"/>
<connect gate="D" pin="IO" pad="H19"/>
<connect gate="D" pin="IO_10" pad="C26"/>
<connect gate="D" pin="IO_11" pad="C27"/>
<connect gate="D" pin="IO_12" pad="C28"/>
<connect gate="D" pin="IO_13" pad="D10"/>
<connect gate="D" pin="IO_14" pad="D11"/>
<connect gate="D" pin="IO_15" pad="D12"/>
<connect gate="D" pin="IO_16" pad="D13"/>
<connect gate="D" pin="IO_17" pad="D14"/>
<connect gate="D" pin="IO_18" pad="D15"/>
<connect gate="D" pin="IO_19" pad="D16"/>
<connect gate="D" pin="IO_2" pad="C18"/>
<connect gate="D" pin="IO_20" pad="D17"/>
<connect gate="D" pin="IO_21" pad="D18"/>
<connect gate="D" pin="IO_22" pad="D19"/>
<connect gate="D" pin="IO_23" pad="D20"/>
<connect gate="D" pin="IO_24" pad="D21"/>
<connect gate="D" pin="IO_25" pad="D22"/>
<connect gate="D" pin="IO_26" pad="D23"/>
<connect gate="D" pin="IO_27" pad="D27"/>
<connect gate="D" pin="IO_28" pad="D28"/>
<connect gate="D" pin="IO_29" pad="E10"/>
<connect gate="D" pin="IO_3" pad="C19"/>
<connect gate="D" pin="IO_30" pad="E11"/>
<connect gate="D" pin="IO_31" pad="E13"/>
<connect gate="D" pin="IO_32" pad="E14"/>
<connect gate="D" pin="IO_33" pad="E16"/>
<connect gate="D" pin="IO_34" pad="E17"/>
<connect gate="D" pin="IO_35" pad="E25"/>
<connect gate="D" pin="IO_36" pad="E26"/>
<connect gate="D" pin="IO_37" pad="E28"/>
<connect gate="D" pin="IO_38" pad="F11"/>
<connect gate="D" pin="IO_39" pad="F13"/>
<connect gate="D" pin="IO_4" pad="C20"/>
<connect gate="D" pin="IO_40" pad="F14"/>
<connect gate="D" pin="IO_41" pad="F15"/>
<connect gate="D" pin="IO_42" pad="F16"/>
<connect gate="D" pin="IO_43" pad="F17"/>
<connect gate="D" pin="IO_44" pad="F18"/>
<connect gate="D" pin="IO_45" pad="F19"/>
<connect gate="D" pin="IO_46" pad="F20"/>
<connect gate="D" pin="IO_47" pad="F21"/>
<connect gate="D" pin="IO_48" pad="F22"/>
<connect gate="D" pin="IO_49" pad="F23"/>
<connect gate="D" pin="IO_5" pad="C21"/>
<connect gate="D" pin="IO_50" pad="F24"/>
<connect gate="D" pin="IO_51" pad="F26"/>
<connect gate="D" pin="IO_52" pad="F27"/>
<connect gate="D" pin="IO_53" pad="F28"/>
<connect gate="D" pin="IO_54" pad="G10"/>
<connect gate="D" pin="IO_55" pad="G11"/>
<connect gate="D" pin="IO_56" pad="G12"/>
<connect gate="D" pin="IO_57" pad="G13"/>
<connect gate="D" pin="IO_58" pad="G14"/>
<connect gate="D" pin="IO_59" pad="G15"/>
<connect gate="D" pin="IO_6" pad="C22"/>
<connect gate="D" pin="IO_60" pad="G16"/>
<connect gate="D" pin="IO_61" pad="G17"/>
<connect gate="D" pin="IO_62" pad="G18"/>
<connect gate="D" pin="IO_63" pad="G19"/>
<connect gate="D" pin="IO_64" pad="G20"/>
<connect gate="D" pin="IO_65" pad="G21"/>
<connect gate="D" pin="IO_66" pad="G22"/>
<connect gate="D" pin="IO_67" pad="G23"/>
<connect gate="D" pin="IO_68" pad="G24"/>
<connect gate="D" pin="IO_69" pad="G25"/>
<connect gate="D" pin="IO_7" pad="C23"/>
<connect gate="D" pin="IO_70" pad="G26"/>
<connect gate="D" pin="IO_71" pad="G27"/>
<connect gate="D" pin="IO_72" pad="G28"/>
<connect gate="D" pin="IO_73" pad="H10"/>
<connect gate="D" pin="IO_74" pad="H11"/>
<connect gate="D" pin="IO_75" pad="H13"/>
<connect gate="D" pin="IO_8" pad="C24"/>
<connect gate="D" pin="IO_9" pad="C25"/>
<connect gate="D" pin="NC" pad="F25"/>
<connect gate="D" pin="NCE" pad="D24"/>
<connect gate="D" pin="NC_2" pad="C17"/>
<connect gate="D" pin="NC_3" pad="E22"/>
<connect gate="D" pin="NSTATUS" pad="E23"/>
<connect gate="D" pin="VCCIO3" pad="H17"/>
<connect gate="D" pin="VCCIO4" pad="H14"/>
<connect gate="D" pin="VREFB3N0" pad="E19"/>
<connect gate="D" pin="VREFB3N1" pad="E20"/>
<connect gate="D" pin="VREFB4N0" pad="F10"/>
<connect gate="D" pin="VREFB4N1" pad="F12"/>
<connect gate="E" pin="GND" pad="N19"/>
<connect gate="E" pin="GNDA_PLL5" pad="K15"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="J16"/>
<connect gate="E" pin="GND_10" pad="L27"/>
<connect gate="E" pin="GND_11" pad="M12"/>
<connect gate="E" pin="GND_12" pad="M14"/>
<connect gate="E" pin="GND_13" pad="M16"/>
<connect gate="E" pin="GND_14" pad="M18"/>
<connect gate="E" pin="GND_15" pad="M19"/>
<connect gate="E" pin="GND_16" pad="N10"/>
<connect gate="E" pin="GND_17" pad="N11"/>
<connect gate="E" pin="GND_18" pad="N13"/>
<connect gate="E" pin="GND_19" pad="N15"/>
<connect gate="E" pin="GND_2" pad="H21"/>
<connect gate="E" pin="GND_20" pad="N17"/>
<connect gate="E" pin="GND_3" pad="H24"/>
<connect gate="E" pin="GND_4" pad="H27"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="L15"/>
<connect gate="E" pin="GND_7" pad="L18"/>
<connect gate="E" pin="GND_8" pad="L21"/>
<connect gate="E" pin="GND_9" pad="L24"/>
<connect gate="E" pin="IO" pad="N20"/>
<connect gate="E" pin="IO_10" pad="J20"/>
<connect gate="E" pin="IO_11" pad="J21"/>
<connect gate="E" pin="IO_12" pad="J23"/>
<connect gate="E" pin="IO_13" pad="J24"/>
<connect gate="E" pin="IO_14" pad="J25"/>
<connect gate="E" pin="IO_15" pad="J26"/>
<connect gate="E" pin="IO_16" pad="J27"/>
<connect gate="E" pin="IO_17" pad="J28"/>
<connect gate="E" pin="IO_18" pad="K10"/>
<connect gate="E" pin="IO_19" pad="K11"/>
<connect gate="E" pin="IO_2" pad="H22"/>
<connect gate="E" pin="IO_20" pad="K12"/>
<connect gate="E" pin="IO_21" pad="K13"/>
<connect gate="E" pin="IO_22" pad="K14"/>
<connect gate="E" pin="IO_23" pad="K17"/>
<connect gate="E" pin="IO_24" pad="K18"/>
<connect gate="E" pin="IO_25" pad="K19"/>
<connect gate="E" pin="IO_26" pad="K20"/>
<connect gate="E" pin="IO_27" pad="K21"/>
<connect gate="E" pin="IO_28" pad="K22"/>
<connect gate="E" pin="IO_29" pad="K23"/>
<connect gate="E" pin="IO_3" pad="H23"/>
<connect gate="E" pin="IO_30" pad="K24"/>
<connect gate="E" pin="IO_31" pad="K25"/>
<connect gate="E" pin="IO_32" pad="K26"/>
<connect gate="E" pin="IO_33" pad="K27"/>
<connect gate="E" pin="IO_34" pad="K28"/>
<connect gate="E" pin="IO_35" pad="L12"/>
<connect gate="E" pin="IO_36" pad="L13"/>
<connect gate="E" pin="IO_37" pad="L14"/>
<connect gate="E" pin="IO_38" pad="L16"/>
<connect gate="E" pin="IO_39" pad="L17"/>
<connect gate="E" pin="IO_4" pad="H25"/>
<connect gate="E" pin="IO_40" pad="L19"/>
<connect gate="E" pin="IO_41" pad="L20"/>
<connect gate="E" pin="IO_42" pad="L23"/>
<connect gate="E" pin="IO_43" pad="L25"/>
<connect gate="E" pin="IO_44" pad="L26"/>
<connect gate="E" pin="IO_45" pad="L28"/>
<connect gate="E" pin="IO_46" pad="M20"/>
<connect gate="E" pin="IO_47" pad="M21"/>
<connect gate="E" pin="IO_48" pad="M22"/>
<connect gate="E" pin="IO_49" pad="M24"/>
<connect gate="E" pin="IO_5" pad="H26"/>
<connect gate="E" pin="IO_50" pad="M25"/>
<connect gate="E" pin="IO_51" pad="M26"/>
<connect gate="E" pin="IO_52" pad="M27"/>
<connect gate="E" pin="IO_53" pad="M28"/>
<connect gate="E" pin="IO_6" pad="H28"/>
<connect gate="E" pin="IO_7" pad="J10"/>
<connect gate="E" pin="IO_8" pad="J11"/>
<connect gate="E" pin="IO_9" pad="J18"/>
<connect gate="E" pin="VCCA_PLL5" pad="J15"/>
<connect gate="E" pin="VCCD_PLL1" pad="N22"/>
<connect gate="E" pin="VCCD_PLL5" pad="K16"/>
<connect gate="E" pin="VCCINT" pad="N18"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="M13"/>
<connect gate="E" pin="VCCINT_4" pad="M15"/>
<connect gate="E" pin="VCCINT_5" pad="M17"/>
<connect gate="E" pin="VCCINT_6" pad="N12"/>
<connect gate="E" pin="VCCINT_7" pad="N14"/>
<connect gate="E" pin="VCCINT_8" pad="N16"/>
<connect gate="E" pin="VCCIO2" pad="N21"/>
<connect gate="E" pin="VCCIO2_2" pad="J22"/>
<connect gate="E" pin="VCCIO2_3" pad="L22"/>
<connect gate="E" pin="VCCIO3" pad="J19"/>
<connect gate="E" pin="VCCIO3_2" pad="H20"/>
<connect gate="E" pin="VCCIO4" pad="J12"/>
<connect gate="E" pin="VCCP" pad="M10"/>
<connect gate="E" pin="VCCPD3" pad="J17"/>
<connect gate="E" pin="VCCPD4" pad="J13"/>
<connect gate="E" pin="VCCP_2" pad="L10"/>
<connect gate="E" pin="VCC_PLL5_OUT" pad="J14"/>
<connect gate="E" pin="VREFB2N1" pad="M23"/>
<connect gate="F" pin="CLK1N" pad="T24"/>
<connect gate="F" pin="CLK1P" pad="T25"/>
<connect gate="F" pin="CLK3N" pad="U25"/>
<connect gate="F" pin="CLK3P" pad="U26"/>
<connect gate="F" pin="GND" pad="V24"/>
<connect gate="F" pin="GNDA_PLL1" pad="P23"/>
<connect gate="F" pin="GNDA_PLL1_2" pad="P22"/>
<connect gate="F" pin="GNDA_PLL2" pad="R23"/>
<connect gate="F" pin="GNDA_PLL2_2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="P21"/>
<connect gate="F" pin="GND_11" pad="R11"/>
<connect gate="F" pin="GND_12" pad="R13"/>
<connect gate="F" pin="GND_13" pad="R15"/>
<connect gate="F" pin="GND_14" pad="R17"/>
<connect gate="F" pin="GND_15" pad="R19"/>
<connect gate="F" pin="GND_16" pad="R24"/>
<connect gate="F" pin="GND_17" pad="R27"/>
<connect gate="F" pin="GND_18" pad="T12"/>
<connect gate="F" pin="GND_19" pad="T14"/>
<connect gate="F" pin="GND_2" pad="N24"/>
<connect gate="F" pin="GND_20" pad="T16"/>
<connect gate="F" pin="GND_21" pad="T18"/>
<connect gate="F" pin="GND_22" pad="U10"/>
<connect gate="F" pin="GND_23" pad="U11"/>
<connect gate="F" pin="GND_24" pad="U13"/>
<connect gate="F" pin="GND_25" pad="U15"/>
<connect gate="F" pin="GND_26" pad="U17"/>
<connect gate="F" pin="GND_27" pad="U21"/>
<connect gate="F" pin="GND_28" pad="V10"/>
<connect gate="F" pin="GND_29" pad="V12"/>
<connect gate="F" pin="GND_3" pad="N27"/>
<connect gate="F" pin="GND_30" pad="V15"/>
<connect gate="F" pin="GND_31" pad="V18"/>
<connect gate="F" pin="GND_4" pad="P10"/>
<connect gate="F" pin="GND_5" pad="P12"/>
<connect gate="F" pin="GND_6" pad="P14"/>
<connect gate="F" pin="GND_7" pad="P16"/>
<connect gate="F" pin="GND_8" pad="P18"/>
<connect gate="F" pin="GND_9" pad="P19"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="R20"/>
<connect gate="F" pin="IO_11" pad="R21"/>
<connect gate="F" pin="IO_12" pad="R25"/>
<connect gate="F" pin="IO_13" pad="R26"/>
<connect gate="F" pin="IO_14" pad="R28"/>
<connect gate="F" pin="IO_15" pad="T19"/>
<connect gate="F" pin="IO_16" pad="T26"/>
<connect gate="F" pin="IO_17" pad="T27"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U19"/>
<connect gate="F" pin="IO_2" pad="N25"/>
<connect gate="F" pin="IO_20" pad="U20"/>
<connect gate="F" pin="IO_21" pad="U23"/>
<connect gate="F" pin="IO_22" pad="U24"/>
<connect gate="F" pin="IO_23" pad="U27"/>
<connect gate="F" pin="IO_24" pad="U28"/>
<connect gate="F" pin="IO_25" pad="V11"/>
<connect gate="F" pin="IO_26" pad="V13"/>
<connect gate="F" pin="IO_27" pad="V20"/>
<connect gate="F" pin="IO_28" pad="V22"/>
<connect gate="F" pin="IO_29" pad="V23"/>
<connect gate="F" pin="IO_3" pad="N26"/>
<connect gate="F" pin="IO_4" pad="N28"/>
<connect gate="F" pin="IO_5" pad="P24"/>
<connect gate="F" pin="IO_6" pad="P25"/>
<connect gate="F" pin="IO_7" pad="P26"/>
<connect gate="F" pin="IO_8" pad="P27"/>
<connect gate="F" pin="IO_9" pad="P28"/>
<connect gate="F" pin="NCONFIG" pad="V17"/>
<connect gate="F" pin="TCK" pad="V16"/>
<connect gate="F" pin="TDI" pad="V19"/>
<connect gate="F" pin="VCCA_PLL1" pad="N23"/>
<connect gate="F" pin="VCCA_PLL2" pad="T23"/>
<connect gate="F" pin="VCCD_PLL2" pad="T22"/>
<connect gate="F" pin="VCCD_PLL6" pad="V14"/>
<connect gate="F" pin="VCCINT" pad="U18"/>
<connect gate="F" pin="VCCINT_10" pad="T11"/>
<connect gate="F" pin="VCCINT_11" pad="T13"/>
<connect gate="F" pin="VCCINT_12" pad="T15"/>
<connect gate="F" pin="VCCINT_13" pad="T17"/>
<connect gate="F" pin="VCCINT_14" pad="U12"/>
<connect gate="F" pin="VCCINT_15" pad="U14"/>
<connect gate="F" pin="VCCINT_16" pad="U16"/>
<connect gate="F" pin="VCCINT_2" pad="P11"/>
<connect gate="F" pin="VCCINT_3" pad="P13"/>
<connect gate="F" pin="VCCINT_4" pad="P15"/>
<connect gate="F" pin="VCCINT_5" pad="P17"/>
<connect gate="F" pin="VCCINT_6" pad="R12"/>
<connect gate="F" pin="VCCINT_7" pad="R14"/>
<connect gate="F" pin="VCCINT_8" pad="R16"/>
<connect gate="F" pin="VCCINT_9" pad="R18"/>
<connect gate="F" pin="VCCIO1" pad="V21"/>
<connect gate="F" pin="VCCIO1_2" pad="U22"/>
<connect gate="F" pin="VCCP" pad="T10"/>
<connect gate="F" pin="VCCPD1" pad="T20"/>
<connect gate="F" pin="VCCPD2" pad="P20"/>
<connect gate="F" pin="VCCP_2" pad="R10"/>
<connect gate="F" pin="VREFB2N0" pad="T21"/>
<connect gate="G" pin="GND" pad="AA27"/>
<connect gate="G" pin="GNDA_PLL6" pad="W14"/>
<connect gate="G" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="G" pin="GND_10" pad="AA21"/>
<connect gate="G" pin="GND_11" pad="AA24"/>
<connect gate="G" pin="GND_2" pad="V27"/>
<connect gate="G" pin="GND_3" pad="W20"/>
<connect gate="G" pin="GND_4" pad="W22"/>
<connect gate="G" pin="GND_5" pad="Y20"/>
<connect gate="G" pin="GND_6" pad="AA12"/>
<connect gate="G" pin="GND_7" pad="AA15"/>
<connect gate="G" pin="GND_8" pad="AA18"/>
<connect gate="G" pin="GND_9" pad="AA20"/>
<connect gate="G" pin="IO" pad="AB20"/>
<connect gate="G" pin="IO_10" pad="AC11"/>
<connect gate="G" pin="IO_11" pad="AC12"/>
<connect gate="G" pin="IO_12" pad="AC13"/>
<connect gate="G" pin="IO_13" pad="AC14"/>
<connect gate="G" pin="IO_14" pad="AC15"/>
<connect gate="G" pin="IO_15" pad="AC16"/>
<connect gate="G" pin="IO_16" pad="AC17"/>
<connect gate="G" pin="IO_17" pad="AC18"/>
<connect gate="G" pin="IO_18" pad="AC19"/>
<connect gate="G" pin="IO_19" pad="AC20"/>
<connect gate="G" pin="IO_2" pad="AB21"/>
<connect gate="G" pin="IO_20" pad="AC21"/>
<connect gate="G" pin="IO_21" pad="AC22"/>
<connect gate="G" pin="IO_22" pad="AC23"/>
<connect gate="G" pin="IO_23" pad="AC24"/>
<connect gate="G" pin="IO_24" pad="AC25"/>
<connect gate="G" pin="IO_25" pad="AC26"/>
<connect gate="G" pin="IO_26" pad="AC27"/>
<connect gate="G" pin="IO_27" pad="AC28"/>
<connect gate="G" pin="IO_28" pad="V26"/>
<connect gate="G" pin="IO_29" pad="V28"/>
<connect gate="G" pin="IO_3" pad="AB22"/>
<connect gate="G" pin="IO_30" pad="W10"/>
<connect gate="G" pin="IO_31" pad="W11"/>
<connect gate="G" pin="IO_32" pad="W12"/>
<connect gate="G" pin="IO_33" pad="W15"/>
<connect gate="G" pin="IO_34" pad="W16"/>
<connect gate="G" pin="IO_35" pad="W21"/>
<connect gate="G" pin="IO_36" pad="W24"/>
<connect gate="G" pin="IO_37" pad="W25"/>
<connect gate="G" pin="IO_38" pad="W26"/>
<connect gate="G" pin="IO_39" pad="W27"/>
<connect gate="G" pin="IO_4" pad="AB23"/>
<connect gate="G" pin="IO_40" pad="W28"/>
<connect gate="G" pin="IO_41" pad="Y10"/>
<connect gate="G" pin="IO_42" pad="Y11"/>
<connect gate="G" pin="IO_43" pad="Y13"/>
<connect gate="G" pin="IO_44" pad="Y15"/>
<connect gate="G" pin="IO_45" pad="Y17"/>
<connect gate="G" pin="IO_46" pad="Y21"/>
<connect gate="G" pin="IO_47" pad="Y24"/>
<connect gate="G" pin="IO_48" pad="Y25"/>
<connect gate="G" pin="IO_49" pad="Y26"/>
<connect gate="G" pin="IO_5" pad="AB24"/>
<connect gate="G" pin="IO_50" pad="Y27"/>
<connect gate="G" pin="IO_51" pad="Y28"/>
<connect gate="G" pin="IO_52" pad="AA11"/>
<connect gate="G" pin="IO_53" pad="AA17"/>
<connect gate="G" pin="IO_54" pad="AA19"/>
<connect gate="G" pin="IO_55" pad="AA22"/>
<connect gate="G" pin="IO_56" pad="AA23"/>
<connect gate="G" pin="IO_57" pad="AA25"/>
<connect gate="G" pin="IO_58" pad="AA26"/>
<connect gate="G" pin="IO_59" pad="AA28"/>
<connect gate="G" pin="IO_6" pad="AB25"/>
<connect gate="G" pin="IO_60" pad="AB10"/>
<connect gate="G" pin="IO_61" pad="AB11"/>
<connect gate="G" pin="IO_62" pad="AB12"/>
<connect gate="G" pin="IO_63" pad="AB13"/>
<connect gate="G" pin="IO_64" pad="AB15"/>
<connect gate="G" pin="IO_65" pad="AB16"/>
<connect gate="G" pin="IO_66" pad="AB17"/>
<connect gate="G" pin="IO_67" pad="AB18"/>
<connect gate="G" pin="IO_68" pad="AB19"/>
<connect gate="G" pin="IO_7" pad="AB26"/>
<connect gate="G" pin="IO_8" pad="AB27"/>
<connect gate="G" pin="IO_9" pad="AB28"/>
<connect gate="G" pin="TMS" pad="W19"/>
<connect gate="G" pin="TRST" pad="W17"/>
<connect gate="G" pin="VCCA_PLL6" pad="Y14"/>
<connect gate="G" pin="VCCIO1" pad="Y22"/>
<connect gate="G" pin="VCCIO7" pad="AA13"/>
<connect gate="G" pin="VCCIO7_2" pad="AA10"/>
<connect gate="G" pin="VCCIO8" pad="AA16"/>
<connect gate="G" pin="VCCIO8_2" pad="Y18"/>
<connect gate="G" pin="VCCIO8_3" pad="Y19"/>
<connect gate="G" pin="VCCPD7" pad="Y12"/>
<connect gate="G" pin="VCCPD8" pad="Y16"/>
<connect gate="G" pin="VCCSEL" pad="W18"/>
<connect gate="G" pin="VCC_PLL6_OUT" pad="AA14"/>
<connect gate="G" pin="VREFB1N0" pad="Y23"/>
<connect gate="G" pin="VREFB1N1" pad="W23"/>
<connect gate="G" pin="VREFB7N0" pad="AB14"/>
<connect gate="G" pin="VREFB7N1" pad="AC10"/>
<connect gate="H" pin="GND" pad="AH27"/>
<connect gate="H" pin="GND_10" pad="AG18"/>
<connect gate="H" pin="GND_11" pad="AG21"/>
<connect gate="H" pin="GND_12" pad="AG24"/>
<connect gate="H" pin="GND_13" pad="AG27"/>
<connect gate="H" pin="GND_14" pad="AG28"/>
<connect gate="H" pin="GND_2" pad="AD12"/>
<connect gate="H" pin="GND_3" pad="AD15"/>
<connect gate="H" pin="GND_4" pad="AD18"/>
<connect gate="H" pin="GND_5" pad="AD21"/>
<connect gate="H" pin="GND_6" pad="AD24"/>
<connect gate="H" pin="GND_7" pad="AD27"/>
<connect gate="H" pin="GND_8" pad="AG12"/>
<connect gate="H" pin="GND_9" pad="AG15"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD28"/>
<connect gate="H" pin="IO_11" pad="AE10"/>
<connect gate="H" pin="IO_12" pad="AE11"/>
<connect gate="H" pin="IO_13" pad="AE12"/>
<connect gate="H" pin="IO_14" pad="AE13"/>
<connect gate="H" pin="IO_15" pad="AE14"/>
<connect gate="H" pin="IO_16" pad="AE15"/>
<connect gate="H" pin="IO_17" pad="AE17"/>
<connect gate="H" pin="IO_18" pad="AE18"/>
<connect gate="H" pin="IO_19" pad="AE19"/>
<connect gate="H" pin="IO_2" pad="AD10"/>
<connect gate="H" pin="IO_20" pad="AE20"/>
<connect gate="H" pin="IO_21" pad="AE21"/>
<connect gate="H" pin="IO_22" pad="AE22"/>
<connect gate="H" pin="IO_23" pad="AE23"/>
<connect gate="H" pin="IO_24" pad="AE24"/>
<connect gate="H" pin="IO_25" pad="AE25"/>
<connect gate="H" pin="IO_26" pad="AE26"/>
<connect gate="H" pin="IO_27" pad="AE27"/>
<connect gate="H" pin="IO_28" pad="AE28"/>
<connect gate="H" pin="IO_29" pad="AF10"/>
<connect gate="H" pin="IO_3" pad="AD11"/>
<connect gate="H" pin="IO_30" pad="AF11"/>
<connect gate="H" pin="IO_31" pad="AF12"/>
<connect gate="H" pin="IO_32" pad="AF21"/>
<connect gate="H" pin="IO_33" pad="AF22"/>
<connect gate="H" pin="IO_34" pad="AF23"/>
<connect gate="H" pin="IO_35" pad="AF24"/>
<connect gate="H" pin="IO_36" pad="AF25"/>
<connect gate="H" pin="IO_37" pad="AF26"/>
<connect gate="H" pin="IO_38" pad="AF27"/>
<connect gate="H" pin="IO_39" pad="AF28"/>
<connect gate="H" pin="IO_4" pad="AD13"/>
<connect gate="H" pin="IO_40" pad="AG10"/>
<connect gate="H" pin="IO_41" pad="AG11"/>
<connect gate="H" pin="IO_42" pad="AG13"/>
<connect gate="H" pin="IO_43" pad="AG14"/>
<connect gate="H" pin="IO_44" pad="AG16"/>
<connect gate="H" pin="IO_45" pad="AG17"/>
<connect gate="H" pin="IO_46" pad="AG19"/>
<connect gate="H" pin="IO_47" pad="AG20"/>
<connect gate="H" pin="IO_48" pad="AG22"/>
<connect gate="H" pin="IO_49" pad="AG23"/>
<connect gate="H" pin="IO_5" pad="AD14"/>
<connect gate="H" pin="IO_50" pad="AG25"/>
<connect gate="H" pin="IO_51" pad="AG26"/>
<connect gate="H" pin="IO_52" pad="AH10"/>
<connect gate="H" pin="IO_53" pad="AH11"/>
<connect gate="H" pin="IO_54" pad="AH12"/>
<connect gate="H" pin="IO_55" pad="AH13"/>
<connect gate="H" pin="IO_56" pad="AH14"/>
<connect gate="H" pin="IO_57" pad="AH15"/>
<connect gate="H" pin="IO_58" pad="AH16"/>
<connect gate="H" pin="IO_59" pad="AF13"/>
<connect gate="H" pin="IO_6" pad="AD16"/>
<connect gate="H" pin="IO_60" pad="AH17"/>
<connect gate="H" pin="IO_61" pad="AF14"/>
<connect gate="H" pin="IO_62" pad="AH18"/>
<connect gate="H" pin="IO_63" pad="AF15"/>
<connect gate="H" pin="IO_64" pad="AH19"/>
<connect gate="H" pin="IO_65" pad="AF17"/>
<connect gate="H" pin="IO_66" pad="AH20"/>
<connect gate="H" pin="IO_67" pad="AF18"/>
<connect gate="H" pin="IO_68" pad="AH21"/>
<connect gate="H" pin="IO_69" pad="AF19"/>
<connect gate="H" pin="IO_7" pad="AD20"/>
<connect gate="H" pin="IO_70" pad="AH22"/>
<connect gate="H" pin="IO_71" pad="AF20"/>
<connect gate="H" pin="IO_72" pad="AH23"/>
<connect gate="H" pin="IO_73" pad="AH24"/>
<connect gate="H" pin="IO_74" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD25"/>
<connect gate="H" pin="IO_9" pad="AD26"/>
<connect gate="H" pin="NC" pad="AF16"/>
<connect gate="H" pin="NC_2" pad="AD22"/>
<connect gate="H" pin="NC_3" pad="AD23"/>
<connect gate="H" pin="NC_4" pad="AE16"/>
<connect gate="H" pin="VREFB8N0" pad="AD19"/>
<connect gate="H" pin="VREFB8N1" pad="AD17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2SGX30CF780C5N"/>
<attribute name="OC_FARNELL" value="1637242"/>
<attribute name="OC_NEWARK" value="51R0578"/>
<attribute name="PACKAGE" value="BGA-780"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2SGX30DF780C3N">
<description>FPGA, STRATIX II GX</description>
<gates>
<gate name="A" symbol="EP2SGX30DF780C3N_A"/>
<gate name="B" symbol="EP2SGX30DF780C3N_B"/>
<gate name="C" symbol="EP2SGX30DF780C3N_C"/>
<gate name="D" symbol="EP2SGX30DF780C3N_D"/>
<gate name="E" symbol="EP2SGX30DF780C3N_E"/>
<gate name="F" symbol="EP2SGX30DF780C3N_F"/>
<gate name="G" symbol="EP2SGX30DF780C3N_G"/>
<gate name="H" symbol="EP2SGX30DF780C3N_H"/>
</gates>
<devices>
<device name="" package="BGA780C100P28X28_2900X2900X350">
<connects>
<connect gate="A" pin="GND" pad="L3"/>
<connect gate="A" pin="GND_10" pad="B4"/>
<connect gate="A" pin="GND_11" pad="B5"/>
<connect gate="A" pin="GND_12" pad="B6"/>
<connect gate="A" pin="GND_13" pad="B7"/>
<connect gate="A" pin="GND_14" pad="B9"/>
<connect gate="A" pin="GND_15" pad="C1"/>
<connect gate="A" pin="GND_16" pad="C2"/>
<connect gate="A" pin="GND_17" pad="C3"/>
<connect gate="A" pin="GND_18" pad="C6"/>
<connect gate="A" pin="GND_19" pad="D1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_20" pad="D2"/>
<connect gate="A" pin="GND_21" pad="D3"/>
<connect gate="A" pin="GND_22" pad="D4"/>
<connect gate="A" pin="GND_23" pad="D5"/>
<connect gate="A" pin="GND_24" pad="D6"/>
<connect gate="A" pin="GND_25" pad="E3"/>
<connect gate="A" pin="GND_26" pad="E6"/>
<connect gate="A" pin="GND_27" pad="E7"/>
<connect gate="A" pin="GND_28" pad="E9"/>
<connect gate="A" pin="GND_29" pad="F1"/>
<connect gate="A" pin="GND_3" pad="A3"/>
<connect gate="A" pin="GND_30" pad="F2"/>
<connect gate="A" pin="GND_31" pad="F3"/>
<connect gate="A" pin="GND_32" pad="F4"/>
<connect gate="A" pin="GND_33" pad="F5"/>
<connect gate="A" pin="GND_34" pad="F6"/>
<connect gate="A" pin="GND_35" pad="G3"/>
<connect gate="A" pin="GND_36" pad="G6"/>
<connect gate="A" pin="GND_37" pad="H1"/>
<connect gate="A" pin="GND_38" pad="H2"/>
<connect gate="A" pin="GND_39" pad="H3"/>
<connect gate="A" pin="GND_4" pad="A4"/>
<connect gate="A" pin="GND_40" pad="H4"/>
<connect gate="A" pin="GND_41" pad="H5"/>
<connect gate="A" pin="GND_42" pad="H6"/>
<connect gate="A" pin="GND_43" pad="H7"/>
<connect gate="A" pin="GND_44" pad="H9"/>
<connect gate="A" pin="GND_45" pad="J3"/>
<connect gate="A" pin="GND_46" pad="J5"/>
<connect gate="A" pin="GND_47" pad="J6"/>
<connect gate="A" pin="GND_48" pad="J7"/>
<connect gate="A" pin="GND_49" pad="K1"/>
<connect gate="A" pin="GND_5" pad="A5"/>
<connect gate="A" pin="GND_50" pad="K2"/>
<connect gate="A" pin="GND_51" pad="K3"/>
<connect gate="A" pin="GND_52" pad="K4"/>
<connect gate="A" pin="GND_53" pad="K5"/>
<connect gate="A" pin="GND_54" pad="K6"/>
<connect gate="A" pin="GND_6" pad="A6"/>
<connect gate="A" pin="GND_7" pad="B1"/>
<connect gate="A" pin="GND_8" pad="B2"/>
<connect gate="A" pin="GND_9" pad="B3"/>
<connect gate="A" pin="GXB_RX0N" pad="G2"/>
<connect gate="A" pin="GXB_RX0P" pad="G1"/>
<connect gate="A" pin="GXB_RX1N" pad="E2"/>
<connect gate="A" pin="GXB_RX1P" pad="E1"/>
<connect gate="A" pin="GXB_RX2N" pad="L2"/>
<connect gate="A" pin="GXB_RX2P" pad="L1"/>
<connect gate="A" pin="GXB_TX0N" pad="E5"/>
<connect gate="A" pin="GXB_TX0P" pad="E4"/>
<connect gate="A" pin="GXB_TX1N" pad="C5"/>
<connect gate="A" pin="GXB_TX1P" pad="C4"/>
<connect gate="A" pin="GXB_TX2N" pad="L5"/>
<connect gate="A" pin="GXB_TX2P" pad="L4"/>
<connect gate="A" pin="IO" pad="G9"/>
<connect gate="A" pin="IO_10" pad="D8"/>
<connect gate="A" pin="IO_11" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A8"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_5" pad="B8"/>
<connect gate="A" pin="IO_6" pad="C7"/>
<connect gate="A" pin="IO_7" pad="C8"/>
<connect gate="A" pin="IO_8" pad="C9"/>
<connect gate="A" pin="IO_9" pad="D7"/>
<connect gate="A" pin="MSEL0" pad="J8"/>
<connect gate="A" pin="MSEL1" pad="E8"/>
<connect gate="A" pin="MSEL2" pad="H8"/>
<connect gate="A" pin="MSEL3" pad="G8"/>
<connect gate="A" pin="NC" pad="K8"/>
<connect gate="A" pin="NC_2" pad="F9"/>
<connect gate="A" pin="NC_3" pad="K7"/>
<connect gate="A" pin="REFCLK0_B13N" pad="J2"/>
<connect gate="A" pin="REFCLK0_B13P" pad="J1"/>
<connect gate="A" pin="REFCLK1_B13N" pad="G5"/>
<connect gate="A" pin="REFCLK1_B13P" pad="G4"/>
<connect gate="A" pin="RREFB13" pad="J4"/>
<connect gate="A" pin="TDO" pad="F8"/>
<connect gate="A" pin="TEMPDIODEN" pad="G7"/>
<connect gate="A" pin="TEMPDIODEP" pad="F7"/>
<connect gate="A" pin="VCCA" pad="L6"/>
<connect gate="A" pin="VCCA_2" pad="K9"/>
<connect gate="A" pin="VCCH_B13" pad="L9"/>
<connect gate="A" pin="VCCIO4" pad="J9"/>
<connect gate="A" pin="VCCR" pad="L7"/>
<connect gate="A" pin="VCCT_B13" pad="L8"/>
<connect gate="B" pin="GND" pad="Y6"/>
<connect gate="B" pin="GND_10" pad="N9"/>
<connect gate="B" pin="GND_11" pad="P1"/>
<connect gate="B" pin="GND_12" pad="P2"/>
<connect gate="B" pin="GND_13" pad="P3"/>
<connect gate="B" pin="GND_14" pad="P4"/>
<connect gate="B" pin="GND_15" pad="P5"/>
<connect gate="B" pin="GND_16" pad="P6"/>
<connect gate="B" pin="GND_17" pad="P8"/>
<connect gate="B" pin="GND_18" pad="R1"/>
<connect gate="B" pin="GND_19" pad="R2"/>
<connect gate="B" pin="GND_2" pad="M1"/>
<connect gate="B" pin="GND_20" pad="R3"/>
<connect gate="B" pin="GND_21" pad="R4"/>
<connect gate="B" pin="GND_22" pad="R5"/>
<connect gate="B" pin="GND_23" pad="T3"/>
<connect gate="B" pin="GND_24" pad="U1"/>
<connect gate="B" pin="GND_25" pad="U2"/>
<connect gate="B" pin="GND_26" pad="U3"/>
<connect gate="B" pin="GND_27" pad="U4"/>
<connect gate="B" pin="GND_28" pad="U5"/>
<connect gate="B" pin="GND_29" pad="U7"/>
<connect gate="B" pin="GND_3" pad="M2"/>
<connect gate="B" pin="GND_30" pad="U8"/>
<connect gate="B" pin="GND_31" pad="U9"/>
<connect gate="B" pin="GND_32" pad="V3"/>
<connect gate="B" pin="GND_33" pad="V6"/>
<connect gate="B" pin="GND_34" pad="V8"/>
<connect gate="B" pin="GND_35" pad="W1"/>
<connect gate="B" pin="GND_36" pad="W2"/>
<connect gate="B" pin="GND_37" pad="W3"/>
<connect gate="B" pin="GND_38" pad="W4"/>
<connect gate="B" pin="GND_39" pad="W5"/>
<connect gate="B" pin="GND_4" pad="M3"/>
<connect gate="B" pin="GND_40" pad="W6"/>
<connect gate="B" pin="GND_41" pad="W7"/>
<connect gate="B" pin="GND_42" pad="W8"/>
<connect gate="B" pin="GND_43" pad="Y3"/>
<connect gate="B" pin="GND_44" pad="Y5"/>
<connect gate="B" pin="GND_5" pad="M4"/>
<connect gate="B" pin="GND_6" pad="M5"/>
<connect gate="B" pin="GND_7" pad="N3"/>
<connect gate="B" pin="GND_8" pad="N7"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GXB_RX3N" pad="N2"/>
<connect gate="B" pin="GXB_RX3P" pad="N1"/>
<connect gate="B" pin="GXB_TX3N" pad="N5"/>
<connect gate="B" pin="GXB_TX3P" pad="N4"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="A17"/>
<connect gate="B" pin="IO_11" pad="A18"/>
<connect gate="B" pin="IO_12" pad="A19"/>
<connect gate="B" pin="IO_13" pad="A20"/>
<connect gate="B" pin="IO_14" pad="A21"/>
<connect gate="B" pin="IO_15" pad="A22"/>
<connect gate="B" pin="IO_16" pad="A23"/>
<connect gate="B" pin="IO_17" pad="A24"/>
<connect gate="B" pin="IO_18" pad="A25"/>
<connect gate="B" pin="IO_2" pad="W9"/>
<connect gate="B" pin="IO_3" pad="A10"/>
<connect gate="B" pin="IO_4" pad="A11"/>
<connect gate="B" pin="IO_5" pad="A12"/>
<connect gate="B" pin="IO_6" pad="A13"/>
<connect gate="B" pin="IO_7" pad="A14"/>
<connect gate="B" pin="IO_8" pad="A15"/>
<connect gate="B" pin="IO_9" pad="A16"/>
<connect gate="B" pin="NC" pad="Y4"/>
<connect gate="B" pin="NC_10" pad="Y1"/>
<connect gate="B" pin="NC_11" pad="Y2"/>
<connect gate="B" pin="NC_2" pad="T1"/>
<connect gate="B" pin="NC_3" pad="T2"/>
<connect gate="B" pin="NC_4" pad="T4"/>
<connect gate="B" pin="NC_5" pad="T5"/>
<connect gate="B" pin="NC_6" pad="V1"/>
<connect gate="B" pin="NC_7" pad="V2"/>
<connect gate="B" pin="NC_8" pad="V4"/>
<connect gate="B" pin="NC_9" pad="V5"/>
<connect gate="B" pin="NIO_PULLUP" pad="Y7"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA" pad="V9"/>
<connect gate="B" pin="VCCA_2" pad="M6"/>
<connect gate="B" pin="VCCA_3" pad="P7"/>
<connect gate="B" pin="VCCA_4" pad="P9"/>
<connect gate="B" pin="VCCA_5" pad="R6"/>
<connect gate="B" pin="VCCA_6" pad="T6"/>
<connect gate="B" pin="VCCA_7" pad="V7"/>
<connect gate="B" pin="VCCH_B13" pad="M9"/>
<connect gate="B" pin="VCCH_B14" pad="T9"/>
<connect gate="B" pin="VCCH_B14_2" pad="R9"/>
<connect gate="B" pin="VCCIO7" pad="Y9"/>
<connect gate="B" pin="VCCL_B13" pad="N6"/>
<connect gate="B" pin="VCCL_B14" pad="U6"/>
<connect gate="B" pin="VCCR" pad="T7"/>
<connect gate="B" pin="VCCR_2" pad="M7"/>
<connect gate="B" pin="VCCR_3" pad="R7"/>
<connect gate="B" pin="VCCT_B13" pad="M8"/>
<connect gate="B" pin="VCCT_B14" pad="T8"/>
<connect gate="B" pin="VCCT_B14_2" pad="R8"/>
<connect gate="C" pin="GND" pad="B28"/>
<connect gate="C" pin="GND_10" pad="AA9"/>
<connect gate="C" pin="GND_11" pad="AB3"/>
<connect gate="C" pin="GND_12" pad="AB6"/>
<connect gate="C" pin="GND_13" pad="AC1"/>
<connect gate="C" pin="GND_14" pad="AC2"/>
<connect gate="C" pin="GND_15" pad="AC3"/>
<connect gate="C" pin="GND_16" pad="AC4"/>
<connect gate="C" pin="GND_17" pad="AC5"/>
<connect gate="C" pin="GND_18" pad="AC6"/>
<connect gate="C" pin="GND_19" pad="AC7"/>
<connect gate="C" pin="GND_2" pad="A27"/>
<connect gate="C" pin="GND_20" pad="AD3"/>
<connect gate="C" pin="GND_21" pad="AD6"/>
<connect gate="C" pin="GND_22" pad="AD7"/>
<connect gate="C" pin="GND_23" pad="AD9"/>
<connect gate="C" pin="GND_24" pad="AE1"/>
<connect gate="C" pin="GND_25" pad="AE2"/>
<connect gate="C" pin="GND_26" pad="AE3"/>
<connect gate="C" pin="GND_27" pad="AE4"/>
<connect gate="C" pin="GND_28" pad="AE5"/>
<connect gate="C" pin="GND_29" pad="AE6"/>
<connect gate="C" pin="GND_3" pad="AA1"/>
<connect gate="C" pin="GND_30" pad="AF1"/>
<connect gate="C" pin="GND_31" pad="AF2"/>
<connect gate="C" pin="GND_32" pad="AF3"/>
<connect gate="C" pin="GND_33" pad="AF6"/>
<connect gate="C" pin="GND_34" pad="AG1"/>
<connect gate="C" pin="GND_35" pad="AG2"/>
<connect gate="C" pin="GND_36" pad="AG3"/>
<connect gate="C" pin="GND_37" pad="AG4"/>
<connect gate="C" pin="GND_38" pad="AG5"/>
<connect gate="C" pin="GND_39" pad="AG6"/>
<connect gate="C" pin="GND_4" pad="AA2"/>
<connect gate="C" pin="GND_40" pad="AG7"/>
<connect gate="C" pin="GND_41" pad="AG9"/>
<connect gate="C" pin="GND_42" pad="AH2"/>
<connect gate="C" pin="GND_43" pad="AH3"/>
<connect gate="C" pin="GND_44" pad="AH4"/>
<connect gate="C" pin="GND_45" pad="AH5"/>
<connect gate="C" pin="GND_46" pad="AH6"/>
<connect gate="C" pin="GND_47" pad="B12"/>
<connect gate="C" pin="GND_48" pad="B15"/>
<connect gate="C" pin="GND_49" pad="B18"/>
<connect gate="C" pin="GND_5" pad="AA3"/>
<connect gate="C" pin="GND_50" pad="B21"/>
<connect gate="C" pin="GND_51" pad="B24"/>
<connect gate="C" pin="GND_52" pad="B27"/>
<connect gate="C" pin="GND_6" pad="AA4"/>
<connect gate="C" pin="GND_7" pad="AA5"/>
<connect gate="C" pin="GND_8" pad="AA6"/>
<connect gate="C" pin="GND_9" pad="AA7"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AF8"/>
<connect gate="C" pin="IO_11" pad="AF9"/>
<connect gate="C" pin="IO_12" pad="AG8"/>
<connect gate="C" pin="IO_13" pad="AH7"/>
<connect gate="C" pin="IO_14" pad="AH8"/>
<connect gate="C" pin="IO_15" pad="AH9"/>
<connect gate="C" pin="IO_16" pad="B10"/>
<connect gate="C" pin="IO_17" pad="B11"/>
<connect gate="C" pin="IO_18" pad="B13"/>
<connect gate="C" pin="IO_19" pad="B14"/>
<connect gate="C" pin="IO_2" pad="AB8"/>
<connect gate="C" pin="IO_20" pad="B16"/>
<connect gate="C" pin="IO_21" pad="B17"/>
<connect gate="C" pin="IO_22" pad="B19"/>
<connect gate="C" pin="IO_23" pad="B20"/>
<connect gate="C" pin="IO_24" pad="B22"/>
<connect gate="C" pin="IO_25" pad="B23"/>
<connect gate="C" pin="IO_26" pad="B25"/>
<connect gate="C" pin="IO_27" pad="B26"/>
<connect gate="C" pin="IO_28" pad="C10"/>
<connect gate="C" pin="IO_29" pad="C11"/>
<connect gate="C" pin="IO_3" pad="AB9"/>
<connect gate="C" pin="IO_30" pad="C12"/>
<connect gate="C" pin="IO_31" pad="C13"/>
<connect gate="C" pin="IO_32" pad="C14"/>
<connect gate="C" pin="IO_33" pad="C15"/>
<connect gate="C" pin="IO_4" pad="AC8"/>
<connect gate="C" pin="IO_5" pad="AC9"/>
<connect gate="C" pin="IO_6" pad="AE7"/>
<connect gate="C" pin="IO_7" pad="AE8"/>
<connect gate="C" pin="IO_8" pad="AE9"/>
<connect gate="C" pin="IO_9" pad="AF7"/>
<connect gate="C" pin="NC" pad="AF5"/>
<connect gate="C" pin="NCEO" pad="AB7"/>
<connect gate="C" pin="NC_10" pad="AB1"/>
<connect gate="C" pin="NC_11" pad="AF4"/>
<connect gate="C" pin="NC_2" pad="AB2"/>
<connect gate="C" pin="NC_3" pad="AB4"/>
<connect gate="C" pin="NC_4" pad="AB5"/>
<connect gate="C" pin="NC_5" pad="AD1"/>
<connect gate="C" pin="NC_6" pad="AD2"/>
<connect gate="C" pin="NC_7" pad="AD4"/>
<connect gate="C" pin="NC_8" pad="AD5"/>
<connect gate="C" pin="NC_9" pad="AD8"/>
<connect gate="C" pin="PLL_ENA" pad="AA8"/>
<connect gate="D" pin="CONF_DONE" pad="D26"/>
<connect gate="D" pin="DCLK" pad="D25"/>
<connect gate="D" pin="GND" pad="H18"/>
<connect gate="D" pin="GND_10" pad="H16"/>
<connect gate="D" pin="GND_2" pad="E12"/>
<connect gate="D" pin="GND_3" pad="E15"/>
<connect gate="D" pin="GND_4" pad="E18"/>
<connect gate="D" pin="GND_5" pad="E21"/>
<connect gate="D" pin="GND_6" pad="E24"/>
<connect gate="D" pin="GND_7" pad="E27"/>
<connect gate="D" pin="GND_8" pad="H12"/>
<connect gate="D" pin="GND_9" pad="H15"/>
<connect gate="D" pin="IO" pad="H19"/>
<connect gate="D" pin="IO_10" pad="C26"/>
<connect gate="D" pin="IO_11" pad="C27"/>
<connect gate="D" pin="IO_12" pad="C28"/>
<connect gate="D" pin="IO_13" pad="D10"/>
<connect gate="D" pin="IO_14" pad="D11"/>
<connect gate="D" pin="IO_15" pad="D12"/>
<connect gate="D" pin="IO_16" pad="D13"/>
<connect gate="D" pin="IO_17" pad="D14"/>
<connect gate="D" pin="IO_18" pad="D15"/>
<connect gate="D" pin="IO_19" pad="D16"/>
<connect gate="D" pin="IO_2" pad="C18"/>
<connect gate="D" pin="IO_20" pad="D17"/>
<connect gate="D" pin="IO_21" pad="D18"/>
<connect gate="D" pin="IO_22" pad="D19"/>
<connect gate="D" pin="IO_23" pad="D20"/>
<connect gate="D" pin="IO_24" pad="D21"/>
<connect gate="D" pin="IO_25" pad="D22"/>
<connect gate="D" pin="IO_26" pad="D23"/>
<connect gate="D" pin="IO_27" pad="D27"/>
<connect gate="D" pin="IO_28" pad="D28"/>
<connect gate="D" pin="IO_29" pad="E10"/>
<connect gate="D" pin="IO_3" pad="C19"/>
<connect gate="D" pin="IO_30" pad="E11"/>
<connect gate="D" pin="IO_31" pad="E13"/>
<connect gate="D" pin="IO_32" pad="E14"/>
<connect gate="D" pin="IO_33" pad="E16"/>
<connect gate="D" pin="IO_34" pad="E17"/>
<connect gate="D" pin="IO_35" pad="E25"/>
<connect gate="D" pin="IO_36" pad="E26"/>
<connect gate="D" pin="IO_37" pad="E28"/>
<connect gate="D" pin="IO_38" pad="F11"/>
<connect gate="D" pin="IO_39" pad="F13"/>
<connect gate="D" pin="IO_4" pad="C20"/>
<connect gate="D" pin="IO_40" pad="F14"/>
<connect gate="D" pin="IO_41" pad="F15"/>
<connect gate="D" pin="IO_42" pad="F16"/>
<connect gate="D" pin="IO_43" pad="F17"/>
<connect gate="D" pin="IO_44" pad="F18"/>
<connect gate="D" pin="IO_45" pad="F19"/>
<connect gate="D" pin="IO_46" pad="F20"/>
<connect gate="D" pin="IO_47" pad="F21"/>
<connect gate="D" pin="IO_48" pad="F22"/>
<connect gate="D" pin="IO_49" pad="F23"/>
<connect gate="D" pin="IO_5" pad="C21"/>
<connect gate="D" pin="IO_50" pad="F24"/>
<connect gate="D" pin="IO_51" pad="F26"/>
<connect gate="D" pin="IO_52" pad="F27"/>
<connect gate="D" pin="IO_53" pad="F28"/>
<connect gate="D" pin="IO_54" pad="G10"/>
<connect gate="D" pin="IO_55" pad="G11"/>
<connect gate="D" pin="IO_56" pad="G12"/>
<connect gate="D" pin="IO_57" pad="G13"/>
<connect gate="D" pin="IO_58" pad="G14"/>
<connect gate="D" pin="IO_59" pad="G15"/>
<connect gate="D" pin="IO_6" pad="C22"/>
<connect gate="D" pin="IO_60" pad="G16"/>
<connect gate="D" pin="IO_61" pad="G17"/>
<connect gate="D" pin="IO_62" pad="G18"/>
<connect gate="D" pin="IO_63" pad="G19"/>
<connect gate="D" pin="IO_64" pad="G20"/>
<connect gate="D" pin="IO_65" pad="G21"/>
<connect gate="D" pin="IO_66" pad="G22"/>
<connect gate="D" pin="IO_67" pad="G23"/>
<connect gate="D" pin="IO_68" pad="G24"/>
<connect gate="D" pin="IO_69" pad="G25"/>
<connect gate="D" pin="IO_7" pad="C23"/>
<connect gate="D" pin="IO_70" pad="G26"/>
<connect gate="D" pin="IO_71" pad="G27"/>
<connect gate="D" pin="IO_72" pad="G28"/>
<connect gate="D" pin="IO_73" pad="H10"/>
<connect gate="D" pin="IO_74" pad="H11"/>
<connect gate="D" pin="IO_75" pad="H13"/>
<connect gate="D" pin="IO_8" pad="C24"/>
<connect gate="D" pin="IO_9" pad="C25"/>
<connect gate="D" pin="NC" pad="F25"/>
<connect gate="D" pin="NCE" pad="D24"/>
<connect gate="D" pin="NC_2" pad="C17"/>
<connect gate="D" pin="NC_3" pad="E22"/>
<connect gate="D" pin="NSTATUS" pad="E23"/>
<connect gate="D" pin="VCCIO3" pad="H17"/>
<connect gate="D" pin="VCCIO4" pad="H14"/>
<connect gate="D" pin="VREFB3N0" pad="E19"/>
<connect gate="D" pin="VREFB3N1" pad="E20"/>
<connect gate="D" pin="VREFB4N0" pad="F10"/>
<connect gate="D" pin="VREFB4N1" pad="F12"/>
<connect gate="E" pin="GND" pad="N19"/>
<connect gate="E" pin="GNDA_PLL5" pad="K15"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="J16"/>
<connect gate="E" pin="GND_10" pad="L27"/>
<connect gate="E" pin="GND_11" pad="M12"/>
<connect gate="E" pin="GND_12" pad="M14"/>
<connect gate="E" pin="GND_13" pad="M16"/>
<connect gate="E" pin="GND_14" pad="M18"/>
<connect gate="E" pin="GND_15" pad="M19"/>
<connect gate="E" pin="GND_16" pad="N10"/>
<connect gate="E" pin="GND_17" pad="N11"/>
<connect gate="E" pin="GND_18" pad="N13"/>
<connect gate="E" pin="GND_19" pad="N15"/>
<connect gate="E" pin="GND_2" pad="H21"/>
<connect gate="E" pin="GND_20" pad="N17"/>
<connect gate="E" pin="GND_3" pad="H24"/>
<connect gate="E" pin="GND_4" pad="H27"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="L15"/>
<connect gate="E" pin="GND_7" pad="L18"/>
<connect gate="E" pin="GND_8" pad="L21"/>
<connect gate="E" pin="GND_9" pad="L24"/>
<connect gate="E" pin="IO" pad="N20"/>
<connect gate="E" pin="IO_10" pad="J20"/>
<connect gate="E" pin="IO_11" pad="J21"/>
<connect gate="E" pin="IO_12" pad="J23"/>
<connect gate="E" pin="IO_13" pad="J24"/>
<connect gate="E" pin="IO_14" pad="J25"/>
<connect gate="E" pin="IO_15" pad="J26"/>
<connect gate="E" pin="IO_16" pad="J27"/>
<connect gate="E" pin="IO_17" pad="J28"/>
<connect gate="E" pin="IO_18" pad="K10"/>
<connect gate="E" pin="IO_19" pad="K11"/>
<connect gate="E" pin="IO_2" pad="H22"/>
<connect gate="E" pin="IO_20" pad="K12"/>
<connect gate="E" pin="IO_21" pad="K13"/>
<connect gate="E" pin="IO_22" pad="K14"/>
<connect gate="E" pin="IO_23" pad="K17"/>
<connect gate="E" pin="IO_24" pad="K18"/>
<connect gate="E" pin="IO_25" pad="K19"/>
<connect gate="E" pin="IO_26" pad="K20"/>
<connect gate="E" pin="IO_27" pad="K21"/>
<connect gate="E" pin="IO_28" pad="K22"/>
<connect gate="E" pin="IO_29" pad="K23"/>
<connect gate="E" pin="IO_3" pad="H23"/>
<connect gate="E" pin="IO_30" pad="K24"/>
<connect gate="E" pin="IO_31" pad="K25"/>
<connect gate="E" pin="IO_32" pad="K26"/>
<connect gate="E" pin="IO_33" pad="K27"/>
<connect gate="E" pin="IO_34" pad="K28"/>
<connect gate="E" pin="IO_35" pad="L12"/>
<connect gate="E" pin="IO_36" pad="L13"/>
<connect gate="E" pin="IO_37" pad="L14"/>
<connect gate="E" pin="IO_38" pad="L16"/>
<connect gate="E" pin="IO_39" pad="L17"/>
<connect gate="E" pin="IO_4" pad="H25"/>
<connect gate="E" pin="IO_40" pad="L19"/>
<connect gate="E" pin="IO_41" pad="L20"/>
<connect gate="E" pin="IO_42" pad="L23"/>
<connect gate="E" pin="IO_43" pad="L25"/>
<connect gate="E" pin="IO_44" pad="L26"/>
<connect gate="E" pin="IO_45" pad="L28"/>
<connect gate="E" pin="IO_46" pad="M20"/>
<connect gate="E" pin="IO_47" pad="M21"/>
<connect gate="E" pin="IO_48" pad="M22"/>
<connect gate="E" pin="IO_49" pad="M24"/>
<connect gate="E" pin="IO_5" pad="H26"/>
<connect gate="E" pin="IO_50" pad="M25"/>
<connect gate="E" pin="IO_51" pad="M26"/>
<connect gate="E" pin="IO_52" pad="M27"/>
<connect gate="E" pin="IO_53" pad="M28"/>
<connect gate="E" pin="IO_6" pad="H28"/>
<connect gate="E" pin="IO_7" pad="J10"/>
<connect gate="E" pin="IO_8" pad="J11"/>
<connect gate="E" pin="IO_9" pad="J18"/>
<connect gate="E" pin="VCCA_PLL5" pad="J15"/>
<connect gate="E" pin="VCCD_PLL1" pad="N22"/>
<connect gate="E" pin="VCCD_PLL5" pad="K16"/>
<connect gate="E" pin="VCCINT" pad="N18"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="M13"/>
<connect gate="E" pin="VCCINT_4" pad="M15"/>
<connect gate="E" pin="VCCINT_5" pad="M17"/>
<connect gate="E" pin="VCCINT_6" pad="N12"/>
<connect gate="E" pin="VCCINT_7" pad="N14"/>
<connect gate="E" pin="VCCINT_8" pad="N16"/>
<connect gate="E" pin="VCCIO2" pad="N21"/>
<connect gate="E" pin="VCCIO2_2" pad="J22"/>
<connect gate="E" pin="VCCIO2_3" pad="L22"/>
<connect gate="E" pin="VCCIO3" pad="J19"/>
<connect gate="E" pin="VCCIO3_2" pad="H20"/>
<connect gate="E" pin="VCCIO4" pad="J12"/>
<connect gate="E" pin="VCCP" pad="M10"/>
<connect gate="E" pin="VCCPD3" pad="J17"/>
<connect gate="E" pin="VCCPD4" pad="J13"/>
<connect gate="E" pin="VCCP_2" pad="L10"/>
<connect gate="E" pin="VCC_PLL5_OUT" pad="J14"/>
<connect gate="E" pin="VREFB2N1" pad="M23"/>
<connect gate="F" pin="CLK1N" pad="T24"/>
<connect gate="F" pin="CLK1P" pad="T25"/>
<connect gate="F" pin="CLK3N" pad="U25"/>
<connect gate="F" pin="CLK3P" pad="U26"/>
<connect gate="F" pin="GND" pad="V24"/>
<connect gate="F" pin="GNDA_PLL1" pad="P23"/>
<connect gate="F" pin="GNDA_PLL1_2" pad="P22"/>
<connect gate="F" pin="GNDA_PLL2" pad="R23"/>
<connect gate="F" pin="GNDA_PLL2_2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="P21"/>
<connect gate="F" pin="GND_11" pad="R11"/>
<connect gate="F" pin="GND_12" pad="R13"/>
<connect gate="F" pin="GND_13" pad="R15"/>
<connect gate="F" pin="GND_14" pad="R17"/>
<connect gate="F" pin="GND_15" pad="R19"/>
<connect gate="F" pin="GND_16" pad="R24"/>
<connect gate="F" pin="GND_17" pad="R27"/>
<connect gate="F" pin="GND_18" pad="T12"/>
<connect gate="F" pin="GND_19" pad="T14"/>
<connect gate="F" pin="GND_2" pad="N24"/>
<connect gate="F" pin="GND_20" pad="T16"/>
<connect gate="F" pin="GND_21" pad="T18"/>
<connect gate="F" pin="GND_22" pad="U10"/>
<connect gate="F" pin="GND_23" pad="U11"/>
<connect gate="F" pin="GND_24" pad="U13"/>
<connect gate="F" pin="GND_25" pad="U15"/>
<connect gate="F" pin="GND_26" pad="U17"/>
<connect gate="F" pin="GND_27" pad="U21"/>
<connect gate="F" pin="GND_28" pad="V10"/>
<connect gate="F" pin="GND_29" pad="V12"/>
<connect gate="F" pin="GND_3" pad="N27"/>
<connect gate="F" pin="GND_30" pad="V15"/>
<connect gate="F" pin="GND_31" pad="V18"/>
<connect gate="F" pin="GND_4" pad="P10"/>
<connect gate="F" pin="GND_5" pad="P12"/>
<connect gate="F" pin="GND_6" pad="P14"/>
<connect gate="F" pin="GND_7" pad="P16"/>
<connect gate="F" pin="GND_8" pad="P18"/>
<connect gate="F" pin="GND_9" pad="P19"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="R20"/>
<connect gate="F" pin="IO_11" pad="R21"/>
<connect gate="F" pin="IO_12" pad="R25"/>
<connect gate="F" pin="IO_13" pad="R26"/>
<connect gate="F" pin="IO_14" pad="R28"/>
<connect gate="F" pin="IO_15" pad="T19"/>
<connect gate="F" pin="IO_16" pad="T26"/>
<connect gate="F" pin="IO_17" pad="T27"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U19"/>
<connect gate="F" pin="IO_2" pad="N25"/>
<connect gate="F" pin="IO_20" pad="U20"/>
<connect gate="F" pin="IO_21" pad="U23"/>
<connect gate="F" pin="IO_22" pad="U24"/>
<connect gate="F" pin="IO_23" pad="U27"/>
<connect gate="F" pin="IO_24" pad="U28"/>
<connect gate="F" pin="IO_25" pad="V11"/>
<connect gate="F" pin="IO_26" pad="V13"/>
<connect gate="F" pin="IO_27" pad="V20"/>
<connect gate="F" pin="IO_28" pad="V22"/>
<connect gate="F" pin="IO_29" pad="V23"/>
<connect gate="F" pin="IO_3" pad="N26"/>
<connect gate="F" pin="IO_4" pad="N28"/>
<connect gate="F" pin="IO_5" pad="P24"/>
<connect gate="F" pin="IO_6" pad="P25"/>
<connect gate="F" pin="IO_7" pad="P26"/>
<connect gate="F" pin="IO_8" pad="P27"/>
<connect gate="F" pin="IO_9" pad="P28"/>
<connect gate="F" pin="NCONFIG" pad="V17"/>
<connect gate="F" pin="TCK" pad="V16"/>
<connect gate="F" pin="TDI" pad="V19"/>
<connect gate="F" pin="VCCA_PLL1" pad="N23"/>
<connect gate="F" pin="VCCA_PLL2" pad="T23"/>
<connect gate="F" pin="VCCD_PLL2" pad="T22"/>
<connect gate="F" pin="VCCD_PLL6" pad="V14"/>
<connect gate="F" pin="VCCINT" pad="U18"/>
<connect gate="F" pin="VCCINT_10" pad="T11"/>
<connect gate="F" pin="VCCINT_11" pad="T13"/>
<connect gate="F" pin="VCCINT_12" pad="T15"/>
<connect gate="F" pin="VCCINT_13" pad="T17"/>
<connect gate="F" pin="VCCINT_14" pad="U12"/>
<connect gate="F" pin="VCCINT_15" pad="U14"/>
<connect gate="F" pin="VCCINT_16" pad="U16"/>
<connect gate="F" pin="VCCINT_2" pad="P11"/>
<connect gate="F" pin="VCCINT_3" pad="P13"/>
<connect gate="F" pin="VCCINT_4" pad="P15"/>
<connect gate="F" pin="VCCINT_5" pad="P17"/>
<connect gate="F" pin="VCCINT_6" pad="R12"/>
<connect gate="F" pin="VCCINT_7" pad="R14"/>
<connect gate="F" pin="VCCINT_8" pad="R16"/>
<connect gate="F" pin="VCCINT_9" pad="R18"/>
<connect gate="F" pin="VCCIO1" pad="V21"/>
<connect gate="F" pin="VCCIO1_2" pad="U22"/>
<connect gate="F" pin="VCCP" pad="T10"/>
<connect gate="F" pin="VCCPD1" pad="T20"/>
<connect gate="F" pin="VCCPD2" pad="P20"/>
<connect gate="F" pin="VCCP_2" pad="R10"/>
<connect gate="F" pin="VREFB2N0" pad="T21"/>
<connect gate="G" pin="GND" pad="AA27"/>
<connect gate="G" pin="GNDA_PLL6" pad="W14"/>
<connect gate="G" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="G" pin="GND_10" pad="AA21"/>
<connect gate="G" pin="GND_11" pad="AA24"/>
<connect gate="G" pin="GND_2" pad="V27"/>
<connect gate="G" pin="GND_3" pad="W20"/>
<connect gate="G" pin="GND_4" pad="W22"/>
<connect gate="G" pin="GND_5" pad="Y20"/>
<connect gate="G" pin="GND_6" pad="AA12"/>
<connect gate="G" pin="GND_7" pad="AA15"/>
<connect gate="G" pin="GND_8" pad="AA18"/>
<connect gate="G" pin="GND_9" pad="AA20"/>
<connect gate="G" pin="IO" pad="AB20"/>
<connect gate="G" pin="IO_10" pad="AC11"/>
<connect gate="G" pin="IO_11" pad="AC12"/>
<connect gate="G" pin="IO_12" pad="AC13"/>
<connect gate="G" pin="IO_13" pad="AC14"/>
<connect gate="G" pin="IO_14" pad="AC15"/>
<connect gate="G" pin="IO_15" pad="AC16"/>
<connect gate="G" pin="IO_16" pad="AC17"/>
<connect gate="G" pin="IO_17" pad="AC18"/>
<connect gate="G" pin="IO_18" pad="AC19"/>
<connect gate="G" pin="IO_19" pad="AC20"/>
<connect gate="G" pin="IO_2" pad="AB21"/>
<connect gate="G" pin="IO_20" pad="AC21"/>
<connect gate="G" pin="IO_21" pad="AC22"/>
<connect gate="G" pin="IO_22" pad="AC23"/>
<connect gate="G" pin="IO_23" pad="AC24"/>
<connect gate="G" pin="IO_24" pad="AC25"/>
<connect gate="G" pin="IO_25" pad="AC26"/>
<connect gate="G" pin="IO_26" pad="AC27"/>
<connect gate="G" pin="IO_27" pad="AC28"/>
<connect gate="G" pin="IO_28" pad="V26"/>
<connect gate="G" pin="IO_29" pad="V28"/>
<connect gate="G" pin="IO_3" pad="AB22"/>
<connect gate="G" pin="IO_30" pad="W10"/>
<connect gate="G" pin="IO_31" pad="W11"/>
<connect gate="G" pin="IO_32" pad="W12"/>
<connect gate="G" pin="IO_33" pad="W15"/>
<connect gate="G" pin="IO_34" pad="W16"/>
<connect gate="G" pin="IO_35" pad="W21"/>
<connect gate="G" pin="IO_36" pad="W24"/>
<connect gate="G" pin="IO_37" pad="W25"/>
<connect gate="G" pin="IO_38" pad="W26"/>
<connect gate="G" pin="IO_39" pad="W27"/>
<connect gate="G" pin="IO_4" pad="AB23"/>
<connect gate="G" pin="IO_40" pad="W28"/>
<connect gate="G" pin="IO_41" pad="Y10"/>
<connect gate="G" pin="IO_42" pad="Y11"/>
<connect gate="G" pin="IO_43" pad="Y13"/>
<connect gate="G" pin="IO_44" pad="Y15"/>
<connect gate="G" pin="IO_45" pad="Y17"/>
<connect gate="G" pin="IO_46" pad="Y21"/>
<connect gate="G" pin="IO_47" pad="Y24"/>
<connect gate="G" pin="IO_48" pad="Y25"/>
<connect gate="G" pin="IO_49" pad="Y26"/>
<connect gate="G" pin="IO_5" pad="AB24"/>
<connect gate="G" pin="IO_50" pad="Y27"/>
<connect gate="G" pin="IO_51" pad="Y28"/>
<connect gate="G" pin="IO_52" pad="AA11"/>
<connect gate="G" pin="IO_53" pad="AA17"/>
<connect gate="G" pin="IO_54" pad="AA19"/>
<connect gate="G" pin="IO_55" pad="AA22"/>
<connect gate="G" pin="IO_56" pad="AA23"/>
<connect gate="G" pin="IO_57" pad="AA25"/>
<connect gate="G" pin="IO_58" pad="AA26"/>
<connect gate="G" pin="IO_59" pad="AA28"/>
<connect gate="G" pin="IO_6" pad="AB25"/>
<connect gate="G" pin="IO_60" pad="AB10"/>
<connect gate="G" pin="IO_61" pad="AB11"/>
<connect gate="G" pin="IO_62" pad="AB12"/>
<connect gate="G" pin="IO_63" pad="AB13"/>
<connect gate="G" pin="IO_64" pad="AB15"/>
<connect gate="G" pin="IO_65" pad="AB16"/>
<connect gate="G" pin="IO_66" pad="AB17"/>
<connect gate="G" pin="IO_67" pad="AB18"/>
<connect gate="G" pin="IO_68" pad="AB19"/>
<connect gate="G" pin="IO_7" pad="AB26"/>
<connect gate="G" pin="IO_8" pad="AB27"/>
<connect gate="G" pin="IO_9" pad="AB28"/>
<connect gate="G" pin="TMS" pad="W19"/>
<connect gate="G" pin="TRST" pad="W17"/>
<connect gate="G" pin="VCCA_PLL6" pad="Y14"/>
<connect gate="G" pin="VCCIO1" pad="Y22"/>
<connect gate="G" pin="VCCIO7" pad="AA13"/>
<connect gate="G" pin="VCCIO7_2" pad="AA10"/>
<connect gate="G" pin="VCCIO8" pad="AA16"/>
<connect gate="G" pin="VCCIO8_2" pad="Y18"/>
<connect gate="G" pin="VCCIO8_3" pad="Y19"/>
<connect gate="G" pin="VCCPD7" pad="Y12"/>
<connect gate="G" pin="VCCPD8" pad="Y16"/>
<connect gate="G" pin="VCCSEL" pad="W18"/>
<connect gate="G" pin="VCC_PLL6_OUT" pad="AA14"/>
<connect gate="G" pin="VREFB1N0" pad="Y23"/>
<connect gate="G" pin="VREFB1N1" pad="W23"/>
<connect gate="G" pin="VREFB7N0" pad="AB14"/>
<connect gate="G" pin="VREFB7N1" pad="AC10"/>
<connect gate="H" pin="GND" pad="AH27"/>
<connect gate="H" pin="GND_10" pad="AG18"/>
<connect gate="H" pin="GND_11" pad="AG21"/>
<connect gate="H" pin="GND_12" pad="AG24"/>
<connect gate="H" pin="GND_13" pad="AG27"/>
<connect gate="H" pin="GND_14" pad="AG28"/>
<connect gate="H" pin="GND_2" pad="AD12"/>
<connect gate="H" pin="GND_3" pad="AD15"/>
<connect gate="H" pin="GND_4" pad="AD18"/>
<connect gate="H" pin="GND_5" pad="AD21"/>
<connect gate="H" pin="GND_6" pad="AD24"/>
<connect gate="H" pin="GND_7" pad="AD27"/>
<connect gate="H" pin="GND_8" pad="AG12"/>
<connect gate="H" pin="GND_9" pad="AG15"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD28"/>
<connect gate="H" pin="IO_11" pad="AE10"/>
<connect gate="H" pin="IO_12" pad="AE11"/>
<connect gate="H" pin="IO_13" pad="AE12"/>
<connect gate="H" pin="IO_14" pad="AE13"/>
<connect gate="H" pin="IO_15" pad="AE14"/>
<connect gate="H" pin="IO_16" pad="AE15"/>
<connect gate="H" pin="IO_17" pad="AE17"/>
<connect gate="H" pin="IO_18" pad="AE18"/>
<connect gate="H" pin="IO_19" pad="AE19"/>
<connect gate="H" pin="IO_2" pad="AD10"/>
<connect gate="H" pin="IO_20" pad="AE20"/>
<connect gate="H" pin="IO_21" pad="AE21"/>
<connect gate="H" pin="IO_22" pad="AE22"/>
<connect gate="H" pin="IO_23" pad="AE23"/>
<connect gate="H" pin="IO_24" pad="AE24"/>
<connect gate="H" pin="IO_25" pad="AE25"/>
<connect gate="H" pin="IO_26" pad="AE26"/>
<connect gate="H" pin="IO_27" pad="AE27"/>
<connect gate="H" pin="IO_28" pad="AE28"/>
<connect gate="H" pin="IO_29" pad="AF10"/>
<connect gate="H" pin="IO_3" pad="AD11"/>
<connect gate="H" pin="IO_30" pad="AF11"/>
<connect gate="H" pin="IO_31" pad="AF12"/>
<connect gate="H" pin="IO_32" pad="AF21"/>
<connect gate="H" pin="IO_33" pad="AF22"/>
<connect gate="H" pin="IO_34" pad="AF23"/>
<connect gate="H" pin="IO_35" pad="AF24"/>
<connect gate="H" pin="IO_36" pad="AF25"/>
<connect gate="H" pin="IO_37" pad="AF26"/>
<connect gate="H" pin="IO_38" pad="AF27"/>
<connect gate="H" pin="IO_39" pad="AF28"/>
<connect gate="H" pin="IO_4" pad="AD13"/>
<connect gate="H" pin="IO_40" pad="AG10"/>
<connect gate="H" pin="IO_41" pad="AG11"/>
<connect gate="H" pin="IO_42" pad="AG13"/>
<connect gate="H" pin="IO_43" pad="AG14"/>
<connect gate="H" pin="IO_44" pad="AG16"/>
<connect gate="H" pin="IO_45" pad="AG17"/>
<connect gate="H" pin="IO_46" pad="AG19"/>
<connect gate="H" pin="IO_47" pad="AG20"/>
<connect gate="H" pin="IO_48" pad="AG22"/>
<connect gate="H" pin="IO_49" pad="AG23"/>
<connect gate="H" pin="IO_5" pad="AD14"/>
<connect gate="H" pin="IO_50" pad="AG25"/>
<connect gate="H" pin="IO_51" pad="AG26"/>
<connect gate="H" pin="IO_52" pad="AH10"/>
<connect gate="H" pin="IO_53" pad="AH11"/>
<connect gate="H" pin="IO_54" pad="AH12"/>
<connect gate="H" pin="IO_55" pad="AH13"/>
<connect gate="H" pin="IO_56" pad="AH14"/>
<connect gate="H" pin="IO_57" pad="AH15"/>
<connect gate="H" pin="IO_58" pad="AH16"/>
<connect gate="H" pin="IO_59" pad="AF13"/>
<connect gate="H" pin="IO_6" pad="AD16"/>
<connect gate="H" pin="IO_60" pad="AH17"/>
<connect gate="H" pin="IO_61" pad="AF14"/>
<connect gate="H" pin="IO_62" pad="AH18"/>
<connect gate="H" pin="IO_63" pad="AF15"/>
<connect gate="H" pin="IO_64" pad="AH19"/>
<connect gate="H" pin="IO_65" pad="AF17"/>
<connect gate="H" pin="IO_66" pad="AH20"/>
<connect gate="H" pin="IO_67" pad="AF18"/>
<connect gate="H" pin="IO_68" pad="AH21"/>
<connect gate="H" pin="IO_69" pad="AF19"/>
<connect gate="H" pin="IO_7" pad="AD20"/>
<connect gate="H" pin="IO_70" pad="AH22"/>
<connect gate="H" pin="IO_71" pad="AF20"/>
<connect gate="H" pin="IO_72" pad="AH23"/>
<connect gate="H" pin="IO_73" pad="AH24"/>
<connect gate="H" pin="IO_74" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD25"/>
<connect gate="H" pin="IO_9" pad="AD26"/>
<connect gate="H" pin="NC" pad="AF16"/>
<connect gate="H" pin="NC_2" pad="AD22"/>
<connect gate="H" pin="NC_3" pad="AD23"/>
<connect gate="H" pin="NC_4" pad="AE16"/>
<connect gate="H" pin="VREFB8N0" pad="AD19"/>
<connect gate="H" pin="VREFB8N1" pad="AD17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2SGX30DF780C3N"/>
<attribute name="OC_FARNELL" value="1549490"/>
<attribute name="OC_NEWARK" value="52R0628"/>
<attribute name="PACKAGE" value="BGA-780"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2SGX60CF780C5N">
<description>FPGA, STRATIX II GX</description>
<gates>
<gate name="A" symbol="EP2SGX60CF780C5N_A"/>
<gate name="B" symbol="EP2SGX60CF780C5N_B"/>
<gate name="C" symbol="EP2SGX60CF780C5N_C"/>
<gate name="D" symbol="EP2SGX60CF780C5N_D"/>
<gate name="E" symbol="EP2SGX60CF780C5N_E"/>
<gate name="F" symbol="EP2SGX60CF780C5N_F"/>
<gate name="G" symbol="EP2SGX60CF780C5N_G"/>
<gate name="H" symbol="EP2SGX60CF780C5N_H"/>
</gates>
<devices>
<device name="" package="BGA780C100P28X28_2900X2900X350">
<connects>
<connect gate="A" pin="GND" pad="L3"/>
<connect gate="A" pin="GND_10" pad="B4"/>
<connect gate="A" pin="GND_11" pad="B5"/>
<connect gate="A" pin="GND_12" pad="B6"/>
<connect gate="A" pin="GND_13" pad="B7"/>
<connect gate="A" pin="GND_14" pad="B9"/>
<connect gate="A" pin="GND_15" pad="C1"/>
<connect gate="A" pin="GND_16" pad="C2"/>
<connect gate="A" pin="GND_17" pad="C3"/>
<connect gate="A" pin="GND_18" pad="C6"/>
<connect gate="A" pin="GND_19" pad="D1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_20" pad="D2"/>
<connect gate="A" pin="GND_21" pad="D3"/>
<connect gate="A" pin="GND_22" pad="D4"/>
<connect gate="A" pin="GND_23" pad="D5"/>
<connect gate="A" pin="GND_24" pad="D6"/>
<connect gate="A" pin="GND_25" pad="E3"/>
<connect gate="A" pin="GND_26" pad="E6"/>
<connect gate="A" pin="GND_27" pad="E7"/>
<connect gate="A" pin="GND_28" pad="E9"/>
<connect gate="A" pin="GND_29" pad="F1"/>
<connect gate="A" pin="GND_3" pad="A3"/>
<connect gate="A" pin="GND_30" pad="F2"/>
<connect gate="A" pin="GND_31" pad="F3"/>
<connect gate="A" pin="GND_32" pad="F4"/>
<connect gate="A" pin="GND_33" pad="F5"/>
<connect gate="A" pin="GND_34" pad="F6"/>
<connect gate="A" pin="GND_35" pad="G3"/>
<connect gate="A" pin="GND_36" pad="G6"/>
<connect gate="A" pin="GND_37" pad="H1"/>
<connect gate="A" pin="GND_38" pad="H2"/>
<connect gate="A" pin="GND_39" pad="H3"/>
<connect gate="A" pin="GND_4" pad="A4"/>
<connect gate="A" pin="GND_40" pad="H4"/>
<connect gate="A" pin="GND_41" pad="H5"/>
<connect gate="A" pin="GND_42" pad="H6"/>
<connect gate="A" pin="GND_43" pad="H7"/>
<connect gate="A" pin="GND_44" pad="H9"/>
<connect gate="A" pin="GND_45" pad="J3"/>
<connect gate="A" pin="GND_46" pad="J5"/>
<connect gate="A" pin="GND_47" pad="J6"/>
<connect gate="A" pin="GND_48" pad="J7"/>
<connect gate="A" pin="GND_49" pad="K1"/>
<connect gate="A" pin="GND_5" pad="A5"/>
<connect gate="A" pin="GND_50" pad="K2"/>
<connect gate="A" pin="GND_51" pad="K3"/>
<connect gate="A" pin="GND_52" pad="K4"/>
<connect gate="A" pin="GND_53" pad="K5"/>
<connect gate="A" pin="GND_54" pad="K6"/>
<connect gate="A" pin="GND_6" pad="A6"/>
<connect gate="A" pin="GND_7" pad="B1"/>
<connect gate="A" pin="GND_8" pad="B2"/>
<connect gate="A" pin="GND_9" pad="B3"/>
<connect gate="A" pin="GXB_RX0N" pad="G2"/>
<connect gate="A" pin="GXB_RX0P" pad="G1"/>
<connect gate="A" pin="GXB_RX1N" pad="E2"/>
<connect gate="A" pin="GXB_RX1P" pad="E1"/>
<connect gate="A" pin="GXB_RX2N" pad="L2"/>
<connect gate="A" pin="GXB_RX2P" pad="L1"/>
<connect gate="A" pin="GXB_TX0N" pad="E5"/>
<connect gate="A" pin="GXB_TX0P" pad="E4"/>
<connect gate="A" pin="GXB_TX1N" pad="C5"/>
<connect gate="A" pin="GXB_TX1P" pad="C4"/>
<connect gate="A" pin="GXB_TX2N" pad="L5"/>
<connect gate="A" pin="GXB_TX2P" pad="L4"/>
<connect gate="A" pin="IO" pad="G9"/>
<connect gate="A" pin="IO_10" pad="D8"/>
<connect gate="A" pin="IO_11" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A8"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_5" pad="B8"/>
<connect gate="A" pin="IO_6" pad="C7"/>
<connect gate="A" pin="IO_7" pad="C8"/>
<connect gate="A" pin="IO_8" pad="C9"/>
<connect gate="A" pin="IO_9" pad="D7"/>
<connect gate="A" pin="MSEL0" pad="J8"/>
<connect gate="A" pin="MSEL1" pad="E8"/>
<connect gate="A" pin="MSEL2" pad="H8"/>
<connect gate="A" pin="MSEL3" pad="G8"/>
<connect gate="A" pin="NC" pad="K8"/>
<connect gate="A" pin="NC_2" pad="K7"/>
<connect gate="A" pin="REFCLK0_B13N" pad="J2"/>
<connect gate="A" pin="REFCLK0_B13P" pad="J1"/>
<connect gate="A" pin="REFCLK1_B13N" pad="G5"/>
<connect gate="A" pin="REFCLK1_B13P" pad="G4"/>
<connect gate="A" pin="RREFB13" pad="J4"/>
<connect gate="A" pin="TDO" pad="F8"/>
<connect gate="A" pin="TEMPDIODEN" pad="G7"/>
<connect gate="A" pin="TEMPDIODEP" pad="F7"/>
<connect gate="A" pin="VCCA" pad="L6"/>
<connect gate="A" pin="VCCA_2" pad="K9"/>
<connect gate="A" pin="VCCH_B13" pad="L9"/>
<connect gate="A" pin="VCCIO4" pad="J9"/>
<connect gate="A" pin="VCCR" pad="L7"/>
<connect gate="A" pin="VCCT_B13" pad="L8"/>
<connect gate="A" pin="VREFB4N0" pad="F9"/>
<connect gate="B" pin="GND" pad="Y6"/>
<connect gate="B" pin="GND_10" pad="N9"/>
<connect gate="B" pin="GND_11" pad="P1"/>
<connect gate="B" pin="GND_12" pad="P2"/>
<connect gate="B" pin="GND_13" pad="P3"/>
<connect gate="B" pin="GND_14" pad="P4"/>
<connect gate="B" pin="GND_15" pad="P5"/>
<connect gate="B" pin="GND_16" pad="P6"/>
<connect gate="B" pin="GND_17" pad="P8"/>
<connect gate="B" pin="GND_18" pad="R1"/>
<connect gate="B" pin="GND_19" pad="R2"/>
<connect gate="B" pin="GND_2" pad="M1"/>
<connect gate="B" pin="GND_20" pad="R3"/>
<connect gate="B" pin="GND_21" pad="R4"/>
<connect gate="B" pin="GND_22" pad="R5"/>
<connect gate="B" pin="GND_23" pad="T3"/>
<connect gate="B" pin="GND_24" pad="U1"/>
<connect gate="B" pin="GND_25" pad="U2"/>
<connect gate="B" pin="GND_26" pad="U3"/>
<connect gate="B" pin="GND_27" pad="U4"/>
<connect gate="B" pin="GND_28" pad="U5"/>
<connect gate="B" pin="GND_29" pad="U7"/>
<connect gate="B" pin="GND_3" pad="M2"/>
<connect gate="B" pin="GND_30" pad="U8"/>
<connect gate="B" pin="GND_31" pad="U9"/>
<connect gate="B" pin="GND_32" pad="V3"/>
<connect gate="B" pin="GND_33" pad="V6"/>
<connect gate="B" pin="GND_34" pad="V8"/>
<connect gate="B" pin="GND_35" pad="W1"/>
<connect gate="B" pin="GND_36" pad="W2"/>
<connect gate="B" pin="GND_37" pad="W3"/>
<connect gate="B" pin="GND_38" pad="W4"/>
<connect gate="B" pin="GND_39" pad="W5"/>
<connect gate="B" pin="GND_4" pad="M3"/>
<connect gate="B" pin="GND_40" pad="W6"/>
<connect gate="B" pin="GND_41" pad="W7"/>
<connect gate="B" pin="GND_42" pad="W8"/>
<connect gate="B" pin="GND_43" pad="Y3"/>
<connect gate="B" pin="GND_44" pad="Y5"/>
<connect gate="B" pin="GND_5" pad="M4"/>
<connect gate="B" pin="GND_6" pad="M5"/>
<connect gate="B" pin="GND_7" pad="N3"/>
<connect gate="B" pin="GND_8" pad="N7"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GXB_RX3N" pad="N2"/>
<connect gate="B" pin="GXB_RX3P" pad="N1"/>
<connect gate="B" pin="GXB_TX3N" pad="N5"/>
<connect gate="B" pin="GXB_TX3P" pad="N4"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="A17"/>
<connect gate="B" pin="IO_11" pad="A18"/>
<connect gate="B" pin="IO_12" pad="A19"/>
<connect gate="B" pin="IO_13" pad="A20"/>
<connect gate="B" pin="IO_14" pad="A21"/>
<connect gate="B" pin="IO_15" pad="A22"/>
<connect gate="B" pin="IO_16" pad="A23"/>
<connect gate="B" pin="IO_17" pad="A24"/>
<connect gate="B" pin="IO_18" pad="A25"/>
<connect gate="B" pin="IO_2" pad="W9"/>
<connect gate="B" pin="IO_3" pad="A10"/>
<connect gate="B" pin="IO_4" pad="A11"/>
<connect gate="B" pin="IO_5" pad="A12"/>
<connect gate="B" pin="IO_6" pad="A13"/>
<connect gate="B" pin="IO_7" pad="A14"/>
<connect gate="B" pin="IO_8" pad="A15"/>
<connect gate="B" pin="IO_9" pad="A16"/>
<connect gate="B" pin="NC" pad="Y4"/>
<connect gate="B" pin="NC_10" pad="Y1"/>
<connect gate="B" pin="NC_11" pad="Y2"/>
<connect gate="B" pin="NC_2" pad="T1"/>
<connect gate="B" pin="NC_3" pad="T2"/>
<connect gate="B" pin="NC_4" pad="T4"/>
<connect gate="B" pin="NC_5" pad="T5"/>
<connect gate="B" pin="NC_6" pad="V1"/>
<connect gate="B" pin="NC_7" pad="V2"/>
<connect gate="B" pin="NC_8" pad="V4"/>
<connect gate="B" pin="NC_9" pad="V5"/>
<connect gate="B" pin="NIO_PULLUP" pad="Y7"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA" pad="V9"/>
<connect gate="B" pin="VCCA_2" pad="M6"/>
<connect gate="B" pin="VCCA_3" pad="P7"/>
<connect gate="B" pin="VCCA_4" pad="P9"/>
<connect gate="B" pin="VCCA_5" pad="R6"/>
<connect gate="B" pin="VCCA_6" pad="T6"/>
<connect gate="B" pin="VCCA_7" pad="V7"/>
<connect gate="B" pin="VCCH_B13" pad="M9"/>
<connect gate="B" pin="VCCH_B14" pad="T9"/>
<connect gate="B" pin="VCCH_B14_2" pad="R9"/>
<connect gate="B" pin="VCCIO7" pad="Y9"/>
<connect gate="B" pin="VCCL_B13" pad="N6"/>
<connect gate="B" pin="VCCL_B14" pad="U6"/>
<connect gate="B" pin="VCCR" pad="T7"/>
<connect gate="B" pin="VCCR_2" pad="M7"/>
<connect gate="B" pin="VCCR_3" pad="R7"/>
<connect gate="B" pin="VCCT_B13" pad="M8"/>
<connect gate="B" pin="VCCT_B14" pad="T8"/>
<connect gate="B" pin="VCCT_B14_2" pad="R8"/>
<connect gate="C" pin="GND" pad="B28"/>
<connect gate="C" pin="GND_10" pad="AA9"/>
<connect gate="C" pin="GND_11" pad="AB3"/>
<connect gate="C" pin="GND_12" pad="AB6"/>
<connect gate="C" pin="GND_13" pad="AC1"/>
<connect gate="C" pin="GND_14" pad="AC2"/>
<connect gate="C" pin="GND_15" pad="AC3"/>
<connect gate="C" pin="GND_16" pad="AC4"/>
<connect gate="C" pin="GND_17" pad="AC5"/>
<connect gate="C" pin="GND_18" pad="AC6"/>
<connect gate="C" pin="GND_19" pad="AC7"/>
<connect gate="C" pin="GND_2" pad="A27"/>
<connect gate="C" pin="GND_20" pad="AD3"/>
<connect gate="C" pin="GND_21" pad="AD6"/>
<connect gate="C" pin="GND_22" pad="AD7"/>
<connect gate="C" pin="GND_23" pad="AD9"/>
<connect gate="C" pin="GND_24" pad="AE1"/>
<connect gate="C" pin="GND_25" pad="AE2"/>
<connect gate="C" pin="GND_26" pad="AE3"/>
<connect gate="C" pin="GND_27" pad="AE4"/>
<connect gate="C" pin="GND_28" pad="AE5"/>
<connect gate="C" pin="GND_29" pad="AE6"/>
<connect gate="C" pin="GND_3" pad="AA1"/>
<connect gate="C" pin="GND_30" pad="AF1"/>
<connect gate="C" pin="GND_31" pad="AF2"/>
<connect gate="C" pin="GND_32" pad="AF3"/>
<connect gate="C" pin="GND_33" pad="AF6"/>
<connect gate="C" pin="GND_34" pad="AG1"/>
<connect gate="C" pin="GND_35" pad="AG2"/>
<connect gate="C" pin="GND_36" pad="AG3"/>
<connect gate="C" pin="GND_37" pad="AG4"/>
<connect gate="C" pin="GND_38" pad="AG5"/>
<connect gate="C" pin="GND_39" pad="AG6"/>
<connect gate="C" pin="GND_4" pad="AA2"/>
<connect gate="C" pin="GND_40" pad="AG7"/>
<connect gate="C" pin="GND_41" pad="AG9"/>
<connect gate="C" pin="GND_42" pad="AH2"/>
<connect gate="C" pin="GND_43" pad="AH3"/>
<connect gate="C" pin="GND_44" pad="AH4"/>
<connect gate="C" pin="GND_45" pad="AH5"/>
<connect gate="C" pin="GND_46" pad="AH6"/>
<connect gate="C" pin="GND_47" pad="B12"/>
<connect gate="C" pin="GND_48" pad="B15"/>
<connect gate="C" pin="GND_49" pad="B18"/>
<connect gate="C" pin="GND_5" pad="AA3"/>
<connect gate="C" pin="GND_50" pad="B21"/>
<connect gate="C" pin="GND_51" pad="B24"/>
<connect gate="C" pin="GND_52" pad="B27"/>
<connect gate="C" pin="GND_6" pad="AA4"/>
<connect gate="C" pin="GND_7" pad="AA5"/>
<connect gate="C" pin="GND_8" pad="AA6"/>
<connect gate="C" pin="GND_9" pad="AA7"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AF8"/>
<connect gate="C" pin="IO_11" pad="AF9"/>
<connect gate="C" pin="IO_12" pad="AG8"/>
<connect gate="C" pin="IO_13" pad="AH7"/>
<connect gate="C" pin="IO_14" pad="AH8"/>
<connect gate="C" pin="IO_15" pad="AH9"/>
<connect gate="C" pin="IO_16" pad="B10"/>
<connect gate="C" pin="IO_17" pad="B11"/>
<connect gate="C" pin="IO_18" pad="B13"/>
<connect gate="C" pin="IO_19" pad="B14"/>
<connect gate="C" pin="IO_2" pad="AB8"/>
<connect gate="C" pin="IO_20" pad="B16"/>
<connect gate="C" pin="IO_21" pad="B17"/>
<connect gate="C" pin="IO_22" pad="B19"/>
<connect gate="C" pin="IO_23" pad="B20"/>
<connect gate="C" pin="IO_24" pad="B22"/>
<connect gate="C" pin="IO_25" pad="B23"/>
<connect gate="C" pin="IO_26" pad="B25"/>
<connect gate="C" pin="IO_27" pad="B26"/>
<connect gate="C" pin="IO_28" pad="C10"/>
<connect gate="C" pin="IO_29" pad="C11"/>
<connect gate="C" pin="IO_3" pad="AB9"/>
<connect gate="C" pin="IO_30" pad="C12"/>
<connect gate="C" pin="IO_31" pad="C13"/>
<connect gate="C" pin="IO_32" pad="C14"/>
<connect gate="C" pin="IO_33" pad="C15"/>
<connect gate="C" pin="IO_4" pad="AC8"/>
<connect gate="C" pin="IO_5" pad="AC9"/>
<connect gate="C" pin="IO_6" pad="AE7"/>
<connect gate="C" pin="IO_7" pad="AE8"/>
<connect gate="C" pin="IO_8" pad="AE9"/>
<connect gate="C" pin="IO_9" pad="AF7"/>
<connect gate="C" pin="NC" pad="AF5"/>
<connect gate="C" pin="NCEO" pad="AB7"/>
<connect gate="C" pin="NC_10" pad="AF4"/>
<connect gate="C" pin="NC_2" pad="AB2"/>
<connect gate="C" pin="NC_3" pad="AB4"/>
<connect gate="C" pin="NC_4" pad="AB5"/>
<connect gate="C" pin="NC_5" pad="AD1"/>
<connect gate="C" pin="NC_6" pad="AD2"/>
<connect gate="C" pin="NC_7" pad="AD4"/>
<connect gate="C" pin="NC_8" pad="AD5"/>
<connect gate="C" pin="NC_9" pad="AB1"/>
<connect gate="C" pin="PLL_ENA" pad="AA8"/>
<connect gate="C" pin="VREFB7N2" pad="AD8"/>
<connect gate="D" pin="CONF_DONE" pad="D26"/>
<connect gate="D" pin="DCLK" pad="D25"/>
<connect gate="D" pin="GND" pad="H18"/>
<connect gate="D" pin="GND_10" pad="H16"/>
<connect gate="D" pin="GND_2" pad="E12"/>
<connect gate="D" pin="GND_3" pad="E15"/>
<connect gate="D" pin="GND_4" pad="E18"/>
<connect gate="D" pin="GND_5" pad="E21"/>
<connect gate="D" pin="GND_6" pad="E24"/>
<connect gate="D" pin="GND_7" pad="E27"/>
<connect gate="D" pin="GND_8" pad="H12"/>
<connect gate="D" pin="GND_9" pad="H15"/>
<connect gate="D" pin="IO" pad="F17"/>
<connect gate="D" pin="IO_10" pad="F27"/>
<connect gate="D" pin="IO_11" pad="F28"/>
<connect gate="D" pin="IO_12" pad="G10"/>
<connect gate="D" pin="IO_13" pad="G11"/>
<connect gate="D" pin="IO_14" pad="G12"/>
<connect gate="D" pin="IO_15" pad="G13"/>
<connect gate="D" pin="IO_16" pad="G14"/>
<connect gate="D" pin="IO_17" pad="G15"/>
<connect gate="D" pin="IO_18" pad="G16"/>
<connect gate="D" pin="IO_19" pad="G17"/>
<connect gate="D" pin="IO_2" pad="F18"/>
<connect gate="D" pin="IO_20" pad="G18"/>
<connect gate="D" pin="IO_21" pad="G19"/>
<connect gate="D" pin="IO_22" pad="G20"/>
<connect gate="D" pin="IO_23" pad="G21"/>
<connect gate="D" pin="IO_24" pad="G22"/>
<connect gate="D" pin="IO_25" pad="G23"/>
<connect gate="D" pin="IO_26" pad="G24"/>
<connect gate="D" pin="IO_27" pad="G25"/>
<connect gate="D" pin="IO_28" pad="G26"/>
<connect gate="D" pin="IO_29" pad="G27"/>
<connect gate="D" pin="IO_3" pad="F19"/>
<connect gate="D" pin="IO_30" pad="G28"/>
<connect gate="D" pin="IO_31" pad="H10"/>
<connect gate="D" pin="IO_32" pad="C17"/>
<connect gate="D" pin="IO_33" pad="H11"/>
<connect gate="D" pin="IO_34" pad="H13"/>
<connect gate="D" pin="IO_35" pad="H19"/>
<connect gate="D" pin="IO_36" pad="C18"/>
<connect gate="D" pin="IO_37" pad="C19"/>
<connect gate="D" pin="IO_38" pad="C20"/>
<connect gate="D" pin="IO_39" pad="C21"/>
<connect gate="D" pin="IO_4" pad="F20"/>
<connect gate="D" pin="IO_40" pad="C22"/>
<connect gate="D" pin="IO_41" pad="C23"/>
<connect gate="D" pin="IO_42" pad="C24"/>
<connect gate="D" pin="IO_43" pad="C25"/>
<connect gate="D" pin="IO_44" pad="C26"/>
<connect gate="D" pin="IO_45" pad="C27"/>
<connect gate="D" pin="IO_46" pad="C28"/>
<connect gate="D" pin="IO_47" pad="D10"/>
<connect gate="D" pin="IO_48" pad="D11"/>
<connect gate="D" pin="IO_49" pad="D12"/>
<connect gate="D" pin="IO_5" pad="F21"/>
<connect gate="D" pin="IO_50" pad="D13"/>
<connect gate="D" pin="IO_51" pad="D14"/>
<connect gate="D" pin="IO_52" pad="D15"/>
<connect gate="D" pin="IO_53" pad="D16"/>
<connect gate="D" pin="IO_54" pad="D17"/>
<connect gate="D" pin="IO_55" pad="D18"/>
<connect gate="D" pin="IO_56" pad="D19"/>
<connect gate="D" pin="IO_57" pad="D20"/>
<connect gate="D" pin="IO_58" pad="D21"/>
<connect gate="D" pin="IO_59" pad="D22"/>
<connect gate="D" pin="IO_6" pad="F22"/>
<connect gate="D" pin="IO_60" pad="D23"/>
<connect gate="D" pin="IO_61" pad="D27"/>
<connect gate="D" pin="IO_62" pad="D28"/>
<connect gate="D" pin="IO_63" pad="E10"/>
<connect gate="D" pin="IO_64" pad="E11"/>
<connect gate="D" pin="IO_65" pad="E13"/>
<connect gate="D" pin="IO_66" pad="E14"/>
<connect gate="D" pin="IO_67" pad="E16"/>
<connect gate="D" pin="IO_68" pad="E17"/>
<connect gate="D" pin="IO_69" pad="E25"/>
<connect gate="D" pin="IO_7" pad="F23"/>
<connect gate="D" pin="IO_70" pad="E26"/>
<connect gate="D" pin="IO_71" pad="E28"/>
<connect gate="D" pin="IO_72" pad="F11"/>
<connect gate="D" pin="IO_73" pad="F13"/>
<connect gate="D" pin="IO_74" pad="F14"/>
<connect gate="D" pin="IO_75" pad="F15"/>
<connect gate="D" pin="IO_76" pad="F16"/>
<connect gate="D" pin="IO_8" pad="F24"/>
<connect gate="D" pin="IO_9" pad="F26"/>
<connect gate="D" pin="NCE" pad="D24"/>
<connect gate="D" pin="NSTATUS" pad="E23"/>
<connect gate="D" pin="VCCIO3" pad="H17"/>
<connect gate="D" pin="VCCIO4" pad="H14"/>
<connect gate="D" pin="VREFB2N2" pad="F25"/>
<connect gate="D" pin="VREFB3N0" pad="E19"/>
<connect gate="D" pin="VREFB3N1" pad="E20"/>
<connect gate="D" pin="VREFB3N2" pad="E22"/>
<connect gate="D" pin="VREFB4N1" pad="F10"/>
<connect gate="D" pin="VREFB4N2" pad="F12"/>
<connect gate="E" pin="GND" pad="N19"/>
<connect gate="E" pin="GNDA_PLL5" pad="K15"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="J16"/>
<connect gate="E" pin="GND_10" pad="L27"/>
<connect gate="E" pin="GND_11" pad="M12"/>
<connect gate="E" pin="GND_12" pad="M14"/>
<connect gate="E" pin="GND_13" pad="M16"/>
<connect gate="E" pin="GND_14" pad="M18"/>
<connect gate="E" pin="GND_15" pad="M19"/>
<connect gate="E" pin="GND_16" pad="N10"/>
<connect gate="E" pin="GND_17" pad="N11"/>
<connect gate="E" pin="GND_18" pad="N13"/>
<connect gate="E" pin="GND_19" pad="N15"/>
<connect gate="E" pin="GND_2" pad="H21"/>
<connect gate="E" pin="GND_20" pad="N17"/>
<connect gate="E" pin="GND_3" pad="H24"/>
<connect gate="E" pin="GND_4" pad="H27"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="L15"/>
<connect gate="E" pin="GND_7" pad="L18"/>
<connect gate="E" pin="GND_8" pad="L21"/>
<connect gate="E" pin="GND_9" pad="L24"/>
<connect gate="E" pin="IO" pad="N20"/>
<connect gate="E" pin="IO_10" pad="J20"/>
<connect gate="E" pin="IO_11" pad="J21"/>
<connect gate="E" pin="IO_12" pad="J23"/>
<connect gate="E" pin="IO_13" pad="J24"/>
<connect gate="E" pin="IO_14" pad="J25"/>
<connect gate="E" pin="IO_15" pad="J26"/>
<connect gate="E" pin="IO_16" pad="J27"/>
<connect gate="E" pin="IO_17" pad="J28"/>
<connect gate="E" pin="IO_18" pad="K10"/>
<connect gate="E" pin="IO_19" pad="K11"/>
<connect gate="E" pin="IO_2" pad="H22"/>
<connect gate="E" pin="IO_20" pad="K12"/>
<connect gate="E" pin="IO_21" pad="K13"/>
<connect gate="E" pin="IO_22" pad="K14"/>
<connect gate="E" pin="IO_23" pad="K17"/>
<connect gate="E" pin="IO_24" pad="K18"/>
<connect gate="E" pin="IO_25" pad="K19"/>
<connect gate="E" pin="IO_26" pad="K20"/>
<connect gate="E" pin="IO_27" pad="K21"/>
<connect gate="E" pin="IO_28" pad="K22"/>
<connect gate="E" pin="IO_29" pad="K23"/>
<connect gate="E" pin="IO_3" pad="H23"/>
<connect gate="E" pin="IO_30" pad="K24"/>
<connect gate="E" pin="IO_31" pad="K25"/>
<connect gate="E" pin="IO_32" pad="K26"/>
<connect gate="E" pin="IO_33" pad="K27"/>
<connect gate="E" pin="IO_34" pad="K28"/>
<connect gate="E" pin="IO_35" pad="L12"/>
<connect gate="E" pin="IO_36" pad="L13"/>
<connect gate="E" pin="IO_37" pad="L14"/>
<connect gate="E" pin="IO_38" pad="L16"/>
<connect gate="E" pin="IO_39" pad="L17"/>
<connect gate="E" pin="IO_4" pad="H25"/>
<connect gate="E" pin="IO_40" pad="L19"/>
<connect gate="E" pin="IO_41" pad="L20"/>
<connect gate="E" pin="IO_42" pad="L23"/>
<connect gate="E" pin="IO_43" pad="L25"/>
<connect gate="E" pin="IO_44" pad="L26"/>
<connect gate="E" pin="IO_45" pad="L28"/>
<connect gate="E" pin="IO_46" pad="M20"/>
<connect gate="E" pin="IO_47" pad="M21"/>
<connect gate="E" pin="IO_48" pad="M22"/>
<connect gate="E" pin="IO_49" pad="M24"/>
<connect gate="E" pin="IO_5" pad="H26"/>
<connect gate="E" pin="IO_50" pad="M25"/>
<connect gate="E" pin="IO_51" pad="M26"/>
<connect gate="E" pin="IO_52" pad="M27"/>
<connect gate="E" pin="IO_53" pad="M28"/>
<connect gate="E" pin="IO_6" pad="H28"/>
<connect gate="E" pin="IO_7" pad="J10"/>
<connect gate="E" pin="IO_8" pad="J11"/>
<connect gate="E" pin="IO_9" pad="J18"/>
<connect gate="E" pin="VCCA_PLL5" pad="J15"/>
<connect gate="E" pin="VCCD_PLL1" pad="N22"/>
<connect gate="E" pin="VCCD_PLL5" pad="K16"/>
<connect gate="E" pin="VCCINT" pad="N18"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="M13"/>
<connect gate="E" pin="VCCINT_4" pad="M15"/>
<connect gate="E" pin="VCCINT_5" pad="M17"/>
<connect gate="E" pin="VCCINT_6" pad="N12"/>
<connect gate="E" pin="VCCINT_7" pad="N14"/>
<connect gate="E" pin="VCCINT_8" pad="N16"/>
<connect gate="E" pin="VCCIO2" pad="N21"/>
<connect gate="E" pin="VCCIO2_2" pad="J22"/>
<connect gate="E" pin="VCCIO2_3" pad="L22"/>
<connect gate="E" pin="VCCIO3" pad="J19"/>
<connect gate="E" pin="VCCIO3_2" pad="H20"/>
<connect gate="E" pin="VCCIO4" pad="J12"/>
<connect gate="E" pin="VCCP" pad="M10"/>
<connect gate="E" pin="VCCPD3" pad="J17"/>
<connect gate="E" pin="VCCPD4" pad="J13"/>
<connect gate="E" pin="VCCP_2" pad="L10"/>
<connect gate="E" pin="VCC_PLL5_OUT" pad="J14"/>
<connect gate="E" pin="VREFB2N1" pad="M23"/>
<connect gate="F" pin="CLK1N" pad="T24"/>
<connect gate="F" pin="CLK1P" pad="T25"/>
<connect gate="F" pin="CLK3N" pad="U25"/>
<connect gate="F" pin="CLK3P" pad="U26"/>
<connect gate="F" pin="GND" pad="V24"/>
<connect gate="F" pin="GNDA_PLL1" pad="P23"/>
<connect gate="F" pin="GNDA_PLL1_2" pad="P22"/>
<connect gate="F" pin="GNDA_PLL2" pad="R23"/>
<connect gate="F" pin="GNDA_PLL2_2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="P21"/>
<connect gate="F" pin="GND_11" pad="R11"/>
<connect gate="F" pin="GND_12" pad="R13"/>
<connect gate="F" pin="GND_13" pad="R15"/>
<connect gate="F" pin="GND_14" pad="R17"/>
<connect gate="F" pin="GND_15" pad="R19"/>
<connect gate="F" pin="GND_16" pad="R24"/>
<connect gate="F" pin="GND_17" pad="R27"/>
<connect gate="F" pin="GND_18" pad="T12"/>
<connect gate="F" pin="GND_19" pad="T14"/>
<connect gate="F" pin="GND_2" pad="N24"/>
<connect gate="F" pin="GND_20" pad="T16"/>
<connect gate="F" pin="GND_21" pad="T18"/>
<connect gate="F" pin="GND_22" pad="U10"/>
<connect gate="F" pin="GND_23" pad="U11"/>
<connect gate="F" pin="GND_24" pad="U13"/>
<connect gate="F" pin="GND_25" pad="U15"/>
<connect gate="F" pin="GND_26" pad="U17"/>
<connect gate="F" pin="GND_27" pad="U21"/>
<connect gate="F" pin="GND_28" pad="V10"/>
<connect gate="F" pin="GND_29" pad="V12"/>
<connect gate="F" pin="GND_3" pad="N27"/>
<connect gate="F" pin="GND_30" pad="V15"/>
<connect gate="F" pin="GND_31" pad="V18"/>
<connect gate="F" pin="GND_4" pad="P10"/>
<connect gate="F" pin="GND_5" pad="P12"/>
<connect gate="F" pin="GND_6" pad="P14"/>
<connect gate="F" pin="GND_7" pad="P16"/>
<connect gate="F" pin="GND_8" pad="P18"/>
<connect gate="F" pin="GND_9" pad="P19"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="R20"/>
<connect gate="F" pin="IO_11" pad="R21"/>
<connect gate="F" pin="IO_12" pad="R25"/>
<connect gate="F" pin="IO_13" pad="R26"/>
<connect gate="F" pin="IO_14" pad="R28"/>
<connect gate="F" pin="IO_15" pad="T19"/>
<connect gate="F" pin="IO_16" pad="T26"/>
<connect gate="F" pin="IO_17" pad="T27"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U19"/>
<connect gate="F" pin="IO_2" pad="N25"/>
<connect gate="F" pin="IO_20" pad="U20"/>
<connect gate="F" pin="IO_21" pad="U23"/>
<connect gate="F" pin="IO_22" pad="U24"/>
<connect gate="F" pin="IO_23" pad="U27"/>
<connect gate="F" pin="IO_24" pad="U28"/>
<connect gate="F" pin="IO_25" pad="V11"/>
<connect gate="F" pin="IO_26" pad="V13"/>
<connect gate="F" pin="IO_27" pad="V20"/>
<connect gate="F" pin="IO_28" pad="V22"/>
<connect gate="F" pin="IO_29" pad="V23"/>
<connect gate="F" pin="IO_3" pad="N26"/>
<connect gate="F" pin="IO_4" pad="N28"/>
<connect gate="F" pin="IO_5" pad="P24"/>
<connect gate="F" pin="IO_6" pad="P25"/>
<connect gate="F" pin="IO_7" pad="P26"/>
<connect gate="F" pin="IO_8" pad="P27"/>
<connect gate="F" pin="IO_9" pad="P28"/>
<connect gate="F" pin="NCONFIG" pad="V17"/>
<connect gate="F" pin="TCK" pad="V16"/>
<connect gate="F" pin="TDI" pad="V19"/>
<connect gate="F" pin="VCCA_PLL1" pad="N23"/>
<connect gate="F" pin="VCCA_PLL2" pad="T23"/>
<connect gate="F" pin="VCCD_PLL2" pad="T22"/>
<connect gate="F" pin="VCCD_PLL6" pad="V14"/>
<connect gate="F" pin="VCCINT" pad="U18"/>
<connect gate="F" pin="VCCINT_10" pad="T11"/>
<connect gate="F" pin="VCCINT_11" pad="T13"/>
<connect gate="F" pin="VCCINT_12" pad="T15"/>
<connect gate="F" pin="VCCINT_13" pad="T17"/>
<connect gate="F" pin="VCCINT_14" pad="U12"/>
<connect gate="F" pin="VCCINT_15" pad="U14"/>
<connect gate="F" pin="VCCINT_16" pad="U16"/>
<connect gate="F" pin="VCCINT_2" pad="P11"/>
<connect gate="F" pin="VCCINT_3" pad="P13"/>
<connect gate="F" pin="VCCINT_4" pad="P15"/>
<connect gate="F" pin="VCCINT_5" pad="P17"/>
<connect gate="F" pin="VCCINT_6" pad="R12"/>
<connect gate="F" pin="VCCINT_7" pad="R14"/>
<connect gate="F" pin="VCCINT_8" pad="R16"/>
<connect gate="F" pin="VCCINT_9" pad="R18"/>
<connect gate="F" pin="VCCIO1" pad="V21"/>
<connect gate="F" pin="VCCIO1_2" pad="U22"/>
<connect gate="F" pin="VCCP" pad="T10"/>
<connect gate="F" pin="VCCPD1" pad="T20"/>
<connect gate="F" pin="VCCPD2" pad="P20"/>
<connect gate="F" pin="VCCP_2" pad="R10"/>
<connect gate="F" pin="VREFB2N0" pad="T21"/>
<connect gate="G" pin="GND" pad="AA27"/>
<connect gate="G" pin="GNDA_PLL6" pad="W14"/>
<connect gate="G" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="G" pin="GND_10" pad="AA21"/>
<connect gate="G" pin="GND_11" pad="AA24"/>
<connect gate="G" pin="GND_2" pad="V27"/>
<connect gate="G" pin="GND_3" pad="W20"/>
<connect gate="G" pin="GND_4" pad="W22"/>
<connect gate="G" pin="GND_5" pad="Y20"/>
<connect gate="G" pin="GND_6" pad="AA12"/>
<connect gate="G" pin="GND_7" pad="AA15"/>
<connect gate="G" pin="GND_8" pad="AA18"/>
<connect gate="G" pin="GND_9" pad="AA20"/>
<connect gate="G" pin="IO" pad="AB20"/>
<connect gate="G" pin="IO_10" pad="AC11"/>
<connect gate="G" pin="IO_11" pad="AC12"/>
<connect gate="G" pin="IO_12" pad="AC13"/>
<connect gate="G" pin="IO_13" pad="AC14"/>
<connect gate="G" pin="IO_14" pad="AC15"/>
<connect gate="G" pin="IO_15" pad="AC16"/>
<connect gate="G" pin="IO_16" pad="AC17"/>
<connect gate="G" pin="IO_17" pad="AC18"/>
<connect gate="G" pin="IO_18" pad="AC19"/>
<connect gate="G" pin="IO_19" pad="AC20"/>
<connect gate="G" pin="IO_2" pad="AB21"/>
<connect gate="G" pin="IO_20" pad="AC21"/>
<connect gate="G" pin="IO_21" pad="AC22"/>
<connect gate="G" pin="IO_22" pad="AC23"/>
<connect gate="G" pin="IO_23" pad="AC24"/>
<connect gate="G" pin="IO_24" pad="AC25"/>
<connect gate="G" pin="IO_25" pad="AC26"/>
<connect gate="G" pin="IO_26" pad="AC27"/>
<connect gate="G" pin="IO_27" pad="AC28"/>
<connect gate="G" pin="IO_28" pad="V26"/>
<connect gate="G" pin="IO_29" pad="V28"/>
<connect gate="G" pin="IO_3" pad="AB22"/>
<connect gate="G" pin="IO_30" pad="W10"/>
<connect gate="G" pin="IO_31" pad="W11"/>
<connect gate="G" pin="IO_32" pad="W12"/>
<connect gate="G" pin="IO_33" pad="W15"/>
<connect gate="G" pin="IO_34" pad="W16"/>
<connect gate="G" pin="IO_35" pad="W21"/>
<connect gate="G" pin="IO_36" pad="W24"/>
<connect gate="G" pin="IO_37" pad="W25"/>
<connect gate="G" pin="IO_38" pad="W26"/>
<connect gate="G" pin="IO_39" pad="W27"/>
<connect gate="G" pin="IO_4" pad="AB23"/>
<connect gate="G" pin="IO_40" pad="W28"/>
<connect gate="G" pin="IO_41" pad="Y10"/>
<connect gate="G" pin="IO_42" pad="Y11"/>
<connect gate="G" pin="IO_43" pad="Y13"/>
<connect gate="G" pin="IO_44" pad="Y15"/>
<connect gate="G" pin="IO_45" pad="Y17"/>
<connect gate="G" pin="IO_46" pad="Y21"/>
<connect gate="G" pin="IO_47" pad="Y24"/>
<connect gate="G" pin="IO_48" pad="Y25"/>
<connect gate="G" pin="IO_49" pad="Y26"/>
<connect gate="G" pin="IO_5" pad="AB24"/>
<connect gate="G" pin="IO_50" pad="Y27"/>
<connect gate="G" pin="IO_51" pad="Y28"/>
<connect gate="G" pin="IO_52" pad="AA11"/>
<connect gate="G" pin="IO_53" pad="AA17"/>
<connect gate="G" pin="IO_54" pad="AA19"/>
<connect gate="G" pin="IO_55" pad="AA22"/>
<connect gate="G" pin="IO_56" pad="AA23"/>
<connect gate="G" pin="IO_57" pad="AA25"/>
<connect gate="G" pin="IO_58" pad="AA26"/>
<connect gate="G" pin="IO_59" pad="AA28"/>
<connect gate="G" pin="IO_6" pad="AB25"/>
<connect gate="G" pin="IO_60" pad="AB10"/>
<connect gate="G" pin="IO_61" pad="AB11"/>
<connect gate="G" pin="IO_62" pad="AB12"/>
<connect gate="G" pin="IO_63" pad="AB13"/>
<connect gate="G" pin="IO_64" pad="AB15"/>
<connect gate="G" pin="IO_65" pad="AB16"/>
<connect gate="G" pin="IO_66" pad="AB17"/>
<connect gate="G" pin="IO_67" pad="AB18"/>
<connect gate="G" pin="IO_68" pad="AB19"/>
<connect gate="G" pin="IO_7" pad="AB26"/>
<connect gate="G" pin="IO_8" pad="AB27"/>
<connect gate="G" pin="IO_9" pad="AB28"/>
<connect gate="G" pin="TMS" pad="W19"/>
<connect gate="G" pin="TRST" pad="W17"/>
<connect gate="G" pin="VCCA_PLL6" pad="Y14"/>
<connect gate="G" pin="VCCIO1" pad="Y22"/>
<connect gate="G" pin="VCCIO7" pad="AA13"/>
<connect gate="G" pin="VCCIO7_2" pad="AA10"/>
<connect gate="G" pin="VCCIO8" pad="AA16"/>
<connect gate="G" pin="VCCIO8_2" pad="Y18"/>
<connect gate="G" pin="VCCIO8_3" pad="Y19"/>
<connect gate="G" pin="VCCPD7" pad="Y12"/>
<connect gate="G" pin="VCCPD8" pad="Y16"/>
<connect gate="G" pin="VCCSEL" pad="W18"/>
<connect gate="G" pin="VCC_PLL6_OUT" pad="AA14"/>
<connect gate="G" pin="VREFB1N1" pad="Y23"/>
<connect gate="G" pin="VREFB1N2" pad="W23"/>
<connect gate="G" pin="VREFB7N0" pad="AB14"/>
<connect gate="G" pin="VREFB7N1" pad="AC10"/>
<connect gate="H" pin="GND" pad="AH27"/>
<connect gate="H" pin="GND_10" pad="AG18"/>
<connect gate="H" pin="GND_11" pad="AG21"/>
<connect gate="H" pin="GND_12" pad="AG24"/>
<connect gate="H" pin="GND_13" pad="AG27"/>
<connect gate="H" pin="GND_14" pad="AG28"/>
<connect gate="H" pin="GND_2" pad="AD12"/>
<connect gate="H" pin="GND_3" pad="AD15"/>
<connect gate="H" pin="GND_4" pad="AD18"/>
<connect gate="H" pin="GND_5" pad="AD21"/>
<connect gate="H" pin="GND_6" pad="AD24"/>
<connect gate="H" pin="GND_7" pad="AD27"/>
<connect gate="H" pin="GND_8" pad="AG12"/>
<connect gate="H" pin="GND_9" pad="AG15"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD28"/>
<connect gate="H" pin="IO_11" pad="AE10"/>
<connect gate="H" pin="IO_12" pad="AE11"/>
<connect gate="H" pin="IO_13" pad="AE12"/>
<connect gate="H" pin="IO_14" pad="AE13"/>
<connect gate="H" pin="IO_15" pad="AE14"/>
<connect gate="H" pin="IO_16" pad="AE15"/>
<connect gate="H" pin="IO_17" pad="AE17"/>
<connect gate="H" pin="IO_18" pad="AE18"/>
<connect gate="H" pin="IO_19" pad="AE19"/>
<connect gate="H" pin="IO_2" pad="AD10"/>
<connect gate="H" pin="IO_20" pad="AE20"/>
<connect gate="H" pin="IO_21" pad="AE21"/>
<connect gate="H" pin="IO_22" pad="AE22"/>
<connect gate="H" pin="IO_23" pad="AE23"/>
<connect gate="H" pin="IO_24" pad="AE24"/>
<connect gate="H" pin="IO_25" pad="AE25"/>
<connect gate="H" pin="IO_26" pad="AE26"/>
<connect gate="H" pin="IO_27" pad="AE27"/>
<connect gate="H" pin="IO_28" pad="AE28"/>
<connect gate="H" pin="IO_29" pad="AF10"/>
<connect gate="H" pin="IO_3" pad="AD11"/>
<connect gate="H" pin="IO_30" pad="AF11"/>
<connect gate="H" pin="IO_31" pad="AF12"/>
<connect gate="H" pin="IO_32" pad="AF21"/>
<connect gate="H" pin="IO_33" pad="AF22"/>
<connect gate="H" pin="IO_34" pad="AF23"/>
<connect gate="H" pin="IO_35" pad="AF24"/>
<connect gate="H" pin="IO_36" pad="AF25"/>
<connect gate="H" pin="IO_37" pad="AF26"/>
<connect gate="H" pin="IO_38" pad="AF27"/>
<connect gate="H" pin="IO_39" pad="AF28"/>
<connect gate="H" pin="IO_4" pad="AD13"/>
<connect gate="H" pin="IO_40" pad="AG10"/>
<connect gate="H" pin="IO_41" pad="AG11"/>
<connect gate="H" pin="IO_42" pad="AG13"/>
<connect gate="H" pin="IO_43" pad="AG14"/>
<connect gate="H" pin="IO_44" pad="AG16"/>
<connect gate="H" pin="IO_45" pad="AG17"/>
<connect gate="H" pin="IO_46" pad="AG19"/>
<connect gate="H" pin="IO_47" pad="AG20"/>
<connect gate="H" pin="IO_48" pad="AG22"/>
<connect gate="H" pin="IO_49" pad="AG23"/>
<connect gate="H" pin="IO_5" pad="AD14"/>
<connect gate="H" pin="IO_50" pad="AG25"/>
<connect gate="H" pin="IO_51" pad="AG26"/>
<connect gate="H" pin="IO_52" pad="AH10"/>
<connect gate="H" pin="IO_53" pad="AH11"/>
<connect gate="H" pin="IO_54" pad="AH12"/>
<connect gate="H" pin="IO_55" pad="AH13"/>
<connect gate="H" pin="IO_56" pad="AH14"/>
<connect gate="H" pin="IO_57" pad="AH15"/>
<connect gate="H" pin="IO_58" pad="AH16"/>
<connect gate="H" pin="IO_59" pad="AF13"/>
<connect gate="H" pin="IO_6" pad="AD16"/>
<connect gate="H" pin="IO_60" pad="AH17"/>
<connect gate="H" pin="IO_61" pad="AF14"/>
<connect gate="H" pin="IO_62" pad="AH18"/>
<connect gate="H" pin="IO_63" pad="AF15"/>
<connect gate="H" pin="IO_64" pad="AH19"/>
<connect gate="H" pin="IO_65" pad="AF17"/>
<connect gate="H" pin="IO_66" pad="AH20"/>
<connect gate="H" pin="IO_67" pad="AF18"/>
<connect gate="H" pin="IO_68" pad="AH21"/>
<connect gate="H" pin="IO_69" pad="AF19"/>
<connect gate="H" pin="IO_7" pad="AD20"/>
<connect gate="H" pin="IO_70" pad="AE16"/>
<connect gate="H" pin="IO_71" pad="AH22"/>
<connect gate="H" pin="IO_72" pad="AF16"/>
<connect gate="H" pin="IO_73" pad="AF20"/>
<connect gate="H" pin="IO_74" pad="AH23"/>
<connect gate="H" pin="IO_75" pad="AH24"/>
<connect gate="H" pin="IO_76" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD25"/>
<connect gate="H" pin="IO_9" pad="AD26"/>
<connect gate="H" pin="VREFB1N0" pad="AD23"/>
<connect gate="H" pin="VREFB8N0" pad="AD22"/>
<connect gate="H" pin="VREFB8N1" pad="AD19"/>
<connect gate="H" pin="VREFB8N2" pad="AD17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2SGX60CF780C5N"/>
<attribute name="OC_FARNELL" value="1549491"/>
<attribute name="OC_NEWARK" value="52R0641"/>
<attribute name="PACKAGE" value="BGA-780"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2SGX60DF780C5N">
<description>FPGA, STRATIX II GX</description>
<gates>
<gate name="A" symbol="EP2SGX60DF780C5N_A"/>
<gate name="B" symbol="EP2SGX60DF780C5N_B"/>
<gate name="C" symbol="EP2SGX60DF780C5N_C"/>
<gate name="D" symbol="EP2SGX60DF780C5N_D"/>
<gate name="E" symbol="EP2SGX60DF780C5N_E"/>
<gate name="F" symbol="EP2SGX60DF780C5N_F"/>
<gate name="G" symbol="EP2SGX60DF780C5N_G"/>
<gate name="H" symbol="EP2SGX60DF780C5N_H"/>
</gates>
<devices>
<device name="" package="BGA780C100P28X28_2900X2900X350">
<connects>
<connect gate="A" pin="GND" pad="L3"/>
<connect gate="A" pin="GND_10" pad="B4"/>
<connect gate="A" pin="GND_11" pad="B5"/>
<connect gate="A" pin="GND_12" pad="B6"/>
<connect gate="A" pin="GND_13" pad="B7"/>
<connect gate="A" pin="GND_14" pad="B9"/>
<connect gate="A" pin="GND_15" pad="C1"/>
<connect gate="A" pin="GND_16" pad="C2"/>
<connect gate="A" pin="GND_17" pad="C3"/>
<connect gate="A" pin="GND_18" pad="C6"/>
<connect gate="A" pin="GND_19" pad="D1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="GND_20" pad="D2"/>
<connect gate="A" pin="GND_21" pad="D3"/>
<connect gate="A" pin="GND_22" pad="D4"/>
<connect gate="A" pin="GND_23" pad="D5"/>
<connect gate="A" pin="GND_24" pad="D6"/>
<connect gate="A" pin="GND_25" pad="E3"/>
<connect gate="A" pin="GND_26" pad="E6"/>
<connect gate="A" pin="GND_27" pad="E7"/>
<connect gate="A" pin="GND_28" pad="E9"/>
<connect gate="A" pin="GND_29" pad="F1"/>
<connect gate="A" pin="GND_3" pad="A3"/>
<connect gate="A" pin="GND_30" pad="F2"/>
<connect gate="A" pin="GND_31" pad="F3"/>
<connect gate="A" pin="GND_32" pad="F4"/>
<connect gate="A" pin="GND_33" pad="F5"/>
<connect gate="A" pin="GND_34" pad="F6"/>
<connect gate="A" pin="GND_35" pad="G3"/>
<connect gate="A" pin="GND_36" pad="G6"/>
<connect gate="A" pin="GND_37" pad="H1"/>
<connect gate="A" pin="GND_38" pad="H2"/>
<connect gate="A" pin="GND_39" pad="H3"/>
<connect gate="A" pin="GND_4" pad="A4"/>
<connect gate="A" pin="GND_40" pad="H4"/>
<connect gate="A" pin="GND_41" pad="H5"/>
<connect gate="A" pin="GND_42" pad="H6"/>
<connect gate="A" pin="GND_43" pad="H7"/>
<connect gate="A" pin="GND_44" pad="H9"/>
<connect gate="A" pin="GND_45" pad="J3"/>
<connect gate="A" pin="GND_46" pad="J5"/>
<connect gate="A" pin="GND_47" pad="J6"/>
<connect gate="A" pin="GND_48" pad="J7"/>
<connect gate="A" pin="GND_49" pad="K1"/>
<connect gate="A" pin="GND_5" pad="A5"/>
<connect gate="A" pin="GND_50" pad="K2"/>
<connect gate="A" pin="GND_51" pad="K3"/>
<connect gate="A" pin="GND_52" pad="K4"/>
<connect gate="A" pin="GND_53" pad="K5"/>
<connect gate="A" pin="GND_54" pad="K6"/>
<connect gate="A" pin="GND_6" pad="A6"/>
<connect gate="A" pin="GND_7" pad="B1"/>
<connect gate="A" pin="GND_8" pad="B2"/>
<connect gate="A" pin="GND_9" pad="B3"/>
<connect gate="A" pin="GXB_RX0N" pad="G2"/>
<connect gate="A" pin="GXB_RX0P" pad="G1"/>
<connect gate="A" pin="GXB_RX1N" pad="E2"/>
<connect gate="A" pin="GXB_RX1P" pad="E1"/>
<connect gate="A" pin="GXB_RX2N" pad="L2"/>
<connect gate="A" pin="GXB_RX2P" pad="L1"/>
<connect gate="A" pin="GXB_TX0N" pad="E5"/>
<connect gate="A" pin="GXB_TX0P" pad="E4"/>
<connect gate="A" pin="GXB_TX1N" pad="C5"/>
<connect gate="A" pin="GXB_TX1P" pad="C4"/>
<connect gate="A" pin="GXB_TX2N" pad="L5"/>
<connect gate="A" pin="GXB_TX2P" pad="L4"/>
<connect gate="A" pin="IO" pad="G9"/>
<connect gate="A" pin="IO_10" pad="D8"/>
<connect gate="A" pin="IO_11" pad="D9"/>
<connect gate="A" pin="IO_2" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A8"/>
<connect gate="A" pin="IO_4" pad="A9"/>
<connect gate="A" pin="IO_5" pad="B8"/>
<connect gate="A" pin="IO_6" pad="C7"/>
<connect gate="A" pin="IO_7" pad="C8"/>
<connect gate="A" pin="IO_8" pad="C9"/>
<connect gate="A" pin="IO_9" pad="D7"/>
<connect gate="A" pin="MSEL0" pad="J8"/>
<connect gate="A" pin="MSEL1" pad="E8"/>
<connect gate="A" pin="MSEL2" pad="H8"/>
<connect gate="A" pin="MSEL3" pad="G8"/>
<connect gate="A" pin="NC" pad="K8"/>
<connect gate="A" pin="NC_2" pad="K7"/>
<connect gate="A" pin="REFCLK0_B13N" pad="J2"/>
<connect gate="A" pin="REFCLK0_B13P" pad="J1"/>
<connect gate="A" pin="REFCLK1_B13N" pad="G5"/>
<connect gate="A" pin="REFCLK1_B13P" pad="G4"/>
<connect gate="A" pin="RREFB13" pad="J4"/>
<connect gate="A" pin="TDO" pad="F8"/>
<connect gate="A" pin="TEMPDIODEN" pad="G7"/>
<connect gate="A" pin="TEMPDIODEP" pad="F7"/>
<connect gate="A" pin="VCCA" pad="L6"/>
<connect gate="A" pin="VCCA_2" pad="K9"/>
<connect gate="A" pin="VCCH_B13" pad="L9"/>
<connect gate="A" pin="VCCIO4" pad="J9"/>
<connect gate="A" pin="VCCR" pad="L7"/>
<connect gate="A" pin="VCCT_B13" pad="L8"/>
<connect gate="A" pin="VREFB4N0" pad="F9"/>
<connect gate="B" pin="GND" pad="Y6"/>
<connect gate="B" pin="GND_10" pad="N9"/>
<connect gate="B" pin="GND_11" pad="P1"/>
<connect gate="B" pin="GND_12" pad="P2"/>
<connect gate="B" pin="GND_13" pad="P3"/>
<connect gate="B" pin="GND_14" pad="P4"/>
<connect gate="B" pin="GND_15" pad="P5"/>
<connect gate="B" pin="GND_16" pad="P6"/>
<connect gate="B" pin="GND_17" pad="P8"/>
<connect gate="B" pin="GND_18" pad="R1"/>
<connect gate="B" pin="GND_19" pad="R2"/>
<connect gate="B" pin="GND_2" pad="M1"/>
<connect gate="B" pin="GND_20" pad="R3"/>
<connect gate="B" pin="GND_21" pad="R4"/>
<connect gate="B" pin="GND_22" pad="R5"/>
<connect gate="B" pin="GND_23" pad="T3"/>
<connect gate="B" pin="GND_24" pad="U1"/>
<connect gate="B" pin="GND_25" pad="U2"/>
<connect gate="B" pin="GND_26" pad="U3"/>
<connect gate="B" pin="GND_27" pad="U4"/>
<connect gate="B" pin="GND_28" pad="U5"/>
<connect gate="B" pin="GND_29" pad="U7"/>
<connect gate="B" pin="GND_3" pad="M2"/>
<connect gate="B" pin="GND_30" pad="U8"/>
<connect gate="B" pin="GND_31" pad="U9"/>
<connect gate="B" pin="GND_32" pad="V3"/>
<connect gate="B" pin="GND_33" pad="V6"/>
<connect gate="B" pin="GND_34" pad="V8"/>
<connect gate="B" pin="GND_35" pad="W1"/>
<connect gate="B" pin="GND_36" pad="W2"/>
<connect gate="B" pin="GND_37" pad="W3"/>
<connect gate="B" pin="GND_38" pad="W4"/>
<connect gate="B" pin="GND_39" pad="W5"/>
<connect gate="B" pin="GND_4" pad="M3"/>
<connect gate="B" pin="GND_40" pad="W6"/>
<connect gate="B" pin="GND_41" pad="W7"/>
<connect gate="B" pin="GND_42" pad="W8"/>
<connect gate="B" pin="GND_43" pad="Y3"/>
<connect gate="B" pin="GND_44" pad="Y5"/>
<connect gate="B" pin="GND_5" pad="M4"/>
<connect gate="B" pin="GND_6" pad="M5"/>
<connect gate="B" pin="GND_7" pad="N3"/>
<connect gate="B" pin="GND_8" pad="N7"/>
<connect gate="B" pin="GND_9" pad="N8"/>
<connect gate="B" pin="GXB_RX3N" pad="N2"/>
<connect gate="B" pin="GXB_RX3P" pad="N1"/>
<connect gate="B" pin="GXB_TX3N" pad="N5"/>
<connect gate="B" pin="GXB_TX3P" pad="N4"/>
<connect gate="B" pin="IO" pad="A26"/>
<connect gate="B" pin="IO_10" pad="A17"/>
<connect gate="B" pin="IO_11" pad="A18"/>
<connect gate="B" pin="IO_12" pad="A19"/>
<connect gate="B" pin="IO_13" pad="A20"/>
<connect gate="B" pin="IO_14" pad="A21"/>
<connect gate="B" pin="IO_15" pad="A22"/>
<connect gate="B" pin="IO_16" pad="A23"/>
<connect gate="B" pin="IO_17" pad="A24"/>
<connect gate="B" pin="IO_18" pad="A25"/>
<connect gate="B" pin="IO_2" pad="W9"/>
<connect gate="B" pin="IO_3" pad="A10"/>
<connect gate="B" pin="IO_4" pad="A11"/>
<connect gate="B" pin="IO_5" pad="A12"/>
<connect gate="B" pin="IO_6" pad="A13"/>
<connect gate="B" pin="IO_7" pad="A14"/>
<connect gate="B" pin="IO_8" pad="A15"/>
<connect gate="B" pin="IO_9" pad="A16"/>
<connect gate="B" pin="NC" pad="Y4"/>
<connect gate="B" pin="NC_10" pad="Y1"/>
<connect gate="B" pin="NC_11" pad="Y2"/>
<connect gate="B" pin="NC_2" pad="T1"/>
<connect gate="B" pin="NC_3" pad="T2"/>
<connect gate="B" pin="NC_4" pad="T4"/>
<connect gate="B" pin="NC_5" pad="T5"/>
<connect gate="B" pin="NC_6" pad="V1"/>
<connect gate="B" pin="NC_7" pad="V2"/>
<connect gate="B" pin="NC_8" pad="V4"/>
<connect gate="B" pin="NC_9" pad="V5"/>
<connect gate="B" pin="NIO_PULLUP" pad="Y7"/>
<connect gate="B" pin="PORSEL" pad="Y8"/>
<connect gate="B" pin="VCCA" pad="V9"/>
<connect gate="B" pin="VCCA_2" pad="M6"/>
<connect gate="B" pin="VCCA_3" pad="P7"/>
<connect gate="B" pin="VCCA_4" pad="P9"/>
<connect gate="B" pin="VCCA_5" pad="R6"/>
<connect gate="B" pin="VCCA_6" pad="T6"/>
<connect gate="B" pin="VCCA_7" pad="V7"/>
<connect gate="B" pin="VCCH_B13" pad="M9"/>
<connect gate="B" pin="VCCH_B14" pad="T9"/>
<connect gate="B" pin="VCCH_B14_2" pad="R9"/>
<connect gate="B" pin="VCCIO7" pad="Y9"/>
<connect gate="B" pin="VCCL_B13" pad="N6"/>
<connect gate="B" pin="VCCL_B14" pad="U6"/>
<connect gate="B" pin="VCCR" pad="T7"/>
<connect gate="B" pin="VCCR_2" pad="M7"/>
<connect gate="B" pin="VCCR_3" pad="R7"/>
<connect gate="B" pin="VCCT_B13" pad="M8"/>
<connect gate="B" pin="VCCT_B14" pad="T8"/>
<connect gate="B" pin="VCCT_B14_2" pad="R8"/>
<connect gate="C" pin="GND" pad="B28"/>
<connect gate="C" pin="GND_10" pad="AA9"/>
<connect gate="C" pin="GND_11" pad="AB3"/>
<connect gate="C" pin="GND_12" pad="AB6"/>
<connect gate="C" pin="GND_13" pad="AC1"/>
<connect gate="C" pin="GND_14" pad="AC2"/>
<connect gate="C" pin="GND_15" pad="AC3"/>
<connect gate="C" pin="GND_16" pad="AC4"/>
<connect gate="C" pin="GND_17" pad="AC5"/>
<connect gate="C" pin="GND_18" pad="AC6"/>
<connect gate="C" pin="GND_19" pad="AC7"/>
<connect gate="C" pin="GND_2" pad="A27"/>
<connect gate="C" pin="GND_20" pad="AD3"/>
<connect gate="C" pin="GND_21" pad="AD6"/>
<connect gate="C" pin="GND_22" pad="AD7"/>
<connect gate="C" pin="GND_23" pad="AD9"/>
<connect gate="C" pin="GND_24" pad="AE1"/>
<connect gate="C" pin="GND_25" pad="AE2"/>
<connect gate="C" pin="GND_26" pad="AE3"/>
<connect gate="C" pin="GND_27" pad="AE4"/>
<connect gate="C" pin="GND_28" pad="AE5"/>
<connect gate="C" pin="GND_29" pad="AE6"/>
<connect gate="C" pin="GND_3" pad="AA1"/>
<connect gate="C" pin="GND_30" pad="AF1"/>
<connect gate="C" pin="GND_31" pad="AF2"/>
<connect gate="C" pin="GND_32" pad="AF3"/>
<connect gate="C" pin="GND_33" pad="AF6"/>
<connect gate="C" pin="GND_34" pad="AG1"/>
<connect gate="C" pin="GND_35" pad="AG2"/>
<connect gate="C" pin="GND_36" pad="AG3"/>
<connect gate="C" pin="GND_37" pad="AG4"/>
<connect gate="C" pin="GND_38" pad="AG5"/>
<connect gate="C" pin="GND_39" pad="AG6"/>
<connect gate="C" pin="GND_4" pad="AA2"/>
<connect gate="C" pin="GND_40" pad="AG7"/>
<connect gate="C" pin="GND_41" pad="AG9"/>
<connect gate="C" pin="GND_42" pad="AH2"/>
<connect gate="C" pin="GND_43" pad="AH3"/>
<connect gate="C" pin="GND_44" pad="AH4"/>
<connect gate="C" pin="GND_45" pad="AH5"/>
<connect gate="C" pin="GND_46" pad="AH6"/>
<connect gate="C" pin="GND_47" pad="B12"/>
<connect gate="C" pin="GND_48" pad="B15"/>
<connect gate="C" pin="GND_49" pad="B18"/>
<connect gate="C" pin="GND_5" pad="AA3"/>
<connect gate="C" pin="GND_50" pad="B21"/>
<connect gate="C" pin="GND_51" pad="B24"/>
<connect gate="C" pin="GND_52" pad="B27"/>
<connect gate="C" pin="GND_6" pad="AA4"/>
<connect gate="C" pin="GND_7" pad="AA5"/>
<connect gate="C" pin="GND_8" pad="AA6"/>
<connect gate="C" pin="GND_9" pad="AA7"/>
<connect gate="C" pin="IO" pad="C16"/>
<connect gate="C" pin="IO_10" pad="AF8"/>
<connect gate="C" pin="IO_11" pad="AF9"/>
<connect gate="C" pin="IO_12" pad="AG8"/>
<connect gate="C" pin="IO_13" pad="AH7"/>
<connect gate="C" pin="IO_14" pad="AH8"/>
<connect gate="C" pin="IO_15" pad="AH9"/>
<connect gate="C" pin="IO_16" pad="B10"/>
<connect gate="C" pin="IO_17" pad="B11"/>
<connect gate="C" pin="IO_18" pad="B13"/>
<connect gate="C" pin="IO_19" pad="B14"/>
<connect gate="C" pin="IO_2" pad="AB8"/>
<connect gate="C" pin="IO_20" pad="B16"/>
<connect gate="C" pin="IO_21" pad="B17"/>
<connect gate="C" pin="IO_22" pad="B19"/>
<connect gate="C" pin="IO_23" pad="B20"/>
<connect gate="C" pin="IO_24" pad="B22"/>
<connect gate="C" pin="IO_25" pad="B23"/>
<connect gate="C" pin="IO_26" pad="B25"/>
<connect gate="C" pin="IO_27" pad="B26"/>
<connect gate="C" pin="IO_28" pad="C10"/>
<connect gate="C" pin="IO_29" pad="C11"/>
<connect gate="C" pin="IO_3" pad="AB9"/>
<connect gate="C" pin="IO_30" pad="C12"/>
<connect gate="C" pin="IO_31" pad="C13"/>
<connect gate="C" pin="IO_32" pad="C14"/>
<connect gate="C" pin="IO_33" pad="C15"/>
<connect gate="C" pin="IO_4" pad="AC8"/>
<connect gate="C" pin="IO_5" pad="AC9"/>
<connect gate="C" pin="IO_6" pad="AE7"/>
<connect gate="C" pin="IO_7" pad="AE8"/>
<connect gate="C" pin="IO_8" pad="AE9"/>
<connect gate="C" pin="IO_9" pad="AF7"/>
<connect gate="C" pin="NC" pad="AF5"/>
<connect gate="C" pin="NCEO" pad="AB7"/>
<connect gate="C" pin="NC_10" pad="AF4"/>
<connect gate="C" pin="NC_2" pad="AB2"/>
<connect gate="C" pin="NC_3" pad="AB4"/>
<connect gate="C" pin="NC_4" pad="AB5"/>
<connect gate="C" pin="NC_5" pad="AD1"/>
<connect gate="C" pin="NC_6" pad="AD2"/>
<connect gate="C" pin="NC_7" pad="AD4"/>
<connect gate="C" pin="NC_8" pad="AD5"/>
<connect gate="C" pin="NC_9" pad="AB1"/>
<connect gate="C" pin="PLL_ENA" pad="AA8"/>
<connect gate="C" pin="VREFB7N2" pad="AD8"/>
<connect gate="D" pin="CONF_DONE" pad="D26"/>
<connect gate="D" pin="DCLK" pad="D25"/>
<connect gate="D" pin="GND" pad="H18"/>
<connect gate="D" pin="GND_10" pad="H16"/>
<connect gate="D" pin="GND_2" pad="E12"/>
<connect gate="D" pin="GND_3" pad="E15"/>
<connect gate="D" pin="GND_4" pad="E18"/>
<connect gate="D" pin="GND_5" pad="E21"/>
<connect gate="D" pin="GND_6" pad="E24"/>
<connect gate="D" pin="GND_7" pad="E27"/>
<connect gate="D" pin="GND_8" pad="H12"/>
<connect gate="D" pin="GND_9" pad="H15"/>
<connect gate="D" pin="IO" pad="F17"/>
<connect gate="D" pin="IO_10" pad="F27"/>
<connect gate="D" pin="IO_11" pad="F28"/>
<connect gate="D" pin="IO_12" pad="G10"/>
<connect gate="D" pin="IO_13" pad="G11"/>
<connect gate="D" pin="IO_14" pad="G12"/>
<connect gate="D" pin="IO_15" pad="G13"/>
<connect gate="D" pin="IO_16" pad="G14"/>
<connect gate="D" pin="IO_17" pad="G15"/>
<connect gate="D" pin="IO_18" pad="G16"/>
<connect gate="D" pin="IO_19" pad="G17"/>
<connect gate="D" pin="IO_2" pad="F18"/>
<connect gate="D" pin="IO_20" pad="G18"/>
<connect gate="D" pin="IO_21" pad="G19"/>
<connect gate="D" pin="IO_22" pad="G20"/>
<connect gate="D" pin="IO_23" pad="G21"/>
<connect gate="D" pin="IO_24" pad="G22"/>
<connect gate="D" pin="IO_25" pad="G23"/>
<connect gate="D" pin="IO_26" pad="G24"/>
<connect gate="D" pin="IO_27" pad="G25"/>
<connect gate="D" pin="IO_28" pad="G26"/>
<connect gate="D" pin="IO_29" pad="G27"/>
<connect gate="D" pin="IO_3" pad="F19"/>
<connect gate="D" pin="IO_30" pad="G28"/>
<connect gate="D" pin="IO_31" pad="H10"/>
<connect gate="D" pin="IO_32" pad="C17"/>
<connect gate="D" pin="IO_33" pad="H11"/>
<connect gate="D" pin="IO_34" pad="H13"/>
<connect gate="D" pin="IO_35" pad="H19"/>
<connect gate="D" pin="IO_36" pad="C18"/>
<connect gate="D" pin="IO_37" pad="C19"/>
<connect gate="D" pin="IO_38" pad="C20"/>
<connect gate="D" pin="IO_39" pad="C21"/>
<connect gate="D" pin="IO_4" pad="F20"/>
<connect gate="D" pin="IO_40" pad="C22"/>
<connect gate="D" pin="IO_41" pad="C23"/>
<connect gate="D" pin="IO_42" pad="C24"/>
<connect gate="D" pin="IO_43" pad="C25"/>
<connect gate="D" pin="IO_44" pad="C26"/>
<connect gate="D" pin="IO_45" pad="C27"/>
<connect gate="D" pin="IO_46" pad="C28"/>
<connect gate="D" pin="IO_47" pad="D10"/>
<connect gate="D" pin="IO_48" pad="D11"/>
<connect gate="D" pin="IO_49" pad="D12"/>
<connect gate="D" pin="IO_5" pad="F21"/>
<connect gate="D" pin="IO_50" pad="D13"/>
<connect gate="D" pin="IO_51" pad="D14"/>
<connect gate="D" pin="IO_52" pad="D15"/>
<connect gate="D" pin="IO_53" pad="D16"/>
<connect gate="D" pin="IO_54" pad="D17"/>
<connect gate="D" pin="IO_55" pad="D18"/>
<connect gate="D" pin="IO_56" pad="D19"/>
<connect gate="D" pin="IO_57" pad="D20"/>
<connect gate="D" pin="IO_58" pad="D21"/>
<connect gate="D" pin="IO_59" pad="D22"/>
<connect gate="D" pin="IO_6" pad="F22"/>
<connect gate="D" pin="IO_60" pad="D23"/>
<connect gate="D" pin="IO_61" pad="D27"/>
<connect gate="D" pin="IO_62" pad="D28"/>
<connect gate="D" pin="IO_63" pad="E10"/>
<connect gate="D" pin="IO_64" pad="E11"/>
<connect gate="D" pin="IO_65" pad="E13"/>
<connect gate="D" pin="IO_66" pad="E14"/>
<connect gate="D" pin="IO_67" pad="E16"/>
<connect gate="D" pin="IO_68" pad="E17"/>
<connect gate="D" pin="IO_69" pad="E25"/>
<connect gate="D" pin="IO_7" pad="F23"/>
<connect gate="D" pin="IO_70" pad="E26"/>
<connect gate="D" pin="IO_71" pad="E28"/>
<connect gate="D" pin="IO_72" pad="F11"/>
<connect gate="D" pin="IO_73" pad="F13"/>
<connect gate="D" pin="IO_74" pad="F14"/>
<connect gate="D" pin="IO_75" pad="F15"/>
<connect gate="D" pin="IO_76" pad="F16"/>
<connect gate="D" pin="IO_8" pad="F24"/>
<connect gate="D" pin="IO_9" pad="F26"/>
<connect gate="D" pin="NCE" pad="D24"/>
<connect gate="D" pin="NSTATUS" pad="E23"/>
<connect gate="D" pin="VCCIO3" pad="H17"/>
<connect gate="D" pin="VCCIO4" pad="H14"/>
<connect gate="D" pin="VREFB2N2" pad="F25"/>
<connect gate="D" pin="VREFB3N0" pad="E19"/>
<connect gate="D" pin="VREFB3N1" pad="E20"/>
<connect gate="D" pin="VREFB3N2" pad="E22"/>
<connect gate="D" pin="VREFB4N1" pad="F10"/>
<connect gate="D" pin="VREFB4N2" pad="F12"/>
<connect gate="E" pin="GND" pad="N19"/>
<connect gate="E" pin="GNDA_PLL5" pad="K15"/>
<connect gate="E" pin="GNDA_PLL5_2" pad="J16"/>
<connect gate="E" pin="GND_10" pad="L27"/>
<connect gate="E" pin="GND_11" pad="M12"/>
<connect gate="E" pin="GND_12" pad="M14"/>
<connect gate="E" pin="GND_13" pad="M16"/>
<connect gate="E" pin="GND_14" pad="M18"/>
<connect gate="E" pin="GND_15" pad="M19"/>
<connect gate="E" pin="GND_16" pad="N10"/>
<connect gate="E" pin="GND_17" pad="N11"/>
<connect gate="E" pin="GND_18" pad="N13"/>
<connect gate="E" pin="GND_19" pad="N15"/>
<connect gate="E" pin="GND_2" pad="H21"/>
<connect gate="E" pin="GND_20" pad="N17"/>
<connect gate="E" pin="GND_3" pad="H24"/>
<connect gate="E" pin="GND_4" pad="H27"/>
<connect gate="E" pin="GND_5" pad="L11"/>
<connect gate="E" pin="GND_6" pad="L15"/>
<connect gate="E" pin="GND_7" pad="L18"/>
<connect gate="E" pin="GND_8" pad="L21"/>
<connect gate="E" pin="GND_9" pad="L24"/>
<connect gate="E" pin="IO" pad="N20"/>
<connect gate="E" pin="IO_10" pad="J20"/>
<connect gate="E" pin="IO_11" pad="J21"/>
<connect gate="E" pin="IO_12" pad="J23"/>
<connect gate="E" pin="IO_13" pad="J24"/>
<connect gate="E" pin="IO_14" pad="J25"/>
<connect gate="E" pin="IO_15" pad="J26"/>
<connect gate="E" pin="IO_16" pad="J27"/>
<connect gate="E" pin="IO_17" pad="J28"/>
<connect gate="E" pin="IO_18" pad="K10"/>
<connect gate="E" pin="IO_19" pad="K11"/>
<connect gate="E" pin="IO_2" pad="H22"/>
<connect gate="E" pin="IO_20" pad="K12"/>
<connect gate="E" pin="IO_21" pad="K13"/>
<connect gate="E" pin="IO_22" pad="K14"/>
<connect gate="E" pin="IO_23" pad="K17"/>
<connect gate="E" pin="IO_24" pad="K18"/>
<connect gate="E" pin="IO_25" pad="K19"/>
<connect gate="E" pin="IO_26" pad="K20"/>
<connect gate="E" pin="IO_27" pad="K21"/>
<connect gate="E" pin="IO_28" pad="K22"/>
<connect gate="E" pin="IO_29" pad="K23"/>
<connect gate="E" pin="IO_3" pad="H23"/>
<connect gate="E" pin="IO_30" pad="K24"/>
<connect gate="E" pin="IO_31" pad="K25"/>
<connect gate="E" pin="IO_32" pad="K26"/>
<connect gate="E" pin="IO_33" pad="K27"/>
<connect gate="E" pin="IO_34" pad="K28"/>
<connect gate="E" pin="IO_35" pad="L12"/>
<connect gate="E" pin="IO_36" pad="L13"/>
<connect gate="E" pin="IO_37" pad="L14"/>
<connect gate="E" pin="IO_38" pad="L16"/>
<connect gate="E" pin="IO_39" pad="L17"/>
<connect gate="E" pin="IO_4" pad="H25"/>
<connect gate="E" pin="IO_40" pad="L19"/>
<connect gate="E" pin="IO_41" pad="L20"/>
<connect gate="E" pin="IO_42" pad="L23"/>
<connect gate="E" pin="IO_43" pad="L25"/>
<connect gate="E" pin="IO_44" pad="L26"/>
<connect gate="E" pin="IO_45" pad="L28"/>
<connect gate="E" pin="IO_46" pad="M20"/>
<connect gate="E" pin="IO_47" pad="M21"/>
<connect gate="E" pin="IO_48" pad="M22"/>
<connect gate="E" pin="IO_49" pad="M24"/>
<connect gate="E" pin="IO_5" pad="H26"/>
<connect gate="E" pin="IO_50" pad="M25"/>
<connect gate="E" pin="IO_51" pad="M26"/>
<connect gate="E" pin="IO_52" pad="M27"/>
<connect gate="E" pin="IO_53" pad="M28"/>
<connect gate="E" pin="IO_6" pad="H28"/>
<connect gate="E" pin="IO_7" pad="J10"/>
<connect gate="E" pin="IO_8" pad="J11"/>
<connect gate="E" pin="IO_9" pad="J18"/>
<connect gate="E" pin="VCCA_PLL5" pad="J15"/>
<connect gate="E" pin="VCCD_PLL1" pad="N22"/>
<connect gate="E" pin="VCCD_PLL5" pad="K16"/>
<connect gate="E" pin="VCCINT" pad="N18"/>
<connect gate="E" pin="VCCINT_2" pad="M11"/>
<connect gate="E" pin="VCCINT_3" pad="M13"/>
<connect gate="E" pin="VCCINT_4" pad="M15"/>
<connect gate="E" pin="VCCINT_5" pad="M17"/>
<connect gate="E" pin="VCCINT_6" pad="N12"/>
<connect gate="E" pin="VCCINT_7" pad="N14"/>
<connect gate="E" pin="VCCINT_8" pad="N16"/>
<connect gate="E" pin="VCCIO2" pad="N21"/>
<connect gate="E" pin="VCCIO2_2" pad="J22"/>
<connect gate="E" pin="VCCIO2_3" pad="L22"/>
<connect gate="E" pin="VCCIO3" pad="J19"/>
<connect gate="E" pin="VCCIO3_2" pad="H20"/>
<connect gate="E" pin="VCCIO4" pad="J12"/>
<connect gate="E" pin="VCCP" pad="M10"/>
<connect gate="E" pin="VCCPD3" pad="J17"/>
<connect gate="E" pin="VCCPD4" pad="J13"/>
<connect gate="E" pin="VCCP_2" pad="L10"/>
<connect gate="E" pin="VCC_PLL5_OUT" pad="J14"/>
<connect gate="E" pin="VREFB2N1" pad="M23"/>
<connect gate="F" pin="CLK1N" pad="T24"/>
<connect gate="F" pin="CLK1P" pad="T25"/>
<connect gate="F" pin="CLK3N" pad="U25"/>
<connect gate="F" pin="CLK3P" pad="U26"/>
<connect gate="F" pin="GND" pad="V24"/>
<connect gate="F" pin="GNDA_PLL1" pad="P23"/>
<connect gate="F" pin="GNDA_PLL1_2" pad="P22"/>
<connect gate="F" pin="GNDA_PLL2" pad="R23"/>
<connect gate="F" pin="GNDA_PLL2_2" pad="R22"/>
<connect gate="F" pin="GND_10" pad="P21"/>
<connect gate="F" pin="GND_11" pad="R11"/>
<connect gate="F" pin="GND_12" pad="R13"/>
<connect gate="F" pin="GND_13" pad="R15"/>
<connect gate="F" pin="GND_14" pad="R17"/>
<connect gate="F" pin="GND_15" pad="R19"/>
<connect gate="F" pin="GND_16" pad="R24"/>
<connect gate="F" pin="GND_17" pad="R27"/>
<connect gate="F" pin="GND_18" pad="T12"/>
<connect gate="F" pin="GND_19" pad="T14"/>
<connect gate="F" pin="GND_2" pad="N24"/>
<connect gate="F" pin="GND_20" pad="T16"/>
<connect gate="F" pin="GND_21" pad="T18"/>
<connect gate="F" pin="GND_22" pad="U10"/>
<connect gate="F" pin="GND_23" pad="U11"/>
<connect gate="F" pin="GND_24" pad="U13"/>
<connect gate="F" pin="GND_25" pad="U15"/>
<connect gate="F" pin="GND_26" pad="U17"/>
<connect gate="F" pin="GND_27" pad="U21"/>
<connect gate="F" pin="GND_28" pad="V10"/>
<connect gate="F" pin="GND_29" pad="V12"/>
<connect gate="F" pin="GND_3" pad="N27"/>
<connect gate="F" pin="GND_30" pad="V15"/>
<connect gate="F" pin="GND_31" pad="V18"/>
<connect gate="F" pin="GND_4" pad="P10"/>
<connect gate="F" pin="GND_5" pad="P12"/>
<connect gate="F" pin="GND_6" pad="P14"/>
<connect gate="F" pin="GND_7" pad="P16"/>
<connect gate="F" pin="GND_8" pad="P18"/>
<connect gate="F" pin="GND_9" pad="P19"/>
<connect gate="F" pin="IO" pad="V25"/>
<connect gate="F" pin="IO_10" pad="R20"/>
<connect gate="F" pin="IO_11" pad="R21"/>
<connect gate="F" pin="IO_12" pad="R25"/>
<connect gate="F" pin="IO_13" pad="R26"/>
<connect gate="F" pin="IO_14" pad="R28"/>
<connect gate="F" pin="IO_15" pad="T19"/>
<connect gate="F" pin="IO_16" pad="T26"/>
<connect gate="F" pin="IO_17" pad="T27"/>
<connect gate="F" pin="IO_18" pad="T28"/>
<connect gate="F" pin="IO_19" pad="U19"/>
<connect gate="F" pin="IO_2" pad="N25"/>
<connect gate="F" pin="IO_20" pad="U20"/>
<connect gate="F" pin="IO_21" pad="U23"/>
<connect gate="F" pin="IO_22" pad="U24"/>
<connect gate="F" pin="IO_23" pad="U27"/>
<connect gate="F" pin="IO_24" pad="U28"/>
<connect gate="F" pin="IO_25" pad="V11"/>
<connect gate="F" pin="IO_26" pad="V13"/>
<connect gate="F" pin="IO_27" pad="V20"/>
<connect gate="F" pin="IO_28" pad="V22"/>
<connect gate="F" pin="IO_29" pad="V23"/>
<connect gate="F" pin="IO_3" pad="N26"/>
<connect gate="F" pin="IO_4" pad="N28"/>
<connect gate="F" pin="IO_5" pad="P24"/>
<connect gate="F" pin="IO_6" pad="P25"/>
<connect gate="F" pin="IO_7" pad="P26"/>
<connect gate="F" pin="IO_8" pad="P27"/>
<connect gate="F" pin="IO_9" pad="P28"/>
<connect gate="F" pin="NCONFIG" pad="V17"/>
<connect gate="F" pin="TCK" pad="V16"/>
<connect gate="F" pin="TDI" pad="V19"/>
<connect gate="F" pin="VCCA_PLL1" pad="N23"/>
<connect gate="F" pin="VCCA_PLL2" pad="T23"/>
<connect gate="F" pin="VCCD_PLL2" pad="T22"/>
<connect gate="F" pin="VCCD_PLL6" pad="V14"/>
<connect gate="F" pin="VCCINT" pad="U18"/>
<connect gate="F" pin="VCCINT_10" pad="T11"/>
<connect gate="F" pin="VCCINT_11" pad="T13"/>
<connect gate="F" pin="VCCINT_12" pad="T15"/>
<connect gate="F" pin="VCCINT_13" pad="T17"/>
<connect gate="F" pin="VCCINT_14" pad="U12"/>
<connect gate="F" pin="VCCINT_15" pad="U14"/>
<connect gate="F" pin="VCCINT_16" pad="U16"/>
<connect gate="F" pin="VCCINT_2" pad="P11"/>
<connect gate="F" pin="VCCINT_3" pad="P13"/>
<connect gate="F" pin="VCCINT_4" pad="P15"/>
<connect gate="F" pin="VCCINT_5" pad="P17"/>
<connect gate="F" pin="VCCINT_6" pad="R12"/>
<connect gate="F" pin="VCCINT_7" pad="R14"/>
<connect gate="F" pin="VCCINT_8" pad="R16"/>
<connect gate="F" pin="VCCINT_9" pad="R18"/>
<connect gate="F" pin="VCCIO1" pad="V21"/>
<connect gate="F" pin="VCCIO1_2" pad="U22"/>
<connect gate="F" pin="VCCP" pad="T10"/>
<connect gate="F" pin="VCCPD1" pad="T20"/>
<connect gate="F" pin="VCCPD2" pad="P20"/>
<connect gate="F" pin="VCCP_2" pad="R10"/>
<connect gate="F" pin="VREFB2N0" pad="T21"/>
<connect gate="G" pin="GND" pad="AA27"/>
<connect gate="G" pin="GNDA_PLL6" pad="W14"/>
<connect gate="G" pin="GNDA_PLL6_2" pad="W13"/>
<connect gate="G" pin="GND_10" pad="AA21"/>
<connect gate="G" pin="GND_11" pad="AA24"/>
<connect gate="G" pin="GND_2" pad="V27"/>
<connect gate="G" pin="GND_3" pad="W20"/>
<connect gate="G" pin="GND_4" pad="W22"/>
<connect gate="G" pin="GND_5" pad="Y20"/>
<connect gate="G" pin="GND_6" pad="AA12"/>
<connect gate="G" pin="GND_7" pad="AA15"/>
<connect gate="G" pin="GND_8" pad="AA18"/>
<connect gate="G" pin="GND_9" pad="AA20"/>
<connect gate="G" pin="IO" pad="AB20"/>
<connect gate="G" pin="IO_10" pad="AC11"/>
<connect gate="G" pin="IO_11" pad="AC12"/>
<connect gate="G" pin="IO_12" pad="AC13"/>
<connect gate="G" pin="IO_13" pad="AC14"/>
<connect gate="G" pin="IO_14" pad="AC15"/>
<connect gate="G" pin="IO_15" pad="AC16"/>
<connect gate="G" pin="IO_16" pad="AC17"/>
<connect gate="G" pin="IO_17" pad="AC18"/>
<connect gate="G" pin="IO_18" pad="AC19"/>
<connect gate="G" pin="IO_19" pad="AC20"/>
<connect gate="G" pin="IO_2" pad="AB21"/>
<connect gate="G" pin="IO_20" pad="AC21"/>
<connect gate="G" pin="IO_21" pad="AC22"/>
<connect gate="G" pin="IO_22" pad="AC23"/>
<connect gate="G" pin="IO_23" pad="AC24"/>
<connect gate="G" pin="IO_24" pad="AC25"/>
<connect gate="G" pin="IO_25" pad="AC26"/>
<connect gate="G" pin="IO_26" pad="AC27"/>
<connect gate="G" pin="IO_27" pad="AC28"/>
<connect gate="G" pin="IO_28" pad="V26"/>
<connect gate="G" pin="IO_29" pad="V28"/>
<connect gate="G" pin="IO_3" pad="AB22"/>
<connect gate="G" pin="IO_30" pad="W10"/>
<connect gate="G" pin="IO_31" pad="W11"/>
<connect gate="G" pin="IO_32" pad="W12"/>
<connect gate="G" pin="IO_33" pad="W15"/>
<connect gate="G" pin="IO_34" pad="W16"/>
<connect gate="G" pin="IO_35" pad="W21"/>
<connect gate="G" pin="IO_36" pad="W24"/>
<connect gate="G" pin="IO_37" pad="W25"/>
<connect gate="G" pin="IO_38" pad="W26"/>
<connect gate="G" pin="IO_39" pad="W27"/>
<connect gate="G" pin="IO_4" pad="AB23"/>
<connect gate="G" pin="IO_40" pad="W28"/>
<connect gate="G" pin="IO_41" pad="Y10"/>
<connect gate="G" pin="IO_42" pad="Y11"/>
<connect gate="G" pin="IO_43" pad="Y13"/>
<connect gate="G" pin="IO_44" pad="Y15"/>
<connect gate="G" pin="IO_45" pad="Y17"/>
<connect gate="G" pin="IO_46" pad="Y21"/>
<connect gate="G" pin="IO_47" pad="Y24"/>
<connect gate="G" pin="IO_48" pad="Y25"/>
<connect gate="G" pin="IO_49" pad="Y26"/>
<connect gate="G" pin="IO_5" pad="AB24"/>
<connect gate="G" pin="IO_50" pad="Y27"/>
<connect gate="G" pin="IO_51" pad="Y28"/>
<connect gate="G" pin="IO_52" pad="AA11"/>
<connect gate="G" pin="IO_53" pad="AA17"/>
<connect gate="G" pin="IO_54" pad="AA19"/>
<connect gate="G" pin="IO_55" pad="AA22"/>
<connect gate="G" pin="IO_56" pad="AA23"/>
<connect gate="G" pin="IO_57" pad="AA25"/>
<connect gate="G" pin="IO_58" pad="AA26"/>
<connect gate="G" pin="IO_59" pad="AA28"/>
<connect gate="G" pin="IO_6" pad="AB25"/>
<connect gate="G" pin="IO_60" pad="AB10"/>
<connect gate="G" pin="IO_61" pad="AB11"/>
<connect gate="G" pin="IO_62" pad="AB12"/>
<connect gate="G" pin="IO_63" pad="AB13"/>
<connect gate="G" pin="IO_64" pad="AB15"/>
<connect gate="G" pin="IO_65" pad="AB16"/>
<connect gate="G" pin="IO_66" pad="AB17"/>
<connect gate="G" pin="IO_67" pad="AB18"/>
<connect gate="G" pin="IO_68" pad="AB19"/>
<connect gate="G" pin="IO_7" pad="AB26"/>
<connect gate="G" pin="IO_8" pad="AB27"/>
<connect gate="G" pin="IO_9" pad="AB28"/>
<connect gate="G" pin="TMS" pad="W19"/>
<connect gate="G" pin="TRST" pad="W17"/>
<connect gate="G" pin="VCCA_PLL6" pad="Y14"/>
<connect gate="G" pin="VCCIO1" pad="Y22"/>
<connect gate="G" pin="VCCIO7" pad="AA13"/>
<connect gate="G" pin="VCCIO7_2" pad="AA10"/>
<connect gate="G" pin="VCCIO8" pad="AA16"/>
<connect gate="G" pin="VCCIO8_2" pad="Y18"/>
<connect gate="G" pin="VCCIO8_3" pad="Y19"/>
<connect gate="G" pin="VCCPD7" pad="Y12"/>
<connect gate="G" pin="VCCPD8" pad="Y16"/>
<connect gate="G" pin="VCCSEL" pad="W18"/>
<connect gate="G" pin="VCC_PLL6_OUT" pad="AA14"/>
<connect gate="G" pin="VREFB1N1" pad="Y23"/>
<connect gate="G" pin="VREFB1N2" pad="W23"/>
<connect gate="G" pin="VREFB7N0" pad="AB14"/>
<connect gate="G" pin="VREFB7N1" pad="AC10"/>
<connect gate="H" pin="GND" pad="AH27"/>
<connect gate="H" pin="GND_10" pad="AG18"/>
<connect gate="H" pin="GND_11" pad="AG21"/>
<connect gate="H" pin="GND_12" pad="AG24"/>
<connect gate="H" pin="GND_13" pad="AG27"/>
<connect gate="H" pin="GND_14" pad="AG28"/>
<connect gate="H" pin="GND_2" pad="AD12"/>
<connect gate="H" pin="GND_3" pad="AD15"/>
<connect gate="H" pin="GND_4" pad="AD18"/>
<connect gate="H" pin="GND_5" pad="AD21"/>
<connect gate="H" pin="GND_6" pad="AD24"/>
<connect gate="H" pin="GND_7" pad="AD27"/>
<connect gate="H" pin="GND_8" pad="AG12"/>
<connect gate="H" pin="GND_9" pad="AG15"/>
<connect gate="H" pin="IO" pad="AH26"/>
<connect gate="H" pin="IO_10" pad="AD28"/>
<connect gate="H" pin="IO_11" pad="AE10"/>
<connect gate="H" pin="IO_12" pad="AE11"/>
<connect gate="H" pin="IO_13" pad="AE12"/>
<connect gate="H" pin="IO_14" pad="AE13"/>
<connect gate="H" pin="IO_15" pad="AE14"/>
<connect gate="H" pin="IO_16" pad="AE15"/>
<connect gate="H" pin="IO_17" pad="AE17"/>
<connect gate="H" pin="IO_18" pad="AE18"/>
<connect gate="H" pin="IO_19" pad="AE19"/>
<connect gate="H" pin="IO_2" pad="AD10"/>
<connect gate="H" pin="IO_20" pad="AE20"/>
<connect gate="H" pin="IO_21" pad="AE21"/>
<connect gate="H" pin="IO_22" pad="AE22"/>
<connect gate="H" pin="IO_23" pad="AE23"/>
<connect gate="H" pin="IO_24" pad="AE24"/>
<connect gate="H" pin="IO_25" pad="AE25"/>
<connect gate="H" pin="IO_26" pad="AE26"/>
<connect gate="H" pin="IO_27" pad="AE27"/>
<connect gate="H" pin="IO_28" pad="AE28"/>
<connect gate="H" pin="IO_29" pad="AF10"/>
<connect gate="H" pin="IO_3" pad="AD11"/>
<connect gate="H" pin="IO_30" pad="AF11"/>
<connect gate="H" pin="IO_31" pad="AF12"/>
<connect gate="H" pin="IO_32" pad="AF21"/>
<connect gate="H" pin="IO_33" pad="AF22"/>
<connect gate="H" pin="IO_34" pad="AF23"/>
<connect gate="H" pin="IO_35" pad="AF24"/>
<connect gate="H" pin="IO_36" pad="AF25"/>
<connect gate="H" pin="IO_37" pad="AF26"/>
<connect gate="H" pin="IO_38" pad="AF27"/>
<connect gate="H" pin="IO_39" pad="AF28"/>
<connect gate="H" pin="IO_4" pad="AD13"/>
<connect gate="H" pin="IO_40" pad="AG10"/>
<connect gate="H" pin="IO_41" pad="AG11"/>
<connect gate="H" pin="IO_42" pad="AG13"/>
<connect gate="H" pin="IO_43" pad="AG14"/>
<connect gate="H" pin="IO_44" pad="AG16"/>
<connect gate="H" pin="IO_45" pad="AG17"/>
<connect gate="H" pin="IO_46" pad="AG19"/>
<connect gate="H" pin="IO_47" pad="AG20"/>
<connect gate="H" pin="IO_48" pad="AG22"/>
<connect gate="H" pin="IO_49" pad="AG23"/>
<connect gate="H" pin="IO_5" pad="AD14"/>
<connect gate="H" pin="IO_50" pad="AG25"/>
<connect gate="H" pin="IO_51" pad="AG26"/>
<connect gate="H" pin="IO_52" pad="AH10"/>
<connect gate="H" pin="IO_53" pad="AH11"/>
<connect gate="H" pin="IO_54" pad="AH12"/>
<connect gate="H" pin="IO_55" pad="AH13"/>
<connect gate="H" pin="IO_56" pad="AH14"/>
<connect gate="H" pin="IO_57" pad="AH15"/>
<connect gate="H" pin="IO_58" pad="AH16"/>
<connect gate="H" pin="IO_59" pad="AF13"/>
<connect gate="H" pin="IO_6" pad="AD16"/>
<connect gate="H" pin="IO_60" pad="AH17"/>
<connect gate="H" pin="IO_61" pad="AF14"/>
<connect gate="H" pin="IO_62" pad="AH18"/>
<connect gate="H" pin="IO_63" pad="AF15"/>
<connect gate="H" pin="IO_64" pad="AH19"/>
<connect gate="H" pin="IO_65" pad="AF17"/>
<connect gate="H" pin="IO_66" pad="AH20"/>
<connect gate="H" pin="IO_67" pad="AF18"/>
<connect gate="H" pin="IO_68" pad="AH21"/>
<connect gate="H" pin="IO_69" pad="AF19"/>
<connect gate="H" pin="IO_7" pad="AD20"/>
<connect gate="H" pin="IO_70" pad="AE16"/>
<connect gate="H" pin="IO_71" pad="AH22"/>
<connect gate="H" pin="IO_72" pad="AF16"/>
<connect gate="H" pin="IO_73" pad="AF20"/>
<connect gate="H" pin="IO_74" pad="AH23"/>
<connect gate="H" pin="IO_75" pad="AH24"/>
<connect gate="H" pin="IO_76" pad="AH25"/>
<connect gate="H" pin="IO_8" pad="AD25"/>
<connect gate="H" pin="IO_9" pad="AD26"/>
<connect gate="H" pin="VREFB1N0" pad="AD23"/>
<connect gate="H" pin="VREFB8N0" pad="AD22"/>
<connect gate="H" pin="VREFB8N1" pad="AD19"/>
<connect gate="H" pin="VREFB8N2" pad="AD17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2SGX60DF780C5N"/>
<attribute name="OC_FARNELL" value="1549493"/>
<attribute name="OC_NEWARK" value="52R0647"/>
<attribute name="PACKAGE" value="BGA-780"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2SGX60EF1152C5N">
<description>FPGA, STRATIX IIGX</description>
<gates>
<gate name="A" symbol="EP2SGX60EF1152C5N_A"/>
<gate name="B" symbol="EP2SGX60EF1152C5N_B"/>
<gate name="C" symbol="EP2SGX60EF1152C5N_C"/>
<gate name="D" symbol="EP2SGX60EF1152C5N_D"/>
<gate name="E" symbol="EP2SGX60EF1152C5N_E"/>
<gate name="F" symbol="EP2SGX60EF1152C5N_F"/>
<gate name="G" symbol="EP2SGX60EF1152C5N_G"/>
<gate name="H" symbol="EP2SGX60EF1152C5N_H"/>
<gate name="I" symbol="EP2SGX60EF1152C5N_I"/>
<gate name="J" symbol="EP2SGX60EF1152C5N_J"/>
<gate name="K" symbol="EP2SGX60EF1152C5N_K"/>
<gate name="L" symbol="EP2SGX60EF1152C5N_L"/>
</gates>
<devices>
<device name="" package="BGA1152C100P34X34_3500X3500X35">
<connects>
<connect gate="A" pin="GND" pad="K9"/>
<connect gate="A" pin="GND_10" pad="B6"/>
<connect gate="A" pin="GND_11" pad="E9"/>
<connect gate="A" pin="GND_12" pad="B7"/>
<connect gate="A" pin="GND_13" pad="F1"/>
<connect gate="A" pin="GND_14" pad="D1"/>
<connect gate="A" pin="GND_15" pad="F2"/>
<connect gate="A" pin="GND_16" pad="C3"/>
<connect gate="A" pin="GND_17" pad="G3"/>
<connect gate="A" pin="GND_18" pad="G5"/>
<connect gate="A" pin="GND_19" pad="F3"/>
<connect gate="A" pin="GND_2" pad="B1"/>
<connect gate="A" pin="GND_20" pad="D2"/>
<connect gate="A" pin="GND_21" pad="G6"/>
<connect gate="A" pin="GND_22" pad="H1"/>
<connect gate="A" pin="GND_23" pad="F4"/>
<connect gate="A" pin="GND_24" pad="H2"/>
<connect gate="A" pin="GND_25" pad="C6"/>
<connect gate="A" pin="GND_26" pad="E6"/>
<connect gate="A" pin="GND_27" pad="H3"/>
<connect gate="A" pin="GND_28" pad="F5"/>
<connect gate="A" pin="GND_29" pad="K1"/>
<connect gate="A" pin="GND_3" pad="B2"/>
<connect gate="A" pin="GND_30" pad="H4"/>
<connect gate="A" pin="GND_31" pad="K2"/>
<connect gate="A" pin="GND_32" pad="E3"/>
<connect gate="A" pin="GND_33" pad="K3"/>
<connect gate="A" pin="GND_34" pad="H5"/>
<connect gate="A" pin="GND_35" pad="H9"/>
<connect gate="A" pin="GND_36" pad="J3"/>
<connect gate="A" pin="GND_37" pad="K4"/>
<connect gate="A" pin="GND_38" pad="B9"/>
<connect gate="A" pin="GND_39" pad="F6"/>
<connect gate="A" pin="GND_4" pad="B3"/>
<connect gate="A" pin="GND_40" pad="J6"/>
<connect gate="A" pin="GND_41" pad="K5"/>
<connect gate="A" pin="GND_42" pad="E7"/>
<connect gate="A" pin="GND_43" pad="H6"/>
<connect gate="A" pin="GND_44" pad="D3"/>
<connect gate="A" pin="GND_45" pad="K6"/>
<connect gate="A" pin="GND_46" pad="D4"/>
<connect gate="A" pin="GND_47" pad="H7"/>
<connect gate="A" pin="GND_48" pad="L3"/>
<connect gate="A" pin="GND_49" pad="K7"/>
<connect gate="A" pin="GND_5" pad="B4"/>
<connect gate="A" pin="GND_50" pad="D5"/>
<connect gate="A" pin="GND_51" pad="K8"/>
<connect gate="A" pin="GND_52" pad="L6"/>
<connect gate="A" pin="GND_53" pad="D6"/>
<connect gate="A" pin="GND_6" pad="A2"/>
<connect gate="A" pin="GND_7" pad="B5"/>
<connect gate="A" pin="GND_8" pad="A3"/>
<connect gate="A" pin="GND_9" pad="A6"/>
<connect gate="A" pin="GXB_RX0N" pad="E2"/>
<connect gate="A" pin="GXB_RX0P" pad="E1"/>
<connect gate="A" pin="GXB_RX1N" pad="C2"/>
<connect gate="A" pin="GXB_RX1P" pad="C1"/>
<connect gate="A" pin="GXB_RX2N" pad="J2"/>
<connect gate="A" pin="GXB_RX2P" pad="J1"/>
<connect gate="A" pin="GXB_RX3N" pad="L2"/>
<connect gate="A" pin="GXB_RX3P" pad="L1"/>
<connect gate="A" pin="GXB_TX0N" pad="C5"/>
<connect gate="A" pin="GXB_TX0P" pad="C4"/>
<connect gate="A" pin="GXB_TX1N" pad="A5"/>
<connect gate="A" pin="GXB_TX1P" pad="A4"/>
<connect gate="A" pin="GXB_TX2N" pad="J5"/>
<connect gate="A" pin="GXB_TX2P" pad="J4"/>
<connect gate="A" pin="GXB_TX3N" pad="L5"/>
<connect gate="A" pin="GXB_TX3P" pad="L4"/>
<connect gate="A" pin="IO" pad="H8"/>
<connect gate="A" pin="IO_10" pad="D7"/>
<connect gate="A" pin="IO_11" pad="D8"/>
<connect gate="A" pin="IO_12" pad="D9"/>
<connect gate="A" pin="IO_13" pad="F7"/>
<connect gate="A" pin="IO_14" pad="F8"/>
<connect gate="A" pin="IO_15" pad="F9"/>
<connect gate="A" pin="IO_16" pad="G7"/>
<connect gate="A" pin="IO_17" pad="G8"/>
<connect gate="A" pin="IO_18" pad="G9"/>
<connect gate="A" pin="IO_2" pad="C7"/>
<connect gate="A" pin="IO_3" pad="C8"/>
<connect gate="A" pin="IO_4" pad="C9"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_6" pad="A8"/>
<connect gate="A" pin="IO_7" pad="A9"/>
<connect gate="A" pin="IO_8" pad="B8"/>
<connect gate="A" pin="IO_9" pad="E8"/>
<connect gate="A" pin="MSEL1" pad="J9"/>
<connect gate="A" pin="NC" pad="L7"/>
<connect gate="A" pin="REFCLK0_B13N" pad="G2"/>
<connect gate="A" pin="REFCLK0_B13P" pad="G1"/>
<connect gate="A" pin="REFCLK1_B13N" pad="E5"/>
<connect gate="A" pin="REFCLK1_B13P" pad="E4"/>
<connect gate="A" pin="RREFB13" pad="G4"/>
<connect gate="A" pin="TEMPDIODEN" pad="J7"/>
<connect gate="A" pin="TEMPDIODEP" pad="J8"/>
<connect gate="B" pin="GND" pad="P7"/>
<connect gate="B" pin="GND_10" pad="P1"/>
<connect gate="B" pin="GND_11" pad="M4"/>
<connect gate="B" pin="GND_12" pad="T1"/>
<connect gate="B" pin="GND_13" pad="R6"/>
<connect gate="B" pin="GND_14" pad="T2"/>
<connect gate="B" pin="GND_15" pad="P2"/>
<connect gate="B" pin="GND_16" pad="T3"/>
<connect gate="B" pin="GND_17" pad="R7"/>
<connect gate="B" pin="GND_18" pad="T4"/>
<connect gate="B" pin="GND_19" pad="M5"/>
<connect gate="B" pin="GND_2" pad="P9"/>
<connect gate="B" pin="GND_20" pad="T5"/>
<connect gate="B" pin="GND_21" pad="R8"/>
<connect gate="B" pin="GND_22" pad="T6"/>
<connect gate="B" pin="GND_23" pad="P3"/>
<connect gate="B" pin="GND_24" pad="T7"/>
<connect gate="B" pin="GND_25" pad="U1"/>
<connect gate="B" pin="GND_26" pad="M6"/>
<connect gate="B" pin="GND_27" pad="U2"/>
<connect gate="B" pin="GND_28" pad="V5"/>
<connect gate="B" pin="GND_29" pad="V9"/>
<connect gate="B" pin="GND_3" pad="M1"/>
<connect gate="B" pin="GND_30" pad="P4"/>
<connect gate="B" pin="GND_31" pad="W2"/>
<connect gate="B" pin="GND_32" pad="U3"/>
<connect gate="B" pin="GND_33" pad="W1"/>
<connect gate="B" pin="GND_34" pad="V6"/>
<connect gate="B" pin="GND_35" pad="W3"/>
<connect gate="B" pin="GND_36" pad="V7"/>
<connect gate="B" pin="GND_37" pad="Y3"/>
<connect gate="B" pin="GND_38" pad="W4"/>
<connect gate="B" pin="GND_39" pad="Y6"/>
<connect gate="B" pin="GND_4" pad="N6"/>
<connect gate="B" pin="GND_40" pad="M7"/>
<connect gate="B" pin="GND_41" pad="Y7"/>
<connect gate="B" pin="GND_42" pad="W5"/>
<connect gate="B" pin="GND_43" pad="V3"/>
<connect gate="B" pin="GND_44" pad="W6"/>
<connect gate="B" pin="GND_45" pad="U4"/>
<connect gate="B" pin="GND_46" pad="P5"/>
<connect gate="B" pin="GND_47" pad="U5"/>
<connect gate="B" pin="GND_48" pad="P6"/>
<connect gate="B" pin="GND_5" pad="M2"/>
<connect gate="B" pin="GND_6" pad="N7"/>
<connect gate="B" pin="GND_7" pad="R3"/>
<connect gate="B" pin="GND_8" pad="M3"/>
<connect gate="B" pin="GND_9" pad="N3"/>
<connect gate="B" pin="GXB_RX4N" pad="R2"/>
<connect gate="B" pin="GXB_RX4P" pad="R1"/>
<connect gate="B" pin="GXB_RX5N" pad="N2"/>
<connect gate="B" pin="GXB_RX5P" pad="N1"/>
<connect gate="B" pin="GXB_RX6N" pad="Y2"/>
<connect gate="B" pin="GXB_RX6P" pad="Y1"/>
<connect gate="B" pin="GXB_TX4N" pad="R5"/>
<connect gate="B" pin="GXB_TX4P" pad="R4"/>
<connect gate="B" pin="GXB_TX5N" pad="N5"/>
<connect gate="B" pin="GXB_TX5P" pad="N4"/>
<connect gate="B" pin="GXB_TX6N" pad="Y5"/>
<connect gate="B" pin="GXB_TX6P" pad="Y4"/>
<connect gate="B" pin="IO" pad="A22"/>
<connect gate="B" pin="IO_10" pad="A18"/>
<connect gate="B" pin="IO_11" pad="A19"/>
<connect gate="B" pin="IO_12" pad="A20"/>
<connect gate="B" pin="IO_13" pad="A21"/>
<connect gate="B" pin="IO_2" pad="A10"/>
<connect gate="B" pin="IO_3" pad="A11"/>
<connect gate="B" pin="IO_4" pad="A12"/>
<connect gate="B" pin="IO_5" pad="A13"/>
<connect gate="B" pin="IO_6" pad="A14"/>
<connect gate="B" pin="IO_7" pad="A15"/>
<connect gate="B" pin="IO_8" pad="A16"/>
<connect gate="B" pin="IO_9" pad="A17"/>
<connect gate="B" pin="NC" pad="W8"/>
<connect gate="B" pin="NC_2" pad="W7"/>
<connect gate="B" pin="NC_3" pad="L8"/>
<connect gate="B" pin="REFCLK0_B14N" pad="V2"/>
<connect gate="B" pin="REFCLK0_B14P" pad="V1"/>
<connect gate="B" pin="REFCLK1_B14N" pad="U7"/>
<connect gate="B" pin="REFCLK1_B14P" pad="U6"/>
<connect gate="B" pin="RREFB14" pad="V4"/>
<connect gate="B" pin="VCCA" pad="W9"/>
<connect gate="B" pin="VCCA_2" pad="M8"/>
<connect gate="B" pin="VCCA_3" pad="N8"/>
<connect gate="B" pin="VCCA_4" pad="L9"/>
<connect gate="B" pin="VCCA_5" pad="R9"/>
<connect gate="B" pin="VCCA_6" pad="T8"/>
<connect gate="B" pin="VCCA_7" pad="U8"/>
<connect gate="B" pin="VCCA_8" pad="Y8"/>
<connect gate="B" pin="VCCL_B13" pad="P8"/>
<connect gate="B" pin="VCCL_B14" pad="V8"/>
<connect gate="B" pin="VCCR" pad="M9"/>
<connect gate="B" pin="VCCR_2" pad="N9"/>
<connect gate="B" pin="VCCR_3" pad="U9"/>
<connect gate="B" pin="VCCR_4" pad="T9"/>
<connect gate="B" pin="VCCR_5" pad="Y9"/>
<connect gate="C" pin="GND" pad="AJ6"/>
<connect gate="C" pin="GND_10" pad="AA5"/>
<connect gate="C" pin="GND_11" pad="AA6"/>
<connect gate="C" pin="GND_12" pad="AB9"/>
<connect gate="C" pin="GND_13" pad="AA7"/>
<connect gate="C" pin="GND_14" pad="AC1"/>
<connect gate="C" pin="GND_15" pad="AC2"/>
<connect gate="C" pin="GND_16" pad="AC3"/>
<connect gate="C" pin="GND_17" pad="AC4"/>
<connect gate="C" pin="GND_18" pad="AC5"/>
<connect gate="C" pin="GND_19" pad="AC6"/>
<connect gate="C" pin="GND_2" pad="A33"/>
<connect gate="C" pin="GND_20" pad="AC7"/>
<connect gate="C" pin="GND_21" pad="AK3"/>
<connect gate="C" pin="GND_22" pad="AC8"/>
<connect gate="C" pin="GND_23" pad="AD6"/>
<connect gate="C" pin="GND_24" pad="AD3"/>
<connect gate="C" pin="GND_25" pad="AD7"/>
<connect gate="C" pin="GND_26" pad="AD8"/>
<connect gate="C" pin="GND_27" pad="AD9"/>
<connect gate="C" pin="GND_28" pad="AF6"/>
<connect gate="C" pin="GND_29" pad="AE1"/>
<connect gate="C" pin="GND_3" pad="AA1"/>
<connect gate="C" pin="GND_30" pad="AF7"/>
<connect gate="C" pin="GND_31" pad="AE2"/>
<connect gate="C" pin="GND_32" pad="AE3"/>
<connect gate="C" pin="GND_33" pad="AE4"/>
<connect gate="C" pin="GND_34" pad="AF3"/>
<connect gate="C" pin="GND_35" pad="AE5"/>
<connect gate="C" pin="GND_36" pad="AG4"/>
<connect gate="C" pin="GND_37" pad="AE6"/>
<connect gate="C" pin="GND_38" pad="AG5"/>
<connect gate="C" pin="GND_39" pad="AG1"/>
<connect gate="C" pin="GND_4" pad="AA2"/>
<connect gate="C" pin="GND_40" pad="AH3"/>
<connect gate="C" pin="GND_41" pad="AG2"/>
<connect gate="C" pin="GND_42" pad="AG6"/>
<connect gate="C" pin="GND_43" pad="AG3"/>
<connect gate="C" pin="GND_44" pad="AG7"/>
<connect gate="C" pin="GND_45" pad="AG9"/>
<connect gate="C" pin="GND_46" pad="AH5"/>
<connect gate="C" pin="GND_47" pad="AH6"/>
<connect gate="C" pin="GND_48" pad="AJ1"/>
<connect gate="C" pin="GND_49" pad="AJ2"/>
<connect gate="C" pin="GND_5" pad="AA3"/>
<connect gate="C" pin="GND_50" pad="AJ3"/>
<connect gate="C" pin="GND_51" pad="AJ4"/>
<connect gate="C" pin="GND_52" pad="AJ5"/>
<connect gate="C" pin="GND_6" pad="AA4"/>
<connect gate="C" pin="GND_7" pad="AB6"/>
<connect gate="C" pin="GND_8" pad="AB3"/>
<connect gate="C" pin="GND_9" pad="AB7"/>
<connect gate="C" pin="GXB_RX10N" pad="AK2"/>
<connect gate="C" pin="GXB_RX10P" pad="AK1"/>
<connect gate="C" pin="GXB_RX7N" pad="AB2"/>
<connect gate="C" pin="GXB_RX7P" pad="AB1"/>
<connect gate="C" pin="GXB_RX8N" pad="AF2"/>
<connect gate="C" pin="GXB_RX8P" pad="AF1"/>
<connect gate="C" pin="GXB_RX9N" pad="AD2"/>
<connect gate="C" pin="GXB_RX9P" pad="AD1"/>
<connect gate="C" pin="GXB_TX7N" pad="AB5"/>
<connect gate="C" pin="GXB_TX7P" pad="AB4"/>
<connect gate="C" pin="GXB_TX8N" pad="AF5"/>
<connect gate="C" pin="GXB_TX8P" pad="AF4"/>
<connect gate="C" pin="GXB_TX9N" pad="AD5"/>
<connect gate="C" pin="GXB_TX9P" pad="AD4"/>
<connect gate="C" pin="IO" pad="AJ9"/>
<connect gate="C" pin="IO_10" pad="A31"/>
<connect gate="C" pin="IO_11" pad="A32"/>
<connect gate="C" pin="IO_12" pad="AE9"/>
<connect gate="C" pin="IO_13" pad="AG8"/>
<connect gate="C" pin="IO_14" pad="AH7"/>
<connect gate="C" pin="IO_15" pad="AH8"/>
<connect gate="C" pin="IO_16" pad="AH9"/>
<connect gate="C" pin="IO_17" pad="AJ7"/>
<connect gate="C" pin="IO_18" pad="AJ8"/>
<connect gate="C" pin="IO_2" pad="A23"/>
<connect gate="C" pin="IO_3" pad="A24"/>
<connect gate="C" pin="IO_4" pad="A25"/>
<connect gate="C" pin="IO_5" pad="A26"/>
<connect gate="C" pin="IO_6" pad="A27"/>
<connect gate="C" pin="IO_7" pad="A28"/>
<connect gate="C" pin="IO_8" pad="A29"/>
<connect gate="C" pin="IO_9" pad="A30"/>
<connect gate="C" pin="NCEO" pad="AF9"/>
<connect gate="C" pin="NO_PULLUP" pad="AE7"/>
<connect gate="C" pin="PLL_ENA" pad="AF8"/>
<connect gate="C" pin="PORSEL" pad="AE8"/>
<connect gate="C" pin="REFCLK0_B15P" pad="AK4"/>
<connect gate="C" pin="REFCLK1_B15N" pad="AH2"/>
<connect gate="C" pin="REFCLK1_B15P" pad="AH1"/>
<connect gate="C" pin="RREFB15" pad="AH4"/>
<connect gate="C" pin="VCCA" pad="AC9"/>
<connect gate="C" pin="VCCA_2" pad="AA8"/>
<connect gate="C" pin="VCCL_B15" pad="AB8"/>
<connect gate="C" pin="VCCR" pad="AA9"/>
<connect gate="D" pin="DCLK" pad="C32"/>
<connect gate="D" pin="FPLL7CLKN" pad="C33"/>
<connect gate="D" pin="FPLL7CLKP" pad="C34"/>
<connect gate="D" pin="GND" pad="AN7"/>
<connect gate="D" pin="GND_10" pad="AL4"/>
<connect gate="D" pin="GND_11" pad="B15"/>
<connect gate="D" pin="GND_12" pad="AL5"/>
<connect gate="D" pin="GND_13" pad="B18"/>
<connect gate="D" pin="GND_14" pad="AL6"/>
<connect gate="D" pin="GND_15" pad="AP6"/>
<connect gate="D" pin="GND_16" pad="B12"/>
<connect gate="D" pin="GND_17" pad="AN9"/>
<connect gate="D" pin="GND_18" pad="B21"/>
<connect gate="D" pin="GND_19" pad="AP2"/>
<connect gate="D" pin="GND_2" pad="AK6"/>
<connect gate="D" pin="GND_20" pad="B24"/>
<connect gate="D" pin="GND_21" pad="B27"/>
<connect gate="D" pin="GND_22" pad="B30"/>
<connect gate="D" pin="GND_23" pad="AN1"/>
<connect gate="D" pin="GND_24" pad="B33"/>
<connect gate="D" pin="GND_25" pad="AN2"/>
<connect gate="D" pin="GND_26" pad="B34"/>
<connect gate="D" pin="GND_27" pad="AN3"/>
<connect gate="D" pin="GND_28" pad="AN4"/>
<connect gate="D" pin="GND_29" pad="AN5"/>
<connect gate="D" pin="GND_3" pad="AK7"/>
<connect gate="D" pin="GND_30" pad="AN6"/>
<connect gate="D" pin="GND_31" pad="AM6"/>
<connect gate="D" pin="GND_4" pad="AK9"/>
<connect gate="D" pin="GND_5" pad="AL1"/>
<connect gate="D" pin="GND_6" pad="AL2"/>
<connect gate="D" pin="GND_7" pad="AM3"/>
<connect gate="D" pin="GND_8" pad="AL3"/>
<connect gate="D" pin="GND_9" pad="AP3"/>
<connect gate="D" pin="GXB_RX11N" pad="AM2"/>
<connect gate="D" pin="GXB_RX11P" pad="AM1"/>
<connect gate="D" pin="GXB_TX10N" pad="AM5"/>
<connect gate="D" pin="GXB_TX10P" pad="AM4"/>
<connect gate="D" pin="GXB_TX11N" pad="AP5"/>
<connect gate="D" pin="GXB_TX11P" pad="AP4"/>
<connect gate="D" pin="IO" pad="D15"/>
<connect gate="D" pin="IO_10" pad="AN8"/>
<connect gate="D" pin="IO_11" pad="AP8"/>
<connect gate="D" pin="IO_12" pad="B13"/>
<connect gate="D" pin="IO_13" pad="AP9"/>
<connect gate="D" pin="IO_14" pad="B14"/>
<connect gate="D" pin="IO_15" pad="B10"/>
<connect gate="D" pin="IO_16" pad="B11"/>
<connect gate="D" pin="IO_17" pad="B16"/>
<connect gate="D" pin="IO_18" pad="B17"/>
<connect gate="D" pin="IO_19" pad="B19"/>
<connect gate="D" pin="IO_2" pad="AM7"/>
<connect gate="D" pin="IO_20" pad="B20"/>
<connect gate="D" pin="IO_21" pad="B22"/>
<connect gate="D" pin="IO_22" pad="B23"/>
<connect gate="D" pin="IO_23" pad="B25"/>
<connect gate="D" pin="IO_24" pad="B26"/>
<connect gate="D" pin="IO_25" pad="B28"/>
<connect gate="D" pin="IO_26" pad="B29"/>
<connect gate="D" pin="IO_27" pad="B31"/>
<connect gate="D" pin="IO_28" pad="B32"/>
<connect gate="D" pin="IO_29" pad="C10"/>
<connect gate="D" pin="IO_3" pad="AL7"/>
<connect gate="D" pin="IO_30" pad="C11"/>
<connect gate="D" pin="IO_31" pad="C12"/>
<connect gate="D" pin="IO_32" pad="C13"/>
<connect gate="D" pin="IO_33" pad="C14"/>
<connect gate="D" pin="IO_34" pad="C15"/>
<connect gate="D" pin="IO_35" pad="C16"/>
<connect gate="D" pin="IO_36" pad="C17"/>
<connect gate="D" pin="IO_37" pad="C18"/>
<connect gate="D" pin="IO_38" pad="C19"/>
<connect gate="D" pin="IO_39" pad="C20"/>
<connect gate="D" pin="IO_4" pad="AK8"/>
<connect gate="D" pin="IO_40" pad="C21"/>
<connect gate="D" pin="IO_41" pad="C22"/>
<connect gate="D" pin="IO_42" pad="C23"/>
<connect gate="D" pin="IO_43" pad="C24"/>
<connect gate="D" pin="IO_44" pad="C25"/>
<connect gate="D" pin="IO_45" pad="C26"/>
<connect gate="D" pin="IO_46" pad="C27"/>
<connect gate="D" pin="IO_47" pad="C28"/>
<connect gate="D" pin="IO_48" pad="C29"/>
<connect gate="D" pin="IO_49" pad="C30"/>
<connect gate="D" pin="IO_5" pad="AM8"/>
<connect gate="D" pin="IO_50" pad="D10"/>
<connect gate="D" pin="IO_51" pad="D11"/>
<connect gate="D" pin="IO_52" pad="D12"/>
<connect gate="D" pin="IO_53" pad="D13"/>
<connect gate="D" pin="IO_54" pad="D14"/>
<connect gate="D" pin="IO_6" pad="AL8"/>
<connect gate="D" pin="IO_7" pad="AM9"/>
<connect gate="D" pin="IO_8" pad="AL9"/>
<connect gate="D" pin="IO_9" pad="AP7"/>
<connect gate="D" pin="NSTATUS" pad="C31"/>
<connect gate="D" pin="REFCLK0_B15N" pad="AK5"/>
<connect gate="E" pin="CONF_DONE" pad="D31"/>
<connect gate="E" pin="GND" pad="E33"/>
<connect gate="E" pin="GND_2" pad="E18"/>
<connect gate="E" pin="GND_3" pad="E12"/>
<connect gate="E" pin="GND_4" pad="E21"/>
<connect gate="E" pin="GND_5" pad="E27"/>
<connect gate="E" pin="GND_6" pad="E15"/>
<connect gate="E" pin="GND_7" pad="G17"/>
<connect gate="E" pin="GND_8" pad="E24"/>
<connect gate="E" pin="GND_9" pad="E30"/>
<connect gate="E" pin="IO" pad="G34"/>
<connect gate="E" pin="IO_10" pad="D34"/>
<connect gate="E" pin="IO_11" pad="D24"/>
<connect gate="E" pin="IO_12" pad="D25"/>
<connect gate="E" pin="IO_13" pad="E11"/>
<connect gate="E" pin="IO_14" pad="D26"/>
<connect gate="E" pin="IO_15" pad="D27"/>
<connect gate="E" pin="IO_16" pad="D28"/>
<connect gate="E" pin="IO_17" pad="D29"/>
<connect gate="E" pin="IO_18" pad="E19"/>
<connect gate="E" pin="IO_19" pad="E20"/>
<connect gate="E" pin="IO_2" pad="D16"/>
<connect gate="E" pin="IO_20" pad="E14"/>
<connect gate="E" pin="IO_21" pad="E34"/>
<connect gate="E" pin="IO_22" pad="E23"/>
<connect gate="E" pin="IO_23" pad="F10"/>
<connect gate="E" pin="IO_24" pad="F11"/>
<connect gate="E" pin="IO_25" pad="E29"/>
<connect gate="E" pin="IO_26" pad="F12"/>
<connect gate="E" pin="IO_27" pad="E17"/>
<connect gate="E" pin="IO_28" pad="F13"/>
<connect gate="E" pin="IO_29" pad="E26"/>
<connect gate="E" pin="IO_3" pad="D17"/>
<connect gate="E" pin="IO_30" pad="F14"/>
<connect gate="E" pin="IO_31" pad="F15"/>
<connect gate="E" pin="IO_32" pad="F16"/>
<connect gate="E" pin="IO_33" pad="F17"/>
<connect gate="E" pin="IO_34" pad="F18"/>
<connect gate="E" pin="IO_35" pad="F19"/>
<connect gate="E" pin="IO_36" pad="F20"/>
<connect gate="E" pin="IO_37" pad="F21"/>
<connect gate="E" pin="IO_38" pad="F22"/>
<connect gate="E" pin="IO_39" pad="F23"/>
<connect gate="E" pin="IO_4" pad="D18"/>
<connect gate="E" pin="IO_40" pad="F24"/>
<connect gate="E" pin="IO_41" pad="F25"/>
<connect gate="E" pin="IO_42" pad="F26"/>
<connect gate="E" pin="IO_43" pad="F27"/>
<connect gate="E" pin="IO_44" pad="F28"/>
<connect gate="E" pin="IO_45" pad="F29"/>
<connect gate="E" pin="IO_46" pad="F31"/>
<connect gate="E" pin="IO_47" pad="F32"/>
<connect gate="E" pin="IO_48" pad="F33"/>
<connect gate="E" pin="IO_49" pad="F34"/>
<connect gate="E" pin="IO_5" pad="D19"/>
<connect gate="E" pin="IO_50" pad="G10"/>
<connect gate="E" pin="IO_51" pad="G11"/>
<connect gate="E" pin="IO_52" pad="G12"/>
<connect gate="E" pin="IO_53" pad="G13"/>
<connect gate="E" pin="IO_54" pad="G14"/>
<connect gate="E" pin="IO_55" pad="G15"/>
<connect gate="E" pin="IO_56" pad="G16"/>
<connect gate="E" pin="IO_57" pad="G18"/>
<connect gate="E" pin="IO_58" pad="G19"/>
<connect gate="E" pin="IO_59" pad="G20"/>
<connect gate="E" pin="IO_6" pad="D20"/>
<connect gate="E" pin="IO_60" pad="G21"/>
<connect gate="E" pin="IO_61" pad="G22"/>
<connect gate="E" pin="IO_62" pad="G23"/>
<connect gate="E" pin="IO_63" pad="G24"/>
<connect gate="E" pin="IO_64" pad="G25"/>
<connect gate="E" pin="IO_65" pad="G26"/>
<connect gate="E" pin="IO_66" pad="G27"/>
<connect gate="E" pin="IO_67" pad="G28"/>
<connect gate="E" pin="IO_68" pad="G29"/>
<connect gate="E" pin="IO_69" pad="G32"/>
<connect gate="E" pin="IO_7" pad="D21"/>
<connect gate="E" pin="IO_70" pad="G33"/>
<connect gate="E" pin="IO_8" pad="D22"/>
<connect gate="E" pin="IO_9" pad="D23"/>
<connect gate="E" pin="MSEL3" pad="H11"/>
<connect gate="E" pin="NC" pad="G31"/>
<connect gate="E" pin="NCE" pad="D30"/>
<connect gate="E" pin="NC_2" pad="F30"/>
<connect gate="E" pin="NC_3" pad="E31"/>
<connect gate="E" pin="NC_4" pad="D32"/>
<connect gate="E" pin="NC_5" pad="E32"/>
<connect gate="E" pin="NC_6" pad="D33"/>
<connect gate="E" pin="NC_7" pad="G30"/>
<connect gate="E" pin="TDO" pad="H10"/>
<connect gate="E" pin="VREFB3N0" pad="E22"/>
<connect gate="E" pin="VREFB3N1" pad="E25"/>
<connect gate="E" pin="VREFB3N2" pad="E28"/>
<connect gate="E" pin="VREFB4N0" pad="E10"/>
<connect gate="E" pin="VREFB4N1" pad="E13"/>
<connect gate="E" pin="VREFB4N2" pad="E16"/>
<connect gate="F" pin="GND" pad="L18"/>
<connect gate="F" pin="GNDA_PLL11" pad="J18"/>
<connect gate="F" pin="GNDA_PLL11_2" pad="K18"/>
<connect gate="F" pin="GNDA_PLL5" pad="J17"/>
<connect gate="F" pin="GNDA_PLL5_2" pad="J16"/>
<connect gate="F" pin="GNDA_PLL7" pad="J25"/>
<connect gate="F" pin="GNDA_PLL7_2" pad="K26"/>
<connect gate="F" pin="GND_10" pad="H30"/>
<connect gate="F" pin="GND_11" pad="H15"/>
<connect gate="F" pin="GND_12" pad="H24"/>
<connect gate="F" pin="GND_13" pad="H21"/>
<connect gate="F" pin="GND_14" pad="L21"/>
<connect gate="F" pin="GND_15" pad="L24"/>
<connect gate="F" pin="GND_16" pad="L27"/>
<connect gate="F" pin="GND_17" pad="L30"/>
<connect gate="F" pin="GND_2" pad="L10"/>
<connect gate="F" pin="GND_3" pad="L11"/>
<connect gate="F" pin="GND_4" pad="L12"/>
<connect gate="F" pin="GND_5" pad="H18"/>
<connect gate="F" pin="GND_6" pad="L15"/>
<connect gate="F" pin="GND_7" pad="H27"/>
<connect gate="F" pin="GND_8" pad="H12"/>
<connect gate="F" pin="GND_9" pad="H33"/>
<connect gate="F" pin="IO" pad="L32"/>
<connect gate="F" pin="IO_10" pad="J20"/>
<connect gate="F" pin="IO_11" pad="H23"/>
<connect gate="F" pin="IO_12" pad="J11"/>
<connect gate="F" pin="IO_13" pad="J22"/>
<connect gate="F" pin="IO_14" pad="H25"/>
<connect gate="F" pin="IO_15" pad="J13"/>
<connect gate="F" pin="IO_16" pad="J14"/>
<connect gate="F" pin="IO_17" pad="J27"/>
<connect gate="F" pin="IO_18" pad="J23"/>
<connect gate="F" pin="IO_19" pad="J28"/>
<connect gate="F" pin="IO_2" pad="H28"/>
<connect gate="F" pin="IO_20" pad="H26"/>
<connect gate="F" pin="IO_21" pad="J29"/>
<connect gate="F" pin="IO_22" pad="J24"/>
<connect gate="F" pin="IO_23" pad="J30"/>
<connect gate="F" pin="IO_24" pad="J31"/>
<connect gate="F" pin="IO_25" pad="J32"/>
<connect gate="F" pin="IO_26" pad="J33"/>
<connect gate="F" pin="IO_27" pad="J34"/>
<connect gate="F" pin="IO_28" pad="K11"/>
<connect gate="F" pin="IO_29" pad="K13"/>
<connect gate="F" pin="IO_3" pad="H20"/>
<connect gate="F" pin="IO_30" pad="K14"/>
<connect gate="F" pin="IO_31" pad="K23"/>
<connect gate="F" pin="IO_32" pad="K24"/>
<connect gate="F" pin="IO_33" pad="K27"/>
<connect gate="F" pin="IO_34" pad="K28"/>
<connect gate="F" pin="IO_35" pad="K29"/>
<connect gate="F" pin="IO_36" pad="K30"/>
<connect gate="F" pin="IO_37" pad="K32"/>
<connect gate="F" pin="IO_38" pad="K33"/>
<connect gate="F" pin="IO_39" pad="K34"/>
<connect gate="F" pin="IO_4" pad="H13"/>
<connect gate="F" pin="IO_40" pad="L13"/>
<connect gate="F" pin="IO_41" pad="L14"/>
<connect gate="F" pin="IO_42" pad="L22"/>
<connect gate="F" pin="IO_43" pad="L23"/>
<connect gate="F" pin="IO_44" pad="L25"/>
<connect gate="F" pin="IO_45" pad="L26"/>
<connect gate="F" pin="IO_46" pad="L28"/>
<connect gate="F" pin="IO_47" pad="L29"/>
<connect gate="F" pin="IO_48" pad="L31"/>
<connect gate="F" pin="IO_5" pad="H31"/>
<connect gate="F" pin="IO_6" pad="H32"/>
<connect gate="F" pin="IO_7" pad="H14"/>
<connect gate="F" pin="IO_8" pad="H22"/>
<connect gate="F" pin="IO_9" pad="H34"/>
<connect gate="F" pin="MSEL0" pad="K10"/>
<connect gate="F" pin="MSEL2" pad="J10"/>
<connect gate="F" pin="NC" pad="K22"/>
<connect gate="F" pin="NC_2" pad="H29"/>
<connect gate="F" pin="VCCA_PLL11" pad="K17"/>
<connect gate="F" pin="VCCA_PLL5" pad="K16"/>
<connect gate="F" pin="VCCA_PLL7" pad="J26"/>
<connect gate="F" pin="VCCD_PLL11" pad="J19"/>
<connect gate="F" pin="VCCD_PLL5" pad="H17"/>
<connect gate="F" pin="VCCD_PLL7" pad="K25"/>
<connect gate="F" pin="VCCIO3" pad="K21"/>
<connect gate="F" pin="VCCIO3_2" pad="J21"/>
<connect gate="F" pin="VCCIO3_3" pad="H19"/>
<connect gate="F" pin="VCCIO3_4" pad="K19"/>
<connect gate="F" pin="VCCIO4" pad="J15"/>
<connect gate="F" pin="VCCIO4_2" pad="K12"/>
<connect gate="F" pin="VCCIO4_3" pad="J12"/>
<connect gate="F" pin="VCCIO4_4" pad="K15"/>
<connect gate="F" pin="VCCPD3" pad="L20"/>
<connect gate="F" pin="VCCPD3_2" pad="L19"/>
<connect gate="F" pin="VCCPD4" pad="L17"/>
<connect gate="F" pin="VCCPD4_2" pad="L16"/>
<connect gate="F" pin="VCC_PLL11_OUT" pad="K20"/>
<connect gate="F" pin="VCC_PLL5_OUT" pad="H16"/>
<connect gate="F" pin="VREFB2N2" pad="K31"/>
<connect gate="G" pin="GND" pad="R14"/>
<connect gate="G" pin="GNDA_PLL1" pad="R26"/>
<connect gate="G" pin="GND_10" pad="N16"/>
<connect gate="G" pin="GND_11" pad="P22"/>
<connect gate="G" pin="GND_12" pad="P10"/>
<connect gate="G" pin="GND_13" pad="P24"/>
<connect gate="G" pin="GND_14" pad="P11"/>
<connect gate="G" pin="GND_15" pad="P12"/>
<connect gate="G" pin="GND_16" pad="P13"/>
<connect gate="G" pin="GND_17" pad="R12"/>
<connect gate="G" pin="GND_18" pad="P30"/>
<connect gate="G" pin="GND_19" pad="R20"/>
<connect gate="G" pin="GND_2" pad="P15"/>
<connect gate="G" pin="GND_20" pad="L33"/>
<connect gate="G" pin="GND_21" pad="R16"/>
<connect gate="G" pin="GND_22" pad="P27"/>
<connect gate="G" pin="GND_23" pad="R22"/>
<connect gate="G" pin="GND_24" pad="P33"/>
<connect gate="G" pin="GND_25" pad="R18"/>
<connect gate="G" pin="GND_26" pad="R10"/>
<connect gate="G" pin="GND_3" pad="P17"/>
<connect gate="G" pin="GND_4" pad="N13"/>
<connect gate="G" pin="GND_5" pad="N14"/>
<connect gate="G" pin="GND_6" pad="P19"/>
<connect gate="G" pin="GND_7" pad="N20"/>
<connect gate="G" pin="GND_8" pad="N15"/>
<connect gate="G" pin="GND_9" pad="P21"/>
<connect gate="G" pin="IO" pad="R28"/>
<connect gate="G" pin="IO_10" pad="M19"/>
<connect gate="G" pin="IO_11" pad="M20"/>
<connect gate="G" pin="IO_12" pad="M34"/>
<connect gate="G" pin="IO_13" pad="N23"/>
<connect gate="G" pin="IO_14" pad="M21"/>
<connect gate="G" pin="IO_15" pad="N24"/>
<connect gate="G" pin="IO_16" pad="L34"/>
<connect gate="G" pin="IO_17" pad="N25"/>
<connect gate="G" pin="IO_18" pad="M22"/>
<connect gate="G" pin="IO_19" pad="N26"/>
<connect gate="G" pin="IO_2" pad="M31"/>
<connect gate="G" pin="IO_20" pad="M23"/>
<connect gate="G" pin="IO_21" pad="N17"/>
<connect gate="G" pin="IO_22" pad="N27"/>
<connect gate="G" pin="IO_23" pad="M24"/>
<connect gate="G" pin="IO_24" pad="N18"/>
<connect gate="G" pin="IO_25" pad="N28"/>
<connect gate="G" pin="IO_26" pad="M25"/>
<connect gate="G" pin="IO_27" pad="N29"/>
<connect gate="G" pin="IO_28" pad="M26"/>
<connect gate="G" pin="IO_29" pad="N21"/>
<connect gate="G" pin="IO_3" pad="M32"/>
<connect gate="G" pin="IO_30" pad="N30"/>
<connect gate="G" pin="IO_31" pad="M27"/>
<connect gate="G" pin="IO_32" pad="M28"/>
<connect gate="G" pin="IO_33" pad="M29"/>
<connect gate="G" pin="IO_34" pad="N31"/>
<connect gate="G" pin="IO_35" pad="N32"/>
<connect gate="G" pin="IO_36" pad="N33"/>
<connect gate="G" pin="IO_37" pad="N34"/>
<connect gate="G" pin="IO_38" pad="P23"/>
<connect gate="G" pin="IO_39" pad="P28"/>
<connect gate="G" pin="IO_4" pad="M14"/>
<connect gate="G" pin="IO_40" pad="P29"/>
<connect gate="G" pin="IO_41" pad="P31"/>
<connect gate="G" pin="IO_42" pad="P32"/>
<connect gate="G" pin="IO_43" pad="P34"/>
<connect gate="G" pin="IO_44" pad="R23"/>
<connect gate="G" pin="IO_5" pad="M33"/>
<connect gate="G" pin="IO_6" pad="M15"/>
<connect gate="G" pin="IO_7" pad="M16"/>
<connect gate="G" pin="IO_8" pad="M17"/>
<connect gate="G" pin="IO_9" pad="M18"/>
<connect gate="G" pin="NC" pad="N22"/>
<connect gate="G" pin="NC_2" pad="N19"/>
<connect gate="G" pin="NC_3" pad="M13"/>
<connect gate="G" pin="VCCA" pad="R11"/>
<connect gate="G" pin="VCCD_PLL1" pad="R27"/>
<connect gate="G" pin="VCCH_B13" pad="N11"/>
<connect gate="G" pin="VCCH_B13_2" pad="M11"/>
<connect gate="G" pin="VCCINT" pad="R21"/>
<connect gate="G" pin="VCCINT_2" pad="R17"/>
<connect gate="G" pin="VCCINT_3" pad="P14"/>
<connect gate="G" pin="VCCINT_4" pad="R13"/>
<connect gate="G" pin="VCCINT_5" pad="P16"/>
<connect gate="G" pin="VCCINT_6" pad="R15"/>
<connect gate="G" pin="VCCINT_7" pad="P20"/>
<connect gate="G" pin="VCCINT_8" pad="R19"/>
<connect gate="G" pin="VCCINT_9" pad="P18"/>
<connect gate="G" pin="VCCIO2" pad="P26"/>
<connect gate="G" pin="VCCIO2_2" pad="P25"/>
<connect gate="G" pin="VCCP" pad="N12"/>
<connect gate="G" pin="VCCPD2" pad="R25"/>
<connect gate="G" pin="VCCPD2_2" pad="R24"/>
<connect gate="G" pin="VCCP_2" pad="M12"/>
<connect gate="G" pin="VCCT_B13" pad="M10"/>
<connect gate="G" pin="VCCT_B13_2" pad="N10"/>
<connect gate="G" pin="VREFB2N1" pad="M30"/>
<connect gate="H" pin="CLK1N" pad="U32"/>
<connect gate="H" pin="CLK1P" pad="U33"/>
<connect gate="H" pin="CLK3N" pad="V31"/>
<connect gate="H" pin="CLK3P" pad="V32"/>
<connect gate="H" pin="GND" pad="W22"/>
<connect gate="H" pin="GNDA_PLL1" pad="T26"/>
<connect gate="H" pin="GNDA_PLL2" pad="V26"/>
<connect gate="H" pin="GND_10" pad="T33"/>
<connect gate="H" pin="GND_11" pad="U22"/>
<connect gate="H" pin="GND_12" pad="T21"/>
<connect gate="H" pin="GND_13" pad="T30"/>
<connect gate="H" pin="GND_14" pad="T27"/>
<connect gate="H" pin="GND_15" pad="T24"/>
<connect gate="H" pin="GND_16" pad="V10"/>
<connect gate="H" pin="GND_17" pad="V11"/>
<connect gate="H" pin="GND_18" pad="V12"/>
<connect gate="H" pin="GND_19" pad="V13"/>
<connect gate="H" pin="GND_2" pad="U18"/>
<connect gate="H" pin="GND_20" pad="V19"/>
<connect gate="H" pin="GND_21" pad="V15"/>
<connect gate="H" pin="GND_22" pad="W18"/>
<connect gate="H" pin="GND_23" pad="V27"/>
<connect gate="H" pin="GND_24" pad="V17"/>
<connect gate="H" pin="GND_25" pad="V21"/>
<connect gate="H" pin="GND_26" pad="V30"/>
<connect gate="H" pin="GND_27" pad="V33"/>
<connect gate="H" pin="GND_28" pad="W14"/>
<connect gate="H" pin="GND_29" pad="V22"/>
<connect gate="H" pin="GND_3" pad="T13"/>
<connect gate="H" pin="GND_30" pad="W20"/>
<connect gate="H" pin="GND_31" pad="V24"/>
<connect gate="H" pin="GND_32" pad="W10"/>
<connect gate="H" pin="GND_33" pad="W16"/>
<connect gate="H" pin="GND_4" pad="T15"/>
<connect gate="H" pin="GND_5" pad="U20"/>
<connect gate="H" pin="GND_6" pad="U16"/>
<connect gate="H" pin="GND_7" pad="T17"/>
<connect gate="H" pin="GND_8" pad="U14"/>
<connect gate="H" pin="GND_9" pad="T19"/>
<connect gate="H" pin="IO" pad="W23"/>
<connect gate="H" pin="IO_10" pad="R32"/>
<connect gate="H" pin="IO_11" pad="T32"/>
<connect gate="H" pin="IO_12" pad="R33"/>
<connect gate="H" pin="IO_13" pad="R34"/>
<connect gate="H" pin="IO_14" pad="T34"/>
<connect gate="H" pin="IO_15" pad="U27"/>
<connect gate="H" pin="IO_16" pad="U28"/>
<connect gate="H" pin="IO_17" pad="U29"/>
<connect gate="H" pin="IO_18" pad="U30"/>
<connect gate="H" pin="IO_19" pad="U31"/>
<connect gate="H" pin="IO_2" pad="T28"/>
<connect gate="H" pin="IO_20" pad="U34"/>
<connect gate="H" pin="IO_21" pad="V23"/>
<connect gate="H" pin="IO_22" pad="V28"/>
<connect gate="H" pin="IO_23" pad="V29"/>
<connect gate="H" pin="IO_24" pad="V34"/>
<connect gate="H" pin="IO_3" pad="T23"/>
<connect gate="H" pin="IO_4" pad="R29"/>
<connect gate="H" pin="IO_5" pad="T29"/>
<connect gate="H" pin="IO_6" pad="U23"/>
<connect gate="H" pin="IO_7" pad="U24"/>
<connect gate="H" pin="IO_8" pad="R31"/>
<connect gate="H" pin="IO_9" pad="T31"/>
<connect gate="H" pin="VCCA" pad="W12"/>
<connect gate="H" pin="VCCA_2" pad="W11"/>
<connect gate="H" pin="VCCA_PLL1" pad="T25"/>
<connect gate="H" pin="VCCA_PLL2" pad="V25"/>
<connect gate="H" pin="VCCH_B14" pad="U11"/>
<connect gate="H" pin="VCCH_B14_2" pad="T11"/>
<connect gate="H" pin="VCCINT" pad="U17"/>
<connect gate="H" pin="VCCINT_10" pad="U15"/>
<connect gate="H" pin="VCCINT_11" pad="W13"/>
<connect gate="H" pin="VCCINT_12" pad="U19"/>
<connect gate="H" pin="VCCINT_13" pad="W21"/>
<connect gate="H" pin="VCCINT_14" pad="T20"/>
<connect gate="H" pin="VCCINT_15" pad="V14"/>
<connect gate="H" pin="VCCINT_16" pad="T22"/>
<connect gate="H" pin="VCCINT_17" pad="W15"/>
<connect gate="H" pin="VCCINT_18" pad="U21"/>
<connect gate="H" pin="VCCINT_19" pad="V16"/>
<connect gate="H" pin="VCCINT_2" pad="T14"/>
<connect gate="H" pin="VCCINT_3" pad="V20"/>
<connect gate="H" pin="VCCINT_4" pad="U13"/>
<connect gate="H" pin="VCCINT_5" pad="W17"/>
<connect gate="H" pin="VCCINT_6" pad="T16"/>
<connect gate="H" pin="VCCINT_7" pad="V18"/>
<connect gate="H" pin="VCCINT_8" pad="T18"/>
<connect gate="H" pin="VCCINT_9" pad="W19"/>
<connect gate="H" pin="VCCIO2" pad="U26"/>
<connect gate="H" pin="VCCIO2_2" pad="U25"/>
<connect gate="H" pin="VCCP" pad="T12"/>
<connect gate="H" pin="VCCPD1" pad="W24"/>
<connect gate="H" pin="VCCP_2" pad="U12"/>
<connect gate="H" pin="VCCT_B14" pad="U10"/>
<connect gate="H" pin="VCCT_B14_2" pad="T10"/>
<connect gate="H" pin="VREFB2N0" pad="R30"/>
<connect gate="I" pin="GND" pad="AC12"/>
<connect gate="I" pin="GNDA_PLL2" pad="W26"/>
<connect gate="I" pin="GND_10" pad="AA27"/>
<connect gate="I" pin="GND_11" pad="Y21"/>
<connect gate="I" pin="GND_12" pad="AA30"/>
<connect gate="I" pin="GND_13" pad="AA18"/>
<connect gate="I" pin="GND_14" pad="AA33"/>
<connect gate="I" pin="GND_15" pad="AB10"/>
<connect gate="I" pin="GND_16" pad="AA20"/>
<connect gate="I" pin="GND_17" pad="AB11"/>
<connect gate="I" pin="GND_18" pad="AB12"/>
<connect gate="I" pin="GND_19" pad="AB13"/>
<connect gate="I" pin="GND_2" pad="AA14"/>
<connect gate="I" pin="GND_20" pad="AB14"/>
<connect gate="I" pin="GND_21" pad="AB15"/>
<connect gate="I" pin="GND_22" pad="AC10"/>
<connect gate="I" pin="GND_23" pad="AB19"/>
<connect gate="I" pin="GND_3" pad="Y15"/>
<connect gate="I" pin="GND_4" pad="AA22"/>
<connect gate="I" pin="GND_5" pad="Y19"/>
<connect gate="I" pin="GND_6" pad="AA24"/>
<connect gate="I" pin="GND_7" pad="Y13"/>
<connect gate="I" pin="GND_8" pad="AA16"/>
<connect gate="I" pin="GND_9" pad="Y17"/>
<connect gate="I" pin="IO" pad="AC20"/>
<connect gate="I" pin="IO_10" pad="W32"/>
<connect gate="I" pin="IO_11" pad="Y34"/>
<connect gate="I" pin="IO_12" pad="W33"/>
<connect gate="I" pin="IO_13" pad="Y24"/>
<connect gate="I" pin="IO_14" pad="W34"/>
<connect gate="I" pin="IO_15" pad="Y27"/>
<connect gate="I" pin="IO_16" pad="Y28"/>
<connect gate="I" pin="IO_17" pad="Y29"/>
<connect gate="I" pin="IO_18" pad="AA23"/>
<connect gate="I" pin="IO_19" pad="AA25"/>
<connect gate="I" pin="IO_2" pad="W28"/>
<connect gate="I" pin="IO_20" pad="AA26"/>
<connect gate="I" pin="IO_21" pad="AA28"/>
<connect gate="I" pin="IO_22" pad="AA29"/>
<connect gate="I" pin="IO_23" pad="AA31"/>
<connect gate="I" pin="IO_24" pad="AA32"/>
<connect gate="I" pin="IO_25" pad="AA34"/>
<connect gate="I" pin="IO_26" pad="AB18"/>
<connect gate="I" pin="IO_27" pad="AB20"/>
<connect gate="I" pin="IO_28" pad="AB21"/>
<connect gate="I" pin="IO_29" pad="AB23"/>
<connect gate="I" pin="IO_3" pad="Y31"/>
<connect gate="I" pin="IO_30" pad="AB24"/>
<connect gate="I" pin="IO_31" pad="AB25"/>
<connect gate="I" pin="IO_32" pad="AB26"/>
<connect gate="I" pin="IO_33" pad="AB27"/>
<connect gate="I" pin="IO_34" pad="AB28"/>
<connect gate="I" pin="IO_35" pad="AB29"/>
<connect gate="I" pin="IO_36" pad="AB30"/>
<connect gate="I" pin="IO_37" pad="AB31"/>
<connect gate="I" pin="IO_38" pad="AB32"/>
<connect gate="I" pin="IO_39" pad="AB33"/>
<connect gate="I" pin="IO_4" pad="W29"/>
<connect gate="I" pin="IO_40" pad="AB34"/>
<connect gate="I" pin="IO_41" pad="AC13"/>
<connect gate="I" pin="IO_42" pad="AC14"/>
<connect gate="I" pin="IO_43" pad="AC15"/>
<connect gate="I" pin="IO_44" pad="AC16"/>
<connect gate="I" pin="IO_45" pad="AC18"/>
<connect gate="I" pin="IO_46" pad="AC19"/>
<connect gate="I" pin="IO_5" pad="Y32"/>
<connect gate="I" pin="IO_6" pad="W30"/>
<connect gate="I" pin="IO_7" pad="Y33"/>
<connect gate="I" pin="IO_8" pad="W31"/>
<connect gate="I" pin="IO_9" pad="Y23"/>
<connect gate="I" pin="NC" pad="AB22"/>
<connect gate="I" pin="NC_2" pad="AB16"/>
<connect gate="I" pin="NC_3" pad="AB17"/>
<connect gate="I" pin="NC_4" pad="AC17"/>
<connect gate="I" pin="VCCA" pad="AC11"/>
<connect gate="I" pin="VCCD_PLL2" pad="W27"/>
<connect gate="I" pin="VCCH_B15" pad="AA11"/>
<connect gate="I" pin="VCCH_B15_2" pad="Y11"/>
<connect gate="I" pin="VCCINT" pad="AA21"/>
<connect gate="I" pin="VCCINT_10" pad="AA19"/>
<connect gate="I" pin="VCCINT_2" pad="Y14"/>
<connect gate="I" pin="VCCINT_3" pad="AA13"/>
<connect gate="I" pin="VCCINT_4" pad="Y16"/>
<connect gate="I" pin="VCCINT_5" pad="Y20"/>
<connect gate="I" pin="VCCINT_6" pad="Y18"/>
<connect gate="I" pin="VCCINT_7" pad="Y22"/>
<connect gate="I" pin="VCCINT_8" pad="AA15"/>
<connect gate="I" pin="VCCINT_9" pad="AA17"/>
<connect gate="I" pin="VCCIO1" pad="Y26"/>
<connect gate="I" pin="VCCIO1_2" pad="Y25"/>
<connect gate="I" pin="VCCP" pad="AA12"/>
<connect gate="I" pin="VCCPD1" pad="W25"/>
<connect gate="I" pin="VCCP_2" pad="Y12"/>
<connect gate="I" pin="VCCT_B15" pad="AA10"/>
<connect gate="I" pin="VCCT_B15_2" pad="Y10"/>
<connect gate="I" pin="VREFB1N2" pad="Y30"/>
<connect gate="J" pin="GND" pad="AD33"/>
<connect gate="J" pin="GNDA_PLL12" pad="AF19"/>
<connect gate="J" pin="GNDA_PLL12_2" pad="AF18"/>
<connect gate="J" pin="GNDA_PLL6" pad="AE17"/>
<connect gate="J" pin="GNDA_PLL6_2" pad="AF17"/>
<connect gate="J" pin="GNDA_PLL8" pad="AF25"/>
<connect gate="J" pin="GNDA_PLL8_2" pad="AE26"/>
<connect gate="J" pin="GND_10" pad="AD11"/>
<connect gate="J" pin="GND_11" pad="AD24"/>
<connect gate="J" pin="GND_12" pad="AD12"/>
<connect gate="J" pin="GND_2" pad="AD27"/>
<connect gate="J" pin="GND_3" pad="AD21"/>
<connect gate="J" pin="GND_4" pad="AD15"/>
<connect gate="J" pin="GND_5" pad="AG12"/>
<connect gate="J" pin="GND_6" pad="AD18"/>
<connect gate="J" pin="GND_7" pad="AG15"/>
<connect gate="J" pin="GND_8" pad="AD10"/>
<connect gate="J" pin="GND_9" pad="AD30"/>
<connect gate="J" pin="IO" pad="AG14"/>
<connect gate="J" pin="IO_10" pad="AD22"/>
<connect gate="J" pin="IO_11" pad="AC32"/>
<connect gate="J" pin="IO_12" pad="AD28"/>
<connect gate="J" pin="IO_13" pad="AD25"/>
<connect gate="J" pin="IO_14" pad="AD34"/>
<connect gate="J" pin="IO_15" pad="AD29"/>
<connect gate="J" pin="IO_16" pad="AE10"/>
<connect gate="J" pin="IO_17" pad="AD23"/>
<connect gate="J" pin="IO_18" pad="AE11"/>
<connect gate="J" pin="IO_19" pad="AD26"/>
<connect gate="J" pin="IO_2" pad="AC21"/>
<connect gate="J" pin="IO_20" pad="AD31"/>
<connect gate="J" pin="IO_21" pad="AE13"/>
<connect gate="J" pin="IO_22" pad="AC33"/>
<connect gate="J" pin="IO_23" pad="AE14"/>
<connect gate="J" pin="IO_24" pad="AD32"/>
<connect gate="J" pin="IO_25" pad="AC34"/>
<connect gate="J" pin="IO_26" pad="AD13"/>
<connect gate="J" pin="IO_27" pad="AD14"/>
<connect gate="J" pin="IO_28" pad="AE22"/>
<connect gate="J" pin="IO_29" pad="AE23"/>
<connect gate="J" pin="IO_3" pad="AC22"/>
<connect gate="J" pin="IO_30" pad="AE27"/>
<connect gate="J" pin="IO_31" pad="AE28"/>
<connect gate="J" pin="IO_32" pad="AE29"/>
<connect gate="J" pin="IO_33" pad="AE30"/>
<connect gate="J" pin="IO_34" pad="AE32"/>
<connect gate="J" pin="IO_35" pad="AE33"/>
<connect gate="J" pin="IO_36" pad="AE34"/>
<connect gate="J" pin="IO_37" pad="AF10"/>
<connect gate="J" pin="IO_38" pad="AF11"/>
<connect gate="J" pin="IO_39" pad="AF13"/>
<connect gate="J" pin="IO_4" pad="AC23"/>
<connect gate="J" pin="IO_40" pad="AF14"/>
<connect gate="J" pin="IO_41" pad="AF22"/>
<connect gate="J" pin="IO_42" pad="AF23"/>
<connect gate="J" pin="IO_43" pad="AF27"/>
<connect gate="J" pin="IO_44" pad="AF28"/>
<connect gate="J" pin="IO_45" pad="AF29"/>
<connect gate="J" pin="IO_46" pad="AF30"/>
<connect gate="J" pin="IO_47" pad="AF31"/>
<connect gate="J" pin="IO_48" pad="AF32"/>
<connect gate="J" pin="IO_49" pad="AF33"/>
<connect gate="J" pin="IO_5" pad="AC24"/>
<connect gate="J" pin="IO_50" pad="AF34"/>
<connect gate="J" pin="IO_51" pad="AG10"/>
<connect gate="J" pin="IO_52" pad="AG11"/>
<connect gate="J" pin="IO_53" pad="AG13"/>
<connect gate="J" pin="IO_6" pad="AC27"/>
<connect gate="J" pin="IO_7" pad="AC28"/>
<connect gate="J" pin="IO_8" pad="AC29"/>
<connect gate="J" pin="IO_9" pad="AC31"/>
<connect gate="J" pin="NCONFIG" pad="AE24"/>
<connect gate="J" pin="VCCA_PLL12" pad="AE18"/>
<connect gate="J" pin="VCCA_PLL6" pad="AE16"/>
<connect gate="J" pin="VCCA_PLL8" pad="AF26"/>
<connect gate="J" pin="VCCD_PLL12" pad="AF20"/>
<connect gate="J" pin="VCCD_PLL6" pad="AF16"/>
<connect gate="J" pin="VCCD_PLL8" pad="AE25"/>
<connect gate="J" pin="VCCIO1" pad="AC26"/>
<connect gate="J" pin="VCCIO1_2" pad="AC25"/>
<connect gate="J" pin="VCCIO7" pad="AE12"/>
<connect gate="J" pin="VCCIO7_2" pad="AE15"/>
<connect gate="J" pin="VCCIO7_3" pad="AF12"/>
<connect gate="J" pin="VCCIO7_4" pad="AF15"/>
<connect gate="J" pin="VCCIO8" pad="AE21"/>
<connect gate="J" pin="VCCIO8_2" pad="AE19"/>
<connect gate="J" pin="VCCIO8_3" pad="AF21"/>
<connect gate="J" pin="VCCPD7" pad="AD17"/>
<connect gate="J" pin="VCCPD7_2" pad="AD16"/>
<connect gate="J" pin="VCCPD8" pad="AD20"/>
<connect gate="J" pin="VCCPD8_2" pad="AD19"/>
<connect gate="J" pin="VCCSEL" pad="AF24"/>
<connect gate="J" pin="VCC_PLL12_OUT" pad="AE20"/>
<connect gate="J" pin="VCC_PLL6_OUT" pad="AG16"/>
<connect gate="J" pin="VREFB1N0" pad="AE31"/>
<connect gate="J" pin="VREFB1N1" pad="AC30"/>
<connect gate="K" pin="GND" pad="AK33"/>
<connect gate="K" pin="GND_10" pad="AK21"/>
<connect gate="K" pin="GND_11" pad="AK27"/>
<connect gate="K" pin="GND_12" pad="AK30"/>
<connect gate="K" pin="GND_13" pad="AG17"/>
<connect gate="K" pin="GND_14" pad="AK24"/>
<connect gate="K" pin="GND_15" pad="AG18"/>
<connect gate="K" pin="GND_2" pad="AG27"/>
<connect gate="K" pin="GND_3" pad="AG21"/>
<connect gate="K" pin="GND_4" pad="AG30"/>
<connect gate="K" pin="GND_5" pad="AG33"/>
<connect gate="K" pin="GND_6" pad="AG24"/>
<connect gate="K" pin="GND_7" pad="AK12"/>
<connect gate="K" pin="GND_8" pad="AK15"/>
<connect gate="K" pin="GND_9" pad="AK18"/>
<connect gate="K" pin="IO" pad="AL12"/>
<connect gate="K" pin="IO_10" pad="AH14"/>
<connect gate="K" pin="IO_11" pad="AH15"/>
<connect gate="K" pin="IO_12" pad="AG25"/>
<connect gate="K" pin="IO_13" pad="AH16"/>
<connect gate="K" pin="IO_14" pad="AG26"/>
<connect gate="K" pin="IO_15" pad="AH17"/>
<connect gate="K" pin="IO_16" pad="AH18"/>
<connect gate="K" pin="IO_17" pad="AG28"/>
<connect gate="K" pin="IO_18" pad="AH19"/>
<connect gate="K" pin="IO_19" pad="AG29"/>
<connect gate="K" pin="IO_2" pad="AG34"/>
<connect gate="K" pin="IO_20" pad="AH20"/>
<connect gate="K" pin="IO_21" pad="AH21"/>
<connect gate="K" pin="IO_22" pad="AG31"/>
<connect gate="K" pin="IO_23" pad="AH22"/>
<connect gate="K" pin="IO_24" pad="AG32"/>
<connect gate="K" pin="IO_25" pad="AH23"/>
<connect gate="K" pin="IO_26" pad="AH24"/>
<connect gate="K" pin="IO_27" pad="AH25"/>
<connect gate="K" pin="IO_28" pad="AH26"/>
<connect gate="K" pin="IO_29" pad="AH27"/>
<connect gate="K" pin="IO_3" pad="AH10"/>
<connect gate="K" pin="IO_30" pad="AH28"/>
<connect gate="K" pin="IO_31" pad="AH29"/>
<connect gate="K" pin="IO_32" pad="AH30"/>
<connect gate="K" pin="IO_33" pad="AH31"/>
<connect gate="K" pin="IO_34" pad="AH32"/>
<connect gate="K" pin="IO_35" pad="AH33"/>
<connect gate="K" pin="IO_36" pad="AH34"/>
<connect gate="K" pin="IO_37" pad="AJ10"/>
<connect gate="K" pin="IO_38" pad="AJ11"/>
<connect gate="K" pin="IO_39" pad="AJ12"/>
<connect gate="K" pin="IO_4" pad="AG20"/>
<connect gate="K" pin="IO_40" pad="AJ13"/>
<connect gate="K" pin="IO_41" pad="AJ14"/>
<connect gate="K" pin="IO_42" pad="AJ15"/>
<connect gate="K" pin="IO_43" pad="AJ16"/>
<connect gate="K" pin="IO_44" pad="AJ17"/>
<connect gate="K" pin="IO_45" pad="AJ18"/>
<connect gate="K" pin="IO_46" pad="AJ19"/>
<connect gate="K" pin="IO_47" pad="AJ20"/>
<connect gate="K" pin="IO_48" pad="AJ21"/>
<connect gate="K" pin="IO_49" pad="AJ22"/>
<connect gate="K" pin="IO_5" pad="AH11"/>
<connect gate="K" pin="IO_50" pad="AJ23"/>
<connect gate="K" pin="IO_51" pad="AJ24"/>
<connect gate="K" pin="IO_52" pad="AJ25"/>
<connect gate="K" pin="IO_53" pad="AJ26"/>
<connect gate="K" pin="IO_54" pad="AJ27"/>
<connect gate="K" pin="IO_55" pad="AJ28"/>
<connect gate="K" pin="IO_56" pad="AJ31"/>
<connect gate="K" pin="IO_57" pad="AJ32"/>
<connect gate="K" pin="IO_58" pad="AJ33"/>
<connect gate="K" pin="IO_59" pad="AJ34"/>
<connect gate="K" pin="IO_6" pad="AH12"/>
<connect gate="K" pin="IO_60" pad="AK11"/>
<connect gate="K" pin="IO_61" pad="AK14"/>
<connect gate="K" pin="IO_62" pad="AK16"/>
<connect gate="K" pin="IO_63" pad="AK19"/>
<connect gate="K" pin="IO_64" pad="AK20"/>
<connect gate="K" pin="IO_65" pad="AK23"/>
<connect gate="K" pin="IO_66" pad="AK26"/>
<connect gate="K" pin="IO_67" pad="AK29"/>
<connect gate="K" pin="IO_68" pad="AL10"/>
<connect gate="K" pin="IO_69" pad="AL11"/>
<connect gate="K" pin="IO_7" pad="AG22"/>
<connect gate="K" pin="IO_8" pad="AH13"/>
<connect gate="K" pin="IO_9" pad="AG23"/>
<connect gate="K" pin="NC" pad="AK34"/>
<connect gate="K" pin="NC_2" pad="AJ29"/>
<connect gate="K" pin="NC_3" pad="AJ30"/>
<connect gate="K" pin="NC_4" pad="AK31"/>
<connect gate="K" pin="NC_5" pad="AK32"/>
<connect gate="K" pin="VCCIO8" pad="AG19"/>
<connect gate="K" pin="VREFB7N0" pad="AK17"/>
<connect gate="K" pin="VREFB7N1" pad="AK13"/>
<connect gate="K" pin="VREFB7N2" pad="AK10"/>
<connect gate="K" pin="VREFB8N0" pad="AK28"/>
<connect gate="K" pin="VREFB8N1" pad="AK25"/>
<connect gate="K" pin="VREFB8N2" pad="AK22"/>
<connect gate="L" pin="FPLL8CLKN" pad="AM33"/>
<connect gate="L" pin="FPLL8CLKP" pad="AM34"/>
<connect gate="L" pin="GND" pad="AP33"/>
<connect gate="L" pin="GND_10" pad="AN34"/>
<connect gate="L" pin="GND_2" pad="AN12"/>
<connect gate="L" pin="GND_3" pad="AN15"/>
<connect gate="L" pin="GND_4" pad="AN18"/>
<connect gate="L" pin="GND_5" pad="AN21"/>
<connect gate="L" pin="GND_6" pad="AN24"/>
<connect gate="L" pin="GND_7" pad="AN27"/>
<connect gate="L" pin="GND_8" pad="AN30"/>
<connect gate="L" pin="GND_9" pad="AN33"/>
<connect gate="L" pin="IO" pad="AP32"/>
<connect gate="L" pin="IO_10" pad="AL21"/>
<connect gate="L" pin="IO_11" pad="AL22"/>
<connect gate="L" pin="IO_12" pad="AL23"/>
<connect gate="L" pin="IO_13" pad="AL24"/>
<connect gate="L" pin="IO_14" pad="AL25"/>
<connect gate="L" pin="IO_15" pad="AL26"/>
<connect gate="L" pin="IO_16" pad="AL27"/>
<connect gate="L" pin="IO_17" pad="AL28"/>
<connect gate="L" pin="IO_18" pad="AL29"/>
<connect gate="L" pin="IO_19" pad="AM10"/>
<connect gate="L" pin="IO_2" pad="AL13"/>
<connect gate="L" pin="IO_20" pad="AM11"/>
<connect gate="L" pin="IO_21" pad="AM12"/>
<connect gate="L" pin="IO_22" pad="AM13"/>
<connect gate="L" pin="IO_23" pad="AM14"/>
<connect gate="L" pin="IO_24" pad="AM15"/>
<connect gate="L" pin="IO_25" pad="AM16"/>
<connect gate="L" pin="IO_26" pad="AM17"/>
<connect gate="L" pin="IO_27" pad="AM18"/>
<connect gate="L" pin="IO_28" pad="AM19"/>
<connect gate="L" pin="IO_29" pad="AM20"/>
<connect gate="L" pin="IO_3" pad="AL14"/>
<connect gate="L" pin="IO_30" pad="AM21"/>
<connect gate="L" pin="IO_31" pad="AM22"/>
<connect gate="L" pin="IO_32" pad="AM23"/>
<connect gate="L" pin="IO_33" pad="AM24"/>
<connect gate="L" pin="IO_34" pad="AM25"/>
<connect gate="L" pin="IO_35" pad="AM26"/>
<connect gate="L" pin="IO_36" pad="AM27"/>
<connect gate="L" pin="IO_37" pad="AM28"/>
<connect gate="L" pin="IO_38" pad="AM29"/>
<connect gate="L" pin="IO_39" pad="AM30"/>
<connect gate="L" pin="IO_4" pad="AL15"/>
<connect gate="L" pin="IO_40" pad="AN10"/>
<connect gate="L" pin="IO_41" pad="AN11"/>
<connect gate="L" pin="IO_42" pad="AN13"/>
<connect gate="L" pin="IO_43" pad="AN14"/>
<connect gate="L" pin="IO_44" pad="AN16"/>
<connect gate="L" pin="IO_45" pad="AN17"/>
<connect gate="L" pin="IO_46" pad="AN19"/>
<connect gate="L" pin="IO_47" pad="AN20"/>
<connect gate="L" pin="IO_48" pad="AN22"/>
<connect gate="L" pin="IO_49" pad="AN23"/>
<connect gate="L" pin="IO_5" pad="AL16"/>
<connect gate="L" pin="IO_50" pad="AN25"/>
<connect gate="L" pin="IO_51" pad="AN26"/>
<connect gate="L" pin="IO_52" pad="AN28"/>
<connect gate="L" pin="IO_53" pad="AN29"/>
<connect gate="L" pin="IO_54" pad="AN31"/>
<connect gate="L" pin="IO_55" pad="AN32"/>
<connect gate="L" pin="IO_56" pad="AP10"/>
<connect gate="L" pin="IO_57" pad="AP11"/>
<connect gate="L" pin="IO_58" pad="AP12"/>
<connect gate="L" pin="IO_59" pad="AP13"/>
<connect gate="L" pin="IO_6" pad="AL17"/>
<connect gate="L" pin="IO_60" pad="AP14"/>
<connect gate="L" pin="IO_61" pad="AP15"/>
<connect gate="L" pin="IO_62" pad="AP16"/>
<connect gate="L" pin="IO_63" pad="AP17"/>
<connect gate="L" pin="IO_64" pad="AP18"/>
<connect gate="L" pin="IO_65" pad="AP19"/>
<connect gate="L" pin="IO_66" pad="AP20"/>
<connect gate="L" pin="IO_67" pad="AP21"/>
<connect gate="L" pin="IO_68" pad="AP22"/>
<connect gate="L" pin="IO_69" pad="AP23"/>
<connect gate="L" pin="IO_7" pad="AL18"/>
<connect gate="L" pin="IO_70" pad="AP24"/>
<connect gate="L" pin="IO_71" pad="AP25"/>
<connect gate="L" pin="IO_72" pad="AP26"/>
<connect gate="L" pin="IO_73" pad="AP27"/>
<connect gate="L" pin="IO_74" pad="AP28"/>
<connect gate="L" pin="IO_75" pad="AP29"/>
<connect gate="L" pin="IO_76" pad="AP30"/>
<connect gate="L" pin="IO_77" pad="AP31"/>
<connect gate="L" pin="IO_8" pad="AL19"/>
<connect gate="L" pin="IO_9" pad="AL20"/>
<connect gate="L" pin="NC" pad="AL34"/>
<connect gate="L" pin="NC_2" pad="AL32"/>
<connect gate="L" pin="NC_3" pad="AL33"/>
<connect gate="L" pin="TCK" pad="AL30"/>
<connect gate="L" pin="TDI" pad="AL31"/>
<connect gate="L" pin="TMS" pad="AM32"/>
<connect gate="L" pin="TRST" pad="AM31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP2SGX60EF1152C5N"/>
<attribute name="OC_FARNELL" value="1637243"/>
<attribute name="OC_NEWARK" value="51R0579"/>
<attribute name="PACKAGE" value="BGA-1152"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP3C25E144C8NES">
<description>Cyclone Devices</description>
<gates>
<gate name="A" symbol="EP3C25E144C8NES_A"/>
<gate name="B" symbol="EP3C25E144C8NES_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-145N">
<connects>
<connect gate="A" pin="CLK0" pad="22"/>
<connect gate="A" pin="CLK1" pad="23"/>
<connect gate="A" pin="CLK12" pad="55"/>
<connect gate="A" pin="CLK13" pad="54"/>
<connect gate="A" pin="CLK14" pad="53"/>
<connect gate="A" pin="CLK15" pad="52"/>
<connect gate="A" pin="CLK2" pad="24"/>
<connect gate="A" pin="CLK3" pad="25"/>
<connect gate="A" pin="DCLK" pad="12"/>
<connect gate="A" pin="GND" pad="63"/>
<connect gate="A" pin="GNDA1" pad="36"/>
<connect gate="A" pin="GNDA3" pad="2"/>
<connect gate="A" pin="GND_2" pad="27"/>
<connect gate="A" pin="GND_3" pad="19"/>
<connect gate="A" pin="GND_4" pad="57"/>
<connect gate="A" pin="GND_5" pad="48"/>
<connect gate="A" pin="GND_6" pad="41"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO_10" pad="30"/>
<connect gate="A" pin="IO_11" pad="31"/>
<connect gate="A" pin="IO_12" pad="32"/>
<connect gate="A" pin="IO_13" pad="33"/>
<connect gate="A" pin="IO_14" pad="39"/>
<connect gate="A" pin="IO_15" pad="42"/>
<connect gate="A" pin="IO_16" pad="43"/>
<connect gate="A" pin="IO_17" pad="44"/>
<connect gate="A" pin="IO_18" pad="46"/>
<connect gate="A" pin="IO_19" pad="49"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="50"/>
<connect gate="A" pin="IO_21" pad="51"/>
<connect gate="A" pin="IO_22" pad="58"/>
<connect gate="A" pin="IO_23" pad="59"/>
<connect gate="A" pin="IO_24" pad="60"/>
<connect gate="A" pin="IO_25" pad="64"/>
<connect gate="A" pin="IO_26" pad="65"/>
<connect gate="A" pin="IO_27" pad="66"/>
<connect gate="A" pin="IO_28" pad="67"/>
<connect gate="A" pin="IO_29" pad="68"/>
<connect gate="A" pin="IO_3" pad="6"/>
<connect gate="A" pin="IO_30" pad="69"/>
<connect gate="A" pin="IO_31" pad="71"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="10"/>
<connect gate="A" pin="IO_7" pad="11"/>
<connect gate="A" pin="IO_8" pad="13"/>
<connect gate="A" pin="IO_9" pad="28"/>
<connect gate="A" pin="NCE" pad="21"/>
<connect gate="A" pin="NCONFIG" pad="14"/>
<connect gate="A" pin="NSTATUS" pad="9"/>
<connect gate="A" pin="TCK" pad="16"/>
<connect gate="A" pin="TDI" pad="15"/>
<connect gate="A" pin="TDO" pad="20"/>
<connect gate="A" pin="TMS" pad="18"/>
<connect gate="A" pin="VCCA1" pad="35"/>
<connect gate="A" pin="VCCA3" pad="3"/>
<connect gate="A" pin="VCCD_PLL1" pad="37"/>
<connect gate="A" pin="VCCD_PLL3" pad="1"/>
<connect gate="A" pin="VCCD_PLL4" pad="73"/>
<connect gate="A" pin="VCCINT" pad="5"/>
<connect gate="A" pin="VCCINT_2" pad="61"/>
<connect gate="A" pin="VCCINT_3" pad="45"/>
<connect gate="A" pin="VCCINT_4" pad="29"/>
<connect gate="A" pin="VCCINT_5" pad="70"/>
<connect gate="A" pin="VCCINT_6" pad="34"/>
<connect gate="A" pin="VCCINT_7" pad="38"/>
<connect gate="A" pin="VCCIO1" pad="17"/>
<connect gate="A" pin="VCCIO2" pad="26"/>
<connect gate="A" pin="VCCIO3" pad="47"/>
<connect gate="A" pin="VCCIO3_2" pad="40"/>
<connect gate="A" pin="VCCIO4" pad="62"/>
<connect gate="A" pin="VCCIO4_2" pad="56"/>
<connect gate="B" pin="CLK10" pad="128"/>
<connect gate="B" pin="CLK11" pad="129"/>
<connect gate="B" pin="CLK4" pad="91"/>
<connect gate="B" pin="CLK5" pad="90"/>
<connect gate="B" pin="CLK6" pad="89"/>
<connect gate="B" pin="CLK7" pad="88"/>
<connect gate="B" pin="CLK8" pad="126"/>
<connect gate="B" pin="CLK9" pad="127"/>
<connect gate="B" pin="CONF_DONE" pad="92"/>
<connect gate="B" pin="EPAD" pad="145"/>
<connect gate="B" pin="GND" pad="123"/>
<connect gate="B" pin="GNDA2" pad="108"/>
<connect gate="B" pin="GNDA4" pad="74"/>
<connect gate="B" pin="GND_2" pad="82"/>
<connect gate="B" pin="GND_3" pad="95"/>
<connect gate="B" pin="GND_4" pad="140"/>
<connect gate="B" pin="GND_5" pad="118"/>
<connect gate="B" pin="GND_6" pad="131"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO_10" pad="98"/>
<connect gate="B" pin="IO_11" pad="99"/>
<connect gate="B" pin="IO_12" pad="100"/>
<connect gate="B" pin="IO_13" pad="101"/>
<connect gate="B" pin="IO_14" pad="103"/>
<connect gate="B" pin="IO_15" pad="104"/>
<connect gate="B" pin="IO_16" pad="105"/>
<connect gate="B" pin="IO_17" pad="106"/>
<connect gate="B" pin="IO_18" pad="110"/>
<connect gate="B" pin="IO_19" pad="111"/>
<connect gate="B" pin="IO_2" pad="76"/>
<connect gate="B" pin="IO_20" pad="112"/>
<connect gate="B" pin="IO_21" pad="113"/>
<connect gate="B" pin="IO_22" pad="114"/>
<connect gate="B" pin="IO_23" pad="115"/>
<connect gate="B" pin="IO_24" pad="119"/>
<connect gate="B" pin="IO_25" pad="120"/>
<connect gate="B" pin="IO_26" pad="121"/>
<connect gate="B" pin="IO_27" pad="125"/>
<connect gate="B" pin="IO_28" pad="132"/>
<connect gate="B" pin="IO_29" pad="133"/>
<connect gate="B" pin="IO_3" pad="77"/>
<connect gate="B" pin="IO_30" pad="135"/>
<connect gate="B" pin="IO_31" pad="136"/>
<connect gate="B" pin="IO_32" pad="137"/>
<connect gate="B" pin="IO_33" pad="141"/>
<connect gate="B" pin="IO_34" pad="142"/>
<connect gate="B" pin="IO_35" pad="143"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="94"/>
<connect gate="B" pin="MSEL1" pad="96"/>
<connect gate="B" pin="MSEL2" pad="97"/>
<connect gate="B" pin="VCCA2" pad="107"/>
<connect gate="B" pin="VCCA4" pad="75"/>
<connect gate="B" pin="VCCD_PLL2" pad="109"/>
<connect gate="B" pin="VCCINT" pad="138"/>
<connect gate="B" pin="VCCINT_2" pad="124"/>
<connect gate="B" pin="VCCINT_3" pad="134"/>
<connect gate="B" pin="VCCINT_4" pad="78"/>
<connect gate="B" pin="VCCINT_5" pad="102"/>
<connect gate="B" pin="VCCINT_6" pad="116"/>
<connect gate="B" pin="VCCINT_7" pad="84"/>
<connect gate="B" pin="VCCIO5" pad="81"/>
<connect gate="B" pin="VCCIO6" pad="93"/>
<connect gate="B" pin="VCCIO7" pad="122"/>
<connect gate="B" pin="VCCIO7_2" pad="117"/>
<connect gate="B" pin="VCCIO8" pad="139"/>
<connect gate="B" pin="VCCIO8_2" pad="130"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP3C25E144C8NES"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="52R1223"/>
<attribute name="PACKAGE" value="EQFP-144"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP3SL150F1152C4N">
<description>FPGA, STRATIX III</description>
<gates>
<gate name="A" symbol="EP3SL150F1152C4N_A"/>
<gate name="B" symbol="EP3SL150F1152C4N_B"/>
<gate name="C" symbol="EP3SL150F1152C4N_C"/>
<gate name="D" symbol="EP3SL150F1152C4N_D"/>
<gate name="E" symbol="EP3SL150F1152C4N_E"/>
<gate name="F" symbol="EP3SL150F1152C4N_F"/>
<gate name="G" symbol="EP3SL150F1152C4N_G"/>
<gate name="H" symbol="EP3SL150F1152C4N_H"/>
<gate name="I" symbol="EP3SL150F1152C4N_I"/>
<gate name="J" symbol="EP3SL150F1152C4N_J"/>
<gate name="K" symbol="EP3SL150F1152C4N_K"/>
<gate name="L" symbol="EP3SL150F1152C4N_L"/>
</gates>
<devices>
<device name="" package="BGA1152C100P34X34_3500X3500X35">
<connects>
<connect gate="A" pin="GND" pad="C2"/>
<connect gate="A" pin="GND_10" pad="J5"/>
<connect gate="A" pin="GND_11" pad="B9"/>
<connect gate="A" pin="GND_12" pad="J8"/>
<connect gate="A" pin="GND_2" pad="H9"/>
<connect gate="A" pin="GND_3" pad="B3"/>
<connect gate="A" pin="GND_4" pad="E6"/>
<connect gate="A" pin="GND_5" pad="E9"/>
<connect gate="A" pin="GND_6" pad="J2"/>
<connect gate="A" pin="GND_7" pad="B6"/>
<connect gate="A" pin="GND_8" pad="F2"/>
<connect gate="A" pin="GND_9" pad="F5"/>
<connect gate="A" pin="IO_6" pad="L7"/>
<connect gate="A" pin="IO_6_10" pad="F4"/>
<connect gate="A" pin="IO_6_11" pad="G1"/>
<connect gate="A" pin="IO_6_12" pad="G2"/>
<connect gate="A" pin="IO_6_13" pad="G4"/>
<connect gate="A" pin="IO_6_14" pad="G5"/>
<connect gate="A" pin="IO_6_15" pad="H1"/>
<connect gate="A" pin="IO_6_16" pad="H2"/>
<connect gate="A" pin="IO_6_17" pad="H3"/>
<connect gate="A" pin="IO_6_18" pad="H4"/>
<connect gate="A" pin="IO_6_19" pad="H5"/>
<connect gate="A" pin="IO_6_2" pad="C1"/>
<connect gate="A" pin="IO_6_20" pad="H6"/>
<connect gate="A" pin="IO_6_21" pad="J1"/>
<connect gate="A" pin="IO_6_22" pad="J3"/>
<connect gate="A" pin="IO_6_23" pad="J4"/>
<connect gate="A" pin="IO_6_24" pad="J6"/>
<connect gate="A" pin="IO_6_25" pad="J7"/>
<connect gate="A" pin="IO_6_26" pad="K1"/>
<connect gate="A" pin="IO_6_27" pad="K2"/>
<connect gate="A" pin="IO_6_28" pad="K3"/>
<connect gate="A" pin="IO_6_29" pad="K4"/>
<connect gate="A" pin="IO_6_3" pad="D1"/>
<connect gate="A" pin="IO_6_30" pad="K5"/>
<connect gate="A" pin="IO_6_31" pad="K6"/>
<connect gate="A" pin="IO_6_32" pad="K7"/>
<connect gate="A" pin="IO_6_33" pad="K8"/>
<connect gate="A" pin="IO_6_34" pad="L1"/>
<connect gate="A" pin="IO_6_35" pad="L2"/>
<connect gate="A" pin="IO_6_36" pad="L4"/>
<connect gate="A" pin="IO_6_37" pad="L5"/>
<connect gate="A" pin="IO_6_38" pad="L6"/>
<connect gate="A" pin="IO_6_4" pad="D2"/>
<connect gate="A" pin="IO_6_5" pad="D3"/>
<connect gate="A" pin="IO_6_6" pad="E1"/>
<connect gate="A" pin="IO_6_7" pad="E2"/>
<connect gate="A" pin="IO_6_8" pad="F1"/>
<connect gate="A" pin="IO_6_9" pad="F3"/>
<connect gate="A" pin="IO_6_RDN6A" pad="E3"/>
<connect gate="A" pin="IO_6_RUP6A" pad="E4"/>
<connect gate="A" pin="IO_7" pad="G9"/>
<connect gate="A" pin="IO_7_10" pad="B2"/>
<connect gate="A" pin="IO_7_11" pad="B4"/>
<connect gate="A" pin="IO_7_12" pad="B5"/>
<connect gate="A" pin="IO_7_13" pad="B7"/>
<connect gate="A" pin="IO_7_14" pad="B8"/>
<connect gate="A" pin="IO_7_15" pad="C3"/>
<connect gate="A" pin="IO_7_16" pad="C4"/>
<connect gate="A" pin="IO_7_17" pad="C5"/>
<connect gate="A" pin="IO_7_18" pad="C6"/>
<connect gate="A" pin="IO_7_19" pad="C7"/>
<connect gate="A" pin="IO_7_2" pad="A2"/>
<connect gate="A" pin="IO_7_20" pad="C9"/>
<connect gate="A" pin="IO_7_21" pad="D6"/>
<connect gate="A" pin="IO_7_22" pad="D7"/>
<connect gate="A" pin="IO_7_23" pad="D8"/>
<connect gate="A" pin="IO_7_24" pad="D9"/>
<connect gate="A" pin="IO_7_25" pad="E8"/>
<connect gate="A" pin="IO_7_26" pad="F6"/>
<connect gate="A" pin="IO_7_27" pad="F8"/>
<connect gate="A" pin="IO_7_28" pad="F9"/>
<connect gate="A" pin="IO_7_29" pad="G8"/>
<connect gate="A" pin="IO_7_3" pad="A3"/>
<connect gate="A" pin="IO_7_4" pad="A4"/>
<connect gate="A" pin="IO_7_5" pad="A5"/>
<connect gate="A" pin="IO_7_6" pad="A6"/>
<connect gate="A" pin="IO_7_7" pad="A7"/>
<connect gate="A" pin="IO_7_8" pad="A8"/>
<connect gate="A" pin="IO_7_9" pad="A9"/>
<connect gate="A" pin="IO_7_RDN7A" pad="E7"/>
<connect gate="A" pin="IO_7_RUP7A" pad="F7"/>
<connect gate="A" pin="MSEL1" pad="J9"/>
<connect gate="A" pin="MSEL2" pad="K9"/>
<connect gate="A" pin="NC" pad="G7"/>
<connect gate="A" pin="TEMPDIODEN" pad="D4"/>
<connect gate="A" pin="TEMPDIODEP" pad="E5"/>
<connect gate="A" pin="VCCBAT" pad="G6"/>
<connect gate="A" pin="VCCIO6A" pad="H7"/>
<connect gate="A" pin="VCCIO6A_2" pad="G3"/>
<connect gate="A" pin="VCCIO6A_3" pad="B1"/>
<connect gate="A" pin="VCCIO6C" pad="L3"/>
<connect gate="A" pin="VCCIO7A" pad="C8"/>
<connect gate="A" pin="VCCIO7A_2" pad="D5"/>
<connect gate="A" pin="VCCPT" pad="H8"/>
<connect gate="B" pin="CLK10N" pad="U1"/>
<connect gate="B" pin="CLK10P" pad="U2"/>
<connect gate="B" pin="CLK8N" pad="W1"/>
<connect gate="B" pin="CLK8P" pad="W2"/>
<connect gate="B" pin="GND" pad="V8"/>
<connect gate="B" pin="GND_2" pad="R2"/>
<connect gate="B" pin="GND_3" pad="R5"/>
<connect gate="B" pin="GND_4" pad="M2"/>
<connect gate="B" pin="GND_5" pad="V2"/>
<connect gate="B" pin="GND_6" pad="R8"/>
<connect gate="B" pin="GND_7" pad="V5"/>
<connect gate="B" pin="GND_8" pad="M5"/>
<connect gate="B" pin="GND_9" pad="M8"/>
<connect gate="B" pin="IO_5" pad="Y9"/>
<connect gate="B" pin="IO_5_10" pad="Y2"/>
<connect gate="B" pin="IO_5_11" pad="Y3"/>
<connect gate="B" pin="IO_5_12" pad="Y4"/>
<connect gate="B" pin="IO_5_13" pad="Y5"/>
<connect gate="B" pin="IO_5_14" pad="Y6"/>
<connect gate="B" pin="IO_5_15" pad="Y7"/>
<connect gate="B" pin="IO_5_16" pad="Y8"/>
<connect gate="B" pin="IO_5_2" pad="V3"/>
<connect gate="B" pin="IO_5_3" pad="V4"/>
<connect gate="B" pin="IO_5_4" pad="W3"/>
<connect gate="B" pin="IO_5_5" pad="W5"/>
<connect gate="B" pin="IO_5_6" pad="W6"/>
<connect gate="B" pin="IO_5_7" pad="W7"/>
<connect gate="B" pin="IO_5_8" pad="W8"/>
<connect gate="B" pin="IO_5_9" pad="Y1"/>
<connect gate="B" pin="IO_5_CLK9N" pad="U3"/>
<connect gate="B" pin="IO_5_CLK9P" pad="U4"/>
<connect gate="B" pin="IO_5_PLL_R3_CLKOUT0N" pad="W9"/>
<connect gate="B" pin="IO_6" pad="R9"/>
<connect gate="B" pin="IO_6_10" pad="M1"/>
<connect gate="B" pin="IO_6_11" pad="M3"/>
<connect gate="B" pin="IO_6_12" pad="M4"/>
<connect gate="B" pin="IO_6_13" pad="M6"/>
<connect gate="B" pin="IO_6_14" pad="M7"/>
<connect gate="B" pin="IO_6_15" pad="M9"/>
<connect gate="B" pin="IO_6_16" pad="N1"/>
<connect gate="B" pin="IO_6_17" pad="N2"/>
<connect gate="B" pin="IO_6_18" pad="N3"/>
<connect gate="B" pin="IO_6_19" pad="N4"/>
<connect gate="B" pin="IO_6_2" pad="T4"/>
<connect gate="B" pin="IO_6_20" pad="N5"/>
<connect gate="B" pin="IO_6_21" pad="N6"/>
<connect gate="B" pin="IO_6_22" pad="N8"/>
<connect gate="B" pin="IO_6_23" pad="N9"/>
<connect gate="B" pin="IO_6_24" pad="P1"/>
<connect gate="B" pin="IO_6_25" pad="P2"/>
<connect gate="B" pin="IO_6_26" pad="P3"/>
<connect gate="B" pin="IO_6_27" pad="P4"/>
<connect gate="B" pin="IO_6_28" pad="P5"/>
<connect gate="B" pin="IO_6_29" pad="P6"/>
<connect gate="B" pin="IO_6_3" pad="T5"/>
<connect gate="B" pin="IO_6_30" pad="P7"/>
<connect gate="B" pin="IO_6_31" pad="P8"/>
<connect gate="B" pin="IO_6_32" pad="R1"/>
<connect gate="B" pin="IO_6_33" pad="R3"/>
<connect gate="B" pin="IO_6_34" pad="R4"/>
<connect gate="B" pin="IO_6_35" pad="R6"/>
<connect gate="B" pin="IO_6_36" pad="R7"/>
<connect gate="B" pin="IO_6_4" pad="T7"/>
<connect gate="B" pin="IO_6_5" pad="U6"/>
<connect gate="B" pin="IO_6_6" pad="T8"/>
<connect gate="B" pin="IO_6_7" pad="T9"/>
<connect gate="B" pin="IO_6_8" pad="L8"/>
<connect gate="B" pin="IO_6_9" pad="L9"/>
<connect gate="B" pin="IO_6_CLK11N" pad="T1"/>
<connect gate="B" pin="IO_6_CLK11P" pad="T2"/>
<connect gate="B" pin="IO_7" pad="A15"/>
<connect gate="B" pin="IO_7_2" pad="A10"/>
<connect gate="B" pin="IO_7_3" pad="A11"/>
<connect gate="B" pin="IO_7_4" pad="A12"/>
<connect gate="B" pin="IO_7_5" pad="A13"/>
<connect gate="B" pin="IO_7_6" pad="A14"/>
<connect gate="B" pin="IO_7_CLK12N" pad="A17"/>
<connect gate="B" pin="IO_7_CLK13N" pad="A16"/>
<connect gate="B" pin="IO_8" pad="A22"/>
<connect gate="B" pin="IO_8_2" pad="A21"/>
<connect gate="B" pin="IO_8_CLK14N" pad="A19"/>
<connect gate="B" pin="IO_8_CLK15N" pad="A20"/>
<connect gate="B" pin="VCCA_PLL_R2" pad="U7"/>
<connect gate="B" pin="VCCA_PLL_R3" pad="V7"/>
<connect gate="B" pin="VCCD_PLL_R2" pad="U9"/>
<connect gate="B" pin="VCCD_PLL_R3" pad="V9"/>
<connect gate="B" pin="VCCIO5C" pad="V1"/>
<connect gate="B" pin="VCCIO5C_2" pad="W4"/>
<connect gate="B" pin="VCCIO5C_3" pad="U5"/>
<connect gate="B" pin="VCCIO6A" pad="N7"/>
<connect gate="B" pin="VCCIO6C" pad="T6"/>
<connect gate="B" pin="VCCIO6C_2" pad="T3"/>
<connect gate="B" pin="VCCIO8C" pad="A18"/>
<connect gate="B" pin="VCCPT" pad="V6"/>
<connect gate="B" pin="VREF6A" pad="P9"/>
<connect gate="B" pin="VREF6C" pad="U8"/>
<connect gate="C" pin="ASDO" pad="AH6"/>
<connect gate="C" pin="GND" pad="AD8"/>
<connect gate="C" pin="GND_10" pad="AG5"/>
<connect gate="C" pin="GND_11" pad="AD5"/>
<connect gate="C" pin="GND_2" pad="AK2"/>
<connect gate="C" pin="GND_3" pad="AF9"/>
<connect gate="C" pin="GND_4" pad="AG2"/>
<connect gate="C" pin="GND_5" pad="AA2"/>
<connect gate="C" pin="GND_6" pad="AG8"/>
<connect gate="C" pin="GND_7" pad="AA5"/>
<connect gate="C" pin="GND_8" pad="AD2"/>
<connect gate="C" pin="GND_9" pad="AA8"/>
<connect gate="C" pin="IO_4" pad="AH8"/>
<connect gate="C" pin="IO_4_2" pad="AJ6"/>
<connect gate="C" pin="IO_4_3" pad="AJ7"/>
<connect gate="C" pin="IO_4_4" pad="AJ8"/>
<connect gate="C" pin="IO_4_5" pad="AJ9"/>
<connect gate="C" pin="IO_4_RDN4A" pad="AH9"/>
<connect gate="C" pin="IO_4_RUP4A" pad="AG9"/>
<connect gate="C" pin="IO_5" pad="AD7"/>
<connect gate="C" pin="IO_5_10" pad="AF4"/>
<connect gate="C" pin="IO_5_11" pad="AF5"/>
<connect gate="C" pin="IO_5_12" pad="AJ1"/>
<connect gate="C" pin="IO_5_13" pad="AF6"/>
<connect gate="C" pin="IO_5_14" pad="AJ2"/>
<connect gate="C" pin="IO_5_15" pad="AG1"/>
<connect gate="C" pin="IO_5_16" pad="AJ3"/>
<connect gate="C" pin="IO_5_17" pad="AG3"/>
<connect gate="C" pin="IO_5_18" pad="AJ4"/>
<connect gate="C" pin="IO_5_19" pad="AG4"/>
<connect gate="C" pin="IO_5_2" pad="AH1"/>
<connect gate="C" pin="IO_5_20" pad="AE1"/>
<connect gate="C" pin="IO_5_21" pad="AE2"/>
<connect gate="C" pin="IO_5_22" pad="AE3"/>
<connect gate="C" pin="IO_5_23" pad="AE4"/>
<connect gate="C" pin="IO_5_24" pad="AE5"/>
<connect gate="C" pin="IO_5_25" pad="AE6"/>
<connect gate="C" pin="IO_5_26" pad="AE7"/>
<connect gate="C" pin="IO_5_27" pad="AE8"/>
<connect gate="C" pin="IO_5_28" pad="AA1"/>
<connect gate="C" pin="IO_5_29" pad="AA3"/>
<connect gate="C" pin="IO_5_3" pad="AH2"/>
<connect gate="C" pin="IO_5_30" pad="AA4"/>
<connect gate="C" pin="IO_5_31" pad="AA6"/>
<connect gate="C" pin="IO_5_32" pad="AA7"/>
<connect gate="C" pin="IO_5_33" pad="AB1"/>
<connect gate="C" pin="IO_5_34" pad="AB2"/>
<connect gate="C" pin="IO_5_35" pad="AB3"/>
<connect gate="C" pin="IO_5_36" pad="AB4"/>
<connect gate="C" pin="IO_5_37" pad="AB5"/>
<connect gate="C" pin="IO_5_38" pad="AB6"/>
<connect gate="C" pin="IO_5_39" pad="AB8"/>
<connect gate="C" pin="IO_5_4" pad="AH4"/>
<connect gate="C" pin="IO_5_40" pad="AB9"/>
<connect gate="C" pin="IO_5_41" pad="AC1"/>
<connect gate="C" pin="IO_5_42" pad="AC2"/>
<connect gate="C" pin="IO_5_43" pad="AC4"/>
<connect gate="C" pin="IO_5_44" pad="AC5"/>
<connect gate="C" pin="IO_5_45" pad="AC6"/>
<connect gate="C" pin="IO_5_46" pad="AC7"/>
<connect gate="C" pin="IO_5_47" pad="AC8"/>
<connect gate="C" pin="IO_5_48" pad="AC9"/>
<connect gate="C" pin="IO_5_49" pad="AD1"/>
<connect gate="C" pin="IO_5_5" pad="AH5"/>
<connect gate="C" pin="IO_5_50" pad="AD3"/>
<connect gate="C" pin="IO_5_51" pad="AD4"/>
<connect gate="C" pin="IO_5_52" pad="AD6"/>
<connect gate="C" pin="IO_5_6" pad="AF1"/>
<connect gate="C" pin="IO_5_7" pad="AF2"/>
<connect gate="C" pin="IO_5_8" pad="AK1"/>
<connect gate="C" pin="IO_5_9" pad="AF3"/>
<connect gate="C" pin="IO_5_RDN5A" pad="AK3"/>
<connect gate="C" pin="IO_5_RUP5A" pad="AK4"/>
<connect gate="C" pin="IO_8" pad="A33"/>
<connect gate="C" pin="IO_8_10" pad="A31"/>
<connect gate="C" pin="IO_8_11" pad="A32"/>
<connect gate="C" pin="IO_8_2" pad="A23"/>
<connect gate="C" pin="IO_8_3" pad="A24"/>
<connect gate="C" pin="IO_8_4" pad="A25"/>
<connect gate="C" pin="IO_8_5" pad="A26"/>
<connect gate="C" pin="IO_8_6" pad="A27"/>
<connect gate="C" pin="IO_8_7" pad="A28"/>
<connect gate="C" pin="IO_8_8" pad="A29"/>
<connect gate="C" pin="IO_8_9" pad="A30"/>
<connect gate="C" pin="NC" pad="AH7"/>
<connect gate="C" pin="NCEO" pad="AJ5"/>
<connect gate="C" pin="NCSO" pad="AE9"/>
<connect gate="C" pin="NIO_PULLUP" pad="AF8"/>
<connect gate="C" pin="VCCIO5A" pad="AD9"/>
<connect gate="C" pin="VCCIO5A_2" pad="AB7"/>
<connect gate="C" pin="VCCIO5A_3" pad="AG6"/>
<connect gate="C" pin="VCCIO5A_4" pad="AH3"/>
<connect gate="C" pin="VCCIO5C" pad="AC3"/>
<connect gate="C" pin="VCCPT" pad="AG7"/>
<connect gate="C" pin="VREF5A" pad="AF7"/>
<connect gate="C" pin="VREF5C" pad="AA9"/>
<connect gate="D" pin="DCLK" pad="AL3"/>
<connect gate="D" pin="GND" pad="B33"/>
<connect gate="D" pin="GND_10" pad="B21"/>
<connect gate="D" pin="GND_11" pad="B24"/>
<connect gate="D" pin="GND_12" pad="B27"/>
<connect gate="D" pin="GND_13" pad="B30"/>
<connect gate="D" pin="GND_2" pad="AK8"/>
<connect gate="D" pin="GND_3" pad="AN2"/>
<connect gate="D" pin="GND_4" pad="AN5"/>
<connect gate="D" pin="GND_5" pad="AN8"/>
<connect gate="D" pin="GND_6" pad="B12"/>
<connect gate="D" pin="GND_7" pad="AK5"/>
<connect gate="D" pin="GND_8" pad="B15"/>
<connect gate="D" pin="GND_9" pad="B18"/>
<connect gate="D" pin="IO_1" pad="C34"/>
<connect gate="D" pin="IO_1_2" pad="C33"/>
<connect gate="D" pin="IO_4" pad="AP9"/>
<connect gate="D" pin="IO_4_10" pad="AM4"/>
<connect gate="D" pin="IO_4_11" pad="AM5"/>
<connect gate="D" pin="IO_4_12" pad="AM6"/>
<connect gate="D" pin="IO_4_13" pad="AM7"/>
<connect gate="D" pin="IO_4_14" pad="AM8"/>
<connect gate="D" pin="IO_4_15" pad="AM9"/>
<connect gate="D" pin="IO_4_16" pad="AN3"/>
<connect gate="D" pin="IO_4_17" pad="AN4"/>
<connect gate="D" pin="IO_4_18" pad="AN6"/>
<connect gate="D" pin="IO_4_19" pad="AN7"/>
<connect gate="D" pin="IO_4_2" pad="AK6"/>
<connect gate="D" pin="IO_4_20" pad="AN9"/>
<connect gate="D" pin="IO_4_21" pad="AP2"/>
<connect gate="D" pin="IO_4_22" pad="AP3"/>
<connect gate="D" pin="IO_4_23" pad="AP4"/>
<connect gate="D" pin="IO_4_24" pad="AP5"/>
<connect gate="D" pin="IO_4_25" pad="AP6"/>
<connect gate="D" pin="IO_4_26" pad="AP7"/>
<connect gate="D" pin="IO_4_27" pad="AP8"/>
<connect gate="D" pin="IO_4_3" pad="AK7"/>
<connect gate="D" pin="IO_4_4" pad="AK9"/>
<connect gate="D" pin="IO_4_5" pad="AL4"/>
<connect gate="D" pin="IO_4_6" pad="AL5"/>
<connect gate="D" pin="IO_4_7" pad="AL7"/>
<connect gate="D" pin="IO_4_8" pad="AL8"/>
<connect gate="D" pin="IO_4_9" pad="AL9"/>
<connect gate="D" pin="IO_5" pad="AM2"/>
<connect gate="D" pin="IO_5_2" pad="AL1"/>
<connect gate="D" pin="IO_5_3" pad="AL2"/>
<connect gate="D" pin="IO_5_4" pad="AM1"/>
<connect gate="D" pin="IO_7" pad="D15"/>
<connect gate="D" pin="IO_7_10" pad="B13"/>
<connect gate="D" pin="IO_7_11" pad="C17"/>
<connect gate="D" pin="IO_7_12" pad="D10"/>
<connect gate="D" pin="IO_7_13" pad="D11"/>
<connect gate="D" pin="IO_7_14" pad="D12"/>
<connect gate="D" pin="IO_7_15" pad="D13"/>
<connect gate="D" pin="IO_7_16" pad="D14"/>
<connect gate="D" pin="IO_7_2" pad="B14"/>
<connect gate="D" pin="IO_7_3" pad="C11"/>
<connect gate="D" pin="IO_7_4" pad="C12"/>
<connect gate="D" pin="IO_7_5" pad="C14"/>
<connect gate="D" pin="IO_7_6" pad="C15"/>
<connect gate="D" pin="IO_7_7" pad="C16"/>
<connect gate="D" pin="IO_7_8" pad="B10"/>
<connect gate="D" pin="IO_7_9" pad="B11"/>
<connect gate="D" pin="IO_7_CLK12P" pad="B17"/>
<connect gate="D" pin="IO_7_CLK13P" pad="B16"/>
<connect gate="D" pin="IO_8" pad="C31"/>
<connect gate="D" pin="IO_8_10" pad="C19"/>
<connect gate="D" pin="IO_8_11" pad="C20"/>
<connect gate="D" pin="IO_8_12" pad="C21"/>
<connect gate="D" pin="IO_8_13" pad="C23"/>
<connect gate="D" pin="IO_8_14" pad="C24"/>
<connect gate="D" pin="IO_8_15" pad="C26"/>
<connect gate="D" pin="IO_8_16" pad="C27"/>
<connect gate="D" pin="IO_8_17" pad="C28"/>
<connect gate="D" pin="IO_8_18" pad="C29"/>
<connect gate="D" pin="IO_8_19" pad="C30"/>
<connect gate="D" pin="IO_8_2" pad="B22"/>
<connect gate="D" pin="IO_8_3" pad="B23"/>
<connect gate="D" pin="IO_8_4" pad="B25"/>
<connect gate="D" pin="IO_8_5" pad="B26"/>
<connect gate="D" pin="IO_8_6" pad="B28"/>
<connect gate="D" pin="IO_8_7" pad="B29"/>
<connect gate="D" pin="IO_8_8" pad="B31"/>
<connect gate="D" pin="IO_8_9" pad="B32"/>
<connect gate="D" pin="IO_8_CLK14P" pad="B19"/>
<connect gate="D" pin="IO_8_CLK15P" pad="B20"/>
<connect gate="D" pin="IO_8_PLL_T1_FBN/CLKOUT2" pad="C18"/>
<connect gate="D" pin="VCCIO1A" pad="B34"/>
<connect gate="D" pin="VCCIO4A" pad="AM3"/>
<connect gate="D" pin="VCCIO4A_2" pad="AL6"/>
<connect gate="D" pin="VCCIO5A" pad="AN1"/>
<connect gate="D" pin="VCCIO7B" pad="C10"/>
<connect gate="D" pin="VCCIO7C" pad="C13"/>
<connect gate="D" pin="VCCIO8A" pad="C32"/>
<connect gate="D" pin="VCCIO8B" pad="C25"/>
<connect gate="D" pin="VCCIO8C" pad="C22"/>
<connect gate="E" pin="GND" pad="E33"/>
<connect gate="E" pin="GND_2" pad="E12"/>
<connect gate="E" pin="GND_3" pad="E15"/>
<connect gate="E" pin="GND_4" pad="E18"/>
<connect gate="E" pin="GND_5" pad="E21"/>
<connect gate="E" pin="GND_6" pad="E24"/>
<connect gate="E" pin="GND_7" pad="E27"/>
<connect gate="E" pin="GND_8" pad="E30"/>
<connect gate="E" pin="IO_1" pad="G34"/>
<connect gate="E" pin="IO_1_10" pad="G31"/>
<connect gate="E" pin="IO_1_11" pad="G33"/>
<connect gate="E" pin="IO_1_2" pad="F31"/>
<connect gate="E" pin="IO_1_3" pad="F32"/>
<connect gate="E" pin="IO_1_4" pad="F33"/>
<connect gate="E" pin="IO_1_5" pad="F34"/>
<connect gate="E" pin="IO_1_6" pad="D33"/>
<connect gate="E" pin="IO_1_7" pad="D34"/>
<connect gate="E" pin="IO_1_8" pad="E34"/>
<connect gate="E" pin="IO_1_9" pad="G30"/>
<connect gate="E" pin="IO_1_RDN1A" pad="E32"/>
<connect gate="E" pin="IO_1_RUP1A" pad="E31"/>
<connect gate="E" pin="IO_7" pad="H11"/>
<connect gate="E" pin="IO_7_10" pad="E11"/>
<connect gate="E" pin="IO_7_11" pad="E13"/>
<connect gate="E" pin="IO_7_12" pad="E14"/>
<connect gate="E" pin="IO_7_13" pad="E17"/>
<connect gate="E" pin="IO_7_14" pad="F11"/>
<connect gate="E" pin="IO_7_15" pad="F12"/>
<connect gate="E" pin="IO_7_16" pad="F13"/>
<connect gate="E" pin="IO_7_17" pad="F14"/>
<connect gate="E" pin="IO_7_18" pad="F15"/>
<connect gate="E" pin="IO_7_2" pad="G10"/>
<connect gate="E" pin="IO_7_3" pad="G11"/>
<connect gate="E" pin="IO_7_4" pad="G12"/>
<connect gate="E" pin="IO_7_5" pad="G13"/>
<connect gate="E" pin="IO_7_6" pad="G16"/>
<connect gate="E" pin="IO_7_7" pad="D16"/>
<connect gate="E" pin="IO_7_8" pad="D17"/>
<connect gate="E" pin="IO_7_9" pad="E10"/>
<connect gate="E" pin="IO_7_PLL_T2_FBN/CLKOUT2" pad="E16"/>
<connect gate="E" pin="IO_7_PLL_T2_FBP/CLKOUT1" pad="F16"/>
<connect gate="E" pin="IO_8" pad="G27"/>
<connect gate="E" pin="IO_8_10" pad="F27"/>
<connect gate="E" pin="IO_8_11" pad="F28"/>
<connect gate="E" pin="IO_8_12" pad="F29"/>
<connect gate="E" pin="IO_8_13" pad="G20"/>
<connect gate="E" pin="IO_8_14" pad="G21"/>
<connect gate="E" pin="IO_8_15" pad="D19"/>
<connect gate="E" pin="IO_8_16" pad="D20"/>
<connect gate="E" pin="IO_8_17" pad="D21"/>
<connect gate="E" pin="IO_8_18" pad="D22"/>
<connect gate="E" pin="IO_8_19" pad="D23"/>
<connect gate="E" pin="IO_8_2" pad="F19"/>
<connect gate="E" pin="IO_8_20" pad="D24"/>
<connect gate="E" pin="IO_8_21" pad="D25"/>
<connect gate="E" pin="IO_8_22" pad="D26"/>
<connect gate="E" pin="IO_8_23" pad="D27"/>
<connect gate="E" pin="IO_8_24" pad="D28"/>
<connect gate="E" pin="IO_8_25" pad="D30"/>
<connect gate="E" pin="IO_8_26" pad="D31"/>
<connect gate="E" pin="IO_8_27" pad="E19"/>
<connect gate="E" pin="IO_8_28" pad="E20"/>
<connect gate="E" pin="IO_8_29" pad="E22"/>
<connect gate="E" pin="IO_8_3" pad="F20"/>
<connect gate="E" pin="IO_8_30" pad="E23"/>
<connect gate="E" pin="IO_8_31" pad="E25"/>
<connect gate="E" pin="IO_8_32" pad="E26"/>
<connect gate="E" pin="IO_8_33" pad="E28"/>
<connect gate="E" pin="IO_8_34" pad="E29"/>
<connect gate="E" pin="IO_8_35" pad="G23"/>
<connect gate="E" pin="IO_8_36" pad="G24"/>
<connect gate="E" pin="IO_8_4" pad="F21"/>
<connect gate="E" pin="IO_8_5" pad="F22"/>
<connect gate="E" pin="IO_8_6" pad="F23"/>
<connect gate="E" pin="IO_8_7" pad="F24"/>
<connect gate="E" pin="IO_8_8" pad="F25"/>
<connect gate="E" pin="IO_8_9" pad="F26"/>
<connect gate="E" pin="IO_8_PLL_T1_FBP/CLKOUT1" pad="D18"/>
<connect gate="E" pin="IO_8_RDN8A" pad="G26"/>
<connect gate="E" pin="NC" pad="D32"/>
<connect gate="E" pin="TCK" pad="F30"/>
<connect gate="E" pin="TDI" pad="G28"/>
<connect gate="E" pin="TDO" pad="G29"/>
<connect gate="E" pin="VCCA_PLL_T1" pad="G18"/>
<connect gate="E" pin="VCCA_PLL_T2" pad="G17"/>
<connect gate="E" pin="VCCIO1A" pad="G32"/>
<connect gate="E" pin="VCCIO7A" pad="F10"/>
<connect gate="E" pin="VCCIO7C" pad="F17"/>
<connect gate="E" pin="VCCIO7C_2" pad="G14"/>
<connect gate="E" pin="VCCIO8A" pad="D29"/>
<connect gate="E" pin="VCCIO8A_2" pad="G25"/>
<connect gate="E" pin="VCCIO8B" pad="G22"/>
<connect gate="E" pin="VCCPT" pad="F18"/>
<connect gate="E" pin="VREF7A" pad="H10"/>
<connect gate="E" pin="VREF7C" pad="G15"/>
<connect gate="E" pin="VREF8C" pad="G19"/>
<connect gate="F" pin="GND" pad="L24"/>
<connect gate="F" pin="GND_10" pad="H33"/>
<connect gate="F" pin="GND_11" pad="H21"/>
<connect gate="F" pin="GND_12" pad="L15"/>
<connect gate="F" pin="GND_13" pad="L30"/>
<connect gate="F" pin="GND_14" pad="L18"/>
<connect gate="F" pin="GND_15" pad="L21"/>
<connect gate="F" pin="GND_2" pad="H15"/>
<connect gate="F" pin="GND_3" pad="L12"/>
<connect gate="F" pin="GND_4" pad="H12"/>
<connect gate="F" pin="GND_5" pad="H24"/>
<connect gate="F" pin="GND_6" pad="H30"/>
<connect gate="F" pin="GND_7" pad="L27"/>
<connect gate="F" pin="GND_8" pad="H18"/>
<connect gate="F" pin="GND_9" pad="H27"/>
<connect gate="F" pin="IO_1" pad="L32"/>
<connect gate="F" pin="IO_1_10" pad="J34"/>
<connect gate="F" pin="IO_1_11" pad="K27"/>
<connect gate="F" pin="IO_1_12" pad="K28"/>
<connect gate="F" pin="IO_1_13" pad="K29"/>
<connect gate="F" pin="IO_1_14" pad="K30"/>
<connect gate="F" pin="IO_1_15" pad="K31"/>
<connect gate="F" pin="IO_1_16" pad="K32"/>
<connect gate="F" pin="IO_1_17" pad="K33"/>
<connect gate="F" pin="IO_1_18" pad="K34"/>
<connect gate="F" pin="IO_1_19" pad="L28"/>
<connect gate="F" pin="IO_1_2" pad="H31"/>
<connect gate="F" pin="IO_1_20" pad="L29"/>
<connect gate="F" pin="IO_1_21" pad="L31"/>
<connect gate="F" pin="IO_1_3" pad="H32"/>
<connect gate="F" pin="IO_1_4" pad="H34"/>
<connect gate="F" pin="IO_1_5" pad="J29"/>
<connect gate="F" pin="IO_1_6" pad="J30"/>
<connect gate="F" pin="IO_1_7" pad="J31"/>
<connect gate="F" pin="IO_1_8" pad="J32"/>
<connect gate="F" pin="IO_1_9" pad="J33"/>
<connect gate="F" pin="IO_7" pad="L14"/>
<connect gate="F" pin="IO_7_10" pad="K12"/>
<connect gate="F" pin="IO_7_11" pad="K13"/>
<connect gate="F" pin="IO_7_12" pad="K14"/>
<connect gate="F" pin="IO_7_13" pad="K15"/>
<connect gate="F" pin="IO_7_14" pad="L13"/>
<connect gate="F" pin="IO_7_2" pad="H14"/>
<connect gate="F" pin="IO_7_3" pad="H16"/>
<connect gate="F" pin="IO_7_4" pad="J11"/>
<connect gate="F" pin="IO_7_5" pad="J12"/>
<connect gate="F" pin="IO_7_6" pad="J14"/>
<connect gate="F" pin="IO_7_7" pad="J15"/>
<connect gate="F" pin="IO_7_8" pad="J16"/>
<connect gate="F" pin="IO_7_9" pad="K11"/>
<connect gate="F" pin="IO_7_PLL_T2_CLKOUT0N" pad="K17"/>
<connect gate="F" pin="IO_7_PLL_T2_CLKOUT0P" pad="L17"/>
<connect gate="F" pin="IO_7_PLL_T2_CLKOUT3" pad="K16"/>
<connect gate="F" pin="IO_7_PLL_T2_CLKOUT4" pad="L16"/>
<connect gate="F" pin="IO_8" pad="L23"/>
<connect gate="F" pin="IO_8_10" pad="K21"/>
<connect gate="F" pin="IO_8_11" pad="K22"/>
<connect gate="F" pin="IO_8_12" pad="K23"/>
<connect gate="F" pin="IO_8_13" pad="K24"/>
<connect gate="F" pin="IO_8_14" pad="K25"/>
<connect gate="F" pin="IO_8_15" pad="L22"/>
<connect gate="F" pin="IO_8_2" pad="H20"/>
<connect gate="F" pin="IO_8_3" pad="H23"/>
<connect gate="F" pin="IO_8_4" pad="J20"/>
<connect gate="F" pin="IO_8_5" pad="J21"/>
<connect gate="F" pin="IO_8_6" pad="J22"/>
<connect gate="F" pin="IO_8_7" pad="J24"/>
<connect gate="F" pin="IO_8_8" pad="J25"/>
<connect gate="F" pin="IO_8_9" pad="K20"/>
<connect gate="F" pin="IO_8_PLL_T1_CLKOUT0N" pad="J19"/>
<connect gate="F" pin="IO_8_PLL_T1_CLKOUT0P" pad="K19"/>
<connect gate="F" pin="IO_8_PLL_T1_CLKOUT3" pad="L19"/>
<connect gate="F" pin="IO_8_PLL_T1_CLKOUT4" pad="L20"/>
<connect gate="F" pin="IO_8_RUP8A" pad="H26"/>
<connect gate="F" pin="MSEL0" pad="K10"/>
<connect gate="F" pin="NC" pad="L25"/>
<connect gate="F" pin="NC_2" pad="K26"/>
<connect gate="F" pin="NC_3" pad="L11"/>
<connect gate="F" pin="TMS" pad="H28"/>
<connect gate="F" pin="TRST" pad="J28"/>
<connect gate="F" pin="VCCD_PLL_T1" pad="J18"/>
<connect gate="F" pin="VCCD_PLL_T2" pad="J17"/>
<connect gate="F" pin="VCCIO1A" pad="L26"/>
<connect gate="F" pin="VCCIO1A_2" pad="H29"/>
<connect gate="F" pin="VCCIO6A" pad="L10"/>
<connect gate="F" pin="VCCIO7A" pad="J10"/>
<connect gate="F" pin="VCCIO7B" pad="J13"/>
<connect gate="F" pin="VCCIO8A" pad="J23"/>
<connect gate="F" pin="VCCIO8C" pad="H19"/>
<connect gate="F" pin="VCCPT" pad="J27"/>
<connect gate="F" pin="VCC_CLKIN7C" pad="H17"/>
<connect gate="F" pin="VCC_CLKIN8C" pad="K18"/>
<connect gate="F" pin="VREF1A" pad="J26"/>
<connect gate="F" pin="VREF7B" pad="H13"/>
<connect gate="F" pin="VREF8A" pad="H25"/>
<connect gate="F" pin="VREF8B" pad="H22"/>
<connect gate="G" pin="GND" pad="R20"/>
<connect gate="G" pin="GND_10" pad="M17"/>
<connect gate="G" pin="GND_11" pad="N20"/>
<connect gate="G" pin="GND_12" pad="M21"/>
<connect gate="G" pin="GND_13" pad="N22"/>
<connect gate="G" pin="GND_14" pad="P24"/>
<connect gate="G" pin="GND_15" pad="R22"/>
<connect gate="G" pin="GND_16" pad="P27"/>
<connect gate="G" pin="GND_17" pad="P30"/>
<connect gate="G" pin="GND_18" pad="P33"/>
<connect gate="G" pin="GND_19" pad="R11"/>
<connect gate="G" pin="GND_2" pad="N16"/>
<connect gate="G" pin="GND_20" pad="P15"/>
<connect gate="G" pin="GND_21" pad="P13"/>
<connect gate="G" pin="GND_22" pad="R14"/>
<connect gate="G" pin="GND_23" pad="P17"/>
<connect gate="G" pin="GND_24" pad="R16"/>
<connect gate="G" pin="GND_25" pad="P19"/>
<connect gate="G" pin="GND_26" pad="R18"/>
<connect gate="G" pin="GND_27" pad="P21"/>
<connect gate="G" pin="GND_3" pad="M15"/>
<connect gate="G" pin="GND_4" pad="M19"/>
<connect gate="G" pin="GND_5" pad="N12"/>
<connect gate="G" pin="GND_6" pad="N18"/>
<connect gate="G" pin="GND_7" pad="M11"/>
<connect gate="G" pin="GND_8" pad="L33"/>
<connect gate="G" pin="GND_9" pad="N14"/>
<connect gate="G" pin="IO_1" pad="P29"/>
<connect gate="G" pin="IO_1_10" pad="L34"/>
<connect gate="G" pin="IO_1_11" pad="M24"/>
<connect gate="G" pin="IO_1_12" pad="M26"/>
<connect gate="G" pin="IO_1_13" pad="M27"/>
<connect gate="G" pin="IO_1_14" pad="M28"/>
<connect gate="G" pin="IO_1_15" pad="M29"/>
<connect gate="G" pin="IO_1_16" pad="M30"/>
<connect gate="G" pin="IO_1_17" pad="M31"/>
<connect gate="G" pin="IO_1_18" pad="M33"/>
<connect gate="G" pin="IO_1_19" pad="M34"/>
<connect gate="G" pin="IO_1_2" pad="P31"/>
<connect gate="G" pin="IO_1_20" pad="N24"/>
<connect gate="G" pin="IO_1_21" pad="N25"/>
<connect gate="G" pin="IO_1_22" pad="N26"/>
<connect gate="G" pin="IO_1_23" pad="N27"/>
<connect gate="G" pin="IO_1_24" pad="N29"/>
<connect gate="G" pin="IO_1_25" pad="N30"/>
<connect gate="G" pin="IO_1_26" pad="N31"/>
<connect gate="G" pin="IO_1_27" pad="N32"/>
<connect gate="G" pin="IO_1_28" pad="N33"/>
<connect gate="G" pin="IO_1_29" pad="N34"/>
<connect gate="G" pin="IO_1_3" pad="P32"/>
<connect gate="G" pin="IO_1_30" pad="P23"/>
<connect gate="G" pin="IO_1_31" pad="P25"/>
<connect gate="G" pin="IO_1_32" pad="P28"/>
<connect gate="G" pin="IO_1_4" pad="P34"/>
<connect gate="G" pin="IO_1_5" pad="R24"/>
<connect gate="G" pin="IO_1_6" pad="R25"/>
<connect gate="G" pin="IO_1_7" pad="R26"/>
<connect gate="G" pin="IO_1_8" pad="R27"/>
<connect gate="G" pin="IO_1_9" pad="R28"/>
<connect gate="G" pin="IO_6" pad="P11"/>
<connect gate="G" pin="IO_6_2" pad="R10"/>
<connect gate="G" pin="IO_6_3" pad="R12"/>
<connect gate="G" pin="IO_6_4" pad="M10"/>
<connect gate="G" pin="IO_6_5" pad="N10"/>
<connect gate="G" pin="IO_6_6" pad="N11"/>
<connect gate="G" pin="IO_6_7" pad="P10"/>
<connect gate="G" pin="IO_7" pad="M13"/>
<connect gate="G" pin="IO_8" pad="M23"/>
<connect gate="G" pin="NC" pad="M25"/>
<connect gate="G" pin="VCC" pad="R13"/>
<connect gate="G" pin="VCCIO1A" pad="N28"/>
<connect gate="G" pin="VCCIO1C" pad="M32"/>
<connect gate="G" pin="VCCL" pad="R17"/>
<connect gate="G" pin="VCCL_10" pad="R19"/>
<connect gate="G" pin="VCCL_11" pad="R21"/>
<connect gate="G" pin="VCCL_2" pad="N21"/>
<connect gate="G" pin="VCCL_3" pad="N13"/>
<connect gate="G" pin="VCCL_4" pad="P18"/>
<connect gate="G" pin="VCCL_5" pad="P14"/>
<connect gate="G" pin="VCCL_6" pad="P16"/>
<connect gate="G" pin="VCCL_7" pad="P20"/>
<connect gate="G" pin="VCCL_8" pad="P22"/>
<connect gate="G" pin="VCCL_9" pad="R15"/>
<connect gate="G" pin="VCCPD1A" pad="N23"/>
<connect gate="G" pin="VCCPD1C" pad="R23"/>
<connect gate="G" pin="VCCPD6A" pad="P12"/>
<connect gate="G" pin="VCCPD7A" pad="M12"/>
<connect gate="G" pin="VCCPD7B" pad="M14"/>
<connect gate="G" pin="VCCPD7C" pad="M16"/>
<connect gate="G" pin="VCCPD8A" pad="M22"/>
<connect gate="G" pin="VCCPD8B" pad="M20"/>
<connect gate="G" pin="VCCPD8C" pad="M18"/>
<connect gate="G" pin="VCC_2" pad="N19"/>
<connect gate="G" pin="VCC_3" pad="N15"/>
<connect gate="G" pin="VCC_4" pad="N17"/>
<connect gate="G" pin="VREF1C" pad="P26"/>
<connect gate="H" pin="CLK1N" pad="T34"/>
<connect gate="H" pin="CLK1P" pad="T33"/>
<connect gate="H" pin="CLK3N" pad="V34"/>
<connect gate="H" pin="CLK3P" pad="V33"/>
<connect gate="H" pin="DNU" pad="U18"/>
<connect gate="H" pin="GND" pad="U16"/>
<connect gate="H" pin="GND_10" pad="U20"/>
<connect gate="H" pin="GND_11" pad="V23"/>
<connect gate="H" pin="GND_12" pad="U24"/>
<connect gate="H" pin="GND_13" pad="W16"/>
<connect gate="H" pin="GND_14" pad="T21"/>
<connect gate="H" pin="GND_15" pad="U12"/>
<connect gate="H" pin="GND_16" pad="T13"/>
<connect gate="H" pin="GND_17" pad="U30"/>
<connect gate="H" pin="GND_18" pad="V17"/>
<connect gate="H" pin="GND_19" pad="T19"/>
<connect gate="H" pin="GND_2" pad="W22"/>
<connect gate="H" pin="GND_20" pad="V19"/>
<connect gate="H" pin="GND_21" pad="V11"/>
<connect gate="H" pin="GND_22" pad="U33"/>
<connect gate="H" pin="GND_23" pad="V15"/>
<connect gate="H" pin="GND_24" pad="V12"/>
<connect gate="H" pin="GND_25" pad="T17"/>
<connect gate="H" pin="GND_26" pad="V13"/>
<connect gate="H" pin="GND_27" pad="U14"/>
<connect gate="H" pin="GND_28" pad="U27"/>
<connect gate="H" pin="GND_3" pad="V21"/>
<connect gate="H" pin="GND_4" pad="T15"/>
<connect gate="H" pin="GND_5" pad="W18"/>
<connect gate="H" pin="GND_6" pad="U22"/>
<connect gate="H" pin="GND_7" pad="W14"/>
<connect gate="H" pin="GND_8" pad="U23"/>
<connect gate="H" pin="GND_9" pad="W20"/>
<connect gate="H" pin="IO_1" pad="U32"/>
<connect gate="H" pin="IO_1_10" pad="T25"/>
<connect gate="H" pin="IO_1_11" pad="T26"/>
<connect gate="H" pin="IO_1_12" pad="T27"/>
<connect gate="H" pin="IO_1_13" pad="T28"/>
<connect gate="H" pin="IO_1_14" pad="T32"/>
<connect gate="H" pin="IO_1_15" pad="U25"/>
<connect gate="H" pin="IO_1_16" pad="U31"/>
<connect gate="H" pin="IO_1_2" pad="R29"/>
<connect gate="H" pin="IO_1_3" pad="R30"/>
<connect gate="H" pin="IO_1_4" pad="R31"/>
<connect gate="H" pin="IO_1_5" pad="R32"/>
<connect gate="H" pin="IO_1_6" pad="R33"/>
<connect gate="H" pin="IO_1_7" pad="R34"/>
<connect gate="H" pin="IO_1_8" pad="T23"/>
<connect gate="H" pin="IO_1_9" pad="T24"/>
<connect gate="H" pin="IO_1_CLK0N" pad="V32"/>
<connect gate="H" pin="IO_1_CLK0P" pad="V31"/>
<connect gate="H" pin="IO_1_PLL_L2_CLKOUT0N" pad="T30"/>
<connect gate="H" pin="IO_1_PLL_L2_FB_CLKOUT0P" pad="T29"/>
<connect gate="H" pin="IO_2" pad="W24"/>
<connect gate="H" pin="IO_2_2" pad="V24"/>
<connect gate="H" pin="IO_2_3" pad="V25"/>
<connect gate="H" pin="IO_2_PLL_L3_CLKOUT0N" pad="V29"/>
<connect gate="H" pin="IO_5" pad="W12"/>
<connect gate="H" pin="IO_5_2" pad="W10"/>
<connect gate="H" pin="IO_5_3" pad="W11"/>
<connect gate="H" pin="IO_5_PLL_R3_FB_CLKOUT0P" pad="V10"/>
<connect gate="H" pin="IO_6" pad="T11"/>
<connect gate="H" pin="IO_6_PLL_R2_CLKOUT0N" pad="U10"/>
<connect gate="H" pin="IO_6_PLL_R2_FB_CLKOUT0P" pad="U11"/>
<connect gate="H" pin="VCC" pad="V22"/>
<connect gate="H" pin="VCCA_PLL_L2" pad="U28"/>
<connect gate="H" pin="VCCA_PLL_L3" pad="V28"/>
<connect gate="H" pin="VCCD_PLL_L2" pad="U26"/>
<connect gate="H" pin="VCCD_PLL_L3" pad="V26"/>
<connect gate="H" pin="VCCIO1C" pad="V30"/>
<connect gate="H" pin="VCCIO1C_2" pad="T31"/>
<connect gate="H" pin="VCCIO1C_3" pad="U34"/>
<connect gate="H" pin="VCCIO6C" pad="T10"/>
<connect gate="H" pin="VCCL" pad="W17"/>
<connect gate="H" pin="VCCL_10" pad="U17"/>
<connect gate="H" pin="VCCL_11" pad="V18"/>
<connect gate="H" pin="VCCL_12" pad="T20"/>
<connect gate="H" pin="VCCL_13" pad="W21"/>
<connect gate="H" pin="VCCL_14" pad="V20"/>
<connect gate="H" pin="VCCL_15" pad="W19"/>
<connect gate="H" pin="VCCL_16" pad="W15"/>
<connect gate="H" pin="VCCL_2" pad="T14"/>
<connect gate="H" pin="VCCL_3" pad="U19"/>
<connect gate="H" pin="VCCL_4" pad="V14"/>
<connect gate="H" pin="VCCL_5" pad="T16"/>
<connect gate="H" pin="VCCL_6" pad="U21"/>
<connect gate="H" pin="VCCL_7" pad="V16"/>
<connect gate="H" pin="VCCL_8" pad="T18"/>
<connect gate="H" pin="VCCL_9" pad="U15"/>
<connect gate="H" pin="VCCPD2C" pad="W23"/>
<connect gate="H" pin="VCCPD6C" pad="T12"/>
<connect gate="H" pin="VCCPT" pad="U29"/>
<connect gate="H" pin="VCC_2" pad="T22"/>
<connect gate="H" pin="VCC_3" pad="U13"/>
<connect gate="H" pin="VCC_4" pad="W13"/>
<connect gate="H" pin="VREF2C" pad="V27"/>
<connect gate="I" pin="GND" pad="AC18"/>
<connect gate="I" pin="GND_10" pad="AB13"/>
<connect gate="I" pin="GND_11" pad="Y30"/>
<connect gate="I" pin="GND_12" pad="AA20"/>
<connect gate="I" pin="GND_13" pad="Y13"/>
<connect gate="I" pin="GND_14" pad="AB17"/>
<connect gate="I" pin="GND_15" pad="Y15"/>
<connect gate="I" pin="GND_16" pad="Y33"/>
<connect gate="I" pin="GND_17" pad="Y17"/>
<connect gate="I" pin="GND_18" pad="AB19"/>
<connect gate="I" pin="GND_19" pad="Y19"/>
<connect gate="I" pin="GND_2" pad="AC20"/>
<connect gate="I" pin="GND_20" pad="AA11"/>
<connect gate="I" pin="GND_21" pad="Y21"/>
<connect gate="I" pin="GND_22" pad="AB15"/>
<connect gate="I" pin="GND_23" pad="AC14"/>
<connect gate="I" pin="GND_24" pad="AB21"/>
<connect gate="I" pin="GND_25" pad="AC16"/>
<connect gate="I" pin="GND_3" pad="AA14"/>
<connect gate="I" pin="GND_4" pad="AA22"/>
<connect gate="I" pin="GND_5" pad="Y24"/>
<connect gate="I" pin="GND_6" pad="AA16"/>
<connect gate="I" pin="GND_7" pad="AB23"/>
<connect gate="I" pin="GND_8" pad="Y27"/>
<connect gate="I" pin="GND_9" pad="AA18"/>
<connect gate="I" pin="IO_2" pad="AB34"/>
<connect gate="I" pin="IO_2_10" pad="Y29"/>
<connect gate="I" pin="IO_2_11" pad="Y31"/>
<connect gate="I" pin="IO_2_12" pad="Y32"/>
<connect gate="I" pin="IO_2_13" pad="Y34"/>
<connect gate="I" pin="IO_2_14" pad="AA24"/>
<connect gate="I" pin="IO_2_15" pad="AA25"/>
<connect gate="I" pin="IO_2_16" pad="AA27"/>
<connect gate="I" pin="IO_2_17" pad="AA28"/>
<connect gate="I" pin="IO_2_18" pad="AA29"/>
<connect gate="I" pin="IO_2_19" pad="AA30"/>
<connect gate="I" pin="IO_2_2" pad="W26"/>
<connect gate="I" pin="IO_2_20" pad="AA31"/>
<connect gate="I" pin="IO_2_21" pad="AA32"/>
<connect gate="I" pin="IO_2_22" pad="AA33"/>
<connect gate="I" pin="IO_2_23" pad="AA34"/>
<connect gate="I" pin="IO_2_24" pad="AB24"/>
<connect gate="I" pin="IO_2_25" pad="AB25"/>
<connect gate="I" pin="IO_2_26" pad="AB26"/>
<connect gate="I" pin="IO_2_27" pad="AB27"/>
<connect gate="I" pin="IO_2_28" pad="AB29"/>
<connect gate="I" pin="IO_2_29" pad="AB30"/>
<connect gate="I" pin="IO_2_3" pad="W27"/>
<connect gate="I" pin="IO_2_30" pad="AB31"/>
<connect gate="I" pin="IO_2_31" pad="AB32"/>
<connect gate="I" pin="IO_2_32" pad="AB33"/>
<connect gate="I" pin="IO_2_4" pad="W30"/>
<connect gate="I" pin="IO_2_5" pad="W31"/>
<connect gate="I" pin="IO_2_6" pad="Y23"/>
<connect gate="I" pin="IO_2_7" pad="Y25"/>
<connect gate="I" pin="IO_2_8" pad="Y26"/>
<connect gate="I" pin="IO_2_9" pad="Y28"/>
<connect gate="I" pin="IO_2_CLK2N" pad="W34"/>
<connect gate="I" pin="IO_2_CLK2P" pad="W33"/>
<connect gate="I" pin="IO_2_PLL_L3_FB_CLKOUT0P" pad="W28"/>
<connect gate="I" pin="IO_4" pad="AC12"/>
<connect gate="I" pin="IO_5" pad="AC11"/>
<connect gate="I" pin="IO_5_2" pad="Y10"/>
<connect gate="I" pin="IO_5_3" pad="Y11"/>
<connect gate="I" pin="IO_5_4" pad="AA10"/>
<connect gate="I" pin="IO_5_5" pad="AA12"/>
<connect gate="I" pin="IO_5_6" pad="AB10"/>
<connect gate="I" pin="IO_5_7" pad="AB11"/>
<connect gate="I" pin="NC" pad="AC10"/>
<connect gate="I" pin="VCC" pad="Y22"/>
<connect gate="I" pin="VCCIO2A" pad="AB28"/>
<connect gate="I" pin="VCCIO2C" pad="W32"/>
<connect gate="I" pin="VCCIO2C_2" pad="W25"/>
<connect gate="I" pin="VCCIO2C_3" pad="W29"/>
<connect gate="I" pin="VCCL" pad="AB22"/>
<connect gate="I" pin="VCCL_10" pad="AA15"/>
<connect gate="I" pin="VCCL_11" pad="AB14"/>
<connect gate="I" pin="VCCL_2" pad="Y14"/>
<connect gate="I" pin="VCCL_3" pad="Y16"/>
<connect gate="I" pin="VCCL_4" pad="AA21"/>
<connect gate="I" pin="VCCL_5" pad="Y18"/>
<connect gate="I" pin="VCCL_6" pad="AA17"/>
<connect gate="I" pin="VCCL_7" pad="AA19"/>
<connect gate="I" pin="VCCL_8" pad="Y20"/>
<connect gate="I" pin="VCCL_9" pad="AA13"/>
<connect gate="I" pin="VCCPD2A" pad="AA23"/>
<connect gate="I" pin="VCCPD3C" pad="AC19"/>
<connect gate="I" pin="VCCPD4A" pad="AC13"/>
<connect gate="I" pin="VCCPD4B" pad="AC15"/>
<connect gate="I" pin="VCCPD4C" pad="AC17"/>
<connect gate="I" pin="VCCPD5A" pad="AB12"/>
<connect gate="I" pin="VCCPD5C" pad="Y12"/>
<connect gate="I" pin="VCC_2" pad="AB16"/>
<connect gate="I" pin="VCC_3" pad="AB18"/>
<connect gate="I" pin="VCC_4" pad="AB20"/>
<connect gate="I" pin="VREF2A" pad="AA26"/>
<connect gate="J" pin="GND" pad="AG14"/>
<connect gate="J" pin="GND_10" pad="AD23"/>
<connect gate="J" pin="GND_11" pad="AF27"/>
<connect gate="J" pin="GND_12" pad="AG11"/>
<connect gate="J" pin="GND_13" pad="AF30"/>
<connect gate="J" pin="GND_14" pad="AF33"/>
<connect gate="J" pin="GND_2" pad="AD11"/>
<connect gate="J" pin="GND_3" pad="AC24"/>
<connect gate="J" pin="GND_4" pad="AD14"/>
<connect gate="J" pin="GND_5" pad="AC27"/>
<connect gate="J" pin="GND_6" pad="AD17"/>
<connect gate="J" pin="GND_7" pad="AC30"/>
<connect gate="J" pin="GND_8" pad="AD20"/>
<connect gate="J" pin="GND_9" pad="AC33"/>
<connect gate="J" pin="IO_2" pad="AF34"/>
<connect gate="J" pin="IO_2_10" pad="AD27"/>
<connect gate="J" pin="IO_2_11" pad="AD28"/>
<connect gate="J" pin="IO_2_12" pad="AD29"/>
<connect gate="J" pin="IO_2_13" pad="AD30"/>
<connect gate="J" pin="IO_2_14" pad="AD31"/>
<connect gate="J" pin="IO_2_15" pad="AD33"/>
<connect gate="J" pin="IO_2_16" pad="AD34"/>
<connect gate="J" pin="IO_2_17" pad="AE27"/>
<connect gate="J" pin="IO_2_18" pad="AE28"/>
<connect gate="J" pin="IO_2_19" pad="AE29"/>
<connect gate="J" pin="IO_2_2" pad="AC25"/>
<connect gate="J" pin="IO_2_20" pad="AE30"/>
<connect gate="J" pin="IO_2_21" pad="AE31"/>
<connect gate="J" pin="IO_2_22" pad="AE32"/>
<connect gate="J" pin="IO_2_23" pad="AE33"/>
<connect gate="J" pin="IO_2_24" pad="AE34"/>
<connect gate="J" pin="IO_2_25" pad="AF28"/>
<connect gate="J" pin="IO_2_26" pad="AF29"/>
<connect gate="J" pin="IO_2_27" pad="AF31"/>
<connect gate="J" pin="IO_2_28" pad="AF32"/>
<connect gate="J" pin="IO_2_3" pad="AC26"/>
<connect gate="J" pin="IO_2_4" pad="AC28"/>
<connect gate="J" pin="IO_2_5" pad="AC29"/>
<connect gate="J" pin="IO_2_6" pad="AC31"/>
<connect gate="J" pin="IO_2_7" pad="AC32"/>
<connect gate="J" pin="IO_2_8" pad="AC34"/>
<connect gate="J" pin="IO_2_9" pad="AD26"/>
<connect gate="J" pin="IO_3" pad="AF24"/>
<connect gate="J" pin="IO_3_10" pad="AF19"/>
<connect gate="J" pin="IO_3_11" pad="AF20"/>
<connect gate="J" pin="IO_3_12" pad="AF21"/>
<connect gate="J" pin="IO_3_13" pad="AF23"/>
<connect gate="J" pin="IO_3_2" pad="AC22"/>
<connect gate="J" pin="IO_3_3" pad="AD21"/>
<connect gate="J" pin="IO_3_4" pad="AD22"/>
<connect gate="J" pin="IO_3_5" pad="AE20"/>
<connect gate="J" pin="IO_3_6" pad="AE21"/>
<connect gate="J" pin="IO_3_7" pad="AE22"/>
<connect gate="J" pin="IO_3_8" pad="AE23"/>
<connect gate="J" pin="IO_3_9" pad="AE24"/>
<connect gate="J" pin="IO_3_PLL_B1_CLKOUT0N" pad="AE18"/>
<connect gate="J" pin="IO_3_PLL_B1_CLKOUT0P" pad="AD18"/>
<connect gate="J" pin="IO_3_PLL_B1_CLKOUT3" pad="AD19"/>
<connect gate="J" pin="IO_3_PLL_B1_CLKOUT4" pad="AE19"/>
<connect gate="J" pin="IO_4" pad="AG15"/>
<connect gate="J" pin="IO_4_10" pad="AF10"/>
<connect gate="J" pin="IO_4_11" pad="AF11"/>
<connect gate="J" pin="IO_4_12" pad="AF13"/>
<connect gate="J" pin="IO_4_13" pad="AF14"/>
<connect gate="J" pin="IO_4_14" pad="AF15"/>
<connect gate="J" pin="IO_4_15" pad="AG12"/>
<connect gate="J" pin="IO_4_2" pad="AD12"/>
<connect gate="J" pin="IO_4_3" pad="AD13"/>
<connect gate="J" pin="IO_4_4" pad="AE10"/>
<connect gate="J" pin="IO_4_5" pad="AE11"/>
<connect gate="J" pin="IO_4_6" pad="AE12"/>
<connect gate="J" pin="IO_4_7" pad="AE13"/>
<connect gate="J" pin="IO_4_8" pad="AE14"/>
<connect gate="J" pin="IO_4_9" pad="AE15"/>
<connect gate="J" pin="IO_4_PLL_B2_CLKOUT0N" pad="AF16"/>
<connect gate="J" pin="IO_4_PLL_B2_CLKOUT0P" pad="AE16"/>
<connect gate="J" pin="IO_4_PLL_B2_CLKOUT3" pad="AD15"/>
<connect gate="J" pin="IO_4_PLL_B2_CLKOUT4" pad="AD16"/>
<connect gate="J" pin="NCE" pad="AE26"/>
<connect gate="J" pin="NCONFIG" pad="AE25"/>
<connect gate="J" pin="PORSEL" pad="AF26"/>
<connect gate="J" pin="VCCD_PLL_B1" pad="AF18"/>
<connect gate="J" pin="VCCD_PLL_B2" pad="AF17"/>
<connect gate="J" pin="VCCIO2A" pad="AD25"/>
<connect gate="J" pin="VCCIO2C" pad="AD32"/>
<connect gate="J" pin="VCCIO3A" pad="AF25"/>
<connect gate="J" pin="VCCIO3B" pad="AF22"/>
<connect gate="J" pin="VCCIO4A" pad="AF12"/>
<connect gate="J" pin="VCCIO4C" pad="AG16"/>
<connect gate="J" pin="VCCPD3A" pad="AC23"/>
<connect gate="J" pin="VCCPD3B" pad="AC21"/>
<connect gate="J" pin="VCCPGM" pad="AD10"/>
<connect gate="J" pin="VCCPGM_2" pad="AD24"/>
<connect gate="J" pin="VCC_CLKIN4C" pad="AE17"/>
<connect gate="J" pin="VREF4A" pad="AG10"/>
<connect gate="J" pin="VREF4B" pad="AG13"/>
<connect gate="K" pin="CONF_DONE" pad="AH29"/>
<connect gate="K" pin="GND" pad="AK29"/>
<connect gate="K" pin="GND_10" pad="AK17"/>
<connect gate="K" pin="GND_11" pad="AK20"/>
<connect gate="K" pin="GND_12" pad="AK23"/>
<connect gate="K" pin="GND_13" pad="AK26"/>
<connect gate="K" pin="GND_2" pad="AJ30"/>
<connect gate="K" pin="GND_3" pad="AG26"/>
<connect gate="K" pin="GND_4" pad="AJ33"/>
<connect gate="K" pin="GND_5" pad="AG17"/>
<connect gate="K" pin="GND_6" pad="AK11"/>
<connect gate="K" pin="GND_7" pad="AG23"/>
<connect gate="K" pin="GND_8" pad="AK14"/>
<connect gate="K" pin="GND_9" pad="AG20"/>
<connect gate="K" pin="IO_2" pad="AK34"/>
<connect gate="K" pin="IO_2_10" pad="AH33"/>
<connect gate="K" pin="IO_2_11" pad="AH34"/>
<connect gate="K" pin="IO_2_12" pad="AJ31"/>
<connect gate="K" pin="IO_2_13" pad="AJ32"/>
<connect gate="K" pin="IO_2_14" pad="AJ34"/>
<connect gate="K" pin="IO_2_15" pad="AK33"/>
<connect gate="K" pin="IO_2_2" pad="AG29"/>
<connect gate="K" pin="IO_2_3" pad="AG30"/>
<connect gate="K" pin="IO_2_4" pad="AG31"/>
<connect gate="K" pin="IO_2_5" pad="AG32"/>
<connect gate="K" pin="IO_2_6" pad="AG33"/>
<connect gate="K" pin="IO_2_7" pad="AG34"/>
<connect gate="K" pin="IO_2_8" pad="AH30"/>
<connect gate="K" pin="IO_2_9" pad="AH31"/>
<connect gate="K" pin="IO_2_RDN2A" pad="AK32"/>
<connect gate="K" pin="IO_2_RUP2A" pad="AK31"/>
<connect gate="K" pin="IO_3" pad="AK27"/>
<connect gate="K" pin="IO_3_10" pad="AH26"/>
<connect gate="K" pin="IO_3_11" pad="AH27"/>
<connect gate="K" pin="IO_3_12" pad="AJ20"/>
<connect gate="K" pin="IO_3_13" pad="AJ21"/>
<connect gate="K" pin="IO_3_14" pad="AJ22"/>
<connect gate="K" pin="IO_3_15" pad="AJ23"/>
<connect gate="K" pin="IO_3_16" pad="AJ24"/>
<connect gate="K" pin="IO_3_17" pad="AJ26"/>
<connect gate="K" pin="IO_3_18" pad="AJ27"/>
<connect gate="K" pin="IO_3_19" pad="AJ29"/>
<connect gate="K" pin="IO_3_2" pad="AG19"/>
<connect gate="K" pin="IO_3_20" pad="AK18"/>
<connect gate="K" pin="IO_3_21" pad="AK21"/>
<connect gate="K" pin="IO_3_22" pad="AK22"/>
<connect gate="K" pin="IO_3_23" pad="AK24"/>
<connect gate="K" pin="IO_3_24" pad="AK25"/>
<connect gate="K" pin="IO_3_3" pad="AG21"/>
<connect gate="K" pin="IO_3_4" pad="AG24"/>
<connect gate="K" pin="IO_3_5" pad="AH19"/>
<connect gate="K" pin="IO_3_6" pad="AH22"/>
<connect gate="K" pin="IO_3_7" pad="AH23"/>
<connect gate="K" pin="IO_3_8" pad="AH24"/>
<connect gate="K" pin="IO_3_9" pad="AH25"/>
<connect gate="K" pin="IO_3_PLL_B1_FBN/CLKOUT2" pad="AK19"/>
<connect gate="K" pin="IO_3_PLL_B1_FBP/CLKOUT1" pad="AJ19"/>
<connect gate="K" pin="IO_3_RDN3A" pad="AK28"/>
<connect gate="K" pin="IO_3_RUP3A" pad="AJ28"/>
<connect gate="K" pin="IO_4" pad="AL12"/>
<connect gate="K" pin="IO_4_10" pad="AJ14"/>
<connect gate="K" pin="IO_4_11" pad="AJ15"/>
<connect gate="K" pin="IO_4_12" pad="AJ16"/>
<connect gate="K" pin="IO_4_13" pad="AK10"/>
<connect gate="K" pin="IO_4_14" pad="AK12"/>
<connect gate="K" pin="IO_4_15" pad="AK13"/>
<connect gate="K" pin="IO_4_16" pad="AK15"/>
<connect gate="K" pin="IO_4_17" pad="AK16"/>
<connect gate="K" pin="IO_4_18" pad="AL10"/>
<connect gate="K" pin="IO_4_19" pad="AL11"/>
<connect gate="K" pin="IO_4_2" pad="AH11"/>
<connect gate="K" pin="IO_4_3" pad="AH12"/>
<connect gate="K" pin="IO_4_4" pad="AH14"/>
<connect gate="K" pin="IO_4_5" pad="AH15"/>
<connect gate="K" pin="IO_4_6" pad="AJ10"/>
<connect gate="K" pin="IO_4_7" pad="AJ11"/>
<connect gate="K" pin="IO_4_8" pad="AJ12"/>
<connect gate="K" pin="IO_4_9" pad="AJ13"/>
<connect gate="K" pin="NC" pad="AK30"/>
<connect gate="K" pin="NSTATUS" pad="AH28"/>
<connect gate="K" pin="VCCA_PLL_B1" pad="AH18"/>
<connect gate="K" pin="VCCA_PLL_B2" pad="AH17"/>
<connect gate="K" pin="VCCIO2A" pad="AH32"/>
<connect gate="K" pin="VCCIO2A_2" pad="AG28"/>
<connect gate="K" pin="VCCIO3A" pad="AJ25"/>
<connect gate="K" pin="VCCIO3C" pad="AJ18"/>
<connect gate="K" pin="VCCIO3C_2" pad="AH21"/>
<connect gate="K" pin="VCCIO4A" pad="AH10"/>
<connect gate="K" pin="VCCIO4B" pad="AH13"/>
<connect gate="K" pin="VCCPT" pad="AJ17"/>
<connect gate="K" pin="VCCPT_2" pad="AG27"/>
<connect gate="K" pin="VCC_CLKIN3C" pad="AG18"/>
<connect gate="K" pin="VREF3A" pad="AG25"/>
<connect gate="K" pin="VREF3B" pad="AG22"/>
<connect gate="K" pin="VREF3C" pad="AH20"/>
<connect gate="K" pin="VREF4C" pad="AH16"/>
<connect gate="L" pin="GND" pad="AN32"/>
<connect gate="L" pin="GND_2" pad="AM33"/>
<connect gate="L" pin="GND_3" pad="AN11"/>
<connect gate="L" pin="GND_4" pad="AN14"/>
<connect gate="L" pin="GND_5" pad="AN17"/>
<connect gate="L" pin="GND_6" pad="AN20"/>
<connect gate="L" pin="GND_7" pad="AN23"/>
<connect gate="L" pin="GND_8" pad="AN26"/>
<connect gate="L" pin="GND_9" pad="AN29"/>
<connect gate="L" pin="IO_2" pad="AM34"/>
<connect gate="L" pin="IO_2_2" pad="AL32"/>
<connect gate="L" pin="IO_2_3" pad="AL33"/>
<connect gate="L" pin="IO_2_4" pad="AL34"/>
<connect gate="L" pin="IO_3" pad="AP33"/>
<connect gate="L" pin="IO_3_10" pad="AL26"/>
<connect gate="L" pin="IO_3_11" pad="AL27"/>
<connect gate="L" pin="IO_3_12" pad="AL28"/>
<connect gate="L" pin="IO_3_13" pad="AL29"/>
<connect gate="L" pin="IO_3_14" pad="AM18"/>
<connect gate="L" pin="IO_3_15" pad="AM19"/>
<connect gate="L" pin="IO_3_16" pad="AM21"/>
<connect gate="L" pin="IO_3_17" pad="AM22"/>
<connect gate="L" pin="IO_3_18" pad="AM23"/>
<connect gate="L" pin="IO_3_19" pad="AM24"/>
<connect gate="L" pin="IO_3_2" pad="AL18"/>
<connect gate="L" pin="IO_3_20" pad="AM26"/>
<connect gate="L" pin="IO_3_21" pad="AM28"/>
<connect gate="L" pin="IO_3_22" pad="AM29"/>
<connect gate="L" pin="IO_3_23" pad="AM30"/>
<connect gate="L" pin="IO_3_24" pad="AM31"/>
<connect gate="L" pin="IO_3_25" pad="AM32"/>
<connect gate="L" pin="IO_3_26" pad="AN21"/>
<connect gate="L" pin="IO_3_27" pad="AN22"/>
<connect gate="L" pin="IO_3_28" pad="AN24"/>
<connect gate="L" pin="IO_3_29" pad="AN25"/>
<connect gate="L" pin="IO_3_3" pad="AL19"/>
<connect gate="L" pin="IO_3_30" pad="AN27"/>
<connect gate="L" pin="IO_3_31" pad="AN28"/>
<connect gate="L" pin="IO_3_32" pad="AN30"/>
<connect gate="L" pin="IO_3_33" pad="AN31"/>
<connect gate="L" pin="IO_3_34" pad="AN33"/>
<connect gate="L" pin="IO_3_35" pad="AP20"/>
<connect gate="L" pin="IO_3_36" pad="AP21"/>
<connect gate="L" pin="IO_3_37" pad="AP22"/>
<connect gate="L" pin="IO_3_38" pad="AP23"/>
<connect gate="L" pin="IO_3_39" pad="AP24"/>
<connect gate="L" pin="IO_3_4" pad="AL20"/>
<connect gate="L" pin="IO_3_40" pad="AP25"/>
<connect gate="L" pin="IO_3_41" pad="AP26"/>
<connect gate="L" pin="IO_3_42" pad="AP27"/>
<connect gate="L" pin="IO_3_43" pad="AP28"/>
<connect gate="L" pin="IO_3_44" pad="AP29"/>
<connect gate="L" pin="IO_3_45" pad="AP30"/>
<connect gate="L" pin="IO_3_46" pad="AP31"/>
<connect gate="L" pin="IO_3_47" pad="AP32"/>
<connect gate="L" pin="IO_3_5" pad="AL21"/>
<connect gate="L" pin="IO_3_6" pad="AL22"/>
<connect gate="L" pin="IO_3_7" pad="AL23"/>
<connect gate="L" pin="IO_3_8" pad="AL24"/>
<connect gate="L" pin="IO_3_9" pad="AL25"/>
<connect gate="L" pin="IO_3_CLK4N" pad="AP18"/>
<connect gate="L" pin="IO_3_CLK4P" pad="AN18"/>
<connect gate="L" pin="IO_3_CLK5N" pad="AP19"/>
<connect gate="L" pin="IO_3_CLK5P" pad="AN19"/>
<connect gate="L" pin="IO_4" pad="AP14"/>
<connect gate="L" pin="IO_4_10" pad="AL13"/>
<connect gate="L" pin="IO_4_11" pad="AL14"/>
<connect gate="L" pin="IO_4_12" pad="AL15"/>
<connect gate="L" pin="IO_4_13" pad="AL16"/>
<connect gate="L" pin="IO_4_14" pad="AP10"/>
<connect gate="L" pin="IO_4_15" pad="AP11"/>
<connect gate="L" pin="IO_4_16" pad="AP12"/>
<connect gate="L" pin="IO_4_17" pad="AP13"/>
<connect gate="L" pin="IO_4_2" pad="AM11"/>
<connect gate="L" pin="IO_4_3" pad="AM12"/>
<connect gate="L" pin="IO_4_4" pad="AM14"/>
<connect gate="L" pin="IO_4_5" pad="AM15"/>
<connect gate="L" pin="IO_4_6" pad="AM16"/>
<connect gate="L" pin="IO_4_7" pad="AN10"/>
<connect gate="L" pin="IO_4_8" pad="AN12"/>
<connect gate="L" pin="IO_4_9" pad="AN13"/>
<connect gate="L" pin="IO_4_CLK6N" pad="AP16"/>
<connect gate="L" pin="IO_4_CLK6P" pad="AN16"/>
<connect gate="L" pin="IO_4_CLK7N" pad="AP15"/>
<connect gate="L" pin="IO_4_CLK7P" pad="AN15"/>
<connect gate="L" pin="IO_4_PLL_B2_FBN/CLKOUT2" pad="AM17"/>
<connect gate="L" pin="IO_4_PLL_B2_FBP/CLKOUT1" pad="AL17"/>
<connect gate="L" pin="NC" pad="AL31"/>
<connect gate="L" pin="VCCIO2A" pad="AN34"/>
<connect gate="L" pin="VCCIO3A" pad="AM27"/>
<connect gate="L" pin="VCCIO3A_2" pad="AL30"/>
<connect gate="L" pin="VCCIO3B" pad="AM25"/>
<connect gate="L" pin="VCCIO3C" pad="AM20"/>
<connect gate="L" pin="VCCIO4B" pad="AM10"/>
<connect gate="L" pin="VCCIO4C" pad="AM13"/>
<connect gate="L" pin="VCCIO4C_2" pad="AP17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EP3SL150F1152C4N"/>
<attribute name="OC_FARNELL" value="1637245"/>
<attribute name="OC_NEWARK" value="51R0631"/>
<attribute name="PACKAGE" value="BGA-1152"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC1064PC8">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC1064PC8"/>
</gates>
<devices>
<device name="" package="DIP254P762X431-8">
<connects>
<connect gate="A" pin="DATA" pad="1"/>
<connect gate="A" pin="DCLK" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NCASC" pad="6"/>
<connect gate="A" pin="NCS" pad="4"/>
<connect gate="A" pin="OE" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VCC_2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC1064PC8"/>
<attribute name="OC_FARNELL" value="1783974"/>
<attribute name="OC_NEWARK" value="51R8715"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC1441LC20N">
<description>CONFIG MEMORY</description>
<gates>
<gate name="A" symbol="EPC1441LC20N"/>
</gates>
<devices>
<device name="" package="PLCC127P1000X1000X457-20N">
<connects>
<connect gate="A" pin="DATA" pad="2"/>
<connect gate="A" pin="DCLK" pad="4"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="N.C" pad="3"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NCASC" pad="12"/>
<connect gate="A" pin="NCS" pad="9"/>
<connect gate="A" pin="NC_10" pad="17"/>
<connect gate="A" pin="NC_11" pad="19"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="11"/>
<connect gate="A" pin="NC_5" pad="14"/>
<connect gate="A" pin="NC_6" pad="6"/>
<connect gate="A" pin="NC_7" pad="15"/>
<connect gate="A" pin="NC_8" pad="16"/>
<connect gate="A" pin="NC_9" pad="1"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC1441LC20N"/>
<attribute name="OC_FARNELL" value="1549341"/>
<attribute name="OC_NEWARK" value="51R0472"/>
<attribute name="PACKAGE" value="PLCC-20"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC1441TC32N" prefix="U">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC1441TC32N"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="DATA" pad="31"/>
<connect gate="A" pin="DCLK" pad="2"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="N.C" pad="6"/>
<connect gate="A" pin="N.C_10" pad="26"/>
<connect gate="A" pin="N.C_11" pad="15"/>
<connect gate="A" pin="N.C_12" pad="18"/>
<connect gate="A" pin="N.C_13" pad="5"/>
<connect gate="A" pin="N.C_14" pad="24"/>
<connect gate="A" pin="N.C_15" pad="19"/>
<connect gate="A" pin="N.C_16" pad="4"/>
<connect gate="A" pin="N.C_17" pad="29"/>
<connect gate="A" pin="N.C_18" pad="1"/>
<connect gate="A" pin="N.C_19" pad="20"/>
<connect gate="A" pin="N.C_2" pad="28"/>
<connect gate="A" pin="N.C_20" pad="21"/>
<connect gate="A" pin="N.C_21" pad="30"/>
<connect gate="A" pin="N.C_22" pad="11"/>
<connect gate="A" pin="N.C_23" pad="22"/>
<connect gate="A" pin="N.C_24" pad="9"/>
<connect gate="A" pin="N.C_25" pad="14"/>
<connect gate="A" pin="N.C_3" pad="3"/>
<connect gate="A" pin="N.C_4" pad="16"/>
<connect gate="A" pin="N.C_5" pad="17"/>
<connect gate="A" pin="N.C_6" pad="32"/>
<connect gate="A" pin="N.C_7" pad="25"/>
<connect gate="A" pin="N.C_8" pad="13"/>
<connect gate="A" pin="N.C_9" pad="8"/>
<connect gate="A" pin="NCS" pad="10"/>
<connect gate="A" pin="OE" pad="7"/>
<connect gate="A" pin="VCC" pad="27"/>
<connect gate="A" pin="VCC_2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC1441TC32N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8726"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC16QC100N">
<description>Enhanced Configuration Devices</description>
<gates>
<gate name="A" symbol="EPC16QC100N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="A10" pad="31"/>
<connect gate="A" pin="A11" pad="29"/>
<connect gate="A" pin="A12" pad="28"/>
<connect gate="A" pin="A13" pad="27"/>
<connect gate="A" pin="A14" pad="26"/>
<connect gate="A" pin="A17" pad="49"/>
<connect gate="A" pin="A18" pad="47"/>
<connect gate="A" pin="A19" pad="46"/>
<connect gate="A" pin="A2" pad="55"/>
<connect gate="A" pin="A3" pad="54"/>
<connect gate="A" pin="A4" pad="53"/>
<connect gate="A" pin="A5" pad="52"/>
<connect gate="A" pin="A6" pad="51"/>
<connect gate="A" pin="A7" pad="50"/>
<connect gate="A" pin="A8" pad="34"/>
<connect gate="A" pin="A9" pad="32"/>
<connect gate="A" pin="C-A0" pad="65"/>
<connect gate="A" pin="C-A1" pad="62"/>
<connect gate="A" pin="C-A15" pad="21"/>
<connect gate="A" pin="C-A16" pad="17"/>
<connect gate="A" pin="DATA0" pad="73"/>
<connect gate="A" pin="DATA1" pad="84"/>
<connect gate="A" pin="DATA2" pad="88"/>
<connect gate="A" pin="DATA3" pad="91"/>
<connect gate="A" pin="DATA4" pad="96"/>
<connect gate="A" pin="DATA5" pad="10"/>
<connect gate="A" pin="DATA6" pad="9"/>
<connect gate="A" pin="DATA7" pad="8"/>
<connect gate="A" pin="DCLK" pad="11"/>
<connect gate="A" pin="DQ0" pad="81"/>
<connect gate="A" pin="DQ1" pad="83"/>
<connect gate="A" pin="DQ10" pad="87"/>
<connect gate="A" pin="DQ11" pad="90"/>
<connect gate="A" pin="DQ12" pad="94"/>
<connect gate="A" pin="DQ13" pad="97"/>
<connect gate="A" pin="DQ14" pad="99"/>
<connect gate="A" pin="DQ15" pad="1"/>
<connect gate="A" pin="DQ2" pad="86"/>
<connect gate="A" pin="DQ3" pad="89"/>
<connect gate="A" pin="DQ4" pad="93"/>
<connect gate="A" pin="DQ5" pad="95"/>
<connect gate="A" pin="DQ6" pad="98"/>
<connect gate="A" pin="DQ7" pad="100"/>
<connect gate="A" pin="DQ8" pad="82"/>
<connect gate="A" pin="DQ9" pad="85"/>
<connect gate="A" pin="EXCLK" pad="61"/>
<connect gate="A" pin="F-A0" pad="75"/>
<connect gate="A" pin="F-A1" pad="56"/>
<connect gate="A" pin="F-A15" pad="25"/>
<connect gate="A" pin="F-A16" pad="6"/>
<connect gate="A" pin="FLOATING" pad="36"/>
<connect gate="A" pin="FLOATING_2" pad="7"/>
<connect gate="A" pin="FLOATING_3" pad="74"/>
<connect gate="A" pin="FLOATING_4" pad="24"/>
<connect gate="A" pin="FLOATING_5" pad="57"/>
<connect gate="A" pin="GND/NC" pad="79"/>
<connect gate="A" pin="GND/NC_2" pad="58"/>
<connect gate="A" pin="GND/NC_3" pad="2"/>
<connect gate="A" pin="GND/NC_4" pad="41"/>
<connect gate="A" pin="GND/NC_5" pad="69"/>
<connect gate="A" pin="GND/NC_6" pad="70"/>
<connect gate="A" pin="NC" pad="64"/>
<connect gate="A" pin="NCS" pad="60"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_2" pad="18"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="19"/>
<connect gate="A" pin="NC_5" pad="30"/>
<connect gate="A" pin="NC_6" pad="76"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="63"/>
<connect gate="A" pin="NC_9" pad="77"/>
<connect gate="A" pin="OE" pad="23"/>
<connect gate="A" pin="PGM0" pad="14"/>
<connect gate="A" pin="PGM1" pad="13"/>
<connect gate="A" pin="PGM2" pad="15"/>
<connect gate="A" pin="PORSEL" pad="66"/>
<connect gate="A" pin="RY/~BY~/FLOATING" pad="37"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="42"/>
<connect gate="A" pin="TDO" pad="44"/>
<connect gate="A" pin="TM0" pad="71"/>
<connect gate="A" pin="TM1" pad="40"/>
<connect gate="A" pin="TMS" pad="48"/>
<connect gate="A" pin="VCC" pad="92"/>
<connect gate="A" pin="VCCW" pad="43"/>
<connect gate="A" pin="VCC_2" pad="59"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="67"/>
<connect gate="A" pin="VCC_5" pad="22"/>
<connect gate="A" pin="VCC_6" pad="68"/>
<connect gate="A" pin="~BYTE/VCC" pad="5"/>
<connect gate="A" pin="~C-RP~" pad="72"/>
<connect gate="A" pin="~C-WE~" pad="33"/>
<connect gate="A" pin="~CE~" pad="78"/>
<connect gate="A" pin="~F-RP~" pad="39"/>
<connect gate="A" pin="~F_-WE~" pad="38"/>
<connect gate="A" pin="~INIT_CONF~" pad="16"/>
<connect gate="A" pin="~OE~" pad="80"/>
<connect gate="A" pin="~WP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC16QC100N"/>
<attribute name="OC_FARNELL" value="1742173"/>
<attribute name="OC_NEWARK" value="51R0473"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC16QI100N">
<description>Enhanced Configuration Devices</description>
<gates>
<gate name="A" symbol="EPC16QI100N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="A10" pad="31"/>
<connect gate="A" pin="A11" pad="29"/>
<connect gate="A" pin="A12" pad="28"/>
<connect gate="A" pin="A13" pad="27"/>
<connect gate="A" pin="A14" pad="26"/>
<connect gate="A" pin="A17" pad="49"/>
<connect gate="A" pin="A18" pad="47"/>
<connect gate="A" pin="A19" pad="46"/>
<connect gate="A" pin="A2" pad="55"/>
<connect gate="A" pin="A3" pad="54"/>
<connect gate="A" pin="A4" pad="53"/>
<connect gate="A" pin="A5" pad="52"/>
<connect gate="A" pin="A6" pad="51"/>
<connect gate="A" pin="A7" pad="50"/>
<connect gate="A" pin="A8" pad="34"/>
<connect gate="A" pin="A9" pad="32"/>
<connect gate="A" pin="C-A0" pad="65"/>
<connect gate="A" pin="C-A1" pad="62"/>
<connect gate="A" pin="C-A15" pad="21"/>
<connect gate="A" pin="C-A16" pad="17"/>
<connect gate="A" pin="DATA0" pad="73"/>
<connect gate="A" pin="DATA1" pad="84"/>
<connect gate="A" pin="DATA2" pad="88"/>
<connect gate="A" pin="DATA3" pad="91"/>
<connect gate="A" pin="DATA4" pad="96"/>
<connect gate="A" pin="DATA5" pad="10"/>
<connect gate="A" pin="DATA6" pad="9"/>
<connect gate="A" pin="DATA7" pad="8"/>
<connect gate="A" pin="DCLK" pad="11"/>
<connect gate="A" pin="DQ0" pad="81"/>
<connect gate="A" pin="DQ1" pad="83"/>
<connect gate="A" pin="DQ10" pad="87"/>
<connect gate="A" pin="DQ11" pad="90"/>
<connect gate="A" pin="DQ12" pad="94"/>
<connect gate="A" pin="DQ13" pad="97"/>
<connect gate="A" pin="DQ14" pad="99"/>
<connect gate="A" pin="DQ15" pad="1"/>
<connect gate="A" pin="DQ2" pad="86"/>
<connect gate="A" pin="DQ3" pad="89"/>
<connect gate="A" pin="DQ4" pad="93"/>
<connect gate="A" pin="DQ5" pad="95"/>
<connect gate="A" pin="DQ6" pad="98"/>
<connect gate="A" pin="DQ7" pad="100"/>
<connect gate="A" pin="DQ8" pad="82"/>
<connect gate="A" pin="DQ9" pad="85"/>
<connect gate="A" pin="EXCLK" pad="61"/>
<connect gate="A" pin="F-A0" pad="75"/>
<connect gate="A" pin="F-A1" pad="56"/>
<connect gate="A" pin="F-A15" pad="25"/>
<connect gate="A" pin="F-A16" pad="6"/>
<connect gate="A" pin="FLOATING" pad="36"/>
<connect gate="A" pin="FLOATING_2" pad="7"/>
<connect gate="A" pin="FLOATING_3" pad="74"/>
<connect gate="A" pin="FLOATING_4" pad="24"/>
<connect gate="A" pin="FLOATING_5" pad="57"/>
<connect gate="A" pin="GND/NC" pad="79"/>
<connect gate="A" pin="GND/NC_2" pad="58"/>
<connect gate="A" pin="GND/NC_3" pad="2"/>
<connect gate="A" pin="GND/NC_4" pad="41"/>
<connect gate="A" pin="GND/NC_5" pad="69"/>
<connect gate="A" pin="GND/NC_6" pad="70"/>
<connect gate="A" pin="NC" pad="64"/>
<connect gate="A" pin="NCS" pad="60"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_2" pad="18"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="19"/>
<connect gate="A" pin="NC_5" pad="30"/>
<connect gate="A" pin="NC_6" pad="76"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="63"/>
<connect gate="A" pin="NC_9" pad="77"/>
<connect gate="A" pin="OE" pad="23"/>
<connect gate="A" pin="PGM0" pad="14"/>
<connect gate="A" pin="PGM1" pad="13"/>
<connect gate="A" pin="PGM2" pad="15"/>
<connect gate="A" pin="PORSEL" pad="66"/>
<connect gate="A" pin="RY/~BY~/FLOATING" pad="37"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="42"/>
<connect gate="A" pin="TDO" pad="44"/>
<connect gate="A" pin="TM0" pad="71"/>
<connect gate="A" pin="TM1" pad="40"/>
<connect gate="A" pin="TMS" pad="48"/>
<connect gate="A" pin="VCC" pad="92"/>
<connect gate="A" pin="VCCW" pad="43"/>
<connect gate="A" pin="VCC_2" pad="59"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="67"/>
<connect gate="A" pin="VCC_5" pad="22"/>
<connect gate="A" pin="VCC_6" pad="68"/>
<connect gate="A" pin="~BYTE/VCC" pad="5"/>
<connect gate="A" pin="~C-RP~" pad="72"/>
<connect gate="A" pin="~C-WE~" pad="33"/>
<connect gate="A" pin="~CE~" pad="78"/>
<connect gate="A" pin="~F-RP~" pad="39"/>
<connect gate="A" pin="~F_-WE~" pad="38"/>
<connect gate="A" pin="~INIT_CONF~" pad="16"/>
<connect gate="A" pin="~OE~" pad="80"/>
<connect gate="A" pin="~WP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC16QI100N"/>
<attribute name="OC_FARNELL" value="1637247"/>
<attribute name="OC_NEWARK" value="51R0474"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC16UC88N" prefix="U">
<description>Enhanced Configuration Devices</description>
<gates>
<gate name="A" symbol="EPC16UC88N"/>
</gates>
<devices>
<device name="" package="BGA88C12X8X80P_800X1100X140">
<connects>
<connect gate="A" pin="A0" pad="H6"/>
<connect gate="A" pin="A1" pad="G9"/>
<connect gate="A" pin="A10" pad="B5"/>
<connect gate="A" pin="A11" pad="A4"/>
<connect gate="A" pin="A12" pad="A8"/>
<connect gate="A" pin="A13" pad="A7"/>
<connect gate="A" pin="A14" pad="A6"/>
<connect gate="A" pin="A15" pad="A5"/>
<connect gate="A" pin="A16" pad="B3"/>
<connect gate="A" pin="A17" pad="G4"/>
<connect gate="A" pin="A18" pad="G3"/>
<connect gate="A" pin="A19" pad="E5"/>
<connect gate="A" pin="A2" pad="G8"/>
<connect gate="A" pin="A20" pad="A3"/>
<connect gate="A" pin="A3" pad="G7"/>
<connect gate="A" pin="A4" pad="H5"/>
<connect gate="A" pin="A5" pad="H4"/>
<connect gate="A" pin="A6" pad="G6"/>
<connect gate="A" pin="A7" pad="G5"/>
<connect gate="A" pin="A8" pad="B4"/>
<connect gate="A" pin="A9" pad="B6"/>
<connect gate="A" pin="CE" pad="H7"/>
<connect gate="A" pin="C_-WE" pad="B2"/>
<connect gate="A" pin="C_-_RP" pad="D8"/>
<connect gate="A" pin="DATA0" pad="G12"/>
<connect gate="A" pin="DATA1" pad="F11"/>
<connect gate="A" pin="DATA2" pad="E11"/>
<connect gate="A" pin="DATA3" pad="D11"/>
<connect gate="A" pin="DATA4" pad="C11"/>
<connect gate="A" pin="DATA5" pad="B11"/>
<connect gate="A" pin="DATA6" pad="B12"/>
<connect gate="A" pin="DATA7" pad="A11"/>
<connect gate="A" pin="DCLK" pad="A10"/>
<connect gate="A" pin="DQ1" pad="F10"/>
<connect gate="A" pin="DQ10" pad="E8"/>
<connect gate="A" pin="DQ11" pad="E6"/>
<connect gate="A" pin="DQ12" pad="D7"/>
<connect gate="A" pin="DQ13" pad="C7"/>
<connect gate="A" pin="DQ14" pad="B9"/>
<connect gate="A" pin="DQ15" pad="B7"/>
<connect gate="A" pin="DQ1_2" pad="E9"/>
<connect gate="A" pin="DQ2" pad="F9"/>
<connect gate="A" pin="DQ3" pad="E10"/>
<connect gate="A" pin="DQ4" pad="C9"/>
<connect gate="A" pin="DQ5" pad="C10"/>
<connect gate="A" pin="DQ6" pad="C8"/>
<connect gate="A" pin="DQ7" pad="B10"/>
<connect gate="A" pin="DQ8" pad="F8"/>
<connect gate="A" pin="DQ9" pad="F7"/>
<connect gate="A" pin="EXCLK" pad="H3"/>
<connect gate="A" pin="F_-WE" pad="C3"/>
<connect gate="A" pin="F_-_RP" pad="D4"/>
<connect gate="A" pin="GND" pad="G11"/>
<connect gate="A" pin="GND_2" pad="A9"/>
<connect gate="A" pin="GND_3" pad="H11"/>
<connect gate="A" pin="GND_4" pad="H2"/>
<connect gate="A" pin="GND_5" pad="H8"/>
<connect gate="A" pin="GND_6" pad="D3"/>
<connect gate="A" pin="NC" pad="H12"/>
<connect gate="A" pin="NCS" pad="G2"/>
<connect gate="A" pin="NC_2" pad="A12"/>
<connect gate="A" pin="NC_3" pad="F3"/>
<connect gate="A" pin="NC_4" pad="A1"/>
<connect gate="A" pin="NC_5" pad="F4"/>
<connect gate="A" pin="NC_6" pad="H1"/>
<connect gate="A" pin="N_INIT___CONF" pad="C5"/>
<connect gate="A" pin="OE" pad="B1"/>
<connect gate="A" pin="OE_2" pad="H9"/>
<connect gate="A" pin="PGM0" pad="B8"/>
<connect gate="A" pin="PGM1" pad="C6"/>
<connect gate="A" pin="PGM2" pad="F5"/>
<connect gate="A" pin="PORSEL" pad="F6"/>
<connect gate="A" pin="RY/BY" pad="C4"/>
<connect gate="A" pin="TCK" pad="C2"/>
<connect gate="A" pin="TDI" pad="D2"/>
<connect gate="A" pin="TDO" pad="E2"/>
<connect gate="A" pin="TM0" pad="H10"/>
<connect gate="A" pin="TM1" pad="D5"/>
<connect gate="A" pin="TMS" pad="F2"/>
<connect gate="A" pin="VCC" pad="G10"/>
<connect gate="A" pin="VCCW" pad="E4"/>
<connect gate="A" pin="VCC_2" pad="D6"/>
<connect gate="A" pin="VCC_3" pad="D9"/>
<connect gate="A" pin="VCC_4" pad="E7"/>
<connect gate="A" pin="VCC_5" pad="D10"/>
<connect gate="A" pin="VCC_6" pad="A2"/>
<connect gate="A" pin="VCC_7" pad="G1"/>
<connect gate="A" pin="WP" pad="E3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC16UC88N"/>
<attribute name="OC_FARNELL" value="1549338"/>
<attribute name="OC_NEWARK" value="51R0475"/>
<attribute name="PACKAGE" value="UFBGA-88"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC1LC20N">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC1LC20N"/>
</gates>
<devices>
<device name="" package="PLCC127P1000X1000X457-20N">
<connects>
<connect gate="A" pin="DATA" pad="2"/>
<connect gate="A" pin="DCLK" pad="4"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="NCASC" pad="12"/>
<connect gate="A" pin="NCS" pad="9"/>
<connect gate="A" pin="NC_2" pad="15"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="NC_4" pad="16"/>
<connect gate="A" pin="NC_5" pad="7"/>
<connect gate="A" pin="NINIT_CONF" pad="13"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="TCK" pad="3"/>
<connect gate="A" pin="TDI" pad="11"/>
<connect gate="A" pin="TDO" pad="1"/>
<connect gate="A" pin="TMS" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCCSEL" pad="5"/>
<connect gate="A" pin="VPP" pad="18"/>
<connect gate="A" pin="VPPSEL" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC1LC20N"/>
<attribute name="OC_FARNELL" value="1549342"/>
<attribute name="OC_NEWARK" value="51R8709"/>
<attribute name="PACKAGE" value="PLCC-20"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC1PI8">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC1PI8"/>
</gates>
<devices>
<device name="" package="DIP254P762X431-8">
<connects>
<connect gate="A" pin="DATA" pad="1"/>
<connect gate="A" pin="DCLK" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NCASC" pad="6"/>
<connect gate="A" pin="NCS" pad="4"/>
<connect gate="A" pin="OE" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VCC_2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC1PI8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8713"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC2LC20">
<description>IC CONFIG DEVICE</description>
<gates>
<gate name="A" symbol="EPC2LC20"/>
</gates>
<devices>
<device name="" package="PLCC127P990X990X457-20N">
<connects>
<connect gate="A" pin="DATA" pad="2"/>
<connect gate="A" pin="DCLK" pad="4"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="15"/>
<connect gate="A" pin="NC_5" pad="16"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="TCK" pad="3"/>
<connect gate="A" pin="TDI" pad="11"/>
<connect gate="A" pin="TDO" pad="1"/>
<connect gate="A" pin="TMS" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCCSEL" pad="5"/>
<connect gate="A" pin="VPP" pad="18"/>
<connect gate="A" pin="VPPSEL" pad="14"/>
<connect gate="A" pin="~CASC" pad="12"/>
<connect gate="A" pin="~CS" pad="9"/>
<connect gate="A" pin="~INIT_CONF" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC2LC20"/>
<attribute name="OC_FARNELL" value="1839419"/>
<attribute name="OC_NEWARK" value="51R8734"/>
<attribute name="PACKAGE" value="PLCC-20"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC2LI20N">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC2LI20N"/>
</gates>
<devices>
<device name="" package="PLCC127P1000X1000X457-20N">
<connects>
<connect gate="A" pin="DATA" pad="2"/>
<connect gate="A" pin="DCLK" pad="4"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="N.C" pad="3"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NCASC" pad="12"/>
<connect gate="A" pin="NCS" pad="9"/>
<connect gate="A" pin="NC_10" pad="17"/>
<connect gate="A" pin="NC_11" pad="19"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="11"/>
<connect gate="A" pin="NC_5" pad="14"/>
<connect gate="A" pin="NC_6" pad="6"/>
<connect gate="A" pin="NC_7" pad="15"/>
<connect gate="A" pin="NC_8" pad="16"/>
<connect gate="A" pin="NC_9" pad="1"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC2LI20N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8736"/>
<attribute name="PACKAGE" value="PLCC-20"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC2TC32N" prefix="U">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC2TC32N"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="DATA" pad="31"/>
<connect gate="A" pin="DCLK" pad="2"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NCASC" pad="15"/>
<connect gate="A" pin="NCS" pad="10"/>
<connect gate="A" pin="NCS_2" pad="8"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_11" pad="21"/>
<connect gate="A" pin="NC_12" pad="30"/>
<connect gate="A" pin="NC_13" pad="11"/>
<connect gate="A" pin="NC_14" pad="22"/>
<connect gate="A" pin="NC_15" pad="9"/>
<connect gate="A" pin="NC_16" pad="14"/>
<connect gate="A" pin="NC_2" pad="26"/>
<connect gate="A" pin="NC_3" pad="18"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="24"/>
<connect gate="A" pin="NC_6" pad="19"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="29"/>
<connect gate="A" pin="NC_9" pad="1"/>
<connect gate="A" pin="NINIT_CONF" pad="16"/>
<connect gate="A" pin="OE" pad="7"/>
<connect gate="A" pin="TCK" pad="32"/>
<connect gate="A" pin="TDI" pad="13"/>
<connect gate="A" pin="TDO" pad="28"/>
<connect gate="A" pin="TMS" pad="25"/>
<connect gate="A" pin="VCC" pad="27"/>
<connect gate="A" pin="VCCSEL" pad="3"/>
<connect gate="A" pin="VPP" pad="23"/>
<connect gate="A" pin="VPPSEL" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC2TC32N"/>
<attribute name="OC_FARNELL" value="1549337"/>
<attribute name="OC_NEWARK" value="51R0477"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC2TI32N" prefix="U">
<description>Configuration Devices for SRAM-Based LUT Devices</description>
<gates>
<gate name="A" symbol="EPC2TI32N"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="DATA" pad="31"/>
<connect gate="A" pin="DCLK" pad="2"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NCASC" pad="15"/>
<connect gate="A" pin="NCS" pad="10"/>
<connect gate="A" pin="NCS_2" pad="8"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_11" pad="21"/>
<connect gate="A" pin="NC_12" pad="30"/>
<connect gate="A" pin="NC_13" pad="11"/>
<connect gate="A" pin="NC_14" pad="22"/>
<connect gate="A" pin="NC_15" pad="9"/>
<connect gate="A" pin="NC_16" pad="14"/>
<connect gate="A" pin="NC_2" pad="26"/>
<connect gate="A" pin="NC_3" pad="18"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="24"/>
<connect gate="A" pin="NC_6" pad="19"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="29"/>
<connect gate="A" pin="NC_9" pad="1"/>
<connect gate="A" pin="NINIT_CONF" pad="16"/>
<connect gate="A" pin="OE" pad="7"/>
<connect gate="A" pin="TCK" pad="32"/>
<connect gate="A" pin="TDI" pad="13"/>
<connect gate="A" pin="TDO" pad="28"/>
<connect gate="A" pin="TMS" pad="25"/>
<connect gate="A" pin="VCC" pad="27"/>
<connect gate="A" pin="VCCSEL" pad="3"/>
<connect gate="A" pin="VPP" pad="23"/>
<connect gate="A" pin="VPPSEL" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC2TI32N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8739"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC4QC100N">
<description>FPGA CONFIGURATION DEVIC</description>
<gates>
<gate name="A" symbol="EPC4QC100N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="A10" pad="31"/>
<connect gate="A" pin="A11" pad="29"/>
<connect gate="A" pin="A12" pad="28"/>
<connect gate="A" pin="A13" pad="27"/>
<connect gate="A" pin="A14" pad="26"/>
<connect gate="A" pin="A17" pad="49"/>
<connect gate="A" pin="A18" pad="47"/>
<connect gate="A" pin="A19" pad="46"/>
<connect gate="A" pin="A2" pad="55"/>
<connect gate="A" pin="A3" pad="54"/>
<connect gate="A" pin="A4" pad="53"/>
<connect gate="A" pin="A5" pad="52"/>
<connect gate="A" pin="A6" pad="51"/>
<connect gate="A" pin="A7" pad="50"/>
<connect gate="A" pin="A8" pad="34"/>
<connect gate="A" pin="A9" pad="32"/>
<connect gate="A" pin="C-A0" pad="65"/>
<connect gate="A" pin="C-A1" pad="62"/>
<connect gate="A" pin="C-A15" pad="21"/>
<connect gate="A" pin="C-A16" pad="17"/>
<connect gate="A" pin="DATA0" pad="73"/>
<connect gate="A" pin="DATA1" pad="84"/>
<connect gate="A" pin="DATA2" pad="88"/>
<connect gate="A" pin="DATA3" pad="91"/>
<connect gate="A" pin="DATA4" pad="96"/>
<connect gate="A" pin="DATA5" pad="10"/>
<connect gate="A" pin="DATA6" pad="9"/>
<connect gate="A" pin="DATA7" pad="8"/>
<connect gate="A" pin="DCLK" pad="11"/>
<connect gate="A" pin="DQ0" pad="81"/>
<connect gate="A" pin="DQ1" pad="83"/>
<connect gate="A" pin="DQ10" pad="87"/>
<connect gate="A" pin="DQ11" pad="90"/>
<connect gate="A" pin="DQ12" pad="94"/>
<connect gate="A" pin="DQ13" pad="97"/>
<connect gate="A" pin="DQ14" pad="99"/>
<connect gate="A" pin="DQ15" pad="1"/>
<connect gate="A" pin="DQ2" pad="86"/>
<connect gate="A" pin="DQ3" pad="89"/>
<connect gate="A" pin="DQ4" pad="93"/>
<connect gate="A" pin="DQ5" pad="95"/>
<connect gate="A" pin="DQ6" pad="98"/>
<connect gate="A" pin="DQ7" pad="100"/>
<connect gate="A" pin="DQ8" pad="82"/>
<connect gate="A" pin="DQ9" pad="85"/>
<connect gate="A" pin="EXCLK" pad="61"/>
<connect gate="A" pin="F-A0" pad="75"/>
<connect gate="A" pin="F-A1" pad="56"/>
<connect gate="A" pin="F-A15" pad="25"/>
<connect gate="A" pin="F-A16" pad="6"/>
<connect gate="A" pin="FLOATING" pad="36"/>
<connect gate="A" pin="FLOATING_2" pad="7"/>
<connect gate="A" pin="FLOATING_3" pad="74"/>
<connect gate="A" pin="FLOATING_4" pad="24"/>
<connect gate="A" pin="FLOATING_5" pad="57"/>
<connect gate="A" pin="GND/NC" pad="79"/>
<connect gate="A" pin="GND/NC_2" pad="58"/>
<connect gate="A" pin="GND/NC_3" pad="2"/>
<connect gate="A" pin="GND/NC_4" pad="41"/>
<connect gate="A" pin="GND/NC_5" pad="69"/>
<connect gate="A" pin="GND/NC_6" pad="70"/>
<connect gate="A" pin="NC" pad="64"/>
<connect gate="A" pin="NCS" pad="60"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_2" pad="18"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="19"/>
<connect gate="A" pin="NC_5" pad="30"/>
<connect gate="A" pin="NC_6" pad="76"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="63"/>
<connect gate="A" pin="NC_9" pad="77"/>
<connect gate="A" pin="OE" pad="23"/>
<connect gate="A" pin="PGM0" pad="14"/>
<connect gate="A" pin="PGM1" pad="13"/>
<connect gate="A" pin="PGM2" pad="15"/>
<connect gate="A" pin="PORSEL" pad="66"/>
<connect gate="A" pin="RY/~BY~/FLOATING" pad="37"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="42"/>
<connect gate="A" pin="TDO" pad="44"/>
<connect gate="A" pin="TM0" pad="71"/>
<connect gate="A" pin="TM1" pad="40"/>
<connect gate="A" pin="TMS" pad="48"/>
<connect gate="A" pin="VCC" pad="92"/>
<connect gate="A" pin="VCCW" pad="43"/>
<connect gate="A" pin="VCC_2" pad="59"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="67"/>
<connect gate="A" pin="VCC_5" pad="22"/>
<connect gate="A" pin="VCC_6" pad="68"/>
<connect gate="A" pin="~BYTE/VCC" pad="5"/>
<connect gate="A" pin="~C-RP~" pad="72"/>
<connect gate="A" pin="~C-WE~" pad="33"/>
<connect gate="A" pin="~CE~" pad="78"/>
<connect gate="A" pin="~F-RP~" pad="39"/>
<connect gate="A" pin="~F_-WE~" pad="38"/>
<connect gate="A" pin="~INIT_CONF~" pad="16"/>
<connect gate="A" pin="~OE~" pad="80"/>
<connect gate="A" pin="~WP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC4QC100N"/>
<attribute name="OC_FARNELL" value="1742174"/>
<attribute name="OC_NEWARK" value="51R0478"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC8QC100N">
<description>FPGA CONFIGURATION DEVIC</description>
<gates>
<gate name="A" symbol="EPC8QC100N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="A10" pad="31"/>
<connect gate="A" pin="A11" pad="29"/>
<connect gate="A" pin="A12" pad="28"/>
<connect gate="A" pin="A13" pad="27"/>
<connect gate="A" pin="A14" pad="26"/>
<connect gate="A" pin="A17" pad="49"/>
<connect gate="A" pin="A18" pad="47"/>
<connect gate="A" pin="A19" pad="46"/>
<connect gate="A" pin="A2" pad="55"/>
<connect gate="A" pin="A3" pad="54"/>
<connect gate="A" pin="A4" pad="53"/>
<connect gate="A" pin="A5" pad="52"/>
<connect gate="A" pin="A6" pad="51"/>
<connect gate="A" pin="A7" pad="50"/>
<connect gate="A" pin="A8" pad="34"/>
<connect gate="A" pin="A9" pad="32"/>
<connect gate="A" pin="C-A0" pad="65"/>
<connect gate="A" pin="C-A1" pad="62"/>
<connect gate="A" pin="C-A15" pad="21"/>
<connect gate="A" pin="C-A16" pad="17"/>
<connect gate="A" pin="DATA0" pad="73"/>
<connect gate="A" pin="DATA1" pad="84"/>
<connect gate="A" pin="DATA2" pad="88"/>
<connect gate="A" pin="DATA3" pad="91"/>
<connect gate="A" pin="DATA4" pad="96"/>
<connect gate="A" pin="DATA5" pad="10"/>
<connect gate="A" pin="DATA6" pad="9"/>
<connect gate="A" pin="DATA7" pad="8"/>
<connect gate="A" pin="DCLK" pad="11"/>
<connect gate="A" pin="DQ0" pad="81"/>
<connect gate="A" pin="DQ1" pad="83"/>
<connect gate="A" pin="DQ10" pad="87"/>
<connect gate="A" pin="DQ11" pad="90"/>
<connect gate="A" pin="DQ12" pad="94"/>
<connect gate="A" pin="DQ13" pad="97"/>
<connect gate="A" pin="DQ14" pad="99"/>
<connect gate="A" pin="DQ15" pad="1"/>
<connect gate="A" pin="DQ2" pad="86"/>
<connect gate="A" pin="DQ3" pad="89"/>
<connect gate="A" pin="DQ4" pad="93"/>
<connect gate="A" pin="DQ5" pad="95"/>
<connect gate="A" pin="DQ6" pad="98"/>
<connect gate="A" pin="DQ7" pad="100"/>
<connect gate="A" pin="DQ8" pad="82"/>
<connect gate="A" pin="DQ9" pad="85"/>
<connect gate="A" pin="EXCLK" pad="61"/>
<connect gate="A" pin="F-A0" pad="75"/>
<connect gate="A" pin="F-A1" pad="56"/>
<connect gate="A" pin="F-A15" pad="25"/>
<connect gate="A" pin="F-A16" pad="6"/>
<connect gate="A" pin="FLOATING" pad="36"/>
<connect gate="A" pin="FLOATING_2" pad="7"/>
<connect gate="A" pin="FLOATING_3" pad="74"/>
<connect gate="A" pin="FLOATING_4" pad="24"/>
<connect gate="A" pin="FLOATING_5" pad="57"/>
<connect gate="A" pin="GND/NC" pad="79"/>
<connect gate="A" pin="GND/NC_2" pad="58"/>
<connect gate="A" pin="GND/NC_3" pad="2"/>
<connect gate="A" pin="GND/NC_4" pad="41"/>
<connect gate="A" pin="GND/NC_5" pad="69"/>
<connect gate="A" pin="GND/NC_6" pad="70"/>
<connect gate="A" pin="NC" pad="64"/>
<connect gate="A" pin="NCS" pad="60"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_2" pad="18"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="19"/>
<connect gate="A" pin="NC_5" pad="30"/>
<connect gate="A" pin="NC_6" pad="76"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="63"/>
<connect gate="A" pin="NC_9" pad="77"/>
<connect gate="A" pin="OE" pad="23"/>
<connect gate="A" pin="PGM0" pad="14"/>
<connect gate="A" pin="PGM1" pad="13"/>
<connect gate="A" pin="PGM2" pad="15"/>
<connect gate="A" pin="PORSEL" pad="66"/>
<connect gate="A" pin="RY/~BY~/FLOATING" pad="37"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="42"/>
<connect gate="A" pin="TDO" pad="44"/>
<connect gate="A" pin="TM0" pad="71"/>
<connect gate="A" pin="TM1" pad="40"/>
<connect gate="A" pin="TMS" pad="48"/>
<connect gate="A" pin="VCC" pad="92"/>
<connect gate="A" pin="VCCW" pad="43"/>
<connect gate="A" pin="VCC_2" pad="59"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="67"/>
<connect gate="A" pin="VCC_5" pad="22"/>
<connect gate="A" pin="VCC_6" pad="68"/>
<connect gate="A" pin="~BYTE/VCC" pad="5"/>
<connect gate="A" pin="~C-RP~" pad="72"/>
<connect gate="A" pin="~C-WE~" pad="33"/>
<connect gate="A" pin="~CE~" pad="78"/>
<connect gate="A" pin="~F-RP~" pad="39"/>
<connect gate="A" pin="~F_-WE~" pad="38"/>
<connect gate="A" pin="~INIT_CONF~" pad="16"/>
<connect gate="A" pin="~OE~" pad="80"/>
<connect gate="A" pin="~WP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC8QC100N"/>
<attribute name="OC_FARNELL" value="1549335"/>
<attribute name="OC_NEWARK" value="51R0479"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPC8QI100N">
<description>FPGA CONFIGURATION DEVIC</description>
<gates>
<gate name="A" symbol="EPC8QI100N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="A10" pad="31"/>
<connect gate="A" pin="A11" pad="29"/>
<connect gate="A" pin="A12" pad="28"/>
<connect gate="A" pin="A13" pad="27"/>
<connect gate="A" pin="A14" pad="26"/>
<connect gate="A" pin="A17" pad="49"/>
<connect gate="A" pin="A18" pad="47"/>
<connect gate="A" pin="A19" pad="46"/>
<connect gate="A" pin="A2" pad="55"/>
<connect gate="A" pin="A3" pad="54"/>
<connect gate="A" pin="A4" pad="53"/>
<connect gate="A" pin="A5" pad="52"/>
<connect gate="A" pin="A6" pad="51"/>
<connect gate="A" pin="A7" pad="50"/>
<connect gate="A" pin="A8" pad="34"/>
<connect gate="A" pin="A9" pad="32"/>
<connect gate="A" pin="C-A0" pad="65"/>
<connect gate="A" pin="C-A1" pad="62"/>
<connect gate="A" pin="C-A15" pad="21"/>
<connect gate="A" pin="C-A16" pad="17"/>
<connect gate="A" pin="DATA0" pad="73"/>
<connect gate="A" pin="DATA1" pad="84"/>
<connect gate="A" pin="DATA2" pad="88"/>
<connect gate="A" pin="DATA3" pad="91"/>
<connect gate="A" pin="DATA4" pad="96"/>
<connect gate="A" pin="DATA5" pad="10"/>
<connect gate="A" pin="DATA6" pad="9"/>
<connect gate="A" pin="DATA7" pad="8"/>
<connect gate="A" pin="DCLK" pad="11"/>
<connect gate="A" pin="DQ0" pad="81"/>
<connect gate="A" pin="DQ1" pad="83"/>
<connect gate="A" pin="DQ10" pad="87"/>
<connect gate="A" pin="DQ11" pad="90"/>
<connect gate="A" pin="DQ12" pad="94"/>
<connect gate="A" pin="DQ13" pad="97"/>
<connect gate="A" pin="DQ14" pad="99"/>
<connect gate="A" pin="DQ15" pad="1"/>
<connect gate="A" pin="DQ2" pad="86"/>
<connect gate="A" pin="DQ3" pad="89"/>
<connect gate="A" pin="DQ4" pad="93"/>
<connect gate="A" pin="DQ5" pad="95"/>
<connect gate="A" pin="DQ6" pad="98"/>
<connect gate="A" pin="DQ7" pad="100"/>
<connect gate="A" pin="DQ8" pad="82"/>
<connect gate="A" pin="DQ9" pad="85"/>
<connect gate="A" pin="EXCLK" pad="61"/>
<connect gate="A" pin="F-A0" pad="75"/>
<connect gate="A" pin="F-A1" pad="56"/>
<connect gate="A" pin="F-A15" pad="25"/>
<connect gate="A" pin="F-A16" pad="6"/>
<connect gate="A" pin="FLOATING" pad="36"/>
<connect gate="A" pin="FLOATING_2" pad="7"/>
<connect gate="A" pin="FLOATING_3" pad="74"/>
<connect gate="A" pin="FLOATING_4" pad="24"/>
<connect gate="A" pin="FLOATING_5" pad="57"/>
<connect gate="A" pin="GND/NC" pad="79"/>
<connect gate="A" pin="GND/NC_2" pad="58"/>
<connect gate="A" pin="GND/NC_3" pad="2"/>
<connect gate="A" pin="GND/NC_4" pad="41"/>
<connect gate="A" pin="GND/NC_5" pad="69"/>
<connect gate="A" pin="GND/NC_6" pad="70"/>
<connect gate="A" pin="NC" pad="64"/>
<connect gate="A" pin="NCS" pad="60"/>
<connect gate="A" pin="NC_10" pad="20"/>
<connect gate="A" pin="NC_2" pad="18"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="19"/>
<connect gate="A" pin="NC_5" pad="30"/>
<connect gate="A" pin="NC_6" pad="76"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="63"/>
<connect gate="A" pin="NC_9" pad="77"/>
<connect gate="A" pin="OE" pad="23"/>
<connect gate="A" pin="PGM0" pad="14"/>
<connect gate="A" pin="PGM1" pad="13"/>
<connect gate="A" pin="PGM2" pad="15"/>
<connect gate="A" pin="PORSEL" pad="66"/>
<connect gate="A" pin="RY/~BY~/FLOATING" pad="37"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="42"/>
<connect gate="A" pin="TDO" pad="44"/>
<connect gate="A" pin="TM0" pad="71"/>
<connect gate="A" pin="TM1" pad="40"/>
<connect gate="A" pin="TMS" pad="48"/>
<connect gate="A" pin="VCC" pad="92"/>
<connect gate="A" pin="VCCW" pad="43"/>
<connect gate="A" pin="VCC_2" pad="59"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="67"/>
<connect gate="A" pin="VCC_5" pad="22"/>
<connect gate="A" pin="VCC_6" pad="68"/>
<connect gate="A" pin="~BYTE/VCC" pad="5"/>
<connect gate="A" pin="~C-RP~" pad="72"/>
<connect gate="A" pin="~C-WE~" pad="33"/>
<connect gate="A" pin="~CE~" pad="78"/>
<connect gate="A" pin="~F-RP~" pad="39"/>
<connect gate="A" pin="~F_-WE~" pad="38"/>
<connect gate="A" pin="~INIT_CONF~" pad="16"/>
<connect gate="A" pin="~OE~" pad="80"/>
<connect gate="A" pin="~WP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPC8QI100N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8745"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPCS1SI8N" prefix="U">
<description>Serial Configuration Devices</description>
<gates>
<gate name="A" symbol="EPCS1SI8N"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ASDI" pad="5"/>
<connect gate="A" pin="DATA" pad="2"/>
<connect gate="A" pin="DCLK" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NCS" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Serial Configuration Devices"/>
<attribute name="MPN" value="EPCS1SI8N"/>
<attribute name="OC_FARNELL" value="1453504"/>
<attribute name="OC_NEWARK" value="51R0466"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPCS64SI16N">
<description>IC FPGA</description>
<gates>
<gate name="A" symbol="EPCS64SI16N"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="ASDI" pad="15"/>
<connect gate="A" pin="DATA" pad="8"/>
<connect gate="A" pin="DCLK" pad="16"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="N/C" pad="3"/>
<connect gate="A" pin="N/C_2" pad="11"/>
<connect gate="A" pin="N/C_3" pad="12"/>
<connect gate="A" pin="N/C_4" pad="6"/>
<connect gate="A" pin="N/C_5" pad="13"/>
<connect gate="A" pin="N/C_6" pad="14"/>
<connect gate="A" pin="N/C_7" pad="4"/>
<connect gate="A" pin="N/C_8" pad="5"/>
<connect gate="A" pin="NCS" pad="7"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPCS64SI16N"/>
<attribute name="OC_FARNELL" value="1854175"/>
<attribute name="OC_NEWARK" value="51R0470"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K10QC208-4N">
<description>Embedded Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPF10K10QC208-4N_A"/>
<gate name="B" symbol="EPF10K10QC208-4N_B"/>
<gate name="C" symbol="EPF10K10QC208-4N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="49"/>
<connect gate="A" pin="GNDINT_2" pad="21"/>
<connect gate="A" pin="GNDINT_3" pad="33"/>
<connect gate="A" pin="GNDIO" pad="48"/>
<connect gate="A" pin="GNDIO_2" pad="20"/>
<connect gate="A" pin="GNDIO_3" pad="59"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/CLKUSR" pad="10"/>
<connect gate="A" pin="IO/INIT_DONE" pad="19"/>
<connect gate="A" pin="IO/RDY/NBSY" pad="16"/>
<connect gate="A" pin="IO_10" pad="27"/>
<connect gate="A" pin="IO_11" pad="28"/>
<connect gate="A" pin="IO_12" pad="29"/>
<connect gate="A" pin="IO_13" pad="30"/>
<connect gate="A" pin="IO_14" pad="31"/>
<connect gate="A" pin="IO_15" pad="38"/>
<connect gate="A" pin="IO_16" pad="39"/>
<connect gate="A" pin="IO_17" pad="40"/>
<connect gate="A" pin="IO_18" pad="41"/>
<connect gate="A" pin="IO_19" pad="44"/>
<connect gate="A" pin="IO_2" pad="11"/>
<connect gate="A" pin="IO_20" pad="45"/>
<connect gate="A" pin="IO_21" pad="46"/>
<connect gate="A" pin="IO_22" pad="47"/>
<connect gate="A" pin="IO_23" pad="53"/>
<connect gate="A" pin="IO_24" pad="54"/>
<connect gate="A" pin="IO_25" pad="55"/>
<connect gate="A" pin="IO_26" pad="56"/>
<connect gate="A" pin="IO_27" pad="57"/>
<connect gate="A" pin="IO_28" pad="58"/>
<connect gate="A" pin="IO_29" pad="60"/>
<connect gate="A" pin="IO_3" pad="12"/>
<connect gate="A" pin="IO_30" pad="61"/>
<connect gate="A" pin="IO_31" pad="62"/>
<connect gate="A" pin="IO_32" pad="63"/>
<connect gate="A" pin="IO_33" pad="64"/>
<connect gate="A" pin="IO_34" pad="65"/>
<connect gate="A" pin="IO_35" pad="67"/>
<connect gate="A" pin="IO_36" pad="68"/>
<connect gate="A" pin="IO_37" pad="69"/>
<connect gate="A" pin="IO_4" pad="13"/>
<connect gate="A" pin="IO_5" pad="17"/>
<connect gate="A" pin="IO_6" pad="18"/>
<connect gate="A" pin="IO_7" pad="24"/>
<connect gate="A" pin="IO_8" pad="25"/>
<connect gate="A" pin="IO_9" pad="26"/>
<connect gate="A" pin="NC" pad="15"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="36"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="NC_5" pad="37"/>
<connect gate="A" pin="NC_6" pad="9"/>
<connect gate="A" pin="NC_7" pad="14"/>
<connect gate="A" pin="NSTATUS" pad="52"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="50"/>
<connect gate="A" pin="TRST" pad="51"/>
<connect gate="A" pin="VCCINT" pad="35"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="43"/>
<connect gate="A" pin="VCCINT_4" pad="23"/>
<connect gate="A" pin="VCCIO" pad="42"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="22"/>
<connect gate="A" pin="VCCIO_4" pad="34"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="B" pin="CLOCK" pad="79"/>
<connect gate="B" pin="GNDINT" pad="129"/>
<connect gate="B" pin="GNDINT_2" pad="81"/>
<connect gate="B" pin="GNDINT_3" pad="82"/>
<connect gate="B" pin="GNDINT_4" pad="123"/>
<connect gate="B" pin="GNDIO" pad="124"/>
<connect gate="B" pin="GNDIO_2" pad="72"/>
<connect gate="B" pin="GNDIO_3" pad="91"/>
<connect gate="B" pin="GNDIO_4" pad="130"/>
<connect gate="B" pin="INPUT" pad="80"/>
<connect gate="B" pin="INPUT_2" pad="78"/>
<connect gate="B" pin="IO" pad="136"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="89"/>
<connect gate="B" pin="IO_12" pad="90"/>
<connect gate="B" pin="IO_13" pad="92"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="94"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="103"/>
<connect gate="B" pin="IO_24" pad="104"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="115"/>
<connect gate="B" pin="IO_28" pad="116"/>
<connect gate="B" pin="IO_29" pad="119"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="120"/>
<connect gate="B" pin="IO_31" pad="121"/>
<connect gate="B" pin="IO_32" pad="122"/>
<connect gate="B" pin="IO_33" pad="127"/>
<connect gate="B" pin="IO_34" pad="128"/>
<connect gate="B" pin="IO_35" pad="131"/>
<connect gate="B" pin="IO_36" pad="132"/>
<connect gate="B" pin="IO_37" pad="133"/>
<connect gate="B" pin="IO_38" pad="134"/>
<connect gate="B" pin="IO_39" pad="135"/>
<connect gate="B" pin="IO_4" pad="74"/>
<connect gate="B" pin="IO_5" pad="75"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="85"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="MSEL0" pad="108"/>
<connect gate="B" pin="MSEL1" pad="107"/>
<connect gate="B" pin="NC" pad="126"/>
<connect gate="B" pin="NCONFIG" pad="105"/>
<connect gate="B" pin="NC_2" pad="113"/>
<connect gate="B" pin="NC_3" pad="114"/>
<connect gate="B" pin="NC_4" pad="139"/>
<connect gate="B" pin="NC_5" pad="125"/>
<connect gate="B" pin="NC_6" pad="140"/>
<connect gate="B" pin="VCCINT" pad="77"/>
<connect gate="B" pin="VCCINT_2" pad="137"/>
<connect gate="B" pin="VCCINT_3" pad="76"/>
<connect gate="B" pin="VCCINT_4" pad="106"/>
<connect gate="B" pin="VCCINT_5" pad="109"/>
<connect gate="B" pin="VCCINT_6" pad="117"/>
<connect gate="B" pin="VCCIO" pad="138"/>
<connect gate="B" pin="VCCIO_2" pad="84"/>
<connect gate="B" pin="VCCIO_3" pad="98"/>
<connect gate="B" pin="VCCIO_4" pad="110"/>
<connect gate="B" pin="VCCIO_5" pad="118"/>
<connect gate="C" pin="CLOCK" pad="183"/>
<connect gate="C" pin="DATA0" pad="156"/>
<connect gate="C" pin="DCLK" pad="155"/>
<connect gate="C" pin="GNDINT" pad="151"/>
<connect gate="C" pin="GNDINT_2" pad="185"/>
<connect gate="C" pin="GNDIO" pad="188"/>
<connect gate="C" pin="GNDIO_2" pad="152"/>
<connect gate="C" pin="GNDIO_3" pad="171"/>
<connect gate="C" pin="GNDIO_4" pad="201"/>
<connect gate="C" pin="INPUT" pad="184"/>
<connect gate="C" pin="INPUT_2" pad="182"/>
<connect gate="C" pin="IO" pad="203"/>
<connect gate="C" pin="IO/CS" pad="207"/>
<connect gate="C" pin="IO/DATA1" pad="157"/>
<connect gate="C" pin="IO/DATA2" pad="158"/>
<connect gate="C" pin="IO/DATA3" pad="159"/>
<connect gate="C" pin="IO/DATA4" pad="161"/>
<connect gate="C" pin="IO/DATA5" pad="162"/>
<connect gate="C" pin="IO/DATA6" pad="164"/>
<connect gate="C" pin="IO/DATA7" pad="166"/>
<connect gate="C" pin="IO/DEV_NCLR" pad="180"/>
<connect gate="C" pin="IO/DEV_OE" pad="186"/>
<connect gate="C" pin="IO/NCS" pad="208"/>
<connect gate="C" pin="IO/NRS" pad="204"/>
<connect gate="C" pin="IO/NWS" pad="206"/>
<connect gate="C" pin="IO_10" pad="169"/>
<connect gate="C" pin="IO_11" pad="148"/>
<connect gate="C" pin="IO_12" pad="170"/>
<connect gate="C" pin="IO_13" pad="160"/>
<connect gate="C" pin="IO_14" pad="172"/>
<connect gate="C" pin="IO_15" pad="149"/>
<connect gate="C" pin="IO_16" pad="173"/>
<connect gate="C" pin="IO_17" pad="150"/>
<connect gate="C" pin="IO_18" pad="174"/>
<connect gate="C" pin="IO_19" pad="175"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="176"/>
<connect gate="C" pin="IO_21" pad="177"/>
<connect gate="C" pin="IO_22" pad="179"/>
<connect gate="C" pin="IO_23" pad="187"/>
<connect gate="C" pin="IO_24" pad="189"/>
<connect gate="C" pin="IO_25" pad="190"/>
<connect gate="C" pin="IO_26" pad="191"/>
<connect gate="C" pin="IO_27" pad="192"/>
<connect gate="C" pin="IO_28" pad="193"/>
<connect gate="C" pin="IO_29" pad="195"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="196"/>
<connect gate="C" pin="IO_31" pad="197"/>
<connect gate="C" pin="IO_32" pad="198"/>
<connect gate="C" pin="IO_33" pad="199"/>
<connect gate="C" pin="IO_34" pad="200"/>
<connect gate="C" pin="IO_35" pad="202"/>
<connect gate="C" pin="IO_36" pad="205"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_5" pad="144"/>
<connect gate="C" pin="IO_6" pad="167"/>
<connect gate="C" pin="IO_7" pad="147"/>
<connect gate="C" pin="IO_8" pad="168"/>
<connect gate="C" pin="IO_9" pad="163"/>
<connect gate="C" pin="NCE" pad="154"/>
<connect gate="C" pin="TDI" pad="153"/>
<connect gate="C" pin="VCCINT" pad="145"/>
<connect gate="C" pin="VCCINT_2" pad="181"/>
<connect gate="C" pin="VCCIO" pad="194"/>
<connect gate="C" pin="VCCIO_2" pad="146"/>
<connect gate="C" pin="VCCIO_3" pad="178"/>
<connect gate="C" pin="VCCIO_4" pad="165"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF10K10QC208-4N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8768"/>
<attribute name="PACKAGE" value="208-PQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K10TC144-3N">
<description>Embedded Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPF10K10TC144-3N_A"/>
<gate name="B" symbol="EPF10K10TC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="58"/>
<connect gate="A" pin="GNDINT_2" pad="16"/>
<connect gate="A" pin="GNDINT_3" pad="57"/>
<connect gate="A" pin="GNDIO" pad="66"/>
<connect gate="A" pin="GNDIO_2" pad="15"/>
<connect gate="A" pin="GNDIO_3" pad="40"/>
<connect gate="A" pin="GNDIO_4" pad="50"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/RDY/NBSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="46"/>
<connect gate="A" pin="IO_31" pad="47"/>
<connect gate="A" pin="IO_32" pad="48"/>
<connect gate="A" pin="IO_33" pad="49"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_44" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="53"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="25"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCIO" pad="71"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="45"/>
<connect gate="A" pin="VCCIO_5" pad="61"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="127"/>
<connect gate="B" pin="GNDINT_2" pad="84"/>
<connect gate="B" pin="GNDINT_3" pad="103"/>
<connect gate="B" pin="GNDIO" pad="139"/>
<connect gate="B" pin="GNDIO_2" pad="85"/>
<connect gate="B" pin="GNDIO_3" pad="104"/>
<connect gate="B" pin="GNDIO_4" pad="129"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="90"/>
<connect gate="B" pin="IO_14" pad="91"/>
<connect gate="B" pin="IO_15" pad="92"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="98"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="99"/>
<connect gate="B" pin="IO_21" pad="100"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="117"/>
<connect gate="B" pin="IO_25" pad="118"/>
<connect gate="B" pin="IO_26" pad="119"/>
<connect gate="B" pin="IO_27" pad="120"/>
<connect gate="B" pin="IO_28" pad="121"/>
<connect gate="B" pin="IO_29" pad="130"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="131"/>
<connect gate="B" pin="IO_31" pad="132"/>
<connect gate="B" pin="IO_32" pad="133"/>
<connect gate="B" pin="IO_33" pad="135"/>
<connect gate="B" pin="IO_34" pad="136"/>
<connect gate="B" pin="IO_35" pad="137"/>
<connect gate="B" pin="IO_36" pad="138"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="75"/>
<connect gate="B" pin="VCCINT_3" pad="93"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF10K10TC144-3N"/>
<attribute name="OC_FARNELL" value="1549377"/>
<attribute name="OC_NEWARK" value="51R8772"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K10TI144-4N">
<description>Embedded Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPF10K10TI144-4N_A"/>
<gate name="B" symbol="EPF10K10TI144-4N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="58"/>
<connect gate="A" pin="GNDINT_2" pad="16"/>
<connect gate="A" pin="GNDINT_3" pad="57"/>
<connect gate="A" pin="GNDIO" pad="66"/>
<connect gate="A" pin="GNDIO_2" pad="15"/>
<connect gate="A" pin="GNDIO_3" pad="40"/>
<connect gate="A" pin="GNDIO_4" pad="50"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/RDY/NBSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="46"/>
<connect gate="A" pin="IO_31" pad="47"/>
<connect gate="A" pin="IO_32" pad="48"/>
<connect gate="A" pin="IO_33" pad="49"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_44" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="53"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="25"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCIO" pad="71"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="45"/>
<connect gate="A" pin="VCCIO_5" pad="61"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="127"/>
<connect gate="B" pin="GNDINT_2" pad="84"/>
<connect gate="B" pin="GNDINT_3" pad="103"/>
<connect gate="B" pin="GNDIO" pad="139"/>
<connect gate="B" pin="GNDIO_2" pad="85"/>
<connect gate="B" pin="GNDIO_3" pad="104"/>
<connect gate="B" pin="GNDIO_4" pad="129"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="90"/>
<connect gate="B" pin="IO_14" pad="91"/>
<connect gate="B" pin="IO_15" pad="92"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="98"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="99"/>
<connect gate="B" pin="IO_21" pad="100"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="117"/>
<connect gate="B" pin="IO_25" pad="118"/>
<connect gate="B" pin="IO_26" pad="119"/>
<connect gate="B" pin="IO_27" pad="120"/>
<connect gate="B" pin="IO_28" pad="121"/>
<connect gate="B" pin="IO_29" pad="130"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="131"/>
<connect gate="B" pin="IO_31" pad="132"/>
<connect gate="B" pin="IO_32" pad="133"/>
<connect gate="B" pin="IO_33" pad="135"/>
<connect gate="B" pin="IO_34" pad="136"/>
<connect gate="B" pin="IO_35" pad="137"/>
<connect gate="B" pin="IO_36" pad="138"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="75"/>
<connect gate="B" pin="VCCINT_3" pad="93"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF10K10TI144-4N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8776"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K20TC144-3N">
<description>Embedded Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPF10K20TC144-3N_A"/>
<gate name="B" symbol="EPF10K20TC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="58"/>
<connect gate="A" pin="GNDINT_2" pad="16"/>
<connect gate="A" pin="GNDINT_3" pad="57"/>
<connect gate="A" pin="GNDIO" pad="66"/>
<connect gate="A" pin="GNDIO_2" pad="15"/>
<connect gate="A" pin="GNDIO_3" pad="40"/>
<connect gate="A" pin="GNDIO_4" pad="50"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/RDY/NBSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="46"/>
<connect gate="A" pin="IO_31" pad="47"/>
<connect gate="A" pin="IO_32" pad="48"/>
<connect gate="A" pin="IO_33" pad="49"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_44" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="53"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="25"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCIO" pad="71"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="45"/>
<connect gate="A" pin="VCCIO_5" pad="61"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="127"/>
<connect gate="B" pin="GNDINT_2" pad="84"/>
<connect gate="B" pin="GNDINT_3" pad="103"/>
<connect gate="B" pin="GNDIO" pad="139"/>
<connect gate="B" pin="GNDIO_2" pad="85"/>
<connect gate="B" pin="GNDIO_3" pad="104"/>
<connect gate="B" pin="GNDIO_4" pad="129"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="90"/>
<connect gate="B" pin="IO_14" pad="91"/>
<connect gate="B" pin="IO_15" pad="92"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="98"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="99"/>
<connect gate="B" pin="IO_21" pad="100"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="117"/>
<connect gate="B" pin="IO_25" pad="118"/>
<connect gate="B" pin="IO_26" pad="119"/>
<connect gate="B" pin="IO_27" pad="120"/>
<connect gate="B" pin="IO_28" pad="121"/>
<connect gate="B" pin="IO_29" pad="130"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="131"/>
<connect gate="B" pin="IO_31" pad="132"/>
<connect gate="B" pin="IO_32" pad="133"/>
<connect gate="B" pin="IO_33" pad="135"/>
<connect gate="B" pin="IO_34" pad="136"/>
<connect gate="B" pin="IO_35" pad="137"/>
<connect gate="B" pin="IO_36" pad="138"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="75"/>
<connect gate="B" pin="VCCINT_3" pad="93"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF10K20TC144-3N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8892"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K20TI144-4N">
<description>Embedded Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPF10K20TI144-4N_A"/>
<gate name="B" symbol="EPF10K20TI144-4N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="58"/>
<connect gate="A" pin="GNDINT_2" pad="16"/>
<connect gate="A" pin="GNDINT_3" pad="57"/>
<connect gate="A" pin="GNDIO" pad="66"/>
<connect gate="A" pin="GNDIO_2" pad="15"/>
<connect gate="A" pin="GNDIO_3" pad="40"/>
<connect gate="A" pin="GNDIO_4" pad="50"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/RDY/NBSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="46"/>
<connect gate="A" pin="IO_31" pad="47"/>
<connect gate="A" pin="IO_32" pad="48"/>
<connect gate="A" pin="IO_33" pad="49"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_44" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="53"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="25"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCIO" pad="71"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="45"/>
<connect gate="A" pin="VCCIO_5" pad="61"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="127"/>
<connect gate="B" pin="GNDINT_2" pad="84"/>
<connect gate="B" pin="GNDINT_3" pad="103"/>
<connect gate="B" pin="GNDIO" pad="139"/>
<connect gate="B" pin="GNDIO_2" pad="85"/>
<connect gate="B" pin="GNDIO_3" pad="104"/>
<connect gate="B" pin="GNDIO_4" pad="129"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="90"/>
<connect gate="B" pin="IO_14" pad="91"/>
<connect gate="B" pin="IO_15" pad="92"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="98"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="99"/>
<connect gate="B" pin="IO_21" pad="100"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="117"/>
<connect gate="B" pin="IO_25" pad="118"/>
<connect gate="B" pin="IO_26" pad="119"/>
<connect gate="B" pin="IO_27" pad="120"/>
<connect gate="B" pin="IO_28" pad="121"/>
<connect gate="B" pin="IO_29" pad="130"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="131"/>
<connect gate="B" pin="IO_31" pad="132"/>
<connect gate="B" pin="IO_32" pad="133"/>
<connect gate="B" pin="IO_33" pad="135"/>
<connect gate="B" pin="IO_34" pad="136"/>
<connect gate="B" pin="IO_35" pad="137"/>
<connect gate="B" pin="IO_36" pad="138"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="75"/>
<connect gate="B" pin="VCCINT_3" pad="93"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF10K20TI144-4N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8895"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30ATC144-3N">
<description>Embedded Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPF10K30ATC144-3N_A"/>
<gate name="B" symbol="EPF10K30ATC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="CLOCK" pad="55"/>
<connect gate="A" pin="CONF_DONE" pad="2"/>
<connect gate="A" pin="GNDINT" pad="58"/>
<connect gate="A" pin="GNDINT_2" pad="16"/>
<connect gate="A" pin="GNDINT_3" pad="57"/>
<connect gate="A" pin="GNDIO" pad="66"/>
<connect gate="A" pin="GNDIO_2" pad="15"/>
<connect gate="A" pin="GNDIO_3" pad="40"/>
<connect gate="A" pin="GNDIO_4" pad="50"/>
<connect gate="A" pin="INPUT" pad="56"/>
<connect gate="A" pin="INPUT_2" pad="54"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/CLKUSR" pad="7"/>
<connect gate="A" pin="IO/INIT_DONE" pad="14"/>
<connect gate="A" pin="IO/RDY/NBSY" pad="11"/>
<connect gate="A" pin="IO_10" pad="20"/>
<connect gate="A" pin="IO_11" pad="21"/>
<connect gate="A" pin="IO_12" pad="22"/>
<connect gate="A" pin="IO_13" pad="23"/>
<connect gate="A" pin="IO_14" pad="26"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="9"/>
<connect gate="A" pin="IO_30" pad="46"/>
<connect gate="A" pin="IO_31" pad="47"/>
<connect gate="A" pin="IO_32" pad="48"/>
<connect gate="A" pin="IO_33" pad="49"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="59"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="64"/>
<connect gate="A" pin="IO_4" pad="10"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_44" pad="70"/>
<connect gate="A" pin="IO_5" pad="12"/>
<connect gate="A" pin="IO_6" pad="13"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="19"/>
<connect gate="A" pin="NCEO" pad="3"/>
<connect gate="A" pin="NSTATUS" pad="35"/>
<connect gate="A" pin="TCK" pad="1"/>
<connect gate="A" pin="TDO" pad="4"/>
<connect gate="A" pin="TMS" pad="34"/>
<connect gate="A" pin="VCCINT" pad="53"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="25"/>
<connect gate="A" pin="VCCINT_4" pad="52"/>
<connect gate="A" pin="VCCIO" pad="71"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="24"/>
<connect gate="A" pin="VCCIO_4" pad="45"/>
<connect gate="A" pin="VCCIO_5" pad="61"/>
<connect gate="B" pin="CLOCK" pad="125"/>
<connect gate="B" pin="DATA0" pad="108"/>
<connect gate="B" pin="DCLK" pad="107"/>
<connect gate="B" pin="GNDINT" pad="127"/>
<connect gate="B" pin="GNDINT_2" pad="84"/>
<connect gate="B" pin="GNDINT_3" pad="103"/>
<connect gate="B" pin="GNDIO" pad="139"/>
<connect gate="B" pin="GNDIO_2" pad="85"/>
<connect gate="B" pin="GNDIO_3" pad="104"/>
<connect gate="B" pin="GNDIO_4" pad="129"/>
<connect gate="B" pin="INPUT" pad="126"/>
<connect gate="B" pin="INPUT_2" pad="124"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/CS" pad="143"/>
<connect gate="B" pin="IO/DATA1" pad="109"/>
<connect gate="B" pin="IO/DATA2" pad="110"/>
<connect gate="B" pin="IO/DATA3" pad="111"/>
<connect gate="B" pin="IO/DATA4" pad="112"/>
<connect gate="B" pin="IO/DATA5" pad="113"/>
<connect gate="B" pin="IO/DATA6" pad="114"/>
<connect gate="B" pin="IO/DATA7" pad="116"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="122"/>
<connect gate="B" pin="IO/DEV_OE" pad="128"/>
<connect gate="B" pin="IO/NCS" pad="144"/>
<connect gate="B" pin="IO/NRS" pad="141"/>
<connect gate="B" pin="IO/NWS" pad="142"/>
<connect gate="B" pin="IO_10" pad="87"/>
<connect gate="B" pin="IO_11" pad="88"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="90"/>
<connect gate="B" pin="IO_14" pad="91"/>
<connect gate="B" pin="IO_15" pad="92"/>
<connect gate="B" pin="IO_16" pad="95"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="97"/>
<connect gate="B" pin="IO_19" pad="98"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="99"/>
<connect gate="B" pin="IO_21" pad="100"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="117"/>
<connect gate="B" pin="IO_25" pad="118"/>
<connect gate="B" pin="IO_26" pad="119"/>
<connect gate="B" pin="IO_27" pad="120"/>
<connect gate="B" pin="IO_28" pad="121"/>
<connect gate="B" pin="IO_29" pad="130"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="131"/>
<connect gate="B" pin="IO_31" pad="132"/>
<connect gate="B" pin="IO_32" pad="133"/>
<connect gate="B" pin="IO_33" pad="135"/>
<connect gate="B" pin="IO_34" pad="136"/>
<connect gate="B" pin="IO_35" pad="137"/>
<connect gate="B" pin="IO_36" pad="138"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="86"/>
<connect gate="B" pin="MSEL0" pad="77"/>
<connect gate="B" pin="MSEL1" pad="76"/>
<connect gate="B" pin="NCE" pad="106"/>
<connect gate="B" pin="NCONFIG" pad="74"/>
<connect gate="B" pin="TDI" pad="105"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="75"/>
<connect gate="B" pin="VCCINT_3" pad="93"/>
<connect gate="B" pin="VCCIO" pad="134"/>
<connect gate="B" pin="VCCIO_2" pad="94"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF10K30ATC144-3N"/>
<attribute name="OC_FARNELL" value="1549379"/>
<attribute name="OC_NEWARK" value="51R8966"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF6016ATC144-3N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPF6016ATC144-3N_A"/>
<gate name="B" symbol="EPF6016ATC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GND" pad="30"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="54"/>
<connect gate="A" pin="GND_4" pad="18"/>
<connect gate="A" pin="IN" pad="17"/>
<connect gate="A" pin="IN_2" pad="20"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/NCEO" pad="70"/>
<connect gate="A" pin="IO/TCK" pad="34"/>
<connect gate="A" pin="IO/TDI" pad="13"/>
<connect gate="A" pin="IO/TMS" pad="27"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="16"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="28"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="35"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="43"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="44"/>
<connect gate="A" pin="IO_31" pad="45"/>
<connect gate="A" pin="IO_32" pad="46"/>
<connect gate="A" pin="IO_33" pad="47"/>
<connect gate="A" pin="IO_34" pad="48"/>
<connect gate="A" pin="IO_35" pad="49"/>
<connect gate="A" pin="IO_36" pad="50"/>
<connect gate="A" pin="IO_37" pad="51"/>
<connect gate="A" pin="IO_38" pad="52"/>
<connect gate="A" pin="IO_39" pad="57"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="58"/>
<connect gate="A" pin="IO_41" pad="59"/>
<connect gate="A" pin="IO_42" pad="60"/>
<connect gate="A" pin="IO_43" pad="61"/>
<connect gate="A" pin="IO_44" pad="62"/>
<connect gate="A" pin="IO_45" pad="63"/>
<connect gate="A" pin="IO_46" pad="64"/>
<connect gate="A" pin="IO_47" pad="65"/>
<connect gate="A" pin="IO_48" pad="66"/>
<connect gate="A" pin="IO_49" pad="67"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="68"/>
<connect gate="A" pin="IO_51" pad="69"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="MSEL" pad="33"/>
<connect gate="A" pin="NCE" pad="4"/>
<connect gate="A" pin="NCONFIG" pad="53"/>
<connect gate="A" pin="NSTATUS" pad="56"/>
<connect gate="A" pin="VCCINT" pad="6"/>
<connect gate="A" pin="VCCINT_2" pad="31"/>
<connect gate="A" pin="VCCIO" pad="32"/>
<connect gate="A" pin="VCCIO_2" pad="7"/>
<connect gate="A" pin="VCCIO_3" pad="55"/>
<connect gate="A" pin="VCCIO_4" pad="19"/>
<connect gate="B" pin="CONF_DONE" pad="105"/>
<connect gate="B" pin="DATA" pad="125"/>
<connect gate="B" pin="DCLK" pad="128"/>
<connect gate="B" pin="GND" pad="102"/>
<connect gate="B" pin="GND_2" pad="126"/>
<connect gate="B" pin="GND_3" pad="76"/>
<connect gate="B" pin="GND_4" pad="90"/>
<connect gate="B" pin="IN" pad="89"/>
<connect gate="B" pin="IN_2" pad="92"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/CLKUSR" pad="100"/>
<connect gate="B" pin="IO/CS" pad="114"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="130"/>
<connect gate="B" pin="IO/DEV_OE" pad="123"/>
<connect gate="B" pin="IO/INIT_DONE" pad="94"/>
<connect gate="B" pin="IO/NCS" pad="111"/>
<connect gate="B" pin="IO/NRS" pad="120"/>
<connect gate="B" pin="IO/NWS" pad="117"/>
<connect gate="B" pin="IO/RDYNBUSY" pad="97"/>
<connect gate="B" pin="IO/TDO" pad="73"/>
<connect gate="B" pin="IO_10" pad="82"/>
<connect gate="B" pin="IO_11" pad="83"/>
<connect gate="B" pin="IO_12" pad="98"/>
<connect gate="B" pin="IO_13" pad="84"/>
<connect gate="B" pin="IO_14" pad="106"/>
<connect gate="B" pin="IO_15" pad="99"/>
<connect gate="B" pin="IO_16" pad="107"/>
<connect gate="B" pin="IO_17" pad="85"/>
<connect gate="B" pin="IO_18" pad="108"/>
<connect gate="B" pin="IO_19" pad="86"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="101"/>
<connect gate="B" pin="IO_21" pad="87"/>
<connect gate="B" pin="IO_22" pad="88"/>
<connect gate="B" pin="IO_23" pad="109"/>
<connect gate="B" pin="IO_24" pad="110"/>
<connect gate="B" pin="IO_25" pad="115"/>
<connect gate="B" pin="IO_26" pad="118"/>
<connect gate="B" pin="IO_27" pad="116"/>
<connect gate="B" pin="IO_28" pad="119"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="75"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="131"/>
<connect gate="B" pin="IO_32" pad="124"/>
<connect gate="B" pin="IO_33" pad="132"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="133"/>
<connect gate="B" pin="IO_36" pad="122"/>
<connect gate="B" pin="IO_37" pad="134"/>
<connect gate="B" pin="IO_38" pad="129"/>
<connect gate="B" pin="IO_39" pad="135"/>
<connect gate="B" pin="IO_4" pad="95"/>
<connect gate="B" pin="IO_40" pad="136"/>
<connect gate="B" pin="IO_41" pad="137"/>
<connect gate="B" pin="IO_42" pad="138"/>
<connect gate="B" pin="IO_43" pad="139"/>
<connect gate="B" pin="IO_44" pad="140"/>
<connect gate="B" pin="IO_45" pad="141"/>
<connect gate="B" pin="IO_46" pad="142"/>
<connect gate="B" pin="IO_47" pad="143"/>
<connect gate="B" pin="IO_5" pad="79"/>
<connect gate="B" pin="IO_6" pad="96"/>
<connect gate="B" pin="IO_7" pad="80"/>
<connect gate="B" pin="IO_8" pad="93"/>
<connect gate="B" pin="IO_9" pad="81"/>
<connect gate="B" pin="VCCINT" pad="103"/>
<connect gate="B" pin="VCCINT_2" pad="77"/>
<connect gate="B" pin="VCCIO" pad="104"/>
<connect gate="B" pin="VCCIO_2" pad="91"/>
<connect gate="B" pin="VCCIO_3" pad="127"/>
<connect gate="B" pin="VCCIO_4" pad="78"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF6016ATC144-3N"/>
<attribute name="OC_FARNELL" value="15493964"/>
<attribute name="OC_NEWARK" value="51R9167"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF6016QC208-2N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPF6016QC208-2N_A"/>
<gate name="B" symbol="EPF6016QC208-2N_B"/>
<gate name="C" symbol="EPF6016QC208-2N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="GND" pad="62"/>
<connect gate="A" pin="GND_2" pad="43"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="GND_4" pad="25"/>
<connect gate="A" pin="INPUT" pad="28"/>
<connect gate="A" pin="INPUT_2" pad="24"/>
<connect gate="A" pin="IO" pad="61"/>
<connect gate="A" pin="IO/TCK" pad="47"/>
<connect gate="A" pin="IO/TDI" pad="19"/>
<connect gate="A" pin="IO/TMS" pad="38"/>
<connect gate="A" pin="IO_10" pad="32"/>
<connect gate="A" pin="IO_11" pad="18"/>
<connect gate="A" pin="IO_12" pad="33"/>
<connect gate="A" pin="IO_13" pad="34"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="35"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="22"/>
<connect gate="A" pin="IO_18" pad="23"/>
<connect gate="A" pin="IO_19" pad="1"/>
<connect gate="A" pin="IO_2" pad="10"/>
<connect gate="A" pin="IO_20" pad="2"/>
<connect gate="A" pin="IO_21" pad="3"/>
<connect gate="A" pin="IO_22" pad="4"/>
<connect gate="A" pin="IO_23" pad="5"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_29" pad="41"/>
<connect gate="A" pin="IO_3" pad="11"/>
<connect gate="A" pin="IO_30" pad="64"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="65"/>
<connect gate="A" pin="IO_33" pad="66"/>
<connect gate="A" pin="IO_34" pad="36"/>
<connect gate="A" pin="IO_35" pad="67"/>
<connect gate="A" pin="IO_36" pad="37"/>
<connect gate="A" pin="IO_37" pad="68"/>
<connect gate="A" pin="IO_38" pad="69"/>
<connect gate="A" pin="IO_39" pad="70"/>
<connect gate="A" pin="IO_4" pad="12"/>
<connect gate="A" pin="IO_40" pad="48"/>
<connect gate="A" pin="IO_41" pad="49"/>
<connect gate="A" pin="IO_42" pad="50"/>
<connect gate="A" pin="IO_43" pad="51"/>
<connect gate="A" pin="IO_44" pad="52"/>
<connect gate="A" pin="IO_45" pad="53"/>
<connect gate="A" pin="IO_46" pad="54"/>
<connect gate="A" pin="IO_47" pad="55"/>
<connect gate="A" pin="IO_48" pad="56"/>
<connect gate="A" pin="IO_49" pad="57"/>
<connect gate="A" pin="IO_5" pad="13"/>
<connect gate="A" pin="IO_50" pad="58"/>
<connect gate="A" pin="IO_51" pad="59"/>
<connect gate="A" pin="IO_52" pad="60"/>
<connect gate="A" pin="IO_6" pad="14"/>
<connect gate="A" pin="IO_7" pad="15"/>
<connect gate="A" pin="IO_8" pad="16"/>
<connect gate="A" pin="IO_9" pad="17"/>
<connect gate="A" pin="MSEL" pad="46"/>
<connect gate="A" pin="NCE" pad="6"/>
<connect gate="A" pin="VCCINT" pad="8"/>
<connect gate="A" pin="VCCINT_2" pad="26"/>
<connect gate="A" pin="VCCINT_3" pad="44"/>
<connect gate="A" pin="VCCIO" pad="45"/>
<connect gate="A" pin="VCCIO_2" pad="63"/>
<connect gate="A" pin="VCCIO_3" pad="9"/>
<connect gate="A" pin="VCCIO_4" pad="27"/>
<connect gate="B" pin="GND" pad="129"/>
<connect gate="B" pin="GND_2" pad="110"/>
<connect gate="B" pin="GND_3" pad="95"/>
<connect gate="B" pin="GND_4" pad="78"/>
<connect gate="B" pin="INPUT" pad="132"/>
<connect gate="B" pin="INPUT_2" pad="128"/>
<connect gate="B" pin="IO" pad="139"/>
<connect gate="B" pin="IO/INIT_DONE" pad="135"/>
<connect gate="B" pin="IO/NCEO" pad="102"/>
<connect gate="B" pin="IO/RDYNBUSY" pad="140"/>
<connect gate="B" pin="IO/TDO" pad="107"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="72"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="73"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="74"/>
<connect gate="B" pin="IO_16" pad="91"/>
<connect gate="B" pin="IO_17" pad="75"/>
<connect gate="B" pin="IO_18" pad="92"/>
<connect gate="B" pin="IO_19" pad="76"/>
<connect gate="B" pin="IO_2" pad="81"/>
<connect gate="B" pin="IO_20" pad="93"/>
<connect gate="B" pin="IO_21" pad="94"/>
<connect gate="B" pin="IO_22" pad="97"/>
<connect gate="B" pin="IO_23" pad="98"/>
<connect gate="B" pin="IO_24" pad="99"/>
<connect gate="B" pin="IO_25" pad="100"/>
<connect gate="B" pin="IO_26" pad="101"/>
<connect gate="B" pin="IO_27" pad="103"/>
<connect gate="B" pin="IO_28" pad="104"/>
<connect gate="B" pin="IO_29" pad="105"/>
<connect gate="B" pin="IO_3" pad="82"/>
<connect gate="B" pin="IO_30" pad="106"/>
<connect gate="B" pin="IO_31" pad="108"/>
<connect gate="B" pin="IO_32" pad="109"/>
<connect gate="B" pin="IO_33" pad="113"/>
<connect gate="B" pin="IO_34" pad="114"/>
<connect gate="B" pin="IO_35" pad="115"/>
<connect gate="B" pin="IO_36" pad="116"/>
<connect gate="B" pin="IO_37" pad="117"/>
<connect gate="B" pin="IO_38" pad="118"/>
<connect gate="B" pin="IO_39" pad="119"/>
<connect gate="B" pin="IO_4" pad="83"/>
<connect gate="B" pin="IO_40" pad="120"/>
<connect gate="B" pin="IO_41" pad="121"/>
<connect gate="B" pin="IO_42" pad="122"/>
<connect gate="B" pin="IO_43" pad="133"/>
<connect gate="B" pin="IO_44" pad="123"/>
<connect gate="B" pin="IO_45" pad="134"/>
<connect gate="B" pin="IO_46" pad="124"/>
<connect gate="B" pin="IO_47" pad="125"/>
<connect gate="B" pin="IO_48" pad="136"/>
<connect gate="B" pin="IO_49" pad="126"/>
<connect gate="B" pin="IO_5" pad="84"/>
<connect gate="B" pin="IO_50" pad="137"/>
<connect gate="B" pin="IO_51" pad="127"/>
<connect gate="B" pin="IO_52" pad="138"/>
<connect gate="B" pin="IO_6" pad="85"/>
<connect gate="B" pin="IO_7" pad="86"/>
<connect gate="B" pin="IO_8" pad="87"/>
<connect gate="B" pin="IO_9" pad="71"/>
<connect gate="B" pin="NCONFIG" pad="77"/>
<connect gate="B" pin="NSTATUS" pad="80"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="111"/>
<connect gate="B" pin="VCCIO" pad="131"/>
<connect gate="B" pin="VCCIO_2" pad="79"/>
<connect gate="B" pin="VCCIO_3" pad="96"/>
<connect gate="B" pin="VCCIO_4" pad="112"/>
<connect gate="C" pin="CLKUSR" pad="144"/>
<connect gate="C" pin="CONF_DONE" pad="150"/>
<connect gate="C" pin="DATA" pad="181"/>
<connect gate="C" pin="DCLK" pad="184"/>
<connect gate="C" pin="GND" pad="199"/>
<connect gate="C" pin="GND_2" pad="147"/>
<connect gate="C" pin="GND_3" pad="165"/>
<connect gate="C" pin="GND_4" pad="182"/>
<connect gate="C" pin="IO" pad="208"/>
<connect gate="C" pin="IO/CS" pad="162"/>
<connect gate="C" pin="IO/DEV_CLRN" pad="187"/>
<connect gate="C" pin="IO/DEV_OE" pad="178"/>
<connect gate="C" pin="IO/NCS" pad="159"/>
<connect gate="C" pin="IO/NRS" pad="174"/>
<connect gate="C" pin="IO/NWS" pad="169"/>
<connect gate="C" pin="IO_10" pad="154"/>
<connect gate="C" pin="IO_11" pad="155"/>
<connect gate="C" pin="IO_12" pad="156"/>
<connect gate="C" pin="IO_13" pad="157"/>
<connect gate="C" pin="IO_14" pad="158"/>
<connect gate="C" pin="IO_15" pad="163"/>
<connect gate="C" pin="IO_16" pad="160"/>
<connect gate="C" pin="IO_17" pad="164"/>
<connect gate="C" pin="IO_18" pad="161"/>
<connect gate="C" pin="IO_19" pad="168"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="167"/>
<connect gate="C" pin="IO_21" pad="170"/>
<connect gate="C" pin="IO_22" pad="171"/>
<connect gate="C" pin="IO_23" pad="172"/>
<connect gate="C" pin="IO_24" pad="173"/>
<connect gate="C" pin="IO_25" pad="175"/>
<connect gate="C" pin="IO_26" pad="176"/>
<connect gate="C" pin="IO_27" pad="177"/>
<connect gate="C" pin="IO_28" pad="188"/>
<connect gate="C" pin="IO_29" pad="179"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="189"/>
<connect gate="C" pin="IO_31" pad="180"/>
<connect gate="C" pin="IO_32" pad="190"/>
<connect gate="C" pin="IO_33" pad="185"/>
<connect gate="C" pin="IO_34" pad="191"/>
<connect gate="C" pin="IO_35" pad="186"/>
<connect gate="C" pin="IO_36" pad="192"/>
<connect gate="C" pin="IO_37" pad="193"/>
<connect gate="C" pin="IO_38" pad="194"/>
<connect gate="C" pin="IO_39" pad="195"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_40" pad="196"/>
<connect gate="C" pin="IO_41" pad="197"/>
<connect gate="C" pin="IO_42" pad="198"/>
<connect gate="C" pin="IO_43" pad="201"/>
<connect gate="C" pin="IO_44" pad="202"/>
<connect gate="C" pin="IO_45" pad="203"/>
<connect gate="C" pin="IO_46" pad="204"/>
<connect gate="C" pin="IO_47" pad="205"/>
<connect gate="C" pin="IO_48" pad="206"/>
<connect gate="C" pin="IO_49" pad="207"/>
<connect gate="C" pin="IO_5" pad="145"/>
<connect gate="C" pin="IO_6" pad="151"/>
<connect gate="C" pin="IO_7" pad="146"/>
<connect gate="C" pin="IO_8" pad="152"/>
<connect gate="C" pin="IO_9" pad="153"/>
<connect gate="C" pin="VCCINT" pad="148"/>
<connect gate="C" pin="VCCIO" pad="200"/>
<connect gate="C" pin="VCCIO_2" pad="166"/>
<connect gate="C" pin="VCCIO_3" pad="149"/>
<connect gate="C" pin="VCCIO_4" pad="183"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF6016QC208-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9176"/>
<attribute name="PACKAGE" value="PQFP-208"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF6016TC144-2N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPF6016TC144-2N_A"/>
<gate name="B" symbol="EPF6016TC144-2N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GND" pad="30"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="54"/>
<connect gate="A" pin="GND_4" pad="18"/>
<connect gate="A" pin="IN" pad="17"/>
<connect gate="A" pin="IN_2" pad="20"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/NCEO" pad="70"/>
<connect gate="A" pin="IO/TCK" pad="34"/>
<connect gate="A" pin="IO/TDI" pad="13"/>
<connect gate="A" pin="IO/TMS" pad="27"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="16"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="28"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="35"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="43"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="44"/>
<connect gate="A" pin="IO_31" pad="45"/>
<connect gate="A" pin="IO_32" pad="46"/>
<connect gate="A" pin="IO_33" pad="47"/>
<connect gate="A" pin="IO_34" pad="48"/>
<connect gate="A" pin="IO_35" pad="49"/>
<connect gate="A" pin="IO_36" pad="50"/>
<connect gate="A" pin="IO_37" pad="51"/>
<connect gate="A" pin="IO_38" pad="52"/>
<connect gate="A" pin="IO_39" pad="57"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="58"/>
<connect gate="A" pin="IO_41" pad="59"/>
<connect gate="A" pin="IO_42" pad="60"/>
<connect gate="A" pin="IO_43" pad="61"/>
<connect gate="A" pin="IO_44" pad="62"/>
<connect gate="A" pin="IO_45" pad="63"/>
<connect gate="A" pin="IO_46" pad="64"/>
<connect gate="A" pin="IO_47" pad="65"/>
<connect gate="A" pin="IO_48" pad="66"/>
<connect gate="A" pin="IO_49" pad="67"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="68"/>
<connect gate="A" pin="IO_51" pad="69"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="MSEL" pad="33"/>
<connect gate="A" pin="NCE" pad="4"/>
<connect gate="A" pin="NCONFIG" pad="53"/>
<connect gate="A" pin="NSTATUS" pad="56"/>
<connect gate="A" pin="VCCINT" pad="6"/>
<connect gate="A" pin="VCCINT_2" pad="31"/>
<connect gate="A" pin="VCCIO" pad="32"/>
<connect gate="A" pin="VCCIO_2" pad="7"/>
<connect gate="A" pin="VCCIO_3" pad="55"/>
<connect gate="A" pin="VCCIO_4" pad="19"/>
<connect gate="B" pin="CONF_DONE" pad="105"/>
<connect gate="B" pin="DATA" pad="125"/>
<connect gate="B" pin="DCLK" pad="128"/>
<connect gate="B" pin="GND" pad="102"/>
<connect gate="B" pin="GND_2" pad="126"/>
<connect gate="B" pin="GND_3" pad="76"/>
<connect gate="B" pin="GND_4" pad="90"/>
<connect gate="B" pin="IN" pad="89"/>
<connect gate="B" pin="IN_2" pad="92"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/CLKUSR" pad="100"/>
<connect gate="B" pin="IO/CS" pad="114"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="130"/>
<connect gate="B" pin="IO/DEV_OE" pad="123"/>
<connect gate="B" pin="IO/INIT_DONE" pad="94"/>
<connect gate="B" pin="IO/NCS" pad="111"/>
<connect gate="B" pin="IO/NRS" pad="120"/>
<connect gate="B" pin="IO/NWS" pad="117"/>
<connect gate="B" pin="IO/RDYNBUSY" pad="97"/>
<connect gate="B" pin="IO/TDO" pad="73"/>
<connect gate="B" pin="IO_10" pad="82"/>
<connect gate="B" pin="IO_11" pad="83"/>
<connect gate="B" pin="IO_12" pad="98"/>
<connect gate="B" pin="IO_13" pad="84"/>
<connect gate="B" pin="IO_14" pad="106"/>
<connect gate="B" pin="IO_15" pad="99"/>
<connect gate="B" pin="IO_16" pad="107"/>
<connect gate="B" pin="IO_17" pad="85"/>
<connect gate="B" pin="IO_18" pad="108"/>
<connect gate="B" pin="IO_19" pad="86"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="101"/>
<connect gate="B" pin="IO_21" pad="87"/>
<connect gate="B" pin="IO_22" pad="88"/>
<connect gate="B" pin="IO_23" pad="109"/>
<connect gate="B" pin="IO_24" pad="110"/>
<connect gate="B" pin="IO_25" pad="115"/>
<connect gate="B" pin="IO_26" pad="118"/>
<connect gate="B" pin="IO_27" pad="116"/>
<connect gate="B" pin="IO_28" pad="119"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="75"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="131"/>
<connect gate="B" pin="IO_32" pad="124"/>
<connect gate="B" pin="IO_33" pad="132"/>
<connect gate="B" pin="IO_34" pad="121"/>
<connect gate="B" pin="IO_35" pad="133"/>
<connect gate="B" pin="IO_36" pad="122"/>
<connect gate="B" pin="IO_37" pad="134"/>
<connect gate="B" pin="IO_38" pad="129"/>
<connect gate="B" pin="IO_39" pad="135"/>
<connect gate="B" pin="IO_4" pad="95"/>
<connect gate="B" pin="IO_40" pad="136"/>
<connect gate="B" pin="IO_41" pad="137"/>
<connect gate="B" pin="IO_42" pad="138"/>
<connect gate="B" pin="IO_43" pad="139"/>
<connect gate="B" pin="IO_44" pad="140"/>
<connect gate="B" pin="IO_45" pad="141"/>
<connect gate="B" pin="IO_46" pad="142"/>
<connect gate="B" pin="IO_47" pad="143"/>
<connect gate="B" pin="IO_5" pad="79"/>
<connect gate="B" pin="IO_6" pad="96"/>
<connect gate="B" pin="IO_7" pad="80"/>
<connect gate="B" pin="IO_8" pad="93"/>
<connect gate="B" pin="IO_9" pad="81"/>
<connect gate="B" pin="VCCINT" pad="103"/>
<connect gate="B" pin="VCCINT_2" pad="77"/>
<connect gate="B" pin="VCCIO" pad="104"/>
<connect gate="B" pin="VCCIO_2" pad="91"/>
<connect gate="B" pin="VCCIO_3" pad="127"/>
<connect gate="B" pin="VCCIO_4" pad="78"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF6016TC144-2N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9186"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF6016TC144-3N" prefix="U">
<description>IC FLEX 6000 FPGA 16K 144-TQFP</description>
<gates>
<gate name="A" symbol="EPF6016TC144-3N_A"/>
<gate name="B" symbol="EPF6016TC144-3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="*CE" pad="4"/>
<connect gate="A" pin="*CONFIG" pad="53"/>
<connect gate="A" pin="*STATUS" pad="56"/>
<connect gate="A" pin="GND" pad="30"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="54"/>
<connect gate="A" pin="GND_4" pad="18"/>
<connect gate="A" pin="INPUT" pad="17"/>
<connect gate="A" pin="INPUT_2" pad="20"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/*CEO" pad="70"/>
<connect gate="A" pin="IO/TCK" pad="34"/>
<connect gate="A" pin="IO/TDI" pad="13"/>
<connect gate="A" pin="IO/TMS" pad="27"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="16"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="28"/>
<connect gate="A" pin="IO_19" pad="26"/>
<connect gate="A" pin="IO_2" pad="8"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="35"/>
<connect gate="A" pin="IO_22" pad="36"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="43"/>
<connect gate="A" pin="IO_3" pad="1"/>
<connect gate="A" pin="IO_30" pad="44"/>
<connect gate="A" pin="IO_31" pad="45"/>
<connect gate="A" pin="IO_32" pad="46"/>
<connect gate="A" pin="IO_33" pad="47"/>
<connect gate="A" pin="IO_34" pad="48"/>
<connect gate="A" pin="IO_35" pad="49"/>
<connect gate="A" pin="IO_36" pad="50"/>
<connect gate="A" pin="IO_37" pad="51"/>
<connect gate="A" pin="IO_38" pad="52"/>
<connect gate="A" pin="IO_39" pad="57"/>
<connect gate="A" pin="IO_4" pad="9"/>
<connect gate="A" pin="IO_40" pad="58"/>
<connect gate="A" pin="IO_41" pad="59"/>
<connect gate="A" pin="IO_42" pad="60"/>
<connect gate="A" pin="IO_43" pad="61"/>
<connect gate="A" pin="IO_44" pad="62"/>
<connect gate="A" pin="IO_45" pad="63"/>
<connect gate="A" pin="IO_46" pad="64"/>
<connect gate="A" pin="IO_47" pad="65"/>
<connect gate="A" pin="IO_48" pad="66"/>
<connect gate="A" pin="IO_49" pad="67"/>
<connect gate="A" pin="IO_5" pad="2"/>
<connect gate="A" pin="IO_50" pad="68"/>
<connect gate="A" pin="IO_51" pad="69"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="10"/>
<connect gate="A" pin="IO_7" pad="3"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="MSEL" pad="33"/>
<connect gate="A" pin="VCCINT" pad="31"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCIO" pad="19"/>
<connect gate="A" pin="VCCIO_2" pad="32"/>
<connect gate="A" pin="VCCIO_3" pad="7"/>
<connect gate="A" pin="VCCIO_4" pad="55"/>
<connect gate="B" pin="CONF_DONE" pad="105"/>
<connect gate="B" pin="DATA" pad="125"/>
<connect gate="B" pin="DCLK" pad="128"/>
<connect gate="B" pin="GND" pad="126"/>
<connect gate="B" pin="GND_2" pad="90"/>
<connect gate="B" pin="GND_3" pad="76"/>
<connect gate="B" pin="GND_4" pad="102"/>
<connect gate="B" pin="INPUT" pad="92"/>
<connect gate="B" pin="INPUT_2" pad="89"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/*CS" pad="111"/>
<connect gate="B" pin="IO/*RS" pad="120"/>
<connect gate="B" pin="IO/*WS" pad="117"/>
<connect gate="B" pin="IO/CLKUSR" pad="100"/>
<connect gate="B" pin="IO/CS" pad="114"/>
<connect gate="B" pin="IO/DEV_*CLR" pad="130"/>
<connect gate="B" pin="IO/DEV_OE" pad="123"/>
<connect gate="B" pin="IO/INIT_DONE" pad="94"/>
<connect gate="B" pin="IO/RDY/*BUSY" pad="97"/>
<connect gate="B" pin="IO/TDO" pad="73"/>
<connect gate="B" pin="IO_10" pad="85"/>
<connect gate="B" pin="IO_11" pad="86"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="88"/>
<connect gate="B" pin="IO_14" pad="93"/>
<connect gate="B" pin="IO_15" pad="95"/>
<connect gate="B" pin="IO_16" pad="96"/>
<connect gate="B" pin="IO_17" pad="98"/>
<connect gate="B" pin="IO_18" pad="99"/>
<connect gate="B" pin="IO_19" pad="101"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="106"/>
<connect gate="B" pin="IO_21" pad="107"/>
<connect gate="B" pin="IO_22" pad="108"/>
<connect gate="B" pin="IO_23" pad="109"/>
<connect gate="B" pin="IO_24" pad="110"/>
<connect gate="B" pin="IO_25" pad="112"/>
<connect gate="B" pin="IO_26" pad="113"/>
<connect gate="B" pin="IO_27" pad="115"/>
<connect gate="B" pin="IO_28" pad="116"/>
<connect gate="B" pin="IO_29" pad="118"/>
<connect gate="B" pin="IO_3" pad="75"/>
<connect gate="B" pin="IO_30" pad="119"/>
<connect gate="B" pin="IO_31" pad="121"/>
<connect gate="B" pin="IO_32" pad="122"/>
<connect gate="B" pin="IO_33" pad="129"/>
<connect gate="B" pin="IO_34" pad="124"/>
<connect gate="B" pin="IO_35" pad="131"/>
<connect gate="B" pin="IO_36" pad="132"/>
<connect gate="B" pin="IO_37" pad="133"/>
<connect gate="B" pin="IO_38" pad="134"/>
<connect gate="B" pin="IO_39" pad="135"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_40" pad="136"/>
<connect gate="B" pin="IO_41" pad="137"/>
<connect gate="B" pin="IO_42" pad="138"/>
<connect gate="B" pin="IO_43" pad="139"/>
<connect gate="B" pin="IO_44" pad="140"/>
<connect gate="B" pin="IO_45" pad="141"/>
<connect gate="B" pin="IO_46" pad="142"/>
<connect gate="B" pin="IO_47" pad="143"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="84"/>
<connect gate="B" pin="VCCINT" pad="103"/>
<connect gate="B" pin="VCCINT_2" pad="77"/>
<connect gate="B" pin="VCCIO" pad="78"/>
<connect gate="B" pin="VCCIO_2" pad="91"/>
<connect gate="B" pin="VCCIO_3" pad="127"/>
<connect gate="B" pin="VCCIO_4" pad="104"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF6016TC144-3N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R0481"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF6024AQC208-3N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPF6024AQC208-3N_A"/>
<gate name="B" symbol="EPF6024AQC208-3N_B"/>
<gate name="C" symbol="EPF6024AQC208-3N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="GND" pad="62"/>
<connect gate="A" pin="GND_2" pad="43"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="GND_4" pad="25"/>
<connect gate="A" pin="INPUT" pad="28"/>
<connect gate="A" pin="INPUT_2" pad="24"/>
<connect gate="A" pin="IO" pad="61"/>
<connect gate="A" pin="IO/TCK" pad="47"/>
<connect gate="A" pin="IO/TDI" pad="19"/>
<connect gate="A" pin="IO/TMS" pad="38"/>
<connect gate="A" pin="IO_10" pad="32"/>
<connect gate="A" pin="IO_11" pad="18"/>
<connect gate="A" pin="IO_12" pad="33"/>
<connect gate="A" pin="IO_13" pad="34"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="35"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="22"/>
<connect gate="A" pin="IO_18" pad="23"/>
<connect gate="A" pin="IO_19" pad="1"/>
<connect gate="A" pin="IO_2" pad="10"/>
<connect gate="A" pin="IO_20" pad="2"/>
<connect gate="A" pin="IO_21" pad="3"/>
<connect gate="A" pin="IO_22" pad="4"/>
<connect gate="A" pin="IO_23" pad="5"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_29" pad="41"/>
<connect gate="A" pin="IO_3" pad="11"/>
<connect gate="A" pin="IO_30" pad="64"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="65"/>
<connect gate="A" pin="IO_33" pad="66"/>
<connect gate="A" pin="IO_34" pad="36"/>
<connect gate="A" pin="IO_35" pad="67"/>
<connect gate="A" pin="IO_36" pad="37"/>
<connect gate="A" pin="IO_37" pad="68"/>
<connect gate="A" pin="IO_38" pad="69"/>
<connect gate="A" pin="IO_39" pad="70"/>
<connect gate="A" pin="IO_4" pad="12"/>
<connect gate="A" pin="IO_40" pad="48"/>
<connect gate="A" pin="IO_41" pad="49"/>
<connect gate="A" pin="IO_42" pad="50"/>
<connect gate="A" pin="IO_43" pad="51"/>
<connect gate="A" pin="IO_44" pad="52"/>
<connect gate="A" pin="IO_45" pad="53"/>
<connect gate="A" pin="IO_46" pad="54"/>
<connect gate="A" pin="IO_47" pad="55"/>
<connect gate="A" pin="IO_48" pad="56"/>
<connect gate="A" pin="IO_49" pad="57"/>
<connect gate="A" pin="IO_5" pad="13"/>
<connect gate="A" pin="IO_50" pad="58"/>
<connect gate="A" pin="IO_51" pad="59"/>
<connect gate="A" pin="IO_52" pad="60"/>
<connect gate="A" pin="IO_6" pad="14"/>
<connect gate="A" pin="IO_7" pad="15"/>
<connect gate="A" pin="IO_8" pad="16"/>
<connect gate="A" pin="IO_9" pad="17"/>
<connect gate="A" pin="MSEL" pad="46"/>
<connect gate="A" pin="NCE" pad="6"/>
<connect gate="A" pin="VCCINT" pad="8"/>
<connect gate="A" pin="VCCINT_2" pad="26"/>
<connect gate="A" pin="VCCINT_3" pad="44"/>
<connect gate="A" pin="VCCIO" pad="45"/>
<connect gate="A" pin="VCCIO_2" pad="63"/>
<connect gate="A" pin="VCCIO_3" pad="9"/>
<connect gate="A" pin="VCCIO_4" pad="27"/>
<connect gate="B" pin="GND" pad="129"/>
<connect gate="B" pin="GND_2" pad="110"/>
<connect gate="B" pin="GND_3" pad="95"/>
<connect gate="B" pin="GND_4" pad="78"/>
<connect gate="B" pin="INPUT" pad="132"/>
<connect gate="B" pin="INPUT_2" pad="128"/>
<connect gate="B" pin="IO" pad="139"/>
<connect gate="B" pin="IO/INIT_DONE" pad="135"/>
<connect gate="B" pin="IO/NCEO" pad="102"/>
<connect gate="B" pin="IO/RDYNBUSY" pad="140"/>
<connect gate="B" pin="IO/TDO" pad="107"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="72"/>
<connect gate="B" pin="IO_12" pad="89"/>
<connect gate="B" pin="IO_13" pad="73"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="74"/>
<connect gate="B" pin="IO_16" pad="91"/>
<connect gate="B" pin="IO_17" pad="75"/>
<connect gate="B" pin="IO_18" pad="92"/>
<connect gate="B" pin="IO_19" pad="76"/>
<connect gate="B" pin="IO_2" pad="81"/>
<connect gate="B" pin="IO_20" pad="93"/>
<connect gate="B" pin="IO_21" pad="94"/>
<connect gate="B" pin="IO_22" pad="97"/>
<connect gate="B" pin="IO_23" pad="98"/>
<connect gate="B" pin="IO_24" pad="99"/>
<connect gate="B" pin="IO_25" pad="100"/>
<connect gate="B" pin="IO_26" pad="101"/>
<connect gate="B" pin="IO_27" pad="103"/>
<connect gate="B" pin="IO_28" pad="104"/>
<connect gate="B" pin="IO_29" pad="105"/>
<connect gate="B" pin="IO_3" pad="82"/>
<connect gate="B" pin="IO_30" pad="106"/>
<connect gate="B" pin="IO_31" pad="108"/>
<connect gate="B" pin="IO_32" pad="109"/>
<connect gate="B" pin="IO_33" pad="113"/>
<connect gate="B" pin="IO_34" pad="114"/>
<connect gate="B" pin="IO_35" pad="115"/>
<connect gate="B" pin="IO_36" pad="116"/>
<connect gate="B" pin="IO_37" pad="117"/>
<connect gate="B" pin="IO_38" pad="118"/>
<connect gate="B" pin="IO_39" pad="119"/>
<connect gate="B" pin="IO_4" pad="83"/>
<connect gate="B" pin="IO_40" pad="120"/>
<connect gate="B" pin="IO_41" pad="121"/>
<connect gate="B" pin="IO_42" pad="122"/>
<connect gate="B" pin="IO_43" pad="133"/>
<connect gate="B" pin="IO_44" pad="123"/>
<connect gate="B" pin="IO_45" pad="134"/>
<connect gate="B" pin="IO_46" pad="124"/>
<connect gate="B" pin="IO_47" pad="125"/>
<connect gate="B" pin="IO_48" pad="136"/>
<connect gate="B" pin="IO_49" pad="126"/>
<connect gate="B" pin="IO_5" pad="84"/>
<connect gate="B" pin="IO_50" pad="137"/>
<connect gate="B" pin="IO_51" pad="127"/>
<connect gate="B" pin="IO_52" pad="138"/>
<connect gate="B" pin="IO_6" pad="85"/>
<connect gate="B" pin="IO_7" pad="86"/>
<connect gate="B" pin="IO_8" pad="87"/>
<connect gate="B" pin="IO_9" pad="71"/>
<connect gate="B" pin="NCONFIG" pad="77"/>
<connect gate="B" pin="NSTATUS" pad="80"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="111"/>
<connect gate="B" pin="VCCIO" pad="131"/>
<connect gate="B" pin="VCCIO_2" pad="79"/>
<connect gate="B" pin="VCCIO_3" pad="96"/>
<connect gate="B" pin="VCCIO_4" pad="112"/>
<connect gate="C" pin="CLKUSR" pad="144"/>
<connect gate="C" pin="CONF_DONE" pad="150"/>
<connect gate="C" pin="DATA" pad="181"/>
<connect gate="C" pin="DCLK" pad="184"/>
<connect gate="C" pin="GND" pad="199"/>
<connect gate="C" pin="GND_2" pad="147"/>
<connect gate="C" pin="GND_3" pad="165"/>
<connect gate="C" pin="GND_4" pad="182"/>
<connect gate="C" pin="IO" pad="208"/>
<connect gate="C" pin="IO/CS" pad="162"/>
<connect gate="C" pin="IO/DEV_CLRN" pad="187"/>
<connect gate="C" pin="IO/DEV_OE" pad="178"/>
<connect gate="C" pin="IO/NCS" pad="159"/>
<connect gate="C" pin="IO/NRS" pad="174"/>
<connect gate="C" pin="IO/NWS" pad="169"/>
<connect gate="C" pin="IO_10" pad="154"/>
<connect gate="C" pin="IO_11" pad="155"/>
<connect gate="C" pin="IO_12" pad="156"/>
<connect gate="C" pin="IO_13" pad="157"/>
<connect gate="C" pin="IO_14" pad="158"/>
<connect gate="C" pin="IO_15" pad="163"/>
<connect gate="C" pin="IO_16" pad="160"/>
<connect gate="C" pin="IO_17" pad="164"/>
<connect gate="C" pin="IO_18" pad="161"/>
<connect gate="C" pin="IO_19" pad="168"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="167"/>
<connect gate="C" pin="IO_21" pad="170"/>
<connect gate="C" pin="IO_22" pad="171"/>
<connect gate="C" pin="IO_23" pad="172"/>
<connect gate="C" pin="IO_24" pad="173"/>
<connect gate="C" pin="IO_25" pad="175"/>
<connect gate="C" pin="IO_26" pad="176"/>
<connect gate="C" pin="IO_27" pad="177"/>
<connect gate="C" pin="IO_28" pad="188"/>
<connect gate="C" pin="IO_29" pad="179"/>
<connect gate="C" pin="IO_3" pad="142"/>
<connect gate="C" pin="IO_30" pad="189"/>
<connect gate="C" pin="IO_31" pad="180"/>
<connect gate="C" pin="IO_32" pad="190"/>
<connect gate="C" pin="IO_33" pad="185"/>
<connect gate="C" pin="IO_34" pad="191"/>
<connect gate="C" pin="IO_35" pad="186"/>
<connect gate="C" pin="IO_36" pad="192"/>
<connect gate="C" pin="IO_37" pad="193"/>
<connect gate="C" pin="IO_38" pad="194"/>
<connect gate="C" pin="IO_39" pad="195"/>
<connect gate="C" pin="IO_4" pad="143"/>
<connect gate="C" pin="IO_40" pad="196"/>
<connect gate="C" pin="IO_41" pad="197"/>
<connect gate="C" pin="IO_42" pad="198"/>
<connect gate="C" pin="IO_43" pad="201"/>
<connect gate="C" pin="IO_44" pad="202"/>
<connect gate="C" pin="IO_45" pad="203"/>
<connect gate="C" pin="IO_46" pad="204"/>
<connect gate="C" pin="IO_47" pad="205"/>
<connect gate="C" pin="IO_48" pad="206"/>
<connect gate="C" pin="IO_49" pad="207"/>
<connect gate="C" pin="IO_5" pad="145"/>
<connect gate="C" pin="IO_6" pad="151"/>
<connect gate="C" pin="IO_7" pad="146"/>
<connect gate="C" pin="IO_8" pad="152"/>
<connect gate="C" pin="IO_9" pad="153"/>
<connect gate="C" pin="VCCINT" pad="148"/>
<connect gate="C" pin="VCCIO" pad="200"/>
<connect gate="C" pin="VCCIO_2" pad="166"/>
<connect gate="C" pin="VCCIO_3" pad="149"/>
<connect gate="C" pin="VCCIO_4" pad="183"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF6024AQC208-3N"/>
<attribute name="OC_FARNELL" value="1549399"/>
<attribute name="OC_NEWARK" value="51R9204"/>
<attribute name="PACKAGE" value="PQFP-208"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF8282ATC100-4N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPF8282ATC100-4N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CLKUSR" pad="47"/>
<connect gate="A" pin="CONF_DONE" pad="1"/>
<connect gate="A" pin="DATA0" pad="5"/>
<connect gate="A" pin="DATA1" pad="4"/>
<connect gate="A" pin="DATA2" pad="99"/>
<connect gate="A" pin="DATA3" pad="97"/>
<connect gate="A" pin="DATA4" pad="95"/>
<connect gate="A" pin="DATA5" pad="92"/>
<connect gate="A" pin="DATA6" pad="91"/>
<connect gate="A" pin="DATA7" pad="90"/>
<connect gate="A" pin="DCLK" pad="100"/>
<connect gate="A" pin="GND" pad="30"/>
<connect gate="A" pin="GND_2" pad="13"/>
<connect gate="A" pin="GND_3" pad="80"/>
<connect gate="A" pin="GND_4" pad="2"/>
<connect gate="A" pin="GND_5" pad="52"/>
<connect gate="A" pin="GND_6" pad="94"/>
<connect gate="A" pin="GND_7" pad="63"/>
<connect gate="A" pin="GND_8" pad="44"/>
<connect gate="A" pin="INPUT" pad="73"/>
<connect gate="A" pin="INPUT_2" pad="3"/>
<connect gate="A" pin="INPUT_3" pad="53"/>
<connect gate="A" pin="INPUT_4" pad="23"/>
<connect gate="A" pin="IO" pad="98"/>
<connect gate="A" pin="IO/*CS" pad="21"/>
<connect gate="A" pin="IO/ADD0" pad="78"/>
<connect gate="A" pin="IO/ADD1" pad="76"/>
<connect gate="A" pin="IO/ADD10" pad="61"/>
<connect gate="A" pin="IO/ADD11" pad="60"/>
<connect gate="A" pin="IO/ADD12" pad="59"/>
<connect gate="A" pin="IO/ADD13" pad="58"/>
<connect gate="A" pin="IO/ADD14" pad="57"/>
<connect gate="A" pin="IO/ADD15" pad="55"/>
<connect gate="A" pin="IO/ADD16" pad="28"/>
<connect gate="A" pin="IO/ADD17" pad="49"/>
<connect gate="A" pin="IO/ADD2" pad="71"/>
<connect gate="A" pin="IO/ADD3" pad="69"/>
<connect gate="A" pin="IO/ADD4" pad="68"/>
<connect gate="A" pin="IO/ADD5" pad="67"/>
<connect gate="A" pin="IO/ADD6" pad="66"/>
<connect gate="A" pin="IO/ADD7" pad="65"/>
<connect gate="A" pin="IO/ADD8" pad="64"/>
<connect gate="A" pin="IO/ADD9" pad="62"/>
<connect gate="A" pin="IO/CS" pad="19"/>
<connect gate="A" pin="IO/NWS" pad="22"/>
<connect gate="A" pin="IO/SDOUT" pad="79"/>
<connect gate="A" pin="IO/TCK" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="54"/>
<connect gate="A" pin="IO/TDO" pad="18"/>
<connect gate="A" pin="IO/TMS" pad="11"/>
<connect gate="A" pin="IO_10" pad="31"/>
<connect gate="A" pin="IO_11" pad="33"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="34"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="35"/>
<connect gate="A" pin="IO_16" pad="16"/>
<connect gate="A" pin="IO_17" pad="36"/>
<connect gate="A" pin="IO_18" pad="17"/>
<connect gate="A" pin="IO_19" pad="38"/>
<connect gate="A" pin="IO_2" pad="7"/>
<connect gate="A" pin="IO_20" pad="48"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="39"/>
<connect gate="A" pin="IO_23" pad="40"/>
<connect gate="A" pin="IO_24" pad="41"/>
<connect gate="A" pin="IO_25" pad="46"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_27" pad="81"/>
<connect gate="A" pin="IO_28" pad="82"/>
<connect gate="A" pin="IO_29" pad="83"/>
<connect gate="A" pin="IO_3" pad="26"/>
<connect gate="A" pin="IO_30" pad="84"/>
<connect gate="A" pin="IO_31" pad="85"/>
<connect gate="A" pin="IO_32" pad="86"/>
<connect gate="A" pin="IO_33" pad="88"/>
<connect gate="A" pin="IO_34" pad="89"/>
<connect gate="A" pin="IO_35" pad="93"/>
<connect gate="A" pin="IO_36" pad="96"/>
<connect gate="A" pin="IO_4" pad="27"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="32"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="MSEL0" pad="74"/>
<connect gate="A" pin="MSEL1" pad="51"/>
<connect gate="A" pin="NCONFIG" pad="25"/>
<connect gate="A" pin="NRS" pad="42"/>
<connect gate="A" pin="NSP" pad="75"/>
<connect gate="A" pin="NSTATUS" pad="24"/>
<connect gate="A" pin="RDCLK" pad="45"/>
<connect gate="A" pin="RDYNBUSY" pad="77"/>
<connect gate="A" pin="TRST" pad="50"/>
<connect gate="A" pin="VCCINT" pad="70"/>
<connect gate="A" pin="VCCINT_2" pad="6"/>
<connect gate="A" pin="VCCINT_3" pad="20"/>
<connect gate="A" pin="VCCINT_4" pad="56"/>
<connect gate="A" pin="VCCINT_5" pad="87"/>
<connect gate="A" pin="VCCINT_6" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPF8282ATC100-4N"/>
<attribute name="OC_FARNELL" value="1549401"/>
<attribute name="OC_NEWARK" value="51R9236"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270F256C3N">
<description>MAX II Devices</description>
<gates>
<gate name="A" symbol="EPM1270F256C3N_A"/>
<gate name="B" symbol="EPM1270F256C3N_B"/>
<gate name="C" symbol="EPM1270F256C3N_C"/>
</gates>
<devices>
<device name="" package="BGA256C16X16X100P_1700X1700X22">
<connects>
<connect gate="A" pin="GNDINT" pad="H7"/>
<connect gate="A" pin="GNDINT_2" pad="J8"/>
<connect gate="A" pin="GNDINT_3" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="B2"/>
<connect gate="A" pin="GNDIO_3" pad="G7"/>
<connect gate="A" pin="GNDIO_4" pad="A1"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="G1"/>
<connect gate="A" pin="IO_51" pad="G2"/>
<connect gate="A" pin="IO_52" pad="G3"/>
<connect gate="A" pin="IO_53" pad="G4"/>
<connect gate="A" pin="IO_54" pad="G5"/>
<connect gate="A" pin="IO_55" pad="G6"/>
<connect gate="A" pin="IO_56" pad="H1"/>
<connect gate="A" pin="IO_57" pad="H2"/>
<connect gate="A" pin="IO_58" pad="H3"/>
<connect gate="A" pin="IO_59" pad="H4"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="J1"/>
<connect gate="A" pin="IO_61" pad="J2"/>
<connect gate="A" pin="IO_62" pad="J3"/>
<connect gate="A" pin="IO_63" pad="J4"/>
<connect gate="A" pin="IO_64" pad="K1"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_66" pad="K3"/>
<connect gate="A" pin="IO_67" pad="K4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="H8"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="C1"/>
<connect gate="A" pin="VCCIO1_2" pad="H6"/>
<connect gate="A" pin="VCCIO1_3" pad="J6"/>
<connect gate="A" pin="VCCIO2" pad="A3"/>
<connect gate="A" pin="VCCIO2_2" pad="F8"/>
<connect gate="A" pin="VCCIO2_3" pad="F9"/>
<connect gate="B" pin="GNDIO" pad="K9"/>
<connect gate="B" pin="GNDIO_2" pad="B15"/>
<connect gate="B" pin="GNDIO_3" pad="A16"/>
<connect gate="B" pin="GNDIO_4" pad="R2"/>
<connect gate="B" pin="GNDIO_5" pad="T1"/>
<connect gate="B" pin="GNDIO_6" pad="K7"/>
<connect gate="B" pin="GNDIO_7" pad="K8"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="M2"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="M4"/>
<connect gate="B" pin="IO_13" pad="M6"/>
<connect gate="B" pin="IO_14" pad="M7"/>
<connect gate="B" pin="IO_15" pad="N1"/>
<connect gate="B" pin="IO_16" pad="N2"/>
<connect gate="B" pin="IO_17" pad="N3"/>
<connect gate="B" pin="IO_18" pad="N5"/>
<connect gate="B" pin="IO_19" pad="N6"/>
<connect gate="B" pin="IO_2" pad="K6"/>
<connect gate="B" pin="IO_20" pad="N7"/>
<connect gate="B" pin="IO_21" pad="N8"/>
<connect gate="B" pin="IO_22" pad="N9"/>
<connect gate="B" pin="IO_23" pad="P2"/>
<connect gate="B" pin="IO_24" pad="P4"/>
<connect gate="B" pin="IO_25" pad="P5"/>
<connect gate="B" pin="IO_26" pad="P6"/>
<connect gate="B" pin="IO_27" pad="P7"/>
<connect gate="B" pin="IO_28" pad="P8"/>
<connect gate="B" pin="IO_29" pad="P9"/>
<connect gate="B" pin="IO_3" pad="L1"/>
<connect gate="B" pin="IO_30" pad="R1"/>
<connect gate="B" pin="IO_31" pad="R3"/>
<connect gate="B" pin="IO_32" pad="R4"/>
<connect gate="B" pin="IO_33" pad="R5"/>
<connect gate="B" pin="IO_34" pad="R6"/>
<connect gate="B" pin="IO_35" pad="R7"/>
<connect gate="B" pin="IO_36" pad="R8"/>
<connect gate="B" pin="IO_37" pad="R9"/>
<connect gate="B" pin="IO_38" pad="T2"/>
<connect gate="B" pin="IO_39" pad="T4"/>
<connect gate="B" pin="IO_4" pad="L2"/>
<connect gate="B" pin="IO_40" pad="T5"/>
<connect gate="B" pin="IO_41" pad="T6"/>
<connect gate="B" pin="IO_42" pad="T7"/>
<connect gate="B" pin="IO_43" pad="T8"/>
<connect gate="B" pin="IO_44" pad="T9"/>
<connect gate="B" pin="IO_45" pad="A10"/>
<connect gate="B" pin="IO_46" pad="A11"/>
<connect gate="B" pin="IO_47" pad="A12"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="L3"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B16"/>
<connect gate="B" pin="IO_56" pad="C10"/>
<connect gate="B" pin="IO_57" pad="C11"/>
<connect gate="B" pin="IO_58" pad="C12"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="L4"/>
<connect gate="B" pin="IO_60" pad="C14"/>
<connect gate="B" pin="IO_61" pad="C15"/>
<connect gate="B" pin="IO_62" pad="D10"/>
<connect gate="B" pin="IO_63" pad="D11"/>
<connect gate="B" pin="IO_64" pad="D12"/>
<connect gate="B" pin="IO_65" pad="D13"/>
<connect gate="B" pin="IO_66" pad="D14"/>
<connect gate="B" pin="IO_67" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L5"/>
<connect gate="B" pin="IO_8" pad="L7"/>
<connect gate="B" pin="IO_9" pad="M1"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="L9"/>
<connect gate="B" pin="VCCIO4_2" pad="T3"/>
<connect gate="B" pin="VCCIO4_3" pad="L8"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="T16"/>
<connect gate="C" pin="GNDIO_3" pad="R15"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="F11"/>
<connect gate="C" pin="IO_11" pad="F12"/>
<connect gate="C" pin="IO_12" pad="F13"/>
<connect gate="C" pin="IO_13" pad="F14"/>
<connect gate="C" pin="IO_14" pad="F15"/>
<connect gate="C" pin="IO_15" pad="F16"/>
<connect gate="C" pin="IO_16" pad="G11"/>
<connect gate="C" pin="IO_17" pad="G12"/>
<connect gate="C" pin="IO_18" pad="G13"/>
<connect gate="C" pin="IO_19" pad="G14"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="G15"/>
<connect gate="C" pin="IO_21" pad="G16"/>
<connect gate="C" pin="IO_22" pad="H13"/>
<connect gate="C" pin="IO_23" pad="H14"/>
<connect gate="C" pin="IO_24" pad="H15"/>
<connect gate="C" pin="IO_25" pad="H16"/>
<connect gate="C" pin="IO_26" pad="J13"/>
<connect gate="C" pin="IO_27" pad="J14"/>
<connect gate="C" pin="IO_28" pad="J15"/>
<connect gate="C" pin="IO_29" pad="J16"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="K11"/>
<connect gate="C" pin="IO_31" pad="K12"/>
<connect gate="C" pin="IO_32" pad="K13"/>
<connect gate="C" pin="IO_33" pad="K14"/>
<connect gate="C" pin="IO_34" pad="K15"/>
<connect gate="C" pin="IO_35" pad="K16"/>
<connect gate="C" pin="IO_36" pad="L10"/>
<connect gate="C" pin="IO_37" pad="L11"/>
<connect gate="C" pin="IO_38" pad="L12"/>
<connect gate="C" pin="IO_39" pad="L13"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="L14"/>
<connect gate="C" pin="IO_41" pad="L15"/>
<connect gate="C" pin="IO_42" pad="L16"/>
<connect gate="C" pin="IO_43" pad="M10"/>
<connect gate="C" pin="IO_44" pad="M11"/>
<connect gate="C" pin="IO_45" pad="M12"/>
<connect gate="C" pin="IO_46" pad="M13"/>
<connect gate="C" pin="IO_47" pad="M14"/>
<connect gate="C" pin="IO_48" pad="M15"/>
<connect gate="C" pin="IO_49" pad="M16"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="N10"/>
<connect gate="C" pin="IO_51" pad="N11"/>
<connect gate="C" pin="IO_52" pad="N12"/>
<connect gate="C" pin="IO_53" pad="N13"/>
<connect gate="C" pin="IO_54" pad="N14"/>
<connect gate="C" pin="IO_55" pad="N15"/>
<connect gate="C" pin="IO_56" pad="N16"/>
<connect gate="C" pin="IO_57" pad="P10"/>
<connect gate="C" pin="IO_58" pad="P11"/>
<connect gate="C" pin="IO_59" pad="P12"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_60" pad="P13"/>
<connect gate="C" pin="IO_61" pad="P14"/>
<connect gate="C" pin="IO_62" pad="P15"/>
<connect gate="C" pin="IO_63" pad="R10"/>
<connect gate="C" pin="IO_64" pad="R11"/>
<connect gate="C" pin="IO_65" pad="R12"/>
<connect gate="C" pin="IO_66" pad="R13"/>
<connect gate="C" pin="IO_67" pad="R14"/>
<connect gate="C" pin="IO_68" pad="R16"/>
<connect gate="C" pin="IO_69" pad="T10"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_70" pad="T11"/>
<connect gate="C" pin="IO_71" pad="T12"/>
<connect gate="C" pin="IO_72" pad="T13"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="F10"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="H11"/>
<connect gate="C" pin="VCCIO3_3" pad="J11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270F256C3N"/>
<attribute name="OC_FARNELL" value="1794142"/>
<attribute name="OC_NEWARK" value="51R9275"/>
<attribute name="PACKAGE" value="FBGA-256"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270F256C4N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270F256C4N_A"/>
<gate name="B" symbol="EPM1270F256C4N_B"/>
<gate name="C" symbol="EPM1270F256C4N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="H7"/>
<connect gate="A" pin="GNDINT_2" pad="J8"/>
<connect gate="A" pin="GNDINT_3" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="G7"/>
<connect gate="A" pin="GNDIO_3" pad="A1"/>
<connect gate="A" pin="GNDIO_4" pad="B2"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A4"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A5"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A6"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="A7"/>
<connect gate="A" pin="IO_50" pad="G1"/>
<connect gate="A" pin="IO_51" pad="G2"/>
<connect gate="A" pin="IO_52" pad="G3"/>
<connect gate="A" pin="IO_53" pad="G4"/>
<connect gate="A" pin="IO_54" pad="G5"/>
<connect gate="A" pin="IO_55" pad="G6"/>
<connect gate="A" pin="IO_56" pad="H1"/>
<connect gate="A" pin="IO_57" pad="H2"/>
<connect gate="A" pin="IO_58" pad="H3"/>
<connect gate="A" pin="IO_59" pad="H4"/>
<connect gate="A" pin="IO_6" pad="A2"/>
<connect gate="A" pin="IO_60" pad="J1"/>
<connect gate="A" pin="IO_61" pad="J2"/>
<connect gate="A" pin="IO_62" pad="J3"/>
<connect gate="A" pin="IO_63" pad="J4"/>
<connect gate="A" pin="IO_64" pad="K1"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_66" pad="K3"/>
<connect gate="A" pin="IO_67" pad="K4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="J7"/>
<connect gate="A" pin="VCCINT_3" pad="H8"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO1_3" pad="J6"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="F8"/>
<connect gate="A" pin="VCCIO2_3" pad="A3"/>
<connect gate="B" pin="GNDIO" pad="K9"/>
<connect gate="B" pin="GNDIO_2" pad="R2"/>
<connect gate="B" pin="GNDIO_3" pad="T1"/>
<connect gate="B" pin="GNDIO_4" pad="A16"/>
<connect gate="B" pin="GNDIO_5" pad="B15"/>
<connect gate="B" pin="GNDIO_6" pad="K7"/>
<connect gate="B" pin="GNDIO_7" pad="K8"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="N9"/>
<connect gate="B" pin="IO_11" pad="L3"/>
<connect gate="B" pin="IO_12" pad="K6"/>
<connect gate="B" pin="IO_13" pad="P2"/>
<connect gate="B" pin="IO_14" pad="L4"/>
<connect gate="B" pin="IO_15" pad="M1"/>
<connect gate="B" pin="IO_16" pad="P4"/>
<connect gate="B" pin="IO_17" pad="M2"/>
<connect gate="B" pin="IO_18" pad="P5"/>
<connect gate="B" pin="IO_19" pad="M3"/>
<connect gate="B" pin="IO_2" pad="N5"/>
<connect gate="B" pin="IO_20" pad="P6"/>
<connect gate="B" pin="IO_21" pad="M4"/>
<connect gate="B" pin="IO_22" pad="P7"/>
<connect gate="B" pin="IO_23" pad="M6"/>
<connect gate="B" pin="IO_24" pad="P8"/>
<connect gate="B" pin="IO_25" pad="M7"/>
<connect gate="B" pin="IO_26" pad="P9"/>
<connect gate="B" pin="IO_27" pad="N1"/>
<connect gate="B" pin="IO_28" pad="R1"/>
<connect gate="B" pin="IO_29" pad="N2"/>
<connect gate="B" pin="IO_3" pad="L5"/>
<connect gate="B" pin="IO_30" pad="N3"/>
<connect gate="B" pin="IO_31" pad="R3"/>
<connect gate="B" pin="IO_32" pad="R4"/>
<connect gate="B" pin="IO_33" pad="R5"/>
<connect gate="B" pin="IO_34" pad="R6"/>
<connect gate="B" pin="IO_35" pad="R7"/>
<connect gate="B" pin="IO_36" pad="R8"/>
<connect gate="B" pin="IO_37" pad="R9"/>
<connect gate="B" pin="IO_38" pad="T2"/>
<connect gate="B" pin="IO_39" pad="T4"/>
<connect gate="B" pin="IO_4" pad="N6"/>
<connect gate="B" pin="IO_40" pad="T5"/>
<connect gate="B" pin="IO_41" pad="T6"/>
<connect gate="B" pin="IO_42" pad="T7"/>
<connect gate="B" pin="IO_43" pad="T8"/>
<connect gate="B" pin="IO_44" pad="T9"/>
<connect gate="B" pin="IO_45" pad="A10"/>
<connect gate="B" pin="IO_46" pad="A11"/>
<connect gate="B" pin="IO_47" pad="A12"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="L1"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B16"/>
<connect gate="B" pin="IO_56" pad="C10"/>
<connect gate="B" pin="IO_57" pad="C11"/>
<connect gate="B" pin="IO_58" pad="C12"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="N7"/>
<connect gate="B" pin="IO_60" pad="C14"/>
<connect gate="B" pin="IO_61" pad="C15"/>
<connect gate="B" pin="IO_62" pad="D10"/>
<connect gate="B" pin="IO_63" pad="D11"/>
<connect gate="B" pin="IO_64" pad="D12"/>
<connect gate="B" pin="IO_65" pad="D13"/>
<connect gate="B" pin="IO_66" pad="D14"/>
<connect gate="B" pin="IO_67" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L2"/>
<connect gate="B" pin="IO_8" pad="N8"/>
<connect gate="B" pin="IO_9" pad="L7"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="L9"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="T3"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="G10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="K10"/>
<connect gate="C" pin="GNDIO_4" pad="T16"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="F10"/>
<connect gate="C" pin="IO_11" pad="G12"/>
<connect gate="C" pin="IO_12" pad="F11"/>
<connect gate="C" pin="IO_13" pad="G13"/>
<connect gate="C" pin="IO_14" pad="F12"/>
<connect gate="C" pin="IO_15" pad="G14"/>
<connect gate="C" pin="IO_16" pad="F13"/>
<connect gate="C" pin="IO_17" pad="G15"/>
<connect gate="C" pin="IO_18" pad="F14"/>
<connect gate="C" pin="IO_19" pad="G16"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="F15"/>
<connect gate="C" pin="IO_21" pad="F16"/>
<connect gate="C" pin="IO_22" pad="J13"/>
<connect gate="C" pin="IO_23" pad="J14"/>
<connect gate="C" pin="IO_24" pad="H13"/>
<connect gate="C" pin="IO_25" pad="J15"/>
<connect gate="C" pin="IO_26" pad="H14"/>
<connect gate="C" pin="IO_27" pad="J16"/>
<connect gate="C" pin="IO_28" pad="H15"/>
<connect gate="C" pin="IO_29" pad="H16"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="K11"/>
<connect gate="C" pin="IO_31" pad="K12"/>
<connect gate="C" pin="IO_32" pad="K13"/>
<connect gate="C" pin="IO_33" pad="K14"/>
<connect gate="C" pin="IO_34" pad="K15"/>
<connect gate="C" pin="IO_35" pad="K16"/>
<connect gate="C" pin="IO_36" pad="L10"/>
<connect gate="C" pin="IO_37" pad="L11"/>
<connect gate="C" pin="IO_38" pad="L12"/>
<connect gate="C" pin="IO_39" pad="L13"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="L14"/>
<connect gate="C" pin="IO_41" pad="L15"/>
<connect gate="C" pin="IO_42" pad="L16"/>
<connect gate="C" pin="IO_43" pad="M10"/>
<connect gate="C" pin="IO_44" pad="M11"/>
<connect gate="C" pin="IO_45" pad="M12"/>
<connect gate="C" pin="IO_46" pad="M13"/>
<connect gate="C" pin="IO_47" pad="M14"/>
<connect gate="C" pin="IO_48" pad="M15"/>
<connect gate="C" pin="IO_49" pad="M16"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="N10"/>
<connect gate="C" pin="IO_51" pad="N11"/>
<connect gate="C" pin="IO_52" pad="N12"/>
<connect gate="C" pin="IO_53" pad="N13"/>
<connect gate="C" pin="IO_54" pad="N14"/>
<connect gate="C" pin="IO_55" pad="N15"/>
<connect gate="C" pin="IO_56" pad="N16"/>
<connect gate="C" pin="IO_57" pad="P10"/>
<connect gate="C" pin="IO_58" pad="P11"/>
<connect gate="C" pin="IO_59" pad="P12"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_60" pad="P13"/>
<connect gate="C" pin="IO_61" pad="P14"/>
<connect gate="C" pin="IO_62" pad="P15"/>
<connect gate="C" pin="IO_63" pad="R10"/>
<connect gate="C" pin="IO_64" pad="R11"/>
<connect gate="C" pin="IO_65" pad="R12"/>
<connect gate="C" pin="IO_66" pad="R13"/>
<connect gate="C" pin="IO_67" pad="R14"/>
<connect gate="C" pin="IO_68" pad="R16"/>
<connect gate="C" pin="IO_69" pad="T10"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_70" pad="T11"/>
<connect gate="C" pin="IO_71" pad="T12"/>
<connect gate="C" pin="IO_72" pad="T13"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="G11"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="J11"/>
<connect gate="C" pin="VCCIO3_3" pad="H11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270F256C4N"/>
<attribute name="OC_FARNELL" value="1549477"/>
<attribute name="OC_NEWARK" value="51R0483"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270F256C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270F256C5N_A"/>
<gate name="B" symbol="EPM1270F256C5N_B"/>
<gate name="C" symbol="EPM1270F256C5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="H7"/>
<connect gate="A" pin="GNDINT_3" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J4"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B8"/>
<connect gate="A" pin="IO_11" pad="A6"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="A7"/>
<connect gate="A" pin="IO_14" pad="A8"/>
<connect gate="A" pin="IO_15" pad="C2"/>
<connect gate="A" pin="IO_16" pad="A9"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A2"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="B5"/>
<connect gate="A" pin="IO_50" pad="G1"/>
<connect gate="A" pin="IO_51" pad="G2"/>
<connect gate="A" pin="IO_52" pad="G3"/>
<connect gate="A" pin="IO_53" pad="K1"/>
<connect gate="A" pin="IO_54" pad="G4"/>
<connect gate="A" pin="IO_55" pad="K2"/>
<connect gate="A" pin="IO_56" pad="G5"/>
<connect gate="A" pin="IO_57" pad="K3"/>
<connect gate="A" pin="IO_58" pad="G6"/>
<connect gate="A" pin="IO_59" pad="K4"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_60" pad="H1"/>
<connect gate="A" pin="IO_61" pad="K5"/>
<connect gate="A" pin="IO_62" pad="H2"/>
<connect gate="A" pin="IO_63" pad="H3"/>
<connect gate="A" pin="IO_64" pad="H4"/>
<connect gate="A" pin="IO_65" pad="J1"/>
<connect gate="A" pin="IO_66" pad="J2"/>
<connect gate="A" pin="IO_67" pad="J3"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J7"/>
<connect gate="A" pin="VCCINT_3" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO1_3" pad="J6"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="M1"/>
<connect gate="B" pin="IO_11" pad="P4"/>
<connect gate="B" pin="IO_12" pad="N7"/>
<connect gate="B" pin="IO_13" pad="P5"/>
<connect gate="B" pin="IO_14" pad="L5"/>
<connect gate="B" pin="IO_15" pad="P6"/>
<connect gate="B" pin="IO_16" pad="N8"/>
<connect gate="B" pin="IO_17" pad="P7"/>
<connect gate="B" pin="IO_18" pad="M2"/>
<connect gate="B" pin="IO_19" pad="P8"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="N9"/>
<connect gate="B" pin="IO_21" pad="P9"/>
<connect gate="B" pin="IO_22" pad="M3"/>
<connect gate="B" pin="IO_23" pad="R1"/>
<connect gate="B" pin="IO_24" pad="M4"/>
<connect gate="B" pin="IO_25" pad="P2"/>
<connect gate="B" pin="IO_26" pad="R3"/>
<connect gate="B" pin="IO_27" pad="M6"/>
<connect gate="B" pin="IO_28" pad="N1"/>
<connect gate="B" pin="IO_29" pad="M7"/>
<connect gate="B" pin="IO_3" pad="L7"/>
<connect gate="B" pin="IO_30" pad="N3"/>
<connect gate="B" pin="IO_31" pad="N2"/>
<connect gate="B" pin="IO_32" pad="R4"/>
<connect gate="B" pin="IO_33" pad="R5"/>
<connect gate="B" pin="IO_34" pad="R6"/>
<connect gate="B" pin="IO_35" pad="R7"/>
<connect gate="B" pin="IO_36" pad="R8"/>
<connect gate="B" pin="IO_37" pad="R9"/>
<connect gate="B" pin="IO_38" pad="T2"/>
<connect gate="B" pin="IO_39" pad="T4"/>
<connect gate="B" pin="IO_4" pad="K6"/>
<connect gate="B" pin="IO_40" pad="T5"/>
<connect gate="B" pin="IO_41" pad="T6"/>
<connect gate="B" pin="IO_42" pad="T7"/>
<connect gate="B" pin="IO_43" pad="T8"/>
<connect gate="B" pin="IO_44" pad="T9"/>
<connect gate="B" pin="IO_45" pad="A10"/>
<connect gate="B" pin="IO_46" pad="A11"/>
<connect gate="B" pin="IO_47" pad="A12"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="L2"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B16"/>
<connect gate="B" pin="IO_56" pad="C10"/>
<connect gate="B" pin="IO_57" pad="C11"/>
<connect gate="B" pin="IO_58" pad="C12"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="L3"/>
<connect gate="B" pin="IO_60" pad="C14"/>
<connect gate="B" pin="IO_61" pad="C15"/>
<connect gate="B" pin="IO_62" pad="D10"/>
<connect gate="B" pin="IO_63" pad="D11"/>
<connect gate="B" pin="IO_64" pad="D12"/>
<connect gate="B" pin="IO_65" pad="D13"/>
<connect gate="B" pin="IO_66" pad="D14"/>
<connect gate="B" pin="IO_67" pad="D15"/>
<connect gate="B" pin="IO_7" pad="N5"/>
<connect gate="B" pin="IO_8" pad="L4"/>
<connect gate="B" pin="IO_9" pad="N6"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="F11"/>
<connect gate="C" pin="IO_11" pad="F12"/>
<connect gate="C" pin="IO_12" pad="F13"/>
<connect gate="C" pin="IO_13" pad="F14"/>
<connect gate="C" pin="IO_14" pad="F15"/>
<connect gate="C" pin="IO_15" pad="F16"/>
<connect gate="C" pin="IO_16" pad="H13"/>
<connect gate="C" pin="IO_17" pad="H14"/>
<connect gate="C" pin="IO_18" pad="G11"/>
<connect gate="C" pin="IO_19" pad="H15"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="G12"/>
<connect gate="C" pin="IO_21" pad="H16"/>
<connect gate="C" pin="IO_22" pad="K11"/>
<connect gate="C" pin="IO_23" pad="G13"/>
<connect gate="C" pin="IO_24" pad="K12"/>
<connect gate="C" pin="IO_25" pad="G14"/>
<connect gate="C" pin="IO_26" pad="K13"/>
<connect gate="C" pin="IO_27" pad="G15"/>
<connect gate="C" pin="IO_28" pad="K14"/>
<connect gate="C" pin="IO_29" pad="G16"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="K15"/>
<connect gate="C" pin="IO_31" pad="J13"/>
<connect gate="C" pin="IO_32" pad="K16"/>
<connect gate="C" pin="IO_33" pad="J14"/>
<connect gate="C" pin="IO_34" pad="L10"/>
<connect gate="C" pin="IO_35" pad="J15"/>
<connect gate="C" pin="IO_36" pad="J16"/>
<connect gate="C" pin="IO_37" pad="L11"/>
<connect gate="C" pin="IO_38" pad="L12"/>
<connect gate="C" pin="IO_39" pad="L13"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="L14"/>
<connect gate="C" pin="IO_41" pad="L15"/>
<connect gate="C" pin="IO_42" pad="L16"/>
<connect gate="C" pin="IO_43" pad="M10"/>
<connect gate="C" pin="IO_44" pad="M11"/>
<connect gate="C" pin="IO_45" pad="M12"/>
<connect gate="C" pin="IO_46" pad="M13"/>
<connect gate="C" pin="IO_47" pad="M14"/>
<connect gate="C" pin="IO_48" pad="M15"/>
<connect gate="C" pin="IO_49" pad="M16"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="N10"/>
<connect gate="C" pin="IO_51" pad="N11"/>
<connect gate="C" pin="IO_52" pad="N12"/>
<connect gate="C" pin="IO_53" pad="N13"/>
<connect gate="C" pin="IO_54" pad="N14"/>
<connect gate="C" pin="IO_55" pad="N15"/>
<connect gate="C" pin="IO_56" pad="N16"/>
<connect gate="C" pin="IO_57" pad="P10"/>
<connect gate="C" pin="IO_58" pad="P11"/>
<connect gate="C" pin="IO_59" pad="P12"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_60" pad="P13"/>
<connect gate="C" pin="IO_61" pad="P14"/>
<connect gate="C" pin="IO_62" pad="P15"/>
<connect gate="C" pin="IO_63" pad="R10"/>
<connect gate="C" pin="IO_64" pad="R11"/>
<connect gate="C" pin="IO_65" pad="R12"/>
<connect gate="C" pin="IO_66" pad="R13"/>
<connect gate="C" pin="IO_67" pad="R14"/>
<connect gate="C" pin="IO_68" pad="R16"/>
<connect gate="C" pin="IO_69" pad="T10"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_70" pad="T11"/>
<connect gate="C" pin="IO_71" pad="T12"/>
<connect gate="C" pin="IO_72" pad="T13"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="F10"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO3" pad="J11"/>
<connect gate="C" pin="VCCIO3_2" pad="P16"/>
<connect gate="C" pin="VCCIO3_3" pad="H11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270F256C5N"/>
<attribute name="OC_FARNELL" value="1635101"/>
<attribute name="OC_NEWARK" value="51R0484"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270F256I5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270F256I5N_A"/>
<gate name="B" symbol="EPM1270F256I5N_B"/>
<gate name="C" symbol="EPM1270F256I5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="H7"/>
<connect gate="A" pin="GNDINT_3" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J4"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B8"/>
<connect gate="A" pin="IO_11" pad="A6"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="A7"/>
<connect gate="A" pin="IO_14" pad="A8"/>
<connect gate="A" pin="IO_15" pad="C2"/>
<connect gate="A" pin="IO_16" pad="A9"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A2"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="B5"/>
<connect gate="A" pin="IO_50" pad="G1"/>
<connect gate="A" pin="IO_51" pad="G2"/>
<connect gate="A" pin="IO_52" pad="G3"/>
<connect gate="A" pin="IO_53" pad="K1"/>
<connect gate="A" pin="IO_54" pad="G4"/>
<connect gate="A" pin="IO_55" pad="K2"/>
<connect gate="A" pin="IO_56" pad="G5"/>
<connect gate="A" pin="IO_57" pad="K3"/>
<connect gate="A" pin="IO_58" pad="G6"/>
<connect gate="A" pin="IO_59" pad="K4"/>
<connect gate="A" pin="IO_6" pad="B6"/>
<connect gate="A" pin="IO_60" pad="H1"/>
<connect gate="A" pin="IO_61" pad="K5"/>
<connect gate="A" pin="IO_62" pad="H2"/>
<connect gate="A" pin="IO_63" pad="H3"/>
<connect gate="A" pin="IO_64" pad="H4"/>
<connect gate="A" pin="IO_65" pad="J1"/>
<connect gate="A" pin="IO_66" pad="J2"/>
<connect gate="A" pin="IO_67" pad="J3"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J7"/>
<connect gate="A" pin="VCCINT_3" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO1_3" pad="J6"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="M1"/>
<connect gate="B" pin="IO_11" pad="P4"/>
<connect gate="B" pin="IO_12" pad="N7"/>
<connect gate="B" pin="IO_13" pad="P5"/>
<connect gate="B" pin="IO_14" pad="L5"/>
<connect gate="B" pin="IO_15" pad="P6"/>
<connect gate="B" pin="IO_16" pad="N8"/>
<connect gate="B" pin="IO_17" pad="P7"/>
<connect gate="B" pin="IO_18" pad="M2"/>
<connect gate="B" pin="IO_19" pad="P8"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="N9"/>
<connect gate="B" pin="IO_21" pad="P9"/>
<connect gate="B" pin="IO_22" pad="M3"/>
<connect gate="B" pin="IO_23" pad="R1"/>
<connect gate="B" pin="IO_24" pad="M4"/>
<connect gate="B" pin="IO_25" pad="P2"/>
<connect gate="B" pin="IO_26" pad="R3"/>
<connect gate="B" pin="IO_27" pad="M6"/>
<connect gate="B" pin="IO_28" pad="N1"/>
<connect gate="B" pin="IO_29" pad="M7"/>
<connect gate="B" pin="IO_3" pad="L7"/>
<connect gate="B" pin="IO_30" pad="N3"/>
<connect gate="B" pin="IO_31" pad="N2"/>
<connect gate="B" pin="IO_32" pad="R4"/>
<connect gate="B" pin="IO_33" pad="R5"/>
<connect gate="B" pin="IO_34" pad="R6"/>
<connect gate="B" pin="IO_35" pad="R7"/>
<connect gate="B" pin="IO_36" pad="R8"/>
<connect gate="B" pin="IO_37" pad="R9"/>
<connect gate="B" pin="IO_38" pad="T2"/>
<connect gate="B" pin="IO_39" pad="T4"/>
<connect gate="B" pin="IO_4" pad="K6"/>
<connect gate="B" pin="IO_40" pad="T5"/>
<connect gate="B" pin="IO_41" pad="T6"/>
<connect gate="B" pin="IO_42" pad="T7"/>
<connect gate="B" pin="IO_43" pad="T8"/>
<connect gate="B" pin="IO_44" pad="T9"/>
<connect gate="B" pin="IO_45" pad="A10"/>
<connect gate="B" pin="IO_46" pad="A11"/>
<connect gate="B" pin="IO_47" pad="A12"/>
<connect gate="B" pin="IO_48" pad="A13"/>
<connect gate="B" pin="IO_49" pad="A15"/>
<connect gate="B" pin="IO_5" pad="L2"/>
<connect gate="B" pin="IO_50" pad="B10"/>
<connect gate="B" pin="IO_51" pad="B11"/>
<connect gate="B" pin="IO_52" pad="B12"/>
<connect gate="B" pin="IO_53" pad="B13"/>
<connect gate="B" pin="IO_54" pad="B14"/>
<connect gate="B" pin="IO_55" pad="B16"/>
<connect gate="B" pin="IO_56" pad="C10"/>
<connect gate="B" pin="IO_57" pad="C11"/>
<connect gate="B" pin="IO_58" pad="C12"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="L3"/>
<connect gate="B" pin="IO_60" pad="C14"/>
<connect gate="B" pin="IO_61" pad="C15"/>
<connect gate="B" pin="IO_62" pad="D10"/>
<connect gate="B" pin="IO_63" pad="D11"/>
<connect gate="B" pin="IO_64" pad="D12"/>
<connect gate="B" pin="IO_65" pad="D13"/>
<connect gate="B" pin="IO_66" pad="D14"/>
<connect gate="B" pin="IO_67" pad="D15"/>
<connect gate="B" pin="IO_7" pad="N5"/>
<connect gate="B" pin="IO_8" pad="L4"/>
<connect gate="B" pin="IO_9" pad="N6"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="F11"/>
<connect gate="C" pin="IO_11" pad="F12"/>
<connect gate="C" pin="IO_12" pad="F13"/>
<connect gate="C" pin="IO_13" pad="F14"/>
<connect gate="C" pin="IO_14" pad="F15"/>
<connect gate="C" pin="IO_15" pad="F16"/>
<connect gate="C" pin="IO_16" pad="H13"/>
<connect gate="C" pin="IO_17" pad="H14"/>
<connect gate="C" pin="IO_18" pad="G11"/>
<connect gate="C" pin="IO_19" pad="H15"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="G12"/>
<connect gate="C" pin="IO_21" pad="H16"/>
<connect gate="C" pin="IO_22" pad="K11"/>
<connect gate="C" pin="IO_23" pad="G13"/>
<connect gate="C" pin="IO_24" pad="K12"/>
<connect gate="C" pin="IO_25" pad="G14"/>
<connect gate="C" pin="IO_26" pad="K13"/>
<connect gate="C" pin="IO_27" pad="G15"/>
<connect gate="C" pin="IO_28" pad="K14"/>
<connect gate="C" pin="IO_29" pad="G16"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="K15"/>
<connect gate="C" pin="IO_31" pad="J13"/>
<connect gate="C" pin="IO_32" pad="K16"/>
<connect gate="C" pin="IO_33" pad="J14"/>
<connect gate="C" pin="IO_34" pad="L10"/>
<connect gate="C" pin="IO_35" pad="J15"/>
<connect gate="C" pin="IO_36" pad="J16"/>
<connect gate="C" pin="IO_37" pad="L11"/>
<connect gate="C" pin="IO_38" pad="L12"/>
<connect gate="C" pin="IO_39" pad="L13"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="L14"/>
<connect gate="C" pin="IO_41" pad="L15"/>
<connect gate="C" pin="IO_42" pad="L16"/>
<connect gate="C" pin="IO_43" pad="M10"/>
<connect gate="C" pin="IO_44" pad="M11"/>
<connect gate="C" pin="IO_45" pad="M12"/>
<connect gate="C" pin="IO_46" pad="M13"/>
<connect gate="C" pin="IO_47" pad="M14"/>
<connect gate="C" pin="IO_48" pad="M15"/>
<connect gate="C" pin="IO_49" pad="M16"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="N10"/>
<connect gate="C" pin="IO_51" pad="N11"/>
<connect gate="C" pin="IO_52" pad="N12"/>
<connect gate="C" pin="IO_53" pad="N13"/>
<connect gate="C" pin="IO_54" pad="N14"/>
<connect gate="C" pin="IO_55" pad="N15"/>
<connect gate="C" pin="IO_56" pad="N16"/>
<connect gate="C" pin="IO_57" pad="P10"/>
<connect gate="C" pin="IO_58" pad="P11"/>
<connect gate="C" pin="IO_59" pad="P12"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_60" pad="P13"/>
<connect gate="C" pin="IO_61" pad="P14"/>
<connect gate="C" pin="IO_62" pad="P15"/>
<connect gate="C" pin="IO_63" pad="R10"/>
<connect gate="C" pin="IO_64" pad="R11"/>
<connect gate="C" pin="IO_65" pad="R12"/>
<connect gate="C" pin="IO_66" pad="R13"/>
<connect gate="C" pin="IO_67" pad="R14"/>
<connect gate="C" pin="IO_68" pad="R16"/>
<connect gate="C" pin="IO_69" pad="T10"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_70" pad="T11"/>
<connect gate="C" pin="IO_71" pad="T12"/>
<connect gate="C" pin="IO_72" pad="T13"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="F10"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO3" pad="J11"/>
<connect gate="C" pin="VCCIO3_2" pad="P16"/>
<connect gate="C" pin="VCCIO3_3" pad="H11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270F256I5N"/>
<attribute name="OC_FARNELL" value="1549478"/>
<attribute name="OC_NEWARK" value="51R9279"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270GM256C5N">
<description>IC MAX II CPLD 1270 LE 256-MBGA</description>
<gates>
<gate name="A" symbol="EPM1270GM256C5N_A"/>
<gate name="B" symbol="EPM1270GM256C5N_B"/>
<gate name="C" symbol="EPM1270GM256C5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C50P20X20_1100X1100X120">
<connects>
<connect gate="A" pin="GNDINT" pad="J4"/>
<connect gate="A" pin="GNDIO" pad="N3"/>
<connect gate="A" pin="GNDIO_2" pad="C8"/>
<connect gate="A" pin="GNDIO_3" pad="D9"/>
<connect gate="A" pin="GNDIO_4" pad="H3"/>
<connect gate="A" pin="GNDIO_5" pad="J3"/>
<connect gate="A" pin="GNDIO_6" pad="M4"/>
<connect gate="A" pin="IO" pad="U1"/>
<connect gate="A" pin="IO/GCLK0" pad="K1"/>
<connect gate="A" pin="IO/GCLK1" pad="L1"/>
<connect gate="A" pin="IO_10" pad="A9"/>
<connect gate="A" pin="IO_11" pad="B1"/>
<connect gate="A" pin="IO_12" pad="B2"/>
<connect gate="A" pin="IO_13" pad="B3"/>
<connect gate="A" pin="IO_14" pad="B4"/>
<connect gate="A" pin="IO_15" pad="B5"/>
<connect gate="A" pin="IO_16" pad="B6"/>
<connect gate="A" pin="IO_17" pad="B7"/>
<connect gate="A" pin="IO_18" pad="B8"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A1"/>
<connect gate="A" pin="IO_20" pad="C1"/>
<connect gate="A" pin="IO_21" pad="C2"/>
<connect gate="A" pin="IO_22" pad="C3"/>
<connect gate="A" pin="IO_23" pad="C4"/>
<connect gate="A" pin="IO_24" pad="C5"/>
<connect gate="A" pin="IO_25" pad="C6"/>
<connect gate="A" pin="IO_26" pad="C7"/>
<connect gate="A" pin="IO_27" pad="D1"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D3"/>
<connect gate="A" pin="IO_3" pad="A2"/>
<connect gate="A" pin="IO_30" pad="D4"/>
<connect gate="A" pin="IO_31" pad="D5"/>
<connect gate="A" pin="IO_32" pad="D6"/>
<connect gate="A" pin="IO_33" pad="D7"/>
<connect gate="A" pin="IO_34" pad="D8"/>
<connect gate="A" pin="IO_35" pad="E1"/>
<connect gate="A" pin="IO_36" pad="E2"/>
<connect gate="A" pin="IO_37" pad="E3"/>
<connect gate="A" pin="IO_38" pad="E4"/>
<connect gate="A" pin="IO_39" pad="F1"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="F2"/>
<connect gate="A" pin="IO_41" pad="F3"/>
<connect gate="A" pin="IO_42" pad="F4"/>
<connect gate="A" pin="IO_43" pad="G1"/>
<connect gate="A" pin="IO_44" pad="G2"/>
<connect gate="A" pin="IO_45" pad="G3"/>
<connect gate="A" pin="IO_46" pad="G4"/>
<connect gate="A" pin="IO_47" pad="H1"/>
<connect gate="A" pin="IO_48" pad="H2"/>
<connect gate="A" pin="IO_49" pad="H4"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="J1"/>
<connect gate="A" pin="IO_51" pad="J2"/>
<connect gate="A" pin="IO_52" pad="K2"/>
<connect gate="A" pin="IO_53" pad="L2"/>
<connect gate="A" pin="IO_54" pad="M1"/>
<connect gate="A" pin="IO_55" pad="M2"/>
<connect gate="A" pin="IO_56" pad="N1"/>
<connect gate="A" pin="IO_57" pad="N2"/>
<connect gate="A" pin="IO_58" pad="N4"/>
<connect gate="A" pin="IO_59" pad="P1"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_60" pad="P2"/>
<connect gate="A" pin="IO_61" pad="P3"/>
<connect gate="A" pin="IO_62" pad="P4"/>
<connect gate="A" pin="IO_63" pad="R1"/>
<connect gate="A" pin="IO_64" pad="R2"/>
<connect gate="A" pin="IO_65" pad="R3"/>
<connect gate="A" pin="IO_66" pad="T1"/>
<connect gate="A" pin="IO_67" pad="T2"/>
<connect gate="A" pin="IO_68" pad="T4"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="A8"/>
<connect gate="A" pin="R4" pad="R4"/>
<connect gate="A" pin="TDI" pad="U2"/>
<connect gate="A" pin="TMS" pad="T3"/>
<connect gate="A" pin="VCCINT" pad="K4"/>
<connect gate="A" pin="VCCIO1" pad="M3"/>
<connect gate="A" pin="VCCIO1_2" pad="K3"/>
<connect gate="A" pin="VCCIO1_3" pad="L3"/>
<connect gate="A" pin="VCCIO1_4" pad="L4"/>
<connect gate="A" pin="VCCIO2" pad="C9"/>
<connect gate="B" pin="GNDINT" pad="D12"/>
<connect gate="B" pin="GNDIO" pad="C13"/>
<connect gate="B" pin="GNDIO_2" pad="U9"/>
<connect gate="B" pin="GNDIO_3" pad="V8"/>
<connect gate="B" pin="GNDIO_4" pad="V9"/>
<connect gate="B" pin="GNDIO_5" pad="C12"/>
<connect gate="B" pin="IO" pad="D17"/>
<connect gate="B" pin="IO_10" pad="V4"/>
<connect gate="B" pin="IO_11" pad="V5"/>
<connect gate="B" pin="IO_12" pad="V6"/>
<connect gate="B" pin="IO_13" pad="V7"/>
<connect gate="B" pin="IO_14" pad="W1"/>
<connect gate="B" pin="IO_15" pad="W3"/>
<connect gate="B" pin="IO_16" pad="W4"/>
<connect gate="B" pin="IO_17" pad="W5"/>
<connect gate="B" pin="IO_18" pad="W6"/>
<connect gate="B" pin="IO_19" pad="W7"/>
<connect gate="B" pin="IO_2" pad="U3"/>
<connect gate="B" pin="IO_20" pad="W8"/>
<connect gate="B" pin="IO_21" pad="W9"/>
<connect gate="B" pin="IO_22" pad="Y1"/>
<connect gate="B" pin="IO_23" pad="Y2"/>
<connect gate="B" pin="IO_24" pad="D18"/>
<connect gate="B" pin="IO_25" pad="D19"/>
<connect gate="B" pin="IO_26" pad="D20"/>
<connect gate="B" pin="IO_27" pad="E17"/>
<connect gate="B" pin="IO_28" pad="E18"/>
<connect gate="B" pin="IO_29" pad="E19"/>
<connect gate="B" pin="IO_3" pad="U4"/>
<connect gate="B" pin="IO_30" pad="E20"/>
<connect gate="B" pin="IO_31" pad="F17"/>
<connect gate="B" pin="IO_32" pad="F18"/>
<connect gate="B" pin="IO_33" pad="F19"/>
<connect gate="B" pin="IO_34" pad="F20"/>
<connect gate="B" pin="IO_35" pad="Y3"/>
<connect gate="B" pin="IO_36" pad="Y4"/>
<connect gate="B" pin="IO_37" pad="Y5"/>
<connect gate="B" pin="IO_38" pad="Y6"/>
<connect gate="B" pin="IO_39" pad="Y7"/>
<connect gate="B" pin="IO_4" pad="U5"/>
<connect gate="B" pin="IO_40" pad="Y8"/>
<connect gate="B" pin="IO_41" pad="Y9"/>
<connect gate="B" pin="IO_42" pad="A10"/>
<connect gate="B" pin="IO_43" pad="A11"/>
<connect gate="B" pin="IO_44" pad="A12"/>
<connect gate="B" pin="IO_45" pad="A13"/>
<connect gate="B" pin="IO_46" pad="A14"/>
<connect gate="B" pin="IO_47" pad="A15"/>
<connect gate="B" pin="IO_48" pad="A16"/>
<connect gate="B" pin="IO_49" pad="A17"/>
<connect gate="B" pin="IO_5" pad="U6"/>
<connect gate="B" pin="IO_50" pad="A18"/>
<connect gate="B" pin="IO_51" pad="A19"/>
<connect gate="B" pin="IO_52" pad="A20"/>
<connect gate="B" pin="IO_53" pad="B10"/>
<connect gate="B" pin="IO_54" pad="B11"/>
<connect gate="B" pin="IO_55" pad="B12"/>
<connect gate="B" pin="IO_56" pad="B13"/>
<connect gate="B" pin="IO_57" pad="B14"/>
<connect gate="B" pin="IO_58" pad="B15"/>
<connect gate="B" pin="IO_59" pad="B16"/>
<connect gate="B" pin="IO_6" pad="U7"/>
<connect gate="B" pin="IO_60" pad="B17"/>
<connect gate="B" pin="IO_61" pad="B18"/>
<connect gate="B" pin="IO_62" pad="B19"/>
<connect gate="B" pin="IO_63" pad="B20"/>
<connect gate="B" pin="IO_64" pad="C14"/>
<connect gate="B" pin="IO_65" pad="C15"/>
<connect gate="B" pin="IO_66" pad="C16"/>
<connect gate="B" pin="IO_67" pad="C17"/>
<connect gate="B" pin="IO_68" pad="C18"/>
<connect gate="B" pin="IO_69" pad="C19"/>
<connect gate="B" pin="IO_7" pad="U8"/>
<connect gate="B" pin="IO_70" pad="C20"/>
<connect gate="B" pin="IO_71" pad="D13"/>
<connect gate="B" pin="IO_72" pad="D14"/>
<connect gate="B" pin="IO_73" pad="D15"/>
<connect gate="B" pin="IO_74" pad="D16"/>
<connect gate="B" pin="IO_8" pad="V1"/>
<connect gate="B" pin="IO_9" pad="V3"/>
<connect gate="B" pin="TCK" pad="W2"/>
<connect gate="B" pin="TDO" pad="V2"/>
<connect gate="B" pin="VCCINT" pad="D11"/>
<connect gate="B" pin="VCCIO2" pad="D10"/>
<connect gate="B" pin="VCCIO2_2" pad="C10"/>
<connect gate="B" pin="VCCIO2_3" pad="C11"/>
<connect gate="C" pin="GNDINT" pad="U12"/>
<connect gate="C" pin="GNDINT_2" pad="M17"/>
<connect gate="C" pin="GNDIO" pad="N18"/>
<connect gate="C" pin="GNDIO_2" pad="H18"/>
<connect gate="C" pin="GNDIO_3" pad="J17"/>
<connect gate="C" pin="GNDIO_4" pad="V13"/>
<connect gate="C" pin="GNDIO_5" pad="M18"/>
<connect gate="C" pin="IO" pad="Y10"/>
<connect gate="C" pin="IO/DEV_CLRN" pad="Y13"/>
<connect gate="C" pin="IO/DEV_OE" pad="W12"/>
<connect gate="C" pin="IO/GCLK2" pad="M20"/>
<connect gate="C" pin="IO/GCLK3" pad="L20"/>
<connect gate="C" pin="IO_10" pad="J20"/>
<connect gate="C" pin="IO_11" pad="K19"/>
<connect gate="C" pin="IO_12" pad="K20"/>
<connect gate="C" pin="IO_13" pad="L19"/>
<connect gate="C" pin="IO_14" pad="M19"/>
<connect gate="C" pin="IO_15" pad="N17"/>
<connect gate="C" pin="IO_16" pad="Y11"/>
<connect gate="C" pin="IO_17" pad="Y12"/>
<connect gate="C" pin="IO_18" pad="Y14"/>
<connect gate="C" pin="IO_19" pad="Y15"/>
<connect gate="C" pin="IO_2" pad="G17"/>
<connect gate="C" pin="IO_20" pad="Y16"/>
<connect gate="C" pin="IO_21" pad="Y17"/>
<connect gate="C" pin="IO_22" pad="Y18"/>
<connect gate="C" pin="IO_23" pad="Y19"/>
<connect gate="C" pin="IO_24" pad="Y20"/>
<connect gate="C" pin="IO_25" pad="N19"/>
<connect gate="C" pin="IO_26" pad="N20"/>
<connect gate="C" pin="IO_27" pad="P17"/>
<connect gate="C" pin="IO_28" pad="P18"/>
<connect gate="C" pin="IO_29" pad="P19"/>
<connect gate="C" pin="IO_3" pad="G18"/>
<connect gate="C" pin="IO_30" pad="P20"/>
<connect gate="C" pin="IO_31" pad="R17"/>
<connect gate="C" pin="IO_32" pad="R18"/>
<connect gate="C" pin="IO_33" pad="R19"/>
<connect gate="C" pin="IO_34" pad="R20"/>
<connect gate="C" pin="IO_35" pad="T17"/>
<connect gate="C" pin="IO_36" pad="T18"/>
<connect gate="C" pin="IO_37" pad="T19"/>
<connect gate="C" pin="IO_38" pad="T20"/>
<connect gate="C" pin="IO_39" pad="U13"/>
<connect gate="C" pin="IO_4" pad="G19"/>
<connect gate="C" pin="IO_40" pad="U14"/>
<connect gate="C" pin="IO_41" pad="U15"/>
<connect gate="C" pin="IO_42" pad="U16"/>
<connect gate="C" pin="IO_43" pad="U17"/>
<connect gate="C" pin="IO_44" pad="U18"/>
<connect gate="C" pin="IO_45" pad="U19"/>
<connect gate="C" pin="IO_46" pad="U20"/>
<connect gate="C" pin="IO_47" pad="V14"/>
<connect gate="C" pin="IO_48" pad="V15"/>
<connect gate="C" pin="IO_49" pad="V16"/>
<connect gate="C" pin="IO_5" pad="G20"/>
<connect gate="C" pin="IO_50" pad="V17"/>
<connect gate="C" pin="IO_51" pad="V18"/>
<connect gate="C" pin="IO_52" pad="V19"/>
<connect gate="C" pin="IO_53" pad="V20"/>
<connect gate="C" pin="IO_54" pad="W10"/>
<connect gate="C" pin="IO_55" pad="W11"/>
<connect gate="C" pin="IO_56" pad="W13"/>
<connect gate="C" pin="IO_57" pad="W14"/>
<connect gate="C" pin="IO_58" pad="W15"/>
<connect gate="C" pin="IO_59" pad="W16"/>
<connect gate="C" pin="IO_6" pad="H17"/>
<connect gate="C" pin="IO_60" pad="W17"/>
<connect gate="C" pin="IO_61" pad="W18"/>
<connect gate="C" pin="IO_62" pad="W19"/>
<connect gate="C" pin="IO_63" pad="W20"/>
<connect gate="C" pin="IO_7" pad="H19"/>
<connect gate="C" pin="IO_8" pad="H20"/>
<connect gate="C" pin="IO_9" pad="J19"/>
<connect gate="C" pin="VCCINT" pad="U11"/>
<connect gate="C" pin="VCCINT_2" pad="L17"/>
<connect gate="C" pin="VCCIO3" pad="L18"/>
<connect gate="C" pin="VCCIO3_2" pad="J18"/>
<connect gate="C" pin="VCCIO3_3" pad="K17"/>
<connect gate="C" pin="VCCIO3_4" pad="K18"/>
<connect gate="C" pin="VCCIO4" pad="V12"/>
<connect gate="C" pin="VCCIO4_2" pad="V10"/>
<connect gate="C" pin="VCCIO4_3" pad="U10"/>
<connect gate="C" pin="VCCIO4_4" pad="V11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270GM256C5N"/>
<attribute name="OC_FARNELL" value="1549483"/>
<attribute name="OC_NEWARK" value="51R9288"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270GT144C4N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270GT144C4N_A"/>
<gate name="B" symbol="EPM1270GT144C4N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="9"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO4" pad="64"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="116"/>
<connect gate="B" pin="VCCIO3" pad="82"/>
<connect gate="B" pin="VCCIO3_2" pad="100"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270GT144C4N"/>
<attribute name="OC_FARNELL" value="1742175"/>
<attribute name="OC_NEWARK" value="51R0485"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270GT144C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270GT144C5N_A"/>
<gate name="B" symbol="EPM1270GT144C5N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="9"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO4" pad="64"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="116"/>
<connect gate="B" pin="VCCIO3" pad="82"/>
<connect gate="B" pin="VCCIO3_2" pad="100"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270GT144C5N"/>
<attribute name="OC_FARNELL" value="1549472"/>
<attribute name="OC_NEWARK" value="51R9294"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270M256C5N">
<description>IC MAX II CPLD 1270 LE 256-MBGA</description>
<gates>
<gate name="A" symbol="EPM1270M256C5N_A"/>
<gate name="B" symbol="EPM1270M256C5N_B"/>
<gate name="C" symbol="EPM1270M256C5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C50P20X20_1100X1100X120">
<connects>
<connect gate="A" pin="GNDINT" pad="J4"/>
<connect gate="A" pin="GNDIO" pad="N3"/>
<connect gate="A" pin="GNDIO_2" pad="C8"/>
<connect gate="A" pin="GNDIO_3" pad="D9"/>
<connect gate="A" pin="GNDIO_4" pad="H3"/>
<connect gate="A" pin="GNDIO_5" pad="J3"/>
<connect gate="A" pin="GNDIO_6" pad="M4"/>
<connect gate="A" pin="IO" pad="U1"/>
<connect gate="A" pin="IO/GCLK0" pad="K1"/>
<connect gate="A" pin="IO/GCLK1" pad="L1"/>
<connect gate="A" pin="IO_10" pad="A9"/>
<connect gate="A" pin="IO_11" pad="B1"/>
<connect gate="A" pin="IO_12" pad="B2"/>
<connect gate="A" pin="IO_13" pad="B3"/>
<connect gate="A" pin="IO_14" pad="B4"/>
<connect gate="A" pin="IO_15" pad="B5"/>
<connect gate="A" pin="IO_16" pad="B6"/>
<connect gate="A" pin="IO_17" pad="B7"/>
<connect gate="A" pin="IO_18" pad="B8"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A1"/>
<connect gate="A" pin="IO_20" pad="C1"/>
<connect gate="A" pin="IO_21" pad="C2"/>
<connect gate="A" pin="IO_22" pad="C3"/>
<connect gate="A" pin="IO_23" pad="C4"/>
<connect gate="A" pin="IO_24" pad="C5"/>
<connect gate="A" pin="IO_25" pad="C6"/>
<connect gate="A" pin="IO_26" pad="C7"/>
<connect gate="A" pin="IO_27" pad="D1"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D3"/>
<connect gate="A" pin="IO_3" pad="A2"/>
<connect gate="A" pin="IO_30" pad="D4"/>
<connect gate="A" pin="IO_31" pad="D5"/>
<connect gate="A" pin="IO_32" pad="D6"/>
<connect gate="A" pin="IO_33" pad="D7"/>
<connect gate="A" pin="IO_34" pad="D8"/>
<connect gate="A" pin="IO_35" pad="E1"/>
<connect gate="A" pin="IO_36" pad="E2"/>
<connect gate="A" pin="IO_37" pad="E3"/>
<connect gate="A" pin="IO_38" pad="E4"/>
<connect gate="A" pin="IO_39" pad="F1"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="F2"/>
<connect gate="A" pin="IO_41" pad="F3"/>
<connect gate="A" pin="IO_42" pad="F4"/>
<connect gate="A" pin="IO_43" pad="G1"/>
<connect gate="A" pin="IO_44" pad="G2"/>
<connect gate="A" pin="IO_45" pad="G3"/>
<connect gate="A" pin="IO_46" pad="G4"/>
<connect gate="A" pin="IO_47" pad="H1"/>
<connect gate="A" pin="IO_48" pad="H2"/>
<connect gate="A" pin="IO_49" pad="H4"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="J1"/>
<connect gate="A" pin="IO_51" pad="J2"/>
<connect gate="A" pin="IO_52" pad="K2"/>
<connect gate="A" pin="IO_53" pad="L2"/>
<connect gate="A" pin="IO_54" pad="M1"/>
<connect gate="A" pin="IO_55" pad="M2"/>
<connect gate="A" pin="IO_56" pad="N1"/>
<connect gate="A" pin="IO_57" pad="N2"/>
<connect gate="A" pin="IO_58" pad="N4"/>
<connect gate="A" pin="IO_59" pad="P1"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_60" pad="P2"/>
<connect gate="A" pin="IO_61" pad="P3"/>
<connect gate="A" pin="IO_62" pad="P4"/>
<connect gate="A" pin="IO_63" pad="R1"/>
<connect gate="A" pin="IO_64" pad="R2"/>
<connect gate="A" pin="IO_65" pad="R3"/>
<connect gate="A" pin="IO_66" pad="T1"/>
<connect gate="A" pin="IO_67" pad="T2"/>
<connect gate="A" pin="IO_68" pad="T4"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="A8"/>
<connect gate="A" pin="R4" pad="R4"/>
<connect gate="A" pin="TDI" pad="U2"/>
<connect gate="A" pin="TMS" pad="T3"/>
<connect gate="A" pin="VCCINT" pad="K4"/>
<connect gate="A" pin="VCCIO1" pad="M3"/>
<connect gate="A" pin="VCCIO1_2" pad="K3"/>
<connect gate="A" pin="VCCIO1_3" pad="L3"/>
<connect gate="A" pin="VCCIO1_4" pad="L4"/>
<connect gate="A" pin="VCCIO2" pad="C9"/>
<connect gate="B" pin="GNDINT" pad="D12"/>
<connect gate="B" pin="GNDIO" pad="C13"/>
<connect gate="B" pin="GNDIO_2" pad="U9"/>
<connect gate="B" pin="GNDIO_3" pad="V8"/>
<connect gate="B" pin="GNDIO_4" pad="V9"/>
<connect gate="B" pin="GNDIO_5" pad="C12"/>
<connect gate="B" pin="IO" pad="D17"/>
<connect gate="B" pin="IO_10" pad="V4"/>
<connect gate="B" pin="IO_11" pad="V5"/>
<connect gate="B" pin="IO_12" pad="V6"/>
<connect gate="B" pin="IO_13" pad="V7"/>
<connect gate="B" pin="IO_14" pad="W1"/>
<connect gate="B" pin="IO_15" pad="W3"/>
<connect gate="B" pin="IO_16" pad="W4"/>
<connect gate="B" pin="IO_17" pad="W5"/>
<connect gate="B" pin="IO_18" pad="W6"/>
<connect gate="B" pin="IO_19" pad="W7"/>
<connect gate="B" pin="IO_2" pad="U3"/>
<connect gate="B" pin="IO_20" pad="W8"/>
<connect gate="B" pin="IO_21" pad="W9"/>
<connect gate="B" pin="IO_22" pad="Y1"/>
<connect gate="B" pin="IO_23" pad="Y2"/>
<connect gate="B" pin="IO_24" pad="D18"/>
<connect gate="B" pin="IO_25" pad="D19"/>
<connect gate="B" pin="IO_26" pad="D20"/>
<connect gate="B" pin="IO_27" pad="E17"/>
<connect gate="B" pin="IO_28" pad="E18"/>
<connect gate="B" pin="IO_29" pad="E19"/>
<connect gate="B" pin="IO_3" pad="U4"/>
<connect gate="B" pin="IO_30" pad="E20"/>
<connect gate="B" pin="IO_31" pad="F17"/>
<connect gate="B" pin="IO_32" pad="F18"/>
<connect gate="B" pin="IO_33" pad="F19"/>
<connect gate="B" pin="IO_34" pad="F20"/>
<connect gate="B" pin="IO_35" pad="Y3"/>
<connect gate="B" pin="IO_36" pad="Y4"/>
<connect gate="B" pin="IO_37" pad="Y5"/>
<connect gate="B" pin="IO_38" pad="Y6"/>
<connect gate="B" pin="IO_39" pad="Y7"/>
<connect gate="B" pin="IO_4" pad="U5"/>
<connect gate="B" pin="IO_40" pad="Y8"/>
<connect gate="B" pin="IO_41" pad="Y9"/>
<connect gate="B" pin="IO_42" pad="A10"/>
<connect gate="B" pin="IO_43" pad="A11"/>
<connect gate="B" pin="IO_44" pad="A12"/>
<connect gate="B" pin="IO_45" pad="A13"/>
<connect gate="B" pin="IO_46" pad="A14"/>
<connect gate="B" pin="IO_47" pad="A15"/>
<connect gate="B" pin="IO_48" pad="A16"/>
<connect gate="B" pin="IO_49" pad="A17"/>
<connect gate="B" pin="IO_5" pad="U6"/>
<connect gate="B" pin="IO_50" pad="A18"/>
<connect gate="B" pin="IO_51" pad="A19"/>
<connect gate="B" pin="IO_52" pad="A20"/>
<connect gate="B" pin="IO_53" pad="B10"/>
<connect gate="B" pin="IO_54" pad="B11"/>
<connect gate="B" pin="IO_55" pad="B12"/>
<connect gate="B" pin="IO_56" pad="B13"/>
<connect gate="B" pin="IO_57" pad="B14"/>
<connect gate="B" pin="IO_58" pad="B15"/>
<connect gate="B" pin="IO_59" pad="B16"/>
<connect gate="B" pin="IO_6" pad="U7"/>
<connect gate="B" pin="IO_60" pad="B17"/>
<connect gate="B" pin="IO_61" pad="B18"/>
<connect gate="B" pin="IO_62" pad="B19"/>
<connect gate="B" pin="IO_63" pad="B20"/>
<connect gate="B" pin="IO_64" pad="C14"/>
<connect gate="B" pin="IO_65" pad="C15"/>
<connect gate="B" pin="IO_66" pad="C16"/>
<connect gate="B" pin="IO_67" pad="C17"/>
<connect gate="B" pin="IO_68" pad="C18"/>
<connect gate="B" pin="IO_69" pad="C19"/>
<connect gate="B" pin="IO_7" pad="U8"/>
<connect gate="B" pin="IO_70" pad="C20"/>
<connect gate="B" pin="IO_71" pad="D13"/>
<connect gate="B" pin="IO_72" pad="D14"/>
<connect gate="B" pin="IO_73" pad="D15"/>
<connect gate="B" pin="IO_74" pad="D16"/>
<connect gate="B" pin="IO_8" pad="V1"/>
<connect gate="B" pin="IO_9" pad="V3"/>
<connect gate="B" pin="TCK" pad="W2"/>
<connect gate="B" pin="TDO" pad="V2"/>
<connect gate="B" pin="VCCINT" pad="D11"/>
<connect gate="B" pin="VCCIO2" pad="D10"/>
<connect gate="B" pin="VCCIO2_2" pad="C10"/>
<connect gate="B" pin="VCCIO2_3" pad="C11"/>
<connect gate="C" pin="GNDINT" pad="U12"/>
<connect gate="C" pin="GNDINT_2" pad="M17"/>
<connect gate="C" pin="GNDIO" pad="N18"/>
<connect gate="C" pin="GNDIO_2" pad="H18"/>
<connect gate="C" pin="GNDIO_3" pad="J17"/>
<connect gate="C" pin="GNDIO_4" pad="V13"/>
<connect gate="C" pin="GNDIO_5" pad="M18"/>
<connect gate="C" pin="IO" pad="Y10"/>
<connect gate="C" pin="IO/DEV_CLRN" pad="Y13"/>
<connect gate="C" pin="IO/DEV_OE" pad="W12"/>
<connect gate="C" pin="IO/GCLK2" pad="M20"/>
<connect gate="C" pin="IO/GCLK3" pad="L20"/>
<connect gate="C" pin="IO_10" pad="J20"/>
<connect gate="C" pin="IO_11" pad="K19"/>
<connect gate="C" pin="IO_12" pad="K20"/>
<connect gate="C" pin="IO_13" pad="L19"/>
<connect gate="C" pin="IO_14" pad="M19"/>
<connect gate="C" pin="IO_15" pad="N17"/>
<connect gate="C" pin="IO_16" pad="Y11"/>
<connect gate="C" pin="IO_17" pad="Y12"/>
<connect gate="C" pin="IO_18" pad="Y14"/>
<connect gate="C" pin="IO_19" pad="Y15"/>
<connect gate="C" pin="IO_2" pad="G17"/>
<connect gate="C" pin="IO_20" pad="Y16"/>
<connect gate="C" pin="IO_21" pad="Y17"/>
<connect gate="C" pin="IO_22" pad="Y18"/>
<connect gate="C" pin="IO_23" pad="Y19"/>
<connect gate="C" pin="IO_24" pad="Y20"/>
<connect gate="C" pin="IO_25" pad="N19"/>
<connect gate="C" pin="IO_26" pad="N20"/>
<connect gate="C" pin="IO_27" pad="P17"/>
<connect gate="C" pin="IO_28" pad="P18"/>
<connect gate="C" pin="IO_29" pad="P19"/>
<connect gate="C" pin="IO_3" pad="G18"/>
<connect gate="C" pin="IO_30" pad="P20"/>
<connect gate="C" pin="IO_31" pad="R17"/>
<connect gate="C" pin="IO_32" pad="R18"/>
<connect gate="C" pin="IO_33" pad="R19"/>
<connect gate="C" pin="IO_34" pad="R20"/>
<connect gate="C" pin="IO_35" pad="T17"/>
<connect gate="C" pin="IO_36" pad="T18"/>
<connect gate="C" pin="IO_37" pad="T19"/>
<connect gate="C" pin="IO_38" pad="T20"/>
<connect gate="C" pin="IO_39" pad="U13"/>
<connect gate="C" pin="IO_4" pad="G19"/>
<connect gate="C" pin="IO_40" pad="U14"/>
<connect gate="C" pin="IO_41" pad="U15"/>
<connect gate="C" pin="IO_42" pad="U16"/>
<connect gate="C" pin="IO_43" pad="U17"/>
<connect gate="C" pin="IO_44" pad="U18"/>
<connect gate="C" pin="IO_45" pad="U19"/>
<connect gate="C" pin="IO_46" pad="U20"/>
<connect gate="C" pin="IO_47" pad="V14"/>
<connect gate="C" pin="IO_48" pad="V15"/>
<connect gate="C" pin="IO_49" pad="V16"/>
<connect gate="C" pin="IO_5" pad="G20"/>
<connect gate="C" pin="IO_50" pad="V17"/>
<connect gate="C" pin="IO_51" pad="V18"/>
<connect gate="C" pin="IO_52" pad="V19"/>
<connect gate="C" pin="IO_53" pad="V20"/>
<connect gate="C" pin="IO_54" pad="W10"/>
<connect gate="C" pin="IO_55" pad="W11"/>
<connect gate="C" pin="IO_56" pad="W13"/>
<connect gate="C" pin="IO_57" pad="W14"/>
<connect gate="C" pin="IO_58" pad="W15"/>
<connect gate="C" pin="IO_59" pad="W16"/>
<connect gate="C" pin="IO_6" pad="H17"/>
<connect gate="C" pin="IO_60" pad="W17"/>
<connect gate="C" pin="IO_61" pad="W18"/>
<connect gate="C" pin="IO_62" pad="W19"/>
<connect gate="C" pin="IO_63" pad="W20"/>
<connect gate="C" pin="IO_7" pad="H19"/>
<connect gate="C" pin="IO_8" pad="H20"/>
<connect gate="C" pin="IO_9" pad="J19"/>
<connect gate="C" pin="VCCINT" pad="U11"/>
<connect gate="C" pin="VCCINT_2" pad="L17"/>
<connect gate="C" pin="VCCIO3" pad="L18"/>
<connect gate="C" pin="VCCIO3_2" pad="J18"/>
<connect gate="C" pin="VCCIO3_3" pad="K17"/>
<connect gate="C" pin="VCCIO3_4" pad="K18"/>
<connect gate="C" pin="VCCIO4" pad="V12"/>
<connect gate="C" pin="VCCIO4_2" pad="V10"/>
<connect gate="C" pin="VCCIO4_3" pad="U10"/>
<connect gate="C" pin="VCCIO4_4" pad="V11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270M256C5N"/>
<attribute name="OC_FARNELL" value="1635102"/>
<attribute name="OC_NEWARK" value="51R0486"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270T144C3N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270T144C3N_A"/>
<gate name="B" symbol="EPM1270T144C3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="9"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO4" pad="64"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="116"/>
<connect gate="B" pin="VCCIO3" pad="82"/>
<connect gate="B" pin="VCCIO3_2" pad="100"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270T144C3N"/>
<attribute name="OC_FARNELL" value="1453471"/>
<attribute name="OC_NEWARK" value="51R9301"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270T144C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270T144C5N_A"/>
<gate name="B" symbol="EPM1270T144C5N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="9"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO4" pad="64"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="116"/>
<connect gate="B" pin="VCCIO3" pad="82"/>
<connect gate="B" pin="VCCIO3_2" pad="100"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270T144C5N"/>
<attribute name="OC_FARNELL" value="1453481"/>
<attribute name="OC_NEWARK" value="51R0487"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM1270T144I5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM1270T144I5N_A"/>
<gate name="B" symbol="EPM1270T144I5N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="9"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO4" pad="64"/>
<connect gate="A" pin="VCCIO4_2" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="116"/>
<connect gate="B" pin="VCCIO3" pad="82"/>
<connect gate="B" pin="VCCIO3_2" pad="100"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM1270T144I5N"/>
<attribute name="OC_FARNELL" value="1549473"/>
<attribute name="OC_NEWARK" value="51R9306"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210F256C4N">
<description>IC CPLD FLASH 1700 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM2210F256C4N_A"/>
<gate name="B" symbol="EPM2210F256C4N_B"/>
<gate name="C" symbol="EPM2210F256C4N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="F7"/>
<connect gate="A" pin="GNDINT_3" pad="G6"/>
<connect gate="A" pin="GNDINT_4" pad="H7"/>
<connect gate="A" pin="GNDINT_5" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J3"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D3"/>
<connect gate="A" pin="IO_26" pad="D1"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="K4"/>
<connect gate="A" pin="IO_35" pad="G4"/>
<connect gate="A" pin="IO_36" pad="E8"/>
<connect gate="A" pin="IO_37" pad="D6"/>
<connect gate="A" pin="IO_38" pad="E9"/>
<connect gate="A" pin="IO_39" pad="F4"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="H4"/>
<connect gate="A" pin="IO_41" pad="D7"/>
<connect gate="A" pin="IO_42" pad="F5"/>
<connect gate="A" pin="IO_43" pad="F6"/>
<connect gate="A" pin="IO_44" pad="G5"/>
<connect gate="A" pin="IO_45" pad="D8"/>
<connect gate="A" pin="IO_46" pad="J4"/>
<connect gate="A" pin="IO_47" pad="D9"/>
<connect gate="A" pin="IO_48" pad="K5"/>
<connect gate="A" pin="IO_49" pad="E5"/>
<connect gate="A" pin="IO_5" pad="A2"/>
<connect gate="A" pin="IO_50" pad="E6"/>
<connect gate="A" pin="IO_51" pad="E7"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="F1"/>
<connect gate="A" pin="IO_55" pad="G3"/>
<connect gate="A" pin="IO_56" pad="F2"/>
<connect gate="A" pin="IO_57" pad="H2"/>
<connect gate="A" pin="IO_58" pad="K3"/>
<connect gate="A" pin="IO_59" pad="H3"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="K1"/>
<connect gate="A" pin="IO_61" pad="F3"/>
<connect gate="A" pin="IO_62" pad="H1"/>
<connect gate="A" pin="IO_63" pad="J1"/>
<connect gate="A" pin="IO_64" pad="J2"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="J6"/>
<connect gate="A" pin="VCCIO1_3" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="L3"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="P5"/>
<connect gate="B" pin="IO_15" pad="L4"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P6"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N3"/>
<connect gate="B" pin="IO_20" pad="P7"/>
<connect gate="B" pin="IO_21" pad="M2"/>
<connect gate="B" pin="IO_22" pad="N1"/>
<connect gate="B" pin="IO_23" pad="M6"/>
<connect gate="B" pin="IO_24" pad="L5"/>
<connect gate="B" pin="IO_25" pad="M7"/>
<connect gate="B" pin="IO_26" pad="N7"/>
<connect gate="B" pin="IO_27" pad="N8"/>
<connect gate="B" pin="IO_28" pad="N6"/>
<connect gate="B" pin="IO_29" pad="N9"/>
<connect gate="B" pin="IO_3" pad="L1"/>
<connect gate="B" pin="IO_30" pad="D10"/>
<connect gate="B" pin="IO_31" pad="R4"/>
<connect gate="B" pin="IO_32" pad="R5"/>
<connect gate="B" pin="IO_33" pad="R6"/>
<connect gate="B" pin="IO_34" pad="R7"/>
<connect gate="B" pin="IO_35" pad="R8"/>
<connect gate="B" pin="IO_36" pad="R9"/>
<connect gate="B" pin="IO_37" pad="T2"/>
<connect gate="B" pin="IO_38" pad="T4"/>
<connect gate="B" pin="IO_39" pad="T5"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="T7"/>
<connect gate="B" pin="IO_42" pad="T8"/>
<connect gate="B" pin="IO_43" pad="T9"/>
<connect gate="B" pin="IO_44" pad="A10"/>
<connect gate="B" pin="IO_45" pad="A11"/>
<connect gate="B" pin="IO_46" pad="A12"/>
<connect gate="B" pin="IO_47" pad="A13"/>
<connect gate="B" pin="IO_48" pad="A15"/>
<connect gate="B" pin="IO_49" pad="B10"/>
<connect gate="B" pin="IO_5" pad="M1"/>
<connect gate="B" pin="IO_50" pad="B11"/>
<connect gate="B" pin="IO_51" pad="B12"/>
<connect gate="B" pin="IO_52" pad="B13"/>
<connect gate="B" pin="IO_53" pad="B14"/>
<connect gate="B" pin="IO_54" pad="B16"/>
<connect gate="B" pin="IO_55" pad="C10"/>
<connect gate="B" pin="IO_56" pad="C11"/>
<connect gate="B" pin="IO_57" pad="C12"/>
<connect gate="B" pin="IO_58" pad="D11"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_60" pad="D12"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="D13"/>
<connect gate="B" pin="IO_63" pad="C15"/>
<connect gate="B" pin="IO_64" pad="D14"/>
<connect gate="B" pin="IO_65" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L2"/>
<connect gate="B" pin="IO_8" pad="P4"/>
<connect gate="B" pin="IO_9" pad="P9"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCINT" pad="K6"/>
<connect gate="B" pin="VCCINT_2" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDINT_2" pad="K11"/>
<connect gate="C" pin="GNDINT_3" pad="L10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="E15"/>
<connect gate="C" pin="IO_11" pad="G15"/>
<connect gate="C" pin="IO_12" pad="H14"/>
<connect gate="C" pin="IO_13" pad="J15"/>
<connect gate="C" pin="IO_14" pad="K14"/>
<connect gate="C" pin="IO_15" pad="E16"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="G16"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="K16"/>
<connect gate="C" pin="IO_2" pad="F13"/>
<connect gate="C" pin="IO_20" pad="J14"/>
<connect gate="C" pin="IO_21" pad="K15"/>
<connect gate="C" pin="IO_22" pad="E10"/>
<connect gate="C" pin="IO_23" pad="H13"/>
<connect gate="C" pin="IO_24" pad="M10"/>
<connect gate="C" pin="IO_25" pad="E11"/>
<connect gate="C" pin="IO_26" pad="J13"/>
<connect gate="C" pin="IO_27" pad="M11"/>
<connect gate="C" pin="IO_28" pad="E12"/>
<connect gate="C" pin="IO_29" pad="G12"/>
<connect gate="C" pin="IO_3" pad="F14"/>
<connect gate="C" pin="IO_30" pad="N10"/>
<connect gate="C" pin="IO_31" pad="F11"/>
<connect gate="C" pin="IO_32" pad="G13"/>
<connect gate="C" pin="IO_33" pad="L11"/>
<connect gate="C" pin="IO_34" pad="L12"/>
<connect gate="C" pin="IO_35" pad="K12"/>
<connect gate="C" pin="IO_36" pad="M12"/>
<connect gate="C" pin="IO_37" pad="N11"/>
<connect gate="C" pin="IO_38" pad="F12"/>
<connect gate="C" pin="IO_39" pad="K13"/>
<connect gate="C" pin="IO_4" pad="E13"/>
<connect gate="C" pin="IO_40" pad="N12"/>
<connect gate="C" pin="IO_41" pad="L13"/>
<connect gate="C" pin="IO_42" pad="N13"/>
<connect gate="C" pin="IO_43" pad="L14"/>
<connect gate="C" pin="IO_44" pad="N14"/>
<connect gate="C" pin="IO_45" pad="L15"/>
<connect gate="C" pin="IO_46" pad="N15"/>
<connect gate="C" pin="IO_47" pad="L16"/>
<connect gate="C" pin="IO_48" pad="N16"/>
<connect gate="C" pin="IO_49" pad="P10"/>
<connect gate="C" pin="IO_5" pad="F15"/>
<connect gate="C" pin="IO_50" pad="P11"/>
<connect gate="C" pin="IO_51" pad="P12"/>
<connect gate="C" pin="IO_52" pad="M13"/>
<connect gate="C" pin="IO_53" pad="P13"/>
<connect gate="C" pin="IO_54" pad="M14"/>
<connect gate="C" pin="IO_55" pad="P14"/>
<connect gate="C" pin="IO_56" pad="M15"/>
<connect gate="C" pin="IO_57" pad="P15"/>
<connect gate="C" pin="IO_58" pad="M16"/>
<connect gate="C" pin="IO_59" pad="R10"/>
<connect gate="C" pin="IO_6" pad="H15"/>
<connect gate="C" pin="IO_60" pad="R11"/>
<connect gate="C" pin="IO_61" pad="R12"/>
<connect gate="C" pin="IO_62" pad="R13"/>
<connect gate="C" pin="IO_63" pad="R14"/>
<connect gate="C" pin="IO_64" pad="R16"/>
<connect gate="C" pin="IO_65" pad="T10"/>
<connect gate="C" pin="IO_66" pad="T11"/>
<connect gate="C" pin="IO_67" pad="T12"/>
<connect gate="C" pin="IO_68" pad="T13"/>
<connect gate="C" pin="IO_7" pad="E14"/>
<connect gate="C" pin="IO_8" pad="H16"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="VCCINT" pad="F10"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="G11"/>
<connect gate="C" pin="VCCIO3" pad="J11"/>
<connect gate="C" pin="VCCIO3_2" pad="P16"/>
<connect gate="C" pin="VCCIO3_3" pad="H11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210F256C4N"/>
<attribute name="OC_FARNELL" value="1549481"/>
<attribute name="OC_NEWARK" value="51R0488"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210F256C5N">
<description>IC CPLD FLASH 1700 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM2210F256C5N_A"/>
<gate name="B" symbol="EPM2210F256C5N_B"/>
<gate name="C" symbol="EPM2210F256C5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="F7"/>
<connect gate="A" pin="GNDINT_3" pad="G6"/>
<connect gate="A" pin="GNDINT_4" pad="H7"/>
<connect gate="A" pin="GNDINT_5" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J3"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D3"/>
<connect gate="A" pin="IO_26" pad="D1"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="K4"/>
<connect gate="A" pin="IO_35" pad="G4"/>
<connect gate="A" pin="IO_36" pad="E8"/>
<connect gate="A" pin="IO_37" pad="D6"/>
<connect gate="A" pin="IO_38" pad="E9"/>
<connect gate="A" pin="IO_39" pad="F4"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="H4"/>
<connect gate="A" pin="IO_41" pad="D7"/>
<connect gate="A" pin="IO_42" pad="F5"/>
<connect gate="A" pin="IO_43" pad="F6"/>
<connect gate="A" pin="IO_44" pad="G5"/>
<connect gate="A" pin="IO_45" pad="D8"/>
<connect gate="A" pin="IO_46" pad="J4"/>
<connect gate="A" pin="IO_47" pad="D9"/>
<connect gate="A" pin="IO_48" pad="K5"/>
<connect gate="A" pin="IO_49" pad="E5"/>
<connect gate="A" pin="IO_5" pad="A2"/>
<connect gate="A" pin="IO_50" pad="E6"/>
<connect gate="A" pin="IO_51" pad="E7"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="F1"/>
<connect gate="A" pin="IO_55" pad="G3"/>
<connect gate="A" pin="IO_56" pad="F2"/>
<connect gate="A" pin="IO_57" pad="H2"/>
<connect gate="A" pin="IO_58" pad="K3"/>
<connect gate="A" pin="IO_59" pad="H3"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="K1"/>
<connect gate="A" pin="IO_61" pad="F3"/>
<connect gate="A" pin="IO_62" pad="H1"/>
<connect gate="A" pin="IO_63" pad="J1"/>
<connect gate="A" pin="IO_64" pad="J2"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="J6"/>
<connect gate="A" pin="VCCIO1_3" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="L3"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="P5"/>
<connect gate="B" pin="IO_15" pad="L4"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P6"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N3"/>
<connect gate="B" pin="IO_20" pad="P7"/>
<connect gate="B" pin="IO_21" pad="M2"/>
<connect gate="B" pin="IO_22" pad="N1"/>
<connect gate="B" pin="IO_23" pad="M6"/>
<connect gate="B" pin="IO_24" pad="L5"/>
<connect gate="B" pin="IO_25" pad="M7"/>
<connect gate="B" pin="IO_26" pad="N7"/>
<connect gate="B" pin="IO_27" pad="N8"/>
<connect gate="B" pin="IO_28" pad="N6"/>
<connect gate="B" pin="IO_29" pad="N9"/>
<connect gate="B" pin="IO_3" pad="L1"/>
<connect gate="B" pin="IO_30" pad="D10"/>
<connect gate="B" pin="IO_31" pad="R4"/>
<connect gate="B" pin="IO_32" pad="R5"/>
<connect gate="B" pin="IO_33" pad="R6"/>
<connect gate="B" pin="IO_34" pad="R7"/>
<connect gate="B" pin="IO_35" pad="R8"/>
<connect gate="B" pin="IO_36" pad="R9"/>
<connect gate="B" pin="IO_37" pad="T2"/>
<connect gate="B" pin="IO_38" pad="T4"/>
<connect gate="B" pin="IO_39" pad="T5"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="T7"/>
<connect gate="B" pin="IO_42" pad="T8"/>
<connect gate="B" pin="IO_43" pad="T9"/>
<connect gate="B" pin="IO_44" pad="A10"/>
<connect gate="B" pin="IO_45" pad="A11"/>
<connect gate="B" pin="IO_46" pad="A12"/>
<connect gate="B" pin="IO_47" pad="A13"/>
<connect gate="B" pin="IO_48" pad="A15"/>
<connect gate="B" pin="IO_49" pad="B10"/>
<connect gate="B" pin="IO_5" pad="M1"/>
<connect gate="B" pin="IO_50" pad="B11"/>
<connect gate="B" pin="IO_51" pad="B12"/>
<connect gate="B" pin="IO_52" pad="B13"/>
<connect gate="B" pin="IO_53" pad="B14"/>
<connect gate="B" pin="IO_54" pad="B16"/>
<connect gate="B" pin="IO_55" pad="C10"/>
<connect gate="B" pin="IO_56" pad="C11"/>
<connect gate="B" pin="IO_57" pad="C12"/>
<connect gate="B" pin="IO_58" pad="D11"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_60" pad="D12"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="D13"/>
<connect gate="B" pin="IO_63" pad="C15"/>
<connect gate="B" pin="IO_64" pad="D14"/>
<connect gate="B" pin="IO_65" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L2"/>
<connect gate="B" pin="IO_8" pad="P4"/>
<connect gate="B" pin="IO_9" pad="P9"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCINT" pad="K6"/>
<connect gate="B" pin="VCCINT_2" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDINT_2" pad="K11"/>
<connect gate="C" pin="GNDINT_3" pad="L10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="E15"/>
<connect gate="C" pin="IO_11" pad="G15"/>
<connect gate="C" pin="IO_12" pad="H14"/>
<connect gate="C" pin="IO_13" pad="J15"/>
<connect gate="C" pin="IO_14" pad="K14"/>
<connect gate="C" pin="IO_15" pad="E16"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="G16"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="K16"/>
<connect gate="C" pin="IO_2" pad="F13"/>
<connect gate="C" pin="IO_20" pad="J14"/>
<connect gate="C" pin="IO_21" pad="K15"/>
<connect gate="C" pin="IO_22" pad="E10"/>
<connect gate="C" pin="IO_23" pad="H13"/>
<connect gate="C" pin="IO_24" pad="M10"/>
<connect gate="C" pin="IO_25" pad="E11"/>
<connect gate="C" pin="IO_26" pad="J13"/>
<connect gate="C" pin="IO_27" pad="M11"/>
<connect gate="C" pin="IO_28" pad="E12"/>
<connect gate="C" pin="IO_29" pad="G12"/>
<connect gate="C" pin="IO_3" pad="F14"/>
<connect gate="C" pin="IO_30" pad="N10"/>
<connect gate="C" pin="IO_31" pad="F11"/>
<connect gate="C" pin="IO_32" pad="G13"/>
<connect gate="C" pin="IO_33" pad="L11"/>
<connect gate="C" pin="IO_34" pad="L12"/>
<connect gate="C" pin="IO_35" pad="K12"/>
<connect gate="C" pin="IO_36" pad="M12"/>
<connect gate="C" pin="IO_37" pad="N11"/>
<connect gate="C" pin="IO_38" pad="F12"/>
<connect gate="C" pin="IO_39" pad="K13"/>
<connect gate="C" pin="IO_4" pad="E13"/>
<connect gate="C" pin="IO_40" pad="N12"/>
<connect gate="C" pin="IO_41" pad="L13"/>
<connect gate="C" pin="IO_42" pad="N13"/>
<connect gate="C" pin="IO_43" pad="L14"/>
<connect gate="C" pin="IO_44" pad="N14"/>
<connect gate="C" pin="IO_45" pad="L15"/>
<connect gate="C" pin="IO_46" pad="N15"/>
<connect gate="C" pin="IO_47" pad="L16"/>
<connect gate="C" pin="IO_48" pad="N16"/>
<connect gate="C" pin="IO_49" pad="P10"/>
<connect gate="C" pin="IO_5" pad="F15"/>
<connect gate="C" pin="IO_50" pad="P11"/>
<connect gate="C" pin="IO_51" pad="P12"/>
<connect gate="C" pin="IO_52" pad="M13"/>
<connect gate="C" pin="IO_53" pad="P13"/>
<connect gate="C" pin="IO_54" pad="M14"/>
<connect gate="C" pin="IO_55" pad="P14"/>
<connect gate="C" pin="IO_56" pad="M15"/>
<connect gate="C" pin="IO_57" pad="P15"/>
<connect gate="C" pin="IO_58" pad="M16"/>
<connect gate="C" pin="IO_59" pad="R10"/>
<connect gate="C" pin="IO_6" pad="H15"/>
<connect gate="C" pin="IO_60" pad="R11"/>
<connect gate="C" pin="IO_61" pad="R12"/>
<connect gate="C" pin="IO_62" pad="R13"/>
<connect gate="C" pin="IO_63" pad="R14"/>
<connect gate="C" pin="IO_64" pad="R16"/>
<connect gate="C" pin="IO_65" pad="T10"/>
<connect gate="C" pin="IO_66" pad="T11"/>
<connect gate="C" pin="IO_67" pad="T12"/>
<connect gate="C" pin="IO_68" pad="T13"/>
<connect gate="C" pin="IO_7" pad="E14"/>
<connect gate="C" pin="IO_8" pad="H16"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="VCCINT" pad="F10"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="G11"/>
<connect gate="C" pin="VCCIO3" pad="J11"/>
<connect gate="C" pin="VCCIO3_2" pad="P16"/>
<connect gate="C" pin="VCCIO3_3" pad="H11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210F256C5N"/>
<attribute name="OC_FARNELL" value="1635103"/>
<attribute name="OC_NEWARK" value="51R0489"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210F256I5N">
<description>IC CPLD FLASH 1700 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM2210F256I5N_A"/>
<gate name="B" symbol="EPM2210F256I5N_B"/>
<gate name="C" symbol="EPM2210F256I5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="F7"/>
<connect gate="A" pin="GNDINT_3" pad="G6"/>
<connect gate="A" pin="GNDINT_4" pad="H7"/>
<connect gate="A" pin="GNDINT_5" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J3"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D3"/>
<connect gate="A" pin="IO_26" pad="D1"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="K4"/>
<connect gate="A" pin="IO_35" pad="G4"/>
<connect gate="A" pin="IO_36" pad="E8"/>
<connect gate="A" pin="IO_37" pad="D6"/>
<connect gate="A" pin="IO_38" pad="E9"/>
<connect gate="A" pin="IO_39" pad="F4"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="H4"/>
<connect gate="A" pin="IO_41" pad="D7"/>
<connect gate="A" pin="IO_42" pad="F5"/>
<connect gate="A" pin="IO_43" pad="F6"/>
<connect gate="A" pin="IO_44" pad="G5"/>
<connect gate="A" pin="IO_45" pad="D8"/>
<connect gate="A" pin="IO_46" pad="J4"/>
<connect gate="A" pin="IO_47" pad="D9"/>
<connect gate="A" pin="IO_48" pad="K5"/>
<connect gate="A" pin="IO_49" pad="E5"/>
<connect gate="A" pin="IO_5" pad="A2"/>
<connect gate="A" pin="IO_50" pad="E6"/>
<connect gate="A" pin="IO_51" pad="E7"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="F1"/>
<connect gate="A" pin="IO_55" pad="G3"/>
<connect gate="A" pin="IO_56" pad="F2"/>
<connect gate="A" pin="IO_57" pad="H2"/>
<connect gate="A" pin="IO_58" pad="K3"/>
<connect gate="A" pin="IO_59" pad="H3"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="K1"/>
<connect gate="A" pin="IO_61" pad="F3"/>
<connect gate="A" pin="IO_62" pad="H1"/>
<connect gate="A" pin="IO_63" pad="J1"/>
<connect gate="A" pin="IO_64" pad="J2"/>
<connect gate="A" pin="IO_65" pad="K2"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="J6"/>
<connect gate="A" pin="VCCIO1_3" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="L3"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="P5"/>
<connect gate="B" pin="IO_15" pad="L4"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P6"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N3"/>
<connect gate="B" pin="IO_20" pad="P7"/>
<connect gate="B" pin="IO_21" pad="M2"/>
<connect gate="B" pin="IO_22" pad="N1"/>
<connect gate="B" pin="IO_23" pad="M6"/>
<connect gate="B" pin="IO_24" pad="L5"/>
<connect gate="B" pin="IO_25" pad="M7"/>
<connect gate="B" pin="IO_26" pad="N7"/>
<connect gate="B" pin="IO_27" pad="N8"/>
<connect gate="B" pin="IO_28" pad="N6"/>
<connect gate="B" pin="IO_29" pad="N9"/>
<connect gate="B" pin="IO_3" pad="L1"/>
<connect gate="B" pin="IO_30" pad="D10"/>
<connect gate="B" pin="IO_31" pad="R4"/>
<connect gate="B" pin="IO_32" pad="R5"/>
<connect gate="B" pin="IO_33" pad="R6"/>
<connect gate="B" pin="IO_34" pad="R7"/>
<connect gate="B" pin="IO_35" pad="R8"/>
<connect gate="B" pin="IO_36" pad="R9"/>
<connect gate="B" pin="IO_37" pad="T2"/>
<connect gate="B" pin="IO_38" pad="T4"/>
<connect gate="B" pin="IO_39" pad="T5"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="T6"/>
<connect gate="B" pin="IO_41" pad="T7"/>
<connect gate="B" pin="IO_42" pad="T8"/>
<connect gate="B" pin="IO_43" pad="T9"/>
<connect gate="B" pin="IO_44" pad="A10"/>
<connect gate="B" pin="IO_45" pad="A11"/>
<connect gate="B" pin="IO_46" pad="A12"/>
<connect gate="B" pin="IO_47" pad="A13"/>
<connect gate="B" pin="IO_48" pad="A15"/>
<connect gate="B" pin="IO_49" pad="B10"/>
<connect gate="B" pin="IO_5" pad="M1"/>
<connect gate="B" pin="IO_50" pad="B11"/>
<connect gate="B" pin="IO_51" pad="B12"/>
<connect gate="B" pin="IO_52" pad="B13"/>
<connect gate="B" pin="IO_53" pad="B14"/>
<connect gate="B" pin="IO_54" pad="B16"/>
<connect gate="B" pin="IO_55" pad="C10"/>
<connect gate="B" pin="IO_56" pad="C11"/>
<connect gate="B" pin="IO_57" pad="C12"/>
<connect gate="B" pin="IO_58" pad="D11"/>
<connect gate="B" pin="IO_59" pad="C13"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_60" pad="D12"/>
<connect gate="B" pin="IO_61" pad="C14"/>
<connect gate="B" pin="IO_62" pad="D13"/>
<connect gate="B" pin="IO_63" pad="C15"/>
<connect gate="B" pin="IO_64" pad="D14"/>
<connect gate="B" pin="IO_65" pad="D15"/>
<connect gate="B" pin="IO_7" pad="L2"/>
<connect gate="B" pin="IO_8" pad="P4"/>
<connect gate="B" pin="IO_9" pad="P9"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCINT" pad="K6"/>
<connect gate="B" pin="VCCINT_2" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDINT_2" pad="K11"/>
<connect gate="C" pin="GNDINT_3" pad="L10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="E15"/>
<connect gate="C" pin="IO_11" pad="G15"/>
<connect gate="C" pin="IO_12" pad="H14"/>
<connect gate="C" pin="IO_13" pad="J15"/>
<connect gate="C" pin="IO_14" pad="K14"/>
<connect gate="C" pin="IO_15" pad="E16"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="G16"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="K16"/>
<connect gate="C" pin="IO_2" pad="F13"/>
<connect gate="C" pin="IO_20" pad="J14"/>
<connect gate="C" pin="IO_21" pad="K15"/>
<connect gate="C" pin="IO_22" pad="E10"/>
<connect gate="C" pin="IO_23" pad="H13"/>
<connect gate="C" pin="IO_24" pad="M10"/>
<connect gate="C" pin="IO_25" pad="E11"/>
<connect gate="C" pin="IO_26" pad="J13"/>
<connect gate="C" pin="IO_27" pad="M11"/>
<connect gate="C" pin="IO_28" pad="E12"/>
<connect gate="C" pin="IO_29" pad="G12"/>
<connect gate="C" pin="IO_3" pad="F14"/>
<connect gate="C" pin="IO_30" pad="N10"/>
<connect gate="C" pin="IO_31" pad="F11"/>
<connect gate="C" pin="IO_32" pad="G13"/>
<connect gate="C" pin="IO_33" pad="L11"/>
<connect gate="C" pin="IO_34" pad="L12"/>
<connect gate="C" pin="IO_35" pad="K12"/>
<connect gate="C" pin="IO_36" pad="M12"/>
<connect gate="C" pin="IO_37" pad="N11"/>
<connect gate="C" pin="IO_38" pad="F12"/>
<connect gate="C" pin="IO_39" pad="K13"/>
<connect gate="C" pin="IO_4" pad="E13"/>
<connect gate="C" pin="IO_40" pad="N12"/>
<connect gate="C" pin="IO_41" pad="L13"/>
<connect gate="C" pin="IO_42" pad="N13"/>
<connect gate="C" pin="IO_43" pad="L14"/>
<connect gate="C" pin="IO_44" pad="N14"/>
<connect gate="C" pin="IO_45" pad="L15"/>
<connect gate="C" pin="IO_46" pad="N15"/>
<connect gate="C" pin="IO_47" pad="L16"/>
<connect gate="C" pin="IO_48" pad="N16"/>
<connect gate="C" pin="IO_49" pad="P10"/>
<connect gate="C" pin="IO_5" pad="F15"/>
<connect gate="C" pin="IO_50" pad="P11"/>
<connect gate="C" pin="IO_51" pad="P12"/>
<connect gate="C" pin="IO_52" pad="M13"/>
<connect gate="C" pin="IO_53" pad="P13"/>
<connect gate="C" pin="IO_54" pad="M14"/>
<connect gate="C" pin="IO_55" pad="P14"/>
<connect gate="C" pin="IO_56" pad="M15"/>
<connect gate="C" pin="IO_57" pad="P15"/>
<connect gate="C" pin="IO_58" pad="M16"/>
<connect gate="C" pin="IO_59" pad="R10"/>
<connect gate="C" pin="IO_6" pad="H15"/>
<connect gate="C" pin="IO_60" pad="R11"/>
<connect gate="C" pin="IO_61" pad="R12"/>
<connect gate="C" pin="IO_62" pad="R13"/>
<connect gate="C" pin="IO_63" pad="R14"/>
<connect gate="C" pin="IO_64" pad="R16"/>
<connect gate="C" pin="IO_65" pad="T10"/>
<connect gate="C" pin="IO_66" pad="T11"/>
<connect gate="C" pin="IO_67" pad="T12"/>
<connect gate="C" pin="IO_68" pad="T13"/>
<connect gate="C" pin="IO_7" pad="E14"/>
<connect gate="C" pin="IO_8" pad="H16"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="VCCINT" pad="F10"/>
<connect gate="C" pin="VCCINT_2" pad="H10"/>
<connect gate="C" pin="VCCINT_3" pad="G11"/>
<connect gate="C" pin="VCCIO3" pad="J11"/>
<connect gate="C" pin="VCCIO3_2" pad="P16"/>
<connect gate="C" pin="VCCIO3_3" pad="H11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210F256I5N"/>
<attribute name="OC_FARNELL" value="1549482"/>
<attribute name="OC_NEWARK" value="51R9314"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210F324C3N">
<description>IC MAX II CPLD 2210 LE 324-FBGA</description>
<gates>
<gate name="A" symbol="EPM2210F324C3N_A"/>
<gate name="B" symbol="EPM2210F324C3N_B"/>
<gate name="C" symbol="EPM2210F324C3N_C"/>
<gate name="D" symbol="EPM2210F324C3N_D"/>
</gates>
<devices>
<device name="" package="BGA324N100P18X18_1900X1900X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="G8"/>
<connect gate="A" pin="GNDINT_3" pad="H7"/>
<connect gate="A" pin="GNDIO" pad="H9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="H8"/>
<connect gate="A" pin="IO" pad="J5"/>
<connect gate="A" pin="IO/GCLK0" pad="J6"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="F8"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="G3"/>
<connect gate="A" pin="IO_55" pad="G4"/>
<connect gate="A" pin="IO_56" pad="G5"/>
<connect gate="A" pin="IO_57" pad="G6"/>
<connect gate="A" pin="IO_58" pad="G7"/>
<connect gate="A" pin="IO_59" pad="H1"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="H2"/>
<connect gate="A" pin="IO_61" pad="H3"/>
<connect gate="A" pin="IO_62" pad="H4"/>
<connect gate="A" pin="IO_63" pad="H5"/>
<connect gate="A" pin="IO_64" pad="H6"/>
<connect gate="A" pin="IO_65" pad="J1"/>
<connect gate="A" pin="IO_66" pad="J2"/>
<connect gate="A" pin="IO_67" pad="J3"/>
<connect gate="A" pin="IO_68" pad="J4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="J7"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="G9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="B" pin="GNDINT" pad="K9"/>
<connect gate="B" pin="GNDIO" pad="V1"/>
<connect gate="B" pin="GNDIO_2" pad="L8"/>
<connect gate="B" pin="GNDIO_3" pad="L9"/>
<connect gate="B" pin="GNDIO_4" pad="U2"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO/DEV_OE" pad="N9"/>
<connect gate="B" pin="IO/GCLK1" pad="K6"/>
<connect gate="B" pin="IO_10" pad="L4"/>
<connect gate="B" pin="IO_11" pad="L5"/>
<connect gate="B" pin="IO_12" pad="L6"/>
<connect gate="B" pin="IO_13" pad="M1"/>
<connect gate="B" pin="IO_14" pad="M2"/>
<connect gate="B" pin="IO_15" pad="M3"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="M5"/>
<connect gate="B" pin="IO_18" pad="M6"/>
<connect gate="B" pin="IO_19" pad="N1"/>
<connect gate="B" pin="IO_2" pad="K1"/>
<connect gate="B" pin="IO_20" pad="N2"/>
<connect gate="B" pin="IO_21" pad="N3"/>
<connect gate="B" pin="IO_22" pad="N4"/>
<connect gate="B" pin="IO_23" pad="N5"/>
<connect gate="B" pin="IO_24" pad="N7"/>
<connect gate="B" pin="IO_25" pad="N8"/>
<connect gate="B" pin="IO_26" pad="P1"/>
<connect gate="B" pin="IO_27" pad="P2"/>
<connect gate="B" pin="IO_28" pad="P3"/>
<connect gate="B" pin="IO_29" pad="P4"/>
<connect gate="B" pin="IO_3" pad="K2"/>
<connect gate="B" pin="IO_30" pad="P6"/>
<connect gate="B" pin="IO_31" pad="P7"/>
<connect gate="B" pin="IO_32" pad="P8"/>
<connect gate="B" pin="IO_33" pad="P9"/>
<connect gate="B" pin="IO_34" pad="R1"/>
<connect gate="B" pin="IO_35" pad="R2"/>
<connect gate="B" pin="IO_36" pad="R3"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="K3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T3"/>
<connect gate="B" pin="IO_44" pad="T4"/>
<connect gate="B" pin="IO_45" pad="T5"/>
<connect gate="B" pin="IO_46" pad="T6"/>
<connect gate="B" pin="IO_47" pad="T7"/>
<connect gate="B" pin="IO_48" pad="T8"/>
<connect gate="B" pin="IO_49" pad="T9"/>
<connect gate="B" pin="IO_5" pad="K4"/>
<connect gate="B" pin="IO_50" pad="U1"/>
<connect gate="B" pin="IO_51" pad="U3"/>
<connect gate="B" pin="IO_52" pad="U4"/>
<connect gate="B" pin="IO_53" pad="U5"/>
<connect gate="B" pin="IO_54" pad="U6"/>
<connect gate="B" pin="IO_55" pad="U7"/>
<connect gate="B" pin="IO_56" pad="U8"/>
<connect gate="B" pin="IO_57" pad="U9"/>
<connect gate="B" pin="IO_58" pad="V2"/>
<connect gate="B" pin="IO_59" pad="V4"/>
<connect gate="B" pin="IO_6" pad="K5"/>
<connect gate="B" pin="IO_60" pad="V5"/>
<connect gate="B" pin="IO_61" pad="V6"/>
<connect gate="B" pin="IO_62" pad="V7"/>
<connect gate="B" pin="IO_63" pad="V8"/>
<connect gate="B" pin="IO_7" pad="L1"/>
<connect gate="B" pin="IO_8" pad="L2"/>
<connect gate="B" pin="IO_9" pad="L3"/>
<connect gate="B" pin="TCK" pad="R4"/>
<connect gate="B" pin="TDI" pad="M7"/>
<connect gate="B" pin="TDO" pad="N6"/>
<connect gate="B" pin="TMS" pad="P5"/>
<connect gate="B" pin="VCCINT" pad="M8"/>
<connect gate="B" pin="VCCINT_2" pad="K8"/>
<connect gate="B" pin="VCCINT_3" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="T1"/>
<connect gate="B" pin="VCCIO1_2" pad="K7"/>
<connect gate="B" pin="VCCIO4" pad="V3"/>
<connect gate="B" pin="VCCIO4_2" pad="M9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="H11"/>
<connect gate="C" pin="GNDIO_2" pad="A18"/>
<connect gate="C" pin="GNDIO_3" pad="B17"/>
<connect gate="C" pin="GNDIO_4" pad="H10"/>
<connect gate="C" pin="IO" pad="J18"/>
<connect gate="C" pin="IO/GCLK3" pad="J13"/>
<connect gate="C" pin="IO_10" pad="B11"/>
<connect gate="C" pin="IO_11" pad="B12"/>
<connect gate="C" pin="IO_12" pad="B13"/>
<connect gate="C" pin="IO_13" pad="B14"/>
<connect gate="C" pin="IO_14" pad="B15"/>
<connect gate="C" pin="IO_15" pad="B16"/>
<connect gate="C" pin="IO_16" pad="B18"/>
<connect gate="C" pin="IO_17" pad="C10"/>
<connect gate="C" pin="IO_18" pad="C11"/>
<connect gate="C" pin="IO_19" pad="C12"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C13"/>
<connect gate="C" pin="IO_21" pad="C14"/>
<connect gate="C" pin="IO_22" pad="C15"/>
<connect gate="C" pin="IO_23" pad="C16"/>
<connect gate="C" pin="IO_24" pad="C17"/>
<connect gate="C" pin="IO_25" pad="D10"/>
<connect gate="C" pin="IO_26" pad="D11"/>
<connect gate="C" pin="IO_27" pad="D12"/>
<connect gate="C" pin="IO_28" pad="D13"/>
<connect gate="C" pin="IO_29" pad="D14"/>
<connect gate="C" pin="IO_3" pad="A11"/>
<connect gate="C" pin="IO_30" pad="D15"/>
<connect gate="C" pin="IO_31" pad="D16"/>
<connect gate="C" pin="IO_32" pad="D17"/>
<connect gate="C" pin="IO_33" pad="D18"/>
<connect gate="C" pin="IO_34" pad="E10"/>
<connect gate="C" pin="IO_35" pad="E11"/>
<connect gate="C" pin="IO_36" pad="E12"/>
<connect gate="C" pin="IO_37" pad="E13"/>
<connect gate="C" pin="IO_38" pad="E14"/>
<connect gate="C" pin="IO_39" pad="E15"/>
<connect gate="C" pin="IO_4" pad="A12"/>
<connect gate="C" pin="IO_40" pad="E16"/>
<connect gate="C" pin="IO_41" pad="E17"/>
<connect gate="C" pin="IO_42" pad="E18"/>
<connect gate="C" pin="IO_43" pad="F10"/>
<connect gate="C" pin="IO_44" pad="F11"/>
<connect gate="C" pin="IO_45" pad="F12"/>
<connect gate="C" pin="IO_46" pad="F13"/>
<connect gate="C" pin="IO_47" pad="F14"/>
<connect gate="C" pin="IO_48" pad="F15"/>
<connect gate="C" pin="IO_49" pad="F16"/>
<connect gate="C" pin="IO_5" pad="A13"/>
<connect gate="C" pin="IO_50" pad="F17"/>
<connect gate="C" pin="IO_51" pad="F18"/>
<connect gate="C" pin="IO_52" pad="G12"/>
<connect gate="C" pin="IO_53" pad="G13"/>
<connect gate="C" pin="IO_54" pad="G14"/>
<connect gate="C" pin="IO_55" pad="G15"/>
<connect gate="C" pin="IO_56" pad="G16"/>
<connect gate="C" pin="IO_57" pad="G17"/>
<connect gate="C" pin="IO_58" pad="G18"/>
<connect gate="C" pin="IO_59" pad="H13"/>
<connect gate="C" pin="IO_6" pad="A14"/>
<connect gate="C" pin="IO_60" pad="H14"/>
<connect gate="C" pin="IO_61" pad="H15"/>
<connect gate="C" pin="IO_62" pad="H16"/>
<connect gate="C" pin="IO_63" pad="H17"/>
<connect gate="C" pin="IO_64" pad="H18"/>
<connect gate="C" pin="IO_65" pad="J14"/>
<connect gate="C" pin="IO_66" pad="J15"/>
<connect gate="C" pin="IO_67" pad="J16"/>
<connect gate="C" pin="IO_68" pad="J17"/>
<connect gate="C" pin="IO_7" pad="A15"/>
<connect gate="C" pin="IO_8" pad="A17"/>
<connect gate="C" pin="IO_9" pad="B10"/>
<connect gate="C" pin="VCCINT" pad="J11"/>
<connect gate="C" pin="VCCINT_2" pad="G11"/>
<connect gate="C" pin="VCCINT_3" pad="H12"/>
<connect gate="C" pin="VCCIO2" pad="G10"/>
<connect gate="C" pin="VCCIO2_2" pad="A16"/>
<connect gate="C" pin="VCCIO3" pad="J12"/>
<connect gate="C" pin="VCCIO3_2" pad="C18"/>
<connect gate="D" pin="GNDINT" pad="M11"/>
<connect gate="D" pin="GNDINT_2" pad="K11"/>
<connect gate="D" pin="GNDINT_3" pad="L12"/>
<connect gate="D" pin="GNDIO" pad="V18"/>
<connect gate="D" pin="GNDIO_2" pad="L10"/>
<connect gate="D" pin="GNDIO_3" pad="L11"/>
<connect gate="D" pin="GNDIO_4" pad="U17"/>
<connect gate="D" pin="IO" pad="V17"/>
<connect gate="D" pin="IO/*DEV_CLR" pad="N10"/>
<connect gate="D" pin="IO/GCLK2" pad="K13"/>
<connect gate="D" pin="IO_10" pad="L16"/>
<connect gate="D" pin="IO_11" pad="L17"/>
<connect gate="D" pin="IO_12" pad="L18"/>
<connect gate="D" pin="IO_13" pad="M12"/>
<connect gate="D" pin="IO_14" pad="M13"/>
<connect gate="D" pin="IO_15" pad="M14"/>
<connect gate="D" pin="IO_16" pad="M15"/>
<connect gate="D" pin="IO_17" pad="M16"/>
<connect gate="D" pin="IO_18" pad="M17"/>
<connect gate="D" pin="IO_19" pad="M18"/>
<connect gate="D" pin="IO_2" pad="K14"/>
<connect gate="D" pin="IO_20" pad="N11"/>
<connect gate="D" pin="IO_21" pad="N12"/>
<connect gate="D" pin="IO_22" pad="N13"/>
<connect gate="D" pin="IO_23" pad="N14"/>
<connect gate="D" pin="IO_24" pad="N15"/>
<connect gate="D" pin="IO_25" pad="N16"/>
<connect gate="D" pin="IO_26" pad="N17"/>
<connect gate="D" pin="IO_27" pad="N18"/>
<connect gate="D" pin="IO_28" pad="P10"/>
<connect gate="D" pin="IO_29" pad="P11"/>
<connect gate="D" pin="IO_3" pad="K15"/>
<connect gate="D" pin="IO_30" pad="P12"/>
<connect gate="D" pin="IO_31" pad="P13"/>
<connect gate="D" pin="IO_32" pad="P14"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="R10"/>
<connect gate="D" pin="IO_38" pad="R11"/>
<connect gate="D" pin="IO_39" pad="R12"/>
<connect gate="D" pin="IO_4" pad="K16"/>
<connect gate="D" pin="IO_40" pad="R13"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_44" pad="R17"/>
<connect gate="D" pin="IO_45" pad="R18"/>
<connect gate="D" pin="IO_46" pad="T10"/>
<connect gate="D" pin="IO_47" pad="T11"/>
<connect gate="D" pin="IO_48" pad="T12"/>
<connect gate="D" pin="IO_49" pad="T13"/>
<connect gate="D" pin="IO_5" pad="K17"/>
<connect gate="D" pin="IO_50" pad="T14"/>
<connect gate="D" pin="IO_51" pad="T15"/>
<connect gate="D" pin="IO_52" pad="T16"/>
<connect gate="D" pin="IO_53" pad="T17"/>
<connect gate="D" pin="IO_54" pad="U10"/>
<connect gate="D" pin="IO_55" pad="U11"/>
<connect gate="D" pin="IO_56" pad="U12"/>
<connect gate="D" pin="IO_57" pad="U13"/>
<connect gate="D" pin="IO_58" pad="U14"/>
<connect gate="D" pin="IO_59" pad="U15"/>
<connect gate="D" pin="IO_6" pad="K18"/>
<connect gate="D" pin="IO_60" pad="U16"/>
<connect gate="D" pin="IO_61" pad="U18"/>
<connect gate="D" pin="IO_62" pad="V10"/>
<connect gate="D" pin="IO_63" pad="V11"/>
<connect gate="D" pin="IO_64" pad="V12"/>
<connect gate="D" pin="IO_65" pad="V13"/>
<connect gate="D" pin="IO_66" pad="V14"/>
<connect gate="D" pin="IO_67" pad="V15"/>
<connect gate="D" pin="IO_7" pad="L13"/>
<connect gate="D" pin="IO_8" pad="L14"/>
<connect gate="D" pin="IO_9" pad="L15"/>
<connect gate="D" pin="VCCINT" pad="K10"/>
<connect gate="D" pin="VCCIO3" pad="T18"/>
<connect gate="D" pin="VCCIO3_2" pad="K12"/>
<connect gate="D" pin="VCCIO4" pad="V16"/>
<connect gate="D" pin="VCCIO4_2" pad="M10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210F324C3N"/>
<attribute name="OC_FARNELL" value="1872690"/>
<attribute name="OC_NEWARK" value="51R9317"/>
<attribute name="PACKAGE" value="324-FBGA"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210F324C4N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM2210F324C4N_A"/>
<gate name="B" symbol="EPM2210F324C4N_B"/>
<gate name="C" symbol="EPM2210F324C4N_C"/>
<gate name="D" symbol="EPM2210F324C4N_D"/>
</gates>
<devices>
<device name="" package="BGA324C100P18X18_1900X1900X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="H7"/>
<connect gate="A" pin="GNDINT_3" pad="G8"/>
<connect gate="A" pin="GNDIO" pad="H9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="H8"/>
<connect gate="A" pin="GNDIO_4" pad="B2"/>
<connect gate="A" pin="IO" pad="J5"/>
<connect gate="A" pin="IO/GCLK0" pad="J6"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="F8"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="G3"/>
<connect gate="A" pin="IO_55" pad="G4"/>
<connect gate="A" pin="IO_56" pad="G5"/>
<connect gate="A" pin="IO_57" pad="G6"/>
<connect gate="A" pin="IO_58" pad="G7"/>
<connect gate="A" pin="IO_59" pad="H1"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="H2"/>
<connect gate="A" pin="IO_61" pad="H3"/>
<connect gate="A" pin="IO_62" pad="H4"/>
<connect gate="A" pin="IO_63" pad="H5"/>
<connect gate="A" pin="IO_64" pad="H6"/>
<connect gate="A" pin="IO_65" pad="J1"/>
<connect gate="A" pin="IO_66" pad="J2"/>
<connect gate="A" pin="IO_67" pad="J3"/>
<connect gate="A" pin="IO_68" pad="J4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="J7"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="A3"/>
<connect gate="A" pin="VCCIO2_2" pad="G9"/>
<connect gate="B" pin="GNDINT" pad="K9"/>
<connect gate="B" pin="GNDIO" pad="V1"/>
<connect gate="B" pin="GNDIO_2" pad="L8"/>
<connect gate="B" pin="GNDIO_3" pad="L9"/>
<connect gate="B" pin="GNDIO_4" pad="U2"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO/DEV_OE" pad="N9"/>
<connect gate="B" pin="IO/GCLK1" pad="K6"/>
<connect gate="B" pin="IO_10" pad="L4"/>
<connect gate="B" pin="IO_11" pad="L5"/>
<connect gate="B" pin="IO_12" pad="L6"/>
<connect gate="B" pin="IO_13" pad="M1"/>
<connect gate="B" pin="IO_14" pad="M2"/>
<connect gate="B" pin="IO_15" pad="M3"/>
<connect gate="B" pin="IO_16" pad="N1"/>
<connect gate="B" pin="IO_17" pad="M4"/>
<connect gate="B" pin="IO_18" pad="N2"/>
<connect gate="B" pin="IO_19" pad="M5"/>
<connect gate="B" pin="IO_2" pad="K1"/>
<connect gate="B" pin="IO_20" pad="N3"/>
<connect gate="B" pin="IO_21" pad="M6"/>
<connect gate="B" pin="IO_22" pad="N4"/>
<connect gate="B" pin="IO_23" pad="N5"/>
<connect gate="B" pin="IO_24" pad="N7"/>
<connect gate="B" pin="IO_25" pad="N8"/>
<connect gate="B" pin="IO_26" pad="P2"/>
<connect gate="B" pin="IO_27" pad="P1"/>
<connect gate="B" pin="IO_28" pad="P3"/>
<connect gate="B" pin="IO_29" pad="P4"/>
<connect gate="B" pin="IO_3" pad="K2"/>
<connect gate="B" pin="IO_30" pad="P6"/>
<connect gate="B" pin="IO_31" pad="P7"/>
<connect gate="B" pin="IO_32" pad="P8"/>
<connect gate="B" pin="IO_33" pad="P9"/>
<connect gate="B" pin="IO_34" pad="R1"/>
<connect gate="B" pin="IO_35" pad="R2"/>
<connect gate="B" pin="IO_36" pad="R3"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="K3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T3"/>
<connect gate="B" pin="IO_44" pad="T4"/>
<connect gate="B" pin="IO_45" pad="T5"/>
<connect gate="B" pin="IO_46" pad="T6"/>
<connect gate="B" pin="IO_47" pad="T7"/>
<connect gate="B" pin="IO_48" pad="T8"/>
<connect gate="B" pin="IO_49" pad="T9"/>
<connect gate="B" pin="IO_5" pad="K4"/>
<connect gate="B" pin="IO_50" pad="U1"/>
<connect gate="B" pin="IO_51" pad="U3"/>
<connect gate="B" pin="IO_52" pad="U4"/>
<connect gate="B" pin="IO_53" pad="U5"/>
<connect gate="B" pin="IO_54" pad="U6"/>
<connect gate="B" pin="IO_55" pad="U7"/>
<connect gate="B" pin="IO_56" pad="U8"/>
<connect gate="B" pin="IO_57" pad="U9"/>
<connect gate="B" pin="IO_58" pad="V2"/>
<connect gate="B" pin="IO_59" pad="V4"/>
<connect gate="B" pin="IO_6" pad="K5"/>
<connect gate="B" pin="IO_60" pad="V5"/>
<connect gate="B" pin="IO_61" pad="V6"/>
<connect gate="B" pin="IO_62" pad="V7"/>
<connect gate="B" pin="IO_63" pad="V8"/>
<connect gate="B" pin="IO_7" pad="L1"/>
<connect gate="B" pin="IO_8" pad="L2"/>
<connect gate="B" pin="IO_9" pad="L3"/>
<connect gate="B" pin="TCK" pad="R4"/>
<connect gate="B" pin="TDI" pad="M7"/>
<connect gate="B" pin="TDO" pad="N6"/>
<connect gate="B" pin="TMS" pad="P5"/>
<connect gate="B" pin="VCCINT" pad="M8"/>
<connect gate="B" pin="VCCINT_2" pad="K8"/>
<connect gate="B" pin="VCCINT_3" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="K7"/>
<connect gate="B" pin="VCCIO1_2" pad="T1"/>
<connect gate="B" pin="VCCIO4" pad="V3"/>
<connect gate="B" pin="VCCIO4_2" pad="M9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="H11"/>
<connect gate="C" pin="GNDIO_2" pad="A18"/>
<connect gate="C" pin="GNDIO_3" pad="B17"/>
<connect gate="C" pin="GNDIO_4" pad="H10"/>
<connect gate="C" pin="IO" pad="J18"/>
<connect gate="C" pin="IO/GCLK3" pad="J13"/>
<connect gate="C" pin="IO_10" pad="B11"/>
<connect gate="C" pin="IO_11" pad="B12"/>
<connect gate="C" pin="IO_12" pad="B13"/>
<connect gate="C" pin="IO_13" pad="B14"/>
<connect gate="C" pin="IO_14" pad="B15"/>
<connect gate="C" pin="IO_15" pad="B16"/>
<connect gate="C" pin="IO_16" pad="B18"/>
<connect gate="C" pin="IO_17" pad="C10"/>
<connect gate="C" pin="IO_18" pad="C11"/>
<connect gate="C" pin="IO_19" pad="C12"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C13"/>
<connect gate="C" pin="IO_21" pad="C14"/>
<connect gate="C" pin="IO_22" pad="C15"/>
<connect gate="C" pin="IO_23" pad="C16"/>
<connect gate="C" pin="IO_24" pad="C17"/>
<connect gate="C" pin="IO_25" pad="D10"/>
<connect gate="C" pin="IO_26" pad="D11"/>
<connect gate="C" pin="IO_27" pad="D12"/>
<connect gate="C" pin="IO_28" pad="D13"/>
<connect gate="C" pin="IO_29" pad="D14"/>
<connect gate="C" pin="IO_3" pad="A11"/>
<connect gate="C" pin="IO_30" pad="D15"/>
<connect gate="C" pin="IO_31" pad="D16"/>
<connect gate="C" pin="IO_32" pad="D17"/>
<connect gate="C" pin="IO_33" pad="D18"/>
<connect gate="C" pin="IO_34" pad="E10"/>
<connect gate="C" pin="IO_35" pad="E11"/>
<connect gate="C" pin="IO_36" pad="E12"/>
<connect gate="C" pin="IO_37" pad="E13"/>
<connect gate="C" pin="IO_38" pad="E14"/>
<connect gate="C" pin="IO_39" pad="E15"/>
<connect gate="C" pin="IO_4" pad="A12"/>
<connect gate="C" pin="IO_40" pad="E16"/>
<connect gate="C" pin="IO_41" pad="E17"/>
<connect gate="C" pin="IO_42" pad="E18"/>
<connect gate="C" pin="IO_43" pad="F10"/>
<connect gate="C" pin="IO_44" pad="F11"/>
<connect gate="C" pin="IO_45" pad="F12"/>
<connect gate="C" pin="IO_46" pad="F13"/>
<connect gate="C" pin="IO_47" pad="F14"/>
<connect gate="C" pin="IO_48" pad="F15"/>
<connect gate="C" pin="IO_49" pad="F16"/>
<connect gate="C" pin="IO_5" pad="A13"/>
<connect gate="C" pin="IO_50" pad="F17"/>
<connect gate="C" pin="IO_51" pad="F18"/>
<connect gate="C" pin="IO_52" pad="G12"/>
<connect gate="C" pin="IO_53" pad="G13"/>
<connect gate="C" pin="IO_54" pad="G14"/>
<connect gate="C" pin="IO_55" pad="G15"/>
<connect gate="C" pin="IO_56" pad="G16"/>
<connect gate="C" pin="IO_57" pad="G17"/>
<connect gate="C" pin="IO_58" pad="G18"/>
<connect gate="C" pin="IO_59" pad="H13"/>
<connect gate="C" pin="IO_6" pad="A14"/>
<connect gate="C" pin="IO_60" pad="H14"/>
<connect gate="C" pin="IO_61" pad="H15"/>
<connect gate="C" pin="IO_62" pad="H16"/>
<connect gate="C" pin="IO_63" pad="H17"/>
<connect gate="C" pin="IO_64" pad="H18"/>
<connect gate="C" pin="IO_65" pad="J14"/>
<connect gate="C" pin="IO_66" pad="J15"/>
<connect gate="C" pin="IO_67" pad="J16"/>
<connect gate="C" pin="IO_68" pad="J17"/>
<connect gate="C" pin="IO_7" pad="A15"/>
<connect gate="C" pin="IO_8" pad="B10"/>
<connect gate="C" pin="IO_9" pad="A17"/>
<connect gate="C" pin="VCCINT" pad="G11"/>
<connect gate="C" pin="VCCINT_2" pad="H12"/>
<connect gate="C" pin="VCCINT_3" pad="J11"/>
<connect gate="C" pin="VCCIO2" pad="G10"/>
<connect gate="C" pin="VCCIO2_2" pad="A16"/>
<connect gate="C" pin="VCCIO3" pad="J12"/>
<connect gate="C" pin="VCCIO3_2" pad="C18"/>
<connect gate="D" pin="GNDINT" pad="M11"/>
<connect gate="D" pin="GNDINT_2" pad="K11"/>
<connect gate="D" pin="GNDINT_3" pad="L12"/>
<connect gate="D" pin="GNDIO" pad="V18"/>
<connect gate="D" pin="GNDIO_2" pad="L10"/>
<connect gate="D" pin="GNDIO_3" pad="U17"/>
<connect gate="D" pin="GNDIO_4" pad="L11"/>
<connect gate="D" pin="IO" pad="V17"/>
<connect gate="D" pin="IO/DEV_CLRN" pad="N10"/>
<connect gate="D" pin="IO/GCLK2" pad="K13"/>
<connect gate="D" pin="IO_10" pad="L16"/>
<connect gate="D" pin="IO_11" pad="L17"/>
<connect gate="D" pin="IO_12" pad="L18"/>
<connect gate="D" pin="IO_13" pad="M12"/>
<connect gate="D" pin="IO_14" pad="M13"/>
<connect gate="D" pin="IO_15" pad="M14"/>
<connect gate="D" pin="IO_16" pad="M15"/>
<connect gate="D" pin="IO_17" pad="M16"/>
<connect gate="D" pin="IO_18" pad="N11"/>
<connect gate="D" pin="IO_19" pad="M17"/>
<connect gate="D" pin="IO_2" pad="K14"/>
<connect gate="D" pin="IO_20" pad="N12"/>
<connect gate="D" pin="IO_21" pad="M18"/>
<connect gate="D" pin="IO_22" pad="N13"/>
<connect gate="D" pin="IO_23" pad="N14"/>
<connect gate="D" pin="IO_24" pad="N15"/>
<connect gate="D" pin="IO_25" pad="N16"/>
<connect gate="D" pin="IO_26" pad="N17"/>
<connect gate="D" pin="IO_27" pad="N18"/>
<connect gate="D" pin="IO_28" pad="P10"/>
<connect gate="D" pin="IO_29" pad="P11"/>
<connect gate="D" pin="IO_3" pad="K15"/>
<connect gate="D" pin="IO_30" pad="P12"/>
<connect gate="D" pin="IO_31" pad="P13"/>
<connect gate="D" pin="IO_32" pad="P14"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="R10"/>
<connect gate="D" pin="IO_38" pad="R11"/>
<connect gate="D" pin="IO_39" pad="R12"/>
<connect gate="D" pin="IO_4" pad="K16"/>
<connect gate="D" pin="IO_40" pad="R13"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_44" pad="R17"/>
<connect gate="D" pin="IO_45" pad="R18"/>
<connect gate="D" pin="IO_46" pad="T10"/>
<connect gate="D" pin="IO_47" pad="T11"/>
<connect gate="D" pin="IO_48" pad="T12"/>
<connect gate="D" pin="IO_49" pad="T13"/>
<connect gate="D" pin="IO_5" pad="K17"/>
<connect gate="D" pin="IO_50" pad="T14"/>
<connect gate="D" pin="IO_51" pad="T15"/>
<connect gate="D" pin="IO_52" pad="T16"/>
<connect gate="D" pin="IO_53" pad="T17"/>
<connect gate="D" pin="IO_54" pad="U10"/>
<connect gate="D" pin="IO_55" pad="U11"/>
<connect gate="D" pin="IO_56" pad="U12"/>
<connect gate="D" pin="IO_57" pad="U13"/>
<connect gate="D" pin="IO_58" pad="U14"/>
<connect gate="D" pin="IO_59" pad="U15"/>
<connect gate="D" pin="IO_6" pad="K18"/>
<connect gate="D" pin="IO_60" pad="U16"/>
<connect gate="D" pin="IO_61" pad="U18"/>
<connect gate="D" pin="IO_62" pad="V10"/>
<connect gate="D" pin="IO_63" pad="V11"/>
<connect gate="D" pin="IO_64" pad="V12"/>
<connect gate="D" pin="IO_65" pad="V13"/>
<connect gate="D" pin="IO_66" pad="V14"/>
<connect gate="D" pin="IO_67" pad="V15"/>
<connect gate="D" pin="IO_7" pad="L13"/>
<connect gate="D" pin="IO_8" pad="L14"/>
<connect gate="D" pin="IO_9" pad="L15"/>
<connect gate="D" pin="VCCINT" pad="K10"/>
<connect gate="D" pin="VCCIO3" pad="K12"/>
<connect gate="D" pin="VCCIO3_2" pad="T18"/>
<connect gate="D" pin="VCCIO4" pad="M10"/>
<connect gate="D" pin="VCCIO4_2" pad="V16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210F324C4N"/>
<attribute name="OC_FARNELL" value="1742177"/>
<attribute name="OC_NEWARK" value="51R0490"/>
<attribute name="PACKAGE" value="BGA-324"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210F324C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM2210F324C5N_A"/>
<gate name="B" symbol="EPM2210F324C5N_B"/>
<gate name="C" symbol="EPM2210F324C5N_C"/>
<gate name="D" symbol="EPM2210F324C5N_D"/>
</gates>
<devices>
<device name="" package="BGA324C100P18X18_1900X1900X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="H7"/>
<connect gate="A" pin="GNDINT_3" pad="G8"/>
<connect gate="A" pin="GNDIO" pad="H9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="H8"/>
<connect gate="A" pin="GNDIO_4" pad="B2"/>
<connect gate="A" pin="IO" pad="J5"/>
<connect gate="A" pin="IO/GCLK0" pad="J6"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="F8"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="G3"/>
<connect gate="A" pin="IO_55" pad="G4"/>
<connect gate="A" pin="IO_56" pad="G5"/>
<connect gate="A" pin="IO_57" pad="G6"/>
<connect gate="A" pin="IO_58" pad="G7"/>
<connect gate="A" pin="IO_59" pad="H1"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="H2"/>
<connect gate="A" pin="IO_61" pad="H3"/>
<connect gate="A" pin="IO_62" pad="H4"/>
<connect gate="A" pin="IO_63" pad="H5"/>
<connect gate="A" pin="IO_64" pad="H6"/>
<connect gate="A" pin="IO_65" pad="J1"/>
<connect gate="A" pin="IO_66" pad="J2"/>
<connect gate="A" pin="IO_67" pad="J3"/>
<connect gate="A" pin="IO_68" pad="J4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="J7"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="A3"/>
<connect gate="A" pin="VCCIO2_2" pad="G9"/>
<connect gate="B" pin="GNDINT" pad="K9"/>
<connect gate="B" pin="GNDIO" pad="V1"/>
<connect gate="B" pin="GNDIO_2" pad="L8"/>
<connect gate="B" pin="GNDIO_3" pad="L9"/>
<connect gate="B" pin="GNDIO_4" pad="U2"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO/DEV_OE" pad="N9"/>
<connect gate="B" pin="IO/GCLK1" pad="K6"/>
<connect gate="B" pin="IO_10" pad="L4"/>
<connect gate="B" pin="IO_11" pad="L5"/>
<connect gate="B" pin="IO_12" pad="L6"/>
<connect gate="B" pin="IO_13" pad="M1"/>
<connect gate="B" pin="IO_14" pad="M2"/>
<connect gate="B" pin="IO_15" pad="M3"/>
<connect gate="B" pin="IO_16" pad="N1"/>
<connect gate="B" pin="IO_17" pad="M4"/>
<connect gate="B" pin="IO_18" pad="N2"/>
<connect gate="B" pin="IO_19" pad="M5"/>
<connect gate="B" pin="IO_2" pad="K1"/>
<connect gate="B" pin="IO_20" pad="N3"/>
<connect gate="B" pin="IO_21" pad="M6"/>
<connect gate="B" pin="IO_22" pad="N4"/>
<connect gate="B" pin="IO_23" pad="N5"/>
<connect gate="B" pin="IO_24" pad="N7"/>
<connect gate="B" pin="IO_25" pad="N8"/>
<connect gate="B" pin="IO_26" pad="P2"/>
<connect gate="B" pin="IO_27" pad="P1"/>
<connect gate="B" pin="IO_28" pad="P3"/>
<connect gate="B" pin="IO_29" pad="P4"/>
<connect gate="B" pin="IO_3" pad="K2"/>
<connect gate="B" pin="IO_30" pad="P6"/>
<connect gate="B" pin="IO_31" pad="P7"/>
<connect gate="B" pin="IO_32" pad="P8"/>
<connect gate="B" pin="IO_33" pad="P9"/>
<connect gate="B" pin="IO_34" pad="R1"/>
<connect gate="B" pin="IO_35" pad="R2"/>
<connect gate="B" pin="IO_36" pad="R3"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="K3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T3"/>
<connect gate="B" pin="IO_44" pad="T4"/>
<connect gate="B" pin="IO_45" pad="T5"/>
<connect gate="B" pin="IO_46" pad="T6"/>
<connect gate="B" pin="IO_47" pad="T7"/>
<connect gate="B" pin="IO_48" pad="T8"/>
<connect gate="B" pin="IO_49" pad="T9"/>
<connect gate="B" pin="IO_5" pad="K4"/>
<connect gate="B" pin="IO_50" pad="U1"/>
<connect gate="B" pin="IO_51" pad="U3"/>
<connect gate="B" pin="IO_52" pad="U4"/>
<connect gate="B" pin="IO_53" pad="U5"/>
<connect gate="B" pin="IO_54" pad="U6"/>
<connect gate="B" pin="IO_55" pad="U7"/>
<connect gate="B" pin="IO_56" pad="U8"/>
<connect gate="B" pin="IO_57" pad="U9"/>
<connect gate="B" pin="IO_58" pad="V2"/>
<connect gate="B" pin="IO_59" pad="V4"/>
<connect gate="B" pin="IO_6" pad="K5"/>
<connect gate="B" pin="IO_60" pad="V5"/>
<connect gate="B" pin="IO_61" pad="V6"/>
<connect gate="B" pin="IO_62" pad="V7"/>
<connect gate="B" pin="IO_63" pad="V8"/>
<connect gate="B" pin="IO_7" pad="L1"/>
<connect gate="B" pin="IO_8" pad="L2"/>
<connect gate="B" pin="IO_9" pad="L3"/>
<connect gate="B" pin="TCK" pad="R4"/>
<connect gate="B" pin="TDI" pad="M7"/>
<connect gate="B" pin="TDO" pad="N6"/>
<connect gate="B" pin="TMS" pad="P5"/>
<connect gate="B" pin="VCCINT" pad="M8"/>
<connect gate="B" pin="VCCINT_2" pad="K8"/>
<connect gate="B" pin="VCCINT_3" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="K7"/>
<connect gate="B" pin="VCCIO1_2" pad="T1"/>
<connect gate="B" pin="VCCIO4" pad="V3"/>
<connect gate="B" pin="VCCIO4_2" pad="M9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="H11"/>
<connect gate="C" pin="GNDIO_2" pad="A18"/>
<connect gate="C" pin="GNDIO_3" pad="B17"/>
<connect gate="C" pin="GNDIO_4" pad="H10"/>
<connect gate="C" pin="IO" pad="J18"/>
<connect gate="C" pin="IO/GCLK3" pad="J13"/>
<connect gate="C" pin="IO_10" pad="B11"/>
<connect gate="C" pin="IO_11" pad="B12"/>
<connect gate="C" pin="IO_12" pad="B13"/>
<connect gate="C" pin="IO_13" pad="B14"/>
<connect gate="C" pin="IO_14" pad="B15"/>
<connect gate="C" pin="IO_15" pad="B16"/>
<connect gate="C" pin="IO_16" pad="B18"/>
<connect gate="C" pin="IO_17" pad="C10"/>
<connect gate="C" pin="IO_18" pad="C11"/>
<connect gate="C" pin="IO_19" pad="C12"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C13"/>
<connect gate="C" pin="IO_21" pad="C14"/>
<connect gate="C" pin="IO_22" pad="C15"/>
<connect gate="C" pin="IO_23" pad="C16"/>
<connect gate="C" pin="IO_24" pad="C17"/>
<connect gate="C" pin="IO_25" pad="D10"/>
<connect gate="C" pin="IO_26" pad="D11"/>
<connect gate="C" pin="IO_27" pad="D12"/>
<connect gate="C" pin="IO_28" pad="D13"/>
<connect gate="C" pin="IO_29" pad="D14"/>
<connect gate="C" pin="IO_3" pad="A11"/>
<connect gate="C" pin="IO_30" pad="D15"/>
<connect gate="C" pin="IO_31" pad="D16"/>
<connect gate="C" pin="IO_32" pad="D17"/>
<connect gate="C" pin="IO_33" pad="D18"/>
<connect gate="C" pin="IO_34" pad="E10"/>
<connect gate="C" pin="IO_35" pad="E11"/>
<connect gate="C" pin="IO_36" pad="E12"/>
<connect gate="C" pin="IO_37" pad="E13"/>
<connect gate="C" pin="IO_38" pad="E14"/>
<connect gate="C" pin="IO_39" pad="E15"/>
<connect gate="C" pin="IO_4" pad="A12"/>
<connect gate="C" pin="IO_40" pad="E16"/>
<connect gate="C" pin="IO_41" pad="E17"/>
<connect gate="C" pin="IO_42" pad="E18"/>
<connect gate="C" pin="IO_43" pad="F10"/>
<connect gate="C" pin="IO_44" pad="F11"/>
<connect gate="C" pin="IO_45" pad="F12"/>
<connect gate="C" pin="IO_46" pad="F13"/>
<connect gate="C" pin="IO_47" pad="F14"/>
<connect gate="C" pin="IO_48" pad="F15"/>
<connect gate="C" pin="IO_49" pad="F16"/>
<connect gate="C" pin="IO_5" pad="A13"/>
<connect gate="C" pin="IO_50" pad="F17"/>
<connect gate="C" pin="IO_51" pad="F18"/>
<connect gate="C" pin="IO_52" pad="G12"/>
<connect gate="C" pin="IO_53" pad="G13"/>
<connect gate="C" pin="IO_54" pad="G14"/>
<connect gate="C" pin="IO_55" pad="G15"/>
<connect gate="C" pin="IO_56" pad="G16"/>
<connect gate="C" pin="IO_57" pad="G17"/>
<connect gate="C" pin="IO_58" pad="G18"/>
<connect gate="C" pin="IO_59" pad="H13"/>
<connect gate="C" pin="IO_6" pad="A14"/>
<connect gate="C" pin="IO_60" pad="H14"/>
<connect gate="C" pin="IO_61" pad="H15"/>
<connect gate="C" pin="IO_62" pad="H16"/>
<connect gate="C" pin="IO_63" pad="H17"/>
<connect gate="C" pin="IO_64" pad="H18"/>
<connect gate="C" pin="IO_65" pad="J14"/>
<connect gate="C" pin="IO_66" pad="J15"/>
<connect gate="C" pin="IO_67" pad="J16"/>
<connect gate="C" pin="IO_68" pad="J17"/>
<connect gate="C" pin="IO_7" pad="A15"/>
<connect gate="C" pin="IO_8" pad="B10"/>
<connect gate="C" pin="IO_9" pad="A17"/>
<connect gate="C" pin="VCCINT" pad="G11"/>
<connect gate="C" pin="VCCINT_2" pad="H12"/>
<connect gate="C" pin="VCCINT_3" pad="J11"/>
<connect gate="C" pin="VCCIO2" pad="G10"/>
<connect gate="C" pin="VCCIO2_2" pad="A16"/>
<connect gate="C" pin="VCCIO3" pad="J12"/>
<connect gate="C" pin="VCCIO3_2" pad="C18"/>
<connect gate="D" pin="GNDINT" pad="M11"/>
<connect gate="D" pin="GNDINT_2" pad="K11"/>
<connect gate="D" pin="GNDINT_3" pad="L12"/>
<connect gate="D" pin="GNDIO" pad="V18"/>
<connect gate="D" pin="GNDIO_2" pad="L10"/>
<connect gate="D" pin="GNDIO_3" pad="U17"/>
<connect gate="D" pin="GNDIO_4" pad="L11"/>
<connect gate="D" pin="IO" pad="V17"/>
<connect gate="D" pin="IO/DEV_CLRN" pad="N10"/>
<connect gate="D" pin="IO/GCLK2" pad="K13"/>
<connect gate="D" pin="IO_10" pad="L16"/>
<connect gate="D" pin="IO_11" pad="L17"/>
<connect gate="D" pin="IO_12" pad="L18"/>
<connect gate="D" pin="IO_13" pad="M12"/>
<connect gate="D" pin="IO_14" pad="M13"/>
<connect gate="D" pin="IO_15" pad="M14"/>
<connect gate="D" pin="IO_16" pad="M15"/>
<connect gate="D" pin="IO_17" pad="M16"/>
<connect gate="D" pin="IO_18" pad="N11"/>
<connect gate="D" pin="IO_19" pad="M17"/>
<connect gate="D" pin="IO_2" pad="K14"/>
<connect gate="D" pin="IO_20" pad="N12"/>
<connect gate="D" pin="IO_21" pad="M18"/>
<connect gate="D" pin="IO_22" pad="N13"/>
<connect gate="D" pin="IO_23" pad="N14"/>
<connect gate="D" pin="IO_24" pad="N15"/>
<connect gate="D" pin="IO_25" pad="N16"/>
<connect gate="D" pin="IO_26" pad="N17"/>
<connect gate="D" pin="IO_27" pad="N18"/>
<connect gate="D" pin="IO_28" pad="P10"/>
<connect gate="D" pin="IO_29" pad="P11"/>
<connect gate="D" pin="IO_3" pad="K15"/>
<connect gate="D" pin="IO_30" pad="P12"/>
<connect gate="D" pin="IO_31" pad="P13"/>
<connect gate="D" pin="IO_32" pad="P14"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="R10"/>
<connect gate="D" pin="IO_38" pad="R11"/>
<connect gate="D" pin="IO_39" pad="R12"/>
<connect gate="D" pin="IO_4" pad="K16"/>
<connect gate="D" pin="IO_40" pad="R13"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_44" pad="R17"/>
<connect gate="D" pin="IO_45" pad="R18"/>
<connect gate="D" pin="IO_46" pad="T10"/>
<connect gate="D" pin="IO_47" pad="T11"/>
<connect gate="D" pin="IO_48" pad="T12"/>
<connect gate="D" pin="IO_49" pad="T13"/>
<connect gate="D" pin="IO_5" pad="K17"/>
<connect gate="D" pin="IO_50" pad="T14"/>
<connect gate="D" pin="IO_51" pad="T15"/>
<connect gate="D" pin="IO_52" pad="T16"/>
<connect gate="D" pin="IO_53" pad="T17"/>
<connect gate="D" pin="IO_54" pad="U10"/>
<connect gate="D" pin="IO_55" pad="U11"/>
<connect gate="D" pin="IO_56" pad="U12"/>
<connect gate="D" pin="IO_57" pad="U13"/>
<connect gate="D" pin="IO_58" pad="U14"/>
<connect gate="D" pin="IO_59" pad="U15"/>
<connect gate="D" pin="IO_6" pad="K18"/>
<connect gate="D" pin="IO_60" pad="U16"/>
<connect gate="D" pin="IO_61" pad="U18"/>
<connect gate="D" pin="IO_62" pad="V10"/>
<connect gate="D" pin="IO_63" pad="V11"/>
<connect gate="D" pin="IO_64" pad="V12"/>
<connect gate="D" pin="IO_65" pad="V13"/>
<connect gate="D" pin="IO_66" pad="V14"/>
<connect gate="D" pin="IO_67" pad="V15"/>
<connect gate="D" pin="IO_7" pad="L13"/>
<connect gate="D" pin="IO_8" pad="L14"/>
<connect gate="D" pin="IO_9" pad="L15"/>
<connect gate="D" pin="VCCINT" pad="K10"/>
<connect gate="D" pin="VCCIO3" pad="K12"/>
<connect gate="D" pin="VCCIO3_2" pad="T18"/>
<connect gate="D" pin="VCCIO4" pad="M10"/>
<connect gate="D" pin="VCCIO4_2" pad="V16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210F324C5N"/>
<attribute name="OC_FARNELL" value="1635105"/>
<attribute name="OC_NEWARK" value="51R0491"/>
<attribute name="PACKAGE" value="BGA-324"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210GF256C3N">
<description>IC, CPLD, FLASH</description>
<gates>
<gate name="A" symbol="EPM2210GF256C3N_A"/>
<gate name="B" symbol="EPM2210GF256C3N_B"/>
<gate name="C" symbol="EPM2210GF256C3N_C"/>
</gates>
<devices>
<device name="" package="BGA256C16X16X100C_1700X1700X15">
<connects>
<connect gate="A" pin="GNDINT" pad="H7"/>
<connect gate="A" pin="GNDINT_2" pad="H9"/>
<connect gate="A" pin="GNDINT_3" pad="F7"/>
<connect gate="A" pin="GNDINT_4" pad="J8"/>
<connect gate="A" pin="GNDINT_5" pad="G6"/>
<connect gate="A" pin="GNDIO" pad="A1"/>
<connect gate="A" pin="GNDIO_2" pad="B2"/>
<connect gate="A" pin="GNDIO_3" pad="G7"/>
<connect gate="A" pin="GNDIO_4" pad="G8"/>
<connect gate="A" pin="GNDIO_5" pad="G9"/>
<connect gate="A" pin="IO" pad="K5"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="G1"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="G2"/>
<connect gate="A" pin="IO_51" pad="G3"/>
<connect gate="A" pin="IO_52" pad="G4"/>
<connect gate="A" pin="IO_53" pad="G5"/>
<connect gate="A" pin="IO_54" pad="H1"/>
<connect gate="A" pin="IO_55" pad="H2"/>
<connect gate="A" pin="IO_56" pad="H3"/>
<connect gate="A" pin="IO_57" pad="J1"/>
<connect gate="A" pin="IO_58" pad="H4"/>
<connect gate="A" pin="IO_59" pad="J2"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="J3"/>
<connect gate="A" pin="IO_61" pad="J4"/>
<connect gate="A" pin="IO_62" pad="K1"/>
<connect gate="A" pin="IO_63" pad="K2"/>
<connect gate="A" pin="IO_64" pad="K3"/>
<connect gate="A" pin="IO_65" pad="K4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCINT_2" pad="H8"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="J6"/>
<connect gate="A" pin="VCCIO1_2" pad="H6"/>
<connect gate="A" pin="VCCIO1_3" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="A3"/>
<connect gate="A" pin="VCCIO2_2" pad="F8"/>
<connect gate="A" pin="VCCIO2_3" pad="F9"/>
<connect gate="B" pin="GNDIO" pad="K9"/>
<connect gate="B" pin="GNDIO_2" pad="R2"/>
<connect gate="B" pin="GNDIO_3" pad="T1"/>
<connect gate="B" pin="GNDIO_4" pad="A16"/>
<connect gate="B" pin="GNDIO_5" pad="B15"/>
<connect gate="B" pin="GNDIO_6" pad="K7"/>
<connect gate="B" pin="GNDIO_7" pad="K8"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="M4"/>
<connect gate="B" pin="IO_11" pad="M6"/>
<connect gate="B" pin="IO_12" pad="M7"/>
<connect gate="B" pin="IO_13" pad="N1"/>
<connect gate="B" pin="IO_14" pad="N2"/>
<connect gate="B" pin="IO_15" pad="N3"/>
<connect gate="B" pin="IO_16" pad="N5"/>
<connect gate="B" pin="IO_17" pad="N6"/>
<connect gate="B" pin="IO_18" pad="N7"/>
<connect gate="B" pin="IO_19" pad="N8"/>
<connect gate="B" pin="IO_2" pad="L1"/>
<connect gate="B" pin="IO_20" pad="N9"/>
<connect gate="B" pin="IO_21" pad="P2"/>
<connect gate="B" pin="IO_22" pad="P4"/>
<connect gate="B" pin="IO_23" pad="P5"/>
<connect gate="B" pin="IO_24" pad="P6"/>
<connect gate="B" pin="IO_25" pad="P7"/>
<connect gate="B" pin="IO_26" pad="P8"/>
<connect gate="B" pin="IO_27" pad="P9"/>
<connect gate="B" pin="IO_28" pad="R1"/>
<connect gate="B" pin="IO_29" pad="R3"/>
<connect gate="B" pin="IO_3" pad="L2"/>
<connect gate="B" pin="IO_30" pad="R4"/>
<connect gate="B" pin="IO_31" pad="R5"/>
<connect gate="B" pin="IO_32" pad="R6"/>
<connect gate="B" pin="IO_33" pad="R7"/>
<connect gate="B" pin="IO_34" pad="R8"/>
<connect gate="B" pin="IO_35" pad="R9"/>
<connect gate="B" pin="IO_36" pad="T2"/>
<connect gate="B" pin="IO_37" pad="T4"/>
<connect gate="B" pin="IO_38" pad="T5"/>
<connect gate="B" pin="IO_39" pad="T6"/>
<connect gate="B" pin="IO_4" pad="L3"/>
<connect gate="B" pin="IO_40" pad="T7"/>
<connect gate="B" pin="IO_41" pad="T8"/>
<connect gate="B" pin="IO_42" pad="T9"/>
<connect gate="B" pin="IO_43" pad="A10"/>
<connect gate="B" pin="IO_44" pad="A11"/>
<connect gate="B" pin="IO_45" pad="A12"/>
<connect gate="B" pin="IO_46" pad="A13"/>
<connect gate="B" pin="IO_47" pad="A15"/>
<connect gate="B" pin="IO_48" pad="B10"/>
<connect gate="B" pin="IO_49" pad="B11"/>
<connect gate="B" pin="IO_5" pad="L4"/>
<connect gate="B" pin="IO_50" pad="B12"/>
<connect gate="B" pin="IO_51" pad="B13"/>
<connect gate="B" pin="IO_52" pad="B14"/>
<connect gate="B" pin="IO_53" pad="B16"/>
<connect gate="B" pin="IO_54" pad="C10"/>
<connect gate="B" pin="IO_55" pad="C11"/>
<connect gate="B" pin="IO_56" pad="C12"/>
<connect gate="B" pin="IO_57" pad="C13"/>
<connect gate="B" pin="IO_58" pad="C14"/>
<connect gate="B" pin="IO_59" pad="C15"/>
<connect gate="B" pin="IO_6" pad="L5"/>
<connect gate="B" pin="IO_60" pad="D10"/>
<connect gate="B" pin="IO_61" pad="D11"/>
<connect gate="B" pin="IO_62" pad="D12"/>
<connect gate="B" pin="IO_63" pad="D13"/>
<connect gate="B" pin="IO_64" pad="D14"/>
<connect gate="B" pin="IO_65" pad="D15"/>
<connect gate="B" pin="IO_7" pad="M1"/>
<connect gate="B" pin="IO_8" pad="M2"/>
<connect gate="B" pin="IO_9" pad="M3"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCINT" pad="L7"/>
<connect gate="B" pin="VCCINT_2" pad="K6"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO3" pad="C16"/>
<connect gate="B" pin="VCCIO4" pad="T3"/>
<connect gate="B" pin="VCCIO4_2" pad="L8"/>
<connect gate="B" pin="VCCIO4_3" pad="L9"/>
<connect gate="C" pin="GNDINT" pad="L10"/>
<connect gate="C" pin="GNDINT_2" pad="K11"/>
<connect gate="C" pin="GNDINT_3" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="T16"/>
<connect gate="C" pin="GNDIO_2" pad="G10"/>
<connect gate="C" pin="GNDIO_3" pad="K10"/>
<connect gate="C" pin="GNDIO_4" pad="R15"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="F12"/>
<connect gate="C" pin="IO_11" pad="F13"/>
<connect gate="C" pin="IO_12" pad="F14"/>
<connect gate="C" pin="IO_13" pad="F15"/>
<connect gate="C" pin="IO_14" pad="F16"/>
<connect gate="C" pin="IO_15" pad="G12"/>
<connect gate="C" pin="IO_16" pad="G13"/>
<connect gate="C" pin="IO_17" pad="G14"/>
<connect gate="C" pin="IO_18" pad="G15"/>
<connect gate="C" pin="IO_19" pad="G16"/>
<connect gate="C" pin="IO_2" pad="E10"/>
<connect gate="C" pin="IO_20" pad="H13"/>
<connect gate="C" pin="IO_21" pad="H14"/>
<connect gate="C" pin="IO_22" pad="H15"/>
<connect gate="C" pin="IO_23" pad="H16"/>
<connect gate="C" pin="IO_24" pad="J13"/>
<connect gate="C" pin="IO_25" pad="J14"/>
<connect gate="C" pin="IO_26" pad="J15"/>
<connect gate="C" pin="IO_27" pad="J16"/>
<connect gate="C" pin="IO_28" pad="K12"/>
<connect gate="C" pin="IO_29" pad="K13"/>
<connect gate="C" pin="IO_3" pad="E11"/>
<connect gate="C" pin="IO_30" pad="K14"/>
<connect gate="C" pin="IO_31" pad="K15"/>
<connect gate="C" pin="IO_32" pad="K16"/>
<connect gate="C" pin="IO_33" pad="L11"/>
<connect gate="C" pin="IO_34" pad="L12"/>
<connect gate="C" pin="IO_35" pad="L13"/>
<connect gate="C" pin="IO_36" pad="L14"/>
<connect gate="C" pin="IO_37" pad="L15"/>
<connect gate="C" pin="IO_38" pad="L16"/>
<connect gate="C" pin="IO_39" pad="M10"/>
<connect gate="C" pin="IO_4" pad="E12"/>
<connect gate="C" pin="IO_40" pad="M11"/>
<connect gate="C" pin="IO_41" pad="M12"/>
<connect gate="C" pin="IO_42" pad="M13"/>
<connect gate="C" pin="IO_43" pad="M14"/>
<connect gate="C" pin="IO_44" pad="M15"/>
<connect gate="C" pin="IO_45" pad="M16"/>
<connect gate="C" pin="IO_46" pad="N10"/>
<connect gate="C" pin="IO_47" pad="N11"/>
<connect gate="C" pin="IO_48" pad="N12"/>
<connect gate="C" pin="IO_49" pad="N13"/>
<connect gate="C" pin="IO_5" pad="E13"/>
<connect gate="C" pin="IO_50" pad="N14"/>
<connect gate="C" pin="IO_51" pad="N15"/>
<connect gate="C" pin="IO_52" pad="N16"/>
<connect gate="C" pin="IO_53" pad="P10"/>
<connect gate="C" pin="IO_54" pad="P11"/>
<connect gate="C" pin="IO_55" pad="P12"/>
<connect gate="C" pin="IO_56" pad="P13"/>
<connect gate="C" pin="IO_57" pad="P14"/>
<connect gate="C" pin="IO_58" pad="P15"/>
<connect gate="C" pin="IO_59" pad="R10"/>
<connect gate="C" pin="IO_6" pad="E14"/>
<connect gate="C" pin="IO_60" pad="R11"/>
<connect gate="C" pin="IO_61" pad="R12"/>
<connect gate="C" pin="IO_62" pad="R13"/>
<connect gate="C" pin="IO_63" pad="R14"/>
<connect gate="C" pin="IO_64" pad="R16"/>
<connect gate="C" pin="IO_65" pad="T10"/>
<connect gate="C" pin="IO_66" pad="T11"/>
<connect gate="C" pin="IO_67" pad="T12"/>
<connect gate="C" pin="IO_68" pad="T13"/>
<connect gate="C" pin="IO_7" pad="E15"/>
<connect gate="C" pin="IO_8" pad="E16"/>
<connect gate="C" pin="IO_9" pad="F11"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCINT_2" pad="F10"/>
<connect gate="C" pin="VCCINT_3" pad="G11"/>
<connect gate="C" pin="VCCIO3" pad="P16"/>
<connect gate="C" pin="VCCIO3_2" pad="H11"/>
<connect gate="C" pin="VCCIO3_3" pad="J11"/>
<connect gate="C" pin="VCCIO4" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210GF256C3N"/>
<attribute name="OC_FARNELL" value="1872693"/>
<attribute name="OC_NEWARK" value="51R9323"/>
<attribute name="PACKAGE" value="256-FBGA"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM2210GF324C5N" prefix="U">
<description>IC MAX II CPLD 2210 LE 324-FBGA</description>
<gates>
<gate name="A" symbol="EPM2210GF324C5N_A"/>
<gate name="B" symbol="EPM2210GF324C5N_B"/>
<gate name="C" symbol="EPM2210GF324C5N_C"/>
<gate name="D" symbol="EPM2210GF324C5N_D"/>
</gates>
<devices>
<device name="" package="BGA324N100P18X18_1900X1900X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="G8"/>
<connect gate="A" pin="GNDINT_3" pad="H7"/>
<connect gate="A" pin="GNDIO" pad="H9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="H8"/>
<connect gate="A" pin="IO" pad="J5"/>
<connect gate="A" pin="IO/GCLK0" pad="J6"/>
<connect gate="A" pin="IO_10" pad="B3"/>
<connect gate="A" pin="IO_11" pad="B4"/>
<connect gate="A" pin="IO_12" pad="B5"/>
<connect gate="A" pin="IO_13" pad="B6"/>
<connect gate="A" pin="IO_14" pad="B7"/>
<connect gate="A" pin="IO_15" pad="B8"/>
<connect gate="A" pin="IO_16" pad="B9"/>
<connect gate="A" pin="IO_17" pad="C2"/>
<connect gate="A" pin="IO_18" pad="C3"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="A2"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D1"/>
<connect gate="A" pin="IO_26" pad="D2"/>
<connect gate="A" pin="IO_27" pad="D3"/>
<connect gate="A" pin="IO_28" pad="D4"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="A4"/>
<connect gate="A" pin="IO_30" pad="D6"/>
<connect gate="A" pin="IO_31" pad="D7"/>
<connect gate="A" pin="IO_32" pad="D8"/>
<connect gate="A" pin="IO_33" pad="D9"/>
<connect gate="A" pin="IO_34" pad="E1"/>
<connect gate="A" pin="IO_35" pad="E2"/>
<connect gate="A" pin="IO_36" pad="E3"/>
<connect gate="A" pin="IO_37" pad="E4"/>
<connect gate="A" pin="IO_38" pad="E5"/>
<connect gate="A" pin="IO_39" pad="E6"/>
<connect gate="A" pin="IO_4" pad="A5"/>
<connect gate="A" pin="IO_40" pad="E7"/>
<connect gate="A" pin="IO_41" pad="E8"/>
<connect gate="A" pin="IO_42" pad="E9"/>
<connect gate="A" pin="IO_43" pad="F1"/>
<connect gate="A" pin="IO_44" pad="F2"/>
<connect gate="A" pin="IO_45" pad="F3"/>
<connect gate="A" pin="IO_46" pad="F4"/>
<connect gate="A" pin="IO_47" pad="F5"/>
<connect gate="A" pin="IO_48" pad="F6"/>
<connect gate="A" pin="IO_49" pad="F7"/>
<connect gate="A" pin="IO_5" pad="A6"/>
<connect gate="A" pin="IO_50" pad="F8"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="G3"/>
<connect gate="A" pin="IO_55" pad="G4"/>
<connect gate="A" pin="IO_56" pad="G5"/>
<connect gate="A" pin="IO_57" pad="G6"/>
<connect gate="A" pin="IO_58" pad="G7"/>
<connect gate="A" pin="IO_59" pad="H1"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_60" pad="H2"/>
<connect gate="A" pin="IO_61" pad="H3"/>
<connect gate="A" pin="IO_62" pad="H4"/>
<connect gate="A" pin="IO_63" pad="H5"/>
<connect gate="A" pin="IO_64" pad="H6"/>
<connect gate="A" pin="IO_65" pad="J1"/>
<connect gate="A" pin="IO_66" pad="J2"/>
<connect gate="A" pin="IO_67" pad="J3"/>
<connect gate="A" pin="IO_68" pad="J4"/>
<connect gate="A" pin="IO_7" pad="A8"/>
<connect gate="A" pin="IO_8" pad="A9"/>
<connect gate="A" pin="IO_9" pad="B1"/>
<connect gate="A" pin="VCCINT" pad="J9"/>
<connect gate="A" pin="VCCIO1" pad="J7"/>
<connect gate="A" pin="VCCIO1_2" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="G9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="B" pin="GNDINT" pad="K9"/>
<connect gate="B" pin="GNDIO" pad="V1"/>
<connect gate="B" pin="GNDIO_2" pad="L8"/>
<connect gate="B" pin="GNDIO_3" pad="L9"/>
<connect gate="B" pin="GNDIO_4" pad="U2"/>
<connect gate="B" pin="IO" pad="V9"/>
<connect gate="B" pin="IO/DEV_OE" pad="N9"/>
<connect gate="B" pin="IO/GCLK1" pad="K6"/>
<connect gate="B" pin="IO_10" pad="L4"/>
<connect gate="B" pin="IO_11" pad="L5"/>
<connect gate="B" pin="IO_12" pad="L6"/>
<connect gate="B" pin="IO_13" pad="M1"/>
<connect gate="B" pin="IO_14" pad="M2"/>
<connect gate="B" pin="IO_15" pad="M3"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="M5"/>
<connect gate="B" pin="IO_18" pad="M6"/>
<connect gate="B" pin="IO_19" pad="N1"/>
<connect gate="B" pin="IO_2" pad="K1"/>
<connect gate="B" pin="IO_20" pad="N2"/>
<connect gate="B" pin="IO_21" pad="N3"/>
<connect gate="B" pin="IO_22" pad="N4"/>
<connect gate="B" pin="IO_23" pad="N5"/>
<connect gate="B" pin="IO_24" pad="N7"/>
<connect gate="B" pin="IO_25" pad="N8"/>
<connect gate="B" pin="IO_26" pad="P1"/>
<connect gate="B" pin="IO_27" pad="P2"/>
<connect gate="B" pin="IO_28" pad="P3"/>
<connect gate="B" pin="IO_29" pad="P4"/>
<connect gate="B" pin="IO_3" pad="K2"/>
<connect gate="B" pin="IO_30" pad="P6"/>
<connect gate="B" pin="IO_31" pad="P7"/>
<connect gate="B" pin="IO_32" pad="P8"/>
<connect gate="B" pin="IO_33" pad="P9"/>
<connect gate="B" pin="IO_34" pad="R1"/>
<connect gate="B" pin="IO_35" pad="R2"/>
<connect gate="B" pin="IO_36" pad="R3"/>
<connect gate="B" pin="IO_37" pad="R5"/>
<connect gate="B" pin="IO_38" pad="R6"/>
<connect gate="B" pin="IO_39" pad="R7"/>
<connect gate="B" pin="IO_4" pad="K3"/>
<connect gate="B" pin="IO_40" pad="R8"/>
<connect gate="B" pin="IO_41" pad="R9"/>
<connect gate="B" pin="IO_42" pad="T2"/>
<connect gate="B" pin="IO_43" pad="T3"/>
<connect gate="B" pin="IO_44" pad="T4"/>
<connect gate="B" pin="IO_45" pad="T5"/>
<connect gate="B" pin="IO_46" pad="T6"/>
<connect gate="B" pin="IO_47" pad="T7"/>
<connect gate="B" pin="IO_48" pad="T8"/>
<connect gate="B" pin="IO_49" pad="T9"/>
<connect gate="B" pin="IO_5" pad="K4"/>
<connect gate="B" pin="IO_50" pad="U1"/>
<connect gate="B" pin="IO_51" pad="U3"/>
<connect gate="B" pin="IO_52" pad="U4"/>
<connect gate="B" pin="IO_53" pad="U5"/>
<connect gate="B" pin="IO_54" pad="U6"/>
<connect gate="B" pin="IO_55" pad="U7"/>
<connect gate="B" pin="IO_56" pad="U8"/>
<connect gate="B" pin="IO_57" pad="U9"/>
<connect gate="B" pin="IO_58" pad="V2"/>
<connect gate="B" pin="IO_59" pad="V4"/>
<connect gate="B" pin="IO_6" pad="K5"/>
<connect gate="B" pin="IO_60" pad="V5"/>
<connect gate="B" pin="IO_61" pad="V6"/>
<connect gate="B" pin="IO_62" pad="V7"/>
<connect gate="B" pin="IO_63" pad="V8"/>
<connect gate="B" pin="IO_7" pad="L1"/>
<connect gate="B" pin="IO_8" pad="L2"/>
<connect gate="B" pin="IO_9" pad="L3"/>
<connect gate="B" pin="TCK" pad="R4"/>
<connect gate="B" pin="TDI" pad="M7"/>
<connect gate="B" pin="TDO" pad="N6"/>
<connect gate="B" pin="TMS" pad="P5"/>
<connect gate="B" pin="VCCINT" pad="M8"/>
<connect gate="B" pin="VCCINT_2" pad="K8"/>
<connect gate="B" pin="VCCINT_3" pad="L7"/>
<connect gate="B" pin="VCCIO1" pad="T1"/>
<connect gate="B" pin="VCCIO1_2" pad="K7"/>
<connect gate="B" pin="VCCIO4" pad="V3"/>
<connect gate="B" pin="VCCIO4_2" pad="M9"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="H11"/>
<connect gate="C" pin="GNDIO_2" pad="A18"/>
<connect gate="C" pin="GNDIO_3" pad="B17"/>
<connect gate="C" pin="GNDIO_4" pad="H10"/>
<connect gate="C" pin="IO" pad="J18"/>
<connect gate="C" pin="IO/GCLK3" pad="J13"/>
<connect gate="C" pin="IO_10" pad="B11"/>
<connect gate="C" pin="IO_11" pad="B12"/>
<connect gate="C" pin="IO_12" pad="B13"/>
<connect gate="C" pin="IO_13" pad="B14"/>
<connect gate="C" pin="IO_14" pad="B15"/>
<connect gate="C" pin="IO_15" pad="B16"/>
<connect gate="C" pin="IO_16" pad="B18"/>
<connect gate="C" pin="IO_17" pad="C10"/>
<connect gate="C" pin="IO_18" pad="C11"/>
<connect gate="C" pin="IO_19" pad="C12"/>
<connect gate="C" pin="IO_2" pad="A10"/>
<connect gate="C" pin="IO_20" pad="C13"/>
<connect gate="C" pin="IO_21" pad="C14"/>
<connect gate="C" pin="IO_22" pad="C15"/>
<connect gate="C" pin="IO_23" pad="C16"/>
<connect gate="C" pin="IO_24" pad="C17"/>
<connect gate="C" pin="IO_25" pad="D10"/>
<connect gate="C" pin="IO_26" pad="D11"/>
<connect gate="C" pin="IO_27" pad="D12"/>
<connect gate="C" pin="IO_28" pad="D13"/>
<connect gate="C" pin="IO_29" pad="D14"/>
<connect gate="C" pin="IO_3" pad="A11"/>
<connect gate="C" pin="IO_30" pad="D15"/>
<connect gate="C" pin="IO_31" pad="D16"/>
<connect gate="C" pin="IO_32" pad="D17"/>
<connect gate="C" pin="IO_33" pad="D18"/>
<connect gate="C" pin="IO_34" pad="E10"/>
<connect gate="C" pin="IO_35" pad="E11"/>
<connect gate="C" pin="IO_36" pad="E12"/>
<connect gate="C" pin="IO_37" pad="E13"/>
<connect gate="C" pin="IO_38" pad="E14"/>
<connect gate="C" pin="IO_39" pad="E15"/>
<connect gate="C" pin="IO_4" pad="A12"/>
<connect gate="C" pin="IO_40" pad="E16"/>
<connect gate="C" pin="IO_41" pad="E17"/>
<connect gate="C" pin="IO_42" pad="E18"/>
<connect gate="C" pin="IO_43" pad="F10"/>
<connect gate="C" pin="IO_44" pad="F11"/>
<connect gate="C" pin="IO_45" pad="F12"/>
<connect gate="C" pin="IO_46" pad="F13"/>
<connect gate="C" pin="IO_47" pad="F14"/>
<connect gate="C" pin="IO_48" pad="F15"/>
<connect gate="C" pin="IO_49" pad="F16"/>
<connect gate="C" pin="IO_5" pad="A13"/>
<connect gate="C" pin="IO_50" pad="F17"/>
<connect gate="C" pin="IO_51" pad="F18"/>
<connect gate="C" pin="IO_52" pad="G12"/>
<connect gate="C" pin="IO_53" pad="G13"/>
<connect gate="C" pin="IO_54" pad="G14"/>
<connect gate="C" pin="IO_55" pad="G15"/>
<connect gate="C" pin="IO_56" pad="G16"/>
<connect gate="C" pin="IO_57" pad="G17"/>
<connect gate="C" pin="IO_58" pad="G18"/>
<connect gate="C" pin="IO_59" pad="H13"/>
<connect gate="C" pin="IO_6" pad="A14"/>
<connect gate="C" pin="IO_60" pad="H14"/>
<connect gate="C" pin="IO_61" pad="H15"/>
<connect gate="C" pin="IO_62" pad="H16"/>
<connect gate="C" pin="IO_63" pad="H17"/>
<connect gate="C" pin="IO_64" pad="H18"/>
<connect gate="C" pin="IO_65" pad="J14"/>
<connect gate="C" pin="IO_66" pad="J15"/>
<connect gate="C" pin="IO_67" pad="J16"/>
<connect gate="C" pin="IO_68" pad="J17"/>
<connect gate="C" pin="IO_7" pad="A15"/>
<connect gate="C" pin="IO_8" pad="A17"/>
<connect gate="C" pin="IO_9" pad="B10"/>
<connect gate="C" pin="VCCINT" pad="J11"/>
<connect gate="C" pin="VCCINT_2" pad="G11"/>
<connect gate="C" pin="VCCINT_3" pad="H12"/>
<connect gate="C" pin="VCCIO2" pad="G10"/>
<connect gate="C" pin="VCCIO2_2" pad="A16"/>
<connect gate="C" pin="VCCIO3" pad="J12"/>
<connect gate="C" pin="VCCIO3_2" pad="C18"/>
<connect gate="D" pin="GNDINT" pad="M11"/>
<connect gate="D" pin="GNDINT_2" pad="K11"/>
<connect gate="D" pin="GNDINT_3" pad="L12"/>
<connect gate="D" pin="GNDIO" pad="V18"/>
<connect gate="D" pin="GNDIO_2" pad="L10"/>
<connect gate="D" pin="GNDIO_3" pad="L11"/>
<connect gate="D" pin="GNDIO_4" pad="U17"/>
<connect gate="D" pin="IO" pad="V17"/>
<connect gate="D" pin="IO/*DEV_CLR" pad="N10"/>
<connect gate="D" pin="IO/GCLK2" pad="K13"/>
<connect gate="D" pin="IO_10" pad="L16"/>
<connect gate="D" pin="IO_11" pad="L17"/>
<connect gate="D" pin="IO_12" pad="L18"/>
<connect gate="D" pin="IO_13" pad="M12"/>
<connect gate="D" pin="IO_14" pad="M13"/>
<connect gate="D" pin="IO_15" pad="M14"/>
<connect gate="D" pin="IO_16" pad="M15"/>
<connect gate="D" pin="IO_17" pad="M16"/>
<connect gate="D" pin="IO_18" pad="M17"/>
<connect gate="D" pin="IO_19" pad="M18"/>
<connect gate="D" pin="IO_2" pad="K14"/>
<connect gate="D" pin="IO_20" pad="N11"/>
<connect gate="D" pin="IO_21" pad="N12"/>
<connect gate="D" pin="IO_22" pad="N13"/>
<connect gate="D" pin="IO_23" pad="N14"/>
<connect gate="D" pin="IO_24" pad="N15"/>
<connect gate="D" pin="IO_25" pad="N16"/>
<connect gate="D" pin="IO_26" pad="N17"/>
<connect gate="D" pin="IO_27" pad="N18"/>
<connect gate="D" pin="IO_28" pad="P10"/>
<connect gate="D" pin="IO_29" pad="P11"/>
<connect gate="D" pin="IO_3" pad="K15"/>
<connect gate="D" pin="IO_30" pad="P12"/>
<connect gate="D" pin="IO_31" pad="P13"/>
<connect gate="D" pin="IO_32" pad="P14"/>
<connect gate="D" pin="IO_33" pad="P15"/>
<connect gate="D" pin="IO_34" pad="P16"/>
<connect gate="D" pin="IO_35" pad="P17"/>
<connect gate="D" pin="IO_36" pad="P18"/>
<connect gate="D" pin="IO_37" pad="R10"/>
<connect gate="D" pin="IO_38" pad="R11"/>
<connect gate="D" pin="IO_39" pad="R12"/>
<connect gate="D" pin="IO_4" pad="K16"/>
<connect gate="D" pin="IO_40" pad="R13"/>
<connect gate="D" pin="IO_41" pad="R14"/>
<connect gate="D" pin="IO_42" pad="R15"/>
<connect gate="D" pin="IO_43" pad="R16"/>
<connect gate="D" pin="IO_44" pad="R17"/>
<connect gate="D" pin="IO_45" pad="R18"/>
<connect gate="D" pin="IO_46" pad="T10"/>
<connect gate="D" pin="IO_47" pad="T11"/>
<connect gate="D" pin="IO_48" pad="T12"/>
<connect gate="D" pin="IO_49" pad="T13"/>
<connect gate="D" pin="IO_5" pad="K17"/>
<connect gate="D" pin="IO_50" pad="T14"/>
<connect gate="D" pin="IO_51" pad="T15"/>
<connect gate="D" pin="IO_52" pad="T16"/>
<connect gate="D" pin="IO_53" pad="T17"/>
<connect gate="D" pin="IO_54" pad="U10"/>
<connect gate="D" pin="IO_55" pad="U11"/>
<connect gate="D" pin="IO_56" pad="U12"/>
<connect gate="D" pin="IO_57" pad="U13"/>
<connect gate="D" pin="IO_58" pad="U14"/>
<connect gate="D" pin="IO_59" pad="U15"/>
<connect gate="D" pin="IO_6" pad="K18"/>
<connect gate="D" pin="IO_60" pad="U16"/>
<connect gate="D" pin="IO_61" pad="U18"/>
<connect gate="D" pin="IO_62" pad="V10"/>
<connect gate="D" pin="IO_63" pad="V11"/>
<connect gate="D" pin="IO_64" pad="V12"/>
<connect gate="D" pin="IO_65" pad="V13"/>
<connect gate="D" pin="IO_66" pad="V14"/>
<connect gate="D" pin="IO_67" pad="V15"/>
<connect gate="D" pin="IO_7" pad="L13"/>
<connect gate="D" pin="IO_8" pad="L14"/>
<connect gate="D" pin="IO_9" pad="L15"/>
<connect gate="D" pin="VCCINT" pad="K10"/>
<connect gate="D" pin="VCCIO3" pad="T18"/>
<connect gate="D" pin="VCCIO3_2" pad="K12"/>
<connect gate="D" pin="VCCIO4" pad="V16"/>
<connect gate="D" pin="VCCIO4_2" pad="M10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM2210GF324C5N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9335"/>
<attribute name="PACKAGE" value="324-FBGA"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240GM100C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM240GM100C5N"/>
</gates>
<devices>
<device name="" package="BGA100C50P11X11_600X600X120">
<connects>
<connect gate="A" pin="GNDINT" pad="G4"/>
<connect gate="A" pin="GNDINT_2" pad="E8"/>
<connect gate="A" pin="GNDIO" pad="H7"/>
<connect gate="A" pin="GNDIO_2" pad="E4"/>
<connect gate="A" pin="GNDIO_3" pad="D5"/>
<connect gate="A" pin="GNDIO_4" pad="H5"/>
<connect gate="A" pin="GNDIO_5" pad="D7"/>
<connect gate="A" pin="GNDIO_6" pad="G8"/>
<connect gate="A" pin="IO" pad="L11"/>
<connect gate="A" pin="IO/DEV_OE" pad="L8"/>
<connect gate="A" pin="IO/GCLK0" pad="F2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F10"/>
<connect gate="A" pin="IO/GCLK3" pad="G11"/>
<connect gate="A" pin="IO/NDEV_CLR" pad="K8"/>
<connect gate="A" pin="IO_10" pad="G2"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="A5"/>
<connect gate="A" pin="IO_13" pad="A6"/>
<connect gate="A" pin="IO_14" pad="A7"/>
<connect gate="A" pin="IO_15" pad="A8"/>
<connect gate="A" pin="IO_16" pad="A9"/>
<connect gate="A" pin="IO_17" pad="B1"/>
<connect gate="A" pin="IO_18" pad="B2"/>
<connect gate="A" pin="IO_19" pad="B3"/>
<connect gate="A" pin="IO_2" pad="E2"/>
<connect gate="A" pin="IO_20" pad="B4"/>
<connect gate="A" pin="IO_21" pad="B5"/>
<connect gate="A" pin="IO_22" pad="C5"/>
<connect gate="A" pin="IO_23" pad="B6"/>
<connect gate="A" pin="IO_24" pad="C6"/>
<connect gate="A" pin="IO_25" pad="B7"/>
<connect gate="A" pin="IO_26" pad="C7"/>
<connect gate="A" pin="IO_27" pad="B8"/>
<connect gate="A" pin="IO_28" pad="B9"/>
<connect gate="A" pin="IO_29" pad="D1"/>
<connect gate="A" pin="IO_3" pad="F1"/>
<connect gate="A" pin="IO_30" pad="C1"/>
<connect gate="A" pin="IO_31" pad="D2"/>
<connect gate="A" pin="IO_32" pad="H1"/>
<connect gate="A" pin="IO_33" pad="C2"/>
<connect gate="A" pin="IO_34" pad="H2"/>
<connect gate="A" pin="IO_35" pad="D9"/>
<connect gate="A" pin="IO_36" pad="H3"/>
<connect gate="A" pin="IO_37" pad="D3"/>
<connect gate="A" pin="IO_38" pad="H9"/>
<connect gate="A" pin="IO_39" pad="J5"/>
<connect gate="A" pin="IO_4" pad="F3"/>
<connect gate="A" pin="IO_40" pad="J6"/>
<connect gate="A" pin="IO_41" pad="J7"/>
<connect gate="A" pin="IO_42" pad="K3"/>
<connect gate="A" pin="IO_43" pad="K4"/>
<connect gate="A" pin="IO_44" pad="K5"/>
<connect gate="A" pin="IO_45" pad="K6"/>
<connect gate="A" pin="IO_46" pad="L9"/>
<connect gate="A" pin="IO_47" pad="K7"/>
<connect gate="A" pin="IO_48" pad="A10"/>
<connect gate="A" pin="IO_49" pad="A11"/>
<connect gate="A" pin="IO_5" pad="A1"/>
<connect gate="A" pin="IO_50" pad="B10"/>
<connect gate="A" pin="IO_51" pad="K9"/>
<connect gate="A" pin="IO_52" pad="B11"/>
<connect gate="A" pin="IO_53" pad="L1"/>
<connect gate="A" pin="IO_54" pad="C10"/>
<connect gate="A" pin="IO_55" pad="L2"/>
<connect gate="A" pin="IO_56" pad="C11"/>
<connect gate="A" pin="IO_57" pad="L3"/>
<connect gate="A" pin="IO_58" pad="D10"/>
<connect gate="A" pin="IO_59" pad="L4"/>
<connect gate="A" pin="IO_6" pad="F9"/>
<connect gate="A" pin="IO_60" pad="D11"/>
<connect gate="A" pin="IO_61" pad="L5"/>
<connect gate="A" pin="IO_62" pad="E10"/>
<connect gate="A" pin="IO_63" pad="L6"/>
<connect gate="A" pin="IO_64" pad="E11"/>
<connect gate="A" pin="IO_65" pad="L7"/>
<connect gate="A" pin="IO_66" pad="F11"/>
<connect gate="A" pin="IO_67" pad="G10"/>
<connect gate="A" pin="IO_68" pad="H10"/>
<connect gate="A" pin="IO_69" pad="H11"/>
<connect gate="A" pin="IO_7" pad="A2"/>
<connect gate="A" pin="IO_70" pad="J10"/>
<connect gate="A" pin="IO_71" pad="J11"/>
<connect gate="A" pin="IO_72" pad="K10"/>
<connect gate="A" pin="IO_73" pad="K11"/>
<connect gate="A" pin="IO_74" pad="L10"/>
<connect gate="A" pin="IO_8" pad="G1"/>
<connect gate="A" pin="IO_9" pad="A3"/>
<connect gate="A" pin="TCK" pad="K1"/>
<connect gate="A" pin="TDI" pad="J2"/>
<connect gate="A" pin="TDO" pad="K2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="G3"/>
<connect gate="A" pin="VCCINT_2" pad="E9"/>
<connect gate="A" pin="VCCIO1" pad="J8"/>
<connect gate="A" pin="VCCIO1_2" pad="E3"/>
<connect gate="A" pin="VCCIO1_3" pad="J4"/>
<connect gate="A" pin="VCCIO2" pad="C4"/>
<connect gate="A" pin="VCCIO2_2" pad="C8"/>
<connect gate="A" pin="VCCIO2_3" pad="G9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM240GM100C5N"/>
<attribute name="OC_FARNELL" value="1549462"/>
<attribute name="OC_NEWARK" value="51R9343"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240GT100C3N">
<description>IC CPLD FLASH 192 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM240GT100C3N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="11"/>
<connect gate="A" pin="GNDINT_2" pad="65"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="46"/>
<connect gate="A" pin="GNDIO_3" pad="32"/>
<connect gate="A" pin="GNDIO_4" pad="60"/>
<connect gate="A" pin="GNDIO_5" pad="93"/>
<connect gate="A" pin="GNDIO_6" pad="10"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="34"/>
<connect gate="A" pin="IO_11" pad="35"/>
<connect gate="A" pin="IO_12" pad="1"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="36"/>
<connect gate="A" pin="IO_15" pad="2"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="37"/>
<connect gate="A" pin="IO_19" pad="3"/>
<connect gate="A" pin="IO_2" pad="15"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="30"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="4"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="5"/>
<connect gate="A" pin="IO_26" pad="47"/>
<connect gate="A" pin="IO_27" pad="40"/>
<connect gate="A" pin="IO_28" pad="48"/>
<connect gate="A" pin="IO_29" pad="6"/>
<connect gate="A" pin="IO_3" pad="16"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="41"/>
<connect gate="A" pin="IO_32" pad="50"/>
<connect gate="A" pin="IO_33" pad="7"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="8"/>
<connect gate="A" pin="IO_36" pad="51"/>
<connect gate="A" pin="IO_37" pad="52"/>
<connect gate="A" pin="IO_38" pad="53"/>
<connect gate="A" pin="IO_39" pad="54"/>
<connect gate="A" pin="IO_4" pad="17"/>
<connect gate="A" pin="IO_40" pad="55"/>
<connect gate="A" pin="IO_41" pad="56"/>
<connect gate="A" pin="IO_42" pad="66"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="68"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="69"/>
<connect gate="A" pin="IO_49" pad="70"/>
<connect gate="A" pin="IO_5" pad="18"/>
<connect gate="A" pin="IO_50" pad="71"/>
<connect gate="A" pin="IO_51" pad="72"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_58" pad="81"/>
<connect gate="A" pin="IO_59" pad="82"/>
<connect gate="A" pin="IO_6" pad="19"/>
<connect gate="A" pin="IO_60" pad="83"/>
<connect gate="A" pin="IO_61" pad="84"/>
<connect gate="A" pin="IO_62" pad="85"/>
<connect gate="A" pin="IO_63" pad="86"/>
<connect gate="A" pin="IO_64" pad="87"/>
<connect gate="A" pin="IO_65" pad="88"/>
<connect gate="A" pin="IO_66" pad="89"/>
<connect gate="A" pin="IO_67" pad="90"/>
<connect gate="A" pin="IO_68" pad="91"/>
<connect gate="A" pin="IO_69" pad="92"/>
<connect gate="A" pin="IO_7" pad="20"/>
<connect gate="A" pin="IO_70" pad="95"/>
<connect gate="A" pin="IO_71" pad="96"/>
<connect gate="A" pin="IO_72" pad="97"/>
<connect gate="A" pin="IO_73" pad="98"/>
<connect gate="A" pin="IO_74" pad="99"/>
<connect gate="A" pin="IO_8" pad="21"/>
<connect gate="A" pin="IO_9" pad="33"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCIO1" pad="31"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="45"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM240GT100C3N"/>
<attribute name="OC_FARNELL" value="1549465"/>
<attribute name="OC_NEWARK" value="51R9346"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240M100C4N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM240M100C4N"/>
</gates>
<devices>
<device name="" package="BGA100C50P11X11_600X600X120">
<connects>
<connect gate="A" pin="GNDINT" pad="G4"/>
<connect gate="A" pin="GNDINT_2" pad="E8"/>
<connect gate="A" pin="GNDIO" pad="H7"/>
<connect gate="A" pin="GNDIO_2" pad="E4"/>
<connect gate="A" pin="GNDIO_3" pad="D5"/>
<connect gate="A" pin="GNDIO_4" pad="H5"/>
<connect gate="A" pin="GNDIO_5" pad="D7"/>
<connect gate="A" pin="GNDIO_6" pad="G8"/>
<connect gate="A" pin="IO" pad="L11"/>
<connect gate="A" pin="IO/DEV_OE" pad="L8"/>
<connect gate="A" pin="IO/GCLK0" pad="F2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F10"/>
<connect gate="A" pin="IO/GCLK3" pad="G11"/>
<connect gate="A" pin="IO/NDEV_CLR" pad="K8"/>
<connect gate="A" pin="IO_10" pad="G2"/>
<connect gate="A" pin="IO_11" pad="A4"/>
<connect gate="A" pin="IO_12" pad="A5"/>
<connect gate="A" pin="IO_13" pad="A6"/>
<connect gate="A" pin="IO_14" pad="A7"/>
<connect gate="A" pin="IO_15" pad="A8"/>
<connect gate="A" pin="IO_16" pad="A9"/>
<connect gate="A" pin="IO_17" pad="B1"/>
<connect gate="A" pin="IO_18" pad="B2"/>
<connect gate="A" pin="IO_19" pad="B3"/>
<connect gate="A" pin="IO_2" pad="E2"/>
<connect gate="A" pin="IO_20" pad="B4"/>
<connect gate="A" pin="IO_21" pad="B5"/>
<connect gate="A" pin="IO_22" pad="C5"/>
<connect gate="A" pin="IO_23" pad="B6"/>
<connect gate="A" pin="IO_24" pad="C6"/>
<connect gate="A" pin="IO_25" pad="B7"/>
<connect gate="A" pin="IO_26" pad="C7"/>
<connect gate="A" pin="IO_27" pad="B8"/>
<connect gate="A" pin="IO_28" pad="B9"/>
<connect gate="A" pin="IO_29" pad="D1"/>
<connect gate="A" pin="IO_3" pad="F1"/>
<connect gate="A" pin="IO_30" pad="C1"/>
<connect gate="A" pin="IO_31" pad="D2"/>
<connect gate="A" pin="IO_32" pad="H1"/>
<connect gate="A" pin="IO_33" pad="C2"/>
<connect gate="A" pin="IO_34" pad="H2"/>
<connect gate="A" pin="IO_35" pad="D9"/>
<connect gate="A" pin="IO_36" pad="H3"/>
<connect gate="A" pin="IO_37" pad="D3"/>
<connect gate="A" pin="IO_38" pad="H9"/>
<connect gate="A" pin="IO_39" pad="J5"/>
<connect gate="A" pin="IO_4" pad="F3"/>
<connect gate="A" pin="IO_40" pad="J6"/>
<connect gate="A" pin="IO_41" pad="J7"/>
<connect gate="A" pin="IO_42" pad="K3"/>
<connect gate="A" pin="IO_43" pad="K4"/>
<connect gate="A" pin="IO_44" pad="K5"/>
<connect gate="A" pin="IO_45" pad="K6"/>
<connect gate="A" pin="IO_46" pad="L9"/>
<connect gate="A" pin="IO_47" pad="K7"/>
<connect gate="A" pin="IO_48" pad="A10"/>
<connect gate="A" pin="IO_49" pad="A11"/>
<connect gate="A" pin="IO_5" pad="A1"/>
<connect gate="A" pin="IO_50" pad="B10"/>
<connect gate="A" pin="IO_51" pad="K9"/>
<connect gate="A" pin="IO_52" pad="B11"/>
<connect gate="A" pin="IO_53" pad="L1"/>
<connect gate="A" pin="IO_54" pad="C10"/>
<connect gate="A" pin="IO_55" pad="L2"/>
<connect gate="A" pin="IO_56" pad="C11"/>
<connect gate="A" pin="IO_57" pad="L3"/>
<connect gate="A" pin="IO_58" pad="D10"/>
<connect gate="A" pin="IO_59" pad="L4"/>
<connect gate="A" pin="IO_6" pad="F9"/>
<connect gate="A" pin="IO_60" pad="D11"/>
<connect gate="A" pin="IO_61" pad="L5"/>
<connect gate="A" pin="IO_62" pad="E10"/>
<connect gate="A" pin="IO_63" pad="L6"/>
<connect gate="A" pin="IO_64" pad="E11"/>
<connect gate="A" pin="IO_65" pad="L7"/>
<connect gate="A" pin="IO_66" pad="F11"/>
<connect gate="A" pin="IO_67" pad="G10"/>
<connect gate="A" pin="IO_68" pad="H10"/>
<connect gate="A" pin="IO_69" pad="H11"/>
<connect gate="A" pin="IO_7" pad="A2"/>
<connect gate="A" pin="IO_70" pad="J10"/>
<connect gate="A" pin="IO_71" pad="J11"/>
<connect gate="A" pin="IO_72" pad="K10"/>
<connect gate="A" pin="IO_73" pad="K11"/>
<connect gate="A" pin="IO_74" pad="L10"/>
<connect gate="A" pin="IO_8" pad="G1"/>
<connect gate="A" pin="IO_9" pad="A3"/>
<connect gate="A" pin="TCK" pad="K1"/>
<connect gate="A" pin="TDI" pad="J2"/>
<connect gate="A" pin="TDO" pad="K2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="G3"/>
<connect gate="A" pin="VCCINT_2" pad="E9"/>
<connect gate="A" pin="VCCIO1" pad="J8"/>
<connect gate="A" pin="VCCIO1_2" pad="E3"/>
<connect gate="A" pin="VCCIO1_3" pad="J4"/>
<connect gate="A" pin="VCCIO2" pad="C4"/>
<connect gate="A" pin="VCCIO2_2" pad="C8"/>
<connect gate="A" pin="VCCIO2_3" pad="G9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM240M100C4N"/>
<attribute name="OC_FARNELL" value="1742178"/>
<attribute name="OC_NEWARK" value="51R0493"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240T100C3N">
<description>IC CPLD FLASH 192 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM240T100C3N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="11"/>
<connect gate="A" pin="GNDINT_2" pad="65"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="46"/>
<connect gate="A" pin="GNDIO_3" pad="32"/>
<connect gate="A" pin="GNDIO_4" pad="60"/>
<connect gate="A" pin="GNDIO_5" pad="93"/>
<connect gate="A" pin="GNDIO_6" pad="10"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="34"/>
<connect gate="A" pin="IO_11" pad="35"/>
<connect gate="A" pin="IO_12" pad="1"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="36"/>
<connect gate="A" pin="IO_15" pad="2"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="37"/>
<connect gate="A" pin="IO_19" pad="3"/>
<connect gate="A" pin="IO_2" pad="15"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="30"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="4"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="5"/>
<connect gate="A" pin="IO_26" pad="47"/>
<connect gate="A" pin="IO_27" pad="40"/>
<connect gate="A" pin="IO_28" pad="48"/>
<connect gate="A" pin="IO_29" pad="6"/>
<connect gate="A" pin="IO_3" pad="16"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="41"/>
<connect gate="A" pin="IO_32" pad="50"/>
<connect gate="A" pin="IO_33" pad="7"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="8"/>
<connect gate="A" pin="IO_36" pad="51"/>
<connect gate="A" pin="IO_37" pad="52"/>
<connect gate="A" pin="IO_38" pad="53"/>
<connect gate="A" pin="IO_39" pad="54"/>
<connect gate="A" pin="IO_4" pad="17"/>
<connect gate="A" pin="IO_40" pad="55"/>
<connect gate="A" pin="IO_41" pad="56"/>
<connect gate="A" pin="IO_42" pad="66"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="68"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="69"/>
<connect gate="A" pin="IO_49" pad="70"/>
<connect gate="A" pin="IO_5" pad="18"/>
<connect gate="A" pin="IO_50" pad="71"/>
<connect gate="A" pin="IO_51" pad="72"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_58" pad="81"/>
<connect gate="A" pin="IO_59" pad="82"/>
<connect gate="A" pin="IO_6" pad="19"/>
<connect gate="A" pin="IO_60" pad="83"/>
<connect gate="A" pin="IO_61" pad="84"/>
<connect gate="A" pin="IO_62" pad="85"/>
<connect gate="A" pin="IO_63" pad="86"/>
<connect gate="A" pin="IO_64" pad="87"/>
<connect gate="A" pin="IO_65" pad="88"/>
<connect gate="A" pin="IO_66" pad="89"/>
<connect gate="A" pin="IO_67" pad="90"/>
<connect gate="A" pin="IO_68" pad="91"/>
<connect gate="A" pin="IO_69" pad="92"/>
<connect gate="A" pin="IO_7" pad="20"/>
<connect gate="A" pin="IO_70" pad="95"/>
<connect gate="A" pin="IO_71" pad="96"/>
<connect gate="A" pin="IO_72" pad="97"/>
<connect gate="A" pin="IO_73" pad="98"/>
<connect gate="A" pin="IO_74" pad="99"/>
<connect gate="A" pin="IO_8" pad="21"/>
<connect gate="A" pin="IO_9" pad="33"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCIO1" pad="31"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="45"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM240T100C3N"/>
<attribute name="OC_FARNELL" value="1549466"/>
<attribute name="OC_NEWARK" value="51R9356"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240T100C5N">
<description>IC CPLD FLASH 192 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM240T100C5N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="11"/>
<connect gate="A" pin="GNDINT_2" pad="65"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="46"/>
<connect gate="A" pin="GNDIO_3" pad="32"/>
<connect gate="A" pin="GNDIO_4" pad="60"/>
<connect gate="A" pin="GNDIO_5" pad="93"/>
<connect gate="A" pin="GNDIO_6" pad="10"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="34"/>
<connect gate="A" pin="IO_11" pad="35"/>
<connect gate="A" pin="IO_12" pad="1"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="36"/>
<connect gate="A" pin="IO_15" pad="2"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="37"/>
<connect gate="A" pin="IO_19" pad="3"/>
<connect gate="A" pin="IO_2" pad="15"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="30"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="4"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="5"/>
<connect gate="A" pin="IO_26" pad="47"/>
<connect gate="A" pin="IO_27" pad="40"/>
<connect gate="A" pin="IO_28" pad="48"/>
<connect gate="A" pin="IO_29" pad="6"/>
<connect gate="A" pin="IO_3" pad="16"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="41"/>
<connect gate="A" pin="IO_32" pad="50"/>
<connect gate="A" pin="IO_33" pad="7"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="8"/>
<connect gate="A" pin="IO_36" pad="51"/>
<connect gate="A" pin="IO_37" pad="52"/>
<connect gate="A" pin="IO_38" pad="53"/>
<connect gate="A" pin="IO_39" pad="54"/>
<connect gate="A" pin="IO_4" pad="17"/>
<connect gate="A" pin="IO_40" pad="55"/>
<connect gate="A" pin="IO_41" pad="56"/>
<connect gate="A" pin="IO_42" pad="66"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="68"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="69"/>
<connect gate="A" pin="IO_49" pad="70"/>
<connect gate="A" pin="IO_5" pad="18"/>
<connect gate="A" pin="IO_50" pad="71"/>
<connect gate="A" pin="IO_51" pad="72"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_58" pad="81"/>
<connect gate="A" pin="IO_59" pad="82"/>
<connect gate="A" pin="IO_6" pad="19"/>
<connect gate="A" pin="IO_60" pad="83"/>
<connect gate="A" pin="IO_61" pad="84"/>
<connect gate="A" pin="IO_62" pad="85"/>
<connect gate="A" pin="IO_63" pad="86"/>
<connect gate="A" pin="IO_64" pad="87"/>
<connect gate="A" pin="IO_65" pad="88"/>
<connect gate="A" pin="IO_66" pad="89"/>
<connect gate="A" pin="IO_67" pad="90"/>
<connect gate="A" pin="IO_68" pad="91"/>
<connect gate="A" pin="IO_69" pad="92"/>
<connect gate="A" pin="IO_7" pad="20"/>
<connect gate="A" pin="IO_70" pad="95"/>
<connect gate="A" pin="IO_71" pad="96"/>
<connect gate="A" pin="IO_72" pad="97"/>
<connect gate="A" pin="IO_73" pad="98"/>
<connect gate="A" pin="IO_74" pad="99"/>
<connect gate="A" pin="IO_8" pad="21"/>
<connect gate="A" pin="IO_9" pad="33"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCIO1" pad="31"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="45"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM240T100C5N"/>
<attribute name="OC_FARNELL" value="1453503"/>
<attribute name="OC_NEWARK" value="51R0496"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240T100I5N">
<description>IC CPLD FLASH 192 MACROCELL</description>
<gates>
<gate name="A" symbol="EPM240T100I5N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="11"/>
<connect gate="A" pin="GNDINT_2" pad="65"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="46"/>
<connect gate="A" pin="GNDIO_3" pad="32"/>
<connect gate="A" pin="GNDIO_4" pad="60"/>
<connect gate="A" pin="GNDIO_5" pad="93"/>
<connect gate="A" pin="GNDIO_6" pad="10"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="34"/>
<connect gate="A" pin="IO_11" pad="35"/>
<connect gate="A" pin="IO_12" pad="1"/>
<connect gate="A" pin="IO_13" pad="26"/>
<connect gate="A" pin="IO_14" pad="36"/>
<connect gate="A" pin="IO_15" pad="2"/>
<connect gate="A" pin="IO_16" pad="27"/>
<connect gate="A" pin="IO_17" pad="28"/>
<connect gate="A" pin="IO_18" pad="37"/>
<connect gate="A" pin="IO_19" pad="3"/>
<connect gate="A" pin="IO_2" pad="15"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="30"/>
<connect gate="A" pin="IO_22" pad="38"/>
<connect gate="A" pin="IO_23" pad="4"/>
<connect gate="A" pin="IO_24" pad="39"/>
<connect gate="A" pin="IO_25" pad="5"/>
<connect gate="A" pin="IO_26" pad="47"/>
<connect gate="A" pin="IO_27" pad="40"/>
<connect gate="A" pin="IO_28" pad="48"/>
<connect gate="A" pin="IO_29" pad="6"/>
<connect gate="A" pin="IO_3" pad="16"/>
<connect gate="A" pin="IO_30" pad="49"/>
<connect gate="A" pin="IO_31" pad="41"/>
<connect gate="A" pin="IO_32" pad="50"/>
<connect gate="A" pin="IO_33" pad="7"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="8"/>
<connect gate="A" pin="IO_36" pad="51"/>
<connect gate="A" pin="IO_37" pad="52"/>
<connect gate="A" pin="IO_38" pad="53"/>
<connect gate="A" pin="IO_39" pad="54"/>
<connect gate="A" pin="IO_4" pad="17"/>
<connect gate="A" pin="IO_40" pad="55"/>
<connect gate="A" pin="IO_41" pad="56"/>
<connect gate="A" pin="IO_42" pad="66"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="68"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="69"/>
<connect gate="A" pin="IO_49" pad="70"/>
<connect gate="A" pin="IO_5" pad="18"/>
<connect gate="A" pin="IO_50" pad="71"/>
<connect gate="A" pin="IO_51" pad="72"/>
<connect gate="A" pin="IO_52" pad="73"/>
<connect gate="A" pin="IO_53" pad="74"/>
<connect gate="A" pin="IO_54" pad="75"/>
<connect gate="A" pin="IO_55" pad="76"/>
<connect gate="A" pin="IO_56" pad="77"/>
<connect gate="A" pin="IO_57" pad="78"/>
<connect gate="A" pin="IO_58" pad="81"/>
<connect gate="A" pin="IO_59" pad="82"/>
<connect gate="A" pin="IO_6" pad="19"/>
<connect gate="A" pin="IO_60" pad="83"/>
<connect gate="A" pin="IO_61" pad="84"/>
<connect gate="A" pin="IO_62" pad="85"/>
<connect gate="A" pin="IO_63" pad="86"/>
<connect gate="A" pin="IO_64" pad="87"/>
<connect gate="A" pin="IO_65" pad="88"/>
<connect gate="A" pin="IO_66" pad="89"/>
<connect gate="A" pin="IO_67" pad="90"/>
<connect gate="A" pin="IO_68" pad="91"/>
<connect gate="A" pin="IO_69" pad="92"/>
<connect gate="A" pin="IO_7" pad="20"/>
<connect gate="A" pin="IO_70" pad="95"/>
<connect gate="A" pin="IO_71" pad="96"/>
<connect gate="A" pin="IO_72" pad="97"/>
<connect gate="A" pin="IO_73" pad="98"/>
<connect gate="A" pin="IO_74" pad="99"/>
<connect gate="A" pin="IO_8" pad="21"/>
<connect gate="A" pin="IO_9" pad="33"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCIO1" pad="31"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="45"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM240T100I5N"/>
<attribute name="OC_FARNELL" value="1549468"/>
<attribute name="OC_NEWARK" value="51R9360"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3032ALC44-10N">
<description>IC PLD EEPROM</description>
<gates>
<gate name="A" symbol="EPM3032ALC44-10N"/>
</gates>
<devices>
<device name="" package="PLCC127P1752X1752X457-44N">
<connects>
<connect gate="A" pin="GNDINT" pad="22"/>
<connect gate="A" pin="GNDINT_2" pad="42"/>
<connect gate="A" pin="GNDIO" pad="17"/>
<connect gate="A" pin="GNDIO_2" pad="10"/>
<connect gate="A" pin="GNDIO_3" pad="30"/>
<connect gate="A" pin="GNDIO_4" pad="36"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/GCLRN" pad="1"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="IO" pad="31"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDI" pad="7"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="19"/>
<connect gate="A" pin="IO_11" pad="11"/>
<connect gate="A" pin="IO_12" pad="20"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="33"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="34"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="37"/>
<connect gate="A" pin="IO_19" pad="25"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="26"/>
<connect gate="A" pin="IO_21" pad="39"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="40"/>
<connect gate="A" pin="IO_24" pad="28"/>
<connect gate="A" pin="IO_25" pad="41"/>
<connect gate="A" pin="IO_26" pad="29"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="14"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="16"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="18"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="VCCINT" pad="23"/>
<connect gate="A" pin="VCCINT_2" pad="3"/>
<connect gate="A" pin="VCCIO" pad="15"/>
<connect gate="A" pin="VCCIO_2" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3032ALC44-10N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R0499"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3032ATC44-4N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM3032ATC44-4N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="16"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCC_2" pad="17"/>
<connect gate="A" pin="VCC_3" pad="29"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3032ATC44-4N"/>
<attribute name="OC_FARNELL" value="1549414"/>
<attribute name="OC_NEWARK" value="51R0501"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3032ATC44-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM3032ATC44-7N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="16"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCC_2" pad="17"/>
<connect gate="A" pin="VCC_3" pad="29"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3032ATC44-7N"/>
<attribute name="OC_FARNELL" value="1549415"/>
<attribute name="OC_NEWARK" value="51R9374"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3032ATI44-10N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM3032ATI44-10N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="16"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCC_2" pad="17"/>
<connect gate="A" pin="VCC_3" pad="29"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3032ATI44-10N"/>
<attribute name="OC_FARNELL" value="1549416"/>
<attribute name="OC_NEWARK" value="51R9376"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ALC44-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ALC44-10N"/>
</gates>
<devices>
<device name="" package="PLCC127P1765X1765X457-44N">
<connects>
<connect gate="A" pin="GND" pad="42"/>
<connect gate="A" pin="GND_2" pad="17"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="30"/>
<connect gate="A" pin="GND_6" pad="36"/>
<connect gate="A" pin="I/O/TDI" pad="7"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/GCLRN" pad="1"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="IO" pad="31"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="39"/>
<connect gate="A" pin="IO_14" pad="16"/>
<connect gate="A" pin="IO_15" pad="40"/>
<connect gate="A" pin="IO_16" pad="18"/>
<connect gate="A" pin="IO_17" pad="41"/>
<connect gate="A" pin="IO_18" pad="19"/>
<connect gate="A" pin="IO_19" pad="20"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="21"/>
<connect gate="A" pin="IO_21" pad="24"/>
<connect gate="A" pin="IO_22" pad="25"/>
<connect gate="A" pin="IO_23" pad="26"/>
<connect gate="A" pin="IO_24" pad="27"/>
<connect gate="A" pin="IO_25" pad="28"/>
<connect gate="A" pin="IO_26" pad="29"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_5" pad="33"/>
<connect gate="A" pin="IO_6" pad="34"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="37"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="35"/>
<connect gate="A" pin="VCC_4" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ALC44-10N"/>
<attribute name="OC_FARNELL" value="1549412"/>
<attribute name="OC_NEWARK" value="51R0503"/>
<attribute name="PACKAGE" value="44-PLCC"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATC100-10N" prefix="U">
<description>IC MAX 3000A CPLD 64 100-TQFP</description>
<gates>
<gate name="A" symbol="EPM3064ATC100-10N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="65"/>
<connect gate="A" pin="GNDIO_10" pad="33"/>
<connect gate="A" pin="GNDIO_2" pad="53"/>
<connect gate="A" pin="GNDIO_3" pad="11"/>
<connect gate="A" pin="GNDIO_4" pad="26"/>
<connect gate="A" pin="GNDIO_5" pad="78"/>
<connect gate="A" pin="GNDIO_6" pad="95"/>
<connect gate="A" pin="GNDIO_7" pad="59"/>
<connect gate="A" pin="GNDIO_8" pad="74"/>
<connect gate="A" pin="GNDIO_9" pad="43"/>
<connect gate="A" pin="INPUT/*GCLR" pad="89"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="23"/>
<connect gate="A" pin="IO_11" pad="25"/>
<connect gate="A" pin="IO_12" pad="29"/>
<connect gate="A" pin="IO_13" pad="30"/>
<connect gate="A" pin="IO_14" pad="31"/>
<connect gate="A" pin="IO_15" pad="32"/>
<connect gate="A" pin="IO_16" pad="35"/>
<connect gate="A" pin="IO_17" pad="36"/>
<connect gate="A" pin="IO_18" pad="40"/>
<connect gate="A" pin="IO_19" pad="37"/>
<connect gate="A" pin="IO_2" pad="12"/>
<connect gate="A" pin="IO_20" pad="41"/>
<connect gate="A" pin="IO_21" pad="44"/>
<connect gate="A" pin="IO_22" pad="42"/>
<connect gate="A" pin="IO_23" pad="45"/>
<connect gate="A" pin="IO_24" pad="46"/>
<connect gate="A" pin="IO_25" pad="47"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="52"/>
<connect gate="A" pin="IO_28" pad="54"/>
<connect gate="A" pin="IO_29" pad="56"/>
<connect gate="A" pin="IO_3" pad="13"/>
<connect gate="A" pin="IO_30" pad="57"/>
<connect gate="A" pin="IO_31" pad="60"/>
<connect gate="A" pin="IO_32" pad="58"/>
<connect gate="A" pin="IO_33" pad="61"/>
<connect gate="A" pin="IO_34" pad="63"/>
<connect gate="A" pin="IO_35" pad="75"/>
<connect gate="A" pin="IO_36" pad="64"/>
<connect gate="A" pin="IO_37" pad="76"/>
<connect gate="A" pin="IO_38" pad="67"/>
<connect gate="A" pin="IO_39" pad="79"/>
<connect gate="A" pin="IO_4" pad="16"/>
<connect gate="A" pin="IO_40" pad="68"/>
<connect gate="A" pin="IO_41" pad="80"/>
<connect gate="A" pin="IO_42" pad="71"/>
<connect gate="A" pin="IO_43" pad="83"/>
<connect gate="A" pin="IO_44" pad="69"/>
<connect gate="A" pin="IO_45" pad="81"/>
<connect gate="A" pin="IO_46" pad="84"/>
<connect gate="A" pin="IO_47" pad="85"/>
<connect gate="A" pin="IO_48" pad="6"/>
<connect gate="A" pin="IO_49" pad="8"/>
<connect gate="A" pin="IO_5" pad="14"/>
<connect gate="A" pin="IO_50" pad="9"/>
<connect gate="A" pin="IO_51" pad="10"/>
<connect gate="A" pin="IO_52" pad="92"/>
<connect gate="A" pin="IO_53" pad="93"/>
<connect gate="A" pin="IO_54" pad="94"/>
<connect gate="A" pin="IO_55" pad="96"/>
<connect gate="A" pin="IO_56" pad="97"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="19"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_8" pad="20"/>
<connect gate="A" pin="IO_9" pad="21"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="N.C._10" pad="77"/>
<connect gate="A" pin="N.C._11" pad="50"/>
<connect gate="A" pin="N.C._12" pad="1"/>
<connect gate="A" pin="N.C._13" pad="7"/>
<connect gate="A" pin="N.C._14" pad="2"/>
<connect gate="A" pin="N.C._2" pad="24"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="27"/>
<connect gate="A" pin="N.C._5" pad="70"/>
<connect gate="A" pin="N.C._6" pad="22"/>
<connect gate="A" pin="N.C._7" pad="72"/>
<connect gate="A" pin="N.C._8" pad="49"/>
<connect gate="A" pin="N.C._9" pad="28"/>
<connect gate="A" pin="VCCINT" pad="91"/>
<connect gate="A" pin="VCCINT_2" pad="39"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="51"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATC100-10N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R0504"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATC100-4N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATC100-4N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="86"/>
<connect gate="A" pin="GNDINT_2" pad="38"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_10" pad="43"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="53"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="65"/>
<connect gate="A" pin="GNDIO_7" pad="74"/>
<connect gate="A" pin="GNDIO_8" pad="78"/>
<connect gate="A" pin="GNDIO_9" pad="26"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="60"/>
<connect gate="A" pin="IO_12" pad="61"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="13"/>
<connect gate="A" pin="IO_15" pad="63"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="64"/>
<connect gate="A" pin="IO_18" pad="16"/>
<connect gate="A" pin="IO_19" pad="17"/>
<connect gate="A" pin="IO_2" pad="52"/>
<connect gate="A" pin="IO_20" pad="67"/>
<connect gate="A" pin="IO_21" pad="68"/>
<connect gate="A" pin="IO_22" pad="19"/>
<connect gate="A" pin="IO_23" pad="69"/>
<connect gate="A" pin="IO_24" pad="20"/>
<connect gate="A" pin="IO_25" pad="21"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="23"/>
<connect gate="A" pin="IO_28" pad="25"/>
<connect gate="A" pin="IO_29" pad="75"/>
<connect gate="A" pin="IO_3" pad="54"/>
<connect gate="A" pin="IO_30" pad="76"/>
<connect gate="A" pin="IO_31" pad="29"/>
<connect gate="A" pin="IO_32" pad="79"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="31"/>
<connect gate="A" pin="IO_36" pad="81"/>
<connect gate="A" pin="IO_37" pad="32"/>
<connect gate="A" pin="IO_38" pad="83"/>
<connect gate="A" pin="IO_39" pad="84"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="35"/>
<connect gate="A" pin="IO_41" pad="85"/>
<connect gate="A" pin="IO_42" pad="36"/>
<connect gate="A" pin="IO_43" pad="37"/>
<connect gate="A" pin="IO_44" pad="40"/>
<connect gate="A" pin="IO_45" pad="41"/>
<connect gate="A" pin="IO_46" pad="42"/>
<connect gate="A" pin="IO_47" pad="92"/>
<connect gate="A" pin="IO_48" pad="93"/>
<connect gate="A" pin="IO_49" pad="44"/>
<connect gate="A" pin="IO_5" pad="56"/>
<connect gate="A" pin="IO_50" pad="94"/>
<connect gate="A" pin="IO_51" pad="45"/>
<connect gate="A" pin="IO_52" pad="46"/>
<connect gate="A" pin="IO_53" pad="96"/>
<connect gate="A" pin="IO_54" pad="47"/>
<connect gate="A" pin="IO_55" pad="97"/>
<connect gate="A" pin="IO_56" pad="48"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="57"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="58"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="N.C." pad="28"/>
<connect gate="A" pin="N.C._10" pad="22"/>
<connect gate="A" pin="N.C._11" pad="72"/>
<connect gate="A" pin="N.C._12" pad="24"/>
<connect gate="A" pin="N.C._13" pad="27"/>
<connect gate="A" pin="N.C._14" pad="77"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="1"/>
<connect gate="A" pin="N.C._5" pad="49"/>
<connect gate="A" pin="N.C._6" pad="70"/>
<connect gate="A" pin="N.C._7" pad="2"/>
<connect gate="A" pin="N.C._8" pad="50"/>
<connect gate="A" pin="N.C._9" pad="7"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="66"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="51"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATC100-4N"/>
<attribute name="OC_FARNELL" value="1549405"/>
<attribute name="OC_NEWARK" value="51R9385"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATC100-7N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATC100-7N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="86"/>
<connect gate="A" pin="GNDINT_2" pad="38"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_10" pad="43"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="53"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="65"/>
<connect gate="A" pin="GNDIO_7" pad="74"/>
<connect gate="A" pin="GNDIO_8" pad="78"/>
<connect gate="A" pin="GNDIO_9" pad="26"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="60"/>
<connect gate="A" pin="IO_12" pad="61"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="13"/>
<connect gate="A" pin="IO_15" pad="63"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="64"/>
<connect gate="A" pin="IO_18" pad="16"/>
<connect gate="A" pin="IO_19" pad="17"/>
<connect gate="A" pin="IO_2" pad="52"/>
<connect gate="A" pin="IO_20" pad="67"/>
<connect gate="A" pin="IO_21" pad="68"/>
<connect gate="A" pin="IO_22" pad="19"/>
<connect gate="A" pin="IO_23" pad="69"/>
<connect gate="A" pin="IO_24" pad="20"/>
<connect gate="A" pin="IO_25" pad="21"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="23"/>
<connect gate="A" pin="IO_28" pad="25"/>
<connect gate="A" pin="IO_29" pad="75"/>
<connect gate="A" pin="IO_3" pad="54"/>
<connect gate="A" pin="IO_30" pad="76"/>
<connect gate="A" pin="IO_31" pad="29"/>
<connect gate="A" pin="IO_32" pad="79"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="31"/>
<connect gate="A" pin="IO_36" pad="81"/>
<connect gate="A" pin="IO_37" pad="32"/>
<connect gate="A" pin="IO_38" pad="83"/>
<connect gate="A" pin="IO_39" pad="84"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="35"/>
<connect gate="A" pin="IO_41" pad="85"/>
<connect gate="A" pin="IO_42" pad="36"/>
<connect gate="A" pin="IO_43" pad="37"/>
<connect gate="A" pin="IO_44" pad="40"/>
<connect gate="A" pin="IO_45" pad="41"/>
<connect gate="A" pin="IO_46" pad="42"/>
<connect gate="A" pin="IO_47" pad="92"/>
<connect gate="A" pin="IO_48" pad="93"/>
<connect gate="A" pin="IO_49" pad="44"/>
<connect gate="A" pin="IO_5" pad="56"/>
<connect gate="A" pin="IO_50" pad="94"/>
<connect gate="A" pin="IO_51" pad="45"/>
<connect gate="A" pin="IO_52" pad="46"/>
<connect gate="A" pin="IO_53" pad="96"/>
<connect gate="A" pin="IO_54" pad="47"/>
<connect gate="A" pin="IO_55" pad="97"/>
<connect gate="A" pin="IO_56" pad="48"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="57"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="58"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="N.C." pad="28"/>
<connect gate="A" pin="N.C._10" pad="22"/>
<connect gate="A" pin="N.C._11" pad="72"/>
<connect gate="A" pin="N.C._12" pad="24"/>
<connect gate="A" pin="N.C._13" pad="27"/>
<connect gate="A" pin="N.C._14" pad="77"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="1"/>
<connect gate="A" pin="N.C._5" pad="49"/>
<connect gate="A" pin="N.C._6" pad="70"/>
<connect gate="A" pin="N.C._7" pad="2"/>
<connect gate="A" pin="N.C._8" pad="50"/>
<connect gate="A" pin="N.C._9" pad="7"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="66"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="51"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATC100-7N"/>
<attribute name="OC_FARNELL" value="1549407"/>
<attribute name="OC_NEWARK" value="51R9387"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATC44-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATC44-10N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="16"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLR" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATC44-10N"/>
<attribute name="OC_FARNELL" value="1549417"/>
<attribute name="OC_NEWARK" value="51R0505"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATC44-4N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATC44-4N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="16"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLR" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATC44-4N"/>
<attribute name="OC_FARNELL" value="1549419"/>
<attribute name="OC_NEWARK" value="51R0506"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATC44-7N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATC44-7N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="16"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLR" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATC44-7N"/>
<attribute name="OC_FARNELL" value="1549422"/>
<attribute name="OC_NEWARK" value="51R9391"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATI100-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATI100-10N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="86"/>
<connect gate="A" pin="GNDINT_2" pad="38"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_10" pad="43"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="53"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="65"/>
<connect gate="A" pin="GNDIO_7" pad="74"/>
<connect gate="A" pin="GNDIO_8" pad="78"/>
<connect gate="A" pin="GNDIO_9" pad="26"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="60"/>
<connect gate="A" pin="IO_12" pad="61"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="13"/>
<connect gate="A" pin="IO_15" pad="63"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="64"/>
<connect gate="A" pin="IO_18" pad="16"/>
<connect gate="A" pin="IO_19" pad="17"/>
<connect gate="A" pin="IO_2" pad="52"/>
<connect gate="A" pin="IO_20" pad="67"/>
<connect gate="A" pin="IO_21" pad="68"/>
<connect gate="A" pin="IO_22" pad="19"/>
<connect gate="A" pin="IO_23" pad="69"/>
<connect gate="A" pin="IO_24" pad="20"/>
<connect gate="A" pin="IO_25" pad="21"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="23"/>
<connect gate="A" pin="IO_28" pad="25"/>
<connect gate="A" pin="IO_29" pad="75"/>
<connect gate="A" pin="IO_3" pad="54"/>
<connect gate="A" pin="IO_30" pad="76"/>
<connect gate="A" pin="IO_31" pad="29"/>
<connect gate="A" pin="IO_32" pad="79"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="31"/>
<connect gate="A" pin="IO_36" pad="81"/>
<connect gate="A" pin="IO_37" pad="32"/>
<connect gate="A" pin="IO_38" pad="83"/>
<connect gate="A" pin="IO_39" pad="84"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="35"/>
<connect gate="A" pin="IO_41" pad="85"/>
<connect gate="A" pin="IO_42" pad="36"/>
<connect gate="A" pin="IO_43" pad="37"/>
<connect gate="A" pin="IO_44" pad="40"/>
<connect gate="A" pin="IO_45" pad="41"/>
<connect gate="A" pin="IO_46" pad="42"/>
<connect gate="A" pin="IO_47" pad="92"/>
<connect gate="A" pin="IO_48" pad="93"/>
<connect gate="A" pin="IO_49" pad="44"/>
<connect gate="A" pin="IO_5" pad="56"/>
<connect gate="A" pin="IO_50" pad="94"/>
<connect gate="A" pin="IO_51" pad="45"/>
<connect gate="A" pin="IO_52" pad="46"/>
<connect gate="A" pin="IO_53" pad="96"/>
<connect gate="A" pin="IO_54" pad="47"/>
<connect gate="A" pin="IO_55" pad="97"/>
<connect gate="A" pin="IO_56" pad="48"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="57"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="58"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="N.C." pad="28"/>
<connect gate="A" pin="N.C._10" pad="22"/>
<connect gate="A" pin="N.C._11" pad="72"/>
<connect gate="A" pin="N.C._12" pad="24"/>
<connect gate="A" pin="N.C._13" pad="27"/>
<connect gate="A" pin="N.C._14" pad="77"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="1"/>
<connect gate="A" pin="N.C._5" pad="49"/>
<connect gate="A" pin="N.C._6" pad="70"/>
<connect gate="A" pin="N.C._7" pad="2"/>
<connect gate="A" pin="N.C._8" pad="50"/>
<connect gate="A" pin="N.C._9" pad="7"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="66"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="51"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATI100-10N"/>
<attribute name="OC_FARNELL" value="1549410"/>
<attribute name="OC_NEWARK" value="51R9393"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3064ATI44-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3064ATI44-10N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="16"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLR" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="23"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="33"/>
<connect gate="A" pin="IO_23" pad="34"/>
<connect gate="A" pin="IO_24" pad="35"/>
<connect gate="A" pin="IO_25" pad="42"/>
<connect gate="A" pin="IO_26" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="13"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3064ATI44-10N"/>
<attribute name="OC_FARNELL" value="1549423"/>
<attribute name="OC_NEWARK" value="51R9395"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3128ATC100-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3128ATC100-10N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="86"/>
<connect gate="A" pin="GNDINT_2" pad="38"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_10" pad="43"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="53"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="65"/>
<connect gate="A" pin="GNDIO_7" pad="74"/>
<connect gate="A" pin="GNDIO_8" pad="78"/>
<connect gate="A" pin="GNDIO_9" pad="26"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="60"/>
<connect gate="A" pin="IO_12" pad="61"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="13"/>
<connect gate="A" pin="IO_15" pad="63"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="64"/>
<connect gate="A" pin="IO_18" pad="16"/>
<connect gate="A" pin="IO_19" pad="17"/>
<connect gate="A" pin="IO_2" pad="52"/>
<connect gate="A" pin="IO_20" pad="67"/>
<connect gate="A" pin="IO_21" pad="68"/>
<connect gate="A" pin="IO_22" pad="19"/>
<connect gate="A" pin="IO_23" pad="69"/>
<connect gate="A" pin="IO_24" pad="20"/>
<connect gate="A" pin="IO_25" pad="21"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="23"/>
<connect gate="A" pin="IO_28" pad="25"/>
<connect gate="A" pin="IO_29" pad="75"/>
<connect gate="A" pin="IO_3" pad="54"/>
<connect gate="A" pin="IO_30" pad="76"/>
<connect gate="A" pin="IO_31" pad="29"/>
<connect gate="A" pin="IO_32" pad="79"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="31"/>
<connect gate="A" pin="IO_36" pad="81"/>
<connect gate="A" pin="IO_37" pad="32"/>
<connect gate="A" pin="IO_38" pad="83"/>
<connect gate="A" pin="IO_39" pad="84"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="35"/>
<connect gate="A" pin="IO_41" pad="85"/>
<connect gate="A" pin="IO_42" pad="36"/>
<connect gate="A" pin="IO_43" pad="37"/>
<connect gate="A" pin="IO_44" pad="40"/>
<connect gate="A" pin="IO_45" pad="41"/>
<connect gate="A" pin="IO_46" pad="42"/>
<connect gate="A" pin="IO_47" pad="92"/>
<connect gate="A" pin="IO_48" pad="93"/>
<connect gate="A" pin="IO_49" pad="44"/>
<connect gate="A" pin="IO_5" pad="56"/>
<connect gate="A" pin="IO_50" pad="94"/>
<connect gate="A" pin="IO_51" pad="45"/>
<connect gate="A" pin="IO_52" pad="46"/>
<connect gate="A" pin="IO_53" pad="96"/>
<connect gate="A" pin="IO_54" pad="47"/>
<connect gate="A" pin="IO_55" pad="97"/>
<connect gate="A" pin="IO_56" pad="48"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="57"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="58"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="N.C." pad="28"/>
<connect gate="A" pin="N.C._10" pad="22"/>
<connect gate="A" pin="N.C._11" pad="72"/>
<connect gate="A" pin="N.C._12" pad="24"/>
<connect gate="A" pin="N.C._13" pad="27"/>
<connect gate="A" pin="N.C._14" pad="77"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="1"/>
<connect gate="A" pin="N.C._5" pad="49"/>
<connect gate="A" pin="N.C._6" pad="70"/>
<connect gate="A" pin="N.C._7" pad="2"/>
<connect gate="A" pin="N.C._8" pad="50"/>
<connect gate="A" pin="N.C._9" pad="7"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="66"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="51"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3128ATC100-10N"/>
<attribute name="OC_FARNELL" value="1453461"/>
<attribute name="OC_NEWARK" value="51R0507"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3128ATC100-5N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3128ATC100-5N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="86"/>
<connect gate="A" pin="GNDINT_2" pad="38"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_10" pad="43"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="53"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="65"/>
<connect gate="A" pin="GNDIO_7" pad="74"/>
<connect gate="A" pin="GNDIO_8" pad="78"/>
<connect gate="A" pin="GNDIO_9" pad="26"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="60"/>
<connect gate="A" pin="IO_12" pad="61"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="13"/>
<connect gate="A" pin="IO_15" pad="63"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="64"/>
<connect gate="A" pin="IO_18" pad="16"/>
<connect gate="A" pin="IO_19" pad="17"/>
<connect gate="A" pin="IO_2" pad="52"/>
<connect gate="A" pin="IO_20" pad="67"/>
<connect gate="A" pin="IO_21" pad="68"/>
<connect gate="A" pin="IO_22" pad="19"/>
<connect gate="A" pin="IO_23" pad="69"/>
<connect gate="A" pin="IO_24" pad="20"/>
<connect gate="A" pin="IO_25" pad="21"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="23"/>
<connect gate="A" pin="IO_28" pad="25"/>
<connect gate="A" pin="IO_29" pad="75"/>
<connect gate="A" pin="IO_3" pad="54"/>
<connect gate="A" pin="IO_30" pad="76"/>
<connect gate="A" pin="IO_31" pad="29"/>
<connect gate="A" pin="IO_32" pad="79"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="31"/>
<connect gate="A" pin="IO_36" pad="81"/>
<connect gate="A" pin="IO_37" pad="32"/>
<connect gate="A" pin="IO_38" pad="83"/>
<connect gate="A" pin="IO_39" pad="84"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="35"/>
<connect gate="A" pin="IO_41" pad="85"/>
<connect gate="A" pin="IO_42" pad="36"/>
<connect gate="A" pin="IO_43" pad="37"/>
<connect gate="A" pin="IO_44" pad="40"/>
<connect gate="A" pin="IO_45" pad="41"/>
<connect gate="A" pin="IO_46" pad="42"/>
<connect gate="A" pin="IO_47" pad="92"/>
<connect gate="A" pin="IO_48" pad="93"/>
<connect gate="A" pin="IO_49" pad="44"/>
<connect gate="A" pin="IO_5" pad="56"/>
<connect gate="A" pin="IO_50" pad="94"/>
<connect gate="A" pin="IO_51" pad="45"/>
<connect gate="A" pin="IO_52" pad="46"/>
<connect gate="A" pin="IO_53" pad="96"/>
<connect gate="A" pin="IO_54" pad="47"/>
<connect gate="A" pin="IO_55" pad="97"/>
<connect gate="A" pin="IO_56" pad="48"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="57"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="58"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="N.C." pad="28"/>
<connect gate="A" pin="N.C._10" pad="22"/>
<connect gate="A" pin="N.C._11" pad="72"/>
<connect gate="A" pin="N.C._12" pad="24"/>
<connect gate="A" pin="N.C._13" pad="27"/>
<connect gate="A" pin="N.C._14" pad="77"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="1"/>
<connect gate="A" pin="N.C._5" pad="49"/>
<connect gate="A" pin="N.C._6" pad="70"/>
<connect gate="A" pin="N.C._7" pad="2"/>
<connect gate="A" pin="N.C._8" pad="50"/>
<connect gate="A" pin="N.C._9" pad="7"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="66"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="51"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3128ATC100-5N"/>
<attribute name="OC_FARNELL" value="1549408"/>
<attribute name="OC_NEWARK" value="51R9401"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3128ATC100-7N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3128ATC100-7N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="86"/>
<connect gate="A" pin="GNDINT_2" pad="38"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_10" pad="43"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="53"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="65"/>
<connect gate="A" pin="GNDIO_7" pad="74"/>
<connect gate="A" pin="GNDIO_8" pad="78"/>
<connect gate="A" pin="GNDIO_9" pad="26"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="10"/>
<connect gate="A" pin="IO_11" pad="60"/>
<connect gate="A" pin="IO_12" pad="61"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="13"/>
<connect gate="A" pin="IO_15" pad="63"/>
<connect gate="A" pin="IO_16" pad="14"/>
<connect gate="A" pin="IO_17" pad="64"/>
<connect gate="A" pin="IO_18" pad="16"/>
<connect gate="A" pin="IO_19" pad="17"/>
<connect gate="A" pin="IO_2" pad="52"/>
<connect gate="A" pin="IO_20" pad="67"/>
<connect gate="A" pin="IO_21" pad="68"/>
<connect gate="A" pin="IO_22" pad="19"/>
<connect gate="A" pin="IO_23" pad="69"/>
<connect gate="A" pin="IO_24" pad="20"/>
<connect gate="A" pin="IO_25" pad="21"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="23"/>
<connect gate="A" pin="IO_28" pad="25"/>
<connect gate="A" pin="IO_29" pad="75"/>
<connect gate="A" pin="IO_3" pad="54"/>
<connect gate="A" pin="IO_30" pad="76"/>
<connect gate="A" pin="IO_31" pad="29"/>
<connect gate="A" pin="IO_32" pad="79"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="31"/>
<connect gate="A" pin="IO_36" pad="81"/>
<connect gate="A" pin="IO_37" pad="32"/>
<connect gate="A" pin="IO_38" pad="83"/>
<connect gate="A" pin="IO_39" pad="84"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="35"/>
<connect gate="A" pin="IO_41" pad="85"/>
<connect gate="A" pin="IO_42" pad="36"/>
<connect gate="A" pin="IO_43" pad="37"/>
<connect gate="A" pin="IO_44" pad="40"/>
<connect gate="A" pin="IO_45" pad="41"/>
<connect gate="A" pin="IO_46" pad="42"/>
<connect gate="A" pin="IO_47" pad="92"/>
<connect gate="A" pin="IO_48" pad="93"/>
<connect gate="A" pin="IO_49" pad="44"/>
<connect gate="A" pin="IO_5" pad="56"/>
<connect gate="A" pin="IO_50" pad="94"/>
<connect gate="A" pin="IO_51" pad="45"/>
<connect gate="A" pin="IO_52" pad="46"/>
<connect gate="A" pin="IO_53" pad="96"/>
<connect gate="A" pin="IO_54" pad="47"/>
<connect gate="A" pin="IO_55" pad="97"/>
<connect gate="A" pin="IO_56" pad="48"/>
<connect gate="A" pin="IO_57" pad="98"/>
<connect gate="A" pin="IO_58" pad="99"/>
<connect gate="A" pin="IO_6" pad="57"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="58"/>
<connect gate="A" pin="IO_9" pad="9"/>
<connect gate="A" pin="N.C." pad="28"/>
<connect gate="A" pin="N.C._10" pad="22"/>
<connect gate="A" pin="N.C._11" pad="72"/>
<connect gate="A" pin="N.C._12" pad="24"/>
<connect gate="A" pin="N.C._13" pad="27"/>
<connect gate="A" pin="N.C._14" pad="77"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="55"/>
<connect gate="A" pin="N.C._4" pad="1"/>
<connect gate="A" pin="N.C._5" pad="49"/>
<connect gate="A" pin="N.C._6" pad="70"/>
<connect gate="A" pin="N.C._7" pad="2"/>
<connect gate="A" pin="N.C._8" pad="50"/>
<connect gate="A" pin="N.C._9" pad="7"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="34"/>
<connect gate="A" pin="VCCIO_2" pad="18"/>
<connect gate="A" pin="VCCIO_3" pad="66"/>
<connect gate="A" pin="VCCIO_4" pad="3"/>
<connect gate="A" pin="VCCIO_5" pad="51"/>
<connect gate="A" pin="VCCIO_6" pad="82"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3128ATC100-7N"/>
<attribute name="OC_FARNELL" value="1549409"/>
<attribute name="OC_NEWARK" value="51R0508"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3128ATC144-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3128ATC144-10N_A"/>
<gate name="B" symbol="EPM3128ATC144-10N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="17"/>
<connect gate="A" pin="GNDIO_2" pad="59"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="26"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="3"/>
<connect gate="A" pin="GNDIO_7" pad="13"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="25"/>
<connect gate="A" pin="IO_17" pad="27"/>
<connect gate="A" pin="IO_18" pad="28"/>
<connect gate="A" pin="IO_19" pad="29"/>
<connect gate="A" pin="IO_2" pad="5"/>
<connect gate="A" pin="IO_20" pad="30"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="32"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="6"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="53"/>
<connect gate="A" pin="IO_32" pad="54"/>
<connect gate="A" pin="IO_33" pad="55"/>
<connect gate="A" pin="IO_34" pad="56"/>
<connect gate="A" pin="IO_35" pad="60"/>
<connect gate="A" pin="IO_36" pad="61"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_44" pad="71"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="N.C." pad="49"/>
<connect gate="A" pin="N.C._10" pad="46"/>
<connect gate="A" pin="N.C._11" pad="47"/>
<connect gate="A" pin="N.C._12" pad="12"/>
<connect gate="A" pin="N.C._13" pad="48"/>
<connect gate="A" pin="N.C._2" pad="34"/>
<connect gate="A" pin="N.C._3" pad="66"/>
<connect gate="A" pin="N.C._4" pad="19"/>
<connect gate="A" pin="N.C._5" pad="35"/>
<connect gate="A" pin="N.C._6" pad="36"/>
<connect gate="A" pin="N.C._7" pad="1"/>
<connect gate="A" pin="N.C._8" pad="43"/>
<connect gate="A" pin="N.C._9" pad="2"/>
<connect gate="A" pin="VCCINT" pad="58"/>
<connect gate="A" pin="VCCINT_2" pad="51"/>
<connect gate="A" pin="VCCIO" pad="50"/>
<connect gate="A" pin="VCCIO_2" pad="24"/>
<connect gate="B" pin="GNDINT" pad="124"/>
<connect gate="B" pin="GNDINT_2" pad="129"/>
<connect gate="B" pin="GNDIO" pad="114"/>
<connect gate="B" pin="GNDIO_2" pad="135"/>
<connect gate="B" pin="GNDIO_3" pad="77"/>
<connect gate="B" pin="GNDIO_4" pad="105"/>
<connect gate="B" pin="GNDIO_5" pad="85"/>
<connect gate="B" pin="GNDIO_6" pad="94"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/GCLR" pad="127"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="143"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="91"/>
<connect gate="B" pin="IO_14" pad="92"/>
<connect gate="B" pin="IO_15" pad="93"/>
<connect gate="B" pin="IO_16" pad="96"/>
<connect gate="B" pin="IO_17" pad="97"/>
<connect gate="B" pin="IO_18" pad="98"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="109"/>
<connect gate="B" pin="IO_26" pad="110"/>
<connect gate="B" pin="IO_27" pad="111"/>
<connect gate="B" pin="IO_28" pad="112"/>
<connect gate="B" pin="IO_29" pad="113"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="117"/>
<connect gate="B" pin="IO_32" pad="118"/>
<connect gate="B" pin="IO_33" pad="119"/>
<connect gate="B" pin="IO_34" pad="131"/>
<connect gate="B" pin="IO_35" pad="132"/>
<connect gate="B" pin="IO_36" pad="133"/>
<connect gate="B" pin="IO_37" pad="134"/>
<connect gate="B" pin="IO_38" pad="136"/>
<connect gate="B" pin="IO_39" pad="137"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_40" pad="138"/>
<connect gate="B" pin="IO_41" pad="139"/>
<connect gate="B" pin="IO_42" pad="140"/>
<connect gate="B" pin="IO_43" pad="141"/>
<connect gate="B" pin="IO_44" pad="142"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="84"/>
<connect gate="B" pin="N.C." pad="103"/>
<connect gate="B" pin="N.C._2" pad="75"/>
<connect gate="B" pin="N.C._3" pad="120"/>
<connect gate="B" pin="N.C._4" pad="90"/>
<connect gate="B" pin="N.C._5" pad="121"/>
<connect gate="B" pin="N.C._6" pad="108"/>
<connect gate="B" pin="N.C._7" pad="122"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="123"/>
<connect gate="B" pin="VCCIO" pad="115"/>
<connect gate="B" pin="VCCIO_2" pad="144"/>
<connect gate="B" pin="VCCIO_3" pad="73"/>
<connect gate="B" pin="VCCIO_4" pad="76"/>
<connect gate="B" pin="VCCIO_5" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3128ATC144-10N"/>
<attribute name="OC_FARNELL" value="1549411"/>
<attribute name="OC_NEWARK" value="51R0509"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3128ATC144-5N">
<description>IC MAX 3000A CPLD 128 144-TQFP</description>
<gates>
<gate name="A" symbol="EPM3128ATC144-5N_A"/>
<gate name="B" symbol="EPM3128ATC144-5N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="13"/>
<connect gate="A" pin="GNDIO_2" pad="3"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="17"/>
<connect gate="A" pin="GNDIO_5" pad="26"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="GNDIO_7" pad="33"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="25"/>
<connect gate="A" pin="IO_17" pad="27"/>
<connect gate="A" pin="IO_18" pad="28"/>
<connect gate="A" pin="IO_19" pad="29"/>
<connect gate="A" pin="IO_2" pad="5"/>
<connect gate="A" pin="IO_20" pad="30"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="32"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="6"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="53"/>
<connect gate="A" pin="IO_32" pad="54"/>
<connect gate="A" pin="IO_33" pad="55"/>
<connect gate="A" pin="IO_34" pad="56"/>
<connect gate="A" pin="IO_35" pad="60"/>
<connect gate="A" pin="IO_36" pad="61"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_44" pad="71"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="N.C." pad="19"/>
<connect gate="A" pin="N.C._10" pad="35"/>
<connect gate="A" pin="N.C._11" pad="36"/>
<connect gate="A" pin="N.C._12" pad="66"/>
<connect gate="A" pin="N.C._13" pad="12"/>
<connect gate="A" pin="N.C._2" pad="1"/>
<connect gate="A" pin="N.C._3" pad="2"/>
<connect gate="A" pin="N.C._4" pad="49"/>
<connect gate="A" pin="N.C._5" pad="48"/>
<connect gate="A" pin="N.C._6" pad="47"/>
<connect gate="A" pin="N.C._7" pad="46"/>
<connect gate="A" pin="N.C._8" pad="43"/>
<connect gate="A" pin="N.C._9" pad="34"/>
<connect gate="A" pin="VCCINT" pad="51"/>
<connect gate="A" pin="VCCINT_2" pad="58"/>
<connect gate="A" pin="VCCIO" pad="24"/>
<connect gate="A" pin="VCCIO_2" pad="50"/>
<connect gate="B" pin="GNDINT" pad="129"/>
<connect gate="B" pin="GNDINT_2" pad="124"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="94"/>
<connect gate="B" pin="GNDIO_3" pad="77"/>
<connect gate="B" pin="GNDIO_4" pad="85"/>
<connect gate="B" pin="GNDIO_5" pad="105"/>
<connect gate="B" pin="GNDIO_6" pad="114"/>
<connect gate="B" pin="INPUT/*GCLR" pad="127"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="74"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="88"/>
<connect gate="B" pin="IO_11" pad="91"/>
<connect gate="B" pin="IO_12" pad="92"/>
<connect gate="B" pin="IO_13" pad="93"/>
<connect gate="B" pin="IO_14" pad="96"/>
<connect gate="B" pin="IO_15" pad="97"/>
<connect gate="B" pin="IO_16" pad="98"/>
<connect gate="B" pin="IO_17" pad="99"/>
<connect gate="B" pin="IO_18" pad="100"/>
<connect gate="B" pin="IO_19" pad="101"/>
<connect gate="B" pin="IO_2" pad="79"/>
<connect gate="B" pin="IO_20" pad="102"/>
<connect gate="B" pin="IO_21" pad="106"/>
<connect gate="B" pin="IO_22" pad="107"/>
<connect gate="B" pin="IO_23" pad="109"/>
<connect gate="B" pin="IO_24" pad="110"/>
<connect gate="B" pin="IO_25" pad="111"/>
<connect gate="B" pin="IO_26" pad="112"/>
<connect gate="B" pin="IO_27" pad="113"/>
<connect gate="B" pin="IO_28" pad="116"/>
<connect gate="B" pin="IO_29" pad="117"/>
<connect gate="B" pin="IO_3" pad="80"/>
<connect gate="B" pin="IO_30" pad="118"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="131"/>
<connect gate="B" pin="IO_33" pad="132"/>
<connect gate="B" pin="IO_34" pad="133"/>
<connect gate="B" pin="IO_35" pad="134"/>
<connect gate="B" pin="IO_36" pad="136"/>
<connect gate="B" pin="IO_37" pad="137"/>
<connect gate="B" pin="IO_38" pad="138"/>
<connect gate="B" pin="IO_39" pad="139"/>
<connect gate="B" pin="IO_4" pad="81"/>
<connect gate="B" pin="IO_40" pad="140"/>
<connect gate="B" pin="IO_41" pad="141"/>
<connect gate="B" pin="IO_42" pad="142"/>
<connect gate="B" pin="IO_43" pad="143"/>
<connect gate="B" pin="IO_44" pad="78"/>
<connect gate="B" pin="IO_5" pad="82"/>
<connect gate="B" pin="IO_6" pad="83"/>
<connect gate="B" pin="IO_7" pad="84"/>
<connect gate="B" pin="IO_8" pad="86"/>
<connect gate="B" pin="IO_9" pad="87"/>
<connect gate="B" pin="N.C." pad="122"/>
<connect gate="B" pin="N.C._2" pad="103"/>
<connect gate="B" pin="N.C._3" pad="90"/>
<connect gate="B" pin="N.C._4" pad="75"/>
<connect gate="B" pin="N.C._5" pad="108"/>
<connect gate="B" pin="N.C._6" pad="120"/>
<connect gate="B" pin="N.C._7" pad="121"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="130"/>
<connect gate="B" pin="VCCIO" pad="95"/>
<connect gate="B" pin="VCCIO_2" pad="144"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
<connect gate="B" pin="VCCIO_4" pad="76"/>
<connect gate="B" pin="VCCIO_5" pad="73"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3128ATC144-5N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9405"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3128ATC144-7N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3128ATC144-7N_A"/>
<gate name="B" symbol="EPM3128ATC144-7N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="17"/>
<connect gate="A" pin="GNDIO_2" pad="59"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="26"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="3"/>
<connect gate="A" pin="GNDIO_7" pad="13"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="25"/>
<connect gate="A" pin="IO_17" pad="27"/>
<connect gate="A" pin="IO_18" pad="28"/>
<connect gate="A" pin="IO_19" pad="29"/>
<connect gate="A" pin="IO_2" pad="5"/>
<connect gate="A" pin="IO_20" pad="30"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="32"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="6"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="53"/>
<connect gate="A" pin="IO_32" pad="54"/>
<connect gate="A" pin="IO_33" pad="55"/>
<connect gate="A" pin="IO_34" pad="56"/>
<connect gate="A" pin="IO_35" pad="60"/>
<connect gate="A" pin="IO_36" pad="61"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_44" pad="71"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="N.C." pad="49"/>
<connect gate="A" pin="N.C._10" pad="46"/>
<connect gate="A" pin="N.C._11" pad="47"/>
<connect gate="A" pin="N.C._12" pad="12"/>
<connect gate="A" pin="N.C._13" pad="48"/>
<connect gate="A" pin="N.C._2" pad="34"/>
<connect gate="A" pin="N.C._3" pad="66"/>
<connect gate="A" pin="N.C._4" pad="19"/>
<connect gate="A" pin="N.C._5" pad="35"/>
<connect gate="A" pin="N.C._6" pad="36"/>
<connect gate="A" pin="N.C._7" pad="1"/>
<connect gate="A" pin="N.C._8" pad="43"/>
<connect gate="A" pin="N.C._9" pad="2"/>
<connect gate="A" pin="VCCINT" pad="58"/>
<connect gate="A" pin="VCCINT_2" pad="51"/>
<connect gate="A" pin="VCCIO" pad="50"/>
<connect gate="A" pin="VCCIO_2" pad="24"/>
<connect gate="B" pin="GNDINT" pad="124"/>
<connect gate="B" pin="GNDINT_2" pad="129"/>
<connect gate="B" pin="GNDIO" pad="114"/>
<connect gate="B" pin="GNDIO_2" pad="135"/>
<connect gate="B" pin="GNDIO_3" pad="77"/>
<connect gate="B" pin="GNDIO_4" pad="105"/>
<connect gate="B" pin="GNDIO_5" pad="85"/>
<connect gate="B" pin="GNDIO_6" pad="94"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/GCLR" pad="127"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="143"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="91"/>
<connect gate="B" pin="IO_14" pad="92"/>
<connect gate="B" pin="IO_15" pad="93"/>
<connect gate="B" pin="IO_16" pad="96"/>
<connect gate="B" pin="IO_17" pad="97"/>
<connect gate="B" pin="IO_18" pad="98"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="109"/>
<connect gate="B" pin="IO_26" pad="110"/>
<connect gate="B" pin="IO_27" pad="111"/>
<connect gate="B" pin="IO_28" pad="112"/>
<connect gate="B" pin="IO_29" pad="113"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="117"/>
<connect gate="B" pin="IO_32" pad="118"/>
<connect gate="B" pin="IO_33" pad="119"/>
<connect gate="B" pin="IO_34" pad="131"/>
<connect gate="B" pin="IO_35" pad="132"/>
<connect gate="B" pin="IO_36" pad="133"/>
<connect gate="B" pin="IO_37" pad="134"/>
<connect gate="B" pin="IO_38" pad="136"/>
<connect gate="B" pin="IO_39" pad="137"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_40" pad="138"/>
<connect gate="B" pin="IO_41" pad="139"/>
<connect gate="B" pin="IO_42" pad="140"/>
<connect gate="B" pin="IO_43" pad="141"/>
<connect gate="B" pin="IO_44" pad="142"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="84"/>
<connect gate="B" pin="N.C." pad="103"/>
<connect gate="B" pin="N.C._2" pad="75"/>
<connect gate="B" pin="N.C._3" pad="120"/>
<connect gate="B" pin="N.C._4" pad="90"/>
<connect gate="B" pin="N.C._5" pad="121"/>
<connect gate="B" pin="N.C._6" pad="108"/>
<connect gate="B" pin="N.C._7" pad="122"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="123"/>
<connect gate="B" pin="VCCIO" pad="115"/>
<connect gate="B" pin="VCCIO_2" pad="144"/>
<connect gate="B" pin="VCCIO_3" pad="73"/>
<connect gate="B" pin="VCCIO_4" pad="76"/>
<connect gate="B" pin="VCCIO_5" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3128ATC144-7N"/>
<attribute name="OC_FARNELL" value="1742179"/>
<attribute name="OC_NEWARK" value="51R0510"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3256AQC208-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3256AQC208-10N_A"/>
<gate name="B" symbol="EPM3256AQC208-10N_B"/>
<gate name="C" symbol="EPM3256AQC208-10N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="GNDIO" pad="32"/>
<connect gate="A" pin="GNDIO_2" pad="6"/>
<connect gate="A" pin="GNDIO_3" pad="14"/>
<connect gate="A" pin="GNDIO_4" pad="40"/>
<connect gate="A" pin="GNDIO_5" pad="50"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/TCK" pad="30"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="16"/>
<connect gate="A" pin="IO_13" pad="17"/>
<connect gate="A" pin="IO_14" pad="18"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="24"/>
<connect gate="A" pin="IO_2" pad="3"/>
<connect gate="A" pin="IO_20" pad="25"/>
<connect gate="A" pin="IO_21" pad="26"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="31"/>
<connect gate="A" pin="IO_26" pad="33"/>
<connect gate="A" pin="IO_27" pad="34"/>
<connect gate="A" pin="IO_28" pad="35"/>
<connect gate="A" pin="IO_29" pad="36"/>
<connect gate="A" pin="IO_3" pad="4"/>
<connect gate="A" pin="IO_30" pad="37"/>
<connect gate="A" pin="IO_31" pad="38"/>
<connect gate="A" pin="IO_32" pad="39"/>
<connect gate="A" pin="IO_33" pad="42"/>
<connect gate="A" pin="IO_34" pad="43"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="56"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="58"/>
<connect gate="A" pin="IO_45" pad="59"/>
<connect gate="A" pin="IO_46" pad="60"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="62"/>
<connect gate="A" pin="IO_49" pad="64"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="65"/>
<connect gate="A" pin="IO_51" pad="66"/>
<connect gate="A" pin="IO_52" pad="67"/>
<connect gate="A" pin="IO_53" pad="68"/>
<connect gate="A" pin="IO_54" pad="69"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="N.C." pad="54"/>
<connect gate="A" pin="N.C._2" pad="51"/>
<connect gate="A" pin="N.C._3" pad="1"/>
<connect gate="A" pin="N.C._4" pad="52"/>
<connect gate="A" pin="N.C._5" pad="2"/>
<connect gate="A" pin="N.C._6" pad="53"/>
<connect gate="A" pin="VCCIO" pad="63"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="23"/>
<connect gate="A" pin="VCCIO_4" pad="41"/>
<connect gate="B" pin="GNDINT" pad="75"/>
<connect gate="B" pin="GNDINT_2" pad="82"/>
<connect gate="B" pin="GNDIO" pad="72"/>
<connect gate="B" pin="GNDIO_2" pad="108"/>
<connect gate="B" pin="GNDIO_3" pad="116"/>
<connect gate="B" pin="GNDIO_4" pad="84"/>
<connect gate="B" pin="GNDIO_5" pad="94"/>
<connect gate="B" pin="GNDIO_6" pad="134"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/TMS" pad="127"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="89"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="91"/>
<connect gate="B" pin="IO_16" pad="92"/>
<connect gate="B" pin="IO_17" pad="93"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="98"/>
<connect gate="B" pin="IO_22" pad="99"/>
<connect gate="B" pin="IO_23" pad="100"/>
<connect gate="B" pin="IO_24" pad="101"/>
<connect gate="B" pin="IO_25" pad="102"/>
<connect gate="B" pin="IO_26" pad="109"/>
<connect gate="B" pin="IO_27" pad="110"/>
<connect gate="B" pin="IO_28" pad="111"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="114"/>
<connect gate="B" pin="IO_32" pad="115"/>
<connect gate="B" pin="IO_33" pad="117"/>
<connect gate="B" pin="IO_34" pad="118"/>
<connect gate="B" pin="IO_35" pad="119"/>
<connect gate="B" pin="IO_36" pad="120"/>
<connect gate="B" pin="IO_37" pad="121"/>
<connect gate="B" pin="IO_38" pad="122"/>
<connect gate="B" pin="IO_39" pad="123"/>
<connect gate="B" pin="IO_4" pad="76"/>
<connect gate="B" pin="IO_40" pad="124"/>
<connect gate="B" pin="IO_41" pad="126"/>
<connect gate="B" pin="IO_42" pad="128"/>
<connect gate="B" pin="IO_43" pad="129"/>
<connect gate="B" pin="IO_44" pad="130"/>
<connect gate="B" pin="IO_45" pad="131"/>
<connect gate="B" pin="IO_46" pad="132"/>
<connect gate="B" pin="IO_47" pad="133"/>
<connect gate="B" pin="IO_48" pad="135"/>
<connect gate="B" pin="IO_49" pad="136"/>
<connect gate="B" pin="IO_5" pad="77"/>
<connect gate="B" pin="IO_50" pad="137"/>
<connect gate="B" pin="IO_51" pad="138"/>
<connect gate="B" pin="IO_52" pad="139"/>
<connect gate="B" pin="IO_6" pad="78"/>
<connect gate="B" pin="IO_7" pad="79"/>
<connect gate="B" pin="IO_8" pad="80"/>
<connect gate="B" pin="IO_9" pad="81"/>
<connect gate="B" pin="N.C." pad="106"/>
<connect gate="B" pin="N.C._2" pad="103"/>
<connect gate="B" pin="N.C._3" pad="104"/>
<connect gate="B" pin="N.C._4" pad="105"/>
<connect gate="B" pin="VCCINT" pad="83"/>
<connect gate="B" pin="VCCINT_2" pad="74"/>
<connect gate="B" pin="VCCIO" pad="125"/>
<connect gate="B" pin="VCCIO_2" pad="107"/>
<connect gate="B" pin="VCCIO_3" pad="85"/>
<connect gate="C" pin="GNDINT" pad="180"/>
<connect gate="C" pin="GNDINT_2" pad="185"/>
<connect gate="C" pin="GNDIO" pad="142"/>
<connect gate="C" pin="GNDIO_2" pad="152"/>
<connect gate="C" pin="GNDIO_3" pad="190"/>
<connect gate="C" pin="GNDIO_4" pad="174"/>
<connect gate="C" pin="GNDIO_5" pad="200"/>
<connect gate="C" pin="INPUT/GCLK1" pad="184"/>
<connect gate="C" pin="INPUT/GCLR" pad="182"/>
<connect gate="C" pin="INPUT/OE1" pad="183"/>
<connect gate="C" pin="INPUT/OE2/GCLK2" pad="181"/>
<connect gate="C" pin="IO" pad="206"/>
<connect gate="C" pin="IO/TDI" pad="176"/>
<connect gate="C" pin="IO/TDO" pad="189"/>
<connect gate="C" pin="IO_10" pad="151"/>
<connect gate="C" pin="IO_11" pad="153"/>
<connect gate="C" pin="IO_12" pad="154"/>
<connect gate="C" pin="IO_13" pad="159"/>
<connect gate="C" pin="IO_14" pad="160"/>
<connect gate="C" pin="IO_15" pad="161"/>
<connect gate="C" pin="IO_16" pad="162"/>
<connect gate="C" pin="IO_17" pad="163"/>
<connect gate="C" pin="IO_18" pad="164"/>
<connect gate="C" pin="IO_19" pad="166"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="167"/>
<connect gate="C" pin="IO_21" pad="168"/>
<connect gate="C" pin="IO_22" pad="169"/>
<connect gate="C" pin="IO_23" pad="170"/>
<connect gate="C" pin="IO_24" pad="171"/>
<connect gate="C" pin="IO_25" pad="172"/>
<connect gate="C" pin="IO_26" pad="173"/>
<connect gate="C" pin="IO_27" pad="175"/>
<connect gate="C" pin="IO_28" pad="177"/>
<connect gate="C" pin="IO_29" pad="178"/>
<connect gate="C" pin="IO_3" pad="144"/>
<connect gate="C" pin="IO_30" pad="187"/>
<connect gate="C" pin="IO_31" pad="188"/>
<connect gate="C" pin="IO_32" pad="192"/>
<connect gate="C" pin="IO_33" pad="193"/>
<connect gate="C" pin="IO_34" pad="194"/>
<connect gate="C" pin="IO_35" pad="195"/>
<connect gate="C" pin="IO_36" pad="196"/>
<connect gate="C" pin="IO_37" pad="197"/>
<connect gate="C" pin="IO_38" pad="198"/>
<connect gate="C" pin="IO_39" pad="199"/>
<connect gate="C" pin="IO_4" pad="145"/>
<connect gate="C" pin="IO_40" pad="201"/>
<connect gate="C" pin="IO_41" pad="202"/>
<connect gate="C" pin="IO_42" pad="203"/>
<connect gate="C" pin="IO_43" pad="204"/>
<connect gate="C" pin="IO_44" pad="205"/>
<connect gate="C" pin="IO_5" pad="146"/>
<connect gate="C" pin="IO_6" pad="147"/>
<connect gate="C" pin="IO_7" pad="148"/>
<connect gate="C" pin="IO_8" pad="149"/>
<connect gate="C" pin="IO_9" pad="150"/>
<connect gate="C" pin="N.C." pad="158"/>
<connect gate="C" pin="N.C._2" pad="155"/>
<connect gate="C" pin="N.C._3" pad="156"/>
<connect gate="C" pin="N.C._4" pad="207"/>
<connect gate="C" pin="N.C._5" pad="157"/>
<connect gate="C" pin="N.C._6" pad="208"/>
<connect gate="C" pin="VCCINT" pad="186"/>
<connect gate="C" pin="VCCINT_2" pad="179"/>
<connect gate="C" pin="VCCIO" pad="143"/>
<connect gate="C" pin="VCCIO_2" pad="165"/>
<connect gate="C" pin="VCCIO_3" pad="191"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3256AQC208-10N"/>
<attribute name="OC_FARNELL" value="1637252"/>
<attribute name="OC_NEWARK" value="51R0511"/>
<attribute name="PACKAGE" value="PQFP-208"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3256AQC208-7N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3256AQC208-7N_A"/>
<gate name="B" symbol="EPM3256AQC208-7N_B"/>
<gate name="C" symbol="EPM3256AQC208-7N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="GNDIO" pad="32"/>
<connect gate="A" pin="GNDIO_2" pad="6"/>
<connect gate="A" pin="GNDIO_3" pad="14"/>
<connect gate="A" pin="GNDIO_4" pad="40"/>
<connect gate="A" pin="GNDIO_5" pad="50"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/TCK" pad="30"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="16"/>
<connect gate="A" pin="IO_13" pad="17"/>
<connect gate="A" pin="IO_14" pad="18"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="24"/>
<connect gate="A" pin="IO_2" pad="3"/>
<connect gate="A" pin="IO_20" pad="25"/>
<connect gate="A" pin="IO_21" pad="26"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="31"/>
<connect gate="A" pin="IO_26" pad="33"/>
<connect gate="A" pin="IO_27" pad="34"/>
<connect gate="A" pin="IO_28" pad="35"/>
<connect gate="A" pin="IO_29" pad="36"/>
<connect gate="A" pin="IO_3" pad="4"/>
<connect gate="A" pin="IO_30" pad="37"/>
<connect gate="A" pin="IO_31" pad="38"/>
<connect gate="A" pin="IO_32" pad="39"/>
<connect gate="A" pin="IO_33" pad="42"/>
<connect gate="A" pin="IO_34" pad="43"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="56"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="58"/>
<connect gate="A" pin="IO_45" pad="59"/>
<connect gate="A" pin="IO_46" pad="60"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="62"/>
<connect gate="A" pin="IO_49" pad="64"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="65"/>
<connect gate="A" pin="IO_51" pad="66"/>
<connect gate="A" pin="IO_52" pad="67"/>
<connect gate="A" pin="IO_53" pad="68"/>
<connect gate="A" pin="IO_54" pad="69"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="N.C." pad="54"/>
<connect gate="A" pin="N.C._2" pad="51"/>
<connect gate="A" pin="N.C._3" pad="1"/>
<connect gate="A" pin="N.C._4" pad="52"/>
<connect gate="A" pin="N.C._5" pad="2"/>
<connect gate="A" pin="N.C._6" pad="53"/>
<connect gate="A" pin="VCCIO" pad="63"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="23"/>
<connect gate="A" pin="VCCIO_4" pad="41"/>
<connect gate="B" pin="GNDINT" pad="75"/>
<connect gate="B" pin="GNDINT_2" pad="82"/>
<connect gate="B" pin="GNDIO" pad="72"/>
<connect gate="B" pin="GNDIO_2" pad="108"/>
<connect gate="B" pin="GNDIO_3" pad="116"/>
<connect gate="B" pin="GNDIO_4" pad="84"/>
<connect gate="B" pin="GNDIO_5" pad="94"/>
<connect gate="B" pin="GNDIO_6" pad="134"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/TMS" pad="127"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="89"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="91"/>
<connect gate="B" pin="IO_16" pad="92"/>
<connect gate="B" pin="IO_17" pad="93"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="98"/>
<connect gate="B" pin="IO_22" pad="99"/>
<connect gate="B" pin="IO_23" pad="100"/>
<connect gate="B" pin="IO_24" pad="101"/>
<connect gate="B" pin="IO_25" pad="102"/>
<connect gate="B" pin="IO_26" pad="109"/>
<connect gate="B" pin="IO_27" pad="110"/>
<connect gate="B" pin="IO_28" pad="111"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="114"/>
<connect gate="B" pin="IO_32" pad="115"/>
<connect gate="B" pin="IO_33" pad="117"/>
<connect gate="B" pin="IO_34" pad="118"/>
<connect gate="B" pin="IO_35" pad="119"/>
<connect gate="B" pin="IO_36" pad="120"/>
<connect gate="B" pin="IO_37" pad="121"/>
<connect gate="B" pin="IO_38" pad="122"/>
<connect gate="B" pin="IO_39" pad="123"/>
<connect gate="B" pin="IO_4" pad="76"/>
<connect gate="B" pin="IO_40" pad="124"/>
<connect gate="B" pin="IO_41" pad="126"/>
<connect gate="B" pin="IO_42" pad="128"/>
<connect gate="B" pin="IO_43" pad="129"/>
<connect gate="B" pin="IO_44" pad="130"/>
<connect gate="B" pin="IO_45" pad="131"/>
<connect gate="B" pin="IO_46" pad="132"/>
<connect gate="B" pin="IO_47" pad="133"/>
<connect gate="B" pin="IO_48" pad="135"/>
<connect gate="B" pin="IO_49" pad="136"/>
<connect gate="B" pin="IO_5" pad="77"/>
<connect gate="B" pin="IO_50" pad="137"/>
<connect gate="B" pin="IO_51" pad="138"/>
<connect gate="B" pin="IO_52" pad="139"/>
<connect gate="B" pin="IO_6" pad="78"/>
<connect gate="B" pin="IO_7" pad="79"/>
<connect gate="B" pin="IO_8" pad="80"/>
<connect gate="B" pin="IO_9" pad="81"/>
<connect gate="B" pin="N.C." pad="106"/>
<connect gate="B" pin="N.C._2" pad="103"/>
<connect gate="B" pin="N.C._3" pad="104"/>
<connect gate="B" pin="N.C._4" pad="105"/>
<connect gate="B" pin="VCCINT" pad="83"/>
<connect gate="B" pin="VCCINT_2" pad="74"/>
<connect gate="B" pin="VCCIO" pad="125"/>
<connect gate="B" pin="VCCIO_2" pad="107"/>
<connect gate="B" pin="VCCIO_3" pad="85"/>
<connect gate="C" pin="GNDINT" pad="180"/>
<connect gate="C" pin="GNDINT_2" pad="185"/>
<connect gate="C" pin="GNDIO" pad="142"/>
<connect gate="C" pin="GNDIO_2" pad="152"/>
<connect gate="C" pin="GNDIO_3" pad="190"/>
<connect gate="C" pin="GNDIO_4" pad="174"/>
<connect gate="C" pin="GNDIO_5" pad="200"/>
<connect gate="C" pin="INPUT/GCLK1" pad="184"/>
<connect gate="C" pin="INPUT/GCLR" pad="182"/>
<connect gate="C" pin="INPUT/OE1" pad="183"/>
<connect gate="C" pin="INPUT/OE2/GCLK2" pad="181"/>
<connect gate="C" pin="IO" pad="206"/>
<connect gate="C" pin="IO/TDI" pad="176"/>
<connect gate="C" pin="IO/TDO" pad="189"/>
<connect gate="C" pin="IO_10" pad="151"/>
<connect gate="C" pin="IO_11" pad="153"/>
<connect gate="C" pin="IO_12" pad="154"/>
<connect gate="C" pin="IO_13" pad="159"/>
<connect gate="C" pin="IO_14" pad="160"/>
<connect gate="C" pin="IO_15" pad="161"/>
<connect gate="C" pin="IO_16" pad="162"/>
<connect gate="C" pin="IO_17" pad="163"/>
<connect gate="C" pin="IO_18" pad="164"/>
<connect gate="C" pin="IO_19" pad="166"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="167"/>
<connect gate="C" pin="IO_21" pad="168"/>
<connect gate="C" pin="IO_22" pad="169"/>
<connect gate="C" pin="IO_23" pad="170"/>
<connect gate="C" pin="IO_24" pad="171"/>
<connect gate="C" pin="IO_25" pad="172"/>
<connect gate="C" pin="IO_26" pad="173"/>
<connect gate="C" pin="IO_27" pad="175"/>
<connect gate="C" pin="IO_28" pad="177"/>
<connect gate="C" pin="IO_29" pad="178"/>
<connect gate="C" pin="IO_3" pad="144"/>
<connect gate="C" pin="IO_30" pad="187"/>
<connect gate="C" pin="IO_31" pad="188"/>
<connect gate="C" pin="IO_32" pad="192"/>
<connect gate="C" pin="IO_33" pad="193"/>
<connect gate="C" pin="IO_34" pad="194"/>
<connect gate="C" pin="IO_35" pad="195"/>
<connect gate="C" pin="IO_36" pad="196"/>
<connect gate="C" pin="IO_37" pad="197"/>
<connect gate="C" pin="IO_38" pad="198"/>
<connect gate="C" pin="IO_39" pad="199"/>
<connect gate="C" pin="IO_4" pad="145"/>
<connect gate="C" pin="IO_40" pad="201"/>
<connect gate="C" pin="IO_41" pad="202"/>
<connect gate="C" pin="IO_42" pad="203"/>
<connect gate="C" pin="IO_43" pad="204"/>
<connect gate="C" pin="IO_44" pad="205"/>
<connect gate="C" pin="IO_5" pad="146"/>
<connect gate="C" pin="IO_6" pad="147"/>
<connect gate="C" pin="IO_7" pad="148"/>
<connect gate="C" pin="IO_8" pad="149"/>
<connect gate="C" pin="IO_9" pad="150"/>
<connect gate="C" pin="N.C." pad="158"/>
<connect gate="C" pin="N.C._2" pad="155"/>
<connect gate="C" pin="N.C._3" pad="156"/>
<connect gate="C" pin="N.C._4" pad="207"/>
<connect gate="C" pin="N.C._5" pad="157"/>
<connect gate="C" pin="N.C._6" pad="208"/>
<connect gate="C" pin="VCCINT" pad="186"/>
<connect gate="C" pin="VCCINT_2" pad="179"/>
<connect gate="C" pin="VCCIO" pad="143"/>
<connect gate="C" pin="VCCIO_2" pad="165"/>
<connect gate="C" pin="VCCIO_3" pad="191"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3256AQC208-7N"/>
<attribute name="OC_FARNELL" value="1742180"/>
<attribute name="OC_NEWARK" value="51R0512"/>
<attribute name="PACKAGE" value="PQFP-208"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3256ATC144-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3256ATC144-10N_A"/>
<gate name="B" symbol="EPM3256ATC144-10N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="17"/>
<connect gate="A" pin="GNDIO_2" pad="59"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="26"/>
<connect gate="A" pin="GNDIO_5" pad="33"/>
<connect gate="A" pin="GNDIO_6" pad="3"/>
<connect gate="A" pin="GNDIO_7" pad="13"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="25"/>
<connect gate="A" pin="IO_17" pad="27"/>
<connect gate="A" pin="IO_18" pad="28"/>
<connect gate="A" pin="IO_19" pad="29"/>
<connect gate="A" pin="IO_2" pad="5"/>
<connect gate="A" pin="IO_20" pad="30"/>
<connect gate="A" pin="IO_21" pad="31"/>
<connect gate="A" pin="IO_22" pad="32"/>
<connect gate="A" pin="IO_23" pad="37"/>
<connect gate="A" pin="IO_24" pad="38"/>
<connect gate="A" pin="IO_25" pad="39"/>
<connect gate="A" pin="IO_26" pad="40"/>
<connect gate="A" pin="IO_27" pad="41"/>
<connect gate="A" pin="IO_28" pad="42"/>
<connect gate="A" pin="IO_29" pad="44"/>
<connect gate="A" pin="IO_3" pad="6"/>
<connect gate="A" pin="IO_30" pad="45"/>
<connect gate="A" pin="IO_31" pad="53"/>
<connect gate="A" pin="IO_32" pad="54"/>
<connect gate="A" pin="IO_33" pad="55"/>
<connect gate="A" pin="IO_34" pad="56"/>
<connect gate="A" pin="IO_35" pad="60"/>
<connect gate="A" pin="IO_36" pad="61"/>
<connect gate="A" pin="IO_37" pad="62"/>
<connect gate="A" pin="IO_38" pad="63"/>
<connect gate="A" pin="IO_39" pad="65"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="67"/>
<connect gate="A" pin="IO_41" pad="68"/>
<connect gate="A" pin="IO_42" pad="69"/>
<connect gate="A" pin="IO_43" pad="70"/>
<connect gate="A" pin="IO_44" pad="71"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="N.C." pad="49"/>
<connect gate="A" pin="N.C._10" pad="46"/>
<connect gate="A" pin="N.C._11" pad="47"/>
<connect gate="A" pin="N.C._12" pad="12"/>
<connect gate="A" pin="N.C._13" pad="48"/>
<connect gate="A" pin="N.C._2" pad="34"/>
<connect gate="A" pin="N.C._3" pad="66"/>
<connect gate="A" pin="N.C._4" pad="19"/>
<connect gate="A" pin="N.C._5" pad="35"/>
<connect gate="A" pin="N.C._6" pad="36"/>
<connect gate="A" pin="N.C._7" pad="1"/>
<connect gate="A" pin="N.C._8" pad="43"/>
<connect gate="A" pin="N.C._9" pad="2"/>
<connect gate="A" pin="VCCINT" pad="58"/>
<connect gate="A" pin="VCCINT_2" pad="51"/>
<connect gate="A" pin="VCCIO" pad="50"/>
<connect gate="A" pin="VCCIO_2" pad="24"/>
<connect gate="B" pin="GNDINT" pad="124"/>
<connect gate="B" pin="GNDINT_2" pad="129"/>
<connect gate="B" pin="GNDIO" pad="114"/>
<connect gate="B" pin="GNDIO_2" pad="135"/>
<connect gate="B" pin="GNDIO_3" pad="77"/>
<connect gate="B" pin="GNDIO_4" pad="105"/>
<connect gate="B" pin="GNDIO_5" pad="85"/>
<connect gate="B" pin="GNDIO_6" pad="94"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/GCLR" pad="127"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="143"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="91"/>
<connect gate="B" pin="IO_14" pad="92"/>
<connect gate="B" pin="IO_15" pad="93"/>
<connect gate="B" pin="IO_16" pad="96"/>
<connect gate="B" pin="IO_17" pad="97"/>
<connect gate="B" pin="IO_18" pad="98"/>
<connect gate="B" pin="IO_19" pad="99"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="100"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="102"/>
<connect gate="B" pin="IO_23" pad="106"/>
<connect gate="B" pin="IO_24" pad="107"/>
<connect gate="B" pin="IO_25" pad="109"/>
<connect gate="B" pin="IO_26" pad="110"/>
<connect gate="B" pin="IO_27" pad="111"/>
<connect gate="B" pin="IO_28" pad="112"/>
<connect gate="B" pin="IO_29" pad="113"/>
<connect gate="B" pin="IO_3" pad="78"/>
<connect gate="B" pin="IO_30" pad="116"/>
<connect gate="B" pin="IO_31" pad="117"/>
<connect gate="B" pin="IO_32" pad="118"/>
<connect gate="B" pin="IO_33" pad="119"/>
<connect gate="B" pin="IO_34" pad="131"/>
<connect gate="B" pin="IO_35" pad="132"/>
<connect gate="B" pin="IO_36" pad="133"/>
<connect gate="B" pin="IO_37" pad="134"/>
<connect gate="B" pin="IO_38" pad="136"/>
<connect gate="B" pin="IO_39" pad="137"/>
<connect gate="B" pin="IO_4" pad="79"/>
<connect gate="B" pin="IO_40" pad="138"/>
<connect gate="B" pin="IO_41" pad="139"/>
<connect gate="B" pin="IO_42" pad="140"/>
<connect gate="B" pin="IO_43" pad="141"/>
<connect gate="B" pin="IO_44" pad="142"/>
<connect gate="B" pin="IO_5" pad="80"/>
<connect gate="B" pin="IO_6" pad="81"/>
<connect gate="B" pin="IO_7" pad="82"/>
<connect gate="B" pin="IO_8" pad="83"/>
<connect gate="B" pin="IO_9" pad="84"/>
<connect gate="B" pin="N.C." pad="103"/>
<connect gate="B" pin="N.C._2" pad="75"/>
<connect gate="B" pin="N.C._3" pad="120"/>
<connect gate="B" pin="N.C._4" pad="90"/>
<connect gate="B" pin="N.C._5" pad="121"/>
<connect gate="B" pin="N.C._6" pad="108"/>
<connect gate="B" pin="N.C._7" pad="122"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="123"/>
<connect gate="B" pin="VCCIO" pad="115"/>
<connect gate="B" pin="VCCIO_2" pad="144"/>
<connect gate="B" pin="VCCIO_3" pad="73"/>
<connect gate="B" pin="VCCIO_4" pad="76"/>
<connect gate="B" pin="VCCIO_5" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3256ATC144-10N"/>
<attribute name="OC_FARNELL" value="1662245"/>
<attribute name="OC_NEWARK" value="51R0513"/>
<attribute name="PACKAGE" value="TQFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3256ATC144-7N" prefix="U">
<description>IC MAX 3000A CPLD 256 144-TQFP</description>
<gates>
<gate name="A" symbol="EPM3256ATC144-7N_A"/>
<gate name="B" symbol="EPM3256ATC144-7N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="33"/>
<connect gate="A" pin="GNDIO_2" pad="17"/>
<connect gate="A" pin="GNDIO_3" pad="59"/>
<connect gate="A" pin="GNDIO_4" pad="3"/>
<connect gate="A" pin="GNDIO_5" pad="13"/>
<connect gate="A" pin="GNDIO_6" pad="26"/>
<connect gate="A" pin="GNDIO_7" pad="64"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="14"/>
<connect gate="A" pin="IO_11" pad="11"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="12"/>
<connect gate="A" pin="IO_14" pad="16"/>
<connect gate="A" pin="IO_15" pad="18"/>
<connect gate="A" pin="IO_16" pad="19"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="25"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="23"/>
<connect gate="A" pin="IO_21" pad="27"/>
<connect gate="A" pin="IO_22" pad="28"/>
<connect gate="A" pin="IO_23" pad="29"/>
<connect gate="A" pin="IO_24" pad="30"/>
<connect gate="A" pin="IO_25" pad="31"/>
<connect gate="A" pin="IO_26" pad="32"/>
<connect gate="A" pin="IO_27" pad="34"/>
<connect gate="A" pin="IO_28" pad="35"/>
<connect gate="A" pin="IO_29" pad="36"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="37"/>
<connect gate="A" pin="IO_31" pad="38"/>
<connect gate="A" pin="IO_32" pad="39"/>
<connect gate="A" pin="IO_33" pad="40"/>
<connect gate="A" pin="IO_34" pad="41"/>
<connect gate="A" pin="IO_35" pad="42"/>
<connect gate="A" pin="IO_36" pad="43"/>
<connect gate="A" pin="IO_37" pad="44"/>
<connect gate="A" pin="IO_38" pad="45"/>
<connect gate="A" pin="IO_39" pad="46"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="47"/>
<connect gate="A" pin="IO_41" pad="48"/>
<connect gate="A" pin="IO_42" pad="49"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="60"/>
<connect gate="A" pin="IO_46" pad="55"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="56"/>
<connect gate="A" pin="IO_49" pad="62"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="63"/>
<connect gate="A" pin="IO_51" pad="65"/>
<connect gate="A" pin="IO_52" pad="66"/>
<connect gate="A" pin="IO_53" pad="67"/>
<connect gate="A" pin="IO_54" pad="68"/>
<connect gate="A" pin="IO_55" pad="69"/>
<connect gate="A" pin="IO_56" pad="70"/>
<connect gate="A" pin="IO_57" pad="71"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="51"/>
<connect gate="A" pin="VCCINT_2" pad="58"/>
<connect gate="A" pin="VCCIO" pad="24"/>
<connect gate="A" pin="VCCIO_2" pad="50"/>
<connect gate="B" pin="GNDINT" pad="124"/>
<connect gate="B" pin="GNDINT_2" pad="129"/>
<connect gate="B" pin="GNDIO" pad="105"/>
<connect gate="B" pin="GNDIO_2" pad="94"/>
<connect gate="B" pin="GNDIO_3" pad="135"/>
<connect gate="B" pin="GNDIO_4" pad="77"/>
<connect gate="B" pin="GNDIO_5" pad="85"/>
<connect gate="B" pin="GNDIO_6" pad="114"/>
<connect gate="B" pin="INPUT/*GCLR" pad="127"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="108"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="84"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="86"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="91"/>
<connect gate="B" pin="IO_16" pad="92"/>
<connect gate="B" pin="IO_17" pad="96"/>
<connect gate="B" pin="IO_18" pad="93"/>
<connect gate="B" pin="IO_19" pad="97"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="98"/>
<connect gate="B" pin="IO_21" pad="109"/>
<connect gate="B" pin="IO_22" pad="110"/>
<connect gate="B" pin="IO_23" pad="111"/>
<connect gate="B" pin="IO_24" pad="112"/>
<connect gate="B" pin="IO_25" pad="113"/>
<connect gate="B" pin="IO_26" pad="116"/>
<connect gate="B" pin="IO_27" pad="117"/>
<connect gate="B" pin="IO_28" pad="118"/>
<connect gate="B" pin="IO_29" pad="119"/>
<connect gate="B" pin="IO_3" pad="75"/>
<connect gate="B" pin="IO_30" pad="120"/>
<connect gate="B" pin="IO_31" pad="121"/>
<connect gate="B" pin="IO_32" pad="131"/>
<connect gate="B" pin="IO_33" pad="122"/>
<connect gate="B" pin="IO_34" pad="132"/>
<connect gate="B" pin="IO_35" pad="133"/>
<connect gate="B" pin="IO_36" pad="134"/>
<connect gate="B" pin="IO_37" pad="136"/>
<connect gate="B" pin="IO_38" pad="137"/>
<connect gate="B" pin="IO_39" pad="138"/>
<connect gate="B" pin="IO_4" pad="78"/>
<connect gate="B" pin="IO_40" pad="139"/>
<connect gate="B" pin="IO_41" pad="140"/>
<connect gate="B" pin="IO_42" pad="141"/>
<connect gate="B" pin="IO_43" pad="142"/>
<connect gate="B" pin="IO_44" pad="143"/>
<connect gate="B" pin="IO_45" pad="99"/>
<connect gate="B" pin="IO_46" pad="100"/>
<connect gate="B" pin="IO_47" pad="101"/>
<connect gate="B" pin="IO_48" pad="102"/>
<connect gate="B" pin="IO_49" pad="106"/>
<connect gate="B" pin="IO_5" pad="79"/>
<connect gate="B" pin="IO_50" pad="103"/>
<connect gate="B" pin="IO_51" pad="107"/>
<connect gate="B" pin="IO_6" pad="80"/>
<connect gate="B" pin="IO_7" pad="81"/>
<connect gate="B" pin="IO_8" pad="82"/>
<connect gate="B" pin="IO_9" pad="83"/>
<connect gate="B" pin="VCCINT" pad="123"/>
<connect gate="B" pin="VCCINT_2" pad="130"/>
<connect gate="B" pin="VCCIO" pad="144"/>
<connect gate="B" pin="VCCIO_2" pad="76"/>
<connect gate="B" pin="VCCIO_3" pad="73"/>
<connect gate="B" pin="VCCIO_4" pad="95"/>
<connect gate="B" pin="VCCIO_5" pad="115"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3256ATC144-7N"/>
<attribute name="OC_FARNELL" value="1792406"/>
<attribute name="OC_NEWARK" value="51R0514"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM3512AQC208-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM3512AQC208-10N_A"/>
<gate name="B" symbol="EPM3512AQC208-10N_B"/>
<gate name="C" symbol="EPM3512AQC208-10N_C"/>
</gates>
<devices>
<device name="" package="QFP50P3060X3060X410-208N">
<connects>
<connect gate="A" pin="GNDIO" pad="32"/>
<connect gate="A" pin="GNDIO_2" pad="6"/>
<connect gate="A" pin="GNDIO_3" pad="14"/>
<connect gate="A" pin="GNDIO_4" pad="40"/>
<connect gate="A" pin="GNDIO_5" pad="50"/>
<connect gate="A" pin="IO" pad="70"/>
<connect gate="A" pin="IO/TCK" pad="30"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="15"/>
<connect gate="A" pin="IO_12" pad="16"/>
<connect gate="A" pin="IO_13" pad="17"/>
<connect gate="A" pin="IO_14" pad="18"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="24"/>
<connect gate="A" pin="IO_2" pad="3"/>
<connect gate="A" pin="IO_20" pad="25"/>
<connect gate="A" pin="IO_21" pad="26"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="31"/>
<connect gate="A" pin="IO_26" pad="33"/>
<connect gate="A" pin="IO_27" pad="34"/>
<connect gate="A" pin="IO_28" pad="35"/>
<connect gate="A" pin="IO_29" pad="36"/>
<connect gate="A" pin="IO_3" pad="4"/>
<connect gate="A" pin="IO_30" pad="37"/>
<connect gate="A" pin="IO_31" pad="38"/>
<connect gate="A" pin="IO_32" pad="39"/>
<connect gate="A" pin="IO_33" pad="42"/>
<connect gate="A" pin="IO_34" pad="43"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="56"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="58"/>
<connect gate="A" pin="IO_45" pad="59"/>
<connect gate="A" pin="IO_46" pad="60"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="62"/>
<connect gate="A" pin="IO_49" pad="64"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="65"/>
<connect gate="A" pin="IO_51" pad="66"/>
<connect gate="A" pin="IO_52" pad="67"/>
<connect gate="A" pin="IO_53" pad="68"/>
<connect gate="A" pin="IO_54" pad="69"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="N.C." pad="54"/>
<connect gate="A" pin="N.C._2" pad="51"/>
<connect gate="A" pin="N.C._3" pad="1"/>
<connect gate="A" pin="N.C._4" pad="52"/>
<connect gate="A" pin="N.C._5" pad="2"/>
<connect gate="A" pin="N.C._6" pad="53"/>
<connect gate="A" pin="VCCIO" pad="63"/>
<connect gate="A" pin="VCCIO_2" pad="5"/>
<connect gate="A" pin="VCCIO_3" pad="23"/>
<connect gate="A" pin="VCCIO_4" pad="41"/>
<connect gate="B" pin="GNDINT" pad="75"/>
<connect gate="B" pin="GNDINT_2" pad="82"/>
<connect gate="B" pin="GNDIO" pad="72"/>
<connect gate="B" pin="GNDIO_2" pad="108"/>
<connect gate="B" pin="GNDIO_3" pad="116"/>
<connect gate="B" pin="GNDIO_4" pad="84"/>
<connect gate="B" pin="GNDIO_5" pad="94"/>
<connect gate="B" pin="GNDIO_6" pad="134"/>
<connect gate="B" pin="IO" pad="140"/>
<connect gate="B" pin="IO/TMS" pad="127"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="87"/>
<connect gate="B" pin="IO_12" pad="88"/>
<connect gate="B" pin="IO_13" pad="89"/>
<connect gate="B" pin="IO_14" pad="90"/>
<connect gate="B" pin="IO_15" pad="91"/>
<connect gate="B" pin="IO_16" pad="92"/>
<connect gate="B" pin="IO_17" pad="93"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="71"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="98"/>
<connect gate="B" pin="IO_22" pad="99"/>
<connect gate="B" pin="IO_23" pad="100"/>
<connect gate="B" pin="IO_24" pad="101"/>
<connect gate="B" pin="IO_25" pad="102"/>
<connect gate="B" pin="IO_26" pad="109"/>
<connect gate="B" pin="IO_27" pad="110"/>
<connect gate="B" pin="IO_28" pad="111"/>
<connect gate="B" pin="IO_29" pad="112"/>
<connect gate="B" pin="IO_3" pad="73"/>
<connect gate="B" pin="IO_30" pad="113"/>
<connect gate="B" pin="IO_31" pad="114"/>
<connect gate="B" pin="IO_32" pad="115"/>
<connect gate="B" pin="IO_33" pad="117"/>
<connect gate="B" pin="IO_34" pad="118"/>
<connect gate="B" pin="IO_35" pad="119"/>
<connect gate="B" pin="IO_36" pad="120"/>
<connect gate="B" pin="IO_37" pad="121"/>
<connect gate="B" pin="IO_38" pad="122"/>
<connect gate="B" pin="IO_39" pad="123"/>
<connect gate="B" pin="IO_4" pad="76"/>
<connect gate="B" pin="IO_40" pad="124"/>
<connect gate="B" pin="IO_41" pad="126"/>
<connect gate="B" pin="IO_42" pad="128"/>
<connect gate="B" pin="IO_43" pad="129"/>
<connect gate="B" pin="IO_44" pad="130"/>
<connect gate="B" pin="IO_45" pad="131"/>
<connect gate="B" pin="IO_46" pad="132"/>
<connect gate="B" pin="IO_47" pad="133"/>
<connect gate="B" pin="IO_48" pad="135"/>
<connect gate="B" pin="IO_49" pad="136"/>
<connect gate="B" pin="IO_5" pad="77"/>
<connect gate="B" pin="IO_50" pad="137"/>
<connect gate="B" pin="IO_51" pad="138"/>
<connect gate="B" pin="IO_52" pad="139"/>
<connect gate="B" pin="IO_6" pad="78"/>
<connect gate="B" pin="IO_7" pad="79"/>
<connect gate="B" pin="IO_8" pad="80"/>
<connect gate="B" pin="IO_9" pad="81"/>
<connect gate="B" pin="N.C." pad="106"/>
<connect gate="B" pin="N.C._2" pad="103"/>
<connect gate="B" pin="N.C._3" pad="104"/>
<connect gate="B" pin="N.C._4" pad="105"/>
<connect gate="B" pin="VCCINT" pad="83"/>
<connect gate="B" pin="VCCINT_2" pad="74"/>
<connect gate="B" pin="VCCIO" pad="125"/>
<connect gate="B" pin="VCCIO_2" pad="107"/>
<connect gate="B" pin="VCCIO_3" pad="85"/>
<connect gate="C" pin="GNDINT" pad="180"/>
<connect gate="C" pin="GNDINT_2" pad="185"/>
<connect gate="C" pin="GNDIO" pad="142"/>
<connect gate="C" pin="GNDIO_2" pad="152"/>
<connect gate="C" pin="GNDIO_3" pad="190"/>
<connect gate="C" pin="GNDIO_4" pad="174"/>
<connect gate="C" pin="GNDIO_5" pad="200"/>
<connect gate="C" pin="INPUT/GCLK1" pad="184"/>
<connect gate="C" pin="INPUT/GCLR" pad="182"/>
<connect gate="C" pin="INPUT/OE1" pad="183"/>
<connect gate="C" pin="INPUT/OE2/GCLK2" pad="181"/>
<connect gate="C" pin="IO" pad="206"/>
<connect gate="C" pin="IO/TDI" pad="176"/>
<connect gate="C" pin="IO/TDO" pad="189"/>
<connect gate="C" pin="IO_10" pad="151"/>
<connect gate="C" pin="IO_11" pad="153"/>
<connect gate="C" pin="IO_12" pad="154"/>
<connect gate="C" pin="IO_13" pad="159"/>
<connect gate="C" pin="IO_14" pad="160"/>
<connect gate="C" pin="IO_15" pad="161"/>
<connect gate="C" pin="IO_16" pad="162"/>
<connect gate="C" pin="IO_17" pad="163"/>
<connect gate="C" pin="IO_18" pad="164"/>
<connect gate="C" pin="IO_19" pad="166"/>
<connect gate="C" pin="IO_2" pad="141"/>
<connect gate="C" pin="IO_20" pad="167"/>
<connect gate="C" pin="IO_21" pad="168"/>
<connect gate="C" pin="IO_22" pad="169"/>
<connect gate="C" pin="IO_23" pad="170"/>
<connect gate="C" pin="IO_24" pad="171"/>
<connect gate="C" pin="IO_25" pad="172"/>
<connect gate="C" pin="IO_26" pad="173"/>
<connect gate="C" pin="IO_27" pad="175"/>
<connect gate="C" pin="IO_28" pad="177"/>
<connect gate="C" pin="IO_29" pad="178"/>
<connect gate="C" pin="IO_3" pad="144"/>
<connect gate="C" pin="IO_30" pad="187"/>
<connect gate="C" pin="IO_31" pad="188"/>
<connect gate="C" pin="IO_32" pad="192"/>
<connect gate="C" pin="IO_33" pad="193"/>
<connect gate="C" pin="IO_34" pad="194"/>
<connect gate="C" pin="IO_35" pad="195"/>
<connect gate="C" pin="IO_36" pad="196"/>
<connect gate="C" pin="IO_37" pad="197"/>
<connect gate="C" pin="IO_38" pad="198"/>
<connect gate="C" pin="IO_39" pad="199"/>
<connect gate="C" pin="IO_4" pad="145"/>
<connect gate="C" pin="IO_40" pad="201"/>
<connect gate="C" pin="IO_41" pad="202"/>
<connect gate="C" pin="IO_42" pad="203"/>
<connect gate="C" pin="IO_43" pad="204"/>
<connect gate="C" pin="IO_44" pad="205"/>
<connect gate="C" pin="IO_5" pad="146"/>
<connect gate="C" pin="IO_6" pad="147"/>
<connect gate="C" pin="IO_7" pad="148"/>
<connect gate="C" pin="IO_8" pad="149"/>
<connect gate="C" pin="IO_9" pad="150"/>
<connect gate="C" pin="N.C." pad="158"/>
<connect gate="C" pin="N.C._2" pad="155"/>
<connect gate="C" pin="N.C._3" pad="156"/>
<connect gate="C" pin="N.C._4" pad="207"/>
<connect gate="C" pin="N.C._5" pad="157"/>
<connect gate="C" pin="N.C._6" pad="208"/>
<connect gate="C" pin="VCCINT" pad="186"/>
<connect gate="C" pin="VCCINT_2" pad="179"/>
<connect gate="C" pin="VCCIO" pad="143"/>
<connect gate="C" pin="VCCIO_2" pad="165"/>
<connect gate="C" pin="VCCIO_3" pad="191"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM3512AQC208-10N"/>
<attribute name="OC_FARNELL" value="1742181"/>
<attribute name="OC_NEWARK" value="51R0515"/>
<attribute name="PACKAGE" value="PQFP-208"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570F100C4N" prefix="U">
<description>IC MAX II CPLD 570 LE 100-FBGA</description>
<gates>
<gate name="A" symbol="EPM570F100C4N"/>
</gates>
<devices>
<device name="" package="BGA100N100P10X10_1100X1100X170">
<connects>
<connect gate="A" pin="GNDINT" pad="C5"/>
<connect gate="A" pin="GNDINT_2" pad="H5"/>
<connect gate="A" pin="GNDINT_3" pad="F5"/>
<connect gate="A" pin="GNDINT_4" pad="E6"/>
<connect gate="A" pin="GNDIO" pad="F6"/>
<connect gate="A" pin="GNDIO_2" pad="D5"/>
<connect gate="A" pin="GNDIO_3" pad="D7"/>
<connect gate="A" pin="GNDIO_4" pad="E5"/>
<connect gate="A" pin="GNDIO_5" pad="G7"/>
<connect gate="A" pin="GNDIO_6" pad="G5"/>
<connect gate="A" pin="IO" pad="D3"/>
<connect gate="A" pin="IO/*DEV_CLR" pad="K9"/>
<connect gate="A" pin="IO/DEV_OE" pad="J7"/>
<connect gate="A" pin="IO/GCLK0" pad="E2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F8"/>
<connect gate="A" pin="IO/GCLK3" pad="E10"/>
<connect gate="A" pin="IO_10" pad="A9"/>
<connect gate="A" pin="IO_11" pad="B1"/>
<connect gate="A" pin="IO_12" pad="B2"/>
<connect gate="A" pin="IO_13" pad="B3"/>
<connect gate="A" pin="IO_14" pad="B4"/>
<connect gate="A" pin="IO_15" pad="B5"/>
<connect gate="A" pin="IO_16" pad="B6"/>
<connect gate="A" pin="IO_17" pad="B7"/>
<connect gate="A" pin="IO_18" pad="B8"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A1"/>
<connect gate="A" pin="IO_20" pad="C1"/>
<connect gate="A" pin="IO_21" pad="C2"/>
<connect gate="A" pin="IO_22" pad="C3"/>
<connect gate="A" pin="IO_23" pad="C4"/>
<connect gate="A" pin="IO_24" pad="D8"/>
<connect gate="A" pin="IO_25" pad="D9"/>
<connect gate="A" pin="IO_26" pad="E3"/>
<connect gate="A" pin="IO_27" pad="E8"/>
<connect gate="A" pin="IO_28" pad="E9"/>
<connect gate="A" pin="IO_29" pad="F1"/>
<connect gate="A" pin="IO_3" pad="A2"/>
<connect gate="A" pin="IO_30" pad="F2"/>
<connect gate="A" pin="IO_31" pad="F3"/>
<connect gate="A" pin="IO_32" pad="F9"/>
<connect gate="A" pin="IO_33" pad="G1"/>
<connect gate="A" pin="IO_34" pad="G2"/>
<connect gate="A" pin="IO_35" pad="G3"/>
<connect gate="A" pin="IO_36" pad="G8"/>
<connect gate="A" pin="IO_37" pad="G9"/>
<connect gate="A" pin="IO_38" pad="H1"/>
<connect gate="A" pin="IO_39" pad="H4"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="H7"/>
<connect gate="A" pin="IO_41" pad="H8"/>
<connect gate="A" pin="IO_42" pad="H9"/>
<connect gate="A" pin="IO_43" pad="J3"/>
<connect gate="A" pin="IO_44" pad="J4"/>
<connect gate="A" pin="IO_45" pad="J5"/>
<connect gate="A" pin="IO_46" pad="J6"/>
<connect gate="A" pin="IO_47" pad="J8"/>
<connect gate="A" pin="IO_48" pad="J9"/>
<connect gate="A" pin="IO_49" pad="K1"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="K2"/>
<connect gate="A" pin="IO_51" pad="K3"/>
<connect gate="A" pin="IO_52" pad="K4"/>
<connect gate="A" pin="IO_53" pad="K5"/>
<connect gate="A" pin="IO_54" pad="K6"/>
<connect gate="A" pin="IO_55" pad="K7"/>
<connect gate="A" pin="IO_56" pad="K8"/>
<connect gate="A" pin="IO_57" pad="A10"/>
<connect gate="A" pin="IO_58" pad="B10"/>
<connect gate="A" pin="IO_59" pad="C10"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_60" pad="D10"/>
<connect gate="A" pin="IO_61" pad="F10"/>
<connect gate="A" pin="IO_62" pad="G10"/>
<connect gate="A" pin="IO_63" pad="H10"/>
<connect gate="A" pin="IO_64" pad="J10"/>
<connect gate="A" pin="IO_65" pad="K10"/>
<connect gate="A" pin="IO_66" pad="C7"/>
<connect gate="A" pin="IO_67" pad="C8"/>
<connect gate="A" pin="IO_68" pad="C9"/>
<connect gate="A" pin="IO_69" pad="D1"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_70" pad="D2"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="A8"/>
<connect gate="A" pin="TCK" pad="H3"/>
<connect gate="A" pin="TDI" pad="H2"/>
<connect gate="A" pin="TDO" pad="J2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="C6"/>
<connect gate="A" pin="VCCINT_2" pad="H6"/>
<connect gate="A" pin="VCCINT_3" pad="F4"/>
<connect gate="A" pin="VCCINT_4" pad="E7"/>
<connect gate="A" pin="VCCIO1" pad="G4"/>
<connect gate="A" pin="VCCIO1_2" pad="E4"/>
<connect gate="A" pin="VCCIO1_3" pad="G6"/>
<connect gate="A" pin="VCCIO2" pad="F7"/>
<connect gate="A" pin="VCCIO2_2" pad="D4"/>
<connect gate="A" pin="VCCIO2_3" pad="D6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570F100C4N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9433"/>
<attribute name="PACKAGE" value="100-FBGA"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570F256C4N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570F256C4N_A"/>
<gate name="B" symbol="EPM570F256C4N_B"/>
<gate name="C" symbol="EPM570F256C4N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="H7"/>
<connect gate="A" pin="GNDINT_3" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J3"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D3"/>
<connect gate="A" pin="IO_26" pad="D1"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="G1"/>
<connect gate="A" pin="IO_35" pad="G2"/>
<connect gate="A" pin="IO_36" pad="F1"/>
<connect gate="A" pin="IO_37" pad="G3"/>
<connect gate="A" pin="IO_38" pad="F2"/>
<connect gate="A" pin="IO_39" pad="H2"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="K3"/>
<connect gate="A" pin="IO_41" pad="H3"/>
<connect gate="A" pin="IO_42" pad="K1"/>
<connect gate="A" pin="IO_43" pad="F3"/>
<connect gate="A" pin="IO_44" pad="H1"/>
<connect gate="A" pin="IO_45" pad="J1"/>
<connect gate="A" pin="IO_46" pad="J2"/>
<connect gate="A" pin="IO_47" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A2"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="NC" pad="E7"/>
<connect gate="A" pin="NC_10" pad="G6"/>
<connect gate="A" pin="NC_11" pad="D6"/>
<connect gate="A" pin="NC_12" pad="H4"/>
<connect gate="A" pin="NC_13" pad="D7"/>
<connect gate="A" pin="NC_14" pad="G5"/>
<connect gate="A" pin="NC_15" pad="D8"/>
<connect gate="A" pin="NC_16" pad="J4"/>
<connect gate="A" pin="NC_17" pad="D9"/>
<connect gate="A" pin="NC_18" pad="K5"/>
<connect gate="A" pin="NC_19" pad="E5"/>
<connect gate="A" pin="NC_2" pad="E8"/>
<connect gate="A" pin="NC_20" pad="E6"/>
<connect gate="A" pin="NC_3" pad="E9"/>
<connect gate="A" pin="NC_4" pad="F4"/>
<connect gate="A" pin="NC_5" pad="F5"/>
<connect gate="A" pin="NC_6" pad="F6"/>
<connect gate="A" pin="NC_7" pad="F7"/>
<connect gate="A" pin="NC_8" pad="K4"/>
<connect gate="A" pin="NC_9" pad="G4"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="J6"/>
<connect gate="A" pin="VCCIO1_3" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="L3"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="P5"/>
<connect gate="B" pin="IO_15" pad="L4"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P6"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N3"/>
<connect gate="B" pin="IO_20" pad="P7"/>
<connect gate="B" pin="IO_21" pad="M2"/>
<connect gate="B" pin="IO_22" pad="N1"/>
<connect gate="B" pin="IO_23" pad="R4"/>
<connect gate="B" pin="IO_24" pad="R5"/>
<connect gate="B" pin="IO_25" pad="R6"/>
<connect gate="B" pin="IO_26" pad="R7"/>
<connect gate="B" pin="IO_27" pad="R8"/>
<connect gate="B" pin="IO_28" pad="R9"/>
<connect gate="B" pin="IO_29" pad="T2"/>
<connect gate="B" pin="IO_3" pad="L1"/>
<connect gate="B" pin="IO_30" pad="T4"/>
<connect gate="B" pin="IO_31" pad="T5"/>
<connect gate="B" pin="IO_32" pad="T6"/>
<connect gate="B" pin="IO_33" pad="T7"/>
<connect gate="B" pin="IO_34" pad="T8"/>
<connect gate="B" pin="IO_35" pad="T9"/>
<connect gate="B" pin="IO_36" pad="A10"/>
<connect gate="B" pin="IO_37" pad="A11"/>
<connect gate="B" pin="IO_38" pad="A12"/>
<connect gate="B" pin="IO_39" pad="A13"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="A15"/>
<connect gate="B" pin="IO_41" pad="B10"/>
<connect gate="B" pin="IO_42" pad="B11"/>
<connect gate="B" pin="IO_43" pad="B12"/>
<connect gate="B" pin="IO_44" pad="B13"/>
<connect gate="B" pin="IO_45" pad="B14"/>
<connect gate="B" pin="IO_46" pad="B16"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M1"/>
<connect gate="B" pin="IO_50" pad="D11"/>
<connect gate="B" pin="IO_51" pad="C13"/>
<connect gate="B" pin="IO_52" pad="D12"/>
<connect gate="B" pin="IO_53" pad="C14"/>
<connect gate="B" pin="IO_54" pad="D13"/>
<connect gate="B" pin="IO_55" pad="C15"/>
<connect gate="B" pin="IO_56" pad="D14"/>
<connect gate="B" pin="IO_57" pad="D15"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_7" pad="L2"/>
<connect gate="B" pin="IO_8" pad="P4"/>
<connect gate="B" pin="IO_9" pad="P9"/>
<connect gate="B" pin="NC" pad="K6"/>
<connect gate="B" pin="NC_10" pad="D10"/>
<connect gate="B" pin="NC_2" pad="L7"/>
<connect gate="B" pin="NC_3" pad="M6"/>
<connect gate="B" pin="NC_4" pad="L5"/>
<connect gate="B" pin="NC_5" pad="M7"/>
<connect gate="B" pin="NC_6" pad="N7"/>
<connect gate="B" pin="NC_7" pad="N8"/>
<connect gate="B" pin="NC_8" pad="N6"/>
<connect gate="B" pin="NC_9" pad="N9"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO1_2" pad="L8"/>
<connect gate="B" pin="VCCIO1_3" pad="L9"/>
<connect gate="B" pin="VCCIO1_4" pad="T3"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO2_2" pad="C16"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="E15"/>
<connect gate="C" pin="IO_11" pad="G15"/>
<connect gate="C" pin="IO_12" pad="H14"/>
<connect gate="C" pin="IO_13" pad="J15"/>
<connect gate="C" pin="IO_14" pad="K14"/>
<connect gate="C" pin="IO_15" pad="E16"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="G16"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="K16"/>
<connect gate="C" pin="IO_2" pad="F13"/>
<connect gate="C" pin="IO_20" pad="J14"/>
<connect gate="C" pin="IO_21" pad="K15"/>
<connect gate="C" pin="IO_22" pad="N12"/>
<connect gate="C" pin="IO_23" pad="L13"/>
<connect gate="C" pin="IO_24" pad="N13"/>
<connect gate="C" pin="IO_25" pad="L14"/>
<connect gate="C" pin="IO_26" pad="N14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="N15"/>
<connect gate="C" pin="IO_29" pad="L16"/>
<connect gate="C" pin="IO_3" pad="F14"/>
<connect gate="C" pin="IO_30" pad="N16"/>
<connect gate="C" pin="IO_31" pad="P10"/>
<connect gate="C" pin="IO_32" pad="P11"/>
<connect gate="C" pin="IO_33" pad="P12"/>
<connect gate="C" pin="IO_34" pad="M13"/>
<connect gate="C" pin="IO_35" pad="P13"/>
<connect gate="C" pin="IO_36" pad="M14"/>
<connect gate="C" pin="IO_37" pad="P14"/>
<connect gate="C" pin="IO_38" pad="M15"/>
<connect gate="C" pin="IO_39" pad="P15"/>
<connect gate="C" pin="IO_4" pad="E13"/>
<connect gate="C" pin="IO_40" pad="M16"/>
<connect gate="C" pin="IO_41" pad="R10"/>
<connect gate="C" pin="IO_42" pad="R11"/>
<connect gate="C" pin="IO_43" pad="R12"/>
<connect gate="C" pin="IO_44" pad="R13"/>
<connect gate="C" pin="IO_45" pad="R14"/>
<connect gate="C" pin="IO_46" pad="R16"/>
<connect gate="C" pin="IO_47" pad="T10"/>
<connect gate="C" pin="IO_48" pad="T11"/>
<connect gate="C" pin="IO_49" pad="T12"/>
<connect gate="C" pin="IO_5" pad="F15"/>
<connect gate="C" pin="IO_50" pad="T13"/>
<connect gate="C" pin="IO_6" pad="H15"/>
<connect gate="C" pin="IO_7" pad="E14"/>
<connect gate="C" pin="IO_8" pad="H16"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="K13"/>
<connect gate="C" pin="NC_10" pad="J13"/>
<connect gate="C" pin="NC_11" pad="G12"/>
<connect gate="C" pin="NC_12" pad="L11"/>
<connect gate="C" pin="NC_13" pad="L10"/>
<connect gate="C" pin="NC_14" pad="N10"/>
<connect gate="C" pin="NC_15" pad="F11"/>
<connect gate="C" pin="NC_16" pad="K11"/>
<connect gate="C" pin="NC_17" pad="G13"/>
<connect gate="C" pin="NC_18" pad="L12"/>
<connect gate="C" pin="NC_19" pad="K12"/>
<connect gate="C" pin="NC_2" pad="E10"/>
<connect gate="C" pin="NC_20" pad="M12"/>
<connect gate="C" pin="NC_21" pad="N11"/>
<connect gate="C" pin="NC_22" pad="F12"/>
<connect gate="C" pin="NC_3" pad="H13"/>
<connect gate="C" pin="NC_4" pad="M10"/>
<connect gate="C" pin="NC_5" pad="E11"/>
<connect gate="C" pin="NC_6" pad="M11"/>
<connect gate="C" pin="NC_7" pad="E12"/>
<connect gate="C" pin="NC_8" pad="G11"/>
<connect gate="C" pin="NC_9" pad="F10"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO1" pad="T14"/>
<connect gate="C" pin="VCCIO2" pad="J11"/>
<connect gate="C" pin="VCCIO2_2" pad="P16"/>
<connect gate="C" pin="VCCIO2_3" pad="H11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570F256C4N"/>
<attribute name="OC_FARNELL" value="1453479"/>
<attribute name="OC_NEWARK" value="51R9439"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570F256C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570F256C5N_A"/>
<gate name="B" symbol="EPM570F256C5N_B"/>
<gate name="C" symbol="EPM570F256C5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C100P16X16_1700X1700X220">
<connects>
<connect gate="A" pin="GNDINT" pad="J8"/>
<connect gate="A" pin="GNDINT_2" pad="H7"/>
<connect gate="A" pin="GNDINT_3" pad="H9"/>
<connect gate="A" pin="GNDIO" pad="G9"/>
<connect gate="A" pin="GNDIO_2" pad="A1"/>
<connect gate="A" pin="GNDIO_3" pad="B2"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="IO" pad="J3"/>
<connect gate="A" pin="IO/GCLK0" pad="H5"/>
<connect gate="A" pin="IO/GCLK1" pad="J5"/>
<connect gate="A" pin="IO_10" pad="B5"/>
<connect gate="A" pin="IO_11" pad="A8"/>
<connect gate="A" pin="IO_12" pad="B9"/>
<connect gate="A" pin="IO_13" pad="C2"/>
<connect gate="A" pin="IO_14" pad="B8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="A6"/>
<connect gate="A" pin="IO_17" pad="C3"/>
<connect gate="A" pin="IO_18" pad="B1"/>
<connect gate="A" pin="IO_19" pad="C4"/>
<connect gate="A" pin="IO_2" pad="B3"/>
<connect gate="A" pin="IO_20" pad="C5"/>
<connect gate="A" pin="IO_21" pad="C6"/>
<connect gate="A" pin="IO_22" pad="C7"/>
<connect gate="A" pin="IO_23" pad="C8"/>
<connect gate="A" pin="IO_24" pad="C9"/>
<connect gate="A" pin="IO_25" pad="D3"/>
<connect gate="A" pin="IO_26" pad="D1"/>
<connect gate="A" pin="IO_27" pad="D4"/>
<connect gate="A" pin="IO_28" pad="D2"/>
<connect gate="A" pin="IO_29" pad="D5"/>
<connect gate="A" pin="IO_3" pad="B4"/>
<connect gate="A" pin="IO_30" pad="E1"/>
<connect gate="A" pin="IO_31" pad="E2"/>
<connect gate="A" pin="IO_32" pad="E3"/>
<connect gate="A" pin="IO_33" pad="E4"/>
<connect gate="A" pin="IO_34" pad="G1"/>
<connect gate="A" pin="IO_35" pad="G2"/>
<connect gate="A" pin="IO_36" pad="F1"/>
<connect gate="A" pin="IO_37" pad="G3"/>
<connect gate="A" pin="IO_38" pad="F2"/>
<connect gate="A" pin="IO_39" pad="H2"/>
<connect gate="A" pin="IO_4" pad="B6"/>
<connect gate="A" pin="IO_40" pad="K3"/>
<connect gate="A" pin="IO_41" pad="H3"/>
<connect gate="A" pin="IO_42" pad="K1"/>
<connect gate="A" pin="IO_43" pad="F3"/>
<connect gate="A" pin="IO_44" pad="H1"/>
<connect gate="A" pin="IO_45" pad="J1"/>
<connect gate="A" pin="IO_46" pad="J2"/>
<connect gate="A" pin="IO_47" pad="K2"/>
<connect gate="A" pin="IO_5" pad="A2"/>
<connect gate="A" pin="IO_6" pad="A7"/>
<connect gate="A" pin="IO_7" pad="A4"/>
<connect gate="A" pin="IO_8" pad="B7"/>
<connect gate="A" pin="IO_9" pad="A5"/>
<connect gate="A" pin="NC" pad="E7"/>
<connect gate="A" pin="NC_10" pad="G6"/>
<connect gate="A" pin="NC_11" pad="D6"/>
<connect gate="A" pin="NC_12" pad="H4"/>
<connect gate="A" pin="NC_13" pad="D7"/>
<connect gate="A" pin="NC_14" pad="G5"/>
<connect gate="A" pin="NC_15" pad="D8"/>
<connect gate="A" pin="NC_16" pad="J4"/>
<connect gate="A" pin="NC_17" pad="D9"/>
<connect gate="A" pin="NC_18" pad="K5"/>
<connect gate="A" pin="NC_19" pad="E5"/>
<connect gate="A" pin="NC_2" pad="E8"/>
<connect gate="A" pin="NC_20" pad="E6"/>
<connect gate="A" pin="NC_3" pad="E9"/>
<connect gate="A" pin="NC_4" pad="F4"/>
<connect gate="A" pin="NC_5" pad="F5"/>
<connect gate="A" pin="NC_6" pad="F6"/>
<connect gate="A" pin="NC_7" pad="F7"/>
<connect gate="A" pin="NC_8" pad="K4"/>
<connect gate="A" pin="NC_9" pad="G4"/>
<connect gate="A" pin="VCCINT" pad="H8"/>
<connect gate="A" pin="VCCINT_2" pad="J9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCIO1" pad="H6"/>
<connect gate="A" pin="VCCIO1_2" pad="J6"/>
<connect gate="A" pin="VCCIO1_3" pad="C1"/>
<connect gate="A" pin="VCCIO2" pad="F9"/>
<connect gate="A" pin="VCCIO2_2" pad="A3"/>
<connect gate="A" pin="VCCIO2_3" pad="F8"/>
<connect gate="B" pin="GNDIO" pad="B15"/>
<connect gate="B" pin="GNDIO_2" pad="K7"/>
<connect gate="B" pin="GNDIO_3" pad="R2"/>
<connect gate="B" pin="GNDIO_4" pad="T1"/>
<connect gate="B" pin="GNDIO_5" pad="K8"/>
<connect gate="B" pin="GNDIO_6" pad="A16"/>
<connect gate="B" pin="GNDIO_7" pad="K9"/>
<connect gate="B" pin="IO" pad="D16"/>
<connect gate="B" pin="IO/DEV_CLRN" pad="M9"/>
<connect gate="B" pin="IO/DEV_OE" pad="M8"/>
<connect gate="B" pin="IO_10" pad="L3"/>
<connect gate="B" pin="IO_11" pad="M3"/>
<connect gate="B" pin="IO_12" pad="N5"/>
<connect gate="B" pin="IO_13" pad="R1"/>
<connect gate="B" pin="IO_14" pad="P5"/>
<connect gate="B" pin="IO_15" pad="L4"/>
<connect gate="B" pin="IO_16" pad="M4"/>
<connect gate="B" pin="IO_17" pad="P2"/>
<connect gate="B" pin="IO_18" pad="P6"/>
<connect gate="B" pin="IO_19" pad="R3"/>
<connect gate="B" pin="IO_2" pad="N3"/>
<connect gate="B" pin="IO_20" pad="P7"/>
<connect gate="B" pin="IO_21" pad="M2"/>
<connect gate="B" pin="IO_22" pad="N1"/>
<connect gate="B" pin="IO_23" pad="R4"/>
<connect gate="B" pin="IO_24" pad="R5"/>
<connect gate="B" pin="IO_25" pad="R6"/>
<connect gate="B" pin="IO_26" pad="R7"/>
<connect gate="B" pin="IO_27" pad="R8"/>
<connect gate="B" pin="IO_28" pad="R9"/>
<connect gate="B" pin="IO_29" pad="T2"/>
<connect gate="B" pin="IO_3" pad="L1"/>
<connect gate="B" pin="IO_30" pad="T4"/>
<connect gate="B" pin="IO_31" pad="T5"/>
<connect gate="B" pin="IO_32" pad="T6"/>
<connect gate="B" pin="IO_33" pad="T7"/>
<connect gate="B" pin="IO_34" pad="T8"/>
<connect gate="B" pin="IO_35" pad="T9"/>
<connect gate="B" pin="IO_36" pad="A10"/>
<connect gate="B" pin="IO_37" pad="A11"/>
<connect gate="B" pin="IO_38" pad="A12"/>
<connect gate="B" pin="IO_39" pad="A13"/>
<connect gate="B" pin="IO_4" pad="N2"/>
<connect gate="B" pin="IO_40" pad="A15"/>
<connect gate="B" pin="IO_41" pad="B10"/>
<connect gate="B" pin="IO_42" pad="B11"/>
<connect gate="B" pin="IO_43" pad="B12"/>
<connect gate="B" pin="IO_44" pad="B13"/>
<connect gate="B" pin="IO_45" pad="B14"/>
<connect gate="B" pin="IO_46" pad="B16"/>
<connect gate="B" pin="IO_47" pad="C10"/>
<connect gate="B" pin="IO_48" pad="C11"/>
<connect gate="B" pin="IO_49" pad="C12"/>
<connect gate="B" pin="IO_5" pad="M1"/>
<connect gate="B" pin="IO_50" pad="D11"/>
<connect gate="B" pin="IO_51" pad="C13"/>
<connect gate="B" pin="IO_52" pad="D12"/>
<connect gate="B" pin="IO_53" pad="C14"/>
<connect gate="B" pin="IO_54" pad="D13"/>
<connect gate="B" pin="IO_55" pad="C15"/>
<connect gate="B" pin="IO_56" pad="D14"/>
<connect gate="B" pin="IO_57" pad="D15"/>
<connect gate="B" pin="IO_6" pad="P8"/>
<connect gate="B" pin="IO_7" pad="L2"/>
<connect gate="B" pin="IO_8" pad="P4"/>
<connect gate="B" pin="IO_9" pad="P9"/>
<connect gate="B" pin="NC" pad="K6"/>
<connect gate="B" pin="NC_10" pad="D10"/>
<connect gate="B" pin="NC_2" pad="L7"/>
<connect gate="B" pin="NC_3" pad="M6"/>
<connect gate="B" pin="NC_4" pad="L5"/>
<connect gate="B" pin="NC_5" pad="M7"/>
<connect gate="B" pin="NC_6" pad="N7"/>
<connect gate="B" pin="NC_7" pad="N8"/>
<connect gate="B" pin="NC_8" pad="N6"/>
<connect gate="B" pin="NC_9" pad="N9"/>
<connect gate="B" pin="TCK" pad="P3"/>
<connect gate="B" pin="TDI" pad="L6"/>
<connect gate="B" pin="TDO" pad="M5"/>
<connect gate="B" pin="TMS" pad="N4"/>
<connect gate="B" pin="VCCIO1" pad="P1"/>
<connect gate="B" pin="VCCIO1_2" pad="L8"/>
<connect gate="B" pin="VCCIO1_3" pad="L9"/>
<connect gate="B" pin="VCCIO1_4" pad="T3"/>
<connect gate="B" pin="VCCIO2" pad="A14"/>
<connect gate="B" pin="VCCIO2_2" pad="C16"/>
<connect gate="C" pin="GNDINT" pad="J10"/>
<connect gate="C" pin="GNDIO" pad="K10"/>
<connect gate="C" pin="GNDIO_2" pad="R15"/>
<connect gate="C" pin="GNDIO_3" pad="T16"/>
<connect gate="C" pin="GNDIO_4" pad="G10"/>
<connect gate="C" pin="IO" pad="T15"/>
<connect gate="C" pin="IO/GCLK2" pad="J12"/>
<connect gate="C" pin="IO/GCLK3" pad="H12"/>
<connect gate="C" pin="IO_10" pad="E15"/>
<connect gate="C" pin="IO_11" pad="G15"/>
<connect gate="C" pin="IO_12" pad="H14"/>
<connect gate="C" pin="IO_13" pad="J15"/>
<connect gate="C" pin="IO_14" pad="K14"/>
<connect gate="C" pin="IO_15" pad="E16"/>
<connect gate="C" pin="IO_16" pad="J16"/>
<connect gate="C" pin="IO_17" pad="G16"/>
<connect gate="C" pin="IO_18" pad="G14"/>
<connect gate="C" pin="IO_19" pad="K16"/>
<connect gate="C" pin="IO_2" pad="F13"/>
<connect gate="C" pin="IO_20" pad="J14"/>
<connect gate="C" pin="IO_21" pad="K15"/>
<connect gate="C" pin="IO_22" pad="N12"/>
<connect gate="C" pin="IO_23" pad="L13"/>
<connect gate="C" pin="IO_24" pad="N13"/>
<connect gate="C" pin="IO_25" pad="L14"/>
<connect gate="C" pin="IO_26" pad="N14"/>
<connect gate="C" pin="IO_27" pad="L15"/>
<connect gate="C" pin="IO_28" pad="N15"/>
<connect gate="C" pin="IO_29" pad="L16"/>
<connect gate="C" pin="IO_3" pad="F14"/>
<connect gate="C" pin="IO_30" pad="N16"/>
<connect gate="C" pin="IO_31" pad="P10"/>
<connect gate="C" pin="IO_32" pad="P11"/>
<connect gate="C" pin="IO_33" pad="P12"/>
<connect gate="C" pin="IO_34" pad="M13"/>
<connect gate="C" pin="IO_35" pad="P13"/>
<connect gate="C" pin="IO_36" pad="M14"/>
<connect gate="C" pin="IO_37" pad="P14"/>
<connect gate="C" pin="IO_38" pad="M15"/>
<connect gate="C" pin="IO_39" pad="P15"/>
<connect gate="C" pin="IO_4" pad="E13"/>
<connect gate="C" pin="IO_40" pad="M16"/>
<connect gate="C" pin="IO_41" pad="R10"/>
<connect gate="C" pin="IO_42" pad="R11"/>
<connect gate="C" pin="IO_43" pad="R12"/>
<connect gate="C" pin="IO_44" pad="R13"/>
<connect gate="C" pin="IO_45" pad="R14"/>
<connect gate="C" pin="IO_46" pad="R16"/>
<connect gate="C" pin="IO_47" pad="T10"/>
<connect gate="C" pin="IO_48" pad="T11"/>
<connect gate="C" pin="IO_49" pad="T12"/>
<connect gate="C" pin="IO_5" pad="F15"/>
<connect gate="C" pin="IO_50" pad="T13"/>
<connect gate="C" pin="IO_6" pad="H15"/>
<connect gate="C" pin="IO_7" pad="E14"/>
<connect gate="C" pin="IO_8" pad="H16"/>
<connect gate="C" pin="IO_9" pad="F16"/>
<connect gate="C" pin="NC" pad="K13"/>
<connect gate="C" pin="NC_10" pad="J13"/>
<connect gate="C" pin="NC_11" pad="G12"/>
<connect gate="C" pin="NC_12" pad="L11"/>
<connect gate="C" pin="NC_13" pad="L10"/>
<connect gate="C" pin="NC_14" pad="N10"/>
<connect gate="C" pin="NC_15" pad="F11"/>
<connect gate="C" pin="NC_16" pad="K11"/>
<connect gate="C" pin="NC_17" pad="G13"/>
<connect gate="C" pin="NC_18" pad="L12"/>
<connect gate="C" pin="NC_19" pad="K12"/>
<connect gate="C" pin="NC_2" pad="E10"/>
<connect gate="C" pin="NC_20" pad="M12"/>
<connect gate="C" pin="NC_21" pad="N11"/>
<connect gate="C" pin="NC_22" pad="F12"/>
<connect gate="C" pin="NC_3" pad="H13"/>
<connect gate="C" pin="NC_4" pad="M10"/>
<connect gate="C" pin="NC_5" pad="E11"/>
<connect gate="C" pin="NC_6" pad="M11"/>
<connect gate="C" pin="NC_7" pad="E12"/>
<connect gate="C" pin="NC_8" pad="G11"/>
<connect gate="C" pin="NC_9" pad="F10"/>
<connect gate="C" pin="VCCINT" pad="H10"/>
<connect gate="C" pin="VCCIO1" pad="T14"/>
<connect gate="C" pin="VCCIO2" pad="J11"/>
<connect gate="C" pin="VCCIO2_2" pad="P16"/>
<connect gate="C" pin="VCCIO2_3" pad="H11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570F256C5N"/>
<attribute name="OC_FARNELL" value="1453483"/>
<attribute name="OC_NEWARK" value="51R0517"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570GF100C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570GF100C5N"/>
</gates>
<devices>
<device name="" package="BGA100C100P10X10_1100X1100X170">
<connects>
<connect gate="A" pin="GNDINT" pad="E6"/>
<connect gate="A" pin="GNDINT_2" pad="C5"/>
<connect gate="A" pin="GNDINT_3" pad="F5"/>
<connect gate="A" pin="GNDINT_4" pad="H5"/>
<connect gate="A" pin="GNDIO" pad="G5"/>
<connect gate="A" pin="GNDIO_2" pad="D5"/>
<connect gate="A" pin="GNDIO_3" pad="D7"/>
<connect gate="A" pin="GNDIO_4" pad="G7"/>
<connect gate="A" pin="GNDIO_5" pad="E5"/>
<connect gate="A" pin="GNDIO_6" pad="F6"/>
<connect gate="A" pin="IO" pad="C10"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="K9"/>
<connect gate="A" pin="IO/DEV_OE" pad="J7"/>
<connect gate="A" pin="IO/GCLK0" pad="E2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F8"/>
<connect gate="A" pin="IO/GCLK3" pad="E10"/>
<connect gate="A" pin="IO_10" pad="A4"/>
<connect gate="A" pin="IO_11" pad="A5"/>
<connect gate="A" pin="IO_12" pad="A6"/>
<connect gate="A" pin="IO_13" pad="A7"/>
<connect gate="A" pin="IO_14" pad="A8"/>
<connect gate="A" pin="IO_15" pad="A9"/>
<connect gate="A" pin="IO_16" pad="B1"/>
<connect gate="A" pin="IO_17" pad="B2"/>
<connect gate="A" pin="IO_18" pad="B3"/>
<connect gate="A" pin="IO_19" pad="B4"/>
<connect gate="A" pin="IO_2" pad="E8"/>
<connect gate="A" pin="IO_20" pad="B5"/>
<connect gate="A" pin="IO_21" pad="B6"/>
<connect gate="A" pin="IO_22" pad="B7"/>
<connect gate="A" pin="IO_23" pad="B8"/>
<connect gate="A" pin="IO_24" pad="B9"/>
<connect gate="A" pin="IO_25" pad="C1"/>
<connect gate="A" pin="IO_26" pad="C2"/>
<connect gate="A" pin="IO_27" pad="C3"/>
<connect gate="A" pin="IO_28" pad="C7"/>
<connect gate="A" pin="IO_29" pad="C4"/>
<connect gate="A" pin="IO_3" pad="E9"/>
<connect gate="A" pin="IO_30" pad="C8"/>
<connect gate="A" pin="IO_31" pad="C9"/>
<connect gate="A" pin="IO_32" pad="D1"/>
<connect gate="A" pin="IO_33" pad="D2"/>
<connect gate="A" pin="IO_34" pad="D3"/>
<connect gate="A" pin="IO_35" pad="D8"/>
<connect gate="A" pin="IO_36" pad="D9"/>
<connect gate="A" pin="IO_37" pad="E3"/>
<connect gate="A" pin="IO_38" pad="F9"/>
<connect gate="A" pin="IO_39" pad="G1"/>
<connect gate="A" pin="IO_4" pad="F1"/>
<connect gate="A" pin="IO_40" pad="G2"/>
<connect gate="A" pin="IO_41" pad="G3"/>
<connect gate="A" pin="IO_42" pad="G8"/>
<connect gate="A" pin="IO_43" pad="G9"/>
<connect gate="A" pin="IO_44" pad="J4"/>
<connect gate="A" pin="IO_45" pad="H1"/>
<connect gate="A" pin="IO_46" pad="J8"/>
<connect gate="A" pin="IO_47" pad="H4"/>
<connect gate="A" pin="IO_48" pad="J5"/>
<connect gate="A" pin="IO_49" pad="H7"/>
<connect gate="A" pin="IO_5" pad="F2"/>
<connect gate="A" pin="IO_50" pad="J9"/>
<connect gate="A" pin="IO_51" pad="H8"/>
<connect gate="A" pin="IO_52" pad="J6"/>
<connect gate="A" pin="IO_53" pad="H9"/>
<connect gate="A" pin="IO_54" pad="K1"/>
<connect gate="A" pin="IO_55" pad="K2"/>
<connect gate="A" pin="IO_56" pad="K3"/>
<connect gate="A" pin="IO_57" pad="J3"/>
<connect gate="A" pin="IO_58" pad="D10"/>
<connect gate="A" pin="IO_59" pad="K4"/>
<connect gate="A" pin="IO_6" pad="F3"/>
<connect gate="A" pin="IO_60" pad="K5"/>
<connect gate="A" pin="IO_61" pad="F10"/>
<connect gate="A" pin="IO_62" pad="K6"/>
<connect gate="A" pin="IO_63" pad="G10"/>
<connect gate="A" pin="IO_64" pad="K7"/>
<connect gate="A" pin="IO_65" pad="H10"/>
<connect gate="A" pin="IO_66" pad="K8"/>
<connect gate="A" pin="IO_67" pad="J10"/>
<connect gate="A" pin="IO_68" pad="K10"/>
<connect gate="A" pin="IO_69" pad="A10"/>
<connect gate="A" pin="IO_7" pad="A1"/>
<connect gate="A" pin="IO_70" pad="B10"/>
<connect gate="A" pin="IO_8" pad="A2"/>
<connect gate="A" pin="IO_9" pad="A3"/>
<connect gate="A" pin="TCK" pad="H3"/>
<connect gate="A" pin="TDI" pad="H2"/>
<connect gate="A" pin="TDO" pad="J2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="H6"/>
<connect gate="A" pin="VCCINT_2" pad="C6"/>
<connect gate="A" pin="VCCINT_3" pad="E7"/>
<connect gate="A" pin="VCCINT_4" pad="F4"/>
<connect gate="A" pin="VCCIO1" pad="E4"/>
<connect gate="A" pin="VCCIO1_2" pad="G4"/>
<connect gate="A" pin="VCCIO1_3" pad="G6"/>
<connect gate="A" pin="VCCIO2" pad="F7"/>
<connect gate="A" pin="VCCIO2_2" pad="D6"/>
<connect gate="A" pin="VCCIO2_3" pad="D4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570GF100C5N"/>
<attribute name="OC_FARNELL" value="1549461"/>
<attribute name="OC_NEWARK" value="51R9443"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570GM100C5N">
<description>IC MAX II CPLD 570 LE 100-MBGA</description>
<gates>
<gate name="A" symbol="EPM570GM100C5N"/>
</gates>
<devices>
<device name="" package="BGA100C50P11X11_600X600X120">
<connects>
<connect gate="A" pin="GNDINT" pad="E8"/>
<connect gate="A" pin="GNDINT_2" pad="C5"/>
<connect gate="A" pin="GNDINT_3" pad="G4"/>
<connect gate="A" pin="GNDINT_4" pad="J5"/>
<connect gate="A" pin="GNDIO" pad="H7"/>
<connect gate="A" pin="GNDIO_2" pad="D5"/>
<connect gate="A" pin="GNDIO_3" pad="E4"/>
<connect gate="A" pin="GNDIO_4" pad="D7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="GNDIO_6" pad="H5"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="K8"/>
<connect gate="A" pin="IO/DEV_OE" pad="L8"/>
<connect gate="A" pin="IO/GCLK0" pad="F2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F10"/>
<connect gate="A" pin="IO/GCLK3" pad="G11"/>
<connect gate="A" pin="IO_10" pad="D11"/>
<connect gate="A" pin="IO_11" pad="E10"/>
<connect gate="A" pin="IO_12" pad="E11"/>
<connect gate="A" pin="IO_13" pad="F11"/>
<connect gate="A" pin="IO_14" pad="G10"/>
<connect gate="A" pin="IO_15" pad="H10"/>
<connect gate="A" pin="IO_16" pad="H11"/>
<connect gate="A" pin="IO_17" pad="J10"/>
<connect gate="A" pin="IO_18" pad="J11"/>
<connect gate="A" pin="IO_19" pad="K10"/>
<connect gate="A" pin="IO_2" pad="L9"/>
<connect gate="A" pin="IO_20" pad="K11"/>
<connect gate="A" pin="IO_21" pad="L10"/>
<connect gate="A" pin="IO_22" pad="L11"/>
<connect gate="A" pin="IO_23" pad="A1"/>
<connect gate="A" pin="IO_24" pad="A2"/>
<connect gate="A" pin="IO_25" pad="A3"/>
<connect gate="A" pin="IO_26" pad="A4"/>
<connect gate="A" pin="IO_27" pad="A5"/>
<connect gate="A" pin="IO_28" pad="A6"/>
<connect gate="A" pin="IO_29" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A10"/>
<connect gate="A" pin="IO_30" pad="A8"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="B1"/>
<connect gate="A" pin="IO_33" pad="B2"/>
<connect gate="A" pin="IO_34" pad="B3"/>
<connect gate="A" pin="IO_35" pad="B4"/>
<connect gate="A" pin="IO_36" pad="B5"/>
<connect gate="A" pin="IO_37" pad="B6"/>
<connect gate="A" pin="IO_38" pad="B7"/>
<connect gate="A" pin="IO_39" pad="B8"/>
<connect gate="A" pin="IO_4" pad="A11"/>
<connect gate="A" pin="IO_40" pad="B9"/>
<connect gate="A" pin="IO_41" pad="C1"/>
<connect gate="A" pin="IO_42" pad="C2"/>
<connect gate="A" pin="IO_43" pad="C6"/>
<connect gate="A" pin="IO_44" pad="D1"/>
<connect gate="A" pin="IO_45" pad="D2"/>
<connect gate="A" pin="IO_46" pad="D3"/>
<connect gate="A" pin="IO_47" pad="D9"/>
<connect gate="A" pin="IO_48" pad="E2"/>
<connect gate="A" pin="IO_49" pad="F1"/>
<connect gate="A" pin="IO_5" pad="B10"/>
<connect gate="A" pin="IO_50" pad="F3"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="H1"/>
<connect gate="A" pin="IO_55" pad="H2"/>
<connect gate="A" pin="IO_56" pad="H3"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J6"/>
<connect gate="A" pin="IO_59" pad="K3"/>
<connect gate="A" pin="IO_6" pad="B11"/>
<connect gate="A" pin="IO_60" pad="K4"/>
<connect gate="A" pin="IO_61" pad="K5"/>
<connect gate="A" pin="IO_62" pad="K6"/>
<connect gate="A" pin="IO_63" pad="K7"/>
<connect gate="A" pin="IO_64" pad="K9"/>
<connect gate="A" pin="IO_65" pad="L1"/>
<connect gate="A" pin="IO_66" pad="L2"/>
<connect gate="A" pin="IO_67" pad="L3"/>
<connect gate="A" pin="IO_68" pad="L4"/>
<connect gate="A" pin="IO_69" pad="L5"/>
<connect gate="A" pin="IO_7" pad="C10"/>
<connect gate="A" pin="IO_70" pad="L6"/>
<connect gate="A" pin="IO_8" pad="C11"/>
<connect gate="A" pin="IO_9" pad="D10"/>
<connect gate="A" pin="TCK" pad="K1"/>
<connect gate="A" pin="TDI" pad="J2"/>
<connect gate="A" pin="TDO" pad="K2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="G3"/>
<connect gate="A" pin="VCCINT_2" pad="C7"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCINT_4" pad="E9"/>
<connect gate="A" pin="VCCIO1" pad="J8"/>
<connect gate="A" pin="VCCIO1_2" pad="E3"/>
<connect gate="A" pin="VCCIO1_3" pad="J4"/>
<connect gate="A" pin="VCCIO2" pad="G9"/>
<connect gate="A" pin="VCCIO2_2" pad="C8"/>
<connect gate="A" pin="VCCIO2_3" pad="C4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570GM100C5N"/>
<attribute name="OC_FARNELL" value="1549463"/>
<attribute name="OC_NEWARK" value="51R9453"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570GT100C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570GT100C5N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="65"/>
<connect gate="A" pin="GNDINT_2" pad="11"/>
<connect gate="A" pin="GNDINT_3" pad="37"/>
<connect gate="A" pin="GNDINT_4" pad="90"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="10"/>
<connect gate="A" pin="GNDIO_3" pad="46"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="GNDIO_5" pad="60"/>
<connect gate="A" pin="GNDIO_6" pad="93"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="5"/>
<connect gate="A" pin="IO_11" pad="19"/>
<connect gate="A" pin="IO_12" pad="6"/>
<connect gate="A" pin="IO_13" pad="20"/>
<connect gate="A" pin="IO_14" pad="40"/>
<connect gate="A" pin="IO_15" pad="7"/>
<connect gate="A" pin="IO_16" pad="41"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="42"/>
<connect gate="A" pin="IO_19" pad="8"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="34"/>
<connect gate="A" pin="IO_22" pad="35"/>
<connect gate="A" pin="IO_23" pad="36"/>
<connect gate="A" pin="IO_24" pad="47"/>
<connect gate="A" pin="IO_25" pad="26"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="27"/>
<connect gate="A" pin="IO_28" pad="49"/>
<connect gate="A" pin="IO_29" pad="38"/>
<connect gate="A" pin="IO_3" pad="15"/>
<connect gate="A" pin="IO_30" pad="50"/>
<connect gate="A" pin="IO_31" pad="28"/>
<connect gate="A" pin="IO_32" pad="29"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="52"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="2"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="66"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_49" pad="72"/>
<connect gate="A" pin="IO_5" pad="16"/>
<connect gate="A" pin="IO_50" pad="73"/>
<connect gate="A" pin="IO_51" pad="74"/>
<connect gate="A" pin="IO_52" pad="75"/>
<connect gate="A" pin="IO_53" pad="76"/>
<connect gate="A" pin="IO_54" pad="77"/>
<connect gate="A" pin="IO_55" pad="78"/>
<connect gate="A" pin="IO_56" pad="81"/>
<connect gate="A" pin="IO_57" pad="82"/>
<connect gate="A" pin="IO_58" pad="83"/>
<connect gate="A" pin="IO_59" pad="84"/>
<connect gate="A" pin="IO_6" pad="3"/>
<connect gate="A" pin="IO_60" pad="85"/>
<connect gate="A" pin="IO_61" pad="86"/>
<connect gate="A" pin="IO_62" pad="87"/>
<connect gate="A" pin="IO_63" pad="89"/>
<connect gate="A" pin="IO_64" pad="91"/>
<connect gate="A" pin="IO_65" pad="92"/>
<connect gate="A" pin="IO_66" pad="95"/>
<connect gate="A" pin="IO_67" pad="96"/>
<connect gate="A" pin="IO_68" pad="97"/>
<connect gate="A" pin="IO_69" pad="98"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_70" pad="99"/>
<connect gate="A" pin="IO_8" pad="4"/>
<connect gate="A" pin="IO_9" pad="18"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCINT_3" pad="39"/>
<connect gate="A" pin="VCCINT_4" pad="88"/>
<connect gate="A" pin="VCCIO1" pad="45"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="31"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570GT100C5N"/>
<attribute name="OC_FARNELL" value="1549469"/>
<attribute name="OC_NEWARK" value="51R9462"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570GT144C3N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570GT144C3N_A"/>
<gate name="B" symbol="EPM570GT144C3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="64"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO1_3" pad="9"/>
<connect gate="A" pin="VCCIO1_4" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="100"/>
<connect gate="B" pin="VCCIO2_3" pad="82"/>
<connect gate="B" pin="VCCIO2_4" pad="116"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570GT144C3N"/>
<attribute name="OC_FARNELL" value="1549474"/>
<attribute name="OC_NEWARK" value="51R9466"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570M100C4N">
<description>IC MAX II CPLD 570 LE 100-MBGA</description>
<gates>
<gate name="A" symbol="EPM570M100C4N"/>
</gates>
<devices>
<device name="" package="BGA100C50P11X11_600X600X120">
<connects>
<connect gate="A" pin="GNDINT" pad="E8"/>
<connect gate="A" pin="GNDINT_2" pad="C5"/>
<connect gate="A" pin="GNDINT_3" pad="G4"/>
<connect gate="A" pin="GNDINT_4" pad="J5"/>
<connect gate="A" pin="GNDIO" pad="H7"/>
<connect gate="A" pin="GNDIO_2" pad="D5"/>
<connect gate="A" pin="GNDIO_3" pad="E4"/>
<connect gate="A" pin="GNDIO_4" pad="D7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="GNDIO_6" pad="H5"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="K8"/>
<connect gate="A" pin="IO/DEV_OE" pad="L8"/>
<connect gate="A" pin="IO/GCLK0" pad="F2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F10"/>
<connect gate="A" pin="IO/GCLK3" pad="G11"/>
<connect gate="A" pin="IO_10" pad="D11"/>
<connect gate="A" pin="IO_11" pad="E10"/>
<connect gate="A" pin="IO_12" pad="E11"/>
<connect gate="A" pin="IO_13" pad="F11"/>
<connect gate="A" pin="IO_14" pad="G10"/>
<connect gate="A" pin="IO_15" pad="H10"/>
<connect gate="A" pin="IO_16" pad="H11"/>
<connect gate="A" pin="IO_17" pad="J10"/>
<connect gate="A" pin="IO_18" pad="J11"/>
<connect gate="A" pin="IO_19" pad="K10"/>
<connect gate="A" pin="IO_2" pad="L9"/>
<connect gate="A" pin="IO_20" pad="K11"/>
<connect gate="A" pin="IO_21" pad="L10"/>
<connect gate="A" pin="IO_22" pad="L11"/>
<connect gate="A" pin="IO_23" pad="A1"/>
<connect gate="A" pin="IO_24" pad="A2"/>
<connect gate="A" pin="IO_25" pad="A3"/>
<connect gate="A" pin="IO_26" pad="A4"/>
<connect gate="A" pin="IO_27" pad="A5"/>
<connect gate="A" pin="IO_28" pad="A6"/>
<connect gate="A" pin="IO_29" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A10"/>
<connect gate="A" pin="IO_30" pad="A8"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="B1"/>
<connect gate="A" pin="IO_33" pad="B2"/>
<connect gate="A" pin="IO_34" pad="B3"/>
<connect gate="A" pin="IO_35" pad="B4"/>
<connect gate="A" pin="IO_36" pad="B5"/>
<connect gate="A" pin="IO_37" pad="B6"/>
<connect gate="A" pin="IO_38" pad="B7"/>
<connect gate="A" pin="IO_39" pad="B8"/>
<connect gate="A" pin="IO_4" pad="A11"/>
<connect gate="A" pin="IO_40" pad="B9"/>
<connect gate="A" pin="IO_41" pad="C1"/>
<connect gate="A" pin="IO_42" pad="C2"/>
<connect gate="A" pin="IO_43" pad="C6"/>
<connect gate="A" pin="IO_44" pad="D1"/>
<connect gate="A" pin="IO_45" pad="D2"/>
<connect gate="A" pin="IO_46" pad="D3"/>
<connect gate="A" pin="IO_47" pad="D9"/>
<connect gate="A" pin="IO_48" pad="E2"/>
<connect gate="A" pin="IO_49" pad="F1"/>
<connect gate="A" pin="IO_5" pad="B10"/>
<connect gate="A" pin="IO_50" pad="F3"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="H1"/>
<connect gate="A" pin="IO_55" pad="H2"/>
<connect gate="A" pin="IO_56" pad="H3"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J6"/>
<connect gate="A" pin="IO_59" pad="K3"/>
<connect gate="A" pin="IO_6" pad="B11"/>
<connect gate="A" pin="IO_60" pad="K4"/>
<connect gate="A" pin="IO_61" pad="K5"/>
<connect gate="A" pin="IO_62" pad="K6"/>
<connect gate="A" pin="IO_63" pad="K7"/>
<connect gate="A" pin="IO_64" pad="K9"/>
<connect gate="A" pin="IO_65" pad="L1"/>
<connect gate="A" pin="IO_66" pad="L2"/>
<connect gate="A" pin="IO_67" pad="L3"/>
<connect gate="A" pin="IO_68" pad="L4"/>
<connect gate="A" pin="IO_69" pad="L5"/>
<connect gate="A" pin="IO_7" pad="C10"/>
<connect gate="A" pin="IO_70" pad="L6"/>
<connect gate="A" pin="IO_8" pad="C11"/>
<connect gate="A" pin="IO_9" pad="D10"/>
<connect gate="A" pin="TCK" pad="K1"/>
<connect gate="A" pin="TDI" pad="J2"/>
<connect gate="A" pin="TDO" pad="K2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="G3"/>
<connect gate="A" pin="VCCINT_2" pad="C7"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCINT_4" pad="E9"/>
<connect gate="A" pin="VCCIO1" pad="J8"/>
<connect gate="A" pin="VCCIO1_2" pad="E3"/>
<connect gate="A" pin="VCCIO1_3" pad="J4"/>
<connect gate="A" pin="VCCIO2" pad="G9"/>
<connect gate="A" pin="VCCIO2_2" pad="C8"/>
<connect gate="A" pin="VCCIO2_3" pad="C4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570M100C4N"/>
<attribute name="OC_FARNELL" value="1549464"/>
<attribute name="OC_NEWARK" value="51R9473"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570M100C5N">
<description>IC MAX II CPLD 570 LE 100-MBGA</description>
<gates>
<gate name="A" symbol="EPM570M100C5N"/>
</gates>
<devices>
<device name="" package="BGA100C50P11X11_600X600X120">
<connects>
<connect gate="A" pin="GNDINT" pad="E8"/>
<connect gate="A" pin="GNDINT_2" pad="C5"/>
<connect gate="A" pin="GNDINT_3" pad="G4"/>
<connect gate="A" pin="GNDINT_4" pad="J5"/>
<connect gate="A" pin="GNDIO" pad="H7"/>
<connect gate="A" pin="GNDIO_2" pad="D5"/>
<connect gate="A" pin="GNDIO_3" pad="E4"/>
<connect gate="A" pin="GNDIO_4" pad="D7"/>
<connect gate="A" pin="GNDIO_5" pad="G8"/>
<connect gate="A" pin="GNDIO_6" pad="H5"/>
<connect gate="A" pin="IO" pad="L7"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="K8"/>
<connect gate="A" pin="IO/DEV_OE" pad="L8"/>
<connect gate="A" pin="IO/GCLK0" pad="F2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F10"/>
<connect gate="A" pin="IO/GCLK3" pad="G11"/>
<connect gate="A" pin="IO_10" pad="D11"/>
<connect gate="A" pin="IO_11" pad="E10"/>
<connect gate="A" pin="IO_12" pad="E11"/>
<connect gate="A" pin="IO_13" pad="F11"/>
<connect gate="A" pin="IO_14" pad="G10"/>
<connect gate="A" pin="IO_15" pad="H10"/>
<connect gate="A" pin="IO_16" pad="H11"/>
<connect gate="A" pin="IO_17" pad="J10"/>
<connect gate="A" pin="IO_18" pad="J11"/>
<connect gate="A" pin="IO_19" pad="K10"/>
<connect gate="A" pin="IO_2" pad="L9"/>
<connect gate="A" pin="IO_20" pad="K11"/>
<connect gate="A" pin="IO_21" pad="L10"/>
<connect gate="A" pin="IO_22" pad="L11"/>
<connect gate="A" pin="IO_23" pad="A1"/>
<connect gate="A" pin="IO_24" pad="A2"/>
<connect gate="A" pin="IO_25" pad="A3"/>
<connect gate="A" pin="IO_26" pad="A4"/>
<connect gate="A" pin="IO_27" pad="A5"/>
<connect gate="A" pin="IO_28" pad="A6"/>
<connect gate="A" pin="IO_29" pad="A7"/>
<connect gate="A" pin="IO_3" pad="A10"/>
<connect gate="A" pin="IO_30" pad="A8"/>
<connect gate="A" pin="IO_31" pad="A9"/>
<connect gate="A" pin="IO_32" pad="B1"/>
<connect gate="A" pin="IO_33" pad="B2"/>
<connect gate="A" pin="IO_34" pad="B3"/>
<connect gate="A" pin="IO_35" pad="B4"/>
<connect gate="A" pin="IO_36" pad="B5"/>
<connect gate="A" pin="IO_37" pad="B6"/>
<connect gate="A" pin="IO_38" pad="B7"/>
<connect gate="A" pin="IO_39" pad="B8"/>
<connect gate="A" pin="IO_4" pad="A11"/>
<connect gate="A" pin="IO_40" pad="B9"/>
<connect gate="A" pin="IO_41" pad="C1"/>
<connect gate="A" pin="IO_42" pad="C2"/>
<connect gate="A" pin="IO_43" pad="C6"/>
<connect gate="A" pin="IO_44" pad="D1"/>
<connect gate="A" pin="IO_45" pad="D2"/>
<connect gate="A" pin="IO_46" pad="D3"/>
<connect gate="A" pin="IO_47" pad="D9"/>
<connect gate="A" pin="IO_48" pad="E2"/>
<connect gate="A" pin="IO_49" pad="F1"/>
<connect gate="A" pin="IO_5" pad="B10"/>
<connect gate="A" pin="IO_50" pad="F3"/>
<connect gate="A" pin="IO_51" pad="F9"/>
<connect gate="A" pin="IO_52" pad="G1"/>
<connect gate="A" pin="IO_53" pad="G2"/>
<connect gate="A" pin="IO_54" pad="H1"/>
<connect gate="A" pin="IO_55" pad="H2"/>
<connect gate="A" pin="IO_56" pad="H3"/>
<connect gate="A" pin="IO_57" pad="H9"/>
<connect gate="A" pin="IO_58" pad="J6"/>
<connect gate="A" pin="IO_59" pad="K3"/>
<connect gate="A" pin="IO_6" pad="B11"/>
<connect gate="A" pin="IO_60" pad="K4"/>
<connect gate="A" pin="IO_61" pad="K5"/>
<connect gate="A" pin="IO_62" pad="K6"/>
<connect gate="A" pin="IO_63" pad="K7"/>
<connect gate="A" pin="IO_64" pad="K9"/>
<connect gate="A" pin="IO_65" pad="L1"/>
<connect gate="A" pin="IO_66" pad="L2"/>
<connect gate="A" pin="IO_67" pad="L3"/>
<connect gate="A" pin="IO_68" pad="L4"/>
<connect gate="A" pin="IO_69" pad="L5"/>
<connect gate="A" pin="IO_7" pad="C10"/>
<connect gate="A" pin="IO_70" pad="L6"/>
<connect gate="A" pin="IO_8" pad="C11"/>
<connect gate="A" pin="IO_9" pad="D10"/>
<connect gate="A" pin="TCK" pad="K1"/>
<connect gate="A" pin="TDI" pad="J2"/>
<connect gate="A" pin="TDO" pad="K2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="G3"/>
<connect gate="A" pin="VCCINT_2" pad="C7"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCINT_4" pad="E9"/>
<connect gate="A" pin="VCCIO1" pad="J8"/>
<connect gate="A" pin="VCCIO1_2" pad="E3"/>
<connect gate="A" pin="VCCIO1_3" pad="J4"/>
<connect gate="A" pin="VCCIO2" pad="G9"/>
<connect gate="A" pin="VCCIO2_2" pad="C8"/>
<connect gate="A" pin="VCCIO2_3" pad="C4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570M100C5N"/>
<attribute name="OC_FARNELL" value="1635097"/>
<attribute name="OC_NEWARK" value="51R0518"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570M100I5N" prefix="U">
<description>IC MAX II CPLD 570 LE 100-MBGA</description>
<gates>
<gate name="A" symbol="EPM570M100I5N"/>
</gates>
<devices>
<device name="" package="BGA100C50P11X11_600X600X120">
<connects>
<connect gate="A" pin="GNDINT" pad="G4"/>
<connect gate="A" pin="GNDINT_2" pad="E8"/>
<connect gate="A" pin="GNDINT_3" pad="C5"/>
<connect gate="A" pin="GNDINT_4" pad="J5"/>
<connect gate="A" pin="GNDIO" pad="E4"/>
<connect gate="A" pin="GNDIO_2" pad="D5"/>
<connect gate="A" pin="GNDIO_3" pad="D7"/>
<connect gate="A" pin="GNDIO_4" pad="H5"/>
<connect gate="A" pin="GNDIO_5" pad="H7"/>
<connect gate="A" pin="GNDIO_6" pad="G8"/>
<connect gate="A" pin="IO" pad="H3"/>
<connect gate="A" pin="IO/*DEV_CLR" pad="K8"/>
<connect gate="A" pin="IO/DEV_OE" pad="L8"/>
<connect gate="A" pin="IO/GCLK0" pad="F2"/>
<connect gate="A" pin="IO/GCLK1" pad="E1"/>
<connect gate="A" pin="IO/GCLK2" pad="F10"/>
<connect gate="A" pin="IO/GCLK3" pad="G11"/>
<connect gate="A" pin="IO_10" pad="A9"/>
<connect gate="A" pin="IO_11" pad="B1"/>
<connect gate="A" pin="IO_12" pad="B2"/>
<connect gate="A" pin="IO_13" pad="B3"/>
<connect gate="A" pin="IO_14" pad="B4"/>
<connect gate="A" pin="IO_15" pad="B5"/>
<connect gate="A" pin="IO_16" pad="B6"/>
<connect gate="A" pin="IO_17" pad="B7"/>
<connect gate="A" pin="IO_18" pad="B8"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A1"/>
<connect gate="A" pin="IO_20" pad="C1"/>
<connect gate="A" pin="IO_21" pad="C2"/>
<connect gate="A" pin="IO_22" pad="D1"/>
<connect gate="A" pin="IO_23" pad="D9"/>
<connect gate="A" pin="IO_24" pad="D2"/>
<connect gate="A" pin="IO_25" pad="C6"/>
<connect gate="A" pin="IO_26" pad="D3"/>
<connect gate="A" pin="IO_27" pad="E2"/>
<connect gate="A" pin="IO_28" pad="H9"/>
<connect gate="A" pin="IO_29" pad="J6"/>
<connect gate="A" pin="IO_3" pad="A2"/>
<connect gate="A" pin="IO_30" pad="K3"/>
<connect gate="A" pin="IO_31" pad="K4"/>
<connect gate="A" pin="IO_32" pad="K5"/>
<connect gate="A" pin="IO_33" pad="K6"/>
<connect gate="A" pin="IO_34" pad="K7"/>
<connect gate="A" pin="IO_35" pad="K9"/>
<connect gate="A" pin="IO_36" pad="L1"/>
<connect gate="A" pin="IO_37" pad="L2"/>
<connect gate="A" pin="IO_38" pad="L3"/>
<connect gate="A" pin="IO_39" pad="L4"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="L5"/>
<connect gate="A" pin="IO_41" pad="L6"/>
<connect gate="A" pin="IO_42" pad="L7"/>
<connect gate="A" pin="IO_43" pad="L9"/>
<connect gate="A" pin="IO_44" pad="A10"/>
<connect gate="A" pin="IO_45" pad="A11"/>
<connect gate="A" pin="IO_46" pad="B10"/>
<connect gate="A" pin="IO_47" pad="B11"/>
<connect gate="A" pin="IO_48" pad="C10"/>
<connect gate="A" pin="IO_49" pad="C11"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="D10"/>
<connect gate="A" pin="IO_51" pad="D11"/>
<connect gate="A" pin="IO_52" pad="E10"/>
<connect gate="A" pin="IO_53" pad="E11"/>
<connect gate="A" pin="IO_54" pad="F11"/>
<connect gate="A" pin="IO_55" pad="G10"/>
<connect gate="A" pin="IO_56" pad="H10"/>
<connect gate="A" pin="IO_57" pad="H11"/>
<connect gate="A" pin="IO_58" pad="J10"/>
<connect gate="A" pin="IO_59" pad="J11"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_60" pad="K10"/>
<connect gate="A" pin="IO_61" pad="K11"/>
<connect gate="A" pin="IO_62" pad="L10"/>
<connect gate="A" pin="IO_63" pad="L11"/>
<connect gate="A" pin="IO_64" pad="F1"/>
<connect gate="A" pin="IO_65" pad="F3"/>
<connect gate="A" pin="IO_66" pad="F9"/>
<connect gate="A" pin="IO_67" pad="G1"/>
<connect gate="A" pin="IO_68" pad="G2"/>
<connect gate="A" pin="IO_69" pad="H1"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_70" pad="H2"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="A8"/>
<connect gate="A" pin="TCK" pad="K1"/>
<connect gate="A" pin="TDI" pad="J2"/>
<connect gate="A" pin="TDO" pad="K2"/>
<connect gate="A" pin="TMS" pad="J1"/>
<connect gate="A" pin="VCCINT" pad="C7"/>
<connect gate="A" pin="VCCINT_2" pad="E9"/>
<connect gate="A" pin="VCCINT_3" pad="J7"/>
<connect gate="A" pin="VCCINT_4" pad="G3"/>
<connect gate="A" pin="VCCIO1" pad="E3"/>
<connect gate="A" pin="VCCIO1_2" pad="J4"/>
<connect gate="A" pin="VCCIO1_3" pad="J8"/>
<connect gate="A" pin="VCCIO2" pad="G9"/>
<connect gate="A" pin="VCCIO2_2" pad="C4"/>
<connect gate="A" pin="VCCIO2_3" pad="C8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570M100I5N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9474"/>
<attribute name="PACKAGE" value="100-MBGA"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570M256C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570M256C5N_A"/>
<gate name="B" symbol="EPM570M256C5N_B"/>
<gate name="C" symbol="EPM570M256C5N_C"/>
</gates>
<devices>
<device name="" package="BGA256C50P20X20_1100X1100X120">
<connects>
<connect gate="A" pin="GNDINT" pad="J4"/>
<connect gate="A" pin="GNDIO" pad="N3"/>
<connect gate="A" pin="GNDIO_2" pad="C8"/>
<connect gate="A" pin="GNDIO_3" pad="D9"/>
<connect gate="A" pin="GNDIO_4" pad="M4"/>
<connect gate="A" pin="GNDIO_5" pad="H3"/>
<connect gate="A" pin="GNDIO_6" pad="J3"/>
<connect gate="A" pin="IO" pad="U1"/>
<connect gate="A" pin="IO/GCLK0" pad="K1"/>
<connect gate="A" pin="IO/GCLK1" pad="L1"/>
<connect gate="A" pin="IO_10" pad="A9"/>
<connect gate="A" pin="IO_11" pad="B1"/>
<connect gate="A" pin="IO_12" pad="B2"/>
<connect gate="A" pin="IO_13" pad="B3"/>
<connect gate="A" pin="IO_14" pad="B4"/>
<connect gate="A" pin="IO_15" pad="B5"/>
<connect gate="A" pin="IO_16" pad="B6"/>
<connect gate="A" pin="IO_17" pad="B7"/>
<connect gate="A" pin="IO_18" pad="B8"/>
<connect gate="A" pin="IO_19" pad="B9"/>
<connect gate="A" pin="IO_2" pad="A1"/>
<connect gate="A" pin="IO_20" pad="C1"/>
<connect gate="A" pin="IO_21" pad="C2"/>
<connect gate="A" pin="IO_22" pad="C3"/>
<connect gate="A" pin="IO_23" pad="F1"/>
<connect gate="A" pin="IO_24" pad="C5"/>
<connect gate="A" pin="IO_25" pad="F2"/>
<connect gate="A" pin="IO_26" pad="F3"/>
<connect gate="A" pin="IO_27" pad="E1"/>
<connect gate="A" pin="IO_28" pad="E2"/>
<connect gate="A" pin="IO_29" pad="E3"/>
<connect gate="A" pin="IO_3" pad="A2"/>
<connect gate="A" pin="IO_30" pad="D1"/>
<connect gate="A" pin="IO_31" pad="D2"/>
<connect gate="A" pin="IO_32" pad="D3"/>
<connect gate="A" pin="IO_33" pad="G1"/>
<connect gate="A" pin="IO_34" pad="G2"/>
<connect gate="A" pin="IO_35" pad="H1"/>
<connect gate="A" pin="IO_36" pad="H2"/>
<connect gate="A" pin="IO_37" pad="J1"/>
<connect gate="A" pin="IO_38" pad="J2"/>
<connect gate="A" pin="IO_39" pad="M1"/>
<connect gate="A" pin="IO_4" pad="A3"/>
<connect gate="A" pin="IO_40" pad="M2"/>
<connect gate="A" pin="IO_41" pad="N1"/>
<connect gate="A" pin="IO_42" pad="N2"/>
<connect gate="A" pin="IO_43" pad="P1"/>
<connect gate="A" pin="IO_44" pad="P2"/>
<connect gate="A" pin="IO_45" pad="R1"/>
<connect gate="A" pin="IO_46" pad="R2"/>
<connect gate="A" pin="IO_47" pad="R3"/>
<connect gate="A" pin="IO_48" pad="T1"/>
<connect gate="A" pin="IO_49" pad="T2"/>
<connect gate="A" pin="IO_5" pad="A4"/>
<connect gate="A" pin="IO_50" pad="T4"/>
<connect gate="A" pin="IO_6" pad="A5"/>
<connect gate="A" pin="IO_7" pad="A6"/>
<connect gate="A" pin="IO_8" pad="A7"/>
<connect gate="A" pin="IO_9" pad="A8"/>
<connect gate="A" pin="N.C" pad="R4"/>
<connect gate="A" pin="N.C_10" pad="C6"/>
<connect gate="A" pin="N.C_11" pad="K2"/>
<connect gate="A" pin="N.C_12" pad="C7"/>
<connect gate="A" pin="N.C_13" pad="D6"/>
<connect gate="A" pin="N.C_14" pad="P3"/>
<connect gate="A" pin="N.C_15" pad="D7"/>
<connect gate="A" pin="N.C_16" pad="G4"/>
<connect gate="A" pin="N.C_17" pad="D8"/>
<connect gate="A" pin="N.C_18" pad="L2"/>
<connect gate="A" pin="N.C_19" pad="P4"/>
<connect gate="A" pin="N.C_2" pad="F4"/>
<connect gate="A" pin="N.C_3" pad="E4"/>
<connect gate="A" pin="N.C_4" pad="G3"/>
<connect gate="A" pin="N.C_5" pad="N4"/>
<connect gate="A" pin="N.C_6" pad="D4"/>
<connect gate="A" pin="N.C_7" pad="C4"/>
<connect gate="A" pin="N.C_8" pad="H4"/>
<connect gate="A" pin="N.C_9" pad="D5"/>
<connect gate="A" pin="TDI" pad="U2"/>
<connect gate="A" pin="TMS" pad="T3"/>
<connect gate="A" pin="VCCINT" pad="K4"/>
<connect gate="A" pin="VCCIO1" pad="K3"/>
<connect gate="A" pin="VCCIO1_2" pad="L3"/>
<connect gate="A" pin="VCCIO1_3" pad="L4"/>
<connect gate="A" pin="VCCIO1_4" pad="M3"/>
<connect gate="A" pin="VCCIO2" pad="C9"/>
<connect gate="B" pin="GNDINT" pad="D12"/>
<connect gate="B" pin="GNDIO" pad="V9"/>
<connect gate="B" pin="GNDIO_2" pad="V8"/>
<connect gate="B" pin="GNDIO_3" pad="C12"/>
<connect gate="B" pin="GNDIO_4" pad="U9"/>
<connect gate="B" pin="GNDIO_5" pad="C13"/>
<connect gate="B" pin="IO" pad="F20"/>
<connect gate="B" pin="IO_10" pad="W7"/>
<connect gate="B" pin="IO_11" pad="V4"/>
<connect gate="B" pin="IO_12" pad="W8"/>
<connect gate="B" pin="IO_13" pad="U4"/>
<connect gate="B" pin="IO_14" pad="V5"/>
<connect gate="B" pin="IO_15" pad="Y1"/>
<connect gate="B" pin="IO_16" pad="V6"/>
<connect gate="B" pin="IO_17" pad="Y2"/>
<connect gate="B" pin="IO_18" pad="Y3"/>
<connect gate="B" pin="IO_19" pad="Y4"/>
<connect gate="B" pin="IO_2" pad="W1"/>
<connect gate="B" pin="IO_20" pad="Y5"/>
<connect gate="B" pin="IO_21" pad="Y6"/>
<connect gate="B" pin="IO_22" pad="Y7"/>
<connect gate="B" pin="IO_23" pad="Y8"/>
<connect gate="B" pin="IO_24" pad="Y9"/>
<connect gate="B" pin="IO_25" pad="A10"/>
<connect gate="B" pin="IO_26" pad="A11"/>
<connect gate="B" pin="IO_27" pad="A12"/>
<connect gate="B" pin="IO_28" pad="A13"/>
<connect gate="B" pin="IO_29" pad="A14"/>
<connect gate="B" pin="IO_3" pad="W3"/>
<connect gate="B" pin="IO_30" pad="A15"/>
<connect gate="B" pin="IO_31" pad="A16"/>
<connect gate="B" pin="IO_32" pad="A17"/>
<connect gate="B" pin="IO_33" pad="A18"/>
<connect gate="B" pin="IO_34" pad="A19"/>
<connect gate="B" pin="IO_35" pad="A20"/>
<connect gate="B" pin="IO_36" pad="B12"/>
<connect gate="B" pin="IO_37" pad="B13"/>
<connect gate="B" pin="IO_38" pad="B14"/>
<connect gate="B" pin="IO_39" pad="B15"/>
<connect gate="B" pin="IO_4" pad="W4"/>
<connect gate="B" pin="IO_40" pad="B16"/>
<connect gate="B" pin="IO_41" pad="B17"/>
<connect gate="B" pin="IO_42" pad="B18"/>
<connect gate="B" pin="IO_43" pad="B19"/>
<connect gate="B" pin="IO_44" pad="B20"/>
<connect gate="B" pin="IO_45" pad="C15"/>
<connect gate="B" pin="IO_46" pad="C16"/>
<connect gate="B" pin="IO_47" pad="C17"/>
<connect gate="B" pin="IO_48" pad="C18"/>
<connect gate="B" pin="IO_49" pad="C19"/>
<connect gate="B" pin="IO_5" pad="V1"/>
<connect gate="B" pin="IO_50" pad="C20"/>
<connect gate="B" pin="IO_51" pad="D18"/>
<connect gate="B" pin="IO_52" pad="D19"/>
<connect gate="B" pin="IO_53" pad="D20"/>
<connect gate="B" pin="IO_54" pad="E17"/>
<connect gate="B" pin="IO_55" pad="E18"/>
<connect gate="B" pin="IO_56" pad="E19"/>
<connect gate="B" pin="IO_57" pad="E20"/>
<connect gate="B" pin="IO_58" pad="F19"/>
<connect gate="B" pin="IO_6" pad="W5"/>
<connect gate="B" pin="IO_7" pad="V3"/>
<connect gate="B" pin="IO_8" pad="W6"/>
<connect gate="B" pin="IO_9" pad="U3"/>
<connect gate="B" pin="N.C" pad="F18"/>
<connect gate="B" pin="N.C_10" pad="C14"/>
<connect gate="B" pin="N.C_11" pad="D13"/>
<connect gate="B" pin="N.C_12" pad="D14"/>
<connect gate="B" pin="N.C_13" pad="D15"/>
<connect gate="B" pin="N.C_14" pad="D16"/>
<connect gate="B" pin="N.C_15" pad="D17"/>
<connect gate="B" pin="N.C_16" pad="F17"/>
<connect gate="B" pin="N.C_2" pad="U5"/>
<connect gate="B" pin="N.C_3" pad="U6"/>
<connect gate="B" pin="N.C_4" pad="U7"/>
<connect gate="B" pin="N.C_5" pad="V7"/>
<connect gate="B" pin="N.C_6" pad="W9"/>
<connect gate="B" pin="N.C_7" pad="B10"/>
<connect gate="B" pin="N.C_8" pad="U8"/>
<connect gate="B" pin="N.C_9" pad="B11"/>
<connect gate="B" pin="TCK" pad="W2"/>
<connect gate="B" pin="TDO" pad="V2"/>
<connect gate="B" pin="VCCINT" pad="D11"/>
<connect gate="B" pin="VCCIO2" pad="D10"/>
<connect gate="B" pin="VCCIO2_2" pad="C10"/>
<connect gate="B" pin="VCCIO2_3" pad="C11"/>
<connect gate="C" pin="GNDINT" pad="U12"/>
<connect gate="C" pin="GNDINT_2" pad="M17"/>
<connect gate="C" pin="GNDIO" pad="V13"/>
<connect gate="C" pin="GNDIO_2" pad="H18"/>
<connect gate="C" pin="GNDIO_3" pad="J17"/>
<connect gate="C" pin="GNDIO_4" pad="N18"/>
<connect gate="C" pin="GNDIO_5" pad="M18"/>
<connect gate="C" pin="IO" pad="Y20"/>
<connect gate="C" pin="IO/DEV_CLRN" pad="Y13"/>
<connect gate="C" pin="IO/DEV_OE" pad="W12"/>
<connect gate="C" pin="IO/GCLK2" pad="M20"/>
<connect gate="C" pin="IO/GCLK3" pad="L20"/>
<connect gate="C" pin="IO_10" pad="N19"/>
<connect gate="C" pin="IO_11" pad="H20"/>
<connect gate="C" pin="IO_12" pad="R19"/>
<connect gate="C" pin="IO_13" pad="P20"/>
<connect gate="C" pin="IO_14" pad="T18"/>
<connect gate="C" pin="IO_15" pad="R20"/>
<connect gate="C" pin="IO_16" pad="T19"/>
<connect gate="C" pin="IO_17" pad="M19"/>
<connect gate="C" pin="IO_18" pad="T20"/>
<connect gate="C" pin="IO_19" pad="N20"/>
<connect gate="C" pin="IO_2" pad="K20"/>
<connect gate="C" pin="IO_20" pad="U17"/>
<connect gate="C" pin="IO_21" pad="U18"/>
<connect gate="C" pin="IO_22" pad="U19"/>
<connect gate="C" pin="IO_23" pad="U20"/>
<connect gate="C" pin="IO_24" pad="V16"/>
<connect gate="C" pin="IO_25" pad="V17"/>
<connect gate="C" pin="IO_26" pad="V18"/>
<connect gate="C" pin="IO_27" pad="V19"/>
<connect gate="C" pin="IO_28" pad="V20"/>
<connect gate="C" pin="IO_29" pad="W11"/>
<connect gate="C" pin="IO_3" pad="J19"/>
<connect gate="C" pin="IO_30" pad="W13"/>
<connect gate="C" pin="IO_31" pad="W14"/>
<connect gate="C" pin="IO_32" pad="W15"/>
<connect gate="C" pin="IO_33" pad="W16"/>
<connect gate="C" pin="IO_34" pad="W17"/>
<connect gate="C" pin="IO_35" pad="W18"/>
<connect gate="C" pin="IO_36" pad="W19"/>
<connect gate="C" pin="IO_37" pad="W20"/>
<connect gate="C" pin="IO_38" pad="Y10"/>
<connect gate="C" pin="IO_39" pad="Y11"/>
<connect gate="C" pin="IO_4" pad="P19"/>
<connect gate="C" pin="IO_40" pad="Y12"/>
<connect gate="C" pin="IO_41" pad="Y14"/>
<connect gate="C" pin="IO_42" pad="Y15"/>
<connect gate="C" pin="IO_43" pad="Y16"/>
<connect gate="C" pin="IO_44" pad="Y17"/>
<connect gate="C" pin="IO_45" pad="Y18"/>
<connect gate="C" pin="IO_46" pad="Y19"/>
<connect gate="C" pin="IO_5" pad="G19"/>
<connect gate="C" pin="IO_6" pad="J20"/>
<connect gate="C" pin="IO_7" pad="H19"/>
<connect gate="C" pin="IO_8" pad="R18"/>
<connect gate="C" pin="IO_9" pad="G20"/>
<connect gate="C" pin="N.C" pad="W10"/>
<connect gate="C" pin="N.C_10" pad="U15"/>
<connect gate="C" pin="N.C_11" pad="G18"/>
<connect gate="C" pin="N.C_12" pad="U16"/>
<connect gate="C" pin="N.C_13" pad="P18"/>
<connect gate="C" pin="N.C_14" pad="V14"/>
<connect gate="C" pin="N.C_15" pad="T17"/>
<connect gate="C" pin="N.C_16" pad="V15"/>
<connect gate="C" pin="N.C_17" pad="R17"/>
<connect gate="C" pin="N.C_2" pad="N17"/>
<connect gate="C" pin="N.C_3" pad="G17"/>
<connect gate="C" pin="N.C_4" pad="K19"/>
<connect gate="C" pin="N.C_5" pad="L19"/>
<connect gate="C" pin="N.C_6" pad="U13"/>
<connect gate="C" pin="N.C_7" pad="H17"/>
<connect gate="C" pin="N.C_8" pad="U14"/>
<connect gate="C" pin="N.C_9" pad="P17"/>
<connect gate="C" pin="VCCINT" pad="U11"/>
<connect gate="C" pin="VCCINT_2" pad="L17"/>
<connect gate="C" pin="VCCIO1" pad="U10"/>
<connect gate="C" pin="VCCIO1_2" pad="V10"/>
<connect gate="C" pin="VCCIO1_3" pad="V11"/>
<connect gate="C" pin="VCCIO1_4" pad="V12"/>
<connect gate="C" pin="VCCIO2" pad="K18"/>
<connect gate="C" pin="VCCIO2_2" pad="K17"/>
<connect gate="C" pin="VCCIO2_3" pad="J18"/>
<connect gate="C" pin="VCCIO2_4" pad="L18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570M256C5N"/>
<attribute name="OC_FARNELL" value="1635100"/>
<attribute name="OC_NEWARK" value="51R0519"/>
<attribute name="PACKAGE" value="BGA-256"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T100C3N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T100C3N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="65"/>
<connect gate="A" pin="GNDINT_2" pad="11"/>
<connect gate="A" pin="GNDINT_3" pad="37"/>
<connect gate="A" pin="GNDINT_4" pad="90"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="10"/>
<connect gate="A" pin="GNDIO_3" pad="46"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="GNDIO_5" pad="60"/>
<connect gate="A" pin="GNDIO_6" pad="93"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="5"/>
<connect gate="A" pin="IO_11" pad="19"/>
<connect gate="A" pin="IO_12" pad="6"/>
<connect gate="A" pin="IO_13" pad="20"/>
<connect gate="A" pin="IO_14" pad="40"/>
<connect gate="A" pin="IO_15" pad="7"/>
<connect gate="A" pin="IO_16" pad="41"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="42"/>
<connect gate="A" pin="IO_19" pad="8"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="34"/>
<connect gate="A" pin="IO_22" pad="35"/>
<connect gate="A" pin="IO_23" pad="36"/>
<connect gate="A" pin="IO_24" pad="47"/>
<connect gate="A" pin="IO_25" pad="26"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="27"/>
<connect gate="A" pin="IO_28" pad="49"/>
<connect gate="A" pin="IO_29" pad="38"/>
<connect gate="A" pin="IO_3" pad="15"/>
<connect gate="A" pin="IO_30" pad="50"/>
<connect gate="A" pin="IO_31" pad="28"/>
<connect gate="A" pin="IO_32" pad="29"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="52"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="2"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="66"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_49" pad="72"/>
<connect gate="A" pin="IO_5" pad="16"/>
<connect gate="A" pin="IO_50" pad="73"/>
<connect gate="A" pin="IO_51" pad="74"/>
<connect gate="A" pin="IO_52" pad="75"/>
<connect gate="A" pin="IO_53" pad="76"/>
<connect gate="A" pin="IO_54" pad="77"/>
<connect gate="A" pin="IO_55" pad="78"/>
<connect gate="A" pin="IO_56" pad="81"/>
<connect gate="A" pin="IO_57" pad="82"/>
<connect gate="A" pin="IO_58" pad="83"/>
<connect gate="A" pin="IO_59" pad="84"/>
<connect gate="A" pin="IO_6" pad="3"/>
<connect gate="A" pin="IO_60" pad="85"/>
<connect gate="A" pin="IO_61" pad="86"/>
<connect gate="A" pin="IO_62" pad="87"/>
<connect gate="A" pin="IO_63" pad="89"/>
<connect gate="A" pin="IO_64" pad="91"/>
<connect gate="A" pin="IO_65" pad="92"/>
<connect gate="A" pin="IO_66" pad="95"/>
<connect gate="A" pin="IO_67" pad="96"/>
<connect gate="A" pin="IO_68" pad="97"/>
<connect gate="A" pin="IO_69" pad="98"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_70" pad="99"/>
<connect gate="A" pin="IO_8" pad="4"/>
<connect gate="A" pin="IO_9" pad="18"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCINT_3" pad="39"/>
<connect gate="A" pin="VCCINT_4" pad="88"/>
<connect gate="A" pin="VCCIO1" pad="45"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="31"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T100C3N"/>
<attribute name="OC_FARNELL" value="1549470"/>
<attribute name="OC_NEWARK" value="51R9479"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T100C4N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T100C4N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="65"/>
<connect gate="A" pin="GNDINT_2" pad="11"/>
<connect gate="A" pin="GNDINT_3" pad="37"/>
<connect gate="A" pin="GNDINT_4" pad="90"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="10"/>
<connect gate="A" pin="GNDIO_3" pad="46"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="GNDIO_5" pad="60"/>
<connect gate="A" pin="GNDIO_6" pad="93"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="5"/>
<connect gate="A" pin="IO_11" pad="19"/>
<connect gate="A" pin="IO_12" pad="6"/>
<connect gate="A" pin="IO_13" pad="20"/>
<connect gate="A" pin="IO_14" pad="40"/>
<connect gate="A" pin="IO_15" pad="7"/>
<connect gate="A" pin="IO_16" pad="41"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="42"/>
<connect gate="A" pin="IO_19" pad="8"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="34"/>
<connect gate="A" pin="IO_22" pad="35"/>
<connect gate="A" pin="IO_23" pad="36"/>
<connect gate="A" pin="IO_24" pad="47"/>
<connect gate="A" pin="IO_25" pad="26"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="27"/>
<connect gate="A" pin="IO_28" pad="49"/>
<connect gate="A" pin="IO_29" pad="38"/>
<connect gate="A" pin="IO_3" pad="15"/>
<connect gate="A" pin="IO_30" pad="50"/>
<connect gate="A" pin="IO_31" pad="28"/>
<connect gate="A" pin="IO_32" pad="29"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="52"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="2"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="66"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_49" pad="72"/>
<connect gate="A" pin="IO_5" pad="16"/>
<connect gate="A" pin="IO_50" pad="73"/>
<connect gate="A" pin="IO_51" pad="74"/>
<connect gate="A" pin="IO_52" pad="75"/>
<connect gate="A" pin="IO_53" pad="76"/>
<connect gate="A" pin="IO_54" pad="77"/>
<connect gate="A" pin="IO_55" pad="78"/>
<connect gate="A" pin="IO_56" pad="81"/>
<connect gate="A" pin="IO_57" pad="82"/>
<connect gate="A" pin="IO_58" pad="83"/>
<connect gate="A" pin="IO_59" pad="84"/>
<connect gate="A" pin="IO_6" pad="3"/>
<connect gate="A" pin="IO_60" pad="85"/>
<connect gate="A" pin="IO_61" pad="86"/>
<connect gate="A" pin="IO_62" pad="87"/>
<connect gate="A" pin="IO_63" pad="89"/>
<connect gate="A" pin="IO_64" pad="91"/>
<connect gate="A" pin="IO_65" pad="92"/>
<connect gate="A" pin="IO_66" pad="95"/>
<connect gate="A" pin="IO_67" pad="96"/>
<connect gate="A" pin="IO_68" pad="97"/>
<connect gate="A" pin="IO_69" pad="98"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_70" pad="99"/>
<connect gate="A" pin="IO_8" pad="4"/>
<connect gate="A" pin="IO_9" pad="18"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCINT_3" pad="39"/>
<connect gate="A" pin="VCCINT_4" pad="88"/>
<connect gate="A" pin="VCCIO1" pad="45"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="31"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T100C4N"/>
<attribute name="OC_FARNELL" value="1453489"/>
<attribute name="OC_NEWARK" value="51R9481"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T100C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T100C5N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="65"/>
<connect gate="A" pin="GNDINT_2" pad="11"/>
<connect gate="A" pin="GNDINT_3" pad="37"/>
<connect gate="A" pin="GNDINT_4" pad="90"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="10"/>
<connect gate="A" pin="GNDIO_3" pad="46"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="GNDIO_5" pad="60"/>
<connect gate="A" pin="GNDIO_6" pad="93"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="5"/>
<connect gate="A" pin="IO_11" pad="19"/>
<connect gate="A" pin="IO_12" pad="6"/>
<connect gate="A" pin="IO_13" pad="20"/>
<connect gate="A" pin="IO_14" pad="40"/>
<connect gate="A" pin="IO_15" pad="7"/>
<connect gate="A" pin="IO_16" pad="41"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="42"/>
<connect gate="A" pin="IO_19" pad="8"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="34"/>
<connect gate="A" pin="IO_22" pad="35"/>
<connect gate="A" pin="IO_23" pad="36"/>
<connect gate="A" pin="IO_24" pad="47"/>
<connect gate="A" pin="IO_25" pad="26"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="27"/>
<connect gate="A" pin="IO_28" pad="49"/>
<connect gate="A" pin="IO_29" pad="38"/>
<connect gate="A" pin="IO_3" pad="15"/>
<connect gate="A" pin="IO_30" pad="50"/>
<connect gate="A" pin="IO_31" pad="28"/>
<connect gate="A" pin="IO_32" pad="29"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="52"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="2"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="66"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_49" pad="72"/>
<connect gate="A" pin="IO_5" pad="16"/>
<connect gate="A" pin="IO_50" pad="73"/>
<connect gate="A" pin="IO_51" pad="74"/>
<connect gate="A" pin="IO_52" pad="75"/>
<connect gate="A" pin="IO_53" pad="76"/>
<connect gate="A" pin="IO_54" pad="77"/>
<connect gate="A" pin="IO_55" pad="78"/>
<connect gate="A" pin="IO_56" pad="81"/>
<connect gate="A" pin="IO_57" pad="82"/>
<connect gate="A" pin="IO_58" pad="83"/>
<connect gate="A" pin="IO_59" pad="84"/>
<connect gate="A" pin="IO_6" pad="3"/>
<connect gate="A" pin="IO_60" pad="85"/>
<connect gate="A" pin="IO_61" pad="86"/>
<connect gate="A" pin="IO_62" pad="87"/>
<connect gate="A" pin="IO_63" pad="89"/>
<connect gate="A" pin="IO_64" pad="91"/>
<connect gate="A" pin="IO_65" pad="92"/>
<connect gate="A" pin="IO_66" pad="95"/>
<connect gate="A" pin="IO_67" pad="96"/>
<connect gate="A" pin="IO_68" pad="97"/>
<connect gate="A" pin="IO_69" pad="98"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_70" pad="99"/>
<connect gate="A" pin="IO_8" pad="4"/>
<connect gate="A" pin="IO_9" pad="18"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCINT_3" pad="39"/>
<connect gate="A" pin="VCCINT_4" pad="88"/>
<connect gate="A" pin="VCCIO1" pad="45"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="31"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T100C5N"/>
<attribute name="OC_FARNELL" value="1453498"/>
<attribute name="OC_NEWARK" value="51R0520"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T100I5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T100I5N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="65"/>
<connect gate="A" pin="GNDINT_2" pad="11"/>
<connect gate="A" pin="GNDINT_3" pad="37"/>
<connect gate="A" pin="GNDINT_4" pad="90"/>
<connect gate="A" pin="GNDIO" pad="79"/>
<connect gate="A" pin="GNDIO_2" pad="10"/>
<connect gate="A" pin="GNDIO_3" pad="46"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="GNDIO_5" pad="60"/>
<connect gate="A" pin="GNDIO_6" pad="93"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="44"/>
<connect gate="A" pin="IO/DEV_OE" pad="43"/>
<connect gate="A" pin="IO/GCLK0" pad="12"/>
<connect gate="A" pin="IO/GCLK1" pad="14"/>
<connect gate="A" pin="IO/GCLK2" pad="62"/>
<connect gate="A" pin="IO/GCLK3" pad="64"/>
<connect gate="A" pin="IO_10" pad="5"/>
<connect gate="A" pin="IO_11" pad="19"/>
<connect gate="A" pin="IO_12" pad="6"/>
<connect gate="A" pin="IO_13" pad="20"/>
<connect gate="A" pin="IO_14" pad="40"/>
<connect gate="A" pin="IO_15" pad="7"/>
<connect gate="A" pin="IO_16" pad="41"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="42"/>
<connect gate="A" pin="IO_19" pad="8"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="33"/>
<connect gate="A" pin="IO_21" pad="34"/>
<connect gate="A" pin="IO_22" pad="35"/>
<connect gate="A" pin="IO_23" pad="36"/>
<connect gate="A" pin="IO_24" pad="47"/>
<connect gate="A" pin="IO_25" pad="26"/>
<connect gate="A" pin="IO_26" pad="48"/>
<connect gate="A" pin="IO_27" pad="27"/>
<connect gate="A" pin="IO_28" pad="49"/>
<connect gate="A" pin="IO_29" pad="38"/>
<connect gate="A" pin="IO_3" pad="15"/>
<connect gate="A" pin="IO_30" pad="50"/>
<connect gate="A" pin="IO_31" pad="28"/>
<connect gate="A" pin="IO_32" pad="29"/>
<connect gate="A" pin="IO_33" pad="30"/>
<connect gate="A" pin="IO_34" pad="51"/>
<connect gate="A" pin="IO_35" pad="52"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="2"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="61"/>
<connect gate="A" pin="IO_43" pad="66"/>
<connect gate="A" pin="IO_44" pad="67"/>
<connect gate="A" pin="IO_45" pad="68"/>
<connect gate="A" pin="IO_46" pad="69"/>
<connect gate="A" pin="IO_47" pad="70"/>
<connect gate="A" pin="IO_48" pad="71"/>
<connect gate="A" pin="IO_49" pad="72"/>
<connect gate="A" pin="IO_5" pad="16"/>
<connect gate="A" pin="IO_50" pad="73"/>
<connect gate="A" pin="IO_51" pad="74"/>
<connect gate="A" pin="IO_52" pad="75"/>
<connect gate="A" pin="IO_53" pad="76"/>
<connect gate="A" pin="IO_54" pad="77"/>
<connect gate="A" pin="IO_55" pad="78"/>
<connect gate="A" pin="IO_56" pad="81"/>
<connect gate="A" pin="IO_57" pad="82"/>
<connect gate="A" pin="IO_58" pad="83"/>
<connect gate="A" pin="IO_59" pad="84"/>
<connect gate="A" pin="IO_6" pad="3"/>
<connect gate="A" pin="IO_60" pad="85"/>
<connect gate="A" pin="IO_61" pad="86"/>
<connect gate="A" pin="IO_62" pad="87"/>
<connect gate="A" pin="IO_63" pad="89"/>
<connect gate="A" pin="IO_64" pad="91"/>
<connect gate="A" pin="IO_65" pad="92"/>
<connect gate="A" pin="IO_66" pad="95"/>
<connect gate="A" pin="IO_67" pad="96"/>
<connect gate="A" pin="IO_68" pad="97"/>
<connect gate="A" pin="IO_69" pad="98"/>
<connect gate="A" pin="IO_7" pad="17"/>
<connect gate="A" pin="IO_70" pad="99"/>
<connect gate="A" pin="IO_8" pad="4"/>
<connect gate="A" pin="IO_9" pad="18"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="23"/>
<connect gate="A" pin="TDO" pad="25"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="63"/>
<connect gate="A" pin="VCCINT_2" pad="13"/>
<connect gate="A" pin="VCCINT_3" pad="39"/>
<connect gate="A" pin="VCCINT_4" pad="88"/>
<connect gate="A" pin="VCCIO1" pad="45"/>
<connect gate="A" pin="VCCIO1_2" pad="9"/>
<connect gate="A" pin="VCCIO1_3" pad="31"/>
<connect gate="A" pin="VCCIO2" pad="94"/>
<connect gate="A" pin="VCCIO2_2" pad="59"/>
<connect gate="A" pin="VCCIO2_3" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T100I5N"/>
<attribute name="OC_FARNELL" value="1549471"/>
<attribute name="OC_NEWARK" value="51R9484"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T144C3N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T144C3N_A"/>
<gate name="B" symbol="EPM570T144C3N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="64"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO1_3" pad="9"/>
<connect gate="A" pin="VCCIO1_4" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="100"/>
<connect gate="B" pin="VCCIO2_3" pad="82"/>
<connect gate="B" pin="VCCIO2_4" pad="116"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T144C3N"/>
<attribute name="OC_FARNELL" value="1549475"/>
<attribute name="OC_NEWARK" value="51R9487"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T144C5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T144C5N_A"/>
<gate name="B" symbol="EPM570T144C5N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="64"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO1_3" pad="9"/>
<connect gate="A" pin="VCCIO1_4" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="100"/>
<connect gate="B" pin="VCCIO2_3" pad="82"/>
<connect gate="B" pin="VCCIO2_4" pad="116"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T144C5N"/>
<attribute name="OC_FARNELL" value="1635099"/>
<attribute name="OC_NEWARK" value="51R0521"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM570T144I5N">
<description>CPLD, MAX II</description>
<gates>
<gate name="A" symbol="EPM570T144I5N_A"/>
<gate name="B" symbol="EPM570T144I5N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="17"/>
<connect gate="A" pin="GNDINT_2" pad="54"/>
<connect gate="A" pin="GNDIO" pad="10"/>
<connect gate="A" pin="GNDIO_2" pad="47"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="65"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/DEV_CLRN" pad="61"/>
<connect gate="A" pin="IO/DEV_OE" pad="60"/>
<connect gate="A" pin="IO/GCLK0" pad="18"/>
<connect gate="A" pin="IO/GCLK1" pad="20"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="13"/>
<connect gate="A" pin="IO_13" pad="14"/>
<connect gate="A" pin="IO_14" pad="15"/>
<connect gate="A" pin="IO_15" pad="16"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="22"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="23"/>
<connect gate="A" pin="IO_22" pad="29"/>
<connect gate="A" pin="IO_23" pad="30"/>
<connect gate="A" pin="IO_24" pad="31"/>
<connect gate="A" pin="IO_25" pad="32"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="38"/>
<connect gate="A" pin="IO_28" pad="39"/>
<connect gate="A" pin="IO_29" pad="40"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="41"/>
<connect gate="A" pin="IO_31" pad="42"/>
<connect gate="A" pin="IO_32" pad="43"/>
<connect gate="A" pin="IO_33" pad="44"/>
<connect gate="A" pin="IO_34" pad="45"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="53"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="62"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="58"/>
<connect gate="A" pin="IO_46" pad="66"/>
<connect gate="A" pin="IO_47" pad="59"/>
<connect gate="A" pin="IO_48" pad="67"/>
<connect gate="A" pin="IO_49" pad="68"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="69"/>
<connect gate="A" pin="IO_51" pad="70"/>
<connect gate="A" pin="IO_52" pad="71"/>
<connect gate="A" pin="IO_6" pad="5"/>
<connect gate="A" pin="IO_7" pad="6"/>
<connect gate="A" pin="IO_8" pad="7"/>
<connect gate="A" pin="IO_9" pad="8"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="34"/>
<connect gate="A" pin="TDO" pad="36"/>
<connect gate="A" pin="TMS" pad="33"/>
<connect gate="A" pin="VCCINT" pad="56"/>
<connect gate="A" pin="VCCINT_2" pad="19"/>
<connect gate="A" pin="VCCIO1" pad="64"/>
<connect gate="A" pin="VCCIO1_2" pad="25"/>
<connect gate="A" pin="VCCIO1_3" pad="9"/>
<connect gate="A" pin="VCCIO1_4" pad="46"/>
<connect gate="B" pin="GNDINT" pad="128"/>
<connect gate="B" pin="GNDINT_2" pad="92"/>
<connect gate="B" pin="GNDIO" pad="135"/>
<connect gate="B" pin="GNDIO_2" pad="83"/>
<connect gate="B" pin="GNDIO_3" pad="99"/>
<connect gate="B" pin="GNDIO_4" pad="115"/>
<connect gate="B" pin="IO" pad="144"/>
<connect gate="B" pin="IO/GCLK2" pad="89"/>
<connect gate="B" pin="IO/GCLK3" pad="91"/>
<connect gate="B" pin="IO_10" pad="86"/>
<connect gate="B" pin="IO_11" pad="79"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="80"/>
<connect gate="B" pin="IO_14" pad="88"/>
<connect gate="B" pin="IO_15" pad="81"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="95"/>
<connect gate="B" pin="IO_19" pad="96"/>
<connect gate="B" pin="IO_2" pad="73"/>
<connect gate="B" pin="IO_20" pad="97"/>
<connect gate="B" pin="IO_21" pad="101"/>
<connect gate="B" pin="IO_22" pad="98"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="104"/>
<connect gate="B" pin="IO_26" pad="105"/>
<connect gate="B" pin="IO_27" pad="106"/>
<connect gate="B" pin="IO_28" pad="107"/>
<connect gate="B" pin="IO_29" pad="108"/>
<connect gate="B" pin="IO_3" pad="74"/>
<connect gate="B" pin="IO_30" pad="109"/>
<connect gate="B" pin="IO_31" pad="110"/>
<connect gate="B" pin="IO_32" pad="111"/>
<connect gate="B" pin="IO_33" pad="112"/>
<connect gate="B" pin="IO_34" pad="113"/>
<connect gate="B" pin="IO_35" pad="114"/>
<connect gate="B" pin="IO_36" pad="117"/>
<connect gate="B" pin="IO_37" pad="118"/>
<connect gate="B" pin="IO_38" pad="119"/>
<connect gate="B" pin="IO_39" pad="120"/>
<connect gate="B" pin="IO_4" pad="75"/>
<connect gate="B" pin="IO_40" pad="121"/>
<connect gate="B" pin="IO_41" pad="122"/>
<connect gate="B" pin="IO_42" pad="123"/>
<connect gate="B" pin="IO_43" pad="124"/>
<connect gate="B" pin="IO_44" pad="125"/>
<connect gate="B" pin="IO_45" pad="127"/>
<connect gate="B" pin="IO_46" pad="129"/>
<connect gate="B" pin="IO_47" pad="130"/>
<connect gate="B" pin="IO_48" pad="131"/>
<connect gate="B" pin="IO_49" pad="132"/>
<connect gate="B" pin="IO_5" pad="76"/>
<connect gate="B" pin="IO_50" pad="133"/>
<connect gate="B" pin="IO_51" pad="134"/>
<connect gate="B" pin="IO_52" pad="137"/>
<connect gate="B" pin="IO_53" pad="138"/>
<connect gate="B" pin="IO_54" pad="139"/>
<connect gate="B" pin="IO_55" pad="140"/>
<connect gate="B" pin="IO_56" pad="141"/>
<connect gate="B" pin="IO_57" pad="142"/>
<connect gate="B" pin="IO_58" pad="143"/>
<connect gate="B" pin="IO_6" pad="84"/>
<connect gate="B" pin="IO_7" pad="77"/>
<connect gate="B" pin="IO_8" pad="85"/>
<connect gate="B" pin="IO_9" pad="78"/>
<connect gate="B" pin="VCCINT" pad="126"/>
<connect gate="B" pin="VCCINT_2" pad="90"/>
<connect gate="B" pin="VCCIO2" pad="136"/>
<connect gate="B" pin="VCCIO2_2" pad="100"/>
<connect gate="B" pin="VCCIO2_3" pad="82"/>
<connect gate="B" pin="VCCIO2_4" pad="116"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM570T144I5N"/>
<attribute name="OC_FARNELL" value="1549476"/>
<attribute name="OC_NEWARK" value="51R9492"/>
<attribute name="PACKAGE" value="QFP-144"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7032AETC44-10N">
<description>CPLD EEPROM</description>
<gates>
<gate name="A" symbol="EPM7032AETC44-10N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1N" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="30"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="25"/>
<connect gate="A" pin="IO_21" pad="27"/>
<connect gate="A" pin="IO_22" pad="28"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7032AETC44-10N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9507"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7032AETC44-4N">
<description>CPLD EEPROM</description>
<gates>
<gate name="A" symbol="EPM7032AETC44-4N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1N" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="30"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="25"/>
<connect gate="A" pin="IO_21" pad="27"/>
<connect gate="A" pin="IO_22" pad="28"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7032AETC44-4N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9509"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7032AETI44-7N">
<description>CPLD EEPROM</description>
<gates>
<gate name="A" symbol="EPM7032AETI44-7N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="36"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1N" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="30"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="25"/>
<connect gate="A" pin="IO_21" pad="27"/>
<connect gate="A" pin="IO_22" pad="28"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCC" pad="29"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VCC_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7032AETI44-7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9513"/>
<attribute name="PACKAGE" value="44-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064AETI44-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064AETI44-7N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GNDINT" pad="36"/>
<connect gate="A" pin="GNDINT_2" pad="16"/>
<connect gate="A" pin="GNDIO" pad="24"/>
<connect gate="A" pin="GNDIO_2" pad="4"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/GCLRN" pad="39"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="19"/>
<connect gate="A" pin="IO_15" pad="20"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="22"/>
<connect gate="A" pin="IO_18" pad="23"/>
<connect gate="A" pin="IO_19" pad="25"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="27"/>
<connect gate="A" pin="IO_21" pad="28"/>
<connect gate="A" pin="IO_22" pad="30"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCCINT" pad="41"/>
<connect gate="A" pin="VCCINT_2" pad="17"/>
<connect gate="A" pin="VCCIO" pad="9"/>
<connect gate="A" pin="VCCIO_2" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064AETI44-7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9581"/>
<attribute name="PACKAGE" value="QFP-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064LC44-15">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064LC44-15"/>
</gates>
<devices>
<device name="" package="PLCC127P1752X1752X457-44N">
<connects>
<connect gate="A" pin="GND" pad="42"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="INPUT/~GCLR" pad="1"/>
<connect gate="A" pin="IO" pad="41"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDI" pad="7"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="17"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="31"/>
<connect gate="A" pin="IO_23" pad="33"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="36"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="11"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="15"/>
<connect gate="A" pin="VCC_4" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064LC44-15"/>
<attribute name="OC_FARNELL" value="1781948"/>
<attribute name="OC_NEWARK" value="51R9599"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064LI44-15">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064LI44-15"/>
</gates>
<devices>
<device name="" package="PLCC127P1752X1752X457-44N">
<connects>
<connect gate="A" pin="GND" pad="42"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="INPUT/~GCLR" pad="1"/>
<connect gate="A" pin="IO" pad="41"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDI" pad="7"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="17"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="31"/>
<connect gate="A" pin="IO_23" pad="33"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="36"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="11"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="15"/>
<connect gate="A" pin="VCC_4" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064LI44-15"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9609"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064SLC44-10">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064SLC44-10"/>
</gates>
<devices>
<device name="" package="PLCC127P1752X1752X457-44N">
<connects>
<connect gate="A" pin="GND" pad="42"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="INPUT/~GCLR" pad="1"/>
<connect gate="A" pin="IO" pad="41"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDI" pad="7"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="17"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="31"/>
<connect gate="A" pin="IO_23" pad="33"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="36"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="11"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="15"/>
<connect gate="A" pin="VCC_4" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064SLC44-10"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R8599"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064SLC44-10N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064SLC44-10N"/>
</gates>
<devices>
<device name="" package="PLCC127P1752X1752X457-44N">
<connects>
<connect gate="A" pin="GND" pad="42"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="INPUT/~GCLR" pad="1"/>
<connect gate="A" pin="IO" pad="41"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDI" pad="7"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="17"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="31"/>
<connect gate="A" pin="IO_23" pad="33"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="36"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="11"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="15"/>
<connect gate="A" pin="VCC_4" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064SLC44-10N"/>
<attribute name="OC_FARNELL" value="1637255"/>
<attribute name="OC_NEWARK" value="51R0526"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064SLI44-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064SLI44-7N"/>
</gates>
<devices>
<device name="" package="PLCC127P1752X1752X457-44N">
<connects>
<connect gate="A" pin="GND" pad="42"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="30"/>
<connect gate="A" pin="INPUT/GCLK1" pad="43"/>
<connect gate="A" pin="INPUT/OE1" pad="44"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="INPUT/~GCLR" pad="1"/>
<connect gate="A" pin="IO" pad="41"/>
<connect gate="A" pin="IO/TCK" pad="32"/>
<connect gate="A" pin="IO/TDI" pad="7"/>
<connect gate="A" pin="IO/TDO" pad="38"/>
<connect gate="A" pin="IO/TMS" pad="13"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="17"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="19"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="24"/>
<connect gate="A" pin="IO_17" pad="25"/>
<connect gate="A" pin="IO_18" pad="26"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="31"/>
<connect gate="A" pin="IO_23" pad="33"/>
<connect gate="A" pin="IO_24" pad="34"/>
<connect gate="A" pin="IO_25" pad="36"/>
<connect gate="A" pin="IO_26" pad="37"/>
<connect gate="A" pin="IO_27" pad="39"/>
<connect gate="A" pin="IO_28" pad="40"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="11"/>
<connect gate="A" pin="IO_8" pad="12"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="15"/>
<connect gate="A" pin="VCC_4" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064SLI44-7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9630"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064STC44-10N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064STC44-10N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="24"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="36"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="INPUT/~GCLR" pad="39"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="19"/>
<connect gate="A" pin="IO_15" pad="20"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="22"/>
<connect gate="A" pin="IO_18" pad="23"/>
<connect gate="A" pin="IO_19" pad="25"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="27"/>
<connect gate="A" pin="IO_21" pad="28"/>
<connect gate="A" pin="IO_22" pad="30"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCCINT" pad="9"/>
<connect gate="A" pin="VCCINT_2" pad="17"/>
<connect gate="A" pin="VCCINT_3" pad="29"/>
<connect gate="A" pin="VCCINT_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064STC44-10N"/>
<attribute name="OC_FARNELL" value="9925902"/>
<attribute name="OC_NEWARK" value="51R0527"/>
<attribute name="PACKAGE" value="QFP-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064STC44-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064STC44-7N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="24"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="36"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="INPUT/~GCLR" pad="39"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="19"/>
<connect gate="A" pin="IO_15" pad="20"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="22"/>
<connect gate="A" pin="IO_18" pad="23"/>
<connect gate="A" pin="IO_19" pad="25"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="27"/>
<connect gate="A" pin="IO_21" pad="28"/>
<connect gate="A" pin="IO_22" pad="30"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCCINT" pad="9"/>
<connect gate="A" pin="VCCINT_2" pad="17"/>
<connect gate="A" pin="VCCINT_3" pad="29"/>
<connect gate="A" pin="VCCINT_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064STC44-7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9648"/>
<attribute name="PACKAGE" value="QFP-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064STI44-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7064STI44-7N"/>
</gates>
<devices>
<device name="" package="QFP80P1200X1200X120-44N">
<connects>
<connect gate="A" pin="GND" pad="24"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="36"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="INPUT/GCLK1" pad="37"/>
<connect gate="A" pin="INPUT/OE1" pad="38"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="INPUT/~GCLR" pad="39"/>
<connect gate="A" pin="IO" pad="44"/>
<connect gate="A" pin="IO/TCK" pad="26"/>
<connect gate="A" pin="IO/TDI" pad="1"/>
<connect gate="A" pin="IO/TDO" pad="32"/>
<connect gate="A" pin="IO/TMS" pad="7"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="19"/>
<connect gate="A" pin="IO_15" pad="20"/>
<connect gate="A" pin="IO_16" pad="21"/>
<connect gate="A" pin="IO_17" pad="22"/>
<connect gate="A" pin="IO_18" pad="23"/>
<connect gate="A" pin="IO_19" pad="25"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="27"/>
<connect gate="A" pin="IO_21" pad="28"/>
<connect gate="A" pin="IO_22" pad="30"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="43"/>
<connect gate="A" pin="IO_3" pad="3"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_6" pad="8"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCCINT" pad="9"/>
<connect gate="A" pin="VCCINT_2" pad="17"/>
<connect gate="A" pin="VCCINT_3" pad="29"/>
<connect gate="A" pin="VCCINT_4" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7064STI44-7N"/>
<attribute name="OC_FARNELL" value="1549456"/>
<attribute name="OC_NEWARK" value="51R9652"/>
<attribute name="PACKAGE" value="QFP-44"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128AETC100-10N">
<description>Programmable Logic device</description>
<gates>
<gate name="A" symbol="EPM7128AETC100-10N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="43"/>
<connect gate="A" pin="GNDIO_5" pad="74"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="12"/>
<connect gate="A" pin="IO_11" pad="13"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="35"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="36"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="40"/>
<connect gate="A" pin="IO_33" pad="41"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="52"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="60"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="61"/>
<connect gate="A" pin="IO_51" pad="63"/>
<connect gate="A" pin="IO_52" pad="64"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="67"/>
<connect gate="A" pin="IO_55" pad="68"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="75"/>
<connect gate="A" pin="IO_61" pad="76"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="83"/>
<connect gate="A" pin="IO_68" pad="84"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="92"/>
<connect gate="A" pin="IO_71" pad="93"/>
<connect gate="A" pin="IO_72" pad="94"/>
<connect gate="A" pin="IO_73" pad="96"/>
<connect gate="A" pin="IO_74" pad="97"/>
<connect gate="A" pin="IO_75" pad="98"/>
<connect gate="A" pin="IO_76" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="91"/>
<connect gate="A" pin="VCCINT_2" pad="39"/>
<connect gate="A" pin="VCCIO" pad="3"/>
<connect gate="A" pin="VCCIO_2" pad="34"/>
<connect gate="A" pin="VCCIO_3" pad="18"/>
<connect gate="A" pin="VCCIO_4" pad="51"/>
<connect gate="A" pin="VCCIO_5" pad="82"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128AETC100-10N"/>
<attribute name="OC_FARNELL" value="1453460"/>
<attribute name="OC_NEWARK" value="51R9687"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128AETC100-5N">
<description>Programmable Logic device</description>
<gates>
<gate name="A" symbol="EPM7128AETC100-5N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="43"/>
<connect gate="A" pin="GNDIO_5" pad="74"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="12"/>
<connect gate="A" pin="IO_11" pad="13"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="35"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="36"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="40"/>
<connect gate="A" pin="IO_33" pad="41"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="52"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="60"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="61"/>
<connect gate="A" pin="IO_51" pad="63"/>
<connect gate="A" pin="IO_52" pad="64"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="67"/>
<connect gate="A" pin="IO_55" pad="68"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="75"/>
<connect gate="A" pin="IO_61" pad="76"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="83"/>
<connect gate="A" pin="IO_68" pad="84"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="92"/>
<connect gate="A" pin="IO_71" pad="93"/>
<connect gate="A" pin="IO_72" pad="94"/>
<connect gate="A" pin="IO_73" pad="96"/>
<connect gate="A" pin="IO_74" pad="97"/>
<connect gate="A" pin="IO_75" pad="98"/>
<connect gate="A" pin="IO_76" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="91"/>
<connect gate="A" pin="VCCINT_2" pad="39"/>
<connect gate="A" pin="VCCIO" pad="3"/>
<connect gate="A" pin="VCCIO_2" pad="34"/>
<connect gate="A" pin="VCCIO_3" pad="18"/>
<connect gate="A" pin="VCCIO_4" pad="51"/>
<connect gate="A" pin="VCCIO_5" pad="82"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128AETC100-5N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9689"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128AETC144-10N" prefix="U">
<description>IC MAX 7000 CPLD 128 144-TQFP</description>
<gates>
<gate name="A" symbol="EPM7128AETC144-10N_A"/>
<gate name="B" symbol="EPM7128AETC144-10N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="33"/>
<connect gate="A" pin="GNDIO_2" pad="3"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="59"/>
<connect gate="A" pin="GNDIO_5" pad="13"/>
<connect gate="A" pin="GNDIO_6" pad="17"/>
<connect gate="A" pin="IO" pad="72"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="18"/>
<connect gate="A" pin="IO_13" pad="21"/>
<connect gate="A" pin="IO_14" pad="22"/>
<connect gate="A" pin="IO_15" pad="23"/>
<connect gate="A" pin="IO_16" pad="25"/>
<connect gate="A" pin="IO_17" pad="26"/>
<connect gate="A" pin="IO_18" pad="27"/>
<connect gate="A" pin="IO_19" pad="28"/>
<connect gate="A" pin="IO_2" pad="5"/>
<connect gate="A" pin="IO_20" pad="29"/>
<connect gate="A" pin="IO_21" pad="30"/>
<connect gate="A" pin="IO_22" pad="31"/>
<connect gate="A" pin="IO_23" pad="32"/>
<connect gate="A" pin="IO_24" pad="37"/>
<connect gate="A" pin="IO_25" pad="38"/>
<connect gate="A" pin="IO_26" pad="39"/>
<connect gate="A" pin="IO_27" pad="40"/>
<connect gate="A" pin="IO_28" pad="41"/>
<connect gate="A" pin="IO_29" pad="42"/>
<connect gate="A" pin="IO_3" pad="6"/>
<connect gate="A" pin="IO_30" pad="44"/>
<connect gate="A" pin="IO_31" pad="45"/>
<connect gate="A" pin="IO_32" pad="53"/>
<connect gate="A" pin="IO_33" pad="54"/>
<connect gate="A" pin="IO_34" pad="55"/>
<connect gate="A" pin="IO_35" pad="56"/>
<connect gate="A" pin="IO_36" pad="60"/>
<connect gate="A" pin="IO_37" pad="61"/>
<connect gate="A" pin="IO_38" pad="62"/>
<connect gate="A" pin="IO_39" pad="63"/>
<connect gate="A" pin="IO_4" pad="7"/>
<connect gate="A" pin="IO_40" pad="65"/>
<connect gate="A" pin="IO_41" pad="67"/>
<connect gate="A" pin="IO_42" pad="68"/>
<connect gate="A" pin="IO_43" pad="69"/>
<connect gate="A" pin="IO_44" pad="70"/>
<connect gate="A" pin="IO_45" pad="71"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="14"/>
<connect gate="A" pin="N.C." pad="2"/>
<connect gate="A" pin="N.C._10" pad="66"/>
<connect gate="A" pin="N.C._11" pad="12"/>
<connect gate="A" pin="N.C._12" pad="19"/>
<connect gate="A" pin="N.C._13" pad="1"/>
<connect gate="A" pin="N.C._2" pad="34"/>
<connect gate="A" pin="N.C._3" pad="43"/>
<connect gate="A" pin="N.C._4" pad="35"/>
<connect gate="A" pin="N.C._5" pad="36"/>
<connect gate="A" pin="N.C._6" pad="46"/>
<connect gate="A" pin="N.C._7" pad="47"/>
<connect gate="A" pin="N.C._8" pad="48"/>
<connect gate="A" pin="N.C._9" pad="49"/>
<connect gate="A" pin="VCCINT" pad="58"/>
<connect gate="A" pin="VCCINT_2" pad="51"/>
<connect gate="A" pin="VCCIO" pad="50"/>
<connect gate="A" pin="VCCIO_2" pad="24"/>
<connect gate="B" pin="GNDINT" pad="124"/>
<connect gate="B" pin="GNDINT_2" pad="129"/>
<connect gate="B" pin="GNDIO" pad="105"/>
<connect gate="B" pin="GNDIO_2" pad="85"/>
<connect gate="B" pin="GNDIO_3" pad="135"/>
<connect gate="B" pin="INPUT/*GCLR" pad="127"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="143"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="84"/>
<connect gate="B" pin="IO_11" pad="86"/>
<connect gate="B" pin="IO_12" pad="87"/>
<connect gate="B" pin="IO_13" pad="88"/>
<connect gate="B" pin="IO_14" pad="91"/>
<connect gate="B" pin="IO_15" pad="92"/>
<connect gate="B" pin="IO_16" pad="93"/>
<connect gate="B" pin="IO_17" pad="94"/>
<connect gate="B" pin="IO_18" pad="96"/>
<connect gate="B" pin="IO_19" pad="97"/>
<connect gate="B" pin="IO_2" pad="74"/>
<connect gate="B" pin="IO_20" pad="98"/>
<connect gate="B" pin="IO_21" pad="99"/>
<connect gate="B" pin="IO_22" pad="100"/>
<connect gate="B" pin="IO_23" pad="101"/>
<connect gate="B" pin="IO_24" pad="102"/>
<connect gate="B" pin="IO_25" pad="106"/>
<connect gate="B" pin="IO_26" pad="107"/>
<connect gate="B" pin="IO_27" pad="109"/>
<connect gate="B" pin="IO_28" pad="110"/>
<connect gate="B" pin="IO_29" pad="111"/>
<connect gate="B" pin="IO_3" pad="77"/>
<connect gate="B" pin="IO_30" pad="112"/>
<connect gate="B" pin="IO_31" pad="113"/>
<connect gate="B" pin="IO_32" pad="114"/>
<connect gate="B" pin="IO_33" pad="116"/>
<connect gate="B" pin="IO_34" pad="117"/>
<connect gate="B" pin="IO_35" pad="118"/>
<connect gate="B" pin="IO_36" pad="119"/>
<connect gate="B" pin="IO_37" pad="131"/>
<connect gate="B" pin="IO_38" pad="132"/>
<connect gate="B" pin="IO_39" pad="133"/>
<connect gate="B" pin="IO_4" pad="78"/>
<connect gate="B" pin="IO_40" pad="134"/>
<connect gate="B" pin="IO_41" pad="136"/>
<connect gate="B" pin="IO_42" pad="137"/>
<connect gate="B" pin="IO_43" pad="138"/>
<connect gate="B" pin="IO_44" pad="139"/>
<connect gate="B" pin="IO_45" pad="140"/>
<connect gate="B" pin="IO_46" pad="141"/>
<connect gate="B" pin="IO_47" pad="142"/>
<connect gate="B" pin="IO_5" pad="79"/>
<connect gate="B" pin="IO_6" pad="80"/>
<connect gate="B" pin="IO_7" pad="81"/>
<connect gate="B" pin="IO_8" pad="82"/>
<connect gate="B" pin="IO_9" pad="83"/>
<connect gate="B" pin="N.C." pad="90"/>
<connect gate="B" pin="N.C._2" pad="120"/>
<connect gate="B" pin="N.C._3" pad="121"/>
<connect gate="B" pin="N.C._4" pad="122"/>
<connect gate="B" pin="N.C._5" pad="108"/>
<connect gate="B" pin="N.C._6" pad="75"/>
<connect gate="B" pin="N.C._7" pad="103"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="123"/>
<connect gate="B" pin="VCCIO" pad="115"/>
<connect gate="B" pin="VCCIO_2" pad="144"/>
<connect gate="B" pin="VCCIO_3" pad="76"/>
<connect gate="B" pin="VCCIO_4" pad="73"/>
<connect gate="B" pin="VCCIO_5" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128AETC144-10N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9693"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128AETI100-7N">
<description>Programmable Logic device</description>
<gates>
<gate name="A" symbol="EPM7128AETI100-7N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="43"/>
<connect gate="A" pin="GNDIO_5" pad="74"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="12"/>
<connect gate="A" pin="IO_11" pad="13"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="35"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="36"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="40"/>
<connect gate="A" pin="IO_33" pad="41"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="52"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="60"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="61"/>
<connect gate="A" pin="IO_51" pad="63"/>
<connect gate="A" pin="IO_52" pad="64"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="67"/>
<connect gate="A" pin="IO_55" pad="68"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="75"/>
<connect gate="A" pin="IO_61" pad="76"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="83"/>
<connect gate="A" pin="IO_68" pad="84"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="92"/>
<connect gate="A" pin="IO_71" pad="93"/>
<connect gate="A" pin="IO_72" pad="94"/>
<connect gate="A" pin="IO_73" pad="96"/>
<connect gate="A" pin="IO_74" pad="97"/>
<connect gate="A" pin="IO_75" pad="98"/>
<connect gate="A" pin="IO_76" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="91"/>
<connect gate="A" pin="VCCINT_2" pad="39"/>
<connect gate="A" pin="VCCIO" pad="3"/>
<connect gate="A" pin="VCCIO_2" pad="34"/>
<connect gate="A" pin="VCCIO_3" pad="18"/>
<connect gate="A" pin="VCCIO_4" pad="51"/>
<connect gate="A" pin="VCCIO_5" pad="82"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128AETI100-7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9699"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128SLC84-15N">
<description>IC PLD EEPROM</description>
<gates>
<gate name="A" symbol="EPM7128SLC84-15N"/>
</gates>
<devices>
<device name="" package="PLCC127P3022X3022X457-84N">
<connects>
<connect gate="A" pin="GNDINT" pad="82"/>
<connect gate="A" pin="GNDINT_2" pad="42"/>
<connect gate="A" pin="GNDIO" pad="72"/>
<connect gate="A" pin="GNDIO_2" pad="7"/>
<connect gate="A" pin="GNDIO_3" pad="19"/>
<connect gate="A" pin="GNDIO_4" pad="32"/>
<connect gate="A" pin="GNDIO_5" pad="47"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="INPUT/GCLK1" pad="83"/>
<connect gate="A" pin="INPUT/GCLRN" pad="1"/>
<connect gate="A" pin="INPUT/OE1" pad="84"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="IO" pad="81"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="14"/>
<connect gate="A" pin="IO/TDO" pad="71"/>
<connect gate="A" pin="IO/TMS" pad="23"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="17"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="30"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="36"/>
<connect gate="A" pin="IO_28" pad="37"/>
<connect gate="A" pin="IO_29" pad="39"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_30" pad="40"/>
<connect gate="A" pin="IO_31" pad="41"/>
<connect gate="A" pin="IO_32" pad="44"/>
<connect gate="A" pin="IO_33" pad="45"/>
<connect gate="A" pin="IO_34" pad="46"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="54"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="56"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="58"/>
<connect gate="A" pin="IO_45" pad="60"/>
<connect gate="A" pin="IO_46" pad="61"/>
<connect gate="A" pin="IO_47" pad="63"/>
<connect gate="A" pin="IO_48" pad="64"/>
<connect gate="A" pin="IO_49" pad="65"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="67"/>
<connect gate="A" pin="IO_51" pad="68"/>
<connect gate="A" pin="IO_52" pad="69"/>
<connect gate="A" pin="IO_53" pad="70"/>
<connect gate="A" pin="IO_54" pad="73"/>
<connect gate="A" pin="IO_55" pad="74"/>
<connect gate="A" pin="IO_56" pad="75"/>
<connect gate="A" pin="IO_57" pad="76"/>
<connect gate="A" pin="IO_58" pad="77"/>
<connect gate="A" pin="IO_59" pad="79"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_60" pad="80"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCCINT" pad="43"/>
<connect gate="A" pin="VCCINT_2" pad="3"/>
<connect gate="A" pin="VCCIO" pad="78"/>
<connect gate="A" pin="VCCIO_2" pad="13"/>
<connect gate="A" pin="VCCIO_3" pad="26"/>
<connect gate="A" pin="VCCIO_4" pad="38"/>
<connect gate="A" pin="VCCIO_5" pad="53"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128SLC84-15N"/>
<attribute name="OC_FARNELL" value="1772141"/>
<attribute name="OC_NEWARK" value="51R0528"/>
<attribute name="PACKAGE" value="PLCC-84"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128SLI84-10N">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM7128SLC84-10"/>
</gates>
<devices>
<device name="" package="PLCC127P3035X3035X475-84N">
<connects>
<connect gate="A" pin="GND" pad="82"/>
<connect gate="A" pin="GNDINT" pad="42"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="32"/>
<connect gate="A" pin="GND_4" pad="19"/>
<connect gate="A" pin="GND_5" pad="47"/>
<connect gate="A" pin="GND_6" pad="59"/>
<connect gate="A" pin="GND_7" pad="72"/>
<connect gate="A" pin="INPUT/GCLK1" pad="83"/>
<connect gate="A" pin="INPUT/GLCRN" pad="1"/>
<connect gate="A" pin="INPUT/OE1" pad="84"/>
<connect gate="A" pin="INPUT/OE2/(GCLK2)" pad="2"/>
<connect gate="A" pin="IO" pad="81"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="14"/>
<connect gate="A" pin="IO/TDO" pad="71"/>
<connect gate="A" pin="IO/TMS" pad="23"/>
<connect gate="A" pin="IO_10" pad="15"/>
<connect gate="A" pin="IO_11" pad="16"/>
<connect gate="A" pin="IO_12" pad="17"/>
<connect gate="A" pin="IO_13" pad="18"/>
<connect gate="A" pin="IO_14" pad="20"/>
<connect gate="A" pin="IO_15" pad="21"/>
<connect gate="A" pin="IO_16" pad="22"/>
<connect gate="A" pin="IO_17" pad="24"/>
<connect gate="A" pin="IO_18" pad="25"/>
<connect gate="A" pin="IO_19" pad="27"/>
<connect gate="A" pin="IO_2" pad="4"/>
<connect gate="A" pin="IO_20" pad="28"/>
<connect gate="A" pin="IO_21" pad="29"/>
<connect gate="A" pin="IO_22" pad="30"/>
<connect gate="A" pin="IO_23" pad="31"/>
<connect gate="A" pin="IO_24" pad="33"/>
<connect gate="A" pin="IO_25" pad="34"/>
<connect gate="A" pin="IO_26" pad="35"/>
<connect gate="A" pin="IO_27" pad="36"/>
<connect gate="A" pin="IO_28" pad="37"/>
<connect gate="A" pin="IO_29" pad="39"/>
<connect gate="A" pin="IO_3" pad="5"/>
<connect gate="A" pin="IO_30" pad="40"/>
<connect gate="A" pin="IO_31" pad="41"/>
<connect gate="A" pin="IO_32" pad="44"/>
<connect gate="A" pin="IO_33" pad="45"/>
<connect gate="A" pin="IO_34" pad="46"/>
<connect gate="A" pin="IO_35" pad="48"/>
<connect gate="A" pin="IO_36" pad="49"/>
<connect gate="A" pin="IO_37" pad="50"/>
<connect gate="A" pin="IO_38" pad="51"/>
<connect gate="A" pin="IO_39" pad="52"/>
<connect gate="A" pin="IO_4" pad="6"/>
<connect gate="A" pin="IO_40" pad="54"/>
<connect gate="A" pin="IO_41" pad="55"/>
<connect gate="A" pin="IO_42" pad="56"/>
<connect gate="A" pin="IO_43" pad="57"/>
<connect gate="A" pin="IO_44" pad="58"/>
<connect gate="A" pin="IO_45" pad="60"/>
<connect gate="A" pin="IO_46" pad="61"/>
<connect gate="A" pin="IO_47" pad="63"/>
<connect gate="A" pin="IO_48" pad="64"/>
<connect gate="A" pin="IO_49" pad="65"/>
<connect gate="A" pin="IO_5" pad="8"/>
<connect gate="A" pin="IO_50" pad="67"/>
<connect gate="A" pin="IO_51" pad="68"/>
<connect gate="A" pin="IO_52" pad="69"/>
<connect gate="A" pin="IO_53" pad="70"/>
<connect gate="A" pin="IO_54" pad="73"/>
<connect gate="A" pin="IO_55" pad="74"/>
<connect gate="A" pin="IO_56" pad="75"/>
<connect gate="A" pin="IO_57" pad="76"/>
<connect gate="A" pin="IO_58" pad="77"/>
<connect gate="A" pin="IO_59" pad="79"/>
<connect gate="A" pin="IO_6" pad="9"/>
<connect gate="A" pin="IO_60" pad="80"/>
<connect gate="A" pin="IO_7" pad="10"/>
<connect gate="A" pin="IO_8" pad="11"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="VCCINT" pad="3"/>
<connect gate="A" pin="VCCINT_2" pad="43"/>
<connect gate="A" pin="VCCIO" pad="13"/>
<connect gate="A" pin="VCCIO_2" pad="26"/>
<connect gate="A" pin="VCCIO_3" pad="38"/>
<connect gate="A" pin="VCCIO_4" pad="78"/>
<connect gate="A" pin="VCCIO_5" pad="66"/>
<connect gate="A" pin="VCCIO_6" pad="53"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128SLI84-10N"/>
<attribute name="OC_FARNELL" value="1549459"/>
<attribute name="OC_NEWARK" value="51R9746"/>
<attribute name="PACKAGE" value="84-PLCC"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128SQC100-10N" prefix="U">
<description>IC, CPLD, EEPROM</description>
<gates>
<gate name="A" symbol="EPM7128SQC100-10N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="88"/>
<connect gate="A" pin="GNDINT_2" pad="40"/>
<connect gate="A" pin="GNDIO" pad="45"/>
<connect gate="A" pin="GNDIO_2" pad="28"/>
<connect gate="A" pin="GNDIO_3" pad="76"/>
<connect gate="A" pin="GNDIO_4" pad="97"/>
<connect gate="A" pin="GNDIO_5" pad="13"/>
<connect gate="A" pin="GNDIO_6" pad="61"/>
<connect gate="A" pin="INPUT/GCLK1" pad="89"/>
<connect gate="A" pin="INPUT/GCLRN" pad="91"/>
<connect gate="A" pin="INPUT/OE1" pad="90"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="92"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="15"/>
<connect gate="A" pin="IO_14" pad="16"/>
<connect gate="A" pin="IO_15" pad="18"/>
<connect gate="A" pin="IO_16" pad="19"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="26"/>
<connect gate="A" pin="IO_23" pad="27"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="34"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="35"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="38"/>
<connect gate="A" pin="IO_33" pad="39"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="43"/>
<connect gate="A" pin="IO_36" pad="44"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="51"/>
<connect gate="A" pin="IO_43" pad="52"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="59"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="60"/>
<connect gate="A" pin="IO_51" pad="62"/>
<connect gate="A" pin="IO_52" pad="63"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="66"/>
<connect gate="A" pin="IO_55" pad="67"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="73"/>
<connect gate="A" pin="IO_61" pad="74"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="82"/>
<connect gate="A" pin="IO_68" pad="83"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="86"/>
<connect gate="A" pin="IO_71" pad="94"/>
<connect gate="A" pin="IO_72" pad="87"/>
<connect gate="A" pin="IO_73" pad="95"/>
<connect gate="A" pin="IO_74" pad="96"/>
<connect gate="A" pin="IO_75" pad="98"/>
<connect gate="A" pin="IO_76" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="TCK" pad="64"/>
<connect gate="A" pin="TDI" pad="6"/>
<connect gate="A" pin="TDO" pad="75"/>
<connect gate="A" pin="TMS" pad="17"/>
<connect gate="A" pin="VCCINT_(5.0_V_ONLY)" pad="41"/>
<connect gate="A" pin="VCCINT_(5.0_V_ONLY)_2" pad="93"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)" pad="84"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_2" pad="20"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_3" pad="53"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_4" pad="5"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_5" pad="68"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_6" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128SQC100-10N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9749"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128SQC160-15N" prefix="U">
<description>IC, CPLD, EEPROM</description>
<gates>
<gate name="A" symbol="EPM7128SQC160-15N_A"/>
<gate name="B" symbol="EPM7128SQC160-15N_B"/>
</gates>
<devices>
<device name="" package="QFP65P3100X3100X410-160N">
<connects>
<connect gate="A" pin="GNDINT" pad="60"/>
<connect gate="A" pin="GNDIO" pad="42"/>
<connect gate="A" pin="GNDIO_2" pad="66"/>
<connect gate="A" pin="GNDIO_3" pad="17"/>
<connect gate="A" pin="IO" pad="13"/>
<connect gate="A" pin="IO_10" pad="16"/>
<connect gate="A" pin="IO_11" pad="50"/>
<connect gate="A" pin="IO_12" pad="28"/>
<connect gate="A" pin="IO_13" pad="51"/>
<connect gate="A" pin="IO_14" pad="29"/>
<connect gate="A" pin="IO_15" pad="52"/>
<connect gate="A" pin="IO_16" pad="30"/>
<connect gate="A" pin="IO_17" pad="53"/>
<connect gate="A" pin="IO_18" pad="31"/>
<connect gate="A" pin="IO_19" pad="54"/>
<connect gate="A" pin="IO_2" pad="25"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="67"/>
<connect gate="A" pin="IO_23" pad="56"/>
<connect gate="A" pin="IO_24" pad="58"/>
<connect gate="A" pin="IO_25" pad="62"/>
<connect gate="A" pin="IO_26" pad="63"/>
<connect gate="A" pin="IO_27" pad="64"/>
<connect gate="A" pin="IO_28" pad="65"/>
<connect gate="A" pin="IO_29" pad="68"/>
<connect gate="A" pin="IO_3" pad="41"/>
<connect gate="A" pin="IO_30" pad="69"/>
<connect gate="A" pin="IO_31" pad="57"/>
<connect gate="A" pin="IO_32" pad="59"/>
<connect gate="A" pin="IO_33" pad="70"/>
<connect gate="A" pin="IO_34" pad="80"/>
<connect gate="A" pin="IO_35" pad="71"/>
<connect gate="A" pin="IO_36" pad="78"/>
<connect gate="A" pin="IO_37" pad="72"/>
<connect gate="A" pin="IO_38" pad="73"/>
<connect gate="A" pin="IO_39" pad="18"/>
<connect gate="A" pin="IO_4" pad="14"/>
<connect gate="A" pin="IO_40" pad="11"/>
<connect gate="A" pin="IO_41" pad="19"/>
<connect gate="A" pin="IO_42" pad="23"/>
<connect gate="A" pin="IO_43" pad="20"/>
<connect gate="A" pin="IO_44" pad="12"/>
<connect gate="A" pin="IO_45" pad="21"/>
<connect gate="A" pin="IO_46" pad="24"/>
<connect gate="A" pin="IO_47" pad="10"/>
<connect gate="A" pin="IO_5" pad="15"/>
<connect gate="A" pin="IO_6" pad="27"/>
<connect gate="A" pin="IO_7" pad="48"/>
<connect gate="A" pin="IO_8" pad="43"/>
<connect gate="A" pin="IO_9" pad="49"/>
<connect gate="A" pin="NC" pad="40"/>
<connect gate="A" pin="NC_10" pad="35"/>
<connect gate="A" pin="NC_11" pad="4"/>
<connect gate="A" pin="NC_12" pad="74"/>
<connect gate="A" pin="NC_13" pad="36"/>
<connect gate="A" pin="NC_14" pad="38"/>
<connect gate="A" pin="NC_15" pad="75"/>
<connect gate="A" pin="NC_16" pad="39"/>
<connect gate="A" pin="NC_17" pad="5"/>
<connect gate="A" pin="NC_18" pad="77"/>
<connect gate="A" pin="NC_19" pad="7"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_20" pad="76"/>
<connect gate="A" pin="NC_21" pad="6"/>
<connect gate="A" pin="NC_22" pad="37"/>
<connect gate="A" pin="NC_3" pad="44"/>
<connect gate="A" pin="NC_4" pad="2"/>
<connect gate="A" pin="NC_5" pad="45"/>
<connect gate="A" pin="NC_6" pad="34"/>
<connect gate="A" pin="NC_7" pad="46"/>
<connect gate="A" pin="NC_8" pad="3"/>
<connect gate="A" pin="NC_9" pad="47"/>
<connect gate="A" pin="TDI" pad="9"/>
<connect gate="A" pin="TMS" pad="22"/>
<connect gate="A" pin="VCCINT" pad="61"/>
<connect gate="A" pin="VCCIO" pad="79"/>
<connect gate="A" pin="VCCIO_2" pad="26"/>
<connect gate="A" pin="VCCIO_3" pad="8"/>
<connect gate="A" pin="VCCIO_4" pad="55"/>
<connect gate="B" pin="GNDINT" pad="138"/>
<connect gate="B" pin="GNDIO" pad="148"/>
<connect gate="B" pin="GNDIO_2" pad="113"/>
<connect gate="B" pin="GNDIO_3" pad="95"/>
<connect gate="B" pin="INPUT/GCLK1" pad="139"/>
<connect gate="B" pin="INPUT/GCLRN" pad="141"/>
<connect gate="B" pin="INPUT/OE1" pad="140"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="142"/>
<connect gate="B" pin="IO" pad="160"/>
<connect gate="B" pin="IO_10" pad="128"/>
<connect gate="B" pin="IO_11" pad="129"/>
<connect gate="B" pin="IO_12" pad="93"/>
<connect gate="B" pin="IO_13" pad="130"/>
<connect gate="B" pin="IO_14" pad="94"/>
<connect gate="B" pin="IO_15" pad="132"/>
<connect gate="B" pin="IO_16" pad="131"/>
<connect gate="B" pin="IO_17" pad="134"/>
<connect gate="B" pin="IO_18" pad="96"/>
<connect gate="B" pin="IO_19" pad="97"/>
<connect gate="B" pin="IO_2" pad="88"/>
<connect gate="B" pin="IO_20" pad="98"/>
<connect gate="B" pin="IO_21" pad="100"/>
<connect gate="B" pin="IO_22" pad="101"/>
<connect gate="B" pin="IO_23" pad="102"/>
<connect gate="B" pin="IO_24" pad="103"/>
<connect gate="B" pin="IO_25" pad="105"/>
<connect gate="B" pin="IO_26" pad="106"/>
<connect gate="B" pin="IO_27" pad="107"/>
<connect gate="B" pin="IO_28" pad="108"/>
<connect gate="B" pin="IO_29" pad="109"/>
<connect gate="B" pin="IO_3" pad="121"/>
<connect gate="B" pin="IO_30" pad="110"/>
<connect gate="B" pin="IO_31" pad="111"/>
<connect gate="B" pin="IO_32" pad="135"/>
<connect gate="B" pin="IO_33" pad="136"/>
<connect gate="B" pin="IO_34" pad="137"/>
<connect gate="B" pin="IO_35" pad="144"/>
<connect gate="B" pin="IO_36" pad="145"/>
<connect gate="B" pin="IO_37" pad="146"/>
<connect gate="B" pin="IO_38" pad="147"/>
<connect gate="B" pin="IO_39" pad="149"/>
<connect gate="B" pin="IO_4" pad="89"/>
<connect gate="B" pin="IO_40" pad="150"/>
<connect gate="B" pin="IO_41" pad="151"/>
<connect gate="B" pin="IO_42" pad="152"/>
<connect gate="B" pin="IO_43" pad="153"/>
<connect gate="B" pin="IO_44" pad="158"/>
<connect gate="B" pin="IO_45" pad="159"/>
<connect gate="B" pin="IO_5" pad="122"/>
<connect gate="B" pin="IO_6" pad="90"/>
<connect gate="B" pin="IO_7" pad="123"/>
<connect gate="B" pin="IO_8" pad="91"/>
<connect gate="B" pin="IO_9" pad="92"/>
<connect gate="B" pin="NC" pad="120"/>
<connect gate="B" pin="NC_10" pad="117"/>
<connect gate="B" pin="NC_11" pad="115"/>
<connect gate="B" pin="NC_12" pad="127"/>
<connect gate="B" pin="NC_13" pad="83"/>
<connect gate="B" pin="NC_14" pad="155"/>
<connect gate="B" pin="NC_15" pad="119"/>
<connect gate="B" pin="NC_16" pad="126"/>
<connect gate="B" pin="NC_17" pad="87"/>
<connect gate="B" pin="NC_18" pad="156"/>
<connect gate="B" pin="NC_19" pad="116"/>
<connect gate="B" pin="NC_2" pad="82"/>
<connect gate="B" pin="NC_20" pad="157"/>
<connect gate="B" pin="NC_21" pad="85"/>
<connect gate="B" pin="NC_22" pad="81"/>
<connect gate="B" pin="NC_3" pad="124"/>
<connect gate="B" pin="NC_4" pad="84"/>
<connect gate="B" pin="NC_5" pad="86"/>
<connect gate="B" pin="NC_6" pad="114"/>
<connect gate="B" pin="NC_7" pad="118"/>
<connect gate="B" pin="NC_8" pad="125"/>
<connect gate="B" pin="NC_9" pad="154"/>
<connect gate="B" pin="TCK" pad="99"/>
<connect gate="B" pin="TDO" pad="112"/>
<connect gate="B" pin="VCCINT" pad="143"/>
<connect gate="B" pin="VCCIO" pad="133"/>
<connect gate="B" pin="VCCIO_2" pad="104"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128SQC160-15N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9762"/>
<attribute name="PACKAGE" value="QFP-160"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128SQI100-10N" prefix="U">
<description>PLD EEPROM 128 MACROCELL 10NS</description>
<gates>
<gate name="A" symbol="EPM7128SQI100-10N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="88"/>
<connect gate="A" pin="GNDINT_2" pad="40"/>
<connect gate="A" pin="GNDIO" pad="45"/>
<connect gate="A" pin="GNDIO_2" pad="28"/>
<connect gate="A" pin="GNDIO_3" pad="76"/>
<connect gate="A" pin="GNDIO_4" pad="97"/>
<connect gate="A" pin="GNDIO_5" pad="13"/>
<connect gate="A" pin="GNDIO_6" pad="61"/>
<connect gate="A" pin="INPUT/GCLRN" pad="91"/>
<connect gate="A" pin="INPUT/OE1" pad="90"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="92"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO_10" pad="11"/>
<connect gate="A" pin="IO_11" pad="12"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="15"/>
<connect gate="A" pin="IO_14" pad="16"/>
<connect gate="A" pin="IO_15" pad="18"/>
<connect gate="A" pin="IO_16" pad="19"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="26"/>
<connect gate="A" pin="IO_23" pad="27"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="34"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="35"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="38"/>
<connect gate="A" pin="IO_33" pad="39"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="43"/>
<connect gate="A" pin="IO_36" pad="44"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="3"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="51"/>
<connect gate="A" pin="IO_43" pad="52"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="59"/>
<connect gate="A" pin="IO_5" pad="4"/>
<connect gate="A" pin="IO_50" pad="60"/>
<connect gate="A" pin="IO_51" pad="62"/>
<connect gate="A" pin="IO_52" pad="63"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="66"/>
<connect gate="A" pin="IO_55" pad="67"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="73"/>
<connect gate="A" pin="IO_61" pad="74"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="82"/>
<connect gate="A" pin="IO_68" pad="83"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="86"/>
<connect gate="A" pin="IO_71" pad="87"/>
<connect gate="A" pin="IO_72" pad="89"/>
<connect gate="A" pin="IO_73" pad="94"/>
<connect gate="A" pin="IO_74" pad="95"/>
<connect gate="A" pin="IO_75" pad="96"/>
<connect gate="A" pin="IO_76" pad="98"/>
<connect gate="A" pin="IO_77" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="TCK/IO" pad="64"/>
<connect gate="A" pin="TDI/IO" pad="6"/>
<connect gate="A" pin="TDO/IO" pad="75"/>
<connect gate="A" pin="TMS/IO" pad="17"/>
<connect gate="A" pin="VCCINT_(5.0_V_ONLY)" pad="41"/>
<connect gate="A" pin="VCCINT_(5.0_V_ONLY)_2" pad="93"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)" pad="84"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_2" pad="20"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_3" pad="53"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_4" pad="5"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_5" pad="68"/>
<connect gate="A" pin="VCCIO_(3.3_V_OR_5.0_V)_6" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128SQI100-10N"/>
<attribute name="OC_FARNELL" value="1549425"/>
<attribute name="OC_NEWARK" value="51R0531"/>
<attribute name="PACKAGE" value="PQFP-100"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128STC100-15N" prefix="U">
<description>IC MAX 7000 CPLD 128 100-TQFP</description>
<gates>
<gate name="A" symbol="EPM7128STC100-15N"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="26"/>
<connect gate="A" pin="GNDIO_2" pad="43"/>
<connect gate="A" pin="GNDIO_3" pad="11"/>
<connect gate="A" pin="GNDIO_4" pad="95"/>
<connect gate="A" pin="GNDIO_5" pad="59"/>
<connect gate="A" pin="GNDIO_6" pad="74"/>
<connect gate="A" pin="INPUT/*GCLR" pad="89"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="25"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="12"/>
<connect gate="A" pin="IO_11" pad="13"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="27"/>
<connect gate="A" pin="IO_16" pad="28"/>
<connect gate="A" pin="IO_17" pad="29"/>
<connect gate="A" pin="IO_18" pad="30"/>
<connect gate="A" pin="IO_19" pad="31"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="32"/>
<connect gate="A" pin="IO_21" pad="33"/>
<connect gate="A" pin="IO_22" pad="35"/>
<connect gate="A" pin="IO_23" pad="36"/>
<connect gate="A" pin="IO_24" pad="37"/>
<connect gate="A" pin="IO_25" pad="40"/>
<connect gate="A" pin="IO_26" pad="41"/>
<connect gate="A" pin="IO_27" pad="42"/>
<connect gate="A" pin="IO_28" pad="44"/>
<connect gate="A" pin="IO_29" pad="45"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="46"/>
<connect gate="A" pin="IO_31" pad="47"/>
<connect gate="A" pin="IO_32" pad="48"/>
<connect gate="A" pin="IO_33" pad="49"/>
<connect gate="A" pin="IO_34" pad="50"/>
<connect gate="A" pin="IO_35" pad="52"/>
<connect gate="A" pin="IO_36" pad="53"/>
<connect gate="A" pin="IO_37" pad="54"/>
<connect gate="A" pin="IO_38" pad="55"/>
<connect gate="A" pin="IO_39" pad="56"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="57"/>
<connect gate="A" pin="IO_41" pad="58"/>
<connect gate="A" pin="IO_42" pad="60"/>
<connect gate="A" pin="IO_43" pad="61"/>
<connect gate="A" pin="IO_44" pad="63"/>
<connect gate="A" pin="IO_45" pad="64"/>
<connect gate="A" pin="IO_46" pad="65"/>
<connect gate="A" pin="IO_47" pad="67"/>
<connect gate="A" pin="IO_48" pad="68"/>
<connect gate="A" pin="IO_49" pad="69"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="70"/>
<connect gate="A" pin="IO_51" pad="71"/>
<connect gate="A" pin="IO_52" pad="72"/>
<connect gate="A" pin="IO_53" pad="75"/>
<connect gate="A" pin="IO_54" pad="76"/>
<connect gate="A" pin="IO_55" pad="77"/>
<connect gate="A" pin="IO_56" pad="78"/>
<connect gate="A" pin="IO_57" pad="79"/>
<connect gate="A" pin="IO_58" pad="80"/>
<connect gate="A" pin="IO_59" pad="81"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="83"/>
<connect gate="A" pin="IO_61" pad="84"/>
<connect gate="A" pin="IO_62" pad="85"/>
<connect gate="A" pin="IO_63" pad="92"/>
<connect gate="A" pin="IO_64" pad="93"/>
<connect gate="A" pin="IO_65" pad="94"/>
<connect gate="A" pin="IO_66" pad="96"/>
<connect gate="A" pin="IO_67" pad="97"/>
<connect gate="A" pin="IO_68" pad="98"/>
<connect gate="A" pin="IO_69" pad="99"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="100"/>
<connect gate="A" pin="IO_71" pad="19"/>
<connect gate="A" pin="IO_72" pad="20"/>
<connect gate="A" pin="IO_73" pad="21"/>
<connect gate="A" pin="IO_74" pad="22"/>
<connect gate="A" pin="IO_75" pad="23"/>
<connect gate="A" pin="IO_76" pad="24"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="39"/>
<connect gate="A" pin="VCCINT_2" pad="91"/>
<connect gate="A" pin="VCCIO" pad="51"/>
<connect gate="A" pin="VCCIO_2" pad="3"/>
<connect gate="A" pin="VCCIO_3" pad="82"/>
<connect gate="A" pin="VCCIO_4" pad="18"/>
<connect gate="A" pin="VCCIO_5" pad="34"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128STC100-15N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R0532"/>
<attribute name="PACKAGE" value="1100-TQFP"/>
<attribute name="SUPPLIER" value="ALTERA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128STI100-10N">
<description>PLD EEPROM 128 MACROCELL 10NS</description>
<gates>
<gate name="A" symbol="EPM7128STI100-10N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="43"/>
<connect gate="A" pin="GNDIO_5" pad="74"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="12"/>
<connect gate="A" pin="IO_11" pad="13"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="35"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="36"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="40"/>
<connect gate="A" pin="IO_33" pad="41"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="52"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="60"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="61"/>
<connect gate="A" pin="IO_51" pad="63"/>
<connect gate="A" pin="IO_52" pad="64"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="67"/>
<connect gate="A" pin="IO_55" pad="68"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="75"/>
<connect gate="A" pin="IO_61" pad="76"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="83"/>
<connect gate="A" pin="IO_68" pad="84"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="92"/>
<connect gate="A" pin="IO_71" pad="93"/>
<connect gate="A" pin="IO_72" pad="94"/>
<connect gate="A" pin="IO_73" pad="96"/>
<connect gate="A" pin="IO_74" pad="97"/>
<connect gate="A" pin="IO_75" pad="98"/>
<connect gate="A" pin="IO_76" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="91"/>
<connect gate="A" pin="VCCINT_2" pad="39"/>
<connect gate="A" pin="VCCIO" pad="3"/>
<connect gate="A" pin="VCCIO_2" pad="34"/>
<connect gate="A" pin="VCCIO_3" pad="18"/>
<connect gate="A" pin="VCCIO_4" pad="51"/>
<connect gate="A" pin="VCCIO_5" pad="82"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7128STI100-10N"/>
<attribute name="OC_FARNELL" value="1549428"/>
<attribute name="OC_NEWARK" value="51R9780"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7160STI100-10N">
<description>PLD EEPROM 128 MACROCELL 10NS</description>
<gates>
<gate name="A" symbol="EPM7160STI100-10N"/>
</gates>
<devices>
<device name="" package="QFP65P1720X2320X340-100N">
<connects>
<connect gate="A" pin="GNDINT" pad="38"/>
<connect gate="A" pin="GNDINT_2" pad="86"/>
<connect gate="A" pin="GNDIO" pad="95"/>
<connect gate="A" pin="GNDIO_2" pad="11"/>
<connect gate="A" pin="GNDIO_3" pad="26"/>
<connect gate="A" pin="GNDIO_4" pad="43"/>
<connect gate="A" pin="GNDIO_5" pad="74"/>
<connect gate="A" pin="GNDIO_6" pad="59"/>
<connect gate="A" pin="INPUT/GCLK1" pad="87"/>
<connect gate="A" pin="INPUT/GCLR" pad="89"/>
<connect gate="A" pin="INPUT/OE1" pad="88"/>
<connect gate="A" pin="INPUT/OE2/GCLK2" pad="90"/>
<connect gate="A" pin="IO" pad="100"/>
<connect gate="A" pin="IO/TCK" pad="62"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TDO" pad="73"/>
<connect gate="A" pin="IO/TMS" pad="15"/>
<connect gate="A" pin="IO_10" pad="12"/>
<connect gate="A" pin="IO_11" pad="13"/>
<connect gate="A" pin="IO_12" pad="14"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="23"/>
<connect gate="A" pin="IO_2" pad="1"/>
<connect gate="A" pin="IO_20" pad="24"/>
<connect gate="A" pin="IO_21" pad="25"/>
<connect gate="A" pin="IO_22" pad="27"/>
<connect gate="A" pin="IO_23" pad="28"/>
<connect gate="A" pin="IO_24" pad="29"/>
<connect gate="A" pin="IO_25" pad="30"/>
<connect gate="A" pin="IO_26" pad="31"/>
<connect gate="A" pin="IO_27" pad="32"/>
<connect gate="A" pin="IO_28" pad="33"/>
<connect gate="A" pin="IO_29" pad="35"/>
<connect gate="A" pin="IO_3" pad="2"/>
<connect gate="A" pin="IO_30" pad="36"/>
<connect gate="A" pin="IO_31" pad="37"/>
<connect gate="A" pin="IO_32" pad="40"/>
<connect gate="A" pin="IO_33" pad="41"/>
<connect gate="A" pin="IO_34" pad="42"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="47"/>
<connect gate="A" pin="IO_39" pad="48"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="49"/>
<connect gate="A" pin="IO_41" pad="50"/>
<connect gate="A" pin="IO_42" pad="52"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="54"/>
<connect gate="A" pin="IO_45" pad="55"/>
<connect gate="A" pin="IO_46" pad="56"/>
<connect gate="A" pin="IO_47" pad="57"/>
<connect gate="A" pin="IO_48" pad="58"/>
<connect gate="A" pin="IO_49" pad="60"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="61"/>
<connect gate="A" pin="IO_51" pad="63"/>
<connect gate="A" pin="IO_52" pad="64"/>
<connect gate="A" pin="IO_53" pad="65"/>
<connect gate="A" pin="IO_54" pad="67"/>
<connect gate="A" pin="IO_55" pad="68"/>
<connect gate="A" pin="IO_56" pad="69"/>
<connect gate="A" pin="IO_57" pad="70"/>
<connect gate="A" pin="IO_58" pad="71"/>
<connect gate="A" pin="IO_59" pad="72"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="75"/>
<connect gate="A" pin="IO_61" pad="76"/>
<connect gate="A" pin="IO_62" pad="77"/>
<connect gate="A" pin="IO_63" pad="78"/>
<connect gate="A" pin="IO_64" pad="79"/>
<connect gate="A" pin="IO_65" pad="80"/>
<connect gate="A" pin="IO_66" pad="81"/>
<connect gate="A" pin="IO_67" pad="83"/>
<connect gate="A" pin="IO_68" pad="84"/>
<connect gate="A" pin="IO_69" pad="85"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_70" pad="92"/>
<connect gate="A" pin="IO_71" pad="93"/>
<connect gate="A" pin="IO_72" pad="94"/>
<connect gate="A" pin="IO_73" pad="96"/>
<connect gate="A" pin="IO_74" pad="97"/>
<connect gate="A" pin="IO_75" pad="98"/>
<connect gate="A" pin="IO_76" pad="99"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="10"/>
<connect gate="A" pin="VCCINT" pad="91"/>
<connect gate="A" pin="VCCINT_2" pad="39"/>
<connect gate="A" pin="VCCIO" pad="3"/>
<connect gate="A" pin="VCCIO_2" pad="34"/>
<connect gate="A" pin="VCCIO_3" pad="18"/>
<connect gate="A" pin="VCCIO_4" pad="51"/>
<connect gate="A" pin="VCCIO_5" pad="82"/>
<connect gate="A" pin="VCCIO_6" pad="66"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7160STI100-10N"/>
<attribute name="OC_FARNELL" value="1549430"/>
<attribute name="OC_NEWARK" value="51R9810"/>
<attribute name="PACKAGE" value="100-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7192SQI160-10N" prefix="U">
<description>Programmable Logic Device Family</description>
<gates>
<gate name="A" symbol="EPM7192SQI160-10N_A"/>
<gate name="B" symbol="EPM7192SQI160-10N_B"/>
</gates>
<devices>
<device name="" package="QFP65P3120X3120X410-160N">
<connects>
<connect gate="A" pin="GND" pad="66"/>
<connect gate="A" pin="GND_2" pad="18"/>
<connect gate="A" pin="GND_3" pad="57"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="GND_5" pad="47"/>
<connect gate="A" pin="GND_6" pad="64"/>
<connect gate="A" pin="GND_7" pad="32"/>
<connect gate="A" pin="IO" pad="80"/>
<connect gate="A" pin="IO_10" pad="13"/>
<connect gate="A" pin="IO_11" pad="14"/>
<connect gate="A" pin="IO_12" pad="15"/>
<connect gate="A" pin="IO_13" pad="16"/>
<connect gate="A" pin="IO_14" pad="17"/>
<connect gate="A" pin="IO_15" pad="19"/>
<connect gate="A" pin="IO_16" pad="20"/>
<connect gate="A" pin="IO_17" pad="21"/>
<connect gate="A" pin="IO_18" pad="22"/>
<connect gate="A" pin="IO_19" pad="24"/>
<connect gate="A" pin="IO_2" pad="2"/>
<connect gate="A" pin="IO_20" pad="26"/>
<connect gate="A" pin="IO_21" pad="27"/>
<connect gate="A" pin="IO_22" pad="28"/>
<connect gate="A" pin="IO_23" pad="29"/>
<connect gate="A" pin="IO_24" pad="30"/>
<connect gate="A" pin="IO_25" pad="31"/>
<connect gate="A" pin="IO_26" pad="33"/>
<connect gate="A" pin="IO_27" pad="34"/>
<connect gate="A" pin="IO_28" pad="35"/>
<connect gate="A" pin="IO_29" pad="36"/>
<connect gate="A" pin="IO_3" pad="4"/>
<connect gate="A" pin="IO_30" pad="37"/>
<connect gate="A" pin="IO_31" pad="38"/>
<connect gate="A" pin="IO_32" pad="41"/>
<connect gate="A" pin="IO_33" pad="42"/>
<connect gate="A" pin="IO_34" pad="43"/>
<connect gate="A" pin="IO_35" pad="44"/>
<connect gate="A" pin="IO_36" pad="45"/>
<connect gate="A" pin="IO_37" pad="46"/>
<connect gate="A" pin="IO_38" pad="48"/>
<connect gate="A" pin="IO_39" pad="49"/>
<connect gate="A" pin="IO_4" pad="5"/>
<connect gate="A" pin="IO_40" pad="50"/>
<connect gate="A" pin="IO_41" pad="51"/>
<connect gate="A" pin="IO_42" pad="52"/>
<connect gate="A" pin="IO_43" pad="53"/>
<connect gate="A" pin="IO_44" pad="58"/>
<connect gate="A" pin="IO_45" pad="59"/>
<connect gate="A" pin="IO_46" pad="60"/>
<connect gate="A" pin="IO_47" pad="61"/>
<connect gate="A" pin="IO_48" pad="62"/>
<connect gate="A" pin="IO_49" pad="63"/>
<connect gate="A" pin="IO_5" pad="6"/>
<connect gate="A" pin="IO_50" pad="68"/>
<connect gate="A" pin="IO_51" pad="69"/>
<connect gate="A" pin="IO_52" pad="70"/>
<connect gate="A" pin="IO_53" pad="71"/>
<connect gate="A" pin="IO_54" pad="72"/>
<connect gate="A" pin="IO_55" pad="73"/>
<connect gate="A" pin="IO_56" pad="75"/>
<connect gate="A" pin="IO_57" pad="76"/>
<connect gate="A" pin="IO_58" pad="77"/>
<connect gate="A" pin="IO_59" pad="78"/>
<connect gate="A" pin="IO_6" pad="7"/>
<connect gate="A" pin="IO_60" pad="79"/>
<connect gate="A" pin="IO_7" pad="8"/>
<connect gate="A" pin="IO_8" pad="9"/>
<connect gate="A" pin="IO_9" pad="12"/>
<connect gate="A" pin="NC" pad="39"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="54"/>
<connect gate="A" pin="NC_4" pad="67"/>
<connect gate="A" pin="NC_5" pad="11"/>
<connect gate="A" pin="TMS" pad="23"/>
<connect gate="A" pin="VCCINT" pad="65"/>
<connect gate="A" pin="VCCINT_2" pad="56"/>
<connect gate="A" pin="VCCIO" pad="10"/>
<connect gate="A" pin="VCCIO_2" pad="55"/>
<connect gate="A" pin="VCCIO_3" pad="25"/>
<connect gate="A" pin="VCCIO_4" pad="40"/>
<connect gate="A" pin="VCCIO_5" pad="74"/>
<connect gate="B" pin="GND" pad="148"/>
<connect gate="B" pin="GND_2" pad="81"/>
<connect gate="B" pin="GND_3" pad="143"/>
<connect gate="B" pin="GND_4" pad="126"/>
<connect gate="B" pin="GND_5" pad="111"/>
<connect gate="B" pin="GND_6" pad="138"/>
<connect gate="B" pin="GND_7" pad="96"/>
<connect gate="B" pin="INPUT/GCLK1" pad="139"/>
<connect gate="B" pin="INPUT/GCLRN" pad="141"/>
<connect gate="B" pin="INPUT/OE1" pad="140"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="142"/>
<connect gate="B" pin="IO" pad="160"/>
<connect gate="B" pin="IO_10" pad="92"/>
<connect gate="B" pin="IO_11" pad="93"/>
<connect gate="B" pin="IO_12" pad="94"/>
<connect gate="B" pin="IO_13" pad="95"/>
<connect gate="B" pin="IO_14" pad="97"/>
<connect gate="B" pin="IO_15" pad="99"/>
<connect gate="B" pin="IO_16" pad="100"/>
<connect gate="B" pin="IO_17" pad="101"/>
<connect gate="B" pin="IO_18" pad="102"/>
<connect gate="B" pin="IO_19" pad="104"/>
<connect gate="B" pin="IO_2" pad="83"/>
<connect gate="B" pin="IO_20" pad="105"/>
<connect gate="B" pin="IO_21" pad="106"/>
<connect gate="B" pin="IO_22" pad="107"/>
<connect gate="B" pin="IO_23" pad="108"/>
<connect gate="B" pin="IO_24" pad="109"/>
<connect gate="B" pin="IO_25" pad="112"/>
<connect gate="B" pin="IO_26" pad="113"/>
<connect gate="B" pin="IO_27" pad="114"/>
<connect gate="B" pin="IO_28" pad="115"/>
<connect gate="B" pin="IO_29" pad="116"/>
<connect gate="B" pin="IO_3" pad="84"/>
<connect gate="B" pin="IO_30" pad="117"/>
<connect gate="B" pin="IO_31" pad="119"/>
<connect gate="B" pin="IO_32" pad="121"/>
<connect gate="B" pin="IO_33" pad="122"/>
<connect gate="B" pin="IO_34" pad="123"/>
<connect gate="B" pin="IO_35" pad="124"/>
<connect gate="B" pin="IO_36" pad="125"/>
<connect gate="B" pin="IO_37" pad="127"/>
<connect gate="B" pin="IO_38" pad="128"/>
<connect gate="B" pin="IO_39" pad="129"/>
<connect gate="B" pin="IO_4" pad="85"/>
<connect gate="B" pin="IO_40" pad="130"/>
<connect gate="B" pin="IO_41" pad="131"/>
<connect gate="B" pin="IO_42" pad="132"/>
<connect gate="B" pin="IO_43" pad="134"/>
<connect gate="B" pin="IO_44" pad="136"/>
<connect gate="B" pin="IO_45" pad="145"/>
<connect gate="B" pin="IO_46" pad="147"/>
<connect gate="B" pin="IO_47" pad="149"/>
<connect gate="B" pin="IO_48" pad="150"/>
<connect gate="B" pin="IO_49" pad="151"/>
<connect gate="B" pin="IO_5" pad="86"/>
<connect gate="B" pin="IO_50" pad="152"/>
<connect gate="B" pin="IO_51" pad="153"/>
<connect gate="B" pin="IO_52" pad="154"/>
<connect gate="B" pin="IO_53" pad="156"/>
<connect gate="B" pin="IO_54" pad="157"/>
<connect gate="B" pin="IO_55" pad="158"/>
<connect gate="B" pin="IO_56" pad="159"/>
<connect gate="B" pin="IO_6" pad="87"/>
<connect gate="B" pin="IO_7" pad="88"/>
<connect gate="B" pin="IO_8" pad="90"/>
<connect gate="B" pin="IO_9" pad="91"/>
<connect gate="B" pin="NC" pad="120"/>
<connect gate="B" pin="NC_2" pad="110"/>
<connect gate="B" pin="NC_3" pad="82"/>
<connect gate="B" pin="TCK" pad="98"/>
<connect gate="B" pin="TDI" pad="146"/>
<connect gate="B" pin="TDO" pad="135"/>
<connect gate="B" pin="VCCINT" pad="144"/>
<connect gate="B" pin="VCCINT_2" pad="137"/>
<connect gate="B" pin="VCCIO" pad="118"/>
<connect gate="B" pin="VCCIO_2" pad="155"/>
<connect gate="B" pin="VCCIO_3" pad="89"/>
<connect gate="B" pin="VCCIO_4" pad="103"/>
<connect gate="B" pin="VCCIO_5" pad="133"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7192SQI160-10N"/>
<attribute name="OC_FARNELL" value="1549439"/>
<attribute name="OC_NEWARK" value="51R9826"/>
<attribute name="PACKAGE" value="PQFP-160"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7256AETC144-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7256AETC144-7N_A"/>
<gate name="B" symbol="EPM7256AETC144-7N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="33"/>
<connect gate="A" pin="GNDIO_2" pad="59"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="3"/>
<connect gate="A" pin="GNDIO_5" pad="13"/>
<connect gate="A" pin="GNDIO_6" pad="17"/>
<connect gate="A" pin="IO" pad="39"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="48"/>
<connect gate="A" pin="IO_11" pad="49"/>
<connect gate="A" pin="IO_12" pad="53"/>
<connect gate="A" pin="IO_13" pad="54"/>
<connect gate="A" pin="IO_14" pad="55"/>
<connect gate="A" pin="IO_15" pad="56"/>
<connect gate="A" pin="IO_16" pad="60"/>
<connect gate="A" pin="IO_17" pad="61"/>
<connect gate="A" pin="IO_18" pad="62"/>
<connect gate="A" pin="IO_19" pad="63"/>
<connect gate="A" pin="IO_2" pad="40"/>
<connect gate="A" pin="IO_20" pad="65"/>
<connect gate="A" pin="IO_21" pad="66"/>
<connect gate="A" pin="IO_22" pad="67"/>
<connect gate="A" pin="IO_23" pad="68"/>
<connect gate="A" pin="IO_24" pad="69"/>
<connect gate="A" pin="IO_25" pad="70"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="72"/>
<connect gate="A" pin="IO_28" pad="1"/>
<connect gate="A" pin="IO_29" pad="2"/>
<connect gate="A" pin="IO_3" pad="41"/>
<connect gate="A" pin="IO_30" pad="5"/>
<connect gate="A" pin="IO_31" pad="6"/>
<connect gate="A" pin="IO_32" pad="7"/>
<connect gate="A" pin="IO_33" pad="8"/>
<connect gate="A" pin="IO_34" pad="9"/>
<connect gate="A" pin="IO_35" pad="10"/>
<connect gate="A" pin="IO_36" pad="11"/>
<connect gate="A" pin="IO_37" pad="12"/>
<connect gate="A" pin="IO_38" pad="14"/>
<connect gate="A" pin="IO_39" pad="15"/>
<connect gate="A" pin="IO_4" pad="42"/>
<connect gate="A" pin="IO_40" pad="16"/>
<connect gate="A" pin="IO_41" pad="18"/>
<connect gate="A" pin="IO_42" pad="19"/>
<connect gate="A" pin="IO_43" pad="21"/>
<connect gate="A" pin="IO_44" pad="22"/>
<connect gate="A" pin="IO_45" pad="23"/>
<connect gate="A" pin="IO_46" pad="25"/>
<connect gate="A" pin="IO_47" pad="26"/>
<connect gate="A" pin="IO_48" pad="27"/>
<connect gate="A" pin="IO_49" pad="28"/>
<connect gate="A" pin="IO_5" pad="43"/>
<connect gate="A" pin="IO_50" pad="29"/>
<connect gate="A" pin="IO_51" pad="30"/>
<connect gate="A" pin="IO_52" pad="31"/>
<connect gate="A" pin="IO_53" pad="32"/>
<connect gate="A" pin="IO_54" pad="34"/>
<connect gate="A" pin="IO_55" pad="35"/>
<connect gate="A" pin="IO_56" pad="36"/>
<connect gate="A" pin="IO_57" pad="37"/>
<connect gate="A" pin="IO_58" pad="38"/>
<connect gate="A" pin="IO_6" pad="44"/>
<connect gate="A" pin="IO_7" pad="45"/>
<connect gate="A" pin="IO_8" pad="46"/>
<connect gate="A" pin="IO_9" pad="47"/>
<connect gate="A" pin="VCCINT" pad="58"/>
<connect gate="A" pin="VCCINT_2" pad="51"/>
<connect gate="A" pin="VCCIO" pad="50"/>
<connect gate="A" pin="VCCIO_2" pad="24"/>
<connect gate="B" pin="GNDINT" pad="129"/>
<connect gate="B" pin="GNDINT_2" pad="124"/>
<connect gate="B" pin="GNDIO" pad="85"/>
<connect gate="B" pin="GNDIO_2" pad="135"/>
<connect gate="B" pin="GNDIO_3" pad="105"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/GCLRN" pad="127"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="143"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="114"/>
<connect gate="B" pin="IO_11" pad="116"/>
<connect gate="B" pin="IO_12" pad="117"/>
<connect gate="B" pin="IO_13" pad="118"/>
<connect gate="B" pin="IO_14" pad="119"/>
<connect gate="B" pin="IO_15" pad="120"/>
<connect gate="B" pin="IO_16" pad="121"/>
<connect gate="B" pin="IO_17" pad="122"/>
<connect gate="B" pin="IO_18" pad="131"/>
<connect gate="B" pin="IO_19" pad="132"/>
<connect gate="B" pin="IO_2" pad="106"/>
<connect gate="B" pin="IO_20" pad="133"/>
<connect gate="B" pin="IO_21" pad="134"/>
<connect gate="B" pin="IO_22" pad="136"/>
<connect gate="B" pin="IO_23" pad="74"/>
<connect gate="B" pin="IO_24" pad="75"/>
<connect gate="B" pin="IO_25" pad="77"/>
<connect gate="B" pin="IO_26" pad="78"/>
<connect gate="B" pin="IO_27" pad="79"/>
<connect gate="B" pin="IO_28" pad="80"/>
<connect gate="B" pin="IO_29" pad="81"/>
<connect gate="B" pin="IO_3" pad="107"/>
<connect gate="B" pin="IO_30" pad="82"/>
<connect gate="B" pin="IO_31" pad="83"/>
<connect gate="B" pin="IO_32" pad="84"/>
<connect gate="B" pin="IO_33" pad="86"/>
<connect gate="B" pin="IO_34" pad="87"/>
<connect gate="B" pin="IO_35" pad="88"/>
<connect gate="B" pin="IO_36" pad="90"/>
<connect gate="B" pin="IO_37" pad="91"/>
<connect gate="B" pin="IO_38" pad="92"/>
<connect gate="B" pin="IO_39" pad="93"/>
<connect gate="B" pin="IO_4" pad="108"/>
<connect gate="B" pin="IO_40" pad="94"/>
<connect gate="B" pin="IO_41" pad="96"/>
<connect gate="B" pin="IO_42" pad="97"/>
<connect gate="B" pin="IO_43" pad="98"/>
<connect gate="B" pin="IO_44" pad="99"/>
<connect gate="B" pin="IO_45" pad="100"/>
<connect gate="B" pin="IO_46" pad="101"/>
<connect gate="B" pin="IO_47" pad="102"/>
<connect gate="B" pin="IO_48" pad="103"/>
<connect gate="B" pin="IO_49" pad="137"/>
<connect gate="B" pin="IO_5" pad="109"/>
<connect gate="B" pin="IO_50" pad="138"/>
<connect gate="B" pin="IO_51" pad="139"/>
<connect gate="B" pin="IO_52" pad="140"/>
<connect gate="B" pin="IO_53" pad="141"/>
<connect gate="B" pin="IO_54" pad="142"/>
<connect gate="B" pin="IO_6" pad="110"/>
<connect gate="B" pin="IO_7" pad="111"/>
<connect gate="B" pin="IO_8" pad="112"/>
<connect gate="B" pin="IO_9" pad="113"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="123"/>
<connect gate="B" pin="VCCIO" pad="95"/>
<connect gate="B" pin="VCCIO_2" pad="73"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
<connect gate="B" pin="VCCIO_4" pad="144"/>
<connect gate="B" pin="VCCIO_5" pad="76"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7256AETC144-7N"/>
<attribute name="OC_FARNELL" value="1549433"/>
<attribute name="OC_NEWARK" value="51R9858"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7256AETI144-7N">
<description>Programmable Logic Device</description>
<gates>
<gate name="A" symbol="EPM7256AETI144-7N_A"/>
<gate name="B" symbol="EPM7256AETI144-7N_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="GNDINT" pad="57"/>
<connect gate="A" pin="GNDINT_2" pad="52"/>
<connect gate="A" pin="GNDIO" pad="33"/>
<connect gate="A" pin="GNDIO_2" pad="59"/>
<connect gate="A" pin="GNDIO_3" pad="64"/>
<connect gate="A" pin="GNDIO_4" pad="3"/>
<connect gate="A" pin="GNDIO_5" pad="13"/>
<connect gate="A" pin="GNDIO_6" pad="17"/>
<connect gate="A" pin="IO" pad="39"/>
<connect gate="A" pin="IO/TDI" pad="4"/>
<connect gate="A" pin="IO/TMS" pad="20"/>
<connect gate="A" pin="IO_10" pad="48"/>
<connect gate="A" pin="IO_11" pad="49"/>
<connect gate="A" pin="IO_12" pad="53"/>
<connect gate="A" pin="IO_13" pad="54"/>
<connect gate="A" pin="IO_14" pad="55"/>
<connect gate="A" pin="IO_15" pad="56"/>
<connect gate="A" pin="IO_16" pad="60"/>
<connect gate="A" pin="IO_17" pad="61"/>
<connect gate="A" pin="IO_18" pad="62"/>
<connect gate="A" pin="IO_19" pad="63"/>
<connect gate="A" pin="IO_2" pad="40"/>
<connect gate="A" pin="IO_20" pad="65"/>
<connect gate="A" pin="IO_21" pad="66"/>
<connect gate="A" pin="IO_22" pad="67"/>
<connect gate="A" pin="IO_23" pad="68"/>
<connect gate="A" pin="IO_24" pad="69"/>
<connect gate="A" pin="IO_25" pad="70"/>
<connect gate="A" pin="IO_26" pad="71"/>
<connect gate="A" pin="IO_27" pad="72"/>
<connect gate="A" pin="IO_28" pad="1"/>
<connect gate="A" pin="IO_29" pad="2"/>
<connect gate="A" pin="IO_3" pad="41"/>
<connect gate="A" pin="IO_30" pad="5"/>
<connect gate="A" pin="IO_31" pad="6"/>
<connect gate="A" pin="IO_32" pad="7"/>
<connect gate="A" pin="IO_33" pad="8"/>
<connect gate="A" pin="IO_34" pad="9"/>
<connect gate="A" pin="IO_35" pad="10"/>
<connect gate="A" pin="IO_36" pad="11"/>
<connect gate="A" pin="IO_37" pad="12"/>
<connect gate="A" pin="IO_38" pad="14"/>
<connect gate="A" pin="IO_39" pad="15"/>
<connect gate="A" pin="IO_4" pad="42"/>
<connect gate="A" pin="IO_40" pad="16"/>
<connect gate="A" pin="IO_41" pad="18"/>
<connect gate="A" pin="IO_42" pad="19"/>
<connect gate="A" pin="IO_43" pad="21"/>
<connect gate="A" pin="IO_44" pad="22"/>
<connect gate="A" pin="IO_45" pad="23"/>
<connect gate="A" pin="IO_46" pad="25"/>
<connect gate="A" pin="IO_47" pad="26"/>
<connect gate="A" pin="IO_48" pad="27"/>
<connect gate="A" pin="IO_49" pad="28"/>
<connect gate="A" pin="IO_5" pad="43"/>
<connect gate="A" pin="IO_50" pad="29"/>
<connect gate="A" pin="IO_51" pad="30"/>
<connect gate="A" pin="IO_52" pad="31"/>
<connect gate="A" pin="IO_53" pad="32"/>
<connect gate="A" pin="IO_54" pad="34"/>
<connect gate="A" pin="IO_55" pad="35"/>
<connect gate="A" pin="IO_56" pad="36"/>
<connect gate="A" pin="IO_57" pad="37"/>
<connect gate="A" pin="IO_58" pad="38"/>
<connect gate="A" pin="IO_6" pad="44"/>
<connect gate="A" pin="IO_7" pad="45"/>
<connect gate="A" pin="IO_8" pad="46"/>
<connect gate="A" pin="IO_9" pad="47"/>
<connect gate="A" pin="VCCINT" pad="58"/>
<connect gate="A" pin="VCCINT_2" pad="51"/>
<connect gate="A" pin="VCCIO" pad="50"/>
<connect gate="A" pin="VCCIO_2" pad="24"/>
<connect gate="B" pin="GNDINT" pad="129"/>
<connect gate="B" pin="GNDINT_2" pad="124"/>
<connect gate="B" pin="GNDIO" pad="85"/>
<connect gate="B" pin="GNDIO_2" pad="135"/>
<connect gate="B" pin="GNDIO_3" pad="105"/>
<connect gate="B" pin="INPUT/GCLK1" pad="125"/>
<connect gate="B" pin="INPUT/GCLRN" pad="127"/>
<connect gate="B" pin="INPUT/OE1" pad="126"/>
<connect gate="B" pin="INPUT/OE2/GCLK2" pad="128"/>
<connect gate="B" pin="IO" pad="143"/>
<connect gate="B" pin="IO/TCK" pad="89"/>
<connect gate="B" pin="IO/TDO" pad="104"/>
<connect gate="B" pin="IO_10" pad="114"/>
<connect gate="B" pin="IO_11" pad="116"/>
<connect gate="B" pin="IO_12" pad="117"/>
<connect gate="B" pin="IO_13" pad="118"/>
<connect gate="B" pin="IO_14" pad="119"/>
<connect gate="B" pin="IO_15" pad="120"/>
<connect gate="B" pin="IO_16" pad="121"/>
<connect gate="B" pin="IO_17" pad="122"/>
<connect gate="B" pin="IO_18" pad="131"/>
<connect gate="B" pin="IO_19" pad="132"/>
<connect gate="B" pin="IO_2" pad="106"/>
<connect gate="B" pin="IO_20" pad="133"/>
<connect gate="B" pin="IO_21" pad="134"/>
<connect gate="B" pin="IO_22" pad="136"/>
<connect gate="B" pin="IO_23" pad="74"/>
<connect gate="B" pin="IO_24" pad="75"/>
<connect gate="B" pin="IO_25" pad="77"/>
<connect gate="B" pin="IO_26" pad="78"/>
<connect gate="B" pin="IO_27" pad="79"/>
<connect gate="B" pin="IO_28" pad="80"/>
<connect gate="B" pin="IO_29" pad="81"/>
<connect gate="B" pin="IO_3" pad="107"/>
<connect gate="B" pin="IO_30" pad="82"/>
<connect gate="B" pin="IO_31" pad="83"/>
<connect gate="B" pin="IO_32" pad="84"/>
<connect gate="B" pin="IO_33" pad="86"/>
<connect gate="B" pin="IO_34" pad="87"/>
<connect gate="B" pin="IO_35" pad="88"/>
<connect gate="B" pin="IO_36" pad="90"/>
<connect gate="B" pin="IO_37" pad="91"/>
<connect gate="B" pin="IO_38" pad="92"/>
<connect gate="B" pin="IO_39" pad="93"/>
<connect gate="B" pin="IO_4" pad="108"/>
<connect gate="B" pin="IO_40" pad="94"/>
<connect gate="B" pin="IO_41" pad="96"/>
<connect gate="B" pin="IO_42" pad="97"/>
<connect gate="B" pin="IO_43" pad="98"/>
<connect gate="B" pin="IO_44" pad="99"/>
<connect gate="B" pin="IO_45" pad="100"/>
<connect gate="B" pin="IO_46" pad="101"/>
<connect gate="B" pin="IO_47" pad="102"/>
<connect gate="B" pin="IO_48" pad="103"/>
<connect gate="B" pin="IO_49" pad="137"/>
<connect gate="B" pin="IO_5" pad="109"/>
<connect gate="B" pin="IO_50" pad="138"/>
<connect gate="B" pin="IO_51" pad="139"/>
<connect gate="B" pin="IO_52" pad="140"/>
<connect gate="B" pin="IO_53" pad="141"/>
<connect gate="B" pin="IO_54" pad="142"/>
<connect gate="B" pin="IO_6" pad="110"/>
<connect gate="B" pin="IO_7" pad="111"/>
<connect gate="B" pin="IO_8" pad="112"/>
<connect gate="B" pin="IO_9" pad="113"/>
<connect gate="B" pin="VCCINT" pad="130"/>
<connect gate="B" pin="VCCINT_2" pad="123"/>
<connect gate="B" pin="VCCIO" pad="95"/>
<connect gate="B" pin="VCCIO_2" pad="73"/>
<connect gate="B" pin="VCCIO_3" pad="115"/>
<connect gate="B" pin="VCCIO_4" pad="144"/>
<connect gate="B" pin="VCCIO_5" pad="76"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="EPM7256AETI144-7N"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="51R9862"/>
<attribute name="PACKAGE" value="144-TQFP"/>
<attribute name="SUPPLIER" value="Altera"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
